{"text_format":"1","workbook":"xlsx","n_sheets":20,"sheets":["Welcome to Chhaya!","Instructions","STAT","Operative BP","Surface Solar Azimuth Angles","HVAC Dashboard","Lab Data","Radiation","Dry Bulb","Profile angles","Solar Altitude","Incident angle","Input Data","Heat gain from airflow","eq of time","Occupancy","Profile calcs","Solar Azimuth","AST","Stack Ventilation"],"not_rendered":{"charts":13,"images":39,"macros":1,"external_links":0,"defined_names":8,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Welcome to Chhaya!","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[[23,3,23,4],[7,7,15,19]]}
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Welcome to Chhaya!"]
[null,null,null,null,null,null,null,"Chhaya is a tool to determine shading requirements for a building at a preliminary design phase. This is based upon an estimation of a buildings balance point; i.e. where the building needs neither heating or cooling, so the building is in balance with it's climate. Appropriate shading stratagies can extend this period, and thereby reduce a buildings cooling and heating requirements.\n\nThe sunangles and shading reccomendations produced by this tool are not meant to be a substitute for a comprehensive energy analysis, and should be checked as the design progresses. To date, we have found this tool to be reasonably accurate and useful. We hope this helps you practice bioclimatic design!"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"Chhaya (Sanskrit) A shade, shadow, copy; esoterically, the astral image or body of a person. Besides referring to the human astral form, the term is usually applied to the shadows or copies,  -- the astral body-projections -- of the spiritual beings or pitris who played an important part in the early evolutionary development of humankind. In the first root-race, \"the pure, celestial Being (Dhyan Chohan) and the great Pitris of various classes were commissioned -- the one to evolve their images (Chhaya), and make of them physical man, the others to inform and thus endow him with divine intelligence and the comprehension of the Mysteries of Creation\" (SD 2:233n). This idea also appears in the Zohar: \"'In the Tzalam (shadow image) of Elohim (the Pitris), was made Adam (man)' \" (SD 2:137)."]

{"sheet":"Instructions","index":1,"n_rows":69,"n_cols":4,"rows_kept":69,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,null,"Instructions for Chhaya Data Input"]
[]
[]
[]
[null,null,"Weather Data Import"]
[null,null,1,"Copy the following address to your clipboard (or memorize it)"]
[null,null,null,"http://apps1.eere.energy.gov/buildings/energyplus/cfm/weather_data.cfm"]
[null,null,2,"Go to the tab named \"STAT\" (Black tab)."]
[null,null,3,"Follow the steps by clicking the buttons (There is no button for step 2)"]
[]
[null,null,"Step 1","This clears the contents of the cells for import of a new weather file. This is essential"]
[]
[null,null,"Step 2 ","Go to Import Data/From Web. This will open up a web query box. Browse to your desired weather station and use the \"STAT\" option. Once this is selected, select the table and hit import (at the bottom right. Make sure you select $A$! As the destination cell. THIS IS IMPORTANT. "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Step 3","Press the step 3 Button to finish the weather file import. The import will not be complete without this. "]
[]
[null,null,"Step 4","For non- US weather files press this button"]
[]
[null,null,"Step 4","For US weather files press this button"]

{"sheet":"STAT","index":2,"n_rows":545,"n_cols":34,"rows_kept":545,"cut":false,"hidden":false,"merged":[]}
[" -EnergyPlus Weather Converter V7.1.0.010"]
[" Statistics for SAU_Riyadh.404380_IWEC"]
[" Location -- RIYADH - SAU  "]
["{N",24,"ｰ",42,"'}","{E",46,"ｰ",47,"'}","{GMT",3,"Hours}"]
[" Elevation --   612m above sea level"]
[" Standard Pressure at Elevation --  94186Pa"]
[" Data Source -- IWEC Data"]
[]
[" WMO Station 404380"]
[]
[" - Displaying Design Conditions from \"Climate Design Data 2009 ASHRAE Handbook\""]
[" - ASHRAE design conditions are carefully generated from a period of record "]
[" - (typically 30 years) to be representative of that location and to be suitable"]
[" - for use in heating/cooling load calculations."]
[]
["    ","Design Stat","ColdestMonth","DB996","DB990","DP996","HR_DP996","DB_DP996","DP990","HR_DP990","DB_DP990","WS004c","DB_WS004c","WS010c","DB_WS010c","WS_DB996","WD_DB996"]
["    ","Units","{}","{ｰC}","{ｰC}","{ｰC}","{}","{ｰC}","{ｰC}","{}","{ｰC}","{m/s}","{ｰC}","{m/s}","{ｰC}","{m/s}","{deg}"]
["    ","Heating",1,5.9,7.2,-14,1.2,20.5,-11.1,1.6,24.3,10,15.9,9.1,16.8,1.6,320]
[]
["    ","Design Stat","HottestMonth","DBR","DB004","WB_DB004","DB010","WB_DB010","DB020","WB_DB020","WB004","DB_WB004","WB010","DB_WB010","WB020","DB_WB020","WS_DB004","WD_DB004","DP004","HR_DP004","DB_DP004","DP010","HR_DP010","DB_DP010","DP020","HR_DP020","DB_DP020","EN004","DB_EN004","EN010","DB_EN010","EN020","DB_EN020","#Hrs_8-4_&_DB-12.8/20.6"]
["    ","Units","{}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{m/s}","{deg}","{ｰC}","{}","{ｰC}","{ｰC}","{}","{ｰC}","{ｰC}","{}","{ｰC}","{kJ/kg}","{ｰC}","{kJ/kg}","{ｰC}","{kJ/kg}","{ｰC}","{}"]
["    ","Cooling",7,13.5,44.2,18.7,43.8,18.5,42.9,18.2,20.9,36.4,20,36.6,19.399999999999999,37.200000000000003,4.5,0,17.2,13.3,22.3,16.100000000000001,12.3,21.7,14.9,11.4,21.9,63.2,36.700000000000003,60.2,36.799999999999997,57.6,37.200000000000003,604]
[]
["    ","Design Stat","WS010","WS025","WS050","WBmax","DBmin_mean","DBmax_mean","DBmin_stddev","DBmax_stddev","DBmin05years","DBmax05years","DBmin10years","DBmax10years","DBmin20years","DBmax20years","DBmin50years","DBmax50years"]
["    ","Units","{m/s}","{m/s}","{m/s}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}","{ｰC}"]
["    ","Extremes",9.5,8.3000000000000007,7.3,25.5,2.9,46,1.8,0.8,1.6,46.6,0.6,47,-0.4,47.4,-1.7,48]
[]
[" - Displaying Monthly Design Conditions \"Climate Design Data 2009 ASHRAE Handbook\""]
[" - Monthly Optical Sky Depth Beam (taub) and Diffuse (taud)"]
[" ","                        ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","             taub (beam)",0.42399999999999999,0.63200000000000001,0.69899999999999995,0.70899999999999996,0.74399999999999999,0.72099999999999997,0.76600000000000001,0.749,0.64200000000000002,0.48099999999999998,0.499,0.42699999999999999]
[" ","          taud (diffuse)",1.8340000000000001,1.379,1.302,1.3,1.258,1.2669999999999999,1.2390000000000001,1.254,1.3759999999999999,1.6870000000000001,1.63,1.827]
[]
[" ","                    taub",{"$f":" Clear Sky Optical Depth for Beam Irradiance","v":{"$error":"#NAME?"}}]
[" ","                    taud",{"$f":" Clear Sky Optical Depth for Diffuse Irradiance","v":{"$error":"#NAME?"}}]
[]
[" - Monthly Solar Irradiance Wh/mｲ (noon on 21st of month)"]
[" ","               ib (beam)",813,661,646,656,633,644,615,622,678,781,727,789]
[" ","            id (diffuse)",188,310,353,363,379,373,383,375,324,227,226,183]
[]
[" ","                      ib","= Clear Sky Noon Beam Normal Irradiance on 21st Day"]
[" ","                      id","= Clear Sky Noon Diffuse Horizontal Irradiance on 21st Day"]
[]
[" - Monthly Drybulb and Mean Coincident Wetbulb Temperatures ｰC"]
[" ","                        ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","            Drybulb 0.4%",27.8,31,34.6,39.799999999999997,43.2,44.9,46,45.2,43.1,38.9,33.200000000000003,28.5]
[" "," Coincident Wetbulb 0.4%",14.4,15.5,16.2,17.2,17.899999999999999,18.5,19.2,19.7,18.5,16.899999999999999,16,14.8]
[" ","            Drybulb 2.0%",25.2,28,32.299999999999997,37.799999999999997,41.9,43.8,44.3,44.2,42,37.200000000000003,31.7,26.9]
[" "," Coincident Wetbulb 2.0%",13.1,14.1,15.3,17,17.8,18.100000000000001,18.5,19.100000000000001,18.100000000000001,16.399999999999999,15.4,14.3]
[" ","            Drybulb 5.0%",23.1,25.9,30.5,36,40.799999999999997,42.8,43.8,43.2,41,36.200000000000003,30.1,25]
[" "," Coincident Wetbulb 5.0%",12,13.1,14.7,16.600000000000001,17.7,17.899999999999999,18.3,18.7,17.8,16.2,15,13.7]
[" ","            Drybulb 10.%",21,23.8,28.2,34,39.200000000000003,41.9,42.9,42.8,39.9,35.1,28.2,23]
[" "," Coincident Wetbulb 10.%",11.5,12.4,14,16.100000000000001,17.399999999999999,17.5,18,18.5,17.399999999999999,16.100000000000001,14.5,13.3]
[]
[" ","            Drybulb 0.4%","= 0.4% Monthly Design Drybulb Temperature"]
[" "," Coincident Wetbulb 0.4%","= 0.4% Monthly Mean Coincident Wetbulb Temperature"]
[" ","            Drybulb 2.0%","= 2.0% Monthly Design Drybulb Temperature"]
[" "," Coincident Wetbulb 2.0%","= 2.0% Monthly Mean Coincident Wetbulb Temperature"]
[" ","            Drybulb 5.0%","= 5.0% Monthly Design Drybulb Temperature"]
[" "," Coincident Wetbulb 5.0%","= 5.0% Monthly Mean Coincident Wetbulb Temperature"]
[" ","            Drybulb 10.%","= 10.% Monthly Design Drybulb Temperature"]
[" "," Coincident Wetbulb 10.%","= 10.% Monthly Mean Coincident Wetbulb Temperature"]
[]
[" - Monthly Drybulb and Wetbulb Daily Ranges deltaｰC"]
[" ","                        ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","                 Drybulb",10.8,11.4,11.6,12.2,12.8,13.8,13.5,13.5,13.8,13.4,11.6,10.7]
[" ","   Drybulb range - DB 5%",14,13.7,14,14.1,14.1,14.5,14.1,13.7,14.3,14.3,13.5,13.4]
[" ","   Wetbulb range - DB 5%",6.7,6.3,5.9,5.0999999999999996,4.8,4.8,4.7,4.7,5,5.5,5.6,6]
[]
[" ","                 Drybulb",{"$f":" Mean Daily Dry Bulb Temperature Range","v":{"$error":"#NAME?"}}]
[" ","   Drybulb range - DB 5%","= Mean Daily Dry Bulb Temperature Range Coincident with 5% Design Dry Bulb Temperature"]
[" ","   Wetbulb range - DB 5%","= Mean Daily Wet Bulb Temperature Range Coincident with 5% Design Dry Bulb Temperature"]
[]
[" - Displaying Heating/Cooling Degree Days/Hours from \"Climate Design Data 2009 ASHRAE Handbook\""]
[" - Monthly Standard Heating/Cooling Degree Days/Hours"]
[" ","                    ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","       HDD base 10ｰC",3,1,0,0,0,0,0,0,0,0,0,2]
[" ","     HDD base 18.3ｰC",124,64,17,1,0,0,0,0,0,0,11,84]
[]
[" ","       CDD base 10ｰC",144,192,338,497,693,748,813,806,688,556,343,193]
[" ","     CDD base 18.3ｰC",6,22,96,247,434,498,554,548,438,298,104,18]
[]
[" ","     CDH base 23.3ｰC",68,204,903,3032,6972,8723,9899,9712,7175,3942,914,146]
[" ","     CDH base 26.7ｰC",8,47,338,1597,4657,6339,7422,7238,4891,2208,300,18]
[]
["    - 6009 annual (standard) cooling degree-days (10ｰC baseline)"]
["    -    6 annual (standard) heating degree-days (10ｰC baseline)"]
[]
["    - 3264 annual (standard) cooling degree-days (18.3ｰC baseline)"]
["    -  301 annual (standard) heating degree-days (18.3ｰC baseline)"]
[]
[" - Monthly Statistics for Dry Bulb temperatures ｰC"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","Maximum ",28,32,34,37,41,44,45.2,46,41,38,33.299999999999997,28]
[" "," Day:Hour",1.0513888888888889,1.1354166666666667,1.3027777777777778,0.88541666666666663,"19:16:00",0.6777777777777777,1.2604166666666667," 6:15"," 2:16"," 3:16"," 5:15"," 1:14"]
[]
[" ","Minimum ",4.5999999999999996,4,9,14.9,22,25.7,25.2,26.8,24.2,15.6,10,4]
[" "," Day:Hour"," 1:06"," 9:07","18:07:00"," 9:06","10:05:00",0.54583333333333328," 7:06"," 2:06","17:06:00","21:06:00",1.1284722222222221," 6:07"]
[]
[" ","Daily Avg",14,16.7,20.3,25.9,32.1,35.200000000000003,36.200000000000003,36.4,33,27.6,21.6,14.9]
[]
["   - Maximum Dry Bulb temperature of  46.0ｰC on Aug  6"]
["   - Minimum Dry Bulb temperature of   4.0ｰC on Feb  9"]
[]
[" - Monthly Statistics for Extreme Dry Bulb temperatures ｰC"]
[" ","  #Days  ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","Max >= 32","     ",1,1,20,29,30,31,31,30,21,4,"     "]
[" ","Max <=  0","     ","     ","     ","     ","     ","     ","     ","     ","     ","     ","     ","     "]
[" ","Min <=  0","     ","     ","     ","     ","     ","     ","     ","     ","     ","     ","     ","     "]
[" ","Min <=-18","     ","     ","     ","     ","     ","     ","     ","     ","     ","     ","     ","     "]
[]
[" - Monthly Statistics for Dew Point temperatures ｰC"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","Maximum ",10,18,21,18,16.600000000000001,19,12,13,18,20,13,17.2]
[" "," Day:Hour"," 7:12",1.1395833333333334,"11:18:00"," 6:19"," 1:06","15:08:00",1.1284722222222221,1.1729166666666666,"18:05:00","16:09:00"," 6:02",1.0138888888888888]
[]
[" ","Minimum ",-8,-22,-9.4,-16,-12,-20,-17,-8.8000000000000007,-9,-13,-11.9,-10]
[" "," Day:Hour"," 5:18","15:21:00",0.51041666666666663,"21:04:00","15:17:00","13:17:00"," 5:21"," 3:01",0.84027777777777779,"20:15:00",1.2506944444444443,0.67847222222222225]
[]
[" ","Daily Avg",0.9,-0.6,0.7,0.6,0.5,0.1,-3.5,-0.1,2.1,1.1000000000000001,-0.9,5.0999999999999996]
[]
["   - Maximum Dew Point temperature of  21.0ｰC on Mar 11"]
["   - Minimum Dew Point temperature of -22.0ｰC on Feb 15"]
[]
[" - Average Hourly Statistics for Dry Bulb temperatures ｰC"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",11.6,14.1,17.899999999999999,22.8,29.2,32,32.700000000000003,33,29.9,24.5,18.399999999999999,12.7]
[" "," 1:01- 2:00",11.1,13.5,17.2,22.2,28.4,31,31.8,32.1,28.9,23.8,17.5,12.3]
[" "," 2:01- 3:00",10.8,12.9,16.5,21.6,27.8,30.5,31.2,31.2,28,22.9,16.8,11.9]
[" "," 3:01- 4:00",10.3,12.3,16,20.8,27.5,29.9,30.4,30.5,27.2,22.5,16.100000000000001,11.4]
[" "," 4:01- 5:00",9.6999999999999993,11.9,15.5,20.2,26.7,29.2,30,29.9,26.8,21.7,15.3,10.9]
[" "," 5:01- 6:00",9.4,11.5,15.2,19.8,26,28.6,29.6,29.4,26.5,21.2,15.1,10.9]
[" "," 6:01- 7:00",9.4,11.5,15.2,20.8,27.1,30.2,31.1,30.8,27.6,21.7,14.9,10.7]
[" "," 7:01- 8:00",10.7,12.8,16.899999999999999,22.6,29.1,32.200000000000003,33.1,33,30.1,23.9,17.600000000000001,11.6]
[" "," 8:01- 9:00",12.2,14.4,18.100000000000001,25,30.7,34.1,35.5,35.6,32.4,26.2,20.3,13.2]
[" "," 9:01-10:00",13.8,16.100000000000001,19.7,26.9,32.4,35.799999999999997,37.6,37.9,34.4,28.3,22.5,14.9]
[" ","10:01-11:00",15.2,18,21.1,28.5,33.799999999999997,37.299999999999997,39.200000000000003,39.799999999999997,35.799999999999997,30,24.5,16.600000000000001]
[" ","11:01-12:00",16.600000000000001,19.399999999999999,22,29.7,34.9,38.6,40.200000000000003,40.9,36.799999999999997,31.4,25.9,17.8]
[" ","12:01-13:00",17.7,20.9,24,30.4,36,39.299999999999997,41,42,37.799999999999997,32.4,27.1,19]
[" ","13:01-14:00",18.600000000000001,22,24.9,31.2,36.799999999999997,40.5,41.9,42.5,38.4,33.200000000000003,27.6,19.8]
[" ","14:01-15:00",18.899999999999999,22.6,25.5,31.7,37,40.9,42.4,42.7,38.799999999999997,33.700000000000003,28.3,20.2]
[" ","15:01-16:00",19,22.4,25.7,31.3,37.1,41,42.3,42.4,38.700000000000003,33.4,27.8,19.8]
[" ","16:01-17:00",18.399999999999999,21.6,25.1,30.4,37,40.6,42,41.7,37.9,32.799999999999997,26.9,18.7]
[" ","17:01-18:00",17.399999999999999,20.6,24.4,29.6,36.299999999999997,40.1,41.2,40.799999999999997,37.299999999999997,32,25.5,18]
[" ","18:01-19:00",16.399999999999999,19.600000000000001,23.5,28.2,35.4,39,39.799999999999997,39.5,36.299999999999997,30.9,24.4,16.600000000000001]
[" ","19:01-20:00",15.3,18.3,22.1,27.3,34.1,37.6,37.799999999999997,37.9,35,29.2,23,15.6]
[" ","20:01-21:00",14.6,17.3,21.3,26.4,33,36.1,36.200000000000003,36.799999999999997,33.6,28.1,22.1,14.9]
[" ","21:01-22:00",13.8,16.3,20.399999999999999,25.5,32,34.799999999999997,34.700000000000003,35.700000000000003,32.6,27,21,14.2]
[" ","22:01-23:00",13.1,15.5,19.600000000000001,24.3,31,33.799999999999997,33.9,34.799999999999997,31.6,26.1,19.899999999999999,13.7]
[" ","23:01-24:00",12.6,14.6,18.8,23.5,30.1,32.799999999999997,33.200000000000003,33.799999999999997,30.7,25.3,19.2,12.8]
[" "," Max Hour  ",16,15,16,15,16,16,15,15,15,15,15,15]
[" "," Min Hour  ",7,7,6,6,6,6,6,6,6,6,7,7]
[]
[" - Average Hourly Statistics for Dew Point temperatures ｰC"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",1.3,0.2,0.6,1,1.4,0.7,-3.2,-0.5,2.2999999999999998,1.7,-0.9,5.5]
[" "," 1:01- 2:00",1.7,0.2,0.5,1.2,1.5,"19:12:00",-2.6,-0.7,2.6,1.8,-0.7,5.2]
[" "," 2:01- 3:00",1.2,0.4,0.6,1,1.9,1.5,-2.5,-0.4,3,2,-0.6,5.4]
[" "," 3:01- 4:00",1,0.8,1.1000000000000001,1.2,2.2000000000000002,1.5,-1.7,-0.2,3.1,2,-0.6,5.2]
[" "," 4:01- 5:00",0.9,0.7,1.3,1.6,2.4,2.2000000000000002,-2,0.3,3.4,1.9,-0.7,4.8]
[" "," 5:01- 6:00",0.9,0.7,1.5,1.9,2.6,2.5,-1.2,0.5,3.9,2,-0.4,5.0999999999999996]
[" "," 6:01- 7:00",1,0.6,1.7,1.5,2.6,2.5,-1.5,0.9,3.4,2.1,-0.5,5]
[" "," 7:01- 8:00",1,0.5,2.2000000000000002,2.2999999999999998,2.5,2.2000000000000002,-2.2000000000000002,1.2,3.2,3,0.1,5.2]
[" "," 8:01- 9:00",1.2,0.8,1.9,2.1,2,1.8,-3,1.9,2.8,3.5,0.4,5.4]
[" "," 9:01-10:00",1.2,0.2,1.6,1.6,1.1000000000000001,1.3,-2.5,1.5,2.5,3.6,0.5,6.2]
[" ","10:01-11:00",1.1000000000000001,-0.3,1.3,0.7,"12:00:00",1,-2.9,1,2.2000000000000002,2.8,"02:24:00",6.6]
[" ","11:01-12:00",0.7,-0.8,1,"07:12:00",-0.3,0.1,-3.1,"09:36:00",1.7,1.8,-0.4,6.5]
[" ","12:01-13:00",1,-1.6,0.9,0.5,-0.9,-0.6,-3.9,-0.2,1.2,1,-0.8,6.4]
[" ","13:01-14:00",0.8,-1.7,0.6,-0.5,-1,-1.1000000000000001,-4.3,"02:24:00",1.2,0.7,-0.8,6.1]
[" ","14:01-15:00",0.4,-2,-0.1,-1.6,-1.6,-2.2000000000000002,-5.3,-0.9,0.9,-1,-2.1,3.5]
[" ","15:01-16:00",0.5,-2.1,-0.2,-1.5,-1.8,-2.6,-5.9,-1.3,1.1000000000000001,-1.5,-2,4.0999999999999996]
[" ","16:01-17:00",0.2,-2.2000000000000002,-0.6,-1.5,-1.8,-2.7,-6,-1.3,1.3,-1.5,-2,3.9]
[" ","17:01-18:00",-0.2,-2.2000000000000002,0.3,-0.7,-1.5,-2.5,-5.6,-0.7,1,-1.6,-2.1,4.0999999999999996]
[" ","18:01-19:00",0.3,-1.9,-0.1,-0.2,-1.4,-2.2000000000000002,-5.0999999999999996,-0.6,1,-1.1000000000000001,-1.3,4.8]
[" ","19:01-20:00",0.5,-1.6,0.1,-0.3,-0.4,-1.3,-4.5999999999999996,-0.9,1.2,-0.4,-1.5,4.7]
[" ","20:01-21:00",0.9,-0.7,0.2,0.3,0,-0.7,-4.4000000000000004,-0.7,1.7,0.5,-1.6,5]
[" ","21:01-22:00",1,-0.9,0.2,0.5,0.1,-0.8,-4.0999999999999996,-0.7,1.4,0.6,-1.4,4.5999999999999996]
[" ","22:01-23:00",1,-0.5,0.2,0.8,0.3,-0.2,-3.8,-0.9,1.7,1.1000000000000001,-1.1000000000000001,4.9000000000000004]
[" ","23:01-24:00",1.2,-0.1,0.8,1,1.1000000000000001,"04:48:00",-3.4,-0.7,2.1,1.5,-0.8,5.3]
[" "," Max Hour  ",2,4,8,8,7,7,6,9,6,10,10,11]
[" "," Min Hour  ",18,17,17,15,16,17,17,16,15,18,15,15]
[]
[" - Monthly Statistics for Relative Humidity %"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","Maximum  ",100,89,94,78,69,44,32,28,58,84,68,100]
[" "," Day:Hour "," 8:23",1.1395833333333334,"11:18:00"," 5:08"," 1:06","15:08:00",1.1291666666666667,1.1715277777777777,"18:07:00","16:06:00"," 6:02"," 5:01"]
[]
[" ","Minimum  ",12,5,8,3,4,1,2,4,5,5,6,8]
[" "," Day:Hour ",1.0125,"15:19:00",1.0965277777777778,"14:16:00","15:15:00","13:17:00"," 9:19"," 3:13"," 4:12","10:15:00"," 3:15","16:17:00"]
[]
[" ","Daily Avg",43,34,30,24,15,12,8,11,16,21,24,57]
[]
[" - Average Hourly Relative Humidity %"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",50,40,34,27,17,14,10,12,18,25,28,65]
[" "," 1:01- 2:00",53,41,34,28,18,15,11,12,19,26,30,65]
[" "," 2:01- 3:00",53,44,35,29,20,16,12,13,21,28,32,68]
[" "," 3:01- 4:00",54,47,38,31,21,17,13,14,22,29,33,69]
[" "," 4:01- 5:00",56,47,40,32,22,18,13,15,24,30,34,69]
[" "," 5:01- 6:00",57,48,41,34,23,19,14,16,25,31,35,70]
[" "," 6:01- 7:00",57,48,42,32,22,18,12,15,23,30,36,71]
[" "," 7:01- 8:00",53,44,40,31,19,16,10,14,20,29,31,67]
[" "," 8:01- 9:00",48,41,36,27,17,14,9,13,17,26,27,63]
[" "," 9:01-10:00",43,35,33,23,15,12,8,11,15,23,24,60]
[" ","10:01-11:00",40,30,29,19,13,11,7,9,14,20,21,55]
[" ","11:01-12:00",36,26,27,18,12,10,7,8,12,17,19,52]
[" ","12:01-13:00",34,22,23,17,10,9,6,7,11,15,17,48]
[" ","13:01-14:00",32,21,22,15,10,8,5,7,10,14,16,45]
[" ","14:01-15:00",31,20,20,14,9,7,5,7,10,12,14,38]
[" ","15:01-16:00",30,20,20,15,9,7,5,7,10,12,15,40]
[" ","16:01-17:00",31,21,20,16,9,7,5,7,11,12,15,43]
[" ","17:01-18:00",32,23,23,18,9,7,5,8,11,13,16,44]
[" ","18:01-19:00",35,25,23,21,10,8,6,8,11,14,19,50]
[" ","19:01-20:00",38,28,26,21,11,9,7,9,12,16,20,53]
[" ","20:01-21:00",41,32,28,22,13,10,7,9,14,18,21,56]
[" ","21:01-22:00",43,34,29,23,13,11,8,10,14,20,23,57]
[" ","22:01-23:00",46,36,30,26,14,12,9,10,15,22,25,59]
[" ","23:01-24:00",47,38,33,26,16,13,10,11,17,23,27,64]
[" "," Max Hour  ",7,6,7,6,6,6,6,6,6,6,7,7]
[" "," Min Hour  ",16,15,16,15,16,16,16,15,15,16,15,15]
[]
[" - Monthly Indicators for Precipitation/Moisture (kPa)"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","         ",0.6,0.6,0.6,0.6,0.6,0.6,0.4,0.6,0.7,0.6,0.5,0.9]
[]
[" - Monthly Statistics for Wind Chill/Heat Index temperatures ｰC **"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","Minimum WC",0,4,"     ","     ","     ","     ","     ","     ","     ","     ","     ",-4]
[" "," Day:Hour"," 8:23","10:05:00","     ","     ","     ","     ","     ","     ","     ","     ","     "," 5:09"]
[]
[" ","Average WC",6,7,"     ","     ","     ","     ","     ","     ","     ","     ","     ",5]
[" ","Avg Del WC",3,1,"     ","     ","     ","     ","     ","     ","     ","     ","     ",2]
[" "," # Hours WC",49,29,"     ","     ","     ","     ","     ","     ","     ","     ","     ",70]
[]
[" ","Maximum HI","     ","     ","     ",27,28,36,"     ","     ",31,28,"     ","     "]
[" "," Day:Hour","     ","     ","     "," 6:10"," 1:08",0.63124999999999998,"     ","     ",0.96597222222222223,"16:11:00","     ","     "]
[]
[" ","Average HI","     ","     ","     ",27,28,33,"     ","     ",29,27,"     ","     "]
[" ","Avg Del HI","     ","     ","     ",0,0,1,"     ","     ",0,0,"     ","     "]
[" "," # Hours HI","     ","     ","     ",1,1,5,"     ","     ",12,4,"     ","     "]
[]
["   - **WindChill/HeatIndex Temps -- statistics...only those different from Air Temps"]
[]
[" - Monthly Wind Direction % {N=0 or 360,E=90,S=180,W=270}"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","North    ",38,32,32,33,35,51,48,28,49,54,59,28]
[" ","NorthEast",3,14,9,8,8,15,4,20,11,11,4,9]
[" ","East     ",5,12,4,5,8,5,1,9,11,4,5,5]
[" ","SouthEast",26,20,14,8,10,4,1,5,10,9,10,10]
[" ","South    ",6,14,25,18,20,6,1,9,9,10,17,21]
[" ","SouthWest",1,2,2,6,3,0,0,3,0,3,2,3]
[" ","West     ",1,1,4,7,4,2,2,6,1,4,2,4]
[" ","NorthWest",20,6,10,15,10,16,43,19,9,6,1,19]
[]
[" - Monthly Statistics for Wind Speed m/s"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","Maximum ",10.3,10.3,10.3,10.3,16.5,36,11.3,12.9,9.3000000000000007,10.3,6.2,11.8]
[" "," Day:Hour "," 7:17",1.1805555555555556," 1:11",1.0041666666666667,1.2506944444444443,0.55555555555555558,0.42777777777777781,1.05," 2:15",1.0034722222222221," 5:23",1.1284722222222221]
[]
[" ","Minimum ",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," Day:Hour "," 1:01"," 2:06"," 3:03"," 6:05"," 1:03"," 1:05"," 1:03"," 1:05"," 1:01"," 1:22"," 1:01"," 8:04"]
[]
[" ","Daily Avg",3,3,3.6,3.6,3,3.7,4.3,3.5,2.5,2.2000000000000002,1.1000000000000001,2.8]
[]
["   - Maximum Wind Speed of  36.0 m/s on Jun 13"]
["   - Minimum Wind Speed of   0.0 m/s on Jan  1"]
[]
[" - Average Hourly Statistics for Wind Speed m/s"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",2.1,2.5,3,2.7,2.5,2.2999999999999998,3.2,2.6,1.5,1.4,0.3,2.1]
[" "," 1:01- 2:00",1.8,2.6,2.5,2.8,2.1,1.8,2.5,2.8,1.2,1,0.4,2.1]
[" "," 2:01- 3:00",1.9,2.4,2.5,3,2.2000000000000002,1.7,2.2000000000000002,2.4,0.9,1.1000000000000001,0.4,2.1]
[" "," 3:01- 4:00",1.6,2,2.4,2.9,2.2000000000000002,1.8,2.2999999999999998,2.2999999999999998,1.1000000000000001,0.8,0.4,2.2000000000000002]
[" "," 4:01- 5:00",1.7,2,2.2999999999999998,3,2,1.1000000000000001,2.2999999999999998,2.4,1,1.3,0.3,2.2000000000000002]
[" "," 5:01- 6:00",2,2,2,3,1.8,0.7,2.4,2.5,0.7,0.8,0.2,2.1]
[" "," 6:01- 7:00",1.9,2.2999999999999998,2.2000000000000002,3,2.1,1.6,2.5,2.6,0.8,1.1000000000000001,0.3,2]
[" "," 7:01- 8:00",2,2,3,3.3,2.5,2.8,3.5,2.8,1.3,1.6,0.7,2.6]
[" "," 8:01- 9:00",2.5,2.7,3.6,3.6,3.3,3.8,4.4000000000000004,3.4,1.8,2.5,0.8,2.9]
[" "," 9:01-10:00",3.8,3.2,3.9,4.4000000000000004,3.7,4.2,5.6,3.9,2.6,3.3,1.3,3.2]
[" ","10:01-11:00",4.4000000000000004,3,4.2,4.2,3.7,4.3,6,3.8,3.1,3.3,1.6,3.1]
[" ","11:01-12:00",4.5999999999999996,3.1,4.4000000000000004,4,3.8,5,6.1,4,3.1,3,1.9,3.6]
[" ","12:01-13:00",4.5999999999999996,2.9,4.5,4.0999999999999996,3.5,4,5.5,4.2,3.3,2.8,1.7,3.7]
[" ","13:01-14:00",4.4000000000000004,3.6,4.5,4,3.2,5.0999999999999996,5.7,4.2,3.6,3.1,1.7,3.6]
[" ","14:01-15:00",4.0999999999999996,3.4,4.4000000000000004,3.7,3.3,5.7,6.4,4.9000000000000004,3.6,3.3,2.1,3.7]
[" ","15:01-16:00",4,3.5,4.5999999999999996,4.2,3.1,5.6,6.5,4.4000000000000004,4,2.9,2,3.5]
[" ","16:01-17:00",4,3.5,4.3,4.3,3.3,6.4,6.3,4.9000000000000004,4,3,2.1,3.6]
[" ","17:01-18:00",3.7,3.5,4.3,4.5,4.0999999999999996,5.8,6.6,4.5999999999999996,3.7,2.6,1.6,3.2]
[" ","18:01-19:00",3.1,3.8,4.3,4.2,4.0999999999999996,6.6,5.6,3.9,3.3,2.2000000000000002,1.4,2.9]
[" ","19:01-20:00",3.1,4.3,4,4.3,3.7,5.6,3.9,3.7,3.5,2.2999999999999998,1.2,2.7]
[" ","20:01-21:00",2.9,4.0999999999999996,4,4.0999999999999996,3.4,4.0999999999999996,3.7,3.3,3.5,2.5,1.4,2.7]
[" ","21:01-22:00",2.6,4,3.9,3.9,3.9,4.0999999999999996,3.2,3.1,3,2.2999999999999998,1.2,2.7]
[" ","22:01-23:00",2.2000000000000002,3.3,3.5,3.1,3,3.1,3,3.2,2.6,1.8,0.9,2.6]
[" ","23:01-24:00",2.2999999999999998,3,3.2,2.8,2.7,2.5,2.8,3.1,2.1,1.7,0.8,2.2999999999999998]
[" "," Max Hour  ",12,20,16,18,18,19,18,17,16,11,15,13]
[" "," Min Hour  ",4,4,6,1,6,6,3,4,6,6,6,7]
[]
[" - Average Hourly Statistics for Wind Direction ｰ {N=0 or 360,E=90,S=180,W=270}"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",144,135,135,193,119,137,248,204,54,80,41,158]
[" "," 1:01- 2:00",119,124,123,170,142,96,226,215,58,55,37,195]
[" "," 2:01- 3:00",144,142,123,207,143,131,173,194,51,52,29,183]
[" "," 3:01- 4:00",132,132,162,217,126,123,206,190,90,67,32,175]
[" "," 4:01- 5:00",111,131,107,219,117,113,218,196,86,75,16,166]
[" "," 5:01- 6:00",116,163,136,229,104,75,251,261,74,63,9,167]
[" "," 6:01- 7:00",137,146,139,229,142,140,251,250,99,86,29,147]
[" "," 7:01- 8:00",121,176,171,224,174,191,302,268,122,100,57,213]
[" "," 8:01- 9:00",153,156,154,205,181,225,319,204,134,152,59,215]
[" "," 9:01-10:00",176,196,142,196,175,206,274,172,114,151,114,207]
[" ","10:01-11:00",210,181,132,191,158,203,225,139,129,166,138,167]
[" ","11:01-12:00",195,147,173,189,188,206,249,179,160,151,132,176]
[" ","12:01-13:00",182,148,182,207,183,159,230,164,173,165,127,171]
[" ","13:01-14:00",182,168,198,196,165,167,239,141,163,159,126,192]
[" ","14:01-15:00",162,132,178,191,138,188,283,170,179,139,126,184]
[" ","15:01-16:00",194,116,192,206,145,177,294,153,171,151,101,184]
[" ","16:01-17:00",186,158,183,189,171,193,290,151,176,130,102,165]
[" ","17:01-18:00",199,130,142,182,156,186,277,116,173,101,81,137]
[" ","18:01-19:00",170,153,140,153,163,200,269,104,160,100,79,149]
[" ","19:01-20:00",195,137,126,106,138,190,249,112,141,90,64,144]
[" ","20:01-21:00",155,134,127,98,156,213,260,154,99,92,66,117]
[" ","21:01-22:00",159,130,135,109,158,173,245,118,83,92,53,104]
[" ","22:01-23:00",124,117,117,148,117,174,279,110,102,64,39,185]
[" ","23:01-24:00",152,131,128,151,131,133,258,151,57,63,33,176]
[" "," Max Hour  ",11,10,14,6,12,9,9,8,15,11,11,9]
[" "," Min Hour  ",5,16,5,21,6,6,3,19,3,3,6,22]
[]
[" - Monthly Statistics for Solar Radiation  (Direct Normal, Diffuse, Global Horizontal) Wh/mｲ"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","Direct Avg ",5652,5601,5502,5428,6330,7613,7049,6879,6970,7264,5595,4592]
[]
[" ","Direct Max ",8146,8663,8302,8525,8415,8260,7912,7975,7616,7428,6221,7665]
[" ","    Day    ",26,15,29,13,1,2,7,9,8,6,3,31]
[]
[" ","Diffuse Avg",1314,1711,1982,2362,2378,1962,2164,2017,1719,1249,1357,1236]
[]
[" ","Global Avg ",4276,5061,5769,6411,7337,8033,7815,7433,6888,5992,4706,3596]
["   - Maximum Direct Normal Solar of  8663 Wh/mｲ on Feb 15"]
[]
[" - Average Hourly Statistics for Direct Normal Solar Radiation Wh/mｲ"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 1:01- 2:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 2:01- 3:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 3:01- 4:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 4:01- 5:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 5:01- 6:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 6:01- 7:00",0,0,27,155,174,196,207,131,105,85,0,0]
[" "," 7:01- 8:00",330,296,258,396,405,500,395,374,402,437,225,229]
[" "," 8:01- 9:00",518,465,457,510,524,648,591,589,650,700,504,391]
[" "," 9:01-10:00",636,558,550,595,629,763,725,722,789,823,662,485]
[" ","10:01-11:00",677,593,607,625,719,874,843,827,854,900,771,542]
[" ","11:01-12:00",671,610,626,605,711,881,868,862,886,918,840,572]
[" ","12:01-13:00",676,653,676,596,716,883,854,854,876,921,835,604]
[" ","13:01-14:00",657,674,657,579,730,860,823,811,822,900,766,610]
[" ","14:01-15:00",598,684,620,547,658,776,683,708,725,785,620,571]
[" ","15:01-16:00",553,617,579,454,600,664,587,577,558,573,343,446]
[" ","16:01-17:00",335,418,390,302,365,435,367,343,295,222,30,141]
[" ","17:01-18:00",0,33,55,65,99,134,107,82,9,0,0,0]
[" ","18:01-19:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","19:01-20:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","20:01-21:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","21:01-22:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","22:01-23:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","23:01-24:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," Max Hour*","  11*",15,13,"  11*",14,13,12,12,12,13,12,14]
[" "," Min Hour  ",1,1,1,1,1,1,1,1,1,1,1,1]
[]
[" - Average Hourly Statistics for Diffuse Horizontal Solar Radiation Wh/mｲ"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 1:01- 2:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 2:01- 3:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 3:01- 4:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 4:01- 5:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 5:01- 6:00",0,0,0,6,16,20,12,6,3,0,0,0]
[" "," 6:01- 7:00",5,12,31,79,115,126,88,84,73,52,20,8]
[" "," 7:01- 8:00",55,83,127,153,179,169,185,176,162,132,119,66]
[" "," 8:01- 9:00",109,141,177,210,228,202,212,204,174,138,161,106]
[" "," 9:01-10:00",136,186,219,238,246,200,218,208,169,137,179,147]
[" ","10:01-11:00",158,222,226,260,226,148,175,177,164,122,166,170]
[" ","11:01-12:00",180,237,253,283,259,163,174,171,153,126,137,174]
[" ","12:01-13:00",184,234,242,284,255,160,183,176,154,117,130,172]
[" ","13:01-14:00",172,211,223,260,219,153,176,179,166,102,135,149]
[" ","14:01-15:00",150,161,196,216,220,169,228,194,172,119,139,117]
[" ","15:01-16:00",101,121,139,188,176,168,205,192,170,122,128,86]
[" ","16:01-17:00",57,83,110,135,157,167,189,169,127,76,43,39]
[" ","17:01-18:00",7,21,38,52,77,105,106,77,30,6,0,0]
[" ","18:01-19:00",0,0,0,1,5,11,11,4,0,0,0,0]
[" ","19:01-20:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","20:01-21:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","21:01-22:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","22:01-23:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","23:01-24:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," Max Hour*",13,12,12,13,12,"   9*",15,"  10*","   9*","   9*","  10*",12]
[" "," Min Hour  ",1,1,1,1,1,1,1,1,1,1,1,1]
[]
[" - Average Hourly Statistics for Global Horizontal Solar Radiation Wh/mｲ"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 1:01- 2:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 2:01- 3:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 3:01- 4:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 4:01- 5:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," 5:01- 6:00",0,0,0,6,16,20,12,6,3,0,0,0]
[" "," 6:01- 7:00",5,12,34,112,164,185,144,114,93,64,20,8]
[" "," 7:01- 8:00",112,148,211,327,382,422,375,344,328,287,182,111]
[" "," 8:01- 9:00",298,339,418,536,588,651,609,584,572,520,393,255]
[" "," 9:01-10:00",468,518,603,713,774,841,817,789,775,709,577,403]
[" ","10:01-11:00",589,649,722,827,904,974,964,936,913,835,702,509]
[" ","11:01-12:00",647,717,804,863,963,1040,1035,1011,974,889,752,558]
[" ","12:01-13:00",655,751,839,851,956,1033,1028,1006,956,862,724,571]
[" ","13:01-14:00",594,708,764,772,885,950,943,917,858,757,619,511]
[" ","14:01-15:00",469,590,636,633,740,799,787,756,689,584,450,388]
[" ","15:01-16:00",311,410,454,457,551,602,594,555,471,358,241,225]
[" ","16:01-17:00",121,196,242,252,312,368,362,316,224,121,47,56]
[" ","17:01-18:00",7,24,44,62,97,138,134,94,32,6,0,0]
[" ","18:01-19:00",0,0,0,1,5,11,11,4,0,0,0,0]
[" ","19:01-20:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","20:01-21:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","21:01-22:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","22:01-23:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","23:01-24:00",0,0,0,0,0,0,0,0,0,0,0,0]
[" "," Max Hour  ",13,13,13,12,12,12,12,12,12,12,12,13]
[" "," Min Hour  ",1,1,1,1,1,1,1,1,1,1,1,1]
[]
[" - Average Hourly Statistics for Total Sky Cover %"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",19,24,32,21,18,4,11,15,8,0,3,31]
[" "," 1:01- 2:00",18,26,31,21,20,4,11,15,8,0,4,31]
[" "," 2:01- 3:00",18,29,29,23,20,3,12,15,7,0,5,32]
[" "," 3:01- 4:00",17,28,34,24,25,6,15,17,8,0,6,32]
[" "," 4:01- 5:00",17,29,36,26,27,10,16,20,9,0,6,34]
[" "," 5:01- 6:00",17,27,36,27,34,12,17,24,10,0,7,34]
[" "," 6:01- 7:00",21,32,39,28,33,11,15,21,10,2,9,39]
[" "," 7:01- 8:00",25,36,39,29,33,10,13,18,9,2,7,43]
[" "," 8:01- 9:00",30,40,38,29,31,8,11,16,8,2,8,48]
[" "," 9:01-10:00",30,39,37,32,30,8,10,15,8,2,8,46]
[" ","10:01-11:00",31,38,38,34,27,8,10,13,8,2,7,43]
[" ","11:01-12:00",32,38,37,37,26,7,8,11,9,1,7,41]
[" ","12:01-13:00",33,34,35,37,28,9,11,14,12,1,8,39]
[" ","13:01-14:00",33,32,35,39,30,10,14,15,14,1,10,37]
[" ","14:01-15:00",33,29,34,39,30,11,16,16,15,1,10,34]
[" ","15:01-16:00",32,33,34,40,28,11,16,19,17,2,9,36]
[" ","16:01-17:00",31,36,33,41,31,12,17,23,18,2,9,37]
[" ","17:01-18:00",30,39,31,42,31,12,17,25,20,2,8,38]
[" ","18:01-19:00",23,37,32,39,26,9,15,25,17,2,8,35]
[" ","19:01-20:00",18,33,32,35,26,6,12,24,13,3,5,34]
[" ","20:01-21:00",13,29,32,33,25,4,9,22,9,3,3,30]
[" ","21:01-22:00",15,26,32,29,23,4,9,20,8,2,3,30]
[" ","22:01-23:00",17,23,33,26,20,4,11,20,8,1,2,30]
[" ","23:01-24:00",18,19,33,22,18,5,10,17,8,0,2,29]
[" "," Max Hour  ",15,9,7,18,6,6,17,18,18,21,15,9]
[" "," Min Hour  ",21,24,3,1,24,3,12,12,3,1,23,24]
[]
[" - Average Hourly Statistics for Opaque Sky Cover %"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" "," 0:01- 1:00",11,18,19,15,14,3,8,13,5,0,1,19]
[" "," 1:01- 2:00",11,20,20,15,15,2,9,13,5,0,3,17]
[" "," 2:01- 3:00",12,22,21,15,15,1,10,13,5,0,4,15]
[" "," 3:01- 4:00",10,22,23,15,17,2,10,13,6,0,4,18]
[" "," 4:01- 5:00",9,22,24,14,18,3,10,14,6,0,4,21]
[" "," 5:01- 6:00",8,23,24,13,21,4,10,15,6,0,4,22]
[" "," 6:01- 7:00",9,23,24,14,18,5,9,14,6,1,4,24]
[" "," 7:01- 8:00",10,22,23,15,16,5,7,11,5,1,2,23]
[" "," 8:01- 9:00",10,21,22,17,12,5,6,10,4,2,2,24]
[" "," 9:01-10:00",11,23,22,18,12,5,5,8,4,2,2,22]
[" ","10:01-11:00",12,24,23,20,11,5,4,7,4,1,2,20]
[" ","11:01-12:00",11,25,21,20,9,4,3,4,4,1,2,17]
[" ","12:01-13:00",13,22,21,21,15,5,5,7,6,1,2,17]
[" ","13:01-14:00",14,20,21,23,19,5,6,9,9,1,2,17]
[" ","14:01-15:00",14,17,20,23,22,5,7,11,9,1,2,16]
[" ","15:01-16:00",12,20,19,23,22,6,8,12,10,2,2,15]
[" ","16:01-17:00",11,22,19,22,23,6,9,14,10,2,2,15]
[" ","17:01-18:00",9,24,15,22,22,6,9,15,11,2,2,14]
[" ","18:01-19:00",7,20,18,22,21,5,9,13,10,2,1,14]
[" ","19:01-20:00",7,17,19,20,19,4,8,13,8,2,1,15]
[" ","20:01-21:00",5,13,20,19,18,3,7,11,6,2,0,15]
[" ","21:01-22:00",7,13,19,18,16,3,7,12,6,2,0,16]
[" ","22:01-23:00",8,13,18,18,15,3,8,13,6,1,0,18]
[" ","23:01-24:00",10,13,18,17,13,3,8,13,5,0,0,19]
[" "," Max Hour  ",14,12,6,16,17,17,4,6,18,20,3,9]
[" "," Min Hour  ",21,24,18,6,12,3,12,12,10,1,21,18]
[]
[" - Monthly Calculated \"undisturbed\" Ground Temperatures** ｰC"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","   0.5 m  ",20.399999999999999,17,16,16.8,21.5,26.7,31.7,35.200000000000003,36.299999999999997,34.6,30.6,25.5]
[" ","   2.0 m  ",23.5,20.3,18.7,18.7,21.2,24.7,28.6,31.9,33.6,33.299999999999997,31,27.5]
[" ","   4.0 m  ",25.6,23,21.5,21,21.9,24,26.6,29.2,30.9,31.3,30.3,28.3]
[]
["   - **These ground temperatures should NOT BE USED in the GroundTemperatures object to compute building floor losses."]
["   -   The temperatures for 0.5 m depth can be used for GroundTemperatures:Surface."]
["   -   The temperatures for 4.0 m depth can be used for GroundTemperatures:Deep."]
["   -   Calculations use a standard soil diffusivity of 2.3225760E-03 {m**2/day}"]
[]
[" - Heating/Cooling Degree Days/Hours calculated from this weather file."]
[" - Heating/Cooling Degree Days/Hours from design conditions shown earlier in this report."]
[" - Monthly Weather File Heating/Cooling Degree Days/Hours"]
[" ","           ","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[" ","HDD base 10C",0,0,0,0,0,0,0,0,0,0,0,0]
[" ","HDD base 18C",127,59,12,0,0,0,0,0,0,0,0,107]
[]
[" ","CDD base 10C",125,187,319,476,684,757,812,820,691,545,347,153]
[" ","CDD base 18C",4,22,83,236,436,517,564,572,451,297,108,12]
[]
[" ","CDH base 20C",152,558,1532,4357,8969,10970,12060,12232,9391,5730,2145,370]
[" ","CDH base 23C",45,212,665,2690,6741,8810,9828,10000,7231,3803,1049,123]
[" ","CDH base 27C",2,33,148,1171,3992,5936,6854,7025,4415,1822,235,5]
[]
["    - 5915 annual (wthr file) cooling degree-days (10ｰC baseline)"]
["    -    0 annual (wthr file) heating degree-days (10ｰC baseline)"]
[]
["    - 3301 annual (wthr file) cooling degree-days (18ｰC baseline)"]
["    -  305 annual (wthr file) heating degree-days (18ｰC baseline)"]
[]
[" - Climate type \"BWh\" (Kpen classification)**"]
[" - Subtropical hot desert (lat. 15-25ｰN)"]
[" - Unbearably hot dry periods in summer, but passive cooling is possible"]
[" - **Note that the Kpen classification shown here is derived algorithmically from the source weather data."]
[" -   It may not be indicative of the long term climate for this location."]
[]
[" - Climate type \"1B\" (ASHRAE Standards 90.1-2004 and 90.2-2004 Climate Zone)**"]
[" - Very Hot - Dry, Probable Kpen classification=Bw, Arid Tropical Dry"]
[" - **Note that the ASHRAE classification shown here is derived algorithmically from the source weather data."]
[" -   It may not be indicative of the long term climate for this location."]
[]
[" - Typical/Extreme Period Determination"]
[]
[" - Summer is Jun:Aug"]
["     Extreme Summer Week (nearest maximum temperature for summer)"]
["     Extreme Hot Week Period selected: Jul 20:Jul 26, Maximum Temp=  46.00ｰC, Deviation=| 8.571|ｰC"]
["     Typical Summer Week (nearest average temperature for summer)"]
["     Typical Week Period selected: Jun 15:Jun 21, Average Temp=  35.97ｰC, Deviation=| 0.033|ｰC"]
[]
[" - Winter is Dec:Feb"]
["     Extreme Winter Week (nearest minimum temperature for winter)"]
["     Extreme Cold Week Period selected: Dec 22:Jan  5, Minimum Temp=   4.00ｰC, Deviation=| 7.454|ｰC"]
["     Typical Winter Week (nearest average temperature for winter)"]
["     Typical Week Period selected: Feb  3:Feb  9, Average Temp=  15.16ｰC, Deviation=| 0.103|ｰC"]
[]
[" - Autumn is Sep:Nov"]
["     Typical Autumn Week (nearest average temperature for autumn)"]
["     Typical Week Period selected: Oct 13:Oct 19, Average Temp=  27.40ｰC, Deviation=| 0.187|ｰC"]
[]
[" - Spring is Mar:May"]
["     Typical Spring Week (nearest average temperature for spring)"]
["     Typical Week Period selected: Mar 29:Apr  4, Average Temp=  26.07ｰC, Deviation=| 0.063|ｰC"]

{"sheet":"Operative BP","index":3,"n_rows":360,"n_cols":153,"rows_kept":360,"cut":false,"hidden":false,"merged":[[1,29,1,36],[1,4,1,28],[109,41,109,53],[109,55,109,67],[55,41,55,53],[82,41,82,53],[55,55,55,67],[82,55,82,67],[1,38,1,39],[2,3,2,13],[41,15,41,16],[48,15,48,16],[28,1,28,13],[27,15,27,16],[15,27,16,34],[15,35,16,36],[333,1,333,13],[109,1,109,13],[135,1,135,13],[304,1,304,13],[82,1,82,13],[246,1,246,13],[275,1,275,13],[217,1,217,13],[189,1,189,13],[164,1,164,13],[136,41,136,53],[136,55,136,67],[53,22,54,37],[2,55,2,67],[30,32,30,34],[4,24,4,26],[9,33,9,34],[21,24,21,26],[22,28,22,31],[26,33,26,34],[28,33,28,34],[24,22,34,22],[2,23,2,36],[7,22,17,22],[11,33,11,34],[19,23,19,36],[55,1,55,13],[52,27,52,29],[49,35,50,36],[32,27,33,34],[49,27,50,34],[34,15,34,16],[29,41,29,53],[29,55,29,67],[41,22,51,22],[28,55,28,67],[47,32,47,34],[28,41,28,53],[35,27,35,29],[36,23,36,36],[38,24,38,26],[39,28,39,31],[43,33,43,34],[45,33,45,34],[32,35,33,36],[2,41,2,53],[18,27,18,29],[5,28,5,31],[13,32,13,34],[28,69,28,81],[29,83,29,95],[2,69,2,81],[28,83,28,95],[2,140,2,152],[29,126,29,138],[29,140,29,152],[2,111,2,123],[2,126,2,138],[2,83,2,95],[29,69,29,81],[1,97,1,117],[1,118,1,122],[28,97,28,109],[28,111,28,123],[29,97,29,109],[29,111,29,123],[2,97,2,109]]}
[]
[null,null,null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"~ Solar Analysis",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Shading Coefficents from Overhang Projections",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Add Verticals?",null,null,null,null,null,true]
[null,null,null,"Chhaya - Heating & Cooling Season",null,null,null,null,null,null,null,null,null,null,null,30,"Building E-W axis",null,null,null,null,null,null,"SOUTH WINDOW SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI3","v":"South Transmitted"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BW3","v":"East Transmitted"},null,null,null,null,null,null,null,null,null,null,null,null,null,"South Profile",null,null,null,null,null,null,null,null,null,null,null,null,null,"East Profile",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($P$17>45,\"East SC\",\"South SC\")","v":"South SC"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($P$17>45,\"North SC\",\"EastSC\")","v":"EastSC"},null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(DU2,1,0)","v":1},null,{"$f":"'Profile angles'!AR3","v":"Altitude"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"DW3","v":"Altitude"}]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"  (N& S Façade)",null,null,null,null,null,null,7,null,null,0,1,2,3,4,5,6,7,8,9,10,null,null,null,null,{"$f":"'Incident angle'!BI4","v":0},{"$f":"'Incident angle'!BJ4","v":"Jan"},{"$f":"'Incident angle'!BK4","v":"Feb"},{"$f":"'Incident angle'!BL4","v":"Mar"},{"$f":"'Incident angle'!BM4","v":"Apr"},{"$f":"'Incident angle'!BN4","v":"May"},{"$f":"'Incident angle'!BO4","v":"Jun"},{"$f":"'Incident angle'!BP4","v":"Jul"},{"$f":"'Incident angle'!BQ4","v":"Aug"},{"$f":"'Incident angle'!BR4","v":"Sep"},{"$f":"'Incident angle'!BS4","v":"Oct"},{"$f":"'Incident angle'!BT4","v":"Nov"},{"$f":"'Incident angle'!BU4","v":"Dec"},"Average",{"$f":"'Incident angle'!BW4","v":0},{"$f":"'Incident angle'!BX4","v":"Jan"},{"$f":"'Incident angle'!BY4","v":"Feb"},{"$f":"'Incident angle'!BZ4","v":"Mar"},{"$f":"'Incident angle'!CA4","v":"Apr"},{"$f":"'Incident angle'!CB4","v":"May"},{"$f":"'Incident angle'!CC4","v":"Jun"},{"$f":"'Incident angle'!CD4","v":"Jul"},{"$f":"'Incident angle'!CE4","v":"Aug"},{"$f":"'Incident angle'!CF4","v":"Sep"},{"$f":"'Incident angle'!CG4","v":"Oct"},{"$f":"'Incident angle'!CH4","v":"Nov"},{"$f":"'Incident angle'!CI4","v":"Dec"},"Average",{"$f":"'Profile angles'!B4","v":"HR"},{"$f":"'Profile angles'!C4","v":"Jan"},{"$f":"'Profile angles'!D4","v":"Feb"},{"$f":"'Profile angles'!E4","v":"Mar"},{"$f":"'Profile angles'!F4","v":"Apr"},{"$f":"'Profile angles'!G4","v":"May"},{"$f":"'Profile angles'!H4","v":"Jun"},{"$f":"'Profile angles'!I4","v":"Jul"},{"$f":"'Profile angles'!J4","v":"Aug"},{"$f":"'Profile angles'!K4","v":"Sep"},{"$f":"'Profile angles'!L4","v":"Oct"},{"$f":"'Profile angles'!M4","v":"Nov"},{"$f":"'Profile angles'!N4","v":"Dec"},{"$f":"TAN(BS5)","v":12.725208596609132},{"$f":"'Profile angles'!B33","v":"HR"},{"$f":"'Profile angles'!C33","v":"Jan"},{"$f":"'Profile angles'!D33","v":"Feb"},{"$f":"'Profile angles'!E33","v":"Mar"},{"$f":"'Profile angles'!F33","v":"Apr"},{"$f":"'Profile angles'!G33","v":"May"},{"$f":"'Profile angles'!H33","v":"Jun"},{"$f":"'Profile angles'!I33","v":"Jul"},{"$f":"'Profile angles'!J33","v":"Aug"},{"$f":"'Profile angles'!K33","v":"Sep"},{"$f":"'Profile angles'!L33","v":"Oct"},{"$f":"'Profile angles'!M33","v":"Nov"},{"$f":"'Profile angles'!N33","v":"Dec"},null,{"$f":"'Profile angles'!AD4","v":"HR"},{"$f":"'Profile angles'!AE4","v":"Jan"},{"$f":"'Profile angles'!AF4","v":"Feb"},{"$f":"'Profile angles'!AG4","v":"Mar"},{"$f":"'Profile angles'!AH4","v":"Apr"},{"$f":"'Profile angles'!AI4","v":"May"},{"$f":"'Profile angles'!AJ4","v":"Jun"},{"$f":"'Profile angles'!AK4","v":"Jul"},{"$f":"'Profile angles'!AL4","v":"Aug"},{"$f":"'Profile angles'!AM4","v":"Sep"},{"$f":"'Profile angles'!AN4","v":"Oct"},{"$f":"'Profile angles'!AO4","v":"Nov"},{"$f":"'Profile angles'!AP4","v":"Dec"},null,{"$f":"CT4","v":"HR"},{"$f":"CU4","v":"Jan"},"Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,{"$f":"'Profile angles'!AR4","v":0},{"$f":"'Profile angles'!AS4","v":"Jan"},{"$f":"'Profile angles'!AT4","v":"Feb"},{"$f":"'Profile angles'!AU4","v":"Mar"},{"$f":"'Profile angles'!AV4","v":"Apr"},{"$f":"'Profile angles'!AW4","v":"May"},{"$f":"'Profile angles'!AX4","v":"Jun"},{"$f":"'Profile angles'!AY4","v":"Jul"},{"$f":"'Profile angles'!AZ4","v":"Aug"},{"$f":"'Profile angles'!BA4","v":"Sep"},{"$f":"'Profile angles'!BB4","v":"Oct"},{"$f":"'Profile angles'!BC4","v":"Nov"},{"$f":"'Profile angles'!BD4","v":"Dec"}]
[null,1,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D5-C336,'Dry Bulb'!D5-C220)","v":-10.0991932059448},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E5-D336,'Dry Bulb'!E5-D220)","v":-5.5991932059448004},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F5-E336,'Dry Bulb'!F5-E220)","v":-5.759193205944797},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G5-F336,'Dry Bulb'!G5-F220)","v":2.6105560934182677},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H5-G336,'Dry Bulb'!H5-G220)","v":14.580806794055206},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I5-H336,'Dry Bulb'!I5-H220)","v":19.620806794055198},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J5-I336,'Dry Bulb'!J5-I220)","v":20.880806794055204},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K5-J336,'Dry Bulb'!K5-J220)","v":21.42080679405521},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L5-K336,'Dry Bulb'!L5-K220)","v":15.840806794055197},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M5-L336,'Dry Bulb'!M5-L220)","v":6.3734985138004134},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N5-M336,'Dry Bulb'!N5-M220)","v":-7.1288242887473388},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O5-N336,'Dry Bulb'!O5-N220)","v":-8.1191932059447964},null,null,null,"`",null,null,null,null,null,{"$f":"X4*AC10","v":7},"HEAD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI5","v":1},{"$f":"'Incident angle'!BJ5","v":0},{"$f":"'Incident angle'!BK5","v":0},{"$f":"'Incident angle'!BL5","v":0},{"$f":"'Incident angle'!BM5","v":0},{"$f":"'Incident angle'!BN5","v":0},{"$f":"'Incident angle'!BO5","v":0},{"$f":"'Incident angle'!BP5","v":0},{"$f":"'Incident angle'!BQ5","v":0},{"$f":"'Incident angle'!BR5","v":0},{"$f":"'Incident angle'!BS5","v":0},{"$f":"'Incident angle'!BT5","v":0},{"$f":"'Incident angle'!BU5","v":0},{"$f":"AVERAGEIF(AS5:AZ28,\">0\")","v":319.33993181030093},{"$f":"'Incident angle'!BW5","v":1},{"$f":"'Incident angle'!BX5","v":0},{"$f":"'Incident angle'!BY5","v":0},{"$f":"'Incident angle'!BZ5","v":0},{"$f":"'Incident angle'!CA5","v":0},{"$f":"'Incident angle'!CB5","v":0},{"$f":"'Incident angle'!CC5","v":0},{"$f":"'Incident angle'!CD5","v":0},{"$f":"'Incident angle'!CE5","v":0},{"$f":"'Incident angle'!CF5","v":0},{"$f":"'Incident angle'!CG5","v":0},{"$f":"'Incident angle'!CH5","v":0},{"$f":"'Incident angle'!CI5","v":0},{"$f":"AVERAGEIF(BG5:BN28,\">0\")","v":1847.4417930601708},{"$f":"'Profile angles'!B5","v":1},{"$f":"RADIANS('Profile angles'!C5)","v":1.492373321351995},{"$f":"RADIANS('Profile angles'!D5)","v":1.327348921355314},{"$f":"RADIANS('Profile angles'!E5)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!F5)","v":0.92628661869809481},{"$f":"RADIANS('Profile angles'!G5)","v":0.77541332917766936},{"$f":"RADIANS('Profile angles'!H5)","v":0.72105580791449653},{"$f":"RADIANS('Profile angles'!I5)","v":0.77500562596203504},{"$f":"RADIANS('Profile angles'!J5)","v":0.92344909928942365},{"$f":"RADIANS('Profile angles'!K5)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L5)","v":1.3348406596171152},{"$f":"RADIANS('Profile angles'!M5)","v":1.500983956115769},{"$f":"RADIANS('Profile angles'!N5)","v":1.5594894508681831},{"$f":"TAN(BS6)","v":20.018720868577262},{"$f":"'Profile angles'!B34","v":1},{"$f":"RADIANS('Profile angles'!C34)","v":-1.3994410384001574},{"$f":"RADIANS('Profile angles'!D34)","v":-1.3987224426302709},{"$f":"RADIANS('Profile angles'!E34)","v":-1.3535067192060628},{"$f":"RADIANS('Profile angles'!F34)","v":-1.2854751008998169},{"$f":"RADIANS('Profile angles'!G34)","v":-1.2485940409284233},{"$f":"RADIANS('Profile angles'!H34)","v":-1.2646212293363484},{"$f":"RADIANS('Profile angles'!I34)","v":-1.3017917625848774},{"$f":"RADIANS('Profile angles'!J34)","v":-1.3032988016081293},{"$f":"RADIANS('Profile angles'!K34)","v":-1.2822582122157415},{"$f":"RADIANS('Profile angles'!L34)","v":-1.2704099409257712},{"$f":"RADIANS('Profile angles'!M34)","v":-1.2971040377011409},{"$f":"RADIANS('Profile angles'!N34)","v":-1.3530868681716333},null,{"$f":"'Profile angles'!AD5","v":1},{"$f":"(IF($AH$12<DEGREES(BS5),0+$AJ$16,1-((TAN(BS5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT5),0+$AJ$16,1-((TAN(BT5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU5),0+$AJ$16,1-((TAN(BU5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV5),0+$AJ$16,1-((TAN(BV5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA4*$DU$3)+1-$DU$3)","v":5.5233727199850549E-2},{"$f":"(IF($AH$12<DEGREES(BW5),0+$AJ$16,1-((TAN(BW5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB4*$DU$3)+1-$DU$3)","v":0.262491230859765},{"$f":"(IF($AH$12<DEGREES(BX5),0+$AJ$16,1-((TAN(BX5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC4*$DU$3)+1-$DU$3)","v":0.33129399917539931},{"$f":"(IF($AH$12<DEGREES(BY5),0+$AJ$16,1-((TAN(BY5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD4*$DU$3)+1-$DU$3)","v":0.2719539504249272},{"$f":"(IF($AH$12<DEGREES(BZ5),0+$AJ$16,1-((TAN(BZ5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE4*$DU$3)+1-$DU$3)","v":6.0674900522505418E-2},{"$f":"(IF($AH$12<DEGREES(CA5),0+$AJ$16,1-((TAN(CA5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB5),0+$AJ$16,1-((TAN(CB5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC5),0+$AJ$16,1-((TAN(CC5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD5),0+$AJ$16,1-((TAN(CD5)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI4*$DU$3)+1-$DU$3)","v":0},null,{"$f":"CT5","v":1},{"$f":"(IF($AH$46<DEGREES(CG5),0+$AJ$50,1-((TAN(CG5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL4*$DU$3)+1-$DU$3)","v":3.4528760738015651},{"$f":"(IF($AH$46<DEGREES(CH5),0+$AJ$50,1-((TAN(CH5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM4*$DU$3)+1-$DU$3)","v":1.2708494794636043},{"$f":"(IF($AH$46<DEGREES(CI5),0+$AJ$50,1-((TAN(CI5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CJ5),0+$AJ$50,1-((TAN(CJ5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CK5),0+$AJ$50,1-((TAN(CK5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CL5),0+$AJ$50,1-((TAN(CL5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CM5),0+$AJ$50,1-((TAN(CM5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CN5),0+$AJ$50,1-((TAN(CN5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS4*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CO5),0+$AJ$50,1-((TAN(CO5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT4*$DU$3)+1-$DU$3)","v":0.68045300274250919},{"$f":"(IF($AH$46<DEGREES(CP5),0+$AJ$50,1-((TAN(CP5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU4*$DU$3)+1-$DU$3)","v":1.7971465276819723},{"$f":"(IF($AH$46<DEGREES(CQ5),0+$AJ$50,1-((TAN(CQ5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV4*$DU$3)+1-$DU$3)","v":2.7465189205637541},{"$f":"(IF($AH$46<DEGREES(CR5),0+$AJ$50,1-((TAN(CR5)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW4*$DU$3)+1-$DU$3)","v":3.6174103900321075},null,null,{"$f":"'Profile angles'!AR5","v":1},{"$f":"'Profile angles'!AS5","v":-79.238745258454912},{"$f":"'Profile angles'!AT5","v":-73.135890206899091},{"$f":"'Profile angles'!AU5","v":-62.969753990761212},{"$f":"'Profile angles'!AV5","v":-51.103815741194268},{"$f":"'Profile angles'!AW5","v":-42.972420763986918},{"$f":"'Profile angles'!AX5","v":-40.259838967181594},{"$f":"'Profile angles'!AY5","v":-43.397326661656273},{"$f":"'Profile angles'!AZ5","v":-51.194813940312706},{"$f":"'Profile angles'!BA5","v":-61.30334441705341},{"$f":"'Profile angles'!BB5","v":-68.588756925018274},{"$f":"'Profile angles'!BC5","v":-73.864057818332},{"$f":"'Profile angles'!BD5","v":-77.510392918823513},null,{"$f":"DW5","v":1},{"$f":"DX5","v":-79.238745258454912},-73.135890206899091,-62.969753990761212,-51.103815741194268,-42.972420763986918,-40.259838967181594,-43.397326661656273,-51.194813940312706,-61.30334441705341,-68.588756925018274,-73.864057818332,{"$f":"EI5","v":-77.510392918823513}]
[null,2,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D6-C337,'Dry Bulb'!D6-C221)","v":-10.999193205944799},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E6-D337,'Dry Bulb'!E6-D221)","v":-6.6791932059447987},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F6-E337,'Dry Bulb'!F6-E221)","v":-7.0191932059448021},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G6-F337,'Dry Bulb'!G6-F221)","v":1.2824587685774844},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H6-G337,'Dry Bulb'!H6-G221)","v":13.140806794055209},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I6-H337,'Dry Bulb'!I6-H221)","v":17.820806794055201},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J6-I337,'Dry Bulb'!J6-I221)","v":19.260806794055199},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K6-J337,'Dry Bulb'!K6-J221)","v":19.800806794055205},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L6-K337,'Dry Bulb'!L6-K221)","v":14.0408067940552},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M6-L337,'Dry Bulb'!M6-L221)","v":4.8240516348195399},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N6-M337,'Dry Bulb'!N6-M221)","v":-6.4791932059447959},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O6-N337,'Dry Bulb'!O6-N221)","v":-8.8391932059447953},null,30,"Building N-S Axis",null,null,null,null,null,10,null,null,null,null,null,"OVERHANG",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI6","v":2},{"$f":"'Incident angle'!BJ6","v":0},{"$f":"'Incident angle'!BK6","v":0},{"$f":"'Incident angle'!BL6","v":0},{"$f":"'Incident angle'!BM6","v":0},{"$f":"'Incident angle'!BN6","v":0},{"$f":"'Incident angle'!BO6","v":0},{"$f":"'Incident angle'!BP6","v":0},{"$f":"'Incident angle'!BQ6","v":0},{"$f":"'Incident angle'!BR6","v":0},{"$f":"'Incident angle'!BS6","v":0},{"$f":"'Incident angle'!BT6","v":0},{"$f":"'Incident angle'!BU6","v":0},"Max M-N",{"$f":"'Incident angle'!BW6","v":2},{"$f":"'Incident angle'!BX6","v":0},{"$f":"'Incident angle'!BY6","v":0},{"$f":"'Incident angle'!BZ6","v":0},{"$f":"'Incident angle'!CA6","v":0},{"$f":"'Incident angle'!CB6","v":0},{"$f":"'Incident angle'!CC6","v":0},{"$f":"'Incident angle'!CD6","v":0},{"$f":"'Incident angle'!CE6","v":0},{"$f":"'Incident angle'!CF6","v":0},{"$f":"'Incident angle'!CG6","v":0},{"$f":"'Incident angle'!CH6","v":0},{"$f":"'Incident angle'!CI6","v":0},"Max",{"$f":"'Profile angles'!B6","v":2},{"$f":"RADIANS('Profile angles'!C6)","v":1.5208845729807423},{"$f":"RADIANS('Profile angles'!D6)","v":1.3429160432098302},{"$f":"RADIANS('Profile angles'!E6)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!F6)","v":0.90436988504871818},{"$f":"RADIANS('Profile angles'!G6)","v":0.73943113538447891},{"$f":"RADIANS('Profile angles'!H6)","v":0.68354026259431289},{"$f":"RADIANS('Profile angles'!I6)","v":0.7434435505657796},{"$f":"RADIANS('Profile angles'!J6)","v":0.90231514982176797},{"$f":"RADIANS('Profile angles'!K6)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L6)","v":1.3590817446939001},{"$f":"RADIANS('Profile angles'!M6)","v":1.5418396740988676},{"$f":"RADIANS('Profile angles'!N6)","v":-1.542946372430622},-78.543464868124616,{"$f":"'Profile angles'!B35","v":2},{"$f":"RADIANS('Profile angles'!C35)","v":-1.1549210062521438},{"$f":"RADIANS('Profile angles'!D35)","v":-1.1369164007416153},{"$f":"RADIANS('Profile angles'!E35)","v":-1.0718008336148823},{"$f":"RADIANS('Profile angles'!F35)","v":-0.97946880043257922},{"$f":"RADIANS('Profile angles'!G35)","v":-0.9216498218621163},{"$f":"RADIANS('Profile angles'!H35)","v":-0.92627284120998132},{"$f":"RADIANS('Profile angles'!I35)","v":-0.97053375348907012},{"$f":"RADIANS('Profile angles'!J35)","v":-0.99586471792571007},{"$f":"RADIANS('Profile angles'!K35)","v":-1.0030149795642196},{"$f":"RADIANS('Profile angles'!L35)","v":-1.0118824071687469},{"$f":"RADIANS('Profile angles'!M35)","v":-1.0543583507572232},{"$f":"RADIANS('Profile angles'!N35)","v":-1.1157238568704597},null,{"$f":"'Profile angles'!AD6","v":2},{"$f":"(IF($AH$12<DEGREES(BS6),0+$AJ$16,1-((TAN(BS6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX5*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT6),0+$AJ$16,1-((TAN(BT6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY5*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU6),0+$AJ$16,1-((TAN(BU6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ5*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV6),0+$AJ$16,1-((TAN(BV6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA5*$DU$3)+1-$DU$3)","v":6.2999851510503413E-2},{"$f":"(IF($AH$12<DEGREES(BW6),0+$AJ$16,1-((TAN(BW6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB5*$DU$3)+1-$DU$3)","v":0.23644419897453026},{"$f":"(IF($AH$12<DEGREES(BX6),0+$AJ$16,1-((TAN(BX6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC5*$DU$3)+1-$DU$3)","v":0.29825610161615129},{"$f":"(IF($AH$12<DEGREES(BY6),0+$AJ$16,1-((TAN(BY6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD5*$DU$3)+1-$DU$3)","v":0.24424910720440796},{"$f":"(IF($AH$12<DEGREES(BZ6),0+$AJ$16,1-((TAN(BZ6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE5*$DU$3)+1-$DU$3)","v":6.7049510933515952E-2},{"$f":"(IF($AH$12<DEGREES(CA6),0+$AJ$16,1-((TAN(CA6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF5*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB6),0+$AJ$16,1-((TAN(CB6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG5*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC6),0+$AJ$16,1-((TAN(CC6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH5*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD6),0+$AJ$16,1-((TAN(CD6)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI5*$DU$3)+1-$DU$3)","v":0},null,2,{"$f":"(IF($AH$46<DEGREES(CG6),0+$AJ$50,1-((TAN(CG6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL5*$DU$3)+1-$DU$3)","v":2.225199938830023},{"$f":"(IF($AH$46<DEGREES(CH6),0+$AJ$50,1-((TAN(CH6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM5*$DU$3)+1-$DU$3)","v":1.7206307684679754},{"$f":"(IF($AH$46<DEGREES(CI6),0+$AJ$50,1-((TAN(CI6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN5*$DU$3)+1-$DU$3)","v":1.2143902750600699},{"$f":"(IF($AH$46<DEGREES(CJ6),0+$AJ$50,1-((TAN(CJ6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO5*$DU$3)+1-$DU$3)","v":0.78466310025223773},{"$f":"(IF($AH$46<DEGREES(CK6),0+$AJ$50,1-((TAN(CK6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP5*$DU$3)+1-$DU$3)","v":0.49704507573255291},{"$f":"(IF($AH$46<DEGREES(CL6),0+$AJ$50,1-((TAN(CL6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ5*$DU$3)+1-$DU$3)","v":0.32958599643875752},{"$f":"(IF($AH$46<DEGREES(CM6),0+$AJ$50,1-((TAN(CM6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR5*$DU$3)+1-$DU$3)","v":0.38571957946127255},{"$f":"(IF($AH$46<DEGREES(CN6),0+$AJ$50,1-((TAN(CN6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS5*$DU$3)+1-$DU$3)","v":0.75219810814456911},{"$f":"(IF($AH$46<DEGREES(CO6),0+$AJ$50,1-((TAN(CO6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT5*$DU$3)+1-$DU$3)","v":1.2409615953172011},{"$f":"(IF($AH$46<DEGREES(CP6),0+$AJ$50,1-((TAN(CP6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU5*$DU$3)+1-$DU$3)","v":1.6226605616695511},{"$f":"(IF($AH$46<DEGREES(CQ6),0+$AJ$50,1-((TAN(CQ6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV5*$DU$3)+1-$DU$3)","v":2.0041796730270147},{"$f":"(IF($AH$46<DEGREES(CR6),0+$AJ$50,1-((TAN(CR6)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW5*$DU$3)+1-$DU$3)","v":2.1628073629679259},null,null,{"$f":"'Profile angles'!AR6","v":2},{"$f":"'Profile angles'!AS6","v":-66.037221876299029},{"$f":"'Profile angles'!AT6","v":-62.610262119735701},{"$f":"'Profile angles'!AU6","v":-54.505603493104644},{"$f":"'Profile angles'!AV6","v":-44.039138424385058},{"$f":"'Profile angles'!AW6","v":-36.867903866984811},{"$f":"'Profile angles'!AX6","v":-34.787290206430924},{"$f":"'Profile angles'!AY6","v":-37.887883453111968},{"$f":"'Profile angles'!AZ6","v":-44.388788539159933},{"$f":"'Profile angles'!BA6","v":-51.819137025254065},{"$f":"'Profile angles'!BB6","v":-56.521775308526607},{"$f":"'Profile angles'!BC6","v":-60.378308807607461},{"$f":"'Profile angles'!BD6","v":-63.889653492857697},null,{"$f":"DW6","v":2},-66.037221876299029,-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697]
[null,3,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D7-C338,'Dry Bulb'!D7-C222)","v":-11.539193205944798},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E7-D338,'Dry Bulb'!E7-D222)","v":-7.759193205944797},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F7-E338,'Dry Bulb'!F7-E222)","v":-8.279193205944793},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G7-F338,'Dry Bulb'!G7-F222)","v":-4.5638556263270402E-2},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H7-G338,'Dry Bulb'!H7-G222)","v":12.06080679405521},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I7-H338,'Dry Bulb'!I7-H222)","v":16.92080679405521},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J7-I338,'Dry Bulb'!J7-I222)","v":18.180806794055201},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K7-J338,'Dry Bulb'!K7-J222)","v":18.180806794055201},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L7-K338,'Dry Bulb'!L7-K222)","v":12.42080679405521},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M7-L338,'Dry Bulb'!M7-L222)","v":2.8319056475583864},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N7-M338,'Dry Bulb'!N7-M222)","v":-7.7391932059447939},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O7-N338,'Dry Bulb'!O7-N222)","v":-9.5591932059447942},null,null,"  (E&W Façade)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI7","v":3},{"$f":"'Incident angle'!BJ7","v":0},{"$f":"'Incident angle'!BK7","v":0},{"$f":"'Incident angle'!BL7","v":0},{"$f":"'Incident angle'!BM7","v":0},{"$f":"'Incident angle'!BN7","v":0},{"$f":"'Incident angle'!BO7","v":0},{"$f":"'Incident angle'!BP7","v":0},{"$f":"'Incident angle'!BQ7","v":0},{"$f":"'Incident angle'!BR7","v":0},{"$f":"'Incident angle'!BS7","v":0},{"$f":"'Incident angle'!BT7","v":0},{"$f":"'Incident angle'!BU7","v":0},{"$f":"MAX(AS5:AZ28)","v":459.69342121644979},{"$f":"'Incident angle'!BW7","v":3},{"$f":"'Incident angle'!BX7","v":0},{"$f":"'Incident angle'!BY7","v":0},{"$f":"'Incident angle'!BZ7","v":0},{"$f":"'Incident angle'!CA7","v":0},{"$f":"'Incident angle'!CB7","v":0},{"$f":"'Incident angle'!CC7","v":0},{"$f":"'Incident angle'!CD7","v":0},{"$f":"'Incident angle'!CE7","v":0},{"$f":"'Incident angle'!CF7","v":0},{"$f":"'Incident angle'!CG7","v":0},{"$f":"'Incident angle'!CH7","v":0},{"$f":"'Incident angle'!CI7","v":0},{"$f":"MAX(BG5:BN28)","v":3826.0863600764724},{"$f":"'Profile angles'!B7","v":3},{"$f":"RADIANS('Profile angles'!C7)","v":-1.5580652106671682},{"$f":"RADIANS('Profile angles'!D7)","v":1.3784403465863997},{"$f":"RADIANS('Profile angles'!E7)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F7)","v":0.85700339968847628},{"$f":"RADIANS('Profile angles'!G7)","v":0.66444179725335373},{"$f":"RADIANS('Profile angles'!H7)","v":0.60530956821516546},{"$f":"RADIANS('Profile angles'!I7)","v":0.67565393770152993},{"$f":"RADIANS('Profile angles'!J7)","v":0.85622667593368873},{"$f":"RADIANS('Profile angles'!K7)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L7)","v":1.410298559579243},{"$f":"RADIANS('Profile angles'!M7)","v":-1.5164850137084307},{"$f":"RADIANS('Profile angles'!N7)","v":-1.4620905045107382},-7.2736687044920778,{"$f":"'Profile angles'!B36","v":3},{"$f":"RADIANS('Profile angles'!C36)","v":-0.91516630314878677},{"$f":"RADIANS('Profile angles'!D36)","v":-0.8821622416026319},{"$f":"RADIANS('Profile angles'!E36)","v":-0.80144392257758257},{"$f":"RADIANS('Profile angles'!F36)","v":-0.69259090438957494},{"$f":"RADIANS('Profile angles'!G36)","v":-0.62209031311095009},{"$f":"RADIANS('Profile angles'!H36)","v":-0.61897895359016175},{"$f":"RADIANS('Profile angles'!I36)","v":-0.66606658842026967},{"$f":"RADIANS('Profile angles'!J36)","v":-0.70745482580220742},{"$f":"RADIANS('Profile angles'!K36)","v":-0.7359036106296305},{"$f":"RADIANS('Profile angles'!L36)","v":-0.76137198766493486},{"$f":"RADIANS('Profile angles'!M36)","v":-0.81690920458132044},{"$f":"RADIANS('Profile angles'!N36)","v":-0.88265807634038995},null,{"$f":"'Profile angles'!AD7","v":3},{"$f":"(IF($AH$12<DEGREES(BS7),0+$AJ$16,1-((TAN(BS7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX6*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT7),0+$AJ$16,1-((TAN(BT7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY6*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU7),0+$AJ$16,1-((TAN(BU7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ6*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV7),0+$AJ$16,1-((TAN(BV7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA6*$DU$3)+1-$DU$3)","v":5.8360402486520718E-2},{"$f":"(IF($AH$12<DEGREES(BW7),0+$AJ$16,1-((TAN(BW7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB6*$DU$3)+1-$DU$3)","v":0.20501893366355498},{"$f":"(IF($AH$12<DEGREES(BX7),0+$AJ$16,1-((TAN(BX7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC6*$DU$3)+1-$DU$3)","v":0.26520014577375789},{"$f":"(IF($AH$12<DEGREES(BY7),0+$AJ$16,1-((TAN(BY7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD6*$DU$3)+1-$DU$3)","v":0.21511139777587041},{"$f":"(IF($AH$12<DEGREES(BZ7),0+$AJ$16,1-((TAN(BZ7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE6*$DU$3)+1-$DU$3)","v":6.2942674350888947E-2},{"$f":"(IF($AH$12<DEGREES(CA7),0+$AJ$16,1-((TAN(CA7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF6*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB7),0+$AJ$16,1-((TAN(CB7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG6*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC7),0+$AJ$16,1-((TAN(CC7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH6*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD7),0+$AJ$16,1-((TAN(CD7)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI6*$DU$3)+1-$DU$3)","v":0},null,3,{"$f":"(IF($AH$46<DEGREES(CG7),0+$AJ$50,1-((TAN(CG7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL6*$DU$3)+1-$DU$3)","v":1.7653723181341276},{"$f":"(IF($AH$46<DEGREES(CH7),0+$AJ$50,1-((TAN(CH7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM6*$DU$3)+1-$DU$3)","v":1.5244277082270692},{"$f":"(IF($AH$46<DEGREES(CI7),0+$AJ$50,1-((TAN(CI7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN6*$DU$3)+1-$DU$3)","v":1.2349622149603581},{"$f":"(IF($AH$46<DEGREES(CJ7),0+$AJ$50,1-((TAN(CJ7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO6*$DU$3)+1-$DU$3)","v":0.95962238451204485},{"$f":"(IF($AH$46<DEGREES(CK7),0+$AJ$50,1-((TAN(CK7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP6*$DU$3)+1-$DU$3)","v":0.77554221539945478},{"$f":"(IF($AH$46<DEGREES(CL7),0+$AJ$50,1-((TAN(CL7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ6*$DU$3)+1-$DU$3)","v":0.69266037714831585},{"$f":"(IF($AH$46<DEGREES(CM7),0+$AJ$50,1-((TAN(CM7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR6*$DU$3)+1-$DU$3)","v":0.7501065244347781},{"$f":"(IF($AH$46<DEGREES(CN7),0+$AJ$50,1-((TAN(CN7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS6*$DU$3)+1-$DU$3)","v":0.95185934979473219},{"$f":"(IF($AH$46<DEGREES(CO7),0+$AJ$50,1-((TAN(CO7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT6*$DU$3)+1-$DU$3)","v":1.2219332418278925},{"$f":"(IF($AH$46<DEGREES(CP7),0+$AJ$50,1-((TAN(CP7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU6*$DU$3)+1-$DU$3)","v":1.4505785112231291},{"$f":"(IF($AH$46<DEGREES(CQ7),0+$AJ$50,1-((TAN(CQ7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV6*$DU$3)+1-$DU$3)","v":1.5916032178618971},{"$f":"(IF($AH$46<DEGREES(CR7),0+$AJ$50,1-((TAN(CR7)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW6*$DU$3)+1-$DU$3)","v":1.6149413500403891},null,null,{"$f":"'Profile angles'!AR7","v":3},{"$f":"'Profile angles'!AS7","v":-52.431373562484438},{"$f":"'Profile angles'!AT7","v":-49.776364898184575},{"$f":"'Profile angles'!AU7","v":-43.00744408924087},{"$f":"'Profile angles'!AV7","v":-33.970697614512481},{"$f":"'Profile angles'!AW7","v":-27.874166624770901},{"$f":"'Profile angles'!AX7","v":-26.397406240900974},{"$f":"'Profile angles'!AY7","v":-29.298461575777225},{"$f":"'Profile angles'!AZ7","v":-34.480458721023354},{"$f":"'Profile angles'!BA7","v":-39.89507498863518},{"$f":"'Profile angles'!BB7","v":-43.286892300779471},{"$f":"'Profile angles'!BC7","v":-46.757596903257479},{"$f":"'Profile angles'!BD7","v":-50.32692672055552},null,3,-52.431373562484438,-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552]
[null,4,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D8-C339,'Dry Bulb'!D8-C223)","v":-12.439193205944797},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E8-D339,'Dry Bulb'!E8-D223)","v":-8.8391932059447953},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F8-E339,'Dry Bulb'!F8-E223)","v":-9.1791932059447987},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G8-F339,'Dry Bulb'!G8-F223)","v":-1.816434989384291},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H8-G339,'Dry Bulb'!H8-G223)","v":11.520806794055204},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I8-H339,'Dry Bulb'!I8-H223)","v":15.840806794055197},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J8-I339,'Dry Bulb'!J8-I223)","v":16.740806794055203},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K8-J339,'Dry Bulb'!K8-J223)","v":16.92080679405521},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L8-K339,'Dry Bulb'!L8-K223)","v":10.980806794055198},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M8-L339,'Dry Bulb'!M8-L223)","v":1.9465074309978831},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N8-M339,'Dry Bulb'!N8-M223)","v":-8.9991932059447919},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O8-N339,'Dry Bulb'!O8-N223)","v":-10.459193205944793},null,null,null,null,null,"Floors",null,null,"Window Height",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI8","v":4},{"$f":"'Incident angle'!BJ8","v":0},{"$f":"'Incident angle'!BK8","v":0},{"$f":"'Incident angle'!BL8","v":0},{"$f":"'Incident angle'!BM8","v":0},{"$f":"'Incident angle'!BN8","v":0},{"$f":"'Incident angle'!BO8","v":0},{"$f":"'Incident angle'!BP8","v":0},{"$f":"'Incident angle'!BQ8","v":0},{"$f":"'Incident angle'!BR8","v":0},{"$f":"'Incident angle'!BS8","v":0},{"$f":"'Incident angle'!BT8","v":0},{"$f":"'Incident angle'!BU8","v":0},"Av+Max/2",{"$f":"'Incident angle'!BW8","v":4},{"$f":"'Incident angle'!BX8","v":0},{"$f":"'Incident angle'!BY8","v":0},{"$f":"'Incident angle'!BZ8","v":0},{"$f":"'Incident angle'!CA8","v":0},{"$f":"'Incident angle'!CB8","v":0},{"$f":"'Incident angle'!CC8","v":0},{"$f":"'Incident angle'!CD8","v":0},{"$f":"'Incident angle'!CE8","v":0},{"$f":"'Incident angle'!CF8","v":0},{"$f":"'Incident angle'!CG8","v":0},{"$f":"'Incident angle'!CH8","v":0},{"$f":"'Incident angle'!CI8","v":0},"Av+Max/2",{"$f":"'Profile angles'!B8","v":4},{"$f":"RADIANS('Profile angles'!C8)","v":-1.4341706307619093},{"$f":"RADIANS('Profile angles'!D8)","v":1.4532017897405851},{"$f":"RADIANS('Profile angles'!E8)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F8)","v":0.75641890675993251},{"$f":"RADIANS('Profile angles'!G8)","v":0.5162754389988029},{"$f":"RADIANS('Profile angles'!H8)","v":0.4555590077463848},{"$f":"RADIANS('Profile angles'!I8)","v":0.54225140039405473},{"$f":"RADIANS('Profile angles'!J8)","v":0.75895388639250683},{"$f":"RADIANS('Profile angles'!K8)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L8)","v":1.5231003679412918},{"$f":"RADIANS('Profile angles'!M8)","v":-1.3502899956877574},{"$f":"RADIANS('Profile angles'!N8)","v":-1.3073727427737789},-2.4138736537718248,{"$f":"'Profile angles'!B37","v":4},{"$f":"RADIANS('Profile angles'!C37)","v":-0.68085626049108372},{"$f":"RADIANS('Profile angles'!D37)","v":-0.63580151600596946},{"$f":"RADIANS('Profile angles'!E37)","v":-0.54404800401822839},{"$f":"RADIANS('Profile angles'!F37)","v":-0.42586833332700952},{"$f":"RADIANS('Profile angles'!G37)","v":-0.34974170353085882},{"$f":"RADIANS('Profile angles'!H37)","v":-0.34253601746325713},{"$f":"RADIANS('Profile angles'!I37)","v":-0.38955752453780007},{"$f":"RADIANS('Profile angles'!J37)","v":-0.43944775480650367},{"$f":"RADIANS('Profile angles'!K37)","v":-0.48155681326357486},{"$f":"RADIANS('Profile angles'!L37)","v":-0.51888038822348748},{"$f":"RADIANS('Profile angles'!M37)","v":-0.58456796965293845},{"$f":"RADIANS('Profile angles'!N37)","v":-0.6539876584676938},null,{"$f":"'Profile angles'!AD8","v":4},{"$f":"(IF($AH$12<DEGREES(BS8),0+$AJ$16,1-((TAN(BS8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX7*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT8),0+$AJ$16,1-((TAN(BT8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY7*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU8),0+$AJ$16,1-((TAN(BU8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ7*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV8),0+$AJ$16,1-((TAN(BV8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA7*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW8),0+$AJ$16,1-((TAN(BW8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB7*$DU$3)+1-$DU$3)","v":0.13370997006666008},{"$f":"(IF($AH$12<DEGREES(BX8),0+$AJ$16,1-((TAN(BX8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC7*$DU$3)+1-$DU$3)","v":0.20568287226775725},{"$f":"(IF($AH$12<DEGREES(BY8),0+$AJ$16,1-((TAN(BY8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD7*$DU$3)+1-$DU$3)","v":0.15393906385045122},{"$f":"(IF($AH$12<DEGREES(BZ8),0+$AJ$16,1-((TAN(BZ8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE7*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA8),0+$AJ$16,1-((TAN(CA8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF7*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB8),0+$AJ$16,1-((TAN(CB8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG7*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC8),0+$AJ$16,1-((TAN(CC8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH7*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD8),0+$AJ$16,1-((TAN(CD8)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI7*$DU$3)+1-$DU$3)","v":0},null,4,{"$f":"(IF($AH$46<DEGREES(CG8),0+$AJ$50,1-((TAN(CG8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL7*$DU$3)+1-$DU$3)","v":1.4032955693265039},{"$f":"(IF($AH$46<DEGREES(CH8),0+$AJ$50,1-((TAN(CH8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM7*$DU$3)+1-$DU$3)","v":1.379921956174806},{"$f":"(IF($AH$46<DEGREES(CI8),0+$AJ$50,1-((TAN(CI8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN7*$DU$3)+1-$DU$3)","v":1.1733486818169045},{"$f":"(IF($AH$46<DEGREES(CJ8),0+$AJ$50,1-((TAN(CJ8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO7*$DU$3)+1-$DU$3)","v":0.96640104921223335},{"$f":"(IF($AH$46<DEGREES(CK8),0+$AJ$50,1-((TAN(CK8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP7*$DU$3)+1-$DU$3)","v":0.82725041932793253},{"$f":"(IF($AH$46<DEGREES(CL8),0+$AJ$50,1-((TAN(CL8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ7*$DU$3)+1-$DU$3)","v":0.77217005101735159},{"$f":"(IF($AH$46<DEGREES(CM8),0+$AJ$50,1-((TAN(CM8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR7*$DU$3)+1-$DU$3)","v":0.82170231920961312},{"$f":"(IF($AH$46<DEGREES(CN8),0+$AJ$50,1-((TAN(CN8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS7*$DU$3)+1-$DU$3)","v":0.96433573091408953},{"$f":"(IF($AH$46<DEGREES(CO8),0+$AJ$50,1-((TAN(CO8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT7*$DU$3)+1-$DU$3)","v":1.1556883702663534},{"$f":"(IF($AH$46<DEGREES(CP8),0+$AJ$50,1-((TAN(CP8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU7*$DU$3)+1-$DU$3)","v":1.3243462928018961},{"$f":"(IF($AH$46<DEGREES(CQ8),0+$AJ$50,1-((TAN(CQ8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV7*$DU$3)+1-$DU$3)","v":1.2934231543221699},{"$f":"(IF($AH$46<DEGREES(CR8),0+$AJ$50,1-((TAN(CR8)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW7*$DU$3)+1-$DU$3)","v":1.3090115867504339},null,null,{"$f":"'Profile angles'!AR8","v":4},{"$f":"'Profile angles'!AS8","v":-38.837571781392398},{"$f":"'Profile angles'!AT8","v":-36.325136967893741},{"$f":"'Profile angles'!AU8","v":-30.23387910899125},{"$f":"'Profile angles'!AV8","v":-22.236891602714234},{"$f":"'Profile angles'!AW8","v":-17.058579195686843},{"$f":"'Profile angles'!AX8","v":-16.082853037589089},{"$f":"'Profile angles'!AY8","v":-18.740224973134019},{"$f":"'Profile angles'!AZ8","v":-22.841111056638525},{"$f":"'Profile angles'!BA8","v":-26.935985833021629},{"$f":"'Profile angles'!BB8","v":-29.720493919992279},{"$f":"'Profile angles'!BC8","v":-33.206986937806654},{"$f":"'Profile angles'!BD8","v":-36.893522726896833},null,4,-38.837571781392398,-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833]
[null,5,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D9-C340,'Dry Bulb'!D9-C224)","v":-13.519193205944795},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E9-D340,'Dry Bulb'!E9-D224)","v":-9.5591932059447942},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F9-E340,'Dry Bulb'!F9-E224)","v":-3.0791932059447973},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G9-F340,'Dry Bulb'!G9-F224)","v":-3.1445323142250601},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H9-G340,'Dry Bulb'!H9-G224)","v":10.080806794055206},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I9-H340,'Dry Bulb'!I9-H224)","v":14.580806794055206},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J9-I340,'Dry Bulb'!J9-I224)","v":16.020806794055204},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K9-J340,'Dry Bulb'!K9-J224)","v":15.840806794055197},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L9-K340,'Dry Bulb'!L9-K224)","v":10.260806794055213},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M9-L340,'Dry Bulb'!M9-L224)","v":0.17571099787686251},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N9-M340,'Dry Bulb'!N9-M224)","v":-3.4391932059447896},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O9-N340,'Dry Bulb'!O9-N224)","v":-11.359193205944791},null,15,"Building Height",null,null,1,null,null,null,1,null,null,null,null,"Lab Override",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI9","v":5},{"$f":"'Incident angle'!BJ9","v":0},{"$f":"'Incident angle'!BK9","v":0},{"$f":"'Incident angle'!BL9","v":0},{"$f":"'Incident angle'!BM9","v":0},{"$f":"'Incident angle'!BN9","v":0},{"$f":"'Incident angle'!BO9","v":0},{"$f":"'Incident angle'!BP9","v":0},{"$f":"'Incident angle'!BQ9","v":0},{"$f":"'Incident angle'!BR9","v":0},{"$f":"'Incident angle'!BS9","v":0},{"$f":"'Incident angle'!BT9","v":0},{"$f":"'Incident angle'!BU9","v":0},{"$f":"AVERAGE(BC5,BC7)","v":389.51667651337539},{"$f":"'Incident angle'!BW9","v":5},{"$f":"'Incident angle'!BX9","v":0},{"$f":"'Incident angle'!BY9","v":0},{"$f":"'Incident angle'!BZ9","v":0},{"$f":"'Incident angle'!CA9","v":0},{"$f":"'Incident angle'!CB9","v":0},{"$f":"'Incident angle'!CC9","v":0},{"$f":"'Incident angle'!CD9","v":0},{"$f":"'Incident angle'!CE9","v":0},{"$f":"'Incident angle'!CF9","v":0},{"$f":"'Incident angle'!CG9","v":0},{"$f":"'Incident angle'!CH9","v":0},{"$f":"'Incident angle'!CI9","v":0},{"$f":"AVERAGE(BQ5,BQ7)","v":2836.7640765683218},{"$f":"'Profile angles'!B9","v":5},{"$f":"RADIANS('Profile angles'!C9)","v":-1.1780474606511619},{"$f":"RADIANS('Profile angles'!D9)","v":-1.5063837691420776},{"$f":"RADIANS('Profile angles'!E9)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F9)","v":0.50158785009162143},{"$f":"RADIANS('Profile angles'!G9)","v":0.2080737467427515},{"$f":"RADIANS('Profile angles'!H9)","v":0.16549565334901181},{"$f":"RADIANS('Profile angles'!I9)","v":0.26831827706241235},{"$f":"RADIANS('Profile angles'!J9)","v":0.51728377304772166},{"$f":"RADIANS('Profile angles'!K9)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L9)","v":-1.3007610762503927},{"$f":"RADIANS('Profile angles'!M9)","v":-0.99832765575334248},{"$f":"RADIANS('Profile angles'!N9)","v":-1.007647471209566},-0.75761696006821877,{"$f":"'Profile angles'!B38","v":5},{"$f":"RADIANS('Profile angles'!C38)","v":-0.45057174190181387},{"$f":"RADIANS('Profile angles'!D38)","v":-0.39650083624290827},{"$f":"RADIANS('Profile angles'!E38)","v":-0.29766243646613255},{"$f":"RADIANS('Profile angles'!F38)","v":-0.17558478457949336},{"$f":"RADIANS('Profile angles'!G38)","v":-9.8704393140607194E-2},{"$f":"RADIANS('Profile angles'!H38)","v":-9.0149372015666446E-2},{"$f":"RADIANS('Profile angles'!I38)","v":-0.1356210090143263},{"$f":"RADIANS('Profile angles'!J38)","v":-0.18829152816436306},{"$f":"RADIANS('Profile angles'!K38)","v":-0.23731883827832312},{"$f":"RADIANS('Profile angles'!L38)","v":-0.28192945219888416},{"$f":"RADIANS('Profile angles'!M38)","v":-0.35506274589045206},{"$f":"RADIANS('Profile angles'!N38)","v":-0.42785968501246852},null,{"$f":"'Profile angles'!AD9","v":5},{"$f":"(IF($AH$12<DEGREES(BS9),0+$AJ$16,1-((TAN(BS9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT9),0+$AJ$16,1-((TAN(BT9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU9),0+$AJ$16,1-((TAN(BU9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV9),0+$AJ$16,1-((TAN(BV9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW9),0+$AJ$16,1-((TAN(BW9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX9),0+$AJ$16,1-((TAN(BX9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC8*$DU$3)+1-$DU$3)","v":6.7238984412292757E-2},{"$f":"(IF($AH$12<DEGREES(BY9),0+$AJ$16,1-((TAN(BY9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ9),0+$AJ$16,1-((TAN(BZ9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA9),0+$AJ$16,1-((TAN(CA9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB9),0+$AJ$16,1-((TAN(CB9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC9),0+$AJ$16,1-((TAN(CC9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH8*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD9),0+$AJ$16,1-((TAN(CD9)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI8*$DU$3)+1-$DU$3)","v":0},null,5,{"$f":"(IF($AH$46<DEGREES(CG9),0+$AJ$50,1-((TAN(CG9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL8*$DU$3)+1-$DU$3)","v":1.1609671913623092},{"$f":"(IF($AH$46<DEGREES(CH9),0+$AJ$50,1-((TAN(CH9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM8*$DU$3)+1-$DU$3)","v":1.2343102277691405},{"$f":"(IF($AH$46<DEGREES(CI9),0+$AJ$50,1-((TAN(CI9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN8*$DU$3)+1-$DU$3)","v":1.1005293079622112},{"$f":"(IF($AH$46<DEGREES(CJ9),0+$AJ$50,1-((TAN(CJ9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO8*$DU$3)+1-$DU$3)","v":0.92746376357132199},{"$f":"(IF($AH$46<DEGREES(CK9),0+$AJ$50,1-((TAN(CK9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP8*$DU$3)+1-$DU$3)","v":0.81096653885134962},{"$f":"(IF($AH$46<DEGREES(CL9),0+$AJ$50,1-((TAN(CL9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ8*$DU$3)+1-$DU$3)","v":0.76895587399105259},{"$f":"(IF($AH$46<DEGREES(CM9),0+$AJ$50,1-((TAN(CM9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR8*$DU$3)+1-$DU$3)","v":0.81340441519053075},{"$f":"(IF($AH$46<DEGREES(CN9),0+$AJ$50,1-((TAN(CN9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS8*$DU$3)+1-$DU$3)","v":0.92773109607665405},{"$f":"(IF($AH$46<DEGREES(CO9),0+$AJ$50,1-((TAN(CO9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT8*$DU$3)+1-$DU$3)","v":1.0814279375377414},{"$f":"(IF($AH$46<DEGREES(CP9),0+$AJ$50,1-((TAN(CP9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU8*$DU$3)+1-$DU$3)","v":1.1267340063859186},{"$f":"(IF($AH$46<DEGREES(CQ9),0+$AJ$50,1-((TAN(CQ9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV8*$DU$3)+1-$DU$3)","v":1.0764120903340324},{"$f":"(IF($AH$46<DEGREES(CR9),0+$AJ$50,1-((TAN(CR9)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW8*$DU$3)+1-$DU$3)","v":1.0902732846185907},null,null,{"$f":"'Profile angles'!AR9","v":5},{"$f":"'Profile angles'!AS9","v":-25.376333918471747},{"$f":"'Profile angles'!AT9","v":-22.7103856061896},{"$f":"'Profile angles'!AU9","v":-16.897092448538263},{"$f":"'Profile angles'!AV9","v":-9.5810693067706811},{"$f":"'Profile angles'!AW9","v":-5.1231262317655331},{"$f":"'Profile angles'!AX9","v":-4.54535827775074},{"$f":"'Profile angles'!AY9","v":-6.9688312964780383},{"$f":"'Profile angles'!AZ9","v":-10.241982624949756},{"$f":"'Profile angles'!BA9","v":-13.517063375335365},{"$f":"'Profile angles'!BB9","v":-16.104385171900024},{"$f":"'Profile angles'!BC9","v":-19.830528453312528},{"$f":"'Profile angles'!BD9","v":-23.664530366970006},null,5,-25.376333918471747,-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006]
[null,6,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D10-C341,'Dry Bulb'!D10-C225)","v":-14.059193205944794},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E10-D341,'Dry Bulb'!E10-D225)","v":-10.279193205944793},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F10-E341,'Dry Bulb'!F10-E225)","v":-3.6191932059447964},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G10-F341,'Dry Bulb'!G10-F225)","v":-3.8689656717563565},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H10-G341,'Dry Bulb'!H10-G225)","v":10.07126610262651},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I10-H341,'Dry Bulb'!I10-H225)","v":13.951274327024777},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J10-I341,'Dry Bulb'!J10-I225)","v":15.586836445569872},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K10-J341,'Dry Bulb'!K10-J225)","v":15.102136505591019},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L10-K341,'Dry Bulb'!L10-K225)","v":10.893107961765551},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M10-L341,'Dry Bulb'!M10-L225)","v":-0.93103677282378783},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N10-M341,'Dry Bulb'!N10-M225)","v":-3.7991932059447961},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O10-N341,'Dry Bulb'!O10-N225)","v":-11.359193205944791},null,null,null,null,null,null,null,null,null,2,null,null,null,null,{"$f":"'HVAC Dashboard'!AC34","v":1},null,null,"Tanδ =  ",null,{"$f":"IF(X5>0,W6/X5,99999999)","v":1.4285714285714286},null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI10","v":6},{"$f":"'Incident angle'!BJ10","v":0},{"$f":"'Incident angle'!BK10","v":0},{"$f":"'Incident angle'!BL10","v":0},{"$f":"'Incident angle'!BM10","v":0},{"$f":"'Incident angle'!BN10","v":0},{"$f":"'Incident angle'!BO10","v":0},{"$f":"'Incident angle'!BP10","v":0},{"$f":"'Incident angle'!BQ10","v":0},{"$f":"'Incident angle'!BR10","v":0},{"$f":"'Incident angle'!BS10","v":0},{"$f":"'Incident angle'!BT10","v":0},{"$f":"'Incident angle'!BU10","v":0},"Max All",{"$f":"'Incident angle'!BW10","v":6},{"$f":"'Incident angle'!BX10","v":0},{"$f":"'Incident angle'!BY10","v":0},{"$f":"'Incident angle'!BZ10","v":0},{"$f":"'Incident angle'!CA10","v":85.291254678098866},{"$f":"'Incident angle'!CB10","v":200.04067612922577},{"$f":"'Incident angle'!CC10","v":238.69148403224921},{"$f":"'Incident angle'!CD10","v":151.55996159633474},{"$f":"'Incident angle'!CE10","v":85.484580900045813},{"$f":"'Incident angle'!CF10","v":49.076156240520959},{"$f":"'Incident angle'!CG10","v":0},{"$f":"'Incident angle'!CH10","v":0},{"$f":"'Incident angle'!CI10","v":0},null,{"$f":"'Profile angles'!B10","v":6},{"$f":"RADIANS('Profile angles'!C10)","v":-0.64835816681447489},{"$f":"RADIANS('Profile angles'!D10)","v":-0.88647687640734596},{"$f":"RADIANS('Profile angles'!E10)","v":1.1397000015522982},{"$f":"RADIANS('Profile angles'!F10)","v":-0.30683145766901876},{"$f":"RADIANS('Profile angles'!G10)","v":-0.38591275889302951},{"$f":"RADIANS('Profile angles'!H10)","v":-0.34548950434356829},{"$f":"RADIANS('Profile angles'!I10)","v":-0.27681674745400869},{"$f":"RADIANS('Profile angles'!J10)","v":-0.23949897187106284},{"$f":"RADIANS('Profile angles'!K10)","v":1.1397000015523175},{"$f":"RADIANS('Profile angles'!L10)","v":-0.2425098589486748},{"$f":"RADIANS('Profile angles'!M10)","v":-0.35092289852329306},{"$f":"RADIANS('Profile angles'!N10)","v":-0.48669309889480084},3.2137435279028223E-2,{"$f":"'Profile angles'!B39","v":6},{"$f":"RADIANS('Profile angles'!C39)","v":-0.22091645053294795},{"$f":"RADIANS('Profile angles'!D39)","v":-0.16074662252161659},{"$f":"RADIANS('Profile angles'!E39)","v":-5.8021971754234451E-2},{"$f":"RADIANS('Profile angles'!F39)","v":6.4078725586556834E-2},{"$f":"RADIANS('Profile angles'!G39)","v":0.1385056203166444},{"$f":"RADIANS('Profile angles'!H39)","v":0.14648644817173609},{"$f":"RADIANS('Profile angles'!I39)","v":0.1032161832467153},{"$f":"RADIANS('Profile angles'!J39)","v":5.1801075064635951E-2},{"$f":"RADIANS('Profile angles'!K39)","v":1.4535089563001097E-3},{"$f":"RADIANS('Profile angles'!L39)","v":-4.6191080812301957E-2},{"$f":"RADIANS('Profile angles'!M39)","v":-0.12425151109146822},{"$f":"RADIANS('Profile angles'!N39)","v":-0.20052072268814197},null,{"$f":"'Profile angles'!AD10","v":6},{"$f":"(IF($AH$12<DEGREES(BS10),0+$AJ$16,1-((TAN(BS10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT10),0+$AJ$16,1-((TAN(BT10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU10),0+$AJ$16,1-((TAN(BU10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV10),0+$AJ$16,1-((TAN(BV10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW10),0+$AJ$16,1-((TAN(BW10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX10),0+$AJ$16,1-((TAN(BX10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY10),0+$AJ$16,1-((TAN(BY10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ10),0+$AJ$16,1-((TAN(BZ10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA10),0+$AJ$16,1-((TAN(CA10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB10),0+$AJ$16,1-((TAN(CB10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC10),0+$AJ$16,1-((TAN(CC10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH9*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD10),0+$AJ$16,1-((TAN(CD10)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI9*$DU$3)+1-$DU$3)","v":0},null,6,{"$f":"(IF($AH$46<DEGREES(CG10),0+$AJ$50,1-((TAN(CG10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL9*$DU$3)+1-$DU$3)","v":0.96656117013390619},{"$f":"(IF($AH$46<DEGREES(CH10),0+$AJ$50,1-((TAN(CH10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM9*$DU$3)+1-$DU$3)","v":1.0247109476389711},{"$f":"(IF($AH$46<DEGREES(CI10),0+$AJ$50,1-((TAN(CI10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN9*$DU$3)+1-$DU$3)","v":1.021028169283509},{"$f":"(IF($AH$46<DEGREES(CJ10),0+$AJ$50,1-((TAN(CJ10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO9*$DU$3)+1-$DU$3)","v":0.8641375435548988},{"$f":"(IF($AH$46<DEGREES(CK10),0+$AJ$50,1-((TAN(CK10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP9*$DU$3)+1-$DU$3)","v":0.75915737771911762},{"$f":"(IF($AH$46<DEGREES(CL10),0+$AJ$50,1-((TAN(CL10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ9*$DU$3)+1-$DU$3)","v":0.72465488684182011},{"$f":"(IF($AH$46<DEGREES(CM10),0+$AJ$50,1-((TAN(CM10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR9*$DU$3)+1-$DU$3)","v":0.76688372823208661},{"$f":"(IF($AH$46<DEGREES(CN10),0+$AJ$50,1-((TAN(CN10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS9*$DU$3)+1-$DU$3)","v":0.86603014573157333},{"$f":"(IF($AH$46<DEGREES(CO10),0+$AJ$50,1-((TAN(CO10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT9*$DU$3)+1-$DU$3)","v":0.99879391558314168},{"$f":"(IF($AH$46<DEGREES(CP10),0+$AJ$50,1-((TAN(CP10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU9*$DU$3)+1-$DU$3)","v":0.93171562078997672},{"$f":"(IF($AH$46<DEGREES(CQ10),0+$AJ$50,1-((TAN(CQ10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV9*$DU$3)+1-$DU$3)","v":0.89156707648587818},{"$f":"(IF($AH$46<DEGREES(CR10),0+$AJ$50,1-((TAN(CR10)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW9*$DU$3)+1-$DU$3)","v":0.90647367404783274},null,null,{"$f":"'Profile angles'!AR10","v":6},{"$f":"'Profile angles'!AS10","v":-12.151444093159176},{"$f":"'Profile angles'!AT10","v":-9.1319080559186769},{"$f":"'Profile angles'!AU10","v":-3.3232309033445411},{"$f":"'Profile angles'!AV10","v":3.5985816694690373},{"$f":"'Profile angles'!AW10","v":7.5112987220277185},{"$f":"'Profile angles'!AX10","v":7.7738597839019823},{"$f":"'Profile angles'!AY10","v":5.5584053941199079},{"$f":"'Profile angles'!AZ10","v":2.9033723023449274},{"$f":"'Profile angles'!BA10","v":8.3279910069695443E-2},{"$f":"'Profile angles'!BB10","v":-2.6015900354108483},{"$f":"'Profile angles'!BC10","v":-6.7413522567651629},{"$f":"'Profile angles'!BD10","v":-10.743396255327719},null,6,-12.151444093159176,-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719]
[null,7,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D11-C342,'Dry Bulb'!D11-C226)","v":-13.936714294401561},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E11-D342,'Dry Bulb'!E11-D226)","v":-9.9670313369964703},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F11-E342,'Dry Bulb'!F11-E226)","v":-2.7185967790058072},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G11-F342,'Dry Bulb'!G11-F226)","v":0.88270589625417983},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H11-G342,'Dry Bulb'!H11-G226)","v":14.242243678705819},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I11-H342,'Dry Bulb'!I11-H226)","v":20.09454451669167},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J11-I342,'Dry Bulb'!J11-I226)","v":21.082721318187694},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K11-J342,'Dry Bulb'!K11-J226)","v":20.221327665047767},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L11-K342,'Dry Bulb'!L11-K226)","v":14.026273001460723},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M11-L342,'Dry Bulb'!M11-L226)","v":1.660432757975002},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N11-M342,'Dry Bulb'!N11-M226)","v":-3.715788720614789},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O11-N342,'Dry Bulb'!O11-N226)","v":-11.534452031025396},null,0.05,"Walls U- Value",null,null,null,null,null,null,3,null,null,null,null,null,null,null,null,null,"δ=",{"$f":"ATAN(AH10)","v":0.96007036240568799},null,null,null,null,null,null,{"$f":"'Incident angle'!BI11","v":7},{"$f":"'Incident angle'!BJ11","v":0},{"$f":"'Incident angle'!BK11","v":0},{"$f":"'Incident angle'!BL11","v":0},{"$f":"'Incident angle'!BM11","v":0},{"$f":"'Incident angle'!BN11","v":0},{"$f":"'Incident angle'!BO11","v":0},{"$f":"'Incident angle'!BP11","v":0},{"$f":"'Incident angle'!BQ11","v":0},{"$f":"'Incident angle'!BR11","v":0},{"$f":"'Incident angle'!BS11","v":0},{"$f":"'Incident angle'!BT11","v":0},{"$f":"'Incident angle'!BU11","v":1.519164678131067},{"$f":"MAX(AQ5:BB28)","v":3190.3469256777284},{"$f":"'Incident angle'!BW11","v":7},{"$f":"'Incident angle'!BX11","v":64.898513253972396},{"$f":"'Incident angle'!BY11","v":165.40677030899579},{"$f":"'Incident angle'!BZ11","v":477.20353172430015},{"$f":"'Incident angle'!CA11","v":1430.2072767776865},{"$f":"'Incident angle'!CB11","v":1823.5313692542443},{"$f":"'Incident angle'!CC11","v":1967.8167757820027},{"$f":"'Incident angle'!CD11","v":1633.0294584747032},{"$f":"'Incident angle'!CE11","v":1462.7309965171892},{"$f":"'Incident angle'!CF11","v":1232.2064066489952},{"$f":"'Incident angle'!CG11","v":786.71694263200231},{"$f":"'Incident angle'!CH11","v":234.94895166423882},{"$f":"'Incident angle'!CI11","v":96.370565382288561},null,{"$f":"'Profile angles'!B11","v":7},{"$f":"RADIANS('Profile angles'!C11)","v":3.2126378124526907E-2},{"$f":"RADIANS('Profile angles'!D11)","v":0.30400417987737721},{"$f":"RADIANS('Profile angles'!E11)","v":1.1397000015522967},{"$f":"RADIANS('Profile angles'!F11)","v":-1.2672818655170028},{"$f":"RADIANS('Profile angles'!G11)","v":-1.0116130508303163},{"$f":"RADIANS('Profile angles'!H11)","v":-0.90537507022991537},{"$f":"RADIANS('Profile angles'!I11)","v":-0.92689168179647397},{"$f":"RADIANS('Profile angles'!J11)","v":-1.2258417459156576},{"$f":"RADIANS('Profile angles'!K11)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L11)","v":0.56767922585481512},{"$f":"RADIANS('Profile angles'!M11)","v":0.23892272571930667},{"$f":"RADIANS('Profile angles'!N11)","v":6.6151862638080955E-2},0.46960488503776338,{"$f":"'Profile angles'!B40","v":7},{"$f":"RADIANS('Profile angles'!C40)","v":1.3214305906891738E-2},{"$f":"RADIANS('Profile angles'!D40)","v":7.6478952342661624E-2},{"$f":"RADIANS('Profile angles'!E40)","v":0.18024728429187561},{"$f":"RADIANS('Profile angles'!F40)","v":0.29926509663219786},{"$f":"RADIANS('Profile angles'!G40)","v":0.36886077540021189},{"$f":"RADIANS('Profile angles'!H40)","v":0.37484605769803392},{"$f":"RADIANS('Profile angles'!I40)","v":0.33410836517870207},{"$f":"RADIANS('Profile angles'!J40)","v":0.28700384937592222},{"$f":"RADIANS('Profile angles'!K40)","v":0.24026026153093516},{"$f":"RADIANS('Profile angles'!L40)","v":0.1938557876010461},{"$f":"RADIANS('Profile angles'!M40)","v":0.11359911050913243},{"$f":"RADIANS('Profile angles'!N40)","v":3.3555975837619691E-2},null,{"$f":"'Profile angles'!AD11","v":7},{"$f":"(IF($AH$12<DEGREES(BS11),0+$AJ$16,1-((TAN(BS11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT11),0+$AJ$16,1-((TAN(BT11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU11),0+$AJ$16,1-((TAN(BU11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV11),0+$AJ$16,1-((TAN(BV11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW11),0+$AJ$16,1-((TAN(BW11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX11),0+$AJ$16,1-((TAN(BX11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY11),0+$AJ$16,1-((TAN(BY11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ11),0+$AJ$16,1-((TAN(BZ11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA11),0+$AJ$16,1-((TAN(CA11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB11),0+$AJ$16,1-((TAN(CB11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC11),0+$AJ$16,1-((TAN(CC11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH10*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD11),0+$AJ$16,1-((TAN(CD11)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI10*$DU$3)+1-$DU$3)","v":1.2622168932142087E-2},null,7,{"$f":"(IF($AH$46<DEGREES(CG11),0+$AJ$50,1-((TAN(CG11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL10*$DU$3)+1-$DU$3)","v":0.78809867039882386},{"$f":"(IF($AH$46<DEGREES(CH11),0+$AJ$50,1-((TAN(CH11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM10*$DU$3)+1-$DU$3)","v":0.83751276190540225},{"$f":"(IF($AH$46<DEGREES(CI11),0+$AJ$50,1-((TAN(CI11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN10*$DU$3)+1-$DU$3)","v":0.85333983124613355},{"$f":"(IF($AH$46<DEGREES(CJ11),0+$AJ$50,1-((TAN(CJ11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO10*$DU$3)+1-$DU$3)","v":0.77551058729559219},{"$f":"(IF($AH$46<DEGREES(CK11),0+$AJ$50,1-((TAN(CK11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP10*$DU$3)+1-$DU$3)","v":0.67516654410550792},{"$f":"(IF($AH$46<DEGREES(CL11),0+$AJ$50,1-((TAN(CL11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ10*$DU$3)+1-$DU$3)","v":0.64598372329840192},{"$f":"(IF($AH$46<DEGREES(CM11),0+$AJ$50,1-((TAN(CM11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR10*$DU$3)+1-$DU$3)","v":0.68858067773946008},{"$f":"(IF($AH$46<DEGREES(CN11),0+$AJ$50,1-((TAN(CN11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS10*$DU$3)+1-$DU$3)","v":0.7792717305216641},{"$f":"(IF($AH$46<DEGREES(CO11),0+$AJ$50,1-((TAN(CO11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT10*$DU$3)+1-$DU$3)","v":0.80494448577423805},{"$f":"(IF($AH$46<DEGREES(CP11),0+$AJ$50,1-((TAN(CP11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU10*$DU$3)+1-$DU$3)","v":0.74640968095491789},{"$f":"(IF($AH$46<DEGREES(CQ11),0+$AJ$50,1-((TAN(CQ11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV10*$DU$3)+1-$DU$3)","v":0.71337841542490055},{"$f":"(IF($AH$46<DEGREES(CR11),0+$AJ$50,1-((TAN(CR11)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW10*$DU$3)+1-$DU$3)","v":0.73160830296466151},null,null,{"$f":"'Profile angles'!AR11","v":7},{"$f":"'Profile angles'!AS11","v":0.70023973357815916},{"$f":"'Profile angles'!AT11","v":4.2572512510716702},{"$f":"'Profile angles'!AU11","v":10.292097151668541},{"$f":"'Profile angles'!AV11","v":17.071764306110264},{"$f":"'Profile angles'!AW11","v":20.59199880999245},{"$f":"'Profile angles'!AX11","v":20.602944398333847},{"$f":"'Profile angles'!AY11","v":18.567526961418682},{"$f":"'Profile angles'!AZ11","v":16.357318748220177},{"$f":"'Profile angles'!BA11","v":13.682588857300253},{"$f":"'Profile angles'!BB11","v":10.626902061270702},{"$f":"'Profile angles'!BC11","v":5.8987575020687171},{"$f":"'Profile angles'!BD11","v":1.7151458456731048},null,7,0.70023973357815916,4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048]
[null,8,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D12-C343,'Dry Bulb'!D12-C227)","v":-9.3760122870067448},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E12-D343,'Dry Bulb'!E12-D227)","v":-4.9568521148914542},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F12-E343,'Dry Bulb'!F12-E227)","v":-3.2671314893503762},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G12-F343,'Dry Bulb'!G12-F227)","v":8.6789458666020209},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H12-G343,'Dry Bulb'!H12-G227)","v":20.874199895431076},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I12-H343,'Dry Bulb'!I12-H227)","v":26.820958513092975},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J12-I343,'Dry Bulb'!J12-I227)","v":28.217556789967638},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K12-J343,'Dry Bulb'!K12-J227)","v":28.406358852135043},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L12-K343,'Dry Bulb'!L12-K227)","v":22.326637148825441},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M12-L343,'Dry Bulb'!M12-L227)","v":9.9314300110390832},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N12-M343,'Dry Bulb'!N12-M227)","v":-2.6644106943546788},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O12-N343,'Dry Bulb'!O12-N227)","v":-7.6300752560144502},null,null,null,null,null,null,null,null,null,4,null,null,null,null,null,null,null," Profile Angle δ=",null,{"$f":"DEGREES(AI11)","v":55.007979801441337},null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI12","v":8},{"$f":"'Incident angle'!BJ12","v":127.30130569019155},{"$f":"'Incident angle'!BK12","v":0},{"$f":"'Incident angle'!BL12","v":0},{"$f":"'Incident angle'!BM12","v":0},{"$f":"'Incident angle'!BN12","v":0},{"$f":"'Incident angle'!BO12","v":0},{"$f":"'Incident angle'!BP12","v":0},{"$f":"'Incident angle'!BQ12","v":0},{"$f":"'Incident angle'!BR12","v":0},{"$f":"'Incident angle'!BS12","v":0},{"$f":"'Incident angle'!BT12","v":364.2388710559141},{"$f":"'Incident angle'!BU12","v":311.04236889499981},null,{"$f":"'Incident angle'!BW12","v":8},{"$f":"'Incident angle'!BX12","v":1114.2916837321102},{"$f":"'Incident angle'!BY12","v":1580.2679856218936},{"$f":"'Incident angle'!BZ12","v":2274.2562020804671},{"$f":"'Incident angle'!CA12","v":3450.0632210657404},{"$f":"'Incident angle'!CB12","v":3430.0891695915338},{"$f":"'Incident angle'!CC12","v":3624.4253921251366},{"$f":"'Incident angle'!CD12","v":3506.0504040840974},{"$f":"'Incident angle'!CE12","v":3701.4693967750522},{"$f":"'Incident angle'!CF12","v":3245.9243592338794},{"$f":"'Incident angle'!CG12","v":2588.9845220993402},{"$f":"'Incident angle'!CH12","v":1561.7415122729005},{"$f":"'Incident angle'!CI12","v":997.28150482434762},null,{"$f":"'Profile angles'!B12","v":8},{"$f":"RADIANS('Profile angles'!C12)","v":0.43903721208086555},{"$f":"RADIANS('Profile angles'!D12)","v":0.71921811629902932},{"$f":"RADIANS('Profile angles'!E12)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F12)","v":1.5556802149681459},{"$f":"RADIANS('Profile angles'!G12)","v":-1.3507534128601013},{"$f":"RADIANS('Profile angles'!H12)","v":-1.2538060729022262},{"$f":"RADIANS('Profile angles'!I12)","v":-1.3073051411080621},{"$f":"RADIANS('Profile angles'!J12)","v":-1.5687141806333273},{"$f":"RADIANS('Profile angles'!K12)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L12)","v":0.7977743448011565},{"$f":"RADIANS('Profile angles'!M12)","v":0.53602537178498577},{"$f":"RADIANS('Profile angles'!N12)","v":0.40375311848675605},0.72984443156068801,{"$f":"'Profile angles'!B41","v":8},{"$f":"RADIANS('Profile angles'!C41)","v":0.25833513602163805},{"$f":"RADIANS('Profile angles'!D41)","v":0.3210561315745496},{"$f":"RADIANS('Profile angles'!E41)","v":0.42271676310413814},{"$f":"RADIANS('Profile angles'!F41)","v":0.53547976766771499},{"$f":"RADIANS('Profile angles'!G41)","v":0.59803922283315158},{"$f":"RADIANS('Profile angles'!H41)","v":0.600853618256177},{"$f":"RADIANS('Profile angles'!I41)","v":0.5629740216332968},{"$f":"RADIANS('Profile angles'!J41)","v":0.52288181283223811},{"$f":"RADIANS('Profile angles'!K41)","v":0.484596524210885},{"$f":"RADIANS('Profile angles'!L41)","v":0.44426219941003875},{"$f":"RADIANS('Profile angles'!M41)","v":0.36546054525287114},{"$f":"RADIANS('Profile angles'!N41)","v":0.28151379860305881},null,{"$f":"'Profile angles'!AD12","v":8},{"$f":"(IF($AH$12<DEGREES(BS12),0+$AJ$16,1-((TAN(BS12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX11*$DU$3)+1-$DU$3)","v":7.4782517460029521E-2},{"$f":"(IF($AH$12<DEGREES(BT12),0+$AJ$16,1-((TAN(BT12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY11*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU12),0+$AJ$16,1-((TAN(BU12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ11*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV12),0+$AJ$16,1-((TAN(BV12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA11*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW12),0+$AJ$16,1-((TAN(BW12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB11*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX12),0+$AJ$16,1-((TAN(BX12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC11*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY12),0+$AJ$16,1-((TAN(BY12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD11*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ12),0+$AJ$16,1-((TAN(BZ12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE11*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA12),0+$AJ$16,1-((TAN(CA12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF11*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB12),0+$AJ$16,1-((TAN(CB12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG11*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC12),0+$AJ$16,1-((TAN(CC12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH11*$DU$3)+1-$DU$3)","v":0.13072714577991293},{"$f":"(IF($AH$12<DEGREES(CD12),0+$AJ$16,1-((TAN(CD12)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI11*$DU$3)+1-$DU$3)","v":0.18319392582245905},null,8,{"$f":"(IF($AH$46<DEGREES(CG12),0+$AJ$50,1-((TAN(CG12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL11*$DU$3)+1-$DU$3)","v":0.60471879746915114},{"$f":"(IF($AH$46<DEGREES(CH12),0+$AJ$50,1-((TAN(CH12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM11*$DU$3)+1-$DU$3)","v":0.64846565314926308},{"$f":"(IF($AH$46<DEGREES(CI12),0+$AJ$50,1-((TAN(CI12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN11*$DU$3)+1-$DU$3)","v":0.65456984898263215},{"$f":"(IF($AH$46<DEGREES(CJ12),0+$AJ$50,1-((TAN(CJ12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO11*$DU$3)+1-$DU$3)","v":0.64113080818617008},{"$f":"(IF($AH$46<DEGREES(CK12),0+$AJ$50,1-((TAN(CK12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP11*$DU$3)+1-$DU$3)","v":0.54619765527385522},{"$f":"(IF($AH$46<DEGREES(CL12),0+$AJ$50,1-((TAN(CL12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ11*$DU$3)+1-$DU$3)","v":0.5225753536730301},{"$f":"(IF($AH$46<DEGREES(CM12),0+$AJ$50,1-((TAN(CM12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR11*$DU$3)+1-$DU$3)","v":0.56844899007188843},{"$f":"(IF($AH$46<DEGREES(CN12),0+$AJ$50,1-((TAN(CN12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS11*$DU$3)+1-$DU$3)","v":0.65377062785156492},{"$f":"(IF($AH$46<DEGREES(CO12),0+$AJ$50,1-((TAN(CO12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT11*$DU$3)+1-$DU$3)","v":0.60129059129345042},{"$f":"(IF($AH$46<DEGREES(CP12),0+$AJ$50,1-((TAN(CP12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU11*$DU$3)+1-$DU$3)","v":0.54853185326306253},{"$f":"(IF($AH$46<DEGREES(CQ12),0+$AJ$50,1-((TAN(CQ12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV11*$DU$3)+1-$DU$3)","v":0.5222806781548619},{"$f":"(IF($AH$46<DEGREES(CR12),0+$AJ$50,1-((TAN(CR12)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW11*$DU$3)+1-$DU$3)","v":0.54675451397073982},null,null,{"$f":"'Profile angles'!AR12","v":8},{"$f":"'Profile angles'!AS12","v":12.968359542715392},{"$f":"'Profile angles'!AT12","v":17.270303982095768},{"$f":"'Profile angles'!AU12","v":23.773745192987032},{"$f":"'Profile angles'!AV12","v":30.67971943621767},{"$f":"'Profile angles'!AW12","v":33.959814353189685},{"$f":"'Profile angles'!AX12","v":33.770494749028082},{"$f":"'Profile angles'!AY12","v":31.887744015481577},{"$f":"'Profile angles'!AZ12","v":29.958903207045175},{"$f":"'Profile angles'!BA12","v":27.097900221004789},{"$f":"'Profile angles'!BB12","v":23.350930400204959},{"$f":"'Profile angles'!BC12","v":17.832347455280527},{"$f":"'Profile angles'!BD12","v":13.467847656409182},null,8,12.968359542715392,17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182]
[null,9,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D13-C344,'Dry Bulb'!D13-C228)","v":-3.8307478163317086},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E13-D344,'Dry Bulb'!E13-D228)","v":-0.26975203807860737},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F13-E344,'Dry Bulb'!F13-E228)","v":9.6470537321067695E-2},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G13-F344,'Dry Bulb'!G13-F228)","v":13.822149310167518},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H13-G344,'Dry Bulb'!H13-G228)","v":23.320892336433516},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I13-H344,'Dry Bulb'!I13-H228)","v":29.823511787142095},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J13-I344,'Dry Bulb'!J13-I228)","v":32.94307428804386},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K13-J344,'Dry Bulb'!K13-J228)","v":33.321540665395574},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L13-K344,'Dry Bulb'!L13-K228)","v":26.671003272848608},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M13-L344,'Dry Bulb'!M13-L228)","v":15.775618718326349},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N13-M344,'Dry Bulb'!N13-M228)","v":2.9265763640708542},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O13-N344,'Dry Bulb'!O13-N228)","v":-2.784971452619736},null,0.04,"Roof U-Value",null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI13","v":9},{"$f":"'Incident angle'!BJ13","v":811.47757221825918},{"$f":"'Incident angle'!BK13","v":118.60410379936748},{"$f":"'Incident angle'!BL13","v":0},{"$f":"'Incident angle'!BM13","v":0},{"$f":"'Incident angle'!BN13","v":0},{"$f":"'Incident angle'!BO13","v":0},{"$f":"'Incident angle'!BP13","v":0},{"$f":"'Incident angle'!BQ13","v":0},{"$f":"'Incident angle'!BR13","v":0},{"$f":"'Incident angle'!BS13","v":318.42639417912727},{"$f":"'Incident angle'!BT13","v":1182.1451144318978},{"$f":"'Incident angle'!BU13","v":959.6028110723438},null,{"$f":"'Incident angle'!BW13","v":9},{"$f":"'Incident angle'!BX13","v":1937.7499286029749},{"$f":"'Incident angle'!BY13","v":2419.2010350237315},{"$f":"'Incident angle'!BZ13","v":2912.014825963},{"$f":"'Incident angle'!CA13","v":3360.4158657250155},{"$f":"'Incident angle'!CB13","v":3200.4903267677082},{"$f":"'Incident angle'!CC13","v":3403.2308082119139},{"$f":"'Incident angle'!CD13","v":3720.9239883772384},{"$f":"'Incident angle'!CE13","v":3826.0863600764724},{"$f":"'Incident angle'!CF13","v":3354.2128592006602},{"$f":"'Incident angle'!CG13","v":2669.6329341940491},{"$f":"'Incident angle'!CH13","v":1917.4960014801416},{"$f":"'Incident angle'!CI13","v":1389.9804404707747},null,{"$f":"'Profile angles'!B13","v":9},{"$f":"RADIANS('Profile angles'!C13)","v":0.63047626333736551},{"$f":"RADIANS('Profile angles'!D13)","v":0.85493388322458175},{"$f":"RADIANS('Profile angles'!E13)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!F13)","v":1.4368234130045157},{"$f":"RADIANS('Profile angles'!G13)","v":-1.5128901286207534},{"$f":"RADIANS('Profile angles'!H13)","v":-1.4342637641927436},{"$f":"RADIANS('Profile angles'!I13)","v":-1.4895751772040409},{"$f":"RADIANS('Profile angles'!J13)","v":1.4463354753784508},{"$f":"RADIANS('Profile angles'!K13)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L13)","v":0.88713181190644863},{"$f":"RADIANS('Profile angles'!M13)","v":0.67791492684215882},{"$f":"RADIANS('Profile angles'!N13)","v":0.57836247588490297},0.88676638434154909,{"$f":"'Profile angles'!B42","v":9},{"$f":"RADIANS('Profile angles'!C42)","v":0.52181610509407761},{"$f":"RADIANS('Profile angles'!D42)","v":0.57895326435114869},{"$f":"RADIANS('Profile angles'!E42)","v":0.6743232952298458},{"$f":"RADIANS('Profile angles'!F42)","v":0.77696351285009768},{"$f":"RADIANS('Profile angles'!G42)","v":0.83009780925872156},{"$f":"RADIANS('Profile angles'!H42)","v":0.82868950102189065},{"$f":"RADIANS('Profile angles'!I42)","v":0.79414344815942139},{"$f":"RADIANS('Profile angles'!J42)","v":0.76376137451897885},{"$f":"RADIANS('Profile angles'!K42)","v":0.73908870770470358},{"$f":"RADIANS('Profile angles'!L42)","v":0.71062378761726053},{"$f":"RADIANS('Profile angles'!M42)","v":0.63870702042109351},{"$f":"RADIANS('Profile angles'!N42)","v":0.55159011300440908},null,{"$f":"'Profile angles'!AD13","v":9},{"$f":"(IF($AH$12<DEGREES(BS13),0+$AJ$16,1-((TAN(BS13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX12*$DU$3)+1-$DU$3)","v":0.17868418497963579},{"$f":"(IF($AH$12<DEGREES(BT13),0+$AJ$16,1-((TAN(BT13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY12*$DU$3)+1-$DU$3)","v":2.353385462054166E-2},{"$f":"(IF($AH$12<DEGREES(BU13),0+$AJ$16,1-((TAN(BU13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ12*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV13),0+$AJ$16,1-((TAN(BV13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA12*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW13),0+$AJ$16,1-((TAN(BW13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB12*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX13),0+$AJ$16,1-((TAN(BX13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC12*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY13),0+$AJ$16,1-((TAN(BY13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD12*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ13),0+$AJ$16,1-((TAN(BZ13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE12*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA13),0+$AJ$16,1-((TAN(CA13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF12*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB13),0+$AJ$16,1-((TAN(CB13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG12*$DU$3)+1-$DU$3)","v":4.040611213699094E-2},{"$f":"(IF($AH$12<DEGREES(CC13),0+$AJ$16,1-((TAN(CC13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH12*$DU$3)+1-$DU$3)","v":0.19975595994445283},{"$f":"(IF($AH$12<DEGREES(CD13),0+$AJ$16,1-((TAN(CD13)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI12*$DU$3)+1-$DU$3)","v":0.25494621311619342},null,9,{"$f":"(IF($AH$46<DEGREES(CG13),0+$AJ$50,1-((TAN(CG13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL12*$DU$3)+1-$DU$3)","v":0.39700233209577623},{"$f":"(IF($AH$46<DEGREES(CH13),0+$AJ$50,1-((TAN(CH13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM12*$DU$3)+1-$DU$3)","v":0.4350153181294979},{"$f":"(IF($AH$46<DEGREES(CI13),0+$AJ$50,1-((TAN(CI13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN12*$DU$3)+1-$DU$3)","v":0.42474787977658701},{"$f":"(IF($AH$46<DEGREES(CJ13),0+$AJ$50,1-((TAN(CJ13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO12*$DU$3)+1-$DU$3)","v":0.38286695379052571},{"$f":"(IF($AH$46<DEGREES(CK13),0+$AJ$50,1-((TAN(CK13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP12*$DU$3)+1-$DU$3)","v":0.33291258954637587},{"$f":"(IF($AH$46<DEGREES(CL13),0+$AJ$50,1-((TAN(CL13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ12*$DU$3)+1-$DU$3)","v":0.31976890558358645},{"$f":"(IF($AH$46<DEGREES(CM13),0+$AJ$50,1-((TAN(CM13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR12*$DU$3)+1-$DU$3)","v":0.37328399227410625},{"$f":"(IF($AH$46<DEGREES(CN13),0+$AJ$50,1-((TAN(CN13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS12*$DU$3)+1-$DU$3)","v":0.39993400169631432},{"$f":"(IF($AH$46<DEGREES(CO13),0+$AJ$50,1-((TAN(CO13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT12*$DU$3)+1-$DU$3)","v":0.35816682101121894},{"$f":"(IF($AH$46<DEGREES(CP13),0+$AJ$50,1-((TAN(CP13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU12*$DU$3)+1-$DU$3)","v":0.3140760181313233},{"$f":"(IF($AH$46<DEGREES(CQ13),0+$AJ$50,1-((TAN(CQ13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV12*$DU$3)+1-$DU$3)","v":0.29882099852672483},{"$f":"(IF($AH$46<DEGREES(CR13),0+$AJ$50,1-((TAN(CR13)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW12*$DU$3)+1-$DU$3)","v":0.33354643946996582},null,null,{"$f":"'Profile angles'!AR13","v":9},{"$f":"'Profile angles'!AS13","v":24.306538235547787},{"$f":"'Profile angles'!AT13","v":29.607456719563572},{"$f":"'Profile angles'!AU13","v":36.877998514340362},{"$f":"'Profile angles'!AV13","v":44.267398869292073},{"$f":"'Profile angles'!AW13","v":47.503865138538167},{"$f":"'Profile angles'!AX13","v":47.16345799134892},{"$f":"'Profile angles'!AY13","v":45.403126432581416},{"$f":"'Profile angles'!AZ13","v":43.556385601632783},{"$f":"'Profile angles'!BA13","v":40.048756889246128},{"$f":"'Profile angles'!BB13","v":35.170537312656599},{"$f":"'Profile angles'!BC13","v":28.628753160625717},{"$f":"'Profile angles'!BD13","v":24.120985503613159},null,9,24.306538235547787,29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159]
[null,10,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D14-C345,'Dry Bulb'!D14-C229)","v":-1.0620454725222359},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E14-D345,'Dry Bulb'!E14-D229)","v":-5.579009996875584},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F14-E345,'Dry Bulb'!F14-E229)","v":-1.8750275213188132},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G14-F345,'Dry Bulb'!G14-F229)","v":10.624946014897731},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H14-G345,'Dry Bulb'!H14-G229)","v":20.340806794055197},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I14-H345,'Dry Bulb'!I14-H229)","v":26.460806794055202},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J14-I345,'Dry Bulb'!J14-I229)","v":29.71671203781635},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K14-J345,'Dry Bulb'!K14-J229)","v":31.097918362343563},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L14-K345,'Dry Bulb'!L14-K229)","v":24.7590317353541},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M14-L345,'Dry Bulb'!M14-L229)","v":14.382010572980278},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N14-M345,'Dry Bulb'!N14-M229)","v":6.5285091644646798},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O14-N345,'Dry Bulb'!O14-N229)","v":0.25721240810639046},null,null,null,null,null,null,null,null,null,6,null,null,null,null,null,null,null,null,{"$f":"RADIANS(AH12)","v":0.96007036240568799},null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI14","v":10},{"$f":"'Incident angle'!BJ14","v":1506.6043106011446},{"$f":"'Incident angle'!BK14","v":314.83189335756248},{"$f":"'Incident angle'!BL14","v":0},{"$f":"'Incident angle'!BM14","v":0},{"$f":"'Incident angle'!BN14","v":0},{"$f":"'Incident angle'!BO14","v":0},{"$f":"'Incident angle'!BP14","v":0},{"$f":"'Incident angle'!BQ14","v":0},{"$f":"'Incident angle'!BR14","v":0},{"$f":"'Incident angle'!BS14","v":389.84762999128924},{"$f":"'Incident angle'!BT14","v":1971.8064351296152},{"$f":"'Incident angle'!BU14","v":1748.1686302643286},null,{"$f":"'Incident angle'!BW14","v":10},{"$f":"'Incident angle'!BX14","v":1183.6493446461352},{"$f":"'Incident angle'!BY14","v":1497.4376845479851},{"$f":"'Incident angle'!BZ14","v":1259.1168271411946},{"$f":"'Incident angle'!CA14","v":97.570769643937751},{"$f":"'Incident angle'!CB14","v":0},{"$f":"'Incident angle'!CC14","v":0},{"$f":"'Incident angle'!CD14","v":8.4277910379317671},{"$f":"'Incident angle'!CE14","v":454.16199224679519},{"$f":"'Incident angle'!CF14","v":433.5569407707585},{"$f":"'Incident angle'!CG14","v":363.21272236663583},{"$f":"'Incident angle'!CH14","v":456.08173339111073},{"$f":"'Incident angle'!CI14","v":591.97429448104697},null,{"$f":"'Profile angles'!B14","v":10},{"$f":"RADIANS('Profile angles'!C14)","v":0.72545541534435543},{"$f":"RADIANS('Profile angles'!D14)","v":0.91440329211687621},{"$f":"RADIANS('Profile angles'!E14)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!F14)","v":1.3820186383289426},{"$f":"RADIANS('Profile angles'!G14)","v":1.5469473133771072},{"$f":"RADIANS('Profile angles'!H14)","v":-1.52849748779825},{"$f":"RADIANS('Profile angles'!I14)","v":1.5604768548046379},{"$f":"RADIANS('Profile angles'!J14)","v":1.388309158935473},{"$f":"RADIANS('Profile angles'!K14)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L14)","v":0.92900496630503893},{"$f":"RADIANS('Profile angles'!M14)","v":0.74952134450991281},{"$f":"RADIANS('Profile angles'!N14)","v":0.66958505956359171},0.97525340062585675,{"$f":"'Profile angles'!B43","v":10},{"$f":"RADIANS('Profile angles'!C43)","v":0.8103914470438931},{"$f":"RADIANS('Profile angles'!D43)","v":0.85489906581681796},{"$f":"RADIANS('Profile angles'!E43)","v":0.93831409714073843},{"$f":"RADIANS('Profile angles'!F43)","v":1.0260828135826863},{"$f":"RADIANS('Profile angles'!G43)","v":1.0672108131256053},{"$f":"RADIANS('Profile angles'!H43)","v":1.0606626288594174},{"$f":"RADIANS('Profile angles'!I43)","v":1.0301037196118754},{"$f":"RADIANS('Profile angles'!J43)","v":1.0121306417701839},{"$f":"RADIANS('Profile angles'!K43)","v":1.0063600686241212},{"$f":"RADIANS('Profile angles'!L43)","v":0.99633099553482729},{"$f":"RADIANS('Profile angles'!M43)","v":0.93894687408658406},{"$f":"RADIANS('Profile angles'!N43)","v":0.85128249562502745},null,{"$f":"'Profile angles'!AD14","v":10},{"$f":"(IF($AH$12<DEGREES(BS14),0+$AJ$16,1-((TAN(BS14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX13*$DU$3)+1-$DU$3)","v":0.21930685397456046},{"$f":"(IF($AH$12<DEGREES(BT14),0+$AJ$16,1-((TAN(BT14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY13*$DU$3)+1-$DU$3)","v":3.9759298962938797E-2},{"$f":"(IF($AH$12<DEGREES(BU14),0+$AJ$16,1-((TAN(BU14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ13*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV14),0+$AJ$16,1-((TAN(BV14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA13*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW14),0+$AJ$16,1-((TAN(BW14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB13*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX14),0+$AJ$16,1-((TAN(BX14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC13*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY14),0+$AJ$16,1-((TAN(BY14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD13*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ14),0+$AJ$16,1-((TAN(BZ14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE13*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA14),0+$AJ$16,1-((TAN(CA14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF13*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB14),0+$AJ$16,1-((TAN(CB14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG13*$DU$3)+1-$DU$3)","v":3.5906579588347295E-2},{"$f":"(IF($AH$12<DEGREES(CC14),0+$AJ$16,1-((TAN(CC14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH13*$DU$3)+1-$DU$3)","v":0.22980114883775274},{"$f":"(IF($AH$12<DEGREES(CD14),0+$AJ$16,1-((TAN(CD14)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI13*$DU$3)+1-$DU$3)","v":0.29126109856164634},null,10,{"$f":"(IF($AH$46<DEGREES(CG14),0+$AJ$50,1-((TAN(CG14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL13*$DU$3)+1-$DU$3)","v":0.15036640083989539},{"$f":"(IF($AH$46<DEGREES(CH14),0+$AJ$50,1-((TAN(CH14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM13*$DU$3)+1-$DU$3)","v":0.17284854200125752},{"$f":"(IF($AH$46<DEGREES(CI14),0+$AJ$50,1-((TAN(CI14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN13*$DU$3)+1-$DU$3)","v":0.12445386723352218},{"$f":"(IF($AH$46<DEGREES(CJ14),0+$AJ$50,1-((TAN(CJ14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO13*$DU$3)+1-$DU$3)","v":8.1402530192372577E-3},{"$f":"(IF($AH$46<DEGREES(CK14),0+$AJ$50,1-((TAN(CK14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP13*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CL14),0+$AJ$50,1-((TAN(CL14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ13*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CM14),0+$AJ$50,1-((TAN(CM14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR13*$DU$3)+1-$DU$3)","v":6.1344273776698949E-4},{"$f":"(IF($AH$46<DEGREES(CN14),0+$AJ$50,1-((TAN(CN14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS13*$DU$3)+1-$DU$3)","v":3.4216411547719434E-2},{"$f":"(IF($AH$46<DEGREES(CO14),0+$AJ$50,1-((TAN(CO14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT13*$DU$3)+1-$DU$3)","v":3.3336792963262578E-2},{"$f":"(IF($AH$46<DEGREES(CP14),0+$AJ$50,1-((TAN(CP14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU13*$DU$3)+1-$DU$3)","v":3.088113139396775E-2},{"$f":"(IF($AH$46<DEGREES(CQ14),0+$AJ$50,1-((TAN(CQ14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV13*$DU$3)+1-$DU$3)","v":4.7958523399922903E-2},{"$f":"(IF($AH$46<DEGREES(CR14),0+$AJ$50,1-((TAN(CR14)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW13*$DU$3)+1-$DU$3)","v":8.7984454630283357E-2},null,null,{"$f":"'Profile angles'!AR14","v":10},{"$f":"'Profile angles'!AS14","v":34.130498638110296},{"$f":"'Profile angles'!AT14","v":40.716949463115029},{"$f":"'Profile angles'!AU14","v":49.130640449349286},{"$f":"'Profile angles'!AV14","v":57.573642107854539},{"$f":"'Profile angles'!AW14","v":61.123995517612983},{"$f":"'Profile angles'!AX14","v":60.701791836412639},{"$f":"'Profile angles'!AY14","v":59.016860616830343},{"$f":"'Profile angles'!AZ14","v":56.905164678924855},{"$f":"'Profile angles'!BA14","v":51.954064465377563},{"$f":"'Profile angles'!BB14","v":45.326184070335216},{"$f":"'Profile angles'!BC14","v":37.566870997040184},{"$f":"'Profile angles'!BD14","v":33.04159126014769},null,10,34.130498638110296,40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,37.566870997040184,33.04159126014769]
[null,11,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D15-C346,'Dry Bulb'!D15-C230)","v":0.41408205805853981},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E15-D346,'Dry Bulb'!E15-D230)","v":-5.1145703587918234},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F15-E346,'Dry Bulb'!F15-E230)","v":-1.1523863269639065},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G15-F346,'Dry Bulb'!G15-F230)","v":13.320806794055201},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H15-G346,'Dry Bulb'!H15-G230)","v":22.860806794055208},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I15-H346,'Dry Bulb'!I15-H230)","v":29.160806794055205},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J15-I346,'Dry Bulb'!J15-I230)","v":32.580806794055206},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K15-J346,'Dry Bulb'!K15-J230)","v":33.660806794055205},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L15-K346,'Dry Bulb'!L15-K230)","v":26.460806794055202},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M15-L346,'Dry Bulb'!M15-L230)","v":16.50128449199542},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N15-M346,'Dry Bulb'!N15-M230)","v":11.408652454865532},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O15-N346,'Dry Bulb'!O15-N230)","v":-3.4765389620963063},null,75,"Thermostat Setpoint",null,null,68,null,null,null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI15","v":11},{"$f":"'Incident angle'!BJ15","v":2137.1317305137704},{"$f":"'Incident angle'!BK15","v":246.19203113518182},{"$f":"'Incident angle'!BL15","v":0},{"$f":"'Incident angle'!BM15","v":0},{"$f":"'Incident angle'!BN15","v":0},{"$f":"'Incident angle'!BO15","v":0},{"$f":"'Incident angle'!BP15","v":0},{"$f":"'Incident angle'!BQ15","v":0},{"$f":"'Incident angle'!BR15","v":0},{"$f":"'Incident angle'!BS15","v":254.59312019607125},{"$f":"'Incident angle'!BT15","v":2668.0021945218805},{"$f":"'Incident angle'!BU15","v":2449.42891745922},null,{"$f":"'Incident angle'!BW15","v":11},{"$f":"'Incident angle'!BX15","v":0},{"$f":"'Incident angle'!BY15","v":0},{"$f":"'Incident angle'!BZ15","v":0},{"$f":"'Incident angle'!CA15","v":0},{"$f":"'Incident angle'!CB15","v":0},{"$f":"'Incident angle'!CC15","v":0},{"$f":"'Incident angle'!CD15","v":0},{"$f":"'Incident angle'!CE15","v":0},{"$f":"'Incident angle'!CF15","v":0},{"$f":"'Incident angle'!CG15","v":0},{"$f":"'Incident angle'!CH15","v":0},{"$f":"'Incident angle'!CI15","v":0},null,{"$f":"'Profile angles'!B15","v":11},{"$f":"RADIANS('Profile angles'!C15)","v":0.77287050251262801},{"$f":"RADIANS('Profile angles'!D15)","v":0.94279982780897686},{"$f":"RADIANS('Profile angles'!E15)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F15)","v":1.3560531209708369},{"$f":"RADIANS('Profile angles'!G15)","v":1.5069809238556897},{"$f":"RADIANS('Profile angles'!H15)","v":1.5658083868258721},{"$f":"RADIANS('Profile angles'!I15)","v":1.5149166606406734},{"$f":"RADIANS('Profile angles'!J15)","v":1.3606731060385546},{"$f":"RADIANS('Profile angles'!K15)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L15)","v":0.94820534202278628},{"$f":"RADIANS('Profile angles'!M15)","v":0.78354196814002852},{"$f":"RADIANS('Profile angles'!N15)","v":0.71507325853303161},1.0119813555866832,{"$f":"'Profile angles'!B44","v":11},{"$f":"RADIANS('Profile angles'!C44)","v":1.1268272200794016},{"$f":"RADIANS('Profile angles'!D44)","v":1.1501949201099215},{"$f":"RADIANS('Profile angles'!E44)","v":1.2149427363314722},{"$f":"RADIANS('Profile angles'!F44)","v":1.2827675748177341},{"$f":"RADIANS('Profile angles'!G44)","v":1.3094800079043547},{"$f":"RADIANS('Profile angles'!H44)","v":1.2971248839107501},{"$f":"RADIANS('Profile angles'!I44)","v":1.2712928251657776},{"$f":"RADIANS('Profile angles'!J44)","v":1.2680765910530094},{"$f":"RADIANS('Profile angles'!K44)","v":1.2857310025410151},{"$f":"RADIANS('Profile angles'!L44)","v":1.3000930619226609},{"$f":"RADIANS('Profile angles'!M44)","v":1.2658856481778871},{"$f":"RADIANS('Profile angles'!N44)","v":1.1829208364741319},null,{"$f":"'Profile angles'!AD15","v":11},{"$f":"(IF($AH$12<DEGREES(BS15),0+$AJ$16,1-((TAN(BS15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX14*$DU$3)+1-$DU$3)","v":0.2437247161517396},{"$f":"(IF($AH$12<DEGREES(BT15),0+$AJ$16,1-((TAN(BT15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY14*$DU$3)+1-$DU$3)","v":2.482773065723759E-2},{"$f":"(IF($AH$12<DEGREES(BU15),0+$AJ$16,1-((TAN(BU15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV15),0+$AJ$16,1-((TAN(BV15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW15),0+$AJ$16,1-((TAN(BW15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX15),0+$AJ$16,1-((TAN(BX15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY15),0+$AJ$16,1-((TAN(BY15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ15),0+$AJ$16,1-((TAN(BZ15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA15),0+$AJ$16,1-((TAN(CA15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB15),0+$AJ$16,1-((TAN(CB15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG14*$DU$3)+1-$DU$3)","v":2.0034938071647225E-2},{"$f":"(IF($AH$12<DEGREES(CC15),0+$AJ$16,1-((TAN(CC15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH14*$DU$3)+1-$DU$3)","v":0.25515337210891015},{"$f":"(IF($AH$12<DEGREES(CD15),0+$AJ$16,1-((TAN(CD15)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI14*$DU$3)+1-$DU$3)","v":0.32256427887986583},null,11,{"$f":"(IF($AH$46<DEGREES(CG15),0+$AJ$50,1-((TAN(CG15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CH15),0+$AJ$50,1-((TAN(CH15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CI15),0+$AJ$50,1-((TAN(CI15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CJ15),0+$AJ$50,1-((TAN(CJ15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CK15),0+$AJ$50,1-((TAN(CK15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CL15),0+$AJ$50,1-((TAN(CL15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CM15),0+$AJ$50,1-((TAN(CM15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CN15),0+$AJ$50,1-((TAN(CN15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CO15),0+$AJ$50,1-((TAN(CO15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CP15),0+$AJ$50,1-((TAN(CP15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CQ15),0+$AJ$50,1-((TAN(CQ15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV14*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CR15),0+$AJ$50,1-((TAN(CR15)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW14*$DU$3)+1-$DU$3)","v":0},null,null,{"$f":"'Profile angles'!AR15","v":11},{"$f":"'Profile angles'!AS15","v":41.499338482119107},{"$f":"'Profile angles'!AT15","v":49.543356395157261},{"$f":"'Profile angles'!AU15","v":59.402009530792824},{"$f":"'Profile angles'!AV15","v":69.801829865076741},{"$f":"'Profile angles'!AW15","v":74.625870049112294},{"$f":"'Profile angles'!AX15","v":74.317427946135254},{"$f":"'Profile angles'!AY15","v":72.577202871970812},{"$f":"'Profile angles'!AZ15","v":69.283885987295108},{"$f":"'Profile angles'!BA15","v":61.393251168859464},{"$f":"'Profile angles'!BB15","v":52.417946997507137},{"$f":"'Profile angles'!BC15","v":43.550952586854685},{"$f":"'Profile angles'!BD15","v":39.297011346471983},null,11,41.499338482119107,49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983]
[null,12,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D16-C347,'Dry Bulb'!D16-C231)","v":-3.0776873526078887},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E16-D347,'Dry Bulb'!E16-D231)","v":-4.6700025913142156},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F16-E347,'Dry Bulb'!F16-E231)","v":0.83975966029723281},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G16-F347,'Dry Bulb'!G16-F231)","v":15.480806794055212},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H16-G347,'Dry Bulb'!H16-G231)","v":24.840806794055197},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I16-H347,'Dry Bulb'!I16-H231)","v":31.500806794055208},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J16-I347,'Dry Bulb'!J16-I231)","v":34.380806794055204},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K16-J347,'Dry Bulb'!K16-J231)","v":35.640806794055194},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L16-K347,'Dry Bulb'!L16-K231)","v":28.260806794055199},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M16-L347,'Dry Bulb'!M16-L231)","v":18.917013787418355},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N16-M347,'Dry Bulb'!N16-M231)","v":15.493334806657664},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O16-N347,'Dry Bulb'!O16-N231)","v":-0.16028998863284016},null,null,null,null,null,null,null,null,null,8,null,null,null,"Transmittance of Shade Material",null,null,null,null,null,null,null,0,null,null,null,null,null,{"$f":"'Incident angle'!BI16","v":12},{"$f":"'Incident angle'!BJ16","v":2660.7704140368955},{"$f":"'Incident angle'!BK16","v":129.99219692738231},{"$f":"'Incident angle'!BL16","v":0},{"$f":"'Incident angle'!BM16","v":0},{"$f":"'Incident angle'!BN16","v":0},{"$f":"'Incident angle'!BO16","v":0},{"$f":"'Incident angle'!BP16","v":0},{"$f":"'Incident angle'!BQ16","v":0},{"$f":"'Incident angle'!BR16","v":0},{"$f":"'Incident angle'!BS16","v":199.34268060830314},{"$f":"'Incident angle'!BT16","v":3190.3469256777284},{"$f":"'Incident angle'!BU16","v":3062.0963422731697},null,{"$f":"'Incident angle'!BW16","v":12},{"$f":"'Incident angle'!BX16","v":0},{"$f":"'Incident angle'!BY16","v":0},{"$f":"'Incident angle'!BZ16","v":0},{"$f":"'Incident angle'!CA16","v":0},{"$f":"'Incident angle'!CB16","v":0},{"$f":"'Incident angle'!CC16","v":0},{"$f":"'Incident angle'!CD16","v":0},{"$f":"'Incident angle'!CE16","v":0},{"$f":"'Incident angle'!CF16","v":0},{"$f":"'Incident angle'!CG16","v":0},{"$f":"'Incident angle'!CH16","v":0},{"$f":"'Incident angle'!CI16","v":0},null,{"$f":"'Profile angles'!B16","v":12},{"$f":"RADIANS('Profile angles'!C16)","v":0.79135309629409845},{"$f":"RADIANS('Profile angles'!D16)","v":0.95393106557871754},{"$f":"RADIANS('Profile angles'!E16)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F16)","v":1.3474641185275609},{"$f":"RADIANS('Profile angles'!G16)","v":1.494047359637104},{"$f":"RADIANS('Profile angles'!H16)","v":1.549232894297323},{"$f":"RADIANS('Profile angles'!I16)","v":1.498048297172524},{"$f":"RADIANS('Profile angles'!J16)","v":1.3510622858662449},{"$f":"RADIANS('Profile angles'!K16)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L16)","v":0.95283102870472114},{"$f":"RADIANS('Profile angles'!M16)","v":0.79224403056524917},{"$f":"RADIANS('Profile angles'!N16)","v":0.73031386460610437},1.0032623523950577,{"$f":"'Profile angles'!B45","v":12},{"$f":"RADIANS('Profile angles'!C45)","v":1.4652572312778287},{"$f":"RADIANS('Profile angles'!D45)","v":1.4603602289474145},{"$f":"RADIANS('Profile angles'!E45)","v":1.5005364967084425},{"$f":"RADIANS('Profile angles'!F45)","v":1.5443810972198111},{"$f":"RADIANS('Profile angles'!G45)","v":1.555062909254763},{"$f":"RADIANS('Profile angles'!H45)","v":1.536631166126466},{"$f":"RADIANS('Profile angles'!I45)","v":1.5161625036324029},{"$f":"RADIANS('Profile angles'!J45)","v":1.5291230837920124},{"$f":"RADIANS('Profile angles'!K45)","v":1.5690353246394675},{"$f":"RADIANS('Profile angles'!L45)","v":1.5273206771977748},{"$f":"RADIANS('Profile angles'!M45)","v":1.5323869921532096},{"$f":"RADIANS('Profile angles'!N45)","v":1.537600907178335},null,{"$f":"'Profile angles'!AD16","v":12},{"$f":"(IF($AH$12<DEGREES(BS16),0+$AJ$16,1-((TAN(BS16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX15*$DU$3)+1-$DU$3)","v":0.2759823122306071},{"$f":"(IF($AH$12<DEGREES(BT16),0+$AJ$16,1-((TAN(BT16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY15*$DU$3)+1-$DU$3)","v":1.1941708510850118E-2},{"$f":"(IF($AH$12<DEGREES(BU16),0+$AJ$16,1-((TAN(BU16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV16),0+$AJ$16,1-((TAN(BV16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW16),0+$AJ$16,1-((TAN(BW16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX16),0+$AJ$16,1-((TAN(BX16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY16),0+$AJ$16,1-((TAN(BY16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ16),0+$AJ$16,1-((TAN(BZ16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA16),0+$AJ$16,1-((TAN(CA16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB16),0+$AJ$16,1-((TAN(CB16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG15*$DU$3)+1-$DU$3)","v":1.4785265426734929E-2},{"$f":"(IF($AH$12<DEGREES(CC16),0+$AJ$16,1-((TAN(CC16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH15*$DU$3)+1-$DU$3)","v":0.28469384773098488},{"$f":"(IF($AH$12<DEGREES(CD16),0+$AJ$16,1-((TAN(CD16)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI15*$DU$3)+1-$DU$3)","v":0.36761362472822745},null,12,{"$f":"(IF($AH$46<DEGREES(CG16),0+$AJ$50,1-((TAN(CG16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CH16),0+$AJ$50,1-((TAN(CH16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CI16),0+$AJ$50,1-((TAN(CI16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CJ16),0+$AJ$50,1-((TAN(CJ16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CK16),0+$AJ$50,1-((TAN(CK16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CL16),0+$AJ$50,1-((TAN(CL16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CM16),0+$AJ$50,1-((TAN(CM16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CN16),0+$AJ$50,1-((TAN(CN16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CO16),0+$AJ$50,1-((TAN(CO16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CP16),0+$AJ$50,1-((TAN(CP16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CQ16),0+$AJ$50,1-((TAN(CQ16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV15*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CR16),0+$AJ$50,1-((TAN(CR16)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW15*$DU$3)+1-$DU$3)","v":0},null,null,{"$f":"'Profile angles'!AR16","v":12},{"$f":"'Profile angles'!AS16","v":45.177523796213436},{"$f":"'Profile angles'!AT16","v":54.329068465075267},{"$f":"'Profile angles'!AU16","v":65.047371814417531},{"$f":"'Profile angles'!AV16","v":77.120581963762746},{"$f":"'Profile angles'!AW16","v":85.511869047796154},{"$f":"'Profile angles'!AX16","v":87.685706703910299},{"$f":"'Profile angles'!AY16","v":84.793912346691229},{"$f":"'Profile angles'!AZ16","v":77.199736149013034},{"$f":"'Profile angles'!BA16","v":65.299840573859427},{"$f":"'Profile angles'!BB16","v":54.542607240756659},{"$f":"'Profile angles'!BC16","v":45.370517861678998},{"$f":"'Profile angles'!BD16","v":41.831318434437598},null,12,45.177523796213436,54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598]
[null,13,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D17-C348,'Dry Bulb'!D17-C232)","v":-1.3064106796794448},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E17-D348,'Dry Bulb'!E17-D232)","v":-1.284294053726569},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F17-E348,'Dry Bulb'!F17-E232)","v":5.2667507430997915},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G17-F348,'Dry Bulb'!G17-F232)","v":16.740806794055203},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H17-G348,'Dry Bulb'!H17-G232)","v":26.820806794055201},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I17-H348,'Dry Bulb'!I17-H232)","v":32.760806794055199},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J17-I348,'Dry Bulb'!J17-I232)","v":35.820806794055201},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K17-J348,'Dry Bulb'!K17-J232)","v":37.620806794055198},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L17-K348,'Dry Bulb'!L17-K232)","v":30.060806794055196},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M17-L348,'Dry Bulb'!M17-L232)","v":20.936316334744191},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N17-M348,'Dry Bulb'!N17-M232)","v":15.863155342714606},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O17-N348,'Dry Bulb'!O17-N232)","v":-0.50477575186765478},null,{"$f":"Q18-45","v":0},"South Surface Azimuth",null,null,null,null,null,null,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI17","v":13},{"$f":"'Incident angle'!BJ17","v":2550.173141104859},{"$f":"'Incident angle'!BK17","v":164.68058328163184},{"$f":"'Incident angle'!BL17","v":0},{"$f":"'Incident angle'!BM17","v":0},{"$f":"'Incident angle'!BN17","v":0},{"$f":"'Incident angle'!BO17","v":0},{"$f":"'Incident angle'!BP17","v":0},{"$f":"'Incident angle'!BQ17","v":0},{"$f":"'Incident angle'!BR17","v":0},{"$f":"'Incident angle'!BS17","v":315.54561787258626},{"$f":"'Incident angle'!BT17","v":2682.4119372208993},{"$f":"'Incident angle'!BU17","v":2806.1921484791264},null,{"$f":"'Incident angle'!BW17","v":13},{"$f":"'Incident angle'!BX17","v":0},{"$f":"'Incident angle'!BY17","v":0},{"$f":"'Incident angle'!BZ17","v":0},{"$f":"'Incident angle'!CA17","v":0},{"$f":"'Incident angle'!CB17","v":0},{"$f":"'Incident angle'!CC17","v":0},{"$f":"'Incident angle'!CD17","v":0},{"$f":"'Incident angle'!CE17","v":0},{"$f":"'Incident angle'!CF17","v":0},{"$f":"'Incident angle'!CG17","v":0},{"$f":"'Incident angle'!CH17","v":0},{"$f":"'Incident angle'!CI17","v":0},null,{"$f":"'Profile angles'!B17","v":13},{"$f":"RADIANS('Profile angles'!C17)","v":0.78702668175259982},{"$f":"RADIANS('Profile angles'!D17)","v":0.95205108174928044},{"$f":"RADIANS('Profile angles'!E17)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F17)","v":1.3531133844064995},{"$f":"RADIANS('Profile angles'!G17)","v":1.503986673926925},{"$f":"RADIANS('Profile angles'!H17)","v":1.558344195190098},{"$f":"RADIANS('Profile angles'!I17)","v":1.5043943771425594},{"$f":"RADIANS('Profile angles'!J17)","v":1.3559509038151709},{"$f":"RADIANS('Profile angles'!K17)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L17)","v":0.94455934348747927},{"$f":"RADIANS('Profile angles'!M17)","v":0.77841604698882561},{"$f":"RADIANS('Profile angles'!N17)","v":0.71991055223641132},0.94762977205204735,{"$f":"'Profile angles'!B46","v":13},{"$f":"RADIANS('Profile angles'!C46)","v":-1.331864871300116},{"$f":"RADIANS('Profile angles'!D46)","v":-1.3666270114598316},{"$f":"RADIANS('Profile angles'!E46)","v":-1.3535067192060635},{"$f":"RADIANS('Profile angles'!F46)","v":-1.3351101550303341},{"$f":"RADIANS('Profile angles'!G46)","v":-1.3407321893366537},{"$f":"RADIANS('Profile angles'!H46)","v":-1.3650413570281472},{"$f":"RADIANS('Profile angles'!I46)","v":-1.379822745398283},{"$f":"RADIANS('Profile angles'!J46)","v":-1.3506595370421364},{"$f":"RADIANS('Profile angles'!K46)","v":-1.2822582122157398},{"$f":"RADIANS('Profile angles'!L46)","v":-1.2149101170192604},{"$f":"RADIANS('Profile angles'!M46)","v":-1.1912817761692733},{"$f":"RADIANS('Profile angles'!N46)","v":-1.2470964531741524},null,{"$f":"'Profile angles'!AD17","v":13},{"$f":"(IF($AH$12<DEGREES(BS17),0+$AJ$16,1-((TAN(BS17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX16*$DU$3)+1-$DU$3)","v":0.26133852294754345},{"$f":"(IF($AH$12<DEGREES(BT17),0+$AJ$16,1-((TAN(BT17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY16*$DU$3)+1-$DU$3)","v":1.4422770518058832E-2},{"$f":"(IF($AH$12<DEGREES(BU17),0+$AJ$16,1-((TAN(BU17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV17),0+$AJ$16,1-((TAN(BV17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW17),0+$AJ$16,1-((TAN(BW17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX17),0+$AJ$16,1-((TAN(BX17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY17),0+$AJ$16,1-((TAN(BY17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ17),0+$AJ$16,1-((TAN(BZ17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA17),0+$AJ$16,1-((TAN(CA17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB17),0+$AJ$16,1-((TAN(CB17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG16*$DU$3)+1-$DU$3)","v":2.4003381163046483E-2},{"$f":"(IF($AH$12<DEGREES(CC17),0+$AJ$16,1-((TAN(CC17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH16*$DU$3)+1-$DU$3)","v":0.24880047761831087},{"$f":"(IF($AH$12<DEGREES(CD17),0+$AJ$16,1-((TAN(CD17)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI16*$DU$3)+1-$DU$3)","v":0.32935790073096527},null,13,{"$f":"(IF($AH$46<DEGREES(CG17),0+$AJ$50,1-((TAN(CG17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CH17),0+$AJ$50,1-((TAN(CH17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CI17),0+$AJ$50,1-((TAN(CI17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CJ17),0+$AJ$50,1-((TAN(CJ17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO16*$DU$3)+1-$DU$3)","v":1.8873368711019844},{"$f":"(IF($AH$46<DEGREES(CK17),0+$AJ$50,1-((TAN(CK17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP16*$DU$3)+1-$DU$3)","v":3.0530272566002568},{"$f":"(IF($AH$46<DEGREES(CL17),0+$AJ$50,1-((TAN(CL17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ16*$DU$3)+1-$DU$3)","v":3.7592250406101395},{"$f":"(IF($AH$46<DEGREES(CM17),0+$AJ$50,1-((TAN(CM17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR16*$DU$3)+1-$DU$3)","v":3.3977647591442528},{"$f":"(IF($AH$46<DEGREES(CN17),0+$AJ$50,1-((TAN(CN17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS16*$DU$3)+1-$DU$3)","v":1.8863571491428628},{"$f":"(IF($AH$46<DEGREES(CO17),0+$AJ$50,1-((TAN(CO17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT16*$DU$3)+1-$DU$3)","v":0.68045300274252096},{"$f":"(IF($AH$46<DEGREES(CP17),0+$AJ$50,1-((TAN(CP17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU16*$DU$3)+1-$DU$3)","v":7.0537598550977812E-2},{"$f":"(IF($AH$46<DEGREES(CQ17),0+$AJ$50,1-((TAN(CQ17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV16*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CR17),0+$AJ$50,1-((TAN(CR17)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW16*$DU$3)+1-$DU$3)","v":0},null,null,{"$f":"'Profile angles'!AR17","v":13},{"$f":"'Profile angles'!AS17","v":44.262516808487675},{"$f":"'Profile angles'!AT17","v":53.442649547558034},{"$f":"'Profile angles'!AU17","v":62.96975399076122},{"$f":"'Profile angles'!AV17","v":71.918657174425832},{"$f":"'Profile angles'!AW17","v":76.310429689037434},{"$f":"'Profile angles'!AX17","v":78.190731192893594},{"$f":"'Profile angles'!AY17","v":78.445286814888803},{"$f":"'Profile angles'!AZ17","v":72.64341275146262},{"$f":"'Profile angles'!BA17","v":61.303344417053367},{"$f":"'Profile angles'!BB17","v":50.879096974273239},{"$f":"'Profile angles'!BC17","v":42.542599664242438},{"$f":"'Profile angles'!BD17","v":40.072467904514703},null,13,44.262516808487675,53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703]
[null,14,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D18-C349,'Dry Bulb'!D18-C233)","v":-2.7774307486705965},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E18-D349,'Dry Bulb'!E18-D233)","v":1.4548688385635273},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F18-E349,'Dry Bulb'!F18-E233)","v":7.2588967303609309},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G18-F349,'Dry Bulb'!G18-F233)","v":18.180806794055201},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H18-G349,'Dry Bulb'!H18-G233)","v":28.260806794055199},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I18-H349,'Dry Bulb'!I18-H233)","v":34.92080679405521},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J18-I349,'Dry Bulb'!J18-I233)","v":37.440806794055192},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K18-J349,'Dry Bulb'!K18-J233)","v":38.520806794055204},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L18-K349,'Dry Bulb'!L18-K233)","v":31.140806794055194},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M18-L349,'Dry Bulb'!M18-L233)","v":23.94399228783395},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N18-M349,'Dry Bulb'!N18-M233)","v":16.992852059193339},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O18-N349,'Dry Bulb'!O18-N233)","v":0.62234493588297823},null,null,45,null,null,null,null,null,null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI18","v":14},{"$f":"'Incident angle'!BJ18","v":2071.1194620481665},{"$f":"'Incident angle'!BK18","v":325.93097583385139},{"$f":"'Incident angle'!BL18","v":0},{"$f":"'Incident angle'!BM18","v":0},{"$f":"'Incident angle'!BN18","v":0},{"$f":"'Incident angle'!BO18","v":0},{"$f":"'Incident angle'!BP18","v":0},{"$f":"'Incident angle'!BQ18","v":0},{"$f":"'Incident angle'!BR18","v":0},{"$f":"'Incident angle'!BS18","v":459.69342121644979},{"$f":"'Incident angle'!BT18","v":2064.4902305776382},{"$f":"'Incident angle'!BU18","v":2259.4897211870334},null,{"$f":"'Incident angle'!BW18","v":14},{"$f":"'Incident angle'!BX18","v":0},{"$f":"'Incident angle'!BY18","v":0},{"$f":"'Incident angle'!BZ18","v":0},{"$f":"'Incident angle'!CA18","v":0},{"$f":"'Incident angle'!CB18","v":0},{"$f":"'Incident angle'!CC18","v":0},{"$f":"'Incident angle'!CD18","v":0},{"$f":"'Incident angle'!CE18","v":0},{"$f":"'Incident angle'!CF18","v":0},{"$f":"'Incident angle'!CG18","v":0},{"$f":"'Incident angle'!CH18","v":0},{"$f":"'Incident angle'!CI18","v":0},null,{"$f":"'Profile angles'!B18","v":14},{"$f":"RADIANS('Profile angles'!C18)","v":0.75851543012385225},{"$f":"RADIANS('Profile angles'!D18)","v":0.93648395989476452},{"$f":"RADIANS('Profile angles'!E18)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!F18)","v":1.3750301180558759},{"$f":"RADIANS('Profile angles'!G18)","v":1.5399688677201155},{"$f":"RADIANS('Profile angles'!H18)","v":-1.5457329130795114},{"$f":"RADIANS('Profile angles'!I18)","v":1.5359564525388147},{"$f":"RADIANS('Profile angles'!J18)","v":1.3770848532828261},{"$f":"RADIANS('Profile angles'!K18)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L18)","v":0.92031825841069459},{"$f":"RADIANS('Profile angles'!M18)","v":0.73756032900572732},{"$f":"RADIANS('Profile angles'!N18)","v":0.68075372194542327},0.83525713380236288,{"$f":"'Profile angles'!B47","v":14},{"$f":"RADIANS('Profile angles'!C47)","v":-1.0005927212218162},{"$f":"RADIANS('Profile angles'!D47)","v":-1.0600445287944333},{"$f":"RADIANS('Profile angles'!E47)","v":-1.0718008336148819},{"$f":"RADIANS('Profile angles'!F47)","v":-1.0771466448813709},{"$f":"RADIANS('Profile angles'!G47)","v":-1.0979012626620424},{"$f":"RADIANS('Profile angles'!H47)","v":-1.127498795680429},{"$f":"RADIANS('Profile angles'!I47)","v":-1.1367031826073217},{"$f":"RADIANS('Profile angles'!J47)","v":-1.0927120982101921},{"$f":"RADIANS('Profile angles'!K47)","v":-1.0030149795642187},{"$f":"RADIANS('Profile angles'!L47)","v":-0.91563513724759149},{"$f":"RADIANS('Profile angles'!M47)","v":-0.86977254162430351},{"$f":"RADIANS('Profile angles'!N47)","v":-0.91012957488156332},null,{"$f":"'Profile angles'!AD18","v":14},{"$f":"(IF($AH$12<DEGREES(BS18),0+$AJ$16,1-((TAN(BS18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX17*$DU$3)+1-$DU$3)","v":0.23436979703036673},{"$f":"(IF($AH$12<DEGREES(BT18),0+$AJ$16,1-((TAN(BT18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY17*$DU$3)+1-$DU$3)","v":3.0079006005551467E-2},{"$f":"(IF($AH$12<DEGREES(BU18),0+$AJ$16,1-((TAN(BU18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ17*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV18),0+$AJ$16,1-((TAN(BV18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA17*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW18),0+$AJ$16,1-((TAN(BW18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB17*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX18),0+$AJ$16,1-((TAN(BX18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC17*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY18),0+$AJ$16,1-((TAN(BY18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD17*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ18),0+$AJ$16,1-((TAN(BZ18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE17*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA18),0+$AJ$16,1-((TAN(CA18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF17*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB18),0+$AJ$16,1-((TAN(CB18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG17*$DU$3)+1-$DU$3)","v":3.9663440638659592E-2},{"$f":"(IF($AH$12<DEGREES(CC18),0+$AJ$16,1-((TAN(CC18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH17*$DU$3)+1-$DU$3)","v":0.22439774861444234},{"$f":"(IF($AH$12<DEGREES(CD18),0+$AJ$16,1-((TAN(CD18)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI17*$DU$3)+1-$DU$3)","v":0.29677004292270814},null,14,{"$f":"(IF($AH$46<DEGREES(CG18),0+$AJ$50,1-((TAN(CG18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL17*$DU$3)+1-$DU$3)","v":0.34297879737817005},{"$f":"(IF($AH$46<DEGREES(CH18),0+$AJ$50,1-((TAN(CH18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM17*$DU$3)+1-$DU$3)","v":0.71129734676283651},{"$f":"(IF($AH$46<DEGREES(CI18),0+$AJ$50,1-((TAN(CI18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN17*$DU$3)+1-$DU$3)","v":1.2143902750600704},{"$f":"(IF($AH$46<DEGREES(CJ18),0+$AJ$50,1-((TAN(CJ18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO17*$DU$3)+1-$DU$3)","v":1.7253216708585404},{"$f":"(IF($AH$46<DEGREES(CK18),0+$AJ$50,1-((TAN(CK18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP17*$DU$3)+1-$DU$3)","v":2.1072796388773063},{"$f":"(IF($AH$46<DEGREES(CL18),0+$AJ$50,1-((TAN(CL18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ17*$DU$3)+1-$DU$3)","v":2.2038929817144779},{"$f":"(IF($AH$46<DEGREES(CM18),0+$AJ$50,1-((TAN(CM18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR17*$DU$3)+1-$DU$3)","v":2.2080170659475931},{"$f":"(IF($AH$46<DEGREES(CN18),0+$AJ$50,1-((TAN(CN18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS17*$DU$3)+1-$DU$3)","v":1.7494344850523076},{"$f":"(IF($AH$46<DEGREES(CO18),0+$AJ$50,1-((TAN(CO18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT17*$DU$3)+1-$DU$3)","v":1.2409615953172008},{"$f":"(IF($AH$46<DEGREES(CP18),0+$AJ$50,1-((TAN(CP18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU17*$DU$3)+1-$DU$3)","v":0.89903184939971925},{"$f":"(IF($AH$46<DEGREES(CQ18),0+$AJ$50,1-((TAN(CQ18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV17*$DU$3)+1-$DU$3)","v":0.59544756598468784},{"$f":"(IF($AH$46<DEGREES(CR18),0+$AJ$50,1-((TAN(CR18)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW17*$DU$3)+1-$DU$3)","v":0.36440508861958254},null,null,{"$f":"'Profile angles'!AR18","v":14},{"$f":"'Profile angles'!AS18","v":39.001643714284292},{"$f":"'Profile angles'!AT18","v":47.236569251778789},{"$f":"'Profile angles'!AU18","v":54.505603493104616},{"$f":"'Profile angles'!AV18","v":60.167275430762508},{"$f":"'Profile angles'!AW18","v":62.862961225627508},{"$f":"'Profile angles'!AX18","v":64.570010808670432},{"$f":"'Profile angles'!AY18","v":65.066621957768987},{"$f":"'Profile angles'!AZ18","v":61.010544197086858},{"$f":"'Profile angles'!BA18","v":51.819137025254037},{"$f":"'Profile angles'!BB18","v":42.759898297268641},{"$f":"'Profile angles'!BC18","v":35.791762146841563},{"$f":"'Profile angles'!BD18","v":34.427909280399348},null,14,39.001643714284292,47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348]
[null,15,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D19-C350,'Dry Bulb'!D19-C234)","v":0.35512307902079954},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E19-D350,'Dry Bulb'!E19-D234)","v":7.1260810020663286},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F19-E350,'Dry Bulb'!F19-E234)","v":13.560941348088789},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G19-F350,'Dry Bulb'!G19-F234)","v":24.251132033854844},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H19-G350,'Dry Bulb'!H19-G234)","v":33.601620308891569},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I19-H350,'Dry Bulb'!I19-H234)","v":39.167821636698591},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J19-I350,'Dry Bulb'!J19-I234)","v":41.77034906841476},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K19-J350,'Dry Bulb'!K19-J234)","v":44.425658256218824},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L19-K350,'Dry Bulb'!L19-K234)","v":39.265856228707847},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M19-L350,'Dry Bulb'!M19-L234)","v":30.459137567668073},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N19-M350,'Dry Bulb'!N19-M234)","v":20.6477190729684},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O19-N350,'Dry Bulb'!O19-N234)","v":3.2907824743424499},null,null,null,null,null,null,null,null,null,null,null,null,null,"SILL",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI19","v":15},{"$f":"'Incident angle'!BJ19","v":1452.546941542701},{"$f":"'Incident angle'!BK19","v":364.46110364013998},{"$f":"'Incident angle'!BL19","v":0},{"$f":"'Incident angle'!BM19","v":0},{"$f":"'Incident angle'!BN19","v":0},{"$f":"'Incident angle'!BO19","v":0},{"$f":"'Incident angle'!BP19","v":0},{"$f":"'Incident angle'!BQ19","v":0},{"$f":"'Incident angle'!BR19","v":0},{"$f":"'Incident angle'!BS19","v":297.93065860827932},{"$f":"'Incident angle'!BT19","v":1293.4997769469985},{"$f":"'Incident angle'!BU19","v":1490.3099220028244},null,{"$f":"'Incident angle'!BW19","v":15},{"$f":"'Incident angle'!BX19","v":0},{"$f":"'Incident angle'!BY19","v":0},{"$f":"'Incident angle'!BZ19","v":0},{"$f":"'Incident angle'!CA19","v":0},{"$f":"'Incident angle'!CB19","v":0},{"$f":"'Incident angle'!CC19","v":0},{"$f":"'Incident angle'!CD19","v":0},{"$f":"'Incident angle'!CE19","v":0},{"$f":"'Incident angle'!CF19","v":0},{"$f":"'Incident angle'!CG19","v":0},{"$f":"'Incident angle'!CH19","v":0},{"$f":"'Incident angle'!CI19","v":0},null,{"$f":"'Profile angles'!B19","v":15},{"$f":"RADIANS('Profile angles'!C19)","v":0.6958725601819693},{"$f":"RADIANS('Profile angles'!D19)","v":0.90095965651819487},{"$f":"RADIANS('Profile angles'!E19)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F19)","v":1.4223966034161182},{"$f":"RADIANS('Profile angles'!G19)","v":-1.5266344477385527},{"$f":"RADIANS('Profile angles'!H19)","v":-1.4675022187003639},{"$f":"RADIANS('Profile angles'!I19)","v":-1.5378465881867291},{"$f":"RADIANS('Profile angles'!J19)","v":1.4231733271709055},{"$f":"RADIANS('Profile angles'!K19)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L19)","v":0.86910144352535135},{"$f":"RADIANS('Profile angles'!M19)","v":0.65429236322323214},{"$f":"RADIANS('Profile angles'!N19)","v":0.59989785402553941},0.64376271290446829,{"$f":"'Profile angles'!B48","v":15},{"$f":"RADIANS('Profile angles'!C48)","v":-0.69486770530695274},{"$f":"RADIANS('Profile angles'!D48)","v":-0.77035987910152959},{"$f":"RADIANS('Profile angles'!E48)","v":-0.8014439225775819},{"$f":"RADIANS('Profile angles'!F48)","v":-0.82641496006128057},{"$f":"RADIANS('Profile angles'!G48)","v":-0.86009108801295264},{"$f":"RADIANS('Profile angles'!H48)","v":-0.89419996525178802},{"$f":"RADIANS('Profile angles'!I48)","v":-0.89834850121998655},{"$f":"RADIANS('Profile angles'!J48)","v":-0.84181932575908713},{"$f":"RADIANS('Profile angles'!K48)","v":-0.73590361062962995},{"$f":"RADIANS('Profile angles'!L48)","v":-0.63537560318144104},{"$f":"RADIANS('Profile angles'!M48)","v":-0.57579270320512765},{"$f":"RADIANS('Profile angles'!N48)","v":-0.60446464805382871},null,{"$f":"'Profile angles'!AD19","v":15},{"$f":"(IF($AH$12<DEGREES(BS19),0+$AJ$16,1-((TAN(BS19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX18*$DU$3)+1-$DU$3)","v":0.20723537554036472},{"$f":"(IF($AH$12<DEGREES(BT19),0+$AJ$16,1-((TAN(BT19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY18*$DU$3)+1-$DU$3)","v":4.0582121819301542E-2},{"$f":"(IF($AH$12<DEGREES(BU19),0+$AJ$16,1-((TAN(BU19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ18*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV19),0+$AJ$16,1-((TAN(BV19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA18*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW19),0+$AJ$16,1-((TAN(BW19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB18*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX19),0+$AJ$16,1-((TAN(BX19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC18*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY19),0+$AJ$16,1-((TAN(BY19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD18*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ19),0+$AJ$16,1-((TAN(BZ19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE18*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA19),0+$AJ$16,1-((TAN(CA19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF18*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB19),0+$AJ$16,1-((TAN(CB19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG18*$DU$3)+1-$DU$3)","v":3.3965675201247006E-2},{"$f":"(IF($AH$12<DEGREES(CC19),0+$AJ$16,1-((TAN(CC19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH18*$DU$3)+1-$DU$3)","v":0.18952264069369404},{"$f":"(IF($AH$12<DEGREES(CD19),0+$AJ$16,1-((TAN(CD19)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI18*$DU$3)+1-$DU$3)","v":0.26314169321928071},null,15,{"$f":"(IF($AH$46<DEGREES(CG19),0+$AJ$50,1-((TAN(CG19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL18*$DU$3)+1-$DU$3)","v":0.75159642101953361},{"$f":"(IF($AH$46<DEGREES(CH19),0+$AJ$50,1-((TAN(CH19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM18*$DU$3)+1-$DU$3)","v":0.97423680688497971},{"$f":"(IF($AH$46<DEGREES(CI19),0+$AJ$50,1-((TAN(CI19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN18*$DU$3)+1-$DU$3)","v":1.2349622149603583},{"$f":"(IF($AH$46<DEGREES(CJ19),0+$AJ$50,1-((TAN(CJ19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO18*$DU$3)+1-$DU$3)","v":1.5173522535766957},{"$f":"(IF($AH$46<DEGREES(CK19),0+$AJ$50,1-((TAN(CK19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP18*$DU$3)+1-$DU$3)","v":1.6534989168867438},{"$f":"(IF($AH$46<DEGREES(CL19),0+$AJ$50,1-((TAN(CL19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ18*$DU$3)+1-$DU$3)","v":1.6343863843039681},{"$f":"(IF($AH$46<DEGREES(CM19),0+$AJ$50,1-((TAN(CM19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR18*$DU$3)+1-$DU$3)","v":1.7172408356987663},{"$f":"(IF($AH$46<DEGREES(CN19),0+$AJ$50,1-((TAN(CN19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS18*$DU$3)+1-$DU$3)","v":1.5326473910023846},{"$f":"(IF($AH$46<DEGREES(CO19),0+$AJ$50,1-((TAN(CO19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT18*$DU$3)+1-$DU$3)","v":1.221933241827893},{"$f":"(IF($AH$46<DEGREES(CP19),0+$AJ$50,1-((TAN(CP19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU18*$DU$3)+1-$DU$3)","v":0.99294851820756314},{"$f":"(IF($AH$46<DEGREES(CQ19),0+$AJ$50,1-((TAN(CQ19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV18*$DU$3)+1-$DU$3)","v":0.80148051896639905},{"$f":"(IF($AH$46<DEGREES(CR19),0+$AJ$50,1-((TAN(CR19)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW18*$DU$3)+1-$DU$3)","v":0.70026066082878768},null,null,{"$f":"'Profile angles'!AR19","v":15},{"$f":"'Profile angles'!AS19","v":30.541133571003865},{"$f":"'Profile angles'!AT19","v":37.574701882546435},{"$f":"'Profile angles'!AU19","v":43.007444089240849},{"$f":"'Profile angles'!AV19","v":46.978750874484376},{"$f":"'Profile angles'!AW19","v":49.242301300948341},{"$f":"'Profile angles'!AX19","v":51.002542825705397},{"$f":"'Profile angles'!AY19","v":51.447673176445399},{"$f":"'Profile angles'!AZ19","v":47.843171633901541},{"$f":"'Profile angles'!BA19","v":39.895074988635152},{"$f":"'Profile angles'!BB19","v":32.038156511029932},{"$f":"'Profile angles'!BC19","v":26.359057025099464},{"$f":"'Profile angles'!BD19","v":25.920295493187655},null,15,30.541133571003865,37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655]
[null,16,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D20-C351,'Dry Bulb'!D20-C235)","v":0.78250340796105888},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E20-D351,'Dry Bulb'!E20-D235)","v":8.7927944731777217},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F20-E351,'Dry Bulb'!F20-E235)","v":17.421879189978},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G20-F351,'Dry Bulb'!G20-F235)","v":27.371129784225417},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H20-G351,'Dry Bulb'!H20-G235)","v":38.182931614717511},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I20-H351,'Dry Bulb'!I20-H235)","v":44.885261648601478},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J20-I351,'Dry Bulb'!J20-I235)","v":47.463228199839584},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K20-J351,'Dry Bulb'!K20-J235)","v":48.951593394860623},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L20-K351,'Dry Bulb'!L20-K235)","v":41.476432867337543},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M20-L351,'Dry Bulb'!M20-L235)","v":29.807615510285167},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N20-M351,'Dry Bulb'!N20-M235)","v":17.669033337455303},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O20-N351,'Dry Bulb'!O20-N235)","v":1.3579624257894238},null,{"$f":"ABS(15*STAT!L4)","v":45},"Local Time Meridian",null,null,null,null,null,null,"WEST WINDOW SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI20","v":16},{"$f":"'Incident angle'!BJ20","v":713.65975482504973},{"$f":"'Incident angle'!BK20","v":10.376642262278452},{"$f":"'Incident angle'!BL20","v":0},{"$f":"'Incident angle'!BM20","v":0},{"$f":"'Incident angle'!BN20","v":0},{"$f":"'Incident angle'!BO20","v":0},{"$f":"'Incident angle'!BP20","v":0},{"$f":"'Incident angle'!BQ20","v":0},{"$f":"'Incident angle'!BR20","v":0},{"$f":"'Incident angle'!BS20","v":0},{"$f":"'Incident angle'!BT20","v":381.95980659736199},{"$f":"'Incident angle'!BU20","v":690.59594603259609},null,{"$f":"'Incident angle'!BW20","v":16},{"$f":"'Incident angle'!BX20","v":0},{"$f":"'Incident angle'!BY20","v":0},{"$f":"'Incident angle'!BZ20","v":0},{"$f":"'Incident angle'!CA20","v":0},{"$f":"'Incident angle'!CB20","v":0},{"$f":"'Incident angle'!CC20","v":0},{"$f":"'Incident angle'!CD20","v":0},{"$f":"'Incident angle'!CE20","v":0},{"$f":"'Incident angle'!CF20","v":0},{"$f":"'Incident angle'!CG20","v":0},{"$f":"'Incident angle'!CH20","v":0},{"$f":"'Incident angle'!CI20","v":0},null,{"$f":"'Profile angles'!B20","v":16},{"$f":"RADIANS('Profile angles'!C20)","v":0.57197798027671076},{"$f":"RADIANS('Profile angles'!D20)","v":0.82619821336400978},{"$f":"RADIANS('Profile angles'!E20)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!F20)","v":1.5229810963446619},{"$f":"RADIANS('Profile angles'!G20)","v":-1.378468089484002},{"$f":"RADIANS('Profile angles'!H20)","v":-1.3177516582315827},{"$f":"RADIANS('Profile angles'!I20)","v":-1.4044440508792542},{"$f":"RADIANS('Profile angles'!J20)","v":1.5204461167120873},{"$f":"RADIANS('Profile angles'!K20)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L20)","v":0.75629963516330256},{"$f":"RADIANS('Profile angles'!M20)","v":0.48809734520255899},{"$f":"RADIANS('Profile angles'!N20)","v":0.44518009228857974},0.32679527955398463,{"$f":"'Profile angles'!B49","v":16},{"$f":"RADIANS('Profile angles'!C49)","v":-0.41669740220816492},{"$f":"RADIANS('Profile angles'!D49)","v":-0.50015077980007105},{"$f":"RADIANS('Profile angles'!E49)","v":-0.54404800401822806},{"$f":"RADIANS('Profile angles'!F49)","v":-0.58351428900426172},{"$f":"RADIANS('Profile angles'!G49)","v":-0.62746556362485806},{"$f":"RADIANS('Profile angles'!H49)","v":-0.66533748077630195},{"$f":"RADIANS('Profile angles'!I49)","v":-0.66523823915225477},{"$f":"RADIANS('Profile angles'!J49)","v":-0.59872473938789039},{"$f":"RADIANS('Profile angles'!K49)","v":-0.48155681326357536},{"$f":"RADIANS('Profile angles'!L49)","v":-0.37388412364806317},{"$f":"RADIANS('Profile angles'!M49)","v":-0.30789644489665746},{"$f":"RADIANS('Profile angles'!N49)","v":-0.32941416658746181},null,{"$f":"'Profile angles'!AD20","v":16},{"$f":"(IF($AH$12<DEGREES(BS20),0+$AJ$16,1-((TAN(BS20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX19*$DU$3)+1-$DU$3)","v":0.14985444718920451},{"$f":"(IF($AH$12<DEGREES(BT20),0+$AJ$16,1-((TAN(BT20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY19*$DU$3)+1-$DU$3)","v":1.7324783486299719E-3},{"$f":"(IF($AH$12<DEGREES(BU20),0+$AJ$16,1-((TAN(BU20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ19*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV20),0+$AJ$16,1-((TAN(BV20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA19*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW20),0+$AJ$16,1-((TAN(BW20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB19*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX20),0+$AJ$16,1-((TAN(BX20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC19*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY20),0+$AJ$16,1-((TAN(BY20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD19*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ20),0+$AJ$16,1-((TAN(BZ20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE19*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA20),0+$AJ$16,1-((TAN(CA20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF19*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB20),0+$AJ$16,1-((TAN(CB20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG19*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC20),0+$AJ$16,1-((TAN(CC20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH19*$DU$3)+1-$DU$3)","v":0.10380357907320599},{"$f":"(IF($AH$12<DEGREES(CD20),0+$AJ$16,1-((TAN(CD20)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI19*$DU$3)+1-$DU$3)","v":0.20125953950907982},null,16,{"$f":"(IF($AH$46<DEGREES(CG20),0+$AJ$50,1-((TAN(CG20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL19*$DU$3)+1-$DU$3)","v":0.83050073999003016},{"$f":"(IF($AH$46<DEGREES(CH20),0+$AJ$50,1-((TAN(CH20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM19*$DU$3)+1-$DU$3)","v":0.99351459637698469},{"$f":"(IF($AH$46<DEGREES(CI20),0+$AJ$50,1-((TAN(CI20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN19*$DU$3)+1-$DU$3)","v":1.1733486818169041},{"$f":"(IF($AH$46<DEGREES(CJ20),0+$AJ$50,1-((TAN(CJ20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO19*$DU$3)+1-$DU$3)","v":1.374068685620073},{"$f":"(IF($AH$46<DEGREES(CK20),0+$AJ$50,1-((TAN(CK20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP19*$DU$3)+1-$DU$3)","v":1.3338014910381679},{"$f":"(IF($AH$46<DEGREES(CL20),0+$AJ$50,1-((TAN(CL20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ19*$DU$3)+1-$DU$3)","v":1.3215927891111598},{"$f":"(IF($AH$46<DEGREES(CM20),0+$AJ$50,1-((TAN(CM20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR19*$DU$3)+1-$DU$3)","v":1.3738535069287243},{"$f":"(IF($AH$46<DEGREES(CN20),0+$AJ$50,1-((TAN(CN20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS19*$DU$3)+1-$DU$3)","v":1.3851319629365855},{"$f":"(IF($AH$46<DEGREES(CO20),0+$AJ$50,1-((TAN(CO20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT19*$DU$3)+1-$DU$3)","v":1.1556883702663532},{"$f":"(IF($AH$46<DEGREES(CP20),0+$AJ$50,1-((TAN(CP20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU19*$DU$3)+1-$DU$3)","v":0.97852414941374344},{"$f":"(IF($AH$46<DEGREES(CQ20),0+$AJ$50,1-((TAN(CQ20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV19*$DU$3)+1-$DU$3)","v":0.8341901694135071},{"$f":"(IF($AH$46<DEGREES(CR20),0+$AJ$50,1-((TAN(CR20)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW19*$DU$3)+1-$DU$3)","v":0.77337341865305798},null,null,{"$f":"'Profile angles'!AR20","v":16},{"$f":"'Profile angles'!AS20","v":20.038281727598083},{"$f":"'Profile angles'!AT20","v":26.016647471873153},{"$f":"'Profile angles'!AU20","v":30.233879108991232},{"$f":"'Profile angles'!AV20","v":33.419767540103443},{"$f":"'Profile angles'!AW20","v":35.682648220686666},{"$f":"'Profile angles'!AX20","v":37.56104623172925},{"$f":"'Profile angles'!AY20","v":37.876258416390314},{"$f":"'Profile angles'!AZ20","v":34.288646107643089},{"$f":"'Profile angles'!BA20","v":26.935985833021654},{"$f":"'Profile angles'!BB20","v":19.913519068774189},{"$f":"'Profile angles'!BC20","v":15.259931573481456},{"$f":"'Profile angles'!BD20","v":15.530455637101428},null,16,20.038281727598083,26.016647471873153,30.233879108991232,33.419767540103443,35.682648220686666,37.56104623172925,37.876258416390314,34.288646107643089,26.935985833021654,19.913519068774189,15.259931573481456,15.530455637101428]
[null,17,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D21-C352,'Dry Bulb'!D21-C236)","v":-4.125820757135898},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E21-D352,'Dry Bulb'!E21-D236)","v":4.96556626571099},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F21-E352,'Dry Bulb'!F21-E236)","v":14.288511634407705},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G21-F352,'Dry Bulb'!G21-F236)","v":23.497572329604509},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H21-G352,'Dry Bulb'!H21-G236)","v":35.886611243523717},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I21-H352,'Dry Bulb'!I21-H236)","v":43.003262582788011},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J21-I352,'Dry Bulb'!J21-I236)","v":45.721376014699835},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K21-J352,'Dry Bulb'!K21-J236)","v":45.428518850943099},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L21-K352,'Dry Bulb'!L21-K236)","v":36.791069050599617},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M21-L352,'Dry Bulb'!M21-L236)","v":24.61039959111713},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N21-M352,'Dry Bulb'!N21-M236)","v":11.753336278240326},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O21-N352,'Dry Bulb'!O21-N236)","v":-4.927182095724433},null,null,null,null,null,null,null,null,null,7,null,null,0,1,2,3,4,5,6,7,8,9,10,null,null,null,null,{"$f":"'Incident angle'!BI21","v":17},{"$f":"'Incident angle'!BJ21","v":0},{"$f":"'Incident angle'!BK21","v":0},{"$f":"'Incident angle'!BL21","v":0},{"$f":"'Incident angle'!BM21","v":0},{"$f":"'Incident angle'!BN21","v":0},{"$f":"'Incident angle'!BO21","v":0},{"$f":"'Incident angle'!BP21","v":0},{"$f":"'Incident angle'!BQ21","v":0},{"$f":"'Incident angle'!BR21","v":0},{"$f":"'Incident angle'!BS21","v":0},{"$f":"'Incident angle'!BT21","v":0},{"$f":"'Incident angle'!BU21","v":47.993568038259191},null,{"$f":"'Incident angle'!BW21","v":17},{"$f":"'Incident angle'!BX21","v":0},{"$f":"'Incident angle'!BY21","v":0},{"$f":"'Incident angle'!BZ21","v":0},{"$f":"'Incident angle'!CA21","v":0},{"$f":"'Incident angle'!CB21","v":0},{"$f":"'Incident angle'!CC21","v":0},{"$f":"'Incident angle'!CD21","v":0},{"$f":"'Incident angle'!CE21","v":0},{"$f":"'Incident angle'!CF21","v":0},{"$f":"'Incident angle'!CG21","v":0},{"$f":"'Incident angle'!CH21","v":0},{"$f":"'Incident angle'!CI21","v":0},null,{"$f":"'Profile angles'!B21","v":17},{"$f":"RADIANS('Profile angles'!C21)","v":0.31585481016596412},{"$f":"RADIANS('Profile angles'!D21)","v":0.64419111865687895},{"$f":"RADIANS('Profile angles'!E21)","v":1.1397000015522969},{"$f":"RADIANS('Profile angles'!F21)","v":-1.3637805005768204},{"$f":"RADIANS('Profile angles'!G21)","v":-1.0702663972279507},{"$f":"RADIANS('Profile angles'!H21)","v":-1.0276883038342115},{"$f":"RADIANS('Profile angles'!I21)","v":-1.1305109275476111},{"$f":"RADIANS('Profile angles'!J21)","v":-1.3794764235329202},{"$f":"RADIANS('Profile angles'!K21)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L21)","v":0.43856842576519406},{"$f":"RADIANS('Profile angles'!M21)","v":0.13613500526814382},{"$f":"RADIANS('Profile angles'!N21)","v":0.14545482072436786},-0.21715442612286909,{"$f":"'Profile angles'!B50","v":17},{"$f":"RADIANS('Profile angles'!C50)","v":-0.16124242777223324},{"$f":"RADIANS('Profile angles'!D50)","v":-0.24682095640962623},{"$f":"RADIANS('Profile angles'!E50)","v":-0.29766243646613283},{"$f":"RADIANS('Profile angles'!F50)","v":-0.34652947246442356},{"$f":"RADIANS('Profile angles'!G50)","v":-0.39810829518922264},{"$f":"RADIANS('Profile angles'!H50)","v":-0.43915625637623362},{"$f":"RADIANS('Profile angles'!I50)","v":-0.43577963764801336},{"$f":"RADIANS('Profile angles'!J50)","v":-0.36165127468574837},{"$f":"RADIANS('Profile angles'!K50)","v":-0.2373188382783232},{"$f":"RADIANS('Profile angles'!L50)","v":-0.12693435438886347},{"$f":"RADIANS('Profile angles'!M50)","v":-5.9792925815892878E-2},{"$f":"RADIANS('Profile angles'!N50)","v":-7.8011009216174293E-2},null,{"$f":"'Profile angles'!AD21","v":17},{"$f":"(IF($AH$12<DEGREES(BS21),0+$AJ$16,1-((TAN(BS21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT21),0+$AJ$16,1-((TAN(BT21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU21),0+$AJ$16,1-((TAN(BU21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV21),0+$AJ$16,1-((TAN(BV21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW21),0+$AJ$16,1-((TAN(BW21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX21),0+$AJ$16,1-((TAN(BX21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY21),0+$AJ$16,1-((TAN(BY21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ21),0+$AJ$16,1-((TAN(BZ21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA21),0+$AJ$16,1-((TAN(CA21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB21),0+$AJ$16,1-((TAN(CB21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC21),0+$AJ$16,1-((TAN(CC21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH20*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD21),0+$AJ$16,1-((TAN(CD21)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI20*$DU$3)+1-$DU$3)","v":5.6542915176467215E-2},null,17,{"$f":"(IF($AH$46<DEGREES(CG21),0+$AJ$50,1-((TAN(CG21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL20*$DU$3)+1-$DU$3)","v":0.82444249800434677},{"$f":"(IF($AH$46<DEGREES(CH21),0+$AJ$50,1-((TAN(CH21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM20*$DU$3)+1-$DU$3)","v":0.95808728640798413},{"$f":"(IF($AH$46<DEGREES(CI21),0+$AJ$50,1-((TAN(CI21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN20*$DU$3)+1-$DU$3)","v":1.1005293079622112},{"$f":"(IF($AH$46<DEGREES(CJ21),0+$AJ$50,1-((TAN(CJ21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO20*$DU$3)+1-$DU$3)","v":1.170524529867212},{"$f":"(IF($AH$46<DEGREES(CK21),0+$AJ$50,1-((TAN(CK21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP20*$DU$3)+1-$DU$3)","v":1.1082917547993145},{"$f":"(IF($AH$46<DEGREES(CL21),0+$AJ$50,1-((TAN(CL21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ20*$DU$3)+1-$DU$3)","v":1.1001026856557057},{"$f":"(IF($AH$46<DEGREES(CM21),0+$AJ$50,1-((TAN(CM21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR20*$DU$3)+1-$DU$3)","v":1.1390493667968302},{"$f":"(IF($AH$46<DEGREES(CN21),0+$AJ$50,1-((TAN(CN21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS20*$DU$3)+1-$DU$3)","v":1.1820231098152745},{"$f":"(IF($AH$46<DEGREES(CO21),0+$AJ$50,1-((TAN(CO21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT20*$DU$3)+1-$DU$3)","v":1.0814279375377409},{"$f":"(IF($AH$46<DEGREES(CP21),0+$AJ$50,1-((TAN(CP21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU20*$DU$3)+1-$DU$3)","v":0.93010845983425494},{"$f":"(IF($AH$46<DEGREES(CQ21),0+$AJ$50,1-((TAN(CQ21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV20*$DU$3)+1-$DU$3)","v":0.8095588974544754},{"$f":"(IF($AH$46<DEGREES(CR21),0+$AJ$50,1-((TAN(CR21)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW20*$DU$3)+1-$DU$3)","v":0.76757797696205932},null,null,{"$f":"'Profile angles'!AR21","v":17},{"$f":"'Profile angles'!AS21","v":8.2848854255444504},{"$f":"'Profile angles'!AT21","v":13.434807821200849},{"$f":"'Profile angles'!AU21","v":16.897092448538277},{"$f":"'Profile angles'!AV21","v":19.80224832363653},{"$f":"'Profile angles'!AW21","v":22.286756355186323},{"$f":"'Profile angles'!AX21","v":24.319689951925163},{"$f":"'Profile angles'!AY21","v":24.456964963286701},{"$f":"'Profile angles'!AZ21","v":20.670382142796534},{"$f":"'Profile angles'!BA21","v":13.51706337533537},{"$f":"'Profile angles'!BB21","v":7.0202572324504446},{"$f":"'Profile angles'!BC21","v":3.1397975005302774},{"$f":"'Profile angles'!BD21","v":3.9451572875932328},null,17,{"$f":"DX21","v":8.2848854255444504},{"$f":"DY21","v":13.434807821200849},{"$f":"DZ21","v":16.897092448538277},{"$f":"EA21","v":19.80224832363653},{"$f":"EB21","v":22.286756355186323},{"$f":"EC21","v":24.319689951925163},{"$f":"ED21","v":24.456964963286701},{"$f":"EE21","v":20.670382142796534},{"$f":"EF21","v":13.51706337533537},{"$f":"EG21","v":7.0202572324504446},{"$f":"EH21","v":3.1397975005302774},3.9451572875932328]
[null,18,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D22-C353,'Dry Bulb'!D22-C237)","v":-6.6591932059447956},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E22-D353,'Dry Bulb'!E22-D237)","v":-1.4614304937629612},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F22-E353,'Dry Bulb'!F22-E237)","v":7.6994727408267352},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G22-F353,'Dry Bulb'!G22-F237)","v":17.237348584658079},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H22-G353,'Dry Bulb'!H22-G237)","v":30.024030571357756},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I22-H353,'Dry Bulb'!I22-H237)","v":37.744465322205926},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J22-I353,'Dry Bulb'!J22-I237)","v":39.77232756708338},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K22-J353,'Dry Bulb'!K22-J237)","v":38.367333398043229},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L22-K353,'Dry Bulb'!L22-K237)","v":29.160806794055205},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M22-L353,'Dry Bulb'!M22-L237)","v":19.620806794055198},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N22-M353,'Dry Bulb'!N22-M237)","v":8.5869940552016999},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O22-N353,'Dry Bulb'!O22-N237)","v":-5.5791932059447902},null,65,"Natural Ventilation Low",null,null,null,null,null,null,{"$f":"X21*AC27","v":7},"HEAD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI22","v":18},{"$f":"'Incident angle'!BJ22","v":0},{"$f":"'Incident angle'!BK22","v":0},{"$f":"'Incident angle'!BL22","v":0},{"$f":"'Incident angle'!BM22","v":0},{"$f":"'Incident angle'!BN22","v":0},{"$f":"'Incident angle'!BO22","v":0},{"$f":"'Incident angle'!BP22","v":0},{"$f":"'Incident angle'!BQ22","v":0},{"$f":"'Incident angle'!BR22","v":0},{"$f":"'Incident angle'!BS22","v":0},{"$f":"'Incident angle'!BT22","v":0},{"$f":"'Incident angle'!BU22","v":0},null,{"$f":"'Incident angle'!BW22","v":18},{"$f":"'Incident angle'!BX22","v":0},{"$f":"'Incident angle'!BY22","v":0},{"$f":"'Incident angle'!BZ22","v":0},{"$f":"'Incident angle'!CA22","v":0},{"$f":"'Incident angle'!CB22","v":0},{"$f":"'Incident angle'!CC22","v":0},{"$f":"'Incident angle'!CD22","v":0},{"$f":"'Incident angle'!CE22","v":0},{"$f":"'Incident angle'!CF22","v":0},{"$f":"'Incident angle'!CG22","v":0},{"$f":"'Incident angle'!CH22","v":0},{"$f":"'Incident angle'!CI22","v":0},null,{"$f":"'Profile angles'!B22","v":18},{"$f":"RADIANS('Profile angles'!C22)","v":-0.21383448367072511},{"$f":"RADIANS('Profile angles'!D22)","v":2.4284225922147806E-2},{"$f":"RADIANS('Profile angles'!E22)","v":1.1397000015522951},{"$f":"RADIANS('Profile angles'!F22)","v":-0.55536119281617968},{"$f":"RADIANS('Profile angles'!G22)","v":-0.47627989159216866},{"$f":"RADIANS('Profile angles'!H22)","v":-0.51670314614163193},{"$f":"RADIANS('Profile angles'!I22)","v":-0.58537590303118925},{"$f":"RADIANS('Profile angles'!J22)","v":-0.62269367861413683},{"$f":"RADIANS('Profile angles'!K22)","v":1.1397000015523899},{"$f":"RADIANS('Profile angles'!L22)","v":-0.6196827915365295},{"$f":"RADIANS('Profile angles'!M22)","v":-0.51126975196190483},{"$f":"RADIANS('Profile angles'!N22)","v":-0.37549955159039705},-1.2455602196852491,{"$f":"'Profile angles'!B51","v":18},{"$f":"RADIANS('Profile angles'!C51)","v":7.875695115485469E-2},{"$f":"RADIANS('Profile angles'!D51)","v":-5.0811936091930835E-3},{"$f":"RADIANS('Profile angles'!E51)","v":-5.8021971754233764E-2},{"$f":"RADIANS('Profile angles'!F51)","v":-0.11154632270391088},{"$f":"RADIANS('Profile angles'!G51)","v":-0.16818851648487471},{"$f":"RADIANS('Profile angles'!H51)","v":-0.2119948495476848},{"$f":"RADIANS('Profile angles'!I51)","v":-0.20643034646530076},{"$f":"RADIANS('Profile angles'!J51)","v":-0.12678973084122475},{"$f":"RADIANS('Profile angles'!K51)","v":1.4535089563006036E-3},{"$f":"RADIANS('Profile angles'!L51)","v":0.11133018006865014},{"$f":"RADIANS('Profile angles'!M51)","v":0.1759269261728052},{"$f":"RADIANS('Profile angles'!N51)","v":0.15804497456402347},null,{"$f":"'Profile angles'!AD22","v":18},{"$f":"(IF($AH$12<DEGREES(BS22),0+$AJ$16,1-((TAN(BS22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT22),0+$AJ$16,1-((TAN(BT22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU22),0+$AJ$16,1-((TAN(BU22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV22),0+$AJ$16,1-((TAN(BV22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW22),0+$AJ$16,1-((TAN(BW22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX22),0+$AJ$16,1-((TAN(BX22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY22),0+$AJ$16,1-((TAN(BY22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ22),0+$AJ$16,1-((TAN(BZ22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA22),0+$AJ$16,1-((TAN(CA22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB22),0+$AJ$16,1-((TAN(CB22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC22),0+$AJ$16,1-((TAN(CC22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH21*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD22),0+$AJ$16,1-((TAN(CD22)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI21*$DU$3)+1-$DU$3)","v":0},null,18,{"$f":"(IF($AH$46<DEGREES(CG22),0+$AJ$50,1-((TAN(CG22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL21*$DU$3)+1-$DU$3)","v":0.77953800779181948},{"$f":"(IF($AH$46<DEGREES(CH22),0+$AJ$50,1-((TAN(CH22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM21*$DU$3)+1-$DU$3)","v":0.89813029013630952},{"$f":"(IF($AH$46<DEGREES(CI22),0+$AJ$50,1-((TAN(CI22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN21*$DU$3)+1-$DU$3)","v":1.0210281692835088},{"$f":"(IF($AH$46<DEGREES(CJ22),0+$AJ$50,1-((TAN(CJ22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO21*$DU$3)+1-$DU$3)","v":0.97088281389578746},{"$f":"(IF($AH$46<DEGREES(CK22),0+$AJ$50,1-((TAN(CK22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP21*$DU$3)+1-$DU$3)","v":0.92054842583986451},{"$f":"(IF($AH$46<DEGREES(CL22),0+$AJ$50,1-((TAN(CL22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ21*$DU$3)+1-$DU$3)","v":0.91528114379407066},{"$f":"(IF($AH$46<DEGREES(CM22),0+$AJ$50,1-((TAN(CM22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR21*$DU$3)+1-$DU$3)","v":0.94784353590325221},{"$f":"(IF($AH$46<DEGREES(CN22),0+$AJ$50,1-((TAN(CN22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS21*$DU$3)+1-$DU$3)","v":0.9809225554740777},{"$f":"(IF($AH$46<DEGREES(CO22),0+$AJ$50,1-((TAN(CO22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT21*$DU$3)+1-$DU$3)","v":0.99879391558314135},{"$f":"(IF($AH$46<DEGREES(CP22),0+$AJ$50,1-((TAN(CP22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU21*$DU$3)+1-$DU$3)","v":0.85983127032158246},{"$f":"(IF($AH$46<DEGREES(CQ22),0+$AJ$50,1-((TAN(CQ22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV21*$DU$3)+1-$DU$3)","v":0.7518109937403199},{"$f":"(IF($AH$46<DEGREES(CR22),0+$AJ$50,1-((TAN(CR22)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW21*$DU$3)+1-$DU$3)","v":0.72155873370729762},null,null,{"$f":"'Profile angles'!AR22","v":18},{"$f":"'Profile angles'!AS22","v":-4.242067037456934},{"$f":"'Profile angles'!AT22","v":0.28496224246637836},{"$f":"'Profile angles'!AU22","v":3.3232309033445016},{"$f":"'Profile angles'!AV22","v":6.2903017477886056},{"$f":"'Profile angles'!AW22","v":9.1618728727979484},{"$f":"'Profile angles'!AX22","v":11.380032986011807},{"$f":"'Profile angles'!AY22","v":11.292623329902437},{"$f":"'Profile angles'!AZ22","v":7.1538265372891177},{"$f":"'Profile angles'!BA22","v":-8.3279910069723753E-2},{"$f":"'Profile angles'!BB22","v":-6.3024734223343577},{"$f":"'Profile angles'!BC22","v":-9.6180467382750852},{"$f":"'Profile angles'!BD22","v":-8.4049479592926772},null,18,-4.242067037456934,0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772]
[null,19,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D23-C354,'Dry Bulb'!D23-C238)","v":-8.4591932059447998},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E23-D354,'Dry Bulb'!E23-D238)","v":-4.4726296390658149},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F23-E354,'Dry Bulb'!F23-E238)","v":4.1600029723991412},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G23-F354,'Dry Bulb'!G23-F238)","v":12.780806794055195},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H23-G354,'Dry Bulb'!H23-G238)","v":25.740806794055203},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I23-H354,'Dry Bulb'!I23-H238)","v":32.220806794055207},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J23-I354,'Dry Bulb'!J23-I238)","v":33.660806794055205},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K23-J354,'Dry Bulb'!K23-J238)","v":33.120806794055198},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L23-K354,'Dry Bulb'!L23-K238)","v":27.360806794055208},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M23-L354,'Dry Bulb'!M23-L238)","v":17.640806794055194},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N23-M354,'Dry Bulb'!N23-M238)","v":6.1521489596602947},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O23-N354,'Dry Bulb'!O23-N238)","v":-8.0991932059447933},null,80,"Natural Ventilation High",null,null,null,null,null,10,null,null,null,null,null,"OVERHANG",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI23","v":19},{"$f":"'Incident angle'!BJ23","v":0},{"$f":"'Incident angle'!BK23","v":0},{"$f":"'Incident angle'!BL23","v":0},{"$f":"'Incident angle'!BM23","v":0},{"$f":"'Incident angle'!BN23","v":0},{"$f":"'Incident angle'!BO23","v":0},{"$f":"'Incident angle'!BP23","v":0},{"$f":"'Incident angle'!BQ23","v":0},{"$f":"'Incident angle'!BR23","v":0},{"$f":"'Incident angle'!BS23","v":0},{"$f":"'Incident angle'!BT23","v":0},{"$f":"'Incident angle'!BU23","v":0},null,{"$f":"'Incident angle'!BW23","v":19},{"$f":"'Incident angle'!BX23","v":0},{"$f":"'Incident angle'!BY23","v":0},{"$f":"'Incident angle'!BZ23","v":0},{"$f":"'Incident angle'!CA23","v":0},{"$f":"'Incident angle'!CB23","v":0},{"$f":"'Incident angle'!CC23","v":0},{"$f":"'Incident angle'!CD23","v":0},{"$f":"'Incident angle'!CE23","v":0},{"$f":"'Incident angle'!CF23","v":0},{"$f":"'Incident angle'!CG23","v":0},{"$f":"'Incident angle'!CH23","v":0},{"$f":"'Incident angle'!CI23","v":0},null,{"$f":"'Profile angles'!B23","v":19},{"$f":"RADIANS('Profile angles'!C23)","v":-0.8943190286097269},{"$f":"RADIANS('Profile angles'!D23)","v":-1.166196830362576},{"$f":"RADIANS('Profile angles'!E23)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F23)","v":0.40508921503180312},{"$f":"RADIANS('Profile angles'!G23)","v":0.1494204003451183},{"$f":"RADIANS('Profile angles'!H23)","v":4.3182419744715421E-2},{"$f":"RADIANS('Profile angles'!I23)","v":6.4699031311275218E-2},{"$f":"RADIANS('Profile angles'!J23)","v":0.36364909543045837},{"$f":"RADIANS('Profile angles'!K23)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L23)","v":-1.4298718763400156},{"$f":"RADIANS('Profile angles'!M23)","v":-1.1011153762045047},{"$f":"RADIANS('Profile angles'!N23)","v":-0.9283445131232797},null,{"$f":"'Profile angles'!B52","v":19},{"$f":"RADIANS('Profile angles'!C52)","v":0.31044316509225717},{"$f":"RADIANS('Profile angles'!D52)","v":0.23111522112121052},{"$f":"RADIANS('Profile angles'!E52)","v":0.18024728429187611},{"$f":"RADIANS('Profile angles'!F52)","v":0.12673343644358437},{"$f":"RADIANS('Profile angles'!G52)","v":6.7779708344327269E-2},{"$f":"RADIANS('Profile angles'!H52)","v":2.1587753481061966E-2},{"$f":"RADIANS('Profile angles'!I52)","v":2.8054601331330978E-2},{"$f":"RADIANS('Profile angles'!J52)","v":0.11109422861118669},{"$f":"RADIANS('Profile angles'!K52)","v":0.24026026153093591},{"$f":"RADIANS('Profile angles'!L52)","v":0.34689085936294084},{"$f":"RADIANS('Profile angles'!M52)","v":0.40600410951818994},{"$f":"RADIANS('Profile angles'!N52)","v":0.38616028192323892},null,{"$f":"'Profile angles'!AD23","v":19},{"$f":"(IF($AH$12<DEGREES(BS23),0+$AJ$16,1-((TAN(BS23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT23),0+$AJ$16,1-((TAN(BT23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU23),0+$AJ$16,1-((TAN(BU23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV23),0+$AJ$16,1-((TAN(BV23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW23),0+$AJ$16,1-((TAN(BW23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BX23),0+$AJ$16,1-((TAN(BX23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BY23),0+$AJ$16,1-((TAN(BY23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BZ23),0+$AJ$16,1-((TAN(BZ23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA23),0+$AJ$16,1-((TAN(CA23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB23),0+$AJ$16,1-((TAN(CB23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC23),0+$AJ$16,1-((TAN(CC23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH22*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD23),0+$AJ$16,1-((TAN(CD23)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI22*$DU$3)+1-$DU$3)","v":0},null,19,{"$f":"(IF($AH$46<DEGREES(CG23),0+$AJ$50,1-((TAN(CG23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL22*$DU$3)+1-$DU$3)","v":0.70351594796353956},{"$f":"(IF($AH$46<DEGREES(CH23),0+$AJ$50,1-((TAN(CH23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM22*$DU$3)+1-$DU$3)","v":0.81553692527449573},{"$f":"(IF($AH$46<DEGREES(CI23),0+$AJ$50,1-((TAN(CI23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN22*$DU$3)+1-$DU$3)","v":0.85333983124613311},{"$f":"(IF($AH$46<DEGREES(CJ23),0+$AJ$50,1-((TAN(CJ23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO22*$DU$3)+1-$DU$3)","v":0.78633709080545133},{"$f":"(IF($AH$46<DEGREES(CK23),0+$AJ$50,1-((TAN(CK23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP22*$DU$3)+1-$DU$3)","v":0.74298930768415783},{"$f":"(IF($AH$46<DEGREES(CL23),0+$AJ$50,1-((TAN(CL23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ22*$DU$3)+1-$DU$3)","v":0.74043856882082426},{"$f":"(IF($AH$46<DEGREES(CM23),0+$AJ$50,1-((TAN(CM23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR22*$DU$3)+1-$DU$3)","v":0.77024639864242495},{"$f":"(IF($AH$46<DEGREES(CN23),0+$AJ$50,1-((TAN(CN23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS22*$DU$3)+1-$DU$3)","v":0.79631808771856694},{"$f":"(IF($AH$46<DEGREES(CO23),0+$AJ$50,1-((TAN(CO23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT22*$DU$3)+1-$DU$3)","v":0.80494448577423749},{"$f":"(IF($AH$46<DEGREES(CP23),0+$AJ$50,1-((TAN(CP23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU22*$DU$3)+1-$DU$3)","v":0.76301389884783355},{"$f":"(IF($AH$46<DEGREES(CQ23),0+$AJ$50,1-((TAN(CQ23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV22*$DU$3)+1-$DU$3)","v":0.66110868526651356},{"$f":"(IF($AH$46<DEGREES(CR23),0+$AJ$50,1-((TAN(CR23)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW22*$DU$3)+1-$DU$3)","v":0.64103560733224574},null,null,{"$f":"'Profile angles'!AR23","v":19},{"$f":"'Profile angles'!AS23","v":-17.258784755357599},{"$f":"'Profile angles'!AT23","v":-13.177535073458104},{"$f":"'Profile angles'!AU23","v":-10.292097151668569},{"$f":"'Profile angles'!AV23","v":-6.9635212465343193},{"$f":"'Profile angles'!AW23","v":-3.5411252469823715},{"$f":"'Profile angles'!AX23","v":-1.1064784283971907},{"$f":"'Profile angles'!AY23","v":-1.4750612815819091},{"$f":"'Profile angles'!AZ23","v":-6.1102162570653853},{"$f":"'Profile angles'!BA23","v":-13.682588857300294},{"$f":"'Profile angles'!BB23","v":-19.851334869589788},{"$f":"'Profile angles'!BC23","v":-22.782734775346487},{"$f":"'Profile angles'!BD23","v":-21.2544074674176},null,19,-17.258784755357599,-13.177535073458104,-10.292097151668569,-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176]
[null,20,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D24-C355,'Dry Bulb'!D24-C239)","v":-3.4391932059447896},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E24-D355,'Dry Bulb'!E24-D239)","v":-5.0391932059447981},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F24-E355,'Dry Bulb'!F24-E239)","v":1.0611092144373657},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G24-F355,'Dry Bulb'!G24-F239)","v":11.160806794055205},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H24-G355,'Dry Bulb'!H24-G239)","v":23.400806794055214},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I24-H355,'Dry Bulb'!I24-H239)","v":29.700806794055211},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J24-I355,'Dry Bulb'!J24-I239)","v":30.060806794055196},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K24-J355,'Dry Bulb'!K24-J239)","v":30.240806794055203},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L24-K355,'Dry Bulb'!L24-K239)","v":25.020806794055204},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M24-L355,'Dry Bulb'!M24-L239)","v":14.580806794055206},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N24-M355,'Dry Bulb'!N24-M239)","v":3.0532552016985193},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O24-N355,'Dry Bulb'!O24-N239)","v":-9.8991932059447976},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI24","v":20},{"$f":"'Incident angle'!BJ24","v":0},{"$f":"'Incident angle'!BK24","v":0},{"$f":"'Incident angle'!BL24","v":0},{"$f":"'Incident angle'!BM24","v":0},{"$f":"'Incident angle'!BN24","v":0},{"$f":"'Incident angle'!BO24","v":0},{"$f":"'Incident angle'!BP24","v":0},{"$f":"'Incident angle'!BQ24","v":0},{"$f":"'Incident angle'!BR24","v":0},{"$f":"'Incident angle'!BS24","v":0},{"$f":"'Incident angle'!BT24","v":0},{"$f":"'Incident angle'!BU24","v":0},null,{"$f":"'Incident angle'!BW24","v":20},{"$f":"'Incident angle'!BX24","v":0},{"$f":"'Incident angle'!BY24","v":0},{"$f":"'Incident angle'!BZ24","v":0},{"$f":"'Incident angle'!CA24","v":0},{"$f":"'Incident angle'!CB24","v":0},{"$f":"'Incident angle'!CC24","v":0},{"$f":"'Incident angle'!CD24","v":0},{"$f":"'Incident angle'!CE24","v":0},{"$f":"'Incident angle'!CF24","v":0},{"$f":"'Incident angle'!CG24","v":0},{"$f":"'Incident angle'!CH24","v":0},{"$f":"'Incident angle'!CI24","v":0},null,{"$f":"'Profile angles'!B24","v":20},{"$f":"RADIANS('Profile angles'!C24)","v":-1.3012298625660645},{"$f":"RADIANS('Profile angles'!D24)","v":1.5601818868055648},{"$f":"RADIANS('Profile angles'!E24)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F24)","v":0.72371978813644855},{"$f":"RADIANS('Profile angles'!G24)","v":0.4885607623749027},{"$f":"RADIANS('Profile angles'!H24)","v":0.39161342241702657},{"$f":"RADIANS('Profile angles'!I24)","v":0.44511249062286384},{"$f":"RADIANS('Profile angles'!J24)","v":0.70652153014812857},{"$f":"RADIANS('Profile angles'!K24)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L24)","v":1.4816256583034377},{"$f":"RADIANS('Profile angles'!M24)","v":-1.3982180222701845},{"$f":"RADIANS('Profile angles'!N24)","v":-1.2659457689719542},null,{"$f":"'Profile angles'!B53","v":20},{"$f":"RADIANS('Profile angles'!C53)","v":0.53982440647106411},{"$f":"RADIANS('Profile angles'!D53)","v":0.46745924354256657},{"$f":"RADIANS('Profile angles'!E53)","v":0.42271676310413892},{"$f":"RADIANS('Profile angles'!F53)","v":0.37438414286885741},{"$f":"RADIANS('Profile angles'!G53)","v":0.31663095237958916},{"$f":"RADIANS('Profile angles'!H53)","v":0.26866082450954953},{"$f":"RADIANS('Profile angles'!I53)","v":0.27434316021105154},{"$f":"RADIANS('Profile angles'!J53)","v":0.35806173657168089},{"$f":"RADIANS('Profile angles'!K53)","v":0.48459652421088528},{"$f":"RADIANS('Profile angles'!L53)","v":0.58500248706259217},{"$f":"RADIANS('Profile angles'!M53)","v":0.6358430799641186},{"$f":"RADIANS('Profile angles'!N53)","v":0.61217498892976285},null,{"$f":"'Profile angles'!AD24","v":20},{"$f":"(IF($AH$12<DEGREES(BS24),0+$AJ$16,1-((TAN(BS24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX23*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT24),0+$AJ$16,1-((TAN(BT24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY23*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU24),0+$AJ$16,1-((TAN(BU24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ23*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV24),0+$AJ$16,1-((TAN(BV24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA23*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BW24),0+$AJ$16,1-((TAN(BW24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB23*$DU$3)+1-$DU$3)","v":0.11859549184475496},{"$f":"(IF($AH$12<DEGREES(BX24),0+$AJ$16,1-((TAN(BX24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC23*$DU$3)+1-$DU$3)","v":0.17777794686140672},{"$f":"(IF($AH$12<DEGREES(BY24),0+$AJ$16,1-((TAN(BY24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD23*$DU$3)+1-$DU$3)","v":0.10157455370985745},{"$f":"(IF($AH$12<DEGREES(BZ24),0+$AJ$16,1-((TAN(BZ24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE23*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CA24),0+$AJ$16,1-((TAN(CA24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF23*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB24),0+$AJ$16,1-((TAN(CB24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG23*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC24),0+$AJ$16,1-((TAN(CC24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH23*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD24),0+$AJ$16,1-((TAN(CD24)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI23*$DU$3)+1-$DU$3)","v":0},null,20,{"$f":"(IF($AH$46<DEGREES(CG24),0+$AJ$50,1-((TAN(CG24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL23*$DU$3)+1-$DU$3)","v":0.58746881351891111},{"$f":"(IF($AH$46<DEGREES(CH24),0+$AJ$50,1-((TAN(CH24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM23*$DU$3)+1-$DU$3)","v":0.69526814305462892},{"$f":"(IF($AH$46<DEGREES(CI24),0+$AJ$50,1-((TAN(CI24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN23*$DU$3)+1-$DU$3)","v":0.6545698489826316},{"$f":"(IF($AH$46<DEGREES(CJ24),0+$AJ$50,1-((TAN(CJ24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO23*$DU$3)+1-$DU$3)","v":0.59434244307423112},{"$f":"(IF($AH$46<DEGREES(CK24),0+$AJ$50,1-((TAN(CK24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP23*$DU$3)+1-$DU$3)","v":0.55578752822853306},{"$f":"(IF($AH$46<DEGREES(CL24),0+$AJ$50,1-((TAN(CL24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ23*$DU$3)+1-$DU$3)","v":0.5565175435190628},{"$f":"(IF($AH$46<DEGREES(CM24),0+$AJ$50,1-((TAN(CM24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR23*$DU$3)+1-$DU$3)","v":0.5859638622887422},{"$f":"(IF($AH$46<DEGREES(CN24),0+$AJ$50,1-((TAN(CN24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS23*$DU$3)+1-$DU$3)","v":0.60549058716359716},{"$f":"(IF($AH$46<DEGREES(CO24),0+$AJ$50,1-((TAN(CO24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT23*$DU$3)+1-$DU$3)","v":0.60129059129344997},{"$f":"(IF($AH$46<DEGREES(CP24),0+$AJ$50,1-((TAN(CP24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU23*$DU$3)+1-$DU$3)","v":0.58475253469438437},{"$f":"(IF($AH$46<DEGREES(CQ24),0+$AJ$50,1-((TAN(CQ24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV23*$DU$3)+1-$DU$3)","v":0.52129773029111925},{"$f":"(IF($AH$46<DEGREES(CR24),0+$AJ$50,1-((TAN(CR24)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW23*$DU$3)+1-$DU$3)","v":0.51477351947707473},null,null,{"$f":"'Profile angles'!AR24","v":20},{"$f":"'Profile angles'!AS24","v":-30.589239677830651},{"$f":"'Profile angles'!AT24","v":-26.783110901661868},{"$f":"'Profile angles'!AU24","v":-23.773745192987072},{"$f":"'Profile angles'!AV24","v":-19.749387170381588},{"$f":"'Profile angles'!AW24","v":-15.584861719885295},{"$f":"'Profile angles'!AX24","v":-12.902247652391463},{"$f":"'Profile angles'!AY24","v":-13.625605199002544},{"$f":"'Profile angles'!AZ24","v":-18.916708643772196},{"$f":"'Profile angles'!BA24","v":-27.097900221004799},{"$f":"'Profile angles'!BB24","v":-33.472019280706604},{"$f":"'Profile angles'!BC24","v":-36.206670576844481},{"$f":"'Profile angles'!BD24","v":-34.435555539572299},null,20,-30.589239677830651,-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,-12.902247652391463,-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299]
[null,21,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D25-C356,'Dry Bulb'!D25-C240)","v":-4.6991932059447947},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E25-D356,'Dry Bulb'!E25-D240)","v":-6.8391932059447953},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F25-E356,'Dry Bulb'!F25-E240)","v":-0.70968721868365492},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G25-F356,'Dry Bulb'!G25-F240)","v":10.579140042462839},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H25-G356,'Dry Bulb'!H25-G240)","v":21.42080679405521},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I25-H356,'Dry Bulb'!I25-H240)","v":27.000806794055208},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J25-I356,'Dry Bulb'!J25-I240)","v":27.180806794055201},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K25-J356,'Dry Bulb'!K25-J240)","v":28.260806794055199},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L25-K356,'Dry Bulb'!L25-K240)","v":22.500806794055208},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M25-L356,'Dry Bulb'!M25-L240)","v":12.600806794055202},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N25-M356,'Dry Bulb'!N25-M240)","v":1.0611092144373657},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O25-N356,'Dry Bulb'!O25-N240)","v":-4.1591932059447956},null,{"$f":"Q26/8","v":0.5},"Nat Vent Air Changes",null,null,null,null,null,"Window Height",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI25","v":21},{"$f":"'Incident angle'!BJ25","v":0},{"$f":"'Incident angle'!BK25","v":0},{"$f":"'Incident angle'!BL25","v":0},{"$f":"'Incident angle'!BM25","v":0},{"$f":"'Incident angle'!BN25","v":0},{"$f":"'Incident angle'!BO25","v":0},{"$f":"'Incident angle'!BP25","v":0},{"$f":"'Incident angle'!BQ25","v":0},{"$f":"'Incident angle'!BR25","v":0},{"$f":"'Incident angle'!BS25","v":0},{"$f":"'Incident angle'!BT25","v":0},{"$f":"'Incident angle'!BU25","v":0},null,{"$f":"'Incident angle'!BW25","v":21},{"$f":"'Incident angle'!BX25","v":0},{"$f":"'Incident angle'!BY25","v":0},{"$f":"'Incident angle'!BZ25","v":0},{"$f":"'Incident angle'!CA25","v":0},{"$f":"'Incident angle'!CB25","v":0},{"$f":"'Incident angle'!CC25","v":0},{"$f":"'Incident angle'!CD25","v":0},{"$f":"'Incident angle'!CE25","v":0},{"$f":"'Incident angle'!CF25","v":0},{"$f":"'Incident angle'!CG25","v":0},{"$f":"'Incident angle'!CH25","v":0},{"$f":"'Incident angle'!CI25","v":0},null,{"$f":"'Profile angles'!B25","v":21},{"$f":"RADIANS('Profile angles'!C25)","v":-1.4926689138225644},{"$f":"RADIANS('Profile angles'!D25)","v":1.424466119880013},{"$f":"RADIANS('Profile angles'!E25)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F25)","v":0.84257659010007879},{"$f":"RADIANS('Profile angles'!G25)","v":0.65069747813555467},{"$f":"RADIANS('Profile angles'!H25)","v":0.5720711137075446},{"$f":"RADIANS('Profile angles'!I25)","v":0.62738252671884265},{"$f":"RADIANS('Profile angles'!J25)","v":0.8330645277261437},{"$f":"RADIANS('Profile angles'!K25)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L25)","v":1.3922681911981456},{"$f":"RADIANS('Profile angles'!M25)","v":-1.5401075773273574},{"$f":"RADIANS('Profile angles'!N25)","v":-1.440555126370102},{"$f":"TAN($AG$14)","v":1.4285714285714286},{"$f":"'Profile angles'!B54","v":21},{"$f":"RADIANS('Profile angles'!C54)","v":0.77137406354258076},{"$f":"RADIANS('Profile angles'!D54)","v":0.70858778624744145},{"$f":"RADIANS('Profile angles'!E54)","v":0.67432329522984613},{"$f":"RADIANS('Profile angles'!F54)","v":0.63740014217672603},{"$f":"RADIANS('Profile angles'!G54)","v":0.58586265313688612},{"$f":"RADIANS('Profile angles'!H54)","v":0.5374341930134342},{"$f":"RADIANS('Profile angles'!I54)","v":0.53995019403937616},{"$f":"RADIANS('Profile angles'!J54)","v":0.6201738526973527},{"$f":"RADIANS('Profile angles'!K54)","v":0.73908870770470358},{"$f":"RADIANS('Profile angles'!L54)","v":0.82955153298556916},{"$f":"RADIANS('Profile angles'!M54)","v":0.86919421625434168},{"$f":"RADIANS('Profile angles'!N54)","v":0.84017901380444071},null,{"$f":"'Profile angles'!AD25","v":21},{"$f":"(IF($AH$12<DEGREES(BS25),0+$AJ$16,1-((TAN(BS25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX24*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT25),0+$AJ$16,1-((TAN(BT25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY24*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU25),0+$AJ$16,1-((TAN(BU25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ24*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV25),0+$AJ$16,1-((TAN(BV25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA24*$DU$3)+1-$DU$3)","v":5.2200835794105185E-2},{"$f":"(IF($AH$12<DEGREES(BW25),0+$AJ$16,1-((TAN(BW25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB24*$DU$3)+1-$DU$3)","v":0.1991491440752769},{"$f":"(IF($AH$12<DEGREES(BX25),0+$AJ$16,1-((TAN(BX25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC24*$DU$3)+1-$DU$3)","v":0.25254089412404812},{"$f":"(IF($AH$12<DEGREES(BY25),0+$AJ$16,1-((TAN(BY25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD24*$DU$3)+1-$DU$3)","v":0.19455318249198542},{"$f":"(IF($AH$12<DEGREES(BZ25),0+$AJ$16,1-((TAN(BZ25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE24*$DU$3)+1-$DU$3)","v":5.2812448937765856E-2},{"$f":"(IF($AH$12<DEGREES(CA25),0+$AJ$16,1-((TAN(CA25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF24*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB25),0+$AJ$16,1-((TAN(CB25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG24*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC25),0+$AJ$16,1-((TAN(CC25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH24*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD25),0+$AJ$16,1-((TAN(CD25)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI24*$DU$3)+1-$DU$3)","v":0},null,21,{"$f":"(IF($AH$46<DEGREES(CG25),0+$AJ$50,1-((TAN(CG25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL24*$DU$3)+1-$DU$3)","v":0.40074130782736139},{"$f":"(IF($AH$46<DEGREES(CH25),0+$AJ$50,1-((TAN(CH25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM24*$DU$3)+1-$DU$3)","v":0.45507433601232794},{"$f":"(IF($AH$46<DEGREES(CI25),0+$AJ$50,1-((TAN(CI25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN24*$DU$3)+1-$DU$3)","v":0.42474787977658673},{"$f":"(IF($AH$46<DEGREES(CJ25),0+$AJ$50,1-((TAN(CJ25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO24*$DU$3)+1-$DU$3)","v":0.37222431252252275},{"$f":"(IF($AH$46<DEGREES(CK25),0+$AJ$50,1-((TAN(CK25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP24*$DU$3)+1-$DU$3)","v":0.3395545665341676},{"$f":"(IF($AH$46<DEGREES(CL25),0+$AJ$50,1-((TAN(CL25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ24*$DU$3)+1-$DU$3)","v":0.34513497943255733},{"$f":"(IF($AH$46<DEGREES(CM25),0+$AJ$50,1-((TAN(CM25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR24*$DU$3)+1-$DU$3)","v":0.37572004472629239},{"$f":"(IF($AH$46<DEGREES(CN25),0+$AJ$50,1-((TAN(CN25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS24*$DU$3)+1-$DU$3)","v":0.38600679541644528},{"$f":"(IF($AH$46<DEGREES(CO25),0+$AJ$50,1-((TAN(CO25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT24*$DU$3)+1-$DU$3)","v":0.35816682101121894},{"$f":"(IF($AH$46<DEGREES(CP25),0+$AJ$50,1-((TAN(CP25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU24*$DU$3)+1-$DU$3)","v":0.31057179405950269},{"$f":"(IF($AH$46<DEGREES(CQ25),0+$AJ$50,1-((TAN(CQ25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV24*$DU$3)+1-$DU$3)","v":0.28469974411572713},{"$f":"(IF($AH$46<DEGREES(CR25),0+$AJ$50,1-((TAN(CR25)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW24*$DU$3)+1-$DU$3)","v":0.30623183085963968},null,null,{"$f":"'Profile angles'!AR25","v":21},{"$f":"'Profile angles'!AS25","v":-44.11375465474292},{"$f":"'Profile angles'!AT25","v":-40.375142281624065},{"$f":"'Profile angles'!AU25","v":-36.877998514340369},{"$f":"'Profile angles'!AV25","v":-31.713766855869693},{"$f":"'Profile angles'!AW25","v":-26.575515215416551},{"$f":"'Profile angles'!AX25","v":-23.623016903493113},{"$f":"'Profile angles'!AY25","v":-24.79570873532365},{"$f":"'Profile angles'!AZ25","v":-30.92280247893752},{"$f":"'Profile angles'!BA25","v":-40.048756889246128},{"$f":"'Profile angles'!BB25","v":-46.985407153208357},{"$f":"'Profile angles'!BC25","v":-49.782532508401836},{"$f":"'Profile angles'!BD25","v":-47.837496220337762},null,21,-44.11375465474292,-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762]
[null,22,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D26-C357,'Dry Bulb'!D26-C241)","v":-6.1391932059447925},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E26-D357,'Dry Bulb'!E26-D241)","v":-8.6391932059447925},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F26-E357,'Dry Bulb'!F26-E241)","v":-2.7018332059447943},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G26-F357,'Dry Bulb'!G26-F241)","v":8.5869940552016999},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H26-G357,'Dry Bulb'!H26-G241)","v":19.620806794055198},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I26-H357,'Dry Bulb'!I26-H241)","v":24.660806794055205},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J26-I357,'Dry Bulb'!J26-I241)","v":24.480806794055212},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K26-J357,'Dry Bulb'!K26-J241)","v":26.280806794055209},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L26-K357,'Dry Bulb'!L26-K241)","v":20.700806794055211},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M26-L357,'Dry Bulb'!M26-L241)","v":10.620806794055198},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N26-M357,'Dry Bulb'!N26-M241)","v":-1.3737358811040394},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O26-N357,'Dry Bulb'!O26-N241)","v":-5.4191932059447936},null,null,4,null,null,"Occupant Density",null,null,null,1,null,null,null,null,"Lab Override",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI26","v":22},{"$f":"'Incident angle'!BJ26","v":0},{"$f":"'Incident angle'!BK26","v":0},{"$f":"'Incident angle'!BL26","v":0},{"$f":"'Incident angle'!BM26","v":0},{"$f":"'Incident angle'!BN26","v":0},{"$f":"'Incident angle'!BO26","v":0},{"$f":"'Incident angle'!BP26","v":0},{"$f":"'Incident angle'!BQ26","v":0},{"$f":"'Incident angle'!BR26","v":0},{"$f":"'Incident angle'!BS26","v":0},{"$f":"'Incident angle'!BT26","v":0},{"$f":"'Incident angle'!BU26","v":0},null,{"$f":"'Incident angle'!BW26","v":22},{"$f":"'Incident angle'!BX26","v":0},{"$f":"'Incident angle'!BY26","v":0},{"$f":"'Incident angle'!BZ26","v":0},{"$f":"'Incident angle'!CA26","v":0},{"$f":"'Incident angle'!CB26","v":0},{"$f":"'Incident angle'!CC26","v":0},{"$f":"'Incident angle'!CD26","v":0},{"$f":"'Incident angle'!CE26","v":0},{"$f":"'Incident angle'!CF26","v":0},{"$f":"'Incident angle'!CG26","v":0},{"$f":"'Incident angle'!CH26","v":0},{"$f":"'Incident angle'!CI26","v":0},null,{"$f":"'Profile angles'!B26","v":22},{"$f":"RADIANS('Profile angles'!C26)","v":1.5539445877602391},{"$f":"RADIANS('Profile angles'!D26)","v":1.3649967109877184},{"$f":"RADIANS('Profile angles'!E26)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F26)","v":0.89738136477565211},{"$f":"RADIANS('Profile angles'!G26)","v":0.73245268972748756},{"$f":"RADIANS('Profile angles'!H26)","v":0.6663048373130509},{"$f":"RADIANS('Profile angles'!I26)","v":0.71892314829995663},{"$f":"RADIANS('Profile angles'!J26)","v":0.89109084416912154},{"$f":"RADIANS('Profile angles'!K26)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L26)","v":1.3503950367995554},{"$f":"RADIANS('Profile angles'!M26)","v":1.529878658594682},{"$f":"RADIANS('Profile angles'!N26)","v":-1.5317777100487906},null,{"$f":"'Profile angles'!B55","v":22},{"$f":"RADIANS('Profile angles'!C55)","v":1.0077487946336263},{"$f":"RADIANS('Profile angles'!D55)","v":0.95743316995573291},{"$f":"RADIANS('Profile angles'!E55)","v":0.9383140971407391},{"$f":"RADIANS('Profile angles'!F55)","v":0.92011364949964081},{"$f":"RADIANS('Profile angles'!G55)","v":0.88176474027935992},{"$f":"RADIANS('Profile angles'!H55)","v":0.83552237145082953},{"$f":"RADIANS('Profile angles'!I55)","v":0.83162347526531166},{"$f":"RADIANS('Profile angles'!J55)","v":0.90195784379562749},{"$f":"RADIANS('Profile angles'!K55)","v":1.0063600686241212},{"$f":"RADIANS('Profile angles'!L55)","v":1.0823876155652608},{"$f":"RADIANS('Profile angles'!M55)","v":1.1078788719054964},{"$f":"RADIANS('Profile angles'!N55)","v":1.0723844562125873},null,{"$f":"'Profile angles'!AD26","v":22},{"$f":"(IF($AH$12<DEGREES(BS26),0+$AJ$16,1-((TAN(BS26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX25*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT26),0+$AJ$16,1-((TAN(BT26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY25*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU26),0+$AJ$16,1-((TAN(BU26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ25*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV26),0+$AJ$16,1-((TAN(BV26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA25*$DU$3)+1-$DU$3)","v":6.411711493138933E-2},{"$f":"(IF($AH$12<DEGREES(BW26),0+$AJ$16,1-((TAN(BW26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB25*$DU$3)+1-$DU$3)","v":0.23324132788029195},{"$f":"(IF($AH$12<DEGREES(BX26),0+$AJ$16,1-((TAN(BX26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC25*$DU$3)+1-$DU$3)","v":0.28974892003021235},{"$f":"(IF($AH$12<DEGREES(BY26),0+$AJ$16,1-((TAN(BY26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD25*$DU$3)+1-$DU$3)","v":0.23286147677677443},{"$f":"(IF($AH$12<DEGREES(BZ26),0+$AJ$16,1-((TAN(BZ26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE25*$DU$3)+1-$DU$3)","v":6.8399918242291358E-2},{"$f":"(IF($AH$12<DEGREES(CA26),0+$AJ$16,1-((TAN(CA26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF25*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB26),0+$AJ$16,1-((TAN(CB26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG25*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC26),0+$AJ$16,1-((TAN(CC26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH25*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD26),0+$AJ$16,1-((TAN(CD26)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI25*$DU$3)+1-$DU$3)","v":0},null,22,{"$f":"(IF($AH$46<DEGREES(CG26),0+$AJ$50,1-((TAN(CG26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL25*$DU$3)+1-$DU$3)","v":4.8774351679286509E-2},{"$f":"(IF($AH$46<DEGREES(CH26),0+$AJ$50,1-((TAN(CH26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM25*$DU$3)+1-$DU$3)","v":0.12575744451747839},{"$f":"(IF($AH$46<DEGREES(CI26),0+$AJ$50,1-((TAN(CI26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN25*$DU$3)+1-$DU$3)","v":0.12445386723352138},{"$f":"(IF($AH$46<DEGREES(CJ26),0+$AJ$50,1-((TAN(CJ26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO25*$DU$3)+1-$DU$3)","v":0.10084288131344858},{"$f":"(IF($AH$46<DEGREES(CK26),0+$AJ$50,1-((TAN(CK26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP25*$DU$3)+1-$DU$3)","v":8.8280235467356027E-2},{"$f":"(IF($AH$46<DEGREES(CL26),0+$AJ$50,1-((TAN(CL26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ25*$DU$3)+1-$DU$3)","v":9.9943492783885521E-2},{"$f":"(IF($AH$46<DEGREES(CM26),0+$AJ$50,1-((TAN(CM26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR25*$DU$3)+1-$DU$3)","v":0.12757892280304409},{"$f":"(IF($AH$46<DEGREES(CN26),0+$AJ$50,1-((TAN(CN26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS25*$DU$3)+1-$DU$3)","v":0.11771512561354128},{"$f":"(IF($AH$46<DEGREES(CO26),0+$AJ$50,1-((TAN(CO26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT25*$DU$3)+1-$DU$3)","v":3.3336792963262578E-2},{"$f":"(IF($AH$46<DEGREES(CP26),0+$AJ$50,1-((TAN(CP26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU25*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CQ26),0+$AJ$50,1-((TAN(CQ26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV25*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CR26),0+$AJ$50,1-((TAN(CR26)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW25*$DU$3)+1-$DU$3)","v":0},null,null,{"$f":"'Profile angles'!AR26","v":22},{"$f":"'Profile angles'!AS26","v":-57.730536859646747},{"$f":"'Profile angles'!AT26","v":-53.7124665497957},{"$f":"'Profile angles'!AU26","v":-49.130640449349315},{"$f":"'Profile angles'!AV26","v":-42.202232941267965},{"$f":"'Profile angles'!AW26","v":-35.853933091501311},{"$f":"'Profile angles'!AX26","v":-32.649969945256942},{"$f":"'Profile angles'!AY26","v":-34.377195915482893},{"$f":"'Profile angles'!AZ26","v":-41.497131280000914},{"$f":"'Profile angles'!BA26","v":-51.954064465377563},{"$f":"'Profile angles'!BB26","v":-60.030194510304511},{"$f":"'Profile angles'!BC26","v":-63.399939655490947},{"$f":"'Profile angles'!BD26","v":-61.381330079855132},null,22,-57.730536859646747,-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132]
[null,23,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D27-C358,'Dry Bulb'!D27-C242)","v":-7.3991932059447976},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E27-D358,'Dry Bulb'!E27-D242)","v":-3.0791932059447973},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F27-E358,'Dry Bulb'!F27-E242)","v":-4.4726296390658149},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G27-F358,'Dry Bulb'!G27-F242)","v":5.930799405520176},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H27-G358,'Dry Bulb'!H27-G242)","v":17.820806794055201},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I27-H358,'Dry Bulb'!I27-H242)","v":22.860806794055208},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J27-I358,'Dry Bulb'!J27-I242)","v":23.0408067940552},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K27-J358,'Dry Bulb'!K27-J242)","v":24.660806794055205},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L27-K358,'Dry Bulb'!L27-K242)","v":18.900806794055214},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M27-L358,'Dry Bulb'!M27-L242)","v":9.9150913800424689},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N27-M358,'Dry Bulb'!N27-M242)","v":-3.8085809766454446},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O27-N358,'Dry Bulb'!O27-N242)","v":-6.3191932059447993},null,null,null,null,null,200,null,null,null,2,null,null,null,null,{"$f":"'HVAC Dashboard'!AC38","v":1},null,null,"Tanδ =  ",null,{"$f":"IF(X22>0,W23/X22,99999999)","v":1.4285714285714286},null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI27","v":23},{"$f":"'Incident angle'!BJ27","v":0},{"$f":"'Incident angle'!BK27","v":0},{"$f":"'Incident angle'!BL27","v":0},{"$f":"'Incident angle'!BM27","v":0},{"$f":"'Incident angle'!BN27","v":0},{"$f":"'Incident angle'!BO27","v":0},{"$f":"'Incident angle'!BP27","v":0},{"$f":"'Incident angle'!BQ27","v":0},{"$f":"'Incident angle'!BR27","v":0},{"$f":"'Incident angle'!BS27","v":0},{"$f":"'Incident angle'!BT27","v":0},{"$f":"'Incident angle'!BU27","v":0},null,{"$f":"'Incident angle'!BW27","v":23},{"$f":"'Incident angle'!BX27","v":0},{"$f":"'Incident angle'!BY27","v":0},{"$f":"'Incident angle'!BZ27","v":0},{"$f":"'Incident angle'!CA27","v":0},{"$f":"'Incident angle'!CB27","v":0},{"$f":"'Incident angle'!CC27","v":0},{"$f":"'Incident angle'!CD27","v":0},{"$f":"'Incident angle'!CE27","v":0},{"$f":"'Incident angle'!CF27","v":0},{"$f":"'Incident angle'!CG27","v":0},{"$f":"'Incident angle'!CH27","v":0},{"$f":"'Incident angle'!CI27","v":0},null,{"$f":"'Profile angles'!B27","v":23},{"$f":"RADIANS('Profile angles'!C27)","v":1.5065295005919666},{"$f":"RADIANS('Profile angles'!D27)","v":1.3366001752956176},{"$f":"RADIANS('Profile angles'!E27)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!F27)","v":0.92334688213375749},{"$f":"RADIANS('Profile angles'!G27)","v":0.77241907924890529},{"$f":"RADIANS('Profile angles'!H27)","v":0.71359161627872214},{"$f":"RADIANS('Profile angles'!I27)","v":0.76448334246392124},{"$f":"RADIANS('Profile angles'!J27)","v":0.91872689706604016},{"$f":"RADIANS('Profile angles'!K27)","v":1.1397000015522973},{"$f":"RADIANS('Profile angles'!L27)","v":1.3311946610818084},{"$f":"RADIANS('Profile angles'!M27)","v":1.495858034964566},{"$f":"RADIANS('Profile angles'!N27)","v":1.5643267445715632},null,{"$f":"'Profile angles'!B56","v":23},{"$f":"RADIANS('Profile angles'!C56)","v":1.2495488396557735},{"$f":"RADIANS('Profile angles'!D56)","v":1.2145605673757462},{"$f":"RADIANS('Profile angles'!E56)","v":1.2149427363314722},{"$f":"RADIANS('Profile angles'!F56)","v":1.2226710666204357},{"$f":"RADIANS('Profile angles'!G56)","v":1.2055266879907172},{"$f":"RADIANS('Profile angles'!H56)","v":1.1656612779447797},{"$f":"RADIANS('Profile angles'!I56)","v":1.1517497376977253},{"$f":"RADIANS('Profile angles'!J56)","v":1.2039013058414905},{"$f":"RADIANS('Profile angles'!K56)","v":1.2857310025410158},{"$f":"RADIANS('Profile angles'!L56)","v":1.3427580313462963},{"$f":"RADIANS('Profile angles'!M56)","v":1.3516188465533332},{"$f":"RADIANS('Profile angles'!N56)","v":1.309046406575489},null,{"$f":"'Profile angles'!AD27","v":23},{"$f":"(IF($AH$12<DEGREES(BS27),0+$AJ$16,1-((TAN(BS27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT27),0+$AJ$16,1-((TAN(BT27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU27),0+$AJ$16,1-((TAN(BU27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV27),0+$AJ$16,1-((TAN(BV27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA26*$DU$3)+1-$DU$3)","v":5.6474080423750274E-2},{"$f":"(IF($AH$12<DEGREES(BW27),0+$AJ$16,1-((TAN(BW27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB26*$DU$3)+1-$DU$3)","v":0.25870202335873743},{"$f":"(IF($AH$12<DEGREES(BX27),0+$AJ$16,1-((TAN(BX27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC26*$DU$3)+1-$DU$3)","v":0.320808283439937},{"$f":"(IF($AH$12<DEGREES(BY27),0+$AJ$16,1-((TAN(BY27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD26*$DU$3)+1-$DU$3)","v":0.25848175047538002},{"$f":"(IF($AH$12<DEGREES(BZ27),0+$AJ$16,1-((TAN(BZ27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE26*$DU$3)+1-$DU$3)","v":6.2215353109736388E-2},{"$f":"(IF($AH$12<DEGREES(CA27),0+$AJ$16,1-((TAN(CA27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB27),0+$AJ$16,1-((TAN(CB27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC27),0+$AJ$16,1-((TAN(CC27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD27),0+$AJ$16,1-((TAN(CD27)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI26*$DU$3)+1-$DU$3)","v":0},null,23,{"$f":"(IF($AH$46<DEGREES(CG27),0+$AJ$50,1-((TAN(CG27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CH27),0+$AJ$50,1-((TAN(CH27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CI27),0+$AJ$50,1-((TAN(CI27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CJ27),0+$AJ$50,1-((TAN(CJ27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CK27),0+$AJ$50,1-((TAN(CK27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CL27),0+$AJ$50,1-((TAN(CL27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CM27),0+$AJ$50,1-((TAN(CM27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CN27),0+$AJ$50,1-((TAN(CN27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CO27),0+$AJ$50,1-((TAN(CO27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CP27),0+$AJ$50,1-((TAN(CP27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CQ27),0+$AJ$50,1-((TAN(CQ27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV26*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CR27),0+$AJ$50,1-((TAN(CR27)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW26*$DU$3)+1-$DU$3)","v":0},null,null,{"$f":"'Profile angles'!AR27","v":23},{"$f":"'Profile angles'!AS27","v":-71.276413671366612},{"$f":"'Profile angles'!AT27","v":-66.153465993410151},{"$f":"'Profile angles'!AU27","v":-59.402009530792824},{"$f":"'Profile angles'!AV27","v":-50.011386554405469},{"$f":"'Profile angles'!AW27","v":-42.39742803240717},{"$f":"'Profile angles'!AX27","v":-39.064492418979341},{"$f":"'Profile angles'!AY27","v":-41.409864595350896},{"$f":"'Profile angles'!AZ27","v":-49.478233796277678},{"$f":"'Profile angles'!BA27","v":-61.393251168859493},{"$f":"'Profile angles'!BB27","v":-71.378499679687209},{"$f":"'Profile angles'!BC27","v":-76.771747562226409},{"$f":"'Profile angles'!BD27","v":-74.998658692112272},null,23,-71.276413671366612,-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272]
[null,24,{"$f":"IF($T$36=\"y\",'Dry Bulb'!D28-C359,'Dry Bulb'!D28-C243)","v":-8.2991932059447961},{"$f":"IF($T$36=\"y\",'Dry Bulb'!E28-D359,'Dry Bulb'!E28-D243)","v":-4.6991932059447947},{"$f":"IF($T$36=\"y\",'Dry Bulb'!F28-E359,'Dry Bulb'!F28-E243)","v":-6.2434260721868355},{"$f":"IF($T$36=\"y\",'Dry Bulb'!G28-F359,'Dry Bulb'!G28-F243)","v":4.1600029723991412},{"$f":"IF($T$36=\"y\",'Dry Bulb'!H28-G359,'Dry Bulb'!H28-G243)","v":16.200806794055211},{"$f":"IF($T$36=\"y\",'Dry Bulb'!I28-H359,'Dry Bulb'!I28-H243)","v":21.060806794055196},{"$f":"IF($T$36=\"y\",'Dry Bulb'!J28-I359,'Dry Bulb'!J28-I243)","v":21.780806794055209},{"$f":"IF($T$36=\"y\",'Dry Bulb'!K28-J359,'Dry Bulb'!K28-J243)","v":22.860806794055208},{"$f":"IF($T$36=\"y\",'Dry Bulb'!L28-K359,'Dry Bulb'!L28-K243)","v":17.280806794055209},{"$f":"IF($T$36=\"y\",'Dry Bulb'!M28-L359,'Dry Bulb'!M28-L243)","v":8.1442949469214483},{"$f":"IF($T$36=\"y\",'Dry Bulb'!N28-M359,'Dry Bulb'!N28-M243)","v":-5.3580278556263181},{"$f":"IF($T$36=\"y\",'Dry Bulb'!O28-N359,'Dry Bulb'!O28-N243)","v":-7.9391932059447967},null,"South Window",null,"Adiabatic?",null,"ft2/person",null,null,null,3,null,null,null,null,null,null,null,null,null,"δ=",{"$f":"ATAN(AH27)","v":0.96007036240568799},null,null,null,null,null,null,{"$f":"'Incident angle'!BI28","v":24},{"$f":"'Incident angle'!BJ28","v":0},{"$f":"'Incident angle'!BK28","v":0},{"$f":"'Incident angle'!BL28","v":0},{"$f":"'Incident angle'!BM28","v":0},{"$f":"'Incident angle'!BN28","v":0},{"$f":"'Incident angle'!BO28","v":0},{"$f":"'Incident angle'!BP28","v":0},{"$f":"'Incident angle'!BQ28","v":0},{"$f":"'Incident angle'!BR28","v":0},{"$f":"'Incident angle'!BS28","v":0},{"$f":"'Incident angle'!BT28","v":0},{"$f":"'Incident angle'!BU28","v":0},null,{"$f":"'Incident angle'!BW28","v":24},{"$f":"'Incident angle'!BX28","v":0},{"$f":"'Incident angle'!BY28","v":0},{"$f":"'Incident angle'!BZ28","v":0},{"$f":"'Incident angle'!CA28","v":0},{"$f":"'Incident angle'!CB28","v":0},{"$f":"'Incident angle'!CC28","v":0},{"$f":"'Incident angle'!CD28","v":0},{"$f":"'Incident angle'!CE28","v":0},{"$f":"'Incident angle'!CF28","v":0},{"$f":"'Incident angle'!CG28","v":0},{"$f":"'Incident angle'!CH28","v":0},{"$f":"'Incident angle'!CI28","v":0},null,{"$f":"'Profile angles'!B28","v":24},{"$f":"RADIANS('Profile angles'!C28)","v":1.4880469068104962},{"$f":"RADIANS('Profile angles'!D28)","v":1.325468937525877},{"$f":"RADIANS('Profile angles'!E28)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!F28)","v":0.9319358845770338},{"$f":"RADIANS('Profile angles'!G28)","v":0.78535264346749045},{"$f":"RADIANS('Profile angles'!H28)","v":0.73016710880727165},{"$f":"RADIANS('Profile angles'!I28)","v":0.78135170593207048},{"$f":"RADIANS('Profile angles'!J28)","v":0.92833771723835001},{"$f":"RADIANS('Profile angles'!K28)","v":1.1397000015522971},{"$f":"RADIANS('Profile angles'!L28)","v":1.3265689743998734},{"$f":"RADIANS('Profile angles'!M28)","v":1.4871559725393455},{"$f":"RADIANS('Profile angles'!N28)","v":1.5490861384984902},null,{"$f":"'Profile angles'!B57","v":24},{"$f":"RADIANS('Profile angles'!C57)","v":1.4953307389576809},{"$f":"RADIANS('Profile angles'!D57)","v":1.4778229951074291},{"$f":"RADIANS('Profile angles'!E57)","v":1.5005364967084429},{"$f":"RADIANS('Profile angles'!F57)","v":1.5387122061758478},{"$f":"RADIANS('Profile angles'!G57)","v":1.5486122132899969},{"$f":"RADIANS('Profile angles'!H57)","v":1.5196104703977531},{"$f":"RADIANS('Profile angles'!I57)","v":1.4935003073579076},{"$f":"RADIANS('Profile angles'!J57)","v":1.5200112597578945},{"$f":"RADIANS('Profile angles'!K57)","v":1.5690353246394813},{"$f":"RADIANS('Profile angles'!L57)","v":1.5342706134006174},{"$f":"RADIANS('Profile angles'!M57)","v":1.5433489980684403},{"$f":"RADIANS('Profile angles'!N57)","v":1.5486418126575425},null,{"$f":"'Profile angles'!AD28","v":24},{"$f":"(IF($AH$12<DEGREES(BS28),0+$AJ$16,1-((TAN(BS28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BX27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BT28),0+$AJ$16,1-((TAN(BT28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BY27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BU28),0+$AJ$16,1-((TAN(BU28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!BZ27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(BV28),0+$AJ$16,1-((TAN(BV28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CA27*$DU$3)+1-$DU$3)","v":5.6342741734583007E-2},{"$f":"(IF($AH$12<DEGREES(BW28),0+$AJ$16,1-((TAN(BW28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CB27*$DU$3)+1-$DU$3)","v":0.29673515807795192},{"$f":"(IF($AH$12<DEGREES(BX28),0+$AJ$16,1-((TAN(BX28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CC27*$DU$3)+1-$DU$3)","v":0.36478570784189213},{"$f":"(IF($AH$12<DEGREES(BY28),0+$AJ$16,1-((TAN(BY28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CD27*$DU$3)+1-$DU$3)","v":0.29390159691520085},{"$f":"(IF($AH$12<DEGREES(BZ28),0+$AJ$16,1-((TAN(BZ28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CE27*$DU$3)+1-$DU$3)","v":6.2441727372981315E-2},{"$f":"(IF($AH$12<DEGREES(CA28),0+$AJ$16,1-((TAN(CA28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CF27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CB28),0+$AJ$16,1-((TAN(CB28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CG27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CC28),0+$AJ$16,1-((TAN(CC28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CH27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CD28),0+$AJ$16,1-((TAN(CD28)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CI27*$DU$3)+1-$DU$3)","v":0},null,24,{"$f":"(IF($AH$46<DEGREES(CG28),0+$AJ$50,1-((TAN(CG28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CL27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CH28),0+$AJ$50,1-((TAN(CH28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CM27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CI28),0+$AJ$50,1-((TAN(CI28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CN27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CJ28),0+$AJ$50,1-((TAN(CJ28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CO27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CK28),0+$AJ$50,1-((TAN(CK28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CP27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CL28),0+$AJ$50,1-((TAN(CL28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CQ27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CM28),0+$AJ$50,1-((TAN(CM28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CR27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CN28),0+$AJ$50,1-((TAN(CN28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CS27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CO28),0+$AJ$50,1-((TAN(CO28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CT27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CP28),0+$AJ$50,1-((TAN(CP28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CU27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CQ28),0+$AJ$50,1-((TAN(CQ28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CV27*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$46<DEGREES(CR28),0+$AJ$50,1-((TAN(CR28)/TAN($AG$48))*(1-$AJ$50))))*(('Surface Solar Azimuth Angles'!CW27*$DU$3)+1-$DU$3)","v":0},null,null,{"$f":"'Profile angles'!AR28","v":24},{"$f":"'Profile angles'!AS28","v":-83.596484892158756},{"$f":"'Profile angles'!AT28","v":-75.041691580826409},{"$f":"'Profile angles'!AU28","v":-65.047371814417531},{"$f":"'Profile angles'!AV28","v":-53.370409687127484},{"$f":"'Profile angles'!AW28","v":-44.990343292174892},{"$f":"'Profile angles'!AX28","v":-41.805581832384377},{"$f":"'Profile angles'!AY28","v":-44.683864079458822},{"$f":"'Profile angles'!AZ28","v":-53.126563822663151},{"$f":"'Profile angles'!BA28","v":-65.299840573859427},{"$f":"'Profile angles'!BB28","v":-75.863131931954825},{"$f":"'Profile angles'!BC28","v":-84.958601709687045},{"$f":"'Profile angles'!BD28","v":-88.223048770244205},null,24,-83.596484892158756,-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205]
[null,"Heating & Cooling Load(KBTUs)",null,null,null,null,null,null,null,null,null,null,null,null,null,"Area",{"$f":"Q32*'Input Data'!F21*'Input Data'!F19","v":270},null,null,{"$f":"P3*P6*T9/T27","v":4.5},null,null,null,4,null,null,null,null,null,null,null," Shade Angle δ=",null,{"$f":"DEGREES(AI28)","v":55.007979801441337}]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Glass SHGC",0.22,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI58","v":"West Transmitted "},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BW58","v":"North Transmitted"},null,null,null,null,null,null,null,null,null,null,null,null,null,"West Profile",null,null,null,null,null,null,null,null,null,null,null,null,null,"North Profile",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($P$17>45,\"South SC\",\"West SC\")","v":"West SC"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($P$17>45,\"West SC\",\"North SC\")","v":"North SC"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"DW3","v":"Altitude"},{"$f":"DX3","v":0},0,0,0,0,0,0,0,0,0,0,0,null,{"$f":"EK3","v":"Altitude"},{"$f":"EL3","v":0},0,0,0,0,0,0,0,0,0,0,0]
[null,1,{"$f":"IF('Dry Bulb'!D5<60,(('Input Data'!$F$44*('Dry Bulb'!D5-$T$15))+('Heat gain from airflow'!Q4)+((Occupancy!P4*'Input Data'!$F$47)+(Occupancy!B4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D5-$P$15))+('Heat gain from airflow'!Q4)+((Occupancy!P4*'Input Data'!$F$47)+(Occupancy!B4*'Input Data'!$F$49))))/1000","v":-5.3513100000000032E-3},{"$f":"IF('Dry Bulb'!E5<60,(('Input Data'!$F$44*('Dry Bulb'!E5-$T$15))+('Heat gain from airflow'!R4)+((Occupancy!Q4*'Input Data'!$F$47)+(Occupancy!C4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E5-$P$15))+('Heat gain from airflow'!R4)+((Occupancy!Q4*'Input Data'!$F$47)+(Occupancy!C4*'Input Data'!$F$49))))/1000","v":-2.9668725000000029E-3},{"$f":"IF('Dry Bulb'!F5<60,(('Input Data'!$F$44*('Dry Bulb'!F5-$T$15))+('Heat gain from airflow'!S4)+((Occupancy!R4*'Input Data'!$F$47)+(Occupancy!D4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F5-$P$15))+('Heat gain from airflow'!S4)+((Occupancy!R4*'Input Data'!$F$47)+(Occupancy!D4*'Input Data'!$F$49))))/1000","v":-3.0516525000000012},{"$f":"IF('Dry Bulb'!G5<60,(('Input Data'!$F$44*('Dry Bulb'!G5-$T$15))+('Heat gain from airflow'!T4)+((Occupancy!S4*'Input Data'!$F$47)+(Occupancy!E4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G5-$P$15))+('Heat gain from airflow'!T4)+((Occupancy!S4*'Input Data'!$F$47)+(Occupancy!E4*'Input Data'!$F$49))))/1000","v":1.3832684100000037},{"$f":"IF('Dry Bulb'!H5<60,(('Input Data'!$F$44*('Dry Bulb'!H5-$T$15))+('Heat gain from airflow'!U4)+((Occupancy!T4*'Input Data'!$F$47)+(Occupancy!F4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H5-$P$15))+('Heat gain from airflow'!U4)+((Occupancy!T4*'Input Data'!$F$47)+(Occupancy!F4*'Input Data'!$F$49))))/1000","v":7.7260050000000007},{"$f":"IF('Dry Bulb'!I5<60,(('Input Data'!$F$44*('Dry Bulb'!I5-$T$15))+('Heat gain from airflow'!V4)+((Occupancy!U4*'Input Data'!$F$47)+(Occupancy!G4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I5-$P$15))+('Heat gain from airflow'!V4)+((Occupancy!U4*'Input Data'!$F$47)+(Occupancy!G4*'Input Data'!$F$49))))/1000","v":10.396574999999997},{"$f":"IF('Dry Bulb'!J5<60,(('Input Data'!$F$44*('Dry Bulb'!J5-$T$15))+('Heat gain from airflow'!W4)+((Occupancy!V4*'Input Data'!$F$47)+(Occupancy!H4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J5-$P$15))+('Heat gain from airflow'!W4)+((Occupancy!V4*'Input Data'!$F$47)+(Occupancy!H4*'Input Data'!$F$49))))/1000","v":11.064217499999998},{"$f":"IF('Dry Bulb'!K5<60,(('Input Data'!$F$44*('Dry Bulb'!K5-$T$15))+('Heat gain from airflow'!X4)+((Occupancy!W4*'Input Data'!$F$47)+(Occupancy!I4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K5-$P$15))+('Heat gain from airflow'!X4)+((Occupancy!W4*'Input Data'!$F$47)+(Occupancy!I4*'Input Data'!$F$49))))/1000","v":11.350350000000002},{"$f":"IF('Dry Bulb'!L5<60,(('Input Data'!$F$44*('Dry Bulb'!L5-$T$15))+('Heat gain from airflow'!Y4)+((Occupancy!X4*'Input Data'!$F$47)+(Occupancy!J4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L5-$P$15))+('Heat gain from airflow'!Y4)+((Occupancy!X4*'Input Data'!$F$47)+(Occupancy!J4*'Input Data'!$F$49))))/1000","v":8.3936474999999948},{"$f":"IF('Dry Bulb'!M5<60,(('Input Data'!$F$44*('Dry Bulb'!M5-$T$15))+('Heat gain from airflow'!Z4)+((Occupancy!Y4*'Input Data'!$F$47)+(Occupancy!K4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M5-$P$15))+('Heat gain from airflow'!Z4)+((Occupancy!Y4*'Input Data'!$F$47)+(Occupancy!K4*'Input Data'!$F$49))))/1000","v":3.3771575249999959},{"$f":"IF('Dry Bulb'!N5<60,(('Input Data'!$F$44*('Dry Bulb'!N5-$T$15))+('Heat gain from airflow'!AA4)+((Occupancy!Z4*'Input Data'!$F$47)+(Occupancy!L4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N5-$P$15))+('Heat gain from airflow'!AA4)+((Occupancy!Z4*'Input Data'!$F$47)+(Occupancy!L4*'Input Data'!$F$49))))/1000","v":-3.7773857699999973},{"$f":"IF('Dry Bulb'!O5<60,(('Input Data'!$F$44*('Dry Bulb'!O5-$T$15))+('Heat gain from airflow'!AB4)+((Occupancy!AA4*'Input Data'!$F$47)+(Occupancy!M4*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O5-$P$15))+('Heat gain from airflow'!AB4)+((Occupancy!AA4*'Input Data'!$F$47)+(Occupancy!M4*'Input Data'!$F$49))))/1000","v":-4.3021574999999998E-3},null,"U-Value",0.4,false,null,"Equipment",null,null,null,6,null,null,null,null,null,null,null,null,{"$f":"RADIANS(AH29)","v":0.96007036240568799},null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI59","v":0},{"$f":"'Incident angle'!BJ59","v":"Jan"},{"$f":"'Incident angle'!BK59","v":"Feb"},{"$f":"'Incident angle'!BL59","v":"Mar"},{"$f":"'Incident angle'!BM59","v":"Apr"},{"$f":"'Incident angle'!BN59","v":"May"},{"$f":"'Incident angle'!BO59","v":"Jun"},{"$f":"'Incident angle'!BP59","v":"Jul"},{"$f":"'Incident angle'!BQ59","v":"Aug"},{"$f":"'Incident angle'!BR59","v":"Sep"},{"$f":"'Incident angle'!BS59","v":"Oct"},{"$f":"'Incident angle'!BT59","v":"Nov"},{"$f":"'Incident angle'!BU59","v":"Dec"},"Average",{"$f":"'Incident angle'!BW59","v":0},{"$f":"'Incident angle'!BX59","v":"Jan"},{"$f":"'Incident angle'!BY59","v":"Feb"},{"$f":"'Incident angle'!BZ59","v":"Mar"},{"$f":"'Incident angle'!CA59","v":"Apr"},{"$f":"'Incident angle'!CB59","v":"May"},{"$f":"'Incident angle'!CC59","v":"Jun"},{"$f":"'Incident angle'!CD59","v":"Jul"},{"$f":"'Incident angle'!CE59","v":"Aug"},{"$f":"'Incident angle'!CF59","v":"Sep"},{"$f":"'Incident angle'!CG59","v":"Oct"},{"$f":"'Incident angle'!CH59","v":"Nov"},{"$f":"'Incident angle'!CI59","v":"Dec"},"Average",{"$f":"'Profile angles'!P4","v":"HR"},{"$f":"'Profile angles'!Q4","v":"Jan"},{"$f":"'Profile angles'!R4","v":"Feb"},{"$f":"'Profile angles'!S4","v":"Mar"},{"$f":"'Profile angles'!T4","v":"Apr"},{"$f":"'Profile angles'!U4","v":"May"},{"$f":"'Profile angles'!V4","v":"Jun"},{"$f":"'Profile angles'!W4","v":"Jul"},{"$f":"'Profile angles'!X4","v":"Aug"},{"$f":"'Profile angles'!Y4","v":"Sep"},{"$f":"'Profile angles'!Z4","v":"Oct"},{"$f":"'Profile angles'!AA4","v":"Nov"},{"$f":"'Profile angles'!AB4","v":"Dec"},null,{"$f":"'Profile angles'!P33","v":"HR"},{"$f":"'Profile angles'!Q33","v":"Jan"},{"$f":"'Profile angles'!R33","v":"Feb"},{"$f":"'Profile angles'!S33","v":"Mar"},{"$f":"'Profile angles'!T33","v":"Apr"},{"$f":"'Profile angles'!U33","v":"May"},{"$f":"'Profile angles'!V33","v":"Jun"},{"$f":"'Profile angles'!W33","v":"Jul"},{"$f":"'Profile angles'!X33","v":"Aug"},{"$f":"'Profile angles'!Y33","v":"Sep"},{"$f":"'Profile angles'!Z33","v":"Oct"},{"$f":"'Profile angles'!AA33","v":"Nov"},{"$f":"'Profile angles'!AB33","v":"Dec"},null,{"$f":"CT4","v":"HR"},{"$f":"'Profile angles'!AS4","v":"Jan"},{"$f":"'Profile angles'!AT4","v":"Feb"},{"$f":"'Profile angles'!AU4","v":"Mar"},{"$f":"'Profile angles'!AV4","v":"Apr"},{"$f":"'Profile angles'!AW4","v":"May"},{"$f":"'Profile angles'!AX4","v":"Jun"},{"$f":"'Profile angles'!AY4","v":"Jul"},{"$f":"'Profile angles'!AZ4","v":"Aug"},{"$f":"'Profile angles'!BA4","v":"Sep"},{"$f":"'Profile angles'!BB4","v":"Oct"},{"$f":"'Profile angles'!BC4","v":"Nov"},{"$f":"'Profile angles'!BD4","v":"Dec"},null,{"$f":"CT31","v":"HR"},{"$f":"CU31","v":"Jan"},"Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,{"$f":"DW4","v":0},"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$f":"EK4","v":0},0,0,0,0,0,0,0,0,0,0,0,0]
[null,2,{"$f":"IF('Dry Bulb'!D6<60,(('Input Data'!$F$44*('Dry Bulb'!D6-$T$15))+('Heat gain from airflow'!Q5)+((Occupancy!P5*'Input Data'!$F$47)+(Occupancy!B5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D6-$P$15))+('Heat gain from airflow'!Q5)+((Occupancy!P5*'Input Data'!$F$47)+(Occupancy!B5*'Input Data'!$F$49))))/1000","v":-5.8281975000000017E-3},{"$f":"IF('Dry Bulb'!E6<60,(('Input Data'!$F$44*('Dry Bulb'!E6-$T$15))+('Heat gain from airflow'!R5)+((Occupancy!Q5*'Input Data'!$F$47)+(Occupancy!C5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E6-$P$15))+('Heat gain from airflow'!R5)+((Occupancy!Q5*'Input Data'!$F$47)+(Occupancy!C5*'Input Data'!$F$49))))/1000","v":-3.5391375000000014E-3},{"$f":"IF('Dry Bulb'!F6<60,(('Input Data'!$F$44*('Dry Bulb'!F6-$T$15))+('Heat gain from airflow'!S5)+((Occupancy!R5*'Input Data'!$F$47)+(Occupancy!D5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F6-$P$15))+('Heat gain from airflow'!S5)+((Occupancy!R5*'Input Data'!$F$47)+(Occupancy!D5*'Input Data'!$F$49))))/1000","v":-3.7192950000000038},{"$f":"IF('Dry Bulb'!G6<60,(('Input Data'!$F$44*('Dry Bulb'!G6-$T$15))+('Heat gain from airflow'!T5)+((Occupancy!S5*'Input Data'!$F$47)+(Occupancy!E5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G6-$P$15))+('Heat gain from airflow'!T5)+((Occupancy!S5*'Input Data'!$F$47)+(Occupancy!E5*'Input Data'!$F$49))))/1000","v":0.67954283999999554},{"$f":"IF('Dry Bulb'!H6<60,(('Input Data'!$F$44*('Dry Bulb'!H6-$T$15))+('Heat gain from airflow'!U5)+((Occupancy!T5*'Input Data'!$F$47)+(Occupancy!F5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H6-$P$15))+('Heat gain from airflow'!U5)+((Occupancy!T5*'Input Data'!$F$47)+(Occupancy!F5*'Input Data'!$F$49))))/1000","v":6.9629850000000024},{"$f":"IF('Dry Bulb'!I6<60,(('Input Data'!$F$44*('Dry Bulb'!I6-$T$15))+('Heat gain from airflow'!V5)+((Occupancy!U5*'Input Data'!$F$47)+(Occupancy!G5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I6-$P$15))+('Heat gain from airflow'!V5)+((Occupancy!U5*'Input Data'!$F$47)+(Occupancy!G5*'Input Data'!$F$49))))/1000","v":9.4428000000000001},{"$f":"IF('Dry Bulb'!J6<60,(('Input Data'!$F$44*('Dry Bulb'!J6-$T$15))+('Heat gain from airflow'!W5)+((Occupancy!V5*'Input Data'!$F$47)+(Occupancy!H5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J6-$P$15))+('Heat gain from airflow'!W5)+((Occupancy!V5*'Input Data'!$F$47)+(Occupancy!H5*'Input Data'!$F$49))))/1000","v":10.205819999999996},{"$f":"IF('Dry Bulb'!K6<60,(('Input Data'!$F$44*('Dry Bulb'!K6-$T$15))+('Heat gain from airflow'!X5)+((Occupancy!W5*'Input Data'!$F$47)+(Occupancy!I5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K6-$P$15))+('Heat gain from airflow'!X5)+((Occupancy!W5*'Input Data'!$F$47)+(Occupancy!I5*'Input Data'!$F$49))))/1000","v":10.4919525},{"$f":"IF('Dry Bulb'!L6<60,(('Input Data'!$F$44*('Dry Bulb'!L6-$T$15))+('Heat gain from airflow'!Y5)+((Occupancy!X5*'Input Data'!$F$47)+(Occupancy!J5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L6-$P$15))+('Heat gain from airflow'!Y5)+((Occupancy!X5*'Input Data'!$F$47)+(Occupancy!J5*'Input Data'!$F$49))))/1000","v":7.4398724999999981},{"$f":"IF('Dry Bulb'!M6<60,(('Input Data'!$F$44*('Dry Bulb'!M6-$T$15))+('Heat gain from airflow'!Z5)+((Occupancy!Y5*'Input Data'!$F$47)+(Occupancy!K5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M6-$P$15))+('Heat gain from airflow'!Z5)+((Occupancy!Y5*'Input Data'!$F$47)+(Occupancy!K5*'Input Data'!$F$49))))/1000","v":2.556144360000002},{"$f":"IF('Dry Bulb'!N6<60,(('Input Data'!$F$44*('Dry Bulb'!N6-$T$15))+('Heat gain from airflow'!AA5)+((Occupancy!Z5*'Input Data'!$F$47)+(Occupancy!L5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N6-$P$15))+('Heat gain from airflow'!AA5)+((Occupancy!Z5*'Input Data'!$F$47)+(Occupancy!L5*'Input Data'!$F$49))))/1000","v":-3.4331625000000003},{"$f":"IF('Dry Bulb'!O6<60,(('Input Data'!$F$44*('Dry Bulb'!O6-$T$15))+('Heat gain from airflow'!AB5)+((Occupancy!AA5*'Input Data'!$F$47)+(Occupancy!M5*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O6-$P$15))+('Heat gain from airflow'!AB5)+((Occupancy!AA5*'Input Data'!$F$47)+(Occupancy!M5*'Input Data'!$F$49))))/1000","v":-4.6836675000000005E-3},null,"WWR",{"$f":"(Q33/20)*R32","v":0.6},{"$f":"IF(R31,0,1)","v":1},null,"& Lights (w/sf)",null,null,null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI60","v":1},{"$f":"'Incident angle'!BJ60","v":0},{"$f":"'Incident angle'!BK60","v":0},{"$f":"'Incident angle'!BL60","v":0},{"$f":"'Incident angle'!BM60","v":0},{"$f":"'Incident angle'!BN60","v":0},{"$f":"'Incident angle'!BO60","v":0},{"$f":"'Incident angle'!BP60","v":0},{"$f":"'Incident angle'!BQ60","v":0},{"$f":"'Incident angle'!BR60","v":0},{"$f":"'Incident angle'!BS60","v":0},{"$f":"'Incident angle'!BT60","v":0},{"$f":"'Incident angle'!BU60","v":0},{"$f":"AVERAGEIF(AS32:AZ55,\">0\")","v":3213.7234684517707},{"$f":"'Incident angle'!BW60","v":1},{"$f":"'Incident angle'!BX60","v":0},{"$f":"'Incident angle'!BY60","v":0},{"$f":"'Incident angle'!BZ60","v":0},{"$f":"'Incident angle'!CA60","v":0},{"$f":"'Incident angle'!CB60","v":0},{"$f":"'Incident angle'!CC60","v":0},{"$f":"'Incident angle'!CD60","v":0},{"$f":"'Incident angle'!CE60","v":0},{"$f":"'Incident angle'!CF60","v":0},{"$f":"'Incident angle'!CG60","v":0},{"$f":"'Incident angle'!CH60","v":0},{"$f":"'Incident angle'!CI60","v":0},{"$f":"AVERAGEIF(BG32:BN55,\">0\")","v":{"$error":"#DIV/0!"}},{"$f":"'Profile angles'!P5","v":1},{"$f":"RADIANS('Profile angles'!Q5)","v":1.3994410384001574},{"$f":"RADIANS('Profile angles'!R5)","v":1.3987224426302709},{"$f":"RADIANS('Profile angles'!S5)","v":1.353506719206063},{"$f":"RADIANS('Profile angles'!T5)","v":1.2854751008998166},{"$f":"RADIANS('Profile angles'!U5)","v":1.2485940409284226},{"$f":"RADIANS('Profile angles'!V5)","v":1.2646212293363481},{"$f":"RADIANS('Profile angles'!W5)","v":1.3017917625848772},{"$f":"RADIANS('Profile angles'!X5)","v":1.3032988016081293},{"$f":"RADIANS('Profile angles'!Y5)","v":1.2822582122157415},{"$f":"RADIANS('Profile angles'!Z5)","v":1.2704099409257712},{"$f":"RADIANS('Profile angles'!AA5)","v":1.2971040377011409},{"$f":"RADIANS('Profile angles'!AB5)","v":1.3530868681716333},null,{"$f":"'Profile angles'!P34","v":1},{"$f":"RADIANS('Profile angles'!Q34)","v":-1.492373321351995},{"$f":"RADIANS('Profile angles'!R34)","v":-1.327348921355314},{"$f":"RADIANS('Profile angles'!S34)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T34)","v":-0.92628661869809481},{"$f":"RADIANS('Profile angles'!U34)","v":-0.77541332917766936},{"$f":"RADIANS('Profile angles'!V34)","v":-0.72105580791449653},{"$f":"RADIANS('Profile angles'!W34)","v":-0.77500562596203515},{"$f":"RADIANS('Profile angles'!X34)","v":-0.92344909928942354},{"$f":"RADIANS('Profile angles'!Y34)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!Z34)","v":-1.3348406596171152},{"$f":"RADIANS('Profile angles'!AA34)","v":-1.500983956115769},{"$f":"RADIANS('Profile angles'!AB34)","v":-1.5594894508681831},null,{"$f":"'Profile angles'!AR5","v":1},{"$f":"(IF($AH$29<DEGREES(BS32),0+$AJ$33,1-((TAN(BS32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BT32),0+$AJ$33,1-((TAN(BT32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BU32),0+$AJ$33,1-((TAN(BU32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BV32),0+$AJ$33,1-((TAN(BV32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BW32),0+$AJ$33,1-((TAN(BW32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BX32),0+$AJ$33,1-((TAN(BX32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BY32),0+$AJ$33,1-((TAN(BY32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BZ32),0+$AJ$33,1-((TAN(BZ32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CA32),0+$AJ$33,1-((TAN(CA32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CB32),0+$AJ$33,1-((TAN(CB32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CC32),0+$AJ$33,1-((TAN(CC32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CD32),0+$AJ$33,1-((TAN(CD32)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI58*$DU$3)+1-$DU$3)","v":0},null,{"$f":"CT32","v":1},{"$f":"(IF($AH$12<DEGREES(CG32),0+$AJ$16,1-((TAN(CG32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH32),0+$AJ$16,1-((TAN(CH32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM58*$DU$3)+1-$DU$3)","v":2.4824475317243722},{"$f":"(IF($AH$12<DEGREES(CI32),0+$AJ$16,1-((TAN(CI32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN58*$DU$3)+1-$DU$3)","v":1.9166512903452211},{"$f":"(IF($AH$12<DEGREES(CJ32),0+$AJ$16,1-((TAN(CJ32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO58*$DU$3)+1-$DU$3)","v":1.5544877208061749},{"$f":"(IF($AH$12<DEGREES(CK32),0+$AJ$16,1-((TAN(CK32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP58*$DU$3)+1-$DU$3)","v":1.4102743277947025},{"$f":"(IF($AH$12<DEGREES(CL32),0+$AJ$16,1-((TAN(CL32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ58*$DU$3)+1-$DU$3)","v":1.3908603976852976},{"$f":"(IF($AH$12<DEGREES(CM32),0+$AJ$16,1-((TAN(CM32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR58*$DU$3)+1-$DU$3)","v":1.4580307334788438},{"$f":"(IF($AH$12<DEGREES(CN32),0+$AJ$16,1-((TAN(CN32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS58*$DU$3)+1-$DU$3)","v":1.5768170783223932},{"$f":"(IF($AH$12<DEGREES(CO32),0+$AJ$16,1-((TAN(CO32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT58*$DU$3)+1-$DU$3)","v":1.7081697247176337},{"$f":"(IF($AH$12<DEGREES(CP32),0+$AJ$16,1-((TAN(CP32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU58*$DU$3)+1-$DU$3)","v":1.3918052959169831},{"$f":"(IF($AH$12<DEGREES(CQ32),0+$AJ$16,1-((TAN(CQ32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV58*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR32),0+$AJ$16,1-((TAN(CR32)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW58*$DU$3)+1-$DU$3)","v":0},null,null,1,-79.238745258454912,-73.135890206899091,-62.969753990761212,-51.103815741194268,-42.972420763986918,-40.259838967181594,-43.397326661656273,-51.194813940312706,-61.30334441705341,-68.588756925018274,-73.864057818332,-77.510392918823513,null,1,-79.238745258454912,-73.135890206899091,-62.969753990761212,-51.103815741194268,-42.972420763986918,-40.259838967181594,-43.397326661656273,-51.194813940312706,-61.30334441705341,-68.588756925018274,-73.864057818332,-77.510392918823513]
[null,3,{"$f":"IF('Dry Bulb'!D7<60,(('Input Data'!$F$44*('Dry Bulb'!D7-$T$15))+('Heat gain from airflow'!Q6)+((Occupancy!P6*'Input Data'!$F$47)+(Occupancy!B6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D7-$P$15))+('Heat gain from airflow'!Q6)+((Occupancy!P6*'Input Data'!$F$47)+(Occupancy!B6*'Input Data'!$F$49))))/1000","v":-6.114330000000002E-3},{"$f":"IF('Dry Bulb'!E7<60,(('Input Data'!$F$44*('Dry Bulb'!E7-$T$15))+('Heat gain from airflow'!R6)+((Occupancy!Q6*'Input Data'!$F$47)+(Occupancy!C6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E7-$P$15))+('Heat gain from airflow'!R6)+((Occupancy!Q6*'Input Data'!$F$47)+(Occupancy!C6*'Input Data'!$F$49))))/1000","v":-4.1114025000000016E-3},{"$f":"IF('Dry Bulb'!F7<60,(('Input Data'!$F$44*('Dry Bulb'!F7-$T$15))+('Heat gain from airflow'!S6)+((Occupancy!R6*'Input Data'!$F$47)+(Occupancy!D6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F7-$P$15))+('Heat gain from airflow'!S6)+((Occupancy!R6*'Input Data'!$F$47)+(Occupancy!D6*'Input Data'!$F$49))))/1000","v":-4.3869374999999993},{"$f":"IF('Dry Bulb'!G7<60,(('Input Data'!$F$44*('Dry Bulb'!G7-$T$15))+('Heat gain from airflow'!T6)+((Occupancy!S6*'Input Data'!$F$47)+(Occupancy!E6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G7-$P$15))+('Heat gain from airflow'!T6)+((Occupancy!S6*'Input Data'!$F$47)+(Occupancy!E6*'Input Data'!$F$49))))/1000","v":-2.4182730000003174E-2},{"$f":"IF('Dry Bulb'!H7<60,(('Input Data'!$F$44*('Dry Bulb'!H7-$T$15))+('Heat gain from airflow'!U6)+((Occupancy!T6*'Input Data'!$F$47)+(Occupancy!F6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H7-$P$15))+('Heat gain from airflow'!U6)+((Occupancy!T6*'Input Data'!$F$47)+(Occupancy!F6*'Input Data'!$F$49))))/1000","v":6.3907200000000026},{"$f":"IF('Dry Bulb'!I7<60,(('Input Data'!$F$44*('Dry Bulb'!I7-$T$15))+('Heat gain from airflow'!V6)+((Occupancy!U6*'Input Data'!$F$47)+(Occupancy!G6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I7-$P$15))+('Heat gain from airflow'!V6)+((Occupancy!U6*'Input Data'!$F$47)+(Occupancy!G6*'Input Data'!$F$49))))/1000","v":8.9659125000000017},{"$f":"IF('Dry Bulb'!J7<60,(('Input Data'!$F$44*('Dry Bulb'!J7-$T$15))+('Heat gain from airflow'!W6)+((Occupancy!V6*'Input Data'!$F$47)+(Occupancy!H6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J7-$P$15))+('Heat gain from airflow'!W6)+((Occupancy!V6*'Input Data'!$F$47)+(Occupancy!H6*'Input Data'!$F$49))))/1000","v":9.6335549999999959},{"$f":"IF('Dry Bulb'!K7<60,(('Input Data'!$F$44*('Dry Bulb'!K7-$T$15))+('Heat gain from airflow'!X6)+((Occupancy!W6*'Input Data'!$F$47)+(Occupancy!I6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K7-$P$15))+('Heat gain from airflow'!X6)+((Occupancy!W6*'Input Data'!$F$47)+(Occupancy!I6*'Input Data'!$F$49))))/1000","v":9.6335549999999959},{"$f":"IF('Dry Bulb'!L7<60,(('Input Data'!$F$44*('Dry Bulb'!L7-$T$15))+('Heat gain from airflow'!Y6)+((Occupancy!X6*'Input Data'!$F$47)+(Occupancy!J6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L7-$P$15))+('Heat gain from airflow'!Y6)+((Occupancy!X6*'Input Data'!$F$47)+(Occupancy!J6*'Input Data'!$F$49))))/1000","v":6.581475000000002},{"$f":"IF('Dry Bulb'!M7<60,(('Input Data'!$F$44*('Dry Bulb'!M7-$T$15))+('Heat gain from airflow'!Z6)+((Occupancy!Y6*'Input Data'!$F$47)+(Occupancy!K6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M7-$P$15))+('Heat gain from airflow'!Z6)+((Occupancy!Y6*'Input Data'!$F$47)+(Occupancy!K6*'Input Data'!$F$49))))/1000","v":1.5005560049999991},{"$f":"IF('Dry Bulb'!N7<60,(('Input Data'!$F$44*('Dry Bulb'!N7-$T$15))+('Heat gain from airflow'!AA6)+((Occupancy!Z6*'Input Data'!$F$47)+(Occupancy!L6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N7-$P$15))+('Heat gain from airflow'!AA6)+((Occupancy!Z6*'Input Data'!$F$47)+(Occupancy!L6*'Input Data'!$F$49))))/1000","v":-4.1008049999999994},{"$f":"IF('Dry Bulb'!O7<60,(('Input Data'!$F$44*('Dry Bulb'!O7-$T$15))+('Heat gain from airflow'!AB6)+((Occupancy!AA6*'Input Data'!$F$47)+(Occupancy!M6*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O7-$P$15))+('Heat gain from airflow'!AB6)+((Occupancy!AA6*'Input Data'!$F$47)+(Occupancy!M6*'Input Data'!$F$49))))/1000","v":-5.0651775000000003E-3},null,null,12,null,null,0.5,null,null,null,8,null,null,null,"Transmittance of Shade Material",null,null,null,null,null,null,null,0,null,null,null,null,null,{"$f":"'Incident angle'!BI61","v":2},{"$f":"'Incident angle'!BJ61","v":0},{"$f":"'Incident angle'!BK61","v":0},{"$f":"'Incident angle'!BL61","v":0},{"$f":"'Incident angle'!BM61","v":0},{"$f":"'Incident angle'!BN61","v":0},{"$f":"'Incident angle'!BO61","v":0},{"$f":"'Incident angle'!BP61","v":0},{"$f":"'Incident angle'!BQ61","v":0},{"$f":"'Incident angle'!BR61","v":0},{"$f":"'Incident angle'!BS61","v":0},{"$f":"'Incident angle'!BT61","v":0},{"$f":"'Incident angle'!BU61","v":0},"Max",{"$f":"'Incident angle'!BW61","v":2},{"$f":"'Incident angle'!BX61","v":0},{"$f":"'Incident angle'!BY61","v":0},{"$f":"'Incident angle'!BZ61","v":0},{"$f":"'Incident angle'!CA61","v":0},{"$f":"'Incident angle'!CB61","v":0},{"$f":"'Incident angle'!CC61","v":0},{"$f":"'Incident angle'!CD61","v":0},{"$f":"'Incident angle'!CE61","v":0},{"$f":"'Incident angle'!CF61","v":0},{"$f":"'Incident angle'!CG61","v":0},{"$f":"'Incident angle'!CH61","v":0},{"$f":"'Incident angle'!CI61","v":0},"Max",{"$f":"'Profile angles'!P6","v":2},{"$f":"RADIANS('Profile angles'!Q6)","v":1.1549210062521438},{"$f":"RADIANS('Profile angles'!R6)","v":1.136916400741615},{"$f":"RADIANS('Profile angles'!S6)","v":1.0718008336148825},{"$f":"RADIANS('Profile angles'!T6)","v":0.979468800432579},{"$f":"RADIANS('Profile angles'!U6)","v":0.92164982186211586},{"$f":"RADIANS('Profile angles'!V6)","v":0.92627284120998088},{"$f":"RADIANS('Profile angles'!W6)","v":0.97053375348906978},{"$f":"RADIANS('Profile angles'!X6)","v":0.99586471792570996},{"$f":"RADIANS('Profile angles'!Y6)","v":1.0030149795642196},{"$f":"RADIANS('Profile angles'!Z6)","v":1.0118824071687469},{"$f":"RADIANS('Profile angles'!AA6)","v":1.0543583507572232},{"$f":"RADIANS('Profile angles'!AB6)","v":1.1157238568704597},null,{"$f":"'Profile angles'!P35","v":2},{"$f":"RADIANS('Profile angles'!Q35)","v":-1.5208845729807423},{"$f":"RADIANS('Profile angles'!R35)","v":-1.3429160432098304},{"$f":"RADIANS('Profile angles'!S35)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T35)","v":-0.90436988504871829},{"$f":"RADIANS('Profile angles'!U35)","v":-0.73943113538447891},{"$f":"RADIANS('Profile angles'!V35)","v":-0.68354026259431289},{"$f":"RADIANS('Profile angles'!W35)","v":-0.7434435505657796},{"$f":"RADIANS('Profile angles'!X35)","v":-0.90231514982176808},{"$f":"RADIANS('Profile angles'!Y35)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!Z35)","v":-1.3590817446939001},{"$f":"RADIANS('Profile angles'!AA35)","v":-1.5418396740988676},{"$f":"RADIANS('Profile angles'!AB35)","v":1.5429463724306218},null,{"$f":"'Profile angles'!AR6","v":2},{"$f":"(IF($AH$29<DEGREES(BS33),0+$AJ$33,1-((TAN(BS33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BT33),0+$AJ$33,1-((TAN(BT33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BU33),0+$AJ$33,1-((TAN(BU33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BV33),0+$AJ$33,1-((TAN(BV33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BW33),0+$AJ$33,1-((TAN(BW33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB59*$DU$3)+1-$DU$3)","v":2.1529352241533826E-2},{"$f":"(IF($AH$29<DEGREES(BX33),0+$AJ$33,1-((TAN(BX33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC59*$DU$3)+1-$DU$3)","v":1.2582289276639619E-2},{"$f":"(IF($AH$29<DEGREES(BY33),0+$AJ$33,1-((TAN(BY33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BZ33),0+$AJ$33,1-((TAN(BZ33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CA33),0+$AJ$33,1-((TAN(CA33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CB33),0+$AJ$33,1-((TAN(CB33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CC33),0+$AJ$33,1-((TAN(CC33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CD33),0+$AJ$33,1-((TAN(CD33)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI59*$DU$3)+1-$DU$3)","v":0},null,2,{"$f":"(IF($AH$12<DEGREES(CG33),0+$AJ$16,1-((TAN(CG33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH33),0+$AJ$16,1-((TAN(CH33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM59*$DU$3)+1-$DU$3)","v":4.2596832780776766E-3},{"$f":"(IF($AH$12<DEGREES(CI33),0+$AJ$16,1-((TAN(CI33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN59*$DU$3)+1-$DU$3)","v":1.0277881798959132},{"$f":"(IF($AH$12<DEGREES(CJ33),0+$AJ$16,1-((TAN(CJ33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO59*$DU$3)+1-$DU$3)","v":1.0831930448784186},{"$f":"(IF($AH$12<DEGREES(CK33),0+$AJ$16,1-((TAN(CK33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP59*$DU$3)+1-$DU$3)","v":1.0714412062964351},{"$f":"(IF($AH$12<DEGREES(CL33),0+$AJ$16,1-((TAN(CL33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ59*$DU$3)+1-$DU$3)","v":1.0895415348956625},{"$f":"(IF($AH$12<DEGREES(CM33),0+$AJ$16,1-((TAN(CM33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR59*$DU$3)+1-$DU$3)","v":1.1263846008724765},{"$f":"(IF($AH$12<DEGREES(CN33),0+$AJ$16,1-((TAN(CN33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS59*$DU$3)+1-$DU$3)","v":1.112539388792479},{"$f":"(IF($AH$12<DEGREES(CO33),0+$AJ$16,1-((TAN(CO33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT59*$DU$3)+1-$DU$3)","v":0.77325547210928136},{"$f":"(IF($AH$12<DEGREES(CP33),0+$AJ$16,1-((TAN(CP33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ33),0+$AJ$16,1-((TAN(CQ33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV59*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR33),0+$AJ$16,1-((TAN(CR33)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW59*$DU$3)+1-$DU$3)","v":0},null,null,2,-66.037221876299029,-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697,null,2,-66.037221876299029,-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697]
[null,4,{"$f":"IF('Dry Bulb'!D8<60,(('Input Data'!$F$44*('Dry Bulb'!D8-$T$15))+('Heat gain from airflow'!Q7)+((Occupancy!P7*'Input Data'!$F$47)+(Occupancy!B7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D8-$P$15))+('Heat gain from airflow'!Q7)+((Occupancy!P7*'Input Data'!$F$47)+(Occupancy!B7*'Input Data'!$F$49))))/1000","v":-6.5912175000000005E-3},{"$f":"IF('Dry Bulb'!E8<60,(('Input Data'!$F$44*('Dry Bulb'!E8-$T$15))+('Heat gain from airflow'!R7)+((Occupancy!Q7*'Input Data'!$F$47)+(Occupancy!C7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E8-$P$15))+('Heat gain from airflow'!R7)+((Occupancy!Q7*'Input Data'!$F$47)+(Occupancy!C7*'Input Data'!$F$49))))/1000","v":-4.6836675000000005E-3},{"$f":"IF('Dry Bulb'!F8<60,(('Input Data'!$F$44*('Dry Bulb'!F8-$T$15))+('Heat gain from airflow'!S7)+((Occupancy!R7*'Input Data'!$F$47)+(Occupancy!D7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F8-$P$15))+('Heat gain from airflow'!S7)+((Occupancy!R7*'Input Data'!$F$47)+(Occupancy!D7*'Input Data'!$F$49))))/1000","v":-4.8638250000000021},{"$f":"IF('Dry Bulb'!G8<60,(('Input Data'!$F$44*('Dry Bulb'!G8-$T$15))+('Heat gain from airflow'!T7)+((Occupancy!S7*'Input Data'!$F$47)+(Occupancy!E7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G8-$P$15))+('Heat gain from airflow'!T7)+((Occupancy!S7*'Input Data'!$F$47)+(Occupancy!E7*'Input Data'!$F$49))))/1000","v":-0.96248349000000188},{"$f":"IF('Dry Bulb'!H8<60,(('Input Data'!$F$44*('Dry Bulb'!H8-$T$15))+('Heat gain from airflow'!U7)+((Occupancy!T7*'Input Data'!$F$47)+(Occupancy!F7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H8-$P$15))+('Heat gain from airflow'!U7)+((Occupancy!T7*'Input Data'!$F$47)+(Occupancy!F7*'Input Data'!$F$49))))/1000","v":6.1045875000000001},{"$f":"IF('Dry Bulb'!I8<60,(('Input Data'!$F$44*('Dry Bulb'!I8-$T$15))+('Heat gain from airflow'!V7)+((Occupancy!U7*'Input Data'!$F$47)+(Occupancy!G7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I8-$P$15))+('Heat gain from airflow'!V7)+((Occupancy!U7*'Input Data'!$F$47)+(Occupancy!G7*'Input Data'!$F$49))))/1000","v":8.3936474999999948},{"$f":"IF('Dry Bulb'!J8<60,(('Input Data'!$F$44*('Dry Bulb'!J8-$T$15))+('Heat gain from airflow'!W7)+((Occupancy!V7*'Input Data'!$F$47)+(Occupancy!H7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J8-$P$15))+('Heat gain from airflow'!W7)+((Occupancy!V7*'Input Data'!$F$47)+(Occupancy!H7*'Input Data'!$F$49))))/1000","v":8.8705350000000003},{"$f":"IF('Dry Bulb'!K8<60,(('Input Data'!$F$44*('Dry Bulb'!K8-$T$15))+('Heat gain from airflow'!X7)+((Occupancy!W7*'Input Data'!$F$47)+(Occupancy!I7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K8-$P$15))+('Heat gain from airflow'!X7)+((Occupancy!W7*'Input Data'!$F$47)+(Occupancy!I7*'Input Data'!$F$49))))/1000","v":8.9659125000000017},{"$f":"IF('Dry Bulb'!L8<60,(('Input Data'!$F$44*('Dry Bulb'!L8-$T$15))+('Heat gain from airflow'!Y7)+((Occupancy!X7*'Input Data'!$F$47)+(Occupancy!J7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L8-$P$15))+('Heat gain from airflow'!Y7)+((Occupancy!X7*'Input Data'!$F$47)+(Occupancy!J7*'Input Data'!$F$49))))/1000","v":5.8184549999999966},{"$f":"IF('Dry Bulb'!M8<60,(('Input Data'!$F$44*('Dry Bulb'!M8-$T$15))+('Heat gain from airflow'!Z7)+((Occupancy!Y7*'Input Data'!$F$47)+(Occupancy!K7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M8-$P$15))+('Heat gain from airflow'!Z7)+((Occupancy!Y7*'Input Data'!$F$47)+(Occupancy!K7*'Input Data'!$F$49))))/1000","v":1.0314056249999997},{"$f":"IF('Dry Bulb'!N8<60,(('Input Data'!$F$44*('Dry Bulb'!N8-$T$15))+('Heat gain from airflow'!AA7)+((Occupancy!Z7*'Input Data'!$F$47)+(Occupancy!L7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N8-$P$15))+('Heat gain from airflow'!AA7)+((Occupancy!Z7*'Input Data'!$F$47)+(Occupancy!L7*'Input Data'!$F$49))))/1000","v":-4.7684474999999988},{"$f":"IF('Dry Bulb'!O8<60,(('Input Data'!$F$44*('Dry Bulb'!O8-$T$15))+('Heat gain from airflow'!AB7)+((Occupancy!AA7*'Input Data'!$F$47)+(Occupancy!M7*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O8-$P$15))+('Heat gain from airflow'!AB7)+((Occupancy!AA7*'Input Data'!$F$47)+(Occupancy!M7*'Input Data'!$F$49))))/1000","v":-5.5420649999999988E-3},null,null,null,null,null,null,null,null,null,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI62","v":3},{"$f":"'Incident angle'!BJ62","v":0},{"$f":"'Incident angle'!BK62","v":0},{"$f":"'Incident angle'!BL62","v":0},{"$f":"'Incident angle'!BM62","v":0},{"$f":"'Incident angle'!BN62","v":0},{"$f":"'Incident angle'!BO62","v":0},{"$f":"'Incident angle'!BP62","v":0},{"$f":"'Incident angle'!BQ62","v":0},{"$f":"'Incident angle'!BR62","v":0},{"$f":"'Incident angle'!BS62","v":0},{"$f":"'Incident angle'!BT62","v":0},{"$f":"'Incident angle'!BU62","v":0},{"$f":"MAX(AS32:AZ55)","v":5622.3905501017762},{"$f":"'Incident angle'!BW62","v":3},{"$f":"'Incident angle'!BX62","v":0},{"$f":"'Incident angle'!BY62","v":0},{"$f":"'Incident angle'!BZ62","v":0},{"$f":"'Incident angle'!CA62","v":0},{"$f":"'Incident angle'!CB62","v":0},{"$f":"'Incident angle'!CC62","v":0},{"$f":"'Incident angle'!CD62","v":0},{"$f":"'Incident angle'!CE62","v":0},{"$f":"'Incident angle'!CF62","v":0},{"$f":"'Incident angle'!CG62","v":0},{"$f":"'Incident angle'!CH62","v":0},{"$f":"'Incident angle'!CI62","v":0},{"$f":"MAX(BG32:BN55)","v":0},{"$f":"'Profile angles'!P7","v":3},{"$f":"RADIANS('Profile angles'!Q7)","v":0.91516630314878677},{"$f":"RADIANS('Profile angles'!R7)","v":0.8821622416026319},{"$f":"RADIANS('Profile angles'!S7)","v":0.80144392257758257},{"$f":"RADIANS('Profile angles'!T7)","v":0.69259090438957494},{"$f":"RADIANS('Profile angles'!U7)","v":0.62209031311095009},{"$f":"RADIANS('Profile angles'!V7)","v":0.61897895359016175},{"$f":"RADIANS('Profile angles'!W7)","v":0.66606658842026967},{"$f":"RADIANS('Profile angles'!X7)","v":0.70745482580220731},{"$f":"RADIANS('Profile angles'!Y7)","v":0.73590361062963061},{"$f":"RADIANS('Profile angles'!Z7)","v":0.76137198766493475},{"$f":"RADIANS('Profile angles'!AA7)","v":0.81690920458132044},{"$f":"RADIANS('Profile angles'!AB7)","v":0.88265807634038995},null,{"$f":"'Profile angles'!P36","v":3},{"$f":"RADIANS('Profile angles'!Q36)","v":1.5580652106671682},{"$f":"RADIANS('Profile angles'!R36)","v":-1.3784403465863997},{"$f":"RADIANS('Profile angles'!S36)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T36)","v":-0.85700339968847628},{"$f":"RADIANS('Profile angles'!U36)","v":-0.66444179725335362},{"$f":"RADIANS('Profile angles'!V36)","v":-0.60530956821516546},{"$f":"RADIANS('Profile angles'!W36)","v":-0.67565393770152993},{"$f":"RADIANS('Profile angles'!X36)","v":-0.85622667593368862},{"$f":"RADIANS('Profile angles'!Y36)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!Z36)","v":-1.410298559579243},{"$f":"RADIANS('Profile angles'!AA36)","v":1.5164850137084309},{"$f":"RADIANS('Profile angles'!AB36)","v":1.4620905045107382},null,{"$f":"'Profile angles'!AR7","v":3},{"$f":"(IF($AH$29<DEGREES(BS34),0+$AJ$33,1-((TAN(BS34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX60*$DU$3)+1-$DU$3)","v":8.9132570645729284E-2},{"$f":"(IF($AH$29<DEGREES(BT34),0+$AJ$33,1-((TAN(BT34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY60*$DU$3)+1-$DU$3)","v":0.13180855491516269},{"$f":"(IF($AH$29<DEGREES(BU34),0+$AJ$33,1-((TAN(BU34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ60*$DU$3)+1-$DU$3)","v":0.21134708662592533},{"$f":"(IF($AH$29<DEGREES(BV34),0+$AJ$33,1-((TAN(BV34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA60*$DU$3)+1-$DU$3)","v":0.26857852041732161},{"$f":"(IF($AH$29<DEGREES(BW34),0+$AJ$33,1-((TAN(BW34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB60*$DU$3)+1-$DU$3)","v":0.27006618269308391},{"$f":"(IF($AH$29<DEGREES(BX34),0+$AJ$33,1-((TAN(BX34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC60*$DU$3)+1-$DU$3)","v":0.24327765205823773},{"$f":"(IF($AH$29<DEGREES(BY34),0+$AJ$33,1-((TAN(BY34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD60*$DU$3)+1-$DU$3)","v":0.22933059507177717},{"$f":"(IF($AH$29<DEGREES(BZ34),0+$AJ$33,1-((TAN(BZ34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE60*$DU$3)+1-$DU$3)","v":0.25253092127229532},{"$f":"(IF($AH$29<DEGREES(CA34),0+$AJ$33,1-((TAN(CA34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF60*$DU$3)+1-$DU$3)","v":0.28983474395095987},{"$f":"(IF($AH$29<DEGREES(CB34),0+$AJ$33,1-((TAN(CB34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG60*$DU$3)+1-$DU$3)","v":0.30717527601126571},{"$f":"(IF($AH$29<DEGREES(CC34),0+$AJ$33,1-((TAN(CC34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH60*$DU$3)+1-$DU$3)","v":0.24706729880562944},{"$f":"(IF($AH$29<DEGREES(CD34),0+$AJ$33,1-((TAN(CD34)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI60*$DU$3)+1-$DU$3)","v":0.13877234129416038},null,3,{"$f":"(IF($AH$12<DEGREES(CG34),0+$AJ$16,1-((TAN(CG34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL60*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH34),0+$AJ$16,1-((TAN(CH34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM60*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI34),0+$AJ$16,1-((TAN(CI34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN60*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ34),0+$AJ$16,1-((TAN(CJ34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO60*$DU$3)+1-$DU$3)","v":0.55012591715633463},{"$f":"(IF($AH$12<DEGREES(CK34),0+$AJ$16,1-((TAN(CK34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP60*$DU$3)+1-$DU$3)","v":0.70269231165087753},{"$f":"(IF($AH$12<DEGREES(CL34),0+$AJ$16,1-((TAN(CL34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ60*$DU$3)+1-$DU$3)","v":0.76344894483829573},{"$f":"(IF($AH$12<DEGREES(CM34),0+$AJ$16,1-((TAN(CM34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR60*$DU$3)+1-$DU$3)","v":0.76500411178339689},{"$f":"(IF($AH$12<DEGREES(CN34),0+$AJ$16,1-((TAN(CN34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS60*$DU$3)+1-$DU$3)","v":0.58901275392134778},{"$f":"(IF($AH$12<DEGREES(CO34),0+$AJ$16,1-((TAN(CO34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT60*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP34),0+$AJ$16,1-((TAN(CP34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU60*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ34),0+$AJ$16,1-((TAN(CQ34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV60*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR34),0+$AJ$16,1-((TAN(CR34)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW60*$DU$3)+1-$DU$3)","v":0},null,null,3,-52.431373562484438,-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552,null,3,-52.431373562484438,-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552]
[null,5,{"$f":"IF('Dry Bulb'!D9<60,(('Input Data'!$F$44*('Dry Bulb'!D9-$T$15))+('Heat gain from airflow'!Q8)+((Occupancy!P8*'Input Data'!$F$47)+(Occupancy!B8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D9-$P$15))+('Heat gain from airflow'!Q8)+((Occupancy!P8*'Input Data'!$F$47)+(Occupancy!B8*'Input Data'!$F$49))))/1000","v":-7.1634824999999994E-3},{"$f":"IF('Dry Bulb'!E9<60,(('Input Data'!$F$44*('Dry Bulb'!E9-$T$15))+('Heat gain from airflow'!R8)+((Occupancy!Q8*'Input Data'!$F$47)+(Occupancy!C8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E9-$P$15))+('Heat gain from airflow'!R8)+((Occupancy!Q8*'Input Data'!$F$47)+(Occupancy!C8*'Input Data'!$F$49))))/1000","v":-5.0651775000000003E-3},{"$f":"IF('Dry Bulb'!F9<60,(('Input Data'!$F$44*('Dry Bulb'!F9-$T$15))+('Heat gain from airflow'!S8)+((Occupancy!R8*'Input Data'!$F$47)+(Occupancy!D8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F9-$P$15))+('Heat gain from airflow'!S8)+((Occupancy!R8*'Input Data'!$F$47)+(Occupancy!D8*'Input Data'!$F$49))))/1000","v":-1.6315875000000016E-3},{"$f":"IF('Dry Bulb'!G9<60,(('Input Data'!$F$44*('Dry Bulb'!G9-$T$15))+('Heat gain from airflow'!T8)+((Occupancy!S8*'Input Data'!$F$47)+(Occupancy!E8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G9-$P$15))+('Heat gain from airflow'!T8)+((Occupancy!S8*'Input Data'!$F$47)+(Occupancy!E8*'Input Data'!$F$49))))/1000","v":-1.666209060000001},{"$f":"IF('Dry Bulb'!H9<60,(('Input Data'!$F$44*('Dry Bulb'!H9-$T$15))+('Heat gain from airflow'!U8)+((Occupancy!T8*'Input Data'!$F$47)+(Occupancy!F8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H9-$P$15))+('Heat gain from airflow'!U8)+((Occupancy!T8*'Input Data'!$F$47)+(Occupancy!F8*'Input Data'!$F$49))))/1000","v":5.3415675000000009},{"$f":"IF('Dry Bulb'!I9<60,(('Input Data'!$F$44*('Dry Bulb'!I9-$T$15))+('Heat gain from airflow'!V8)+((Occupancy!U8*'Input Data'!$F$47)+(Occupancy!G8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I9-$P$15))+('Heat gain from airflow'!V8)+((Occupancy!U8*'Input Data'!$F$47)+(Occupancy!G8*'Input Data'!$F$49))))/1000","v":7.7260050000000007},{"$f":"IF('Dry Bulb'!J9<60,(('Input Data'!$F$44*('Dry Bulb'!J9-$T$15))+('Heat gain from airflow'!W8)+((Occupancy!V8*'Input Data'!$F$47)+(Occupancy!H8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J9-$P$15))+('Heat gain from airflow'!W8)+((Occupancy!V8*'Input Data'!$F$47)+(Occupancy!H8*'Input Data'!$F$49))))/1000","v":8.4890249999999998},{"$f":"IF('Dry Bulb'!K9<60,(('Input Data'!$F$44*('Dry Bulb'!K9-$T$15))+('Heat gain from airflow'!X8)+((Occupancy!W8*'Input Data'!$F$47)+(Occupancy!I8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K9-$P$15))+('Heat gain from airflow'!X8)+((Occupancy!W8*'Input Data'!$F$47)+(Occupancy!I8*'Input Data'!$F$49))))/1000","v":8.3936474999999948},{"$f":"IF('Dry Bulb'!L9<60,(('Input Data'!$F$44*('Dry Bulb'!L9-$T$15))+('Heat gain from airflow'!Y8)+((Occupancy!X8*'Input Data'!$F$47)+(Occupancy!J8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L9-$P$15))+('Heat gain from airflow'!Y8)+((Occupancy!X8*'Input Data'!$F$47)+(Occupancy!J8*'Input Data'!$F$49))))/1000","v":5.4369450000000041},{"$f":"IF('Dry Bulb'!M9<60,(('Input Data'!$F$44*('Dry Bulb'!M9-$T$15))+('Heat gain from airflow'!Z8)+((Occupancy!Y8*'Input Data'!$F$47)+(Occupancy!K8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M9-$P$15))+('Heat gain from airflow'!Z8)+((Occupancy!Y8*'Input Data'!$F$47)+(Occupancy!K8*'Input Data'!$F$49))))/1000","v":9.3104865000001161E-2},{"$f":"IF('Dry Bulb'!N9<60,(('Input Data'!$F$44*('Dry Bulb'!N9-$T$15))+('Heat gain from airflow'!AA8)+((Occupancy!Z8*'Input Data'!$F$47)+(Occupancy!L8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N9-$P$15))+('Heat gain from airflow'!AA8)+((Occupancy!Z8*'Input Data'!$F$47)+(Occupancy!L8*'Input Data'!$F$49))))/1000","v":-1.8223424999999972E-3},{"$f":"IF('Dry Bulb'!O9<60,(('Input Data'!$F$44*('Dry Bulb'!O9-$T$15))+('Heat gain from airflow'!AB8)+((Occupancy!AA8*'Input Data'!$F$47)+(Occupancy!M8*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O9-$P$15))+('Heat gain from airflow'!AB8)+((Occupancy!AA8*'Input Data'!$F$47)+(Occupancy!M8*'Input Data'!$F$49))))/1000","v":-6.0189524999999973E-3},null,"East Window",null,null,null,"Heavy Mass?",null,null,null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI63","v":4},{"$f":"'Incident angle'!BJ63","v":0},{"$f":"'Incident angle'!BK63","v":0},{"$f":"'Incident angle'!BL63","v":0},{"$f":"'Incident angle'!BM63","v":0},{"$f":"'Incident angle'!BN63","v":0},{"$f":"'Incident angle'!BO63","v":0},{"$f":"'Incident angle'!BP63","v":0},{"$f":"'Incident angle'!BQ63","v":0},{"$f":"'Incident angle'!BR63","v":0},{"$f":"'Incident angle'!BS63","v":0},{"$f":"'Incident angle'!BT63","v":0},{"$f":"'Incident angle'!BU63","v":0},"Av+Max/2",{"$f":"'Incident angle'!BW63","v":4},{"$f":"'Incident angle'!BX63","v":0},{"$f":"'Incident angle'!BY63","v":0},{"$f":"'Incident angle'!BZ63","v":0},{"$f":"'Incident angle'!CA63","v":0},{"$f":"'Incident angle'!CB63","v":0},{"$f":"'Incident angle'!CC63","v":0},{"$f":"'Incident angle'!CD63","v":0},{"$f":"'Incident angle'!CE63","v":0},{"$f":"'Incident angle'!CF63","v":0},{"$f":"'Incident angle'!CG63","v":0},{"$f":"'Incident angle'!CH63","v":0},{"$f":"'Incident angle'!CI63","v":0},"Av+Max/2",{"$f":"'Profile angles'!P8","v":4},{"$f":"RADIANS('Profile angles'!Q8)","v":0.68085626049108372},{"$f":"RADIANS('Profile angles'!R8)","v":0.63580151600596946},{"$f":"RADIANS('Profile angles'!S8)","v":0.54404800401822839},{"$f":"RADIANS('Profile angles'!T8)","v":0.42586833332700952},{"$f":"RADIANS('Profile angles'!U8)","v":0.34974170353085882},{"$f":"RADIANS('Profile angles'!V8)","v":0.34253601746325713},{"$f":"RADIANS('Profile angles'!W8)","v":0.38955752453779996},{"$f":"RADIANS('Profile angles'!X8)","v":0.43944775480650367},{"$f":"RADIANS('Profile angles'!Y8)","v":0.48155681326357486},{"$f":"RADIANS('Profile angles'!Z8)","v":0.51888038822348748},{"$f":"RADIANS('Profile angles'!AA8)","v":0.58456796965293845},{"$f":"RADIANS('Profile angles'!AB8)","v":0.6539876584676938},null,{"$f":"'Profile angles'!P37","v":4},{"$f":"RADIANS('Profile angles'!Q37)","v":1.4341706307619093},{"$f":"RADIANS('Profile angles'!R37)","v":-1.4532017897405851},{"$f":"RADIANS('Profile angles'!S37)","v":-1.1397000015522976},{"$f":"RADIANS('Profile angles'!T37)","v":-0.75641890675993251},{"$f":"RADIANS('Profile angles'!U37)","v":-0.5162754389988029},{"$f":"RADIANS('Profile angles'!V37)","v":-0.4555590077463848},{"$f":"RADIANS('Profile angles'!W37)","v":-0.54225140039405473},{"$f":"RADIANS('Profile angles'!X37)","v":-0.7589538863925066},{"$f":"RADIANS('Profile angles'!Y37)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!Z37)","v":-1.5231003679412916},{"$f":"RADIANS('Profile angles'!AA37)","v":1.3502899956877576},{"$f":"RADIANS('Profile angles'!AB37)","v":1.3073727427737785},null,{"$f":"'Profile angles'!AR8","v":4},{"$f":"(IF($AH$29<DEGREES(BS35),0+$AJ$33,1-((TAN(BS35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX61*$DU$3)+1-$DU$3)","v":0.40883616917910198},{"$f":"(IF($AH$29<DEGREES(BT35),0+$AJ$33,1-((TAN(BT35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY61*$DU$3)+1-$DU$3)","v":0.46230021270867849},{"$f":"(IF($AH$29<DEGREES(BU35),0+$AJ$33,1-((TAN(BU35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ61*$DU$3)+1-$DU$3)","v":0.49632901547601815},{"$f":"(IF($AH$29<DEGREES(BV35),0+$AJ$33,1-((TAN(BV35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA61*$DU$3)+1-$DU$3)","v":0.51842535501492781},{"$f":"(IF($AH$29<DEGREES(BW35),0+$AJ$33,1-((TAN(BW35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB61*$DU$3)+1-$DU$3)","v":0.50543153562033727},{"$f":"(IF($AH$29<DEGREES(BX35),0+$AJ$33,1-((TAN(BX35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC61*$DU$3)+1-$DU$3)","v":0.47730314076804897},{"$f":"(IF($AH$29<DEGREES(BY35),0+$AJ$33,1-((TAN(BY35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD61*$DU$3)+1-$DU$3)","v":0.4698337359631819},{"$f":"(IF($AH$29<DEGREES(BZ35),0+$AJ$33,1-((TAN(BZ35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE61*$DU$3)+1-$DU$3)","v":0.50465332780229777},{"$f":"(IF($AH$29<DEGREES(CA35),0+$AJ$33,1-((TAN(CA35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF61*$DU$3)+1-$DU$3)","v":0.55796803909378501},{"$f":"(IF($AH$29<DEGREES(CB35),0+$AJ$33,1-((TAN(CB35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG61*$DU$3)+1-$DU$3)","v":0.59206573653525008},{"$f":"(IF($AH$29<DEGREES(CC35),0+$AJ$33,1-((TAN(CC35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH61*$DU$3)+1-$DU$3)","v":0.49698802531809105},{"$f":"(IF($AH$29<DEGREES(CD35),0+$AJ$33,1-((TAN(CD35)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI61*$DU$3)+1-$DU$3)","v":0.41553742021201423},null,4,{"$f":"(IF($AH$12<DEGREES(CG35),0+$AJ$16,1-((TAN(CG35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL61*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH35),0+$AJ$16,1-((TAN(CH35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM61*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI35),0+$AJ$16,1-((TAN(CI35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN61*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ35),0+$AJ$16,1-((TAN(CJ35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO61*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK35),0+$AJ$16,1-((TAN(CK35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP61*$DU$3)+1-$DU$3)","v":0.31002178103403261},{"$f":"(IF($AH$12<DEGREES(CL35),0+$AJ$16,1-((TAN(CL35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ61*$DU$3)+1-$DU$3)","v":0.4203977359683565},{"$f":"(IF($AH$12<DEGREES(CM35),0+$AJ$16,1-((TAN(CM35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR61*$DU$3)+1-$DU$3)","v":0.37848798214147028},{"$f":"(IF($AH$12<DEGREES(CN35),0+$AJ$16,1-((TAN(CN35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS61*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO35),0+$AJ$16,1-((TAN(CO35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT61*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP35),0+$AJ$16,1-((TAN(CP35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU61*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ35),0+$AJ$16,1-((TAN(CQ35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV61*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR35),0+$AJ$16,1-((TAN(CR35)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW61*$DU$3)+1-$DU$3)","v":0},null,null,4,-38.837571781392398,-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833,null,4,-38.837571781392398,-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833]
[null,6,{"$f":"IF('Dry Bulb'!D10<60,(('Input Data'!$F$44*('Dry Bulb'!D10-$T$15))+('Heat gain from airflow'!Q9)+((Occupancy!P9*'Input Data'!$F$47)+(Occupancy!B9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D10-$P$15))+('Heat gain from airflow'!Q9)+((Occupancy!P9*'Input Data'!$F$47)+(Occupancy!B9*'Input Data'!$F$49))))/1000","v":-7.4496149999999997E-3},{"$f":"IF('Dry Bulb'!E10<60,(('Input Data'!$F$44*('Dry Bulb'!E10-$T$15))+('Heat gain from airflow'!R9)+((Occupancy!Q9*'Input Data'!$F$47)+(Occupancy!C9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E10-$P$15))+('Heat gain from airflow'!R9)+((Occupancy!Q9*'Input Data'!$F$47)+(Occupancy!C9*'Input Data'!$F$49))))/1000","v":-5.4466874999999993E-3},{"$f":"IF('Dry Bulb'!F10<60,(('Input Data'!$F$44*('Dry Bulb'!F10-$T$15))+('Heat gain from airflow'!S9)+((Occupancy!R9*'Input Data'!$F$47)+(Occupancy!D9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F10-$P$15))+('Heat gain from airflow'!S9)+((Occupancy!R9*'Input Data'!$F$47)+(Occupancy!D9*'Input Data'!$F$49))))/1000","v":-1.9177200000000004E-3},{"$f":"IF('Dry Bulb'!G10<60,(('Input Data'!$F$44*('Dry Bulb'!G10-$T$15))+('Heat gain from airflow'!T9)+((Occupancy!S9*'Input Data'!$F$47)+(Occupancy!E9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G10-$P$15))+('Heat gain from airflow'!T9)+((Occupancy!S9*'Input Data'!$F$47)+(Occupancy!E9*'Input Data'!$F$49))))/1000","v":-2.1353594400000002},{"$f":"IF('Dry Bulb'!H10<60,(('Input Data'!$F$44*('Dry Bulb'!H10-$T$15))+('Heat gain from airflow'!U9)+((Occupancy!T9*'Input Data'!$F$47)+(Occupancy!F9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H10-$P$15))+('Heat gain from airflow'!U9)+((Occupancy!T9*'Input Data'!$F$47)+(Occupancy!F9*'Input Data'!$F$49))))/1000","v":5.1364714499999975},{"$f":"IF('Dry Bulb'!I10<60,(('Input Data'!$F$44*('Dry Bulb'!I10-$T$15))+('Heat gain from airflow'!V9)+((Occupancy!U9*'Input Data'!$F$47)+(Occupancy!G9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I10-$P$15))+('Heat gain from airflow'!V9)+((Occupancy!U9*'Input Data'!$F$47)+(Occupancy!G9*'Input Data'!$F$49))))/1000","v":7.1537400000000018},{"$f":"IF('Dry Bulb'!J10<60,(('Input Data'!$F$44*('Dry Bulb'!J10-$T$15))+('Heat gain from airflow'!W9)+((Occupancy!V9*'Input Data'!$F$47)+(Occupancy!H9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J10-$P$15))+('Heat gain from airflow'!W9)+((Occupancy!V9*'Input Data'!$F$47)+(Occupancy!H9*'Input Data'!$F$49))))/1000","v":8.1075150000000011},{"$f":"IF('Dry Bulb'!K10<60,(('Input Data'!$F$44*('Dry Bulb'!K10-$T$15))+('Heat gain from airflow'!X9)+((Occupancy!W9*'Input Data'!$F$47)+(Occupancy!I9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K10-$P$15))+('Heat gain from airflow'!X9)+((Occupancy!W9*'Input Data'!$F$47)+(Occupancy!I9*'Input Data'!$F$49))))/1000","v":7.9167599999999929},{"$f":"IF('Dry Bulb'!L10<60,(('Input Data'!$F$44*('Dry Bulb'!L10-$T$15))+('Heat gain from airflow'!Y9)+((Occupancy!X9*'Input Data'!$F$47)+(Occupancy!J9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L10-$P$15))+('Heat gain from airflow'!Y9)+((Occupancy!X9*'Input Data'!$F$47)+(Occupancy!J9*'Input Data'!$F$49))))/1000","v":5.7229094250000019},{"$f":"IF('Dry Bulb'!M10<60,(('Input Data'!$F$44*('Dry Bulb'!M10-$T$15))+('Heat gain from airflow'!Z9)+((Occupancy!Y9*'Input Data'!$F$47)+(Occupancy!K9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M10-$P$15))+('Heat gain from airflow'!Z9)+((Occupancy!Y9*'Input Data'!$F$47)+(Occupancy!K9*'Input Data'!$F$49))))/1000","v":-0.4933331100000023},{"$f":"IF('Dry Bulb'!N10<60,(('Input Data'!$F$44*('Dry Bulb'!N10-$T$15))+('Heat gain from airflow'!AA9)+((Occupancy!Z9*'Input Data'!$F$47)+(Occupancy!L9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N10-$P$15))+('Heat gain from airflow'!AA9)+((Occupancy!Z9*'Input Data'!$F$47)+(Occupancy!L9*'Input Data'!$F$49))))/1000","v":-2.0130975000000008E-3},{"$f":"IF('Dry Bulb'!O10<60,(('Input Data'!$F$44*('Dry Bulb'!O10-$T$15))+('Heat gain from airflow'!AB9)+((Occupancy!AA9*'Input Data'!$F$47)+(Occupancy!M9*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O10-$P$15))+('Heat gain from airflow'!AB9)+((Occupancy!AA9*'Input Data'!$F$47)+(Occupancy!M9*'Input Data'!$F$49))))/1000","v":-6.0189524999999973E-3},null,"Area",{"$f":"Q39*'Input Data'!F23*'Input Data'!F19","v":225},"y",null,"n",null,null,null,null,null,null,null,"SILL",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI64","v":5},{"$f":"'Incident angle'!BJ64","v":0},{"$f":"'Incident angle'!BK64","v":0},{"$f":"'Incident angle'!BL64","v":0},{"$f":"'Incident angle'!BM64","v":0},{"$f":"'Incident angle'!BN64","v":0},{"$f":"'Incident angle'!BO64","v":0},{"$f":"'Incident angle'!BP64","v":0},{"$f":"'Incident angle'!BQ64","v":0},{"$f":"'Incident angle'!BR64","v":0},{"$f":"'Incident angle'!BS64","v":0},{"$f":"'Incident angle'!BT64","v":0},{"$f":"'Incident angle'!BU64","v":0},{"$f":"AVERAGE(BC32,BC34)","v":4418.0570092767739},{"$f":"'Incident angle'!BW64","v":5},{"$f":"'Incident angle'!BX64","v":0},{"$f":"'Incident angle'!BY64","v":0},{"$f":"'Incident angle'!BZ64","v":0},{"$f":"'Incident angle'!CA64","v":0},{"$f":"'Incident angle'!CB64","v":0},{"$f":"'Incident angle'!CC64","v":0},{"$f":"'Incident angle'!CD64","v":0},{"$f":"'Incident angle'!CE64","v":0},{"$f":"'Incident angle'!CF64","v":0},{"$f":"'Incident angle'!CG64","v":0},{"$f":"'Incident angle'!CH64","v":0},{"$f":"'Incident angle'!CI64","v":0},{"$f":"AVERAGE(BQ32,BQ34)","v":{"$error":"#DIV/0!"}},{"$f":"'Profile angles'!P9","v":5},{"$f":"RADIANS('Profile angles'!Q9)","v":0.45057174190181387},{"$f":"RADIANS('Profile angles'!R9)","v":0.39650083624290827},{"$f":"RADIANS('Profile angles'!S9)","v":0.29766243646613255},{"$f":"RADIANS('Profile angles'!T9)","v":0.17558478457949331},{"$f":"RADIANS('Profile angles'!U9)","v":9.870439314060718E-2},{"$f":"RADIANS('Profile angles'!V9)","v":9.0149372015666446E-2},{"$f":"RADIANS('Profile angles'!W9)","v":0.1356210090143263},{"$f":"RADIANS('Profile angles'!X9)","v":0.18829152816436306},{"$f":"RADIANS('Profile angles'!Y9)","v":0.23731883827832312},{"$f":"RADIANS('Profile angles'!Z9)","v":0.28192945219888416},{"$f":"RADIANS('Profile angles'!AA9)","v":0.35506274589045206},{"$f":"RADIANS('Profile angles'!AB9)","v":0.42785968501246857},null,{"$f":"'Profile angles'!P38","v":5},{"$f":"RADIANS('Profile angles'!Q38)","v":1.1780474606511624},{"$f":"RADIANS('Profile angles'!R38)","v":1.5063837691420774},{"$f":"RADIANS('Profile angles'!S38)","v":-1.1397000015522976},{"$f":"RADIANS('Profile angles'!T38)","v":-0.50158785009162166},{"$f":"RADIANS('Profile angles'!U38)","v":-0.20807374674275145},{"$f":"RADIANS('Profile angles'!V38)","v":-0.16549565334901178},{"$f":"RADIANS('Profile angles'!W38)","v":-0.26831827706241224},{"$f":"RADIANS('Profile angles'!X38)","v":-0.51728377304772155},{"$f":"RADIANS('Profile angles'!Y38)","v":-1.1397000015522978},{"$f":"RADIANS('Profile angles'!Z38)","v":1.3007610762503929},{"$f":"RADIANS('Profile angles'!AA38)","v":0.9983276557533427},{"$f":"RADIANS('Profile angles'!AB38)","v":1.0076474712095662},null,{"$f":"'Profile angles'!AR9","v":5},{"$f":"(IF($AH$29<DEGREES(BS36),0+$AJ$33,1-((TAN(BS36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX62*$DU$3)+1-$DU$3)","v":0.59509590751783481},{"$f":"(IF($AH$29<DEGREES(BT36),0+$AJ$33,1-((TAN(BT36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY62*$DU$3)+1-$DU$3)","v":0.69738236614041227},{"$f":"(IF($AH$29<DEGREES(BU36),0+$AJ$33,1-((TAN(BU36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ62*$DU$3)+1-$DU$3)","v":0.72985575444174666},{"$f":"(IF($AH$29<DEGREES(BV36),0+$AJ$33,1-((TAN(BV36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA62*$DU$3)+1-$DU$3)","v":0.73413697491561425},{"$f":"(IF($AH$29<DEGREES(BW36),0+$AJ$33,1-((TAN(BW36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB62*$DU$3)+1-$DU$3)","v":0.71242259165975175},{"$f":"(IF($AH$29<DEGREES(BX36),0+$AJ$33,1-((TAN(BX36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC62*$DU$3)+1-$DU$3)","v":0.68324259641096841},{"$f":"(IF($AH$29<DEGREES(BY36),0+$AJ$33,1-((TAN(BY36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD62*$DU$3)+1-$DU$3)","v":0.68002959775522431},{"$f":"(IF($AH$29<DEGREES(BZ36),0+$AJ$33,1-((TAN(BZ36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE62*$DU$3)+1-$DU$3)","v":0.7214981482170949},{"$f":"(IF($AH$29<DEGREES(CA36),0+$AJ$33,1-((TAN(CA36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF62*$DU$3)+1-$DU$3)","v":0.78447891700523564},{"$f":"(IF($AH$29<DEGREES(CB36),0+$AJ$33,1-((TAN(CB36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG62*$DU$3)+1-$DU$3)","v":0.76529016184022669},{"$f":"(IF($AH$29<DEGREES(CC36),0+$AJ$33,1-((TAN(CC36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH62*$DU$3)+1-$DU$3)","v":0.6519905976900795},{"$f":"(IF($AH$29<DEGREES(CD36),0+$AJ$33,1-((TAN(CD36)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI62*$DU$3)+1-$DU$3)","v":0.58277422664909306},null,5,{"$f":"(IF($AH$12<DEGREES(CG36),0+$AJ$16,1-((TAN(CG36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH36),0+$AJ$16,1-((TAN(CH36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI36),0+$AJ$16,1-((TAN(CI36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ36),0+$AJ$16,1-((TAN(CJ36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK36),0+$AJ$16,1-((TAN(CK36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL36),0+$AJ$16,1-((TAN(CL36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ62*$DU$3)+1-$DU$3)","v":8.5043263015680048E-2},{"$f":"(IF($AH$12<DEGREES(CM36),0+$AJ$16,1-((TAN(CM36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN36),0+$AJ$16,1-((TAN(CN36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO36),0+$AJ$16,1-((TAN(CO36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP36),0+$AJ$16,1-((TAN(CP36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ36),0+$AJ$16,1-((TAN(CQ36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV62*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR36),0+$AJ$16,1-((TAN(CR36)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW62*$DU$3)+1-$DU$3)","v":0},null,null,5,-25.376333918471747,-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006,null,5,-25.376333918471747,-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006]
[null,7,{"$f":"IF('Dry Bulb'!D11<60,(('Input Data'!$F$44*('Dry Bulb'!D11-$T$15))+('Heat gain from airflow'!Q10)+((Occupancy!P10*'Input Data'!$F$47)+(Occupancy!B10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D11-$P$15))+('Heat gain from airflow'!Q10)+((Occupancy!P10*'Input Data'!$F$47)+(Occupancy!B10*'Input Data'!$F$49))))/1000","v":-7.4496149999999997E-3},{"$f":"IF('Dry Bulb'!E11<60,(('Input Data'!$F$44*('Dry Bulb'!E11-$T$15))+('Heat gain from airflow'!R10)+((Occupancy!Q10*'Input Data'!$F$47)+(Occupancy!C10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E11-$P$15))+('Heat gain from airflow'!R10)+((Occupancy!Q10*'Input Data'!$F$47)+(Occupancy!C10*'Input Data'!$F$49))))/1000","v":-5.4466874999999993E-3},{"$f":"IF('Dry Bulb'!F11<60,(('Input Data'!$F$44*('Dry Bulb'!F11-$T$15))+('Heat gain from airflow'!S10)+((Occupancy!R10*'Input Data'!$F$47)+(Occupancy!D10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F11-$P$15))+('Heat gain from airflow'!S10)+((Occupancy!R10*'Input Data'!$F$47)+(Occupancy!D10*'Input Data'!$F$49))))/1000","v":-1.9177200000000004E-3},{"$f":"IF('Dry Bulb'!G11<60,(('Input Data'!$F$44*('Dry Bulb'!G11-$T$15))+('Heat gain from airflow'!T10)+((Occupancy!S10*'Input Data'!$F$47)+(Occupancy!E10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G11-$P$15))+('Heat gain from airflow'!T10)+((Occupancy!S10*'Input Data'!$F$47)+(Occupancy!E10*'Input Data'!$F$49))))/1000","v":-0.96248349000000188},{"$f":"IF('Dry Bulb'!H11<60,(('Input Data'!$F$44*('Dry Bulb'!H11-$T$15))+('Heat gain from airflow'!U10)+((Occupancy!T10*'Input Data'!$F$47)+(Occupancy!F10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H11-$P$15))+('Heat gain from airflow'!U10)+((Occupancy!T10*'Input Data'!$F$47)+(Occupancy!F10*'Input Data'!$F$49))))/1000","v":5.7230775000000005},{"$f":"IF('Dry Bulb'!I11<60,(('Input Data'!$F$44*('Dry Bulb'!I11-$T$15))+('Heat gain from airflow'!V10)+((Occupancy!U10*'Input Data'!$F$47)+(Occupancy!G10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I11-$P$15))+('Heat gain from airflow'!V10)+((Occupancy!U10*'Input Data'!$F$47)+(Occupancy!G10*'Input Data'!$F$49))))/1000","v":8.6797799999999992},{"$f":"IF('Dry Bulb'!J11<60,(('Input Data'!$F$44*('Dry Bulb'!J11-$T$15))+('Heat gain from airflow'!W10)+((Occupancy!V10*'Input Data'!$F$47)+(Occupancy!H10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J11-$P$15))+('Heat gain from airflow'!W10)+((Occupancy!V10*'Input Data'!$F$47)+(Occupancy!H10*'Input Data'!$F$49))))/1000","v":9.5381775000000015},{"$f":"IF('Dry Bulb'!K11<60,(('Input Data'!$F$44*('Dry Bulb'!K11-$T$15))+('Heat gain from airflow'!X10)+((Occupancy!W10*'Input Data'!$F$47)+(Occupancy!I10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K11-$P$15))+('Heat gain from airflow'!X10)+((Occupancy!W10*'Input Data'!$F$47)+(Occupancy!I10*'Input Data'!$F$49))))/1000","v":9.252044999999999},{"$f":"IF('Dry Bulb'!L11<60,(('Input Data'!$F$44*('Dry Bulb'!L11-$T$15))+('Heat gain from airflow'!Y10)+((Occupancy!X10*'Input Data'!$F$47)+(Occupancy!J10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L11-$P$15))+('Heat gain from airflow'!Y10)+((Occupancy!X10*'Input Data'!$F$47)+(Occupancy!J10*'Input Data'!$F$49))))/1000","v":6.1999650000000042},{"$f":"IF('Dry Bulb'!M11<60,(('Input Data'!$F$44*('Dry Bulb'!M11-$T$15))+('Heat gain from airflow'!Z10)+((Occupancy!Y10*'Input Data'!$F$47)+(Occupancy!K10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M11-$P$15))+('Heat gain from airflow'!Z10)+((Occupancy!Y10*'Input Data'!$F$47)+(Occupancy!K10*'Input Data'!$F$49))))/1000","v":9.3104865000001161E-2},{"$f":"IF('Dry Bulb'!N11<60,(('Input Data'!$F$44*('Dry Bulb'!N11-$T$15))+('Heat gain from airflow'!AA10)+((Occupancy!Z10*'Input Data'!$F$47)+(Occupancy!L10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N11-$P$15))+('Heat gain from airflow'!AA10)+((Occupancy!Z10*'Input Data'!$F$47)+(Occupancy!L10*'Input Data'!$F$49))))/1000","v":-2.2038524999999998E-3},{"$f":"IF('Dry Bulb'!O11<60,(('Input Data'!$F$44*('Dry Bulb'!O11-$T$15))+('Heat gain from airflow'!AB10)+((Occupancy!AA10*'Input Data'!$F$47)+(Occupancy!M10*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O11-$P$15))+('Heat gain from airflow'!AB10)+((Occupancy!AA10*'Input Data'!$F$47)+(Occupancy!M10*'Input Data'!$F$49))))/1000","v":-6.2097075000000024E-3},null,"Glass SHGC",0.28999999999999998,"n",null,null,null,null,null,"EAST WINDOW SECTION",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI65","v":6},{"$f":"'Incident angle'!BJ65","v":0},{"$f":"'Incident angle'!BK65","v":0},{"$f":"'Incident angle'!BL65","v":0},{"$f":"'Incident angle'!BM65","v":0},{"$f":"'Incident angle'!BN65","v":0},{"$f":"'Incident angle'!BO65","v":0},{"$f":"'Incident angle'!BP65","v":0},{"$f":"'Incident angle'!BQ65","v":0},{"$f":"'Incident angle'!BR65","v":0},{"$f":"'Incident angle'!BS65","v":0},{"$f":"'Incident angle'!BT65","v":0},{"$f":"'Incident angle'!BU65","v":0},null,{"$f":"'Incident angle'!BW65","v":6},{"$f":"'Incident angle'!BX65","v":0},{"$f":"'Incident angle'!BY65","v":0},{"$f":"'Incident angle'!BZ65","v":0},{"$f":"'Incident angle'!CA65","v":0},{"$f":"'Incident angle'!CB65","v":0},{"$f":"'Incident angle'!CC65","v":0},{"$f":"'Incident angle'!CD65","v":0},{"$f":"'Incident angle'!CE65","v":0},{"$f":"'Incident angle'!CF65","v":0},{"$f":"'Incident angle'!CG65","v":0},{"$f":"'Incident angle'!CH65","v":0},{"$f":"'Incident angle'!CI65","v":0},null,{"$f":"'Profile angles'!P10","v":6},{"$f":"RADIANS('Profile angles'!Q10)","v":0.22091645053294795},{"$f":"RADIANS('Profile angles'!R10)","v":0.16074662252161659},{"$f":"RADIANS('Profile angles'!S10)","v":5.8021971754234451E-2},{"$f":"RADIANS('Profile angles'!T10)","v":-6.4078725586556834E-2},{"$f":"RADIANS('Profile angles'!U10)","v":-0.13850562031664443},{"$f":"RADIANS('Profile angles'!V10)","v":-0.14648644817173606},{"$f":"RADIANS('Profile angles'!W10)","v":-0.1032161832467153},{"$f":"RADIANS('Profile angles'!X10)","v":-5.1801075064635944E-2},{"$f":"RADIANS('Profile angles'!Y10)","v":-1.4535089563001097E-3},{"$f":"RADIANS('Profile angles'!Z10)","v":4.619108081230195E-2},{"$f":"RADIANS('Profile angles'!AA10)","v":0.12425151109146822},{"$f":"RADIANS('Profile angles'!AB10)","v":0.20052072268814197},null,{"$f":"'Profile angles'!P39","v":6},{"$f":"RADIANS('Profile angles'!Q39)","v":0.64835816681447511},{"$f":"RADIANS('Profile angles'!R39)","v":0.88647687640734651},{"$f":"RADIANS('Profile angles'!S39)","v":-1.1397000015522964},{"$f":"RADIANS('Profile angles'!T39)","v":0.30683145766901859},{"$f":"RADIANS('Profile angles'!U39)","v":0.38591275889302934},{"$f":"RADIANS('Profile angles'!V39)","v":0.34548950434356818},{"$f":"RADIANS('Profile angles'!W39)","v":0.27681674745400858},{"$f":"RADIANS('Profile angles'!X39)","v":0.23949897187106278},{"$f":"RADIANS('Profile angles'!Y39)","v":-1.1397000015523873},{"$f":"RADIANS('Profile angles'!Z39)","v":0.24250985894867499},{"$f":"RADIANS('Profile angles'!AA39)","v":0.35092289852329323},{"$f":"RADIANS('Profile angles'!AB39)","v":0.48669309889480072},null,{"$f":"'Profile angles'!AR10","v":6},{"$f":"(IF($AH$29<DEGREES(BS37),0+$AJ$33,1-((TAN(BS37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX63*$DU$3)+1-$DU$3)","v":0.71787732072739341},{"$f":"(IF($AH$29<DEGREES(BT37),0+$AJ$33,1-((TAN(BT37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY63*$DU$3)+1-$DU$3)","v":0.82786359906000684},{"$f":"(IF($AH$29<DEGREES(BU37),0+$AJ$33,1-((TAN(BU37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ63*$DU$3)+1-$DU$3)","v":0.94652359620523918},{"$f":"(IF($AH$29<DEGREES(BV37),0+$AJ$33,1-((TAN(BV37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA63*$DU$3)+1-$DU$3)","v":0.93910724218462893},{"$f":"(IF($AH$29<DEGREES(BW37),0+$AJ$33,1-((TAN(BW37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB63*$DU$3)+1-$DU$3)","v":0.90928671162082175},{"$f":"(IF($AH$29<DEGREES(BX37),0+$AJ$33,1-((TAN(BX37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC63*$DU$3)+1-$DU$3)","v":0.87714784354076558},{"$f":"(IF($AH$29<DEGREES(BY37),0+$AJ$33,1-((TAN(BY37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD63*$DU$3)+1-$DU$3)","v":0.87699547793655297},{"$f":"(IF($AH$29<DEGREES(BZ37),0+$AJ$33,1-((TAN(BZ37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE63*$DU$3)+1-$DU$3)","v":0.9262762093757777},{"$f":"(IF($AH$29<DEGREES(CA37),0+$AJ$33,1-((TAN(CA37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF63*$DU$3)+1-$DU$3)","v":1.0006828469329017},{"$f":"(IF($AH$29<DEGREES(CB37),0+$AJ$33,1-((TAN(CB37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG63*$DU$3)+1-$DU$3)","v":0.87723864422449216},{"$f":"(IF($AH$29<DEGREES(CC37),0+$AJ$33,1-((TAN(CC37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH63*$DU$3)+1-$DU$3)","v":0.75690072464350122},{"$f":"(IF($AH$29<DEGREES(CD37),0+$AJ$33,1-((TAN(CD37)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI63*$DU$3)+1-$DU$3)","v":0.69299238650281381},null,6,{"$f":"(IF($AH$12<DEGREES(CG37),0+$AJ$16,1-((TAN(CG37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH37),0+$AJ$16,1-((TAN(CH37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI37),0+$AJ$16,1-((TAN(CI37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ37),0+$AJ$16,1-((TAN(CJ37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK37),0+$AJ$16,1-((TAN(CK37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL37),0+$AJ$16,1-((TAN(CL37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM37),0+$AJ$16,1-((TAN(CM37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN37),0+$AJ$16,1-((TAN(CN37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO37),0+$AJ$16,1-((TAN(CO37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP37),0+$AJ$16,1-((TAN(CP37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ37),0+$AJ$16,1-((TAN(CQ37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV63*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR37),0+$AJ$16,1-((TAN(CR37)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW63*$DU$3)+1-$DU$3)","v":0},null,null,6,-12.151444093159176,-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719,null,6,-12.151444093159176,-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719]
[null,8,{"$f":"IF('Dry Bulb'!D12<60,(('Input Data'!$F$44*('Dry Bulb'!D12-$T$15))+('Heat gain from airflow'!Q11)+((Occupancy!P11*'Input Data'!$F$47)+(Occupancy!B11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D12-$P$15))+('Heat gain from airflow'!Q11)+((Occupancy!P11*'Input Data'!$F$47)+(Occupancy!B11*'Input Data'!$F$49))))/1000","v":-6.2097075000000024E-3},{"$f":"IF('Dry Bulb'!E12<60,(('Input Data'!$F$44*('Dry Bulb'!E12-$T$15))+('Heat gain from airflow'!R11)+((Occupancy!Q11*'Input Data'!$F$47)+(Occupancy!C11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E12-$P$15))+('Heat gain from airflow'!R11)+((Occupancy!Q11*'Input Data'!$F$47)+(Occupancy!C11*'Input Data'!$F$49))))/1000","v":-4.2067800000000011E-3},{"$f":"IF('Dry Bulb'!F12<60,(('Input Data'!$F$44*('Dry Bulb'!F12-$T$15))+('Heat gain from airflow'!S11)+((Occupancy!R11*'Input Data'!$F$47)+(Occupancy!D11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F12-$P$15))+('Heat gain from airflow'!S11)+((Occupancy!R11*'Input Data'!$F$47)+(Occupancy!D11*'Input Data'!$F$49))))/1000","v":-4.0054274999999997},{"$f":"IF('Dry Bulb'!G12<60,(('Input Data'!$F$44*('Dry Bulb'!G12-$T$15))+('Heat gain from airflow'!T11)+((Occupancy!S11*'Input Data'!$F$47)+(Occupancy!E11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G12-$P$15))+('Heat gain from airflow'!T11)+((Occupancy!S11*'Input Data'!$F$47)+(Occupancy!E11*'Input Data'!$F$49))))/1000","v":1.1486932200000042},{"$f":"IF('Dry Bulb'!H12<60,(('Input Data'!$F$44*('Dry Bulb'!H12-$T$15))+('Heat gain from airflow'!U11)+((Occupancy!T11*'Input Data'!$F$47)+(Occupancy!F11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H12-$P$15))+('Heat gain from airflow'!U11)+((Occupancy!T11*'Input Data'!$F$47)+(Occupancy!F11*'Input Data'!$F$49))))/1000","v":7.6306275000000054},{"$f":"IF('Dry Bulb'!I12<60,(('Input Data'!$F$44*('Dry Bulb'!I12-$T$15))+('Heat gain from airflow'!V11)+((Occupancy!U11*'Input Data'!$F$47)+(Occupancy!G11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I12-$P$15))+('Heat gain from airflow'!V11)+((Occupancy!U11*'Input Data'!$F$47)+(Occupancy!G11*'Input Data'!$F$49))))/1000","v":10.587330000000003},{"$f":"IF('Dry Bulb'!J12<60,(('Input Data'!$F$44*('Dry Bulb'!J12-$T$15))+('Heat gain from airflow'!W11)+((Occupancy!V11*'Input Data'!$F$47)+(Occupancy!H11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J12-$P$15))+('Heat gain from airflow'!W11)+((Occupancy!V11*'Input Data'!$F$47)+(Occupancy!H11*'Input Data'!$F$49))))/1000","v":11.445727500000006},{"$f":"IF('Dry Bulb'!K12<60,(('Input Data'!$F$44*('Dry Bulb'!K12-$T$15))+('Heat gain from airflow'!X11)+((Occupancy!W11*'Input Data'!$F$47)+(Occupancy!I11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K12-$P$15))+('Heat gain from airflow'!X11)+((Occupancy!W11*'Input Data'!$F$47)+(Occupancy!I11*'Input Data'!$F$49))))/1000","v":11.350350000000002},{"$f":"IF('Dry Bulb'!L12<60,(('Input Data'!$F$44*('Dry Bulb'!L12-$T$15))+('Heat gain from airflow'!Y11)+((Occupancy!X11*'Input Data'!$F$47)+(Occupancy!J11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L12-$P$15))+('Heat gain from airflow'!Y11)+((Occupancy!X11*'Input Data'!$F$47)+(Occupancy!J11*'Input Data'!$F$49))))/1000","v":8.584402500000003},{"$f":"IF('Dry Bulb'!M12<60,(('Input Data'!$F$44*('Dry Bulb'!M12-$T$15))+('Heat gain from airflow'!Z11)+((Occupancy!Y11*'Input Data'!$F$47)+(Occupancy!K11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M12-$P$15))+('Heat gain from airflow'!Z11)+((Occupancy!Y11*'Input Data'!$F$47)+(Occupancy!K11*'Input Data'!$F$49))))/1000","v":2.6734319549999968},{"$f":"IF('Dry Bulb'!N12<60,(('Input Data'!$F$44*('Dry Bulb'!N12-$T$15))+('Heat gain from airflow'!AA11)+((Occupancy!Z11*'Input Data'!$F$47)+(Occupancy!L11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N12-$P$15))+('Heat gain from airflow'!AA11)+((Occupancy!Z11*'Input Data'!$F$47)+(Occupancy!L11*'Input Data'!$F$49))))/1000","v":-3.3377850000000007},{"$f":"IF('Dry Bulb'!O12<60,(('Input Data'!$F$44*('Dry Bulb'!O12-$T$15))+('Heat gain from airflow'!AB11)+((Occupancy!AA11*'Input Data'!$F$47)+(Occupancy!M11*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O12-$P$15))+('Heat gain from airflow'!AB11)+((Occupancy!AA11*'Input Data'!$F$47)+(Occupancy!M11*'Input Data'!$F$49))))/1000","v":-5.3513100000000032E-3},null,"U-Value",0.45,false,null,"HDD",null,null,null,6,null,null,0,1,2,3,4,5,6,7,8,9,10,null,null,null,null,{"$f":"'Incident angle'!BI66","v":7},{"$f":"'Incident angle'!BJ66","v":0},{"$f":"'Incident angle'!BK66","v":0},{"$f":"'Incident angle'!BL66","v":0},{"$f":"'Incident angle'!BM66","v":0},{"$f":"'Incident angle'!BN66","v":0},{"$f":"'Incident angle'!BO66","v":0},{"$f":"'Incident angle'!BP66","v":0},{"$f":"'Incident angle'!BQ66","v":0},{"$f":"'Incident angle'!BR66","v":0},{"$f":"'Incident angle'!BS66","v":0},{"$f":"'Incident angle'!BT66","v":0},{"$f":"'Incident angle'!BU66","v":0},null,{"$f":"'Incident angle'!BW66","v":7},{"$f":"'Incident angle'!BX66","v":0},{"$f":"'Incident angle'!BY66","v":0},{"$f":"'Incident angle'!BZ66","v":0},{"$f":"'Incident angle'!CA66","v":0},{"$f":"'Incident angle'!CB66","v":0},{"$f":"'Incident angle'!CC66","v":0},{"$f":"'Incident angle'!CD66","v":0},{"$f":"'Incident angle'!CE66","v":0},{"$f":"'Incident angle'!CF66","v":0},{"$f":"'Incident angle'!CG66","v":0},{"$f":"'Incident angle'!CH66","v":0},{"$f":"'Incident angle'!CI66","v":0},null,{"$f":"'Profile angles'!P11","v":7},{"$f":"RADIANS('Profile angles'!Q11)","v":-1.3214305906891738E-2},{"$f":"RADIANS('Profile angles'!R11)","v":-7.6478952342661624E-2},{"$f":"RADIANS('Profile angles'!S11)","v":-0.18024728429187561},{"$f":"RADIANS('Profile angles'!T11)","v":-0.29926509663219786},{"$f":"RADIANS('Profile angles'!U11)","v":-0.36886077540021189},{"$f":"RADIANS('Profile angles'!V11)","v":-0.37484605769803392},{"$f":"RADIANS('Profile angles'!W11)","v":-0.33410836517870207},{"$f":"RADIANS('Profile angles'!X11)","v":-0.28700384937592222},{"$f":"RADIANS('Profile angles'!Y11)","v":-0.24026026153093516},{"$f":"RADIANS('Profile angles'!Z11)","v":-0.1938557876010461},{"$f":"RADIANS('Profile angles'!AA11)","v":-0.11359911050913243},{"$f":"RADIANS('Profile angles'!AB11)","v":-3.3555975837619691E-2},null,{"$f":"'Profile angles'!P40","v":7},{"$f":"RADIANS('Profile angles'!Q40)","v":-3.2126378124526914E-2},{"$f":"RADIANS('Profile angles'!R40)","v":-0.30400417987737716},{"$f":"RADIANS('Profile angles'!S40)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T40)","v":1.2672818655170024},{"$f":"RADIANS('Profile angles'!U40)","v":1.0116130508303161},{"$f":"RADIANS('Profile angles'!V40)","v":0.90537507022991526},{"$f":"RADIANS('Profile angles'!W40)","v":0.92689168179647397},{"$f":"RADIANS('Profile angles'!X40)","v":1.2258417459156572},{"$f":"RADIANS('Profile angles'!Y40)","v":-1.1397000015522976},{"$f":"RADIANS('Profile angles'!Z40)","v":-0.56767922585481523},{"$f":"RADIANS('Profile angles'!AA40)","v":-0.23892272571930678},{"$f":"RADIANS('Profile angles'!AB40)","v":-6.6151862638080941E-2},null,{"$f":"'Profile angles'!AR11","v":7},{"$f":"(IF($AH$29<DEGREES(BS38),0+$AJ$33,1-((TAN(BS38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX64*$DU$3)+1-$DU$3)","v":0.80174609954201725},{"$f":"(IF($AH$29<DEGREES(BT38),0+$AJ$33,1-((TAN(BT38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY64*$DU$3)+1-$DU$3)","v":0.92496396397417835},{"$f":"(IF($AH$29<DEGREES(BU38),0+$AJ$33,1-((TAN(BU38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ64*$DU$3)+1-$DU$3)","v":1.0803048768408492},{"$f":"(IF($AH$29<DEGREES(BV38),0+$AJ$33,1-((TAN(BV38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA64*$DU$3)+1-$DU$3)","v":1.1572226133814683},{"$f":"(IF($AH$29<DEGREES(BW38),0+$AJ$33,1-((TAN(BW38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB64*$DU$3)+1-$DU$3)","v":1.1169034899807895},{"$f":"(IF($AH$29<DEGREES(BX38),0+$AJ$33,1-((TAN(BX38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC64*$DU$3)+1-$DU$3)","v":1.0784967246030717},{"$f":"(IF($AH$29<DEGREES(BY38),0+$AJ$33,1-((TAN(BY38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD64*$DU$3)+1-$DU$3)","v":1.0810489536254193},{"$f":"(IF($AH$29<DEGREES(BZ38),0+$AJ$33,1-((TAN(BZ38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE64*$DU$3)+1-$DU$3)","v":1.1426237755432429},{"$f":"(IF($AH$29<DEGREES(CA38),0+$AJ$33,1-((TAN(CA38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF64*$DU$3)+1-$DU$3)","v":1.1054904428264722},{"$f":"(IF($AH$29<DEGREES(CB38),0+$AJ$33,1-((TAN(CB38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG64*$DU$3)+1-$DU$3)","v":0.96234179842923251},{"$f":"(IF($AH$29<DEGREES(CC38),0+$AJ$33,1-((TAN(CC38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH64*$DU$3)+1-$DU$3)","v":0.82695997509250441},{"$f":"(IF($AH$29<DEGREES(CD38),0+$AJ$33,1-((TAN(CD38)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI64*$DU$3)+1-$DU$3)","v":0.76419132619783015},null,7,{"$f":"(IF($AH$12<DEGREES(CG38),0+$AJ$16,1-((TAN(CG38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH38),0+$AJ$16,1-((TAN(CH38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI38),0+$AJ$16,1-((TAN(CI38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ38),0+$AJ$16,1-((TAN(CJ38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK38),0+$AJ$16,1-((TAN(CK38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL38),0+$AJ$16,1-((TAN(CL38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM38),0+$AJ$16,1-((TAN(CM38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN38),0+$AJ$16,1-((TAN(CN38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO38),0+$AJ$16,1-((TAN(CO38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP38),0+$AJ$16,1-((TAN(CP38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ38),0+$AJ$16,1-((TAN(CQ38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV64*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR38),0+$AJ$16,1-((TAN(CR38)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW64*$DU$3)+1-$DU$3)","v":1.3849778182162376E-2},null,null,7,0.70023973357815916,4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048,null,7,0.70023973357815916,4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048]
[null,9,{"$f":"IF('Dry Bulb'!D13<60,(('Input Data'!$F$44*('Dry Bulb'!D13-$T$15))+('Heat gain from airflow'!Q12)+((Occupancy!P12*'Input Data'!$F$47)+(Occupancy!B12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D13-$P$15))+('Heat gain from airflow'!Q12)+((Occupancy!P12*'Input Data'!$F$47)+(Occupancy!B12*'Input Data'!$F$49))))/1000","v":-4.779045E-3},{"$f":"IF('Dry Bulb'!E13<60,(('Input Data'!$F$44*('Dry Bulb'!E13-$T$15))+('Heat gain from airflow'!R12)+((Occupancy!Q12*'Input Data'!$F$47)+(Occupancy!C12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E13-$P$15))+('Heat gain from airflow'!R12)+((Occupancy!Q12*'Input Data'!$F$47)+(Occupancy!C12*'Input Data'!$F$49))))/1000","v":-2.6807399999999996E-3},{"$f":"IF('Dry Bulb'!F13<60,(('Input Data'!$F$44*('Dry Bulb'!F13-$T$15))+('Heat gain from airflow'!S12)+((Occupancy!R12*'Input Data'!$F$47)+(Occupancy!D12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F13-$P$15))+('Heat gain from airflow'!S12)+((Occupancy!R12*'Input Data'!$F$47)+(Occupancy!D12*'Input Data'!$F$49))))/1000","v":-2.860897500000001},{"$f":"IF('Dry Bulb'!G13<60,(('Input Data'!$F$44*('Dry Bulb'!G13-$T$15))+('Heat gain from airflow'!T12)+((Occupancy!S12*'Input Data'!$F$47)+(Occupancy!E12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G13-$P$15))+('Heat gain from airflow'!T12)+((Occupancy!S12*'Input Data'!$F$47)+(Occupancy!E12*'Input Data'!$F$49))))/1000","v":3.9635954999999994},{"$f":"IF('Dry Bulb'!H13<60,(('Input Data'!$F$44*('Dry Bulb'!H13-$T$15))+('Heat gain from airflow'!U12)+((Occupancy!T12*'Input Data'!$F$47)+(Occupancy!F12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H13-$P$15))+('Heat gain from airflow'!U12)+((Occupancy!T12*'Input Data'!$F$47)+(Occupancy!F12*'Input Data'!$F$49))))/1000","v":9.1566675000000028},{"$f":"IF('Dry Bulb'!I13<60,(('Input Data'!$F$44*('Dry Bulb'!I13-$T$15))+('Heat gain from airflow'!V12)+((Occupancy!U12*'Input Data'!$F$47)+(Occupancy!G12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I13-$P$15))+('Heat gain from airflow'!V12)+((Occupancy!U12*'Input Data'!$F$47)+(Occupancy!G12*'Input Data'!$F$49))))/1000","v":12.399502500000004},{"$f":"IF('Dry Bulb'!J13<60,(('Input Data'!$F$44*('Dry Bulb'!J13-$T$15))+('Heat gain from airflow'!W12)+((Occupancy!V12*'Input Data'!$F$47)+(Occupancy!H12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J13-$P$15))+('Heat gain from airflow'!W12)+((Occupancy!V12*'Input Data'!$F$47)+(Occupancy!H12*'Input Data'!$F$49))))/1000","v":13.734787500000003},{"$f":"IF('Dry Bulb'!K13<60,(('Input Data'!$F$44*('Dry Bulb'!K13-$T$15))+('Heat gain from airflow'!X12)+((Occupancy!W12*'Input Data'!$F$47)+(Occupancy!I12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K13-$P$15))+('Heat gain from airflow'!X12)+((Occupancy!W12*'Input Data'!$F$47)+(Occupancy!I12*'Input Data'!$F$49))))/1000","v":13.830165000000006},{"$f":"IF('Dry Bulb'!L13<60,(('Input Data'!$F$44*('Dry Bulb'!L13-$T$15))+('Heat gain from airflow'!Y12)+((Occupancy!X12*'Input Data'!$F$47)+(Occupancy!J12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L13-$P$15))+('Heat gain from airflow'!Y12)+((Occupancy!X12*'Input Data'!$F$47)+(Occupancy!J12*'Input Data'!$F$49))))/1000","v":10.778084999999995},{"$f":"IF('Dry Bulb'!M13<60,(('Input Data'!$F$44*('Dry Bulb'!M13-$T$15))+('Heat gain from airflow'!Z12)+((Occupancy!Y12*'Input Data'!$F$47)+(Occupancy!K12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M13-$P$15))+('Heat gain from airflow'!Z12)+((Occupancy!Y12*'Input Data'!$F$47)+(Occupancy!K12*'Input Data'!$F$49))))/1000","v":5.3710466399999977},{"$f":"IF('Dry Bulb'!N13<60,(('Input Data'!$F$44*('Dry Bulb'!N13-$T$15))+('Heat gain from airflow'!AA12)+((Occupancy!Z12*'Input Data'!$F$47)+(Occupancy!L12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N13-$P$15))+('Heat gain from airflow'!AA12)+((Occupancy!Z12*'Input Data'!$F$47)+(Occupancy!L12*'Input Data'!$F$49))))/1000","v":-1.5489214649999958},{"$f":"IF('Dry Bulb'!O13<60,(('Input Data'!$F$44*('Dry Bulb'!O13-$T$15))+('Heat gain from airflow'!AB12)+((Occupancy!AA12*'Input Data'!$F$47)+(Occupancy!M12*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O13-$P$15))+('Heat gain from airflow'!AB12)+((Occupancy!AA12*'Input Data'!$F$47)+(Occupancy!M12*'Input Data'!$F$49))))/1000","v":-3.8252700000000017E-3},null,"WWR",{"$f":"(Q40/20)*R39","v":0.5},{"$f":"IF(R38,0,1)","v":1},null,{"$f":"SUM(C166:N189)*-1","v":534.54469642925596},null,null,null,{"$f":"X38*AC44","v":6},"HEAD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI67","v":8},{"$f":"'Incident angle'!BJ67","v":0},{"$f":"'Incident angle'!BK67","v":0},{"$f":"'Incident angle'!BL67","v":0},{"$f":"'Incident angle'!BM67","v":0},{"$f":"'Incident angle'!BN67","v":0},{"$f":"'Incident angle'!BO67","v":0},{"$f":"'Incident angle'!BP67","v":0},{"$f":"'Incident angle'!BQ67","v":0},{"$f":"'Incident angle'!BR67","v":0},{"$f":"'Incident angle'!BS67","v":0},{"$f":"'Incident angle'!BT67","v":0},{"$f":"'Incident angle'!BU67","v":0},null,{"$f":"'Incident angle'!BW67","v":8},{"$f":"'Incident angle'!BX67","v":0},{"$f":"'Incident angle'!BY67","v":0},{"$f":"'Incident angle'!BZ67","v":0},{"$f":"'Incident angle'!CA67","v":0},{"$f":"'Incident angle'!CB67","v":0},{"$f":"'Incident angle'!CC67","v":0},{"$f":"'Incident angle'!CD67","v":0},{"$f":"'Incident angle'!CE67","v":0},{"$f":"'Incident angle'!CF67","v":0},{"$f":"'Incident angle'!CG67","v":0},{"$f":"'Incident angle'!CH67","v":0},{"$f":"'Incident angle'!CI67","v":0},null,{"$f":"'Profile angles'!P12","v":8},{"$f":"RADIANS('Profile angles'!Q12)","v":-0.25833513602163805},{"$f":"RADIANS('Profile angles'!R12)","v":-0.32105613157454954},{"$f":"RADIANS('Profile angles'!S12)","v":-0.42271676310413814},{"$f":"RADIANS('Profile angles'!T12)","v":-0.53547976766771499},{"$f":"RADIANS('Profile angles'!U12)","v":-0.59803922283315158},{"$f":"RADIANS('Profile angles'!V12)","v":-0.600853618256177},{"$f":"RADIANS('Profile angles'!W12)","v":-0.5629740216332968},{"$f":"RADIANS('Profile angles'!X12)","v":-0.52288181283223811},{"$f":"RADIANS('Profile angles'!Y12)","v":-0.484596524210885},{"$f":"RADIANS('Profile angles'!Z12)","v":-0.4442621994100388},{"$f":"RADIANS('Profile angles'!AA12)","v":-0.36546054525287114},{"$f":"RADIANS('Profile angles'!AB12)","v":-0.28151379860305881},null,{"$f":"'Profile angles'!P41","v":8},{"$f":"RADIANS('Profile angles'!Q41)","v":-0.43903721208086549},{"$f":"RADIANS('Profile angles'!R41)","v":-0.71921811629902943},{"$f":"RADIANS('Profile angles'!S41)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!T41)","v":-1.5556802149681459},{"$f":"RADIANS('Profile angles'!U41)","v":1.3507534128601013},{"$f":"RADIANS('Profile angles'!V41)","v":1.253806072902226},{"$f":"RADIANS('Profile angles'!W41)","v":1.3073051411080618},{"$f":"RADIANS('Profile angles'!X41)","v":1.5687141806333271},{"$f":"RADIANS('Profile angles'!Y41)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!Z41)","v":-0.7977743448011565},{"$f":"RADIANS('Profile angles'!AA41)","v":-0.53602537178498588},{"$f":"RADIANS('Profile angles'!AB41)","v":-0.40375311848675605},null,{"$f":"'Profile angles'!AR12","v":8},{"$f":"(IF($AH$29<DEGREES(BS39),0+$AJ$33,1-((TAN(BS39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX65*$DU$3)+1-$DU$3)","v":0.85158593472496513},{"$f":"(IF($AH$29<DEGREES(BT39),0+$AJ$33,1-((TAN(BT39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY65*$DU$3)+1-$DU$3)","v":0.99870238130990363},{"$f":"(IF($AH$29<DEGREES(BU39),0+$AJ$33,1-((TAN(BU39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ65*$DU$3)+1-$DU$3)","v":1.1788590753970067},{"$f":"(IF($AH$29<DEGREES(BV39),0+$AJ$33,1-((TAN(BV39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA65*$DU$3)+1-$DU$3)","v":1.4089641999485556},{"$f":"(IF($AH$29<DEGREES(BW39),0+$AJ$33,1-((TAN(BW39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB65*$DU$3)+1-$DU$3)","v":1.3643640763159175},{"$f":"(IF($AH$29<DEGREES(BX39),0+$AJ$33,1-((TAN(BX39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC65*$DU$3)+1-$DU$3)","v":1.3134143178177133},{"$f":"(IF($AH$29<DEGREES(BY39),0+$AJ$33,1-((TAN(BY39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD65*$DU$3)+1-$DU$3)","v":1.3190411857373288},{"$f":"(IF($AH$29<DEGREES(BZ39),0+$AJ$33,1-((TAN(BZ39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE65*$DU$3)+1-$DU$3)","v":1.4026341160824194},{"$f":"(IF($AH$29<DEGREES(CA39),0+$AJ$33,1-((TAN(CA39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF65*$DU$3)+1-$DU$3)","v":1.2028341087718406},{"$f":"(IF($AH$29<DEGREES(CB39),0+$AJ$33,1-((TAN(CB39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG65*$DU$3)+1-$DU$3)","v":1.0236569813481902},{"$f":"(IF($AH$29<DEGREES(CC39),0+$AJ$33,1-((TAN(CC39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH65*$DU$3)+1-$DU$3)","v":0.85951132518730122},{"$f":"(IF($AH$29<DEGREES(CD39),0+$AJ$33,1-((TAN(CD39)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI65*$DU$3)+1-$DU$3)","v":0.79546310580240509},null,8,{"$f":"(IF($AH$12<DEGREES(CG39),0+$AJ$16,1-((TAN(CG39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL65*$DU$3)+1-$DU$3)","v":0.14802435420908988},{"$f":"(IF($AH$12<DEGREES(CH39),0+$AJ$16,1-((TAN(CH39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM65*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI39),0+$AJ$16,1-((TAN(CI39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN65*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ39),0+$AJ$16,1-((TAN(CJ39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO65*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK39),0+$AJ$16,1-((TAN(CK39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP65*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL39),0+$AJ$16,1-((TAN(CL39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ65*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM39),0+$AJ$16,1-((TAN(CM39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR65*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN39),0+$AJ$16,1-((TAN(CN39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS65*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO39),0+$AJ$16,1-((TAN(CO39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT65*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP39),0+$AJ$16,1-((TAN(CP39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU65*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ39),0+$AJ$16,1-((TAN(CQ39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV65*$DU$3)+1-$DU$3)","v":0.31683656048123038},{"$f":"(IF($AH$12<DEGREES(CR39),0+$AJ$16,1-((TAN(CR39)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW65*$DU$3)+1-$DU$3)","v":0.33951312390264221},null,null,8,12.968359542715392,17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182,null,8,12.968359542715392,17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182]
[null,10,{"$f":"IF('Dry Bulb'!D14<60,(('Input Data'!$F$44*('Dry Bulb'!D14-$T$15))+('Heat gain from airflow'!Q13)+((Occupancy!P13*'Input Data'!$F$47)+(Occupancy!B13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D14-$P$15))+('Heat gain from airflow'!Q13)+((Occupancy!P13*'Input Data'!$F$47)+(Occupancy!B13*'Input Data'!$F$49))))/1000","v":-3.2530049999999981E-3},{"$f":"IF('Dry Bulb'!E14<60,(('Input Data'!$F$44*('Dry Bulb'!E14-$T$15))+('Heat gain from airflow'!R13)+((Occupancy!Q13*'Input Data'!$F$47)+(Occupancy!C13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E14-$P$15))+('Heat gain from airflow'!R13)+((Occupancy!Q13*'Input Data'!$F$47)+(Occupancy!C13*'Input Data'!$F$49))))/1000","v":-4.7684474999999988},{"$f":"IF('Dry Bulb'!F14<60,(('Input Data'!$F$44*('Dry Bulb'!F14-$T$15))+('Heat gain from airflow'!S13)+((Occupancy!R13*'Input Data'!$F$47)+(Occupancy!D13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F14-$P$15))+('Heat gain from airflow'!S13)+((Occupancy!R13*'Input Data'!$F$47)+(Occupancy!D13*'Input Data'!$F$49))))/1000","v":-2.2526470350000043},{"$f":"IF('Dry Bulb'!G14<60,(('Input Data'!$F$44*('Dry Bulb'!G14-$T$15))+('Heat gain from airflow'!T13)+((Occupancy!S13*'Input Data'!$F$47)+(Occupancy!E13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G14-$P$15))+('Heat gain from airflow'!T13)+((Occupancy!S13*'Input Data'!$F$47)+(Occupancy!E13*'Input Data'!$F$49))))/1000","v":5.5323225000000003},{"$f":"IF('Dry Bulb'!H14<60,(('Input Data'!$F$44*('Dry Bulb'!H14-$T$15))+('Heat gain from airflow'!U13)+((Occupancy!T13*'Input Data'!$F$47)+(Occupancy!F13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H14-$P$15))+('Heat gain from airflow'!U13)+((Occupancy!T13*'Input Data'!$F$47)+(Occupancy!F13*'Input Data'!$F$49))))/1000","v":10.778084999999995},{"$f":"IF('Dry Bulb'!I14<60,(('Input Data'!$F$44*('Dry Bulb'!I14-$T$15))+('Heat gain from airflow'!V13)+((Occupancy!U13*'Input Data'!$F$47)+(Occupancy!G13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I14-$P$15))+('Heat gain from airflow'!V13)+((Occupancy!U13*'Input Data'!$F$47)+(Occupancy!G13*'Input Data'!$F$49))))/1000","v":14.020919999999998},{"$f":"IF('Dry Bulb'!J14<60,(('Input Data'!$F$44*('Dry Bulb'!J14-$T$15))+('Heat gain from airflow'!W13)+((Occupancy!V13*'Input Data'!$F$47)+(Occupancy!H13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J14-$P$15))+('Heat gain from airflow'!W13)+((Occupancy!V13*'Input Data'!$F$47)+(Occupancy!H13*'Input Data'!$F$49))))/1000","v":15.737715000000003},{"$f":"IF('Dry Bulb'!K14<60,(('Input Data'!$F$44*('Dry Bulb'!K14-$T$15))+('Heat gain from airflow'!X13)+((Occupancy!W13*'Input Data'!$F$47)+(Occupancy!I13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K14-$P$15))+('Heat gain from airflow'!X13)+((Occupancy!W13*'Input Data'!$F$47)+(Occupancy!I13*'Input Data'!$F$49))))/1000","v":16.023847499999999},{"$f":"IF('Dry Bulb'!L14<60,(('Input Data'!$F$44*('Dry Bulb'!L14-$T$15))+('Heat gain from airflow'!Y13)+((Occupancy!X13*'Input Data'!$F$47)+(Occupancy!J13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L14-$P$15))+('Heat gain from airflow'!Y13)+((Occupancy!X13*'Input Data'!$F$47)+(Occupancy!J13*'Input Data'!$F$49))))/1000","v":12.685634999999992},{"$f":"IF('Dry Bulb'!M14<60,(('Input Data'!$F$44*('Dry Bulb'!M14-$T$15))+('Heat gain from airflow'!Z13)+((Occupancy!Y13*'Input Data'!$F$47)+(Occupancy!K13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M14-$P$15))+('Heat gain from airflow'!Z13)+((Occupancy!Y13*'Input Data'!$F$47)+(Occupancy!K13*'Input Data'!$F$49))))/1000","v":6.8676074999999983},{"$f":"IF('Dry Bulb'!N14<60,(('Input Data'!$F$44*('Dry Bulb'!N14-$T$15))+('Heat gain from airflow'!AA13)+((Occupancy!Z13*'Input Data'!$F$47)+(Occupancy!L13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N14-$P$15))+('Heat gain from airflow'!AA13)+((Occupancy!Z13*'Input Data'!$F$47)+(Occupancy!L13*'Input Data'!$F$49))))/1000","v":1.0314056249999997},{"$f":"IF('Dry Bulb'!O14<60,(('Input Data'!$F$44*('Dry Bulb'!O14-$T$15))+('Heat gain from airflow'!AB13)+((Occupancy!AA13*'Input Data'!$F$47)+(Occupancy!M13*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O14-$P$15))+('Heat gain from airflow'!AB13)+((Occupancy!AA13*'Input Data'!$F$47)+(Occupancy!M13*'Input Data'!$F$49))))/1000","v":-2.2038524999999998E-3},null,null,10,null,null,null,null,null,10,null,null,null,null,null,"OVERHANG",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI68","v":9},{"$f":"'Incident angle'!BJ68","v":0},{"$f":"'Incident angle'!BK68","v":0},{"$f":"'Incident angle'!BL68","v":0},{"$f":"'Incident angle'!BM68","v":0},{"$f":"'Incident angle'!BN68","v":0},{"$f":"'Incident angle'!BO68","v":0},{"$f":"'Incident angle'!BP68","v":0},{"$f":"'Incident angle'!BQ68","v":0},{"$f":"'Incident angle'!BR68","v":0},{"$f":"'Incident angle'!BS68","v":0},{"$f":"'Incident angle'!BT68","v":0},{"$f":"'Incident angle'!BU68","v":0},null,{"$f":"'Incident angle'!BW68","v":9},{"$f":"'Incident angle'!BX68","v":0},{"$f":"'Incident angle'!BY68","v":0},{"$f":"'Incident angle'!BZ68","v":0},{"$f":"'Incident angle'!CA68","v":0},{"$f":"'Incident angle'!CB68","v":0},{"$f":"'Incident angle'!CC68","v":0},{"$f":"'Incident angle'!CD68","v":0},{"$f":"'Incident angle'!CE68","v":0},{"$f":"'Incident angle'!CF68","v":0},{"$f":"'Incident angle'!CG68","v":0},{"$f":"'Incident angle'!CH68","v":0},{"$f":"'Incident angle'!CI68","v":0},null,{"$f":"'Profile angles'!P13","v":9},{"$f":"RADIANS('Profile angles'!Q13)","v":-0.52181610509407761},{"$f":"RADIANS('Profile angles'!R13)","v":-0.57895326435114869},{"$f":"RADIANS('Profile angles'!S13)","v":-0.6743232952298458},{"$f":"RADIANS('Profile angles'!T13)","v":-0.77696351285009768},{"$f":"RADIANS('Profile angles'!U13)","v":-0.83009780925872156},{"$f":"RADIANS('Profile angles'!V13)","v":-0.82868950102189065},{"$f":"RADIANS('Profile angles'!W13)","v":-0.79414344815942139},{"$f":"RADIANS('Profile angles'!X13)","v":-0.76376137451897885},{"$f":"RADIANS('Profile angles'!Y13)","v":-0.73908870770470358},{"$f":"RADIANS('Profile angles'!Z13)","v":-0.71062378761726053},{"$f":"RADIANS('Profile angles'!AA13)","v":-0.63870702042109351},{"$f":"RADIANS('Profile angles'!AB13)","v":-0.55159011300440908},null,{"$f":"'Profile angles'!P42","v":9},{"$f":"RADIANS('Profile angles'!Q42)","v":-0.63047626333736551},{"$f":"RADIANS('Profile angles'!R42)","v":-0.85493388322458175},{"$f":"RADIANS('Profile angles'!S42)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T42)","v":-1.4368234130045159},{"$f":"RADIANS('Profile angles'!U42)","v":1.5128901286207534},{"$f":"RADIANS('Profile angles'!V42)","v":1.4342637641927438},{"$f":"RADIANS('Profile angles'!W42)","v":1.4895751772040409},{"$f":"RADIANS('Profile angles'!X42)","v":-1.4463354753784505},{"$f":"RADIANS('Profile angles'!Y42)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!Z42)","v":-0.88713181190644863},{"$f":"RADIANS('Profile angles'!AA42)","v":-0.67791492684215893},{"$f":"RADIANS('Profile angles'!AB42)","v":-0.57836247588490319},null,{"$f":"'Profile angles'!AR13","v":9},{"$f":"(IF($AH$29<DEGREES(BS40),0+$AJ$33,1-((TAN(BS40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX66*$DU$3)+1-$DU$3)","v":0.85004078773368386},{"$f":"(IF($AH$29<DEGREES(BT40),0+$AJ$33,1-((TAN(BT40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY66*$DU$3)+1-$DU$3)","v":1.0432216536392793},{"$f":"(IF($AH$29<DEGREES(BU40),0+$AJ$33,1-((TAN(BU40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ66*$DU$3)+1-$DU$3)","v":1.2728465214314721},{"$f":"(IF($AH$29<DEGREES(BV40),0+$AJ$33,1-((TAN(BV40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA66*$DU$3)+1-$DU$3)","v":1.576419181794209},{"$f":"(IF($AH$29<DEGREES(BW40),0+$AJ$33,1-((TAN(BW40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB66*$DU$3)+1-$DU$3)","v":1.7095854656912284},{"$f":"(IF($AH$29<DEGREES(BX40),0+$AJ$33,1-((TAN(BX40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC66*$DU$3)+1-$DU$3)","v":1.6312881226253513},{"$f":"(IF($AH$29<DEGREES(BY40),0+$AJ$33,1-((TAN(BY40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD66*$DU$3)+1-$DU$3)","v":1.6414290710591997},{"$f":"(IF($AH$29<DEGREES(BZ40),0+$AJ$33,1-((TAN(BZ40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE66*$DU$3)+1-$DU$3)","v":1.5702855282357961},{"$f":"(IF($AH$29<DEGREES(CA40),0+$AJ$33,1-((TAN(CA40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF66*$DU$3)+1-$DU$3)","v":1.2946652212747105},{"$f":"(IF($AH$29<DEGREES(CB40),0+$AJ$33,1-((TAN(CB40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG66*$DU$3)+1-$DU$3)","v":1.0406364509573172},{"$f":"(IF($AH$29<DEGREES(CC40),0+$AJ$33,1-((TAN(CC40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH66*$DU$3)+1-$DU$3)","v":0.81904138140917238},{"$f":"(IF($AH$29<DEGREES(CD40),0+$AJ$33,1-((TAN(CD40)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI66*$DU$3)+1-$DU$3)","v":0.75648349078064991},null,9,{"$f":"(IF($AH$12<DEGREES(CG40),0+$AJ$16,1-((TAN(CG40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL66*$DU$3)+1-$DU$3)","v":0.55196776489931276},{"$f":"(IF($AH$12<DEGREES(CH40),0+$AJ$16,1-((TAN(CH40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM66*$DU$3)+1-$DU$3)","v":0.21760010477413194},{"$f":"(IF($AH$12<DEGREES(CI40),0+$AJ$16,1-((TAN(CI40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN66*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ40),0+$AJ$16,1-((TAN(CJ40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO66*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK40),0+$AJ$16,1-((TAN(CK40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP66*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL40),0+$AJ$16,1-((TAN(CL40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ66*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM40),0+$AJ$16,1-((TAN(CM40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR66*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN40),0+$AJ$16,1-((TAN(CN40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS66*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO40),0+$AJ$16,1-((TAN(CO40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT66*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP40),0+$AJ$16,1-((TAN(CP40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU66*$DU$3)+1-$DU$3)","v":0.53342005101234624},{"$f":"(IF($AH$12<DEGREES(CQ40),0+$AJ$16,1-((TAN(CQ40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV66*$DU$3)+1-$DU$3)","v":0.71582714323580776},{"$f":"(IF($AH$12<DEGREES(CR40),0+$AJ$16,1-((TAN(CR40)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW66*$DU$3)+1-$DU$3)","v":0.68404998224608837},null,null,9,24.306538235547787,29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159,null,9,24.306538235547787,29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159]
[null,11,{"$f":"IF('Dry Bulb'!D15<60,(('Input Data'!$F$44*('Dry Bulb'!D15-$T$15))+('Heat gain from airflow'!Q14)+((Occupancy!P14*'Input Data'!$F$47)+(Occupancy!B14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D15-$P$15))+('Heat gain from airflow'!Q14)+((Occupancy!P14*'Input Data'!$F$47)+(Occupancy!B14*'Input Data'!$F$49))))/1000","v":-1.9177200000000004E-3},{"$f":"IF('Dry Bulb'!E15<60,(('Input Data'!$F$44*('Dry Bulb'!E15-$T$15))+('Heat gain from airflow'!R14)+((Occupancy!Q14*'Input Data'!$F$47)+(Occupancy!C14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E15-$P$15))+('Heat gain from airflow'!R14)+((Occupancy!Q14*'Input Data'!$F$47)+(Occupancy!C14*'Input Data'!$F$49))))/1000","v":-2.9562749999999971},{"$f":"IF('Dry Bulb'!F15<60,(('Input Data'!$F$44*('Dry Bulb'!F15-$T$15))+('Heat gain from airflow'!S14)+((Occupancy!R14*'Input Data'!$F$47)+(Occupancy!D14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F15-$P$15))+('Heat gain from airflow'!S14)+((Occupancy!R14*'Input Data'!$F$47)+(Occupancy!D14*'Input Data'!$F$49))))/1000","v":-0.61062070499999799},{"$f":"IF('Dry Bulb'!G15<60,(('Input Data'!$F$44*('Dry Bulb'!G15-$T$15))+('Heat gain from airflow'!T14)+((Occupancy!S14*'Input Data'!$F$47)+(Occupancy!E14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G15-$P$15))+('Heat gain from airflow'!T14)+((Occupancy!S14*'Input Data'!$F$47)+(Occupancy!E14*'Input Data'!$F$49))))/1000","v":7.0583624999999985},{"$f":"IF('Dry Bulb'!H15<60,(('Input Data'!$F$44*('Dry Bulb'!H15-$T$15))+('Heat gain from airflow'!U14)+((Occupancy!T14*'Input Data'!$F$47)+(Occupancy!F14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H15-$P$15))+('Heat gain from airflow'!U14)+((Occupancy!T14*'Input Data'!$F$47)+(Occupancy!F14*'Input Data'!$F$49))))/1000","v":12.113370000000002},{"$f":"IF('Dry Bulb'!I15<60,(('Input Data'!$F$44*('Dry Bulb'!I15-$T$15))+('Heat gain from airflow'!V14)+((Occupancy!U14*'Input Data'!$F$47)+(Occupancy!G14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I15-$P$15))+('Heat gain from airflow'!V14)+((Occupancy!U14*'Input Data'!$F$47)+(Occupancy!G14*'Input Data'!$F$49))))/1000","v":15.451582500000001},{"$f":"IF('Dry Bulb'!J15<60,(('Input Data'!$F$44*('Dry Bulb'!J15-$T$15))+('Heat gain from airflow'!W14)+((Occupancy!V14*'Input Data'!$F$47)+(Occupancy!H14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J15-$P$15))+('Heat gain from airflow'!W14)+((Occupancy!V14*'Input Data'!$F$47)+(Occupancy!H14*'Input Data'!$F$49))))/1000","v":17.263755},{"$f":"IF('Dry Bulb'!K15<60,(('Input Data'!$F$44*('Dry Bulb'!K15-$T$15))+('Heat gain from airflow'!X14)+((Occupancy!W14*'Input Data'!$F$47)+(Occupancy!I14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K15-$P$15))+('Heat gain from airflow'!X14)+((Occupancy!W14*'Input Data'!$F$47)+(Occupancy!I14*'Input Data'!$F$49))))/1000","v":17.836020000000001},{"$f":"IF('Dry Bulb'!L15<60,(('Input Data'!$F$44*('Dry Bulb'!L15-$T$15))+('Heat gain from airflow'!Y14)+((Occupancy!X14*'Input Data'!$F$47)+(Occupancy!J14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L15-$P$15))+('Heat gain from airflow'!Y14)+((Occupancy!X14*'Input Data'!$F$47)+(Occupancy!J14*'Input Data'!$F$49))))/1000","v":14.020919999999998},{"$f":"IF('Dry Bulb'!M15<60,(('Input Data'!$F$44*('Dry Bulb'!M15-$T$15))+('Heat gain from airflow'!Z14)+((Occupancy!Y14*'Input Data'!$F$47)+(Occupancy!K14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M15-$P$15))+('Heat gain from airflow'!Z14)+((Occupancy!Y14*'Input Data'!$F$47)+(Occupancy!K14*'Input Data'!$F$49))))/1000","v":8.4890249999999998},{"$f":"IF('Dry Bulb'!N15<60,(('Input Data'!$F$44*('Dry Bulb'!N15-$T$15))+('Heat gain from airflow'!AA14)+((Occupancy!Z14*'Input Data'!$F$47)+(Occupancy!L14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N15-$P$15))+('Heat gain from airflow'!AA14)+((Occupancy!Z14*'Input Data'!$F$47)+(Occupancy!L14*'Input Data'!$F$49))))/1000","v":3.3771575249999959},{"$f":"IF('Dry Bulb'!O15<60,(('Input Data'!$F$44*('Dry Bulb'!O15-$T$15))+('Heat gain from airflow'!AB14)+((Occupancy!AA14*'Input Data'!$F$47)+(Occupancy!M14*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O15-$P$15))+('Heat gain from airflow'!AB14)+((Occupancy!AA14*'Input Data'!$F$47)+(Occupancy!M14*'Input Data'!$F$49))))/1000","v":-4.2915599999999987},null,null,null,null,null,"CDD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI69","v":10},{"$f":"'Incident angle'!BJ69","v":0},{"$f":"'Incident angle'!BK69","v":0},{"$f":"'Incident angle'!BL69","v":0},{"$f":"'Incident angle'!BM69","v":0},{"$f":"'Incident angle'!BN69","v":0},{"$f":"'Incident angle'!BO69","v":0},{"$f":"'Incident angle'!BP69","v":0},{"$f":"'Incident angle'!BQ69","v":0},{"$f":"'Incident angle'!BR69","v":0},{"$f":"'Incident angle'!BS69","v":0},{"$f":"'Incident angle'!BT69","v":0},{"$f":"'Incident angle'!BU69","v":0},null,{"$f":"'Incident angle'!BW69","v":10},{"$f":"'Incident angle'!BX69","v":0},{"$f":"'Incident angle'!BY69","v":0},{"$f":"'Incident angle'!BZ69","v":0},{"$f":"'Incident angle'!CA69","v":0},{"$f":"'Incident angle'!CB69","v":0},{"$f":"'Incident angle'!CC69","v":0},{"$f":"'Incident angle'!CD69","v":0},{"$f":"'Incident angle'!CE69","v":0},{"$f":"'Incident angle'!CF69","v":0},{"$f":"'Incident angle'!CG69","v":0},{"$f":"'Incident angle'!CH69","v":0},{"$f":"'Incident angle'!CI69","v":0},null,{"$f":"'Profile angles'!P14","v":10},{"$f":"RADIANS('Profile angles'!Q14)","v":-0.8103914470438931},{"$f":"RADIANS('Profile angles'!R14)","v":-0.85489906581681829},{"$f":"RADIANS('Profile angles'!S14)","v":-0.93831409714073843},{"$f":"RADIANS('Profile angles'!T14)","v":-1.0260828135826865},{"$f":"RADIANS('Profile angles'!U14)","v":-1.0672108131256053},{"$f":"RADIANS('Profile angles'!V14)","v":-1.0606626288594174},{"$f":"RADIANS('Profile angles'!W14)","v":-1.0301037196118754},{"$f":"RADIANS('Profile angles'!X14)","v":-1.0121306417701839},{"$f":"RADIANS('Profile angles'!Y14)","v":-1.0063600686241212},{"$f":"RADIANS('Profile angles'!Z14)","v":-0.99633099553482729},{"$f":"RADIANS('Profile angles'!AA14)","v":-0.93894687408658406},{"$f":"RADIANS('Profile angles'!AB14)","v":-0.85128249562502767},null,{"$f":"'Profile angles'!P43","v":10},{"$f":"RADIANS('Profile angles'!Q43)","v":-0.7254554153443552},{"$f":"RADIANS('Profile angles'!R43)","v":-0.9144032921168761},{"$f":"RADIANS('Profile angles'!S43)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T43)","v":-1.3820186383289426},{"$f":"RADIANS('Profile angles'!U43)","v":-1.5469473133771072},{"$f":"RADIANS('Profile angles'!V43)","v":1.52849748779825},{"$f":"RADIANS('Profile angles'!W43)","v":-1.5604768548046379},{"$f":"RADIANS('Profile angles'!X43)","v":-1.388309158935473},{"$f":"RADIANS('Profile angles'!Y43)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!Z43)","v":-0.92900496630503882},{"$f":"RADIANS('Profile angles'!AA43)","v":-0.74952134450991281},{"$f":"RADIANS('Profile angles'!AB43)","v":-0.66958505956359182},null,{"$f":"'Profile angles'!AR14","v":10},{"$f":"(IF($AH$29<DEGREES(BS41),0+$AJ$33,1-((TAN(BS41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX67*$DU$3)+1-$DU$3)","v":0.70692636835689493},{"$f":"(IF($AH$29<DEGREES(BT41),0+$AJ$33,1-((TAN(BT41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY67*$DU$3)+1-$DU$3)","v":1.005590783408586},{"$f":"(IF($AH$29<DEGREES(BU41),0+$AJ$33,1-((TAN(BU41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ67*$DU$3)+1-$DU$3)","v":1.3416209454520391},{"$f":"(IF($AH$29<DEGREES(BV41),0+$AJ$33,1-((TAN(BV41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA67*$DU$3)+1-$DU$3)","v":1.8155472501496919},{"$f":"(IF($AH$29<DEGREES(BW41),0+$AJ$33,1-((TAN(BW41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB67*$DU$3)+1-$DU$3)","v":2.2213436717963337},{"$f":"(IF($AH$29<DEGREES(BX41),0+$AJ$33,1-((TAN(BX41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC67*$DU$3)+1-$DU$3)","v":2.1659042807720508},{"$f":"(IF($AH$29<DEGREES(BY41),0+$AJ$33,1-((TAN(BY41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD67*$DU$3)+1-$DU$3)","v":2.1473294714591247},{"$f":"(IF($AH$29<DEGREES(BZ41),0+$AJ$33,1-((TAN(BZ41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE67*$DU$3)+1-$DU$3)","v":1.8069250308978473},{"$f":"(IF($AH$29<DEGREES(CA41),0+$AJ$33,1-((TAN(CA41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF67*$DU$3)+1-$DU$3)","v":1.3407877656520557},{"$f":"(IF($AH$29<DEGREES(CB41),0+$AJ$33,1-((TAN(CB41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG67*$DU$3)+1-$DU$3)","v":0.87986404047025146},{"$f":"(IF($AH$29<DEGREES(CC41),0+$AJ$33,1-((TAN(CC41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH67*$DU$3)+1-$DU$3)","v":0.52045201376974937},{"$f":"(IF($AH$29<DEGREES(CD41),0+$AJ$33,1-((TAN(CD41)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI67*$DU$3)+1-$DU$3)","v":0.5020917366999228},null,10,{"$f":"(IF($AH$12<DEGREES(CG41),0+$AJ$16,1-((TAN(CG41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL67*$DU$3)+1-$DU$3)","v":0.93718110793897635},{"$f":"(IF($AH$12<DEGREES(CH41),0+$AJ$16,1-((TAN(CH41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM67*$DU$3)+1-$DU$3)","v":0.83108539975370022},{"$f":"(IF($AH$12<DEGREES(CI41),0+$AJ$16,1-((TAN(CI41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN67*$DU$3)+1-$DU$3)","v":0.5125908573762884},{"$f":"(IF($AH$12<DEGREES(CJ41),0+$AJ$16,1-((TAN(CJ41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO67*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK41),0+$AJ$16,1-((TAN(CK41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP67*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL41),0+$AJ$16,1-((TAN(CL41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ67*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM41),0+$AJ$16,1-((TAN(CM41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR67*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN41),0+$AJ$16,1-((TAN(CN41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS67*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO41),0+$AJ$16,1-((TAN(CO41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT67*$DU$3)+1-$DU$3)","v":0.78612965191524864},{"$f":"(IF($AH$12<DEGREES(CP41),0+$AJ$16,1-((TAN(CP41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU67*$DU$3)+1-$DU$3)","v":1.0979635045495388},{"$f":"(IF($AH$12<DEGREES(CQ41),0+$AJ$16,1-((TAN(CQ41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV67*$DU$3)+1-$DU$3)","v":1.0889698314704781},{"$f":"(IF($AH$12<DEGREES(CR41),0+$AJ$16,1-((TAN(CR41)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW67*$DU$3)+1-$DU$3)","v":1.0151509490001207},null,null,10,34.130498638110296,40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,37.566870997040184,33.04159126014769,null,10,34.130498638110296,40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,37.566870997040184,33.04159126014769]
[null,12,{"$f":"IF('Dry Bulb'!D16<60,(('Input Data'!$F$44*('Dry Bulb'!D16-$T$15))+('Heat gain from airflow'!Q15)+((Occupancy!P15*'Input Data'!$F$47)+(Occupancy!B15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D16-$P$15))+('Heat gain from airflow'!Q15)+((Occupancy!P15*'Input Data'!$F$47)+(Occupancy!B15*'Input Data'!$F$49))))/1000","v":-4.2915599999999987},{"$f":"IF('Dry Bulb'!E16<60,(('Input Data'!$F$44*('Dry Bulb'!E16-$T$15))+('Heat gain from airflow'!R15)+((Occupancy!Q15*'Input Data'!$F$47)+(Occupancy!C15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E16-$P$15))+('Heat gain from airflow'!R15)+((Occupancy!Q15*'Input Data'!$F$47)+(Occupancy!C15*'Input Data'!$F$49))))/1000","v":-2.6045098199999992},{"$f":"IF('Dry Bulb'!F16<60,(('Input Data'!$F$44*('Dry Bulb'!F16-$T$15))+('Heat gain from airflow'!S15)+((Occupancy!R15*'Input Data'!$F$47)+(Occupancy!D15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F16-$P$15))+('Heat gain from airflow'!S15)+((Occupancy!R15*'Input Data'!$F$47)+(Occupancy!D15*'Input Data'!$F$49))))/1000","v":0.44496764999999594},{"$f":"IF('Dry Bulb'!G16<60,(('Input Data'!$F$44*('Dry Bulb'!G16-$T$15))+('Heat gain from airflow'!T15)+((Occupancy!S15*'Input Data'!$F$47)+(Occupancy!E15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G16-$P$15))+('Heat gain from airflow'!T15)+((Occupancy!S15*'Input Data'!$F$47)+(Occupancy!E15*'Input Data'!$F$49))))/1000","v":8.2028925000000044},{"$f":"IF('Dry Bulb'!H16<60,(('Input Data'!$F$44*('Dry Bulb'!H16-$T$15))+('Heat gain from airflow'!U15)+((Occupancy!T15*'Input Data'!$F$47)+(Occupancy!F15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H16-$P$15))+('Heat gain from airflow'!U15)+((Occupancy!T15*'Input Data'!$F$47)+(Occupancy!F15*'Input Data'!$F$49))))/1000","v":13.162522499999996},{"$f":"IF('Dry Bulb'!I16<60,(('Input Data'!$F$44*('Dry Bulb'!I16-$T$15))+('Heat gain from airflow'!V15)+((Occupancy!U15*'Input Data'!$F$47)+(Occupancy!G15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I16-$P$15))+('Heat gain from airflow'!V15)+((Occupancy!U15*'Input Data'!$F$47)+(Occupancy!G15*'Input Data'!$F$49))))/1000","v":16.691490000000002},{"$f":"IF('Dry Bulb'!J16<60,(('Input Data'!$F$44*('Dry Bulb'!J16-$T$15))+('Heat gain from airflow'!W15)+((Occupancy!V15*'Input Data'!$F$47)+(Occupancy!H15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J16-$P$15))+('Heat gain from airflow'!W15)+((Occupancy!V15*'Input Data'!$F$47)+(Occupancy!H15*'Input Data'!$F$49))))/1000","v":18.21753},{"$f":"IF('Dry Bulb'!K16<60,(('Input Data'!$F$44*('Dry Bulb'!K16-$T$15))+('Heat gain from airflow'!X15)+((Occupancy!W15*'Input Data'!$F$47)+(Occupancy!I15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K16-$P$15))+('Heat gain from airflow'!X15)+((Occupancy!W15*'Input Data'!$F$47)+(Occupancy!I15*'Input Data'!$F$49))))/1000","v":18.885172499999992},{"$f":"IF('Dry Bulb'!L16<60,(('Input Data'!$F$44*('Dry Bulb'!L16-$T$15))+('Heat gain from airflow'!Y15)+((Occupancy!X15*'Input Data'!$F$47)+(Occupancy!J15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L16-$P$15))+('Heat gain from airflow'!Y15)+((Occupancy!X15*'Input Data'!$F$47)+(Occupancy!J15*'Input Data'!$F$49))))/1000","v":14.974694999999995},{"$f":"IF('Dry Bulb'!M16<60,(('Input Data'!$F$44*('Dry Bulb'!M16-$T$15))+('Heat gain from airflow'!Z15)+((Occupancy!Y15*'Input Data'!$F$47)+(Occupancy!K15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M16-$P$15))+('Heat gain from airflow'!Z15)+((Occupancy!Y15*'Input Data'!$F$47)+(Occupancy!K15*'Input Data'!$F$49))))/1000","v":9.824309999999997},{"$f":"IF('Dry Bulb'!N16<60,(('Input Data'!$F$44*('Dry Bulb'!N16-$T$15))+('Heat gain from airflow'!AA15)+((Occupancy!Z15*'Input Data'!$F$47)+(Occupancy!L15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N16-$P$15))+('Heat gain from airflow'!AA15)+((Occupancy!Z15*'Input Data'!$F$47)+(Occupancy!L15*'Input Data'!$F$49))))/1000","v":5.0191838550000032},{"$f":"IF('Dry Bulb'!O16<60,(('Input Data'!$F$44*('Dry Bulb'!O16-$T$15))+('Heat gain from airflow'!AB15)+((Occupancy!AA15*'Input Data'!$F$47)+(Occupancy!M15*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O16-$P$15))+('Heat gain from airflow'!AB15)+((Occupancy!AA15*'Input Data'!$F$47)+(Occupancy!M15*'Input Data'!$F$49))))/1000","v":-3.1470299999999969},null,"West Window",null,null,null,{"$f":"SUM(C191:N214)","v":3928.8346654967154},null,null,"Window Height",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI70","v":11},{"$f":"'Incident angle'!BJ70","v":0},{"$f":"'Incident angle'!BK70","v":0},{"$f":"'Incident angle'!BL70","v":0},{"$f":"'Incident angle'!BM70","v":0},{"$f":"'Incident angle'!BN70","v":0},{"$f":"'Incident angle'!BO70","v":0},{"$f":"'Incident angle'!BP70","v":0},{"$f":"'Incident angle'!BQ70","v":0},{"$f":"'Incident angle'!BR70","v":0},{"$f":"'Incident angle'!BS70","v":0},{"$f":"'Incident angle'!BT70","v":0},{"$f":"'Incident angle'!BU70","v":0},null,{"$f":"'Incident angle'!BW70","v":11},{"$f":"'Incident angle'!BX70","v":0},{"$f":"'Incident angle'!BY70","v":0},{"$f":"'Incident angle'!BZ70","v":0},{"$f":"'Incident angle'!CA70","v":0},{"$f":"'Incident angle'!CB70","v":0},{"$f":"'Incident angle'!CC70","v":0},{"$f":"'Incident angle'!CD70","v":0},{"$f":"'Incident angle'!CE70","v":0},{"$f":"'Incident angle'!CF70","v":0},{"$f":"'Incident angle'!CG70","v":0},{"$f":"'Incident angle'!CH70","v":0},{"$f":"'Incident angle'!CI70","v":0},null,{"$f":"'Profile angles'!P15","v":11},{"$f":"RADIANS('Profile angles'!Q15)","v":-1.1268272200794018},{"$f":"RADIANS('Profile angles'!R15)","v":-1.1501949201099215},{"$f":"RADIANS('Profile angles'!S15)","v":-1.2149427363314722},{"$f":"RADIANS('Profile angles'!T15)","v":-1.2827675748177341},{"$f":"RADIANS('Profile angles'!U15)","v":-1.3094800079043547},{"$f":"RADIANS('Profile angles'!V15)","v":-1.2971248839107501},{"$f":"RADIANS('Profile angles'!W15)","v":-1.2712928251657776},{"$f":"RADIANS('Profile angles'!X15)","v":-1.2680765910530094},{"$f":"RADIANS('Profile angles'!Y15)","v":-1.2857310025410147},{"$f":"RADIANS('Profile angles'!Z15)","v":-1.3000930619226607},{"$f":"RADIANS('Profile angles'!AA15)","v":-1.2658856481778873},{"$f":"RADIANS('Profile angles'!AB15)","v":-1.1829208364741319},null,{"$f":"'Profile angles'!P44","v":11},{"$f":"RADIANS('Profile angles'!Q44)","v":-0.77287050251262801},{"$f":"RADIANS('Profile angles'!R44)","v":-0.94279982780897686},{"$f":"RADIANS('Profile angles'!S44)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T44)","v":-1.3560531209708369},{"$f":"RADIANS('Profile angles'!U44)","v":-1.5069809238556897},{"$f":"RADIANS('Profile angles'!V44)","v":-1.5658083868258725},{"$f":"RADIANS('Profile angles'!W44)","v":-1.5149166606406737},{"$f":"RADIANS('Profile angles'!X44)","v":-1.3606731060385546},{"$f":"RADIANS('Profile angles'!Y44)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!Z44)","v":-0.94820534202278628},{"$f":"RADIANS('Profile angles'!AA44)","v":-0.78354196814002852},{"$f":"RADIANS('Profile angles'!AB44)","v":-0.71507325853303161},null,{"$f":"'Profile angles'!AR15","v":11},{"$f":"(IF($AH$29<DEGREES(BS42),0+$AJ$33,1-((TAN(BS42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX68*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BT42),0+$AJ$33,1-((TAN(BT42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY68*$DU$3)+1-$DU$3)","v":0.48323136350611129},{"$f":"(IF($AH$29<DEGREES(BU42),0+$AJ$33,1-((TAN(BU42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ68*$DU$3)+1-$DU$3)","v":1.0992839539792576},{"$f":"(IF($AH$29<DEGREES(BV42),0+$AJ$33,1-((TAN(BV42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA68*$DU$3)+1-$DU$3)","v":2.1249428015294032},{"$f":"(IF($AH$29<DEGREES(BW42),0+$AJ$33,1-((TAN(BW42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB68*$DU$3)+1-$DU$3)","v":3.1852966672178233},{"$f":"(IF($AH$29<DEGREES(BX42),0+$AJ$33,1-((TAN(BX42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC68*$DU$3)+1-$DU$3)","v":3.4625948921333998},{"$f":"(IF($AH$29<DEGREES(BY42),0+$AJ$33,1-((TAN(BY42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD68*$DU$3)+1-$DU$3)","v":2.9709957321774971},{"$f":"(IF($AH$29<DEGREES(BZ42),0+$AJ$33,1-((TAN(BZ42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE68*$DU$3)+1-$DU$3)","v":2.1346162432755458},{"$f":"(IF($AH$29<DEGREES(CA42),0+$AJ$33,1-((TAN(CA42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF68*$DU$3)+1-$DU$3)","v":0.72934768155389029},{"$f":"(IF($AH$29<DEGREES(CB42),0+$AJ$33,1-((TAN(CB42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG68*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CC42),0+$AJ$33,1-((TAN(CC42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH68*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CD42),0+$AJ$33,1-((TAN(CD42)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI68*$DU$3)+1-$DU$3)","v":0},null,11,{"$f":"(IF($AH$12<DEGREES(CG42),0+$AJ$16,1-((TAN(CG42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL68*$DU$3)+1-$DU$3)","v":1.292407290373538},{"$f":"(IF($AH$12<DEGREES(CH42),0+$AJ$16,1-((TAN(CH42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM68*$DU$3)+1-$DU$3)","v":1.3591076730029019},{"$f":"(IF($AH$12<DEGREES(CI42),0+$AJ$16,1-((TAN(CI42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN68*$DU$3)+1-$DU$3)","v":1.50295407518346},{"$f":"(IF($AH$12<DEGREES(CJ42),0+$AJ$16,1-((TAN(CJ42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO68*$DU$3)+1-$DU$3)","v":1.3504692429989684},{"$f":"(IF($AH$12<DEGREES(CK42),0+$AJ$16,1-((TAN(CK42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP68*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL42),0+$AJ$16,1-((TAN(CL42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ68*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM42),0+$AJ$16,1-((TAN(CM42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR68*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN42),0+$AJ$16,1-((TAN(CN42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS68*$DU$3)+1-$DU$3)","v":1.146731228634895},{"$f":"(IF($AH$12<DEGREES(CO42),0+$AJ$16,1-((TAN(CO42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT68*$DU$3)+1-$DU$3)","v":1.7185185960363529},{"$f":"(IF($AH$12<DEGREES(CP42),0+$AJ$16,1-((TAN(CP42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU68*$DU$3)+1-$DU$3)","v":1.593360613988257},{"$f":"(IF($AH$12<DEGREES(CQ42),0+$AJ$16,1-((TAN(CQ42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV68*$DU$3)+1-$DU$3)","v":1.431287791885884},{"$f":"(IF($AH$12<DEGREES(CR42),0+$AJ$16,1-((TAN(CR42)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW68*$DU$3)+1-$DU$3)","v":1.3226350229813162},null,null,11,41.499338482119107,49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983,null,11,41.499338482119107,49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983]
[null,13,{"$f":"IF('Dry Bulb'!D17<60,(('Input Data'!$F$44*('Dry Bulb'!D17-$T$15))+('Heat gain from airflow'!Q16)+((Occupancy!P16*'Input Data'!$F$47)+(Occupancy!B16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D17-$P$15))+('Heat gain from airflow'!Q16)+((Occupancy!P16*'Input Data'!$F$47)+(Occupancy!B16*'Input Data'!$F$49))))/1000","v":-3.2424075000000001},{"$f":"IF('Dry Bulb'!E17<60,(('Input Data'!$F$44*('Dry Bulb'!E17-$T$15))+('Heat gain from airflow'!R16)+((Occupancy!Q16*'Input Data'!$F$47)+(Occupancy!C16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E17-$P$15))+('Heat gain from airflow'!R16)+((Occupancy!Q16*'Input Data'!$F$47)+(Occupancy!C16*'Input Data'!$F$49))))/1000","v":-0.84519589499999759},{"$f":"IF('Dry Bulb'!F17<60,(('Input Data'!$F$44*('Dry Bulb'!F17-$T$15))+('Heat gain from airflow'!S16)+((Occupancy!R16*'Input Data'!$F$47)+(Occupancy!D16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F17-$P$15))+('Heat gain from airflow'!S16)+((Occupancy!R16*'Input Data'!$F$47)+(Occupancy!D16*'Input Data'!$F$49))))/1000","v":2.7907195500000017},{"$f":"IF('Dry Bulb'!G17<60,(('Input Data'!$F$44*('Dry Bulb'!G17-$T$15))+('Heat gain from airflow'!T16)+((Occupancy!S16*'Input Data'!$F$47)+(Occupancy!E16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G17-$P$15))+('Heat gain from airflow'!T16)+((Occupancy!S16*'Input Data'!$F$47)+(Occupancy!E16*'Input Data'!$F$49))))/1000","v":8.8705350000000003},{"$f":"IF('Dry Bulb'!H17<60,(('Input Data'!$F$44*('Dry Bulb'!H17-$T$15))+('Heat gain from airflow'!U16)+((Occupancy!T16*'Input Data'!$F$47)+(Occupancy!F16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H17-$P$15))+('Heat gain from airflow'!U16)+((Occupancy!T16*'Input Data'!$F$47)+(Occupancy!F16*'Input Data'!$F$49))))/1000","v":14.211674999999998},{"$f":"IF('Dry Bulb'!I17<60,(('Input Data'!$F$44*('Dry Bulb'!I17-$T$15))+('Heat gain from airflow'!V16)+((Occupancy!U16*'Input Data'!$F$47)+(Occupancy!G16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I17-$P$15))+('Heat gain from airflow'!V16)+((Occupancy!U16*'Input Data'!$F$47)+(Occupancy!G16*'Input Data'!$F$49))))/1000","v":17.359132499999998},{"$f":"IF('Dry Bulb'!J17<60,(('Input Data'!$F$44*('Dry Bulb'!J17-$T$15))+('Heat gain from airflow'!W16)+((Occupancy!V16*'Input Data'!$F$47)+(Occupancy!H16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J17-$P$15))+('Heat gain from airflow'!W16)+((Occupancy!V16*'Input Data'!$F$47)+(Occupancy!H16*'Input Data'!$F$49))))/1000","v":18.980549999999997},{"$f":"IF('Dry Bulb'!K17<60,(('Input Data'!$F$44*('Dry Bulb'!K17-$T$15))+('Heat gain from airflow'!X16)+((Occupancy!W16*'Input Data'!$F$47)+(Occupancy!I16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K17-$P$15))+('Heat gain from airflow'!X16)+((Occupancy!W16*'Input Data'!$F$47)+(Occupancy!I16*'Input Data'!$F$49))))/1000","v":19.934324999999998},{"$f":"IF('Dry Bulb'!L17<60,(('Input Data'!$F$44*('Dry Bulb'!L17-$T$15))+('Heat gain from airflow'!Y16)+((Occupancy!X16*'Input Data'!$F$47)+(Occupancy!J16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L17-$P$15))+('Heat gain from airflow'!Y16)+((Occupancy!X16*'Input Data'!$F$47)+(Occupancy!J16*'Input Data'!$F$49))))/1000","v":15.928469999999995},{"$f":"IF('Dry Bulb'!M17<60,(('Input Data'!$F$44*('Dry Bulb'!M17-$T$15))+('Heat gain from airflow'!Z16)+((Occupancy!Y16*'Input Data'!$F$47)+(Occupancy!K16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M17-$P$15))+('Heat gain from airflow'!Z16)+((Occupancy!Y16*'Input Data'!$F$47)+(Occupancy!K16*'Input Data'!$F$49))))/1000","v":10.778084999999995},{"$f":"IF('Dry Bulb'!N17<60,(('Input Data'!$F$44*('Dry Bulb'!N17-$T$15))+('Heat gain from airflow'!AA16)+((Occupancy!Z16*'Input Data'!$F$47)+(Occupancy!L16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N17-$P$15))+('Heat gain from airflow'!AA16)+((Occupancy!Z16*'Input Data'!$F$47)+(Occupancy!L16*'Input Data'!$F$49))))/1000","v":5.7230775000000005},{"$f":"IF('Dry Bulb'!O17<60,(('Input Data'!$F$44*('Dry Bulb'!O17-$T$15))+('Heat gain from airflow'!AB16)+((Occupancy!AA16*'Input Data'!$F$47)+(Occupancy!M16*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O17-$P$15))+('Heat gain from airflow'!AB16)+((Occupancy!AA16*'Input Data'!$F$47)+(Occupancy!M16*'Input Data'!$F$49))))/1000","v":-3.0736601999999986},null,"Area",{"$f":"Q46*'Input Data'!F23*'Input Data'!F19","v":270},null,null,null,null,null,null,1,null,null,null,null,"Lab Override",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI71","v":12},{"$f":"'Incident angle'!BJ71","v":0},{"$f":"'Incident angle'!BK71","v":0},{"$f":"'Incident angle'!BL71","v":0},{"$f":"'Incident angle'!BM71","v":0},{"$f":"'Incident angle'!BN71","v":0},{"$f":"'Incident angle'!BO71","v":0},{"$f":"'Incident angle'!BP71","v":0},{"$f":"'Incident angle'!BQ71","v":0},{"$f":"'Incident angle'!BR71","v":0},{"$f":"'Incident angle'!BS71","v":0},{"$f":"'Incident angle'!BT71","v":0},{"$f":"'Incident angle'!BU71","v":0},null,{"$f":"'Incident angle'!BW71","v":12},{"$f":"'Incident angle'!BX71","v":0},{"$f":"'Incident angle'!BY71","v":0},{"$f":"'Incident angle'!BZ71","v":0},{"$f":"'Incident angle'!CA71","v":0},{"$f":"'Incident angle'!CB71","v":0},{"$f":"'Incident angle'!CC71","v":0},{"$f":"'Incident angle'!CD71","v":0},{"$f":"'Incident angle'!CE71","v":0},{"$f":"'Incident angle'!CF71","v":0},{"$f":"'Incident angle'!CG71","v":0},{"$f":"'Incident angle'!CH71","v":0},{"$f":"'Incident angle'!CI71","v":0},null,{"$f":"'Profile angles'!P16","v":12},{"$f":"RADIANS('Profile angles'!Q16)","v":-1.4652572312778289},{"$f":"RADIANS('Profile angles'!R16)","v":-1.4603602289474145},{"$f":"RADIANS('Profile angles'!S16)","v":-1.5005364967084425},{"$f":"RADIANS('Profile angles'!T16)","v":-1.5443810972198111},{"$f":"RADIANS('Profile angles'!U16)","v":-1.555062909254763},{"$f":"RADIANS('Profile angles'!V16)","v":-1.536631166126466},{"$f":"RADIANS('Profile angles'!W16)","v":-1.5161625036324029},{"$f":"RADIANS('Profile angles'!X16)","v":-1.5291230837920124},{"$f":"RADIANS('Profile angles'!Y16)","v":-1.5690353246394675},{"$f":"RADIANS('Profile angles'!Z16)","v":-1.5273206771977748},{"$f":"RADIANS('Profile angles'!AA16)","v":-1.5323869921532096},{"$f":"RADIANS('Profile angles'!AB16)","v":-1.5376009071783352},null,{"$f":"'Profile angles'!P45","v":12},{"$f":"RADIANS('Profile angles'!Q45)","v":-0.79135309629409845},{"$f":"RADIANS('Profile angles'!R45)","v":-0.95393106557871754},{"$f":"RADIANS('Profile angles'!S45)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T45)","v":-1.3474641185275609},{"$f":"RADIANS('Profile angles'!U45)","v":-1.494047359637104},{"$f":"RADIANS('Profile angles'!V45)","v":-1.549232894297323},{"$f":"RADIANS('Profile angles'!W45)","v":-1.498048297172524},{"$f":"RADIANS('Profile angles'!X45)","v":-1.3510622858662449},{"$f":"RADIANS('Profile angles'!Y45)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!Z45)","v":-0.95283102870472114},{"$f":"RADIANS('Profile angles'!AA45)","v":-0.79224403056524917},{"$f":"RADIANS('Profile angles'!AB45)","v":-0.73031386460610437},null,{"$f":"'Profile angles'!AR16","v":12},{"$f":"(IF($AH$29<DEGREES(BS43),0+$AJ$33,1-((TAN(BS43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX69*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BT43),0+$AJ$33,1-((TAN(BT43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY69*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BU43),0+$AJ$33,1-((TAN(BU43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ69*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BV43),0+$AJ$33,1-((TAN(BV43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA69*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BW43),0+$AJ$33,1-((TAN(BW43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB69*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BX43),0+$AJ$33,1-((TAN(BX43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC69*$DU$3)+1-$DU$3)","v":14.703510957314624},{"$f":"(IF($AH$29<DEGREES(BY43),0+$AJ$33,1-((TAN(BY43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD69*$DU$3)+1-$DU$3)","v":4.6051178893506677},{"$f":"(IF($AH$29<DEGREES(BZ43),0+$AJ$33,1-((TAN(BZ43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE69*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CA43),0+$AJ$33,1-((TAN(CA43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF69*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CB43),0+$AJ$33,1-((TAN(CB43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG69*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CC43),0+$AJ$33,1-((TAN(CC43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH69*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CD43),0+$AJ$33,1-((TAN(CD43)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI69*$DU$3)+1-$DU$3)","v":0},null,12,{"$f":"(IF($AH$12<DEGREES(CG43),0+$AJ$16,1-((TAN(CG43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL69*$DU$3)+1-$DU$3)","v":1.6168157720778558},{"$f":"(IF($AH$12<DEGREES(CH43),0+$AJ$16,1-((TAN(CH43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM69*$DU$3)+1-$DU$3)","v":1.8317000390382643},{"$f":"(IF($AH$12<DEGREES(CI43),0+$AJ$16,1-((TAN(CI43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN69*$DU$3)+1-$DU$3)","v":2.3289734177578625},{"$f":"(IF($AH$12<DEGREES(CJ43),0+$AJ$16,1-((TAN(CJ43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO69*$DU$3)+1-$DU$3)","v":3.8446226002569115},{"$f":"(IF($AH$12<DEGREES(CK43),0+$AJ$16,1-((TAN(CK43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP69*$DU$3)+1-$DU$3)","v":9.0691557557799616},{"$f":"(IF($AH$12<DEGREES(CL43),0+$AJ$16,1-((TAN(CL43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ69*$DU$3)+1-$DU$3)","v":6.9461808605659021},{"$f":"(IF($AH$12<DEGREES(CM43),0+$AJ$16,1-((TAN(CM43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR69*$DU$3)+1-$DU$3)","v":6.6260569396605264},{"$f":"(IF($AH$12<DEGREES(CN43),0+$AJ$16,1-((TAN(CN43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS69*$DU$3)+1-$DU$3)","v":3.7483038027552622},{"$f":"(IF($AH$12<DEGREES(CO43),0+$AJ$16,1-((TAN(CO43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT69*$DU$3)+1-$DU$3)","v":2.5170813394850642},{"$f":"(IF($AH$12<DEGREES(CP43),0+$AJ$16,1-((TAN(CP43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU69*$DU$3)+1-$DU$3)","v":1.9240153710548673},{"$f":"(IF($AH$12<DEGREES(CQ43),0+$AJ$16,1-((TAN(CQ43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV69*$DU$3)+1-$DU$3)","v":1.6763481340596806},{"$f":"(IF($AH$12<DEGREES(CR43),0+$AJ$16,1-((TAN(CR43)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW69*$DU$3)+1-$DU$3)","v":1.6026495204864732},null,null,12,45.177523796213436,54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598,null,12,45.177523796213436,54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598]
[null,14,{"$f":"IF('Dry Bulb'!D18<60,(('Input Data'!$F$44*('Dry Bulb'!D18-$T$15))+('Heat gain from airflow'!Q17)+((Occupancy!P17*'Input Data'!$F$47)+(Occupancy!B17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D18-$P$15))+('Heat gain from airflow'!Q17)+((Occupancy!P17*'Input Data'!$F$47)+(Occupancy!B17*'Input Data'!$F$49))))/1000","v":-3.5428105799999976},{"$f":"IF('Dry Bulb'!E18<60,(('Input Data'!$F$44*('Dry Bulb'!E18-$T$15))+('Heat gain from airflow'!R17)+((Occupancy!Q17*'Input Data'!$F$47)+(Occupancy!C17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E18-$P$15))+('Heat gain from airflow'!R17)+((Occupancy!Q17*'Input Data'!$F$47)+(Occupancy!C17*'Input Data'!$F$49))))/1000","v":0.44496764999999594},{"$f":"IF('Dry Bulb'!F18<60,(('Input Data'!$F$44*('Dry Bulb'!F18-$T$15))+('Heat gain from airflow'!S17)+((Occupancy!R17*'Input Data'!$F$47)+(Occupancy!D17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F18-$P$15))+('Heat gain from airflow'!S17)+((Occupancy!R17*'Input Data'!$F$47)+(Occupancy!D17*'Input Data'!$F$49))))/1000","v":3.8463079049999953},{"$f":"IF('Dry Bulb'!G18<60,(('Input Data'!$F$44*('Dry Bulb'!G18-$T$15))+('Heat gain from airflow'!T17)+((Occupancy!S17*'Input Data'!$F$47)+(Occupancy!E17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G18-$P$15))+('Heat gain from airflow'!T17)+((Occupancy!S17*'Input Data'!$F$47)+(Occupancy!E17*'Input Data'!$F$49))))/1000","v":9.6335549999999959},{"$f":"IF('Dry Bulb'!H18<60,(('Input Data'!$F$44*('Dry Bulb'!H18-$T$15))+('Heat gain from airflow'!U17)+((Occupancy!T17*'Input Data'!$F$47)+(Occupancy!F17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H18-$P$15))+('Heat gain from airflow'!U17)+((Occupancy!T17*'Input Data'!$F$47)+(Occupancy!F17*'Input Data'!$F$49))))/1000","v":14.974694999999995},{"$f":"IF('Dry Bulb'!I18<60,(('Input Data'!$F$44*('Dry Bulb'!I18-$T$15))+('Heat gain from airflow'!V17)+((Occupancy!U17*'Input Data'!$F$47)+(Occupancy!G17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I18-$P$15))+('Heat gain from airflow'!V17)+((Occupancy!U17*'Input Data'!$F$47)+(Occupancy!G17*'Input Data'!$F$49))))/1000","v":18.503662500000001},{"$f":"IF('Dry Bulb'!J18<60,(('Input Data'!$F$44*('Dry Bulb'!J18-$T$15))+('Heat gain from airflow'!W17)+((Occupancy!V17*'Input Data'!$F$47)+(Occupancy!H17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J18-$P$15))+('Heat gain from airflow'!W17)+((Occupancy!V17*'Input Data'!$F$47)+(Occupancy!H17*'Input Data'!$F$49))))/1000","v":19.838947499999996},{"$f":"IF('Dry Bulb'!K18<60,(('Input Data'!$F$44*('Dry Bulb'!K18-$T$15))+('Heat gain from airflow'!X17)+((Occupancy!W17*'Input Data'!$F$47)+(Occupancy!I17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K18-$P$15))+('Heat gain from airflow'!X17)+((Occupancy!W17*'Input Data'!$F$47)+(Occupancy!I17*'Input Data'!$F$49))))/1000","v":20.411212500000001},{"$f":"IF('Dry Bulb'!L18<60,(('Input Data'!$F$44*('Dry Bulb'!L18-$T$15))+('Heat gain from airflow'!Y17)+((Occupancy!X17*'Input Data'!$F$47)+(Occupancy!J17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L18-$P$15))+('Heat gain from airflow'!Y17)+((Occupancy!X17*'Input Data'!$F$47)+(Occupancy!J17*'Input Data'!$F$49))))/1000","v":16.500734999999992},{"$f":"IF('Dry Bulb'!M18<60,(('Input Data'!$F$44*('Dry Bulb'!M18-$T$15))+('Heat gain from airflow'!Z17)+((Occupancy!Y17*'Input Data'!$F$47)+(Occupancy!K17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M18-$P$15))+('Heat gain from airflow'!Z17)+((Occupancy!Y17*'Input Data'!$F$47)+(Occupancy!K17*'Input Data'!$F$49))))/1000","v":11.541105000000003},{"$f":"IF('Dry Bulb'!N18<60,(('Input Data'!$F$44*('Dry Bulb'!N18-$T$15))+('Heat gain from airflow'!AA17)+((Occupancy!Z17*'Input Data'!$F$47)+(Occupancy!L17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N18-$P$15))+('Heat gain from airflow'!AA17)+((Occupancy!Z17*'Input Data'!$F$47)+(Occupancy!L17*'Input Data'!$F$49))))/1000","v":6.1999650000000042},{"$f":"IF('Dry Bulb'!O18<60,(('Input Data'!$F$44*('Dry Bulb'!O18-$T$15))+('Heat gain from airflow'!AB17)+((Occupancy!AA17*'Input Data'!$F$47)+(Occupancy!M17*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O18-$P$15))+('Heat gain from airflow'!AB17)+((Occupancy!AA17*'Input Data'!$F$47)+(Occupancy!M17*'Input Data'!$F$49))))/1000","v":-2.1353594400000002},null,"Glass SHGC",0.28999999999999998,null,null,null,null,null,null,2,null,null,null,null,{"$f":"'HVAC Dashboard'!AC36","v":1},null,null,"Tanδ =  ",null,{"$f":"IF(X39>0,W40/X39,99999999)","v":1.6666666666666667},null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI72","v":13},{"$f":"'Incident angle'!BJ72","v":0},{"$f":"'Incident angle'!BK72","v":0},{"$f":"'Incident angle'!BL72","v":0},{"$f":"'Incident angle'!BM72","v":0},{"$f":"'Incident angle'!BN72","v":0},{"$f":"'Incident angle'!BO72","v":0},{"$f":"'Incident angle'!BP72","v":0},{"$f":"'Incident angle'!BQ72","v":0},{"$f":"'Incident angle'!BR72","v":0},{"$f":"'Incident angle'!BS72","v":0},{"$f":"'Incident angle'!BT72","v":0},{"$f":"'Incident angle'!BU72","v":0},null,{"$f":"'Incident angle'!BW72","v":13},{"$f":"'Incident angle'!BX72","v":0},{"$f":"'Incident angle'!BY72","v":0},{"$f":"'Incident angle'!BZ72","v":0},{"$f":"'Incident angle'!CA72","v":0},{"$f":"'Incident angle'!CB72","v":0},{"$f":"'Incident angle'!CC72","v":0},{"$f":"'Incident angle'!CD72","v":0},{"$f":"'Incident angle'!CE72","v":0},{"$f":"'Incident angle'!CF72","v":0},{"$f":"'Incident angle'!CG72","v":0},{"$f":"'Incident angle'!CH72","v":0},{"$f":"'Incident angle'!CI72","v":0},null,{"$f":"'Profile angles'!P17","v":13},{"$f":"RADIANS('Profile angles'!Q17)","v":1.3318648713001162},{"$f":"RADIANS('Profile angles'!R17)","v":1.3666270114598316},{"$f":"RADIANS('Profile angles'!S17)","v":1.3535067192060637},{"$f":"RADIANS('Profile angles'!T17)","v":1.3351101550303341},{"$f":"RADIANS('Profile angles'!U17)","v":1.3407321893366533},{"$f":"RADIANS('Profile angles'!V17)","v":1.3650413570281472},{"$f":"RADIANS('Profile angles'!W17)","v":1.379822745398283},{"$f":"RADIANS('Profile angles'!X17)","v":1.3506595370421364},{"$f":"RADIANS('Profile angles'!Y17)","v":1.2822582122157398},{"$f":"RADIANS('Profile angles'!Z17)","v":1.2149101170192604},{"$f":"RADIANS('Profile angles'!AA17)","v":1.1912817761692731},{"$f":"RADIANS('Profile angles'!AB17)","v":1.2470964531741522},null,{"$f":"'Profile angles'!P46","v":13},{"$f":"RADIANS('Profile angles'!Q46)","v":-0.78702668175259982},{"$f":"RADIANS('Profile angles'!R46)","v":-0.95205108174928044},{"$f":"RADIANS('Profile angles'!S46)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T46)","v":-1.3531133844064993},{"$f":"RADIANS('Profile angles'!U46)","v":-1.503986673926925},{"$f":"RADIANS('Profile angles'!V46)","v":-1.558344195190098},{"$f":"RADIANS('Profile angles'!W46)","v":-1.5043943771425594},{"$f":"RADIANS('Profile angles'!X46)","v":-1.3559509038151709},{"$f":"RADIANS('Profile angles'!Y46)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!Z46)","v":-0.94455934348747927},{"$f":"RADIANS('Profile angles'!AA46)","v":-0.77841604698882561},{"$f":"RADIANS('Profile angles'!AB46)","v":-0.71991055223641132},null,{"$f":"'Profile angles'!AR17","v":13},{"$f":"(IF($AH$29<DEGREES(BS44),0+$AJ$33,1-((TAN(BS44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BT44),0+$AJ$33,1-((TAN(BT44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BU44),0+$AJ$33,1-((TAN(BU44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BV44),0+$AJ$33,1-((TAN(BV44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BW44),0+$AJ$33,1-((TAN(BW44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BX44),0+$AJ$33,1-((TAN(BX44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BY44),0+$AJ$33,1-((TAN(BY44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BZ44),0+$AJ$33,1-((TAN(BZ44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CA44),0+$AJ$33,1-((TAN(CA44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CB44),0+$AJ$33,1-((TAN(CB44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CC44),0+$AJ$33,1-((TAN(CC44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CD44),0+$AJ$33,1-((TAN(CD44)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI70*$DU$3)+1-$DU$3)","v":0},null,13,{"$f":"(IF($AH$12<DEGREES(CG44),0+$AJ$16,1-((TAN(CG44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL70*$DU$3)+1-$DU$3)","v":1.4942823559875626},{"$f":"(IF($AH$12<DEGREES(CH44),0+$AJ$16,1-((TAN(CH44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM70*$DU$3)+1-$DU$3)","v":1.6947772438639674},{"$f":"(IF($AH$12<DEGREES(CI44),0+$AJ$16,1-((TAN(CI44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN70*$DU$3)+1-$DU$3)","v":1.9166512903452229},{"$f":"(IF($AH$12<DEGREES(CJ44),0+$AJ$16,1-((TAN(CJ44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO70*$DU$3)+1-$DU$3)","v":1.9038528532624603},{"$f":"(IF($AH$12<DEGREES(CK44),0+$AJ$16,1-((TAN(CK44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL44),0+$AJ$16,1-((TAN(CL44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM44),0+$AJ$16,1-((TAN(CM44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR70*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN44),0+$AJ$16,1-((TAN(CN44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS70*$DU$3)+1-$DU$3)","v":2.0504263728731313},{"$f":"(IF($AH$12<DEGREES(CO44),0+$AJ$16,1-((TAN(CO44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT70*$DU$3)+1-$DU$3)","v":1.7081697247176275},{"$f":"(IF($AH$12<DEGREES(CP44),0+$AJ$16,1-((TAN(CP44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU70*$DU$3)+1-$DU$3)","v":1.4621309658224781},{"$f":"(IF($AH$12<DEGREES(CQ44),0+$AJ$16,1-((TAN(CQ44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV70*$DU$3)+1-$DU$3)","v":1.3578806896655302},{"$f":"(IF($AH$12<DEGREES(CR44),0+$AJ$16,1-((TAN(CR44)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW70*$DU$3)+1-$DU$3)","v":1.3764383353242993},null,null,13,44.262516808487675,53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703,null,13,44.262516808487675,53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703]
[null,15,{"$f":"IF('Dry Bulb'!D19<60,(('Input Data'!$F$44*('Dry Bulb'!D19-$T$15))+('Heat gain from airflow'!Q18)+((Occupancy!P18*'Input Data'!$F$47)+(Occupancy!B18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D19-$P$15))+('Heat gain from airflow'!Q18)+((Occupancy!P18*'Input Data'!$F$47)+(Occupancy!B18*'Input Data'!$F$49))))/1000","v":-3.1909477950000027},{"$f":"IF('Dry Bulb'!E19<60,(('Input Data'!$F$44*('Dry Bulb'!E19-$T$15))+('Heat gain from airflow'!R18)+((Occupancy!Q18*'Input Data'!$F$47)+(Occupancy!C18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E19-$P$15))+('Heat gain from airflow'!R18)+((Occupancy!Q18*'Input Data'!$F$47)+(Occupancy!C18*'Input Data'!$F$49))))/1000","v":1.1486932200000042},{"$f":"IF('Dry Bulb'!F19<60,(('Input Data'!$F$44*('Dry Bulb'!F19-$T$15))+('Heat gain from airflow'!S18)+((Occupancy!R18*'Input Data'!$F$47)+(Occupancy!D18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F19-$P$15))+('Heat gain from airflow'!S18)+((Occupancy!R18*'Input Data'!$F$47)+(Occupancy!D18*'Input Data'!$F$49))))/1000","v":4.5500334750000038},{"$f":"IF('Dry Bulb'!G19<60,(('Input Data'!$F$44*('Dry Bulb'!G19-$T$15))+('Heat gain from airflow'!T18)+((Occupancy!S18*'Input Data'!$F$47)+(Occupancy!E18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G19-$P$15))+('Heat gain from airflow'!T18)+((Occupancy!S18*'Input Data'!$F$47)+(Occupancy!E18*'Input Data'!$F$49))))/1000","v":10.110442500000001},{"$f":"IF('Dry Bulb'!H19<60,(('Input Data'!$F$44*('Dry Bulb'!H19-$T$15))+('Heat gain from airflow'!U18)+((Occupancy!T18*'Input Data'!$F$47)+(Occupancy!F18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H19-$P$15))+('Heat gain from airflow'!U18)+((Occupancy!T18*'Input Data'!$F$47)+(Occupancy!F18*'Input Data'!$F$49))))/1000","v":15.165449999999996},{"$f":"IF('Dry Bulb'!I19<60,(('Input Data'!$F$44*('Dry Bulb'!I19-$T$15))+('Heat gain from airflow'!V18)+((Occupancy!U18*'Input Data'!$F$47)+(Occupancy!G18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I19-$P$15))+('Heat gain from airflow'!V18)+((Occupancy!U18*'Input Data'!$F$47)+(Occupancy!G18*'Input Data'!$F$49))))/1000","v":18.885172499999992},{"$f":"IF('Dry Bulb'!J19<60,(('Input Data'!$F$44*('Dry Bulb'!J19-$T$15))+('Heat gain from airflow'!W18)+((Occupancy!V18*'Input Data'!$F$47)+(Occupancy!H18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J19-$P$15))+('Heat gain from airflow'!W18)+((Occupancy!V18*'Input Data'!$F$47)+(Occupancy!H18*'Input Data'!$F$49))))/1000","v":20.315835},{"$f":"IF('Dry Bulb'!K19<60,(('Input Data'!$F$44*('Dry Bulb'!K19-$T$15))+('Heat gain from airflow'!X18)+((Occupancy!W18*'Input Data'!$F$47)+(Occupancy!I18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K19-$P$15))+('Heat gain from airflow'!X18)+((Occupancy!W18*'Input Data'!$F$47)+(Occupancy!I18*'Input Data'!$F$49))))/1000","v":20.601967499999997},{"$f":"IF('Dry Bulb'!L19<60,(('Input Data'!$F$44*('Dry Bulb'!L19-$T$15))+('Heat gain from airflow'!Y18)+((Occupancy!X18*'Input Data'!$F$47)+(Occupancy!J18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L19-$P$15))+('Heat gain from airflow'!Y18)+((Occupancy!X18*'Input Data'!$F$47)+(Occupancy!J18*'Input Data'!$F$49))))/1000","v":16.882245000000001},{"$f":"IF('Dry Bulb'!M19<60,(('Input Data'!$F$44*('Dry Bulb'!M19-$T$15))+('Heat gain from airflow'!Z18)+((Occupancy!Y18*'Input Data'!$F$47)+(Occupancy!K18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M19-$P$15))+('Heat gain from airflow'!Z18)+((Occupancy!Y18*'Input Data'!$F$47)+(Occupancy!K18*'Input Data'!$F$49))))/1000","v":12.017992499999998},{"$f":"IF('Dry Bulb'!N19<60,(('Input Data'!$F$44*('Dry Bulb'!N19-$T$15))+('Heat gain from airflow'!AA18)+((Occupancy!Z18*'Input Data'!$F$47)+(Occupancy!L18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N19-$P$15))+('Heat gain from airflow'!AA18)+((Occupancy!Z18*'Input Data'!$F$47)+(Occupancy!L18*'Input Data'!$F$49))))/1000","v":6.8676074999999983},{"$f":"IF('Dry Bulb'!O19<60,(('Input Data'!$F$44*('Dry Bulb'!O19-$T$15))+('Heat gain from airflow'!AB18)+((Occupancy!AA18*'Input Data'!$F$47)+(Occupancy!M18*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O19-$P$15))+('Heat gain from airflow'!AB18)+((Occupancy!AA18*'Input Data'!$F$47)+(Occupancy!M18*'Input Data'!$F$49))))/1000","v":-1.666209060000001},null,"U-Value",0.45,false,null,"BLC",null,null,null,3,null,null,null,null,null,null,null,null,null,"δ=",{"$f":"ATAN(AH44)","v":1.0303768265243125},null,null,null,null,null,null,{"$f":"'Incident angle'!BI73","v":14},{"$f":"'Incident angle'!BJ73","v":0},{"$f":"'Incident angle'!BK73","v":0},{"$f":"'Incident angle'!BL73","v":0},{"$f":"'Incident angle'!BM73","v":0},{"$f":"'Incident angle'!BN73","v":0},{"$f":"'Incident angle'!BO73","v":0},{"$f":"'Incident angle'!BP73","v":0},{"$f":"'Incident angle'!BQ73","v":0},{"$f":"'Incident angle'!BR73","v":0},{"$f":"'Incident angle'!BS73","v":686.52449229956528},{"$f":"'Incident angle'!BT73","v":739.63225428742817},{"$f":"'Incident angle'!BU73","v":205.63474171395885},null,{"$f":"'Incident angle'!BW73","v":14},{"$f":"'Incident angle'!BX73","v":0},{"$f":"'Incident angle'!BY73","v":0},{"$f":"'Incident angle'!BZ73","v":0},{"$f":"'Incident angle'!CA73","v":0},{"$f":"'Incident angle'!CB73","v":0},{"$f":"'Incident angle'!CC73","v":0},{"$f":"'Incident angle'!CD73","v":0},{"$f":"'Incident angle'!CE73","v":0},{"$f":"'Incident angle'!CF73","v":0},{"$f":"'Incident angle'!CG73","v":0},{"$f":"'Incident angle'!CH73","v":0},{"$f":"'Incident angle'!CI73","v":0},null,{"$f":"'Profile angles'!P18","v":14},{"$f":"RADIANS('Profile angles'!Q18)","v":1.000592721221816},{"$f":"RADIANS('Profile angles'!R18)","v":1.0600445287944333},{"$f":"RADIANS('Profile angles'!S18)","v":1.0718008336148819},{"$f":"RADIANS('Profile angles'!T18)","v":1.0771466448813709},{"$f":"RADIANS('Profile angles'!U18)","v":1.0979012626620424},{"$f":"RADIANS('Profile angles'!V18)","v":1.127498795680429},{"$f":"RADIANS('Profile angles'!W18)","v":1.1367031826073217},{"$f":"RADIANS('Profile angles'!X18)","v":1.0927120982101921},{"$f":"RADIANS('Profile angles'!Y18)","v":1.0030149795642187},{"$f":"RADIANS('Profile angles'!Z18)","v":0.91563513724759149},{"$f":"RADIANS('Profile angles'!AA18)","v":0.86977254162430351},{"$f":"RADIANS('Profile angles'!AB18)","v":0.91012957488156332},null,{"$f":"'Profile angles'!P47","v":14},{"$f":"RADIANS('Profile angles'!Q47)","v":-0.75851543012385236},{"$f":"RADIANS('Profile angles'!R47)","v":-0.93648395989476452},{"$f":"RADIANS('Profile angles'!S47)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!T47)","v":-1.3750301180558762},{"$f":"RADIANS('Profile angles'!U47)","v":-1.5399688677201155},{"$f":"RADIANS('Profile angles'!V47)","v":1.5457329130795117},{"$f":"RADIANS('Profile angles'!W47)","v":-1.5359564525388147},{"$f":"RADIANS('Profile angles'!X47)","v":-1.3770848532828266},{"$f":"RADIANS('Profile angles'!Y47)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!Z47)","v":-0.92031825841069459},{"$f":"RADIANS('Profile angles'!AA47)","v":-0.73756032900572732},{"$f":"RADIANS('Profile angles'!AB47)","v":-0.68075372194542327},null,{"$f":"'Profile angles'!AR18","v":14},{"$f":"(IF($AH$29<DEGREES(BS45),0+$AJ$33,1-((TAN(BS45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BT45),0+$AJ$33,1-((TAN(BT45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BU45),0+$AJ$33,1-((TAN(BU45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BV45),0+$AJ$33,1-((TAN(BV45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BW45),0+$AJ$33,1-((TAN(BW45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BX45),0+$AJ$33,1-((TAN(BX45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BY45),0+$AJ$33,1-((TAN(BY45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BZ45),0+$AJ$33,1-((TAN(BZ45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CA45),0+$AJ$33,1-((TAN(CA45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CB45),0+$AJ$33,1-((TAN(CB45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG71*$DU$3)+1-$DU$3)","v":4.4926248484207183E-2},{"$f":"(IF($AH$29<DEGREES(CC45),0+$AJ$33,1-((TAN(CC45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH71*$DU$3)+1-$DU$3)","v":5.93946620842749E-2},{"$f":"(IF($AH$29<DEGREES(CD45),0+$AJ$33,1-((TAN(CD45)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI71*$DU$3)+1-$DU$3)","v":2.0420469277158401E-2},null,14,{"$f":"(IF($AH$12<DEGREES(CG45),0+$AJ$16,1-((TAN(CG45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL71*$DU$3)+1-$DU$3)","v":1.157957073470917},{"$f":"(IF($AH$12<DEGREES(CH45),0+$AJ$16,1-((TAN(CH45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM71*$DU$3)+1-$DU$3)","v":1.2083125412674398},{"$f":"(IF($AH$12<DEGREES(CI45),0+$AJ$16,1-((TAN(CI45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN71*$DU$3)+1-$DU$3)","v":1.0277881798959112},{"$f":"(IF($AH$12<DEGREES(CJ45),0+$AJ$16,1-((TAN(CJ45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK45),0+$AJ$16,1-((TAN(CK45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL45),0+$AJ$16,1-((TAN(CL45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM45),0+$AJ$16,1-((TAN(CM45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN45),0+$AJ$16,1-((TAN(CN45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS71*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO45),0+$AJ$16,1-((TAN(CO45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT71*$DU$3)+1-$DU$3)","v":0.77325547210927992},{"$f":"(IF($AH$12<DEGREES(CP45),0+$AJ$16,1-((TAN(CP45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU71*$DU$3)+1-$DU$3)","v":0.95058383365640486},{"$f":"(IF($AH$12<DEGREES(CQ45),0+$AJ$16,1-((TAN(CQ45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV71*$DU$3)+1-$DU$3)","v":1.0086857607235808},{"$f":"(IF($AH$12<DEGREES(CR45),0+$AJ$16,1-((TAN(CR45)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW71*$DU$3)+1-$DU$3)","v":1.073790079677087},null,null,14,39.001643714284292,47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348,null,14,39.001643714284292,47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348]
[null,16,{"$f":"IF('Dry Bulb'!D20<60,(('Input Data'!$F$44*('Dry Bulb'!D20-$T$15))+('Heat gain from airflow'!Q19)+((Occupancy!P19*'Input Data'!$F$47)+(Occupancy!B19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D20-$P$15))+('Heat gain from airflow'!Q19)+((Occupancy!P19*'Input Data'!$F$47)+(Occupancy!B19*'Input Data'!$F$49))))/1000","v":-3.0736601999999986},{"$f":"IF('Dry Bulb'!E20<60,(('Input Data'!$F$44*('Dry Bulb'!E20-$T$15))+('Heat gain from airflow'!R19)+((Occupancy!Q19*'Input Data'!$F$47)+(Occupancy!C19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E20-$P$15))+('Heat gain from airflow'!R19)+((Occupancy!Q19*'Input Data'!$F$47)+(Occupancy!C19*'Input Data'!$F$49))))/1000","v":0.91411802999999514},{"$f":"IF('Dry Bulb'!F20<60,(('Input Data'!$F$44*('Dry Bulb'!F20-$T$15))+('Heat gain from airflow'!S19)+((Occupancy!R19*'Input Data'!$F$47)+(Occupancy!D19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F20-$P$15))+('Heat gain from airflow'!S19)+((Occupancy!R19*'Input Data'!$F$47)+(Occupancy!D19*'Input Data'!$F$49))))/1000","v":4.7846086649999942},{"$f":"IF('Dry Bulb'!G20<60,(('Input Data'!$F$44*('Dry Bulb'!G20-$T$15))+('Heat gain from airflow'!T19)+((Occupancy!S19*'Input Data'!$F$47)+(Occupancy!E19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G20-$P$15))+('Heat gain from airflow'!T19)+((Occupancy!S19*'Input Data'!$F$47)+(Occupancy!E19*'Input Data'!$F$49))))/1000","v":9.7289325000000026},{"$f":"IF('Dry Bulb'!H20<60,(('Input Data'!$F$44*('Dry Bulb'!H20-$T$15))+('Heat gain from airflow'!U19)+((Occupancy!T19*'Input Data'!$F$47)+(Occupancy!F19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H20-$P$15))+('Heat gain from airflow'!U19)+((Occupancy!T19*'Input Data'!$F$47)+(Occupancy!F19*'Input Data'!$F$49))))/1000","v":15.2608275},{"$f":"IF('Dry Bulb'!I20<60,(('Input Data'!$F$44*('Dry Bulb'!I20-$T$15))+('Heat gain from airflow'!V19)+((Occupancy!U19*'Input Data'!$F$47)+(Occupancy!G19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I20-$P$15))+('Heat gain from airflow'!V19)+((Occupancy!U19*'Input Data'!$F$47)+(Occupancy!G19*'Input Data'!$F$49))))/1000","v":18.980549999999997},{"$f":"IF('Dry Bulb'!J20<60,(('Input Data'!$F$44*('Dry Bulb'!J20-$T$15))+('Heat gain from airflow'!W19)+((Occupancy!V19*'Input Data'!$F$47)+(Occupancy!H19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J20-$P$15))+('Heat gain from airflow'!W19)+((Occupancy!V19*'Input Data'!$F$47)+(Occupancy!H19*'Input Data'!$F$49))))/1000","v":20.220457499999998},{"$f":"IF('Dry Bulb'!K20<60,(('Input Data'!$F$44*('Dry Bulb'!K20-$T$15))+('Heat gain from airflow'!X19)+((Occupancy!W19*'Input Data'!$F$47)+(Occupancy!I19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K20-$P$15))+('Heat gain from airflow'!X19)+((Occupancy!W19*'Input Data'!$F$47)+(Occupancy!I19*'Input Data'!$F$49))))/1000","v":20.315835},{"$f":"IF('Dry Bulb'!L20<60,(('Input Data'!$F$44*('Dry Bulb'!L20-$T$15))+('Heat gain from airflow'!Y19)+((Occupancy!X19*'Input Data'!$F$47)+(Occupancy!J19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L20-$P$15))+('Heat gain from airflow'!Y19)+((Occupancy!X19*'Input Data'!$F$47)+(Occupancy!J19*'Input Data'!$F$49))))/1000","v":16.7868675},{"$f":"IF('Dry Bulb'!M20<60,(('Input Data'!$F$44*('Dry Bulb'!M20-$T$15))+('Heat gain from airflow'!Z19)+((Occupancy!Y19*'Input Data'!$F$47)+(Occupancy!K19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M20-$P$15))+('Heat gain from airflow'!Z19)+((Occupancy!Y19*'Input Data'!$F$47)+(Occupancy!K19*'Input Data'!$F$49))))/1000","v":11.731859999999996},{"$f":"IF('Dry Bulb'!N20<60,(('Input Data'!$F$44*('Dry Bulb'!N20-$T$15))+('Heat gain from airflow'!AA19)+((Occupancy!Z19*'Input Data'!$F$47)+(Occupancy!L19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N20-$P$15))+('Heat gain from airflow'!AA19)+((Occupancy!Z19*'Input Data'!$F$47)+(Occupancy!L19*'Input Data'!$F$49))))/1000","v":6.3907200000000026},{"$f":"IF('Dry Bulb'!O20<60,(('Input Data'!$F$44*('Dry Bulb'!O20-$T$15))+('Heat gain from airflow'!AB19)+((Occupancy!AA19*'Input Data'!$F$47)+(Occupancy!M19*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O20-$P$15))+('Heat gain from airflow'!AB19)+((Occupancy!AA19*'Input Data'!$F$47)+(Occupancy!M19*'Input Data'!$F$49))))/1000","v":-2.1353594400000002},null,"WWR",{"$f":"(Q47/20)*R46","v":0.6},{"$f":"IF(R45,0,1)","v":1},null,{"$f":"24*('Input Data'!F44-Q31*Q29)","v":10125},null,null,null,4,null,null,null,null,null,null,null," Profile Angle δ=",null,{"$f":"DEGREES(AI45)","v":59.036243467926482},null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI74","v":15},{"$f":"'Incident angle'!BJ74","v":1926.5716949534467},{"$f":"'Incident angle'!BK74","v":2262.7778473297494},{"$f":"'Incident angle'!BL74","v":2635.5703218185467},{"$f":"'Incident angle'!BM74","v":2739.6260864388364},{"$f":"'Incident angle'!BN74","v":2639.208561173924},{"$f":"'Incident angle'!BO74","v":1868.8769897456732},{"$f":"'Incident angle'!BP74","v":1817.2287126262747},{"$f":"'Incident angle'!BQ74","v":2938.0781685139464},{"$f":"'Incident angle'!BR74","v":3923.7505691865708},{"$f":"'Incident angle'!BS74","v":3823.612360059843},{"$f":"'Incident angle'!BT74","v":2779.6028668421336},{"$f":"'Incident angle'!BU74","v":1919.6025015893795},null,{"$f":"'Incident angle'!BW74","v":15},{"$f":"'Incident angle'!BX74","v":0},{"$f":"'Incident angle'!BY74","v":0},{"$f":"'Incident angle'!BZ74","v":0},{"$f":"'Incident angle'!CA74","v":0},{"$f":"'Incident angle'!CB74","v":0},{"$f":"'Incident angle'!CC74","v":0},{"$f":"'Incident angle'!CD74","v":0},{"$f":"'Incident angle'!CE74","v":0},{"$f":"'Incident angle'!CF74","v":0},{"$f":"'Incident angle'!CG74","v":0},{"$f":"'Incident angle'!CH74","v":0},{"$f":"'Incident angle'!CI74","v":0},null,{"$f":"'Profile angles'!P19","v":15},{"$f":"RADIANS('Profile angles'!Q19)","v":0.69486770530695274},{"$f":"RADIANS('Profile angles'!R19)","v":0.77035987910152948},{"$f":"RADIANS('Profile angles'!S19)","v":0.80144392257758212},{"$f":"RADIANS('Profile angles'!T19)","v":0.82641496006128057},{"$f":"RADIANS('Profile angles'!U19)","v":0.86009108801295264},{"$f":"RADIANS('Profile angles'!V19)","v":0.89419996525178802},{"$f":"RADIANS('Profile angles'!W19)","v":0.89834850121998655},{"$f":"RADIANS('Profile angles'!X19)","v":0.84181932575908713},{"$f":"RADIANS('Profile angles'!Y19)","v":0.73590361062962995},{"$f":"RADIANS('Profile angles'!Z19)","v":0.63537560318144093},{"$f":"RADIANS('Profile angles'!AA19)","v":0.57579270320512765},{"$f":"RADIANS('Profile angles'!AB19)","v":0.6044646480538286},null,{"$f":"'Profile angles'!P48","v":15},{"$f":"RADIANS('Profile angles'!Q48)","v":-0.69587256018196952},{"$f":"RADIANS('Profile angles'!R48)","v":-0.90095965651819487},{"$f":"RADIANS('Profile angles'!S48)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T48)","v":-1.4223966034161182},{"$f":"RADIANS('Profile angles'!U48)","v":1.5266344477385527},{"$f":"RADIANS('Profile angles'!V48)","v":1.4675022187003639},{"$f":"RADIANS('Profile angles'!W48)","v":1.5378465881867287},{"$f":"RADIANS('Profile angles'!X48)","v":-1.4231733271709055},{"$f":"RADIANS('Profile angles'!Y48)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!Z48)","v":-0.86910144352535146},{"$f":"RADIANS('Profile angles'!AA48)","v":-0.65429236322323236},{"$f":"RADIANS('Profile angles'!AB48)","v":-0.59989785402553941},null,{"$f":"'Profile angles'!AR19","v":15},{"$f":"(IF($AH$29<DEGREES(BS46),0+$AJ$33,1-((TAN(BS46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX72*$DU$3)+1-$DU$3)","v":0.20868154488909321},{"$f":"(IF($AH$29<DEGREES(BT46),0+$AJ$33,1-((TAN(BT46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY72*$DU$3)+1-$DU$3)","v":0.19749455227413368},{"$f":"(IF($AH$29<DEGREES(BU46),0+$AJ$33,1-((TAN(BU46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ72*$DU$3)+1-$DU$3)","v":0.21134708662592586},{"$f":"(IF($AH$29<DEGREES(BV46),0+$AJ$33,1-((TAN(BV46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA72*$DU$3)+1-$DU$3)","v":0.2206030796298433},{"$f":"(IF($AH$29<DEGREES(BW46),0+$AJ$33,1-((TAN(BW46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB72*$DU$3)+1-$DU$3)","v":0.18196700048290834},{"$f":"(IF($AH$29<DEGREES(BX46),0+$AJ$33,1-((TAN(BX46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC72*$DU$3)+1-$DU$3)","v":0.12003820366778506},{"$f":"(IF($AH$29<DEGREES(BY46),0+$AJ$33,1-((TAN(BY46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD72*$DU$3)+1-$DU$3)","v":0.1183730022320196},{"$f":"(IF($AH$29<DEGREES(BZ46),0+$AJ$33,1-((TAN(BZ46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE72*$DU$3)+1-$DU$3)","v":0.19819396512455364},{"$f":"(IF($AH$29<DEGREES(CA46),0+$AJ$33,1-((TAN(CA46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF72*$DU$3)+1-$DU$3)","v":0.28983474395096065},{"$f":"(IF($AH$29<DEGREES(CB46),0+$AJ$33,1-((TAN(CB46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG72*$DU$3)+1-$DU$3)","v":0.33306465488217968},{"$f":"(IF($AH$29<DEGREES(CC46),0+$AJ$33,1-((TAN(CC46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH72*$DU$3)+1-$DU$3)","v":0.31469640298951801},{"$f":"(IF($AH$29<DEGREES(CD46),0+$AJ$33,1-((TAN(CD46)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI72*$DU$3)+1-$DU$3)","v":0.25571216942973429},null,15,{"$f":"(IF($AH$12<DEGREES(CG46),0+$AJ$16,1-((TAN(CG46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL72*$DU$3)+1-$DU$3)","v":0.79071980300953448},{"$f":"(IF($AH$12<DEGREES(CH46),0+$AJ$16,1-((TAN(CH46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM72*$DU$3)+1-$DU$3)","v":0.65821427477842498},{"$f":"(IF($AH$12<DEGREES(CI46),0+$AJ$16,1-((TAN(CI46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN72*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ46),0+$AJ$16,1-((TAN(CJ46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO72*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK46),0+$AJ$16,1-((TAN(CK46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP72*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL46),0+$AJ$16,1-((TAN(CL46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ72*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM46),0+$AJ$16,1-((TAN(CM46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR72*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN46),0+$AJ$16,1-((TAN(CN46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS72*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO46),0+$AJ$16,1-((TAN(CO46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT72*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP46),0+$AJ$16,1-((TAN(CP46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU72*$DU$3)+1-$DU$3)","v":0.36148132152558898},{"$f":"(IF($AH$12<DEGREES(CQ46),0+$AJ$16,1-((TAN(CQ46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV72*$DU$3)+1-$DU$3)","v":0.62897237282734864},{"$f":"(IF($AH$12<DEGREES(CR46),0+$AJ$16,1-((TAN(CR46)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW72*$DU$3)+1-$DU$3)","v":0.74659372850677441},null,null,15,30.541133571003865,37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655,null,15,30.541133571003865,37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655]
[null,17,{"$f":"IF('Dry Bulb'!D21<60,(('Input Data'!$F$44*('Dry Bulb'!D21-$T$15))+('Heat gain from airflow'!Q20)+((Occupancy!P20*'Input Data'!$F$47)+(Occupancy!B20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D21-$P$15))+('Heat gain from airflow'!Q20)+((Occupancy!P20*'Input Data'!$F$47)+(Occupancy!B20*'Input Data'!$F$49))))/1000","v":-3.7773857699999973},{"$f":"IF('Dry Bulb'!E21<60,(('Input Data'!$F$44*('Dry Bulb'!E21-$T$15))+('Heat gain from airflow'!R20)+((Occupancy!Q20*'Input Data'!$F$47)+(Occupancy!C20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E21-$P$15))+('Heat gain from airflow'!R20)+((Occupancy!Q20*'Input Data'!$F$47)+(Occupancy!C20*'Input Data'!$F$49))))/1000","v":-2.4182730000003174E-2},{"$f":"IF('Dry Bulb'!F21<60,(('Input Data'!$F$44*('Dry Bulb'!F21-$T$15))+('Heat gain from airflow'!S20)+((Occupancy!R20*'Input Data'!$F$47)+(Occupancy!D20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F21-$P$15))+('Heat gain from airflow'!S20)+((Occupancy!R20*'Input Data'!$F$47)+(Occupancy!D20*'Input Data'!$F$49))))/1000","v":4.0808830950000043},{"$f":"IF('Dry Bulb'!G21<60,(('Input Data'!$F$44*('Dry Bulb'!G21-$T$15))+('Heat gain from airflow'!T20)+((Occupancy!S20*'Input Data'!$F$47)+(Occupancy!E20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G21-$P$15))+('Heat gain from airflow'!T20)+((Occupancy!S20*'Input Data'!$F$47)+(Occupancy!E20*'Input Data'!$F$49))))/1000","v":8.8705350000000003},{"$f":"IF('Dry Bulb'!H21<60,(('Input Data'!$F$44*('Dry Bulb'!H21-$T$15))+('Heat gain from airflow'!U20)+((Occupancy!T20*'Input Data'!$F$47)+(Occupancy!F20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H21-$P$15))+('Heat gain from airflow'!U20)+((Occupancy!T20*'Input Data'!$F$47)+(Occupancy!F20*'Input Data'!$F$49))))/1000","v":15.165449999999996},{"$f":"IF('Dry Bulb'!I21<60,(('Input Data'!$F$44*('Dry Bulb'!I21-$T$15))+('Heat gain from airflow'!V20)+((Occupancy!U20*'Input Data'!$F$47)+(Occupancy!G20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I21-$P$15))+('Heat gain from airflow'!V20)+((Occupancy!U20*'Input Data'!$F$47)+(Occupancy!G20*'Input Data'!$F$49))))/1000","v":18.599040000000009},{"$f":"IF('Dry Bulb'!J21<60,(('Input Data'!$F$44*('Dry Bulb'!J21-$T$15))+('Heat gain from airflow'!W20)+((Occupancy!V20*'Input Data'!$F$47)+(Occupancy!H20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J21-$P$15))+('Heat gain from airflow'!W20)+((Occupancy!V20*'Input Data'!$F$47)+(Occupancy!H20*'Input Data'!$F$49))))/1000","v":19.934324999999998},{"$f":"IF('Dry Bulb'!K21<60,(('Input Data'!$F$44*('Dry Bulb'!K21-$T$15))+('Heat gain from airflow'!X20)+((Occupancy!W20*'Input Data'!$F$47)+(Occupancy!I20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K21-$P$15))+('Heat gain from airflow'!X20)+((Occupancy!W20*'Input Data'!$F$47)+(Occupancy!I20*'Input Data'!$F$49))))/1000","v":19.648192499999997},{"$f":"IF('Dry Bulb'!L21<60,(('Input Data'!$F$44*('Dry Bulb'!L21-$T$15))+('Heat gain from airflow'!Y20)+((Occupancy!X20*'Input Data'!$F$47)+(Occupancy!J20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L21-$P$15))+('Heat gain from airflow'!Y20)+((Occupancy!X20*'Input Data'!$F$47)+(Occupancy!J20*'Input Data'!$F$49))))/1000","v":16.023847499999999},{"$f":"IF('Dry Bulb'!M21<60,(('Input Data'!$F$44*('Dry Bulb'!M21-$T$15))+('Heat gain from airflow'!Z20)+((Occupancy!Y20*'Input Data'!$F$47)+(Occupancy!K20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M21-$P$15))+('Heat gain from airflow'!Z20)+((Occupancy!Y20*'Input Data'!$F$47)+(Occupancy!K20*'Input Data'!$F$49))))/1000","v":11.159594999999996},{"$f":"IF('Dry Bulb'!N21<60,(('Input Data'!$F$44*('Dry Bulb'!N21-$T$15))+('Heat gain from airflow'!AA20)+((Occupancy!Z20*'Input Data'!$F$47)+(Occupancy!L20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N21-$P$15))+('Heat gain from airflow'!AA20)+((Occupancy!Z20*'Input Data'!$F$47)+(Occupancy!L20*'Input Data'!$F$49))))/1000","v":5.5323225000000003},{"$f":"IF('Dry Bulb'!O21<60,(('Input Data'!$F$44*('Dry Bulb'!O21-$T$15))+('Heat gain from airflow'!AB20)+((Occupancy!AA20*'Input Data'!$F$47)+(Occupancy!M20*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O21-$P$15))+('Heat gain from airflow'!AB20)+((Occupancy!AA20*'Input Data'!$F$47)+(Occupancy!M20*'Input Data'!$F$49))))/1000","v":-3.4255229850000033},null,null,12,null,null,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI75","v":16},{"$f":"'Incident angle'!BJ75","v":2774.6294384683138},{"$f":"'Incident angle'!BK75","v":3734.587299212772},{"$f":"'Incident angle'!BL75","v":4446.8095707895973},{"$f":"'Incident angle'!BM75","v":4774.3448944164402},{"$f":"'Incident angle'!BN75","v":4971.3533893484409},{"$f":"'Incident angle'!BO75","v":4803.02801605271},{"$f":"'Incident angle'!BP75","v":4929.1205423900001},{"$f":"'Incident angle'!BQ75","v":5622.3905501017762},{"$f":"'Incident angle'!BR75","v":5190.4573655804825},{"$f":"'Incident angle'!BS75","v":4062.4502685123566},{"$f":"'Incident angle'!BT75","v":2589.6992330867606},{"$f":"'Incident angle'!BU75","v":2164.3138343325777},null,{"$f":"'Incident angle'!BW75","v":16},{"$f":"'Incident angle'!BX75","v":0},{"$f":"'Incident angle'!BY75","v":0},{"$f":"'Incident angle'!BZ75","v":0},{"$f":"'Incident angle'!CA75","v":0},{"$f":"'Incident angle'!CB75","v":0},{"$f":"'Incident angle'!CC75","v":0},{"$f":"'Incident angle'!CD75","v":0},{"$f":"'Incident angle'!CE75","v":0},{"$f":"'Incident angle'!CF75","v":0},{"$f":"'Incident angle'!CG75","v":0},{"$f":"'Incident angle'!CH75","v":0},{"$f":"'Incident angle'!CI75","v":0},null,{"$f":"'Profile angles'!P20","v":16},{"$f":"RADIANS('Profile angles'!Q20)","v":0.41669740220816487},{"$f":"RADIANS('Profile angles'!R20)","v":0.50015077980007105},{"$f":"RADIANS('Profile angles'!S20)","v":0.54404800401822806},{"$f":"RADIANS('Profile angles'!T20)","v":0.58351428900426172},{"$f":"RADIANS('Profile angles'!U20)","v":0.62746556362485806},{"$f":"RADIANS('Profile angles'!V20)","v":0.66533748077630195},{"$f":"RADIANS('Profile angles'!W20)","v":0.66523823915225477},{"$f":"RADIANS('Profile angles'!X20)","v":0.59872473938789039},{"$f":"RADIANS('Profile angles'!Y20)","v":0.48155681326357536},{"$f":"RADIANS('Profile angles'!Z20)","v":0.37388412364806317},{"$f":"RADIANS('Profile angles'!AA20)","v":0.30789644489665746},{"$f":"RADIANS('Profile angles'!AB20)","v":0.32941416658746181},null,{"$f":"'Profile angles'!P49","v":16},{"$f":"RADIANS('Profile angles'!Q49)","v":-0.57197798027671087},{"$f":"RADIANS('Profile angles'!R49)","v":-0.82619821336401},{"$f":"RADIANS('Profile angles'!S49)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!T49)","v":-1.5229810963446622},{"$f":"RADIANS('Profile angles'!U49)","v":1.3784680894840018},{"$f":"RADIANS('Profile angles'!V49)","v":1.3177516582315827},{"$f":"RADIANS('Profile angles'!W49)","v":1.4044440508792544},{"$f":"RADIANS('Profile angles'!X49)","v":-1.5204461167120875},{"$f":"RADIANS('Profile angles'!Y49)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!Z49)","v":-0.75629963516330256},{"$f":"RADIANS('Profile angles'!AA49)","v":-0.48809734520255904},{"$f":"RADIANS('Profile angles'!AB49)","v":-0.44518009228857974},null,{"$f":"'Profile angles'!AR20","v":16},{"$f":"(IF($AH$29<DEGREES(BS47),0+$AJ$33,1-((TAN(BS47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX73*$DU$3)+1-$DU$3)","v":0.45290652225986694},{"$f":"(IF($AH$29<DEGREES(BT47),0+$AJ$33,1-((TAN(BT47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY73*$DU$3)+1-$DU$3)","v":0.46196796081147512},{"$f":"(IF($AH$29<DEGREES(BU47),0+$AJ$33,1-((TAN(BU47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ73*$DU$3)+1-$DU$3)","v":0.49632901547601832},{"$f":"(IF($AH$29<DEGREES(BV47),0+$AJ$33,1-((TAN(BV47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA73*$DU$3)+1-$DU$3)","v":0.52936205000611003},{"$f":"(IF($AH$29<DEGREES(BW47),0+$AJ$33,1-((TAN(BW47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB73*$DU$3)+1-$DU$3)","v":0.45756594059614919},{"$f":"(IF($AH$29<DEGREES(BX47),0+$AJ$33,1-((TAN(BX47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC73*$DU$3)+1-$DU$3)","v":0.40498717448435501},{"$f":"(IF($AH$29<DEGREES(BY47),0+$AJ$33,1-((TAN(BY47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD73*$DU$3)+1-$DU$3)","v":0.42113426254969633},{"$f":"(IF($AH$29<DEGREES(BZ47),0+$AJ$33,1-((TAN(BZ47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE73*$DU$3)+1-$DU$3)","v":0.51343295699103364},{"$f":"(IF($AH$29<DEGREES(CA47),0+$AJ$33,1-((TAN(CA47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF73*$DU$3)+1-$DU$3)","v":0.55796803909378434},{"$f":"(IF($AH$29<DEGREES(CB47),0+$AJ$33,1-((TAN(CB47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG73*$DU$3)+1-$DU$3)","v":0.57453749025077872},{"$f":"(IF($AH$29<DEGREES(CC47),0+$AJ$33,1-((TAN(CC47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH73*$DU$3)+1-$DU$3)","v":0.54458400872179935},{"$f":"(IF($AH$29<DEGREES(CD47),0+$AJ$33,1-((TAN(CD47)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI73*$DU$3)+1-$DU$3)","v":0.48816454897346084},null,16,{"$f":"(IF($AH$12<DEGREES(CG47),0+$AJ$16,1-((TAN(CG47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL73*$DU$3)+1-$DU$3)","v":0.39569959018392065},{"$f":"(IF($AH$12<DEGREES(CH47),0+$AJ$16,1-((TAN(CH47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM73*$DU$3)+1-$DU$3)","v":1.2679870208358885E-2},{"$f":"(IF($AH$12<DEGREES(CI47),0+$AJ$16,1-((TAN(CI47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN73*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ47),0+$AJ$16,1-((TAN(CJ47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO73*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK47),0+$AJ$16,1-((TAN(CK47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP73*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL47),0+$AJ$16,1-((TAN(CL47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ73*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM47),0+$AJ$16,1-((TAN(CM47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR73*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN47),0+$AJ$16,1-((TAN(CN47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS73*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO47),0+$AJ$16,1-((TAN(CO47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT73*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP47),0+$AJ$16,1-((TAN(CP47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU73*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ47),0+$AJ$16,1-((TAN(CQ47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV73*$DU$3)+1-$DU$3)","v":0.2266035838034432},{"$f":"(IF($AH$12<DEGREES(CR47),0+$AJ$16,1-((TAN(CR47)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW73*$DU$3)+1-$DU$3)","v":0.40311163135343497},null,null,16,20.038281727598083,26.016647471873153,30.233879108991232,33.419767540103443,35.682648220686666,37.56104623172925,37.876258416390314,34.288646107643089,26.935985833021654,19.913519068774189,15.259931573481456,15.530455637101428,null,{"$f":"EK20","v":16},20.038281727598083,26.016647471873153,30.233879108991232,33.419767540103443,35.682648220686666,37.56104623172925,37.876258416390314,34.288646107643089,26.935985833021654,19.913519068774189,15.259931573481456,15.530455637101428]
[null,18,{"$f":"IF('Dry Bulb'!D22<60,(('Input Data'!$F$44*('Dry Bulb'!D22-$T$15))+('Heat gain from airflow'!Q21)+((Occupancy!P21*'Input Data'!$F$47)+(Occupancy!B21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D22-$P$15))+('Heat gain from airflow'!Q21)+((Occupancy!P21*'Input Data'!$F$47)+(Occupancy!B21*'Input Data'!$F$49))))/1000","v":-3.52854},{"$f":"IF('Dry Bulb'!E22<60,(('Input Data'!$F$44*('Dry Bulb'!E22-$T$15))+('Heat gain from airflow'!R21)+((Occupancy!Q21*'Input Data'!$F$47)+(Occupancy!C21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E22-$P$15))+('Heat gain from airflow'!R21)+((Occupancy!Q21*'Input Data'!$F$47)+(Occupancy!C21*'Input Data'!$F$49))))/1000","v":-1.1970586800000018},{"$f":"IF('Dry Bulb'!F22<60,(('Input Data'!$F$44*('Dry Bulb'!F22-$T$15))+('Heat gain from airflow'!S21)+((Occupancy!R21*'Input Data'!$F$47)+(Occupancy!D21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F22-$P$15))+('Heat gain from airflow'!S21)+((Occupancy!R21*'Input Data'!$F$47)+(Occupancy!D21*'Input Data'!$F$49))))/1000","v":3.2598699300000007},{"$f":"IF('Dry Bulb'!G22<60,(('Input Data'!$F$44*('Dry Bulb'!G22-$T$15))+('Heat gain from airflow'!T21)+((Occupancy!S21*'Input Data'!$F$47)+(Occupancy!E21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G22-$P$15))+('Heat gain from airflow'!T21)+((Occupancy!S21*'Input Data'!$F$47)+(Occupancy!E21*'Input Data'!$F$49))))/1000","v":8.1075150000000011},{"$f":"IF('Dry Bulb'!H22<60,(('Input Data'!$F$44*('Dry Bulb'!H22-$T$15))+('Heat gain from airflow'!U21)+((Occupancy!T21*'Input Data'!$F$47)+(Occupancy!F21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H22-$P$15))+('Heat gain from airflow'!U21)+((Occupancy!T21*'Input Data'!$F$47)+(Occupancy!F21*'Input Data'!$F$49))))/1000","v":14.4978075},{"$f":"IF('Dry Bulb'!I22<60,(('Input Data'!$F$44*('Dry Bulb'!I22-$T$15))+('Heat gain from airflow'!V21)+((Occupancy!U21*'Input Data'!$F$47)+(Occupancy!G21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I22-$P$15))+('Heat gain from airflow'!V21)+((Occupancy!U21*'Input Data'!$F$47)+(Occupancy!G21*'Input Data'!$F$49))))/1000","v":18.122152500000002},{"$f":"IF('Dry Bulb'!J22<60,(('Input Data'!$F$44*('Dry Bulb'!J22-$T$15))+('Heat gain from airflow'!W21)+((Occupancy!V21*'Input Data'!$F$47)+(Occupancy!H21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J22-$P$15))+('Heat gain from airflow'!W21)+((Occupancy!V21*'Input Data'!$F$47)+(Occupancy!H21*'Input Data'!$F$49))))/1000","v":19.171305},{"$f":"IF('Dry Bulb'!K22<60,(('Input Data'!$F$44*('Dry Bulb'!K22-$T$15))+('Heat gain from airflow'!X21)+((Occupancy!W21*'Input Data'!$F$47)+(Occupancy!I21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K22-$P$15))+('Heat gain from airflow'!X21)+((Occupancy!W21*'Input Data'!$F$47)+(Occupancy!I21*'Input Data'!$F$49))))/1000","v":18.789794999999998},{"$f":"IF('Dry Bulb'!L22<60,(('Input Data'!$F$44*('Dry Bulb'!L22-$T$15))+('Heat gain from airflow'!Y21)+((Occupancy!X21*'Input Data'!$F$47)+(Occupancy!J21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L22-$P$15))+('Heat gain from airflow'!Y21)+((Occupancy!X21*'Input Data'!$F$47)+(Occupancy!J21*'Input Data'!$F$49))))/1000","v":15.451582500000001},{"$f":"IF('Dry Bulb'!M22<60,(('Input Data'!$F$44*('Dry Bulb'!M22-$T$15))+('Heat gain from airflow'!Z21)+((Occupancy!Y21*'Input Data'!$F$47)+(Occupancy!K21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M22-$P$15))+('Heat gain from airflow'!Z21)+((Occupancy!Y21*'Input Data'!$F$47)+(Occupancy!K21*'Input Data'!$F$49))))/1000","v":10.396574999999997},{"$f":"IF('Dry Bulb'!N22<60,(('Input Data'!$F$44*('Dry Bulb'!N22-$T$15))+('Heat gain from airflow'!AA21)+((Occupancy!Z21*'Input Data'!$F$47)+(Occupancy!L21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N22-$P$15))+('Heat gain from airflow'!AA21)+((Occupancy!Z21*'Input Data'!$F$47)+(Occupancy!L21*'Input Data'!$F$49))))/1000","v":4.5500334750000038},{"$f":"IF('Dry Bulb'!O22<60,(('Input Data'!$F$44*('Dry Bulb'!O22-$T$15))+('Heat gain from airflow'!AB21)+((Occupancy!AA21*'Input Data'!$F$47)+(Occupancy!M21*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O22-$P$15))+('Heat gain from airflow'!AB21)+((Occupancy!AA21*'Input Data'!$F$47)+(Occupancy!M21*'Input Data'!$F$49))))/1000","v":-2.9562749999999971},null,null,null,null,null,"LOSS RATE",null,null,null,6,null,null,null,null,null,null,null,null,{"$f":"RADIANS(AH46)","v":1.0303768265243125},null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI76","v":17},{"$f":"'Incident angle'!BJ76","v":1591.2164963126143},{"$f":"'Incident angle'!BK76","v":2655.3121550436108},{"$f":"'Incident angle'!BL76","v":3490.2420072817777},{"$f":"'Incident angle'!BM76","v":3580.241138149192},{"$f":"'Incident angle'!BN76","v":3849.9681326621317},{"$f":"'Incident angle'!BO76","v":4187.313761054791},{"$f":"'Incident angle'!BP76","v":4292.2891157890799},{"$f":"'Incident angle'!BQ76","v":4423.2439261434729},{"$f":"'Incident angle'!BR76","v":3470.8202131864714},{"$f":"'Incident angle'!BS76","v":1880.8404833431982},{"$f":"'Incident angle'!BT76","v":695.47656043259258},{"$f":"'Incident angle'!BU76","v":766.73880398976189},null,{"$f":"'Incident angle'!BW76","v":17},{"$f":"'Incident angle'!BX76","v":0},{"$f":"'Incident angle'!BY76","v":0},{"$f":"'Incident angle'!BZ76","v":0},{"$f":"'Incident angle'!CA76","v":0},{"$f":"'Incident angle'!CB76","v":0},{"$f":"'Incident angle'!CC76","v":0},{"$f":"'Incident angle'!CD76","v":0},{"$f":"'Incident angle'!CE76","v":0},{"$f":"'Incident angle'!CF76","v":0},{"$f":"'Incident angle'!CG76","v":0},{"$f":"'Incident angle'!CH76","v":0},{"$f":"'Incident angle'!CI76","v":0},null,{"$f":"'Profile angles'!P21","v":17},{"$f":"RADIANS('Profile angles'!Q21)","v":0.16124242777223324},{"$f":"RADIANS('Profile angles'!R21)","v":0.24682095640962623},{"$f":"RADIANS('Profile angles'!S21)","v":0.29766243646613288},{"$f":"RADIANS('Profile angles'!T21)","v":0.34652947246442356},{"$f":"RADIANS('Profile angles'!U21)","v":0.39810829518922264},{"$f":"RADIANS('Profile angles'!V21)","v":0.43915625637623368},{"$f":"RADIANS('Profile angles'!W21)","v":0.43577963764801336},{"$f":"RADIANS('Profile angles'!X21)","v":0.36165127468574843},{"$f":"RADIANS('Profile angles'!Y21)","v":0.2373188382783232},{"$f":"RADIANS('Profile angles'!Z21)","v":0.12693435438886347},{"$f":"RADIANS('Profile angles'!AA21)","v":5.9792925815892878E-2},{"$f":"RADIANS('Profile angles'!AB21)","v":7.8011009216174293E-2},null,{"$f":"'Profile angles'!P50","v":17},{"$f":"RADIANS('Profile angles'!Q50)","v":-0.31585481016596434},{"$f":"RADIANS('Profile angles'!R50)","v":-0.64419111865687917},{"$f":"RADIANS('Profile angles'!S50)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T50)","v":1.3637805005768209},{"$f":"RADIANS('Profile angles'!U50)","v":1.0702663972279509},{"$f":"RADIANS('Profile angles'!V50)","v":1.0276883038342117},{"$f":"RADIANS('Profile angles'!W50)","v":1.1305109275476111},{"$f":"RADIANS('Profile angles'!X50)","v":1.3794764235329204},{"$f":"RADIANS('Profile angles'!Y50)","v":-1.1397000015522969},{"$f":"RADIANS('Profile angles'!Z50)","v":-0.43856842576519417},{"$f":"RADIANS('Profile angles'!AA50)","v":-0.13613500526814387},{"$f":"RADIANS('Profile angles'!AB50)","v":-0.14545482072436788},null,{"$f":"'Profile angles'!AR21","v":17},{"$f":"(IF($AH$29<DEGREES(BS48),0+$AJ$33,1-((TAN(BS48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX74*$DU$3)+1-$DU$3)","v":0.66561393736738939},{"$f":"(IF($AH$29<DEGREES(BT48),0+$AJ$33,1-((TAN(BT48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY74*$DU$3)+1-$DU$3)","v":0.68548103045370146},{"$f":"(IF($AH$29<DEGREES(BU48),0+$AJ$33,1-((TAN(BU48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ74*$DU$3)+1-$DU$3)","v":0.72985575444174644},{"$f":"(IF($AH$29<DEGREES(BV48),0+$AJ$33,1-((TAN(BV48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA74*$DU$3)+1-$DU$3)","v":0.7188947002762579},{"$f":"(IF($AH$29<DEGREES(BW48),0+$AJ$33,1-((TAN(BW48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB74*$DU$3)+1-$DU$3)","v":0.62444392824715755},{"$f":"(IF($AH$29<DEGREES(BX48),0+$AJ$33,1-((TAN(BX48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC74*$DU$3)+1-$DU$3)","v":0.57601217607571131},{"$f":"(IF($AH$29<DEGREES(BY48),0+$AJ$33,1-((TAN(BY48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD74*$DU$3)+1-$DU$3)","v":0.60012030245874803},{"$f":"(IF($AH$29<DEGREES(BZ48),0+$AJ$33,1-((TAN(BZ48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE74*$DU$3)+1-$DU$3)","v":0.708263403695373},{"$f":"(IF($AH$29<DEGREES(CA48),0+$AJ$33,1-((TAN(CA48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF74*$DU$3)+1-$DU$3)","v":0.78447891700523542},{"$f":"(IF($AH$29<DEGREES(CB48),0+$AJ$33,1-((TAN(CB48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG74*$DU$3)+1-$DU$3)","v":0.78677280706620667},{"$f":"(IF($AH$29<DEGREES(CC48),0+$AJ$33,1-((TAN(CC48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH74*$DU$3)+1-$DU$3)","v":0.74874063850757366},{"$f":"(IF($AH$29<DEGREES(CD48),0+$AJ$33,1-((TAN(CD48)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI74*$DU$3)+1-$DU$3)","v":0.69307080766632501},null,17,{"$f":"(IF($AH$12<DEGREES(CG48),0+$AJ$16,1-((TAN(CG48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH48),0+$AJ$16,1-((TAN(CH48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI48),0+$AJ$16,1-((TAN(CI48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ48),0+$AJ$16,1-((TAN(CJ48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK48),0+$AJ$16,1-((TAN(CK48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL48),0+$AJ$16,1-((TAN(CL48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM48),0+$AJ$16,1-((TAN(CM48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN48),0+$AJ$16,1-((TAN(CN48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO48),0+$AJ$16,1-((TAN(CO48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP48),0+$AJ$16,1-((TAN(CP48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ48),0+$AJ$16,1-((TAN(CQ48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV74*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR48),0+$AJ$16,1-((TAN(CR48)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW74*$DU$3)+1-$DU$3)","v":6.9463985965016475E-2},null,null,17,8.2848854255444504,13.434807821200849,16.897092448538277,19.80224832363653,22.286756355186323,24.319689951925163,24.456964963286701,20.670382142796534,13.51706337533537,7.0202572324504446,3.1397975005302774,3.9451572875932328,null,17,8.2848854255444504,13.434807821200849,16.897092448538277,19.80224832363653,22.286756355186323,24.319689951925163,24.456964963286701,20.670382142796534,13.51706337533537,7.0202572324504446,3.1397975005302774,3.9451572875932328]
[null,19,{"$f":"IF('Dry Bulb'!D23<60,(('Input Data'!$F$44*('Dry Bulb'!D23-$T$15))+('Heat gain from airflow'!Q22)+((Occupancy!P22*'Input Data'!$F$47)+(Occupancy!B22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D23-$P$15))+('Heat gain from airflow'!Q22)+((Occupancy!P22*'Input Data'!$F$47)+(Occupancy!B22*'Input Data'!$F$49))))/1000","v":-4.4823150000000025},{"$f":"IF('Dry Bulb'!E23<60,(('Input Data'!$F$44*('Dry Bulb'!E23-$T$15))+('Heat gain from airflow'!R22)+((Occupancy!Q22*'Input Data'!$F$47)+(Occupancy!C22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E23-$P$15))+('Heat gain from airflow'!R22)+((Occupancy!Q22*'Input Data'!$F$47)+(Occupancy!C22*'Input Data'!$F$49))))/1000","v":-2.3699346299999999},{"$f":"IF('Dry Bulb'!F23<60,(('Input Data'!$F$44*('Dry Bulb'!F23-$T$15))+('Heat gain from airflow'!S22)+((Occupancy!R22*'Input Data'!$F$47)+(Occupancy!D22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F23-$P$15))+('Heat gain from airflow'!S22)+((Occupancy!R22*'Input Data'!$F$47)+(Occupancy!D22*'Input Data'!$F$49))))/1000","v":2.2042815749999978},{"$f":"IF('Dry Bulb'!G23<60,(('Input Data'!$F$44*('Dry Bulb'!G23-$T$15))+('Heat gain from airflow'!T22)+((Occupancy!S22*'Input Data'!$F$47)+(Occupancy!E22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G23-$P$15))+('Heat gain from airflow'!T22)+((Occupancy!S22*'Input Data'!$F$47)+(Occupancy!E22*'Input Data'!$F$49))))/1000","v":6.7722299999999951},{"$f":"IF('Dry Bulb'!H23<60,(('Input Data'!$F$44*('Dry Bulb'!H23-$T$15))+('Heat gain from airflow'!U22)+((Occupancy!T22*'Input Data'!$F$47)+(Occupancy!F22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H23-$P$15))+('Heat gain from airflow'!U22)+((Occupancy!T22*'Input Data'!$F$47)+(Occupancy!F22*'Input Data'!$F$49))))/1000","v":13.63941},{"$f":"IF('Dry Bulb'!I23<60,(('Input Data'!$F$44*('Dry Bulb'!I23-$T$15))+('Heat gain from airflow'!V22)+((Occupancy!U22*'Input Data'!$F$47)+(Occupancy!G22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I23-$P$15))+('Heat gain from airflow'!V22)+((Occupancy!U22*'Input Data'!$F$47)+(Occupancy!G22*'Input Data'!$F$49))))/1000","v":17.073},{"$f":"IF('Dry Bulb'!J23<60,(('Input Data'!$F$44*('Dry Bulb'!J23-$T$15))+('Heat gain from airflow'!W22)+((Occupancy!V22*'Input Data'!$F$47)+(Occupancy!H22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J23-$P$15))+('Heat gain from airflow'!W22)+((Occupancy!V22*'Input Data'!$F$47)+(Occupancy!H22*'Input Data'!$F$49))))/1000","v":17.836020000000001},{"$f":"IF('Dry Bulb'!K23<60,(('Input Data'!$F$44*('Dry Bulb'!K23-$T$15))+('Heat gain from airflow'!X22)+((Occupancy!W22*'Input Data'!$F$47)+(Occupancy!I22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K23-$P$15))+('Heat gain from airflow'!X22)+((Occupancy!W22*'Input Data'!$F$47)+(Occupancy!I22*'Input Data'!$F$49))))/1000","v":17.549887499999997},{"$f":"IF('Dry Bulb'!L23<60,(('Input Data'!$F$44*('Dry Bulb'!L23-$T$15))+('Heat gain from airflow'!Y22)+((Occupancy!X22*'Input Data'!$F$47)+(Occupancy!J22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L23-$P$15))+('Heat gain from airflow'!Y22)+((Occupancy!X22*'Input Data'!$F$47)+(Occupancy!J22*'Input Data'!$F$49))))/1000","v":14.4978075},{"$f":"IF('Dry Bulb'!M23<60,(('Input Data'!$F$44*('Dry Bulb'!M23-$T$15))+('Heat gain from airflow'!Z22)+((Occupancy!Y22*'Input Data'!$F$47)+(Occupancy!K22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M23-$P$15))+('Heat gain from airflow'!Z22)+((Occupancy!Y22*'Input Data'!$F$47)+(Occupancy!K22*'Input Data'!$F$49))))/1000","v":9.3474224999999933},{"$f":"IF('Dry Bulb'!N23<60,(('Input Data'!$F$44*('Dry Bulb'!N23-$T$15))+('Heat gain from airflow'!AA22)+((Occupancy!Z22*'Input Data'!$F$47)+(Occupancy!L22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N23-$P$15))+('Heat gain from airflow'!AA22)+((Occupancy!Z22*'Input Data'!$F$47)+(Occupancy!L22*'Input Data'!$F$49))))/1000","v":3.2598699300000007},{"$f":"IF('Dry Bulb'!O23<60,(('Input Data'!$F$44*('Dry Bulb'!O23-$T$15))+('Heat gain from airflow'!AB22)+((Occupancy!AA22*'Input Data'!$F$47)+(Occupancy!M22*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O23-$P$15))+('Heat gain from airflow'!AB22)+((Occupancy!AA22*'Input Data'!$F$47)+(Occupancy!M22*'Input Data'!$F$49))))/1000","v":-4.2915599999999987},null,"North Window",null,null,null,{"$f":"T46/(P3*P6)","v":11.25},null,null,null,7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI77","v":18},{"$f":"'Incident angle'!BJ77","v":0},{"$f":"'Incident angle'!BK77","v":422.68319711735165},{"$f":"'Incident angle'!BL77","v":819.88818854556575},{"$f":"'Incident angle'!BM77","v":1026.1250812956971},{"$f":"'Incident angle'!BN77","v":1411.1756989981864},{"$f":"'Incident angle'!BO77","v":1877.6960626038615},{"$f":"'Incident angle'!BP77","v":1903.0570696083062},{"$f":"'Incident angle'!BQ77","v":1540.0957842881564},{"$f":"'Incident angle'!BR77","v":0},{"$f":"'Incident angle'!BS77","v":0},{"$f":"'Incident angle'!BT77","v":0},{"$f":"'Incident angle'!BU77","v":0},null,{"$f":"'Incident angle'!BW77","v":18},{"$f":"'Incident angle'!BX77","v":0},{"$f":"'Incident angle'!BY77","v":0},{"$f":"'Incident angle'!BZ77","v":0},{"$f":"'Incident angle'!CA77","v":0},{"$f":"'Incident angle'!CB77","v":0},{"$f":"'Incident angle'!CC77","v":0},{"$f":"'Incident angle'!CD77","v":0},{"$f":"'Incident angle'!CE77","v":0},{"$f":"'Incident angle'!CF77","v":0},{"$f":"'Incident angle'!CG77","v":0},{"$f":"'Incident angle'!CH77","v":0},{"$f":"'Incident angle'!CI77","v":0},null,{"$f":"'Profile angles'!P22","v":18},{"$f":"RADIANS('Profile angles'!Q22)","v":-7.875695115485469E-2},{"$f":"RADIANS('Profile angles'!R22)","v":5.0811936091930835E-3},{"$f":"RADIANS('Profile angles'!S22)","v":5.8021971754233764E-2},{"$f":"RADIANS('Profile angles'!T22)","v":0.11154632270391088},{"$f":"RADIANS('Profile angles'!U22)","v":0.16818851648487471},{"$f":"RADIANS('Profile angles'!V22)","v":0.2119948495476848},{"$f":"RADIANS('Profile angles'!W22)","v":0.20643034646530073},{"$f":"RADIANS('Profile angles'!X22)","v":0.12678973084122475},{"$f":"RADIANS('Profile angles'!Y22)","v":-1.4535089563006036E-3},{"$f":"RADIANS('Profile angles'!Z22)","v":-0.11133018006865013},{"$f":"RADIANS('Profile angles'!AA22)","v":-0.17592692617280517},{"$f":"RADIANS('Profile angles'!AB22)","v":-0.15804497456402347},null,{"$f":"'Profile angles'!P51","v":18},{"$f":"RADIANS('Profile angles'!Q51)","v":0.21383448367072516},{"$f":"RADIANS('Profile angles'!R51)","v":-2.4284225922147823E-2},{"$f":"RADIANS('Profile angles'!S51)","v":-1.1397000015522969},{"$f":"RADIANS('Profile angles'!T51)","v":0.55536119281617979},{"$f":"RADIANS('Profile angles'!U51)","v":0.47627989159216844},{"$f":"RADIANS('Profile angles'!V51)","v":0.51670314614163182},{"$f":"RADIANS('Profile angles'!W51)","v":0.58537590303118936},{"$f":"RADIANS('Profile angles'!X51)","v":0.62269367861413716},{"$f":"RADIANS('Profile angles'!Y51)","v":-1.1397000015523204},{"$f":"RADIANS('Profile angles'!Z51)","v":0.61968279153652928},{"$f":"RADIANS('Profile angles'!AA51)","v":0.51126975196190494},{"$f":"RADIANS('Profile angles'!AB51)","v":0.37549955159039694},null,{"$f":"'Profile angles'!AR22","v":18},{"$f":"(IF($AH$29<DEGREES(BS49),0+$AJ$33,1-((TAN(BS49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX75*$DU$3)+1-$DU$3)","v":0.86349103544106354},{"$f":"(IF($AH$29<DEGREES(BT49),0+$AJ$33,1-((TAN(BT49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY75*$DU$3)+1-$DU$3)","v":0.89221562531024068},{"$f":"(IF($AH$29<DEGREES(BU49),0+$AJ$33,1-((TAN(BU49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ75*$DU$3)+1-$DU$3)","v":0.94652359620523974},{"$f":"(IF($AH$29<DEGREES(BV49),0+$AJ$33,1-((TAN(BV49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA75*$DU$3)+1-$DU$3)","v":0.83841104081794671},{"$f":"(IF($AH$29<DEGREES(BW49),0+$AJ$33,1-((TAN(BW49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB75*$DU$3)+1-$DU$3)","v":0.73614199647192335},{"$f":"(IF($AH$29<DEGREES(BX49),0+$AJ$33,1-((TAN(BX49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC75*$DU$3)+1-$DU$3)","v":0.68847671960367751},{"$f":"(IF($AH$29<DEGREES(BY49),0+$AJ$33,1-((TAN(BY49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD75*$DU$3)+1-$DU$3)","v":0.71860800430836513},{"$f":"(IF($AH$29<DEGREES(BZ49),0+$AJ$33,1-((TAN(BZ49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE75*$DU$3)+1-$DU$3)","v":0.82991785014919472},{"$f":"(IF($AH$29<DEGREES(CA49),0+$AJ$33,1-((TAN(CA49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF75*$DU$3)+1-$DU$3)","v":1.0006828469329017},{"$f":"(IF($AH$29<DEGREES(CB49),0+$AJ$33,1-((TAN(CB49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG75*$DU$3)+1-$DU$3)","v":0.99377502314396693},{"$f":"(IF($AH$29<DEGREES(CC49),0+$AJ$33,1-((TAN(CC49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH75*$DU$3)+1-$DU$3)","v":0.9462933162803806},{"$f":"(IF($AH$29<DEGREES(CD49),0+$AJ$33,1-((TAN(CD49)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI75*$DU$3)+1-$DU$3)","v":0.88686302513811333},null,18,{"$f":"(IF($AH$12<DEGREES(CG49),0+$AJ$16,1-((TAN(CG49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH49),0+$AJ$16,1-((TAN(CH49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI49),0+$AJ$16,1-((TAN(CI49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ49),0+$AJ$16,1-((TAN(CJ49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK49),0+$AJ$16,1-((TAN(CK49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL49),0+$AJ$16,1-((TAN(CL49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM49),0+$AJ$16,1-((TAN(CM49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN49),0+$AJ$16,1-((TAN(CN49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO49),0+$AJ$16,1-((TAN(CO49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP49),0+$AJ$16,1-((TAN(CP49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ49),0+$AJ$16,1-((TAN(CQ49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV75*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR49),0+$AJ$16,1-((TAN(CR49)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW75*$DU$3)+1-$DU$3)","v":0},null,null,18,-4.242067037456934,0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772,null,18,-4.242067037456934,0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772]
[null,20,{"$f":"IF('Dry Bulb'!D24<60,(('Input Data'!$F$44*('Dry Bulb'!D24-$T$15))+('Heat gain from airflow'!Q23)+((Occupancy!P23*'Input Data'!$F$47)+(Occupancy!B23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D24-$P$15))+('Heat gain from airflow'!Q23)+((Occupancy!P23*'Input Data'!$F$47)+(Occupancy!B23*'Input Data'!$F$49))))/1000","v":-1.8223424999999972E-3},{"$f":"IF('Dry Bulb'!E24<60,(('Input Data'!$F$44*('Dry Bulb'!E24-$T$15))+('Heat gain from airflow'!R23)+((Occupancy!Q23*'Input Data'!$F$47)+(Occupancy!C23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E24-$P$15))+('Heat gain from airflow'!R23)+((Occupancy!Q23*'Input Data'!$F$47)+(Occupancy!C23*'Input Data'!$F$49))))/1000","v":-2.6701425000000016},{"$f":"IF('Dry Bulb'!F24<60,(('Input Data'!$F$44*('Dry Bulb'!F24-$T$15))+('Heat gain from airflow'!S23)+((Occupancy!R23*'Input Data'!$F$47)+(Occupancy!D23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F24-$P$15))+('Heat gain from airflow'!S23)+((Occupancy!R23*'Input Data'!$F$47)+(Occupancy!D23*'Input Data'!$F$49))))/1000","v":0.56225524500000024},{"$f":"IF('Dry Bulb'!G24<60,(('Input Data'!$F$44*('Dry Bulb'!G24-$T$15))+('Heat gain from airflow'!T23)+((Occupancy!S23*'Input Data'!$F$47)+(Occupancy!E23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G24-$P$15))+('Heat gain from airflow'!T23)+((Occupancy!S23*'Input Data'!$F$47)+(Occupancy!E23*'Input Data'!$F$49))))/1000","v":5.9138325000000007},{"$f":"IF('Dry Bulb'!H24<60,(('Input Data'!$F$44*('Dry Bulb'!H24-$T$15))+('Heat gain from airflow'!U23)+((Occupancy!T23*'Input Data'!$F$47)+(Occupancy!F23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H24-$P$15))+('Heat gain from airflow'!U23)+((Occupancy!T23*'Input Data'!$F$47)+(Occupancy!F23*'Input Data'!$F$49))))/1000","v":12.399502500000004},{"$f":"IF('Dry Bulb'!I24<60,(('Input Data'!$F$44*('Dry Bulb'!I24-$T$15))+('Heat gain from airflow'!V23)+((Occupancy!U23*'Input Data'!$F$47)+(Occupancy!G23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I24-$P$15))+('Heat gain from airflow'!V23)+((Occupancy!U23*'Input Data'!$F$47)+(Occupancy!G23*'Input Data'!$F$49))))/1000","v":15.737715000000003},{"$f":"IF('Dry Bulb'!J24<60,(('Input Data'!$F$44*('Dry Bulb'!J24-$T$15))+('Heat gain from airflow'!W23)+((Occupancy!V23*'Input Data'!$F$47)+(Occupancy!H23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J24-$P$15))+('Heat gain from airflow'!W23)+((Occupancy!V23*'Input Data'!$F$47)+(Occupancy!H23*'Input Data'!$F$49))))/1000","v":15.928469999999995},{"$f":"IF('Dry Bulb'!K24<60,(('Input Data'!$F$44*('Dry Bulb'!K24-$T$15))+('Heat gain from airflow'!X23)+((Occupancy!W23*'Input Data'!$F$47)+(Occupancy!I23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K24-$P$15))+('Heat gain from airflow'!X23)+((Occupancy!W23*'Input Data'!$F$47)+(Occupancy!I23*'Input Data'!$F$49))))/1000","v":16.023847499999999},{"$f":"IF('Dry Bulb'!L24<60,(('Input Data'!$F$44*('Dry Bulb'!L24-$T$15))+('Heat gain from airflow'!Y23)+((Occupancy!X23*'Input Data'!$F$47)+(Occupancy!J23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L24-$P$15))+('Heat gain from airflow'!Y23)+((Occupancy!X23*'Input Data'!$F$47)+(Occupancy!J23*'Input Data'!$F$49))))/1000","v":13.257899999999999},{"$f":"IF('Dry Bulb'!M24<60,(('Input Data'!$F$44*('Dry Bulb'!M24-$T$15))+('Heat gain from airflow'!Z23)+((Occupancy!Y23*'Input Data'!$F$47)+(Occupancy!K23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M24-$P$15))+('Heat gain from airflow'!Z23)+((Occupancy!Y23*'Input Data'!$F$47)+(Occupancy!K23*'Input Data'!$F$49))))/1000","v":7.7260050000000007},{"$f":"IF('Dry Bulb'!N24<60,(('Input Data'!$F$44*('Dry Bulb'!N24-$T$15))+('Heat gain from airflow'!AA23)+((Occupancy!Z23*'Input Data'!$F$47)+(Occupancy!L23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N24-$P$15))+('Heat gain from airflow'!AA23)+((Occupancy!Z23*'Input Data'!$F$47)+(Occupancy!L23*'Input Data'!$F$49))))/1000","v":1.6178436000000034},{"$f":"IF('Dry Bulb'!O24<60,(('Input Data'!$F$44*('Dry Bulb'!O24-$T$15))+('Heat gain from airflow'!AB23)+((Occupancy!AA23*'Input Data'!$F$47)+(Occupancy!M23*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O24-$P$15))+('Heat gain from airflow'!AB23)+((Occupancy!AA23*'Input Data'!$F$47)+(Occupancy!M23*'Input Data'!$F$49))))/1000","v":-5.2453350000000007},null,"Area",{"$f":"Q53*'Input Data'!F21*'Input Data'!F19","v":247.5},null,null,null,null,null,null,8,null,null,null,"Transmittance of Shade Material",null,null,null,null,null,null,null,0,null,null,null,null,null,{"$f":"'Incident angle'!BI78","v":19},{"$f":"'Incident angle'!BJ78","v":0},{"$f":"'Incident angle'!BK78","v":0},{"$f":"'Incident angle'!BL78","v":0},{"$f":"'Incident angle'!BM78","v":0},{"$f":"'Incident angle'!BN78","v":0},{"$f":"'Incident angle'!BO78","v":0},{"$f":"'Incident angle'!BP78","v":0},{"$f":"'Incident angle'!BQ78","v":0},{"$f":"'Incident angle'!BR78","v":0},{"$f":"'Incident angle'!BS78","v":0},{"$f":"'Incident angle'!BT78","v":0},{"$f":"'Incident angle'!BU78","v":0},null,{"$f":"'Incident angle'!BW78","v":19},{"$f":"'Incident angle'!BX78","v":0},{"$f":"'Incident angle'!BY78","v":0},{"$f":"'Incident angle'!BZ78","v":0},{"$f":"'Incident angle'!CA78","v":0},{"$f":"'Incident angle'!CB78","v":0},{"$f":"'Incident angle'!CC78","v":0},{"$f":"'Incident angle'!CD78","v":0},{"$f":"'Incident angle'!CE78","v":0},{"$f":"'Incident angle'!CF78","v":0},{"$f":"'Incident angle'!CG78","v":0},{"$f":"'Incident angle'!CH78","v":0},{"$f":"'Incident angle'!CI78","v":0},null,{"$f":"'Profile angles'!P23","v":19},{"$f":"RADIANS('Profile angles'!Q23)","v":-0.31044316509225717},{"$f":"RADIANS('Profile angles'!R23)","v":-0.23111522112121052},{"$f":"RADIANS('Profile angles'!S23)","v":-0.18024728429187611},{"$f":"RADIANS('Profile angles'!T23)","v":-0.1267334364435844},{"$f":"RADIANS('Profile angles'!U23)","v":-6.7779708344327269E-2},{"$f":"RADIANS('Profile angles'!V23)","v":-2.1587753481061966E-2},{"$f":"RADIANS('Profile angles'!W23)","v":-2.8054601331330978E-2},{"$f":"RADIANS('Profile angles'!X23)","v":-0.11109422861118669},{"$f":"RADIANS('Profile angles'!Y23)","v":-0.24026026153093591},{"$f":"RADIANS('Profile angles'!Z23)","v":-0.34689085936294084},{"$f":"RADIANS('Profile angles'!AA23)","v":-0.40600410951818994},{"$f":"RADIANS('Profile angles'!AB23)","v":-0.38616028192323892},null,{"$f":"'Profile angles'!P52","v":19},{"$f":"RADIANS('Profile angles'!Q52)","v":0.89431902860972701},{"$f":"RADIANS('Profile angles'!R52)","v":1.1661968303625765},{"$f":"RADIANS('Profile angles'!S52)","v":-1.1397000015522967},{"$f":"RADIANS('Profile angles'!T52)","v":-0.40508921503180328},{"$f":"RADIANS('Profile angles'!U52)","v":-0.14942040034511828},{"$f":"RADIANS('Profile angles'!V52)","v":-4.3182419744715414E-2},{"$f":"RADIANS('Profile angles'!W52)","v":-6.4699031311275204E-2},{"$f":"RADIANS('Profile angles'!X52)","v":-0.36364909543045842},{"$f":"RADIANS('Profile angles'!Y52)","v":-1.1397000015522969},{"$f":"RADIANS('Profile angles'!Z52)","v":1.429871876340016},{"$f":"RADIANS('Profile angles'!AA52)","v":1.1011153762045045},{"$f":"RADIANS('Profile angles'!AB52)","v":0.92834451312327959},null,{"$f":"'Profile angles'!AR23","v":19},{"$f":"(IF($AH$29<DEGREES(BS50),0+$AJ$33,1-((TAN(BS50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX76*$DU$3)+1-$DU$3)","v":1.0668662712283645},{"$f":"(IF($AH$29<DEGREES(BT50),0+$AJ$33,1-((TAN(BT50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY76*$DU$3)+1-$DU$3)","v":1.1060393803474169},{"$f":"(IF($AH$29<DEGREES(BU50),0+$AJ$33,1-((TAN(BU50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ76*$DU$3)+1-$DU$3)","v":1.0803048768408494},{"$f":"(IF($AH$29<DEGREES(BV50),0+$AJ$33,1-((TAN(BV50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA76*$DU$3)+1-$DU$3)","v":0.92736877444081256},{"$f":"(IF($AH$29<DEGREES(BW50),0+$AJ$33,1-((TAN(BW50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB76*$DU$3)+1-$DU$3)","v":0.81134121279877147},{"$f":"(IF($AH$29<DEGREES(BX50),0+$AJ$33,1-((TAN(BX50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC76*$DU$3)+1-$DU$3)","v":0.76149429416058001},{"$f":"(IF($AH$29<DEGREES(BY50),0+$AJ$33,1-((TAN(BY50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD76*$DU$3)+1-$DU$3)","v":0.79882662358245515},{"$f":"(IF($AH$29<DEGREES(BZ50),0+$AJ$33,1-((TAN(BZ50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE76*$DU$3)+1-$DU$3)","v":0.92008371056901717},{"$f":"(IF($AH$29<DEGREES(CA50),0+$AJ$33,1-((TAN(CA50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF76*$DU$3)+1-$DU$3)","v":1.1054904428264725},{"$f":"(IF($AH$29<DEGREES(CB50),0+$AJ$33,1-((TAN(CB50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG76*$DU$3)+1-$DU$3)","v":1.2209245797479256},{"$f":"(IF($AH$29<DEGREES(CC50),0+$AJ$33,1-((TAN(CC50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH76*$DU$3)+1-$DU$3)","v":1.1589939043985926},{"$f":"(IF($AH$29<DEGREES(CD50),0+$AJ$33,1-((TAN(CD50)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI76*$DU$3)+1-$DU$3)","v":1.0891724184971923},null,19,{"$f":"(IF($AH$12<DEGREES(CG50),0+$AJ$16,1-((TAN(CG50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH50),0+$AJ$16,1-((TAN(CH50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI50),0+$AJ$16,1-((TAN(CI50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ50),0+$AJ$16,1-((TAN(CJ50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK50),0+$AJ$16,1-((TAN(CK50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CL50),0+$AJ$16,1-((TAN(CL50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CM50),0+$AJ$16,1-((TAN(CM50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CN50),0+$AJ$16,1-((TAN(CN50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO50),0+$AJ$16,1-((TAN(CO50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP50),0+$AJ$16,1-((TAN(CP50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ50),0+$AJ$16,1-((TAN(CQ50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV76*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR50),0+$AJ$16,1-((TAN(CR50)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW76*$DU$3)+1-$DU$3)","v":0},null,null,19,-17.258784755357599,-13.177535073458104,{"$f":"DZ23","v":-10.292097151668569},-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176,null,19,-17.258784755357599,-13.177535073458104,-10.292097151668569,-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176]
[null,21,{"$f":"IF('Dry Bulb'!D25<60,(('Input Data'!$F$44*('Dry Bulb'!D25-$T$15))+('Heat gain from airflow'!Q24)+((Occupancy!P24*'Input Data'!$F$47)+(Occupancy!B24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D25-$P$15))+('Heat gain from airflow'!Q24)+((Occupancy!P24*'Input Data'!$F$47)+(Occupancy!B24*'Input Data'!$F$49))))/1000","v":-2.4899849999999997E-3},{"$f":"IF('Dry Bulb'!E25<60,(('Input Data'!$F$44*('Dry Bulb'!E25-$T$15))+('Heat gain from airflow'!R24)+((Occupancy!Q24*'Input Data'!$F$47)+(Occupancy!C24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E25-$P$15))+('Heat gain from airflow'!R24)+((Occupancy!Q24*'Input Data'!$F$47)+(Occupancy!C24*'Input Data'!$F$49))))/1000","v":-3.6239175000000006},{"$f":"IF('Dry Bulb'!F25<60,(('Input Data'!$F$44*('Dry Bulb'!F25-$T$15))+('Heat gain from airflow'!S24)+((Occupancy!R24*'Input Data'!$F$47)+(Occupancy!D24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F25-$P$15))+('Heat gain from airflow'!S24)+((Occupancy!R24*'Input Data'!$F$47)+(Occupancy!D24*'Input Data'!$F$49))))/1000","v":-0.37604551499999844},{"$f":"IF('Dry Bulb'!G25<60,(('Input Data'!$F$44*('Dry Bulb'!G25-$T$15))+('Heat gain from airflow'!T24)+((Occupancy!S24*'Input Data'!$F$47)+(Occupancy!E24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G25-$P$15))+('Heat gain from airflow'!T24)+((Occupancy!S24*'Input Data'!$F$47)+(Occupancy!E24*'Input Data'!$F$49))))/1000","v":5.6056218299999969},{"$f":"IF('Dry Bulb'!H25<60,(('Input Data'!$F$44*('Dry Bulb'!H25-$T$15))+('Heat gain from airflow'!U24)+((Occupancy!T24*'Input Data'!$F$47)+(Occupancy!F24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H25-$P$15))+('Heat gain from airflow'!U24)+((Occupancy!T24*'Input Data'!$F$47)+(Occupancy!F24*'Input Data'!$F$49))))/1000","v":11.350350000000002},{"$f":"IF('Dry Bulb'!I25<60,(('Input Data'!$F$44*('Dry Bulb'!I25-$T$15))+('Heat gain from airflow'!V24)+((Occupancy!U24*'Input Data'!$F$47)+(Occupancy!G24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I25-$P$15))+('Heat gain from airflow'!V24)+((Occupancy!U24*'Input Data'!$F$47)+(Occupancy!G24*'Input Data'!$F$49))))/1000","v":14.307052500000001},{"$f":"IF('Dry Bulb'!J25<60,(('Input Data'!$F$44*('Dry Bulb'!J25-$T$15))+('Heat gain from airflow'!W24)+((Occupancy!V24*'Input Data'!$F$47)+(Occupancy!H24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J25-$P$15))+('Heat gain from airflow'!W24)+((Occupancy!V24*'Input Data'!$F$47)+(Occupancy!H24*'Input Data'!$F$49))))/1000","v":14.402429999999999},{"$f":"IF('Dry Bulb'!K25<60,(('Input Data'!$F$44*('Dry Bulb'!K25-$T$15))+('Heat gain from airflow'!X24)+((Occupancy!W24*'Input Data'!$F$47)+(Occupancy!I24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K25-$P$15))+('Heat gain from airflow'!X24)+((Occupancy!W24*'Input Data'!$F$47)+(Occupancy!I24*'Input Data'!$F$49))))/1000","v":14.974694999999995},{"$f":"IF('Dry Bulb'!L25<60,(('Input Data'!$F$44*('Dry Bulb'!L25-$T$15))+('Heat gain from airflow'!Y24)+((Occupancy!X24*'Input Data'!$F$47)+(Occupancy!J24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L25-$P$15))+('Heat gain from airflow'!Y24)+((Occupancy!X24*'Input Data'!$F$47)+(Occupancy!J24*'Input Data'!$F$49))))/1000","v":11.922615000000002},{"$f":"IF('Dry Bulb'!M25<60,(('Input Data'!$F$44*('Dry Bulb'!M25-$T$15))+('Heat gain from airflow'!Z24)+((Occupancy!Y24*'Input Data'!$F$47)+(Occupancy!K24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M25-$P$15))+('Heat gain from airflow'!Z24)+((Occupancy!Y24*'Input Data'!$F$47)+(Occupancy!K24*'Input Data'!$F$49))))/1000","v":6.676852499999999},{"$f":"IF('Dry Bulb'!N25<60,(('Input Data'!$F$44*('Dry Bulb'!N25-$T$15))+('Heat gain from airflow'!AA24)+((Occupancy!Z24*'Input Data'!$F$47)+(Occupancy!L24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N25-$P$15))+('Heat gain from airflow'!AA24)+((Occupancy!Z24*'Input Data'!$F$47)+(Occupancy!L24*'Input Data'!$F$49))))/1000","v":0.56225524500000024},{"$f":"IF('Dry Bulb'!O25<60,(('Input Data'!$F$44*('Dry Bulb'!O25-$T$15))+('Heat gain from airflow'!AB24)+((Occupancy!AA24*'Input Data'!$F$47)+(Occupancy!M24*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O25-$P$15))+('Heat gain from airflow'!AB24)+((Occupancy!AA24*'Input Data'!$F$47)+(Occupancy!M24*'Input Data'!$F$49))))/1000","v":-2.2038524999999998E-3},null,"Glass SHGC",0.28999999999999998,null,null,"LCR",null,null,null,9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI79","v":20},{"$f":"'Incident angle'!BJ79","v":0},{"$f":"'Incident angle'!BK79","v":0},{"$f":"'Incident angle'!BL79","v":0},{"$f":"'Incident angle'!BM79","v":0},{"$f":"'Incident angle'!BN79","v":0},{"$f":"'Incident angle'!BO79","v":0},{"$f":"'Incident angle'!BP79","v":0},{"$f":"'Incident angle'!BQ79","v":0},{"$f":"'Incident angle'!BR79","v":0},{"$f":"'Incident angle'!BS79","v":0},{"$f":"'Incident angle'!BT79","v":0},{"$f":"'Incident angle'!BU79","v":0},null,{"$f":"'Incident angle'!BW79","v":20},{"$f":"'Incident angle'!BX79","v":0},{"$f":"'Incident angle'!BY79","v":0},{"$f":"'Incident angle'!BZ79","v":0},{"$f":"'Incident angle'!CA79","v":0},{"$f":"'Incident angle'!CB79","v":0},{"$f":"'Incident angle'!CC79","v":0},{"$f":"'Incident angle'!CD79","v":0},{"$f":"'Incident angle'!CE79","v":0},{"$f":"'Incident angle'!CF79","v":0},{"$f":"'Incident angle'!CG79","v":0},{"$f":"'Incident angle'!CH79","v":0},{"$f":"'Incident angle'!CI79","v":0},null,{"$f":"'Profile angles'!P24","v":20},{"$f":"RADIANS('Profile angles'!Q24)","v":-0.53982440647106411},{"$f":"RADIANS('Profile angles'!R24)","v":-0.46745924354256657},{"$f":"RADIANS('Profile angles'!S24)","v":-0.42271676310413892},{"$f":"RADIANS('Profile angles'!T24)","v":-0.37438414286885741},{"$f":"RADIANS('Profile angles'!U24)","v":-0.31663095237958921},{"$f":"RADIANS('Profile angles'!V24)","v":-0.26866082450954942},{"$f":"RADIANS('Profile angles'!W24)","v":-0.27434316021105154},{"$f":"RADIANS('Profile angles'!X24)","v":-0.35806173657168094},{"$f":"RADIANS('Profile angles'!Y24)","v":-0.48459652421088528},{"$f":"RADIANS('Profile angles'!Z24)","v":-0.58500248706259217},{"$f":"RADIANS('Profile angles'!AA24)","v":-0.6358430799641186},{"$f":"RADIANS('Profile angles'!AB24)","v":-0.61217498892976285},null,{"$f":"'Profile angles'!P53","v":20},{"$f":"RADIANS('Profile angles'!Q53)","v":1.3012298625660643},{"$f":"RADIANS('Profile angles'!R53)","v":-1.560181886805565},{"$f":"RADIANS('Profile angles'!S53)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!T53)","v":-0.72371978813644844},{"$f":"RADIANS('Profile angles'!U53)","v":-0.48856076237490265},{"$f":"RADIANS('Profile angles'!V53)","v":-0.39161342241702657},{"$f":"RADIANS('Profile angles'!W53)","v":-0.44511249062286379},{"$f":"RADIANS('Profile angles'!X53)","v":-0.70652153014812846},{"$f":"RADIANS('Profile angles'!Y53)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!Z53)","v":-1.4816256583034375},{"$f":"RADIANS('Profile angles'!AA53)","v":1.3982180222701848},{"$f":"RADIANS('Profile angles'!AB53)","v":1.2659457689719542},null,{"$f":"'Profile angles'!AR24","v":20},{"$f":"(IF($AH$29<DEGREES(BS51),0+$AJ$33,1-((TAN(BS51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX77*$DU$3)+1-$DU$3)","v":1.3019391001798422},{"$f":"(IF($AH$29<DEGREES(BT51),0+$AJ$33,1-((TAN(BT51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY77*$DU$3)+1-$DU$3)","v":1.34971590119492},{"$f":"(IF($AH$29<DEGREES(BU51),0+$AJ$33,1-((TAN(BU51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ77*$DU$3)+1-$DU$3)","v":1.1788590753970074},{"$f":"(IF($AH$29<DEGREES(BV51),0+$AJ$33,1-((TAN(BV51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA77*$DU$3)+1-$DU$3)","v":0.99157365834961486},{"$f":"(IF($AH$29<DEGREES(BW51),0+$AJ$33,1-((TAN(BW51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB77*$DU$3)+1-$DU$3)","v":0.85045524576860321},{"$f":"(IF($AH$29<DEGREES(BX51),0+$AJ$33,1-((TAN(BX51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC77*$DU$3)+1-$DU$3)","v":0.7951159558454256},{"$f":"(IF($AH$29<DEGREES(BY51),0+$AJ$33,1-((TAN(BY51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD77*$DU$3)+1-$DU$3)","v":0.84390891519987066},{"$f":"(IF($AH$29<DEGREES(BZ51),0+$AJ$33,1-((TAN(BZ51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE77*$DU$3)+1-$DU$3)","v":0.98530491106618479},{"$f":"(IF($AH$29<DEGREES(CA51),0+$AJ$33,1-((TAN(CA51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF77*$DU$3)+1-$DU$3)","v":1.202834108771841},{"$f":"(IF($AH$29<DEGREES(CB51),0+$AJ$33,1-((TAN(CB51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG77*$DU$3)+1-$DU$3)","v":1.4203019997186082},{"$f":"(IF($AH$29<DEGREES(CC51),0+$AJ$33,1-((TAN(CC51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH77*$DU$3)+1-$DU$3)","v":1.4191039702479158},{"$f":"(IF($AH$29<DEGREES(CD51),0+$AJ$33,1-((TAN(CD51)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI77*$DU$3)+1-$DU$3)","v":1.3267444424189185},null,20,{"$f":"(IF($AH$12<DEGREES(CG51),0+$AJ$16,1-((TAN(CG51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL77*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH51),0+$AJ$16,1-((TAN(CH51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM77*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI51),0+$AJ$16,1-((TAN(CI51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN77*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ51),0+$AJ$16,1-((TAN(CJ51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO77*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CK51),0+$AJ$16,1-((TAN(CK51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP77*$DU$3)+1-$DU$3)","v":0.259144435574934},{"$f":"(IF($AH$12<DEGREES(CL51),0+$AJ$16,1-((TAN(CL51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ77*$DU$3)+1-$DU$3)","v":0.32234254894470965},{"$f":"(IF($AH$12<DEGREES(CM51),0+$AJ$16,1-((TAN(CM51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR77*$DU$3)+1-$DU$3)","v":0.20342156247856},{"$f":"(IF($AH$12<DEGREES(CN51),0+$AJ$16,1-((TAN(CN51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS77*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CO51),0+$AJ$16,1-((TAN(CO51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT77*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP51),0+$AJ$16,1-((TAN(CP51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU77*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ51),0+$AJ$16,1-((TAN(CQ51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV77*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR51),0+$AJ$16,1-((TAN(CR51)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW77*$DU$3)+1-$DU$3)","v":0},null,null,20,-30.589239677830651,-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,-12.902247652391463,-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299,null,20,-30.589239677830651,-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,-12.902247652391463,-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299]
[null,22,{"$f":"IF('Dry Bulb'!D26<60,(('Input Data'!$F$44*('Dry Bulb'!D26-$T$15))+('Heat gain from airflow'!Q25)+((Occupancy!P25*'Input Data'!$F$47)+(Occupancy!B25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D26-$P$15))+('Heat gain from airflow'!Q25)+((Occupancy!P25*'Input Data'!$F$47)+(Occupancy!B25*'Input Data'!$F$49))))/1000","v":-3.2530049999999981E-3},{"$f":"IF('Dry Bulb'!E26<60,(('Input Data'!$F$44*('Dry Bulb'!E26-$T$15))+('Heat gain from airflow'!R25)+((Occupancy!Q25*'Input Data'!$F$47)+(Occupancy!C25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E26-$P$15))+('Heat gain from airflow'!R25)+((Occupancy!Q25*'Input Data'!$F$47)+(Occupancy!C25*'Input Data'!$F$49))))/1000","v":-4.5776924999999986},{"$f":"IF('Dry Bulb'!F26<60,(('Input Data'!$F$44*('Dry Bulb'!F26-$T$15))+('Heat gain from airflow'!S25)+((Occupancy!R25*'Input Data'!$F$47)+(Occupancy!D25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F26-$P$15))+('Heat gain from airflow'!S25)+((Occupancy!R25*'Input Data'!$F$47)+(Occupancy!D25*'Input Data'!$F$49))))/1000","v":-1.4316338700000015},{"$f":"IF('Dry Bulb'!G26<60,(('Input Data'!$F$44*('Dry Bulb'!G26-$T$15))+('Heat gain from airflow'!T25)+((Occupancy!S25*'Input Data'!$F$47)+(Occupancy!E25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G26-$P$15))+('Heat gain from airflow'!T25)+((Occupancy!S25*'Input Data'!$F$47)+(Occupancy!E25*'Input Data'!$F$49))))/1000","v":4.5500334750000038},{"$f":"IF('Dry Bulb'!H26<60,(('Input Data'!$F$44*('Dry Bulb'!H26-$T$15))+('Heat gain from airflow'!U25)+((Occupancy!T25*'Input Data'!$F$47)+(Occupancy!F25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H26-$P$15))+('Heat gain from airflow'!U25)+((Occupancy!T25*'Input Data'!$F$47)+(Occupancy!F25*'Input Data'!$F$49))))/1000","v":10.396574999999997},{"$f":"IF('Dry Bulb'!I26<60,(('Input Data'!$F$44*('Dry Bulb'!I26-$T$15))+('Heat gain from airflow'!V25)+((Occupancy!U25*'Input Data'!$F$47)+(Occupancy!G25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I26-$P$15))+('Heat gain from airflow'!V25)+((Occupancy!U25*'Input Data'!$F$47)+(Occupancy!G25*'Input Data'!$F$49))))/1000","v":13.067145},{"$f":"IF('Dry Bulb'!J26<60,(('Input Data'!$F$44*('Dry Bulb'!J26-$T$15))+('Heat gain from airflow'!W25)+((Occupancy!V25*'Input Data'!$F$47)+(Occupancy!H25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J26-$P$15))+('Heat gain from airflow'!W25)+((Occupancy!V25*'Input Data'!$F$47)+(Occupancy!H25*'Input Data'!$F$49))))/1000","v":12.971767500000004},{"$f":"IF('Dry Bulb'!K26<60,(('Input Data'!$F$44*('Dry Bulb'!K26-$T$15))+('Heat gain from airflow'!X25)+((Occupancy!W25*'Input Data'!$F$47)+(Occupancy!I25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K26-$P$15))+('Heat gain from airflow'!X25)+((Occupancy!W25*'Input Data'!$F$47)+(Occupancy!I25*'Input Data'!$F$49))))/1000","v":13.925542500000002},{"$f":"IF('Dry Bulb'!L26<60,(('Input Data'!$F$44*('Dry Bulb'!L26-$T$15))+('Heat gain from airflow'!Y25)+((Occupancy!X25*'Input Data'!$F$47)+(Occupancy!J25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L26-$P$15))+('Heat gain from airflow'!Y25)+((Occupancy!X25*'Input Data'!$F$47)+(Occupancy!J25*'Input Data'!$F$49))))/1000","v":10.968840000000004},{"$f":"IF('Dry Bulb'!M26<60,(('Input Data'!$F$44*('Dry Bulb'!M26-$T$15))+('Heat gain from airflow'!Z25)+((Occupancy!Y25*'Input Data'!$F$47)+(Occupancy!K25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M26-$P$15))+('Heat gain from airflow'!Z25)+((Occupancy!Y25*'Input Data'!$F$47)+(Occupancy!K25*'Input Data'!$F$49))))/1000","v":5.6276999999999973},{"$f":"IF('Dry Bulb'!N26<60,(('Input Data'!$F$44*('Dry Bulb'!N26-$T$15))+('Heat gain from airflow'!AA25)+((Occupancy!Z25*'Input Data'!$F$47)+(Occupancy!L25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N26-$P$15))+('Heat gain from airflow'!AA25)+((Occupancy!Z25*'Input Data'!$F$47)+(Occupancy!L25*'Input Data'!$F$49))))/1000","v":-0.72790830000000228},{"$f":"IF('Dry Bulb'!O26<60,(('Input Data'!$F$44*('Dry Bulb'!O26-$T$15))+('Heat gain from airflow'!AB25)+((Occupancy!AA25*'Input Data'!$F$47)+(Occupancy!M25*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O26-$P$15))+('Heat gain from airflow'!AB25)+((Occupancy!AA25*'Input Data'!$F$47)+(Occupancy!M25*'Input Data'!$F$49))))/1000","v":-2.8714949999999991E-3},null,"U-Value",0.5,false,null,{"$f":"T46/Q29","v":37.5},null,null,null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI80","v":21},{"$f":"'Incident angle'!BJ80","v":0},{"$f":"'Incident angle'!BK80","v":0},{"$f":"'Incident angle'!BL80","v":0},{"$f":"'Incident angle'!BM80","v":0},{"$f":"'Incident angle'!BN80","v":0},{"$f":"'Incident angle'!BO80","v":0},{"$f":"'Incident angle'!BP80","v":0},{"$f":"'Incident angle'!BQ80","v":0},{"$f":"'Incident angle'!BR80","v":0},{"$f":"'Incident angle'!BS80","v":0},{"$f":"'Incident angle'!BT80","v":0},{"$f":"'Incident angle'!BU80","v":0},null,{"$f":"'Incident angle'!BW80","v":21},{"$f":"'Incident angle'!BX80","v":0},{"$f":"'Incident angle'!BY80","v":0},{"$f":"'Incident angle'!BZ80","v":0},{"$f":"'Incident angle'!CA80","v":0},{"$f":"'Incident angle'!CB80","v":0},{"$f":"'Incident angle'!CC80","v":0},{"$f":"'Incident angle'!CD80","v":0},{"$f":"'Incident angle'!CE80","v":0},{"$f":"'Incident angle'!CF80","v":0},{"$f":"'Incident angle'!CG80","v":0},{"$f":"'Incident angle'!CH80","v":0},{"$f":"'Incident angle'!CI80","v":0},null,{"$f":"'Profile angles'!P25","v":21},{"$f":"RADIANS('Profile angles'!Q25)","v":-0.77137406354258076},{"$f":"RADIANS('Profile angles'!R25)","v":-0.70858778624744145},{"$f":"RADIANS('Profile angles'!S25)","v":-0.67432329522984613},{"$f":"RADIANS('Profile angles'!T25)","v":-0.63740014217672614},{"$f":"RADIANS('Profile angles'!U25)","v":-0.58586265313688612},{"$f":"RADIANS('Profile angles'!V25)","v":-0.5374341930134342},{"$f":"RADIANS('Profile angles'!W25)","v":-0.53995019403937616},{"$f":"RADIANS('Profile angles'!X25)","v":-0.62017385269735259},{"$f":"RADIANS('Profile angles'!Y25)","v":-0.73908870770470358},{"$f":"RADIANS('Profile angles'!Z25)","v":-0.82955153298556916},{"$f":"RADIANS('Profile angles'!AA25)","v":-0.86919421625434168},{"$f":"RADIANS('Profile angles'!AB25)","v":-0.84017901380444071},null,{"$f":"'Profile angles'!P54","v":21},{"$f":"RADIANS('Profile angles'!Q54)","v":1.4926689138225644},{"$f":"RADIANS('Profile angles'!R54)","v":-1.4244661198800128},{"$f":"RADIANS('Profile angles'!S54)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!T54)","v":-0.84257659010007857},{"$f":"RADIANS('Profile angles'!U54)","v":-0.65069747813555467},{"$f":"RADIANS('Profile angles'!V54)","v":-0.57207111370754471},{"$f":"RADIANS('Profile angles'!W54)","v":-0.62738252671884254},{"$f":"RADIANS('Profile angles'!X54)","v":-0.8330645277261437},{"$f":"RADIANS('Profile angles'!Y54)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!Z54)","v":-1.3922681911981456},{"$f":"RADIANS('Profile angles'!AA54)","v":1.5401075773273576},{"$f":"RADIANS('Profile angles'!AB54)","v":1.4405551263701017},null,{"$f":"'Profile angles'!AR25","v":21},{"$f":"(IF($AH$29<DEGREES(BS52),0+$AJ$33,1-((TAN(BS52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX78*$DU$3)+1-$DU$3)","v":1.6166705205321963},{"$f":"(IF($AH$29<DEGREES(BT52),0+$AJ$33,1-((TAN(BT52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY78*$DU$3)+1-$DU$3)","v":1.4989010076812723},{"$f":"(IF($AH$29<DEGREES(BU52),0+$AJ$33,1-((TAN(BU52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ78*$DU$3)+1-$DU$3)","v":1.2728465214314719},{"$f":"(IF($AH$29<DEGREES(BV52),0+$AJ$33,1-((TAN(BV52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA78*$DU$3)+1-$DU$3)","v":1.0170523046607649},{"$f":"(IF($AH$29<DEGREES(BW52),0+$AJ$33,1-((TAN(BW52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB78*$DU$3)+1-$DU$3)","v":0.82624917599364656},{"$f":"(IF($AH$29<DEGREES(BX52),0+$AJ$33,1-((TAN(BX52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC78*$DU$3)+1-$DU$3)","v":0.76134563781345843},{"$f":"(IF($AH$29<DEGREES(BY52),0+$AJ$33,1-((TAN(BY52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD78*$DU$3)+1-$DU$3)","v":0.83286841608570727},{"$f":"(IF($AH$29<DEGREES(BZ52),0+$AJ$33,1-((TAN(BZ52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE78*$DU$3)+1-$DU$3)","v":1.0130923337880067},{"$f":"(IF($AH$29<DEGREES(CA52),0+$AJ$33,1-((TAN(CA52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF78*$DU$3)+1-$DU$3)","v":1.294665221274711},{"$f":"(IF($AH$29<DEGREES(CB52),0+$AJ$33,1-((TAN(CB52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG78*$DU$3)+1-$DU$3)","v":1.5907736217839892},{"$f":"(IF($AH$29<DEGREES(CC52),0+$AJ$33,1-((TAN(CC52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH78*$DU$3)+1-$DU$3)","v":1.7951614933925397},{"$f":"(IF($AH$29<DEGREES(CD52),0+$AJ$33,1-((TAN(CD52)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI78*$DU$3)+1-$DU$3)","v":1.6510333149560343},null,21,{"$f":"(IF($AH$12<DEGREES(CG52),0+$AJ$16,1-((TAN(CG52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL78*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH52),0+$AJ$16,1-((TAN(CH52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM78*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI52),0+$AJ$16,1-((TAN(CI52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN78*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CJ52),0+$AJ$16,1-((TAN(CJ52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO78*$DU$3)+1-$DU$3)","v":0.43339460858381845},{"$f":"(IF($AH$12<DEGREES(CK52),0+$AJ$16,1-((TAN(CK52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP78*$DU$3)+1-$DU$3)","v":0.65358072783872645},{"$f":"(IF($AH$12<DEGREES(CL52),0+$AJ$16,1-((TAN(CL52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ78*$DU$3)+1-$DU$3)","v":0.6670036228222459},{"$f":"(IF($AH$12<DEGREES(CM52),0+$AJ$16,1-((TAN(CM52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR78*$DU$3)+1-$DU$3)","v":0.59563787805256796},{"$f":"(IF($AH$12<DEGREES(CN52),0+$AJ$16,1-((TAN(CN52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS78*$DU$3)+1-$DU$3)","v":0.40668358851258163},{"$f":"(IF($AH$12<DEGREES(CO52),0+$AJ$16,1-((TAN(CO52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT78*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CP52),0+$AJ$16,1-((TAN(CP52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU78*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ52),0+$AJ$16,1-((TAN(CQ52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV78*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR52),0+$AJ$16,1-((TAN(CR52)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW78*$DU$3)+1-$DU$3)","v":0},null,null,21,-44.11375465474292,-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762,null,21,-44.11375465474292,-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762]
[null,23,{"$f":"IF('Dry Bulb'!D27<60,(('Input Data'!$F$44*('Dry Bulb'!D27-$T$15))+('Heat gain from airflow'!Q26)+((Occupancy!P26*'Input Data'!$F$47)+(Occupancy!B26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D27-$P$15))+('Heat gain from airflow'!Q26)+((Occupancy!P26*'Input Data'!$F$47)+(Occupancy!B26*'Input Data'!$F$49))))/1000","v":-3.9206475000000008E-3},{"$f":"IF('Dry Bulb'!E27<60,(('Input Data'!$F$44*('Dry Bulb'!E27-$T$15))+('Heat gain from airflow'!R26)+((Occupancy!Q26*'Input Data'!$F$47)+(Occupancy!C26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E27-$P$15))+('Heat gain from airflow'!R26)+((Occupancy!Q26*'Input Data'!$F$47)+(Occupancy!C26*'Input Data'!$F$49))))/1000","v":-1.6315875000000016E-3},{"$f":"IF('Dry Bulb'!F27<60,(('Input Data'!$F$44*('Dry Bulb'!F27-$T$15))+('Heat gain from airflow'!S26)+((Occupancy!R26*'Input Data'!$F$47)+(Occupancy!D26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F27-$P$15))+('Heat gain from airflow'!S26)+((Occupancy!R26*'Input Data'!$F$47)+(Occupancy!D26*'Input Data'!$F$49))))/1000","v":-2.3699346299999999},{"$f":"IF('Dry Bulb'!G27<60,(('Input Data'!$F$44*('Dry Bulb'!G27-$T$15))+('Heat gain from airflow'!T26)+((Occupancy!S26*'Input Data'!$F$47)+(Occupancy!E26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G27-$P$15))+('Heat gain from airflow'!T26)+((Occupancy!S26*'Input Data'!$F$47)+(Occupancy!E26*'Input Data'!$F$49))))/1000","v":3.1425823350000055},{"$f":"IF('Dry Bulb'!H27<60,(('Input Data'!$F$44*('Dry Bulb'!H27-$T$15))+('Heat gain from airflow'!U26)+((Occupancy!T26*'Input Data'!$F$47)+(Occupancy!F26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H27-$P$15))+('Heat gain from airflow'!U26)+((Occupancy!T26*'Input Data'!$F$47)+(Occupancy!F26*'Input Data'!$F$49))))/1000","v":9.4428000000000001},{"$f":"IF('Dry Bulb'!I27<60,(('Input Data'!$F$44*('Dry Bulb'!I27-$T$15))+('Heat gain from airflow'!V26)+((Occupancy!U26*'Input Data'!$F$47)+(Occupancy!G26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I27-$P$15))+('Heat gain from airflow'!V26)+((Occupancy!U26*'Input Data'!$F$47)+(Occupancy!G26*'Input Data'!$F$49))))/1000","v":12.113370000000002},{"$f":"IF('Dry Bulb'!J27<60,(('Input Data'!$F$44*('Dry Bulb'!J27-$T$15))+('Heat gain from airflow'!W26)+((Occupancy!V26*'Input Data'!$F$47)+(Occupancy!H26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J27-$P$15))+('Heat gain from airflow'!W26)+((Occupancy!V26*'Input Data'!$F$47)+(Occupancy!H26*'Input Data'!$F$49))))/1000","v":12.208747499999998},{"$f":"IF('Dry Bulb'!K27<60,(('Input Data'!$F$44*('Dry Bulb'!K27-$T$15))+('Heat gain from airflow'!X26)+((Occupancy!W26*'Input Data'!$F$47)+(Occupancy!I26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K27-$P$15))+('Heat gain from airflow'!X26)+((Occupancy!W26*'Input Data'!$F$47)+(Occupancy!I26*'Input Data'!$F$49))))/1000","v":13.067145},{"$f":"IF('Dry Bulb'!L27<60,(('Input Data'!$F$44*('Dry Bulb'!L27-$T$15))+('Heat gain from airflow'!Y26)+((Occupancy!X26*'Input Data'!$F$47)+(Occupancy!J26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L27-$P$15))+('Heat gain from airflow'!Y26)+((Occupancy!X26*'Input Data'!$F$47)+(Occupancy!J26*'Input Data'!$F$49))))/1000","v":10.015065000000005},{"$f":"IF('Dry Bulb'!M27<60,(('Input Data'!$F$44*('Dry Bulb'!M27-$T$15))+('Heat gain from airflow'!Z26)+((Occupancy!Y26*'Input Data'!$F$47)+(Occupancy!K26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M27-$P$15))+('Heat gain from airflow'!Z26)+((Occupancy!Y26*'Input Data'!$F$47)+(Occupancy!K26*'Input Data'!$F$49))))/1000","v":5.2537590450000025},{"$f":"IF('Dry Bulb'!N27<60,(('Input Data'!$F$44*('Dry Bulb'!N27-$T$15))+('Heat gain from airflow'!AA26)+((Occupancy!Z26*'Input Data'!$F$47)+(Occupancy!L26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N27-$P$15))+('Heat gain from airflow'!AA26)+((Occupancy!Z26*'Input Data'!$F$47)+(Occupancy!L26*'Input Data'!$F$49))))/1000","v":-2.018071845000005},{"$f":"IF('Dry Bulb'!O27<60,(('Input Data'!$F$44*('Dry Bulb'!O27-$T$15))+('Heat gain from airflow'!AB26)+((Occupancy!AA26*'Input Data'!$F$47)+(Occupancy!M26*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O27-$P$15))+('Heat gain from airflow'!AB26)+((Occupancy!AA26*'Input Data'!$F$47)+(Occupancy!M26*'Input Data'!$F$49))))/1000","v":-3.3483825000000023E-3},null,"WWR",{"$f":"(Q54/20)*R53","v":0.55000000000000004},{"$f":"IF(R52,0,1)","v":1},null,null,null,null,null,null,null,null,null,"SILL",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Profile angles'!P26","v":22},{"$f":"RADIANS('Profile angles'!Q26)","v":-1.0077487946336263},{"$f":"RADIANS('Profile angles'!R26)","v":-0.95743316995573291},{"$f":"RADIANS('Profile angles'!S26)","v":-0.93831409714073899},{"$f":"RADIANS('Profile angles'!T26)","v":-0.92011364949964081},{"$f":"RADIANS('Profile angles'!U26)","v":-0.88176474027935958},{"$f":"RADIANS('Profile angles'!V26)","v":-0.83552237145082942},{"$f":"RADIANS('Profile angles'!W26)","v":-0.83162347526531166},{"$f":"RADIANS('Profile angles'!X26)","v":-0.9019578437956276},{"$f":"RADIANS('Profile angles'!Y26)","v":-1.0063600686241212},{"$f":"RADIANS('Profile angles'!Z26)","v":-1.0823876155652608},{"$f":"RADIANS('Profile angles'!AA26)","v":-1.1078788719054964},{"$f":"RADIANS('Profile angles'!AB26)","v":-1.0723844562125873},null,{"$f":"'Profile angles'!P55","v":22},{"$f":"RADIANS('Profile angles'!Q55)","v":-1.5539445877602389},{"$f":"RADIANS('Profile angles'!R55)","v":-1.3649967109877184},{"$f":"RADIANS('Profile angles'!S55)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T55)","v":-0.89738136477565211},{"$f":"RADIANS('Profile angles'!U55)","v":-0.73245268972748756},{"$f":"RADIANS('Profile angles'!V55)","v":-0.66630483731305101},{"$f":"RADIANS('Profile angles'!W55)","v":-0.71892314829995663},{"$f":"RADIANS('Profile angles'!X55)","v":-0.89109084416912154},{"$f":"RADIANS('Profile angles'!Y55)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!Z55)","v":-1.3503950367995554},{"$f":"RADIANS('Profile angles'!AA55)","v":-1.529878658594682},{"$f":"RADIANS('Profile angles'!AB55)","v":1.5317777100487904},null,{"$f":"'Profile angles'!AR26","v":22},{"$f":"(IF($AH$29<DEGREES(BS53),0+$AJ$33,1-((TAN(BS53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX79*$DU$3)+1-$DU$3)","v":2.0808378925837281},{"$f":"(IF($AH$29<DEGREES(BT53),0+$AJ$33,1-((TAN(BT53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY79*$DU$3)+1-$DU$3)","v":1.6986829717752732},{"$f":"(IF($AH$29<DEGREES(BU53),0+$AJ$33,1-((TAN(BU53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ79*$DU$3)+1-$DU$3)","v":1.3416209454520394},{"$f":"(IF($AH$29<DEGREES(BV53),0+$AJ$33,1-((TAN(BV53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA79*$DU$3)+1-$DU$3)","v":0.91367762823923826},{"$f":"(IF($AH$29<DEGREES(BW53),0+$AJ$33,1-((TAN(BW53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB79*$DU$3)+1-$DU$3)","v":0.60128658696491155},{"$f":"(IF($AH$29<DEGREES(BX53),0+$AJ$33,1-((TAN(BX53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC79*$DU$3)+1-$DU$3)","v":0.52668713047721238},{"$f":"(IF($AH$29<DEGREES(BY53),0+$AJ$33,1-((TAN(BY53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD79*$DU$3)+1-$DU$3)","v":0.65988472592323044},{"$f":"(IF($AH$29<DEGREES(BZ53),0+$AJ$33,1-((TAN(BZ53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE79*$DU$3)+1-$DU$3)","v":0.92158864412692443},{"$f":"(IF($AH$29<DEGREES(CA53),0+$AJ$33,1-((TAN(CA53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF79*$DU$3)+1-$DU$3)","v":1.3407877656520557},{"$f":"(IF($AH$29<DEGREES(CB53),0+$AJ$33,1-((TAN(CB53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG79*$DU$3)+1-$DU$3)","v":1.8288440565187396},{"$f":"(IF($AH$29<DEGREES(CC53),0+$AJ$33,1-((TAN(CC53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH79*$DU$3)+1-$DU$3)","v":2.3040174421243447},{"$f":"(IF($AH$29<DEGREES(CD53),0+$AJ$33,1-((TAN(CD53)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI79*$DU$3)+1-$DU$3)","v":2.2041979740985673},null,22,{"$f":"(IF($AH$12<DEGREES(CG53),0+$AJ$16,1-((TAN(CG53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL79*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH53),0+$AJ$16,1-((TAN(CH53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM79*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CI53),0+$AJ$16,1-((TAN(CI53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN79*$DU$3)+1-$DU$3)","v":0.51259085737628951},{"$f":"(IF($AH$12<DEGREES(CJ53),0+$AJ$16,1-((TAN(CJ53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO79*$DU$3)+1-$DU$3)","v":0.98168918294664198},{"$f":"(IF($AH$12<DEGREES(CK53),0+$AJ$16,1-((TAN(CK53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP79*$DU$3)+1-$DU$3)","v":1.0259604260129886},{"$f":"(IF($AH$12<DEGREES(CL53),0+$AJ$16,1-((TAN(CL53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ79*$DU$3)+1-$DU$3)","v":0.99911256526312908},{"$f":"(IF($AH$12<DEGREES(CM53),0+$AJ$16,1-((TAN(CM53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR79*$DU$3)+1-$DU$3)","v":0.96936141840311363},{"$f":"(IF($AH$12<DEGREES(CN53),0+$AJ$16,1-((TAN(CN53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS79*$DU$3)+1-$DU$3)","v":0.95363620417948125},{"$f":"(IF($AH$12<DEGREES(CO53),0+$AJ$16,1-((TAN(CO53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT79*$DU$3)+1-$DU$3)","v":0.78612965191524864},{"$f":"(IF($AH$12<DEGREES(CP53),0+$AJ$16,1-((TAN(CP53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU79*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CQ53),0+$AJ$16,1-((TAN(CQ53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV79*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR53),0+$AJ$16,1-((TAN(CR53)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW79*$DU$3)+1-$DU$3)","v":0},null,null,22,-57.730536859646747,-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132,null,22,-57.730536859646747,-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132]
[null,24,{"$f":"IF('Dry Bulb'!D28<60,(('Input Data'!$F$44*('Dry Bulb'!D28-$T$15))+('Heat gain from airflow'!Q27)+((Occupancy!P27*'Input Data'!$F$47)+(Occupancy!B27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!D28-$P$15))+('Heat gain from airflow'!Q27)+((Occupancy!P27*'Input Data'!$F$47)+(Occupancy!B27*'Input Data'!$F$49))))/1000","v":-4.3975350000000002E-3},{"$f":"IF('Dry Bulb'!E28<60,(('Input Data'!$F$44*('Dry Bulb'!E28-$T$15))+('Heat gain from airflow'!R27)+((Occupancy!Q27*'Input Data'!$F$47)+(Occupancy!C27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!E28-$P$15))+('Heat gain from airflow'!R27)+((Occupancy!Q27*'Input Data'!$F$47)+(Occupancy!C27*'Input Data'!$F$49))))/1000","v":-2.4899849999999997E-3},{"$f":"IF('Dry Bulb'!F28<60,(('Input Data'!$F$44*('Dry Bulb'!F28-$T$15))+('Heat gain from airflow'!S27)+((Occupancy!R27*'Input Data'!$F$47)+(Occupancy!D27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!F28-$P$15))+('Heat gain from airflow'!S27)+((Occupancy!R27*'Input Data'!$F$47)+(Occupancy!D27*'Input Data'!$F$49))))/1000","v":-3.3082353899999979},{"$f":"IF('Dry Bulb'!G28<60,(('Input Data'!$F$44*('Dry Bulb'!G28-$T$15))+('Heat gain from airflow'!T27)+((Occupancy!S27*'Input Data'!$F$47)+(Occupancy!E27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!G28-$P$15))+('Heat gain from airflow'!T27)+((Occupancy!S27*'Input Data'!$F$47)+(Occupancy!E27*'Input Data'!$F$49))))/1000","v":2.2042815749999978},{"$f":"IF('Dry Bulb'!H28<60,(('Input Data'!$F$44*('Dry Bulb'!H28-$T$15))+('Heat gain from airflow'!U27)+((Occupancy!T27*'Input Data'!$F$47)+(Occupancy!F27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!H28-$P$15))+('Heat gain from airflow'!U27)+((Occupancy!T27*'Input Data'!$F$47)+(Occupancy!F27*'Input Data'!$F$49))))/1000","v":8.584402500000003},{"$f":"IF('Dry Bulb'!I28<60,(('Input Data'!$F$44*('Dry Bulb'!I28-$T$15))+('Heat gain from airflow'!V27)+((Occupancy!U27*'Input Data'!$F$47)+(Occupancy!G27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!I28-$P$15))+('Heat gain from airflow'!V27)+((Occupancy!U27*'Input Data'!$F$47)+(Occupancy!G27*'Input Data'!$F$49))))/1000","v":11.159594999999996},{"$f":"IF('Dry Bulb'!J28<60,(('Input Data'!$F$44*('Dry Bulb'!J28-$T$15))+('Heat gain from airflow'!W27)+((Occupancy!V27*'Input Data'!$F$47)+(Occupancy!H27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!J28-$P$15))+('Heat gain from airflow'!W27)+((Occupancy!V27*'Input Data'!$F$47)+(Occupancy!H27*'Input Data'!$F$49))))/1000","v":11.541105000000003},{"$f":"IF('Dry Bulb'!K28<60,(('Input Data'!$F$44*('Dry Bulb'!K28-$T$15))+('Heat gain from airflow'!X27)+((Occupancy!W27*'Input Data'!$F$47)+(Occupancy!I27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!K28-$P$15))+('Heat gain from airflow'!X27)+((Occupancy!W27*'Input Data'!$F$47)+(Occupancy!I27*'Input Data'!$F$49))))/1000","v":12.113370000000002},{"$f":"IF('Dry Bulb'!L28<60,(('Input Data'!$F$44*('Dry Bulb'!L28-$T$15))+('Heat gain from airflow'!Y27)+((Occupancy!X27*'Input Data'!$F$47)+(Occupancy!J27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!L28-$P$15))+('Heat gain from airflow'!Y27)+((Occupancy!X27*'Input Data'!$F$47)+(Occupancy!J27*'Input Data'!$F$49))))/1000","v":9.1566675000000028},{"$f":"IF('Dry Bulb'!M28<60,(('Input Data'!$F$44*('Dry Bulb'!M28-$T$15))+('Heat gain from airflow'!Z27)+((Occupancy!Y27*'Input Data'!$F$47)+(Occupancy!K27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!M28-$P$15))+('Heat gain from airflow'!Z27)+((Occupancy!Y27*'Input Data'!$F$47)+(Occupancy!K27*'Input Data'!$F$49))))/1000","v":4.3154582850000045},{"$f":"IF('Dry Bulb'!N28<60,(('Input Data'!$F$44*('Dry Bulb'!N28-$T$15))+('Heat gain from airflow'!AA27)+((Occupancy!Z27*'Input Data'!$F$47)+(Occupancy!L27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!N28-$P$15))+('Heat gain from airflow'!AA27)+((Occupancy!Z27*'Input Data'!$F$47)+(Occupancy!L27*'Input Data'!$F$49))))/1000","v":-2.8390850099999989},{"$f":"IF('Dry Bulb'!O28<60,(('Input Data'!$F$44*('Dry Bulb'!O28-$T$15))+('Heat gain from airflow'!AB27)+((Occupancy!AA27*'Input Data'!$F$47)+(Occupancy!M27*'Input Data'!$F$49)))/1000,(('Input Data'!$F$44*('Dry Bulb'!O28-$P$15))+('Heat gain from airflow'!AB27)+((Occupancy!AA27*'Input Data'!$F$47)+(Occupancy!M27*'Input Data'!$F$49))))/1000","v":-4.2067800000000011E-3},null,null,11,null,null,null,null,null,"Chhaya© 2009 Vikram Sami ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Profile angles'!P27","v":23},{"$f":"RADIANS('Profile angles'!Q27)","v":-1.2495488396557735},{"$f":"RADIANS('Profile angles'!R27)","v":-1.2145605673757462},{"$f":"RADIANS('Profile angles'!S27)","v":-1.2149427363314722},{"$f":"RADIANS('Profile angles'!T27)","v":-1.2226710666204359},{"$f":"RADIANS('Profile angles'!U27)","v":-1.2055266879907172},{"$f":"RADIANS('Profile angles'!V27)","v":-1.1656612779447801},{"$f":"RADIANS('Profile angles'!W27)","v":-1.1517497376977255},{"$f":"RADIANS('Profile angles'!X27)","v":-1.2039013058414902},{"$f":"RADIANS('Profile angles'!Y27)","v":-1.2857310025410158},{"$f":"RADIANS('Profile angles'!Z27)","v":-1.3427580313462966},{"$f":"RADIANS('Profile angles'!AA27)","v":-1.3516188465533332},{"$f":"RADIANS('Profile angles'!AB27)","v":-1.309046406575489},null,{"$f":"'Profile angles'!P56","v":23},{"$f":"RADIANS('Profile angles'!Q56)","v":-1.5065295005919663},{"$f":"RADIANS('Profile angles'!R56)","v":-1.3366001752956176},{"$f":"RADIANS('Profile angles'!S56)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!T56)","v":-0.92334688213375749},{"$f":"RADIANS('Profile angles'!U56)","v":-0.77241907924890529},{"$f":"RADIANS('Profile angles'!V56)","v":-0.71359161627872214},{"$f":"RADIANS('Profile angles'!W56)","v":-0.76448334246392102},{"$f":"RADIANS('Profile angles'!X56)","v":-0.91872689706604016},{"$f":"RADIANS('Profile angles'!Y56)","v":-1.1397000015522973},{"$f":"RADIANS('Profile angles'!Z56)","v":-1.3311946610818084},{"$f":"RADIANS('Profile angles'!AA56)","v":-1.495858034964566},{"$f":"RADIANS('Profile angles'!AB56)","v":-1.5643267445715632},null,{"$f":"'Profile angles'!AR27","v":23},{"$f":"(IF($AH$29<DEGREES(BS54),0+$AJ$33,1-((TAN(BS54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX80*$DU$3)+1-$DU$3)","v":2.8034303472885287},{"$f":"(IF($AH$29<DEGREES(BT54),0+$AJ$33,1-((TAN(BT54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY80*$DU$3)+1-$DU$3)","v":1.9575506603652253},{"$f":"(IF($AH$29<DEGREES(BU54),0+$AJ$33,1-((TAN(BU54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ80*$DU$3)+1-$DU$3)","v":1.0992839539792583},{"$f":"(IF($AH$29<DEGREES(BV54),0+$AJ$33,1-((TAN(BV54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA80*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BW54),0+$AJ$33,1-((TAN(BW54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB80*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BX54),0+$AJ$33,1-((TAN(BX54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC80*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BY54),0+$AJ$33,1-((TAN(BY54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD80*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BZ54),0+$AJ$33,1-((TAN(BZ54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE80*$DU$3)+1-$DU$3)","v":1.8780224215121575E-2},{"$f":"(IF($AH$29<DEGREES(CA54),0+$AJ$33,1-((TAN(CA54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF80*$DU$3)+1-$DU$3)","v":0.72934768155388352},{"$f":"(IF($AH$29<DEGREES(CB54),0+$AJ$33,1-((TAN(CB54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG80*$DU$3)+1-$DU$3)","v":1.9023981341396716},{"$f":"(IF($AH$29<DEGREES(CC54),0+$AJ$33,1-((TAN(CC54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH80*$DU$3)+1-$DU$3)","v":3.4443552607726806},{"$f":"(IF($AH$29<DEGREES(CD54),0+$AJ$33,1-((TAN(CD54)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI80*$DU$3)+1-$DU$3)","v":3.5693263173807281},null,23,{"$f":"(IF($AH$12<DEGREES(CG54),0+$AJ$16,1-((TAN(CG54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL80*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CH54),0+$AJ$16,1-((TAN(CH54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM80*$DU$3)+1-$DU$3)","v":0.86602977112640445},{"$f":"(IF($AH$12<DEGREES(CI54),0+$AJ$16,1-((TAN(CI54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN80*$DU$3)+1-$DU$3)","v":1.50295407518346},{"$f":"(IF($AH$12<DEGREES(CJ54),0+$AJ$16,1-((TAN(CJ54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO80*$DU$3)+1-$DU$3)","v":1.4636114251139041},{"$f":"(IF($AH$12<DEGREES(CK54),0+$AJ$16,1-((TAN(CK54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP80*$DU$3)+1-$DU$3)","v":1.368667434534373},{"$f":"(IF($AH$12<DEGREES(CL54),0+$AJ$16,1-((TAN(CL54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ80*$DU$3)+1-$DU$3)","v":1.3078882071895535},{"$f":"(IF($AH$12<DEGREES(CM54),0+$AJ$16,1-((TAN(CM54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR80*$DU$3)+1-$DU$3)","v":1.3143418217082061},{"$f":"(IF($AH$12<DEGREES(CN54),0+$AJ$16,1-((TAN(CN54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS80*$DU$3)+1-$DU$3)","v":1.4344343084478648},{"$f":"(IF($AH$12<DEGREES(CO54),0+$AJ$16,1-((TAN(CO54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT80*$DU$3)+1-$DU$3)","v":1.7185185960363556},{"$f":"(IF($AH$12<DEGREES(CP54),0+$AJ$16,1-((TAN(CP54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU80*$DU$3)+1-$DU$3)","v":2.0293692507184349},{"$f":"(IF($AH$12<DEGREES(CQ54),0+$AJ$16,1-((TAN(CQ54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV80*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$12<DEGREES(CR54),0+$AJ$16,1-((TAN(CR54)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW80*$DU$3)+1-$DU$3)","v":0},null,null,23,-71.276413671366612,-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272,null,23,-71.276413671366612,-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Profile angles'!P28","v":24},{"$f":"RADIANS('Profile angles'!Q28)","v":-1.4953307389576809},{"$f":"RADIANS('Profile angles'!R28)","v":-1.4778229951074291},{"$f":"RADIANS('Profile angles'!S28)","v":-1.5005364967084427},{"$f":"RADIANS('Profile angles'!T28)","v":-1.5387122061758483},{"$f":"RADIANS('Profile angles'!U28)","v":-1.5486122132899969},{"$f":"RADIANS('Profile angles'!V28)","v":-1.5196104703977529},{"$f":"RADIANS('Profile angles'!W28)","v":-1.4935003073579078},{"$f":"RADIANS('Profile angles'!X28)","v":-1.5200112597578945},{"$f":"RADIANS('Profile angles'!Y28)","v":-1.5690353246394813},{"$f":"RADIANS('Profile angles'!Z28)","v":-1.5342706134006174},{"$f":"RADIANS('Profile angles'!AA28)","v":-1.5433489980684403},{"$f":"RADIANS('Profile angles'!AB28)","v":-1.5486418126575425},null,{"$f":"'Profile angles'!P57","v":24},{"$f":"RADIANS('Profile angles'!Q57)","v":-1.4880469068104962},{"$f":"RADIANS('Profile angles'!R57)","v":-1.325468937525877},{"$f":"RADIANS('Profile angles'!S57)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!T57)","v":-0.9319358845770338},{"$f":"RADIANS('Profile angles'!U57)","v":-0.78535264346749045},{"$f":"RADIANS('Profile angles'!V57)","v":-0.73016710880727165},{"$f":"RADIANS('Profile angles'!W57)","v":-0.78135170593207048},{"$f":"RADIANS('Profile angles'!X57)","v":-0.92833771723835001},{"$f":"RADIANS('Profile angles'!Y57)","v":-1.1397000015522971},{"$f":"RADIANS('Profile angles'!Z57)","v":-1.3265689743998734},{"$f":"RADIANS('Profile angles'!AA57)","v":-1.4871559725393455},{"$f":"RADIANS('Profile angles'!AB57)","v":-1.5490861384984902},null,{"$f":"'Profile angles'!AR28","v":24},{"$f":"(IF($AH$29<DEGREES(BS55),0+$AJ$33,1-((TAN(BS55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BX81*$DU$3)+1-$DU$3)","v":4.6318502392156375},{"$f":"(IF($AH$29<DEGREES(BT55),0+$AJ$33,1-((TAN(BT55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BY81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BU55),0+$AJ$33,1-((TAN(BU55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!BZ81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BV55),0+$AJ$33,1-((TAN(BV55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CA81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BW55),0+$AJ$33,1-((TAN(BW55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CB81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BX55),0+$AJ$33,1-((TAN(BX55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CC81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BY55),0+$AJ$33,1-((TAN(BY55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CD81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(BZ55),0+$AJ$33,1-((TAN(BZ55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CE81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CA55),0+$AJ$33,1-((TAN(CA55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CF81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CB55),0+$AJ$33,1-((TAN(CB55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CG81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CC55),0+$AJ$33,1-((TAN(CC55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CH81*$DU$3)+1-$DU$3)","v":0},{"$f":"(IF($AH$29<DEGREES(CD55),0+$AJ$33,1-((TAN(CD55)/TAN($AG$31))*(1-$AJ$33))))*(('Surface Solar Azimuth Angles'!CI81*$DU$3)+1-$DU$3)","v":16.622473558246917},null,24,{"$f":"(IF($AH$12<DEGREES(CG55),0+$AJ$16,1-((TAN(CG55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CL81*$DU$3)+1-$DU$3)","v":5.1371019586487741},{"$f":"(IF($AH$12<DEGREES(CH55),0+$AJ$16,1-((TAN(CH55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CM81*$DU$3)+1-$DU$3)","v":3.0890360638460339},{"$f":"(IF($AH$12<DEGREES(CI55),0+$AJ$16,1-((TAN(CI55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CN81*$DU$3)+1-$DU$3)","v":2.3289734177578629},{"$f":"(IF($AH$12<DEGREES(CJ55),0+$AJ$16,1-((TAN(CJ55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CO81*$DU$3)+1-$DU$3)","v":1.9004474370473066},{"$f":"(IF($AH$12<DEGREES(CK55),0+$AJ$16,1-((TAN(CK55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CP81*$DU$3)+1-$DU$3)","v":1.681079108386534},{"$f":"(IF($AH$12<DEGREES(CL55),0+$AJ$16,1-((TAN(CL55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CQ81*$DU$3)+1-$DU$3)","v":1.5893517055171236},{"$f":"(IF($AH$12<DEGREES(CM55),0+$AJ$16,1-((TAN(CM55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CR81*$DU$3)+1-$DU$3)","v":1.6292723515525944},{"$f":"(IF($AH$12<DEGREES(CN55),0+$AJ$16,1-((TAN(CN55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CS81*$DU$3)+1-$DU$3)","v":1.8696391795625678},{"$f":"(IF($AH$12<DEGREES(CO55),0+$AJ$16,1-((TAN(CO55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CT81*$DU$3)+1-$DU$3)","v":2.517081339485101},{"$f":"(IF($AH$12<DEGREES(CP55),0+$AJ$16,1-((TAN(CP55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CU81*$DU$3)+1-$DU$3)","v":3.5297016800139001},{"$f":"(IF($AH$12<DEGREES(CQ55),0+$AJ$16,1-((TAN(CQ55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CV81*$DU$3)+1-$DU$3)","v":7.8187512313205128},{"$f":"(IF($AH$12<DEGREES(CR55),0+$AJ$16,1-((TAN(CR55)/TAN($AG$14))*(1-$AJ$16))))*(('Surface Solar Azimuth Angles'!CW81*$DU$3)+1-$DU$3)","v":16.278693033686348},null,null,24,-83.596484892158756,-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205,null,24,-83.596484892158756,-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205]
[null,"Total Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UAdeltaT+Solar - South",null,null,null,null,null,null,null,null,null,null,null,null,null,"UAdeltaT+Solar - East",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($AH$29<DEGREES(BS56),0+$AJ$33,1-((TAN(BS56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BT56),0+$AJ$33,1-((TAN(BT56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BU56),0+$AJ$33,1-((TAN(BU56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BV56),0+$AJ$33,1-((TAN(BV56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BW56),0+$AJ$33,1-((TAN(BW56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BX56),0+$AJ$33,1-((TAN(BX56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BY56),0+$AJ$33,1-((TAN(BY56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BZ56),0+$AJ$33,1-((TAN(BZ56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CA56),0+$AJ$33,1-((TAN(CA56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CB56),0+$AJ$33,1-((TAN(CB56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CC56),0+$AJ$33,1-((TAN(CC56)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CD56),0+$AJ$33,1-((TAN(CD56)/TAN($AG$31))*(1-$AJ$16)))","v":1}]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec","Average","HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec","Average",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,1,{"$f":"(AQ5)+(BE5)+(AQ32)+(BE32)","v":0},{"$f":"(AR5)+(BF5)+(AR32)+(BF32)","v":0},{"$f":"(AS5)+(BG5)+(AS32)+(BG32)","v":0},{"$f":"(AT5)+(BH5)+(AT32)+(BH32)","v":0},{"$f":"(AU5)+(BI5)+(AU32)+(BI32)","v":0},{"$f":"(AV5)+(BJ5)+(AV32)+(BJ32)","v":0},{"$f":"(AW5)+(BK5)+(AW32)+(BK32)","v":0},{"$f":"(AX5)+(BL5)+(AX32)+(BL32)","v":0},{"$f":"(AY5)+(BM5)+(AY32)+(BM32)","v":0},{"$f":"(AZ5)+(BN5)+(AZ32)+(BN32)","v":0},{"$f":"(BA5)+(BO5)+(BA32)+(BO32)","v":0},{"$f":"(BB5)+(BP5)+(BB32)+(BP32)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D5-'Operative BP'!$P$15))+AQ5","v":-2588.0400000000004},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E5-'Operative BP'!$P$15))+AR5","v":-2061.5400000000004},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F5-'Operative BP'!$P$15))+AS5","v":-1261.2600000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G5-'Operative BP'!$P$15))+AT5","v":-229.31999999999925},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H5-'Operative BP'!$P$15))+AU5","v":1118.5200000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I5-'Operative BP'!$P$15))+AV5","v":1708.1999999999994},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J5-'Operative BP'!$P$15))+AW5","v":1855.62},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K5-'Operative BP'!$P$15))+AX5","v":1918.8000000000006},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L5-'Operative BP'!$P$15))+AY5","v":1265.9399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M5-'Operative BP'!$P$15))+AZ5","v":128.69999999999933},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N5-'Operative BP'!$P$15))+BA5","v":-1155.9599999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O5-'Operative BP'!$P$15))+BB5","v":-2356.38},{"$f":"AVERAGEIF(AS58:AZ81,\">0\")","v":1945.1771039161772},1,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D5-'Operative BP'!$P$15))+BE5","v":-2488.5000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E5-'Operative BP'!$P$15))+BF5","v":-1982.2500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F5-'Operative BP'!$P$15))+BG5","v":-1212.7500000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G5-'Operative BP'!$P$15))+BH5","v":-220.49999999999929},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H5-'Operative BP'!$P$15))+BI5","v":1075.5000000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I5-'Operative BP'!$P$15))+BJ5","v":1642.4999999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J5-'Operative BP'!$P$15))+BK5","v":1784.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K5-'Operative BP'!$P$15))+BL5","v":1845.0000000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L5-'Operative BP'!$P$15))+BM5","v":1217.2499999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M5-'Operative BP'!$P$15))+BN5","v":123.74999999999936},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N5-'Operative BP'!$P$15))+BO5","v":-1111.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O5-'Operative BP'!$P$15))+BP5","v":-2265.75},{"$f":"AVERAGEIF(BG58:BN81,\">0\")","v":2160.1100591743261},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,2,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,"Heat Load",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D6-'Operative BP'!$P$15))+AQ6","v":-2693.34},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E6-'Operative BP'!$P$15))+AR6","v":-2187.9000000000005},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F6-'Operative BP'!$P$15))+AS6","v":-1408.6800000000007},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G6-'Operative BP'!$P$15))+AT6","v":-355.68000000000075},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H6-'Operative BP'!$P$15))+AU6","v":950.04000000000053},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I6-'Operative BP'!$P$15))+AV6","v":1497.5999999999997},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J6-'Operative BP'!$P$15))+AW6","v":1666.0799999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K6-'Operative BP'!$P$15))+AX6","v":1729.2600000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L6-'Operative BP'!$P$15))+AY6","v":1055.3399999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M6-'Operative BP'!$P$15))+AZ6","v":-18.719999999999601},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N6-'Operative BP'!$P$15))+BA6","v":-1345.5},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O6-'Operative BP'!$P$15))+BB6","v":-2440.62},"Max",2,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D6-'Operative BP'!$P$15))+BE6","v":-2589.7500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E6-'Operative BP'!$P$15))+BF6","v":-2103.7500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F6-'Operative BP'!$P$15))+BG6","v":-1354.5000000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G6-'Operative BP'!$P$15))+BH6","v":-342.00000000000068},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H6-'Operative BP'!$P$15))+BI6","v":913.50000000000045},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I6-'Operative BP'!$P$15))+BJ6","v":1439.9999999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J6-'Operative BP'!$P$15))+BK6","v":1601.9999999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K6-'Operative BP'!$P$15))+BL6","v":1662.7500000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L6-'Operative BP'!$P$15))+BM6","v":1014.7499999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M6-'Operative BP'!$P$15))+BN6","v":-17.999999999999616},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N6-'Operative BP'!$P$15))+BO6","v":-1293.75},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O6-'Operative BP'!$P$15))+BP6","v":-2346.75},"Max",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"(AQ7)+(BE7)+(AQ34)+(BE34)","v":0},0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,{"$f":"SUM(C111:N134)*-1*(365/12)","v":4664.7379602281262},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D7-'Operative BP'!$P$15))+AQ7","v":-2756.5200000000004},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E7-'Operative BP'!$P$15))+AR7","v":-2314.2600000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F7-'Operative BP'!$P$15))+AS7","v":-1556.0999999999997},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G7-'Operative BP'!$P$15))+AT7","v":-482.04000000000053},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H7-'Operative BP'!$P$15))+AU7","v":823.68000000000075},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I7-'Operative BP'!$P$15))+AV7","v":1392.3000000000006},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J7-'Operative BP'!$P$15))+AW7","v":1539.7199999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K7-'Operative BP'!$P$15))+AX7","v":1539.7199999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L7-'Operative BP'!$P$15))+AY7","v":865.80000000000064},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M7-'Operative BP'!$P$15))+AZ7","v":-208.26000000000013},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N7-'Operative BP'!$P$15))+BA7","v":-1492.9199999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O7-'Operative BP'!$P$15))+BB7","v":-2524.8599999999997},{"$f":"MAX(AT58:AY81)","v":3961.62},3,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D7-'Operative BP'!$P$15))+BE7","v":-2650.5000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E7-'Operative BP'!$P$15))+BF7","v":-2225.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F7-'Operative BP'!$P$15))+BG7","v":-1496.2499999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G7-'Operative BP'!$P$15))+BH7","v":-463.50000000000051},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H7-'Operative BP'!$P$15))+BI7","v":792.00000000000068},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I7-'Operative BP'!$P$15))+BJ7","v":1338.7500000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J7-'Operative BP'!$P$15))+BK7","v":1480.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K7-'Operative BP'!$P$15))+BL7","v":1480.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L7-'Operative BP'!$P$15))+BM7","v":832.50000000000068},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M7-'Operative BP'!$P$15))+BN7","v":-200.25000000000011},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N7-'Operative BP'!$P$15))+BO7","v":-1435.4999999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O7-'Operative BP'!$P$15))+BP7","v":-2427.75},{"$f":"MAX(BH58:BM81)","v":6197.5863600764733},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$f":"AVERAGEIF(E58:L81,\">0\")","v":2405.2673084977591},"Average All",null,null,{"$f":"T60/(T9*P3*P6)","v":5.1830421780312514},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D8-'Operative BP'!$P$15))+AQ8","v":-2861.82},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E8-'Operative BP'!$P$15))+AR8","v":-2440.62},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F8-'Operative BP'!$P$15))+AS8","v":-1661.4000000000003},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G8-'Operative BP'!$P$15))+AT8","v":-650.52000000000021},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H8-'Operative BP'!$P$15))+AU8","v":760.5},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I8-'Operative BP'!$P$15))+AV8","v":1265.9399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J8-'Operative BP'!$P$15))+AW8","v":1371.2399999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K8-'Operative BP'!$P$15))+AX8","v":1392.3000000000006},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L8-'Operative BP'!$P$15))+AY8","v":697.31999999999925},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M8-'Operative BP'!$P$15))+AZ8","v":-292.5},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N8-'Operative BP'!$P$15))+BA8","v":-1640.3399999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O8-'Operative BP'!$P$15))+BB8","v":-2630.16},"Av+Max/2",4,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D8-'Operative BP'!$P$15))+BE8","v":-2751.75},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E8-'Operative BP'!$P$15))+BF8","v":-2346.75},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F8-'Operative BP'!$P$15))+BG8","v":-1597.5000000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G8-'Operative BP'!$P$15))+BH8","v":-625.50000000000023},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H8-'Operative BP'!$P$15))+BI8","v":731.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I8-'Operative BP'!$P$15))+BJ8","v":1217.2499999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J8-'Operative BP'!$P$15))+BK8","v":1318.4999999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K8-'Operative BP'!$P$15))+BL8","v":1338.7500000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L8-'Operative BP'!$P$15))+BM8","v":670.49999999999932},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M8-'Operative BP'!$P$15))+BN8","v":-281.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N8-'Operative BP'!$P$15))+BO8","v":-1577.2499999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O8-'Operative BP'!$P$15))+BP8","v":-2528.9999999999995},"Av+Max/2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$f":"MAX(E58:L81)","v":5622.3905501017762},"Max All",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D9-'Operative BP'!$P$15))+AQ9","v":-2988.18},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E9-'Operative BP'!$P$15))+AR9","v":-2524.8599999999997},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F9-'Operative BP'!$P$15))+AS9","v":-1766.7000000000003},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G9-'Operative BP'!$P$15))+AT9","v":-776.88000000000011},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H9-'Operative BP'!$P$15))+AU9","v":592.02000000000021},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I9-'Operative BP'!$P$15))+AV9","v":1118.5200000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J9-'Operative BP'!$P$15))+AW9","v":1287},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K9-'Operative BP'!$P$15))+AX9","v":1265.9399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L9-'Operative BP'!$P$15))+AY9","v":613.08000000000106},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M9-'Operative BP'!$P$15))+AZ9","v":-460.97999999999973},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N9-'Operative BP'!$P$15))+BA9","v":-1808.8199999999993},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O9-'Operative BP'!$P$15))+BB9","v":-2735.4599999999996},{"$f":"AVERAGE(BC58,BC60)","v":2953.3985519580883},5,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D9-'Operative BP'!$P$15))+BE9","v":-2873.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E9-'Operative BP'!$P$15))+BF9","v":-2427.75},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F9-'Operative BP'!$P$15))+BG9","v":-1698.7500000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G9-'Operative BP'!$P$15))+BH9","v":-747.00000000000011},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H9-'Operative BP'!$P$15))+BI9","v":569.25000000000023},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I9-'Operative BP'!$P$15))+BJ9","v":1075.5000000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J9-'Operative BP'!$P$15))+BK9","v":1237.5},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K9-'Operative BP'!$P$15))+BL9","v":1217.2499999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L9-'Operative BP'!$P$15))+BM9","v":589.50000000000102},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M9-'Operative BP'!$P$15))+BN9","v":-443.24999999999977},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N9-'Operative BP'!$P$15))+BO9","v":-1739.2499999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O9-'Operative BP'!$P$15))+BP9","v":-2630.2499999999995},{"$f":"AVERAGE(BQ58,BQ60)","v":4178.8482096253992},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,0,0,0,85.291254678098866,200.04067612922577,238.69148403224921,151.55996159633474,85.484580900045813,49.076156240520959,0,0,0,null,null,null,null,null,"Cool Load",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D10-'Operative BP'!$P$15))+AQ10","v":-3051.3599999999997},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E10-'Operative BP'!$P$15))+AR10","v":-2609.0999999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F10-'Operative BP'!$P$15))+AS10","v":-1829.88},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G10-'Operative BP'!$P$15))+AT10","v":-861.11999999999989},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H10-'Operative BP'!$P$15))+AU10","v":444.59999999999968},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I10-'Operative BP'!$P$15))+AV10","v":992.16000000000042},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J10-'Operative BP'!$P$15))+AW10","v":1202.7600000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K10-'Operative BP'!$P$15))+AX10","v":1160.6399999999985},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L10-'Operative BP'!$P$15))+AY10","v":549.90000000000032},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M10-'Operative BP'!$P$15))+AZ10","v":-566.28000000000043},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N10-'Operative BP'!$P$15))+BA10","v":-1850.94},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O10-'Operative BP'!$P$15))+BB10","v":-2735.4599999999996},null,6,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D10-'Operative BP'!$P$15))+BE10","v":-2934},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E10-'Operative BP'!$P$15))+BF10","v":-2508.7499999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F10-'Operative BP'!$P$15))+BG10","v":-1759.5},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G10-'Operative BP'!$P$15))+BH10","v":-742.70874532190101},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H10-'Operative BP'!$P$15))+BI10","v":627.5406761292254},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I10-'Operative BP'!$P$15))+BJ10","v":1192.6914840322497},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J10-'Operative BP'!$P$15))+BK10","v":1308.0599615963349},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K10-'Operative BP'!$P$15))+BL10","v":1201.4845809000444},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L10-'Operative BP'!$P$15))+BM10","v":577.8261562405213},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M10-'Operative BP'!$P$15))+BN10","v":-544.50000000000034},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N10-'Operative BP'!$P$15))+BO10","v":-1779.75},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O10-'Operative BP'!$P$15))+BP10","v":-2630.2499999999995},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,64.898513253972396,165.40677030899579,477.20353172430015,1430.2072767776865,1823.5313692542443,1967.8167757820027,1633.0294584747032,1462.7309965171892,1232.2064066489952,786.71694263200231,234.94895166423882,97.889730060419623,null,{"$f":"AVERAGE(P61:P62)","v":4013.8289292997679},null,null,null,{"$f":"SUM(C137:N160)*(365/12)","v":57341.417630906246},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D11-'Operative BP'!$P$15))+AQ11","v":-3051.3599999999997},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E11-'Operative BP'!$P$15))+AR11","v":-2609.0999999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F11-'Operative BP'!$P$15))+AS11","v":-1829.88},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G11-'Operative BP'!$P$15))+AT11","v":-650.52000000000021},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H11-'Operative BP'!$P$15))+AU11","v":676.2600000000001},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I11-'Operative BP'!$P$15))+AV11","v":1329.12},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J11-'Operative BP'!$P$15))+AW11","v":1518.6600000000005},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K11-'Operative BP'!$P$15))+AX11","v":1455.4799999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L11-'Operative BP'!$P$15))+AY11","v":781.56000000000085},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M11-'Operative BP'!$P$15))+AZ11","v":-460.97999999999973},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N11-'Operative BP'!$P$15))+BA11","v":-1893.06},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O11-'Operative BP'!$P$15))+BB11","v":-2776.0608353218695},null,7,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D11-'Operative BP'!$P$15))+BE11","v":-2869.1014867460276},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E11-'Operative BP'!$P$15))+BF11","v":-2343.3432296910037},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F11-'Operative BP'!$P$15))+BG11","v":-1282.2964682756999},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G11-'Operative BP'!$P$15))+BH11","v":804.70727677768627},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H11-'Operative BP'!$P$15))+BI11","v":2473.7813692542445},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I11-'Operative BP'!$P$15))+BJ11","v":3245.8167757820029},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J11-'Operative BP'!$P$15))+BK11","v":3093.2794584747035},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K11-'Operative BP'!$P$15))+BL11","v":2862.2309965171889},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L11-'Operative BP'!$P$15))+BM11","v":1983.7064066489961},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M11-'Operative BP'!$P$15))+BN11","v":343.46694263200254},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N11-'Operative BP'!$P$15))+BO11","v":-1585.3010483357612},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O11-'Operative BP'!$P$15))+BP11","v":-2574.3794346177115},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,1241.5929894223018,1580.2679856218936,2274.2562020804671,3450.0632210657404,3430.0891695915338,3624.4253921251366,3506.0504040840974,3701.4693967750522,3245.9243592338794,2588.9845220993402,1925.9803833288147,1308.3238737193474,null,null,null,null,null,{"$f":"T64/(T9*P3*P6)","v":63.712686256562499},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D12-'Operative BP'!$P$15))+AQ12","v":-2650.278694309809},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E12-'Operative BP'!$P$15))+AR12","v":-2335.3200000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F12-'Operative BP'!$P$15))+AS12","v":-1471.86},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G12-'Operative BP'!$P$15))+AT12","v":-271.4399999999992},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H12-'Operative BP'!$P$15))+AU12","v":1097.4600000000012},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I12-'Operative BP'!$P$15))+AV12","v":1750.3200000000008},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J12-'Operative BP'!$P$15))+AW12","v":1939.8600000000015},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K12-'Operative BP'!$P$15))+AX12","v":1918.8000000000006},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L12-'Operative BP'!$P$15))+AY12","v":1308.0600000000009},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M12-'Operative BP'!$P$15))+AZ12","v":2.3399999999995345},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N12-'Operative BP'!$P$15))+BA12","v":-960.20112894408589},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O12-'Operative BP'!$P$15))+BB12","v":-2276.9976311050004},null,8,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D12-'Operative BP'!$P$15))+BE12","v":-1556.4583162678898},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E12-'Operative BP'!$P$15))+BF12","v":-665.23201437810644},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F12-'Operative BP'!$P$15))+BG12","v":859.00620208046735},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G12-'Operative BP'!$P$15))+BH12","v":3189.0632210657413},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H12-'Operative BP'!$P$15))+BI12","v":4485.3391695915352},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I12-'Operative BP'!$P$15))+BJ12","v":5307.4253921251375},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J12-'Operative BP'!$P$15))+BK12","v":5371.3004040840988},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K12-'Operative BP'!$P$15))+BL12","v":5546.4693967750527},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L12-'Operative BP'!$P$15))+BM12","v":4503.6743592338798},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M12-'Operative BP'!$P$15))+BN12","v":2591.2345220993398},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N12-'Operative BP'!$P$15))+BO12","v":288.24151227290054},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O12-'Operative BP'!$P$15))+BP12","v":-1491.2184951756528},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,2749.2275008212341,2537.8051388230988,2912.014825963,3360.4158657250155,3200.4903267677082,3403.2308082119139,3720.9239883772384,3826.0863600764724,3354.2128592006602,2988.0593283731764,3099.6411159120394,2349.5832515431184,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D13-'Operative BP'!$P$15))+AQ13","v":-1650.2024277817407},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E13-'Operative BP'!$P$15))+AR13","v":-1879.7558962006324},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F13-'Operative BP'!$P$15))+AS13","v":-1219.1400000000001},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G13-'Operative BP'!$P$15))+AT13","v":234},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H13-'Operative BP'!$P$15))+AU13","v":1434.4200000000005},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I13-'Operative BP'!$P$15))+AV13","v":2150.4600000000009},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J13-'Operative BP'!$P$15))+AW13","v":2445.3000000000006},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K13-'Operative BP'!$P$15))+AX13","v":2466.3600000000015},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L13-'Operative BP'!$P$15))+AY13","v":1792.4399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M13-'Operative BP'!$P$15))+AZ13","v":805.1463941791269},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N13-'Operative BP'!$P$15))+BA13","v":426.32511443189856},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O13-'Operative BP'!$P$15))+BB13","v":-1291.4771889276567},null,9,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D13-'Operative BP'!$P$15))+BE13","v":-429.25007139702507},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E13-'Operative BP'!$P$15))+BF13","v":497.70103502373172},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F13-'Operative BP'!$P$15))+BG13","v":1739.7648259629998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G13-'Operative BP'!$P$15))+BH13","v":3585.4158657250155},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H13-'Operative BP'!$P$15))+BI13","v":4579.7403267677091},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I13-'Operative BP'!$P$15))+BJ13","v":5470.9808082119143},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J13-'Operative BP'!$P$15))+BK13","v":6072.1739883772389},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K13-'Operative BP'!$P$15))+BL13","v":6197.5863600764733},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L13-'Operative BP'!$P$15))+BM13","v":5077.7128592006593},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M13-'Operative BP'!$P$15))+BN13","v":3137.6329341940486},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N13-'Operative BP'!$P$15))+BO13","v":1190.7460014801422},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O13-'Operative BP'!$P$15))+BP13","v":-774.51955952922526},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,2690.2536552472798,1812.2695779055475,1259.1168271411946,97.570769643937751,0,0,8.4277910379317671,454.16199224679519,433.5569407707585,753.06035235792501,2427.8881685207261,2340.1429247453757,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D14-'Operative BP'!$P$15))+AQ14","v":-618.11568939885524},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E14-'Operative BP'!$P$15))+AR14","v":-1325.508106642437},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F14-'Operative BP'!$P$15))+AS14","v":-882.18000000000075},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G14-'Operative BP'!$P$15))+AT14","v":634.14000000000021},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H14-'Operative BP'!$P$15))+AU14","v":1792.4399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I14-'Operative BP'!$P$15))+AV14","v":2508.4799999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J14-'Operative BP'!$P$15))+AW14","v":2887.5600000000009},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K14-'Operative BP'!$P$15))+AX14","v":2950.74},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L14-'Operative BP'!$P$15))+AY14","v":2213.6399999999985},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M14-'Operative BP'!$P$15))+AZ14","v":1318.8276299912891},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N14-'Operative BP'!$P$15))+BA14","v":1679.3064351296152},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O14-'Operative BP'!$P$15))+BB14","v":-144.89136973567133},null,10,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D14-'Operative BP'!$P$15))+BE14","v":-859.35065535386434},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E14-'Operative BP'!$P$15))+BF14","v":-79.812315452014445},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F14-'Operative BP'!$P$15))+BG14","v":410.86682714119388},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G14-'Operative BP'!$P$15))+BH14","v":707.32076964393798},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H14-'Operative BP'!$P$15))+BI14","v":1723.4999999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I14-'Operative BP'!$P$15))+BJ14","v":2411.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J14-'Operative BP'!$P$15))+BK14","v":2784.9277910379328},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K14-'Operative BP'!$P$15))+BL14","v":3291.4119922467953},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L14-'Operative BP'!$P$15))+BM14","v":2562.0569407707571},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M14-'Operative BP'!$P$15))+BN14","v":1256.4627223666357},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N14-'Operative BP'!$P$15))+BO14","v":174.83173339111073},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O14-'Operative BP'!$P$15))+BP14","v":-1228.2757055189531},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,2137.1317305137704,246.19203113518182,0,0,0,0,0,0,0,254.59312019607125,2668.0021945218805,2449.42891745922,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D15-'Operative BP'!$P$15))+AQ15","v":307.25173051377033},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E15-'Operative BP'!$P$15))+AR15","v":-994.00796886481749},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F15-'Operative BP'!$P$15))+AS15","v":-587.33999999999958},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G15-'Operative BP'!$P$15))+AT15","v":971.09999999999968},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H15-'Operative BP'!$P$15))+AU15","v":2087.2800000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I15-'Operative BP'!$P$15))+AV15","v":2824.38},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J15-'Operative BP'!$P$15))+AW15","v":3224.5200000000004},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K15-'Operative BP'!$P$15))+AX15","v":3350.88},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L15-'Operative BP'!$P$15))+AY15","v":2508.4799999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M15-'Operative BP'!$P$15))+AZ15","v":1541.5931201960711},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N15-'Operative BP'!$P$15))+BA15","v":2796.7021945218798},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O15-'Operative BP'!$P$15))+BB15","v":914.38891745922024},null,11,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D15-'Operative BP'!$P$15))+BE15","v":-1759.5},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E15-'Operative BP'!$P$15))+BF15","v":-1192.4999999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F15-'Operative BP'!$P$15))+BG15","v":-564.74999999999955},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G15-'Operative BP'!$P$15))+BH15","v":933.74999999999966},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H15-'Operative BP'!$P$15))+BI15","v":2007.0000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I15-'Operative BP'!$P$15))+BJ15","v":2715.75},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J15-'Operative BP'!$P$15))+BK15","v":3100.5000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K15-'Operative BP'!$P$15))+BL15","v":3222},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L15-'Operative BP'!$P$15))+BM15","v":2411.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M15-'Operative BP'!$P$15))+BN15","v":1237.5},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N15-'Operative BP'!$P$15))+BO15","v":123.74999999999936},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O15-'Operative BP'!$P$15))+BP15","v":-1475.9999999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,2660.7704140368955,129.99219692738231,0,0,0,0,0,0,0,199.34268060830314,3190.3469256777284,3062.0963422731697,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D16-'Operative BP'!$P$15))+AQ16","v":1125.7304140368958},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E16-'Operative BP'!$P$15))+AR16","v":-815.36780307261745},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F16-'Operative BP'!$P$15))+AS16","v":-397.80000000000064},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G16-'Operative BP'!$P$15))+AT16","v":1223.8200000000008},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H16-'Operative BP'!$P$15))+AU16","v":2318.9399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I16-'Operative BP'!$P$15))+AV16","v":3098.1600000000003},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J16-'Operative BP'!$P$15))+AW16","v":3435.12},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K16-'Operative BP'!$P$15))+AX16","v":3582.5399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L16-'Operative BP'!$P$15))+AY16","v":2719.0799999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M16-'Operative BP'!$P$15))+AZ16","v":1781.1826806083027},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N16-'Operative BP'!$P$15))+BA16","v":3613.8869256777289},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O16-'Operative BP'!$P$15))+BB16","v":1779.7763422731705},null,12,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D16-'Operative BP'!$P$15))+BE16","v":-1475.9999999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E16-'Operative BP'!$P$15))+BF16","v":-908.99999999999977},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F16-'Operative BP'!$P$15))+BG16","v":-382.50000000000063},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G16-'Operative BP'!$P$15))+BH16","v":1176.7500000000009},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H16-'Operative BP'!$P$15))+BI16","v":2229.7499999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I16-'Operative BP'!$P$15))+BJ16","v":2979.0000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J16-'Operative BP'!$P$15))+BK16","v":3303},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K16-'Operative BP'!$P$15))+BL16","v":3444.7499999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L16-'Operative BP'!$P$15))+BM16","v":2614.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M16-'Operative BP'!$P$15))+BN16","v":1520.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N16-'Operative BP'!$P$15))+BO16","v":407.25000000000051},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O16-'Operative BP'!$P$15))+BP16","v":-1232.9999999999993},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,2550.173141104859,164.68058328163184,0,0,0,0,0,0,0,315.54561787258626,2682.4119372208993,2806.1921484791264,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D17-'Operative BP'!$P$15))+AQ17","v":1246.7931411048589},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E17-'Operative BP'!$P$15))+AR17","v":-464.77941671836766},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F17-'Operative BP'!$P$15))+AS17","v":23.400000000000333},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G17-'Operative BP'!$P$15))+AT17","v":1371.2399999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H17-'Operative BP'!$P$15))+AU17","v":2550.5999999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I17-'Operative BP'!$P$15))+AV17","v":3245.5799999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J17-'Operative BP'!$P$15))+AW17","v":3603.5999999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K17-'Operative BP'!$P$15))+AX17","v":3814.1999999999994},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L17-'Operative BP'!$P$15))+AY17","v":2929.6799999999989},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M17-'Operative BP'!$P$15))+AZ17","v":2107.9856178725854},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N17-'Operative BP'!$P$15))+BA17","v":3358.6719372208995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O17-'Operative BP'!$P$15))+BB17","v":1776.5921484791268},null,13,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D17-'Operative BP'!$P$15))+BE17","v":-1253.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E17-'Operative BP'!$P$15))+BF17","v":-605.24999999999955},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F17-'Operative BP'!$P$15))+BG17","v":22.50000000000032},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G17-'Operative BP'!$P$15))+BH17","v":1318.4999999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H17-'Operative BP'!$P$15))+BI17","v":2452.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I17-'Operative BP'!$P$15))+BJ17","v":3120.7499999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J17-'Operative BP'!$P$15))+BK17","v":3464.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K17-'Operative BP'!$P$15))+BL17","v":3667.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L17-'Operative BP'!$P$15))+BM17","v":2816.9999999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M17-'Operative BP'!$P$15))+BN17","v":1723.4999999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N17-'Operative BP'!$P$15))+BO17","v":650.25000000000011},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O17-'Operative BP'!$P$15))+BP17","v":-989.99999999999966},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,2071.1194620481665,325.93097583385139,0,0,0,0,0,0,0,1146.217913516015,2804.1224848650663,2465.1244629009921,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D18-'Operative BP'!$P$15))+AQ18","v":957.27946204816703},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E18-'Operative BP'!$P$15))+AR18","v":-71.869024166149245},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F18-'Operative BP'!$P$15))+AS18","v":212.9399999999992},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G18-'Operative BP'!$P$15))+AT18","v":1539.7199999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H18-'Operative BP'!$P$15))+AU18","v":2719.0799999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I18-'Operative BP'!$P$15))+AV18","v":3498.3000000000006},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J18-'Operative BP'!$P$15))+AW18","v":3793.1399999999985},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K18-'Operative BP'!$P$15))+AX18","v":3919.5},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L18-'Operative BP'!$P$15))+AY18","v":3056.0399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M18-'Operative BP'!$P$15))+AZ18","v":2420.6134212164502},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N18-'Operative BP'!$P$15))+BA18","v":2846.050230577639},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O18-'Operative BP'!$P$15))+BB18","v":1398.3697211870335},null,14,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D18-'Operative BP'!$P$15))+BE18","v":-1070.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E18-'Operative BP'!$P$15))+BF18","v":-382.50000000000063},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F18-'Operative BP'!$P$15))+BG18","v":204.74999999999923},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G18-'Operative BP'!$P$15))+BH18","v":1480.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H18-'Operative BP'!$P$15))+BI18","v":2614.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I18-'Operative BP'!$P$15))+BJ18","v":3363.7500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J18-'Operative BP'!$P$15))+BK18","v":3647.2499999999986},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K18-'Operative BP'!$P$15))+BL18","v":3768.75},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L18-'Operative BP'!$P$15))+BM18","v":2938.4999999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M18-'Operative BP'!$P$15))+BN18","v":1885.5000000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N18-'Operative BP'!$P$15))+BO18","v":751.5000000000008},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O18-'Operative BP'!$P$15))+BP18","v":-827.99999999999989},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,3379.1186364961477,2627.2389509698896,2635.5703218185467,2739.6260864388364,2639.208561173924,1868.8769897456732,1817.2287126262747,2938.0781685139464,3923.7505691865708,4121.5430186681224,4073.1026437891323,3409.9124235922036,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D19-'Operative BP'!$P$15))+AQ19","v":401.88694154270047},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E19-'Operative BP'!$P$15))+AR19","v":93.02110364014078},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F19-'Operative BP'!$P$15))+AS19","v":339.30000000000064},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G19-'Operative BP'!$P$15))+AT19","v":1645.0200000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H19-'Operative BP'!$P$15))+AU19","v":2761.1999999999994},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I19-'Operative BP'!$P$15))+AV19","v":3582.5399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J19-'Operative BP'!$P$15))+AW19","v":3898.4399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K19-'Operative BP'!$P$15))+AX19","v":3961.62},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L19-'Operative BP'!$P$15))+AY19","v":3140.28},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M19-'Operative BP'!$P$15))+AZ19","v":2364.1506586082792},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N19-'Operative BP'!$P$15))+BA19","v":2222.4797769469983},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O19-'Operative BP'!$P$15))+BB19","v":713.42992200282424},null,15,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D19-'Operative BP'!$P$15))+BE19","v":-1010.2500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E19-'Operative BP'!$P$15))+BF19","v":-260.9999999999992},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F19-'Operative BP'!$P$15))+BG19","v":326.25000000000063},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G19-'Operative BP'!$P$15))+BH19","v":1581.7500000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H19-'Operative BP'!$P$15))+BI19","v":2654.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I19-'Operative BP'!$P$15))+BJ19","v":3444.7499999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J19-'Operative BP'!$P$15))+BK19","v":3748.4999999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K19-'Operative BP'!$P$15))+BL19","v":3809.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L19-'Operative BP'!$P$15))+BM19","v":3019.5000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M19-'Operative BP'!$P$15))+BN19","v":1986.7499999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N19-'Operative BP'!$P$15))+BO19","v":893.24999999999977},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O19-'Operative BP'!$P$15))+BP19","v":-747.00000000000011},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,3488.2891932933635,3744.9639414750504,4446.8095707895973,4774.3448944164402,4971.3533893484409,4803.02801605271,4929.1205423900001,5622.3905501017762,5190.4573655804825,4062.4502685123566,2971.6590396841225,2854.9097803651739,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D20-'Operative BP'!$P$15))+AQ20","v":-315.94024517494995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E20-'Operative BP'!$P$15))+AR20","v":-303.18335773772236},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F20-'Operative BP'!$P$15))+AS20","v":381.41999999999894},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G20-'Operative BP'!$P$15))+AT20","v":1560.7800000000004},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H20-'Operative BP'!$P$15))+AU20","v":2782.26},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I20-'Operative BP'!$P$15))+AV20","v":3603.5999999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J20-'Operative BP'!$P$15))+AW20","v":3877.38},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K20-'Operative BP'!$P$15))+AX20","v":3898.4399999999991},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L20-'Operative BP'!$P$15))+AY20","v":3119.22},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M20-'Operative BP'!$P$15))+AZ20","v":2003.0399999999988},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N20-'Operative BP'!$P$15))+BA20","v":1205.6398065973626},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O20-'Operative BP'!$P$15))+BB20","v":-170.5240539674038},null,16,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D20-'Operative BP'!$P$15))+BE20","v":-989.99999999999966},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E20-'Operative BP'!$P$15))+BF20","v":-301.5000000000008},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F20-'Operative BP'!$P$15))+BG20","v":366.74999999999898},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G20-'Operative BP'!$P$15))+BH20","v":1500.7500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H20-'Operative BP'!$P$15))+BI20","v":2675.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I20-'Operative BP'!$P$15))+BJ20","v":3464.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J20-'Operative BP'!$P$15))+BK20","v":3728.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K20-'Operative BP'!$P$15))+BL20","v":3748.4999999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L20-'Operative BP'!$P$15))+BM20","v":2999.2499999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M20-'Operative BP'!$P$15))+BN20","v":1925.9999999999989},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N20-'Operative BP'!$P$15))+BO20","v":792.00000000000068},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O20-'Operative BP'!$P$15))+BP20","v":-827.99999999999989},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,1591.2164963126143,2655.3121550436108,3490.2420072817777,3580.241138149192,3849.9681326621317,4187.313761054791,4292.2891157890799,4423.2439261434729,3470.8202131864714,1880.8404833431982,695.47656043259258,814.73237202802113,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D21-'Operative BP'!$P$15))+AQ21","v":-1155.9599999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E21-'Operative BP'!$P$15))+AR21","v":-482.04000000000053},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F21-'Operative BP'!$P$15))+AS21","v":255.0600000000008},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G21-'Operative BP'!$P$15))+AT21","v":1371.2399999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H21-'Operative BP'!$P$15))+AU21","v":2761.1999999999994},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I21-'Operative BP'!$P$15))+AV21","v":3519.3600000000015},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J21-'Operative BP'!$P$15))+AW21","v":3814.1999999999994},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K21-'Operative BP'!$P$15))+AX21","v":3751.0200000000004},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L21-'Operative BP'!$P$15))+AY21","v":2950.74},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M21-'Operative BP'!$P$15))+AZ21","v":1876.6799999999992},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N21-'Operative BP'!$P$15))+BA21","v":634.14000000000021},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O21-'Operative BP'!$P$15))+BB21","v":-1044.7864319617413},null,17,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D21-'Operative BP'!$P$15))+BE21","v":-1111.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E21-'Operative BP'!$P$15))+BF21","v":-463.50000000000051},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F21-'Operative BP'!$P$15))+BG21","v":245.25000000000077},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G21-'Operative BP'!$P$15))+BH21","v":1318.4999999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H21-'Operative BP'!$P$15))+BI21","v":2654.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I21-'Operative BP'!$P$15))+BJ21","v":3384.0000000000014},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J21-'Operative BP'!$P$15))+BK21","v":3667.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K21-'Operative BP'!$P$15))+BL21","v":3606.7500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L21-'Operative BP'!$P$15))+BM21","v":2837.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M21-'Operative BP'!$P$15))+BN21","v":1804.4999999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N21-'Operative BP'!$P$15))+BO21","v":609.75000000000023},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O21-'Operative BP'!$P$15))+BP21","v":-1050.7500000000005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,0,422.68319711735165,819.88818854556575,1026.1250812956971,1411.1756989981864,1877.6960626038615,1903.0570696083062,1540.0957842881564,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D22-'Operative BP'!$P$15))+AQ22","v":-1366.56},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E22-'Operative BP'!$P$15))+AR22","v":-692.64000000000021},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F22-'Operative BP'!$P$15))+AS22","v":107.6400000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G22-'Operative BP'!$P$15))+AT22","v":1202.7600000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H22-'Operative BP'!$P$15))+AU22","v":2613.7800000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I22-'Operative BP'!$P$15))+AV22","v":3414.0600000000009},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J22-'Operative BP'!$P$15))+AW22","v":3645.72},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K22-'Operative BP'!$P$15))+AX22","v":3561.4799999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L22-'Operative BP'!$P$15))+AY22","v":2824.38},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M22-'Operative BP'!$P$15))+AZ22","v":1708.1999999999994},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N22-'Operative BP'!$P$15))+BA22","v":339.30000000000064},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O22-'Operative BP'!$P$15))+BB22","v":-1240.1999999999994},null,18,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D22-'Operative BP'!$P$15))+BE22","v":-1314},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E22-'Operative BP'!$P$15))+BF22","v":-666.00000000000023},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F22-'Operative BP'!$P$15))+BG22","v":103.5000000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G22-'Operative BP'!$P$15))+BH22","v":1156.5000000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H22-'Operative BP'!$P$15))+BI22","v":2513.2500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I22-'Operative BP'!$P$15))+BJ22","v":3282.7500000000009},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J22-'Operative BP'!$P$15))+BK22","v":3505.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K22-'Operative BP'!$P$15))+BL22","v":3424.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L22-'Operative BP'!$P$15))+BM22","v":2715.75},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M22-'Operative BP'!$P$15))+BN22","v":1642.4999999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N22-'Operative BP'!$P$15))+BO22","v":326.25000000000063},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O22-'Operative BP'!$P$15))+BP22","v":-1192.4999999999993},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D23-'Operative BP'!$P$15))+AQ23","v":-1577.1600000000005},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E23-'Operative BP'!$P$15))+AR23","v":-903.2399999999999},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F23-'Operative BP'!$P$15))+AS23","v":-81.900000000000333},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G23-'Operative BP'!$P$15))+AT23","v":907.91999999999894},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H23-'Operative BP'!$P$15))+AU23","v":2424.2399999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I23-'Operative BP'!$P$15))+AV23","v":3182.4000000000005},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J23-'Operative BP'!$P$15))+AW23","v":3350.88},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K23-'Operative BP'!$P$15))+AX23","v":3287.6999999999994},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L23-'Operative BP'!$P$15))+AY23","v":2613.7800000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M23-'Operative BP'!$P$15))+AZ23","v":1476.5399999999988},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N23-'Operative BP'!$P$15))+BA23","v":107.6400000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O23-'Operative BP'!$P$15))+BB23","v":-1535.0399999999997},null,19,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D23-'Operative BP'!$P$15))+BE23","v":-1516.5000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E23-'Operative BP'!$P$15))+BF23","v":-868.49999999999989},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F23-'Operative BP'!$P$15))+BG23","v":-78.750000000000313},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G23-'Operative BP'!$P$15))+BH23","v":872.99999999999898},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H23-'Operative BP'!$P$15))+BI23","v":2331},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I23-'Operative BP'!$P$15))+BJ23","v":3060.0000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J23-'Operative BP'!$P$15))+BK23","v":3222},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K23-'Operative BP'!$P$15))+BL23","v":3161.2499999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L23-'Operative BP'!$P$15))+BM23","v":2513.2500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M23-'Operative BP'!$P$15))+BN23","v":1419.7499999999989},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N23-'Operative BP'!$P$15))+BO23","v":103.5000000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O23-'Operative BP'!$P$15))+BP23","v":-1475.9999999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D24-'Operative BP'!$P$15))+AQ24","v":-1808.8199999999993},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E24-'Operative BP'!$P$15))+AR24","v":-1177.0200000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F24-'Operative BP'!$P$15))+AS24","v":-376.7399999999999},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G24-'Operative BP'!$P$15))+AT24","v":718.38000000000011},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H24-'Operative BP'!$P$15))+AU24","v":2150.4600000000009},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I24-'Operative BP'!$P$15))+AV24","v":2887.5600000000009},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J24-'Operative BP'!$P$15))+AW24","v":2929.6799999999989},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K24-'Operative BP'!$P$15))+AX24","v":2950.74},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L24-'Operative BP'!$P$15))+AY24","v":2340},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M24-'Operative BP'!$P$15))+AZ24","v":1118.5200000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N24-'Operative BP'!$P$15))+BA24","v":-187.19999999999933},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O24-'Operative BP'!$P$15))+BB24","v":-1745.64},null,20,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D24-'Operative BP'!$P$15))+BE24","v":-1739.2499999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E24-'Operative BP'!$P$15))+BF24","v":-1131.7500000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F24-'Operative BP'!$P$15))+BG24","v":-362.24999999999989},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G24-'Operative BP'!$P$15))+BH24","v":690.75000000000011},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H24-'Operative BP'!$P$15))+BI24","v":2067.7500000000009},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I24-'Operative BP'!$P$15))+BJ24","v":2776.5000000000009},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J24-'Operative BP'!$P$15))+BK24","v":2816.9999999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K24-'Operative BP'!$P$15))+BL24","v":2837.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L24-'Operative BP'!$P$15))+BM24","v":2250},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M24-'Operative BP'!$P$15))+BN24","v":1075.5000000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N24-'Operative BP'!$P$15))+BO24","v":-179.99999999999937},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O24-'Operative BP'!$P$15))+BP24","v":-1678.5000000000002},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D25-'Operative BP'!$P$15))+AQ25","v":-1956.2399999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E25-'Operative BP'!$P$15))+AR25","v":-1387.62},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F25-'Operative BP'!$P$15))+AS25","v":-545.21999999999957},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G25-'Operative BP'!$P$15))+AT25","v":528.83999999999958},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H25-'Operative BP'!$P$15))+AU25","v":1918.8000000000006},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I25-'Operative BP'!$P$15))+AV25","v":2571.6600000000003},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J25-'Operative BP'!$P$15))+AW25","v":2592.7199999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K25-'Operative BP'!$P$15))+AX25","v":2719.0799999999995},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L25-'Operative BP'!$P$15))+AY25","v":2045.1600000000005},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M25-'Operative BP'!$P$15))+AZ25","v":886.85999999999979},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N25-'Operative BP'!$P$15))+BA25","v":-376.7399999999999},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O25-'Operative BP'!$P$15))+BB25","v":-1893.06},null,21,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D25-'Operative BP'!$P$15))+BE25","v":-1880.9999999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E25-'Operative BP'!$P$15))+BF25","v":-1334.25},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F25-'Operative BP'!$P$15))+BG25","v":-524.24999999999966},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G25-'Operative BP'!$P$15))+BH25","v":508.49999999999955},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H25-'Operative BP'!$P$15))+BI25","v":1845.0000000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I25-'Operative BP'!$P$15))+BJ25","v":2472.7500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J25-'Operative BP'!$P$15))+BK25","v":2492.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K25-'Operative BP'!$P$15))+BL25","v":2614.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L25-'Operative BP'!$P$15))+BM25","v":1966.5000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M25-'Operative BP'!$P$15))+BN25","v":852.74999999999977},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N25-'Operative BP'!$P$15))+BO25","v":-362.24999999999989},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O25-'Operative BP'!$P$15))+BP25","v":-1820.25},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D26-'Operative BP'!$P$15))+AQ26","v":-2124.7199999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E26-'Operative BP'!$P$15))+AR26","v":-1598.2199999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F26-'Operative BP'!$P$15))+AS26","v":-734.7600000000001},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G26-'Operative BP'!$P$15))+AT26","v":339.30000000000064},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H26-'Operative BP'!$P$15))+AU26","v":1708.1999999999994},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I26-'Operative BP'!$P$15))+AV26","v":2297.88},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J26-'Operative BP'!$P$15))+AW26","v":2276.8200000000011},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K26-'Operative BP'!$P$15))+AX26","v":2487.4200000000005},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L26-'Operative BP'!$P$15))+AY26","v":1834.5600000000009},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M26-'Operative BP'!$P$15))+AZ26","v":655.19999999999936},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N26-'Operative BP'!$P$15))+BA26","v":-608.40000000000032},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O26-'Operative BP'!$P$15))+BB26","v":-2040.4799999999998},null,22,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D26-'Operative BP'!$P$15))+BE26","v":-2042.9999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E26-'Operative BP'!$P$15))+BF26","v":-1536.7499999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F26-'Operative BP'!$P$15))+BG26","v":-706.50000000000011},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G26-'Operative BP'!$P$15))+BH26","v":326.25000000000063},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H26-'Operative BP'!$P$15))+BI26","v":1642.4999999999993},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I26-'Operative BP'!$P$15))+BJ26","v":2209.5},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J26-'Operative BP'!$P$15))+BK26","v":2189.2500000000009},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K26-'Operative BP'!$P$15))+BL26","v":2391.7500000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L26-'Operative BP'!$P$15))+BM26","v":1764.0000000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M26-'Operative BP'!$P$15))+BN26","v":629.99999999999932},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N26-'Operative BP'!$P$15))+BO26","v":-585.00000000000034},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O26-'Operative BP'!$P$15))+BP26","v":-1961.9999999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D27-'Operative BP'!$P$15))+AQ27","v":-2272.1400000000003},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E27-'Operative BP'!$P$15))+AR27","v":-1766.7000000000003},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F27-'Operative BP'!$P$15))+AS27","v":-903.2399999999999},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G27-'Operative BP'!$P$15))+AT27","v":86.580000000001064},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H27-'Operative BP'!$P$15))+AU27","v":1497.5999999999997},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I27-'Operative BP'!$P$15))+AV27","v":2087.2800000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J27-'Operative BP'!$P$15))+AW27","v":2108.3399999999997},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K27-'Operative BP'!$P$15))+AX27","v":2297.88},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L27-'Operative BP'!$P$15))+AY27","v":1623.9600000000012},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M27-'Operative BP'!$P$15))+AZ27","v":465.66000000000048},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N27-'Operative BP'!$P$15))+BA27","v":-840.06000000000085},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O27-'Operative BP'!$P$15))+BB27","v":-2145.7800000000002},null,23,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D27-'Operative BP'!$P$15))+BE27","v":-2184.75},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E27-'Operative BP'!$P$15))+BF27","v":-1698.7500000000002},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F27-'Operative BP'!$P$15))+BG27","v":-868.49999999999989},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G27-'Operative BP'!$P$15))+BH27","v":83.250000000001023},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H27-'Operative BP'!$P$15))+BI27","v":1439.9999999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I27-'Operative BP'!$P$15))+BJ27","v":2007.0000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J27-'Operative BP'!$P$15))+BK27","v":2027.2499999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K27-'Operative BP'!$P$15))+BL27","v":2209.5},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L27-'Operative BP'!$P$15))+BM27","v":1561.5000000000011},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M27-'Operative BP'!$P$15))+BN27","v":447.75000000000045},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N27-'Operative BP'!$P$15))+BO27","v":-807.7500000000008},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O27-'Operative BP'!$P$15))+BP27","v":-2063.2500000000005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,0,0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,{"$f":"('Input Data'!$F$54*('Dry Bulb'!D28-'Operative BP'!$P$15))+AQ28","v":-2377.44},{"$f":"('Input Data'!$F$54*('Dry Bulb'!E28-'Operative BP'!$P$15))+AR28","v":-1956.2399999999998},{"$f":"('Input Data'!$F$54*('Dry Bulb'!F28-'Operative BP'!$P$15))+AS28","v":-1071.7199999999996},{"$f":"('Input Data'!$F$54*('Dry Bulb'!G28-'Operative BP'!$P$15))+AT28","v":-81.900000000000333},{"$f":"('Input Data'!$F$54*('Dry Bulb'!H28-'Operative BP'!$P$15))+AU28","v":1308.0600000000009},{"$f":"('Input Data'!$F$54*('Dry Bulb'!I28-'Operative BP'!$P$15))+AV28","v":1876.6799999999992},{"$f":"('Input Data'!$F$54*('Dry Bulb'!J28-'Operative BP'!$P$15))+AW28","v":1960.9200000000005},{"$f":"('Input Data'!$F$54*('Dry Bulb'!K28-'Operative BP'!$P$15))+AX28","v":2087.2800000000002},{"$f":"('Input Data'!$F$54*('Dry Bulb'!L28-'Operative BP'!$P$15))+AY28","v":1434.4200000000005},{"$f":"('Input Data'!$F$54*('Dry Bulb'!M28-'Operative BP'!$P$15))+AZ28","v":297.18000000000075},{"$f":"('Input Data'!$F$54*('Dry Bulb'!N28-'Operative BP'!$P$15))+BA28","v":-987.47999999999979},{"$f":"('Input Data'!$F$54*('Dry Bulb'!O28-'Operative BP'!$P$15))+BB28","v":-2335.3200000000002},null,24,{"$f":"('Input Data'!$F$55*('Dry Bulb'!D28-'Operative BP'!$P$15))+BE28","v":-2286},{"$f":"('Input Data'!$F$55*('Dry Bulb'!E28-'Operative BP'!$P$15))+BF28","v":-1880.9999999999998},{"$f":"('Input Data'!$F$55*('Dry Bulb'!F28-'Operative BP'!$P$15))+BG28","v":-1030.4999999999995},{"$f":"('Input Data'!$F$55*('Dry Bulb'!G28-'Operative BP'!$P$15))+BH28","v":-78.750000000000313},{"$f":"('Input Data'!$F$55*('Dry Bulb'!H28-'Operative BP'!$P$15))+BI28","v":1257.7500000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!I28-'Operative BP'!$P$15))+BJ28","v":1804.4999999999991},{"$f":"('Input Data'!$F$55*('Dry Bulb'!J28-'Operative BP'!$P$15))+BK28","v":1885.5000000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!K28-'Operative BP'!$P$15))+BL28","v":2007.0000000000005},{"$f":"('Input Data'!$F$55*('Dry Bulb'!L28-'Operative BP'!$P$15))+BM28","v":1379.2500000000007},{"$f":"('Input Data'!$F$55*('Dry Bulb'!M28-'Operative BP'!$P$15))+BN28","v":285.75000000000068},{"$f":"('Input Data'!$F$55*('Dry Bulb'!N28-'Operative BP'!$P$15))+BO28","v":-949.49999999999977},{"$f":"('Input Data'!$F$55*('Dry Bulb'!O28-'Operative BP'!$P$15))+BP28","v":-2245.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"UAdeltaT+Solar",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UAdeltaT+Solar - West",null,null,null,null,null,null,null,null,null,null,null,null,null,"UAdeltaT+Solar - North",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec","Average","HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec","Average",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,1,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D5-'Operative BP'!$P$15))+C58","v":-10924.515000000003},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E5-'Operative BP'!$P$15))+D58","v":-8702.0775000000031},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F5-'Operative BP'!$P$15))+E58","v":-5323.9725000000008},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G5-'Operative BP'!$P$15))+F58","v":-967.99499999999694},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H5-'Operative BP'!$P$15))+G58","v":4721.4450000000015},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I5-'Operative BP'!$P$15))+H58","v":7210.5749999999971},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J5-'Operative BP'!$P$15))+I58","v":7832.8575000000001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K5-'Operative BP'!$P$15))+J58","v":8099.5500000000029},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L5-'Operative BP'!$P$15))+K58","v":5343.7274999999963},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M5-'Operative BP'!$P$15))+L58","v":543.2624999999972},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N5-'Operative BP'!$P$15))+M58","v":-4879.4849999999979},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O5-'Operative BP'!$P$15))+N58","v":-9946.6424999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D5-'Operative BP'!$P$15))+AQ32","v":-2886.6600000000008},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E5-'Operative BP'!$P$15))+AR32","v":-2299.4100000000008},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F5-'Operative BP'!$P$15))+AS32","v":-1406.7900000000002},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G5-'Operative BP'!$P$15))+AT32","v":-255.77999999999918},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H5-'Operative BP'!$P$15))+AU32","v":1247.5800000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I5-'Operative BP'!$P$15))+AV32","v":1905.2999999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J5-'Operative BP'!$P$15))+AW32","v":2069.73},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K5-'Operative BP'!$P$15))+AX32","v":2140.2000000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L5-'Operative BP'!$P$15))+AY32","v":1412.0099999999991},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M5-'Operative BP'!$P$15))+AZ32","v":143.54999999999927},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N5-'Operative BP'!$P$15))+BA32","v":-1289.3399999999995},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O5-'Operative BP'!$P$15))+BB32","v":-2628.27},{"$f":"AVERAGEIF(AS85:AZ108,\">0\")","v":2780.5144498239301},1,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D5-'Operative BP'!$P$15))+BE32","v":-2961.3150000000005},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E5-'Operative BP'!$P$15))+BF32","v":-2358.8775000000005},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F5-'Operative BP'!$P$15))+BG32","v":-1443.1725000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G5-'Operative BP'!$P$15))+BH32","v":-262.39499999999919},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H5-'Operative BP'!$P$15))+BI32","v":1279.8450000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I5-'Operative BP'!$P$15))+BJ32","v":1954.5749999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J5-'Operative BP'!$P$15))+BK32","v":2123.2574999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K5-'Operative BP'!$P$15))+BL32","v":2195.5500000000006},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L5-'Operative BP'!$P$15))+BM32","v":1448.527499999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M5-'Operative BP'!$P$15))+BN32","v":147.26249999999925},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N5-'Operative BP'!$P$15))+BO32","v":-1322.6849999999995},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O5-'Operative BP'!$P$15))+BP32","v":-2696.2425000000003},{"$f":"AVERAGEIF(BG85:BN108,\">0\")","v":2209.6447641509435},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,2,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D6-'Operative BP'!$P$15))+C59","v":-11369.002500000002},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E6-'Operative BP'!$P$15))+D59","v":-9235.4625000000015},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F6-'Operative BP'!$P$15))+E59","v":-5946.2550000000028},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G6-'Operative BP'!$P$15))+F59","v":-1501.3800000000031},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H6-'Operative BP'!$P$15))+G59","v":4010.2650000000021},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I6-'Operative BP'!$P$15))+H59","v":6321.5999999999985},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J6-'Operative BP'!$P$15))+I59","v":7032.7799999999979},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K6-'Operative BP'!$P$15))+J59","v":7299.4725000000008},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L6-'Operative BP'!$P$15))+K59","v":4454.7524999999978},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M6-'Operative BP'!$P$15))+L59","v":-79.019999999998319},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N6-'Operative BP'!$P$15))+M59","v":-5679.5625},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O6-'Operative BP'!$P$15))+N59","v":-10302.2325},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D6-'Operative BP'!$P$15))+AQ33","v":-3004.1100000000006},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E6-'Operative BP'!$P$15))+AR33","v":-2440.3500000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F6-'Operative BP'!$P$15))+AS33","v":-1571.2200000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G6-'Operative BP'!$P$15))+AT33","v":-396.72000000000082},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H6-'Operative BP'!$P$15))+AU33","v":1059.6600000000005},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I6-'Operative BP'!$P$15))+AV33","v":1670.3999999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J6-'Operative BP'!$P$15))+AW33","v":1858.3199999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K6-'Operative BP'!$P$15))+AX33","v":1928.7900000000002},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L6-'Operative BP'!$P$15))+AY33","v":1177.1099999999994},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M6-'Operative BP'!$P$15))+AZ33","v":-20.879999999999555},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N6-'Operative BP'!$P$15))+BA33","v":-1500.75},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O6-'Operative BP'!$P$15))+BB33","v":-2722.23},"Max",2,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D6-'Operative BP'!$P$15))+BE33","v":-3081.8025000000002},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E6-'Operative BP'!$P$15))+BF33","v":-2503.4625000000005},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F6-'Operative BP'!$P$15))+BG33","v":-1611.8550000000009},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G6-'Operative BP'!$P$15))+BH33","v":-406.98000000000081},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H6-'Operative BP'!$P$15))+BI33","v":1087.0650000000005},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I6-'Operative BP'!$P$15))+BJ33","v":1713.5999999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J6-'Operative BP'!$P$15))+BK33","v":1906.3799999999994},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K6-'Operative BP'!$P$15))+BL33","v":1978.6725000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L6-'Operative BP'!$P$15))+BM33","v":1207.5524999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M6-'Operative BP'!$P$15))+BN33","v":-21.419999999999543},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N6-'Operative BP'!$P$15))+BO33","v":-1539.5625},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O6-'Operative BP'!$P$15))+BP33","v":-2792.6324999999997},"Max",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D7-'Operative BP'!$P$15))+C60","v":-11635.695000000002},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E7-'Operative BP'!$P$15))+D60","v":-9768.8474999999999},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F7-'Operative BP'!$P$15))+E60","v":-6568.5374999999985},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G7-'Operative BP'!$P$15))+F60","v":-2034.7650000000021},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H7-'Operative BP'!$P$15))+G60","v":3476.8800000000033},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I7-'Operative BP'!$P$15))+H60","v":5877.1125000000029},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J7-'Operative BP'!$P$15))+I60","v":6499.3949999999986},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K7-'Operative BP'!$P$15))+J60","v":6499.3949999999986},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L7-'Operative BP'!$P$15))+K60","v":3654.6750000000029},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M7-'Operative BP'!$P$15))+L60","v":-879.09750000000054},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N7-'Operative BP'!$P$15))+M60","v":-6301.8449999999993},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O7-'Operative BP'!$P$15))+N60","v":-10657.822499999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D7-'Operative BP'!$P$15))+AQ34","v":-3074.5800000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E7-'Operative BP'!$P$15))+AR34","v":-2581.29},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F7-'Operative BP'!$P$15))+AS34","v":-1735.6499999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G7-'Operative BP'!$P$15))+AT34","v":-537.66000000000054},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H7-'Operative BP'!$P$15))+AU34","v":918.72000000000082},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I7-'Operative BP'!$P$15))+AV34","v":1552.9500000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J7-'Operative BP'!$P$15))+AW34","v":1717.3799999999997},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K7-'Operative BP'!$P$15))+AX34","v":1717.3799999999997},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L7-'Operative BP'!$P$15))+AY34","v":965.70000000000073},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M7-'Operative BP'!$P$15))+AZ34","v":-232.29000000000013},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N7-'Operative BP'!$P$15))+BA34","v":-1665.1799999999998},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O7-'Operative BP'!$P$15))+BB34","v":-2816.1899999999996},{"$f":"MAX(AT85:AY108)","v":9970.6505501017746},3,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D7-'Operative BP'!$P$15))+BE34","v":-3154.0950000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E7-'Operative BP'!$P$15))+BF34","v":-2648.0475000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F7-'Operative BP'!$P$15))+BG34","v":-1780.5374999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G7-'Operative BP'!$P$15))+BH34","v":-551.56500000000062},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H7-'Operative BP'!$P$15))+BI34","v":942.48000000000081},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I7-'Operative BP'!$P$15))+BJ34","v":1593.1125000000009},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J7-'Operative BP'!$P$15))+BK34","v":1761.7949999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K7-'Operative BP'!$P$15))+BL34","v":1761.7949999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L7-'Operative BP'!$P$15))+BM34","v":990.67500000000075},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M7-'Operative BP'!$P$15))+BN34","v":-238.29750000000016},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N7-'Operative BP'!$P$15))+BO34","v":-1708.2449999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O7-'Operative BP'!$P$15))+BP34","v":-2889.0224999999996},{"$f":"MAX(BH85:BM108)","v":4533.0074999999997},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D8-'Operative BP'!$P$15))+C61","v":-12080.182500000001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E8-'Operative BP'!$P$15))+D61","v":-10302.2325},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F8-'Operative BP'!$P$15))+E61","v":-7013.0250000000015},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G8-'Operative BP'!$P$15))+F61","v":-2745.9450000000011},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H8-'Operative BP'!$P$15))+G61","v":3210.1875},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I8-'Operative BP'!$P$15))+H61","v":5343.7274999999963},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J8-'Operative BP'!$P$15))+I61","v":5788.2149999999992},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K8-'Operative BP'!$P$15))+J61","v":5877.1125000000029},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L8-'Operative BP'!$P$15))+K61","v":2943.4949999999967},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M8-'Operative BP'!$P$15))+L61","v":-1234.6875},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N8-'Operative BP'!$P$15))+M61","v":-6924.1274999999978},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O8-'Operative BP'!$P$15))+N61","v":-11102.309999999998},null,{"$f":"AVERAGEIF(E85:L108,\">0\")","v":9088.0877014615417},"Average",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D8-'Operative BP'!$P$15))+AQ35","v":-3192.03},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E8-'Operative BP'!$P$15))+AR35","v":-2722.23},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F8-'Operative BP'!$P$15))+AS35","v":-1853.1000000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G8-'Operative BP'!$P$15))+AT35","v":-725.58000000000027},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H8-'Operative BP'!$P$15))+AU35","v":848.25},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I8-'Operative BP'!$P$15))+AV35","v":1412.0099999999991},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J8-'Operative BP'!$P$15))+AW35","v":1529.4599999999998},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K8-'Operative BP'!$P$15))+AX35","v":1552.9500000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L8-'Operative BP'!$P$15))+AY35","v":777.77999999999918},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M8-'Operative BP'!$P$15))+AZ35","v":-326.25},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N8-'Operative BP'!$P$15))+BA35","v":-1829.6099999999994},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O8-'Operative BP'!$P$15))+BB35","v":-2933.6399999999994},"Av+Max/2",4,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D8-'Operative BP'!$P$15))+BE35","v":-3274.5825},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E8-'Operative BP'!$P$15))+BF35","v":-2792.6324999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F8-'Operative BP'!$P$15))+BG35","v":-1901.0250000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G8-'Operative BP'!$P$15))+BH35","v":-744.34500000000025},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H8-'Operative BP'!$P$15))+BI35","v":870.1875},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I8-'Operative BP'!$P$15))+BJ35","v":1448.527499999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J8-'Operative BP'!$P$15))+BK35","v":1569.0149999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K8-'Operative BP'!$P$15))+BL35","v":1593.1125000000009},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L8-'Operative BP'!$P$15))+BM35","v":797.89499999999919},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M8-'Operative BP'!$P$15))+BN35","v":-334.6875},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N8-'Operative BP'!$P$15))+BO35","v":-1876.9274999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O8-'Operative BP'!$P$15))+BP35","v":-3009.5099999999998},"Av+Max/2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D9-'Operative BP'!$P$15))+C62","v":-12613.567499999999},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E9-'Operative BP'!$P$15))+D62","v":-10657.822499999998},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F9-'Operative BP'!$P$15))+E62","v":-7457.5125000000007},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G9-'Operative BP'!$P$15))+F62","v":-3279.3300000000004},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H9-'Operative BP'!$P$15))+G62","v":2499.0075000000011},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I9-'Operative BP'!$P$15))+H62","v":4721.4450000000015},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J9-'Operative BP'!$P$15))+I62","v":5432.625},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K9-'Operative BP'!$P$15))+J62","v":5343.7274999999963},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L9-'Operative BP'!$P$15))+K62","v":2587.9050000000043},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M9-'Operative BP'!$P$15))+L62","v":-1945.8674999999989},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N9-'Operative BP'!$P$15))+M62","v":-7635.3074999999972},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O9-'Operative BP'!$P$15))+N62","v":-11546.797499999997},null,{"$f":"MAX(E85:L108)","v":22078.305550101773},"Max",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D9-'Operative BP'!$P$15))+AQ36","v":-3332.97},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E9-'Operative BP'!$P$15))+AR36","v":-2816.1899999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F9-'Operative BP'!$P$15))+AS36","v":-1970.5500000000002},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G9-'Operative BP'!$P$15))+AT36","v":-866.5200000000001},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H9-'Operative BP'!$P$15))+AU36","v":660.33000000000027},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I9-'Operative BP'!$P$15))+AV36","v":1247.5800000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J9-'Operative BP'!$P$15))+AW36","v":1435.5},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K9-'Operative BP'!$P$15))+AX36","v":1412.0099999999991},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L9-'Operative BP'!$P$15))+AY36","v":683.82000000000119},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M9-'Operative BP'!$P$15))+AZ36","v":-514.16999999999973},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N9-'Operative BP'!$P$15))+BA36","v":-2017.5299999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O9-'Operative BP'!$P$15))+BB36","v":-3051.0899999999992},{"$f":"AVERAGE(BC85,BC87)","v":6375.5824999628521},5,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D9-'Operative BP'!$P$15))+BE36","v":-3419.1675},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E9-'Operative BP'!$P$15))+BF36","v":-2889.0224999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F9-'Operative BP'!$P$15))+BG36","v":-2021.5125000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G9-'Operative BP'!$P$15))+BH36","v":-888.93000000000006},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H9-'Operative BP'!$P$15))+BI36","v":677.40750000000025},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I9-'Operative BP'!$P$15))+BJ36","v":1279.8450000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J9-'Operative BP'!$P$15))+BK36","v":1472.625},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K9-'Operative BP'!$P$15))+BL36","v":1448.527499999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L9-'Operative BP'!$P$15))+BM36","v":701.50500000000125},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M9-'Operative BP'!$P$15))+BN36","v":-527.46749999999975},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N9-'Operative BP'!$P$15))+BO36","v":-2069.7074999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O9-'Operative BP'!$P$15))+BP36","v":-3129.9974999999995},{"$f":"AVERAGE(BQ85,BQ87)","v":3371.3261320754718},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D10-'Operative BP'!$P$15))+C63","v":-12880.259999999998},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E10-'Operative BP'!$P$15))+D63","v":-11013.412499999999},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F10-'Operative BP'!$P$15))+E63","v":-7724.2049999999999},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G10-'Operative BP'!$P$15))+F63","v":-3549.6287453219006},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H10-'Operative BP'!$P$15))+G63","v":2076.7656761292242},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I10-'Operative BP'!$P$15))+H63","v":4426.751484032251},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J10-'Operative BP'!$P$15))+I63","v":5228.5949615963355},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K10-'Operative BP'!$P$15))+J63","v":4984.7245809000397},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L10-'Operative BP'!$P$15))+K63","v":2370.2886562405224},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M10-'Operative BP'!$P$15))+L63","v":-2390.3550000000018},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N10-'Operative BP'!$P$15))+M63","v":-7813.1025},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O10-'Operative BP'!$P$15))+N63","v":-11546.797499999997},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D10-'Operative BP'!$P$15))+AQ37","v":-3403.4399999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E10-'Operative BP'!$P$15))+AR37","v":-2910.1499999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F10-'Operative BP'!$P$15))+AS37","v":-2041.02},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G10-'Operative BP'!$P$15))+AT37","v":-960.4799999999999},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H10-'Operative BP'!$P$15))+AU37","v":495.89999999999964},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I10-'Operative BP'!$P$15))+AV37","v":1106.6400000000006},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J10-'Operative BP'!$P$15))+AW37","v":1341.5400000000002},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K10-'Operative BP'!$P$15))+AX37","v":1294.5599999999984},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L10-'Operative BP'!$P$15))+AY37","v":613.35000000000036},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M10-'Operative BP'!$P$15))+AZ37","v":-631.62000000000046},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N10-'Operative BP'!$P$15))+BA37","v":-2064.5100000000002},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O10-'Operative BP'!$P$15))+BB37","v":-3051.0899999999992},null,6,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D10-'Operative BP'!$P$15))+BE37","v":-3491.4599999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E10-'Operative BP'!$P$15))+BF37","v":-2985.4124999999995},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F10-'Operative BP'!$P$15))+BG37","v":-2093.8050000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G10-'Operative BP'!$P$15))+BH37","v":-985.31999999999994},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H10-'Operative BP'!$P$15))+BI37","v":508.72499999999962},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I10-'Operative BP'!$P$15))+BJ37","v":1135.2600000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J10-'Operative BP'!$P$15))+BK37","v":1376.2350000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K10-'Operative BP'!$P$15))+BL37","v":1328.0399999999984},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L10-'Operative BP'!$P$15))+BM37","v":629.21250000000043},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M10-'Operative BP'!$P$15))+BN37","v":-647.9550000000005},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N10-'Operative BP'!$P$15))+BO37","v":-2117.9025000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O10-'Operative BP'!$P$15))+BP37","v":-3129.9974999999995},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D11-'Operative BP'!$P$15))+C64","v":-12815.361486746026},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E11-'Operative BP'!$P$15))+D64","v":-10848.005729691004},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F11-'Operative BP'!$P$15))+E64","v":-7247.0014682757001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G11-'Operative BP'!$P$15))+F64","v":-1315.7377232223146},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H11-'Operative BP'!$P$15))+G64","v":4678.1288692542448},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I11-'Operative BP'!$P$15))+H64","v":7578.236775782003},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J11-'Operative BP'!$P$15))+I64","v":8043.5269584747057},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K11-'Operative BP'!$P$15))+J64","v":7606.5359965171874},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L11-'Operative BP'!$P$15))+K64","v":4531.2914066489984},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M11-'Operative BP'!$P$15))+L64","v":-1159.1505573679965},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N11-'Operative BP'!$P$15))+M64","v":-7755.9485483357612},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O11-'Operative BP'!$P$15))+N64","v":-11626.70276993958},null,{"$f":"AVERAGE(P88:P89)","v":15583.196625781657},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D11-'Operative BP'!$P$15))+AQ38","v":-3403.4399999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E11-'Operative BP'!$P$15))+AR38","v":-2910.1499999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F11-'Operative BP'!$P$15))+AS38","v":-2041.02},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G11-'Operative BP'!$P$15))+AT38","v":-725.58000000000027},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H11-'Operative BP'!$P$15))+AU38","v":754.29000000000019},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I11-'Operative BP'!$P$15))+AV38","v":1482.48},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J11-'Operative BP'!$P$15))+AW38","v":1693.8900000000006},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K11-'Operative BP'!$P$15))+AX38","v":1623.4199999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L11-'Operative BP'!$P$15))+AY38","v":871.74000000000092},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M11-'Operative BP'!$P$15))+AZ38","v":-514.16999999999973},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N11-'Operative BP'!$P$15))+BA38","v":-2111.4899999999998},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O11-'Operative BP'!$P$15))+BB38","v":-3098.07},null,7,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D11-'Operative BP'!$P$15))+BE38","v":-3491.4599999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E11-'Operative BP'!$P$15))+BF38","v":-2985.4124999999995},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F11-'Operative BP'!$P$15))+BG38","v":-2093.8050000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G11-'Operative BP'!$P$15))+BH38","v":-744.34500000000025},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H11-'Operative BP'!$P$15))+BI38","v":773.79750000000013},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I11-'Operative BP'!$P$15))+BJ38","v":1520.82},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J11-'Operative BP'!$P$15))+BK38","v":1737.6975000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K11-'Operative BP'!$P$15))+BL38","v":1665.4049999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L11-'Operative BP'!$P$15))+BM38","v":894.28500000000088},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M11-'Operative BP'!$P$15))+BN38","v":-527.46749999999975},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N11-'Operative BP'!$P$15))+BO38","v":-2166.0974999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O11-'Operative BP'!$P$15))+BP38","v":-3178.1925000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D12-'Operative BP'!$P$15))+C65","v":-10482.999510577698},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E12-'Operative BP'!$P$15))+D65","v":-8277.4770143781079},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F12-'Operative BP'!$P$15))+E65","v":-3938.6912979195322},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G12-'Operative BP'!$P$15))+F65","v":2304.2732210657441},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H12-'Operative BP'!$P$15))+G65","v":8062.6366695915385},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I12-'Operative BP'!$P$15))+H65","v":11012.795392125139},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J12-'Operative BP'!$P$15))+I65","v":11694.497904084104},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K12-'Operative BP'!$P$15))+J65","v":11801.019396775055},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L12-'Operative BP'!$P$15))+K65","v":8767.4468592338835},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M12-'Operative BP'!$P$15))+L65","v":2598.8620220993384},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N12-'Operative BP'!$P$15))+M65","v":-3664.6846166711853},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O12-'Operative BP'!$P$15))+N65","v":-9616.1911262806552},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D12-'Operative BP'!$P$15))+AQ39","v":-3098.07},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E12-'Operative BP'!$P$15))+AR39","v":-2604.7800000000002},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F12-'Operative BP'!$P$15))+AS39","v":-1641.6899999999998},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G12-'Operative BP'!$P$15))+AT39","v":-302.75999999999908},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H12-'Operative BP'!$P$15))+AU39","v":1224.0900000000013},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I12-'Operative BP'!$P$15))+AV39","v":1952.2800000000011},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J12-'Operative BP'!$P$15))+AW39","v":2163.6900000000014},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K12-'Operative BP'!$P$15))+AX39","v":2140.2000000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L12-'Operative BP'!$P$15))+AY39","v":1458.9900000000009},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M12-'Operative BP'!$P$15))+AZ39","v":2.6099999999994807},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N12-'Operative BP'!$P$15))+BA39","v":-1477.26},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O12-'Operative BP'!$P$15))+BB39","v":-2886.6600000000008},null,8,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D12-'Operative BP'!$P$15))+BE39","v":-3178.1925000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E12-'Operative BP'!$P$15))+BF39","v":-2672.145},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F12-'Operative BP'!$P$15))+BG39","v":-1684.1474999999998},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G12-'Operative BP'!$P$15))+BH39","v":-310.58999999999907},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H12-'Operative BP'!$P$15))+BI39","v":1255.7475000000013},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I12-'Operative BP'!$P$15))+BJ39","v":2002.7700000000011},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J12-'Operative BP'!$P$15))+BK39","v":2219.6475000000019},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K12-'Operative BP'!$P$15))+BL39","v":2195.5500000000006},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L12-'Operative BP'!$P$15))+BM39","v":1496.722500000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M12-'Operative BP'!$P$15))+BN39","v":2.6774999999994673},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N12-'Operative BP'!$P$15))+BO39","v":-1515.4650000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O12-'Operative BP'!$P$15))+BP39","v":-2961.3150000000005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D13-'Operative BP'!$P$15))+C66","v":-7641.9024991787646},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E13-'Operative BP'!$P$15))+D66","v":-5897.5798611768996},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F13-'Operative BP'!$P$15))+E66","v":-2234.1626740370007},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G13-'Operative BP'!$P$15))+F66","v":4348.1658657250155},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H13-'Operative BP'!$P$15))+G66","v":9255.3978267677103},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I13-'Operative BP'!$P$15))+H66","v":12480.653308211919},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J13-'Operative BP'!$P$15))+I66","v":14042.911488377242},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K13-'Operative BP'!$P$15))+J66","v":14236.971360076477},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L13-'Operative BP'!$P$15))+K66","v":10920.377859200657},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M13-'Operative BP'!$P$15))+L66","v":5042.5793283731746},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N13-'Operative BP'!$P$15))+M66","v":-90.79138408795734},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O13-'Operative BP'!$P$15))+N66","v":-7152.5717484568822},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D13-'Operative BP'!$P$15))+AQ40","v":-2745.72},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E13-'Operative BP'!$P$15))+AR40","v":-2228.9399999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F13-'Operative BP'!$P$15))+AS40","v":-1359.8100000000002},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G13-'Operative BP'!$P$15))+AT40","v":261},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H13-'Operative BP'!$P$15))+AU40","v":1599.9300000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I13-'Operative BP'!$P$15))+AV40","v":2398.5900000000011},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J13-'Operative BP'!$P$15))+AW40","v":2727.4500000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K13-'Operative BP'!$P$15))+AX40","v":2750.9400000000014},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L13-'Operative BP'!$P$15))+AY40","v":1999.2599999999991},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M13-'Operative BP'!$P$15))+AZ40","v":542.87999999999954},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N13-'Operative BP'!$P$15))+BA40","v":-843.02999999999918},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O13-'Operative BP'!$P$15))+BB40","v":-2510.8200000000002},null,9,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D13-'Operative BP'!$P$15))+BE40","v":-2816.73},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E13-'Operative BP'!$P$15))+BF40","v":-2286.5849999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F13-'Operative BP'!$P$15))+BG40","v":-1394.9775000000002},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G13-'Operative BP'!$P$15))+BH40","v":267.75},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H13-'Operative BP'!$P$15))+BI40","v":1641.3075000000006},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I13-'Operative BP'!$P$15))+BJ40","v":2460.6225000000013},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J13-'Operative BP'!$P$15))+BK40","v":2797.9875000000006},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K13-'Operative BP'!$P$15))+BL40","v":2822.0850000000019},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L13-'Operative BP'!$P$15))+BM40","v":2050.9649999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M13-'Operative BP'!$P$15))+BN40","v":556.9199999999995},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N13-'Operative BP'!$P$15))+BO40","v":-864.83249999999919},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O13-'Operative BP'!$P$15))+BP40","v":-2575.7550000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D14-'Operative BP'!$P$15))+C67","v":-6278.5163447527193},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E14-'Operative BP'!$P$15))+D67","v":-5111.8579220944503},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F14-'Operative BP'!$P$15))+E67","v":-2464.7006728588085},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G14-'Operative BP'!$P$15))+F67","v":2774.3732696439383},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H14-'Operative BP'!$P$15))+G67","v":7566.1649999999963},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I14-'Operative BP'!$P$15))+H67","v":10588.679999999998},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J14-'Operative BP'!$P$15))+I67","v":12197.262791037934},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K14-'Operative BP'!$P$15))+J67","v":12909.689492246795},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L14-'Operative BP'!$P$15))+K67","v":9777.6719407707533},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M14-'Operative BP'!$P$15))+L67","v":4674.4278523579242},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N14-'Operative BP'!$P$15))+M67","v":1193.2006685207261},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O14-'Operative BP'!$P$15))+N67","v":-5650.7545752546248},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D14-'Operative BP'!$P$15))+AQ41","v":-2369.8799999999997},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E14-'Operative BP'!$P$15))+AR41","v":-1829.6099999999994},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F14-'Operative BP'!$P$15))+AS41","v":-983.97000000000082},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G14-'Operative BP'!$P$15))+AT41","v":707.31000000000017},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H14-'Operative BP'!$P$15))+AU41","v":1999.2599999999991},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I14-'Operative BP'!$P$15))+AV41","v":2797.9199999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J14-'Operative BP'!$P$15))+AW41","v":3220.7400000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K14-'Operative BP'!$P$15))+AX41","v":3291.21},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L14-'Operative BP'!$P$15))+AY41","v":2469.0599999999986},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M14-'Operative BP'!$P$15))+AZ41","v":1036.1699999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N14-'Operative BP'!$P$15))+BA41","v":-326.25},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O14-'Operative BP'!$P$15))+BB41","v":-2111.4899999999998},null,10,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D14-'Operative BP'!$P$15))+BE41","v":-2431.1699999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E14-'Operative BP'!$P$15))+BF41","v":-1876.9274999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F14-'Operative BP'!$P$15))+BG41","v":-1009.4175000000008},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G14-'Operative BP'!$P$15))+BH41","v":725.60250000000019},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H14-'Operative BP'!$P$15))+BI41","v":2050.9649999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I14-'Operative BP'!$P$15))+BJ41","v":2870.2799999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J14-'Operative BP'!$P$15))+BK41","v":3304.0350000000008},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K14-'Operative BP'!$P$15))+BL41","v":3376.3274999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L14-'Operative BP'!$P$15))+BM41","v":2532.9149999999981},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M14-'Operative BP'!$P$15))+BN41","v":1062.9674999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N14-'Operative BP'!$P$15))+BO41","v":-334.6875},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O14-'Operative BP'!$P$15))+BP41","v":-2166.0974999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D15-'Operative BP'!$P$15))+C68","v":-5587.073269486229},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E15-'Operative BP'!$P$15))+D68","v":-4988.8829688648157},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F15-'Operative BP'!$P$15))+E68","v":-2479.2524999999982},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G15-'Operative BP'!$P$15))+F68","v":4099.1624999999985},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H15-'Operative BP'!$P$15))+G68","v":8810.7300000000014},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I15-'Operative BP'!$P$15))+H68","v":11922.1425},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J15-'Operative BP'!$P$15))+I68","v":13611.195000000002},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K15-'Operative BP'!$P$15))+J68","v":14144.58},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L15-'Operative BP'!$P$15))+K68","v":10588.679999999998},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M15-'Operative BP'!$P$15))+L68","v":5687.2181201960711},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N15-'Operative BP'!$P$15))+M68","v":3211.2646945218776},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O15-'Operative BP'!$P$15))+N68","v":-4030.2110825407785},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D15-'Operative BP'!$P$15))+AQ42","v":-2041.02},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E15-'Operative BP'!$P$15))+AR42","v":-1383.2999999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F15-'Operative BP'!$P$15))+AS42","v":-655.10999999999945},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G15-'Operative BP'!$P$15))+AT42","v":1083.1499999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H15-'Operative BP'!$P$15))+AU42","v":2328.1200000000003},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I15-'Operative BP'!$P$15))+AV42","v":3150.27},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J15-'Operative BP'!$P$15))+AW42","v":3596.5800000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K15-'Operative BP'!$P$15))+AX42","v":3737.52},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L15-'Operative BP'!$P$15))+AY42","v":2797.9199999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M15-'Operative BP'!$P$15))+AZ42","v":1435.5},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N15-'Operative BP'!$P$15))+BA42","v":143.54999999999927},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O15-'Operative BP'!$P$15))+BB42","v":-1712.1599999999996},null,11,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D15-'Operative BP'!$P$15))+BE42","v":-2093.8050000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E15-'Operative BP'!$P$15))+BF42","v":-1419.0749999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F15-'Operative BP'!$P$15))+BG42","v":-672.05249999999944},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G15-'Operative BP'!$P$15))+BH42","v":1111.1624999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H15-'Operative BP'!$P$15))+BI42","v":2388.3300000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I15-'Operative BP'!$P$15))+BJ42","v":3231.7425000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J15-'Operative BP'!$P$15))+BK42","v":3689.5950000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K15-'Operative BP'!$P$15))+BL42","v":3834.1800000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L15-'Operative BP'!$P$15))+BM42","v":2870.2799999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M15-'Operative BP'!$P$15))+BN42","v":1472.625},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N15-'Operative BP'!$P$15))+BO42","v":147.26249999999925},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O15-'Operative BP'!$P$15))+BP42","v":-1756.4399999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D16-'Operative BP'!$P$15))+C69","v":-3818.869585963103},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E16-'Operative BP'!$P$15))+D69","v":-3860.517803072617},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F16-'Operative BP'!$P$15))+E69","v":-1679.1750000000029},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G16-'Operative BP'!$P$15))+F69","v":5165.9325000000035},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H16-'Operative BP'!$P$15))+G69","v":9788.6024999999972},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I16-'Operative BP'!$P$15))+H69","v":13077.810000000001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J16-'Operative BP'!$P$15))+I69","v":14500.17},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K16-'Operative BP'!$P$15))+J69","v":15122.452499999996},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L16-'Operative BP'!$P$15))+K69","v":11477.654999999997},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M16-'Operative BP'!$P$15))+L69","v":6876.5326806083012},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N16-'Operative BP'!$P$15))+M69","v":4978.1744256777311},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O16-'Operative BP'!$P$15))+N69","v":-2350.7736577268274},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D16-'Operative BP'!$P$15))+AQ43","v":-1712.1599999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E16-'Operative BP'!$P$15))+AR43","v":-1054.4399999999998},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F16-'Operative BP'!$P$15))+AS43","v":-443.70000000000073},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G16-'Operative BP'!$P$15))+AT43","v":1365.0300000000011},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H16-'Operative BP'!$P$15))+AU43","v":2586.5099999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I16-'Operative BP'!$P$15))+AV43","v":3455.6400000000003},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J16-'Operative BP'!$P$15))+AW43","v":3831.48},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K16-'Operative BP'!$P$15))+AX43","v":3995.9099999999989},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L16-'Operative BP'!$P$15))+AY43","v":3032.8199999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M16-'Operative BP'!$P$15))+AZ43","v":1764.3599999999994},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N16-'Operative BP'!$P$15))+BA43","v":472.41000000000059},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O16-'Operative BP'!$P$15))+BB43","v":-1430.2799999999993},null,12,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D16-'Operative BP'!$P$15))+BE43","v":-1756.4399999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E16-'Operative BP'!$P$15))+BF43","v":-1081.7099999999998},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F16-'Operative BP'!$P$15))+BG43","v":-455.17500000000075},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G16-'Operative BP'!$P$15))+BH43","v":1400.3325000000011},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H16-'Operative BP'!$P$15))+BI43","v":2653.4024999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I16-'Operative BP'!$P$15))+BJ43","v":3545.0100000000007},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J16-'Operative BP'!$P$15))+BK43","v":3930.5699999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K16-'Operative BP'!$P$15))+BL43","v":4099.2524999999987},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L16-'Operative BP'!$P$15))+BM43","v":3111.2549999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M16-'Operative BP'!$P$15))+BN43","v":1809.9899999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N16-'Operative BP'!$P$15))+BO43","v":484.62750000000062},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O16-'Operative BP'!$P$15))+BP43","v":-1467.2699999999991},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D17-'Operative BP'!$P$15))+C70","v":-2951.5943588951409},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E17-'Operative BP'!$P$15))+D70","v":-2492.3669167183662},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F17-'Operative BP'!$P$15))+E70","v":98.775000000001398},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G17-'Operative BP'!$P$15))+F70","v":5788.2149999999992},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H17-'Operative BP'!$P$15))+G70","v":10766.474999999999},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I17-'Operative BP'!$P$15))+H70","v":13700.092499999997},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J17-'Operative BP'!$P$15))+I70","v":15211.349999999999},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K17-'Operative BP'!$P$15))+J70","v":16100.324999999997},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L17-'Operative BP'!$P$15))+K70","v":12366.629999999996},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M17-'Operative BP'!$P$15))+L70","v":7881.7106178725826},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N17-'Operative BP'!$P$15))+M70","v":5537.0094372209005},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O17-'Operative BP'!$P$15))+N70","v":-1539.9078515208721},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D17-'Operative BP'!$P$15))+AQ44","v":-1453.77},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E17-'Operative BP'!$P$15))+AR44","v":-702.08999999999946},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F17-'Operative BP'!$P$15))+AS44","v":26.100000000000371},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G17-'Operative BP'!$P$15))+AT44","v":1529.4599999999998},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H17-'Operative BP'!$P$15))+AU44","v":2844.8999999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I17-'Operative BP'!$P$15))+AV44","v":3620.0699999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J17-'Operative BP'!$P$15))+AW44","v":4019.3999999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K17-'Operative BP'!$P$15))+AX44","v":4254.2999999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L17-'Operative BP'!$P$15))+AY44","v":3267.7199999999989},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M17-'Operative BP'!$P$15))+AZ44","v":1999.2599999999991},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N17-'Operative BP'!$P$15))+BA44","v":754.29000000000019},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O17-'Operative BP'!$P$15))+BB44","v":-1148.3999999999996},null,13,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D17-'Operative BP'!$P$15))+BE44","v":-1491.3675000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E17-'Operative BP'!$P$15))+BF44","v":-720.24749999999938},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F17-'Operative BP'!$P$15))+BG44","v":26.775000000000382},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G17-'Operative BP'!$P$15))+BH44","v":1569.0149999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H17-'Operative BP'!$P$15))+BI44","v":2918.4749999999995},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I17-'Operative BP'!$P$15))+BJ44","v":3713.6924999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J17-'Operative BP'!$P$15))+BK44","v":4123.3499999999995},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K17-'Operative BP'!$P$15))+BL44","v":4364.3249999999989},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L17-'Operative BP'!$P$15))+BM44","v":3352.2299999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M17-'Operative BP'!$P$15))+BN44","v":2050.9649999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N17-'Operative BP'!$P$15))+BO44","v":773.79750000000013},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O17-'Operative BP'!$P$15))+BP44","v":-1178.0999999999997},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($AH$29<DEGREES(BS97),0+$AJ$33,1-((TAN(BS97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BT97),0+$AJ$33,1-((TAN(BT97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BU97),0+$AJ$33,1-((TAN(BU97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BV97),0+$AJ$33,1-((TAN(BV97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BW97),0+$AJ$33,1-((TAN(BW97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BX97),0+$AJ$33,1-((TAN(BX97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BY97),0+$AJ$33,1-((TAN(BY97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BZ97),0+$AJ$33,1-((TAN(BZ97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CA97),0+$AJ$33,1-((TAN(CA97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CB97),0+$AJ$33,1-((TAN(CB97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CC97),0+$AJ$33,1-((TAN(CC97)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CD97),0+$AJ$33,1-((TAN(CD97)/TAN($AG$31))*(1-$AJ$16)))","v":1}]
[null,14,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D18-'Operative BP'!$P$15))+C71","v":-2630.5705379518313},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E18-'Operative BP'!$P$15))+D71","v":-1353.2440241661516},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F18-'Operative BP'!$P$15))+E71","v":898.85249999999667},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G18-'Operative BP'!$P$15))+F71","v":6499.3949999999986},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H18-'Operative BP'!$P$15))+G71","v":11477.654999999997},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I18-'Operative BP'!$P$15))+H71","v":14766.862500000003},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J18-'Operative BP'!$P$15))+I71","v":16011.427499999994},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K18-'Operative BP'!$P$15))+J71","v":16544.8125},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L18-'Operative BP'!$P$15))+K71","v":12900.014999999996},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M18-'Operative BP'!$P$15))+L71","v":9423.5629135160179},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N18-'Operative BP'!$P$15))+M71","v":6103.20748486507},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O18-'Operative BP'!$P$15))+N71","v":-1169.7955370990076},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D18-'Operative BP'!$P$15))+AQ45","v":-1242.3599999999994},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E18-'Operative BP'!$P$15))+AR45","v":-443.70000000000073},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F18-'Operative BP'!$P$15))+AS45","v":237.50999999999911},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G18-'Operative BP'!$P$15))+AT45","v":1717.3799999999997},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H18-'Operative BP'!$P$15))+AU45","v":3032.8199999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I18-'Operative BP'!$P$15))+AV45","v":3901.9500000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J18-'Operative BP'!$P$15))+AW45","v":4230.8099999999986},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K18-'Operative BP'!$P$15))+AX45","v":4371.75},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L18-'Operative BP'!$P$15))+AY45","v":3408.6599999999989},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M18-'Operative BP'!$P$15))+AZ45","v":2873.704492299566},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N18-'Operative BP'!$P$15))+BA45","v":1611.3722542874291},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O18-'Operative BP'!$P$15))+BB45","v":-754.84525828604103},null,14,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D18-'Operative BP'!$P$15))+BE45","v":-1274.4899999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E18-'Operative BP'!$P$15))+BF45","v":-455.17500000000075},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F18-'Operative BP'!$P$15))+BG45","v":243.65249999999909},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G18-'Operative BP'!$P$15))+BH45","v":1761.7949999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H18-'Operative BP'!$P$15))+BI45","v":3111.2549999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I18-'Operative BP'!$P$15))+BJ45","v":4002.8625000000006},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J18-'Operative BP'!$P$15))+BK45","v":4340.2274999999981},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K18-'Operative BP'!$P$15))+BL45","v":4484.8125},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L18-'Operative BP'!$P$15))+BM45","v":3496.8149999999987},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M18-'Operative BP'!$P$15))+BN45","v":2243.7450000000008},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N18-'Operative BP'!$P$15))+BO45","v":894.28500000000088},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O18-'Operative BP'!$P$15))+BP45","v":-985.31999999999994},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D19-'Operative BP'!$P$15))+C72","v":-1055.8788635038545},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E19-'Operative BP'!$P$15))+D72","v":1481.4489509698931},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F19-'Operative BP'!$P$15))+E72","v":4067.8078218185497},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G19-'Operative BP'!$P$15))+F72","v":9683.5085864388384},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H19-'Operative BP'!$P$15))+G72","v":14294.658561173921},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I19-'Operative BP'!$P$15))+H72","v":16991.329489745669},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J19-'Operative BP'!$P$15))+I72","v":18273.143712626272},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K19-'Operative BP'!$P$15))+J72","v":19660.685668513943},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L19-'Operative BP'!$P$15))+K72","v":17179.355569186573},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M19-'Operative BP'!$P$15))+L72","v":12843.375518668121},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N19-'Operative BP'!$P$15))+M72","v":7994.4701437891308},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O19-'Operative BP'!$P$15))+N72","v":130.58242359220321},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D19-'Operative BP'!$P$15))+AQ46","v":754.68169495344614},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E19-'Operative BP'!$P$15))+AR46","v":1960.0178473297503},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F19-'Operative BP'!$P$15))+AS46","v":3014.0203218185475},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G19-'Operative BP'!$P$15))+AT46","v":4574.4560864388368},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H19-'Operative BP'!$P$15))+AU46","v":5719.0085611739232},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I19-'Operative BP'!$P$15))+AV46","v":5864.7869897456721},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J19-'Operative BP'!$P$15))+AW46","v":6165.4887126262738},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K19-'Operative BP'!$P$15))+AX46","v":7356.8081685139459},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L19-'Operative BP'!$P$15))+AY46","v":7426.3705691865707},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M19-'Operative BP'!$P$15))+AZ46","v":6128.2423600598431},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N19-'Operative BP'!$P$15))+BA46","v":3815.7728668421332},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O19-'Operative BP'!$P$15))+BB46","v":1053.0825015893793},null,15,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D19-'Operative BP'!$P$15))+BE46","v":-1202.1975000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E19-'Operative BP'!$P$15))+BF46","v":-310.58999999999907},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F19-'Operative BP'!$P$15))+BG46","v":388.23750000000075},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G19-'Operative BP'!$P$15))+BH46","v":1882.2825000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H19-'Operative BP'!$P$15))+BI46","v":3159.4499999999994},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I19-'Operative BP'!$P$15))+BJ46","v":4099.2524999999987},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J19-'Operative BP'!$P$15))+BK46","v":4460.7149999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K19-'Operative BP'!$P$15))+BL46","v":4533.0074999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L19-'Operative BP'!$P$15))+BM46","v":3593.2050000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M19-'Operative BP'!$P$15))+BN46","v":2364.2324999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N19-'Operative BP'!$P$15))+BO46","v":1062.9674999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O19-'Operative BP'!$P$15))+BP46","v":-888.93000000000006},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D20-'Operative BP'!$P$15))+C73","v":-857.81080670663505},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E20-'Operative BP'!$P$15))+D73","v":2421.3789414750472},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F20-'Operative BP'!$P$15))+E73","v":6056.842070789593},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G20-'Operative BP'!$P$15))+F73","v":11362.637394416441},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H20-'Operative BP'!$P$15))+G73","v":16715.700889348442},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I20-'Operative BP'!$P$15))+H73","v":20014.378016052709},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J20-'Operative BP'!$P$15))+I73","v":21296.138042390001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K20-'Operative BP'!$P$15))+J73","v":22078.305550101773},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L20-'Operative BP'!$P$15))+K73","v":18357.164865580482},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M20-'Operative BP'!$P$15))+L73","v":12517.590268512353},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N20-'Operative BP'!$P$15))+M73","v":6448.5390396841258},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O20-'Operative BP'!$P$15))+N73","v":-780.01021963482572},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D20-'Operative BP'!$P$15))+AQ47","v":1626.2294384683141},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E20-'Operative BP'!$P$15))+AR47","v":3384.8472992127708},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F20-'Operative BP'!$P$15))+AS47","v":4872.2395707895957},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G20-'Operative BP'!$P$15))+AT47","v":6515.2148944164401},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H20-'Operative BP'!$P$15))+AU47","v":8074.6433893484409},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I20-'Operative BP'!$P$15))+AV47","v":8822.4280160527087},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J20-'Operative BP'!$P$15))+AW47","v":9253.8905423899996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K20-'Operative BP'!$P$15))+AX47","v":9970.6505501017746},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L20-'Operative BP'!$P$15))+AY47","v":8669.5873655804826},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M20-'Operative BP'!$P$15))+AZ47","v":6296.6102685123551},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N20-'Operative BP'!$P$15))+BA47","v":3508.4192330867613},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O20-'Operative BP'!$P$15))+BB47","v":1203.8338343325777},null,16,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D20-'Operative BP'!$P$15))+BE47","v":-1178.0999999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E20-'Operative BP'!$P$15))+BF47","v":-358.78500000000093},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F20-'Operative BP'!$P$15))+BG47","v":436.43249999999875},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G20-'Operative BP'!$P$15))+BH47","v":1785.8925000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H20-'Operative BP'!$P$15))+BI47","v":3183.5475000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I20-'Operative BP'!$P$15))+BJ47","v":4123.3499999999995},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J20-'Operative BP'!$P$15))+BK47","v":4436.6175000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K20-'Operative BP'!$P$15))+BL47","v":4460.7149999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L20-'Operative BP'!$P$15))+BM47","v":3569.1074999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M20-'Operative BP'!$P$15))+BN47","v":2291.9399999999987},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N20-'Operative BP'!$P$15))+BO47","v":942.48000000000081},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O20-'Operative BP'!$P$15))+BP47","v":-985.31999999999994},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D21-'Operative BP'!$P$15))+C74","v":-3288.2685036873836},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E21-'Operative BP'!$P$15))+D74","v":620.54715504360865},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F21-'Operative BP'!$P$15))+E74","v":4566.8895072817813},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G21-'Operative BP'!$P$15))+F74","v":9368.4561381491912},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H21-'Operative BP'!$P$15))+G74","v":15505.418132662129},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I21-'Operative BP'!$P$15))+H74","v":19043.073761054795},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J21-'Operative BP'!$P$15))+I74","v":20392.614115789078},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K21-'Operative BP'!$P$15))+J74","v":20256.876426143474},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L21-'Operative BP'!$P$15))+K74","v":15926.347713186471},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M21-'Operative BP'!$P$15))+L74","v":9802.5954833431952},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N21-'Operative BP'!$P$15))+M74","v":3372.2790604325933},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O21-'Operative BP'!$P$15))+N74","v":-3798.0601279719804},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D21-'Operative BP'!$P$15))+AQ48","v":301.87649631261479},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E21-'Operative BP'!$P$15))+AR48","v":2117.65215504361},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F21-'Operative BP'!$P$15))+AS48","v":3774.7320072817784},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G21-'Operative BP'!$P$15))+AT48","v":5109.701138149192},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H21-'Operative BP'!$P$15))+AU48","v":6929.7681326621314},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I21-'Operative BP'!$P$15))+AV48","v":8112.7537610547924},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J21-'Operative BP'!$P$15))+AW48","v":8546.5891157890801},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K21-'Operative BP'!$P$15))+AX48","v":8607.0739261434719},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L21-'Operative BP'!$P$15))+AY48","v":6762.0302131864719},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M21-'Operative BP'!$P$15))+AZ48","v":3974.0604833431971},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N21-'Operative BP'!$P$15))+BA48","v":1402.7865604325928},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O21-'Operative BP'!$P$15))+BB48","v":-452.13119601023845},null,17,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D21-'Operative BP'!$P$15))+BE48","v":-1322.6849999999995},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E21-'Operative BP'!$P$15))+BF48","v":-551.56500000000062},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F21-'Operative BP'!$P$15))+BG48","v":291.84750000000093},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G21-'Operative BP'!$P$15))+BH48","v":1569.0149999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H21-'Operative BP'!$P$15))+BI48","v":3159.4499999999994},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I21-'Operative BP'!$P$15))+BJ48","v":4026.9600000000019},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J21-'Operative BP'!$P$15))+BK48","v":4364.3249999999989},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K21-'Operative BP'!$P$15))+BL48","v":4292.0325000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L21-'Operative BP'!$P$15))+BM48","v":3376.3274999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M21-'Operative BP'!$P$15))+BN48","v":2147.3549999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N21-'Operative BP'!$P$15))+BO48","v":725.60250000000019},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O21-'Operative BP'!$P$15))+BP48","v":-1250.3925000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D22-'Operative BP'!$P$15))+C75","v":-5768.46},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E22-'Operative BP'!$P$15))+D75","v":-2501.0568028826492},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F22-'Operative BP'!$P$15))+E75","v":1274.2531885455667},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G22-'Operative BP'!$P$15))+F75","v":6103.1600812956976},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H22-'Operative BP'!$P$15))+G75","v":12444.343198998187},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I22-'Operative BP'!$P$15))+H75","v":16288.968562603864},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J22-'Operative BP'!$P$15))+I75","v":17292.202069608305},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K22-'Operative BP'!$P$15))+J75","v":16573.650784288155},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L22-'Operative BP'!$P$15))+K75","v":11922.1425},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M22-'Operative BP'!$P$15))+L75","v":7210.5749999999971},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N22-'Operative BP'!$P$15))+M75","v":1432.2375000000029},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O22-'Operative BP'!$P$15))+N75","v":-5235.0749999999971},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D22-'Operative BP'!$P$15))+AQ49","v":-1524.24},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E22-'Operative BP'!$P$15))+AR49","v":-349.87680288264852},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F22-'Operative BP'!$P$15))+AS49","v":939.94818854556593},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G22-'Operative BP'!$P$15))+AT49","v":2367.6650812956973},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H22-'Operative BP'!$P$15))+AU49","v":4326.5456989981867},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I22-'Operative BP'!$P$15))+AV49","v":5685.6860626038624},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J22-'Operative BP'!$P$15))+AW49","v":5969.437069608306},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K22-'Operative BP'!$P$15))+AX49","v":5512.5157842881563},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L22-'Operative BP'!$P$15))+AY49","v":3150.27},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M22-'Operative BP'!$P$15))+AZ49","v":1905.2999999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N22-'Operative BP'!$P$15))+BA49","v":378.45000000000073},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O22-'Operative BP'!$P$15))+BB49","v":-1383.2999999999993},null,18,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D22-'Operative BP'!$P$15))+BE49","v":-1563.6599999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E22-'Operative BP'!$P$15))+BF49","v":-792.54000000000019},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F22-'Operative BP'!$P$15))+BG49","v":123.16500000000023},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G22-'Operative BP'!$P$15))+BH49","v":1376.2350000000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H22-'Operative BP'!$P$15))+BI49","v":2990.7675000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I22-'Operative BP'!$P$15))+BJ49","v":3906.4725000000008},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J22-'Operative BP'!$P$15))+BK49","v":4171.5449999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K22-'Operative BP'!$P$15))+BL49","v":4075.1549999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L22-'Operative BP'!$P$15))+BM49","v":3231.7425000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M22-'Operative BP'!$P$15))+BN49","v":1954.5749999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N22-'Operative BP'!$P$15))+BO49","v":388.23750000000075},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O22-'Operative BP'!$P$15))+BP49","v":-1419.0749999999991},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D23-'Operative BP'!$P$15))+C76","v":-6657.4350000000022},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E23-'Operative BP'!$P$15))+D76","v":-3812.7149999999992},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F23-'Operative BP'!$P$15))+E76","v":-345.7125000000014},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G23-'Operative BP'!$P$15))+F76","v":3832.4699999999957},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H23-'Operative BP'!$P$15))+G76","v":10233.09},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I23-'Operative BP'!$P$15))+H76","v":13433.400000000001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J23-'Operative BP'!$P$15))+I76","v":14144.58},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K23-'Operative BP'!$P$15))+J76","v":13877.887499999997},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L23-'Operative BP'!$P$15))+K76","v":11033.167500000001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M23-'Operative BP'!$P$15))+L76","v":6232.7024999999949},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N23-'Operative BP'!$P$15))+M76","v":454.36500000000086},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O23-'Operative BP'!$P$15))+N76","v":-6479.6399999999985},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D23-'Operative BP'!$P$15))+AQ50","v":-1759.1400000000006},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E23-'Operative BP'!$P$15))+AR50","v":-1007.4599999999998},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F23-'Operative BP'!$P$15))+AS50","v":-91.350000000000364},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G23-'Operative BP'!$P$15))+AT50","v":1012.6799999999988},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H23-'Operative BP'!$P$15))+AU50","v":2703.96},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I23-'Operative BP'!$P$15))+AV50","v":3549.6000000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J23-'Operative BP'!$P$15))+AW50","v":3737.52},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K23-'Operative BP'!$P$15))+AX50","v":3667.0499999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L23-'Operative BP'!$P$15))+AY50","v":2915.3700000000003},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M23-'Operative BP'!$P$15))+AZ50","v":1646.9099999999987},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N23-'Operative BP'!$P$15))+BA50","v":120.06000000000023},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O23-'Operative BP'!$P$15))+BB50","v":-1712.1599999999996},null,19,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D23-'Operative BP'!$P$15))+BE50","v":-1804.6350000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E23-'Operative BP'!$P$15))+BF50","v":-1033.5149999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F23-'Operative BP'!$P$15))+BG50","v":-93.712500000000375},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G23-'Operative BP'!$P$15))+BH50","v":1038.8699999999988},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H23-'Operative BP'!$P$15))+BI50","v":2773.89},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I23-'Operative BP'!$P$15))+BJ50","v":3641.4000000000005},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J23-'Operative BP'!$P$15))+BK50","v":3834.1800000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K23-'Operative BP'!$P$15))+BL50","v":3761.8874999999994},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L23-'Operative BP'!$P$15))+BM50","v":2990.7675000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M23-'Operative BP'!$P$15))+BN50","v":1689.5024999999987},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N23-'Operative BP'!$P$15))+BO50","v":123.16500000000023},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O23-'Operative BP'!$P$15))+BP50","v":-1756.4399999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D24-'Operative BP'!$P$15))+C77","v":-7635.3074999999972},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E24-'Operative BP'!$P$15))+D77","v":-4968.3825000000015},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F24-'Operative BP'!$P$15))+E77","v":-1590.2774999999995},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G24-'Operative BP'!$P$15))+F77","v":3032.3925000000004},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H24-'Operative BP'!$P$15))+G77","v":9077.4225000000042},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I24-'Operative BP'!$P$15))+H77","v":12188.835000000003},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J24-'Operative BP'!$P$15))+I77","v":12366.629999999996},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K24-'Operative BP'!$P$15))+J77","v":12455.5275},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L24-'Operative BP'!$P$15))+K77","v":9877.5},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M24-'Operative BP'!$P$15))+L77","v":4721.4450000000015},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N24-'Operative BP'!$P$15))+M77","v":-790.1999999999972},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O24-'Operative BP'!$P$15))+N77","v":-7368.6150000000007},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D24-'Operative BP'!$P$15))+AQ51","v":-2017.5299999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E24-'Operative BP'!$P$15))+AR51","v":-1312.8300000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F24-'Operative BP'!$P$15))+AS51","v":-420.20999999999987},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G24-'Operative BP'!$P$15))+AT51","v":801.2700000000001},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H24-'Operative BP'!$P$15))+AU51","v":2398.5900000000011},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I24-'Operative BP'!$P$15))+AV51","v":3220.7400000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J24-'Operative BP'!$P$15))+AW51","v":3267.7199999999989},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K24-'Operative BP'!$P$15))+AX51","v":3291.21},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L24-'Operative BP'!$P$15))+AY51","v":2610},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M24-'Operative BP'!$P$15))+AZ51","v":1247.5800000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N24-'Operative BP'!$P$15))+BA51","v":-208.79999999999927},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O24-'Operative BP'!$P$15))+BB51","v":-1947.0600000000002},null,20,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D24-'Operative BP'!$P$15))+BE51","v":-2069.7074999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E24-'Operative BP'!$P$15))+BF51","v":-1346.7825000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F24-'Operative BP'!$P$15))+BG51","v":-431.07749999999987},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G24-'Operative BP'!$P$15))+BH51","v":821.99250000000006},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H24-'Operative BP'!$P$15))+BI51","v":2460.6225000000013},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I24-'Operative BP'!$P$15))+BJ51","v":3304.0350000000008},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J24-'Operative BP'!$P$15))+BK51","v":3352.2299999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K24-'Operative BP'!$P$15))+BL51","v":3376.3274999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L24-'Operative BP'!$P$15))+BM51","v":2677.5},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M24-'Operative BP'!$P$15))+BN51","v":1279.8450000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N24-'Operative BP'!$P$15))+BO51","v":-214.19999999999925},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O24-'Operative BP'!$P$15))+BP51","v":-1997.4150000000002},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D25-'Operative BP'!$P$15))+C78","v":-8257.59},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E25-'Operative BP'!$P$15))+D78","v":-5857.3575000000001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F25-'Operative BP'!$P$15))+E78","v":-2301.4574999999982},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G25-'Operative BP'!$P$15))+F78","v":2232.3149999999982},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H25-'Operative BP'!$P$15))+G78","v":8099.5500000000029},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I25-'Operative BP'!$P$15))+H78","v":10855.372500000001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J25-'Operative BP'!$P$15))+I78","v":10944.269999999999},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K25-'Operative BP'!$P$15))+J78","v":11477.654999999997},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L25-'Operative BP'!$P$15))+K78","v":8632.9350000000013},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M25-'Operative BP'!$P$15))+L78","v":3743.5724999999993},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N25-'Operative BP'!$P$15))+M78","v":-1590.2774999999995},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O25-'Operative BP'!$P$15))+N78","v":-7990.8975},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D25-'Operative BP'!$P$15))+AQ52","v":-2181.96},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E25-'Operative BP'!$P$15))+AR52","v":-1547.73},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F25-'Operative BP'!$P$15))+AS52","v":-608.12999999999954},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G25-'Operative BP'!$P$15))+AT52","v":589.85999999999945},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H25-'Operative BP'!$P$15))+AU52","v":2140.2000000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I25-'Operative BP'!$P$15))+AV52","v":2868.3900000000003},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J25-'Operative BP'!$P$15))+AW52","v":2891.8799999999997},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K25-'Operative BP'!$P$15))+AX52","v":3032.8199999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L25-'Operative BP'!$P$15))+AY52","v":2281.1400000000003},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M25-'Operative BP'!$P$15))+AZ52","v":989.18999999999983},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N25-'Operative BP'!$P$15))+BA52","v":-420.20999999999987},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O25-'Operative BP'!$P$15))+BB52","v":-2111.4899999999998},null,21,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D25-'Operative BP'!$P$15))+BE52","v":-2238.39},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E25-'Operative BP'!$P$15))+BF52","v":-1587.7574999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F25-'Operative BP'!$P$15))+BG52","v":-623.8574999999995},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G25-'Operative BP'!$P$15))+BH52","v":605.11499999999944},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H25-'Operative BP'!$P$15))+BI52","v":2195.5500000000006},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I25-'Operative BP'!$P$15))+BJ52","v":2942.5725000000007},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J25-'Operative BP'!$P$15))+BK52","v":2966.6699999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K25-'Operative BP'!$P$15))+BL52","v":3111.2549999999992},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L25-'Operative BP'!$P$15))+BM52","v":2340.1350000000007},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M25-'Operative BP'!$P$15))+BN52","v":1014.7724999999998},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N25-'Operative BP'!$P$15))+BO52","v":-431.07749999999987},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O25-'Operative BP'!$P$15))+BP52","v":-2166.0974999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D26-'Operative BP'!$P$15))+C79","v":-8968.7699999999986},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E26-'Operative BP'!$P$15))+D79","v":-6746.3324999999986},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F26-'Operative BP'!$P$15))+E79","v":-3101.5350000000008},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G26-'Operative BP'!$P$15))+F79","v":1432.2375000000029},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H26-'Operative BP'!$P$15))+G79","v":7210.5749999999971},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I26-'Operative BP'!$P$15))+H79","v":9699.7049999999999},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J26-'Operative BP'!$P$15))+I79","v":9610.8075000000044},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K26-'Operative BP'!$P$15))+J79","v":10499.782500000003},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L26-'Operative BP'!$P$15))+K79","v":7743.9600000000037},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M26-'Operative BP'!$P$15))+L79","v":2765.6999999999971},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N26-'Operative BP'!$P$15))+M79","v":-2568.1500000000015},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O26-'Operative BP'!$P$15))+N79","v":-8613.1799999999985},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D26-'Operative BP'!$P$15))+AQ53","v":-2369.8799999999997},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E26-'Operative BP'!$P$15))+AR53","v":-1782.6299999999997},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F26-'Operative BP'!$P$15))+AS53","v":-819.54000000000019},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G26-'Operative BP'!$P$15))+AT53","v":378.45000000000073},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H26-'Operative BP'!$P$15))+AU53","v":1905.2999999999993},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I26-'Operative BP'!$P$15))+AV53","v":2563.02},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J26-'Operative BP'!$P$15))+AW53","v":2539.5300000000011},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K26-'Operative BP'!$P$15))+AX53","v":2774.4300000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L26-'Operative BP'!$P$15))+AY53","v":2046.2400000000009},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M26-'Operative BP'!$P$15))+AZ53","v":730.79999999999927},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N26-'Operative BP'!$P$15))+BA53","v":-678.60000000000036},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O26-'Operative BP'!$P$15))+BB53","v":-2275.9199999999996},null,22,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D26-'Operative BP'!$P$15))+BE53","v":-2431.1699999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E26-'Operative BP'!$P$15))+BF53","v":-1828.7324999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F26-'Operative BP'!$P$15))+BG53","v":-840.73500000000013},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G26-'Operative BP'!$P$15))+BH53","v":388.23750000000075},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H26-'Operative BP'!$P$15))+BI53","v":1954.5749999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I26-'Operative BP'!$P$15))+BJ53","v":2629.3050000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J26-'Operative BP'!$P$15))+BK53","v":2605.2075000000009},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K26-'Operative BP'!$P$15))+BL53","v":2846.1825000000008},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L26-'Operative BP'!$P$15))+BM53","v":2099.1600000000008},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M26-'Operative BP'!$P$15))+BN53","v":749.69999999999925},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N26-'Operative BP'!$P$15))+BO53","v":-696.15000000000043},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O26-'Operative BP'!$P$15))+BP53","v":-2334.7799999999997},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D27-'Operative BP'!$P$15))+C80","v":-9591.0525000000016},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E27-'Operative BP'!$P$15))+D80","v":-7457.5125000000007},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F27-'Operative BP'!$P$15))+E80","v":-3812.7149999999992},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G27-'Operative BP'!$P$15))+F80","v":365.46750000000452},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H27-'Operative BP'!$P$15))+G80","v":6321.5999999999985},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I27-'Operative BP'!$P$15))+H80","v":8810.7300000000014},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J27-'Operative BP'!$P$15))+I80","v":8899.6274999999987},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K27-'Operative BP'!$P$15))+J80","v":9699.7049999999999},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L27-'Operative BP'!$P$15))+K80","v":6854.9850000000051},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M27-'Operative BP'!$P$15))+L80","v":1965.622500000002},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N27-'Operative BP'!$P$15))+M80","v":-3546.0225000000032},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O27-'Operative BP'!$P$15))+N80","v":-9057.6675000000014},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D27-'Operative BP'!$P$15))+AQ54","v":-2534.3100000000004},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E27-'Operative BP'!$P$15))+AR54","v":-1970.5500000000002},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F27-'Operative BP'!$P$15))+AS54","v":-1007.4599999999998},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G27-'Operative BP'!$P$15))+AT54","v":96.570000000001187},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H27-'Operative BP'!$P$15))+AU54","v":1670.3999999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I27-'Operative BP'!$P$15))+AV54","v":2328.1200000000003},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J27-'Operative BP'!$P$15))+AW54","v":2351.6099999999997},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K27-'Operative BP'!$P$15))+AX54","v":2563.02},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L27-'Operative BP'!$P$15))+AY54","v":1811.3400000000013},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M27-'Operative BP'!$P$15))+AZ54","v":519.39000000000055},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N27-'Operative BP'!$P$15))+BA54","v":-936.99000000000092},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O27-'Operative BP'!$P$15))+BB54","v":-2393.3700000000003},null,23,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D27-'Operative BP'!$P$15))+BE54","v":-2599.8525000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E27-'Operative BP'!$P$15))+BF54","v":-2021.5125000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F27-'Operative BP'!$P$15))+BG54","v":-1033.5149999999999},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G27-'Operative BP'!$P$15))+BH54","v":99.067500000001218},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H27-'Operative BP'!$P$15))+BI54","v":1713.5999999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I27-'Operative BP'!$P$15))+BJ54","v":2388.3300000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J27-'Operative BP'!$P$15))+BK54","v":2412.4274999999993},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K27-'Operative BP'!$P$15))+BL54","v":2629.3050000000003},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L27-'Operative BP'!$P$15))+BM54","v":1858.1850000000013},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M27-'Operative BP'!$P$15))+BN54","v":532.82250000000056},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N27-'Operative BP'!$P$15))+BO54","v":-961.22250000000088},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O27-'Operative BP'!$P$15))+BP54","v":-2455.2675000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!D28-'Operative BP'!$P$15))+C81","v":-10035.540000000001},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!E28-'Operative BP'!$P$15))+D81","v":-8257.59},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!F28-'Operative BP'!$P$15))+E81","v":-4523.8949999999986},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!G28-'Operative BP'!$P$15))+F81","v":-345.7125000000014},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!H28-'Operative BP'!$P$15))+G81","v":5521.5225000000037},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!I28-'Operative BP'!$P$15))+H81","v":7921.7549999999965},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!J28-'Operative BP'!$P$15))+I81","v":8277.345000000003},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!K28-'Operative BP'!$P$15))+J81","v":8810.7300000000014},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!L28-'Operative BP'!$P$15))+K81","v":6054.9075000000021},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!M28-'Operative BP'!$P$15))+L81","v":1254.4425000000031},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!N28-'Operative BP'!$P$15))+M81","v":-4168.3049999999985},{"$f":"(('Input Data'!$F$44-('Input Data'!$F$42*'Input Data'!$F$27))*('Dry Bulb'!O28-'Operative BP'!$P$15))+N81","v":-9857.7450000000008},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,{"$f":"('Input Data'!$F$56*('Dry Bulb'!D28-'Operative BP'!$P$15))+AQ55","v":-2651.76},{"$f":"('Input Data'!$F$56*('Dry Bulb'!E28-'Operative BP'!$P$15))+AR55","v":-2181.96},{"$f":"('Input Data'!$F$56*('Dry Bulb'!F28-'Operative BP'!$P$15))+AS55","v":-1195.3799999999997},{"$f":"('Input Data'!$F$56*('Dry Bulb'!G28-'Operative BP'!$P$15))+AT55","v":-91.350000000000364},{"$f":"('Input Data'!$F$56*('Dry Bulb'!H28-'Operative BP'!$P$15))+AU55","v":1458.9900000000009},{"$f":"('Input Data'!$F$56*('Dry Bulb'!I28-'Operative BP'!$P$15))+AV55","v":2093.2199999999989},{"$f":"('Input Data'!$F$56*('Dry Bulb'!J28-'Operative BP'!$P$15))+AW55","v":2187.1800000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!K28-'Operative BP'!$P$15))+AX55","v":2328.1200000000003},{"$f":"('Input Data'!$F$56*('Dry Bulb'!L28-'Operative BP'!$P$15))+AY55","v":1599.9300000000007},{"$f":"('Input Data'!$F$56*('Dry Bulb'!M28-'Operative BP'!$P$15))+AZ55","v":331.47000000000082},{"$f":"('Input Data'!$F$56*('Dry Bulb'!N28-'Operative BP'!$P$15))+BA55","v":-1101.4199999999996},{"$f":"('Input Data'!$F$56*('Dry Bulb'!O28-'Operative BP'!$P$15))+BB55","v":-2604.7800000000002},null,24,{"$f":"('Input Data'!$F$53*('Dry Bulb'!D28-'Operative BP'!$P$15))+BE55","v":-2720.34},{"$f":"('Input Data'!$F$53*('Dry Bulb'!E28-'Operative BP'!$P$15))+BF55","v":-2238.39},{"$f":"('Input Data'!$F$53*('Dry Bulb'!F28-'Operative BP'!$P$15))+BG55","v":-1226.2949999999996},{"$f":"('Input Data'!$F$53*('Dry Bulb'!G28-'Operative BP'!$P$15))+BH55","v":-93.712500000000375},{"$f":"('Input Data'!$F$53*('Dry Bulb'!H28-'Operative BP'!$P$15))+BI55","v":1496.722500000001},{"$f":"('Input Data'!$F$53*('Dry Bulb'!I28-'Operative BP'!$P$15))+BJ55","v":2147.3549999999991},{"$f":"('Input Data'!$F$53*('Dry Bulb'!J28-'Operative BP'!$P$15))+BK55","v":2243.7450000000008},{"$f":"('Input Data'!$F$53*('Dry Bulb'!K28-'Operative BP'!$P$15))+BL55","v":2388.3300000000004},{"$f":"('Input Data'!$F$53*('Dry Bulb'!L28-'Operative BP'!$P$15))+BM55","v":1641.3075000000006},{"$f":"('Input Data'!$F$53*('Dry Bulb'!M28-'Operative BP'!$P$15))+BN55","v":340.04250000000081},{"$f":"('Input Data'!$F$53*('Dry Bulb'!N28-'Operative BP'!$P$15))+BO55","v":-1129.9049999999997},{"$f":"('Input Data'!$F$53*('Dry Bulb'!O28-'Operative BP'!$P$15))+BP55","v":-2672.145},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"Heating Load",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UA Delta T Only",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,{"$f":"B31","v":1},{"$f":"IF(C31<0,C31,0)","v":-5.3513100000000032E-3},{"$f":"IF(D31<0,D31,0)","v":-2.9668725000000029E-3},-3.0516525000000012,0,0,0,0,0,0,0,-3.7773857699999973,-4.3021574999999998E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec","Average",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,{"$f":"B32","v":2},{"$f":"IF(C32<0,C32,0)","v":-5.8281975000000017E-3},-3.5391375000000014E-3,-3.7192950000000038,0,0,0,0,0,0,0,-3.4331625000000003,-4.6836675000000005E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D5-'Operative BP'!$P$15))","v":-2731.1287500000008},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E5-'Operative BP'!$P$15))","v":-2175.5193750000008},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F5-'Operative BP'!$P$15))","v":-1330.9931250000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G5-'Operative BP'!$P$15))","v":-241.99874999999923},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H5-'Operative BP'!$P$15))","v":1180.3612500000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I5-'Operative BP'!$P$15))","v":1802.6437499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J5-'Operative BP'!$P$15))","v":1958.214375},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K5-'Operative BP'!$P$15))","v":2024.8875000000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L5-'Operative BP'!$P$15))","v":1335.9318749999991},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M5-'Operative BP'!$P$15))","v":135.8156249999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N5-'Operative BP'!$P$15))","v":-1219.8712499999995},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O5-'Operative BP'!$P$15))","v":-2486.660625},{"$f":"AVERAGEIF(AS112:AZ135,\">0\")","v":2037.8866627358491},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"IF(C33<0,C33,0)","v":-6.114330000000002E-3},-4.1114025000000016E-3,-4.3869374999999993,-2.4182730000003174E-2,0,0,0,0,0,0,-4.1008049999999994,-5.0651775000000003E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D6-'Operative BP'!$P$15))","v":-2842.2506250000006},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E6-'Operative BP'!$P$15))","v":-2308.8656250000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F6-'Operative BP'!$P$15))","v":-1486.5637500000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G6-'Operative BP'!$P$15))","v":-375.34500000000077},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H6-'Operative BP'!$P$15))","v":1002.5662500000005},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I6-'Operative BP'!$P$15))","v":1580.3999999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J6-'Operative BP'!$P$15))","v":1758.1949999999995},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K6-'Operative BP'!$P$15))","v":1824.8681250000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L6-'Operative BP'!$P$15))","v":1113.6881249999994},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M6-'Operative BP'!$P$15))","v":-19.75499999999958},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N6-'Operative BP'!$P$15))","v":-1419.890625},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O6-'Operative BP'!$P$15))","v":-2575.558125},"Max",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"IF(C34<0,C34,0)","v":-6.5912175000000005E-3},-4.6836675000000005E-3,-4.8638250000000021,-0.96248349000000188,0,0,0,0,0,0,-4.7684474999999988,-5.5420649999999988E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D7-'Operative BP'!$P$15))","v":-2908.9237500000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E7-'Operative BP'!$P$15))","v":-2442.211875},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F7-'Operative BP'!$P$15))","v":-1642.1343749999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G7-'Operative BP'!$P$15))","v":-508.69125000000054},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H7-'Operative BP'!$P$15))","v":869.22000000000082},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I7-'Operative BP'!$P$15))","v":1469.2781250000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J7-'Operative BP'!$P$15))","v":1624.8487499999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K7-'Operative BP'!$P$15))","v":1624.8487499999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L7-'Operative BP'!$P$15))","v":913.66875000000073},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M7-'Operative BP'!$P$15))","v":-219.77437500000013},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N7-'Operative BP'!$P$15))","v":-1575.4612499999998},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O7-'Operative BP'!$P$15))","v":-2664.4556249999996},{"$f":"MIN(AS112:AZ135)","v":-1931.05125},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"IF(C35<0,C35,0)","v":-7.1634824999999994E-3},-5.0651775000000003E-3,-1.6315875000000016E-3,-1.666209060000001,0,0,0,0,0,0,-1.8223424999999972E-3,-6.0189524999999973E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D8-'Operative BP'!$P$15))","v":-3020.0456250000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E8-'Operative BP'!$P$15))","v":-2575.558125},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F8-'Operative BP'!$P$15))","v":-1753.2562500000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G8-'Operative BP'!$P$15))","v":-686.48625000000027},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H8-'Operative BP'!$P$15))","v":802.546875},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I8-'Operative BP'!$P$15))","v":1335.9318749999991},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J8-'Operative BP'!$P$15))","v":1447.0537499999998},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K8-'Operative BP'!$P$15))","v":1469.2781250000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L8-'Operative BP'!$P$15))","v":735.87374999999918},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M8-'Operative BP'!$P$15))","v":-308.671875},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N8-'Operative BP'!$P$15))","v":-1731.0318749999994},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O8-'Operative BP'!$P$15))","v":-2775.5774999999994},"Av+Max/2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,{"$f":"IF(C36<0,C36,0)","v":-7.4496149999999997E-3},-5.4466874999999993E-3,-1.9177200000000004E-3,-2.1353594400000002,0,0,0,0,0,-0.4933331100000023,-2.0130975000000008E-3,-6.0189524999999973E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D9-'Operative BP'!$P$15))","v":-3153.3918749999998},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E9-'Operative BP'!$P$15))","v":-2664.4556249999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F9-'Operative BP'!$P$15))","v":-1864.3781250000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G9-'Operative BP'!$P$15))","v":-819.8325000000001},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H9-'Operative BP'!$P$15))","v":624.75187500000027},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I9-'Operative BP'!$P$15))","v":1180.3612500000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J9-'Operative BP'!$P$15))","v":1358.15625},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K9-'Operative BP'!$P$15))","v":1335.9318749999991},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L9-'Operative BP'!$P$15))","v":646.97625000000107},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M9-'Operative BP'!$P$15))","v":-486.46687499999973},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N9-'Operative BP'!$P$15))","v":-1908.8268749999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O9-'Operative BP'!$P$15))","v":-2886.6993749999992},{"$f":"AVERAGE(BC112,BC114)","v":53.417706367924552},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,{"$f":"IF(C37<0,C37,0)","v":-7.4496149999999997E-3},-5.4466874999999993E-3,-1.9177200000000004E-3,-0.96248349000000188,0,0,0,0,0,0,-2.2038524999999998E-3,-6.2097075000000024E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D10-'Operative BP'!$P$15))","v":-3220.0649999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E10-'Operative BP'!$P$15))","v":-2753.3531249999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F10-'Operative BP'!$P$15))","v":-1931.05125},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G10-'Operative BP'!$P$15))","v":-908.7299999999999},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H10-'Operative BP'!$P$15))","v":469.18124999999964},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I10-'Operative BP'!$P$15))","v":1047.0150000000006},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J10-'Operative BP'!$P$15))","v":1269.2587500000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K10-'Operative BP'!$P$15))","v":1224.8099999999984},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L10-'Operative BP'!$P$15))","v":580.30312500000036},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M10-'Operative BP'!$P$15))","v":-597.58875000000046},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N10-'Operative BP'!$P$15))","v":-1953.275625},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O10-'Operative BP'!$P$15))","v":-2886.6993749999992},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,{"$f":"IF(C38<0,C38,0)","v":-6.2097075000000024E-3},-4.2067800000000011E-3,-4.0054274999999997,0,0,0,0,0,0,0,-3.3377850000000007,-5.3513100000000032E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D11-'Operative BP'!$P$15))","v":-3220.0649999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E11-'Operative BP'!$P$15))","v":-2753.3531249999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F11-'Operative BP'!$P$15))","v":-1931.05125},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G11-'Operative BP'!$P$15))","v":-686.48625000000027},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H11-'Operative BP'!$P$15))","v":713.64937500000019},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I11-'Operative BP'!$P$15))","v":1402.605},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J11-'Operative BP'!$P$15))","v":1602.6243750000006},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K11-'Operative BP'!$P$15))","v":1535.9512499999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L11-'Operative BP'!$P$15))","v":824.7712500000008},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M11-'Operative BP'!$P$15))","v":-486.46687499999973},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N11-'Operative BP'!$P$15))","v":-1997.724375},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O11-'Operative BP'!$P$15))","v":-2931.1481250000002},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,{"$f":"IF(C39<0,C39,0)","v":-4.779045E-3},-2.6807399999999996E-3,-2.860897500000001,0,0,0,0,0,0,0,-1.5489214649999958,-3.8252700000000017E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D12-'Operative BP'!$P$15))","v":-2931.1481250000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E12-'Operative BP'!$P$15))","v":-2464.4362500000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F12-'Operative BP'!$P$15))","v":-1553.2368749999998},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G12-'Operative BP'!$P$15))","v":-286.44749999999914},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H12-'Operative BP'!$P$15))","v":1158.1368750000013},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I12-'Operative BP'!$P$15))","v":1847.0925000000009},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J12-'Operative BP'!$P$15))","v":2047.1118750000016},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K12-'Operative BP'!$P$15))","v":2024.8875000000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L12-'Operative BP'!$P$15))","v":1380.3806250000009},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M12-'Operative BP'!$P$15))","v":2.4693749999995087},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N12-'Operative BP'!$P$15))","v":-1397.66625},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O12-'Operative BP'!$P$15))","v":-2731.1287500000008},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,{"$f":"IF(C40<0,C40,0)","v":-3.2530049999999981E-3},-4.7684474999999988,-2.2526470350000043,0,0,0,0,0,0,0,0,-2.2038524999999998E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D13-'Operative BP'!$P$15))","v":-2597.7824999999998},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E13-'Operative BP'!$P$15))","v":-2108.8462499999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F13-'Operative BP'!$P$15))","v":-1286.5443750000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G13-'Operative BP'!$P$15))","v":246.9375},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H13-'Operative BP'!$P$15))","v":1513.7268750000005},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I13-'Operative BP'!$P$15))","v":2269.3556250000011},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J13-'Operative BP'!$P$15))","v":2580.4968750000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K13-'Operative BP'!$P$15))","v":2602.7212500000014},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L13-'Operative BP'!$P$15))","v":1891.5412499999991},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M13-'Operative BP'!$P$15))","v":513.62999999999954},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N13-'Operative BP'!$P$15))","v":-797.60812499999918},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O13-'Operative BP'!$P$15))","v":-2375.5387500000002},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,{"$f":"IF(C41<0,C41,0)","v":-1.9177200000000004E-3},-2.9562749999999971,-0.61062070499999799,0,0,0,0,0,0,0,0,-4.2915599999999987,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D14-'Operative BP'!$P$15))","v":-2242.1924999999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E14-'Operative BP'!$P$15))","v":-1731.0318749999994},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F14-'Operative BP'!$P$15))","v":-930.95437500000082},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G14-'Operative BP'!$P$15))","v":669.20062500000017},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H14-'Operative BP'!$P$15))","v":1891.5412499999991},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I14-'Operative BP'!$P$15))","v":2647.1699999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J14-'Operative BP'!$P$15))","v":3047.2087500000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K14-'Operative BP'!$P$15))","v":3113.881875},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L14-'Operative BP'!$P$15))","v":2336.0287499999986},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M14-'Operative BP'!$P$15))","v":980.34187499999973},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N14-'Operative BP'!$P$15))","v":-308.671875},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O14-'Operative BP'!$P$15))","v":-1997.724375},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,{"$f":"IF(C42<0,C42,0)","v":-4.2915599999999987},-2.6045098199999992,0,0,0,0,0,0,0,0,0,-3.1470299999999969,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D15-'Operative BP'!$P$15))","v":-1931.05125},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E15-'Operative BP'!$P$15))","v":-1308.7687499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F15-'Operative BP'!$P$15))","v":-619.81312499999956},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G15-'Operative BP'!$P$15))","v":1024.7906249999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H15-'Operative BP'!$P$15))","v":2202.6825000000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I15-'Operative BP'!$P$15))","v":2980.535625},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J15-'Operative BP'!$P$15))","v":3402.7987500000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K15-'Operative BP'!$P$15))","v":3536.145},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L15-'Operative BP'!$P$15))","v":2647.1699999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M15-'Operative BP'!$P$15))","v":1358.15625},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N15-'Operative BP'!$P$15))","v":135.8156249999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O15-'Operative BP'!$P$15))","v":-1619.9099999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,{"$f":"IF(C43<0,C43,0)","v":-3.2424075000000001},-0.84519589499999759,0,0,0,0,0,0,0,0,0,-3.0736601999999986,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D16-'Operative BP'!$P$15))","v":-1619.9099999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E16-'Operative BP'!$P$15))","v":-997.62749999999983},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F16-'Operative BP'!$P$15))","v":-419.79375000000073},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G16-'Operative BP'!$P$15))","v":1291.4831250000009},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H16-'Operative BP'!$P$15))","v":2447.1506249999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I16-'Operative BP'!$P$15))","v":3269.4525000000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J16-'Operative BP'!$P$15))","v":3625.0425},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K16-'Operative BP'!$P$15))","v":3780.6131249999989},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L16-'Operative BP'!$P$15))","v":2869.4137499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M16-'Operative BP'!$P$15))","v":1669.2974999999994},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N16-'Operative BP'!$P$15))","v":446.95687500000054},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O16-'Operative BP'!$P$15))","v":-1353.2174999999993},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,{"$f":"IF(C44<0,C44,0)","v":-3.5428105799999976},0,0,0,0,0,0,0,0,0,0,-2.1353594400000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D17-'Operative BP'!$P$15))","v":-1375.441875},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E17-'Operative BP'!$P$15))","v":-664.26187499999946},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F17-'Operative BP'!$P$15))","v":24.69375000000035},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G17-'Operative BP'!$P$15))","v":1447.0537499999998},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H17-'Operative BP'!$P$15))","v":2691.6187499999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I17-'Operative BP'!$P$15))","v":3425.0231249999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J17-'Operative BP'!$P$15))","v":3802.8374999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K17-'Operative BP'!$P$15))","v":4025.0812499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L17-'Operative BP'!$P$15))","v":3091.6574999999989},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M17-'Operative BP'!$P$15))","v":1891.5412499999991},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N17-'Operative BP'!$P$15))","v":713.64937500000019},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O17-'Operative BP'!$P$15))","v":-1086.5249999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,{"$f":"IF(C45<0,C45,0)","v":-3.1909477950000027},0,0,0,0,0,0,0,0,0,0,-1.666209060000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D18-'Operative BP'!$P$15))","v":-1175.4224999999994},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E18-'Operative BP'!$P$15))","v":-419.79375000000073},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F18-'Operative BP'!$P$15))","v":224.71312499999917},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G18-'Operative BP'!$P$15))","v":1624.8487499999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H18-'Operative BP'!$P$15))","v":2869.4137499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I18-'Operative BP'!$P$15))","v":3691.7156250000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J18-'Operative BP'!$P$15))","v":4002.8568749999986},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K18-'Operative BP'!$P$15))","v":4136.203125},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L18-'Operative BP'!$P$15))","v":3225.0037499999989},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M18-'Operative BP'!$P$15))","v":2069.3362500000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N18-'Operative BP'!$P$15))","v":824.7712500000008},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O18-'Operative BP'!$P$15))","v":-908.7299999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,{"$f":"IF(C46<0,C46,0)","v":-3.0736601999999986},0,0,0,0,0,0,0,0,0,0,-2.1353594400000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D19-'Operative BP'!$P$15))","v":-1108.7493750000006},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E19-'Operative BP'!$P$15))","v":-286.44749999999914},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F19-'Operative BP'!$P$15))","v":358.05937500000073},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G19-'Operative BP'!$P$15))","v":1735.9706250000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H19-'Operative BP'!$P$15))","v":2913.8624999999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I19-'Operative BP'!$P$15))","v":3780.6131249999989},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J19-'Operative BP'!$P$15))","v":4113.9787499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K19-'Operative BP'!$P$15))","v":4180.6518749999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L19-'Operative BP'!$P$15))","v":3313.9012500000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M19-'Operative BP'!$P$15))","v":2180.4581249999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N19-'Operative BP'!$P$15))","v":980.34187499999973},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O19-'Operative BP'!$P$15))","v":-819.8325000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,{"$f":"IF(C47<0,C47,0)","v":-3.7773857699999973},-2.4182730000003174E-2,0,0,0,0,0,0,0,0,0,-3.4255229850000033,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D20-'Operative BP'!$P$15))","v":-1086.5249999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E20-'Operative BP'!$P$15))","v":-330.89625000000086},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F20-'Operative BP'!$P$15))","v":402.50812499999887},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G20-'Operative BP'!$P$15))","v":1647.0731250000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H20-'Operative BP'!$P$15))","v":2936.086875},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I20-'Operative BP'!$P$15))","v":3802.8374999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J20-'Operative BP'!$P$15))","v":4091.754375},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K20-'Operative BP'!$P$15))","v":4113.9787499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L20-'Operative BP'!$P$15))","v":3291.6768749999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M20-'Operative BP'!$P$15))","v":2113.7849999999989},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N20-'Operative BP'!$P$15))","v":869.22000000000082},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O20-'Operative BP'!$P$15))","v":-908.7299999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,{"$f":"IF(C48<0,C48,0)","v":-3.52854},-1.1970586800000018,0,0,0,0,0,0,0,0,0,-2.9562749999999971,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D21-'Operative BP'!$P$15))","v":-1219.8712499999995},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E21-'Operative BP'!$P$15))","v":-508.69125000000054},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F21-'Operative BP'!$P$15))","v":269.16187500000086},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G21-'Operative BP'!$P$15))","v":1447.0537499999998},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H21-'Operative BP'!$P$15))","v":2913.8624999999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I21-'Operative BP'!$P$15))","v":3713.9400000000014},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J21-'Operative BP'!$P$15))","v":4025.0812499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K21-'Operative BP'!$P$15))","v":3958.4081250000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L21-'Operative BP'!$P$15))","v":3113.881875},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M21-'Operative BP'!$P$15))","v":1980.4387499999991},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N21-'Operative BP'!$P$15))","v":669.20062500000017},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O21-'Operative BP'!$P$15))","v":-1153.1981250000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,{"$f":"IF(C49<0,C49,0)","v":-4.4823150000000025},-2.3699346299999999,0,0,0,0,0,0,0,0,0,-4.2915599999999987,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D22-'Operative BP'!$P$15))","v":-1442.115},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E22-'Operative BP'!$P$15))","v":-730.93500000000017},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F22-'Operative BP'!$P$15))","v":113.59125000000022},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G22-'Operative BP'!$P$15))","v":1269.2587500000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H22-'Operative BP'!$P$15))","v":2758.2918750000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I22-'Operative BP'!$P$15))","v":3602.8181250000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J22-'Operative BP'!$P$15))","v":3847.2862499999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K22-'Operative BP'!$P$15))","v":3758.3887499999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L22-'Operative BP'!$P$15))","v":2980.535625},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M22-'Operative BP'!$P$15))","v":1802.6437499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N22-'Operative BP'!$P$15))","v":358.05937500000073},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O22-'Operative BP'!$P$15))","v":-1308.7687499999993},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,{"$f":"IF(C50<0,C50,0)","v":-1.8223424999999972E-3},-2.6701425000000016,0,0,0,0,0,0,0,0,0,-5.2453350000000007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D23-'Operative BP'!$P$15))","v":-1664.3587500000006},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E23-'Operative BP'!$P$15))","v":-953.17874999999981},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F23-'Operative BP'!$P$15))","v":-86.42812500000035},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G23-'Operative BP'!$P$15))","v":958.11749999999893},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H23-'Operative BP'!$P$15))","v":2558.2725},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I23-'Operative BP'!$P$15))","v":3358.3500000000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J23-'Operative BP'!$P$15))","v":3536.145},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K23-'Operative BP'!$P$15))","v":3469.4718749999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L23-'Operative BP'!$P$15))","v":2758.2918750000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M23-'Operative BP'!$P$15))","v":1558.1756249999987},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N23-'Operative BP'!$P$15))","v":113.59125000000022},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O23-'Operative BP'!$P$15))","v":-1619.9099999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,{"$f":"IF(C51<0,C51,0)","v":-2.4899849999999997E-3},-3.6239175000000006,-0.37604551499999844,0,0,0,0,0,0,0,0,-2.2038524999999998E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D24-'Operative BP'!$P$15))","v":-1908.8268749999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E24-'Operative BP'!$P$15))","v":-1242.0956250000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F24-'Operative BP'!$P$15))","v":-397.56937499999987},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G24-'Operative BP'!$P$15))","v":758.0981250000001},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H24-'Operative BP'!$P$15))","v":2269.3556250000011},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I24-'Operative BP'!$P$15))","v":3047.2087500000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J24-'Operative BP'!$P$15))","v":3091.6574999999989},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K24-'Operative BP'!$P$15))","v":3113.881875},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L24-'Operative BP'!$P$15))","v":2469.375},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M24-'Operative BP'!$P$15))","v":1180.3612500000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N24-'Operative BP'!$P$15))","v":-197.5499999999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O24-'Operative BP'!$P$15))","v":-1842.1537500000002},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,{"$f":"IF(C52<0,C52,0)","v":-3.2530049999999981E-3},-4.5776924999999986,-1.4316338700000015,0,0,0,0,0,0,0,-0.72790830000000228,-2.8714949999999991E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D25-'Operative BP'!$P$15))","v":-2064.3975},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E25-'Operative BP'!$P$15))","v":-1464.339375},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F25-'Operative BP'!$P$15))","v":-575.36437499999954},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G25-'Operative BP'!$P$15))","v":558.07874999999956},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H25-'Operative BP'!$P$15))","v":2024.8875000000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I25-'Operative BP'!$P$15))","v":2713.8431250000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J25-'Operative BP'!$P$15))","v":2736.0674999999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K25-'Operative BP'!$P$15))","v":2869.4137499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L25-'Operative BP'!$P$15))","v":2158.2337500000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M25-'Operative BP'!$P$15))","v":935.89312499999983},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N25-'Operative BP'!$P$15))","v":-397.56937499999987},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O25-'Operative BP'!$P$15))","v":-1997.724375},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,{"$f":"IF(C53<0,C53,0)","v":-3.9206475000000008E-3},-1.6315875000000016E-3,-2.3699346299999999,0,0,0,0,0,0,0,-2.018071845000005,-3.3483825000000023E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D26-'Operative BP'!$P$15))","v":-2242.1924999999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E26-'Operative BP'!$P$15))","v":-1686.5831249999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F26-'Operative BP'!$P$15))","v":-775.38375000000019},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G26-'Operative BP'!$P$15))","v":358.05937500000073},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H26-'Operative BP'!$P$15))","v":1802.6437499999993},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I26-'Operative BP'!$P$15))","v":2424.92625},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J26-'Operative BP'!$P$15))","v":2402.7018750000011},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K26-'Operative BP'!$P$15))","v":2624.9456250000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L26-'Operative BP'!$P$15))","v":1935.9900000000009},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M26-'Operative BP'!$P$15))","v":691.42499999999927},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N26-'Operative BP'!$P$15))","v":-642.03750000000036},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O26-'Operative BP'!$P$15))","v":-2153.2949999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,{"$f":"IF(C54<0,C54,0)","v":-4.3975350000000002E-3},-2.4899849999999997E-3,-3.3082353899999979,0,0,0,0,0,0,0,-2.8390850099999989,-4.2067800000000011E-3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D27-'Operative BP'!$P$15))","v":-2397.7631250000004},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E27-'Operative BP'!$P$15))","v":-1864.3781250000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F27-'Operative BP'!$P$15))","v":-953.17874999999981},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G27-'Operative BP'!$P$15))","v":91.36687500000113},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H27-'Operative BP'!$P$15))","v":1580.3999999999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I27-'Operative BP'!$P$15))","v":2202.6825000000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J27-'Operative BP'!$P$15))","v":2224.9068749999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K27-'Operative BP'!$P$15))","v":2424.92625},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L27-'Operative BP'!$P$15))","v":1713.7462500000013},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M27-'Operative BP'!$P$15))","v":491.4056250000005},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N27-'Operative BP'!$P$15))","v":-886.5056250000008},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O27-'Operative BP'!$P$15))","v":-2264.4168750000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,{"$f":"SUM(C111:C134)","v":-29.207617604999999},{"$f":"SUM(D111:D134)","v":-25.679625479999999},-33.242619172500014,-5.7507182100000085,0,0,0,0,0,-0.4933331100000023,-26.557611682499999,-32.429722747500001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,{"$f":"('Input Data'!$E$53*('Dry Bulb'!D28-'Operative BP'!$P$15))","v":-2508.8850000000002},{"$f":"('Input Data'!$E$53*('Dry Bulb'!E28-'Operative BP'!$P$15))","v":-2064.3975},{"$f":"('Input Data'!$E$53*('Dry Bulb'!F28-'Operative BP'!$P$15))","v":-1130.9737499999997},{"$f":"('Input Data'!$E$53*('Dry Bulb'!G28-'Operative BP'!$P$15))","v":-86.42812500000035},{"$f":"('Input Data'!$E$53*('Dry Bulb'!H28-'Operative BP'!$P$15))","v":1380.3806250000009},{"$f":"('Input Data'!$E$53*('Dry Bulb'!I28-'Operative BP'!$P$15))","v":1980.4387499999991},{"$f":"('Input Data'!$E$53*('Dry Bulb'!J28-'Operative BP'!$P$15))","v":2069.3362500000007},{"$f":"('Input Data'!$E$53*('Dry Bulb'!K28-'Operative BP'!$P$15))","v":2202.6825000000003},{"$f":"('Input Data'!$E$53*('Dry Bulb'!L28-'Operative BP'!$P$15))","v":1513.7268750000005},{"$f":"('Input Data'!$E$53*('Dry Bulb'!M28-'Operative BP'!$P$15))","v":313.61062500000077},{"$f":"('Input Data'!$E$53*('Dry Bulb'!N28-'Operative BP'!$P$15))","v":-1042.0762499999996},{"$f":"('Input Data'!$E$53*('Dry Bulb'!O28-'Operative BP'!$P$15))","v":-2464.4362500000002},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"Cooling Load",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,{"$f":"B111","v":1},{"$f":"IF(C31>0,C31,0)","v":0},{"$f":"IF(D31>0,D31,0)","v":0},0,1.3832684100000037,7.7260050000000007,10.396574999999997,11.064217499999998,11.350350000000002,8.3936474999999948,3.3771575249999959,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,{"$f":"B112","v":2},{"$f":"IF(C32>0,C32,0)","v":0},0,0,0.67954283999999554,6.9629850000000024,9.4428000000000001,10.205819999999996,10.4919525,7.4398724999999981,2.556144360000002,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"IF(C33>0,C33,0)","v":0},0,0,0,6.3907200000000026,8.9659125000000017,9.6335549999999959,9.6335549999999959,6.581475000000002,1.5005560049999991,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"IF(C34>0,C34,0)","v":0},0,0,0,6.1045875000000001,8.3936474999999948,8.8705350000000003,8.9659125000000017,5.8184549999999966,1.0314056249999997,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"IF(C35>0,C35,0)","v":0},0,0,0,5.3415675000000009,7.7260050000000007,8.4890249999999998,8.3936474999999948,5.4369450000000041,9.3104865000001161E-2,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,{"$f":"IF(C36>0,C36,0)","v":0},0,0,0,5.1364714499999975,7.1537400000000018,8.1075150000000011,7.9167599999999929,5.7229094250000019,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,{"$f":"IF(C37>0,C37,0)","v":0},0,0,0,5.7230775000000005,8.6797799999999992,9.5381775000000015,9.252044999999999,6.1999650000000042,9.3104865000001161E-2,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,{"$f":"IF(C38>0,C38,0)","v":0},0,0,1.1486932200000042,7.6306275000000054,10.587330000000003,11.445727500000006,11.350350000000002,8.584402500000003,2.6734319549999968,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,{"$f":"IF(C39>0,C39,0)","v":0},0,0,3.9635954999999994,9.1566675000000028,12.399502500000004,13.734787500000003,13.830165000000006,10.778084999999995,5.3710466399999977,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,{"$f":"IF(C40>0,C40,0)","v":0},0,0,5.5323225000000003,10.778084999999995,14.020919999999998,15.737715000000003,16.023847499999999,12.685634999999992,6.8676074999999983,1.0314056249999997,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,{"$f":"IF(C41>0,C41,0)","v":0},0,0,7.0583624999999985,12.113370000000002,15.451582500000001,17.263755,17.836020000000001,14.020919999999998,8.4890249999999998,3.3771575249999959,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,{"$f":"IF(C42>0,C42,0)","v":0},0,0.44496764999999594,8.2028925000000044,13.162522499999996,16.691490000000002,18.21753,18.885172499999992,14.974694999999995,9.824309999999997,5.0191838550000032,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,{"$f":"IF(C43>0,C43,0)","v":0},0,2.7907195500000017,8.8705350000000003,14.211674999999998,17.359132499999998,18.980549999999997,19.934324999999998,15.928469999999995,10.778084999999995,5.7230775000000005,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,{"$f":"IF(C44>0,C44,0)","v":0},0.44496764999999594,3.8463079049999953,9.6335549999999959,14.974694999999995,18.503662500000001,19.838947499999996,20.411212500000001,16.500734999999992,11.541105000000003,6.1999650000000042,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,{"$f":"IF(C45>0,C45,0)","v":0},1.1486932200000042,4.5500334750000038,10.110442500000001,15.165449999999996,18.885172499999992,20.315835,20.601967499999997,16.882245000000001,12.017992499999998,6.8676074999999983,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,{"$f":"IF(C46>0,C46,0)","v":0},0.91411802999999514,4.7846086649999942,9.7289325000000026,15.2608275,18.980549999999997,20.220457499999998,20.315835,16.7868675,11.731859999999996,6.3907200000000026,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,{"$f":"IF(C47>0,C47,0)","v":0},0,4.0808830950000043,8.8705350000000003,15.165449999999996,18.599040000000009,19.934324999999998,19.648192499999997,16.023847499999999,11.159594999999996,5.5323225000000003,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,{"$f":"IF(C48>0,C48,0)","v":0},0,3.2598699300000007,8.1075150000000011,14.4978075,18.122152500000002,19.171305,18.789794999999998,15.451582500000001,10.396574999999997,4.5500334750000038,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,{"$f":"IF(C49>0,C49,0)","v":0},0,2.2042815749999978,6.7722299999999951,13.63941,17.073,17.836020000000001,17.549887499999997,14.4978075,9.3474224999999933,3.2598699300000007,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,{"$f":"IF(C50>0,C50,0)","v":0},0,0.56225524500000024,5.9138325000000007,12.399502500000004,15.737715000000003,15.928469999999995,16.023847499999999,13.257899999999999,7.7260050000000007,1.6178436000000034,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,{"$f":"IF(C51>0,C51,0)","v":0},0,0,5.6056218299999969,11.350350000000002,14.307052500000001,14.402429999999999,14.974694999999995,11.922615000000002,6.676852499999999,0.56225524500000024,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,{"$f":"IF(C52>0,C52,0)","v":0},0,0,4.5500334750000038,10.396574999999997,13.067145,12.971767500000004,13.925542500000002,10.968840000000004,5.6276999999999973,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,{"$f":"IF(C53>0,C53,0)","v":0},0,0,3.1425823350000055,9.4428000000000001,12.113370000000002,12.208747499999998,13.067145,10.015065000000005,5.2537590450000025,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,{"$f":"IF(C54>0,C54,0)","v":0},0,0,2.2042815749999978,8.584402500000003,11.159594999999996,11.541105000000003,12.113370000000002,9.1566675000000028,4.3154582850000045,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,{"$f":"SUM(C137:C160)","v":0},2.5077788999999955,26.52392708999999,111.47877418500001,251.31563144999998,323.81687249999993,345.65832000000006,351.28559249999995,274.029649425,148.44930417,50.131441755000012,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($AH$29<DEGREES(BS161),0+$AJ$33,1-((TAN(BS161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BT161),0+$AJ$33,1-((TAN(BT161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BU161),0+$AJ$33,1-((TAN(BU161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BV161),0+$AJ$33,1-((TAN(BV161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BW161),0+$AJ$33,1-((TAN(BW161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BX161),0+$AJ$33,1-((TAN(BX161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BY161),0+$AJ$33,1-((TAN(BY161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BZ161),0+$AJ$33,1-((TAN(BZ161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CA161),0+$AJ$33,1-((TAN(CA161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CB161),0+$AJ$33,1-((TAN(CB161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CC161),0+$AJ$33,1-((TAN(CC161)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CD161),0+$AJ$33,1-((TAN(CD161)/TAN($AG$31))*(1-$AJ$16)))","v":1}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"HDD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,{"$f":"B5","v":1},{"$f":"IF(C5<0,C5,0)","v":-10.0991932059448},{"$f":"IF(D5<0,D5,0)","v":-5.5991932059448004},-5.759193205944797,0,0,0,0,0,0,0,-7.1288242887473388,-8.1191932059447964,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,2,{"$f":"IF(C6<0,C6,0)","v":-10.999193205944799},-6.6791932059447987,-7.0191932059448021,0,0,0,0,0,0,0,-6.4791932059447959,-8.8391932059447953,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"IF(C7<0,C7,0)","v":-11.539193205944798},-7.759193205944797,-8.279193205944793,-4.5638556263270402E-2,0,0,0,0,0,0,-7.7391932059447939,-9.5591932059447942,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"IF(C8<0,C8,0)","v":-12.439193205944797},-8.8391932059447953,-9.1791932059447987,-1.816434989384291,0,0,0,0,0,0,-8.9991932059447919,-10.459193205944793,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"IF(C9<0,C9,0)","v":-13.519193205944795},-9.5591932059447942,-3.0791932059447973,-3.1445323142250601,0,0,0,0,0,0,-3.4391932059447896,-11.359193205944791,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,{"$f":"IF(C10<0,C10,0)","v":-14.059193205944794},-10.279193205944793,-3.6191932059447964,-3.8689656717563565,0,0,0,0,0,-0.93103677282378783,-3.7991932059447961,-11.359193205944791,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,{"$f":"IF(C11<0,C11,0)","v":-13.936714294401561},-9.9670313369964703,-2.7185967790058072,0,0,0,0,0,0,0,-3.715788720614789,-11.534452031025396,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,{"$f":"IF(C12<0,C12,0)","v":-9.3760122870067448},-4.9568521148914542,-3.2671314893503762,0,0,0,0,0,0,0,-2.6644106943546788,-7.6300752560144502,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,{"$f":"IF(C13<0,C13,0)","v":-3.8307478163317086},-0.26975203807860737,0,0,0,0,0,0,0,0,0,-2.784971452619736,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,{"$f":"IF(C14<0,C14,0)","v":-1.0620454725222359},-5.579009996875584,-1.8750275213188132,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,{"$f":"IF(C15<0,C15,0)","v":0},-5.1145703587918234,-1.1523863269639065,0,0,0,0,0,0,0,0,-3.4765389620963063,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,{"$f":"IF(C16<0,C16,0)","v":-3.0776873526078887},-4.6700025913142156,0,0,0,0,0,0,0,0,0,-0.16028998863284016,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,{"$f":"IF(C17<0,C17,0)","v":-1.3064106796794448},-1.284294053726569,0,0,0,0,0,0,0,0,0,-0.50477575186765478,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,{"$f":"IF(C18<0,C18,0)","v":-2.7774307486705965},0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,{"$f":"IF(C19<0,C19,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,{"$f":"IF(C20<0,C20,0)","v":0},0,0,0,0,0,0,0,0,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,{"$f":"IF(C21<0,C21,0)","v":-4.125820757135898},0,0,0,0,0,0,0,0,0,0,-4.927182095724433,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,{"$f":"IF(C22<0,C22,0)","v":-6.6591932059447956},-1.4614304937629612,0,0,0,0,0,0,0,0,0,-5.5791932059447902,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,{"$f":"IF(C23<0,C23,0)","v":-8.4591932059447998},-4.4726296390658149,0,0,0,0,0,0,0,0,0,-8.0991932059447933,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,{"$f":"IF(C24<0,C24,0)","v":-3.4391932059447896},-5.0391932059447981,0,0,0,0,0,0,0,0,0,-9.8991932059447976,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,{"$f":"IF(C25<0,C25,0)","v":-4.6991932059447947},-6.8391932059447953,-0.70968721868365492,0,0,0,0,0,0,0,0,-4.1591932059447956,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,{"$f":"IF(C26<0,C26,0)","v":-6.1391932059447925},-8.6391932059447925,-2.7018332059447943,0,0,0,0,0,0,0,-1.3737358811040394,-5.4191932059447936,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,{"$f":"IF(C27<0,C27,0)","v":-7.3991932059447976},-3.0791932059447973,-4.4726296390658149,0,0,0,0,0,0,0,-3.8085809766454446,-6.3191932059447993,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,{"$f":"IF(C28<0,C28,0)","v":-8.2991932059447961},-4.6991932059447947,-6.2434260721868355,0,0,0,0,0,0,0,-5.3580278556263181,-7.9391932059447967,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"CDD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,{"$f":"B5","v":1},{"$f":"IF(C5>0,C5,0)","v":0},{"$f":"IF(D5>0,D5,0)","v":0},0,2.6105560934182677,14.580806794055206,19.620806794055198,20.880806794055204,21.42080679405521,15.840806794055197,6.3734985138004134,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,{"$f":"B6","v":2},{"$f":"IF(C6>0,C6,0)","v":0},0,0,1.2824587685774844,13.140806794055209,17.820806794055201,19.260806794055199,19.800806794055205,14.0408067940552,4.8240516348195399,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"IF(C7>0,C7,0)","v":0},0,0,0,12.06080679405521,16.92080679405521,18.180806794055201,18.180806794055201,12.42080679405521,2.8319056475583864,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"IF(C8>0,C8,0)","v":0},0,0,0,11.520806794055204,15.840806794055197,16.740806794055203,16.92080679405521,10.980806794055198,1.9465074309978831,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"IF(C9>0,C9,0)","v":0},0,0,0,10.080806794055206,14.580806794055206,16.020806794055204,15.840806794055197,10.260806794055213,0.17571099787686251,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,{"$f":"IF(C10>0,C10,0)","v":0},0,0,0,10.07126610262651,13.951274327024777,15.586836445569872,15.102136505591019,10.893107961765551,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,{"$f":"IF(C11>0,C11,0)","v":0},0,0,0.88270589625417983,14.242243678705819,20.09454451669167,21.082721318187694,20.221327665047767,14.026273001460723,1.660432757975002,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,{"$f":"IF(C12>0,C12,0)","v":0},0,0,8.6789458666020209,20.874199895431076,26.820958513092975,28.217556789967638,28.406358852135043,22.326637148825441,9.9314300110390832,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,{"$f":"IF(C13>0,C13,0)","v":0},0,9.6470537321067695E-2,13.822149310167518,23.320892336433516,29.823511787142095,32.94307428804386,33.321540665395574,26.671003272848608,15.775618718326349,2.9265763640708542,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,{"$f":"IF(C14>0,C14,0)","v":0},0,0,10.624946014897731,20.340806794055197,26.460806794055202,29.71671203781635,31.097918362343563,24.7590317353541,14.382010572980278,6.5285091644646798,0.25721240810639046,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,{"$f":"IF(C15>0,C15,0)","v":0.41408205805853981},0,0,13.320806794055201,22.860806794055208,29.160806794055205,32.580806794055206,33.660806794055205,26.460806794055202,16.50128449199542,11.408652454865532,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,{"$f":"IF(C16>0,C16,0)","v":0},0,0.83975966029723281,15.480806794055212,24.840806794055197,31.500806794055208,34.380806794055204,35.640806794055194,28.260806794055199,18.917013787418355,15.493334806657664,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,{"$f":"IF(C17>0,C17,0)","v":0},0,5.2667507430997915,16.740806794055203,26.820806794055201,32.760806794055199,35.820806794055201,37.620806794055198,30.060806794055196,20.936316334744191,15.863155342714606,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,{"$f":"IF(C18>0,C18,0)","v":0},1.4548688385635273,7.2588967303609309,18.180806794055201,28.260806794055199,34.92080679405521,37.440806794055192,38.520806794055204,31.140806794055194,23.94399228783395,16.992852059193339,0.62234493588297823,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,{"$f":"IF(C19>0,C19,0)","v":0.35512307902079954},7.1260810020663286,13.560941348088789,24.251132033854844,33.601620308891569,39.167821636698591,41.77034906841476,44.425658256218824,39.265856228707847,30.459137567668073,20.6477190729684,3.2907824743424499,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,{"$f":"IF(C20>0,C20,0)","v":0.78250340796105888},8.7927944731777217,17.421879189978,27.371129784225417,38.182931614717511,44.885261648601478,47.463228199839584,48.951593394860623,41.476432867337543,29.807615510285167,17.669033337455303,1.3579624257894238,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,{"$f":"IF(C21>0,C21,0)","v":0},4.96556626571099,14.288511634407705,23.497572329604509,35.886611243523717,43.003262582788011,45.721376014699835,45.428518850943099,36.791069050599617,24.61039959111713,11.753336278240326,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,{"$f":"IF(C22>0,C22,0)","v":0},0,7.6994727408267352,17.237348584658079,30.024030571357756,37.744465322205926,39.77232756708338,38.367333398043229,29.160806794055205,19.620806794055198,8.5869940552016999,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,{"$f":"IF(C23>0,C23,0)","v":0},0,4.1600029723991412,12.780806794055195,25.740806794055203,32.220806794055207,33.660806794055205,33.120806794055198,27.360806794055208,17.640806794055194,6.1521489596602947,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,{"$f":"IF(C24>0,C24,0)","v":0},0,1.0611092144373657,11.160806794055205,23.400806794055214,29.700806794055211,30.060806794055196,30.240806794055203,25.020806794055204,14.580806794055206,3.0532552016985193,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,{"$f":"IF(C25>0,C25,0)","v":0},{"$f":"IF(D25>0,D25,0)","v":0},0,10.579140042462839,21.42080679405521,27.000806794055208,27.180806794055201,28.260806794055199,22.500806794055208,12.600806794055202,1.0611092144373657,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,{"$f":"IF(C26>0,C26,0)","v":0},0,0,8.5869940552016999,19.620806794055198,24.660806794055205,24.480806794055212,26.280806794055209,20.700806794055211,10.620806794055198,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,{"$f":"IF(C27>0,C27,0)","v":0},0,0,5.930799405520176,17.820806794055201,22.860806794055208,23.0408067940552,24.660806794055205,18.900806794055214,9.9150913800424689,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,{"$f":"IF(C28>0,C28,0)","v":0},{"$f":"IF(D28>0,D28,0)","v":0},0,4.1600029723991412,16.200806794055211,21.060806794055196,21.780806794055209,22.860806794055208,17.280806794055209,8.1442949469214483,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"Balance Point Temperature",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,1,{"$f":"IF('Dry Bulb'!D5<60,$T$15-(((C58)+('Heat gain from airflow'!Q4)+((Occupancy!P4*'Input Data'!$F$47)+(Occupancy!B4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C58)+('Heat gain from airflow'!Q4)+((Occupancy!P4*'Input Data'!$F$47)+(Occupancy!B4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E5<60,$T$15-(((D58)+('Heat gain from airflow'!R4)+((Occupancy!Q4*'Input Data'!$F$47)+(Occupancy!C4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D58)+('Heat gain from airflow'!R4)+((Occupancy!Q4*'Input Data'!$F$47)+(Occupancy!C4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!F5<60,$T$15-(((E58)+('Heat gain from airflow'!S4)+((Occupancy!R4*'Input Data'!$F$47)+(Occupancy!D4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E58)+('Heat gain from airflow'!S4)+((Occupancy!R4*'Input Data'!$F$47)+(Occupancy!D4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!G5<60,$T$15-(((F58)+('Heat gain from airflow'!T4)+((Occupancy!S4*'Input Data'!$F$47)+(Occupancy!E4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F58)+('Heat gain from airflow'!T4)+((Occupancy!S4*'Input Data'!$F$47)+(Occupancy!E4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.429443906581739},{"$f":"IF('Dry Bulb'!H5<60,$T$15-(((G58)+('Heat gain from airflow'!U4)+((Occupancy!T4*'Input Data'!$F$47)+(Occupancy!F4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G58)+('Heat gain from airflow'!U4)+((Occupancy!T4*'Input Data'!$F$47)+(Occupancy!F4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I5<60,$T$15-(((H58)+('Heat gain from airflow'!V4)+((Occupancy!U4*'Input Data'!$F$47)+(Occupancy!G4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H58)+('Heat gain from airflow'!V4)+((Occupancy!U4*'Input Data'!$F$47)+(Occupancy!G4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J5<60,$T$15-(((I58)+('Heat gain from airflow'!W4)+((Occupancy!V4*'Input Data'!$F$47)+(Occupancy!H4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I58)+('Heat gain from airflow'!W4)+((Occupancy!V4*'Input Data'!$F$47)+(Occupancy!H4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K5<60,$T$15-(((J58)+('Heat gain from airflow'!X4)+((Occupancy!W4*'Input Data'!$F$47)+(Occupancy!I4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J58)+('Heat gain from airflow'!X4)+((Occupancy!W4*'Input Data'!$F$47)+(Occupancy!I4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L5<60,$T$15-(((K58)+('Heat gain from airflow'!Y4)+((Occupancy!X4*'Input Data'!$F$47)+(Occupancy!J4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K58)+('Heat gain from airflow'!Y4)+((Occupancy!X4*'Input Data'!$F$47)+(Occupancy!J4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M5<60,$T$15-(((L58)+('Heat gain from airflow'!Z4)+((Occupancy!Y4*'Input Data'!$F$47)+(Occupancy!K4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L58)+('Heat gain from airflow'!Z4)+((Occupancy!Y4*'Input Data'!$F$47)+(Occupancy!K4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.726501486199581},{"$f":"IF('Dry Bulb'!N5<60,$T$15-(((M58)+('Heat gain from airflow'!AA4)+((Occupancy!Z4*'Input Data'!$F$47)+(Occupancy!L4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M58)+('Heat gain from airflow'!AA4)+((Occupancy!Z4*'Input Data'!$F$47)+(Occupancy!L4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":72.248824288747343},{"$f":"IF('Dry Bulb'!O5<60,$T$15-(((N58)+('Heat gain from airflow'!AB4)+((Occupancy!AA4*'Input Data'!$F$47)+(Occupancy!M4*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N58)+('Heat gain from airflow'!AB4)+((Occupancy!AA4*'Input Data'!$F$47)+(Occupancy!M4*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,2,{"$f":"IF('Dry Bulb'!D6<60,$T$15-(((C59)+('Heat gain from airflow'!Q5)+((Occupancy!P5*'Input Data'!$F$47)+(Occupancy!B5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C59)+('Heat gain from airflow'!Q5)+((Occupancy!P5*'Input Data'!$F$47)+(Occupancy!B5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E6<60,$T$15-(((D59)+('Heat gain from airflow'!R5)+((Occupancy!Q5*'Input Data'!$F$47)+(Occupancy!C5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D59)+('Heat gain from airflow'!R5)+((Occupancy!Q5*'Input Data'!$F$47)+(Occupancy!C5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!F6<60,$T$15-(((E59)+('Heat gain from airflow'!S5)+((Occupancy!R5*'Input Data'!$F$47)+(Occupancy!D5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E59)+('Heat gain from airflow'!S5)+((Occupancy!R5*'Input Data'!$F$47)+(Occupancy!D5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!G6<60,$T$15-(((F59)+('Heat gain from airflow'!T5)+((Occupancy!S5*'Input Data'!$F$47)+(Occupancy!E5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F59)+('Heat gain from airflow'!T5)+((Occupancy!S5*'Input Data'!$F$47)+(Occupancy!E5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.677541231422509},{"$f":"IF('Dry Bulb'!H6<60,$T$15-(((G59)+('Heat gain from airflow'!U5)+((Occupancy!T5*'Input Data'!$F$47)+(Occupancy!F5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G59)+('Heat gain from airflow'!U5)+((Occupancy!T5*'Input Data'!$F$47)+(Occupancy!F5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I6<60,$T$15-(((H59)+('Heat gain from airflow'!V5)+((Occupancy!U5*'Input Data'!$F$47)+(Occupancy!G5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H59)+('Heat gain from airflow'!V5)+((Occupancy!U5*'Input Data'!$F$47)+(Occupancy!G5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J6<60,$T$15-(((I59)+('Heat gain from airflow'!W5)+((Occupancy!V5*'Input Data'!$F$47)+(Occupancy!H5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I59)+('Heat gain from airflow'!W5)+((Occupancy!V5*'Input Data'!$F$47)+(Occupancy!H5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K6<60,$T$15-(((J59)+('Heat gain from airflow'!X5)+((Occupancy!W5*'Input Data'!$F$47)+(Occupancy!I5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J59)+('Heat gain from airflow'!X5)+((Occupancy!W5*'Input Data'!$F$47)+(Occupancy!I5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L6<60,$T$15-(((K59)+('Heat gain from airflow'!Y5)+((Occupancy!X5*'Input Data'!$F$47)+(Occupancy!J5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K59)+('Heat gain from airflow'!Y5)+((Occupancy!X5*'Input Data'!$F$47)+(Occupancy!J5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M6<60,$T$15-(((L59)+('Heat gain from airflow'!Z5)+((Occupancy!Y5*'Input Data'!$F$47)+(Occupancy!K5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L59)+('Heat gain from airflow'!Z5)+((Occupancy!Y5*'Input Data'!$F$47)+(Occupancy!K5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.015948365180463},{"$f":"IF('Dry Bulb'!N6<60,$T$15-(((M59)+('Heat gain from airflow'!AA5)+((Occupancy!Z5*'Input Data'!$F$47)+(Occupancy!L5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M59)+('Heat gain from airflow'!AA5)+((Occupancy!Z5*'Input Data'!$F$47)+(Occupancy!L5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!O6<60,$T$15-(((N59)+('Heat gain from airflow'!AB5)+((Occupancy!AA5*'Input Data'!$F$47)+(Occupancy!M5*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N59)+('Heat gain from airflow'!AB5)+((Occupancy!AA5*'Input Data'!$F$47)+(Occupancy!M5*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"IF('Dry Bulb'!D7<60,$T$15-(((C60)+('Heat gain from airflow'!Q6)+((Occupancy!P6*'Input Data'!$F$47)+(Occupancy!B6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C60)+('Heat gain from airflow'!Q6)+((Occupancy!P6*'Input Data'!$F$47)+(Occupancy!B6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E7<60,$T$15-(((D60)+('Heat gain from airflow'!R6)+((Occupancy!Q6*'Input Data'!$F$47)+(Occupancy!C6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D60)+('Heat gain from airflow'!R6)+((Occupancy!Q6*'Input Data'!$F$47)+(Occupancy!C6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!F7<60,$T$15-(((E60)+('Heat gain from airflow'!S6)+((Occupancy!R6*'Input Data'!$F$47)+(Occupancy!D6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E60)+('Heat gain from airflow'!S6)+((Occupancy!R6*'Input Data'!$F$47)+(Occupancy!D6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!G7<60,$T$15-(((F60)+('Heat gain from airflow'!T6)+((Occupancy!S6*'Input Data'!$F$47)+(Occupancy!E6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F60)+('Heat gain from airflow'!T6)+((Occupancy!S6*'Input Data'!$F$47)+(Occupancy!E6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.925638556263266},{"$f":"IF('Dry Bulb'!H7<60,$T$15-(((G60)+('Heat gain from airflow'!U6)+((Occupancy!T6*'Input Data'!$F$47)+(Occupancy!F6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G60)+('Heat gain from airflow'!U6)+((Occupancy!T6*'Input Data'!$F$47)+(Occupancy!F6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I7<60,$T$15-(((H60)+('Heat gain from airflow'!V6)+((Occupancy!U6*'Input Data'!$F$47)+(Occupancy!G6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H60)+('Heat gain from airflow'!V6)+((Occupancy!U6*'Input Data'!$F$47)+(Occupancy!G6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J7<60,$T$15-(((I60)+('Heat gain from airflow'!W6)+((Occupancy!V6*'Input Data'!$F$47)+(Occupancy!H6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I60)+('Heat gain from airflow'!W6)+((Occupancy!V6*'Input Data'!$F$47)+(Occupancy!H6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K7<60,$T$15-(((J60)+('Heat gain from airflow'!X6)+((Occupancy!W6*'Input Data'!$F$47)+(Occupancy!I6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J60)+('Heat gain from airflow'!X6)+((Occupancy!W6*'Input Data'!$F$47)+(Occupancy!I6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L7<60,$T$15-(((K60)+('Heat gain from airflow'!Y6)+((Occupancy!X6*'Input Data'!$F$47)+(Occupancy!J6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K60)+('Heat gain from airflow'!Y6)+((Occupancy!X6*'Input Data'!$F$47)+(Occupancy!J6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M7<60,$T$15-(((L60)+('Heat gain from airflow'!Z6)+((Occupancy!Y6*'Input Data'!$F$47)+(Occupancy!K6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L60)+('Heat gain from airflow'!Z6)+((Occupancy!Y6*'Input Data'!$F$47)+(Occupancy!K6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.388094352441613},{"$f":"IF('Dry Bulb'!N7<60,$T$15-(((M60)+('Heat gain from airflow'!AA6)+((Occupancy!Z6*'Input Data'!$F$47)+(Occupancy!L6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M60)+('Heat gain from airflow'!AA6)+((Occupancy!Z6*'Input Data'!$F$47)+(Occupancy!L6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!O7<60,$T$15-(((N60)+('Heat gain from airflow'!AB6)+((Occupancy!AA6*'Input Data'!$F$47)+(Occupancy!M6*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N60)+('Heat gain from airflow'!AB6)+((Occupancy!AA6*'Input Data'!$F$47)+(Occupancy!M6*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"IF('Dry Bulb'!D8<60,$T$15-(((C61)+('Heat gain from airflow'!Q7)+((Occupancy!P7*'Input Data'!$F$47)+(Occupancy!B7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C61)+('Heat gain from airflow'!Q7)+((Occupancy!P7*'Input Data'!$F$47)+(Occupancy!B7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E8<60,$T$15-(((D61)+('Heat gain from airflow'!R7)+((Occupancy!Q7*'Input Data'!$F$47)+(Occupancy!C7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D61)+('Heat gain from airflow'!R7)+((Occupancy!Q7*'Input Data'!$F$47)+(Occupancy!C7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!F8<60,$T$15-(((E61)+('Heat gain from airflow'!S7)+((Occupancy!R7*'Input Data'!$F$47)+(Occupancy!D7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E61)+('Heat gain from airflow'!S7)+((Occupancy!R7*'Input Data'!$F$47)+(Occupancy!D7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!G8<60,$T$15-(((F61)+('Heat gain from airflow'!T7)+((Occupancy!S7*'Input Data'!$F$47)+(Occupancy!E7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F61)+('Heat gain from airflow'!T7)+((Occupancy!S7*'Input Data'!$F$47)+(Occupancy!E7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.256434989384289},{"$f":"IF('Dry Bulb'!H8<60,$T$15-(((G61)+('Heat gain from airflow'!U7)+((Occupancy!T7*'Input Data'!$F$47)+(Occupancy!F7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G61)+('Heat gain from airflow'!U7)+((Occupancy!T7*'Input Data'!$F$47)+(Occupancy!F7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I8<60,$T$15-(((H61)+('Heat gain from airflow'!V7)+((Occupancy!U7*'Input Data'!$F$47)+(Occupancy!G7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H61)+('Heat gain from airflow'!V7)+((Occupancy!U7*'Input Data'!$F$47)+(Occupancy!G7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J8<60,$T$15-(((I61)+('Heat gain from airflow'!W7)+((Occupancy!V7*'Input Data'!$F$47)+(Occupancy!H7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I61)+('Heat gain from airflow'!W7)+((Occupancy!V7*'Input Data'!$F$47)+(Occupancy!H7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K8<60,$T$15-(((J61)+('Heat gain from airflow'!X7)+((Occupancy!W7*'Input Data'!$F$47)+(Occupancy!I7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J61)+('Heat gain from airflow'!X7)+((Occupancy!W7*'Input Data'!$F$47)+(Occupancy!I7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L8<60,$T$15-(((K61)+('Heat gain from airflow'!Y7)+((Occupancy!X7*'Input Data'!$F$47)+(Occupancy!J7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K61)+('Heat gain from airflow'!Y7)+((Occupancy!X7*'Input Data'!$F$47)+(Occupancy!J7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M8<60,$T$15-(((L61)+('Heat gain from airflow'!Z7)+((Occupancy!Y7*'Input Data'!$F$47)+(Occupancy!K7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L61)+('Heat gain from airflow'!Z7)+((Occupancy!Y7*'Input Data'!$F$47)+(Occupancy!K7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.553492569002117},{"$f":"IF('Dry Bulb'!N8<60,$T$15-(((M61)+('Heat gain from airflow'!AA7)+((Occupancy!Z7*'Input Data'!$F$47)+(Occupancy!L7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M61)+('Heat gain from airflow'!AA7)+((Occupancy!Z7*'Input Data'!$F$47)+(Occupancy!L7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!O8<60,$T$15-(((N61)+('Heat gain from airflow'!AB7)+((Occupancy!AA7*'Input Data'!$F$47)+(Occupancy!M7*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N61)+('Heat gain from airflow'!AB7)+((Occupancy!AA7*'Input Data'!$F$47)+(Occupancy!M7*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"IF('Dry Bulb'!D9<60,$T$15-(((C62)+('Heat gain from airflow'!Q8)+((Occupancy!P8*'Input Data'!$F$47)+(Occupancy!B8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C62)+('Heat gain from airflow'!Q8)+((Occupancy!P8*'Input Data'!$F$47)+(Occupancy!B8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E9<60,$T$15-(((D62)+('Heat gain from airflow'!R8)+((Occupancy!Q8*'Input Data'!$F$47)+(Occupancy!C8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D62)+('Heat gain from airflow'!R8)+((Occupancy!Q8*'Input Data'!$F$47)+(Occupancy!C8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!F9<60,$T$15-(((E62)+('Heat gain from airflow'!S8)+((Occupancy!R8*'Input Data'!$F$47)+(Occupancy!D8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E62)+('Heat gain from airflow'!S8)+((Occupancy!R8*'Input Data'!$F$47)+(Occupancy!D8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!G9<60,$T$15-(((F62)+('Heat gain from airflow'!T8)+((Occupancy!S8*'Input Data'!$F$47)+(Occupancy!E8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F62)+('Heat gain from airflow'!T8)+((Occupancy!S8*'Input Data'!$F$47)+(Occupancy!E8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.50453231422506},{"$f":"IF('Dry Bulb'!H9<60,$T$15-(((G62)+('Heat gain from airflow'!U8)+((Occupancy!T8*'Input Data'!$F$47)+(Occupancy!F8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G62)+('Heat gain from airflow'!U8)+((Occupancy!T8*'Input Data'!$F$47)+(Occupancy!F8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I9<60,$T$15-(((H62)+('Heat gain from airflow'!V8)+((Occupancy!U8*'Input Data'!$F$47)+(Occupancy!G8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H62)+('Heat gain from airflow'!V8)+((Occupancy!U8*'Input Data'!$F$47)+(Occupancy!G8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J9<60,$T$15-(((I62)+('Heat gain from airflow'!W8)+((Occupancy!V8*'Input Data'!$F$47)+(Occupancy!H8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I62)+('Heat gain from airflow'!W8)+((Occupancy!V8*'Input Data'!$F$47)+(Occupancy!H8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K9<60,$T$15-(((J62)+('Heat gain from airflow'!X8)+((Occupancy!W8*'Input Data'!$F$47)+(Occupancy!I8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J62)+('Heat gain from airflow'!X8)+((Occupancy!W8*'Input Data'!$F$47)+(Occupancy!I8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L9<60,$T$15-(((K62)+('Heat gain from airflow'!Y8)+((Occupancy!X8*'Input Data'!$F$47)+(Occupancy!J8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K62)+('Heat gain from airflow'!Y8)+((Occupancy!X8*'Input Data'!$F$47)+(Occupancy!J8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M9<60,$T$15-(((L62)+('Heat gain from airflow'!Z8)+((Occupancy!Y8*'Input Data'!$F$47)+(Occupancy!K8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L62)+('Heat gain from airflow'!Z8)+((Occupancy!Y8*'Input Data'!$F$47)+(Occupancy!K8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.88428900212314},{"$f":"IF('Dry Bulb'!N9<60,$T$15-(((M62)+('Heat gain from airflow'!AA8)+((Occupancy!Z8*'Input Data'!$F$47)+(Occupancy!L8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M62)+('Heat gain from airflow'!AA8)+((Occupancy!Z8*'Input Data'!$F$47)+(Occupancy!L8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!O9<60,$T$15-(((N62)+('Heat gain from airflow'!AB8)+((Occupancy!AA8*'Input Data'!$F$47)+(Occupancy!M8*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N62)+('Heat gain from airflow'!AB8)+((Occupancy!AA8*'Input Data'!$F$47)+(Occupancy!M8*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,{"$f":"IF('Dry Bulb'!D10<60,$T$15-(((C63)+('Heat gain from airflow'!Q9)+((Occupancy!P9*'Input Data'!$F$47)+(Occupancy!B9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C63)+('Heat gain from airflow'!Q9)+((Occupancy!P9*'Input Data'!$F$47)+(Occupancy!B9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E10<60,$T$15-(((D63)+('Heat gain from airflow'!R9)+((Occupancy!Q9*'Input Data'!$F$47)+(Occupancy!C9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D63)+('Heat gain from airflow'!R9)+((Occupancy!Q9*'Input Data'!$F$47)+(Occupancy!C9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!F10<60,$T$15-(((E63)+('Heat gain from airflow'!S9)+((Occupancy!R9*'Input Data'!$F$47)+(Occupancy!D9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E63)+('Heat gain from airflow'!S9)+((Occupancy!R9*'Input Data'!$F$47)+(Occupancy!D9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!G10<60,$T$15-(((F63)+('Heat gain from airflow'!T9)+((Occupancy!S9*'Input Data'!$F$47)+(Occupancy!E9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F63)+('Heat gain from airflow'!T9)+((Occupancy!S9*'Input Data'!$F$47)+(Occupancy!E9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.508965671756357},{"$f":"IF('Dry Bulb'!H10<60,$T$15-(((G63)+('Heat gain from airflow'!U9)+((Occupancy!T9*'Input Data'!$F$47)+(Occupancy!F9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G63)+('Heat gain from airflow'!U9)+((Occupancy!T9*'Input Data'!$F$47)+(Occupancy!F9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":68.728733897373488},{"$f":"IF('Dry Bulb'!I10<60,$T$15-(((H63)+('Heat gain from airflow'!V9)+((Occupancy!U9*'Input Data'!$F$47)+(Occupancy!G9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H63)+('Heat gain from airflow'!V9)+((Occupancy!U9*'Input Data'!$F$47)+(Occupancy!G9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.528725672975227},{"$f":"IF('Dry Bulb'!J10<60,$T$15-(((I63)+('Heat gain from airflow'!W9)+((Occupancy!V9*'Input Data'!$F$47)+(Occupancy!H9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I63)+('Heat gain from airflow'!W9)+((Occupancy!V9*'Input Data'!$F$47)+(Occupancy!H9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.693163554430129},{"$f":"IF('Dry Bulb'!K10<60,$T$15-(((J63)+('Heat gain from airflow'!X9)+((Occupancy!W9*'Input Data'!$F$47)+(Occupancy!I9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J63)+('Heat gain from airflow'!X9)+((Occupancy!W9*'Input Data'!$F$47)+(Occupancy!I9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.817863494408968},{"$f":"IF('Dry Bulb'!L10<60,$T$15-(((K63)+('Heat gain from airflow'!Y9)+((Occupancy!X9*'Input Data'!$F$47)+(Occupancy!J9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K63)+('Heat gain from airflow'!Y9)+((Occupancy!X9*'Input Data'!$F$47)+(Occupancy!J9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":68.806892038234452},{"$f":"IF('Dry Bulb'!M10<60,$T$15-(((L63)+('Heat gain from airflow'!Z9)+((Occupancy!Y9*'Input Data'!$F$47)+(Occupancy!K9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L63)+('Heat gain from airflow'!Z9)+((Occupancy!Y9*'Input Data'!$F$47)+(Occupancy!K9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.091036772823784},{"$f":"IF('Dry Bulb'!N10<60,$T$15-(((M63)+('Heat gain from airflow'!AA9)+((Occupancy!Z9*'Input Data'!$F$47)+(Occupancy!L9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M63)+('Heat gain from airflow'!AA9)+((Occupancy!Z9*'Input Data'!$F$47)+(Occupancy!L9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!O10<60,$T$15-(((N63)+('Heat gain from airflow'!AB9)+((Occupancy!AA9*'Input Data'!$F$47)+(Occupancy!M9*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N63)+('Heat gain from airflow'!AB9)+((Occupancy!AA9*'Input Data'!$F$47)+(Occupancy!M9*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($AH$29<DEGREES(BS225),0+$AJ$33,1-((TAN(BS225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BT225),0+$AJ$33,1-((TAN(BT225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BU225),0+$AJ$33,1-((TAN(BU225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BV225),0+$AJ$33,1-((TAN(BV225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BW225),0+$AJ$33,1-((TAN(BW225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BX225),0+$AJ$33,1-((TAN(BX225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BY225),0+$AJ$33,1-((TAN(BY225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BZ225),0+$AJ$33,1-((TAN(BZ225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CA225),0+$AJ$33,1-((TAN(CA225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CB225),0+$AJ$33,1-((TAN(CB225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CC225),0+$AJ$33,1-((TAN(CC225)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CD225),0+$AJ$33,1-((TAN(CD225)/TAN($AG$31))*(1-$AJ$16)))","v":1}]
[null,7,{"$f":"IF('Dry Bulb'!D11<60,$T$15-(((C64)+('Heat gain from airflow'!Q10)+((Occupancy!P10*'Input Data'!$F$47)+(Occupancy!B10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C64)+('Heat gain from airflow'!Q10)+((Occupancy!P10*'Input Data'!$F$47)+(Occupancy!B10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.856714294401563},{"$f":"IF('Dry Bulb'!E11<60,$T$15-(((D64)+('Heat gain from airflow'!R10)+((Occupancy!Q10*'Input Data'!$F$47)+(Occupancy!C10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D64)+('Heat gain from airflow'!R10)+((Occupancy!Q10*'Input Data'!$F$47)+(Occupancy!C10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.667031336996473},{"$f":"IF('Dry Bulb'!F11<60,$T$15-(((E64)+('Heat gain from airflow'!S10)+((Occupancy!R10*'Input Data'!$F$47)+(Occupancy!D10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E64)+('Heat gain from airflow'!S10)+((Occupancy!R10*'Input Data'!$F$47)+(Occupancy!D10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.078596779005807},{"$f":"IF('Dry Bulb'!G11<60,$T$15-(((F64)+('Heat gain from airflow'!T10)+((Occupancy!S10*'Input Data'!$F$47)+(Occupancy!E10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F64)+('Heat gain from airflow'!T10)+((Occupancy!S10*'Input Data'!$F$47)+(Occupancy!E10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":68.557294103745818},{"$f":"IF('Dry Bulb'!H11<60,$T$15-(((G64)+('Heat gain from airflow'!U10)+((Occupancy!T10*'Input Data'!$F$47)+(Occupancy!F10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G64)+('Heat gain from airflow'!U10)+((Occupancy!T10*'Input Data'!$F$47)+(Occupancy!F10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.537756321294182},{"$f":"IF('Dry Bulb'!I11<60,$T$15-(((H64)+('Heat gain from airflow'!V10)+((Occupancy!U10*'Input Data'!$F$47)+(Occupancy!G10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H64)+('Heat gain from airflow'!V10)+((Occupancy!U10*'Input Data'!$F$47)+(Occupancy!G10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.26545548330833},{"$f":"IF('Dry Bulb'!J11<60,$T$15-(((I64)+('Heat gain from airflow'!W10)+((Occupancy!V10*'Input Data'!$F$47)+(Occupancy!H10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I64)+('Heat gain from airflow'!W10)+((Occupancy!V10*'Input Data'!$F$47)+(Occupancy!H10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.89727868181231},{"$f":"IF('Dry Bulb'!K11<60,$T$15-(((J64)+('Heat gain from airflow'!X10)+((Occupancy!W10*'Input Data'!$F$47)+(Occupancy!I10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J64)+('Heat gain from airflow'!X10)+((Occupancy!W10*'Input Data'!$F$47)+(Occupancy!I10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":67.218672334952231},{"$f":"IF('Dry Bulb'!L11<60,$T$15-(((K64)+('Heat gain from airflow'!Y10)+((Occupancy!X10*'Input Data'!$F$47)+(Occupancy!J10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K64)+('Heat gain from airflow'!Y10)+((Occupancy!X10*'Input Data'!$F$47)+(Occupancy!J10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":67.653726998539284},{"$f":"IF('Dry Bulb'!M11<60,$T$15-(((L64)+('Heat gain from airflow'!Z10)+((Occupancy!Y10*'Input Data'!$F$47)+(Occupancy!K10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L64)+('Heat gain from airflow'!Z10)+((Occupancy!Y10*'Input Data'!$F$47)+(Occupancy!K10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.399567242025},{"$f":"IF('Dry Bulb'!N11<60,$T$15-(((M64)+('Heat gain from airflow'!AA10)+((Occupancy!Z10*'Input Data'!$F$47)+(Occupancy!L10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M64)+('Heat gain from airflow'!AA10)+((Occupancy!Z10*'Input Data'!$F$47)+(Occupancy!L10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.535788720614789},{"$f":"IF('Dry Bulb'!O11<60,$T$15-(((N64)+('Heat gain from airflow'!AB10)+((Occupancy!AA10*'Input Data'!$F$47)+(Occupancy!M10*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N64)+('Heat gain from airflow'!AB10)+((Occupancy!AA10*'Input Data'!$F$47)+(Occupancy!M10*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.794452031025394},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,{"$f":"IF('Dry Bulb'!D12<60,$T$15-(((C65)+('Heat gain from airflow'!Q11)+((Occupancy!P11*'Input Data'!$F$47)+(Occupancy!B11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C65)+('Heat gain from airflow'!Q11)+((Occupancy!P11*'Input Data'!$F$47)+(Occupancy!B11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":60.636012287006743},{"$f":"IF('Dry Bulb'!E12<60,$T$15-(((D65)+('Heat gain from airflow'!R11)+((Occupancy!Q11*'Input Data'!$F$47)+(Occupancy!C11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D65)+('Heat gain from airflow'!R11)+((Occupancy!Q11*'Input Data'!$F$47)+(Occupancy!C11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":59.996852114891453},{"$f":"IF('Dry Bulb'!F12<60,$T$15-(((E65)+('Heat gain from airflow'!S11)+((Occupancy!R11*'Input Data'!$F$47)+(Occupancy!D11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E65)+('Heat gain from airflow'!S11)+((Occupancy!R11*'Input Data'!$F$47)+(Occupancy!D11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.687131489350378},{"$f":"IF('Dry Bulb'!G12<60,$T$15-(((F65)+('Heat gain from airflow'!T11)+((Occupancy!S11*'Input Data'!$F$47)+(Occupancy!E11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F65)+('Heat gain from airflow'!T11)+((Occupancy!S11*'Input Data'!$F$47)+(Occupancy!E11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.001054133397986},{"$f":"IF('Dry Bulb'!H12<60,$T$15-(((G65)+('Heat gain from airflow'!U11)+((Occupancy!T11*'Input Data'!$F$47)+(Occupancy!F11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G65)+('Heat gain from airflow'!U11)+((Occupancy!T11*'Input Data'!$F$47)+(Occupancy!F11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.505800104568934},{"$f":"IF('Dry Bulb'!I12<60,$T$15-(((H65)+('Heat gain from airflow'!V11)+((Occupancy!U11*'Input Data'!$F$47)+(Occupancy!G11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H65)+('Heat gain from airflow'!V11)+((Occupancy!U11*'Input Data'!$F$47)+(Occupancy!G11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.139041486907033},{"$f":"IF('Dry Bulb'!J12<60,$T$15-(((I65)+('Heat gain from airflow'!W11)+((Occupancy!V11*'Input Data'!$F$47)+(Occupancy!H11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I65)+('Heat gain from airflow'!W11)+((Occupancy!V11*'Input Data'!$F$47)+(Occupancy!H11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.362443210032374},{"$f":"IF('Dry Bulb'!K12<60,$T$15-(((J65)+('Heat gain from airflow'!X11)+((Occupancy!W11*'Input Data'!$F$47)+(Occupancy!I11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J65)+('Heat gain from airflow'!X11)+((Occupancy!W11*'Input Data'!$F$47)+(Occupancy!I11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.993641147864963},{"$f":"IF('Dry Bulb'!L12<60,$T$15-(((K65)+('Heat gain from airflow'!Y11)+((Occupancy!X11*'Input Data'!$F$47)+(Occupancy!J11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K65)+('Heat gain from airflow'!Y11)+((Occupancy!X11*'Input Data'!$F$47)+(Occupancy!J11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.853362851174566},{"$f":"IF('Dry Bulb'!M12<60,$T$15-(((L65)+('Heat gain from airflow'!Z11)+((Occupancy!Y11*'Input Data'!$F$47)+(Occupancy!K11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L65)+('Heat gain from airflow'!Z11)+((Occupancy!Y11*'Input Data'!$F$47)+(Occupancy!K11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.088569988960913},{"$f":"IF('Dry Bulb'!N12<60,$T$15-(((M65)+('Heat gain from airflow'!AA11)+((Occupancy!Z11*'Input Data'!$F$47)+(Occupancy!L11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M65)+('Heat gain from airflow'!AA11)+((Occupancy!Z11*'Input Data'!$F$47)+(Occupancy!L11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.344410694354679},{"$f":"IF('Dry Bulb'!O12<60,$T$15-(((N65)+('Heat gain from airflow'!AB11)+((Occupancy!AA11*'Input Data'!$F$47)+(Occupancy!M11*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N65)+('Heat gain from airflow'!AB11)+((Occupancy!AA11*'Input Data'!$F$47)+(Occupancy!M11*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":60.510075256014446},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,{"$f":"IF('Dry Bulb'!D13<60,$T$15-(((C66)+('Heat gain from airflow'!Q12)+((Occupancy!P12*'Input Data'!$F$47)+(Occupancy!B12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C66)+('Heat gain from airflow'!Q12)+((Occupancy!P12*'Input Data'!$F$47)+(Occupancy!B12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":57.790747816331709},{"$f":"IF('Dry Bulb'!E13<60,$T$15-(((D66)+('Heat gain from airflow'!R12)+((Occupancy!Q12*'Input Data'!$F$47)+(Occupancy!C12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D66)+('Heat gain from airflow'!R12)+((Occupancy!Q12*'Input Data'!$F$47)+(Occupancy!C12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":58.189752038078609},{"$f":"IF('Dry Bulb'!F13<60,$T$15-(((E66)+('Heat gain from airflow'!S12)+((Occupancy!R12*'Input Data'!$F$47)+(Occupancy!D12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E66)+('Heat gain from airflow'!S12)+((Occupancy!R12*'Input Data'!$F$47)+(Occupancy!D12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.483529462678931},{"$f":"IF('Dry Bulb'!G13<60,$T$15-(((F66)+('Heat gain from airflow'!T12)+((Occupancy!S12*'Input Data'!$F$47)+(Occupancy!E12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F66)+('Heat gain from airflow'!T12)+((Occupancy!S12*'Input Data'!$F$47)+(Occupancy!E12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.177850689832482},{"$f":"IF('Dry Bulb'!H13<60,$T$15-(((G66)+('Heat gain from airflow'!U12)+((Occupancy!T12*'Input Data'!$F$47)+(Occupancy!F12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G66)+('Heat gain from airflow'!U12)+((Occupancy!T12*'Input Data'!$F$47)+(Occupancy!F12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.939107663566489},{"$f":"IF('Dry Bulb'!I13<60,$T$15-(((H66)+('Heat gain from airflow'!V12)+((Occupancy!U12*'Input Data'!$F$47)+(Occupancy!G12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H66)+('Heat gain from airflow'!V12)+((Occupancy!U12*'Input Data'!$F$47)+(Occupancy!G12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.556488212857914},{"$f":"IF('Dry Bulb'!J13<60,$T$15-(((I66)+('Heat gain from airflow'!W12)+((Occupancy!V12*'Input Data'!$F$47)+(Occupancy!H12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I66)+('Heat gain from airflow'!W12)+((Occupancy!V12*'Input Data'!$F$47)+(Occupancy!H12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.956925711956146},{"$f":"IF('Dry Bulb'!K13<60,$T$15-(((J66)+('Heat gain from airflow'!X12)+((Occupancy!W12*'Input Data'!$F$47)+(Occupancy!I12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J66)+('Heat gain from airflow'!X12)+((Occupancy!W12*'Input Data'!$F$47)+(Occupancy!I12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.758459334604439},{"$f":"IF('Dry Bulb'!L13<60,$T$15-(((K66)+('Heat gain from airflow'!Y12)+((Occupancy!X12*'Input Data'!$F$47)+(Occupancy!J12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K66)+('Heat gain from airflow'!Y12)+((Occupancy!X12*'Input Data'!$F$47)+(Occupancy!J12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.648996727151385},{"$f":"IF('Dry Bulb'!M13<60,$T$15-(((L66)+('Heat gain from airflow'!Z12)+((Occupancy!Y12*'Input Data'!$F$47)+(Occupancy!K12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L66)+('Heat gain from airflow'!Z12)+((Occupancy!Y12*'Input Data'!$F$47)+(Occupancy!K12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.384381281673647},{"$f":"IF('Dry Bulb'!N13<60,$T$15-(((M66)+('Heat gain from airflow'!AA12)+((Occupancy!Z12*'Input Data'!$F$47)+(Occupancy!L12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M66)+('Heat gain from airflow'!AA12)+((Occupancy!Z12*'Input Data'!$F$47)+(Occupancy!L12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.613423635929152},{"$f":"IF('Dry Bulb'!O13<60,$T$15-(((N66)+('Heat gain from airflow'!AB12)+((Occupancy!AA12*'Input Data'!$F$47)+(Occupancy!M12*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N66)+('Heat gain from airflow'!AB12)+((Occupancy!AA12*'Input Data'!$F$47)+(Occupancy!M12*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":58.544971452619734},null,null,null,"Hot",null,15,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,{"$f":"IF('Dry Bulb'!D14<60,$T$15-(((C67)+('Heat gain from airflow'!Q13)+((Occupancy!P13*'Input Data'!$F$47)+(Occupancy!B13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C67)+('Heat gain from airflow'!Q13)+((Occupancy!P13*'Input Data'!$F$47)+(Occupancy!B13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":57.902045472522239},{"$f":"IF('Dry Bulb'!E14<60,$T$15-(((D67)+('Heat gain from airflow'!R13)+((Occupancy!Q13*'Input Data'!$F$47)+(Occupancy!C13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D67)+('Heat gain from airflow'!R13)+((Occupancy!Q13*'Input Data'!$F$47)+(Occupancy!C13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.559009996875588},{"$f":"IF('Dry Bulb'!F14<60,$T$15-(((E67)+('Heat gain from airflow'!S13)+((Occupancy!R13*'Input Data'!$F$47)+(Occupancy!D13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E67)+('Heat gain from airflow'!S13)+((Occupancy!R13*'Input Data'!$F$47)+(Occupancy!D13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.335027521318807},{"$f":"IF('Dry Bulb'!G14<60,$T$15-(((F67)+('Heat gain from airflow'!T13)+((Occupancy!S13*'Input Data'!$F$47)+(Occupancy!E13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F67)+('Heat gain from airflow'!T13)+((Occupancy!S13*'Input Data'!$F$47)+(Occupancy!E13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.795053985102271},{"$f":"IF('Dry Bulb'!H14<60,$T$15-(((G67)+('Heat gain from airflow'!U13)+((Occupancy!T13*'Input Data'!$F$47)+(Occupancy!F13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G67)+('Heat gain from airflow'!U13)+((Occupancy!T13*'Input Data'!$F$47)+(Occupancy!F13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I14<60,$T$15-(((H67)+('Heat gain from airflow'!V13)+((Occupancy!U13*'Input Data'!$F$47)+(Occupancy!G13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H67)+('Heat gain from airflow'!V13)+((Occupancy!U13*'Input Data'!$F$47)+(Occupancy!G13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J14<60,$T$15-(((I67)+('Heat gain from airflow'!W13)+((Occupancy!V13*'Input Data'!$F$47)+(Occupancy!H13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I67)+('Heat gain from airflow'!W13)+((Occupancy!V13*'Input Data'!$F$47)+(Occupancy!H13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.963287962183657},{"$f":"IF('Dry Bulb'!K14<60,$T$15-(((J67)+('Heat gain from airflow'!X13)+((Occupancy!W13*'Input Data'!$F$47)+(Occupancy!I13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J67)+('Heat gain from airflow'!X13)+((Occupancy!W13*'Input Data'!$F$47)+(Occupancy!I13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.122081637656436},{"$f":"IF('Dry Bulb'!L14<60,$T$15-(((K67)+('Heat gain from airflow'!Y13)+((Occupancy!X13*'Input Data'!$F$47)+(Occupancy!J13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K67)+('Heat gain from airflow'!Y13)+((Occupancy!X13*'Input Data'!$F$47)+(Occupancy!J13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.160968264645888},{"$f":"IF('Dry Bulb'!M14<60,$T$15-(((L67)+('Heat gain from airflow'!Z13)+((Occupancy!Y13*'Input Data'!$F$47)+(Occupancy!K13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L67)+('Heat gain from airflow'!Z13)+((Occupancy!Y13*'Input Data'!$F$47)+(Occupancy!K13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":68.55798942701972},{"$f":"IF('Dry Bulb'!N14<60,$T$15-(((M67)+('Heat gain from airflow'!AA13)+((Occupancy!Z13*'Input Data'!$F$47)+(Occupancy!L13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M67)+('Heat gain from airflow'!AA13)+((Occupancy!Z13*'Input Data'!$F$47)+(Occupancy!L13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.97149083553532},{"$f":"IF('Dry Bulb'!O14<60,$T$15-(((N67)+('Heat gain from airflow'!AB13)+((Occupancy!AA13*'Input Data'!$F$47)+(Occupancy!M13*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N67)+('Heat gain from airflow'!AB13)+((Occupancy!AA13*'Input Data'!$F$47)+(Occupancy!M13*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":58.56278759189361},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,{"$f":"IF('Dry Bulb'!D15<60,$T$15-(((C68)+('Heat gain from airflow'!Q14)+((Occupancy!P14*'Input Data'!$F$47)+(Occupancy!B14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C68)+('Heat gain from airflow'!Q14)+((Occupancy!P14*'Input Data'!$F$47)+(Occupancy!B14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":58.94591794194146},{"$f":"IF('Dry Bulb'!E15<60,$T$15-(((D68)+('Heat gain from airflow'!R14)+((Occupancy!Q14*'Input Data'!$F$47)+(Occupancy!C14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D68)+('Heat gain from airflow'!R14)+((Occupancy!Q14*'Input Data'!$F$47)+(Occupancy!C14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.514570358791829},{"$f":"IF('Dry Bulb'!F15<60,$T$15-(((E68)+('Heat gain from airflow'!S14)+((Occupancy!R14*'Input Data'!$F$47)+(Occupancy!D14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E68)+('Heat gain from airflow'!S14)+((Occupancy!R14*'Input Data'!$F$47)+(Occupancy!D14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.132386326963911},{"$f":"IF('Dry Bulb'!G15<60,$T$15-(((F68)+('Heat gain from airflow'!T14)+((Occupancy!S14*'Input Data'!$F$47)+(Occupancy!E14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F68)+('Heat gain from airflow'!T14)+((Occupancy!S14*'Input Data'!$F$47)+(Occupancy!E14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!H15<60,$T$15-(((G68)+('Heat gain from airflow'!U14)+((Occupancy!T14*'Input Data'!$F$47)+(Occupancy!F14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G68)+('Heat gain from airflow'!U14)+((Occupancy!T14*'Input Data'!$F$47)+(Occupancy!F14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I15<60,$T$15-(((H68)+('Heat gain from airflow'!V14)+((Occupancy!U14*'Input Data'!$F$47)+(Occupancy!G14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H68)+('Heat gain from airflow'!V14)+((Occupancy!U14*'Input Data'!$F$47)+(Occupancy!G14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J15<60,$T$15-(((I68)+('Heat gain from airflow'!W14)+((Occupancy!V14*'Input Data'!$F$47)+(Occupancy!H14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I68)+('Heat gain from airflow'!W14)+((Occupancy!V14*'Input Data'!$F$47)+(Occupancy!H14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K15<60,$T$15-(((J68)+('Heat gain from airflow'!X14)+((Occupancy!W14*'Input Data'!$F$47)+(Occupancy!I14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J68)+('Heat gain from airflow'!X14)+((Occupancy!W14*'Input Data'!$F$47)+(Occupancy!I14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L15<60,$T$15-(((K68)+('Heat gain from airflow'!Y14)+((Occupancy!X14*'Input Data'!$F$47)+(Occupancy!J14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K68)+('Heat gain from airflow'!Y14)+((Occupancy!X14*'Input Data'!$F$47)+(Occupancy!J14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M15<60,$T$15-(((L68)+('Heat gain from airflow'!Z14)+((Occupancy!Y14*'Input Data'!$F$47)+(Occupancy!K14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L68)+('Heat gain from airflow'!Z14)+((Occupancy!Y14*'Input Data'!$F$47)+(Occupancy!K14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.49871550800458},{"$f":"IF('Dry Bulb'!N15<60,$T$15-(((M68)+('Heat gain from airflow'!AA14)+((Occupancy!Z14*'Input Data'!$F$47)+(Occupancy!L14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M68)+('Heat gain from airflow'!AA14)+((Occupancy!Z14*'Input Data'!$F$47)+(Occupancy!L14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.691347545134462},{"$f":"IF('Dry Bulb'!O15<60,$T$15-(((N68)+('Heat gain from airflow'!AB14)+((Occupancy!AA14*'Input Data'!$F$47)+(Occupancy!M14*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N68)+('Heat gain from airflow'!AB14)+((Occupancy!AA14*'Input Data'!$F$47)+(Occupancy!M14*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.356538962096309},null,null,null,"Medium",null,50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,{"$f":"IF('Dry Bulb'!D16<60,$T$15-(((C69)+('Heat gain from airflow'!Q15)+((Occupancy!P15*'Input Data'!$F$47)+(Occupancy!B15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C69)+('Heat gain from airflow'!Q15)+((Occupancy!P15*'Input Data'!$F$47)+(Occupancy!B15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.957687352607891},{"$f":"IF('Dry Bulb'!E16<60,$T$15-(((D69)+('Heat gain from airflow'!R15)+((Occupancy!Q15*'Input Data'!$F$47)+(Occupancy!C15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D69)+('Heat gain from airflow'!R15)+((Occupancy!Q15*'Input Data'!$F$47)+(Occupancy!C15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.590002591314217},{"$f":"IF('Dry Bulb'!F16<60,$T$15-(((E69)+('Heat gain from airflow'!S15)+((Occupancy!R15*'Input Data'!$F$47)+(Occupancy!D15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E69)+('Heat gain from airflow'!S15)+((Occupancy!R15*'Input Data'!$F$47)+(Occupancy!D15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.760240339702762},{"$f":"IF('Dry Bulb'!G16<60,$T$15-(((F69)+('Heat gain from airflow'!T15)+((Occupancy!S15*'Input Data'!$F$47)+(Occupancy!E15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F69)+('Heat gain from airflow'!T15)+((Occupancy!S15*'Input Data'!$F$47)+(Occupancy!E15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!H16<60,$T$15-(((G69)+('Heat gain from airflow'!U15)+((Occupancy!T15*'Input Data'!$F$47)+(Occupancy!F15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G69)+('Heat gain from airflow'!U15)+((Occupancy!T15*'Input Data'!$F$47)+(Occupancy!F15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I16<60,$T$15-(((H69)+('Heat gain from airflow'!V15)+((Occupancy!U15*'Input Data'!$F$47)+(Occupancy!G15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H69)+('Heat gain from airflow'!V15)+((Occupancy!U15*'Input Data'!$F$47)+(Occupancy!G15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J16<60,$T$15-(((I69)+('Heat gain from airflow'!W15)+((Occupancy!V15*'Input Data'!$F$47)+(Occupancy!H15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I69)+('Heat gain from airflow'!W15)+((Occupancy!V15*'Input Data'!$F$47)+(Occupancy!H15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K16<60,$T$15-(((J69)+('Heat gain from airflow'!X15)+((Occupancy!W15*'Input Data'!$F$47)+(Occupancy!I15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J69)+('Heat gain from airflow'!X15)+((Occupancy!W15*'Input Data'!$F$47)+(Occupancy!I15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L16<60,$T$15-(((K69)+('Heat gain from airflow'!Y15)+((Occupancy!X15*'Input Data'!$F$47)+(Occupancy!J15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K69)+('Heat gain from airflow'!Y15)+((Occupancy!X15*'Input Data'!$F$47)+(Occupancy!J15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M16<60,$T$15-(((L69)+('Heat gain from airflow'!Z15)+((Occupancy!Y15*'Input Data'!$F$47)+(Occupancy!K15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L69)+('Heat gain from airflow'!Z15)+((Occupancy!Y15*'Input Data'!$F$47)+(Occupancy!K15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.602986212581641},{"$f":"IF('Dry Bulb'!N16<60,$T$15-(((M69)+('Heat gain from airflow'!AA15)+((Occupancy!Z15*'Input Data'!$F$47)+(Occupancy!L15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M69)+('Heat gain from airflow'!AA15)+((Occupancy!Z15*'Input Data'!$F$47)+(Occupancy!L15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.12666519334234},{"$f":"IF('Dry Bulb'!O16<60,$T$15-(((N69)+('Heat gain from airflow'!AB15)+((Occupancy!AA15*'Input Data'!$F$47)+(Occupancy!M15*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N69)+('Heat gain from airflow'!AB15)+((Occupancy!AA15*'Input Data'!$F$47)+(Occupancy!M15*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.200289988632846},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,{"$f":"IF('Dry Bulb'!D17<60,$T$15-(((C70)+('Heat gain from airflow'!Q16)+((Occupancy!P16*'Input Data'!$F$47)+(Occupancy!B16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C70)+('Heat gain from airflow'!Q16)+((Occupancy!P16*'Input Data'!$F$47)+(Occupancy!B16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.166410679679444},{"$f":"IF('Dry Bulb'!E17<60,$T$15-(((D70)+('Heat gain from airflow'!R16)+((Occupancy!Q16*'Input Data'!$F$47)+(Occupancy!C16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D70)+('Heat gain from airflow'!R16)+((Occupancy!Q16*'Input Data'!$F$47)+(Occupancy!C16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.904294053726574},{"$f":"IF('Dry Bulb'!F17<60,$T$15-(((E70)+('Heat gain from airflow'!S16)+((Occupancy!R16*'Input Data'!$F$47)+(Occupancy!D16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E70)+('Heat gain from airflow'!S16)+((Occupancy!R16*'Input Data'!$F$47)+(Occupancy!D16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.933249256900211},{"$f":"IF('Dry Bulb'!G17<60,$T$15-(((F70)+('Heat gain from airflow'!T16)+((Occupancy!S16*'Input Data'!$F$47)+(Occupancy!E16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F70)+('Heat gain from airflow'!T16)+((Occupancy!S16*'Input Data'!$F$47)+(Occupancy!E16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!H17<60,$T$15-(((G70)+('Heat gain from airflow'!U16)+((Occupancy!T16*'Input Data'!$F$47)+(Occupancy!F16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G70)+('Heat gain from airflow'!U16)+((Occupancy!T16*'Input Data'!$F$47)+(Occupancy!F16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I17<60,$T$15-(((H70)+('Heat gain from airflow'!V16)+((Occupancy!U16*'Input Data'!$F$47)+(Occupancy!G16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H70)+('Heat gain from airflow'!V16)+((Occupancy!U16*'Input Data'!$F$47)+(Occupancy!G16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J17<60,$T$15-(((I70)+('Heat gain from airflow'!W16)+((Occupancy!V16*'Input Data'!$F$47)+(Occupancy!H16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I70)+('Heat gain from airflow'!W16)+((Occupancy!V16*'Input Data'!$F$47)+(Occupancy!H16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K17<60,$T$15-(((J70)+('Heat gain from airflow'!X16)+((Occupancy!W16*'Input Data'!$F$47)+(Occupancy!I16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J70)+('Heat gain from airflow'!X16)+((Occupancy!W16*'Input Data'!$F$47)+(Occupancy!I16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L17<60,$T$15-(((K70)+('Heat gain from airflow'!Y16)+((Occupancy!X16*'Input Data'!$F$47)+(Occupancy!J16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K70)+('Heat gain from airflow'!Y16)+((Occupancy!X16*'Input Data'!$F$47)+(Occupancy!J16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M17<60,$T$15-(((L70)+('Heat gain from airflow'!Z16)+((Occupancy!Y16*'Input Data'!$F$47)+(Occupancy!K16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L70)+('Heat gain from airflow'!Z16)+((Occupancy!Y16*'Input Data'!$F$47)+(Occupancy!K16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.383683665255802},{"$f":"IF('Dry Bulb'!N17<60,$T$15-(((M70)+('Heat gain from airflow'!AA16)+((Occupancy!Z16*'Input Data'!$F$47)+(Occupancy!L16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M70)+('Heat gain from airflow'!AA16)+((Occupancy!Z16*'Input Data'!$F$47)+(Occupancy!L16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.916844657285395},{"$f":"IF('Dry Bulb'!O17<60,$T$15-(((N70)+('Heat gain from airflow'!AB16)+((Occupancy!AA16*'Input Data'!$F$47)+(Occupancy!M16*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N70)+('Heat gain from airflow'!AB16)+((Occupancy!AA16*'Input Data'!$F$47)+(Occupancy!M16*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.704775751867658},null,null,null,"Cold",null,78,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,{"$f":"IF('Dry Bulb'!D18<60,$T$15-(((C71)+('Heat gain from airflow'!Q17)+((Occupancy!P17*'Input Data'!$F$47)+(Occupancy!B17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C71)+('Heat gain from airflow'!Q17)+((Occupancy!P17*'Input Data'!$F$47)+(Occupancy!B17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":68.2574307486706},{"$f":"IF('Dry Bulb'!E18<60,$T$15-(((D71)+('Heat gain from airflow'!R17)+((Occupancy!Q17*'Input Data'!$F$47)+(Occupancy!C17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D71)+('Heat gain from airflow'!R17)+((Occupancy!Q17*'Input Data'!$F$47)+(Occupancy!C17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.145131161436467},{"$f":"IF('Dry Bulb'!F18<60,$T$15-(((E71)+('Heat gain from airflow'!S17)+((Occupancy!R17*'Input Data'!$F$47)+(Occupancy!D17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E71)+('Heat gain from airflow'!S17)+((Occupancy!R17*'Input Data'!$F$47)+(Occupancy!D17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.561103269639062},{"$f":"IF('Dry Bulb'!G18<60,$T$15-(((F71)+('Heat gain from airflow'!T17)+((Occupancy!S17*'Input Data'!$F$47)+(Occupancy!E17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F71)+('Heat gain from airflow'!T17)+((Occupancy!S17*'Input Data'!$F$47)+(Occupancy!E17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!H18<60,$T$15-(((G71)+('Heat gain from airflow'!U17)+((Occupancy!T17*'Input Data'!$F$47)+(Occupancy!F17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G71)+('Heat gain from airflow'!U17)+((Occupancy!T17*'Input Data'!$F$47)+(Occupancy!F17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I18<60,$T$15-(((H71)+('Heat gain from airflow'!V17)+((Occupancy!U17*'Input Data'!$F$47)+(Occupancy!G17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H71)+('Heat gain from airflow'!V17)+((Occupancy!U17*'Input Data'!$F$47)+(Occupancy!G17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J18<60,$T$15-(((I71)+('Heat gain from airflow'!W17)+((Occupancy!V17*'Input Data'!$F$47)+(Occupancy!H17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I71)+('Heat gain from airflow'!W17)+((Occupancy!V17*'Input Data'!$F$47)+(Occupancy!H17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K18<60,$T$15-(((J71)+('Heat gain from airflow'!X17)+((Occupancy!W17*'Input Data'!$F$47)+(Occupancy!I17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J71)+('Heat gain from airflow'!X17)+((Occupancy!W17*'Input Data'!$F$47)+(Occupancy!I17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L18<60,$T$15-(((K71)+('Heat gain from airflow'!Y17)+((Occupancy!X17*'Input Data'!$F$47)+(Occupancy!J17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K71)+('Heat gain from airflow'!Y17)+((Occupancy!X17*'Input Data'!$F$47)+(Occupancy!J17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M18<60,$T$15-(((L71)+('Heat gain from airflow'!Z17)+((Occupancy!Y17*'Input Data'!$F$47)+(Occupancy!K17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L71)+('Heat gain from airflow'!Z17)+((Occupancy!Y17*'Input Data'!$F$47)+(Occupancy!K17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":67.816007712166055},{"$f":"IF('Dry Bulb'!N18<60,$T$15-(((M71)+('Heat gain from airflow'!AA17)+((Occupancy!Z17*'Input Data'!$F$47)+(Occupancy!L17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M71)+('Heat gain from airflow'!AA17)+((Occupancy!Z17*'Input Data'!$F$47)+(Occupancy!L17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.687147940806668},{"$f":"IF('Dry Bulb'!O18<60,$T$15-(((N71)+('Heat gain from airflow'!AB17)+((Occupancy!AA17*'Input Data'!$F$47)+(Occupancy!M17*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N71)+('Heat gain from airflow'!AB17)+((Occupancy!AA17*'Input Data'!$F$47)+(Occupancy!M17*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":67.017655064117022},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,{"$f":"IF('Dry Bulb'!D19<60,$T$15-(((C72)+('Heat gain from airflow'!Q18)+((Occupancy!P18*'Input Data'!$F$47)+(Occupancy!B18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C72)+('Heat gain from airflow'!Q18)+((Occupancy!P18*'Input Data'!$F$47)+(Occupancy!B18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.664876920979196},{"$f":"IF('Dry Bulb'!E19<60,$T$15-(((D72)+('Heat gain from airflow'!R18)+((Occupancy!Q18*'Input Data'!$F$47)+(Occupancy!C18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D72)+('Heat gain from airflow'!R18)+((Occupancy!Q18*'Input Data'!$F$47)+(Occupancy!C18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.553918997933678},{"$f":"IF('Dry Bulb'!F19<60,$T$15-(((E72)+('Heat gain from airflow'!S18)+((Occupancy!R18*'Input Data'!$F$47)+(Occupancy!D18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E72)+('Heat gain from airflow'!S18)+((Occupancy!R18*'Input Data'!$F$47)+(Occupancy!D18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.339058651911216},{"$f":"IF('Dry Bulb'!G19<60,$T$15-(((F72)+('Heat gain from airflow'!T18)+((Occupancy!S18*'Input Data'!$F$47)+(Occupancy!E18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F72)+('Heat gain from airflow'!T18)+((Occupancy!S18*'Input Data'!$F$47)+(Occupancy!E18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.808867966145158},{"$f":"IF('Dry Bulb'!H19<60,$T$15-(((G72)+('Heat gain from airflow'!U18)+((Occupancy!T18*'Input Data'!$F$47)+(Occupancy!F18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G72)+('Heat gain from airflow'!U18)+((Occupancy!T18*'Input Data'!$F$47)+(Occupancy!F18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.998379691108426},{"$f":"IF('Dry Bulb'!I19<60,$T$15-(((H72)+('Heat gain from airflow'!V18)+((Occupancy!U18*'Input Data'!$F$47)+(Occupancy!G18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H72)+('Heat gain from airflow'!V18)+((Occupancy!U18*'Input Data'!$F$47)+(Occupancy!G18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.4521783633014},{"$f":"IF('Dry Bulb'!J19<60,$T$15-(((I72)+('Heat gain from airflow'!W18)+((Occupancy!V18*'Input Data'!$F$47)+(Occupancy!H18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I72)+('Heat gain from airflow'!W18)+((Occupancy!V18*'Input Data'!$F$47)+(Occupancy!H18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.549650931585234},{"$f":"IF('Dry Bulb'!K19<60,$T$15-(((J72)+('Heat gain from airflow'!X18)+((Occupancy!W18*'Input Data'!$F$47)+(Occupancy!I18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J72)+('Heat gain from airflow'!X18)+((Occupancy!W18*'Input Data'!$F$47)+(Occupancy!I18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.434341743781175},{"$f":"IF('Dry Bulb'!L19<60,$T$15-(((K72)+('Heat gain from airflow'!Y18)+((Occupancy!X18*'Input Data'!$F$47)+(Occupancy!J18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K72)+('Heat gain from airflow'!Y18)+((Occupancy!X18*'Input Data'!$F$47)+(Occupancy!J18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.574143771292157},{"$f":"IF('Dry Bulb'!M19<60,$T$15-(((L72)+('Heat gain from airflow'!Z18)+((Occupancy!Y18*'Input Data'!$F$47)+(Occupancy!K18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L72)+('Heat gain from airflow'!Z18)+((Occupancy!Y18*'Input Data'!$F$47)+(Occupancy!K18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.200862432331924},{"$f":"IF('Dry Bulb'!N19<60,$T$15-(((M72)+('Heat gain from airflow'!AA18)+((Occupancy!Z18*'Input Data'!$F$47)+(Occupancy!L18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M72)+('Heat gain from airflow'!AA18)+((Occupancy!Z18*'Input Data'!$F$47)+(Occupancy!L18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.292280927031598},{"$f":"IF('Dry Bulb'!O19<60,$T$15-(((N72)+('Heat gain from airflow'!AB18)+((Occupancy!AA18*'Input Data'!$F$47)+(Occupancy!M18*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N72)+('Heat gain from airflow'!AB18)+((Occupancy!AA18*'Input Data'!$F$47)+(Occupancy!M18*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.06921752565755},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,{"$f":"IF('Dry Bulb'!D20<60,$T$15-(((C73)+('Heat gain from airflow'!Q19)+((Occupancy!P19*'Input Data'!$F$47)+(Occupancy!B19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C73)+('Heat gain from airflow'!Q19)+((Occupancy!P19*'Input Data'!$F$47)+(Occupancy!B19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.417496592038944},{"$f":"IF('Dry Bulb'!E20<60,$T$15-(((D73)+('Heat gain from airflow'!R19)+((Occupancy!Q19*'Input Data'!$F$47)+(Occupancy!C19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D73)+('Heat gain from airflow'!R19)+((Occupancy!Q19*'Input Data'!$F$47)+(Occupancy!C19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.527205526822272},{"$f":"IF('Dry Bulb'!F20<60,$T$15-(((E73)+('Heat gain from airflow'!S19)+((Occupancy!R19*'Input Data'!$F$47)+(Occupancy!D19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E73)+('Heat gain from airflow'!S19)+((Occupancy!R19*'Input Data'!$F$47)+(Occupancy!D19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":60.838120810021991},{"$f":"IF('Dry Bulb'!G20<60,$T$15-(((F73)+('Heat gain from airflow'!T19)+((Occupancy!S19*'Input Data'!$F$47)+(Occupancy!E19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F73)+('Heat gain from airflow'!T19)+((Occupancy!S19*'Input Data'!$F$47)+(Occupancy!E19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":60.968870215774587},{"$f":"IF('Dry Bulb'!H20<60,$T$15-(((G73)+('Heat gain from airflow'!U19)+((Occupancy!T19*'Input Data'!$F$47)+(Occupancy!F19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G73)+('Heat gain from airflow'!U19)+((Occupancy!T19*'Input Data'!$F$47)+(Occupancy!F19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":60.597068385282491},{"$f":"IF('Dry Bulb'!I20<60,$T$15-(((H73)+('Heat gain from airflow'!V19)+((Occupancy!U19*'Input Data'!$F$47)+(Occupancy!G19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H73)+('Heat gain from airflow'!V19)+((Occupancy!U19*'Input Data'!$F$47)+(Occupancy!G19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":60.914738351398519},{"$f":"IF('Dry Bulb'!J20<60,$T$15-(((I73)+('Heat gain from airflow'!W19)+((Occupancy!V19*'Input Data'!$F$47)+(Occupancy!H19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I73)+('Heat gain from airflow'!W19)+((Occupancy!V19*'Input Data'!$F$47)+(Occupancy!H19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":60.676771800160417},{"$f":"IF('Dry Bulb'!K20<60,$T$15-(((J73)+('Heat gain from airflow'!X19)+((Occupancy!W19*'Input Data'!$F$47)+(Occupancy!I19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J73)+('Heat gain from airflow'!X19)+((Occupancy!W19*'Input Data'!$F$47)+(Occupancy!I19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":59.36840660513937},{"$f":"IF('Dry Bulb'!L20<60,$T$15-(((K73)+('Heat gain from airflow'!Y19)+((Occupancy!X19*'Input Data'!$F$47)+(Occupancy!J19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K73)+('Heat gain from airflow'!Y19)+((Occupancy!X19*'Input Data'!$F$47)+(Occupancy!J19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":60.183567132662454},{"$f":"IF('Dry Bulb'!M20<60,$T$15-(((L73)+('Heat gain from airflow'!Z19)+((Occupancy!Y19*'Input Data'!$F$47)+(Occupancy!K19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L73)+('Heat gain from airflow'!Z19)+((Occupancy!Y19*'Input Data'!$F$47)+(Occupancy!K19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.312384489714823},{"$f":"IF('Dry Bulb'!N20<60,$T$15-(((M73)+('Heat gain from airflow'!AA19)+((Occupancy!Z19*'Input Data'!$F$47)+(Occupancy!L19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M73)+('Heat gain from airflow'!AA19)+((Occupancy!Z19*'Input Data'!$F$47)+(Occupancy!L19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":64.370966662544703},{"$f":"IF('Dry Bulb'!O20<60,$T$15-(((N73)+('Heat gain from airflow'!AB19)+((Occupancy!AA19*'Input Data'!$F$47)+(Occupancy!M19*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N73)+('Heat gain from airflow'!AB19)+((Occupancy!AA19*'Input Data'!$F$47)+(Occupancy!M19*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.282037574210577},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,{"$f":"IF('Dry Bulb'!D21<60,$T$15-(((C74)+('Heat gain from airflow'!Q20)+((Occupancy!P20*'Input Data'!$F$47)+(Occupancy!B20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C74)+('Heat gain from airflow'!Q20)+((Occupancy!P20*'Input Data'!$F$47)+(Occupancy!B20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.245820757135903},{"$f":"IF('Dry Bulb'!E21<60,$T$15-(((D74)+('Heat gain from airflow'!R20)+((Occupancy!Q20*'Input Data'!$F$47)+(Occupancy!C20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D74)+('Heat gain from airflow'!R20)+((Occupancy!Q20*'Input Data'!$F$47)+(Occupancy!C20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":65.914433734289005},{"$f":"IF('Dry Bulb'!F21<60,$T$15-(((E74)+('Heat gain from airflow'!S20)+((Occupancy!R20*'Input Data'!$F$47)+(Occupancy!D20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E74)+('Heat gain from airflow'!S20)+((Occupancy!R20*'Input Data'!$F$47)+(Occupancy!D20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.891488365592302},{"$f":"IF('Dry Bulb'!G21<60,$T$15-(((F74)+('Heat gain from airflow'!T20)+((Occupancy!S20*'Input Data'!$F$47)+(Occupancy!E20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F74)+('Heat gain from airflow'!T20)+((Occupancy!S20*'Input Data'!$F$47)+(Occupancy!E20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.22242767039549},{"$f":"IF('Dry Bulb'!H21<60,$T$15-(((G74)+('Heat gain from airflow'!U20)+((Occupancy!T20*'Input Data'!$F$47)+(Occupancy!F20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G74)+('Heat gain from airflow'!U20)+((Occupancy!T20*'Input Data'!$F$47)+(Occupancy!F20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.713388756476277},{"$f":"IF('Dry Bulb'!I21<60,$T$15-(((H74)+('Heat gain from airflow'!V20)+((Occupancy!U20*'Input Data'!$F$47)+(Occupancy!G20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H74)+('Heat gain from airflow'!V20)+((Occupancy!U20*'Input Data'!$F$47)+(Occupancy!G20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.076737417212001},{"$f":"IF('Dry Bulb'!J21<60,$T$15-(((I74)+('Heat gain from airflow'!W20)+((Occupancy!V20*'Input Data'!$F$47)+(Occupancy!H20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I74)+('Heat gain from airflow'!W20)+((Occupancy!V20*'Input Data'!$F$47)+(Occupancy!H20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":61.878623985300159},{"$f":"IF('Dry Bulb'!K21<60,$T$15-(((J74)+('Heat gain from airflow'!X20)+((Occupancy!W20*'Input Data'!$F$47)+(Occupancy!I20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J74)+('Heat gain from airflow'!X20)+((Occupancy!W20*'Input Data'!$F$47)+(Occupancy!I20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":61.631481149056903},{"$f":"IF('Dry Bulb'!L21<60,$T$15-(((K74)+('Heat gain from airflow'!Y20)+((Occupancy!X20*'Input Data'!$F$47)+(Occupancy!J20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K74)+('Heat gain from airflow'!Y20)+((Occupancy!X20*'Input Data'!$F$47)+(Occupancy!J20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":63.428930949400382},{"$f":"IF('Dry Bulb'!M21<60,$T$15-(((L74)+('Heat gain from airflow'!Z20)+((Occupancy!Y20*'Input Data'!$F$47)+(Occupancy!K20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L74)+('Heat gain from airflow'!Z20)+((Occupancy!Y20*'Input Data'!$F$47)+(Occupancy!K20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.429600408882862},{"$f":"IF('Dry Bulb'!N21<60,$T$15-(((M74)+('Heat gain from airflow'!AA20)+((Occupancy!Z20*'Input Data'!$F$47)+(Occupancy!L20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M74)+('Heat gain from airflow'!AA20)+((Occupancy!Z20*'Input Data'!$F$47)+(Occupancy!L20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":68.666663721759676},{"$f":"IF('Dry Bulb'!O21<60,$T$15-(((N74)+('Heat gain from airflow'!AB20)+((Occupancy!AA20*'Input Data'!$F$47)+(Occupancy!M20*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N74)+('Heat gain from airflow'!AB20)+((Occupancy!AA20*'Input Data'!$F$47)+(Occupancy!M20*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.58718209572443},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,{"$f":"IF('Dry Bulb'!D22<60,$T$15-(((C75)+('Heat gain from airflow'!Q21)+((Occupancy!P21*'Input Data'!$F$47)+(Occupancy!B21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C75)+('Heat gain from airflow'!Q21)+((Occupancy!P21*'Input Data'!$F$47)+(Occupancy!B21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!E22<60,$T$15-(((D75)+('Heat gain from airflow'!R21)+((Occupancy!Q21*'Input Data'!$F$47)+(Occupancy!C21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D75)+('Heat gain from airflow'!R21)+((Occupancy!Q21*'Input Data'!$F$47)+(Occupancy!C21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.541430493762959},{"$f":"IF('Dry Bulb'!F22<60,$T$15-(((E75)+('Heat gain from airflow'!S21)+((Occupancy!R21*'Input Data'!$F$47)+(Occupancy!D21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E75)+('Heat gain from airflow'!S21)+((Occupancy!R21*'Input Data'!$F$47)+(Occupancy!D21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":68.220527259173267},{"$f":"IF('Dry Bulb'!G22<60,$T$15-(((F75)+('Heat gain from airflow'!T21)+((Occupancy!S21*'Input Data'!$F$47)+(Occupancy!E21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F75)+('Heat gain from airflow'!T21)+((Occupancy!S21*'Input Data'!$F$47)+(Occupancy!E21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":68.042651415341922},{"$f":"IF('Dry Bulb'!H22<60,$T$15-(((G75)+('Heat gain from airflow'!U21)+((Occupancy!T21*'Input Data'!$F$47)+(Occupancy!F21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G75)+('Heat gain from airflow'!U21)+((Occupancy!T21*'Input Data'!$F$47)+(Occupancy!F21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":67.315969428642248},{"$f":"IF('Dry Bulb'!I22<60,$T$15-(((H75)+('Heat gain from airflow'!V21)+((Occupancy!U21*'Input Data'!$F$47)+(Occupancy!G21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H75)+('Heat gain from airflow'!V21)+((Occupancy!U21*'Input Data'!$F$47)+(Occupancy!G21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.435534677794081},{"$f":"IF('Dry Bulb'!J22<60,$T$15-(((I75)+('Heat gain from airflow'!W21)+((Occupancy!V21*'Input Data'!$F$47)+(Occupancy!H21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I75)+('Heat gain from airflow'!W21)+((Occupancy!V21*'Input Data'!$F$47)+(Occupancy!H21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":66.387672432916617},{"$f":"IF('Dry Bulb'!K22<60,$T$15-(((J75)+('Heat gain from airflow'!X21)+((Occupancy!W21*'Input Data'!$F$47)+(Occupancy!I21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J75)+('Heat gain from airflow'!X21)+((Occupancy!W21*'Input Data'!$F$47)+(Occupancy!I21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":67.072666601956769},{"$f":"IF('Dry Bulb'!L22<60,$T$15-(((K75)+('Heat gain from airflow'!Y21)+((Occupancy!X21*'Input Data'!$F$47)+(Occupancy!J21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K75)+('Heat gain from airflow'!Y21)+((Occupancy!X21*'Input Data'!$F$47)+(Occupancy!J21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M22<60,$T$15-(((L75)+('Heat gain from airflow'!Z21)+((Occupancy!Y21*'Input Data'!$F$47)+(Occupancy!K21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L75)+('Heat gain from airflow'!Z21)+((Occupancy!Y21*'Input Data'!$F$47)+(Occupancy!K21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!N22<60,$T$15-(((M75)+('Heat gain from airflow'!AA21)+((Occupancy!Z21*'Input Data'!$F$47)+(Occupancy!L21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M75)+('Heat gain from airflow'!AA21)+((Occupancy!Z21*'Input Data'!$F$47)+(Occupancy!L21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.313005944798306},{"$f":"IF('Dry Bulb'!O22<60,$T$15-(((N75)+('Heat gain from airflow'!AB21)+((Occupancy!AA21*'Input Data'!$F$47)+(Occupancy!M21*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N75)+('Heat gain from airflow'!AB21)+((Occupancy!AA21*'Input Data'!$F$47)+(Occupancy!M21*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,{"$f":"IF('Dry Bulb'!D23<60,$T$15-(((C76)+('Heat gain from airflow'!Q22)+((Occupancy!P22*'Input Data'!$F$47)+(Occupancy!B22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C76)+('Heat gain from airflow'!Q22)+((Occupancy!P22*'Input Data'!$F$47)+(Occupancy!B22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!E23<60,$T$15-(((D76)+('Heat gain from airflow'!R22)+((Occupancy!Q22*'Input Data'!$F$47)+(Occupancy!C22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D76)+('Heat gain from airflow'!R22)+((Occupancy!Q22*'Input Data'!$F$47)+(Occupancy!C22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.752629639065816},{"$f":"IF('Dry Bulb'!F23<60,$T$15-(((E76)+('Heat gain from airflow'!S22)+((Occupancy!R22*'Input Data'!$F$47)+(Occupancy!D22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E76)+('Heat gain from airflow'!S22)+((Occupancy!R22*'Input Data'!$F$47)+(Occupancy!D22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.139997027600856},{"$f":"IF('Dry Bulb'!G23<60,$T$15-(((F76)+('Heat gain from airflow'!T22)+((Occupancy!S22*'Input Data'!$F$47)+(Occupancy!E22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F76)+('Heat gain from airflow'!T22)+((Occupancy!S22*'Input Data'!$F$47)+(Occupancy!E22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!H23<60,$T$15-(((G76)+('Heat gain from airflow'!U22)+((Occupancy!T22*'Input Data'!$F$47)+(Occupancy!F22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G76)+('Heat gain from airflow'!U22)+((Occupancy!T22*'Input Data'!$F$47)+(Occupancy!F22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I23<60,$T$15-(((H76)+('Heat gain from airflow'!V22)+((Occupancy!U22*'Input Data'!$F$47)+(Occupancy!G22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H76)+('Heat gain from airflow'!V22)+((Occupancy!U22*'Input Data'!$F$47)+(Occupancy!G22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J23<60,$T$15-(((I76)+('Heat gain from airflow'!W22)+((Occupancy!V22*'Input Data'!$F$47)+(Occupancy!H22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I76)+('Heat gain from airflow'!W22)+((Occupancy!V22*'Input Data'!$F$47)+(Occupancy!H22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K23<60,$T$15-(((J76)+('Heat gain from airflow'!X22)+((Occupancy!W22*'Input Data'!$F$47)+(Occupancy!I22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J76)+('Heat gain from airflow'!X22)+((Occupancy!W22*'Input Data'!$F$47)+(Occupancy!I22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L23<60,$T$15-(((K76)+('Heat gain from airflow'!Y22)+((Occupancy!X22*'Input Data'!$F$47)+(Occupancy!J22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K76)+('Heat gain from airflow'!Y22)+((Occupancy!X22*'Input Data'!$F$47)+(Occupancy!J22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M23<60,$T$15-(((L76)+('Heat gain from airflow'!Z22)+((Occupancy!Y22*'Input Data'!$F$47)+(Occupancy!K22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L76)+('Heat gain from airflow'!Z22)+((Occupancy!Y22*'Input Data'!$F$47)+(Occupancy!K22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!N23<60,$T$15-(((M76)+('Heat gain from airflow'!AA22)+((Occupancy!Z22*'Input Data'!$F$47)+(Occupancy!L22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M76)+('Heat gain from airflow'!AA22)+((Occupancy!Z22*'Input Data'!$F$47)+(Occupancy!L22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.767851040339707},{"$f":"IF('Dry Bulb'!O23<60,$T$15-(((N76)+('Heat gain from airflow'!AB22)+((Occupancy!AA22*'Input Data'!$F$47)+(Occupancy!M22*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N76)+('Heat gain from airflow'!AB22)+((Occupancy!AA22*'Input Data'!$F$47)+(Occupancy!M22*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,{"$f":"IF('Dry Bulb'!D24<60,$T$15-(((C77)+('Heat gain from airflow'!Q23)+((Occupancy!P23*'Input Data'!$F$47)+(Occupancy!B23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C77)+('Heat gain from airflow'!Q23)+((Occupancy!P23*'Input Data'!$F$47)+(Occupancy!B23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E24<60,$T$15-(((D77)+('Heat gain from airflow'!R23)+((Occupancy!Q23*'Input Data'!$F$47)+(Occupancy!C23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D77)+('Heat gain from airflow'!R23)+((Occupancy!Q23*'Input Data'!$F$47)+(Occupancy!C23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!F24<60,$T$15-(((E77)+('Heat gain from airflow'!S23)+((Occupancy!R23*'Input Data'!$F$47)+(Occupancy!D23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E77)+('Heat gain from airflow'!S23)+((Occupancy!R23*'Input Data'!$F$47)+(Occupancy!D23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.718890785562635},{"$f":"IF('Dry Bulb'!G24<60,$T$15-(((F77)+('Heat gain from airflow'!T23)+((Occupancy!S23*'Input Data'!$F$47)+(Occupancy!E23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F77)+('Heat gain from airflow'!T23)+((Occupancy!S23*'Input Data'!$F$47)+(Occupancy!E23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!H24<60,$T$15-(((G77)+('Heat gain from airflow'!U23)+((Occupancy!T23*'Input Data'!$F$47)+(Occupancy!F23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G77)+('Heat gain from airflow'!U23)+((Occupancy!T23*'Input Data'!$F$47)+(Occupancy!F23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I24<60,$T$15-(((H77)+('Heat gain from airflow'!V23)+((Occupancy!U23*'Input Data'!$F$47)+(Occupancy!G23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H77)+('Heat gain from airflow'!V23)+((Occupancy!U23*'Input Data'!$F$47)+(Occupancy!G23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J24<60,$T$15-(((I77)+('Heat gain from airflow'!W23)+((Occupancy!V23*'Input Data'!$F$47)+(Occupancy!H23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I77)+('Heat gain from airflow'!W23)+((Occupancy!V23*'Input Data'!$F$47)+(Occupancy!H23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K24<60,$T$15-(((J77)+('Heat gain from airflow'!X23)+((Occupancy!W23*'Input Data'!$F$47)+(Occupancy!I23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J77)+('Heat gain from airflow'!X23)+((Occupancy!W23*'Input Data'!$F$47)+(Occupancy!I23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L24<60,$T$15-(((K77)+('Heat gain from airflow'!Y23)+((Occupancy!X23*'Input Data'!$F$47)+(Occupancy!J23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K77)+('Heat gain from airflow'!Y23)+((Occupancy!X23*'Input Data'!$F$47)+(Occupancy!J23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M24<60,$T$15-(((L77)+('Heat gain from airflow'!Z23)+((Occupancy!Y23*'Input Data'!$F$47)+(Occupancy!K23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L77)+('Heat gain from airflow'!Z23)+((Occupancy!Y23*'Input Data'!$F$47)+(Occupancy!K23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!N24<60,$T$15-(((M77)+('Heat gain from airflow'!AA23)+((Occupancy!Z23*'Input Data'!$F$47)+(Occupancy!L23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M77)+('Heat gain from airflow'!AA23)+((Occupancy!Z23*'Input Data'!$F$47)+(Occupancy!L23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.346744798301486},{"$f":"IF('Dry Bulb'!O24<60,$T$15-(((N77)+('Heat gain from airflow'!AB23)+((Occupancy!AA23*'Input Data'!$F$47)+(Occupancy!M23*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N77)+('Heat gain from airflow'!AB23)+((Occupancy!AA23*'Input Data'!$F$47)+(Occupancy!M23*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,{"$f":"IF('Dry Bulb'!D25<60,$T$15-(((C78)+('Heat gain from airflow'!Q24)+((Occupancy!P24*'Input Data'!$F$47)+(Occupancy!B24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C78)+('Heat gain from airflow'!Q24)+((Occupancy!P24*'Input Data'!$F$47)+(Occupancy!B24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E25<60,$T$15-(((D78)+('Heat gain from airflow'!R24)+((Occupancy!Q24*'Input Data'!$F$47)+(Occupancy!C24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D78)+('Heat gain from airflow'!R24)+((Occupancy!Q24*'Input Data'!$F$47)+(Occupancy!C24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!F25<60,$T$15-(((E78)+('Heat gain from airflow'!S24)+((Occupancy!R24*'Input Data'!$F$47)+(Occupancy!D24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E78)+('Heat gain from airflow'!S24)+((Occupancy!R24*'Input Data'!$F$47)+(Occupancy!D24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.049687218683658},{"$f":"IF('Dry Bulb'!G25<60,$T$15-(((F78)+('Heat gain from airflow'!T24)+((Occupancy!S24*'Input Data'!$F$47)+(Occupancy!E24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F78)+('Heat gain from airflow'!T24)+((Occupancy!S24*'Input Data'!$F$47)+(Occupancy!E24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":68.940859957537157},{"$f":"IF('Dry Bulb'!H25<60,$T$15-(((G78)+('Heat gain from airflow'!U24)+((Occupancy!T24*'Input Data'!$F$47)+(Occupancy!F24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G78)+('Heat gain from airflow'!U24)+((Occupancy!T24*'Input Data'!$F$47)+(Occupancy!F24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I25<60,$T$15-(((H78)+('Heat gain from airflow'!V24)+((Occupancy!U24*'Input Data'!$F$47)+(Occupancy!G24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H78)+('Heat gain from airflow'!V24)+((Occupancy!U24*'Input Data'!$F$47)+(Occupancy!G24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J25<60,$T$15-(((I78)+('Heat gain from airflow'!W24)+((Occupancy!V24*'Input Data'!$F$47)+(Occupancy!H24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I78)+('Heat gain from airflow'!W24)+((Occupancy!V24*'Input Data'!$F$47)+(Occupancy!H24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K25<60,$T$15-(((J78)+('Heat gain from airflow'!X24)+((Occupancy!W24*'Input Data'!$F$47)+(Occupancy!I24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J78)+('Heat gain from airflow'!X24)+((Occupancy!W24*'Input Data'!$F$47)+(Occupancy!I24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L25<60,$T$15-(((K78)+('Heat gain from airflow'!Y24)+((Occupancy!X24*'Input Data'!$F$47)+(Occupancy!J24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K78)+('Heat gain from airflow'!Y24)+((Occupancy!X24*'Input Data'!$F$47)+(Occupancy!J24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M25<60,$T$15-(((L78)+('Heat gain from airflow'!Z24)+((Occupancy!Y24*'Input Data'!$F$47)+(Occupancy!K24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L78)+('Heat gain from airflow'!Z24)+((Occupancy!Y24*'Input Data'!$F$47)+(Occupancy!K24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!N25<60,$T$15-(((M78)+('Heat gain from airflow'!AA24)+((Occupancy!Z24*'Input Data'!$F$47)+(Occupancy!L24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M78)+('Heat gain from airflow'!AA24)+((Occupancy!Z24*'Input Data'!$F$47)+(Occupancy!L24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.718890785562635},{"$f":"IF('Dry Bulb'!O25<60,$T$15-(((N78)+('Heat gain from airflow'!AB24)+((Occupancy!AA24*'Input Data'!$F$47)+(Occupancy!M24*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N78)+('Heat gain from airflow'!AB24)+((Occupancy!AA24*'Input Data'!$F$47)+(Occupancy!M24*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,{"$f":"IF('Dry Bulb'!D26<60,$T$15-(((C79)+('Heat gain from airflow'!Q25)+((Occupancy!P25*'Input Data'!$F$47)+(Occupancy!B25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C79)+('Heat gain from airflow'!Q25)+((Occupancy!P25*'Input Data'!$F$47)+(Occupancy!B25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E26<60,$T$15-(((D79)+('Heat gain from airflow'!R25)+((Occupancy!Q25*'Input Data'!$F$47)+(Occupancy!C25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D79)+('Heat gain from airflow'!R25)+((Occupancy!Q25*'Input Data'!$F$47)+(Occupancy!C25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!F26<60,$T$15-(((E79)+('Heat gain from airflow'!S25)+((Occupancy!R25*'Input Data'!$F$47)+(Occupancy!D25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E79)+('Heat gain from airflow'!S25)+((Occupancy!R25*'Input Data'!$F$47)+(Occupancy!D25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.421833205944793},{"$f":"IF('Dry Bulb'!G26<60,$T$15-(((F79)+('Heat gain from airflow'!T25)+((Occupancy!S25*'Input Data'!$F$47)+(Occupancy!E25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F79)+('Heat gain from airflow'!T25)+((Occupancy!S25*'Input Data'!$F$47)+(Occupancy!E25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.313005944798306},{"$f":"IF('Dry Bulb'!H26<60,$T$15-(((G79)+('Heat gain from airflow'!U25)+((Occupancy!T25*'Input Data'!$F$47)+(Occupancy!F25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G79)+('Heat gain from airflow'!U25)+((Occupancy!T25*'Input Data'!$F$47)+(Occupancy!F25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I26<60,$T$15-(((H79)+('Heat gain from airflow'!V25)+((Occupancy!U25*'Input Data'!$F$47)+(Occupancy!G25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H79)+('Heat gain from airflow'!V25)+((Occupancy!U25*'Input Data'!$F$47)+(Occupancy!G25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J26<60,$T$15-(((I79)+('Heat gain from airflow'!W25)+((Occupancy!V25*'Input Data'!$F$47)+(Occupancy!H25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I79)+('Heat gain from airflow'!W25)+((Occupancy!V25*'Input Data'!$F$47)+(Occupancy!H25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K26<60,$T$15-(((J79)+('Heat gain from airflow'!X25)+((Occupancy!W25*'Input Data'!$F$47)+(Occupancy!I25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J79)+('Heat gain from airflow'!X25)+((Occupancy!W25*'Input Data'!$F$47)+(Occupancy!I25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L26<60,$T$15-(((K79)+('Heat gain from airflow'!Y25)+((Occupancy!X25*'Input Data'!$F$47)+(Occupancy!J25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K79)+('Heat gain from airflow'!Y25)+((Occupancy!X25*'Input Data'!$F$47)+(Occupancy!J25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M26<60,$T$15-(((L79)+('Heat gain from airflow'!Z25)+((Occupancy!Y25*'Input Data'!$F$47)+(Occupancy!K25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L79)+('Heat gain from airflow'!Z25)+((Occupancy!Y25*'Input Data'!$F$47)+(Occupancy!K25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!N26<60,$T$15-(((M79)+('Heat gain from airflow'!AA25)+((Occupancy!Z25*'Input Data'!$F$47)+(Occupancy!L25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M79)+('Heat gain from airflow'!AA25)+((Occupancy!Z25*'Input Data'!$F$47)+(Occupancy!L25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.173735881104037},{"$f":"IF('Dry Bulb'!O26<60,$T$15-(((N79)+('Heat gain from airflow'!AB25)+((Occupancy!AA25*'Input Data'!$F$47)+(Occupancy!M25*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N79)+('Heat gain from airflow'!AB25)+((Occupancy!AA25*'Input Data'!$F$47)+(Occupancy!M25*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,{"$f":"IF('Dry Bulb'!D27<60,$T$15-(((C80)+('Heat gain from airflow'!Q26)+((Occupancy!P26*'Input Data'!$F$47)+(Occupancy!B26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C80)+('Heat gain from airflow'!Q26)+((Occupancy!P26*'Input Data'!$F$47)+(Occupancy!B26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E27<60,$T$15-(((D80)+('Heat gain from airflow'!R26)+((Occupancy!Q26*'Input Data'!$F$47)+(Occupancy!C26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D80)+('Heat gain from airflow'!R26)+((Occupancy!Q26*'Input Data'!$F$47)+(Occupancy!C26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!F27<60,$T$15-(((E80)+('Heat gain from airflow'!S26)+((Occupancy!R26*'Input Data'!$F$47)+(Occupancy!D26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E80)+('Heat gain from airflow'!S26)+((Occupancy!R26*'Input Data'!$F$47)+(Occupancy!D26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.752629639065816},{"$f":"IF('Dry Bulb'!G27<60,$T$15-(((F80)+('Heat gain from airflow'!T26)+((Occupancy!S26*'Input Data'!$F$47)+(Occupancy!E26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F80)+('Heat gain from airflow'!T26)+((Occupancy!S26*'Input Data'!$F$47)+(Occupancy!E26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.809200594479833},{"$f":"IF('Dry Bulb'!H27<60,$T$15-(((G80)+('Heat gain from airflow'!U26)+((Occupancy!T26*'Input Data'!$F$47)+(Occupancy!F26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G80)+('Heat gain from airflow'!U26)+((Occupancy!T26*'Input Data'!$F$47)+(Occupancy!F26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I27<60,$T$15-(((H80)+('Heat gain from airflow'!V26)+((Occupancy!U26*'Input Data'!$F$47)+(Occupancy!G26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H80)+('Heat gain from airflow'!V26)+((Occupancy!U26*'Input Data'!$F$47)+(Occupancy!G26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J27<60,$T$15-(((I80)+('Heat gain from airflow'!W26)+((Occupancy!V26*'Input Data'!$F$47)+(Occupancy!H26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I80)+('Heat gain from airflow'!W26)+((Occupancy!V26*'Input Data'!$F$47)+(Occupancy!H26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K27<60,$T$15-(((J80)+('Heat gain from airflow'!X26)+((Occupancy!W26*'Input Data'!$F$47)+(Occupancy!I26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J80)+('Heat gain from airflow'!X26)+((Occupancy!W26*'Input Data'!$F$47)+(Occupancy!I26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L27<60,$T$15-(((K80)+('Heat gain from airflow'!Y26)+((Occupancy!X26*'Input Data'!$F$47)+(Occupancy!J26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K80)+('Heat gain from airflow'!Y26)+((Occupancy!X26*'Input Data'!$F$47)+(Occupancy!J26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M27<60,$T$15-(((L80)+('Heat gain from airflow'!Z26)+((Occupancy!Y26*'Input Data'!$F$47)+(Occupancy!K26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L80)+('Heat gain from airflow'!Z26)+((Occupancy!Y26*'Input Data'!$F$47)+(Occupancy!K26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.064908619957535},{"$f":"IF('Dry Bulb'!N27<60,$T$15-(((M80)+('Heat gain from airflow'!AA26)+((Occupancy!Z26*'Input Data'!$F$47)+(Occupancy!L26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M80)+('Heat gain from airflow'!AA26)+((Occupancy!Z26*'Input Data'!$F$47)+(Occupancy!L26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.628580976645438},{"$f":"IF('Dry Bulb'!O27<60,$T$15-(((N80)+('Heat gain from airflow'!AB26)+((Occupancy!AA26*'Input Data'!$F$47)+(Occupancy!M26*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N80)+('Heat gain from airflow'!AB26)+((Occupancy!AA26*'Input Data'!$F$47)+(Occupancy!M26*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,{"$f":"IF('Dry Bulb'!D28<60,$T$15-(((C81)+('Heat gain from airflow'!Q27)+((Occupancy!P27*'Input Data'!$F$47)+(Occupancy!B27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((C81)+('Heat gain from airflow'!Q27)+((Occupancy!P27*'Input Data'!$F$47)+(Occupancy!B27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!E28<60,$T$15-(((D81)+('Heat gain from airflow'!R27)+((Occupancy!Q27*'Input Data'!$F$47)+(Occupancy!C27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((D81)+('Heat gain from airflow'!R27)+((Occupancy!Q27*'Input Data'!$F$47)+(Occupancy!C27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},{"$f":"IF('Dry Bulb'!F28<60,$T$15-(((E81)+('Heat gain from airflow'!S27)+((Occupancy!R27*'Input Data'!$F$47)+(Occupancy!D27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((E81)+('Heat gain from airflow'!S27)+((Occupancy!R27*'Input Data'!$F$47)+(Occupancy!D27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":72.083426072186839},{"$f":"IF('Dry Bulb'!G28<60,$T$15-(((F81)+('Heat gain from airflow'!T27)+((Occupancy!S27*'Input Data'!$F$47)+(Occupancy!E27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((F81)+('Heat gain from airflow'!T27)+((Occupancy!S27*'Input Data'!$F$47)+(Occupancy!E27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":70.139997027600856},{"$f":"IF('Dry Bulb'!H28<60,$T$15-(((G81)+('Heat gain from airflow'!U27)+((Occupancy!T27*'Input Data'!$F$47)+(Occupancy!F27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((G81)+('Heat gain from airflow'!U27)+((Occupancy!T27*'Input Data'!$F$47)+(Occupancy!F27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!I28<60,$T$15-(((H81)+('Heat gain from airflow'!V27)+((Occupancy!U27*'Input Data'!$F$47)+(Occupancy!G27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((H81)+('Heat gain from airflow'!V27)+((Occupancy!U27*'Input Data'!$F$47)+(Occupancy!G27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!J28<60,$T$15-(((I81)+('Heat gain from airflow'!W27)+((Occupancy!V27*'Input Data'!$F$47)+(Occupancy!H27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((I81)+('Heat gain from airflow'!W27)+((Occupancy!V27*'Input Data'!$F$47)+(Occupancy!H27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!K28<60,$T$15-(((J81)+('Heat gain from airflow'!X27)+((Occupancy!W27*'Input Data'!$F$47)+(Occupancy!I27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((J81)+('Heat gain from airflow'!X27)+((Occupancy!W27*'Input Data'!$F$47)+(Occupancy!I27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!L28<60,$T$15-(((K81)+('Heat gain from airflow'!Y27)+((Occupancy!X27*'Input Data'!$F$47)+(Occupancy!J27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((K81)+('Heat gain from airflow'!Y27)+((Occupancy!X27*'Input Data'!$F$47)+(Occupancy!J27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.979193205944796},{"$f":"IF('Dry Bulb'!M28<60,$T$15-(((L81)+('Heat gain from airflow'!Z27)+((Occupancy!Y27*'Input Data'!$F$47)+(Occupancy!K27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((L81)+('Heat gain from airflow'!Z27)+((Occupancy!Y27*'Input Data'!$F$47)+(Occupancy!K27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":69.395705053078558},{"$f":"IF('Dry Bulb'!N28<60,$T$15-(((M81)+('Heat gain from airflow'!AA27)+((Occupancy!Z27*'Input Data'!$F$47)+(Occupancy!L27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((M81)+('Heat gain from airflow'!AA27)+((Occupancy!Z27*'Input Data'!$F$47)+(Occupancy!L27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":71.91802785562632},{"$f":"IF('Dry Bulb'!O28<60,$T$15-(((N81)+('Heat gain from airflow'!AB27)+((Occupancy!AA27*'Input Data'!$F$47)+(Occupancy!M27*'Input Data'!$F$49)))/'Input Data'!$F$44),$P$15-(((N81)+('Heat gain from airflow'!AB27)+((Occupancy!AA27*'Input Data'!$F$47)+(Occupancy!M27*'Input Data'!$F$49)))/'Input Data'!$F$44))","v":62.979193205944796},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"Balance Point Temperature",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$f":"'Input Data'!$F$44*('Dry Bulb'!D5-$T$15)","v":-8011.7100000000028},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,1,{"$f":"(3*C220+(4*C243)+3*C242+2*C241)/12","v":62.979193205944796},{"$f":"(3*D220+(4*D243)+3*D242+2*D241)/12","v":64.145859872611467},71.364403269639055,69.991827791932067,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.492953078556269,71.804316581740977,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,2,{"$f":"(3*C221+(4*C220)+3*C243+2*C242)/12","v":62.979193205944796},{"$f":"(3*D221+(4*D220)+3*D243+2*D242)/12","v":62.979193205944796},70.800824161358818,70.315732632696395,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.605898619957529,71.495343524416128,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"(3*C222+(4*C221)+3*C220+2*C243)/12","v":62.979193205944796},{"$f":"(3*D222+(4*D221)+3*D220+2*D243)/12","v":62.979193205944796},70.329898683651805,70.587950530785562,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.933249256900226,70.869740084925681,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"(3*C223+(4*C222)+3*C221+2*C220)/12","v":62.979193205944796},{"$f":"(3*D223+(4*D222)+3*D221+2*D220)/12","v":62.979193205944796},69.979193205944796,70.863614225053084,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,70.226141932059448,70.357465053078556,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"(3*C224+(4*C223)+3*C222+2*C221)/12","v":62.979193205944796},62.979193205944796,68.229193205944796,71.139277919320591,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,70.50525142250531,68.229193205944796,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,62.979193205944796,62.979193205944796,65.895859872611467,71.34713402940406,69.666578378801972,69.8665763227024,69.907685793066122,69.938860778060842,69.686117914017217,70.770577728237797,65.895859872611467,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,62.948573478058989,62.901152738707715,63.920710765876713,70.727850993308891,68.702014215258373,68.900602930962492,69.113371357740121,69.235286417684705,69.007059598189969,70.526891746811984,64.035008751278966,62.933007912214947,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,62.352571672362537,62.129553976865346,63.355978967816526,68.647358371574697,66.90108447524112,66.918625818730803,67.226193452710518,67.272299139876694,67.379504922856157,68.992138938141707,63.672696082937257,62.300333326822404,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,60.870401824343027,60.709678749723388,64.032774257862101,66.18563185481996,65.242605013967065,65.089954031839781,65.199892760857935,65.128473882412322,65.57795055485326,66.740683256048925,64.648638854911681,61.001413157240229,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,59.374216094393084,61.480054763467386,65.596482370061238,65.934526276860197,65.773910269032953,65.509297324716968,65.466621144008116,65.151529197073856,65.745536187762127,66.106361488223868,65.372748047884684,59.748948201354494,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,58.590850311576837,64.111892617324713,67.963510036075377,67.22112132454474,67.390272970120904,67.233491671166789,67.115532918541845,66.724047205666963,67.102930713351768,66.921532337919615,65.624091522836792,60.581319343645958,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,59.995363822984977,67.407068606324501,69.481867318023191,68.799601314715446,68.972512282215078,68.908742373763644,68.804838979339749,68.561459668649306,68.719604224154509,68.270545959514138,64.773892128252427,62.233777624600343,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,62.330985518361558,70.061218633046948,70.408993596086745,69.948503335804375,69.979193205944796,69.979193205944796,69.976542331984604,69.836341277896736,69.842822382394971,69.347926768678931,64.439518254308283,64.175889940017541,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,64.850236075536344,70.654309849228511,70.246816709129519,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.06576228760629,64.374292760154802,65.932168007492734,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,66.286580041822845,69.427930748612923,68.548484790366345,68.686611895994886,68.733989827235703,69.09743949528395,69.121807637354905,68.592980340403898,68.127930847281633,67.101970130549219,63.885774908571854,65.982765005525792,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,66.168092588783693,67.086772846997007,65.701700446702375,66.003170711802369,65.973390829167087,66.537407878093759,66.510407096378842,65.47821273502224,65.061936876073318,64.829666138790159,63.848096402729276,66.132124960112364,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,66.909745074986859,65.733678552235844,63.680527569323054,63.993979515384154,63.790163774647802,64.100340596585326,63.995858196932289,62.969123459246781,63.225156592051412,64.231078492236307,64.977916373180491,67.177721607435188,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,67.875258855371101,66.414290082898262,63.951667914481447,64.128500958935149,63.715785654158019,63.605177123585719,63.483927541966843,62.893152308756534,64.112691029667289,65.582904965597848,66.691927880260906,68.439237981223243,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,69.035567324758262,68.518443595730062,66.137733903026387,66.142767393494807,65.711313364366433,65.311617273620314,65.206473742143501,65.154958556925919,66.709023296261634,67.813993553974313,68.441458449215062,69.514997823100671,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,68.106964464476647,70.033438093663719,68.596768247982979,68.368930169035863,68.1024198533744,67.776202609118329,67.731218142580317,67.861276212133149,68.887482829854051,69.387594406434474,69.615331986181459,70.080524687574737,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,65.895859872611467,70.516258528861414,70.240472533287544,69.396852928742405,69.535322576394364,69.388583451253012,69.380606410440109,69.49477210528012,69.979193205944796,69.979193205944796,70.12276804670914,68.229193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,64.145859872611467,70.27476594479829,70.90840957537155,69.466535307855636,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,70.581058938428882,65.895859872611467,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,62.979193205944796,68.229193205944796,71.294338747346075,69.455049320594483,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.750622059447977,71.035904033970283,64.145859872611467,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,62.979193205944796,65.895859872611467,71.635472569002118,69.623127600849259,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.528559639065818,71.435616390658168,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"Balance Point Temperature",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,1,{"$f":"(3*C249+(4*C272)+3*C271+2*C270)/12","v":63.173637650389246},{"$f":"(3*D249+(4*D272)+3*D271+2*D270)/12","v":66.771510884642595},71.361244623142241,69.647184363057335,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.6502791985138,71.285437107218684,63.756970983722574,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,2,{"$f":"(3*C250+(4*C249)+3*C272+2*C271)/12","v":62.979193205944796},{"$f":"(3*D250+(4*D249)+3*D272+2*D271)/12","v":64.972248761500353},71.279598397027598,69.891165875796176,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.573035934182599,71.506829511677282,63.173637650389246,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"(3*C251+(4*C250)+3*C249+2*C272)/12","v":62.979193205944796},{"$f":"(3*D251+(4*D250)+3*D249+2*D272)/12","v":63.756970983722574},70.963095636942668,70.187376725053085,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.646610063694268,71.406231406581739,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"(3*C252+(4*C251)+3*C250+2*C249)/12","v":62.979193205944796},{"$f":"(3*D252+(4*D251)+3*D250+2*D249)/12","v":63.173637650389246},70.532371114649678,70.489458190021239,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.851252070063708,71.053834936305734,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"(3*C253+(4*C252)+3*C251+2*C250)/12","v":62.979193205944796},62.979193205944796,69.766308067940557,70.772300626326967,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,70.119322250530786,70.143112261146499,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,{"$f":"(3*C254+(4*C253)+3*C252+2*C251)/12","v":62.979193205944796},62.979193205944796,68.433477452229297,71.030438125185412,69.901039499159097,69.951038985134204,69.96131635272512,69.9691100989738,69.905924382962908,70.406471932059461,68.618018980891719,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,{"$f":"(3*C255+(4*C254)+3*C253+2*C252)/12","v":62.971538273973344},62.959683089135531,66.665961484816663,71.059762608800909,69.555693515892258,69.672006676118414,69.738901939600737,69.779772366251777,69.638468040030233,70.552585357085164,66.757581289022852,62.967646882512334,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,{"$f":"(3*C256+(4*C255)+3*C254+2*C253)/12","v":62.812331246587298},62.740769909595912,64.991395499723367,70.431119751234419,68.705785986254355,68.82636704666993,68.984459131681675,69.044417653036746,68.931957776272469,70.200518319283091,65.10867410697098,62.794083138254251,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,{"$f":"(3*C257+(4*C256)+3*C255+2*C254)/12","v":62.23546658404549},62.109091398720359,64.08967422397545,69.002012507457792,67.397612695520408,67.448277234061223,67.63832814606404,67.671516584659969,67.720440498215737,69.10936968480209,64.377787241295323,62.246915243962064,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,{"$f":"(3*C258+(4*C257)+3*C256+2*C255)/12","v":61.213259796146417},61.622487224775597,64.235825214736266,67.495323612600188,66.366619393267271,66.287065951635611,66.425396462422327,66.354662781322531,66.641753728970656,67.776001483076371,64.483408776222532,61.334959419826795,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,{"$f":"(3*C259+(4*C258)+3*C257+2*C256)/12","v":60.048813677504761},62.053670092395379,65.42389502480755,66.77109011572368,66.233036998239825,66.070398170445756,66.105429043304397,65.892356527690552,66.315316533447984,66.949697550923716,64.97121462422156,60.695388080143438,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,{"$f":"(3*C260+(4*C259)+3*C258+2*C257)/12","v":59.517745387260639},63.710691506510102,67.096219810356587,67.121510981878814,67.023797463513489,66.863999486982394,66.806358130493905,66.524341932055165,66.913587099905286,67.024851517249189,65.186130360798487,60.856356763910732,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($AH$29<DEGREES(BS289),0+$AJ$33,1-((TAN(BS289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BT289),0+$AJ$33,1-((TAN(BT289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BU289),0+$AJ$33,1-((TAN(BU289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BV289),0+$AJ$33,1-((TAN(BV289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BW289),0+$AJ$33,1-((TAN(BW289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BX289),0+$AJ$33,1-((TAN(BX289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BY289),0+$AJ$33,1-((TAN(BY289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BZ289),0+$AJ$33,1-((TAN(BZ289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CA289),0+$AJ$33,1-((TAN(CA289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CB289),0+$AJ$33,1-((TAN(CB289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CC289),0+$AJ$33,1-((TAN(CC289)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CD289),0+$AJ$33,1-((TAN(CD289)/TAN($AG$31))*(1-$AJ$16)))","v":1}]
[null,13,{"$f":"(3*C261+(4*C260)+3*C259+2*C258)/12","v":60.124616247545106},66.25897647527897,68.686495409058466,68.214694316135791,68.295522349593611,68.190968231318607,68.119068663079545,67.852505209952994,68.100562379948542,67.841940344524986,65.00265782835119,61.892052896008401,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,{"$f":"(3*C262+(4*C261)+3*C260+2*C259)/12","v":61.753536866013654},68.554399594458019,69.729087211496321,69.214386629523986,69.296036269041721,69.253963575436515,69.207444310072972,69.034618178891932,69.139461937215103,68.603641374326358,64.704234227344031,63.530336278636774,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,{"$f":"(3*C263+(4*C262)+3*C261+2*C260)/12","v":63.770364052389048},69.658235396211879,69.735286385993646,69.451776762383986,69.500112207312569,69.580346306249396,69.568458390873104,69.360638084664984,69.272353413426501,68.512819313928162,64.335069565480367,64.889349342983465,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,{"$f":"(3*C264+(4*C263)+3*C262+2*C261)/12","v":65.238606433081216},69.254784029101842,68.571456485094544,68.549212167402473,68.562674818847341,68.824828970428413,68.825759676696649,68.368068478359177,68.110063199997569,67.399168278228672,64.09077530262968,65.706309900412791,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,{"$f":"(3*C265+(4*C264)+3*C263+2*C262)/12","v":66.163484821386376},67.928378249082613,66.665622690344733,66.834403624436348,66.785367544517371,67.141779849989376,67.11275102502222,66.379795729244208,66.188783019515171,65.954111249894154,64.227670414706978,66.322857974526485,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,{"$f":"(3*C266+(4*C265)+3*C264+2*C263)/12","v":66.861849559671455},66.857813707987916,65.064932078464693,65.312013072144907,65.141347016919823,65.418666365162295,65.350837664789665,64.514712470760927,64.72336431499923,65.197163961933967,64.941940679903027,67.032542105399926,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,{"$f":"(3*C267+(4*C266)+3*C265+2*C264)/12","v":67.639429816523929},66.882256039123732,64.722071414031575,64.910882165498506,64.609529641000748,64.644283155095607,64.546960014821039,63.908440062799059,64.698098127979577,65.677180689883627,66.226835732807402,68.008280011393779,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,{"$f":"(3*C268+(4*C267)+3*C266+2*C265)/12","v":68.159035784045841},67.90702633475648,65.796441603178735,65.837610165721699,65.490016460779884,65.299274123813674,65.205254034673331,64.901780559072193,66.023910662309447,67.052469109705569,67.720287178545689,68.997893542805585,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,{"$f":"(3*C269+(4*C268)+3*C267+2*C266)/12","v":67.747721430063166},69.172203242852149,67.618752344153037,67.362631963393781,67.131763212008011,66.867980571522068,66.804497342667148,66.765050121055324,67.819996907114174,68.50797898639091,68.96148859941836,69.202762316656816,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,{"$f":"(3*C270+(4*C269)+3*C268+2*C267)/12","v":66.534420595935558},70.002211118524315,69.312740950772209,68.614945244386135,68.650729684355667,68.453646316453501,68.422217264301892,68.484201149100514,69.161237293641591,69.47042689740546,69.830263488258154,68.322993512544926,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,{"$f":"(3*C271+(4*C270)+3*C269+2*C268)/12","v":64.95187730458899},69.783524597578278,70.452634053279425,69.263309026458742,69.555429989795456,69.46437566780078,69.454883996507874,69.505101765143351,69.797241476596341,69.823450619402195,70.419242997343062,66.739137341772008,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,{"$f":"(3*C272+(4*C271)+3*C270+2*C269)/12","v":63.756970983722574},68.538430611144278,71.107495540756702,69.490240988831445,69.905214767686388,69.880758246829501,69.87942874002735,69.898456355834014,69.979193205944796,69.790344432059456,70.869931518046727,64.972248761500353,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"Balance Point Temperature",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,1,{"$f":"(3*C278+(4*C301)+3*C300+2*C299)/12","v":64.372772499307999},{"$f":"(3*D278+(4*D301)+3*D300+2*D299)/12","v":68.651937594024034},70.708091674486354,69.326861217720534,69.627182335556469,69.563419353455146,69.555365091339269,69.584592719566785,69.797379288223809,69.710285081399718,70.687857780199039,65.668608920631257,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,2,{"$f":"(3*C279+(4*C278)+3*C301+2*C300)/12","v":63.567233148311423},{"$f":"(3*D279+(4*D278)+3*D301+2*D300)/12","v":67.265427570971738},71.125960701040057,69.604964674919145,69.890071393688643,69.868781543141964,69.866867221225945,69.879993753283529,69.948867917720051,69.694846594298809,71.092543126061074,64.411984821175267,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"(3*C280+(4*C279)+3*C278+2*C301)/12","v":63.157433946685536},{"$f":"(3*D280+(4*D279)+3*D278+2*D301)/12","v":65.712608489448797},71.192200454156549,69.837402395431567,69.966863466235068,69.962787379425578,69.96256579495855,69.96573706425967,69.979193205944796,69.646958365622794,71.320182218683655,63.570628391129979,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"(3*C281+(4*C280)+3*C279+2*C278)/12","v":63.011600613352208},{"$f":"(3*D281+(4*D280)+3*D279+2*D278)/12","v":64.417380411653696},71.000898360757247,70.098812318648285,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.679988555378642,71.323149432059452,63.157433946685536,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"(3*C282+(4*C281)+3*C280+2*C279)/12","v":62.979193205944796},63.570628391129979,70.573074363941956,70.384933047151449,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.979193205944796,69.820739757607939,70.989752480980187,63.011600613352208,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,{"$f":"(3*C283+(4*C282)+3*C281+2*C280)/12","v":62.979193205944796},63.157433946685536,69.824080770523707,70.668637075086153,69.959654779248368,69.972154650742155,69.974723992639881,69.976672429202054,69.96087600019932,70.045306761323431,70.200039467445166,62.979193205944796,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,{"$f":"(3*C284+(4*C283)+3*C282+2*C281)/12","v":62.977279472951928},63.00672308414989,68.67462172470735,70.883071548847312,69.847267047836425,69.893011833218011,69.913161438285556,69.925976960364537,69.86958897347219,70.278676224267755,68.940152203890534,62.976306625086686,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,{"$f":"(3*C285+(4*C284)+3*C283+2*C282)/12","v":62.934926072114941},62.913084009587813,67.205923410917151,70.847360443093095,69.500136410974918,69.581552600981311,69.645943385292739,69.676504927744034,69.585492087476396,70.355829723619152,67.374719078497705,62.929066914544677,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,{"$f":"(3*C286+(4*C285)+3*C284+2*C283)/12","v":62.73572716435794},62.677315792820075,65.75828700247736,70.330890050340386,68.790428464797799,68.880699823957244,68.999346624097612,69.039146471902484,68.968033790479467,70.050073522242755,65.923069998385145,62.73153377869415,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,{"$f":"(3*C287+(4*C286)+3*C285+2*C284)/12","v":62.246809667694151},62.287125264688918,64.781023500742833,69.325575444911394,67.826587829369245,67.873118440283193,68.021723603814138,68.036904364518435,68.073319382387737,69.289350738371425,64.983546682733959,62.275840201259676,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,{"$f":"(3*C288+(4*C287)+3*C286+2*C285)/12","v":61.444211871867587},62.038314432636788,64.622233300395067,68.18023681853451,66.980833218904877,66.946418676116934,67.075147973429821,67.016592147367945,67.211516796951571,68.306853689837425,64.68316574294856,61.646242827344338,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,{"$f":"(3*C289+(4*C288)+3*C287+2*C286)/12","v":60.571600285694267},62.369366613406612,65.32258863520498,67.411574105103938,66.65821866286187,66.552611955479946,66.616136353674534,66.46245611835127,66.780680801404273,67.535007381189644,64.804087532544997,61.15411094664254,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,{"$f":"(3*C290+(4*C289)+3*C288+2*C287)/12","v":60.084815909707082},63.585473348217896,66.598975081041417,67.36950370402451,67.034508890340732,66.901185754707825,66.89580988049768,66.670106541983031,67.015457716479332,67.335526893457967,64.969413029446443,61.154805735312671,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,{"$f":"(3*C291+(4*C290)+3*C289+2*C288)/12","v":60.367494925417738},65.494876615734256,68.005807729283973,67.950720860849898,67.883972049376638,67.771546537785227,67.727378338385634,67.489301185669532,67.766002474837606,67.679386262889508,64.968679527189622,61.843255572663594,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,{"$f":"(3*C292+(4*C291)+3*C290+2*C289)/12","v":61.477881594864861},67.449218083777069,69.031177820987907,68.67499847645108,68.718220306159367,68.671483074034569,68.625422888594798,68.402215538627658,68.541980777399672,68.127378958930265,64.766864984372305,63.014855446612017,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,{"$f":"(3*C293+(4*C292)+3*C291+2*C290)/12","v":63.025593216827588},68.714870450507092,69.267980620988681,68.960607672715582,69.013968899342061,69.078308277102465,69.050965237496698,68.779635227526597,68.753259485436757,68.145298908535636,64.477551875712081,64.254286808424936,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,{"$f":"(3*C294+(4*C293)+3*C292+2*C291)/12","v":64.521920507139868},68.907314686767236,68.578893966032169,68.4570135907599,68.474934255746888,68.664468458441902,68.646796297884876,68.230234309412353,68.091882164437123,67.517062296086195,64.288315800480746,65.293544509287884,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,{"$f":"(3*C295+(4*C294)+3*C293+2*C292)/12","v":65.7080029473818},68.280648083335294,67.253519102003665,67.318736978429627,67.27114667499967,67.53819150160237,67.509809408857834,66.907400161138924,66.816676787492014,66.552590028993407,64.389914061448891,66.107223883459241,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,19,{"$f":"(3*C296+(4*C295)+3*C294+2*C293)/12","v":66.611112918214928},67.53106047956453,65.963810299764731,66.131861166099085,65.989619105160685,66.223542701396752,66.169500261006803,65.471641184657656,65.647852258539686,65.873405685293889,64.942735980617883,66.87801684834885,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,{"$f":"(3*C297+(4*C296)+3*C295+2*C294)/12","v":67.328945411668357},67.306691731907776,65.400304340145496,65.563433802038872,65.325245340511401,65.417876148940763,65.340134767309806,64.720235899932007,65.284315290239547,65.947153706186782,65.945780611332466,67.730845244937044,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,{"$f":"(3*C298+(4*C297)+3*C296+2*C295)/12","v":67.710107999607303},67.792259216744114,65.861508487016522,65.899584099487797,65.622219869665457,65.547601700452688,65.464755295061437,65.054751477447809,65.924721365376456,66.763306949292812,67.19416692255551,68.474148780514497,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,{"$f":"(3*C299+(4*C298)+3*C297+2*C296)/12","v":67.529176207770391},68.6817531174582,67.103891655544018,66.885829867907958,66.680695880453342,66.501604159756752,66.432860274769695,66.252918811194789,67.185968979355749,67.912913778888665,68.412606488641657,68.732522537955532,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,{"$f":"(3*C300+(4*C299)+3*C298+2*C297)/12","v":66.712879179649192},69.390840055408461,68.588167183478632,68.001068689878792,67.970377605366068,67.784183519284156,67.739793428673281,67.712568447761882,68.462040470859733,68.915077885534359,69.408651925034022,68.259455009256442,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,{"$f":"(3*C301+(4*C300)+3*C299+2*C298)/12","v":65.514760568121389},69.425035838751938,69.859062531334217,68.841171561022932,69.012756644943664,68.883056458674687,68.861122390362794,68.89153998479064,69.354187601614399,69.507672869898784,70.141711183926972,67.103983401878125,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"Balance Point Temperature",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,1,{"$f":"(3*C307+(4*C330)+3*C329+2*C328)/12","v":65.864529143741493},{"$f":"(3*D307+(4*D330)+3*D329+2*D328)/12","v":69.09933187818514},69.294400834193326,68.426677975225473,68.517091513620741,68.38152023103585,68.349640472585691,68.330290088628175,68.880578970201654,69.144383994847885,69.806798902390867,67.305430872757213,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,2,{"$f":"(3*C308+(4*C307)+3*C330+2*C329)/12","v":64.846902458819059},{"$f":"(3*D308+(4*D307)+3*D330+2*D329)/12","v":68.621735059673668},70.246980896835453,69.053999246538822,69.263164055737917,69.17312987148658,69.15708467145582,69.173175749001118,69.501897054384827,69.523237874105021,70.439291491735688,66.145104197516517,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,3,{"$f":"(3*C309+(4*C308)+3*C307+2*C330)/12","v":63.99075608895577},{"$f":"(3*D309+(4*D308)+3*D307+2*D330)/12","v":67.583785017650769},70.826903687729782,69.466249388431564,69.697328022501381,69.651654940713271,69.645292193710233,69.662837027849562,69.819463696384574,69.655538538171697,70.889809572395521,64.964468168645084,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,4,{"$f":"(3*C310+(4*C309)+3*C308+2*C307)/12","v":63.425981839195742},{"$f":"(3*D310+(4*D309)+3*D308+2*D307)/12","v":66.266894424476632},71.047130195915898,69.759555249822469,69.894134361246131,69.876826039322737,69.874931220335398,69.88414121448811,69.941309564268437,69.677742422860248,71.158626842457863,64.027332309113731,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,5,{"$f":"(3*C311+(4*C310)+3*C309+2*C308)/12","v":63.132562517326882},65.004173952524539,70.962611608283723,70.022682079348371,69.961257135641333,69.956689805514515,69.95631535574509,69.959295928413312,69.974138991240679,69.709395148317029,71.200624006612614,63.433366036878276,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,6,{"$f":"(3*C312+(4*C311)+3*C310+2*C309)/12","v":63.017001847920113},64.036014468202936,70.595969646493643,70.293073763389359,69.972253642652404,69.974699262724258,69.975304667454182,69.976320321478255,69.974613904508416,69.812730142648618,70.93074508831684,63.133128391129979,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,7,{"$f":"(3*C313+(4*C312)+3*C311+2*C310)/12","v":62.984116007264475},63.433045919657438,69.920100672463093,70.556348893803118,69.939698857518891,69.955301677695545,69.961195526261676,69.965048885635483,69.945686412578155,69.986621008473179,70.26968089904264,63.01628020270558,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,8,{"$f":"(3*C314+(4*C313)+3*C312+2*C311)/12","v":62.967488511489712},63.114975248973302,68.911220680919655,70.73751207035248,69.810569014492089,69.849296291661005,69.872752858235813,69.885152193682174,69.839653880733792,70.163299488926228,69.205365784612596,62.971100674043299,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,9,{"$f":"(3*C315+(4*C314)+3*C313+2*C312)/12","v":62.903092551023242},62.918276713552693,67.64754844718918,70.697383393342321,69.486078478358252,69.549304556411286,69.605895476133355,69.629561238848439,69.564715720179933,70.208348471387922,67.87405182130901,62.89984794011756,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,10,{"$f":"(3*C316+(4*C315)+3*C314+2*C313)/12","v":62.703556235230245},62.693611430200853,66.361936016192018,70.300709246922466,68.903035056324711,68.972736340504881,69.068892528356855,69.095730640427206,69.048978959871235,69.974432326956517,66.55394847375139,62.707789142696917,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,11,{"$f":"(3*C317+(4*C316)+3*C315+2*C314)/12","v":62.283075660306913},62.426796646191825,65.38979181111857,69.5442002727047,68.135034099211239,68.178077871943159,68.300188748202032,68.305653597614423,68.333576122233069,69.411653669747039,65.541861009327704,62.341235371020296,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,12,{"$f":"(3*C318+(4*C317)+3*C316+2*C315)/12","v":61.641960973029292},62.289780412539493,65.026361967864872,68.632848002072066,67.413217440159045,67.402022128305973,67.517738751198365,67.470228581823818,67.612011276678444,68.6500530135432,64.995142134533452,61.861491025872688,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,13,{"$f":"(3*C319+(4*C318)+3*C317+2*C316)/12","v":60.947258651907447},62.576923360464036,65.376335557217914,67.912222406492972,67.027673053160228,66.958291499580028,67.035072182009074,66.915310772541233,67.16252379255711,67.97048939594896,64.845098317736074,61.464272489755039,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,14,{"$f":"(3*C320+(4*C319)+3*C318+2*C317)/12","v":60.503747751324958},63.500937662130646,66.302129668201886,67.66044777925238,67.143856177990685,67.039171320905055,67.063673295419235,66.880740197894198,67.177076190712185,67.633249657145356,64.880190398573902,61.408650679488147,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,15,{"$f":"(3*C321+(4*C320)+3*C319+2*C318)/12","v":60.608439398897936},64.985192832144591,67.463238907802818,67.896628182919514,67.675876092727549,67.575784712360658,67.558790364014087,67.341590268434388,67.608140581982994,67.681356447591838,64.890977267942063,61.8491856441428,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,16,{"$f":"(3*C322+(4*C321)+3*C320+2*C319)/12","v":61.355035218800793},66.633088352522336,68.42866887473771,68.347748909545814,68.302976820956246,68.253155687518088,68.219028503585122,67.979657039838756,68.146385368615029,67.887885428076046,64.778748350423925,62.721805033361584,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,17,{"$f":"(3*C323+(4*C322)+3*C321+2*C320)/12","v":62.569730752013335},67.909902778760809,68.826146108631903,68.59499238451626,68.616940281820021,68.655348398450812,68.622939598849754,68.332874402130457,68.370552643077716,67.90610766041425,64.584425742648889,63.802404853893883,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,18,{"$f":"(3*C324+(4*C323)+3*C322+2*C321)/12","v":63.937019475909779},68.459520876345849,68.495202556256785,68.334673772448113,68.349293696527624,68.487528276495937,68.460029575649386,68.065539540075108,68.013441585944506,67.534722826232709,64.44078258184588,64.857368417169013,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF($AH$29<DEGREES(BS353),0+$AJ$33,1-((TAN(BS353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BT353),0+$AJ$33,1-((TAN(BT353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BU353),0+$AJ$33,1-((TAN(BU353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BV353),0+$AJ$33,1-((TAN(BV353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BW353),0+$AJ$33,1-((TAN(BW353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BX353),0+$AJ$33,1-((TAN(BX353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BY353),0+$AJ$33,1-((TAN(BY353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(BZ353),0+$AJ$33,1-((TAN(BZ353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CA353),0+$AJ$33,1-((TAN(CA353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CB353),0+$AJ$33,1-((TAN(CB353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CC353),0+$AJ$33,1-((TAN(CC353)/TAN($AG$31))*(1-$AJ$16)))","v":1},{"$f":"IF($AH$29<DEGREES(CD353),0+$AJ$33,1-((TAN(CD353)/TAN($AG$31))*(1-$AJ$16)))","v":1}]
[null,19,{"$f":"(3*C325+(4*C324)+3*C323+2*C322)/12","v":65.190191541603895},68.322288227779225,67.598179203948561,67.580232294143883,67.542182048450456,67.747784670010859,67.715838148924988,67.191208131818243,67.166035782481003,66.889363489765444,64.517326278376302,65.787679435299751,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,20,{"$f":"(3*C326+(4*C325)+3*C324+2*C323)/12","v":66.216594813690833},67.891740894793486,66.581208288130895,66.673998682276803,66.558126748222477,66.75760922284168,66.710118847358316,66.102495128389009,66.256512466352305,66.335581544907384,64.946221628481425,66.634446983096666,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,21,{"$f":"(3*C327+(4*C326)+3*C325+2*C324)/12","v":66.974620857908647},67.646501848602298,65.965350993744423,66.082128746814618,65.88989930304362,66.005110067043006,65.94024371292997,65.356243492360178,65.790694633974226,66.23366106554117,65.747804939812326,67.432860469438069,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,22,{"$f":"(3*C328+(4*C327)+3*C326+2*C325)/12","v":67.3864185577646},67.849707697850292,66.073853544555334,66.100820811665827,65.873828445989787,65.866327760891394,65.793083902374832,65.340146034373916,66.033786898947582,66.698353468582113,66.811441745948358,68.086894347286119,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,23,{"$f":"(3*C329+(4*C328)+3*C327+2*C326)/12","v":67.336963099348978},68.407474479175505,66.880433526162719,66.697678786984113,66.51258888566089,66.403127049676584,66.335446400408543,66.062842235022686,66.872732667217562,67.548426419367487,67.945870310000018,68.382716000917426,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,24,{"$f":"(3*C330+(4*C329)+3*C328+2*C327)/12","v":66.783628587123886},68.955687126979385,68.080379022381848,67.582037270440296,67.517192311415513,67.365493277778015,67.31421935835111,67.199429427824953,67.94317286309186,68.454057115590459,68.973824546912752,68.12463628479631,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,1,1,1,1,1,1,1,1,1,1,1]

{"sheet":"Surface Solar Azimuth Angles","index":4,"n_rows":108,"n_cols":157,"rows_kept":108,"cut":false,"hidden":false,"merged":[[10,35,10,40],[19,43,19,44],[48,43,48,44],[49,43,49,44],[50,43,50,44],[51,43,51,44],[52,43,52,44],[43,43,43,44],[44,43,44,44],[45,43,45,44],[46,43,46,44],[47,43,47,44],[38,43,38,44],[39,43,39,44],[40,43,40,44],[41,43,41,44],[42,43,42,44],[33,43,33,44],[34,43,34,44],[35,43,35,44],[36,43,36,44],[37,43,37,44],[26,43,26,44],[27,43,27,44],[55,1,55,3],[55,4,55,9],[55,10,55,13],[1,4,1,9],[1,10,1,13],[1,1,1,3],[27,8,27,12],[11,36,11,37],[19,34,19,42],[20,34,20,42],[50,34,50,42],[51,34,51,42],[52,34,52,42],[53,34,53,42],[45,34,45,42],[46,34,46,42],[4,29,5,29],[9,29,10,29],[16,34,16,42],[54,34,54,42],[30,34,30,42],[31,34,31,42],[32,34,32,42],[33,34,33,42],[81,81,81,85],[81,95,81,99],[14,29,15,29],[1,97,1,100],[27,81,27,85],[27,95,27,99],[55,74,55,76],[55,77,55,82],[27,34,27,42],[28,34,28,42],[29,34,29,42],[7,31,18,31],[1,31,2,44],[41,34,41,42],[42,34,42,42],[43,34,43,42],[44,34,44,42],[35,34,35,42],[36,34,36,42],[37,34,37,42],[38,34,38,42],[31,43,31,44],[32,43,32,44],[34,34,34,42],[64,34,64,42],[64,43,64,44],[65,34,65,42],[65,43,65,44],[66,34,66,42],[66,43,66,44],[28,43,28,44],[29,43,29,44],[30,43,30,44],[47,34,47,42],[48,34,48,42],[49,34,49,42],[40,34,40,42],[54,43,54,44],[59,34,59,42],[59,43,59,44],[60,34,60,42],[60,43,60,44],[61,34,61,42],[61,43,61,44],[57,43,57,44],[58,34,58,42],[58,43,58,44],[55,97,55,100],[1,74,1,76],[1,77,1,82],[1,83,1,86],[1,88,1,90],[1,91,1,96],[81,8,81,12],[81,22,81,26],[9,41,9,42],[11,41,11,42],[1,18,1,23],[1,24,1,27],[55,15,55,17],[55,18,55,23],[55,24,55,27],[1,15,1,17],[27,22,27,26],[4,34,4,43],[39,34,39,42],[55,34,55,42],[20,43,20,44],[26,34,26,42],[53,43,53,44],[63,43,63,44],[55,83,55,86],[55,88,55,90],[55,91,55,96],[72,34,72,42],[72,43,72,44],[73,34,73,42],[73,43,73,44],[55,43,55,44],[56,34,56,42],[56,43,56,44],[67,34,67,42],[67,43,67,44],[68,34,68,42],[68,43,68,44],[69,34,69,42],[69,43,69,44],[70,34,70,42],[70,43,70,44],[71,34,71,42],[71,43,71,44],[62,34,62,42],[62,43,62,44],[63,34,63,42],[57,34,57,42]]}
[]
[null,"Table 5:",null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,"South Surface Azimuth Angles",null,null,null,null,"Table 6:",null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,"East Surface Azimuth Angles",null,null,null,null,null,null,"WINDOW PLAN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Table 5:",null,null,"Shading Coefficients",null,null,null,null,null,"South Surface Azimuth Angles",null,null,null,null,"Table 6:",null,null,"Shading Coefficients",null,null,null,null,null,"East Surface Azimuth Angles"]
[null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$f":"'Profile angles'!B4","v":"HR"},{"$f":"'Profile angles'!C4","v":"Jan"},{"$f":"'Profile angles'!D4","v":"Feb"},{"$f":"'Profile angles'!E4","v":"Mar"},{"$f":"'Profile angles'!F4","v":"Apr"},{"$f":"'Profile angles'!G4","v":"May"},{"$f":"'Profile angles'!H4","v":"Jun"},{"$f":"'Profile angles'!I4","v":"Jul"},{"$f":"'Profile angles'!J4","v":"Aug"},{"$f":"'Profile angles'!K4","v":"Sep"},{"$f":"'Profile angles'!L4","v":"Oct"},{"$f":"'Profile angles'!M4","v":"Nov"},{"$f":"'Profile angles'!N4","v":"Dec"},null,{"$f":"'Profile angles'!B33","v":"HR"},{"$f":"'Profile angles'!C33","v":"Jan"},{"$f":"'Profile angles'!D33","v":"Feb"},{"$f":"'Profile angles'!E33","v":"Mar"},{"$f":"'Profile angles'!F33","v":"Apr"},{"$f":"'Profile angles'!G33","v":"May"},{"$f":"'Profile angles'!H33","v":"Jun"},{"$f":"'Profile angles'!I33","v":"Jul"},{"$f":"'Profile angles'!J33","v":"Aug"},{"$f":"'Profile angles'!K33","v":"Sep"},{"$f":"'Profile angles'!L33","v":"Oct"},{"$f":"'Profile angles'!M33","v":"Nov"},{"$f":"'Profile angles'!N33","v":"Dec"},null,{"$error":"#REF!"},"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$f":"EA3","v":{"$error":"#REF!"}},{"$f":"EB3","v":"Jan"},"Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"('Solar Azimuth'!C3-'Input Data'!$F$9)","v":114.42309856189749},{"$f":"('Solar Azimuth'!D3-'Input Data'!$F$9)","v":145.01866125000959},{"$f":"('Solar Azimuth'!E3-'Input Data'!$F$9)","v":154.35900651846384},{"$f":"('Solar Azimuth'!F3-'Input Data'!$F$9)","v":158.68036485144134},{"$f":"('Solar Azimuth'!G3-'Input Data'!$F$9)","v":161.88012117394979},{"$f":"('Solar Azimuth'!H3-'Input Data'!$F$9)","v":164.47228133381614},{"$f":"('Solar Azimuth'!I3-'Input Data'!$F$9)","v":164.88960695959625},{"$f":"('Solar Azimuth'!J3-'Input Data'!$F$9)","v":160.07401314187376},{"$f":"('Solar Azimuth'!K3-'Input Data'!$F$9)","v":147.16438917420371},{"$f":"('Solar Azimuth'!L3-'Input Data'!$F$9)","v":127.81849177627836},{"$f":"('Solar Azimuth'!M3-'Input Data'!$F$9)","v":103.98661304621145},{"$f":"('Solar Azimuth'!N3-'Input Data'!$F$9)","v":92.926107523614064},null,1,{"$f":"('Solar Azimuth'!C3-('Input Data'!$F$9+90))","v":24.42309856189749},{"$f":"('Solar Azimuth'!D3-('Input Data'!$F$9+90))","v":55.018661250009586},{"$f":"('Solar Azimuth'!E3-('Input Data'!$F$9+90))","v":64.359006518463843},{"$f":"('Solar Azimuth'!F3-('Input Data'!$F$9+90))","v":68.68036485144134},{"$f":"('Solar Azimuth'!G3-('Input Data'!$F$9+90))","v":71.880121173949789},{"$f":"('Solar Azimuth'!H3-('Input Data'!$F$9+90))","v":74.472281333816142},{"$f":"('Solar Azimuth'!I3-('Input Data'!$F$9+90))","v":74.88960695959625},{"$f":"('Solar Azimuth'!J3-('Input Data'!$F$9+90))","v":70.074013141873763},{"$f":"('Solar Azimuth'!K3-('Input Data'!$F$9+90))","v":57.164389174203706},{"$f":"('Solar Azimuth'!L3-('Input Data'!$F$9+90))","v":37.818491776278364},{"$f":"('Solar Azimuth'!M3-('Input Data'!$F$9+90))","v":13.986613046211446},{"$f":"('Solar Azimuth'!N3-('Input Data'!$F$9+90))","v":2.9261075236140641},null,"Azimuth Cutoff",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-C4)))/SIN(RADIANS(90-C4))))","v":4.4042550408088728},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-D4)))/SIN(RADIANS(90-D4))))","v":1.399444521672393},0.95999946988969542,0.78055710398794997,0.65446888269106385,0.55569120627860624,0.5400306321924575,0.725016042310203,1.2906720722658629,2.5766668869984195,8.0295536918245194,39.127720412584544,null,1,{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-Q4)))/SIN(RADIANS(90-Q4))))","v":0.90821261778368101},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-R4)))/SIN(RADIANS(90-R4))))","v":2.8582769363517437},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-S4)))/SIN(RADIANS(90-S4))))","v":4.1666689674939112},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-T4)))/SIN(RADIANS(90-T4))))","v":5.1245449942913481},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-U4)))/SIN(RADIANS(90-U4))))","v":6.1118261017279893},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-V4)))/SIN(RADIANS(90-V4))))","v":7.1982423957857753},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-W4)))/SIN(RADIANS(90-W4))))","v":7.4069872365582157},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-X4)))/SIN(RADIANS(90-X4))))","v":5.5171193002217382},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-Y4)))/SIN(RADIANS(90-Y4))))","v":3.0991605737449071},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-Z4)))/SIN(RADIANS(90-Z4))))","v":1.5523931402167526},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-AA4)))/SIN(RADIANS(90-AA4))))","v":0.49815969274515159},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-AB4)))/SIN(RADIANS(90-AB4))))","v":0.10222931358693441},null,1,{"$f":"IF(AV4>$AG$6, $AD$17, (1-(AV4/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0},{"$f":"IF(AW4>$AG$6, $AD$17, (1-(AW4/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0.6501388695819017},0.76000013252757614,0.80486072400301256,0.83638277932723404,0.86107719843034847,0.86499234195188568,0.81874598942244925,0.67733198193353428,0.35583327825039512,0,0,null,1,{"$f":"IF(BJ4>$AG$6, $AD$17, (1-(BJ4/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.77294684555407978},{"$f":"IF(BK4>$AG$6, $AD$17, (1-(BK4/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.28543076591206407},0,0,0,0,0,0,0.22520985656377324,0.61190171494581191,0.87546007681371207,0.97444267160326636,null,{"$f":"'Profile angles'!B5","v":1},{"$f":"IF('Profile angles'!C5<0,1000,IF(EB4<0,1000,'Profile angles'!C5))","v":1000},{"$f":"IF('Profile angles'!D5<0,1000,IF(EC4<0,1000,'Profile angles'!D5))","v":1000},{"$f":"IF('Profile angles'!E5<0,1000,IF(ED4<0,1000,'Profile angles'!E5))","v":1000},{"$f":"IF('Profile angles'!F5<0,1000,IF(EE4<0,1000,'Profile angles'!F5))","v":1000},{"$f":"IF('Profile angles'!G5<0,1000,IF(EF4<0,1000,'Profile angles'!G5))","v":1000},{"$f":"IF('Profile angles'!H5<0,1000,IF(EG4<0,1000,'Profile angles'!H5))","v":1000},{"$f":"IF('Profile angles'!I5<0,1000,IF(EH4<0,1000,'Profile angles'!I5))","v":1000},{"$f":"IF('Profile angles'!J5<0,1000,IF(EI4<0,1000,'Profile angles'!J5))","v":1000},{"$f":"IF('Profile angles'!K5<0,1000,IF(EJ4<0,1000,'Profile angles'!K5))","v":1000},{"$f":"IF('Profile angles'!L5<0,1000,IF(EK4<0,1000,'Profile angles'!L5))","v":1000},{"$f":"IF('Profile angles'!M5<0,1000,IF(EL4<0,1000,'Profile angles'!M5))","v":1000},{"$f":"IF('Profile angles'!N5<0,1000,IF(EM4<0,1000,'Profile angles'!N5))","v":1000},null,{"$f":"'Profile angles'!B34","v":1},{"$f":"IF('Profile angles'!C34<0,1000,IF(EB4<0,1000,'Profile angles'!C34))","v":1000},{"$f":"IF('Profile angles'!D34<0,1000,IF(EC4<0,1000,'Profile angles'!D34))","v":1000},{"$f":"IF('Profile angles'!E34<0,1000,IF(ED4<0,1000,'Profile angles'!E34))","v":1000},{"$f":"IF('Profile angles'!F34<0,1000,IF(EE4<0,1000,'Profile angles'!F34))","v":1000},{"$f":"IF('Profile angles'!G34<0,1000,IF(EF4<0,1000,'Profile angles'!G34))","v":1000},{"$f":"IF('Profile angles'!H34<0,1000,IF(EG4<0,1000,'Profile angles'!H34))","v":1000},{"$f":"IF('Profile angles'!I34<0,1000,IF(EH4<0,1000,'Profile angles'!I34))","v":1000},{"$f":"IF('Profile angles'!J34<0,1000,IF(EI4<0,1000,'Profile angles'!J34))","v":1000},{"$f":"IF('Profile angles'!K34<0,1000,IF(EJ4<0,1000,'Profile angles'!K34))","v":1000},{"$f":"IF('Profile angles'!L34<0,1000,IF(EK4<0,1000,'Profile angles'!L34))","v":1000},{"$f":"IF('Profile angles'!M34<0,1000,IF(EL4<0,1000,'Profile angles'!M34))","v":1000},{"$f":"IF('Profile angles'!N34<0,1000,IF(EM4<0,1000,'Profile angles'!N34))","v":1000},null,1,{"$f":"'Solar Altitude'!C4","v":-79.238745258454912},{"$f":"'Solar Altitude'!D4","v":-73.135890206899091},{"$f":"'Solar Altitude'!E4","v":-62.969753990761212},{"$f":"'Solar Altitude'!F4","v":-51.103815741194268},{"$f":"'Solar Altitude'!G4","v":-42.972420763986918},{"$f":"'Solar Altitude'!H4","v":-40.259838967181594},{"$f":"'Solar Altitude'!I4","v":-43.397326661656273},{"$f":"'Solar Altitude'!J4","v":-51.194813940312706},{"$f":"'Solar Altitude'!K4","v":-61.30334441705341},{"$f":"'Solar Altitude'!L4","v":-68.588756925018274},{"$f":"'Solar Altitude'!M4","v":-73.864057818332},{"$f":"'Solar Altitude'!N4","v":-77.510392918823513},null,{"$f":"EA4","v":1},{"$f":"EB4","v":-79.238745258454912},{"$f":"EC4","v":-73.135890206899091},{"$f":"ED4","v":-62.969753990761212},{"$f":"EE4","v":-51.103815741194268},{"$f":"EF4","v":-42.972420763986918},{"$f":"EG4","v":-40.259838967181594},{"$f":"EH4","v":-43.397326661656273},{"$f":"EI4","v":-51.194813940312706},{"$f":"EJ4","v":-61.30334441705341},{"$f":"EK4","v":-68.588756925018274},{"$f":"EL4","v":-73.864057818332},{"$f":"EM4","v":-77.510392918823513}]
[null,2,{"$f":"('Solar Azimuth'!C4-'Input Data'!$F$9)","v":96.453295295662869},{"$f":"('Solar Azimuth'!D4-'Input Data'!$F$9)","v":116.58936603917034},{"$f":"('Solar Azimuth'!E4-'Input Data'!$F$9)","v":130.1624952301172},{"$f":"('Solar Azimuth'!F4-'Input Data'!$F$9)","v":139.50906482919788},{"$f":"('Solar Azimuth'!G4-'Input Data'!$F$9)","v":145.31232618983634},{"$f":"('Solar Azimuth'!H4-'Input Data'!$F$9)","v":148.52493328219171},{"$f":"('Solar Azimuth'!I4-'Input Data'!$F$9)","v":147.81507211585009},{"$f":"('Solar Azimuth'!J4-'Input Data'!$F$9)","v":140.63416607539401},{"$f":"('Solar Azimuth'!K4-'Input Data'!$F$9)","v":125.79538213031562},{"$f":"('Solar Azimuth'!L4-'Input Data'!$F$9)","v":108.96560729234663},{"$f":"('Solar Azimuth'!M4-'Input Data'!$F$9)","v":92.920040610035116},{"$f":"('Solar Azimuth'!N4-'Input Data'!$F$9)","v":86.74169228845723},null,2,{"$f":"('Solar Azimuth'!C4-('Input Data'!$F$9+90))","v":6.4532952956628691},{"$f":"('Solar Azimuth'!D4-('Input Data'!$F$9+90))","v":26.589366039170343},{"$f":"('Solar Azimuth'!E4-('Input Data'!$F$9+90))","v":40.162495230117202},{"$f":"('Solar Azimuth'!F4-('Input Data'!$F$9+90))","v":49.509064829197882},{"$f":"('Solar Azimuth'!G4-('Input Data'!$F$9+90))","v":55.312326189836341},{"$f":"('Solar Azimuth'!H4-('Input Data'!$F$9+90))","v":58.524933282191711},{"$f":"('Solar Azimuth'!I4-('Input Data'!$F$9+90))","v":57.815072115850086},{"$f":"('Solar Azimuth'!J4-('Input Data'!$F$9+90))","v":50.634166075394006},{"$f":"('Solar Azimuth'!K4-('Input Data'!$F$9+90))","v":35.795382130315616},{"$f":"('Solar Azimuth'!L4-('Input Data'!$F$9+90))","v":18.965607292346633},{"$f":"('Solar Azimuth'!M4-('Input Data'!$F$9+90))","v":2.9200406100351159},{"$f":"('Solar Azimuth'!N4-('Input Data'!$F$9+90))","v":-3.2583077115427699},null,{"$f":"AR25","v":63.43494882292201},null,null,null,null,"Window Width",null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-C5)))/SIN(RADIANS(90-C5))))","v":17.681910045371961},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-D5)))/SIN(RADIANS(90-D5))))","v":3.9957598545570217},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-E5)))/SIN(RADIANS(90-E5))))","v":2.3698252115741352},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-F5)))/SIN(RADIANS(90-F5))))","v":1.7076142072221561},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-G5)))/SIN(RADIANS(90-G5))))","v":1.3842291894580696},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-H5)))/SIN(RADIANS(90-H5))))","v":1.2244047269763718},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-I5)))/SIN(RADIANS(90-I5))))","v":1.2587325838462309},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-J5)))/SIN(RADIANS(90-J5))))","v":1.6408222005480091},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-K5)))/SIN(RADIANS(90-K5))))","v":2.7735395285704199},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-L5)))/SIN(RADIANS(90-L5))))","v":5.8197678842776277},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-M5)))/SIN(RADIANS(90-M5))))","v":39.209156722249617},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-N5)))/SIN(RADIANS(90-N5))))","v":35.131121160954237},null,2,{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-Q5)))/SIN(RADIANS(90-Q5))))","v":0.22621990439584636},1.0010611612302331,1.6878881954939771,2.3424494731201366,2.8896948788993631,3.2668936274673417,3.1777996782902433,2.4378022180977692,1.4422004657931597,0.68731263506336493,0.10201698619369086,0.11385916155860457,null,2,{"$f":"IF(AV5>$AG$6, $AD$17, (1-(AV5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0},{"$f":"IF(AW5>$AG$6, $AD$17, (1-(AW5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":1.0600363607445873E-3},{"$f":"IF(AX5>$AG$6, $AD$17, (1-(AX5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0.40754369710646621},{"$f":"IF(AY5>$AG$6, $AD$17, (1-(AY5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0.57309644819446093},{"$f":"IF(AZ5>$AG$6, $AD$17, (1-(AZ5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0.6539427026354826},{"$f":"IF(BA5>$AG$6, $AD$17, (1-(BA5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0.69389881825590705},{"$f":"IF(BB5>$AG$6, $AD$17, (1-(BB5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0.68531685403844222},{"$f":"IF(BC5>$AG$6, $AD$17, (1-(BC5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0.58979444986299767},{"$f":"IF(BD5>$AG$6, $AD$17, (1-(BD5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0.30661511785739504},{"$f":"IF(BE5>$AG$6, $AD$17, (1-(BE5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0},{"$f":"IF(BF5>$AG$6, $AD$17, (1-(BF5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0},{"$f":"IF(BG5>$AG$6, $AD$17, (1-(BG5/$AG$6)*(1-$AD$17)))*$AF$23+(1-$AF$23)","v":0},null,2,{"$f":"IF(BJ5>$AG$6, $AD$17, (1-(BJ5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.94344502390103846},{"$f":"IF(BK5>$AG$6, $AD$17, (1-(BK5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.74973470969244171},{"$f":"IF(BL5>$AG$6, $AD$17, (1-(BL5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.57802795112650573},{"$f":"IF(BM5>$AG$6, $AD$17, (1-(BM5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.41438763171996584},{"$f":"IF(BN5>$AG$6, $AD$17, (1-(BN5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.27757628027515924},{"$f":"IF(BO5>$AG$6, $AD$17, (1-(BO5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.18327659313316458},{"$f":"IF(BP5>$AG$6, $AD$17, (1-(BP5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.20555008042743916},{"$f":"IF(BQ5>$AG$6, $AD$17, (1-(BQ5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.3905494454755577},{"$f":"IF(BR5>$AG$6, $AD$17, (1-(BR5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.63944988355171006},{"$f":"IF(BS5>$AG$6, $AD$17, (1-(BS5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.82817184123415877},{"$f":"IF(BT5>$AG$6, $AD$17, (1-(BT5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.97449575345157724},{"$f":"IF(BU5>$AG$6, $AD$17, (1-(BU5/$AG$6)*(1-$AD$17)))*$AF$25+(1-$AF$25)","v":0.97153520961034889},null,{"$f":"'Profile angles'!B6","v":2},{"$f":"IF('Profile angles'!C6<0,1000,IF(EB5<0,1000,'Profile angles'!C6))","v":1000},{"$f":"IF('Profile angles'!D6<0,1000,IF(EC5<0,1000,'Profile angles'!D6))","v":1000},{"$f":"IF('Profile angles'!E6<0,1000,IF(ED5<0,1000,'Profile angles'!E6))","v":1000},{"$f":"IF('Profile angles'!F6<0,1000,IF(EE5<0,1000,'Profile angles'!F6))","v":1000},{"$f":"IF('Profile angles'!G6<0,1000,IF(EF5<0,1000,'Profile angles'!G6))","v":1000},{"$f":"IF('Profile angles'!H6<0,1000,IF(EG5<0,1000,'Profile angles'!H6))","v":1000},{"$f":"IF('Profile angles'!I6<0,1000,IF(EH5<0,1000,'Profile angles'!I6))","v":1000},{"$f":"IF('Profile angles'!J6<0,1000,IF(EI5<0,1000,'Profile angles'!J6))","v":1000},{"$f":"IF('Profile angles'!K6<0,1000,IF(EJ5<0,1000,'Profile angles'!K6))","v":1000},{"$f":"IF('Profile angles'!L6<0,1000,IF(EK5<0,1000,'Profile angles'!L6))","v":1000},{"$f":"IF('Profile angles'!M6<0,1000,IF(EL5<0,1000,'Profile angles'!M6))","v":1000},{"$f":"IF('Profile angles'!N6<0,1000,IF(EM5<0,1000,'Profile angles'!N6))","v":1000},null,{"$f":"'Profile angles'!B35","v":2},{"$f":"IF('Profile angles'!C35<0,1000,IF(EB5<0,1000,'Profile angles'!C35))","v":1000},{"$f":"IF('Profile angles'!D35<0,1000,IF(EC5<0,1000,'Profile angles'!D35))","v":1000},{"$f":"IF('Profile angles'!E35<0,1000,IF(ED5<0,1000,'Profile angles'!E35))","v":1000},{"$f":"IF('Profile angles'!F35<0,1000,IF(EE5<0,1000,'Profile angles'!F35))","v":1000},{"$f":"IF('Profile angles'!G35<0,1000,IF(EF5<0,1000,'Profile angles'!G35))","v":1000},{"$f":"IF('Profile angles'!H35<0,1000,IF(EG5<0,1000,'Profile angles'!H35))","v":1000},{"$f":"IF('Profile angles'!I35<0,1000,IF(EH5<0,1000,'Profile angles'!I35))","v":1000},{"$f":"IF('Profile angles'!J35<0,1000,IF(EI5<0,1000,'Profile angles'!J35))","v":1000},{"$f":"IF('Profile angles'!K35<0,1000,IF(EJ5<0,1000,'Profile angles'!K35))","v":1000},{"$f":"IF('Profile angles'!L35<0,1000,IF(EK5<0,1000,'Profile angles'!L35))","v":1000},{"$f":"IF('Profile angles'!M35<0,1000,IF(EL5<0,1000,'Profile angles'!M35))","v":1000},{"$f":"IF('Profile angles'!N35<0,1000,IF(EM5<0,1000,'Profile angles'!N35))","v":1000},null,2,{"$f":"'Solar Altitude'!C5","v":-66.037221876299029},{"$f":"'Solar Altitude'!D5","v":-62.610262119735701},{"$f":"'Solar Altitude'!E5","v":-54.505603493104644},{"$f":"'Solar Altitude'!F5","v":-44.039138424385058},{"$f":"'Solar Altitude'!G5","v":-36.867903866984811},{"$f":"'Solar Altitude'!H5","v":-34.787290206430924},{"$f":"'Solar Altitude'!I5","v":-37.887883453111968},{"$f":"'Solar Altitude'!J5","v":-44.388788539159933},{"$f":"'Solar Altitude'!K5","v":-51.819137025254065},{"$f":"'Solar Altitude'!L5","v":-56.521775308526607},{"$f":"'Solar Altitude'!M5","v":-60.378308807607461},{"$f":"'Solar Altitude'!N5","v":-63.889653492857697},null,2,-66.037221876299029,-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697]
[null,3,{"$f":"('Solar Azimuth'!C5-'Input Data'!$F$9)","v":89.051635649875607},{"$f":"('Solar Azimuth'!D5-'Input Data'!$F$9)","v":103.31352191067661},{"$f":"('Solar Azimuth'!E5-'Input Data'!$F$9)","v":115.40543082307254},{"$f":"('Solar Azimuth'!F5-'Input Data'!$F$9)","v":125.70260632132135},{"$f":"('Solar Azimuth'!G5-'Input Data'!$F$9)","v":132.47437783928015},{"$f":"('Solar Azimuth'!H5-'Input Data'!$F$9)","v":135.83260490366516},{"$f":"('Solar Azimuth'!I5-'Input Data'!$F$9)","v":134.43597736215381},{"$f":"('Solar Azimuth'!J5-'Input Data'!$F$9)","v":126.56858704244209},{"$f":"('Solar Azimuth'!K5-'Input Data'!$F$9)","v":112.61329653323939},{"$f":"('Solar Azimuth'!L5-'Input Data'!$F$9)","v":98.771121643370421},{"$f":"('Solar Azimuth'!M5-'Input Data'!$F$9)","v":86.68606599673916},{"$f":"('Solar Azimuth'!N5-'Input Data'!$F$9)","v":82.439051076130838},null,3,{"$f":"('Solar Azimuth'!C5-('Input Data'!$F$9+90))","v":-0.94836435012439324},{"$f":"('Solar Azimuth'!D5-('Input Data'!$F$9+90))","v":13.313521910676613},{"$f":"('Solar Azimuth'!E5-('Input Data'!$F$9+90))","v":25.405430823072535},{"$f":"('Solar Azimuth'!F5-('Input Data'!$F$9+90))","v":35.702606321321355},{"$f":"('Solar Azimuth'!G5-('Input Data'!$F$9+90))","v":42.474377839280152},{"$f":"('Solar Azimuth'!H5-('Input Data'!$F$9+90))","v":45.832604903665157},{"$f":"('Solar Azimuth'!I5-('Input Data'!$F$9+90))","v":44.435977362153807},{"$f":"('Solar Azimuth'!J5-('Input Data'!$F$9+90))","v":36.56858704244209},{"$f":"('Solar Azimuth'!K5-('Input Data'!$F$9+90))","v":22.613296533239392},{"$f":"('Solar Azimuth'!L5-('Input Data'!$F$9+90))","v":8.7711216433704209},{"$f":"('Solar Azimuth'!M5-('Input Data'!$F$9+90))","v":-3.3139340032608402},{"$f":"('Solar Azimuth'!N5-('Input Data'!$F$9+90))","v":-7.5609489238691623},null,null,null,1,4,null,null,null,null,null,null,null,null,null,null,null,null,null,3,120.81969749776549,8.4516855754548601,4.2109600610123161,2.7830273607142901,2.184577509371135,1.9427018187758927,2.0397689808814659,2.6960891434555267,4.8015503656555749,12.962424971375222,34.54014086831954,15.067633356475556,null,3,3.3107184365148555E-2,0.47327837320601274,0.9499021463144437,1.43728374951131,1.831017660321635,2.0589881377268808,1.9610063872387353,1.4836304688624931,0.83306425953815111,0.30858423549861658,0.11580728681013655,0.26546969290840466,null,3,0,0,0,0.30424315982142747,0.45385562265721624,0.51432454530602678,0.49005775477963354,0.32597771413611831,0,0,0,0,null,3,0.99172320390871282,0.88168040669849679,0.76252446342138902,0.64067906262217256,0.54224558491959129,0.48525296556827979,0.50974840319031611,0.62909238278437674,0.7917339351154622,0.9228539411253458,0.97104817829746581,0.93363257677289879,null,{"$f":"'Profile angles'!B7","v":3},{"$f":"IF('Profile angles'!C7<0,1000,IF(EB6<0,1000,'Profile angles'!C7))","v":1000},{"$f":"IF('Profile angles'!D7<0,1000,IF(EC6<0,1000,'Profile angles'!D7))","v":1000},{"$f":"IF('Profile angles'!E7<0,1000,IF(ED6<0,1000,'Profile angles'!E7))","v":1000},{"$f":"IF('Profile angles'!F7<0,1000,IF(EE6<0,1000,'Profile angles'!F7))","v":1000},{"$f":"IF('Profile angles'!G7<0,1000,IF(EF6<0,1000,'Profile angles'!G7))","v":1000},{"$f":"IF('Profile angles'!H7<0,1000,IF(EG6<0,1000,'Profile angles'!H7))","v":1000},{"$f":"IF('Profile angles'!I7<0,1000,IF(EH6<0,1000,'Profile angles'!I7))","v":1000},{"$f":"IF('Profile angles'!J7<0,1000,IF(EI6<0,1000,'Profile angles'!J7))","v":1000},{"$f":"IF('Profile angles'!K7<0,1000,IF(EJ6<0,1000,'Profile angles'!K7))","v":1000},{"$f":"IF('Profile angles'!L7<0,1000,IF(EK6<0,1000,'Profile angles'!L7))","v":1000},{"$f":"IF('Profile angles'!M7<0,1000,IF(EL6<0,1000,'Profile angles'!M7))","v":1000},{"$f":"IF('Profile angles'!N7<0,1000,IF(EM6<0,1000,'Profile angles'!N7))","v":1000},null,{"$f":"'Profile angles'!B36","v":3},{"$f":"IF('Profile angles'!C36<0,1000,IF(EB6<0,1000,'Profile angles'!C36))","v":1000},{"$f":"IF('Profile angles'!D36<0,1000,IF(EC6<0,1000,'Profile angles'!D36))","v":1000},{"$f":"IF('Profile angles'!E36<0,1000,IF(ED6<0,1000,'Profile angles'!E36))","v":1000},{"$f":"IF('Profile angles'!F36<0,1000,IF(EE6<0,1000,'Profile angles'!F36))","v":1000},{"$f":"IF('Profile angles'!G36<0,1000,IF(EF6<0,1000,'Profile angles'!G36))","v":1000},{"$f":"IF('Profile angles'!H36<0,1000,IF(EG6<0,1000,'Profile angles'!H36))","v":1000},{"$f":"IF('Profile angles'!I36<0,1000,IF(EH6<0,1000,'Profile angles'!I36))","v":1000},{"$f":"IF('Profile angles'!J36<0,1000,IF(EI6<0,1000,'Profile angles'!J36))","v":1000},{"$f":"IF('Profile angles'!K36<0,1000,IF(EJ6<0,1000,'Profile angles'!K36))","v":1000},{"$f":"IF('Profile angles'!L36<0,1000,IF(EK6<0,1000,'Profile angles'!L36))","v":1000},{"$f":"IF('Profile angles'!M36<0,1000,IF(EL6<0,1000,'Profile angles'!M36))","v":1000},{"$f":"IF('Profile angles'!N36<0,1000,IF(EM6<0,1000,'Profile angles'!N36))","v":1000},null,3,{"$f":"'Solar Altitude'!C6","v":-52.431373562484438},{"$f":"'Solar Altitude'!D6","v":-49.776364898184575},{"$f":"'Solar Altitude'!E6","v":-43.00744408924087},{"$f":"'Solar Altitude'!F6","v":-33.970697614512481},{"$f":"'Solar Altitude'!G6","v":-27.874166624770901},{"$f":"'Solar Altitude'!H6","v":-26.397406240900974},{"$f":"'Solar Altitude'!I6","v":-29.298461575777225},{"$f":"'Solar Altitude'!J6","v":-34.480458721023354},{"$f":"'Solar Altitude'!K6","v":-39.89507498863518},{"$f":"'Solar Altitude'!L6","v":-43.286892300779471},{"$f":"'Solar Altitude'!M6","v":-46.757596903257479},{"$f":"'Solar Altitude'!N6","v":-50.32692672055552},null,3,-52.431373562484438,-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552]
[null,4,{"$f":"('Solar Azimuth'!C6-'Input Data'!$F$9)","v":83.645077965680898},{"$f":"('Solar Azimuth'!D6-'Input Data'!$F$9)","v":94.983105135991053},{"$f":"('Solar Azimuth'!E6-'Input Data'!$F$9)","v":105.54889999051608},{"$f":"('Solar Azimuth'!F6-'Input Data'!$F$9)","v":115.67424185262344},{"$f":"('Solar Azimuth'!G6-'Input Data'!$F$9)","v":122.72328942010087},{"$f":"('Solar Azimuth'!H6-'Input Data'!$F$9)","v":126.04880339758887},{"$f":"('Solar Azimuth'!I6-'Input Data'!$F$9)","v":124.27040515449995},{"$f":"('Solar Azimuth'!J6-'Input Data'!$F$9)","v":116.36534992403649},{"$f":"('Solar Azimuth'!K6-'Input Data'!$F$9)","v":103.51551123372408},{"$f":"('Solar Azimuth'!L6-'Input Data'!$F$9)","v":91.561421644549611},{"$f":"('Solar Azimuth'!M6-'Input Data'!$F$9)","v":81.563139551542861},{"$f":"('Solar Azimuth'!N6-'Input Data'!$F$9)","v":78.320210105456809},null,4,{"$f":"('Solar Azimuth'!C6-('Input Data'!$F$9+90))","v":-6.3549220343191024},{"$f":"('Solar Azimuth'!D6-('Input Data'!$F$9+90))","v":4.9831051359910532},{"$f":"('Solar Azimuth'!E6-('Input Data'!$F$9+90))","v":15.548899990516077},{"$f":"('Solar Azimuth'!F6-('Input Data'!$F$9+90))","v":25.674241852623439},{"$f":"('Solar Azimuth'!G6-('Input Data'!$F$9+90))","v":32.723289420100869},{"$f":"('Solar Azimuth'!H6-('Input Data'!$F$9+90))","v":36.04880339758887},{"$f":"('Solar Azimuth'!I6-('Input Data'!$F$9+90))","v":34.270405154499954},{"$f":"('Solar Azimuth'!J6-('Input Data'!$F$9+90))","v":26.365349924036494},{"$f":"('Solar Azimuth'!K6-('Input Data'!$F$9+90))","v":13.515511233724084},{"$f":"('Solar Azimuth'!L6-('Input Data'!$F$9+90))","v":1.5614216445496112},{"$f":"('Solar Azimuth'!M6-('Input Data'!$F$9+90))","v":-8.4368604484571392},{"$f":"('Solar Azimuth'!N6-('Input Data'!$F$9+90))","v":-11.679789894543191},null,null,null,null,2,null,null,null,null,null,null,null,null,null,null,null,null,null,4,17.957934238690431,22.938004393217032,7.1879392086947727,4.1604785876073329,3.1125364977986134,2.7478387835277731,2.935145908016155,4.0350992590224335,8.3206753801793365,73.371078315963587,13.483941801747021,9.6748191225440916,null,4,0.22274276911995736,0.17438308631516503,0.55648773366940341,0.96142785397686126,1.2851254926099849,1.4556894763908448,1.3627942614626518,0.99130151285771928,0.48073020725317467,5.4517394207762471E-2,0.29664915933423475,0.41344442199226977,null,4,0,0,0,0,0.22186587555034665,0.31304030411805672,0.26621352299596124,0,0,0,0,0,null,4,0.94431430772001068,0.95640422842120876,0.8608780665826492,0.75964303650578469,0.67871862684750384,0.63607763090228886,0.6593014346343371,0.75217462178557015,0.87981744818670637,0.98637065144805935,0.92583771016644134,0.89663889450193257,null,{"$f":"'Profile angles'!B8","v":4},{"$f":"IF('Profile angles'!C8<0,1000,IF(EB7<0,1000,'Profile angles'!C8))","v":1000},{"$f":"IF('Profile angles'!D8<0,1000,IF(EC7<0,1000,'Profile angles'!D8))","v":1000},{"$f":"IF('Profile angles'!E8<0,1000,IF(ED7<0,1000,'Profile angles'!E8))","v":1000},{"$f":"IF('Profile angles'!F8<0,1000,IF(EE7<0,1000,'Profile angles'!F8))","v":1000},{"$f":"IF('Profile angles'!G8<0,1000,IF(EF7<0,1000,'Profile angles'!G8))","v":1000},{"$f":"IF('Profile angles'!H8<0,1000,IF(EG7<0,1000,'Profile angles'!H8))","v":1000},{"$f":"IF('Profile angles'!I8<0,1000,IF(EH7<0,1000,'Profile angles'!I8))","v":1000},{"$f":"IF('Profile angles'!J8<0,1000,IF(EI7<0,1000,'Profile angles'!J8))","v":1000},{"$f":"IF('Profile angles'!K8<0,1000,IF(EJ7<0,1000,'Profile angles'!K8))","v":1000},{"$f":"IF('Profile angles'!L8<0,1000,IF(EK7<0,1000,'Profile angles'!L8))","v":1000},{"$f":"IF('Profile angles'!M8<0,1000,IF(EL7<0,1000,'Profile angles'!M8))","v":1000},{"$f":"IF('Profile angles'!N8<0,1000,IF(EM7<0,1000,'Profile angles'!N8))","v":1000},null,{"$f":"'Profile angles'!B37","v":4},{"$f":"IF('Profile angles'!C37<0,1000,IF(EB7<0,1000,'Profile angles'!C37))","v":1000},{"$f":"IF('Profile angles'!D37<0,1000,IF(EC7<0,1000,'Profile angles'!D37))","v":1000},{"$f":"IF('Profile angles'!E37<0,1000,IF(ED7<0,1000,'Profile angles'!E37))","v":1000},{"$f":"IF('Profile angles'!F37<0,1000,IF(EE7<0,1000,'Profile angles'!F37))","v":1000},{"$f":"IF('Profile angles'!G37<0,1000,IF(EF7<0,1000,'Profile angles'!G37))","v":1000},{"$f":"IF('Profile angles'!H37<0,1000,IF(EG7<0,1000,'Profile angles'!H37))","v":1000},{"$f":"IF('Profile angles'!I37<0,1000,IF(EH7<0,1000,'Profile angles'!I37))","v":1000},{"$f":"IF('Profile angles'!J37<0,1000,IF(EI7<0,1000,'Profile angles'!J37))","v":1000},{"$f":"IF('Profile angles'!K37<0,1000,IF(EJ7<0,1000,'Profile angles'!K37))","v":1000},{"$f":"IF('Profile angles'!L37<0,1000,IF(EK7<0,1000,'Profile angles'!L37))","v":1000},{"$f":"IF('Profile angles'!M37<0,1000,IF(EL7<0,1000,'Profile angles'!M37))","v":1000},{"$f":"IF('Profile angles'!N37<0,1000,IF(EM7<0,1000,'Profile angles'!N37))","v":1000},null,4,{"$f":"'Solar Altitude'!C7","v":-38.837571781392398},{"$f":"'Solar Altitude'!D7","v":-36.325136967893741},{"$f":"'Solar Altitude'!E7","v":-30.23387910899125},{"$f":"'Solar Altitude'!F7","v":-22.236891602714234},{"$f":"'Solar Altitude'!G7","v":-17.058579195686843},{"$f":"'Solar Altitude'!H7","v":-16.082853037589089},{"$f":"'Solar Altitude'!I7","v":-18.740224973134019},{"$f":"'Solar Altitude'!J7","v":-22.841111056638525},{"$f":"'Solar Altitude'!K7","v":-26.935985833021629},{"$f":"'Solar Altitude'!L7","v":-29.720493919992279},{"$f":"'Solar Altitude'!M7","v":-33.206986937806654},{"$f":"'Solar Altitude'!N7","v":-36.893522726896833},null,4,-38.837571781392398,-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833]
[null,5,{"$f":"('Solar Azimuth'!C7-'Input Data'!$F$9)","v":78.667572941814512},{"$f":"('Solar Azimuth'!D7-'Input Data'!$F$9)","v":88.453088384837585},{"$f":"('Solar Azimuth'!E7-'Input Data'!$F$9)","v":98.0315040139551},{"$f":"('Solar Azimuth'!F7-'Input Data'!$F$9)","v":107.92784498628035},{"$f":"('Solar Azimuth'!G7-'Input Data'!$F$9)","v":115.12801284478837},{"$f":"('Solar Azimuth'!H7-'Input Data'!$F$9)","v":118.42261537221856},{"$f":"('Solar Azimuth'!I7-'Input Data'!$F$9)","v":116.3954983583661},{"$f":"('Solar Azimuth'!J7-'Input Data'!$F$9)","v":108.51604214772064},{"$f":"('Solar Azimuth'!K7-'Input Data'!$F$9)","v":96.348104005150986},{"$f":"('Solar Azimuth'!L7-'Input Data'!$F$9)","v":85.416260532668915},{"$f":"('Solar Azimuth'!M7-'Input Data'!$F$9)","v":76.561191142844791},{"$f":"('Solar Azimuth'!N7-'Input Data'!$F$9)","v":73.938144334618258},null,5,{"$f":"('Solar Azimuth'!C7-('Input Data'!$F$9+90))","v":-11.332427058185488},{"$f":"('Solar Azimuth'!D7-('Input Data'!$F$9+90))","v":-1.5469116151624149},{"$f":"('Solar Azimuth'!E7-('Input Data'!$F$9+90))","v":8.0315040139551002},{"$f":"('Solar Azimuth'!F7-('Input Data'!$F$9+90))","v":17.927844986280348},{"$f":"('Solar Azimuth'!G7-('Input Data'!$F$9+90))","v":25.128012844788373},{"$f":"('Solar Azimuth'!H7-('Input Data'!$F$9+90))","v":28.422615372218559},{"$f":"('Solar Azimuth'!I7-('Input Data'!$F$9+90))","v":26.395498358366098},{"$f":"('Solar Azimuth'!J7-('Input Data'!$F$9+90))","v":18.51604214772064},{"$f":"('Solar Azimuth'!K7-('Input Data'!$F$9+90))","v":6.3481040051509865},{"$f":"('Solar Azimuth'!L7-('Input Data'!$F$9+90))","v":-4.5837394673310854},{"$f":"('Solar Azimuth'!M7-('Input Data'!$F$9+90))","v":-13.438808857155209},{"$f":"('Solar Azimuth'!N7-('Input Data'!$F$9+90))","v":-16.061855665381742},null,null,null,"Shade Depth",null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,9.9796245594146473,74.059638237076911,14.174184981987681,6.1818457288801234,4.2641144214942193,3.6954355051440544,4.0297688233982765,5.9718127548691786,17.977380536659624,24.946222456441326,8.3699692169701958,6.9465163476798146,null,5,0.40081668164825418,5.4010525776474243E-2,0.28220317465047434,0.64705594015601919,0.93806113171755146,1.0824164011067143,0.99261277142613535,0.66981336558795468,0.22250182621673756,0.16034491823298747,0.47789900969886012,0.57582819931547824,null,5,0,0,0,0,0,7.6141123713986403E-2,0,0,0,0,0,0,null,5,0.89979582958793647,0.98649736855588144,0.92944920633738137,0.8382360149609952,0.76548471707061216,0.72939589972332142,0.75184680714346619,0.83254665860301136,0.94437454344581562,0.95991377044175308,0.88052524757528494,0.85604295017113041,null,{"$f":"'Profile angles'!B9","v":5},{"$f":"IF('Profile angles'!C9<0,1000,IF(EB8<0,1000,'Profile angles'!C9))","v":1000},{"$f":"IF('Profile angles'!D9<0,1000,IF(EC8<0,1000,'Profile angles'!D9))","v":1000},{"$f":"IF('Profile angles'!E9<0,1000,IF(ED8<0,1000,'Profile angles'!E9))","v":1000},{"$f":"IF('Profile angles'!F9<0,1000,IF(EE8<0,1000,'Profile angles'!F9))","v":1000},{"$f":"IF('Profile angles'!G9<0,1000,IF(EF8<0,1000,'Profile angles'!G9))","v":1000},{"$f":"IF('Profile angles'!H9<0,1000,IF(EG8<0,1000,'Profile angles'!H9))","v":1000},{"$f":"IF('Profile angles'!I9<0,1000,IF(EH8<0,1000,'Profile angles'!I9))","v":1000},{"$f":"IF('Profile angles'!J9<0,1000,IF(EI8<0,1000,'Profile angles'!J9))","v":1000},{"$f":"IF('Profile angles'!K9<0,1000,IF(EJ8<0,1000,'Profile angles'!K9))","v":1000},{"$f":"IF('Profile angles'!L9<0,1000,IF(EK8<0,1000,'Profile angles'!L9))","v":1000},{"$f":"IF('Profile angles'!M9<0,1000,IF(EL8<0,1000,'Profile angles'!M9))","v":1000},{"$f":"IF('Profile angles'!N9<0,1000,IF(EM8<0,1000,'Profile angles'!N9))","v":1000},null,{"$f":"'Profile angles'!B38","v":5},{"$f":"IF('Profile angles'!C38<0,1000,IF(EB8<0,1000,'Profile angles'!C38))","v":1000},{"$f":"IF('Profile angles'!D38<0,1000,IF(EC8<0,1000,'Profile angles'!D38))","v":1000},{"$f":"IF('Profile angles'!E38<0,1000,IF(ED8<0,1000,'Profile angles'!E38))","v":1000},{"$f":"IF('Profile angles'!F38<0,1000,IF(EE8<0,1000,'Profile angles'!F38))","v":1000},{"$f":"IF('Profile angles'!G38<0,1000,IF(EF8<0,1000,'Profile angles'!G38))","v":1000},{"$f":"IF('Profile angles'!H38<0,1000,IF(EG8<0,1000,'Profile angles'!H38))","v":1000},{"$f":"IF('Profile angles'!I38<0,1000,IF(EH8<0,1000,'Profile angles'!I38))","v":1000},{"$f":"IF('Profile angles'!J38<0,1000,IF(EI8<0,1000,'Profile angles'!J38))","v":1000},{"$f":"IF('Profile angles'!K38<0,1000,IF(EJ8<0,1000,'Profile angles'!K38))","v":1000},{"$f":"IF('Profile angles'!L38<0,1000,IF(EK8<0,1000,'Profile angles'!L38))","v":1000},{"$f":"IF('Profile angles'!M38<0,1000,IF(EL8<0,1000,'Profile angles'!M38))","v":1000},{"$f":"IF('Profile angles'!N38<0,1000,IF(EM8<0,1000,'Profile angles'!N38))","v":1000},null,5,{"$f":"'Solar Altitude'!C8","v":-25.376333918471747},{"$f":"'Solar Altitude'!D8","v":-22.7103856061896},{"$f":"'Solar Altitude'!E8","v":-16.897092448538263},{"$f":"'Solar Altitude'!F8","v":-9.5810693067706811},{"$f":"'Solar Altitude'!G8","v":-5.1231262317655331},{"$f":"'Solar Altitude'!H8","v":-4.54535827775074},{"$f":"'Solar Altitude'!I8","v":-6.9688312964780383},{"$f":"'Solar Altitude'!J8","v":-10.241982624949756},{"$f":"'Solar Altitude'!K8","v":-13.517063375335365},{"$f":"'Solar Altitude'!L8","v":-16.104385171900024},{"$f":"'Solar Altitude'!M8","v":-19.830528453312528},{"$f":"'Solar Altitude'!N8","v":-23.664530366970006},null,5,-25.376333918471747,-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006]
[null,6,{"$f":"('Solar Azimuth'!C8-'Input Data'!$F$9)","v":73.488492077926935},{"$f":"('Solar Azimuth'!D8-'Input Data'!$F$9)","v":82.464473557261059},{"$f":"('Solar Azimuth'!E8-'Input Data'!$F$9)","v":91.530413775338687},{"$f":"('Solar Azimuth'!F8-'Input Data'!$F$9)","v":101.44881339595754},{"$f":"('Solar Azimuth'!G8-'Input Data'!$F$9)","v":108.93731604152855},{"$f":"('Solar Azimuth'!H8-'Input Data'!$F$9)","v":112.29007277032856},{"$f":"('Solar Azimuth'!I8-'Input Data'!$F$9)","v":110.03139679027041},{"$f":"('Solar Azimuth'!J8-'Input Data'!$F$9)","v":101.98746755551197},{"$f":"('Solar Azimuth'!K8-'Input Data'!$F$9)","v":89.961695491259746},{"$f":"('Solar Azimuth'!L8-'Input Data'!$F$9)","v":79.416038586607996},{"$f":"('Solar Azimuth'!M8-'Input Data'!$F$9)","v":71.161731793949599},{"$f":"('Solar Azimuth'!N8-'Input Data'!$F$9)","v":68.987603220711861},null,6,{"$f":"('Solar Azimuth'!C8-('Input Data'!$F$9+90))","v":-16.511507922073065},{"$f":"('Solar Azimuth'!D8-('Input Data'!$F$9+90))","v":-7.5355264427389415},{"$f":"('Solar Azimuth'!E8-('Input Data'!$F$9+90))","v":1.5304137753386868},{"$f":"('Solar Azimuth'!F8-('Input Data'!$F$9+90))","v":11.448813395957544},{"$f":"('Solar Azimuth'!G8-('Input Data'!$F$9+90))","v":18.937316041528547},{"$f":"('Solar Azimuth'!H8-('Input Data'!$F$9+90))","v":22.290072770328564},{"$f":"('Solar Azimuth'!I8-('Input Data'!$F$9+90))","v":20.031396790270406},{"$f":"('Solar Azimuth'!J8-('Input Data'!$F$9+90))","v":11.987467555511969},{"$f":"('Solar Azimuth'!K8-('Input Data'!$F$9+90))","v":-3.8304508740253596E-2},{"$f":"('Solar Azimuth'!L8-('Input Data'!$F$9+90))","v":-10.583961413392004},{"$f":"('Solar Azimuth'!M8-('Input Data'!$F$9+90))","v":-18.838268206050401},{"$f":"('Solar Azimuth'!N8-('Input Data'!$F$9+90))","v":-21.012396779288139},null,"Azimuth Opposite",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,6.7469103189992206,15.119060763045432,74.858386165422246,9.8754647527955619,5.8291309022367246,4.8789115498826412,5.4856000083305458,9.4193907563120955,2991.5940896451893,10.703475300182616,5.8621243237896064,5.2068105860398521,null,6,0.59286396452255286,0.26456669912835779,5.3434227010461993E-2,0.40504422831013337,0.686208641920383,0.81985499411158969,0.7291818568480235,0.42465591496132926,1.3370797909533275E-3,0.37371039665329586,0.68234649745779785,0.76822460389178149,null,6,0,0,0,0,0,0,0,0,0,0,0,0,null,6,0.85178400886936179,0.93385832521791057,0.98664144324738445,0.8987389429224667,0.82844783951990419,0.79503625147210255,0.81770453578799418,0.89383602125966766,0.99966573005226167,0.90657240083667601,0.82941337563555051,0.80794384902705463,null,{"$f":"'Profile angles'!B10","v":6},{"$f":"IF('Profile angles'!C10<0,1000,IF(EB9<0,1000,'Profile angles'!C10))","v":1000},{"$f":"IF('Profile angles'!D10<0,1000,IF(EC9<0,1000,'Profile angles'!D10))","v":1000},{"$f":"IF('Profile angles'!E10<0,1000,IF(ED9<0,1000,'Profile angles'!E10))","v":1000},{"$f":"IF('Profile angles'!F10<0,1000,IF(EE9<0,1000,'Profile angles'!F10))","v":1000},{"$f":"IF('Profile angles'!G10<0,1000,IF(EF9<0,1000,'Profile angles'!G10))","v":1000},{"$f":"IF('Profile angles'!H10<0,1000,IF(EG9<0,1000,'Profile angles'!H10))","v":1000},{"$f":"IF('Profile angles'!I10<0,1000,IF(EH9<0,1000,'Profile angles'!I10))","v":1000},{"$f":"IF('Profile angles'!J10<0,1000,IF(EI9<0,1000,'Profile angles'!J10))","v":1000},{"$f":"IF('Profile angles'!K10<0,1000,IF(EJ9<0,1000,'Profile angles'!K10))","v":65.300000000001162},{"$f":"IF('Profile angles'!L10<0,1000,IF(EK9<0,1000,'Profile angles'!L10))","v":1000},{"$f":"IF('Profile angles'!M10<0,1000,IF(EL9<0,1000,'Profile angles'!M10))","v":1000},{"$f":"IF('Profile angles'!N10<0,1000,IF(EM9<0,1000,'Profile angles'!N10))","v":1000},null,{"$f":"'Profile angles'!B39","v":6},{"$f":"IF('Profile angles'!C39<0,1000,IF(EB9<0,1000,'Profile angles'!C39))","v":1000},{"$f":"IF('Profile angles'!D39<0,1000,IF(EC9<0,1000,'Profile angles'!D39))","v":1000},{"$f":"IF('Profile angles'!E39<0,1000,IF(ED9<0,1000,'Profile angles'!E39))","v":1000},{"$f":"IF('Profile angles'!F39<0,1000,IF(EE9<0,1000,'Profile angles'!F39))","v":3.6714405326866673},{"$f":"IF('Profile angles'!G39<0,1000,IF(EF9<0,1000,'Profile angles'!G39))","v":7.9357874829851527},{"$f":"IF('Profile angles'!H39<0,1000,IF(EG9<0,1000,'Profile angles'!H39))","v":8.3930552361023523},{"$f":"IF('Profile angles'!I39<0,1000,IF(EH9<0,1000,'Profile angles'!I39))","v":5.9138516774857015},{"$f":"IF('Profile angles'!J39<0,1000,IF(EI9<0,1000,'Profile angles'!J39))","v":2.9679829754440079},{"$f":"IF('Profile angles'!K39<0,1000,IF(EJ9<0,1000,'Profile angles'!K39))","v":8.3279928680461496E-2},{"$f":"IF('Profile angles'!L39<0,1000,IF(EK9<0,1000,'Profile angles'!L39))","v":1000},{"$f":"IF('Profile angles'!M39<0,1000,IF(EL9<0,1000,'Profile angles'!M39))","v":1000},{"$f":"IF('Profile angles'!N39<0,1000,IF(EM9<0,1000,'Profile angles'!N39))","v":1000},null,6,{"$f":"'Solar Altitude'!C9","v":-12.151444093159176},{"$f":"'Solar Altitude'!D9","v":-9.1319080559186769},{"$f":"'Solar Altitude'!E9","v":-3.3232309033445411},{"$f":"'Solar Altitude'!F9","v":3.5985816694690373},{"$f":"'Solar Altitude'!G9","v":7.5112987220277185},{"$f":"'Solar Altitude'!H9","v":7.7738597839019823},{"$f":"'Solar Altitude'!I9","v":5.5584053941199079},{"$f":"'Solar Altitude'!J9","v":2.9033723023449274},{"$f":"'Solar Altitude'!K9","v":8.3279910069695443E-2},{"$f":"'Solar Altitude'!L9","v":-2.6015900354108483},{"$f":"'Solar Altitude'!M9","v":-6.7413522567651629},{"$f":"'Solar Altitude'!N9","v":-10.743396255327719},null,6,-12.151444093159176,-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719]
[null,7,{"$f":"('Solar Azimuth'!C9-'Input Data'!$F$9)","v":67.647288527019725},{"$f":"('Solar Azimuth'!D9-'Input Data'!$F$9)","v":76.274229184511228},{"$f":"('Solar Azimuth'!E9-'Input Data'!$F$9)","v":85.209001105128564},{"$f":"('Solar Azimuth'!F9-'Input Data'!$F$9)","v":95.51931316773377},{"$f":"('Solar Azimuth'!G9-'Input Data'!$F$9)","v":103.59914856777166},{"$f":"('Solar Azimuth'!H9-'Input Data'!$F$9)","v":107.16015360598314},{"$f":"('Solar Azimuth'!I9-'Input Data'!$F$9)","v":104.6042787468042},{"$f":"('Solar Azimuth'!J9-'Input Data'!$F$9)","v":96.053854503327031},{"$f":"('Solar Azimuth'!K9-'Input Data'!$F$9)","v":83.570803318642589},{"$f":"('Solar Azimuth'!L9-'Input Data'!$F$9)","v":72.888563250533565},{"$f":"('Solar Azimuth'!M9-'Input Data'!$F$9)","v":64.901671637150741},{"$f":"('Solar Azimuth'!N9-'Input Data'!$F$9)","v":63.128359138793968},null,7,{"$f":"('Solar Azimuth'!C9-('Input Data'!$F$9+90))","v":-22.352711472980275},{"$f":"('Solar Azimuth'!D9-('Input Data'!$F$9+90))","v":-13.725770815488772},{"$f":"('Solar Azimuth'!E9-('Input Data'!$F$9+90))","v":-4.7909988948714357},{"$f":"('Solar Azimuth'!F9-('Input Data'!$F$9+90))","v":5.5193131677337703},{"$f":"('Solar Azimuth'!G9-('Input Data'!$F$9+90))","v":13.599148567771664},{"$f":"('Solar Azimuth'!H9-('Input Data'!$F$9+90))","v":17.16015360598314},{"$f":"('Solar Azimuth'!I9-('Input Data'!$F$9+90))","v":14.604278746804198},{"$f":"('Solar Azimuth'!J9-('Input Data'!$F$9+90))","v":6.053854503327031},{"$f":"('Solar Azimuth'!K9-('Input Data'!$F$9+90))","v":-6.4291966813574106},{"$f":"('Solar Azimuth'!L9-('Input Data'!$F$9+90))","v":-17.111436749466435},{"$f":"('Solar Azimuth'!M9-('Input Data'!$F$9+90))","v":-25.098328362849259},{"$f":"('Solar Azimuth'!N9-('Input Data'!$F$9+90))","v":-26.871640861206032},null,{"$f":"AR26","v":26.56505117707799},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,4.8637537065360839,8.1883219166285279,23.862321589616567,20.697663840527742,8.2675467079776812,6.4768982340536345,7.6757683007158697,18.858201658597785,17.748750103620818,6.4964872105347462,4.2698671082428907,3.9470561057713915,null,7,0.82241006460188526,0.48850057932834257,0.16762828314829842,0.19325852573601415,0.4838194619620646,0.61757956593623331,0.52112047202192724,0.21210930248888973,0.22536798234507699,0.61571736699697865,0.93679730506789805,1.0134135144801195,null,7,0,0,0,0,0,0,0,0,0,0,0,1.3235973557152114E-2,null,7,0.79439748384952868,0.8778748551679143,0.95809292921292544,0.9516853685659965,0.87904513450948385,0.84560510851594173,0.86971988199451822,0.94697267437777755,0.94365800441373071,0.84607065825075534,0.76580067373302552,0.74664662137997007,null,{"$f":"'Profile angles'!B11","v":7},{"$f":"IF('Profile angles'!C11<0,1000,IF(EB10<0,1000,'Profile angles'!C11))","v":1.8407058775768048},{"$f":"IF('Profile angles'!D11<0,1000,IF(EC10<0,1000,'Profile angles'!D11))","v":17.418156461309621},{"$f":"IF('Profile angles'!E11<0,1000,IF(ED10<0,1000,'Profile angles'!E11))","v":65.299999999999969},{"$f":"IF('Profile angles'!F11<0,1000,IF(EE10<0,1000,'Profile angles'!F11))","v":1000},{"$f":"IF('Profile angles'!G11<0,1000,IF(EF10<0,1000,'Profile angles'!G11))","v":1000},{"$f":"IF('Profile angles'!H11<0,1000,IF(EG10<0,1000,'Profile angles'!H11))","v":1000},{"$f":"IF('Profile angles'!I11<0,1000,IF(EH10<0,1000,'Profile angles'!I11))","v":1000},{"$f":"IF('Profile angles'!J11<0,1000,IF(EI10<0,1000,'Profile angles'!J11))","v":1000},{"$f":"IF('Profile angles'!K11<0,1000,IF(EJ10<0,1000,'Profile angles'!K11))","v":65.3},{"$f":"IF('Profile angles'!L11<0,1000,IF(EK10<0,1000,'Profile angles'!L11))","v":32.525623758734746},{"$f":"IF('Profile angles'!M11<0,1000,IF(EL10<0,1000,'Profile angles'!M11))","v":13.689263813478037},{"$f":"IF('Profile angles'!N11<0,1000,IF(EM10<0,1000,'Profile angles'!N11))","v":3.7902225360911945},null,{"$f":"'Profile angles'!B40","v":7},{"$f":"IF('Profile angles'!C40<0,1000,IF(EB10<0,1000,'Profile angles'!C40))","v":0.75712395765969032},{"$f":"IF('Profile angles'!D40<0,1000,IF(EC10<0,1000,'Profile angles'!D40))","v":4.3819211908166711},{"$f":"IF('Profile angles'!E40<0,1000,IF(ED10<0,1000,'Profile angles'!E40))","v":10.327408658619172},{"$f":"IF('Profile angles'!F40<0,1000,IF(EE10<0,1000,'Profile angles'!F40))","v":17.146626992599682},{"$f":"IF('Profile angles'!G40<0,1000,IF(EF10<0,1000,'Profile angles'!G40))","v":21.134165658355119},{"$f":"IF('Profile angles'!H40<0,1000,IF(EG10<0,1000,'Profile angles'!H40))","v":21.477097073214686},{"$f":"IF('Profile angles'!I40<0,1000,IF(EH10<0,1000,'Profile angles'!I40))","v":19.142999224755304},{"$f":"IF('Profile angles'!J40<0,1000,IF(EI10<0,1000,'Profile angles'!J40))","v":16.444109273248728},{"$f":"IF('Profile angles'!K40<0,1000,IF(EJ10<0,1000,'Profile angles'!K40))","v":13.765898970431955},{"$f":"IF('Profile angles'!L40<0,1000,IF(EK10<0,1000,'Profile angles'!L40))","v":11.107118463724456},{"$f":"IF('Profile angles'!M40<0,1000,IF(EL10<0,1000,'Profile angles'!M40))","v":6.5087495886135249},{"$f":"IF('Profile angles'!N40<0,1000,IF(EM10<0,1000,'Profile angles'!N40))","v":1.9226157929385757},null,7,{"$f":"'Solar Altitude'!C10","v":0.70023973357815916},{"$f":"'Solar Altitude'!D10","v":4.2572512510716702},{"$f":"'Solar Altitude'!E10","v":10.292097151668541},{"$f":"'Solar Altitude'!F10","v":17.071764306110264},{"$f":"'Solar Altitude'!G10","v":20.59199880999245},{"$f":"'Solar Altitude'!H10","v":20.602944398333847},{"$f":"'Solar Altitude'!I10","v":18.567526961418682},{"$f":"'Solar Altitude'!J10","v":16.357318748220177},{"$f":"'Solar Altitude'!K10","v":13.682588857300253},{"$f":"'Solar Altitude'!L10","v":10.626902061270702},{"$f":"'Solar Altitude'!M10","v":5.8987575020687171},{"$f":"'Solar Altitude'!N10","v":1.7151458456731048},null,7,0.70023973357815916,4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048]
[null,8,{"$f":"('Solar Azimuth'!C10-'Input Data'!$F$9)","v":60.634193010300976},{"$f":"('Solar Azimuth'!D10-'Input Data'!$F$9)","v":69.204562240532979},{"$f":"('Solar Azimuth'!E10-'Input Data'!$F$9)","v":78.310385534053466},{"$f":"('Solar Azimuth'!F10-'Input Data'!$F$9)","v":89.486122264914655},{"$f":"('Solar Azimuth'!G10-'Input Data'!$F$9)","v":98.663754358878165},{"$f":"('Solar Azimuth'!H10-'Input Data'!$F$9)","v":102.67188093597633},{"$f":"('Solar Azimuth'!I10-'Input Data'!$F$9)","v":99.661837469673486},{"$f":"('Solar Azimuth'!J10-'Input Data'!$F$9)","v":90.068762910981377},{"$f":"('Solar Azimuth'!K10-'Input Data'!$F$9)","v":76.387961658043494},{"$f":"('Solar Azimuth'!L10-'Input Data'!$F$9)","v":65.091765063126061},{"$f":"('Solar Azimuth'!M10-'Input Data'!$F$9)","v":57.212438245033646},{"$f":"('Solar Azimuth'!N10-'Input Data'!$F$9)","v":55.905386143263541},null,8,{"$f":"('Solar Azimuth'!C10-('Input Data'!$F$9+90))","v":-29.365806989699024},{"$f":"('Solar Azimuth'!D10-('Input Data'!$F$9+90))","v":-20.795437759467021},{"$f":"('Solar Azimuth'!E10-('Input Data'!$F$9+90))","v":-11.689614465946534},{"$f":"('Solar Azimuth'!F10-('Input Data'!$F$9+90))","v":-0.51387773508534451},{"$f":"('Solar Azimuth'!G10-('Input Data'!$F$9+90))","v":8.6637543588781654},{"$f":"('Solar Azimuth'!H10-('Input Data'!$F$9+90))","v":12.671880935976333},{"$f":"('Solar Azimuth'!I10-('Input Data'!$F$9+90))","v":9.6618374696734861},{"$f":"('Solar Azimuth'!J10-('Input Data'!$F$9+90))","v":6.876291098137699E-2},{"$f":"('Solar Azimuth'!K10-('Input Data'!$F$9+90))","v":-13.612038341956506},{"$f":"('Solar Azimuth'!L10-('Input Data'!$F$9+90))","v":-24.908234936873939},{"$f":"('Solar Azimuth'!M10-('Input Data'!$F$9+90))","v":-32.787561754966354},{"$f":"('Solar Azimuth'!N10-('Input Data'!$F$9+90))","v":-34.094613856736459},null,null,null,null,null,null,null,"Shade Angle (A)",null,null,null,null,null,null,null,null,null,null,8,3.5543862566617617,5.266300319386457,9.6664580849627288,222.98784046926158,13.125586196922347,8.8950523702247182,11.747589961943442,1666.4725558300477,8.2594157539109467,4.3070101234709171,3.1048725874777148,2.9545859005497968,null,8,1.1253700951895853,0.75954650464484219,0.41380203222754919,1.7938197847839114E-2,0.30474829390384939,0.44968818996384918,0.34049537079163317,2.4002795521631936E-3,0.48429575640455508,0.92871850432905312,1.2882976313206642,1.3538276207355047,null,8,0.11140343583455958,0,0,0,0,0,0,0,0,0,0.22378185313057131,0.26135352486255081,null,8,0.71865747620260367,0.81011337383878945,0.89654949194311273,0.99551545053804025,0.92381292652403768,0.8875779525090377,0.91487615730209171,0.99939993011195916,0.87892606089886127,0.76782037391773672,0.67792559216983395,0.66154309481612383,null,{"$f":"'Profile angles'!B12","v":8},{"$f":"IF('Profile angles'!C12<0,1000,IF(EB11<0,1000,'Profile angles'!C12))","v":25.154979301423634},{"$f":"IF('Profile angles'!D12<0,1000,IF(EC11<0,1000,'Profile angles'!D12))","v":41.208162613283584},{"$f":"IF('Profile angles'!E12<0,1000,IF(ED11<0,1000,'Profile angles'!E12))","v":65.300000000000011},{"$f":"IF('Profile angles'!F12<0,1000,IF(EE11<0,1000,'Profile angles'!F12))","v":89.133910589679402},{"$f":"IF('Profile angles'!G12<0,1000,IF(EF11<0,1000,'Profile angles'!G12))","v":1000},{"$f":"IF('Profile angles'!H12<0,1000,IF(EG11<0,1000,'Profile angles'!H12))","v":1000},{"$f":"IF('Profile angles'!I12<0,1000,IF(EH11<0,1000,'Profile angles'!I12))","v":1000},{"$f":"IF('Profile angles'!J12<0,1000,IF(EI11<0,1000,'Profile angles'!J12))","v":1000},{"$f":"IF('Profile angles'!K12<0,1000,IF(EJ11<0,1000,'Profile angles'!K12))","v":65.3},{"$f":"IF('Profile angles'!L12<0,1000,IF(EK11<0,1000,'Profile angles'!L12))","v":45.709102960920774},{"$f":"IF('Profile angles'!M12<0,1000,IF(EL11<0,1000,'Profile angles'!M12))","v":30.711991515210524},{"$f":"IF('Profile angles'!N12<0,1000,IF(EM11<0,1000,'Profile angles'!N12))","v":23.133349654536577},null,{"$f":"'Profile angles'!B41","v":8},{"$f":"IF('Profile angles'!C41<0,1000,IF(EB11<0,1000,'Profile angles'!C41))","v":14.801512993977905},{"$f":"IF('Profile angles'!D41<0,1000,IF(EC11<0,1000,'Profile angles'!D41))","v":18.395161326018542},{"$f":"IF('Profile angles'!E41<0,1000,IF(ED11<0,1000,'Profile angles'!E41))","v":24.21988645529855},{"$f":"IF('Profile angles'!F41<0,1000,IF(EE11<0,1000,'Profile angles'!F41))","v":30.680730702005945},{"$f":"IF('Profile angles'!G41<0,1000,IF(EF11<0,1000,'Profile angles'!G41))","v":34.26512345162336},{"$f":"IF('Profile angles'!H41<0,1000,IF(EG11<0,1000,'Profile angles'!H41))","v":34.426376431243654},{"$f":"IF('Profile angles'!I41<0,1000,IF(EH11<0,1000,'Profile angles'!I41))","v":32.256035415094608},{"$f":"IF('Profile angles'!J41<0,1000,IF(EI11<0,1000,'Profile angles'!J41))","v":29.958921059436694},{"$f":"IF('Profile angles'!K41<0,1000,IF(EJ11<0,1000,'Profile angles'!K41))","v":27.765335603992927},{"$f":"IF('Profile angles'!L41<0,1000,IF(EK11<0,1000,'Profile angles'!L41))","v":25.454349023394592},{"$f":"IF('Profile angles'!M41<0,1000,IF(EL11<0,1000,'Profile angles'!M41))","v":20.939346821539349},{"$f":"IF('Profile angles'!N41<0,1000,IF(EM11<0,1000,'Profile angles'!N41))","v":16.129552534651118},null,8,{"$f":"'Solar Altitude'!C11","v":12.968359542715392},{"$f":"'Solar Altitude'!D11","v":17.270303982095768},{"$f":"'Solar Altitude'!E11","v":23.773745192987032},{"$f":"'Solar Altitude'!F11","v":30.67971943621767},{"$f":"'Solar Altitude'!G11","v":33.959814353189685},{"$f":"'Solar Altitude'!H11","v":33.770494749028082},{"$f":"'Solar Altitude'!I11","v":31.887744015481577},{"$f":"'Solar Altitude'!J11","v":29.958903207045175},{"$f":"'Solar Altitude'!K11","v":27.097900221004789},{"$f":"'Solar Altitude'!L11","v":23.350930400204959},{"$f":"'Solar Altitude'!M11","v":17.832347455280527},{"$f":"'Solar Altitude'!N11","v":13.467847656409182},null,8,12.968359542715392,17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182]
[null,9,{"$f":"('Solar Azimuth'!C11-'Input Data'!$F$9)","v":51.768748339976497},{"$f":"('Solar Azimuth'!D11-'Input Data'!$F$9)","v":60.379685639709628},{"$f":"('Solar Azimuth'!E11-'Input Data'!$F$9)","v":69.814353609182064},{"$f":"('Solar Azimuth'!F11-'Input Data'!$F$9)","v":82.45083421497344},{"$f":"('Solar Azimuth'!G11-'Input Data'!$F$9)","v":93.627688952569216},{"$f":"('Solar Azimuth'!H11-'Input Data'!$F$9)","v":98.521187051411133},{"$f":"('Solar Azimuth'!I11-'Input Data'!$F$9)","v":94.735373704691739},{"$f":"('Solar Azimuth'!J11-'Input Data'!$F$9)","v":83.168099105996617},{"$f":"('Solar Azimuth'!K11-'Input Data'!$F$9)","v":67.256262036750698},{"$f":"('Solar Azimuth'!L11-'Input Data'!$F$9)","v":54.962752878328075},{"$f":"('Solar Azimuth'!M11-'Input Data'!$F$9)","v":47.319157053161554},{"$f":"('Solar Azimuth'!N11-'Input Data'!$F$9)","v":46.69540702919015},null,9,{"$f":"('Solar Azimuth'!C11-('Input Data'!$F$9+90))","v":-38.231251660023503},{"$f":"('Solar Azimuth'!D11-('Input Data'!$F$9+90))","v":-29.620314360290372},{"$f":"('Solar Azimuth'!E11-('Input Data'!$F$9+90))","v":-20.185646390817936},{"$f":"('Solar Azimuth'!F11-('Input Data'!$F$9+90))","v":-7.5491657850265597},{"$f":"('Solar Azimuth'!G11-('Input Data'!$F$9+90))","v":3.6276889525692155},{"$f":"('Solar Azimuth'!H11-('Input Data'!$F$9+90))","v":8.5211870514111325},{"$f":"('Solar Azimuth'!I11-('Input Data'!$F$9+90))","v":4.7353737046917388},{"$f":"('Solar Azimuth'!J11-('Input Data'!$F$9+90))","v":-6.8319008940033825},{"$f":"('Solar Azimuth'!K11-('Input Data'!$F$9+90))","v":-22.743737963249302},{"$f":"('Solar Azimuth'!L11-('Input Data'!$F$9+90))","v":-35.037247121671925},{"$f":"('Solar Azimuth'!M11-('Input Data'!$F$9+90))","v":-42.680842946838446},{"$f":"('Solar Azimuth'!N11-('Input Data'!$F$9+90))","v":-43.30459297080985},null,null,null,null,null,null,null,null,90,null,null,null,null,null,null,null,null,null,9,2.5386961002421038,3.5177320812106507,5.4400459145799314,15.091426776620025,31.545811824337182,13.348544853641274,24.143929269768702,16.693444262962046,4.7709207093241872,2.8523476737013262,2.1688337936394788,2.1220076092754359,null,9,1.5756119842853735,1.1370962619254881,0.73528791168463359,0.26505114852340461,0.12679971662400052,0.29965813081932019,0.1656731162234025,0.23961502114185326,0.83841259239175447,1.4023535899497945,1.8443091451870435,1.8850073781619505,null,9,0.36532597493947405,0.12056697969733732,0,0,0,0,0,0,0,0.28691308157466844,0.4577915515901303,0.46949809768114104,null,9,0.60609700392865662,0.71572593451862798,0.8161780220788416,0.93373721286914879,0.96830007084399983,0.92508546729516994,0.9585817209441494,0.94009624471453668,0.79039685190206144,0.64941160251255137,0.53892271370323908,0.52874815545951237,null,{"$f":"'Profile angles'!B13","v":9},{"$f":"IF('Profile angles'!C13<0,1000,IF(EB12<0,1000,'Profile angles'!C13))","v":36.123628972409719},{"$f":"IF('Profile angles'!D13<0,1000,IF(EC12<0,1000,'Profile angles'!D13))","v":48.984103271498903},{"$f":"IF('Profile angles'!E13<0,1000,IF(ED12<0,1000,'Profile angles'!E13))","v":65.3},{"$f":"IF('Profile angles'!F13<0,1000,IF(EE12<0,1000,'Profile angles'!F13))","v":82.323917470741151},{"$f":"IF('Profile angles'!G13<0,1000,IF(EF12<0,1000,'Profile angles'!G13))","v":1000},{"$f":"IF('Profile angles'!H13<0,1000,IF(EG12<0,1000,'Profile angles'!H13))","v":1000},{"$f":"IF('Profile angles'!I13<0,1000,IF(EH12<0,1000,'Profile angles'!I13))","v":1000},{"$f":"IF('Profile angles'!J13<0,1000,IF(EI12<0,1000,'Profile angles'!J13))","v":82.868918499232819},{"$f":"IF('Profile angles'!K13<0,1000,IF(EJ12<0,1000,'Profile angles'!K13))","v":65.300000000000011},{"$f":"IF('Profile angles'!L13<0,1000,IF(EK12<0,1000,'Profile angles'!L13))","v":50.828908694033096},{"$f":"IF('Profile angles'!M13<0,1000,IF(EL12<0,1000,'Profile angles'!M13))","v":38.841664176975662},{"$f":"IF('Profile angles'!N13<0,1000,IF(EM12<0,1000,'Profile angles'!N13))","v":33.137728896941795},null,{"$f":"'Profile angles'!B42","v":9},{"$f":"IF('Profile angles'!C42<0,1000,IF(EB12<0,1000,'Profile angles'!C42))","v":29.897860503845664},{"$f":"IF('Profile angles'!D42<0,1000,IF(EC12<0,1000,'Profile angles'!D42))","v":33.171578582642681},{"$f":"IF('Profile angles'!E42<0,1000,IF(ED12<0,1000,'Profile angles'!E42))","v":38.635878844024361},{"$f":"IF('Profile angles'!F42<0,1000,IF(EE12<0,1000,'Profile angles'!F42))","v":44.516730121969097},{"$f":"IF('Profile angles'!G42<0,1000,IF(EF12<0,1000,'Profile angles'!G42))","v":47.561101053580373},{"$f":"IF('Profile angles'!H42<0,1000,IF(EG12<0,1000,'Profile angles'!H42))","v":47.480410935356453},{"$f":"IF('Profile angles'!I42<0,1000,IF(EH12<0,1000,'Profile angles'!I42))","v":45.501067907501131},{"$f":"IF('Profile angles'!J42<0,1000,IF(EI12<0,1000,'Profile angles'!J42))","v":43.760303315048105},{"$f":"IF('Profile angles'!K42<0,1000,IF(EJ12<0,1000,'Profile angles'!K42))","v":42.346663637257642},{"$f":"IF('Profile angles'!L42<0,1000,IF(EK12<0,1000,'Profile angles'!L42))","v":40.715743852069998},{"$f":"IF('Profile angles'!M42<0,1000,IF(EL12<0,1000,'Profile angles'!M42))","v":36.595216615504739},{"$f":"IF('Profile angles'!N42<0,1000,IF(EM12<0,1000,'Profile angles'!N42))","v":31.603785496296783},null,9,{"$f":"'Solar Altitude'!C12","v":24.306538235547787},{"$f":"'Solar Altitude'!D12","v":29.607456719563572},{"$f":"'Solar Altitude'!E12","v":36.877998514340362},{"$f":"'Solar Altitude'!F12","v":44.267398869292073},{"$f":"'Solar Altitude'!G12","v":47.503865138538167},{"$f":"'Solar Altitude'!H12","v":47.16345799134892},{"$f":"'Solar Altitude'!I12","v":45.403126432581416},{"$f":"'Solar Altitude'!J12","v":43.556385601632783},{"$f":"'Solar Altitude'!K12","v":40.048756889246128},{"$f":"'Solar Altitude'!L12","v":35.170537312656599},{"$f":"'Solar Altitude'!M12","v":28.628753160625717},{"$f":"'Solar Altitude'!N12","v":24.120985503613159},null,9,24.306538235547787,29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159]
[null,10,{"$f":"('Solar Azimuth'!C12-'Input Data'!$F$9)","v":40.148034381332685},{"$f":"('Solar Azimuth'!D12-'Input Data'!$F$9)","v":48.471328297789526},{"$f":"('Solar Azimuth'!E12-'Input Data'!$F$9)","v":57.889532705571163},{"$f":"('Solar Azimuth'!F12-'Input Data'!$F$9)","v":72.497654057460437},{"$f":"('Solar Azimuth'!G12-'Input Data'!$F$9)","v":87.520988749472963},{"$f":"('Solar Azimuth'!H12-'Input Data'!$F$9)","v":94.32570869615293},{"$f":"('Solar Azimuth'!I12-'Input Data'!$F$9)","v":89.01523478336928},{"$f":"('Solar Azimuth'!J12-'Input Data'!$F$9)","v":73.552305529127068},{"$f":"('Solar Azimuth'!K12-'Input Data'!$F$9)","v":54.003522769149818},{"$f":"('Solar Azimuth'!L12-'Input Data'!$F$9)","v":40.89681624413825},{"$f":"('Solar Azimuth'!M12-'Input Data'!$F$9)","v":34.26382672583707},{"$f":"('Solar Azimuth'!N12-'Input Data'!$F$9)","v":34.744710793512169},null,10,{"$f":"('Solar Azimuth'!C12-('Input Data'!$F$9+90))","v":-49.851965618667315},{"$f":"('Solar Azimuth'!D12-('Input Data'!$F$9+90))","v":-41.528671702210474},{"$f":"('Solar Azimuth'!E12-('Input Data'!$F$9+90))","v":-32.110467294428837},{"$f":"('Solar Azimuth'!F12-('Input Data'!$F$9+90))","v":-17.502345942539563},{"$f":"('Solar Azimuth'!G12-('Input Data'!$F$9+90))","v":-2.4790112505270372},{"$f":"('Solar Azimuth'!H12-('Input Data'!$F$9+90))","v":4.3257086961529296},{"$f":"('Solar Azimuth'!I12-('Input Data'!$F$9+90))","v":-0.98476521663071992},{"$f":"('Solar Azimuth'!J12-('Input Data'!$F$9+90))","v":-16.447694470872932},{"$f":"('Solar Azimuth'!K12-('Input Data'!$F$9+90))","v":-35.996477230850182},{"$f":"('Solar Azimuth'!L12-('Input Data'!$F$9+90))","v":-49.10318375586175},{"$f":"('Solar Azimuth'!M12-('Input Data'!$F$9+90))","v":-55.73617327416293},{"$f":"('Solar Azimuth'!N12-('Input Data'!$F$9+90))","v":-55.255289206487831},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,1.6870240761729263,2.258310602566723,3.1869796629135712,6.342284112487401,46.195854889385153,26.440466318461326,116.35288611892287,6.7745913481285376,2.7531197925276567,1.7322598317242275,1.3624580393835388,1.3871759048764651,null,10,2.3710390719936516,1.7712355401660564,1.2551068482009569,0.6306876086052895,8.6587855329832139E-2,0.15128326224742528,3.4378176024887332E-2,0.5904415180858088,1.4528971862599469,2.3091224115140672,2.9358702318713967,2.883556429965684,null,10,0.57824398095676843,0.43542234935831925,0.20325508427160721,0,0,0,0,0,0.31172005186808582,0.56693504206894318,0.65938549015411529,0.65320602378088366,null,10,0.4072402320015871,0.55719111495848583,0.68622328794976073,0.84232809784867757,0.97835303616754199,0.96217918443814365,0.99140545599377816,0.85238962047854783,0.63677570343501322,0.42271939712148321,0.26603244203215082,0.27911089250857901,null,{"$f":"'Profile angles'!B14","v":10},{"$f":"IF('Profile angles'!C14<0,1000,IF(EB13<0,1000,'Profile angles'!C14))","v":41.565533524141749},{"$f":"IF('Profile angles'!D14<0,1000,IF(EC13<0,1000,'Profile angles'!D14))","v":52.391449411165148},{"$f":"IF('Profile angles'!E14<0,1000,IF(ED13<0,1000,'Profile angles'!E14))","v":65.3},{"$f":"IF('Profile angles'!F14<0,1000,IF(EE13<0,1000,'Profile angles'!F14))","v":79.183835184665355},{"$f":"IF('Profile angles'!G14<0,1000,IF(EF13<0,1000,'Profile angles'!G14))","v":88.633552185609801},{"$f":"IF('Profile angles'!H14<0,1000,IF(EG13<0,1000,'Profile angles'!H14))","v":1000},{"$f":"IF('Profile angles'!I14<0,1000,IF(EH13<0,1000,'Profile angles'!I14))","v":89.408737808154712},{"$f":"IF('Profile angles'!J14<0,1000,IF(EI13<0,1000,'Profile angles'!J14))","v":79.54425546635963},{"$f":"IF('Profile angles'!K14<0,1000,IF(EJ13<0,1000,'Profile angles'!K14))","v":65.3},{"$f":"IF('Profile angles'!L14<0,1000,IF(EK13<0,1000,'Profile angles'!L14))","v":53.228063715971984},{"$f":"IF('Profile angles'!M14<0,1000,IF(EL13<0,1000,'Profile angles'!M14))","v":42.944409695388977},{"$f":"IF('Profile angles'!N14<0,1000,IF(EM13<0,1000,'Profile angles'!N14))","v":38.364397938009645},null,{"$f":"'Profile angles'!B43","v":10},{"$f":"IF('Profile angles'!C43<0,1000,IF(EB13<0,1000,'Profile angles'!C43))","v":46.432009669114628},{"$f":"IF('Profile angles'!D43<0,1000,IF(EC13<0,1000,'Profile angles'!D43))","v":48.982108380980456},{"$f":"IF('Profile angles'!E43<0,1000,IF(ED13<0,1000,'Profile angles'!E43))","v":53.761437623792659},{"$f":"IF('Profile angles'!F43<0,1000,IF(EE13<0,1000,'Profile angles'!F43))","v":58.790214649196741},{"$f":"IF('Profile angles'!G43<0,1000,IF(EF13<0,1000,'Profile angles'!G43))","v":61.14667544282198},{"$f":"IF('Profile angles'!H43<0,1000,IF(EG13<0,1000,'Profile angles'!H43))","v":60.771492120895445},{"$f":"IF('Profile angles'!I43<0,1000,IF(EH13<0,1000,'Profile angles'!I43))","v":59.020595594487986},{"$f":"IF('Profile angles'!J43<0,1000,IF(EI13<0,1000,'Profile angles'!J43))","v":57.990814089298965},{"$f":"IF('Profile angles'!K43<0,1000,IF(EJ13<0,1000,'Profile angles'!K43))","v":57.660184602658042},{"$f":"IF('Profile angles'!L43<0,1000,IF(EK13<0,1000,'Profile angles'!L43))","v":57.085561042213271},{"$f":"IF('Profile angles'!M43<0,1000,IF(EL13<0,1000,'Profile angles'!M43))","v":53.797693072162787},{"$f":"IF('Profile angles'!N43<0,1000,IF(EM13<0,1000,'Profile angles'!N43))","v":48.774894172678039},null,10,{"$f":"'Solar Altitude'!C13","v":34.130498638110296},{"$f":"'Solar Altitude'!D13","v":40.716949463115029},{"$f":"'Solar Altitude'!E13","v":49.130640449349286},{"$f":"'Solar Altitude'!F13","v":57.573642107854539},{"$f":"'Solar Altitude'!G13","v":61.123995517612983},{"$f":"'Solar Altitude'!H13","v":60.701791836412639},{"$f":"'Solar Altitude'!I13","v":59.016860616830343},{"$f":"'Solar Altitude'!J13","v":56.905164678924855},{"$f":"'Solar Altitude'!K13","v":51.954064465377563},{"$f":"'Solar Altitude'!L13","v":45.326184070335216},{"$f":"'Solar Altitude'!M13","v":37.566870997040184},{"$f":"'Solar Altitude'!N13","v":33.04159126014769},null,10,34.130498638110296,40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,37.566870997040184,33.04159126014769]
[null,11,{"$f":"('Solar Azimuth'!C13-'Input Data'!$F$9)","v":24.885076293015025},{"$f":"('Solar Azimuth'!D13-'Input Data'!$F$9)","v":31.635752238757334},{"$f":"('Solar Azimuth'!E13-'Input Data'!$F$9)","v":38.941064079848665},{"$f":"('Solar Azimuth'!F13-'Input Data'!$F$9)","v":53.640222898119461},{"$f":"('Solar Azimuth'!G13-'Input Data'!$F$9)","v":76.561283289908715},{"$f":"('Solar Azimuth'!H13-'Input Data'!$F$9)","v":88.98202668740042},{"$f":"('Solar Azimuth'!I13-'Input Data'!$F$9)","v":79.732186026550423},{"$f":"('Solar Azimuth'!J13-'Input Data'!$F$9)","v":55.672233384753454},{"$f":"('Solar Azimuth'!K13-'Input Data'!$F$9)","v":32.502388308448495},{"$f":"('Solar Azimuth'!L13-'Input Data'!$F$9)","v":21.136723538029337},{"$f":"('Solar Azimuth'!M13-'Input Data'!$F$9)","v":17.409277392405681},{"$f":"('Solar Azimuth'!N13-'Input Data'!$F$9)","v":19.534720568739846},null,11,{"$f":"('Solar Azimuth'!C13-('Input Data'!$F$9+90))","v":-65.114923706984968},{"$f":"('Solar Azimuth'!D13-('Input Data'!$F$9+90))","v":-58.364247761242666},{"$f":"('Solar Azimuth'!E13-('Input Data'!$F$9+90))","v":-51.058935920151335},{"$f":"('Solar Azimuth'!F13-('Input Data'!$F$9+90))","v":-36.359777101880539},{"$f":"('Solar Azimuth'!G13-('Input Data'!$F$9+90))","v":-13.438716710091285},{"$f":"('Solar Azimuth'!H13-('Input Data'!$F$9+90))","v":-1.0179733125995796},{"$f":"('Solar Azimuth'!I13-('Input Data'!$F$9+90))","v":-10.267813973449577},{"$f":"('Solar Azimuth'!J13-('Input Data'!$F$9+90))","v":-34.327766615246546},{"$f":"('Solar Azimuth'!K13-('Input Data'!$F$9+90))","v":-57.497611691551505},{"$f":"('Solar Azimuth'!L13-('Input Data'!$F$9+90))","v":-68.863276461970656},{"$f":"('Solar Azimuth'!M13-('Input Data'!$F$9+90))","v":-72.590722607594316},{"$f":"('Solar Azimuth'!N13-('Input Data'!$F$9+90))","v":-70.465279431260157},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,0.92773598694944515,1.2321291926797207,1.6161646052651486,2.7167249167941012,8.3700287686893855,112.55648827841081,11.040540306780622,2.9288403988884131,1.2742577279073304,0.77320889588019071,0.62711767201041213,0.70960139627763519,null,11,4.3115714559620395,3.2464128143092852,2.474995422476634,1.4723610680172359,0.47789560950652943,3.5537711429890359E-2,0.36230110926214115,1.365728225245092,3.1390823947123003,5.1732462227384932,6.3783882651190709,5.636967487638624,null,11,0.76806600326263874,0.69196770183006984,0.59595884868371285,0.3208187708014747,0,0,0,0.26778990027789673,0.6814355680231674,0.8066977760299523,0.84322058199739702,0.82259965093059118,null,11,0,0.1883967964226787,0.38125114438084151,0.63190973299569109,0.88052609762336764,0.99111557214252743,0.90942472268446473,0.65856794368872706,0.21522940132192492,0,0,0,null,{"$f":"'Profile angles'!B15","v":11},{"$f":"IF('Profile angles'!C15<0,1000,IF(EB14<0,1000,'Profile angles'!C15))","v":44.282217904128672},{"$f":"IF('Profile angles'!D15<0,1000,IF(EC14<0,1000,'Profile angles'!D15))","v":54.018451059115115},{"$f":"IF('Profile angles'!E15<0,1000,IF(ED14<0,1000,'Profile angles'!E15))","v":65.300000000000011},{"$f":"IF('Profile angles'!F15<0,1000,IF(EE14<0,1000,'Profile angles'!F15))","v":77.69612062717222},{"$f":"IF('Profile angles'!G15<0,1000,IF(EF14<0,1000,'Profile angles'!G15))","v":86.343646743656691},{"$f":"IF('Profile angles'!H15<0,1000,IF(EG14<0,1000,'Profile angles'!H15))","v":89.714212091310287},{"$f":"IF('Profile angles'!I15<0,1000,IF(EH14<0,1000,'Profile angles'!I15))","v":86.798330968762983},{"$f":"IF('Profile angles'!J15<0,1000,IF(EI14<0,1000,'Profile angles'!J15))","v":77.960826272965903},{"$f":"IF('Profile angles'!K15<0,1000,IF(EJ14<0,1000,'Profile angles'!K15))","v":65.300000000000011},{"$f":"IF('Profile angles'!L15<0,1000,IF(EK14<0,1000,'Profile angles'!L15))","v":54.328164209664372},{"$f":"IF('Profile angles'!M15<0,1000,IF(EL14<0,1000,'Profile angles'!M15))","v":44.893647845797645},{"$f":"IF('Profile angles'!N15<0,1000,IF(EM14<0,1000,'Profile angles'!N15))","v":40.97067975660989},null,{"$f":"'Profile angles'!B44","v":11},{"$f":"IF('Profile angles'!C44<0,1000,IF(EB14<0,1000,'Profile angles'!C44))","v":64.562443951008888},{"$f":"IF('Profile angles'!D44<0,1000,IF(EC14<0,1000,'Profile angles'!D44))","v":65.901314539685401},{"$f":"IF('Profile angles'!E44<0,1000,IF(ED14<0,1000,'Profile angles'!E44))","v":69.61109114186894},{"$f":"IF('Profile angles'!F44<0,1000,IF(EE14<0,1000,'Profile angles'!F44))","v":73.497168133288227},{"$f":"IF('Profile angles'!G44<0,1000,IF(EF14<0,1000,'Profile angles'!G44))","v":75.027677809677201},{"$f":"IF('Profile angles'!H44<0,1000,IF(EG14<0,1000,'Profile angles'!H44))","v":74.319781349482838},{"$f":"IF('Profile angles'!I44<0,1000,IF(EH14<0,1000,'Profile angles'!I44))","v":72.839713407261911},{"$f":"IF('Profile angles'!J44<0,1000,IF(EI14<0,1000,'Profile angles'!J44))","v":72.655436766674285},{"$f":"IF('Profile angles'!K44<0,1000,IF(EJ14<0,1000,'Profile angles'!K44))","v":73.666960034724283},{"$f":"IF('Profile angles'!L44<0,1000,IF(EK14<0,1000,'Profile angles'!L44))","v":74.489845422408862},{"$f":"IF('Profile angles'!M44<0,1000,IF(EL14<0,1000,'Profile angles'!M44))","v":72.52990498677552},{"$f":"IF('Profile angles'!N44<0,1000,IF(EM14<0,1000,'Profile angles'!N44))","v":67.776371428052769},null,11,{"$f":"'Solar Altitude'!C14","v":41.499338482119107},{"$f":"'Solar Altitude'!D14","v":49.543356395157261},{"$f":"'Solar Altitude'!E14","v":59.402009530792824},{"$f":"'Solar Altitude'!F14","v":69.801829865076741},{"$f":"'Solar Altitude'!G14","v":74.625870049112294},{"$f":"'Solar Altitude'!H14","v":74.317427946135254},{"$f":"'Solar Altitude'!I14","v":72.577202871970812},{"$f":"'Solar Altitude'!J14","v":69.283885987295108},{"$f":"'Solar Altitude'!K14","v":61.393251168859464},{"$f":"'Solar Altitude'!L14","v":52.417946997507137},{"$f":"'Solar Altitude'!M14","v":43.550952586854685},{"$f":"'Solar Altitude'!N14","v":39.297011346471983},null,11,41.499338482119107,49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983]
[null,12,{"$f":"('Solar Azimuth'!C14-'Input Data'!$F$9)","v":6.1188489470903447},{"$f":"('Solar Azimuth'!D14-'Input Data'!$F$9)","v":8.886713641915156},{"$f":"('Solar Azimuth'!E14-'Input Data'!$F$9)","v":8.6992261524728125},{"$f":"('Solar Azimuth'!F14-'Input Data'!$F$9)","v":6.6354940803276321},{"$f":"('Solar Azimuth'!G14-'Input Data'!$F$9)","v":11.563825851086857},{"$f":"('Solar Azimuth'!H14-'Input Data'!$F$9)","v":57.747874143760271},{"$f":"('Solar Azimuth'!I14-'Input Data'!$F$9)","v":36.885376570622384},{"$f":"('Solar Azimuth'!J14-'Input Data'!$F$9)","v":10.575312516834758},{"$f":"('Solar Azimuth'!K14-'Input Data'!$F$9)","v":0.21936712106550094},{"$f":"('Solar Azimuth'!L14-'Input Data'!$F$9)","v":3.5020973891401352},{"$f":"('Solar Azimuth'!M14-'Input Data'!$F$9)","v":2.231001794012502},{"$f":"('Solar Azimuth'!N14-'Input Data'!$F$9)","v":1.7032943301877761},null,12,{"$f":"('Solar Azimuth'!C14-('Input Data'!$F$9+90))","v":-83.881151052909658},{"$f":"('Solar Azimuth'!D14-('Input Data'!$F$9+90))","v":-81.113286358084849},{"$f":"('Solar Azimuth'!E14-('Input Data'!$F$9+90))","v":-81.300773847527182},{"$f":"('Solar Azimuth'!F14-('Input Data'!$F$9+90))","v":-83.364505919672368},{"$f":"('Solar Azimuth'!G14-('Input Data'!$F$9+90))","v":-78.436174148913139},{"$f":"('Solar Azimuth'!H14-('Input Data'!$F$9+90))","v":-32.252125856239729},{"$f":"('Solar Azimuth'!I14-('Input Data'!$F$9+90))","v":-53.114623429377616},{"$f":"('Solar Azimuth'!J14-('Input Data'!$F$9+90))","v":-79.424687483165243},{"$f":"('Solar Azimuth'!K14-('Input Data'!$F$9+90))","v":-89.780632878934497},{"$f":"('Solar Azimuth'!L14-('Input Data'!$F$9+90))","v":-86.497902610859867},{"$f":"('Solar Azimuth'!M14-('Input Data'!$F$9+90))","v":-87.768998205987501},{"$f":"('Solar Azimuth'!N14-('Input Data'!$F$9+90))","v":-88.296705669812226},null,"Shade \nTransmittance",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,0.21440383138307426,0.31271650490177061,0.306015361134644,0.23266354933280642,0.409225289130555,3.169547561940298,1.5008444154962819,0.37339796110233442,7.6573944824832336E-3,0.12239872703679489,7.7916036418668982E-2,5.9473709570599109E-2,null,12,18.656383023553445,12.791138098887552,13.071239251417937,17.192207423425451,9.7745669836252116,1.262009773265975,2.6651663281682172,10.712431284282658,522.37089380083728,32.680078435762887,51.337313650127712,67.256608489365888,null,12,0.94639904215423143,0.92182087377455735,0.92349615971633903,0.9418341126667984,0.89769367771736119,0.20761310951492551,0.62478889612592958,0.90665050972441641,0.99808565137937921,0.96940031824080131,0.98052099089533273,0.98513157260735018,null,12,0,0,0,0,0,0.68449755668350631,0.3337084179579457,0,0,0,0,0,null,{"$f":"'Profile angles'!B16","v":12},{"$f":"IF('Profile angles'!C16<0,1000,IF(EB15<0,1000,'Profile angles'!C16))","v":45.341192522261665},{"$f":"IF('Profile angles'!D16<0,1000,IF(EC15<0,1000,'Profile angles'!D16))","v":54.65622400407787},{"$f":"IF('Profile angles'!E16<0,1000,IF(ED15<0,1000,'Profile angles'!E16))","v":65.300000000000011},{"$f":"IF('Profile angles'!F16<0,1000,IF(EE15<0,1000,'Profile angles'!F16))","v":77.204007036944958},{"$f":"IF('Profile angles'!G16<0,1000,IF(EF15<0,1000,'Profile angles'!G16))","v":85.602608099870324},{"$f":"IF('Profile angles'!H16<0,1000,IF(EG15<0,1000,'Profile angles'!H16))","v":88.764506326073786},{"$f":"IF('Profile angles'!I16<0,1000,IF(EH15<0,1000,'Profile angles'!I16))","v":85.831844934745362},{"$f":"IF('Profile angles'!J16<0,1000,IF(EI15<0,1000,'Profile angles'!J16))","v":77.410166839433359},{"$f":"IF('Profile angles'!K16<0,1000,IF(EJ15<0,1000,'Profile angles'!K16))","v":65.3},{"$f":"IF('Profile angles'!L16<0,1000,IF(EK15<0,1000,'Profile angles'!L16))","v":54.593196533889113},{"$f":"IF('Profile angles'!M16<0,1000,IF(EL15<0,1000,'Profile angles'!M16))","v":45.392239295822165},{"$f":"IF('Profile angles'!N16<0,1000,IF(EM15<0,1000,'Profile angles'!N16))","v":41.843902161818413},null,{"$f":"'Profile angles'!B45","v":12},{"$f":"IF('Profile angles'!C45<0,1000,IF(EB15<0,1000,'Profile angles'!C45))","v":83.953055253243946},{"$f":"IF('Profile angles'!D45<0,1000,IF(EC15<0,1000,'Profile angles'!D45))","v":83.672477687445479},{"$f":"IF('Profile angles'!E45<0,1000,IF(ED15<0,1000,'Profile angles'!E45))","v":85.9744082667399},{"$f":"IF('Profile angles'!F45<0,1000,IF(EE15<0,1000,'Profile angles'!F45))","v":88.486518830478445},{"$f":"IF('Profile angles'!G45<0,1000,IF(EF15<0,1000,'Profile angles'!G45))","v":89.098541577633242},{"$f":"IF('Profile angles'!H45<0,1000,IF(EG15<0,1000,'Profile angles'!H45))","v":88.042480487312574},{"$f":"IF('Profile angles'!I45<0,1000,IF(EH15<0,1000,'Profile angles'!I45))","v":86.869712514125027},{"$f":"IF('Profile angles'!J45<0,1000,IF(EI15<0,1000,'Profile angles'!J45))","v":87.612299057311645},{"$f":"IF('Profile angles'!K45<0,1000,IF(EJ15<0,1000,'Profile angles'!K45))","v":89.899102008780474},{"$f":"IF('Profile angles'!L45<0,1000,IF(EK15<0,1000,'Profile angles'!L45))","v":87.509028766495277},{"$f":"IF('Profile angles'!M45<0,1000,IF(EL15<0,1000,'Profile angles'!M45))","v":87.799307231125709},{"$f":"IF('Profile angles'!N45<0,1000,IF(EM15<0,1000,'Profile angles'!N45))","v":88.09804255680524},null,12,{"$f":"'Solar Altitude'!C15","v":45.177523796213436},{"$f":"'Solar Altitude'!D15","v":54.329068465075267},{"$f":"'Solar Altitude'!E15","v":65.047371814417531},{"$f":"'Solar Altitude'!F15","v":77.120581963762746},{"$f":"'Solar Altitude'!G15","v":85.511869047796154},{"$f":"'Solar Altitude'!H15","v":87.685706703910299},{"$f":"'Solar Altitude'!I15","v":84.793912346691229},{"$f":"'Solar Altitude'!J15","v":77.199736149013034},{"$f":"'Solar Altitude'!K15","v":65.299840573859427},{"$f":"'Solar Altitude'!L15","v":54.542607240756659},{"$f":"'Solar Altitude'!M15","v":45.370517861678998},{"$f":"'Solar Altitude'!N15","v":41.831318434437598},null,12,45.177523796213436,54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598]
[null,13,{"$f":"('Solar Azimuth'!C15-'Input Data'!$F$9)","v":-13.732736529787083},{"$f":"('Solar Azimuth'!D15-'Input Data'!$F$9)","v":-16.214430009759653},{"$f":"('Solar Azimuth'!E15-'Input Data'!$F$9)","v":-25.640993481536086},{"$f":"('Solar Azimuth'!F15-'Input Data'!$F$9)","v":-47.353608937771028},{"$f":"('Solar Azimuth'!G15-'Input Data'!$F$9)","v":-74.056458822561879},{"$f":"('Solar Azimuth'!H15-'Input Data'!$F$9)","v":-86.585446106298974},{"$f":"('Solar Azimuth'!I15-'Input Data'!$F$9)","v":-71.01828631253062},{"$f":"('Solar Azimuth'!J15-'Input Data'!$F$9)","v":-45.719410912822127},{"$f":"('Solar Azimuth'!K15-'Input Data'!$F$9)","v":-32.835610825796458},{"$f":"('Solar Azimuth'!L15-'Input Data'!$F$9)","v":-27.197074749164472},{"$f":"('Solar Azimuth'!M15-'Input Data'!$F$9)","v":-21.470648812116224},{"$f":"('Solar Azimuth'!N15-'Input Data'!$F$9)","v":-16.394081517196998},null,13,{"$f":"('Solar Azimuth'!C15-('Input Data'!$F$9+90))","v":-103.73273652978708},{"$f":"('Solar Azimuth'!D15-('Input Data'!$F$9+90))","v":-106.21443000975965},{"$f":"('Solar Azimuth'!E15-('Input Data'!$F$9+90))","v":-115.64099348153609},{"$f":"('Solar Azimuth'!F15-('Input Data'!$F$9+90))","v":-137.35360893777101},{"$f":"('Solar Azimuth'!G15-('Input Data'!$F$9+90))","v":-164.05645882256186},{"$f":"('Solar Azimuth'!H15-('Input Data'!$F$9+90))","v":-176.58544610629897},{"$f":"('Solar Azimuth'!I15-('Input Data'!$F$9+90))","v":-161.01828631253062},{"$f":"('Solar Azimuth'!J15-('Input Data'!$F$9+90))","v":-135.71941091282213},{"$f":"('Solar Azimuth'!K15-('Input Data'!$F$9+90))","v":-122.83561082579646},{"$f":"('Solar Azimuth'!L15-('Input Data'!$F$9+90))","v":-117.19707474916447},{"$f":"('Solar Azimuth'!M15-('Input Data'!$F$9+90))","v":-111.47064881211622},{"$f":"('Solar Azimuth'!N15-('Input Data'!$F$9+90))","v":-106.39408151719699},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,0.48875824212978791,0.58159997123594698,0.95999946988969254,2.171452305746274,7.0008579295378635,33.520005763030035,5.814449466240724,2.0508657038357132,1.2906720722658713,1.0277313060289506,0.78663766543231828,0.58840752788947104,null,13,8.1840052099578067,6.8775794323023707,4.1666689674939246,1.8420851286555426,0.57135854494679705,0.11933172172696192,0.68794131296942218,1.9503958706407938,3.099160573744888,3.8920678746817527,5.0849332237373757,6.7980095603932824,null,13,0.87781043946755299,0.85460000719101326,0.76000013252757692,0.4571369235634315,0,0,0,0.4872835740410717,0.67733198193353217,0.7430671734927623,0.8033405836419204,0.85289811802763227,null,13,0,0,0,0.53947871783611434,0.85716036376330074,0.97016706956825949,0.82801467175764443,0.51240103233980161,0.22520985656377801,2.6983031329561813E-2,0,0,null,{"$f":"'Profile angles'!B17","v":13},{"$f":"IF('Profile angles'!C17<0,1000,IF(EB16<0,1000,'Profile angles'!C17))","v":45.093307228609767},{"$f":"IF('Profile angles'!D17<0,1000,IF(EC16<0,1000,'Profile angles'!D17))","v":54.548508865098285},{"$f":"IF('Profile angles'!E17<0,1000,IF(ED16<0,1000,'Profile angles'!E17))","v":65.300000000000011},{"$f":"IF('Profile angles'!F17<0,1000,IF(EE16<0,1000,'Profile angles'!F17))","v":77.527686129155398},{"$f":"IF('Profile angles'!G17<0,1000,IF(EF16<0,1000,'Profile angles'!G17))","v":86.172088859931137},{"$f":"IF('Profile angles'!H17<0,1000,IF(EG16<0,1000,'Profile angles'!H17))","v":89.286545413103582},{"$f":"IF('Profile angles'!I17<0,1000,IF(EH16<0,1000,'Profile angles'!I17))","v":86.195448533480899},{"$f":"IF('Profile angles'!J17<0,1000,IF(EI16<0,1000,'Profile angles'!J17))","v":77.690264015558725},{"$f":"IF('Profile angles'!K17<0,1000,IF(EJ16<0,1000,'Profile angles'!K17))","v":65.300000000000011},{"$f":"IF('Profile angles'!L17<0,1000,IF(EK16<0,1000,'Profile angles'!L17))","v":54.1192638814804},{"$f":"IF('Profile angles'!M17<0,1000,IF(EL16<0,1000,'Profile angles'!M17))","v":44.599954197716883},{"$f":"IF('Profile angles'!N17<0,1000,IF(EM16<0,1000,'Profile angles'!N17))","v":41.247836270078757},null,{"$f":"'Profile angles'!B46","v":13},{"$f":"IF('Profile angles'!C46<0,1000,IF(EB16<0,1000,'Profile angles'!C46))","v":1000},{"$f":"IF('Profile angles'!D46<0,1000,IF(EC16<0,1000,'Profile angles'!D46))","v":1000},{"$f":"IF('Profile angles'!E46<0,1000,IF(ED16<0,1000,'Profile angles'!E46))","v":1000},{"$f":"IF('Profile angles'!F46<0,1000,IF(EE16<0,1000,'Profile angles'!F46))","v":1000},{"$f":"IF('Profile angles'!G46<0,1000,IF(EF16<0,1000,'Profile angles'!G46))","v":1000},{"$f":"IF('Profile angles'!H46<0,1000,IF(EG16<0,1000,'Profile angles'!H46))","v":1000},{"$f":"IF('Profile angles'!I46<0,1000,IF(EH16<0,1000,'Profile angles'!I46))","v":1000},{"$f":"IF('Profile angles'!J46<0,1000,IF(EI16<0,1000,'Profile angles'!J46))","v":1000},{"$f":"IF('Profile angles'!K46<0,1000,IF(EJ16<0,1000,'Profile angles'!K46))","v":1000},{"$f":"IF('Profile angles'!L46<0,1000,IF(EK16<0,1000,'Profile angles'!L46))","v":1000},{"$f":"IF('Profile angles'!M46<0,1000,IF(EL16<0,1000,'Profile angles'!M46))","v":1000},{"$f":"IF('Profile angles'!N46<0,1000,IF(EM16<0,1000,'Profile angles'!N46))","v":1000},null,13,{"$f":"'Solar Altitude'!C16","v":44.262516808487675},{"$f":"'Solar Altitude'!D16","v":53.442649547558034},{"$f":"'Solar Altitude'!E16","v":62.96975399076122},{"$f":"'Solar Altitude'!F16","v":71.918657174425832},{"$f":"'Solar Altitude'!G16","v":76.310429689037434},{"$f":"'Solar Altitude'!H16","v":78.190731192893594},{"$f":"'Solar Altitude'!I16","v":78.445286814888803},{"$f":"'Solar Altitude'!J16","v":72.64341275146262},{"$f":"'Solar Altitude'!K16","v":61.303344417053367},{"$f":"'Solar Altitude'!L16","v":50.879096974273239},{"$f":"'Solar Altitude'!M16","v":42.542599664242438},{"$f":"'Solar Altitude'!N16","v":40.072467904514703},null,13,44.262516808487675,53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703]
[null,14,{"$f":"('Solar Azimuth'!C16-'Input Data'!$F$9)","v":-31.28592570493214},{"$f":"('Solar Azimuth'!D16-'Input Data'!$F$9)","v":-37.293205030475256},{"$f":"('Solar Azimuth'!E16-'Input Data'!$F$9)","v":-49.837504769882834},{"$f":"('Solar Azimuth'!F16-'Input Data'!$F$9)","v":-69.769134988610915},{"$f":"('Solar Azimuth'!G16-'Input Data'!$F$9)","v":-86.550699785984065},{"$f":"('Solar Azimuth'!H16-'Input Data'!$F$9)","v":-93.022220626043548},{"$f":"('Solar Azimuth'!I16-'Input Data'!$F$9)","v":-85.700382385824142},{"$f":"('Solar Azimuth'!J16-'Input Data'!$F$9)","v":-69.264391581123419},{"$f":"('Solar Azimuth'!K16-'Input Data'!$F$9)","v":-54.204617869684419},{"$f":"('Solar Azimuth'!L16-'Input Data'!$F$9)","v":-45.278037008383571},{"$f":"('Solar Azimuth'!M16-'Input Data'!$F$9)","v":-37.485193501585897},{"$f":"('Solar Azimuth'!N16-'Input Data'!$F$9)","v":-32.187947719108017},null,14,{"$f":"('Solar Azimuth'!C16-('Input Data'!$F$9+90))","v":-121.28592570493214},{"$f":"('Solar Azimuth'!D16-('Input Data'!$F$9+90))","v":-127.29320503047526},{"$f":"('Solar Azimuth'!E16-('Input Data'!$F$9+90))","v":-139.83750476988283},{"$f":"('Solar Azimuth'!F16-('Input Data'!$F$9+90))","v":-159.76913498861092},{"$f":"('Solar Azimuth'!G16-('Input Data'!$F$9+90))","v":-176.55069978598408},{"$f":"('Solar Azimuth'!H16-('Input Data'!$F$9+90))","v":-183.02222062604355},{"$f":"('Solar Azimuth'!I16-('Input Data'!$F$9+90))","v":-175.70038238582413},{"$f":"('Solar Azimuth'!J16-('Input Data'!$F$9+90))","v":-159.26439158112342},{"$f":"('Solar Azimuth'!K16-('Input Data'!$F$9+90))","v":-144.20461786968443},{"$f":"('Solar Azimuth'!L16-('Input Data'!$F$9+90))","v":-135.27803700838356},{"$f":"('Solar Azimuth'!M16-('Input Data'!$F$9+90))","v":-127.4851935015859},{"$f":"('Solar Azimuth'!N16-('Input Data'!$F$9+90))","v":-122.18794771910802},null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,1.215346258997432,1.5232169054540172,2.3698252115741383,5.4268178445753792,33.181539084901601,37.881173044989119,26.601522701376563,5.2829145881097741,2.7735395285704243,2.0195054514098709,1.5338329813239537,1.2588797548004096,null,14,3.2912431090212069,2.6260212748937035,1.6878881954939753,0.73708020327204837,0.12054895915964599,0.10559335095693795,0.15036733216001241,0.75715780243783948,1.442200465793158,1.9806829425528378,2.6078458663389346,3.1774281735384529,null,14,0.69616343525064206,0.61919577363649569,0.40754369710646543,0,0,0,0,0,0.30661511785739393,0.49512363714753227,0.61654175466901151,0.6852800612998976,null,14,0.17718922274469828,0.34349468127657412,0.57802795112650618,0.81572994918198793,0.96986276021008855,0.9736016622607655,0.96240816695999687,0.8107105493905401,0.63944988355171051,0.50482926436179054,0.34803853341526636,0.20564295661538678,null,{"$f":"'Profile angles'!B18","v":14},{"$f":"IF('Profile angles'!C18<0,1000,IF(EB17<0,1000,'Profile angles'!C18))","v":43.459732841647039},{"$f":"IF('Profile angles'!D18<0,1000,IF(EC17<0,1000,'Profile angles'!D18))","v":53.656578483668653},{"$f":"IF('Profile angles'!E18<0,1000,IF(ED17<0,1000,'Profile angles'!E18))","v":65.3},{"$f":"IF('Profile angles'!F18<0,1000,IF(EE17<0,1000,'Profile angles'!F18))","v":78.783422467977019},{"$f":"IF('Profile angles'!G18<0,1000,IF(EF17<0,1000,'Profile angles'!G18))","v":88.233716701902779},{"$f":"IF('Profile angles'!H18<0,1000,IF(EG17<0,1000,'Profile angles'!H18))","v":1000},{"$f":"IF('Profile angles'!I18<0,1000,IF(EH17<0,1000,'Profile angles'!I18))","v":88.003822246360016},{"$f":"IF('Profile angles'!J18<0,1000,IF(EI17<0,1000,'Profile angles'!J18))","v":78.90115012449813},{"$f":"IF('Profile angles'!K18<0,1000,IF(EJ17<0,1000,'Profile angles'!K18))","v":65.3},{"$f":"IF('Profile angles'!L18<0,1000,IF(EK17<0,1000,'Profile angles'!L18))","v":52.730352015763074},{"$f":"IF('Profile angles'!M18<0,1000,IF(EL17<0,1000,'Profile angles'!M18))","v":42.259093988308607},{"$f":"IF('Profile angles'!N18<0,1000,IF(EM17<0,1000,'Profile angles'!N18))","v":39.004315155295124},null,{"$f":"'Profile angles'!B47","v":14},{"$f":"IF('Profile angles'!C47<0,1000,IF(EB17<0,1000,'Profile angles'!C47))","v":1000},{"$f":"IF('Profile angles'!D47<0,1000,IF(EC17<0,1000,'Profile angles'!D47))","v":1000},{"$f":"IF('Profile angles'!E47<0,1000,IF(ED17<0,1000,'Profile angles'!E47))","v":1000},{"$f":"IF('Profile angles'!F47<0,1000,IF(EE17<0,1000,'Profile angles'!F47))","v":1000},{"$f":"IF('Profile angles'!G47<0,1000,IF(EF17<0,1000,'Profile angles'!G47))","v":1000},{"$f":"IF('Profile angles'!H47<0,1000,IF(EG17<0,1000,'Profile angles'!H47))","v":1000},{"$f":"IF('Profile angles'!I47<0,1000,IF(EH17<0,1000,'Profile angles'!I47))","v":1000},{"$f":"IF('Profile angles'!J47<0,1000,IF(EI17<0,1000,'Profile angles'!J47))","v":1000},{"$f":"IF('Profile angles'!K47<0,1000,IF(EJ17<0,1000,'Profile angles'!K47))","v":1000},{"$f":"IF('Profile angles'!L47<0,1000,IF(EK17<0,1000,'Profile angles'!L47))","v":1000},{"$f":"IF('Profile angles'!M47<0,1000,IF(EL17<0,1000,'Profile angles'!M47))","v":1000},{"$f":"IF('Profile angles'!N47<0,1000,IF(EM17<0,1000,'Profile angles'!N47))","v":1000},null,14,{"$f":"'Solar Altitude'!C17","v":39.001643714284292},{"$f":"'Solar Altitude'!D17","v":47.236569251778789},{"$f":"'Solar Altitude'!E17","v":54.505603493104616},{"$f":"'Solar Altitude'!F17","v":60.167275430762508},{"$f":"'Solar Altitude'!G17","v":62.862961225627508},{"$f":"'Solar Altitude'!H17","v":64.570010808670432},{"$f":"'Solar Altitude'!I17","v":65.066621957768987},{"$f":"'Solar Altitude'!J17","v":61.010544197086858},{"$f":"'Solar Altitude'!K17","v":51.819137025254037},{"$f":"'Solar Altitude'!L17","v":42.759898297268641},{"$f":"'Solar Altitude'!M17","v":35.791762146841563},{"$f":"'Solar Altitude'!N17","v":34.427909280399348},null,14,39.001643714284292,47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348]
[null,15,{"$f":"('Solar Azimuth'!C17-'Input Data'!$F$9)","v":-45.058519967661788},{"$f":"('Solar Azimuth'!D17-'Input Data'!$F$9)","v":-52.457029272774619},{"$f":"('Solar Azimuth'!E17-'Input Data'!$F$9)","v":-64.594569176927493},{"$f":"('Solar Azimuth'!F17-'Input Data'!$F$9)","v":-80.781572637663501},{"$f":"('Solar Azimuth'!G17-'Input Data'!$F$9)","v":-92.938946076383814},{"$f":"('Solar Azimuth'!H17-'Input Data'!$F$9)","v":-97.35546955215915},{"$f":"('Solar Azimuth'!I17-'Input Data'!$F$9)","v":-92.370481478237664},{"$f":"('Solar Azimuth'!J17-'Input Data'!$F$9)","v":-80.54650204480518},{"$f":"('Solar Azimuth'!K17-'Input Data'!$F$9)","v":-67.386703466760636},{"$f":"('Solar Azimuth'!L17-'Input Data'!$F$9)","v":-58.067744603194065},{"$f":"('Solar Azimuth'!M17-'Input Data'!$F$9)","v":-49.756153233223152},{"$f":"('Solar Azimuth'!N17-'Input Data'!$F$9)","v":-44.719738705082868},null,15,{"$f":"('Solar Azimuth'!C17-('Input Data'!$F$9+90))","v":-135.05851996766179},{"$f":"('Solar Azimuth'!D17-('Input Data'!$F$9+90))","v":-142.45702927277461},{"$f":"('Solar Azimuth'!E17-('Input Data'!$F$9+90))","v":-154.59456917692751},{"$f":"('Solar Azimuth'!F17-('Input Data'!$F$9+90))","v":-170.78157263766349},{"$f":"('Solar Azimuth'!G17-('Input Data'!$F$9+90))","v":-182.93894607638381},{"$f":"('Solar Azimuth'!H17-('Input Data'!$F$9+90))","v":-187.35546955215915},{"$f":"('Solar Azimuth'!I17-('Input Data'!$F$9+90))","v":-182.37048147823765},{"$f":"('Solar Azimuth'!J17-('Input Data'!$F$9+90))","v":-170.54650204480518},{"$f":"('Solar Azimuth'!K17-('Input Data'!$F$9+90))","v":-157.38670346676065},{"$f":"('Solar Azimuth'!L17-('Input Data'!$F$9+90))","v":-148.06774460319406},{"$f":"('Solar Azimuth'!M17-('Input Data'!$F$9+90))","v":-139.75615323322316},{"$f":"('Solar Azimuth'!N17-('Input Data'!$F$9+90))","v":-134.71973870508288},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,2.0040896429002015,2.602407206804545,4.210960061012325,12.323259023008628,38.956495851922668,15.493416058645048,48.313463091288696,12.011407449091188,4.8015503656555829,3.2091060065463277,2.3630099729579142,1.9805291565478891,null,15,1.9959187026242171,1.5370384732801048,0.9499021463144417,0.3245894606720221,0.10267863966010557,0.25817418088169602,8.2792657451236026E-2,0.33301676068799585,0.83306425953814978,1.2464530594627632,1.692756292091723,2.0196622638831014,null,15,0.49897758927494962,0.34939819829886376,0,0,0,0,0,0,0,0.19772349836341807,0.40924750676052146,0.50486771086302773,null,15,0.50102032434394572,0.6157403816799738,0.76252446342138958,0.91885263483199453,0.97433034008497366,0.93545645477957595,0.97930183563719098,0.91674580982800102,0.79173393511546253,0.68838673513430915,0.57681092697706926,0.49508443402922464,null,{"$f":"'Profile angles'!B19","v":15},{"$f":"IF('Profile angles'!C19<0,1000,IF(EB18<0,1000,'Profile angles'!C19))","v":39.870560777390224},{"$f":"IF('Profile angles'!D19<0,1000,IF(EC18<0,1000,'Profile angles'!D19))","v":51.621185830048873},{"$f":"IF('Profile angles'!E19<0,1000,IF(ED18<0,1000,'Profile angles'!E19))","v":65.300000000000011},{"$f":"IF('Profile angles'!F19<0,1000,IF(EE18<0,1000,'Profile angles'!F19))","v":81.497322169487106},{"$f":"IF('Profile angles'!G19<0,1000,IF(EF18<0,1000,'Profile angles'!G19))","v":1000},{"$f":"IF('Profile angles'!H19<0,1000,IF(EG18<0,1000,'Profile angles'!H19))","v":1000},{"$f":"IF('Profile angles'!I19<0,1000,IF(EH18<0,1000,'Profile angles'!I19))","v":1000},{"$f":"IF('Profile angles'!J19<0,1000,IF(EI18<0,1000,'Profile angles'!J19))","v":81.541825162483974},{"$f":"IF('Profile angles'!K19<0,1000,IF(EJ18<0,1000,'Profile angles'!K19))","v":65.3},{"$f":"IF('Profile angles'!L19<0,1000,IF(EK18<0,1000,'Profile angles'!L19))","v":49.795844682730099},{"$f":"IF('Profile angles'!M19<0,1000,IF(EL18<0,1000,'Profile angles'!M19))","v":37.488190980331879},{"$f":"IF('Profile angles'!N19<0,1000,IF(EM18<0,1000,'Profile angles'!N19))","v":34.371615174618547},null,{"$f":"'Profile angles'!B48","v":15},{"$f":"IF('Profile angles'!C48<0,1000,IF(EB18<0,1000,'Profile angles'!C48))","v":1000},{"$f":"IF('Profile angles'!D48<0,1000,IF(EC18<0,1000,'Profile angles'!D48))","v":1000},{"$f":"IF('Profile angles'!E48<0,1000,IF(ED18<0,1000,'Profile angles'!E48))","v":1000},{"$f":"IF('Profile angles'!F48<0,1000,IF(EE18<0,1000,'Profile angles'!F48))","v":1000},{"$f":"IF('Profile angles'!G48<0,1000,IF(EF18<0,1000,'Profile angles'!G48))","v":1000},{"$f":"IF('Profile angles'!H48<0,1000,IF(EG18<0,1000,'Profile angles'!H48))","v":1000},{"$f":"IF('Profile angles'!I48<0,1000,IF(EH18<0,1000,'Profile angles'!I48))","v":1000},{"$f":"IF('Profile angles'!J48<0,1000,IF(EI18<0,1000,'Profile angles'!J48))","v":1000},{"$f":"IF('Profile angles'!K48<0,1000,IF(EJ18<0,1000,'Profile angles'!K48))","v":1000},{"$f":"IF('Profile angles'!L48<0,1000,IF(EK18<0,1000,'Profile angles'!L48))","v":1000},{"$f":"IF('Profile angles'!M48<0,1000,IF(EL18<0,1000,'Profile angles'!M48))","v":1000},{"$f":"IF('Profile angles'!N48<0,1000,IF(EM18<0,1000,'Profile angles'!N48))","v":1000},null,15,{"$f":"'Solar Altitude'!C18","v":30.541133571003865},{"$f":"'Solar Altitude'!D18","v":37.574701882546435},{"$f":"'Solar Altitude'!E18","v":43.007444089240849},{"$f":"'Solar Altitude'!F18","v":46.978750874484376},{"$f":"'Solar Altitude'!G18","v":49.242301300948341},{"$f":"'Solar Altitude'!H18","v":51.002542825705397},{"$f":"'Solar Altitude'!I18","v":51.447673176445399},{"$f":"'Solar Altitude'!J18","v":47.843171633901541},{"$f":"'Solar Altitude'!K18","v":39.895074988635152},{"$f":"'Solar Altitude'!L18","v":32.038156511029932},{"$f":"'Solar Altitude'!M18","v":26.359057025099464},{"$f":"'Solar Altitude'!N18","v":25.920295493187655},null,15,30.541133571003865,37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655]
[null,16,{"$f":"('Solar Azimuth'!C18-'Input Data'!$F$9)","v":-55.489647334482406},{"$f":"('Solar Azimuth'!D18-'Input Data'!$F$9)","v":-63.268838319612385},{"$f":"('Solar Azimuth'!E18-'Input Data'!$F$9)","v":-74.451100009483923},{"$f":"('Solar Azimuth'!F18-'Input Data'!$F$9)","v":-88.190523243217299},{"$f":"('Solar Azimuth'!G18-'Input Data'!$F$9)","v":-98.038708423169382},{"$f":"('Solar Azimuth'!H18-'Input Data'!$F$9)","v":-101.47026561710798},{"$f":"('Solar Azimuth'!I18-'Input Data'!$F$9)","v":-97.504147180777991},{"$f":"('Solar Azimuth'!J18-'Input Data'!$F$9)","v":-88.03087166189701},{"$f":"('Solar Azimuth'!K18-'Input Data'!$F$9)","v":-76.484488766275902},{"$f":"('Solar Azimuth'!L18-'Input Data'!$F$9)","v":-67.419407516747285},{"$f":"('Solar Azimuth'!M18-'Input Data'!$F$9)","v":-59.080566092086663},{"$f":"('Solar Azimuth'!N18-'Input Data'!$F$9)","v":-54.377535612582086},null,16,{"$f":"('Solar Azimuth'!C18-('Input Data'!$F$9+90))","v":-145.48964733448241},{"$f":"('Solar Azimuth'!D18-('Input Data'!$F$9+90))","v":-153.26883831961237},{"$f":"('Solar Azimuth'!E18-('Input Data'!$F$9+90))","v":-164.45110000948392},{"$f":"('Solar Azimuth'!F18-('Input Data'!$F$9+90))","v":-178.19052324321729},{"$f":"('Solar Azimuth'!G18-('Input Data'!$F$9+90))","v":-188.0387084231694},{"$f":"('Solar Azimuth'!H18-('Input Data'!$F$9+90))","v":-191.470265617108},{"$f":"('Solar Azimuth'!I18-('Input Data'!$F$9+90))","v":-187.50414718077798},{"$f":"('Solar Azimuth'!J18-('Input Data'!$F$9+90))","v":-178.03087166189701},{"$f":"('Solar Azimuth'!K18-('Input Data'!$F$9+90))","v":-166.48448876627589},{"$f":"('Solar Azimuth'!L18-('Input Data'!$F$9+90))","v":-157.4194075167473},{"$f":"('Solar Azimuth'!M18-('Input Data'!$F$9+90))","v":-149.08056609208666},{"$f":"('Solar Azimuth'!N18-('Input Data'!$F$9+90))","v":-144.37753561258208},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,2.9088919252537493,3.9711753028860199,7.1879392086947735,63.307505302345405,14.161313848302109,9.8564937774812211,15.183015906713186,58.171139425667199,8.3206753801793116,4.8092823364704387,3.3391856742467012,2.79125765827497,null,16,1.3750940573878734,1.0072584801514632,0.55648773366940352,6.3183661730101509E-2,0.28245966743259387,0.40582382440484638,0.26345226960023116,6.8762620768523366E-2,0.48073020725317606,0.83172492695357614,1.197896849776817,1.4330457771039478,null,16,0.27277701868656268,7.2061742784950145E-3,0,0,0,0,0,0,0,0,0.1652035814383247,0.30218558543125751,null,16,0.65622648565303165,0.74818537996213419,0.86087806658264909,0.98420408456747466,0.92938508314185153,0.89854404389878839,0.93413693259994224,0.98280934480786919,0.87981744818670604,0.79206876826160599,0.70052578755579575,0.64173855572401306,null,{"$f":"'Profile angles'!B20","v":16},{"$f":"IF('Profile angles'!C20<0,1000,IF(EB19<0,1000,'Profile angles'!C20))","v":32.771924244272569},{"$f":"IF('Profile angles'!D20<0,1000,IF(EC19<0,1000,'Profile angles'!D20))","v":47.337670667006847},{"$f":"IF('Profile angles'!E20<0,1000,IF(ED19<0,1000,'Profile angles'!E20))","v":65.3},{"$f":"IF('Profile angles'!F20<0,1000,IF(EE19<0,1000,'Profile angles'!F20))","v":87.260389098756136},{"$f":"IF('Profile angles'!G20<0,1000,IF(EF19<0,1000,'Profile angles'!G20))","v":1000},{"$f":"IF('Profile angles'!H20<0,1000,IF(EG19<0,1000,'Profile angles'!H20))","v":1000},{"$f":"IF('Profile angles'!I20<0,1000,IF(EH19<0,1000,'Profile angles'!I20))","v":1000},{"$f":"IF('Profile angles'!J20<0,1000,IF(EI19<0,1000,'Profile angles'!J20))","v":87.115145464657985},{"$f":"IF('Profile angles'!K20<0,1000,IF(EJ19<0,1000,'Profile angles'!K20))","v":65.300000000000011},{"$f":"IF('Profile angles'!L20<0,1000,IF(EK19<0,1000,'Profile angles'!L20))","v":43.332777142141182},{"$f":"IF('Profile angles'!M20<0,1000,IF(EL19<0,1000,'Profile angles'!M20))","v":27.965917871646649},{"$f":"IF('Profile angles'!N20<0,1000,IF(EM19<0,1000,'Profile angles'!N20))","v":25.506940411380103},null,{"$f":"'Profile angles'!B49","v":16},{"$f":"IF('Profile angles'!C49<0,1000,IF(EB19<0,1000,'Profile angles'!C49))","v":1000},{"$f":"IF('Profile angles'!D49<0,1000,IF(EC19<0,1000,'Profile angles'!D49))","v":1000},{"$f":"IF('Profile angles'!E49<0,1000,IF(ED19<0,1000,'Profile angles'!E49))","v":1000},{"$f":"IF('Profile angles'!F49<0,1000,IF(EE19<0,1000,'Profile angles'!F49))","v":1000},{"$f":"IF('Profile angles'!G49<0,1000,IF(EF19<0,1000,'Profile angles'!G49))","v":1000},{"$f":"IF('Profile angles'!H49<0,1000,IF(EG19<0,1000,'Profile angles'!H49))","v":1000},{"$f":"IF('Profile angles'!I49<0,1000,IF(EH19<0,1000,'Profile angles'!I49))","v":1000},{"$f":"IF('Profile angles'!J49<0,1000,IF(EI19<0,1000,'Profile angles'!J49))","v":1000},{"$f":"IF('Profile angles'!K49<0,1000,IF(EJ19<0,1000,'Profile angles'!K49))","v":1000},{"$f":"IF('Profile angles'!L49<0,1000,IF(EK19<0,1000,'Profile angles'!L49))","v":1000},{"$f":"IF('Profile angles'!M49<0,1000,IF(EL19<0,1000,'Profile angles'!M49))","v":1000},{"$f":"IF('Profile angles'!N49<0,1000,IF(EM19<0,1000,'Profile angles'!N49))","v":1000},null,16,{"$f":"'Solar Altitude'!C19","v":20.038281727598083},{"$f":"'Solar Altitude'!D19","v":26.016647471873153},{"$f":"'Solar Altitude'!E19","v":30.233879108991232},{"$f":"'Solar Altitude'!F19","v":33.419767540103443},{"$f":"'Solar Altitude'!G19","v":35.682648220686666},{"$f":"'Solar Altitude'!H19","v":37.56104623172925},{"$f":"'Solar Altitude'!I19","v":37.876258416390314},{"$f":"'Solar Altitude'!J19","v":34.288646107643089},{"$f":"'Solar Altitude'!K19","v":26.935985833021654},{"$f":"'Solar Altitude'!L19","v":19.913519068774189},{"$f":"'Solar Altitude'!M19","v":15.259931573481456},{"$f":"'Solar Altitude'!N19","v":15.530455637101428},null,16,20.038281727598083,26.016647471873153,30.233879108991232,33.419767540103443,35.682648220686666,37.56104623172925,37.876258416390314,34.288646107643089,26.935985833021654,19.913519068774189,15.259931573481456,15.530455637101428]
[null,17,{"$f":"('Solar Azimuth'!C19-'Input Data'!$F$9)","v":-63.539276864661694},{"$f":"('Solar Azimuth'!D19-'Input Data'!$F$9)","v":-71.455355595557094},{"$f":"('Solar Azimuth'!E19-'Input Data'!$F$9)","v":-81.968495986044886},{"$f":"('Solar Azimuth'!F19-'Input Data'!$F$9)","v":-94.337010348548603},{"$f":"('Solar Azimuth'!G19-'Input Data'!$F$9)","v":-102.95522704697413},{"$f":"('Solar Azimuth'!H19-'Input Data'!$F$9)","v":-105.83177114686136},{"$f":"('Solar Azimuth'!I19-'Input Data'!$F$9)","v":-102.37321631179329},{"$f":"('Solar Azimuth'!J19-'Input Data'!$F$9)","v":-94.190598078587101},{"$f":"('Solar Azimuth'!K19-'Input Data'!$F$9)","v":-83.651895994848999},{"$f":"('Solar Azimuth'!L19-'Input Data'!$F$9)","v":-74.778716570691742},{"$f":"('Solar Azimuth'!M19-'Input Data'!$F$9)","v":-66.393607183024301},{"$f":"('Solar Azimuth'!N19-'Input Data'!$F$9)","v":-61.914731817905739},null,17,{"$f":"('Solar Azimuth'!C19-('Input Data'!$F$9+90))","v":-153.5392768646617},{"$f":"('Solar Azimuth'!D19-('Input Data'!$F$9+90))","v":-161.45535559555708},{"$f":"('Solar Azimuth'!E19-('Input Data'!$F$9+90))","v":-171.9684959860449},{"$f":"('Solar Azimuth'!F19-('Input Data'!$F$9+90))","v":-184.3370103485486},{"$f":"('Solar Azimuth'!G19-('Input Data'!$F$9+90))","v":-192.95522704697413},{"$f":"('Solar Azimuth'!H19-('Input Data'!$F$9+90))","v":-195.83177114686134},{"$f":"('Solar Azimuth'!I19-('Input Data'!$F$9+90))","v":-192.37321631179327},{"$f":"('Solar Azimuth'!J19-('Input Data'!$F$9+90))","v":-184.1905980785871},{"$f":"('Solar Azimuth'!K19-('Input Data'!$F$9+90))","v":-173.65189599484899},{"$f":"('Solar Azimuth'!L19-('Input Data'!$F$9+90))","v":-164.77871657069176},{"$f":"('Solar Azimuth'!M19-('Input Data'!$F$9+90))","v":-156.3936071830243},{"$f":"('Solar Azimuth'!N19-('Input Data'!$F$9+90))","v":-151.91473181790573},null,null,null,null,null,null,"Shade Radians",null,null,null,null,null,null,null,null,{"$f":"RADIANS(AK12)","v":1.5707963267948966},null,null,17,4.0182752521401577,5.9619276462022954,14.174184981987658,26.371303241199708,8.6939416079178979,7.0529202264157371,9.1168403323608551,27.296140348853505,17.977380536659513,7.3504303112050398,4.5764272179738388,3.7479861977170321,null,17,0.99545196608161102,0.67092394228366248,0.28220317465047484,0.15168002746829753,0.46009050674518559,0.56714096737101227,0.43874849774452268,0.14654086434487371,0.22250182621673895,0.54418582731168497,0.87404427285330122,1.0672397893131185,null,17,0,0,0,0,0,0,0,0,0,0,0,6.300345057074197E-2,null,17,0.75113700847959719,0.83226901442908441,0.92944920633738126,0.96207999313292558,0.88497737331370363,0.8582147581572469,0.89031287556386929,0.96336478391378155,0.94437454344581528,0.86395354317207873,0.78148893178667467,0.73319005267172033,null,{"$f":"'Profile angles'!B21","v":17},{"$f":"IF('Profile angles'!C21<0,1000,IF(EB20<0,1000,'Profile angles'!C21))","v":18.097147561415554},{"$f":"IF('Profile angles'!D21<0,1000,IF(EC20<0,1000,'Profile angles'!D21))","v":36.90943229885039},{"$f":"IF('Profile angles'!E21<0,1000,IF(ED20<0,1000,'Profile angles'!E21))","v":65.299999999999983},{"$f":"IF('Profile angles'!F21<0,1000,IF(EE20<0,1000,'Profile angles'!F21))","v":1000},{"$f":"IF('Profile angles'!G21<0,1000,IF(EF20<0,1000,'Profile angles'!G21))","v":1000},{"$f":"IF('Profile angles'!H21<0,1000,IF(EG20<0,1000,'Profile angles'!H21))","v":1000},{"$f":"IF('Profile angles'!I21<0,1000,IF(EH20<0,1000,'Profile angles'!I21))","v":1000},{"$f":"IF('Profile angles'!J21<0,1000,IF(EI20<0,1000,'Profile angles'!J21))","v":1000},{"$f":"IF('Profile angles'!K21<0,1000,IF(EJ20<0,1000,'Profile angles'!K21))","v":65.3},{"$f":"IF('Profile angles'!L21<0,1000,IF(EK20<0,1000,'Profile angles'!L21))","v":25.128119824042169},{"$f":"IF('Profile angles'!M21<0,1000,IF(EL20<0,1000,'Profile angles'!M21))","v":7.7999612458558687},{"$f":"IF('Profile angles'!N21<0,1000,IF(EM20<0,1000,'Profile angles'!N21))","v":8.333947337338298},null,{"$f":"'Profile angles'!B50","v":17},{"$f":"IF('Profile angles'!C50<0,1000,IF(EB20<0,1000,'Profile angles'!C50))","v":1000},{"$f":"IF('Profile angles'!D50<0,1000,IF(EC20<0,1000,'Profile angles'!D50))","v":1000},{"$f":"IF('Profile angles'!E50<0,1000,IF(ED20<0,1000,'Profile angles'!E50))","v":1000},{"$f":"IF('Profile angles'!F50<0,1000,IF(EE20<0,1000,'Profile angles'!F50))","v":1000},{"$f":"IF('Profile angles'!G50<0,1000,IF(EF20<0,1000,'Profile angles'!G50))","v":1000},{"$f":"IF('Profile angles'!H50<0,1000,IF(EG20<0,1000,'Profile angles'!H50))","v":1000},{"$f":"IF('Profile angles'!I50<0,1000,IF(EH20<0,1000,'Profile angles'!I50))","v":1000},{"$f":"IF('Profile angles'!J50<0,1000,IF(EI20<0,1000,'Profile angles'!J50))","v":1000},{"$f":"IF('Profile angles'!K50<0,1000,IF(EJ20<0,1000,'Profile angles'!K50))","v":1000},{"$f":"IF('Profile angles'!L50<0,1000,IF(EK20<0,1000,'Profile angles'!L50))","v":1000},{"$f":"IF('Profile angles'!M50<0,1000,IF(EL20<0,1000,'Profile angles'!M50))","v":1000},{"$f":"IF('Profile angles'!N50<0,1000,IF(EM20<0,1000,'Profile angles'!N50))","v":1000},null,17,{"$f":"'Solar Altitude'!C20","v":8.2848854255444504},{"$f":"'Solar Altitude'!D20","v":13.434807821200849},{"$f":"'Solar Altitude'!E20","v":16.897092448538277},{"$f":"'Solar Altitude'!F20","v":19.80224832363653},{"$f":"'Solar Altitude'!G20","v":22.286756355186323},{"$f":"'Solar Altitude'!H20","v":24.319689951925163},{"$f":"'Solar Altitude'!I20","v":24.456964963286701},{"$f":"'Solar Altitude'!J20","v":20.670382142796534},{"$f":"'Solar Altitude'!K20","v":13.51706337533537},{"$f":"'Solar Altitude'!L20","v":7.0202572324504446},{"$f":"'Solar Altitude'!M20","v":3.1397975005302774},{"$f":"'Solar Altitude'!N20","v":3.9451572875932328},null,17,8.2848854255444504,13.434807821200849,16.897092448538277,19.80224832363653,22.286756355186323,24.319689951925163,24.456964963286701,20.670382142796534,13.51706337533537,7.0202572324504446,3.1397975005302774,3.9451572875932328]
[null,18,{"$f":"('Solar Azimuth'!C20-'Input Data'!$F$9)","v":-70.027393642454314},{"$f":"('Solar Azimuth'!D20-'Input Data'!$F$9)","v":-78.184177378909311},{"$f":"('Solar Azimuth'!E20-'Input Data'!$F$9)","v":-88.469586224661327},{"$f":"('Solar Azimuth'!F20-'Input Data'!$F$9)","v":-100.23260842709193},{"$f":"('Solar Azimuth'!G20-'Input Data'!$F$9)","v":-108.21764026515396},{"$f":"('Solar Azimuth'!H20-'Input Data'!$F$9)","v":-110.74646928371035},{"$f":"('Solar Azimuth'!I20-'Input Data'!$F$9)","v":-107.53210586168318},{"$f":"('Solar Azimuth'!J20-'Input Data'!$F$9)","v":-100.0676048936829},{"$f":"('Solar Azimuth'!K20-'Input Data'!$F$9)","v":-90.038304508740268},{"$f":"('Solar Azimuth'!L20-'Input Data'!$F$9)","v":-81.094337680102015},{"$f":"('Solar Azimuth'!M20-'Input Data'!$F$9)","v":-72.41888926958508},{"$f":"('Solar Azimuth'!N20-'Input Data'!$F$9)","v":-67.986814060671676},null,18,{"$f":"('Solar Azimuth'!C20-('Input Data'!$F$9+90))","v":-160.02739364245431},{"$f":"('Solar Azimuth'!D20-('Input Data'!$F$9+90))","v":-168.18417737890931},{"$f":"('Solar Azimuth'!E20-('Input Data'!$F$9+90))","v":-178.46958622466133},{"$f":"('Solar Azimuth'!F20-('Input Data'!$F$9+90))","v":-190.23260842709192},{"$f":"('Solar Azimuth'!G20-('Input Data'!$F$9+90))","v":-198.21764026515396},{"$f":"('Solar Azimuth'!H20-('Input Data'!$F$9+90))","v":-200.74646928371035},{"$f":"('Solar Azimuth'!I20-('Input Data'!$F$9+90))","v":-197.53210586168319},{"$f":"('Solar Azimuth'!J20-('Input Data'!$F$9+90))","v":-190.0676048936829},{"$f":"('Solar Azimuth'!K20-('Input Data'!$F$9+90))","v":-180.03830450874028},{"$f":"('Solar Azimuth'!L20-('Input Data'!$F$9+90))","v":-171.094337680102},{"$f":"('Solar Azimuth'!M20-('Input Data'!$F$9+90))","v":-162.41888926958507},{"$f":"('Solar Azimuth'!N20-('Input Data'!$F$9+90))","v":-157.98681406067169},null,"North",true,{"$f":"IF(AE21,1,0)","v":1},null,null,"Length of third side",null,null,null,null,null,null,null,null,{"$f":"SQRT((AG7^2)+(AG6^2)-(2*(AG6*AG7)*COS(AR20)))","v":4.4721359549995796},null,null,18,5.5031399517667232,9.5602701024262231,74.858386165423227,11.079349760917831,6.0767283992972478,5.2798917832053416,6.3308176881714493,11.264822885349552,2991.5940896429261,12.76348034289985,6.3120181696749285,4.9468956211491015,null,18,0.72685776394181001,0.41839822067211929,5.3434227010461299E-2,0.3610320177913251,0.6582489354736637,0.75759128486751992,0.63182991471601402,0.35508769562654929,1.337079790954339E-3,0.31339414427234541,0.63371173727245489,0.80858791176007261,null,18,0,0,0,0,0,0,0,0,0,0,0,0,null,18,0.81828555901454747,0.89540044483197012,0.98664144324738468,0.90974199555216873,0.83543776613158405,0.81060217878312002,0.84204252132099655,0.91122807609336265,0.99966573005226145,0.92165146393191366,0.84157206568188625,0.79785302205998188,null,{"$f":"'Profile angles'!B22","v":18},{"$f":"IF('Profile angles'!C22<0,1000,IF(EB21<0,1000,'Profile angles'!C22))","v":1000},{"$f":"IF('Profile angles'!D22<0,1000,IF(EC21<0,1000,'Profile angles'!D22))","v":1.391383654081259},{"$f":"IF('Profile angles'!E22<0,1000,IF(ED21<0,1000,'Profile angles'!E22))","v":65.299999999999883},{"$f":"IF('Profile angles'!F22<0,1000,IF(EE21<0,1000,'Profile angles'!F22))","v":1000},{"$f":"IF('Profile angles'!G22<0,1000,IF(EF21<0,1000,'Profile angles'!G22))","v":1000},{"$f":"IF('Profile angles'!H22<0,1000,IF(EG21<0,1000,'Profile angles'!H22))","v":1000},{"$f":"IF('Profile angles'!I22<0,1000,IF(EH21<0,1000,'Profile angles'!I22))","v":1000},{"$f":"IF('Profile angles'!J22<0,1000,IF(EI21<0,1000,'Profile angles'!J22))","v":1000},{"$f":"IF('Profile angles'!K22<0,1000,IF(EJ21<0,1000,'Profile angles'!K22))","v":1000},{"$f":"IF('Profile angles'!L22<0,1000,IF(EK21<0,1000,'Profile angles'!L22))","v":1000},{"$f":"IF('Profile angles'!M22<0,1000,IF(EL21<0,1000,'Profile angles'!M22))","v":1000},{"$f":"IF('Profile angles'!N22<0,1000,IF(EM21<0,1000,'Profile angles'!N22))","v":1000},null,{"$f":"'Profile angles'!B51","v":18},{"$f":"IF('Profile angles'!C51<0,1000,IF(EB21<0,1000,'Profile angles'!C51))","v":1000},{"$f":"IF('Profile angles'!D51<0,1000,IF(EC21<0,1000,'Profile angles'!D51))","v":1000},{"$f":"IF('Profile angles'!E51<0,1000,IF(ED21<0,1000,'Profile angles'!E51))","v":1000},{"$f":"IF('Profile angles'!F51<0,1000,IF(EE21<0,1000,'Profile angles'!F51))","v":1000},{"$f":"IF('Profile angles'!G51<0,1000,IF(EF21<0,1000,'Profile angles'!G51))","v":1000},{"$f":"IF('Profile angles'!H51<0,1000,IF(EG21<0,1000,'Profile angles'!H51))","v":1000},{"$f":"IF('Profile angles'!I51<0,1000,IF(EH21<0,1000,'Profile angles'!I51))","v":1000},{"$f":"IF('Profile angles'!J51<0,1000,IF(EI21<0,1000,'Profile angles'!J51))","v":1000},{"$f":"IF('Profile angles'!K51<0,1000,IF(EJ21<0,1000,'Profile angles'!K51))","v":1000},{"$f":"IF('Profile angles'!L51<0,1000,IF(EK21<0,1000,'Profile angles'!L51))","v":1000},{"$f":"IF('Profile angles'!M51<0,1000,IF(EL21<0,1000,'Profile angles'!M51))","v":1000},{"$f":"IF('Profile angles'!N51<0,1000,IF(EM21<0,1000,'Profile angles'!N51))","v":1000},null,18,{"$f":"'Solar Altitude'!C21","v":-4.242067037456934},{"$f":"'Solar Altitude'!D21","v":0.28496224246637836},{"$f":"'Solar Altitude'!E21","v":3.3232309033445016},{"$f":"'Solar Altitude'!F21","v":6.2903017477886056},{"$f":"'Solar Altitude'!G21","v":9.1618728727979484},{"$f":"'Solar Altitude'!H21","v":11.380032986011807},{"$f":"'Solar Altitude'!I21","v":11.292623329902437},{"$f":"'Solar Altitude'!J21","v":7.1538265372891177},{"$f":"'Solar Altitude'!K21","v":-8.3279910069723753E-2},{"$f":"'Solar Altitude'!L21","v":-6.3024734223343577},{"$f":"'Solar Altitude'!M21","v":-9.6180467382750852},{"$f":"'Solar Altitude'!N21","v":-8.4049479592926772},null,18,-4.242067037456934,0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772]
[null,19,{"$f":"('Solar Azimuth'!C21-'Input Data'!$F$9)","v":-75.556391539792401},{"$f":"('Solar Azimuth'!D21-'Input Data'!$F$9)","v":-84.245727157077454},{"$f":"('Solar Azimuth'!E21-'Input Data'!$F$9)","v":-94.79099889487145},{"$f":"('Solar Azimuth'!F21-'Input Data'!$F$9)","v":-106.54893394025623},{"$f":"('Solar Azimuth'!G21-'Input Data'!$F$9)","v":-114.27191412220648},{"$f":"('Solar Azimuth'!H21-'Input Data'!$F$9)","v":-116.55069372400413},{"$f":"('Solar Azimuth'!I21-'Input Data'!$F$9)","v":-113.41866453412055},{"$f":"('Solar Azimuth'!J21-'Input Data'!$F$9)","v":-106.33684414244284},{"$f":"('Solar Azimuth'!K21-'Input Data'!$F$9)","v":-96.429196681357439},{"$f":"('Solar Azimuth'!L21-'Input Data'!$F$9)","v":-87.064134050269075},{"$f":"('Solar Azimuth'!M21-'Input Data'!$F$9)","v":-77.691193599583684},{"$f":"('Solar Azimuth'!N21-'Input Data'!$F$9)","v":-73.076880837173803},null,19,{"$f":"('Solar Azimuth'!C21-('Input Data'!$F$9+90))","v":-165.5563915397924},{"$f":"('Solar Azimuth'!D21-('Input Data'!$F$9+90))","v":-174.24572715707745},{"$f":"('Solar Azimuth'!E21-('Input Data'!$F$9+90))","v":-184.79099889487145},{"$f":"('Solar Azimuth'!F21-('Input Data'!$F$9+90))","v":-196.54893394025623},{"$f":"('Solar Azimuth'!G21-('Input Data'!$F$9+90))","v":-204.27191412220648},{"$f":"('Solar Azimuth'!H21-('Input Data'!$F$9+90))","v":-206.55069372400413},{"$f":"('Solar Azimuth'!I21-('Input Data'!$F$9+90))","v":-203.41866453412055},{"$f":"('Solar Azimuth'!J21-('Input Data'!$F$9+90))","v":-196.33684414244283},{"$f":"('Solar Azimuth'!K21-('Input Data'!$F$9+90))","v":-186.42919668135744},{"$f":"('Solar Azimuth'!L21-('Input Data'!$F$9+90))","v":-177.06413405026908},{"$f":"('Solar Azimuth'!M21-('Input Data'!$F$9+90))","v":-167.6911935995837},{"$f":"('Solar Azimuth'!N21-('Input Data'!$F$9+90))","v":-163.0768808371738},null,null,null,null,null,null,"Sin of Shade angle at window",null,null,null,null,null,null,null,null,{"$f":"(AG7/AR21)*SIN(AR20)","v":0.44721359549995793},null,null,19,7.7649456024272991,19.847169436799213,23.862321589616478,6.7307722058408661,4.4353045790627483,4.002507104820733,4.6175997495573418,6.8231758966463802,17.748750103620758,38.997438307693677,9.1660593892784732,6.5732382392616566,null,19,0.51513561134924257,0.201540074152009,0.16762828314829903,0.59428545160521973,0.90185463674408117,0.99937361639715461,0.86625091323332171,0.58623726847874702,0.22536798234507777,0.10257083987003367,0.43639254669010696,0.60852807313573087,null,19,0,0,0,0,0,0,0,0,0,0,0,0,null,19,0.87121609716268933,0.94961498146199774,0.95809292921292522,0.8514286370986951,0.77453634081397971,0.75015659590071138,0.78343727169166955,0.85344068288031327,0.9436580044137306,0.97435729003249161,0.89090186332747323,0.84786798171606725,null,{"$f":"'Profile angles'!B23","v":19},{"$f":"IF('Profile angles'!C23<0,1000,IF(EB22<0,1000,'Profile angles'!C23))","v":1000},{"$f":"IF('Profile angles'!D23<0,1000,IF(EC22<0,1000,'Profile angles'!D23))","v":1000},{"$f":"IF('Profile angles'!E23<0,1000,IF(ED22<0,1000,'Profile angles'!E23))","v":1000},{"$f":"IF('Profile angles'!F23<0,1000,IF(EE22<0,1000,'Profile angles'!F23))","v":1000},{"$f":"IF('Profile angles'!G23<0,1000,IF(EF22<0,1000,'Profile angles'!G23))","v":1000},{"$f":"IF('Profile angles'!H23<0,1000,IF(EG22<0,1000,'Profile angles'!H23))","v":1000},{"$f":"IF('Profile angles'!I23<0,1000,IF(EH22<0,1000,'Profile angles'!I23))","v":1000},{"$f":"IF('Profile angles'!J23<0,1000,IF(EI22<0,1000,'Profile angles'!J23))","v":1000},{"$f":"IF('Profile angles'!K23<0,1000,IF(EJ22<0,1000,'Profile angles'!K23))","v":1000},{"$f":"IF('Profile angles'!L23<0,1000,IF(EK22<0,1000,'Profile angles'!L23))","v":1000},{"$f":"IF('Profile angles'!M23<0,1000,IF(EL22<0,1000,'Profile angles'!M23))","v":1000},{"$f":"IF('Profile angles'!N23<0,1000,IF(EM22<0,1000,'Profile angles'!N23))","v":1000},null,{"$f":"'Profile angles'!B52","v":19},{"$f":"IF('Profile angles'!C52<0,1000,IF(EB22<0,1000,'Profile angles'!C52))","v":1000},{"$f":"IF('Profile angles'!D52<0,1000,IF(EC22<0,1000,'Profile angles'!D52))","v":1000},{"$f":"IF('Profile angles'!E52<0,1000,IF(ED22<0,1000,'Profile angles'!E52))","v":1000},{"$f":"IF('Profile angles'!F52<0,1000,IF(EE22<0,1000,'Profile angles'!F52))","v":1000},{"$f":"IF('Profile angles'!G52<0,1000,IF(EF22<0,1000,'Profile angles'!G52))","v":1000},{"$f":"IF('Profile angles'!H52<0,1000,IF(EG22<0,1000,'Profile angles'!H52))","v":1000},{"$f":"IF('Profile angles'!I52<0,1000,IF(EH22<0,1000,'Profile angles'!I52))","v":1000},{"$f":"IF('Profile angles'!J52<0,1000,IF(EI22<0,1000,'Profile angles'!J52))","v":1000},{"$f":"IF('Profile angles'!K52<0,1000,IF(EJ22<0,1000,'Profile angles'!K52))","v":1000},{"$f":"IF('Profile angles'!L52<0,1000,IF(EK22<0,1000,'Profile angles'!L52))","v":1000},{"$f":"IF('Profile angles'!M52<0,1000,IF(EL22<0,1000,'Profile angles'!M52))","v":1000},{"$f":"IF('Profile angles'!N52<0,1000,IF(EM22<0,1000,'Profile angles'!N52))","v":1000},null,19,{"$f":"'Solar Altitude'!C22","v":-17.258784755357599},{"$f":"'Solar Altitude'!D22","v":-13.177535073458104},{"$f":"'Solar Altitude'!E22","v":-10.292097151668569},{"$f":"'Solar Altitude'!F22","v":-6.9635212465343193},{"$f":"'Solar Altitude'!G22","v":-3.5411252469823715},{"$f":"'Solar Altitude'!H22","v":-1.1064784283971907},{"$f":"'Solar Altitude'!I22","v":-1.4750612815819091},{"$f":"'Solar Altitude'!J22","v":-6.1102162570653853},{"$f":"'Solar Altitude'!K22","v":-13.682588857300294},{"$f":"'Solar Altitude'!L22","v":-19.851334869589788},{"$f":"'Solar Altitude'!M22","v":-22.782734775346487},{"$f":"'Solar Altitude'!N22","v":-21.2544074674176},null,19,-17.258784755357599,-13.177535073458104,-10.292097151668569,-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176]
[null,20,{"$f":"('Solar Azimuth'!C22-'Input Data'!$F$9)","v":-80.599865452912837},{"$f":"('Solar Azimuth'!D22-'Input Data'!$F$9)","v":-90.306993062276334},{"$f":"('Solar Azimuth'!E22-'Input Data'!$F$9)","v":-101.68961446594655},{"$f":"('Solar Azimuth'!F22-'Input Data'!$F$9)","v":-113.97185161701486},{"$f":"('Solar Azimuth'!G22-'Input Data'!$F$9)","v":-121.65067573224731},{"$f":"('Solar Azimuth'!H22-'Input Data'!$F$9)","v":-123.69219192139745},{"$f":"('Solar Azimuth'!I22-'Input Data'!$F$9)","v":-120.53929365745837},{"$f":"('Solar Azimuth'!J22-'Input Data'!$F$9)","v":-113.67365388535441},{"$f":"('Solar Azimuth'!K22-'Input Data'!$F$9)","v":-103.61203834195651},{"$f":"('Solar Azimuth'!L22-'Input Data'!$F$9)","v":-93.389012330405194},{"$f":"('Solar Azimuth'!M22-'Input Data'!$F$9)","v":-82.668583232769393},{"$f":"('Solar Azimuth'!N22-'Input Data'!$F$9)","v":-77.541146776659929},null,20,{"$f":"('Solar Azimuth'!C22-('Input Data'!$F$9+90))","v":-170.59986545291284},{"$f":"('Solar Azimuth'!D22-('Input Data'!$F$9+90))","v":-180.30699306227632},{"$f":"('Solar Azimuth'!E22-('Input Data'!$F$9+90))","v":-191.68961446594653},{"$f":"('Solar Azimuth'!F22-('Input Data'!$F$9+90))","v":-203.97185161701486},{"$f":"('Solar Azimuth'!G22-('Input Data'!$F$9+90))","v":-211.65067573224729},{"$f":"('Solar Azimuth'!H22-('Input Data'!$F$9+90))","v":-213.69219192139747},{"$f":"('Solar Azimuth'!I22-('Input Data'!$F$9+90))","v":-210.53929365745836},{"$f":"('Solar Azimuth'!J22-('Input Data'!$F$9+90))","v":-203.67365388535441},{"$f":"('Solar Azimuth'!K22-('Input Data'!$F$9+90))","v":-193.61203834195652},{"$f":"('Solar Azimuth'!L22-('Input Data'!$F$9+90))","v":-183.38901233040519},{"$f":"('Solar Azimuth'!M22-('Input Data'!$F$9+90))","v":-172.66858323276938},{"$f":"('Solar Azimuth'!N22-('Input Data'!$F$9+90))","v":-167.54114677665993},null,"South",true,{"$f":"IF(AE23,1,0)","v":1},null,null,"Shade Angle at window (Radians)",null,null,null,null,null,null,null,null,{"$f":"ASIN(AR22)","v":0.46364760900080609},null,null,20,12.080844592470337,373.26727055993547,9.6664580849627288,4.4980193948280567,3.244520145160624,2.9997590083877665,3.3900077676231657,4.5618254000580603,8.2594157539109343,33.773228874971814,15.544808471997724,9.0521764790055599,null,20,0.33110267824263734,1.0716181984023484E-2,0.41380203222754919,0.8892802918100593,1.2328479470118918,1.3334404493212331,1.1799382993167939,0.87684197644852557,0.48429575640455574,0.11843700271620353,0.25732063583836129,0.44188267973752737,null,20,0,0,0,0,0.18886996370984399,0.25006024790305836,0.15249805809420858,0,0,0,0,0,null,20,0.91722433043934071,0.99732095450399416,0.89654949194311273,0.77767992704748523,0.6917880132470271,0.66663988766969173,0.70501542517080151,0.78078950588786866,0.87892606089886105,0.97039074932094915,0.93566984104040962,0.88952933006561818,null,{"$f":"'Profile angles'!B24","v":20},{"$f":"IF('Profile angles'!C24<0,1000,IF(EB23<0,1000,'Profile angles'!C24))","v":1000},{"$f":"IF('Profile angles'!D24<0,1000,IF(EC23<0,1000,'Profile angles'!D24))","v":1000},{"$f":"IF('Profile angles'!E24<0,1000,IF(ED23<0,1000,'Profile angles'!E24))","v":1000},{"$f":"IF('Profile angles'!F24<0,1000,IF(EE23<0,1000,'Profile angles'!F24))","v":1000},{"$f":"IF('Profile angles'!G24<0,1000,IF(EF23<0,1000,'Profile angles'!G24))","v":1000},{"$f":"IF('Profile angles'!H24<0,1000,IF(EG23<0,1000,'Profile angles'!H24))","v":1000},{"$f":"IF('Profile angles'!I24<0,1000,IF(EH23<0,1000,'Profile angles'!I24))","v":1000},{"$f":"IF('Profile angles'!J24<0,1000,IF(EI23<0,1000,'Profile angles'!J24))","v":1000},{"$f":"IF('Profile angles'!K24<0,1000,IF(EJ23<0,1000,'Profile angles'!K24))","v":1000},{"$f":"IF('Profile angles'!L24<0,1000,IF(EK23<0,1000,'Profile angles'!L24))","v":1000},{"$f":"IF('Profile angles'!M24<0,1000,IF(EL23<0,1000,'Profile angles'!M24))","v":1000},{"$f":"IF('Profile angles'!N24<0,1000,IF(EM23<0,1000,'Profile angles'!N24))","v":1000},null,{"$f":"'Profile angles'!B53","v":20},{"$f":"IF('Profile angles'!C53<0,1000,IF(EB23<0,1000,'Profile angles'!C53))","v":1000},{"$f":"IF('Profile angles'!D53<0,1000,IF(EC23<0,1000,'Profile angles'!D53))","v":1000},{"$f":"IF('Profile angles'!E53<0,1000,IF(ED23<0,1000,'Profile angles'!E53))","v":1000},{"$f":"IF('Profile angles'!F53<0,1000,IF(EE23<0,1000,'Profile angles'!F53))","v":1000},{"$f":"IF('Profile angles'!G53<0,1000,IF(EF23<0,1000,'Profile angles'!G53))","v":1000},{"$f":"IF('Profile angles'!H53<0,1000,IF(EG23<0,1000,'Profile angles'!H53))","v":1000},{"$f":"IF('Profile angles'!I53<0,1000,IF(EH23<0,1000,'Profile angles'!I53))","v":1000},{"$f":"IF('Profile angles'!J53<0,1000,IF(EI23<0,1000,'Profile angles'!J53))","v":1000},{"$f":"IF('Profile angles'!K53<0,1000,IF(EJ23<0,1000,'Profile angles'!K53))","v":1000},{"$f":"IF('Profile angles'!L53<0,1000,IF(EK23<0,1000,'Profile angles'!L53))","v":1000},{"$f":"IF('Profile angles'!M53<0,1000,IF(EL23<0,1000,'Profile angles'!M53))","v":1000},{"$f":"IF('Profile angles'!N53<0,1000,IF(EM23<0,1000,'Profile angles'!N53))","v":1000},null,20,{"$f":"'Solar Altitude'!C23","v":-30.589239677830651},{"$f":"'Solar Altitude'!D23","v":-26.783110901661868},{"$f":"'Solar Altitude'!E23","v":-23.773745192987072},{"$f":"'Solar Altitude'!F23","v":-19.749387170381588},{"$f":"'Solar Altitude'!G23","v":-15.584861719885295},{"$f":"'Solar Altitude'!H23","v":-12.902247652391463},{"$f":"'Solar Altitude'!I23","v":-13.625605199002544},{"$f":"'Solar Altitude'!J23","v":-18.916708643772196},{"$f":"'Solar Altitude'!K23","v":-27.097900221004799},{"$f":"'Solar Altitude'!L23","v":-33.472019280706604},{"$f":"'Solar Altitude'!M23","v":-36.206670576844481},{"$f":"'Solar Altitude'!N23","v":-34.435555539572299},null,20,-30.589239677830651,-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,-12.902247652391463,-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299]
[null,21,{"$f":"('Solar Azimuth'!C23-'Input Data'!$F$9)","v":-85.646972023274472},{"$f":"('Solar Azimuth'!D23-'Input Data'!$F$9)","v":-97.199415582430262},{"$f":"('Solar Azimuth'!E23-'Input Data'!$F$9)","v":-110.18564639081795},{"$f":"('Solar Azimuth'!F23-'Input Data'!$F$9)","v":-123.43780160531772},{"$f":"('Solar Azimuth'!G23-'Input Data'!$F$9)","v":-131.07652361833965},{"$f":"('Solar Azimuth'!H23-'Input Data'!$F$9)","v":-132.785358202845},{"$f":"('Solar Azimuth'!I23-'Input Data'!$F$9)","v":-129.57634581131595},{"$f":"('Solar Azimuth'!J23-'Input Data'!$F$9)","v":-122.98914291063117},{"$f":"('Solar Azimuth'!K23-'Input Data'!$F$9)","v":-112.7437379632493},{"$f":"('Solar Azimuth'!L23-'Input Data'!$F$9)","v":-101.151822128156},{"$f":"('Solar Azimuth'!M23-'Input Data'!$F$9)","v":-87.919466525852556},{"$f":"('Solar Azimuth'!N23-'Input Data'!$F$9)","v":-81.683344132077423},null,21,{"$f":"('Solar Azimuth'!C23-('Input Data'!$F$9+90))","v":-175.64697202327449},{"$f":"('Solar Azimuth'!D23-('Input Data'!$F$9+90))","v":-187.19941558243028},{"$f":"('Solar Azimuth'!E23-('Input Data'!$F$9+90))","v":-200.18564639081796},{"$f":"('Solar Azimuth'!F23-('Input Data'!$F$9+90))","v":-213.4378016053177},{"$f":"('Solar Azimuth'!G23-('Input Data'!$F$9+90))","v":-221.07652361833965},{"$f":"('Solar Azimuth'!H23-('Input Data'!$F$9+90))","v":-222.785358202845},{"$f":"('Solar Azimuth'!I23-('Input Data'!$F$9+90))","v":-219.57634581131595},{"$f":"('Solar Azimuth'!J23-('Input Data'!$F$9+90))","v":-212.98914291063119},{"$f":"('Solar Azimuth'!K23-('Input Data'!$F$9+90))","v":-202.74373796324932},{"$f":"('Solar Azimuth'!L23-('Input Data'!$F$9+90))","v":-191.151822128156},{"$f":"('Solar Azimuth'!M23-('Input Data'!$F$9+90))","v":-177.91946652585256},{"$f":"('Solar Azimuth'!N23-('Input Data'!$F$9+90))","v":-171.68334413207742},null,null,null,null,null,null,"Shade Angle at window (Degrees)",null,null,null,null,null,null,null,null,{"$f":"DEGREES(AR23)","v":26.56505117707799},null,null,21,26.273893675151108,15.832928949472912,5.440045914579926,3.0288091112441542,2.2945402561719939,2.1609109661074113,2.4196178789108935,3.0810079250993034,4.7709207093241863,10.145504397897911,55.053759166178843,13.68165717989673,null,21,0.15224237600470517,0.25263803133109886,0.73528791168463414,1.3206510721162306,1.7432686087073672,1.8510711744896466,1.6531535970466791,1.2982764398021065,0.83841259239175447,0.39426329565524476,7.2656255641437087E-2,0.29236224438348279,null,21,0,0,0,0.24279772218896145,0.42636493595700153,0.45977225847314718,0.39509553027227662,0.22974801872517414,0,0,0,0,null,21,0.96193940599882366,0.93684049216722531,0.81617802207884149,0.66983723197094236,0.5641828478231582,0.53723220637758828,0.58671160073833017,0.67543089004947343,0.79039685190206144,0.90143417608618881,0.9818359360896407,0.92690943890412925,null,{"$f":"'Profile angles'!B25","v":21},{"$f":"IF('Profile angles'!C25<0,1000,IF(EB24<0,1000,'Profile angles'!C25))","v":1000},{"$f":"IF('Profile angles'!D25<0,1000,IF(EC24<0,1000,'Profile angles'!D25))","v":1000},{"$f":"IF('Profile angles'!E25<0,1000,IF(ED24<0,1000,'Profile angles'!E25))","v":1000},{"$f":"IF('Profile angles'!F25<0,1000,IF(EE24<0,1000,'Profile angles'!F25))","v":1000},{"$f":"IF('Profile angles'!G25<0,1000,IF(EF24<0,1000,'Profile angles'!G25))","v":1000},{"$f":"IF('Profile angles'!H25<0,1000,IF(EG24<0,1000,'Profile angles'!H25))","v":1000},{"$f":"IF('Profile angles'!I25<0,1000,IF(EH24<0,1000,'Profile angles'!I25))","v":1000},{"$f":"IF('Profile angles'!J25<0,1000,IF(EI24<0,1000,'Profile angles'!J25))","v":1000},{"$f":"IF('Profile angles'!K25<0,1000,IF(EJ24<0,1000,'Profile angles'!K25))","v":1000},{"$f":"IF('Profile angles'!L25<0,1000,IF(EK24<0,1000,'Profile angles'!L25))","v":1000},{"$f":"IF('Profile angles'!M25<0,1000,IF(EL24<0,1000,'Profile angles'!M25))","v":1000},{"$f":"IF('Profile angles'!N25<0,1000,IF(EM24<0,1000,'Profile angles'!N25))","v":1000},null,{"$f":"'Profile angles'!B54","v":21},{"$f":"IF('Profile angles'!C54<0,1000,IF(EB24<0,1000,'Profile angles'!C54))","v":1000},{"$f":"IF('Profile angles'!D54<0,1000,IF(EC24<0,1000,'Profile angles'!D54))","v":1000},{"$f":"IF('Profile angles'!E54<0,1000,IF(ED24<0,1000,'Profile angles'!E54))","v":1000},{"$f":"IF('Profile angles'!F54<0,1000,IF(EE24<0,1000,'Profile angles'!F54))","v":1000},{"$f":"IF('Profile angles'!G54<0,1000,IF(EF24<0,1000,'Profile angles'!G54))","v":1000},{"$f":"IF('Profile angles'!H54<0,1000,IF(EG24<0,1000,'Profile angles'!H54))","v":1000},{"$f":"IF('Profile angles'!I54<0,1000,IF(EH24<0,1000,'Profile angles'!I54))","v":1000},{"$f":"IF('Profile angles'!J54<0,1000,IF(EI24<0,1000,'Profile angles'!J54))","v":1000},{"$f":"IF('Profile angles'!K54<0,1000,IF(EJ24<0,1000,'Profile angles'!K54))","v":1000},{"$f":"IF('Profile angles'!L54<0,1000,IF(EK24<0,1000,'Profile angles'!L54))","v":1000},{"$f":"IF('Profile angles'!M54<0,1000,IF(EL24<0,1000,'Profile angles'!M54))","v":1000},{"$f":"IF('Profile angles'!N54<0,1000,IF(EM24<0,1000,'Profile angles'!N54))","v":1000},null,21,{"$f":"'Solar Altitude'!C24","v":-44.11375465474292},{"$f":"'Solar Altitude'!D24","v":-40.375142281624065},{"$f":"'Solar Altitude'!E24","v":-36.877998514340369},{"$f":"'Solar Altitude'!F24","v":-31.713766855869693},{"$f":"'Solar Altitude'!G24","v":-26.575515215416551},{"$f":"'Solar Altitude'!H24","v":-23.623016903493113},{"$f":"'Solar Altitude'!I24","v":-24.79570873532365},{"$f":"'Solar Altitude'!J24","v":-30.92280247893752},{"$f":"'Solar Altitude'!K24","v":-40.048756889246128},{"$f":"'Solar Altitude'!L24","v":-46.985407153208357},{"$f":"'Solar Altitude'!M24","v":-49.782532508401836},{"$f":"'Solar Altitude'!N24","v":-47.837496220337762},null,21,-44.11375465474292,-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762]
[null,22,{"$f":"('Solar Azimuth'!C24-'Input Data'!$F$9)","v":-91.529453169268862},{"$f":"('Solar Azimuth'!D24-'Input Data'!$F$9)","v":-106.51792647513759},{"$f":"('Solar Azimuth'!E24-'Input Data'!$F$9)","v":-122.11046729442886},{"$f":"('Solar Azimuth'!F24-'Input Data'!$F$9)","v":-136.34276711408791},{"$f":"('Solar Azimuth'!G24-'Input Data'!$F$9)","v":-143.46901721591678},{"$f":"('Solar Azimuth'!H24-'Input Data'!$F$9)","v":-144.58190194480306},{"$f":"('Solar Azimuth'!I24-'Input Data'!$F$9)","v":-141.41793606781556},{"$f":"('Solar Azimuth'!J24-'Input Data'!$F$9)","v":-135.63829506381219},{"$f":"('Solar Azimuth'!K24-'Input Data'!$F$9)","v":-125.99647723085019},{"$f":"('Solar Azimuth'!L24-'Input Data'!$F$9)","v":-112.86261366161574},{"$f":"('Solar Azimuth'!M24-'Input Data'!$F$9)","v":-94.689514278894165},{"$f":"('Solar Azimuth'!N24-'Input Data'!$F$9)","v":-85.897207065730697},null,22,{"$f":"('Solar Azimuth'!C24-('Input Data'!$F$9+90))","v":-181.52945316926886},{"$f":"('Solar Azimuth'!D24-('Input Data'!$F$9+90))","v":-196.51792647513759},{"$f":"('Solar Azimuth'!E24-('Input Data'!$F$9+90))","v":-212.11046729442887},{"$f":"('Solar Azimuth'!F24-('Input Data'!$F$9+90))","v":-226.34276711408791},{"$f":"('Solar Azimuth'!G24-('Input Data'!$F$9+90))","v":-233.46901721591678},{"$f":"('Solar Azimuth'!H24-('Input Data'!$F$9+90))","v":-234.58190194480306},{"$f":"('Solar Azimuth'!I24-('Input Data'!$F$9+90))","v":-231.41793606781556},{"$f":"('Solar Azimuth'!J24-('Input Data'!$F$9+90))","v":-225.63829506381219},{"$f":"('Solar Azimuth'!K24-('Input Data'!$F$9+90))","v":-215.99647723085019},{"$f":"('Solar Azimuth'!L24-('Input Data'!$F$9+90))","v":-202.86261366161574},{"$f":"('Solar Azimuth'!M24-('Input Data'!$F$9+90))","v":-184.68951427889417},{"$f":"('Solar Azimuth'!N24-('Input Data'!$F$9+90))","v":-175.8972070657307},null,"East",true,{"$f":"IF(AE25,1,0)","v":1},null,null,"Cutoff Angle",null,null,null,null,null,null,null,null,{"$f":"90-AR24","v":63.43494882292201},null,null,22,74.905424953823683,6.7441375859554977,3.1869796629135663,1.9083874042439368,1.4815964922134384,1.4222770294133162,1.5955542096402235,1.9559277551564551,2.7531197925276558,4.743295195028673,24.38110956493119,27.882380142904623,null,22,5.3400671613116311E-2,0.59310771006954288,1.2551068482009584,2.0960104804216706,2.6997904092120133,2.8123916208152386,2.5069659030274796,2.0450653095211258,1.4528971862599469,0.84329560685835003,0.16406144229602501,0.143459775653977,null,22,0,0,0.20325508427160843,0.52290314893901579,0.62960087694664035,0.64443074264667088,0.60111144758994417,0.51101806121088622,0.31172005186808605,0,0,0,null,22,0.98664983209672097,0.85172307248261425,0.6862232879497604,0.47599737989458235,0.32505239769699668,0.29690209479619034,0.37325852424313011,0.48873367261971856,0.63677570343501322,0.78917609828541246,0.95898463942599377,0.96413505608650574,null,{"$f":"'Profile angles'!B26","v":22},{"$f":"IF('Profile angles'!C26<0,1000,IF(EB25<0,1000,'Profile angles'!C26))","v":1000},{"$f":"IF('Profile angles'!D26<0,1000,IF(EC25<0,1000,'Profile angles'!D26))","v":1000},{"$f":"IF('Profile angles'!E26<0,1000,IF(ED25<0,1000,'Profile angles'!E26))","v":1000},{"$f":"IF('Profile angles'!F26<0,1000,IF(EE25<0,1000,'Profile angles'!F26))","v":1000},{"$f":"IF('Profile angles'!G26<0,1000,IF(EF25<0,1000,'Profile angles'!G26))","v":1000},{"$f":"IF('Profile angles'!H26<0,1000,IF(EG25<0,1000,'Profile angles'!H26))","v":1000},{"$f":"IF('Profile angles'!I26<0,1000,IF(EH25<0,1000,'Profile angles'!I26))","v":1000},{"$f":"IF('Profile angles'!J26<0,1000,IF(EI25<0,1000,'Profile angles'!J26))","v":1000},{"$f":"IF('Profile angles'!K26<0,1000,IF(EJ25<0,1000,'Profile angles'!K26))","v":1000},{"$f":"IF('Profile angles'!L26<0,1000,IF(EK25<0,1000,'Profile angles'!L26))","v":1000},{"$f":"IF('Profile angles'!M26<0,1000,IF(EL25<0,1000,'Profile angles'!M26))","v":1000},{"$f":"IF('Profile angles'!N26<0,1000,IF(EM25<0,1000,'Profile angles'!N26))","v":1000},null,{"$f":"'Profile angles'!B55","v":22},{"$f":"IF('Profile angles'!C55<0,1000,IF(EB25<0,1000,'Profile angles'!C55))","v":1000},{"$f":"IF('Profile angles'!D55<0,1000,IF(EC25<0,1000,'Profile angles'!D55))","v":1000},{"$f":"IF('Profile angles'!E55<0,1000,IF(ED25<0,1000,'Profile angles'!E55))","v":1000},{"$f":"IF('Profile angles'!F55<0,1000,IF(EE25<0,1000,'Profile angles'!F55))","v":1000},{"$f":"IF('Profile angles'!G55<0,1000,IF(EF25<0,1000,'Profile angles'!G55))","v":1000},{"$f":"IF('Profile angles'!H55<0,1000,IF(EG25<0,1000,'Profile angles'!H55))","v":1000},{"$f":"IF('Profile angles'!I55<0,1000,IF(EH25<0,1000,'Profile angles'!I55))","v":1000},{"$f":"IF('Profile angles'!J55<0,1000,IF(EI25<0,1000,'Profile angles'!J55))","v":1000},{"$f":"IF('Profile angles'!K55<0,1000,IF(EJ25<0,1000,'Profile angles'!K55))","v":1000},{"$f":"IF('Profile angles'!L55<0,1000,IF(EK25<0,1000,'Profile angles'!L55))","v":1000},{"$f":"IF('Profile angles'!M55<0,1000,IF(EL25<0,1000,'Profile angles'!M55))","v":1000},{"$f":"IF('Profile angles'!N55<0,1000,IF(EM25<0,1000,'Profile angles'!N55))","v":1000},null,22,{"$f":"'Solar Altitude'!C25","v":-57.730536859646747},{"$f":"'Solar Altitude'!D25","v":-53.7124665497957},{"$f":"'Solar Altitude'!E25","v":-49.130640449349315},{"$f":"'Solar Altitude'!F25","v":-42.202232941267965},{"$f":"'Solar Altitude'!G25","v":-35.853933091501311},{"$f":"'Solar Altitude'!H25","v":-32.649969945256942},{"$f":"'Solar Altitude'!I25","v":-34.377195915482893},{"$f":"'Solar Altitude'!J25","v":-41.497131280000914},{"$f":"'Solar Altitude'!K25","v":-51.954064465377563},{"$f":"'Solar Altitude'!L25","v":-60.030194510304511},{"$f":"'Solar Altitude'!M25","v":-63.399939655490947},{"$f":"'Solar Altitude'!N25","v":-61.381330079855132},null,22,-57.730536859646747,-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132]
[null,23,{"$f":"('Solar Azimuth'!C25-'Input Data'!$F$9)","v":-100.94534800876922},{"$f":"('Solar Azimuth'!D25-'Input Data'!$F$9)","v":-122.66538882339935},{"$f":"('Solar Azimuth'!E25-'Input Data'!$F$9)","v":-141.05893592015133},{"$f":"('Solar Azimuth'!F25-'Input Data'!$F$9)","v":-154.36297602700361},{"$f":"('Solar Azimuth'!G25-'Input Data'!$F$9)","v":-159.5630698100631},{"$f":"('Solar Azimuth'!H25-'Input Data'!$F$9)","v":-159.62986186666328},{"$f":"('Solar Azimuth'!I25-'Input Data'!$F$9)","v":-156.86896866670523},{"$f":"('Solar Azimuth'!J25-'Input Data'!$F$9)","v":-153.28158651377788},{"$f":"('Solar Azimuth'!K25-'Input Data'!$F$9)","v":-147.49761169155158},{"$f":"('Solar Azimuth'!L25-'Input Data'!$F$9)","v":-136.46938858849168},{"$f":"('Solar Azimuth'!M25-'Input Data'!$F$9)","v":-108.62615799444323},{"$f":"('Solar Azimuth'!N25-'Input Data'!$F$9)","v":-91.383419869830902},null,23,{"$f":"('Solar Azimuth'!C25-('Input Data'!$F$9+90))","v":-190.9453480087692},{"$f":"('Solar Azimuth'!D25-('Input Data'!$F$9+90))","v":-212.66538882339935},{"$f":"('Solar Azimuth'!E25-('Input Data'!$F$9+90))","v":-231.05893592015133},{"$f":"('Solar Azimuth'!F25-('Input Data'!$F$9+90))","v":-244.36297602700361},{"$f":"('Solar Azimuth'!G25-('Input Data'!$F$9+90))","v":-249.5630698100631},{"$f":"('Solar Azimuth'!H25-('Input Data'!$F$9+90))","v":-249.62986186666328},{"$f":"('Solar Azimuth'!I25-('Input Data'!$F$9+90))","v":-246.86896866670523},{"$f":"('Solar Azimuth'!J25-('Input Data'!$F$9+90))","v":-243.28158651377788},{"$f":"('Solar Azimuth'!K25-('Input Data'!$F$9+90))","v":-237.49761169155158},{"$f":"('Solar Azimuth'!L25-('Input Data'!$F$9+90))","v":-226.46938858849168},{"$f":"('Solar Azimuth'!M25-('Input Data'!$F$9+90))","v":-198.62615799444325},{"$f":"('Solar Azimuth'!N25-('Input Data'!$F$9+90))","v":-181.3834198698309},null,null,null,null,null,null,"Cutoff angle (Side 2)",null,null,null,null,null,null,null,null,{"$f":"90-AR25","v":26.56505117707799},null,null,23,10.341764557378729,3.1194635810799509,1.616164605265149,0.95982898892469137,0.74526108421377935,0.74260701874101931,0.85435285563282681,1.0067006768847977,1.2742577279073264,1.8999609597916522,5.9339167673740292,82.815992452426769,null,23,0.38678118978700277,1.2822717419304526,2.4749954224766335,4.1674090344794088,5.3672465726824301,5.3864290251140092,4.6819062798557196,3.9733756933370383,3.1390823947123114,2.1053064166321813,0.67409101893590329,4.8299849842381351E-2,null,23,0,0.22013410473001227,0.59595884868371274,0.76004275276882716,0.81368472894655519,0.81434824531474514,0.7864117860917933,0.74832483077880063,0.6814355680231684,0.52500976005208688,0,0,null,23,0.90330470255324935,0.6794320645173868,0.38125114438084162,0,0,0,0,6.656076665740418E-3,0.21522940132192214,0.47367339584195467,0.83147724526602418,0.98792503753940464,null,{"$f":"'Profile angles'!B27","v":23},{"$f":"IF('Profile angles'!C27<0,1000,IF(EB26<0,1000,'Profile angles'!C27))","v":1000},{"$f":"IF('Profile angles'!D27<0,1000,IF(EC26<0,1000,'Profile angles'!D27))","v":1000},{"$f":"IF('Profile angles'!E27<0,1000,IF(ED26<0,1000,'Profile angles'!E27))","v":1000},{"$f":"IF('Profile angles'!F27<0,1000,IF(EE26<0,1000,'Profile angles'!F27))","v":1000},{"$f":"IF('Profile angles'!G27<0,1000,IF(EF26<0,1000,'Profile angles'!G27))","v":1000},{"$f":"IF('Profile angles'!H27<0,1000,IF(EG26<0,1000,'Profile angles'!H27))","v":1000},{"$f":"IF('Profile angles'!I27<0,1000,IF(EH26<0,1000,'Profile angles'!I27))","v":1000},{"$f":"IF('Profile angles'!J27<0,1000,IF(EI26<0,1000,'Profile angles'!J27))","v":1000},{"$f":"IF('Profile angles'!K27<0,1000,IF(EJ26<0,1000,'Profile angles'!K27))","v":1000},{"$f":"IF('Profile angles'!L27<0,1000,IF(EK26<0,1000,'Profile angles'!L27))","v":1000},{"$f":"IF('Profile angles'!M27<0,1000,IF(EL26<0,1000,'Profile angles'!M27))","v":1000},{"$f":"IF('Profile angles'!N27<0,1000,IF(EM26<0,1000,'Profile angles'!N27))","v":1000},null,{"$f":"'Profile angles'!B56","v":23},{"$f":"IF('Profile angles'!C56<0,1000,IF(EB26<0,1000,'Profile angles'!C56))","v":1000},{"$f":"IF('Profile angles'!D56<0,1000,IF(EC26<0,1000,'Profile angles'!D56))","v":1000},{"$f":"IF('Profile angles'!E56<0,1000,IF(ED26<0,1000,'Profile angles'!E56))","v":1000},{"$f":"IF('Profile angles'!F56<0,1000,IF(EE26<0,1000,'Profile angles'!F56))","v":1000},{"$f":"IF('Profile angles'!G56<0,1000,IF(EF26<0,1000,'Profile angles'!G56))","v":1000},{"$f":"IF('Profile angles'!H56<0,1000,IF(EG26<0,1000,'Profile angles'!H56))","v":1000},{"$f":"IF('Profile angles'!I56<0,1000,IF(EH26<0,1000,'Profile angles'!I56))","v":1000},{"$f":"IF('Profile angles'!J56<0,1000,IF(EI26<0,1000,'Profile angles'!J56))","v":1000},{"$f":"IF('Profile angles'!K56<0,1000,IF(EJ26<0,1000,'Profile angles'!K56))","v":1000},{"$f":"IF('Profile angles'!L56<0,1000,IF(EK26<0,1000,'Profile angles'!L56))","v":1000},{"$f":"IF('Profile angles'!M56<0,1000,IF(EL26<0,1000,'Profile angles'!M56))","v":1000},{"$f":"IF('Profile angles'!N56<0,1000,IF(EM26<0,1000,'Profile angles'!N56))","v":1000},null,23,{"$f":"'Solar Altitude'!C26","v":-71.276413671366612},{"$f":"'Solar Altitude'!D26","v":-66.153465993410151},{"$f":"'Solar Altitude'!E26","v":-59.402009530792824},{"$f":"'Solar Altitude'!F26","v":-50.011386554405469},{"$f":"'Solar Altitude'!G26","v":-42.39742803240717},{"$f":"'Solar Altitude'!H26","v":-39.064492418979341},{"$f":"'Solar Altitude'!I26","v":-41.409864595350896},{"$f":"'Solar Altitude'!J26","v":-49.478233796277678},{"$f":"'Solar Altitude'!K26","v":-61.393251168859493},{"$f":"'Solar Altitude'!L26","v":-71.378499679687209},{"$f":"'Solar Altitude'!M26","v":-76.771747562226409},{"$f":"'Solar Altitude'!N26","v":-74.998658692112272},null,23,-71.276413671366612,-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272]
[null,24,{"$f":"('Solar Azimuth'!C26-'Input Data'!$F$9)","v":-137.64688656852812},{"$f":"('Solar Azimuth'!D26-'Input Data'!$F$9)","v":-159.57383416203882},{"$f":"('Solar Azimuth'!E26-'Input Data'!$F$9)","v":-171.30077384752721},{"$f":"('Solar Azimuth'!F26-'Input Data'!$F$9)","v":-177.5257986958168},{"$f":"('Solar Azimuth'!G26-'Input Data'!$F$9)","v":-178.72905959747521},{"$f":"('Solar Azimuth'!H26-'Input Data'!$F$9)","v":-177.37410739696531},{"$f":"('Solar Azimuth'!I26-'Input Data'!$F$9)","v":-175.60682113053886},{"$f":"('Solar Azimuth'!J26-'Input Data'!$F$9)","v":-176.11448991066359},{"$f":"('Solar Azimuth'!K26-'Input Data'!$F$9)","v":-179.78063287893619},{"$f":"('Solar Azimuth'!L26-'Input Data'!$F$9)","v":-171.65782889745896},{"$f":"('Solar Azimuth'!M26-'Input Data'!$F$9)","v":-161.86764260752923},{"$f":"('Solar Azimuth'!N26-'Input Data'!$F$9)","v":-134.41945830007725},null,24,{"$f":"('Solar Azimuth'!C26-('Input Data'!$F$9+90))","v":-227.64688656852812},{"$f":"('Solar Azimuth'!D26-('Input Data'!$F$9+90))","v":-249.57383416203882},{"$f":"('Solar Azimuth'!E26-('Input Data'!$F$9+90))","v":-261.30077384752724},{"$f":"('Solar Azimuth'!F26-('Input Data'!$F$9+90))","v":-267.52579869581677},{"$f":"('Solar Azimuth'!G26-('Input Data'!$F$9+90))","v":-268.72905959747521},{"$f":"('Solar Azimuth'!H26-('Input Data'!$F$9+90))","v":-267.37410739696531},{"$f":"('Solar Azimuth'!I26-('Input Data'!$F$9+90))","v":-265.60682113053883},{"$f":"('Solar Azimuth'!J26-('Input Data'!$F$9+90))","v":-266.11448991066356},{"$f":"('Solar Azimuth'!K26-('Input Data'!$F$9+90))","v":-269.78063287893622},{"$f":"('Solar Azimuth'!L26-('Input Data'!$F$9+90))","v":-261.65782889745896},{"$f":"('Solar Azimuth'!M26-('Input Data'!$F$9+90))","v":-251.86764260752923},{"$f":"('Solar Azimuth'!N26-('Input Data'!$F$9+90))","v":-224.41945830007725},null,"West",true,{"$f":"IF(AE27,1,0)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,1.8232519151880098,0.74483319363493783,0.30601536113464184,8.6419642436222133E-2,4.4371467071028382E-2,9.1725173281968345E-2,0.15365210306441027,0.1358381861289035,7.6573944824230231E-3,0.29327198559582457,0.6549511445952011,2.040945734766646,null,24,2.1938822423162105,5.3703299398878599,13.07123925141804,46.285773549133083,90.148022232327591,43.608530318103227,26.032835999148251,29.446800741318963,522.3708938048801,13.639216142221757,6.1073257646907768,1.9598757242104468,null,24,0.54418702120299756,0.81379170159126557,0.92349615971633958,0.97839508939094444,0.98890713323224289,0.97706870667950796,0.96158697423389738,0.96604045346777412,0.9980856513793942,0.92668200360104391,0.8362622138511997,0.4897635663083385,null,24,0.45152943942094736,0,0,0,0,0,0,0,0,0,0,0.51003106894738837,null,{"$f":"'Profile angles'!B28","v":24},{"$f":"IF('Profile angles'!C28<0,1000,IF(EB27<0,1000,'Profile angles'!C28))","v":1000},{"$f":"IF('Profile angles'!D28<0,1000,IF(EC27<0,1000,'Profile angles'!D28))","v":1000},{"$f":"IF('Profile angles'!E28<0,1000,IF(ED27<0,1000,'Profile angles'!E28))","v":1000},{"$f":"IF('Profile angles'!F28<0,1000,IF(EE27<0,1000,'Profile angles'!F28))","v":1000},{"$f":"IF('Profile angles'!G28<0,1000,IF(EF27<0,1000,'Profile angles'!G28))","v":1000},{"$f":"IF('Profile angles'!H28<0,1000,IF(EG27<0,1000,'Profile angles'!H28))","v":1000},{"$f":"IF('Profile angles'!I28<0,1000,IF(EH27<0,1000,'Profile angles'!I28))","v":1000},{"$f":"IF('Profile angles'!J28<0,1000,IF(EI27<0,1000,'Profile angles'!J28))","v":1000},{"$f":"IF('Profile angles'!K28<0,1000,IF(EJ27<0,1000,'Profile angles'!K28))","v":1000},{"$f":"IF('Profile angles'!L28<0,1000,IF(EK27<0,1000,'Profile angles'!L28))","v":1000},{"$f":"IF('Profile angles'!M28<0,1000,IF(EL27<0,1000,'Profile angles'!M28))","v":1000},{"$f":"IF('Profile angles'!N28<0,1000,IF(EM27<0,1000,'Profile angles'!N28))","v":1000},null,{"$f":"'Profile angles'!B57","v":24},{"$f":"IF('Profile angles'!C57<0,1000,IF(EB27<0,1000,'Profile angles'!C57))","v":1000},{"$f":"IF('Profile angles'!D57<0,1000,IF(EC27<0,1000,'Profile angles'!D57))","v":1000},{"$f":"IF('Profile angles'!E57<0,1000,IF(ED27<0,1000,'Profile angles'!E57))","v":1000},{"$f":"IF('Profile angles'!F57<0,1000,IF(EE27<0,1000,'Profile angles'!F57))","v":1000},{"$f":"IF('Profile angles'!G57<0,1000,IF(EF27<0,1000,'Profile angles'!G57))","v":1000},{"$f":"IF('Profile angles'!H57<0,1000,IF(EG27<0,1000,'Profile angles'!H57))","v":1000},{"$f":"IF('Profile angles'!I57<0,1000,IF(EH27<0,1000,'Profile angles'!I57))","v":1000},{"$f":"IF('Profile angles'!J57<0,1000,IF(EI27<0,1000,'Profile angles'!J57))","v":1000},{"$f":"IF('Profile angles'!K57<0,1000,IF(EJ27<0,1000,'Profile angles'!K57))","v":1000},{"$f":"IF('Profile angles'!L57<0,1000,IF(EK27<0,1000,'Profile angles'!L57))","v":1000},{"$f":"IF('Profile angles'!M57<0,1000,IF(EL27<0,1000,'Profile angles'!M57))","v":1000},{"$f":"IF('Profile angles'!N57<0,1000,IF(EM27<0,1000,'Profile angles'!N57))","v":1000},null,24,{"$f":"'Solar Altitude'!C27","v":-83.596484892158756},{"$f":"'Solar Altitude'!D27","v":-75.041691580826409},{"$f":"'Solar Altitude'!E27","v":-65.047371814417531},{"$f":"'Solar Altitude'!F27","v":-53.370409687127484},{"$f":"'Solar Altitude'!G27","v":-44.990343292174892},{"$f":"'Solar Altitude'!H27","v":-41.805581832384377},{"$f":"'Solar Altitude'!I27","v":-44.683864079458822},{"$f":"'Solar Altitude'!J27","v":-53.126563822663151},{"$f":"'Solar Altitude'!K27","v":-65.299840573859427},{"$f":"'Solar Altitude'!L27","v":-75.863131931954825},{"$f":"'Solar Altitude'!M27","v":-84.958601709687045},{"$f":"'Solar Altitude'!N27","v":-88.223048770244205},null,24,-83.596484892158756,-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205]
[null,null,null,null,null,null,null,null,"Horizontal Cutoff",null,null,null,null,{"$f":"'Operative BP'!AH12","v":55.007979801441337},null,null,null,null,null,null,null,null,"Horizontal Cutoff",null,null,null,null,{"$f":"'Operative BP'!AH46","v":59.036243467926482},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Horizontal Cutoff",null,null,null,null,{"$f":"'Operative BP'!CA12","v":1.1397000015522971},null,null,null,null,null,null,null,null,"Horizontal Cutoff",null,null,null,null,{"$f":"'Operative BP'!CA46","v":0.73590361062962995}]
[null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AG16/AR28)*SIN(AR27)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"RADIANS(C4)","v":1.9970598102391},2.5310531156469831,2.6940728938545835,2.7694948249235343,2.8253411080128124,2.8705828375415026,2.8778665437643114,2.7938185762063701,2.5685031327761538,2.2308535264293528,1.8149087756536801,1.6218665373493397,null,1,{"$f":"RADIANS(Q4)","v":0.42626348344420334},0.96025678885208632,1.1232765670596867,1.1986984981286375,1.2545447812179156,1.299786510746606,1.3070702169694146,1.2230222494114735,0.99770680598125705,0.66005719963445619,0.24411244885878353,5.1070210554443142E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"RADIANS(BX4)","v":0},1.1347063869398195E-2,1.3264504628199458E-2,1.4047469653837925E-2,1.4597633306241397E-2,1.502863222645813E-2,1.509696437159708E-2,1.4289813252920405E-2,1.1821673213798921E-2,6.2104622936345229E-3,0,0,null,1,{"$f":"RADIANS(CL4)","v":1.3490467397822786E-2},4.9817066516547135E-3,0,0,0,0,0,0,3.930653504982006E-3,1.0679699624404213E-2,1.5279660810161744E-2,1.700723299140685E-2]
[null,2,{"$f":"RADIANS(C5)","v":1.6834275773076746},2.0348683101963827,2.2717641043769596,2.4348925176477239,2.5361785357446309,2.5922491070791538,2.5798596924944452,2.4545292388121376,2.195543601978446,1.9018086186865921,1.6217606497319532,1.5139281291853537,null,2,{"$f":"RADIANS(Q5)","v":0.11263125051277802},0.46407198340148603,0.70096777758206286,0.86409619085282707,0.96538220894973426,1.021452780284257,1.0090633656995485,0.8837329120172408,0.62474727518354944,0.33101229189169551,5.096432293705655E-2,-5.6868197609542981E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"RADIANS(BX5)","v":0},1.8501124685851417E-5,7.1129793602583225E-3,1.0002419952478456E-2,1.1413453280379371E-2,1.2110819054263314E-2,1.1961035522380216E-2,1.0293855060097928E-2,5.3514433430020044E-3,0,0,0,null,2,{"$f":"RADIANS(CL5)","v":1.6466221978629719E-2},1.3085339200616952E-2,1.0088490915714392E-2,7.2324285530550973E-3,4.8446200162401204E-3,3.1987799920117519E-3,3.5875256811979668E-3,6.8163737153865535E-3,1.1160505869471673E-2,1.445432540183981E-2,1.7008159444432919E-2,1.6956488206753845E-2]
[null,3,{"$f":"RADIANS(C6)","v":1.5542442463766897},1.8031611191726098,2.0142047425451652,2.1939243586452948,2.31211406782645,2.3707261871295522,2.3463504381061453,2.2090385734876463,1.9654728060297433,1.7238812785646462,1.5129572672441984,1.4388328734982576,null,3,{"$f":"RADIANS(Q6)","v":-1.6552080418206955E-2},0.23236479237771329,0.44340841575026874,0.62312803185039822,0.74131774103155357,0.79992986033465552,0.77555411131124863,0.63824224669274987,0.39467647923484672,0.15308495176974971,-5.7839059550698166E-2,-0.13196345329663897,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"RADIANS(BX6)","v":0},0,0,5.3100448655552324E-3,7.9212749440573989E-3,8.9766567394129141E-3,8.5531213458355845E-3,5.6893843998001275E-3,0,0,0,0,null,3,{"$f":"RADIANS(CL6)","v":1.7308835176634136E-2},1.5388226047211436E-2,1.3308562513706304E-2,1.1181959091347846E-2,9.4639708112493805E-3,8.46926195423316E-3,8.8967879924545835E-3,1.0979733378803867E-2,1.3818363967535966E-2,1.6106839787643188E-2,1.6947987906783722E-2,1.6294962468565818E-2]
[null,4,{"$f":"RADIANS(C7)","v":1.4598820135884922},1.6577679183909804,1.8421758266927173,2.0188963800765043,2.1419254692586827,2.1999666374869409,2.1689277327333567,2.0309584914097703,1.8066864979136628,1.5980482755041918,1.4235453334380341,1.3669455371939567,null,4,{"$f":"RADIANS(Q7)","v":-0.11091431320640442},8.6971591596083669E-2,0.27137949989782062,0.44810005328160774,0.5711291424637861,0.62917031069204432,0.59813140593846026,0.46016216461487369,0.23589017111876612,2.7251948709295287E-2,-0.14725099335686243,-0.20385078960093997,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"RADIANS(BX7)","v":0},0,0,0,3.8722900261735351E-3,5.463583998304454E-3,4.6463024896131631E-3,0,0,0,0,0,null,4,{"$f":"RADIANS(CL7)","v":1.6481393843405093E-2},1.669240276594602E-2,1.5025156720070197E-2,1.3258272126873423E-2,1.1845874733103723E-2,1.110164895753017E-2,1.1506980797491359E-2,1.3127923700101268E-2,1.5355711287352641E-2,1.7215415512810011E-2,1.615891638152938E-2,1.5649300910500805E-2]
[null,5,{"$f":"RADIANS(C8)","v":1.3730081623874648},1.5437976258729691,1.7109725157255538,1.8836962495926464,2.0093628854198804,2.066864547068064,2.031484680853143,1.8939622267106639,1.6815916429438205,1.4907949810363581,1.3362448646913618,1.2904640614538805,null,5,{"$f":"RADIANS(Q8)","v":-0.19778816440743177},-2.699870092192758E-2,0.14017618893065711,0.3128999227977497,0.43856655862498395,0.49606822027316749,0.46068835405824654,0.32316589991576744,0.11079531614892379,-8.0001345758538497E-2,-0.23455146210353472,-0.28033226534101602,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"RADIANS(BX8)","v":0},0,0,0,0,1.3289133049773959E-3,0,0,0,0,0,0,null,5,{"$f":"RADIANS(CL8)","v":1.5704399822023304E-2},1.7217627143560111E-2,1.622194888063545E-2,1.4629978369865813E-2,1.3360228686579425E-2,1.2730360000718356E-2,1.3122202255260307E-2,1.4530680369099722E-2,1.6482445155147719E-2,1.6753655829441615E-2,1.5368064717126938E-2,1.4940768018971982E-2]
[null,6,{"$f":"RADIANS(C9)","v":1.2826161490855943},1.439276579498006,1.5975070860924334,1.770615816000789,1.9013148432103089,1.9598314871462639,1.9204101545585393,1.7800171046145765,1.5701277869990202,1.3860713522271735,1.2420065212255516,1.2040608192608664,null,6,{"$f":"RADIANS(Q9)","v":-0.28818017770930227},-0.13151974729689048,2.6710759297536881E-2,0.1998194892058924,0.33051851641541236,0.38903516035136726,0.34961382776364264,0.20922077781967999,-6.6853979587637067E-4,-0.18472497456772313,-0.32878980556934506,-0.36673550753403028,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"RADIANS(BX9)","v":0},0,0,0,0,0,0,0,0,0,0,0,null,6,{"$f":"RADIANS(CL9)","v":1.4866435470606947E-2},1.6298902522212531E-2,1.7220141721295632E-2,1.5685953669890434E-2,1.4459142480655928E-2,1.3876000260901805E-2,1.4271636457992303E-2,1.5600381543907233E-2,1.7447458408764792E-2,1.5822673302309791E-2,1.4475994264920872E-2,1.4101280336758087E-2]
[null,7,{"$f":"RADIANS(C10)","v":1.1806679148430792},1.3312364336904705,1.4871776216199803,1.6671265140205289,1.8081462447703833,1.8702975073672801,1.8256890758056612,1.6764560203146393,1.4585856764469169,1.2721454157699512,1.1327478601164989,1.1017977183534067,null,7,{"$f":"RADIANS(Q10)","v":-0.3901284119518173},-0.23955989310442619,-8.3618705174916222E-2,9.6330187225632344E-2,0.23734991797548677,0.29950118057238351,0.25489274901076453,0.10565969351974271,-0.11221065034797956,-0.29865091102494534,-0.43804846667839764,-0.46899860844148983,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"RADIANS(BX10)","v":0},0,0,0,0,0,0,0,0,0,0,2.3101131827921024E-4,null,7,{"$f":"RADIANS(CL10)","v":1.3864851662732753E-2},1.5321806643148462E-2,1.6721876154842514E-2,1.6610043124532386E-2,1.5342231870826922E-2,1.4758593315287125E-2,1.517947551086089E-2,1.6527791094308363E-2,1.6469939189818785E-2,1.4766718690991408E-2,1.336574317063215E-2,1.3031441891971965E-2]
[null,8,{"$f":"RADIANS(C11)","v":1.058266307319484},1.2078474684986444,1.3667740660753711,1.5618274683649662,1.7220073659413311,1.7919623715483843,1.7394272024332567,1.5719964659947774,1.3332214398200457,1.1360656162861644,0.99854542046976347,0.97573305779876318,null,8,{"$f":"RADIANS(Q11)","v":-0.51253001947541255},-0.36294885829625212,-0.20402226071952556,-8.9688584299304451E-3,0.15121103914643441,0.22116604475348778,0.1686308756383601,1.2001391998807938E-3,-0.23757488697485082,-0.43473071050873219,-0.57225090632513309,-0.59506326899613349,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"RADIANS(BX11)","v":1.9443567533473016E-3},0,0,0,0,0,0,0,0,0,3.9057301433428494E-3,4.5614795205443726E-3,null,8,{"$f":"RADIANS(CL11)","v":1.254293915380823E-2},1.413914568792657E-2,1.564774054148969E-2,1.7375022366363558E-2,1.6123577240328913E-2,1.5491157639392574E-2,1.5967601192915064E-2,1.7442819324654909E-2,1.5340153644269321E-2,1.3400993588758498E-2,1.1832033666895891E-2,1.1546105148374392E-2]
[null,9,{"$f":"RADIANS(C12)","v":0.90353510816893867},1.0538243157320717,1.2184903356318135,1.4390385280672806,1.6341114432554538,1.7195190970203282,1.6534441892541292,1.4515571620245935,1.1738432151253673,0.95928100368681524,0.82587508984596658,0.81498859821827208,null,9,{"$f":"RADIANS(Q12)","v":-0.66726121862595789},-0.51697201106282498,-0.35230599116308309,-0.13175779872761592,6.3315116460557222E-2,0.14872277022543159,8.2647862459232502E-2,-0.11923916477030315,-0.3969531116695294,-0.61151532310808132,-0.74492123694892998,-0.75580772857662459,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"RADIANS(BX12)","v":6.3761411057521146E-3},2.1042907649036924E-3,0,0,0,0,0,0,0,5.0075779405210413E-3,7.9899698630612557E-3,8.1942876363858656E-3,null,9,{"$f":"RADIANS(CL12)","v":1.0578388305028065E-2},1.2491774099263395E-2,1.4244993767690761E-2,1.6296788712961814E-2,1.6900024383522144E-2,1.6145787266651036E-2,1.6730407179908893E-2,1.6407774755903003E-2,1.3795027463088978E-2,1.1334370664496701E-2,9.405975767904284E-3,9.2283962266153218E-3]
[null,10,{"$f":"RADIANS(C13)","v":0.70071538815814005},0.84598427161152567,1.010362948153158,1.265322763274511,1.5275294182792178,1.6462941860249163,1.5536089314055752,1.2837299039160974,0.94253927999738996,0.71378409704331358,0.59801659069868529,0.60640960099999908,null,10,{"$f":"RADIANS(Q13)","v":-0.87008093863675662},-0.72481205518337088,-0.5604333786417387,-0.30547356352038563,-4.3266908515678812E-2,7.5497859230019587E-2,-1.7187395389321281E-2,-0.28706642287879924,-0.6282570467975066,-0.85701222975158298,-0.97277973609621127,-0.96438672579489759,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"RADIANS(BX13)","v":1.0092261347535001E-2},7.5995536330716899E-3,3.5474704419580865E-3,0,0,0,0,0,5.440541249585598E-3,9.8948831290356244E-3,1.1508447843065964E-2,1.1400595808836799E-2,null,10,{"$f":"RADIANS(CL13)","v":7.1076828950132724E-3},9.7248195188838048E-3,1.1976855778584454E-2,1.4701398689520388E-2,1.7075481728006773E-2,1.6793194762599394E-2,1.7303289429327181E-2,1.4877005387175544E-2,1.1113832621643947E-2,7.377845291815322E-3,4.643142030581986E-3,4.8714040524546797E-3]
[null,11,{"$f":"RADIANS(C14)","v":0.4343265159230974},0.5521480379114827,0.67964978242345531,0.93619850107583946,1.3362464729610235,1.5530293407926004,1.3915891659759199,0.97166377450265484,0.56727369074413658,0.3689054188223968,0.30384921089049199,0.34094519238156962,null,11,{"$f":"RADIANS(Q14)","v":-1.136469810871799},-1.0186482888834139,-0.89114654437144136,-0.6345978257190571,-0.2345498538338732,-1.7766986002296141E-2,-0.17920716081897675,-0.59913255229224172,-1.0035226360507601,-1.2018909079724998,-1.2669471159044046,-1.2298511344133272,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,{"$f":"RADIANS(BX14)","v":1.3405280629566555E-2},1.2077114714393111E-2,1.0401444115925463E-2,5.5993438526867811E-3,0,0,0,4.673815463436576E-3,1.1893294302202059E-2,1.4079532260238458E-2,1.4716975476437402E-2,1.4357072334494852E-2,null,11,{"$f":"RADIANS(CL14)","v":0},3.2881443977852182E-3,6.6540877464419624E-3,1.102890541617306E-2,1.5368079553264783E-2,1.7298230001674495E-2,1.5872455709880273E-2,1.1494178965456897E-2,3.7564617001638258E-3,0,0,0]
[null,12,{"$f":"RADIANS(C15)","v":0.10679406055891483},0.15510241273331585,0.15183013873624884,0.11581121919831028,0.20182683522870115,1.0078905398359179,0.64377126699533538,0.18457402284613481,3.8286785332140028E-3,6.1123130165992468E-2,3.8938326923418476E-2,2.972809419232814E-2,null,12,{"$f":"RADIANS(Q15)","v":-1.4640022662359817},-1.415693914061581,-1.4189661880586477,-1.4549851075965863,-1.3689694915661954,-0.56290578695897864,-0.92702505979956129,-1.3862223039487618,-1.5669676482616826,-1.5096731966289041,-1.5318579998714781,-1.5410682326025684,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,{"$f":"RADIANS(BX15)","v":1.6517779323311946E-2},1.6088809360977074E-2,1.6118048616573538E-2,1.6438106273634862E-2,1.5667710350504807E-2,3.6235323313390175E-3,1.0904623367298315E-2,1.5824036559575934E-2,1.7419880833482452E-2,1.6919227323182826E-2,1.7113319676040899E-2,1.7193789507347842E-2,null,12,{"$f":"RADIANS(CL15)","v":0},0,0,0,0,1.1946736085983702E-2,5.8243106349875244E-3,0,0,0,0,0]
[null,13,{"$f":"RADIANS(C16)","v":-0.23968146775368493},-0.28299519000448226,-0.44751975973520858,-0.8264763886659191,-1.292529038821308,-1.5112011188630212,-1.2395029252776819,-0.79795425250097229,-0.57308952081364239,-0.47467850128393096,-0.37473351431083751,-0.28613070031543497,null,13,{"$f":"RADIANS(Q16)","v":-1.8104777945485815},-1.8537915167993788,-2.0183160865301053,-2.3972727154608156,-2.8633253656162041,-3.081997445657918,-2.8102992520725785,-2.368750579295869,-2.143885847608539,-2.0454748280788277,-1.945529841105734,-1.8569270271103315,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,{"$f":"RADIANS(BX16)","v":1.532068237708718E-2},1.4915583913050399E-2,1.3264504628199471E-2,7.9785444486195293E-3,0,0,0,8.5047027579022716E-3,1.1821673213798884E-2,1.2968968740936636E-2,1.4020938199444411E-2,1.4885880343645389E-2,null,13,{"$f":"RADIANS(CL16)","v":0},0,0,9.4156798706776547E-3,1.4960270565261891E-2,1.693260965839101E-2,1.4451582276990999E-2,8.9430851049474829E-3,3.9306535049820892E-3,4.7094273886963677E-4,0,0]
[null,14,{"$f":"RADIANS(C17)","v":-0.54604241308539381},-0.65088921640310549,-0.86982854921283437,-1.217701121819637,-1.5105946811705735,-1.6235440274410409,-1.4957538428507846,-1.2088916874812448,-0.94604905161134778,-0.79025082463613672,-0.65424004734985619,-0.56178566715823386,null,14,{"$f":"RADIANS(Q17)","v":-2.1168387398802904},-2.221685543198002,-2.4406248760077309,-2.7884974486145335,-3.0813910079654705,-3.1943403542359374,-3.0665501696456809,-2.7796880142761413,-2.5168453784062446,-2.3610471514310332,-2.2250363741447527,-2.1325819939531305,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,{"$f":"RADIANS(BX17)","v":1.2150344077118061E-2},1.0807004964390353E-2,7.1129793602583095E-3,0,0,0,0,0,5.3514433430019853E-3,8.6415376726741433E-3,1.0760683594997373E-2,1.1960393367951785E-2,null,14,{"$f":"RADIANS(CL17)","v":3.0925353359446089E-3},5.9951131513647374E-3,1.0088490915714399E-2,1.4237173420351714E-2,1.6927298458146296E-2,1.6992554609340176E-2,1.6797191261535251E-2,1.4149568367517034E-2,1.116050586947168E-2,8.8109328235341147E-3,6.0744183319087035E-3,3.5891466764743536E-3]
[null,15,{"$f":"RADIANS(C18)","v":-0.78641952951130711},-0.91554787662496373,-1.1273879110446283,-1.4099044174661883,-1.622090612366363,-1.6991734885102665,-1.6121690334476861,-1.4058016616461957,-1.1761198475600503,-1.0134733325329046,-0.86840869704656609,-0.78050668103524146,null,15,{"$f":"RADIANS(Q18)","v":-2.3572158563062038},-2.48634420341986,-2.6981842378395253,-2.9807007442610849,-3.1928869391612595,-3.2699698153051631,-3.1829653602425827,-2.976597988441092,-2.7469161743549471,-2.5842696593278012,-2.4392050238414629,-2.351303007830138,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,{"$f":"RADIANS(BX18)","v":8.708801826511816E-3},6.0981489608512235E-3,0,0,0,0,0,0,0,3.450926055003265E-3,7.142716448548852E-3,8.8116038415665763E-3,null,15,{"$f":"RADIANS(CL18)","v":8.7444542792117514E-3},1.0746696997802117E-2,1.3308562513706313E-2,1.6037003818443439E-2,1.7005272436558878E-2,1.6326795144937047E-2,1.7092041402693325E-2,1.6000232785360408E-2,1.3818363967535973E-2,1.2014615055147825E-2,1.0067249837230442E-2,8.6408534491826255E-3]
[null,16,{"$f":"RADIANS(C19)","v":-0.96847704675721324},-1.1042495425891925,-1.299416826897076,-1.5392149996507298,-1.7110982563870039,-1.7709902278917302,-1.7017684026537228,-1.5364285539006752,-1.3349061556761301,-1.1766906409110542,-1.0311504022490317,-0.94906703556002914,null,16,{"$f":"RADIANS(Q19)","v":-2.5392733735521098},-2.6750458693840891,-2.8702131536919726,-3.1100113264456262,-3.2818945831819009,-3.3417865546866268,-3.2725647294486189,-3.107224880695572,-2.9057024824710265,-2.7474869677059508,-2.6019467290439282,-2.5198633623549256,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,{"$f":"RADIANS(BX19)","v":4.760857099854617E-3},1.2577146763226481E-4,0,0,0,0,0,0,0,0,2.8833464321853554E-3,5.2741334178420521E-3,null,16,{"$f":"RADIANS(CL19)","v":1.1453312813436733E-2},1.3058298295624049E-2,1.5025156720070196E-2,1.7177601787279145E-2,1.6220829719746557E-2,1.5682552040218324E-2,1.6303765138349347E-2,1.7153258986265553E-2,1.5355711287352634E-2,1.3824207908380987E-2,1.2226481487974956E-2,1.1200450734377131E-2]
[null,17,{"$f":"RADIANS(C20)","v":-1.108969585624606},-1.2471312233258249,-1.4306201378642391,-1.6464914370701367,-1.7969076941080173,-1.8471128597298661,-1.7867496904971587,-1.6439360608939897,-1.4600010106459727,-1.3051348145742139,-1.1587870476195314,-1.0806159257117494,null,17,{"$f":"RADIANS(Q20)","v":-2.6797659124195028},-2.8179275501207215,-3.0014164646591359,-3.2172877638650332,-3.3677040209029139,-3.4179091865247622,-3.357546017292055,-3.214732387688886,-3.0307973374408688,-2.8759311413691107,-2.7295833744144282,-2.6514122525066459,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,{"$f":"RADIANS(BX20)","v":0},0,0,0,0,0,0,0,0,0,0,1.099617652576948E-3,null,17,{"$f":"RADIANS(CL20)","v":1.3109813931549537E-2},1.4525834564115717E-2,1.622194888063545E-2,1.6791463547733986E-2,1.5445768969975128E-2,1.4978673219050822E-2,1.5538891051488085E-2,1.6813887377059192E-2,1.6482445155147712E-2,1.5078833912623749E-2,1.3639554927570845E-2,1.2796580461992167E-2]
[null,18,{"$f":"RADIANS(C21)","v":-1.2222085856509726},-1.3645713182252377,-1.5440855674973599,-1.749389034914969,-1.8887541313657259,-1.9328905239595118,-1.8767892988894657,-1.7465091799795569,-1.5714648665907731,-1.4153631972418803,-1.2639480583914511,-1.1865937532998967,null,18,{"$f":"RADIANS(Q21)","v":-2.7930049124458693},-2.9353676450201345,-3.1148818942922567,-3.3201853617098651,-3.4595504581606225,-3.5036868507544083,-3.4475856256843627,-3.3173055067744532,-3.1422611933856701,-2.9861595240367764,-2.8347443851863474,-2.7573900800947935,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,{"$f":"RADIANS(BX21)","v":0},0,0,0,0,0,0,0,0,0,0,0,null,18,{"$f":"RADIANS(CL21)","v":1.4281777226326219E-2},1.5627685886139723E-2,1.7220141721295636E-2,1.5877993166048952E-2,1.4581139714502513E-2,1.4147676943605166E-2,1.4696414438845942E-2,1.5903930164442606E-2,1.7447458408764788E-2,1.6085852601437658E-2,1.4688203438958892E-2,1.3925162181933634E-2]
[null,19,{"$f":"RADIANS(C22)","v":-1.3187078032953656},-1.4703653196278037,-1.654415031969813,-1.8596297117474065,-1.994421143988709,-2.0341933509673633,-1.9795291293353241,-1.8559280464656738,-1.6830069771428766,-1.5195557995749016,-1.3559671281170804,-1.2754321776962332,null,19,{"$f":"RADIANS(Q22)","v":-2.8895041300902622},-3.0411616464227005,-3.2252113587647098,-3.4304260385423029,-3.5652174707836055,-3.6049896777622599,-3.5503254561302207,-3.4267243732605701,-3.2538033039377732,-3.0903521263697984,-2.9267634549119772,-2.8462285044911297,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,{"$f":"RADIANS(BX22)","v":0},0,0,0,0,0,0,0,0,0,0,0,null,19,{"$f":"RADIANS(CL22)","v":1.5205589391863757E-2},1.6573908052776778E-2,1.672187615484251E-2,1.4860233063140169E-2,1.3518209323552882E-2,1.3092702504020011E-2,1.3673559873860999E-2,1.489534988673027E-2,1.6469939189818782E-2,1.7005742801876306E-2,1.5549170827216933E-2,1.4798087903184456E-2]
[null,20,{"$f":"RADIANS(C23)","v":-1.4067330288177597},-1.5761543665123987,-1.7748185875144225,-1.9891840653113326,-2.1232048288036793,-2.1588360080371167,-2.1038075523509665,-1.9839795330718792,-1.8083712137697474,-1.6299457503511532,-1.4428389653708038,-1.3533483170249039,null,20,{"$f":"RADIANS(Q23)","v":-2.9775293556126563},-3.146950693307295,-3.3456149143093188,-3.5599803921062292,-3.6940011555985754,-3.7296323348320137,-3.6746038791458631,-3.5547758598667758,-3.3791675405646444,-3.20074207714605,-3.0136352921656999,-2.9241446438198007,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,{"$f":"RADIANS(BX23)","v":0},0,0,0,3.2964027248589818E-3,4.3643746542616144E-3,2.6615932166415288E-3,0,0,0,0,0,null,20,{"$f":"RADIANS(CL23)","v":1.6008584545566942E-2},1.7406534355227269E-2,1.564774054148969E-2,1.3573075253647923E-2,1.2073978556990772E-2,1.163506096496127E-2,1.2304840446578192E-2,1.3627347642762961E-2,1.5340153644269317E-2,1.6936513606545491E-2,1.6330519437767112E-2,1.5525215602704425E-2]
[null,21,{"$f":"RADIANS(C24)","v":-1.494821656169609},-1.6964498329276898,-1.9231023179579798,-2.1543960594363361,-2.2877169092081382,-2.317541699079706,-2.2615338671102263,-2.146565487996356,-1.9677494384644261,-1.7654323405279797,-1.5344841674730674,-1.4256432991443411,null,21,{"$f":"RADIANS(Q24)","v":-3.0656179829645058},-3.2672461597225868,-3.4938986447528766,-3.7251923862312326,-3.8585132360030348,-3.8883380258746025,-3.8323301939051229,-3.717361814791253,-3.5385457652593226,-3.3362286673228763,-3.1052804942679639,-2.9964396259392374,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,{"$f":"RADIANS(BX24)","v":0},0,0,4.2376196685398708E-3,7.4414719475044367E-3,8.0245397196868143E-3,6.8957178631641556E-3,4.0098593766878738E-3,0,0,0,0,null,21,{"$f":"RADIANS(CL24)","v":1.6789009839357966E-2},1.6350951154322228E-2,1.4244993767690757E-2,1.1690865150337971E-2,9.8468482777922337E-3,9.3764708490425945E-3,1.0240049192530255E-2,1.1788492901039118E-2,1.3795027463088978E-2,1.5732994362706327E-2,1.7136269799164848E-2,1.6177621576690275E-2]
[null,22,{"$f":"RADIANS(C25)","v":-1.5974903203537003},-1.8590885293883888,-2.1312297054366356,-2.3796301974206813,-2.5040067250181761,-2.5234302277324065,-2.4682086057582246,-2.3673348406550949,-2.1990533735924034,-1.969824210801528,-1.6526437912808873,-1.4991890815643381,null,22,{"$f":"RADIANS(Q25)","v":-3.1682866471485971},-3.4298848561832855,-3.7020260322315326,-3.9504265242155778,-4.0748030518130731,-4.0942265545273031,-4.0390049325531212,-3.9381311674499915,-3.7698497003872999,-3.5406205375964244,-3.2234401180757839,-3.0699854083592344,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,{"$f":"RADIANS(BX25)","v":0},0,3.5474704419581077E-3,9.1263816180321197E-3,1.0988608276162538E-2,1.1247438260256645E-2,1.0491373931873859E-2,8.9189477052878854E-3,5.4405412495856023E-3,0,0,0,null,22,{"$f":"RADIANS(CL25)","v":1.7220288134337007E-2},1.4865371930023933E-2,1.1976855778584447E-2,8.3077215100267211E-3,5.673234581314625E-3,5.181919110261844E-3,6.5145902091776958E-3,8.5300117525781496E-3,1.1113832621643947E-2,1.3773721293122824E-2,1.6737439434034215E-2,1.6827331162609722E-2]
[null,23,{"$f":"RADIANS(C26)","v":-1.7618286873245246},-2.1409149132073719,-2.4619428711663378,-2.6941421748482886,-2.7849009327751642,-2.7860666740770155,-2.7378799974418255,-2.6752683673459607,-2.5743189628456582,-2.3818401590527567,-1.8958841107945947,-1.5949415584609572,null,23,{"$f":"RADIANS(Q26)","v":-3.3326250141194209},-3.7117112400022685,-4.0327391979612344,-4.2649385016431847,-4.3556972595700607,-4.356863000871912,-4.3086763242367221,-4.2460646941408573,-4.1451152896405548,-3.9526364858476533,-3.4666804375894915,-3.165737885255854,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,{"$f":"RADIANS(BX26)","v":0},3.8420649234687373E-3,1.0401444115925461E-2,1.3265248491737283E-2,1.4201477593315E-2,1.421305813858079E-2,1.3725474943791142E-2,1.3060732171519474E-2,1.1893294302202076E-2,9.1631489180143116E-3,0,0,null,23,{"$f":"RADIANS(CL26)","v":1.576564120830223E-2},1.1858326569450938E-2,6.6540877464419642E-3,0,0,0,0,1.1617045308233635E-4,3.7564617001637772E-3,8.2671603365445274E-3,1.4512015585304556E-2,1.7242544667951189E-2]
[null,24,{"$f":"RADIANS(C27)","v":-2.4023913757399749},-2.785088806158984,-2.9897625148535449,-3.0984096944746589,-3.1194105589691135,-3.0957621818630736,-3.0649172176886541,-3.0737777094114138,-3.1377639750566089,-2.9959943010857266,-2.8251233159428448,-2.3460621260835679,null,24,{"$f":"RADIANS(Q27)","v":-3.9731877025348719},-4.3558851329538806,-4.5605588416484419,-4.669206021269555,-4.6902068857640105,-4.6665585086579702,-4.6357135444835507,-4.6445740362063104,-4.7085603018515059,-4.5667906278806232,-4.3959196427377414,-3.9168584528784645,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,{"$f":"RADIANS(BX27)","v":9.4978552666125007E-3},1.4203344618174761E-2,1.6118048616573549E-2,1.7076215695216224E-2,1.7259685471360874E-2,1.7053065949760127E-2,1.6782858744671388E-2,1.686058662047173E-2,1.7419880833482712E-2,1.6173652081816165E-2,1.4595529041720364E-2,8.5479867883900759E-3,null,24,{"$f":"RADIANS(CL27)","v":7.8806753875798104E-3},0,0,0,0,0,0,0,0,0,0,8.9017214405981374E-3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$error":"#DIV/0!"}]
[]
[null,"Table 7:",null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,"West Surface Azimuth Angles",null,null,null,null,"Table 8:",null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,"North Surface Azimuth Angles",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Table 7:",null,null,"Shading Coefficients",null,null,null,null,null,"West Surface Azimuth Angles",null,null,null,null,"Table 8:",null,null,"Shading Coefficients",null,null,null,null,null,"North Surface Azimuth Angles"]
[null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$f":"'Profile angles'!P4","v":"HR"},{"$f":"'Profile angles'!Q4","v":"Jan"},{"$f":"'Profile angles'!R4","v":"Feb"},{"$f":"'Profile angles'!S4","v":"Mar"},{"$f":"'Profile angles'!T4","v":"Apr"},{"$f":"'Profile angles'!U4","v":"May"},{"$f":"'Profile angles'!V4","v":"Jun"},{"$f":"'Profile angles'!W4","v":"Jul"},{"$f":"'Profile angles'!X4","v":"Aug"},{"$f":"'Profile angles'!Y4","v":"Sep"},{"$f":"'Profile angles'!Z4","v":"Oct"},{"$f":"'Profile angles'!AA4","v":"Nov"},{"$f":"'Profile angles'!AB4","v":"Dec"},null,{"$f":"'Profile angles'!P33","v":"HR"},{"$f":"'Profile angles'!Q33","v":"Jan"},{"$f":"'Profile angles'!R33","v":"Feb"},{"$f":"'Profile angles'!S33","v":"Mar"},{"$f":"'Profile angles'!T33","v":"Apr"},{"$f":"'Profile angles'!U33","v":"May"},{"$f":"'Profile angles'!V33","v":"Jun"},{"$f":"'Profile angles'!W33","v":"Jul"},{"$f":"'Profile angles'!X33","v":"Aug"},{"$f":"'Profile angles'!Y33","v":"Sep"},{"$f":"'Profile angles'!Z33","v":"Oct"},{"$f":"'Profile angles'!AA33","v":"Nov"},{"$f":"'Profile angles'!AB33","v":"Dec"},null,{"$error":"#REF!"},"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$f":"EA57","v":{"$error":"#REF!"}},{"$f":"EB57","v":"Jan"},{"$f":"EC57","v":"Feb"},{"$f":"ED57","v":"Mar"},{"$f":"EE57","v":"Apr"},{"$f":"EF57","v":"May"},{"$f":"EG57","v":"Jun"},{"$f":"EH57","v":"Jul"},{"$f":"EI57","v":"Aug"},{"$f":"EJ57","v":"Sep"},{"$f":"EK57","v":"Oct"},{"$f":"EL57","v":"Nov"},{"$f":"EM57","v":"Dec"}]
[null,1,{"$f":"('Solar Azimuth'!C3-('Input Data'!$F$9-90))","v":204.42309856189749},{"$f":"('Solar Azimuth'!D3-('Input Data'!$F$9-90))","v":235.01866125000959},{"$f":"('Solar Azimuth'!E3-('Input Data'!$F$9-90))","v":244.35900651846384},{"$f":"('Solar Azimuth'!F3-('Input Data'!$F$9-90))","v":248.68036485144134},{"$f":"('Solar Azimuth'!G3-('Input Data'!$F$9-90))","v":251.88012117394979},{"$f":"('Solar Azimuth'!H3-('Input Data'!$F$9-90))","v":254.47228133381614},{"$f":"('Solar Azimuth'!I3-('Input Data'!$F$9-90))","v":254.88960695959625},{"$f":"('Solar Azimuth'!J3-('Input Data'!$F$9-90))","v":250.07401314187376},{"$f":"('Solar Azimuth'!K3-('Input Data'!$F$9-90))","v":237.16438917420371},{"$f":"('Solar Azimuth'!L3-('Input Data'!$F$9-90))","v":217.81849177627836},{"$f":"('Solar Azimuth'!M3-('Input Data'!$F$9-90))","v":193.98661304621146},{"$f":"('Solar Azimuth'!N3-('Input Data'!$F$9-90))","v":182.92610752361406},null,1,{"$f":"('Solar Azimuth'!C3-('Input Data'!$F$9-180))","v":294.42309856189752},{"$f":"('Solar Azimuth'!D3-('Input Data'!$F$9-180))","v":325.01866125000959},{"$f":"('Solar Azimuth'!E3-('Input Data'!$F$9-180))","v":334.35900651846384},{"$f":"('Solar Azimuth'!F3-('Input Data'!$F$9-180))","v":338.68036485144137},{"$f":"('Solar Azimuth'!G3-('Input Data'!$F$9-180))","v":341.88012117394976},{"$f":"('Solar Azimuth'!H3-('Input Data'!$F$9-180))","v":344.47228133381611},{"$f":"('Solar Azimuth'!I3-('Input Data'!$F$9-180))","v":344.88960695959622},{"$f":"('Solar Azimuth'!J3-('Input Data'!$F$9-180))","v":340.07401314187376},{"$f":"('Solar Azimuth'!K3-('Input Data'!$F$9-180))","v":327.16438917420373},{"$f":"('Solar Azimuth'!L3-('Input Data'!$F$9-180))","v":307.81849177627839},{"$f":"('Solar Azimuth'!M3-('Input Data'!$F$9-180))","v":283.98661304621146},{"$f":"('Solar Azimuth'!N3-('Input Data'!$F$9-180))","v":272.92610752361406},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-C58)))/SIN(RADIANS(90-C58))))","v":0.90821261778368101},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-D58)))/SIN(RADIANS(90-D58))))","v":2.8582769363517442},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-E58)))/SIN(RADIANS(90-E58))))","v":4.1666689674939121},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-F58)))/SIN(RADIANS(90-F58))))","v":5.1245449942913472},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-G58)))/SIN(RADIANS(90-G58))))","v":6.111826101727992},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-H58)))/SIN(RADIANS(90-H58))))","v":7.1982423957857717},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-I58)))/SIN(RADIANS(90-I58))))","v":7.406987236558221},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-J58)))/SIN(RADIANS(90-J58))))","v":5.5171193002217374},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-K58)))/SIN(RADIANS(90-K58))))","v":3.0991605737449066},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-L58)))/SIN(RADIANS(90-L58))))","v":1.5523931402167521},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-M58)))/SIN(RADIANS(90-M58))))","v":0.49815969274515193},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-N58)))/SIN(RADIANS(90-N58))))","v":0.10222931358693464},null,1,{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-Q58)))/SIN(RADIANS(90-Q58))))","v":4.4042550408088683},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-R58)))/SIN(RADIANS(90-R58))))","v":1.3994445216723943},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-S58)))/SIN(RADIANS(90-S58))))","v":0.95999946988969564},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-T58)))/SIN(RADIANS(90-T58))))","v":0.78055710398794897},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-U58)))/SIN(RADIANS(90-U58))))","v":0.65446888269106507},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-V58)))/SIN(RADIANS(90-V58))))","v":0.55569120627860658},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-W58)))/SIN(RADIANS(90-W58))))","v":0.54003063219245873},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-X58)))/SIN(RADIANS(90-X58))))","v":0.72501604231020234},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-Y58)))/SIN(RADIANS(90-Y58))))","v":1.290672072265862},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-Z58)))/SIN(RADIANS(90-Z58))))","v":2.5766668869984177},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-AA58)))/SIN(RADIANS(90-AA58))))","v":8.0295536918245141},{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-AB58)))/SIN(RADIANS(90-AB58))))","v":39.127720412584452},null,1,{"$f":"IF(AV58>$AG$6, $AD$17, (1-(AV58/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.77294684555407978},{"$f":"IF(AW58>$AG$6, $AD$17, (1-(AW58/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.28543076591206396},0,0,0,0,0,0,0.22520985656377335,0.61190171494581191,0.87546007681371196,0.97444267160326636,null,1,{"$f":"IF(BJ58>$AG$6, $AD$17, (1-(BJ58/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0},{"$f":"IF(BK58>$AG$6, $AD$17, (1-(BK58/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0.65013886958190148},0.76000013252757603,0.80486072400301278,0.83638277932723371,0.86107719843034836,0.86499234195188535,0.81874598942244936,0.6773319819335345,0.35583327825039557,0,0,null,{"$f":"'Profile angles'!P5","v":1},{"$f":"IF('Profile angles'!Q5<0,1000,IF(EB4<0,1000,'Profile angles'!Q5))","v":1000},{"$f":"IF('Profile angles'!R5<0,1000,IF(EC4<0,1000,'Profile angles'!R5))","v":1000},{"$f":"IF('Profile angles'!S5<0,1000,IF(ED4<0,1000,'Profile angles'!S5))","v":1000},{"$f":"IF('Profile angles'!T5<0,1000,IF(EE4<0,1000,'Profile angles'!T5))","v":1000},{"$f":"IF('Profile angles'!U5<0,1000,IF(EF4<0,1000,'Profile angles'!U5))","v":1000},{"$f":"IF('Profile angles'!V5<0,1000,IF(EG4<0,1000,'Profile angles'!V5))","v":1000},{"$f":"IF('Profile angles'!W5<0,1000,IF(EH4<0,1000,'Profile angles'!W5))","v":1000},{"$f":"IF('Profile angles'!X5<0,1000,IF(EI4<0,1000,'Profile angles'!X5))","v":1000},{"$f":"IF('Profile angles'!Y5<0,1000,IF(EJ4<0,1000,'Profile angles'!Y5))","v":1000},{"$f":"IF('Profile angles'!Z5<0,1000,IF(EK4<0,1000,'Profile angles'!Z5))","v":1000},{"$f":"IF('Profile angles'!AA5<0,1000,IF(EL4<0,1000,'Profile angles'!AA5))","v":1000},{"$f":"IF('Profile angles'!AB5<0,1000,IF(EM4<0,1000,'Profile angles'!AB5))","v":1000},null,{"$f":"'Profile angles'!P34","v":1},{"$f":"IF('Profile angles'!Q34<0,1000,IF(EB4<0,1000,'Profile angles'!Q34))","v":1000},{"$f":"IF('Profile angles'!R34<0,1000,IF(EC4<0,1000,'Profile angles'!R34))","v":1000},{"$f":"IF('Profile angles'!S34<0,1000,IF(ED4<0,1000,'Profile angles'!S34))","v":1000},{"$f":"IF('Profile angles'!T34<0,1000,IF(EE4<0,1000,'Profile angles'!T34))","v":1000},{"$f":"IF('Profile angles'!U34<0,1000,IF(EF4<0,1000,'Profile angles'!U34))","v":1000},{"$f":"IF('Profile angles'!V34<0,1000,IF(EG4<0,1000,'Profile angles'!V34))","v":1000},{"$f":"IF('Profile angles'!W34<0,1000,IF(EH4<0,1000,'Profile angles'!W34))","v":1000},{"$f":"IF('Profile angles'!X34<0,1000,IF(EI4<0,1000,'Profile angles'!X34))","v":1000},{"$f":"IF('Profile angles'!Y34<0,1000,IF(EJ4<0,1000,'Profile angles'!Y34))","v":1000},{"$f":"IF('Profile angles'!Z34<0,1000,IF(EK4<0,1000,'Profile angles'!Z34))","v":1000},{"$f":"IF('Profile angles'!AA34<0,1000,IF(EL4<0,1000,'Profile angles'!AA34))","v":1000},{"$f":"IF('Profile angles'!AB34<0,1000,IF(EM4<0,1000,'Profile angles'!AB34))","v":1000},null,1,{"$f":"EB4","v":-79.238745258454912},{"$f":"EC4","v":-73.135890206899091},-62.969753990761212,-51.103815741194268,-42.972420763986918,-40.259838967181594,-43.397326661656273,-51.194813940312706,-61.30334441705341,-68.588756925018274,-73.864057818332,-77.510392918823513,null,{"$f":"EA58","v":1},{"$f":"EP4","v":-79.238745258454912},{"$f":"EQ4","v":-73.135890206899091},-62.969753990761212,-51.103815741194268,-42.972420763986918,-40.259838967181594,-43.397326661656273,-51.194813940312706,-61.30334441705341,-68.588756925018274,-73.864057818332,-77.510392918823513]
[null,2,{"$f":"('Solar Azimuth'!C4-('Input Data'!$F$9-90))","v":186.45329529566288},{"$f":"('Solar Azimuth'!D4-('Input Data'!$F$9-90))","v":206.58936603917033},{"$f":"('Solar Azimuth'!E4-('Input Data'!$F$9-90))","v":220.1624952301172},{"$f":"('Solar Azimuth'!F4-('Input Data'!$F$9-90))","v":229.50906482919788},{"$f":"('Solar Azimuth'!G4-('Input Data'!$F$9-90))","v":235.31232618983634},{"$f":"('Solar Azimuth'!H4-('Input Data'!$F$9-90))","v":238.52493328219171},{"$f":"('Solar Azimuth'!I4-('Input Data'!$F$9-90))","v":237.81507211585009},{"$f":"('Solar Azimuth'!J4-('Input Data'!$F$9-90))","v":230.63416607539401},{"$f":"('Solar Azimuth'!K4-('Input Data'!$F$9-90))","v":215.7953821303156},{"$f":"('Solar Azimuth'!L4-('Input Data'!$F$9-90))","v":198.96560729234665},{"$f":"('Solar Azimuth'!M4-('Input Data'!$F$9-90))","v":182.92004061003513},{"$f":"('Solar Azimuth'!N4-('Input Data'!$F$9-90))","v":176.74169228845722},null,2,{"$f":"('Solar Azimuth'!C4-('Input Data'!$F$9+180))","v":-83.546704704337131},{"$f":"('Solar Azimuth'!D4-('Input Data'!$F$9+180))","v":-63.410633960829657},{"$f":"('Solar Azimuth'!E4-('Input Data'!$F$9+180))","v":-49.837504769882798},{"$f":"('Solar Azimuth'!F4-('Input Data'!$F$9+180))","v":-40.490935170802118},{"$f":"('Solar Azimuth'!G4-('Input Data'!$F$9+180))","v":-34.687673810163659},{"$f":"('Solar Azimuth'!H4-('Input Data'!$F$9+180))","v":-31.475066717808289},{"$f":"('Solar Azimuth'!I4-('Input Data'!$F$9+180))","v":-32.184927884149914},{"$f":"('Solar Azimuth'!J4-('Input Data'!$F$9+180))","v":-39.365833924605994},{"$f":"('Solar Azimuth'!K4-('Input Data'!$F$9+180))","v":-54.204617869684384},{"$f":"('Solar Azimuth'!L4-('Input Data'!$F$9+180))","v":-71.034392707653367},{"$f":"('Solar Azimuth'!M4-('Input Data'!$F$9+180))","v":-87.079959389964884},{"$f":"('Solar Azimuth'!N4-('Input Data'!$F$9+180))","v":-93.25830771154277},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-C59)))/SIN(RADIANS(90-C59))))","v":0.22621990439584697},1.001061161230232,1.6878881954939773,2.3424494731201366,2.8896948788993622,3.2668936274673417,3.1777996782902438,2.4378022180977688,1.4422004657931595,0.6873126350633656,0.10201698619369085,0.11385916155860504,null,2,{"$f":"ABS($AG$7*(SIN(RADIANS(180-$AK$12-(90-Q59)))/SIN(RADIANS(90-Q59))))","v":17.681910045371943},3.9957598545570243,2.3698252115741356,1.7076142072221565,1.3842291894580694,1.224404726976372,1.2587325838462311,1.6408222005480098,2.7735395285704216,5.8197678842776241,39.209156722249432,35.131121160954244,null,2,{"$f":"IF(AV59>$AG$6, $AD$17, (1-(AV59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.94344502390103824},{"$f":"IF(AW59>$AG$6, $AD$17, (1-(AW59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.74973470969244205},{"$f":"IF(AX59>$AG$6, $AD$17, (1-(AX59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.57802795112650562},{"$f":"IF(AY59>$AG$6, $AD$17, (1-(AY59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.41438763171996584},{"$f":"IF(AZ59>$AG$6, $AD$17, (1-(AZ59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.27757628027515946},{"$f":"IF(BA59>$AG$6, $AD$17, (1-(BA59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.18327659313316458},{"$f":"IF(BB59>$AG$6, $AD$17, (1-(BB59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.20555008042743905},{"$f":"IF(BC59>$AG$6, $AD$17, (1-(BC59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.39054944547555781},{"$f":"IF(BD59>$AG$6, $AD$17, (1-(BD59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.63944988355171017},{"$f":"IF(BE59>$AG$6, $AD$17, (1-(BE59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.82817184123415855},{"$f":"IF(BF59>$AG$6, $AD$17, (1-(BF59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.97449575345157724},{"$f":"IF(BG59>$AG$6, $AD$17, (1-(BG59/$AG$6)*(1-$AD$17)))*$AF$27+(1-$AF$27)","v":0.97153520961034878},null,2,{"$f":"IF(BJ59>$AG$6, $AD$17, (1-(BJ59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0},{"$f":"IF(BK59>$AG$6, $AD$17, (1-(BK59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":1.0600363607439212E-3},{"$f":"IF(BL59>$AG$6, $AD$17, (1-(BL59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0.4075436971064661},{"$f":"IF(BM59>$AG$6, $AD$17, (1-(BM59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0.57309644819446093},{"$f":"IF(BN59>$AG$6, $AD$17, (1-(BN59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0.65394270263548271},{"$f":"IF(BO59>$AG$6, $AD$17, (1-(BO59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0.69389881825590694},{"$f":"IF(BP59>$AG$6, $AD$17, (1-(BP59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0.68531685403844222},{"$f":"IF(BQ59>$AG$6, $AD$17, (1-(BQ59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0.58979444986299756},{"$f":"IF(BR59>$AG$6, $AD$17, (1-(BR59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0.30661511785739459},{"$f":"IF(BS59>$AG$6, $AD$17, (1-(BS59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0},{"$f":"IF(BT59>$AG$6, $AD$17, (1-(BT59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0},{"$f":"IF(BU59>$AG$6, $AD$17, (1-(BU59/$AG$6)*(1-$AD$17)))*$AF$21+(1-$AF$21)","v":0},null,{"$f":"'Profile angles'!P6","v":2},{"$f":"IF('Profile angles'!Q6<0,1000,IF(EB5<0,1000,'Profile angles'!Q6))","v":1000},{"$f":"IF('Profile angles'!R6<0,1000,IF(EC5<0,1000,'Profile angles'!R6))","v":1000},{"$f":"IF('Profile angles'!S6<0,1000,IF(ED5<0,1000,'Profile angles'!S6))","v":1000},{"$f":"IF('Profile angles'!T6<0,1000,IF(EE5<0,1000,'Profile angles'!T6))","v":1000},{"$f":"IF('Profile angles'!U6<0,1000,IF(EF5<0,1000,'Profile angles'!U6))","v":1000},{"$f":"IF('Profile angles'!V6<0,1000,IF(EG5<0,1000,'Profile angles'!V6))","v":1000},{"$f":"IF('Profile angles'!W6<0,1000,IF(EH5<0,1000,'Profile angles'!W6))","v":1000},{"$f":"IF('Profile angles'!X6<0,1000,IF(EI5<0,1000,'Profile angles'!X6))","v":1000},{"$f":"IF('Profile angles'!Y6<0,1000,IF(EJ5<0,1000,'Profile angles'!Y6))","v":1000},{"$f":"IF('Profile angles'!Z6<0,1000,IF(EK5<0,1000,'Profile angles'!Z6))","v":1000},{"$f":"IF('Profile angles'!AA6<0,1000,IF(EL5<0,1000,'Profile angles'!AA6))","v":1000},{"$f":"IF('Profile angles'!AB6<0,1000,IF(EM5<0,1000,'Profile angles'!AB6))","v":1000},null,{"$f":"'Profile angles'!P35","v":2},{"$f":"IF('Profile angles'!Q35<0,1000,IF(EB5<0,1000,'Profile angles'!Q35))","v":1000},{"$f":"IF('Profile angles'!R35<0,1000,IF(EC5<0,1000,'Profile angles'!R35))","v":1000},{"$f":"IF('Profile angles'!S35<0,1000,IF(ED5<0,1000,'Profile angles'!S35))","v":1000},{"$f":"IF('Profile angles'!T35<0,1000,IF(EE5<0,1000,'Profile angles'!T35))","v":1000},{"$f":"IF('Profile angles'!U35<0,1000,IF(EF5<0,1000,'Profile angles'!U35))","v":1000},{"$f":"IF('Profile angles'!V35<0,1000,IF(EG5<0,1000,'Profile angles'!V35))","v":1000},{"$f":"IF('Profile angles'!W35<0,1000,IF(EH5<0,1000,'Profile angles'!W35))","v":1000},{"$f":"IF('Profile angles'!X35<0,1000,IF(EI5<0,1000,'Profile angles'!X35))","v":1000},{"$f":"IF('Profile angles'!Y35<0,1000,IF(EJ5<0,1000,'Profile angles'!Y35))","v":1000},{"$f":"IF('Profile angles'!Z35<0,1000,IF(EK5<0,1000,'Profile angles'!Z35))","v":1000},{"$f":"IF('Profile angles'!AA35<0,1000,IF(EL5<0,1000,'Profile angles'!AA35))","v":1000},{"$f":"IF('Profile angles'!AB35<0,1000,IF(EM5<0,1000,'Profile angles'!AB35))","v":1000},null,2,{"$f":"EB5","v":-66.037221876299029},-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697,null,2,{"$f":"EP5","v":-66.037221876299029},-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697]
[null,3,{"$f":"('Solar Azimuth'!C5-('Input Data'!$F$9-90))","v":179.05163564987561},{"$f":"('Solar Azimuth'!D5-('Input Data'!$F$9-90))","v":193.31352191067663},{"$f":"('Solar Azimuth'!E5-('Input Data'!$F$9-90))","v":205.40543082307255},{"$f":"('Solar Azimuth'!F5-('Input Data'!$F$9-90))","v":215.70260632132135},{"$f":"('Solar Azimuth'!G5-('Input Data'!$F$9-90))","v":222.47437783928015},{"$f":"('Solar Azimuth'!H5-('Input Data'!$F$9-90))","v":225.83260490366516},{"$f":"('Solar Azimuth'!I5-('Input Data'!$F$9-90))","v":224.43597736215381},{"$f":"('Solar Azimuth'!J5-('Input Data'!$F$9-90))","v":216.56858704244209},{"$f":"('Solar Azimuth'!K5-('Input Data'!$F$9-90))","v":202.61329653323941},{"$f":"('Solar Azimuth'!L5-('Input Data'!$F$9-90))","v":188.77112164337041},{"$f":"('Solar Azimuth'!M5-('Input Data'!$F$9-90))","v":176.68606599673916},{"$f":"('Solar Azimuth'!N5-('Input Data'!$F$9-90))","v":172.43905107613085},null,3,{"$f":"('Solar Azimuth'!C5-('Input Data'!$F$9+180))","v":-90.948364350124393},{"$f":"('Solar Azimuth'!D5-('Input Data'!$F$9+180))","v":-76.686478089323387},{"$f":"('Solar Azimuth'!E5-('Input Data'!$F$9+180))","v":-64.594569176927465},{"$f":"('Solar Azimuth'!F5-('Input Data'!$F$9+180))","v":-54.297393678678645},{"$f":"('Solar Azimuth'!G5-('Input Data'!$F$9+180))","v":-47.525622160719848},{"$f":"('Solar Azimuth'!H5-('Input Data'!$F$9+180))","v":-44.167395096334843},{"$f":"('Solar Azimuth'!I5-('Input Data'!$F$9+180))","v":-45.564022637846193},{"$f":"('Solar Azimuth'!J5-('Input Data'!$F$9+180))","v":-53.43141295755791},{"$f":"('Solar Azimuth'!K5-('Input Data'!$F$9+180))","v":-67.386703466760608},{"$f":"('Solar Azimuth'!L5-('Input Data'!$F$9+180))","v":-81.228878356629579},{"$f":"('Solar Azimuth'!M5-('Input Data'!$F$9+180))","v":-93.31393400326084},{"$f":"('Solar Azimuth'!N5-('Input Data'!$F$9+180))","v":-97.560948923869162},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,3.3107184365149103E-2,0.47327837320601324,0.94990214631444447,1.4372837495113098,1.8310176603216346,2.0589881377268808,1.9610063872387353,1.4836304688624924,0.83306425953815133,0.3085842354986158,0.11580728681013672,0.26546969290840439,null,3,120.81969749776529,8.4516855754548423,4.2109600610123152,2.7830273607142897,2.1845775093711346,1.9427018187758924,2.0397689808814654,2.6960891434555263,4.8015503656555705,12.962424971375233,34.540140868319632,15.0676333564756,null,3,0.99172320390871271,0.88168040669849668,0.76252446342138891,0.64067906262217256,0.54224558491959129,0.48525296556827979,0.50974840319031611,0.62909238278437685,0.7917339351154622,0.92285394112534602,0.97104817829746581,0.9336325767728989,null,3,0,0,0,0.30424315982142758,0.45385562265721635,0.51432454530602689,0.49005775477963365,0.32597771413611842,0,0,0,0,null,{"$f":"'Profile angles'!P7","v":3},{"$f":"IF('Profile angles'!Q7<0,1000,IF(EB6<0,1000,'Profile angles'!Q7))","v":1000},{"$f":"IF('Profile angles'!R7<0,1000,IF(EC6<0,1000,'Profile angles'!R7))","v":1000},{"$f":"IF('Profile angles'!S7<0,1000,IF(ED6<0,1000,'Profile angles'!S7))","v":1000},{"$f":"IF('Profile angles'!T7<0,1000,IF(EE6<0,1000,'Profile angles'!T7))","v":1000},{"$f":"IF('Profile angles'!U7<0,1000,IF(EF6<0,1000,'Profile angles'!U7))","v":1000},{"$f":"IF('Profile angles'!V7<0,1000,IF(EG6<0,1000,'Profile angles'!V7))","v":1000},{"$f":"IF('Profile angles'!W7<0,1000,IF(EH6<0,1000,'Profile angles'!W7))","v":1000},{"$f":"IF('Profile angles'!X7<0,1000,IF(EI6<0,1000,'Profile angles'!X7))","v":1000},{"$f":"IF('Profile angles'!Y7<0,1000,IF(EJ6<0,1000,'Profile angles'!Y7))","v":1000},{"$f":"IF('Profile angles'!Z7<0,1000,IF(EK6<0,1000,'Profile angles'!Z7))","v":1000},{"$f":"IF('Profile angles'!AA7<0,1000,IF(EL6<0,1000,'Profile angles'!AA7))","v":1000},{"$f":"IF('Profile angles'!AB7<0,1000,IF(EM6<0,1000,'Profile angles'!AB7))","v":1000},null,{"$f":"'Profile angles'!P36","v":3},{"$f":"IF('Profile angles'!Q36<0,1000,IF(EB6<0,1000,'Profile angles'!Q36))","v":1000},{"$f":"IF('Profile angles'!R36<0,1000,IF(EC6<0,1000,'Profile angles'!R36))","v":1000},{"$f":"IF('Profile angles'!S36<0,1000,IF(ED6<0,1000,'Profile angles'!S36))","v":1000},{"$f":"IF('Profile angles'!T36<0,1000,IF(EE6<0,1000,'Profile angles'!T36))","v":1000},{"$f":"IF('Profile angles'!U36<0,1000,IF(EF6<0,1000,'Profile angles'!U36))","v":1000},{"$f":"IF('Profile angles'!V36<0,1000,IF(EG6<0,1000,'Profile angles'!V36))","v":1000},{"$f":"IF('Profile angles'!W36<0,1000,IF(EH6<0,1000,'Profile angles'!W36))","v":1000},{"$f":"IF('Profile angles'!X36<0,1000,IF(EI6<0,1000,'Profile angles'!X36))","v":1000},{"$f":"IF('Profile angles'!Y36<0,1000,IF(EJ6<0,1000,'Profile angles'!Y36))","v":1000},{"$f":"IF('Profile angles'!Z36<0,1000,IF(EK6<0,1000,'Profile angles'!Z36))","v":1000},{"$f":"IF('Profile angles'!AA36<0,1000,IF(EL6<0,1000,'Profile angles'!AA36))","v":1000},{"$f":"IF('Profile angles'!AB36<0,1000,IF(EM6<0,1000,'Profile angles'!AB36))","v":1000},null,3,{"$f":"EB6","v":-52.431373562484438},-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552,null,3,{"$f":"EP6","v":-52.431373562484438},-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552]
[null,4,{"$f":"('Solar Azimuth'!C6-('Input Data'!$F$9-90))","v":173.64507796568091},{"$f":"('Solar Azimuth'!D6-('Input Data'!$F$9-90))","v":184.98310513599105},{"$f":"('Solar Azimuth'!E6-('Input Data'!$F$9-90))","v":195.54889999051608},{"$f":"('Solar Azimuth'!F6-('Input Data'!$F$9-90))","v":205.67424185262342},{"$f":"('Solar Azimuth'!G6-('Input Data'!$F$9-90))","v":212.72328942010085},{"$f":"('Solar Azimuth'!H6-('Input Data'!$F$9-90))","v":216.04880339758887},{"$f":"('Solar Azimuth'!I6-('Input Data'!$F$9-90))","v":214.27040515449994},{"$f":"('Solar Azimuth'!J6-('Input Data'!$F$9-90))","v":206.36534992403648},{"$f":"('Solar Azimuth'!K6-('Input Data'!$F$9-90))","v":193.51551123372408},{"$f":"('Solar Azimuth'!L6-('Input Data'!$F$9-90))","v":181.56142164454963},{"$f":"('Solar Azimuth'!M6-('Input Data'!$F$9-90))","v":171.56313955154286},{"$f":"('Solar Azimuth'!N6-('Input Data'!$F$9-90))","v":168.32021010545679},null,4,{"$f":"('Solar Azimuth'!C6-('Input Data'!$F$9+180))","v":-96.354922034319102},{"$f":"('Solar Azimuth'!D6-('Input Data'!$F$9+180))","v":-85.016894864008947},{"$f":"('Solar Azimuth'!E6-('Input Data'!$F$9+180))","v":-74.451100009483923},{"$f":"('Solar Azimuth'!F6-('Input Data'!$F$9+180))","v":-64.325758147376561},{"$f":"('Solar Azimuth'!G6-('Input Data'!$F$9+180))","v":-57.276710579899131},{"$f":"('Solar Azimuth'!H6-('Input Data'!$F$9+180))","v":-53.95119660241113},{"$f":"('Solar Azimuth'!I6-('Input Data'!$F$9+180))","v":-55.729594845500046},{"$f":"('Solar Azimuth'!J6-('Input Data'!$F$9+180))","v":-63.634650075963506},{"$f":"('Solar Azimuth'!K6-('Input Data'!$F$9+180))","v":-76.484488766275916},{"$f":"('Solar Azimuth'!L6-('Input Data'!$F$9+180))","v":-88.438578355450389},{"$f":"('Solar Azimuth'!M6-('Input Data'!$F$9+180))","v":-98.436860448457139},{"$f":"('Solar Azimuth'!N6-('Input Data'!$F$9+180))","v":-101.67978989454319},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,0.22274276911995697,0.17438308631516505,0.55648773366940307,0.96142785397686092,1.2851254926099842,1.4556894763908446,1.3627942614626511,0.99130151285771884,0.48073020725317461,5.451739420776306E-2,0.29664915933423452,0.41344442199227066,null,4,17.957934238690502,22.938004393216961,7.1879392086947735,4.1604785876073356,3.1125364977986156,2.7478387835277727,2.9351459080161577,4.0350992590224362,8.3206753801793294,73.371078315963331,13.483941801747012,9.6748191225440809,null,4,0.94431430772001079,0.95640422842120876,0.8608780665826492,0.7596430365057848,0.67871862684750395,0.63607763090228886,0.65930143463433721,0.75217462178557026,0.87981744818670637,0.98637065144805924,0.92583771016644134,0.89663889450193235,null,4,0,0,0,0,0.22186587555034609,0.31304030411805683,0.26621352299596057,0,0,0,0,0,null,{"$f":"'Profile angles'!P8","v":4},{"$f":"IF('Profile angles'!Q8<0,1000,IF(EB7<0,1000,'Profile angles'!Q8))","v":1000},{"$f":"IF('Profile angles'!R8<0,1000,IF(EC7<0,1000,'Profile angles'!R8))","v":1000},{"$f":"IF('Profile angles'!S8<0,1000,IF(ED7<0,1000,'Profile angles'!S8))","v":1000},{"$f":"IF('Profile angles'!T8<0,1000,IF(EE7<0,1000,'Profile angles'!T8))","v":1000},{"$f":"IF('Profile angles'!U8<0,1000,IF(EF7<0,1000,'Profile angles'!U8))","v":1000},{"$f":"IF('Profile angles'!V8<0,1000,IF(EG7<0,1000,'Profile angles'!V8))","v":1000},{"$f":"IF('Profile angles'!W8<0,1000,IF(EH7<0,1000,'Profile angles'!W8))","v":1000},{"$f":"IF('Profile angles'!X8<0,1000,IF(EI7<0,1000,'Profile angles'!X8))","v":1000},{"$f":"IF('Profile angles'!Y8<0,1000,IF(EJ7<0,1000,'Profile angles'!Y8))","v":1000},{"$f":"IF('Profile angles'!Z8<0,1000,IF(EK7<0,1000,'Profile angles'!Z8))","v":1000},{"$f":"IF('Profile angles'!AA8<0,1000,IF(EL7<0,1000,'Profile angles'!AA8))","v":1000},{"$f":"IF('Profile angles'!AB8<0,1000,IF(EM7<0,1000,'Profile angles'!AB8))","v":1000},null,{"$f":"'Profile angles'!P37","v":4},{"$f":"IF('Profile angles'!Q37<0,1000,IF(EB7<0,1000,'Profile angles'!Q37))","v":1000},{"$f":"IF('Profile angles'!R37<0,1000,IF(EC7<0,1000,'Profile angles'!R37))","v":1000},{"$f":"IF('Profile angles'!S37<0,1000,IF(ED7<0,1000,'Profile angles'!S37))","v":1000},{"$f":"IF('Profile angles'!T37<0,1000,IF(EE7<0,1000,'Profile angles'!T37))","v":1000},{"$f":"IF('Profile angles'!U37<0,1000,IF(EF7<0,1000,'Profile angles'!U37))","v":1000},{"$f":"IF('Profile angles'!V37<0,1000,IF(EG7<0,1000,'Profile angles'!V37))","v":1000},{"$f":"IF('Profile angles'!W37<0,1000,IF(EH7<0,1000,'Profile angles'!W37))","v":1000},{"$f":"IF('Profile angles'!X37<0,1000,IF(EI7<0,1000,'Profile angles'!X37))","v":1000},{"$f":"IF('Profile angles'!Y37<0,1000,IF(EJ7<0,1000,'Profile angles'!Y37))","v":1000},{"$f":"IF('Profile angles'!Z37<0,1000,IF(EK7<0,1000,'Profile angles'!Z37))","v":1000},{"$f":"IF('Profile angles'!AA37<0,1000,IF(EL7<0,1000,'Profile angles'!AA37))","v":1000},{"$f":"IF('Profile angles'!AB37<0,1000,IF(EM7<0,1000,'Profile angles'!AB37))","v":1000},null,4,{"$f":"EB7","v":-38.837571781392398},-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833,null,4,{"$f":"EP7","v":-38.837571781392398},-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833]
[null,5,{"$f":"('Solar Azimuth'!C7-('Input Data'!$F$9-90))","v":168.66757294181451},{"$f":"('Solar Azimuth'!D7-('Input Data'!$F$9-90))","v":178.4530883848376},{"$f":"('Solar Azimuth'!E7-('Input Data'!$F$9-90))","v":188.0315040139551},{"$f":"('Solar Azimuth'!F7-('Input Data'!$F$9-90))","v":197.92784498628035},{"$f":"('Solar Azimuth'!G7-('Input Data'!$F$9-90))","v":205.12801284478837},{"$f":"('Solar Azimuth'!H7-('Input Data'!$F$9-90))","v":208.42261537221856},{"$f":"('Solar Azimuth'!I7-('Input Data'!$F$9-90))","v":206.3954983583661},{"$f":"('Solar Azimuth'!J7-('Input Data'!$F$9-90))","v":198.51604214772064},{"$f":"('Solar Azimuth'!K7-('Input Data'!$F$9-90))","v":186.34810400515099},{"$f":"('Solar Azimuth'!L7-('Input Data'!$F$9-90))","v":175.4162605326689},{"$f":"('Solar Azimuth'!M7-('Input Data'!$F$9-90))","v":166.56119114284479},{"$f":"('Solar Azimuth'!N7-('Input Data'!$F$9-90))","v":163.93814433461824},null,5,{"$f":"('Solar Azimuth'!C7-('Input Data'!$F$9+180))","v":-101.33242705818549},{"$f":"('Solar Azimuth'!D7-('Input Data'!$F$9+180))","v":-91.546911615162415},{"$f":"('Solar Azimuth'!E7-('Input Data'!$F$9+180))","v":-81.9684959860449},{"$f":"('Solar Azimuth'!F7-('Input Data'!$F$9+180))","v":-72.072155013719652},{"$f":"('Solar Azimuth'!G7-('Input Data'!$F$9+180))","v":-64.871987155211627},{"$f":"('Solar Azimuth'!H7-('Input Data'!$F$9+180))","v":-61.577384627781441},{"$f":"('Solar Azimuth'!I7-('Input Data'!$F$9+180))","v":-63.604501641633902},{"$f":"('Solar Azimuth'!J7-('Input Data'!$F$9+180))","v":-71.48395785227936},{"$f":"('Solar Azimuth'!K7-('Input Data'!$F$9+180))","v":-83.651895994849014},{"$f":"('Solar Azimuth'!L7-('Input Data'!$F$9+180))","v":-94.583739467331085},{"$f":"('Solar Azimuth'!M7-('Input Data'!$F$9+180))","v":-103.43880885715521},{"$f":"('Solar Azimuth'!N7-('Input Data'!$F$9+180))","v":-106.06185566538174},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,0.40081668164825435,5.4010525776474264E-2,0.28220317465047429,0.64705594015601875,0.93806113171755112,1.0824164011067139,0.99261277142613502,0.66981336558795479,0.22250182621673753,0.16034491823298763,0.47789900969886034,0.57582819931547902,null,5,9.9796245594146544,74.059638237077564,14.174184981987658,6.1818457288801234,4.2641144214942193,3.6954355051440539,4.0297688233982765,5.9718127548691822,17.977380536659588,24.946222456441237,8.3699692169701994,6.9465163476798102,null,5,0.89979582958793647,0.98649736855588144,0.92944920633738137,0.83823601496099531,0.76548471707061227,0.72939589972332153,0.7518468071434663,0.83254665860301125,0.94437454344581562,0.95991377044175308,0.88052524757528494,0.85604295017113019,null,5,0,0,0,0,0,7.6141123713986514E-2,0,0,0,0,0,0,null,{"$f":"'Profile angles'!P9","v":5},{"$f":"IF('Profile angles'!Q9<0,1000,IF(EB8<0,1000,'Profile angles'!Q9))","v":1000},{"$f":"IF('Profile angles'!R9<0,1000,IF(EC8<0,1000,'Profile angles'!R9))","v":1000},{"$f":"IF('Profile angles'!S9<0,1000,IF(ED8<0,1000,'Profile angles'!S9))","v":1000},{"$f":"IF('Profile angles'!T9<0,1000,IF(EE8<0,1000,'Profile angles'!T9))","v":1000},{"$f":"IF('Profile angles'!U9<0,1000,IF(EF8<0,1000,'Profile angles'!U9))","v":1000},{"$f":"IF('Profile angles'!V9<0,1000,IF(EG8<0,1000,'Profile angles'!V9))","v":1000},{"$f":"IF('Profile angles'!W9<0,1000,IF(EH8<0,1000,'Profile angles'!W9))","v":1000},{"$f":"IF('Profile angles'!X9<0,1000,IF(EI8<0,1000,'Profile angles'!X9))","v":1000},{"$f":"IF('Profile angles'!Y9<0,1000,IF(EJ8<0,1000,'Profile angles'!Y9))","v":1000},{"$f":"IF('Profile angles'!Z9<0,1000,IF(EK8<0,1000,'Profile angles'!Z9))","v":1000},{"$f":"IF('Profile angles'!AA9<0,1000,IF(EL8<0,1000,'Profile angles'!AA9))","v":1000},{"$f":"IF('Profile angles'!AB9<0,1000,IF(EM8<0,1000,'Profile angles'!AB9))","v":1000},null,{"$f":"'Profile angles'!P38","v":5},{"$f":"IF('Profile angles'!Q38<0,1000,IF(EB8<0,1000,'Profile angles'!Q38))","v":1000},{"$f":"IF('Profile angles'!R38<0,1000,IF(EC8<0,1000,'Profile angles'!R38))","v":1000},{"$f":"IF('Profile angles'!S38<0,1000,IF(ED8<0,1000,'Profile angles'!S38))","v":1000},{"$f":"IF('Profile angles'!T38<0,1000,IF(EE8<0,1000,'Profile angles'!T38))","v":1000},{"$f":"IF('Profile angles'!U38<0,1000,IF(EF8<0,1000,'Profile angles'!U38))","v":1000},{"$f":"IF('Profile angles'!V38<0,1000,IF(EG8<0,1000,'Profile angles'!V38))","v":1000},{"$f":"IF('Profile angles'!W38<0,1000,IF(EH8<0,1000,'Profile angles'!W38))","v":1000},{"$f":"IF('Profile angles'!X38<0,1000,IF(EI8<0,1000,'Profile angles'!X38))","v":1000},{"$f":"IF('Profile angles'!Y38<0,1000,IF(EJ8<0,1000,'Profile angles'!Y38))","v":1000},{"$f":"IF('Profile angles'!Z38<0,1000,IF(EK8<0,1000,'Profile angles'!Z38))","v":1000},{"$f":"IF('Profile angles'!AA38<0,1000,IF(EL8<0,1000,'Profile angles'!AA38))","v":1000},{"$f":"IF('Profile angles'!AB38<0,1000,IF(EM8<0,1000,'Profile angles'!AB38))","v":1000},null,5,{"$f":"EB8","v":-25.376333918471747},-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006,null,5,{"$f":"EP8","v":-25.376333918471747},-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006]
[null,6,{"$f":"('Solar Azimuth'!C8-('Input Data'!$F$9-90))","v":163.48849207792694},{"$f":"('Solar Azimuth'!D8-('Input Data'!$F$9-90))","v":172.46447355726104},{"$f":"('Solar Azimuth'!E8-('Input Data'!$F$9-90))","v":181.53041377533867},{"$f":"('Solar Azimuth'!F8-('Input Data'!$F$9-90))","v":191.44881339595753},{"$f":"('Solar Azimuth'!G8-('Input Data'!$F$9-90))","v":198.93731604152856},{"$f":"('Solar Azimuth'!H8-('Input Data'!$F$9-90))","v":202.29007277032855},{"$f":"('Solar Azimuth'!I8-('Input Data'!$F$9-90))","v":200.03139679027041},{"$f":"('Solar Azimuth'!J8-('Input Data'!$F$9-90))","v":191.98746755551196},{"$f":"('Solar Azimuth'!K8-('Input Data'!$F$9-90))","v":179.96169549125975},{"$f":"('Solar Azimuth'!L8-('Input Data'!$F$9-90))","v":169.41603858660801},{"$f":"('Solar Azimuth'!M8-('Input Data'!$F$9-90))","v":161.1617317939496},{"$f":"('Solar Azimuth'!N8-('Input Data'!$F$9-90))","v":158.98760322071186},null,6,{"$f":"('Solar Azimuth'!C8-('Input Data'!$F$9+180))","v":-106.51150792207306},{"$f":"('Solar Azimuth'!D8-('Input Data'!$F$9+180))","v":-97.535526442738941},{"$f":"('Solar Azimuth'!E8-('Input Data'!$F$9+180))","v":-88.469586224661313},{"$f":"('Solar Azimuth'!F8-('Input Data'!$F$9+180))","v":-78.551186604042456},{"$f":"('Solar Azimuth'!G8-('Input Data'!$F$9+180))","v":-71.062683958471453},{"$f":"('Solar Azimuth'!H8-('Input Data'!$F$9+180))","v":-67.709927229671436},{"$f":"('Solar Azimuth'!I8-('Input Data'!$F$9+180))","v":-69.968603209729594},{"$f":"('Solar Azimuth'!J8-('Input Data'!$F$9+180))","v":-78.012532444488031},{"$f":"('Solar Azimuth'!K8-('Input Data'!$F$9+180))","v":-90.038304508740254},{"$f":"('Solar Azimuth'!L8-('Input Data'!$F$9+180))","v":-100.583961413392},{"$f":"('Solar Azimuth'!M8-('Input Data'!$F$9+180))","v":-108.8382682060504},{"$f":"('Solar Azimuth'!N8-('Input Data'!$F$9+180))","v":-111.01239677928814},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,0.59286396452255263,0.26456669912835817,5.3434227010461702E-2,0.40504422831013309,0.68620864192038356,0.81985499411158902,0.72918185684802328,0.42465591496132887,1.3370797909530528E-3,0.37371039665329514,0.68234649745779807,0.76822460389178149,null,6,6.7469103189992206,15.119060763045388,74.858386165423227,9.8754647527955779,5.8291309022367166,4.878911549882643,5.4856000083305423,9.4193907563121115,2991.5940896449133,10.703475300182625,5.8621243237896099,5.2068105860398548,null,6,0.85178400886936179,0.93385832521791046,0.98664144324738456,0.8987389429224667,0.82844783951990408,0.79503625147210277,0.81770453578799418,0.89383602125966777,0.99966573005226178,0.90657240083667623,0.82941337563555051,0.80794384902705463,null,6,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$f":"'Profile angles'!P10","v":6},{"$f":"IF('Profile angles'!Q10<0,1000,IF(EB9<0,1000,'Profile angles'!Q10))","v":1000},{"$f":"IF('Profile angles'!R10<0,1000,IF(EC9<0,1000,'Profile angles'!R10))","v":1000},{"$f":"IF('Profile angles'!S10<0,1000,IF(ED9<0,1000,'Profile angles'!S10))","v":1000},{"$f":"IF('Profile angles'!T10<0,1000,IF(EE9<0,1000,'Profile angles'!T10))","v":1000},{"$f":"IF('Profile angles'!U10<0,1000,IF(EF9<0,1000,'Profile angles'!U10))","v":1000},{"$f":"IF('Profile angles'!V10<0,1000,IF(EG9<0,1000,'Profile angles'!V10))","v":1000},{"$f":"IF('Profile angles'!W10<0,1000,IF(EH9<0,1000,'Profile angles'!W10))","v":1000},{"$f":"IF('Profile angles'!X10<0,1000,IF(EI9<0,1000,'Profile angles'!X10))","v":1000},{"$f":"IF('Profile angles'!Y10<0,1000,IF(EJ9<0,1000,'Profile angles'!Y10))","v":1000},{"$f":"IF('Profile angles'!Z10<0,1000,IF(EK9<0,1000,'Profile angles'!Z10))","v":1000},{"$f":"IF('Profile angles'!AA10<0,1000,IF(EL9<0,1000,'Profile angles'!AA10))","v":1000},{"$f":"IF('Profile angles'!AB10<0,1000,IF(EM9<0,1000,'Profile angles'!AB10))","v":1000},null,{"$f":"'Profile angles'!P39","v":6},{"$f":"IF('Profile angles'!Q39<0,1000,IF(EB9<0,1000,'Profile angles'!Q39))","v":1000},{"$f":"IF('Profile angles'!R39<0,1000,IF(EC9<0,1000,'Profile angles'!R39))","v":1000},{"$f":"IF('Profile angles'!S39<0,1000,IF(ED9<0,1000,'Profile angles'!S39))","v":1000},{"$f":"IF('Profile angles'!T39<0,1000,IF(EE9<0,1000,'Profile angles'!T39))","v":17.58014754628174},{"$f":"IF('Profile angles'!U39<0,1000,IF(EF9<0,1000,'Profile angles'!U39))","v":22.111172344820307},{"$f":"IF('Profile angles'!V39<0,1000,IF(EG9<0,1000,'Profile angles'!V39))","v":19.79509046495318},{"$f":"IF('Profile angles'!W39<0,1000,IF(EH9<0,1000,'Profile angles'!W39))","v":15.860431327653469},{"$f":"IF('Profile angles'!X39<0,1000,IF(EI9<0,1000,'Profile angles'!X39))","v":13.722280285934318},{"$f":"IF('Profile angles'!Y39<0,1000,IF(EJ9<0,1000,'Profile angles'!Y39))","v":1000},{"$f":"IF('Profile angles'!Z39<0,1000,IF(EK9<0,1000,'Profile angles'!Z39))","v":1000},{"$f":"IF('Profile angles'!AA39<0,1000,IF(EL9<0,1000,'Profile angles'!AA39))","v":1000},{"$f":"IF('Profile angles'!AB39<0,1000,IF(EM9<0,1000,'Profile angles'!AB39))","v":1000},null,6,{"$f":"EB9","v":-12.151444093159176},-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719,null,6,{"$f":"EP9","v":-12.151444093159176},-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719]
[null,7,{"$f":"('Solar Azimuth'!C9-('Input Data'!$F$9-90))","v":157.64728852701973},{"$f":"('Solar Azimuth'!D9-('Input Data'!$F$9-90))","v":166.27422918451123},{"$f":"('Solar Azimuth'!E9-('Input Data'!$F$9-90))","v":175.20900110512855},{"$f":"('Solar Azimuth'!F9-('Input Data'!$F$9-90))","v":185.51931316773377},{"$f":"('Solar Azimuth'!G9-('Input Data'!$F$9-90))","v":193.59914856777166},{"$f":"('Solar Azimuth'!H9-('Input Data'!$F$9-90))","v":197.16015360598314},{"$f":"('Solar Azimuth'!I9-('Input Data'!$F$9-90))","v":194.6042787468042},{"$f":"('Solar Azimuth'!J9-('Input Data'!$F$9-90))","v":186.05385450332705},{"$f":"('Solar Azimuth'!K9-('Input Data'!$F$9-90))","v":173.57080331864259},{"$f":"('Solar Azimuth'!L9-('Input Data'!$F$9-90))","v":162.88856325053356},{"$f":"('Solar Azimuth'!M9-('Input Data'!$F$9-90))","v":154.90167163715074},{"$f":"('Solar Azimuth'!N9-('Input Data'!$F$9-90))","v":153.12835913879397},null,7,{"$f":"('Solar Azimuth'!C9-('Input Data'!$F$9+180))","v":-112.35271147298027},{"$f":"('Solar Azimuth'!D9-('Input Data'!$F$9+180))","v":-103.72577081548877},{"$f":"('Solar Azimuth'!E9-('Input Data'!$F$9+180))","v":-94.790998894871436},{"$f":"('Solar Azimuth'!F9-('Input Data'!$F$9+180))","v":-84.48068683226623},{"$f":"('Solar Azimuth'!G9-('Input Data'!$F$9+180))","v":-76.400851432228336},{"$f":"('Solar Azimuth'!H9-('Input Data'!$F$9+180))","v":-72.83984639401686},{"$f":"('Solar Azimuth'!I9-('Input Data'!$F$9+180))","v":-75.395721253195802},{"$f":"('Solar Azimuth'!J9-('Input Data'!$F$9+180))","v":-83.946145496672969},{"$f":"('Solar Azimuth'!K9-('Input Data'!$F$9+180))","v":-96.429196681357411},{"$f":"('Solar Azimuth'!L9-('Input Data'!$F$9+180))","v":-107.11143674946644},{"$f":"('Solar Azimuth'!M9-('Input Data'!$F$9+180))","v":-115.09832836284926},{"$f":"('Solar Azimuth'!N9-('Input Data'!$F$9+180))","v":-116.87164086120603},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,0.8224100646018857,0.48850057932834295,0.16762828314829864,0.19325852573601396,0.48381946196206432,0.61757956593623309,0.52112047202192668,0.21210930248889034,0.22536798234507732,0.61571736699697843,0.93679730506789816,1.0134135144801193,null,7,4.8637537065360847,8.1883219166285279,23.862321589616478,20.69766384052771,8.2675467079776759,6.4768982340536319,7.6757683007158679,18.858201658597768,17.748750103620829,6.4964872105347435,4.2698671082428943,3.9470561057713907,null,7,0.79439748384952857,0.8778748551679143,0.95809292921292533,0.9516853685659965,0.87904513450948396,0.84560510851594173,0.86971988199451833,0.94697267437777743,0.94365800441373071,0.84607065825075534,0.76580067373302541,0.74664662137997018,null,7,0,0,0,0,0,0,0,0,0,0,0,1.3235973557152336E-2,null,{"$f":"'Profile angles'!P11","v":7},{"$f":"IF('Profile angles'!Q11<0,1000,IF(EB10<0,1000,'Profile angles'!Q11))","v":1000},{"$f":"IF('Profile angles'!R11<0,1000,IF(EC10<0,1000,'Profile angles'!R11))","v":1000},{"$f":"IF('Profile angles'!S11<0,1000,IF(ED10<0,1000,'Profile angles'!S11))","v":1000},{"$f":"IF('Profile angles'!T11<0,1000,IF(EE10<0,1000,'Profile angles'!T11))","v":1000},{"$f":"IF('Profile angles'!U11<0,1000,IF(EF10<0,1000,'Profile angles'!U11))","v":1000},{"$f":"IF('Profile angles'!V11<0,1000,IF(EG10<0,1000,'Profile angles'!V11))","v":1000},{"$f":"IF('Profile angles'!W11<0,1000,IF(EH10<0,1000,'Profile angles'!W11))","v":1000},{"$f":"IF('Profile angles'!X11<0,1000,IF(EI10<0,1000,'Profile angles'!X11))","v":1000},{"$f":"IF('Profile angles'!Y11<0,1000,IF(EJ10<0,1000,'Profile angles'!Y11))","v":1000},{"$f":"IF('Profile angles'!Z11<0,1000,IF(EK10<0,1000,'Profile angles'!Z11))","v":1000},{"$f":"IF('Profile angles'!AA11<0,1000,IF(EL10<0,1000,'Profile angles'!AA11))","v":1000},{"$f":"IF('Profile angles'!AB11<0,1000,IF(EM10<0,1000,'Profile angles'!AB11))","v":1000},null,{"$f":"'Profile angles'!P40","v":7},{"$f":"IF('Profile angles'!Q40<0,1000,IF(EB10<0,1000,'Profile angles'!Q40))","v":1000},{"$f":"IF('Profile angles'!R40<0,1000,IF(EC10<0,1000,'Profile angles'!R40))","v":1000},{"$f":"IF('Profile angles'!S40<0,1000,IF(ED10<0,1000,'Profile angles'!S40))","v":1000},{"$f":"IF('Profile angles'!T40<0,1000,IF(EE10<0,1000,'Profile angles'!T40))","v":72.609902347589809},{"$f":"IF('Profile angles'!U40<0,1000,IF(EF10<0,1000,'Profile angles'!U40))","v":57.96115831293033},{"$f":"IF('Profile angles'!V40<0,1000,IF(EG10<0,1000,'Profile angles'!V40))","v":51.874170400534645},{"$f":"IF('Profile angles'!W40<0,1000,IF(EH10<0,1000,'Profile angles'!W40))","v":53.106981432720829},{"$f":"IF('Profile angles'!X40<0,1000,IF(EI10<0,1000,'Profile angles'!X40))","v":70.235558391915376},{"$f":"IF('Profile angles'!Y40<0,1000,IF(EJ10<0,1000,'Profile angles'!Y40))","v":1000},{"$f":"IF('Profile angles'!Z40<0,1000,IF(EK10<0,1000,'Profile angles'!Z40))","v":1000},{"$f":"IF('Profile angles'!AA40<0,1000,IF(EL10<0,1000,'Profile angles'!AA40))","v":1000},{"$f":"IF('Profile angles'!AB40<0,1000,IF(EM10<0,1000,'Profile angles'!AB40))","v":1000},null,7,{"$f":"EB10","v":0.70023973357815916},4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048,null,7,{"$f":"EP10","v":0.70023973357815916},4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048]
[null,8,{"$f":"('Solar Azimuth'!C10-('Input Data'!$F$9-90))","v":150.63419301030098},{"$f":"('Solar Azimuth'!D10-('Input Data'!$F$9-90))","v":159.20456224053299},{"$f":"('Solar Azimuth'!E10-('Input Data'!$F$9-90))","v":168.31038553405347},{"$f":"('Solar Azimuth'!F10-('Input Data'!$F$9-90))","v":179.48612226491466},{"$f":"('Solar Azimuth'!G10-('Input Data'!$F$9-90))","v":188.66375435887818},{"$f":"('Solar Azimuth'!H10-('Input Data'!$F$9-90))","v":192.67188093597633},{"$f":"('Solar Azimuth'!I10-('Input Data'!$F$9-90))","v":189.66183746967349},{"$f":"('Solar Azimuth'!J10-('Input Data'!$F$9-90))","v":180.06876291098138},{"$f":"('Solar Azimuth'!K10-('Input Data'!$F$9-90))","v":166.38796165804348},{"$f":"('Solar Azimuth'!L10-('Input Data'!$F$9-90))","v":155.09176506312605},{"$f":"('Solar Azimuth'!M10-('Input Data'!$F$9-90))","v":147.21243824503364},{"$f":"('Solar Azimuth'!N10-('Input Data'!$F$9-90))","v":145.90538614326354},null,8,{"$f":"('Solar Azimuth'!C10-('Input Data'!$F$9+180))","v":-119.36580698969902},{"$f":"('Solar Azimuth'!D10-('Input Data'!$F$9+180))","v":-110.79543775946702},{"$f":"('Solar Azimuth'!E10-('Input Data'!$F$9+180))","v":-101.68961446594653},{"$f":"('Solar Azimuth'!F10-('Input Data'!$F$9+180))","v":-90.513877735085345},{"$f":"('Solar Azimuth'!G10-('Input Data'!$F$9+180))","v":-81.336245641121835},{"$f":"('Solar Azimuth'!H10-('Input Data'!$F$9+180))","v":-77.328119064023667},{"$f":"('Solar Azimuth'!I10-('Input Data'!$F$9+180))","v":-80.338162530326514},{"$f":"('Solar Azimuth'!J10-('Input Data'!$F$9+180))","v":-89.931237089018623},{"$f":"('Solar Azimuth'!K10-('Input Data'!$F$9+180))","v":-103.61203834195651},{"$f":"('Solar Azimuth'!L10-('Input Data'!$F$9+180))","v":-114.90823493687394},{"$f":"('Solar Azimuth'!M10-('Input Data'!$F$9+180))","v":-122.78756175496636},{"$f":"('Solar Azimuth'!N10-('Input Data'!$F$9+180))","v":-124.09461385673646},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,1.1253700951895849,0.75954650464484164,0.41380203222754963,1.7938197847839586E-2,0.30474829390384939,0.44968818996384896,0.34049537079163339,2.4002795521630071E-3,0.48429575640455536,0.92871850432905367,1.288297631320664,1.3538276207355049,null,8,3.5543862566617608,5.2663003193864597,9.6664580849627288,222.98784046926178,13.125586196922328,8.8950523702247128,11.747589961943451,1666.4725558298369,8.2594157539109343,4.3070101234709171,3.104872587477713,2.9545859005497976,null,8,0.71865747620260378,0.81011337383878956,0.89654949194311262,0.99551545053804014,0.92381292652403768,0.8875779525090377,0.9148761573020916,0.99939993011195927,0.87892606089886116,0.76782037391773661,0.67792559216983395,0.66154309481612383,null,8,0.11140343583455981,0,0,0,0,0,0,0,0,0,0.22378185313057175,0.26135352486255059,null,{"$f":"'Profile angles'!P12","v":8},{"$f":"IF('Profile angles'!Q12<0,1000,IF(EB11<0,1000,'Profile angles'!Q12))","v":1000},{"$f":"IF('Profile angles'!R12<0,1000,IF(EC11<0,1000,'Profile angles'!R12))","v":1000},{"$f":"IF('Profile angles'!S12<0,1000,IF(ED11<0,1000,'Profile angles'!S12))","v":1000},{"$f":"IF('Profile angles'!T12<0,1000,IF(EE11<0,1000,'Profile angles'!T12))","v":1000},{"$f":"IF('Profile angles'!U12<0,1000,IF(EF11<0,1000,'Profile angles'!U12))","v":1000},{"$f":"IF('Profile angles'!V12<0,1000,IF(EG11<0,1000,'Profile angles'!V12))","v":1000},{"$f":"IF('Profile angles'!W12<0,1000,IF(EH11<0,1000,'Profile angles'!W12))","v":1000},{"$f":"IF('Profile angles'!X12<0,1000,IF(EI11<0,1000,'Profile angles'!X12))","v":1000},{"$f":"IF('Profile angles'!Y12<0,1000,IF(EJ11<0,1000,'Profile angles'!Y12))","v":1000},{"$f":"IF('Profile angles'!Z12<0,1000,IF(EK11<0,1000,'Profile angles'!Z12))","v":1000},{"$f":"IF('Profile angles'!AA12<0,1000,IF(EL11<0,1000,'Profile angles'!AA12))","v":1000},{"$f":"IF('Profile angles'!AB12<0,1000,IF(EM11<0,1000,'Profile angles'!AB12))","v":1000},null,{"$f":"'Profile angles'!P41","v":8},{"$f":"IF('Profile angles'!Q41<0,1000,IF(EB11<0,1000,'Profile angles'!Q41))","v":1000},{"$f":"IF('Profile angles'!R41<0,1000,IF(EC11<0,1000,'Profile angles'!R41))","v":1000},{"$f":"IF('Profile angles'!S41<0,1000,IF(ED11<0,1000,'Profile angles'!S41))","v":1000},{"$f":"IF('Profile angles'!T41<0,1000,IF(EE11<0,1000,'Profile angles'!T41))","v":1000},{"$f":"IF('Profile angles'!U41<0,1000,IF(EF11<0,1000,'Profile angles'!U41))","v":77.392469719775818},{"$f":"IF('Profile angles'!V41<0,1000,IF(EG11<0,1000,'Profile angles'!V41))","v":71.837796305169562},{"$f":"IF('Profile angles'!W41<0,1000,IF(EH11<0,1000,'Profile angles'!W41))","v":74.90306712124648},{"$f":"IF('Profile angles'!X41<0,1000,IF(EI11<0,1000,'Profile angles'!X41))","v":89.880701812612699},{"$f":"IF('Profile angles'!Y41<0,1000,IF(EJ11<0,1000,'Profile angles'!Y41))","v":1000},{"$f":"IF('Profile angles'!Z41<0,1000,IF(EK11<0,1000,'Profile angles'!Z41))","v":1000},{"$f":"IF('Profile angles'!AA41<0,1000,IF(EL11<0,1000,'Profile angles'!AA41))","v":1000},{"$f":"IF('Profile angles'!AB41<0,1000,IF(EM11<0,1000,'Profile angles'!AB41))","v":1000},null,8,{"$f":"EB11","v":12.968359542715392},17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182,null,8,{"$f":"EP11","v":12.968359542715392},17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182]
[null,9,{"$f":"('Solar Azimuth'!C11-('Input Data'!$F$9-90))","v":141.7687483399765},{"$f":"('Solar Azimuth'!D11-('Input Data'!$F$9-90))","v":150.37968563970963},{"$f":"('Solar Azimuth'!E11-('Input Data'!$F$9-90))","v":159.81435360918206},{"$f":"('Solar Azimuth'!F11-('Input Data'!$F$9-90))","v":172.45083421497344},{"$f":"('Solar Azimuth'!G11-('Input Data'!$F$9-90))","v":183.6276889525692},{"$f":"('Solar Azimuth'!H11-('Input Data'!$F$9-90))","v":188.52118705141112},{"$f":"('Solar Azimuth'!I11-('Input Data'!$F$9-90))","v":184.73537370469174},{"$f":"('Solar Azimuth'!J11-('Input Data'!$F$9-90))","v":173.16809910599662},{"$f":"('Solar Azimuth'!K11-('Input Data'!$F$9-90))","v":157.25626203675068},{"$f":"('Solar Azimuth'!L11-('Input Data'!$F$9-90))","v":144.96275287832808},{"$f":"('Solar Azimuth'!M11-('Input Data'!$F$9-90))","v":137.31915705316155},{"$f":"('Solar Azimuth'!N11-('Input Data'!$F$9-90))","v":136.69540702919016},null,9,{"$f":"('Solar Azimuth'!C11-('Input Data'!$F$9+180))","v":-128.2312516600235},{"$f":"('Solar Azimuth'!D11-('Input Data'!$F$9+180))","v":-119.62031436029037},{"$f":"('Solar Azimuth'!E11-('Input Data'!$F$9+180))","v":-110.18564639081794},{"$f":"('Solar Azimuth'!F11-('Input Data'!$F$9+180))","v":-97.54916578502656},{"$f":"('Solar Azimuth'!G11-('Input Data'!$F$9+180))","v":-86.372311047430784},{"$f":"('Solar Azimuth'!H11-('Input Data'!$F$9+180))","v":-81.478812948588867},{"$f":"('Solar Azimuth'!I11-('Input Data'!$F$9+180))","v":-85.264626295308261},{"$f":"('Solar Azimuth'!J11-('Input Data'!$F$9+180))","v":-96.831900894003383},{"$f":"('Solar Azimuth'!K11-('Input Data'!$F$9+180))","v":-112.7437379632493},{"$f":"('Solar Azimuth'!L11-('Input Data'!$F$9+180))","v":-125.03724712167192},{"$f":"('Solar Azimuth'!M11-('Input Data'!$F$9+180))","v":-132.68084294683845},{"$f":"('Solar Azimuth'!N11-('Input Data'!$F$9+180))","v":-133.30459297080984},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,1.5756119842853733,1.1370962619254887,0.7352879116846337,0.26505114852340489,0.1267997166239998,0.29965813081931914,0.1656731162234025,0.23961502114185332,0.83841259239175514,1.402353589949795,1.8443091451870437,1.8850073781619507,null,9,2.5386961002421029,3.5177320812106525,5.440045914579934,15.09142677662004,31.545811824337239,13.348544853641299,24.143929269768634,16.693444262962078,4.7709207093241863,2.8523476737013262,2.1688337936394784,2.1220076092754372,null,9,0.60609700392865662,0.71572593451862776,0.8161780220788416,0.93373721286914879,0.96830007084400005,0.92508546729517027,0.9585817209441494,0.94009624471453668,0.79039685190206121,0.64941160251255126,0.53892271370323908,0.52874815545951237,null,9,0.36532597493947427,0.12056697969733687,0,0,0,0,0,0,0,0.28691308157466844,0.45779155159013041,0.4694980976811407,null,{"$f":"'Profile angles'!P13","v":9},{"$f":"IF('Profile angles'!Q13<0,1000,IF(EB12<0,1000,'Profile angles'!Q13))","v":1000},{"$f":"IF('Profile angles'!R13<0,1000,IF(EC12<0,1000,'Profile angles'!R13))","v":1000},{"$f":"IF('Profile angles'!S13<0,1000,IF(ED12<0,1000,'Profile angles'!S13))","v":1000},{"$f":"IF('Profile angles'!T13<0,1000,IF(EE12<0,1000,'Profile angles'!T13))","v":1000},{"$f":"IF('Profile angles'!U13<0,1000,IF(EF12<0,1000,'Profile angles'!U13))","v":1000},{"$f":"IF('Profile angles'!V13<0,1000,IF(EG12<0,1000,'Profile angles'!V13))","v":1000},{"$f":"IF('Profile angles'!W13<0,1000,IF(EH12<0,1000,'Profile angles'!W13))","v":1000},{"$f":"IF('Profile angles'!X13<0,1000,IF(EI12<0,1000,'Profile angles'!X13))","v":1000},{"$f":"IF('Profile angles'!Y13<0,1000,IF(EJ12<0,1000,'Profile angles'!Y13))","v":1000},{"$f":"IF('Profile angles'!Z13<0,1000,IF(EK12<0,1000,'Profile angles'!Z13))","v":1000},{"$f":"IF('Profile angles'!AA13<0,1000,IF(EL12<0,1000,'Profile angles'!AA13))","v":1000},{"$f":"IF('Profile angles'!AB13<0,1000,IF(EM12<0,1000,'Profile angles'!AB13))","v":1000},null,{"$f":"'Profile angles'!P42","v":9},{"$f":"IF('Profile angles'!Q42<0,1000,IF(EB12<0,1000,'Profile angles'!Q42))","v":1000},{"$f":"IF('Profile angles'!R42<0,1000,IF(EC12<0,1000,'Profile angles'!R42))","v":1000},{"$f":"IF('Profile angles'!S42<0,1000,IF(ED12<0,1000,'Profile angles'!S42))","v":1000},{"$f":"IF('Profile angles'!T42<0,1000,IF(EE12<0,1000,'Profile angles'!T42))","v":1000},{"$f":"IF('Profile angles'!U42<0,1000,IF(EF12<0,1000,'Profile angles'!U42))","v":86.682219236973438},{"$f":"IF('Profile angles'!V42<0,1000,IF(EG12<0,1000,'Profile angles'!V42))","v":82.177260396790942},{"$f":"IF('Profile angles'!W42<0,1000,IF(EH12<0,1000,'Profile angles'!W42))","v":85.346370921243249},{"$f":"IF('Profile angles'!X42<0,1000,IF(EI12<0,1000,'Profile angles'!X42))","v":1000},{"$f":"IF('Profile angles'!Y42<0,1000,IF(EJ12<0,1000,'Profile angles'!Y42))","v":1000},{"$f":"IF('Profile angles'!Z42<0,1000,IF(EK12<0,1000,'Profile angles'!Z42))","v":1000},{"$f":"IF('Profile angles'!AA42<0,1000,IF(EL12<0,1000,'Profile angles'!AA42))","v":1000},{"$f":"IF('Profile angles'!AB42<0,1000,IF(EM12<0,1000,'Profile angles'!AB42))","v":1000},null,9,{"$f":"EB12","v":24.306538235547787},29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159,null,9,{"$f":"EP12","v":24.306538235547787},29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159]
[null,10,{"$f":"('Solar Azimuth'!C12-('Input Data'!$F$9-90))","v":130.14803438133268},{"$f":"('Solar Azimuth'!D12-('Input Data'!$F$9-90))","v":138.47132829778951},{"$f":"('Solar Azimuth'!E12-('Input Data'!$F$9-90))","v":147.88953270557116},{"$f":"('Solar Azimuth'!F12-('Input Data'!$F$9-90))","v":162.49765405746044},{"$f":"('Solar Azimuth'!G12-('Input Data'!$F$9-90))","v":177.52098874947296},{"$f":"('Solar Azimuth'!H12-('Input Data'!$F$9-90))","v":184.32570869615293},{"$f":"('Solar Azimuth'!I12-('Input Data'!$F$9-90))","v":179.01523478336929},{"$f":"('Solar Azimuth'!J12-('Input Data'!$F$9-90))","v":163.55230552912707},{"$f":"('Solar Azimuth'!K12-('Input Data'!$F$9-90))","v":144.00352276914981},{"$f":"('Solar Azimuth'!L12-('Input Data'!$F$9-90))","v":130.89681624413825},{"$f":"('Solar Azimuth'!M12-('Input Data'!$F$9-90))","v":124.26382672583708},{"$f":"('Solar Azimuth'!N12-('Input Data'!$F$9-90))","v":124.74471079351217},null,10,{"$f":"('Solar Azimuth'!C12-('Input Data'!$F$9+180))","v":-139.85196561866732},{"$f":"('Solar Azimuth'!D12-('Input Data'!$F$9+180))","v":-131.52867170221049},{"$f":"('Solar Azimuth'!E12-('Input Data'!$F$9+180))","v":-122.11046729442884},{"$f":"('Solar Azimuth'!F12-('Input Data'!$F$9+180))","v":-107.50234594253956},{"$f":"('Solar Azimuth'!G12-('Input Data'!$F$9+180))","v":-92.479011250527037},{"$f":"('Solar Azimuth'!H12-('Input Data'!$F$9+180))","v":-85.67429130384707},{"$f":"('Solar Azimuth'!I12-('Input Data'!$F$9+180))","v":-90.98476521663072},{"$f":"('Solar Azimuth'!J12-('Input Data'!$F$9+180))","v":-106.44769447087293},{"$f":"('Solar Azimuth'!K12-('Input Data'!$F$9+180))","v":-125.99647723085019},{"$f":"('Solar Azimuth'!L12-('Input Data'!$F$9+180))","v":-139.10318375586175},{"$f":"('Solar Azimuth'!M12-('Input Data'!$F$9+180))","v":-145.73617327416292},{"$f":"('Solar Azimuth'!N12-('Input Data'!$F$9+180))","v":-145.25528920648782},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,2.3710390719936503,1.7712355401660569,1.2551068482009571,0.63068760860528961,8.6587855329832195E-2,0.15128326224742486,3.4378176024887269E-2,0.59044151808580925,1.4528971862599471,2.3091224115140667,2.9358702318713976,2.8835564299656866,null,10,1.6870240761729258,2.2583106025667221,3.1869796629135707,6.3422841124874045,46.19585488938538,26.440466318461311,116.35288611892474,6.7745913481285376,2.7531197925276558,1.7322598317242273,1.3624580393835388,1.3871759048764662,null,10,0.40724023200158743,0.55719111495848583,0.68622328794976073,0.84232809784867757,0.97835303616754199,0.96217918443814376,0.99140545599377816,0.85238962047854772,0.63677570343501322,0.42271939712148332,0.2660324420321506,0.27911089250857835,null,10,0.57824398095676854,0.43542234935831947,0.20325508427160732,0,0,0,0,0,0.31172005186808605,0.56693504206894318,0.65938549015411529,0.65320602378088344,null,{"$f":"'Profile angles'!P14","v":10},{"$f":"IF('Profile angles'!Q14<0,1000,IF(EB13<0,1000,'Profile angles'!Q14))","v":1000},{"$f":"IF('Profile angles'!R14<0,1000,IF(EC13<0,1000,'Profile angles'!R14))","v":1000},{"$f":"IF('Profile angles'!S14<0,1000,IF(ED13<0,1000,'Profile angles'!S14))","v":1000},{"$f":"IF('Profile angles'!T14<0,1000,IF(EE13<0,1000,'Profile angles'!T14))","v":1000},{"$f":"IF('Profile angles'!U14<0,1000,IF(EF13<0,1000,'Profile angles'!U14))","v":1000},{"$f":"IF('Profile angles'!V14<0,1000,IF(EG13<0,1000,'Profile angles'!V14))","v":1000},{"$f":"IF('Profile angles'!W14<0,1000,IF(EH13<0,1000,'Profile angles'!W14))","v":1000},{"$f":"IF('Profile angles'!X14<0,1000,IF(EI13<0,1000,'Profile angles'!X14))","v":1000},{"$f":"IF('Profile angles'!Y14<0,1000,IF(EJ13<0,1000,'Profile angles'!Y14))","v":1000},{"$f":"IF('Profile angles'!Z14<0,1000,IF(EK13<0,1000,'Profile angles'!Z14))","v":1000},{"$f":"IF('Profile angles'!AA14<0,1000,IF(EL13<0,1000,'Profile angles'!AA14))","v":1000},{"$f":"IF('Profile angles'!AB14<0,1000,IF(EM13<0,1000,'Profile angles'!AB14))","v":1000},null,{"$f":"'Profile angles'!P43","v":10},{"$f":"IF('Profile angles'!Q43<0,1000,IF(EB13<0,1000,'Profile angles'!Q43))","v":1000},{"$f":"IF('Profile angles'!R43<0,1000,IF(EC13<0,1000,'Profile angles'!R43))","v":1000},{"$f":"IF('Profile angles'!S43<0,1000,IF(ED13<0,1000,'Profile angles'!S43))","v":1000},{"$f":"IF('Profile angles'!T43<0,1000,IF(EE13<0,1000,'Profile angles'!T43))","v":1000},{"$f":"IF('Profile angles'!U43<0,1000,IF(EF13<0,1000,'Profile angles'!U43))","v":1000},{"$f":"IF('Profile angles'!V43<0,1000,IF(EG13<0,1000,'Profile angles'!V43))","v":87.576455047188773},{"$f":"IF('Profile angles'!W43<0,1000,IF(EH13<0,1000,'Profile angles'!W43))","v":1000},{"$f":"IF('Profile angles'!X43<0,1000,IF(EI13<0,1000,'Profile angles'!X43))","v":1000},{"$f":"IF('Profile angles'!Y43<0,1000,IF(EJ13<0,1000,'Profile angles'!Y43))","v":1000},{"$f":"IF('Profile angles'!Z43<0,1000,IF(EK13<0,1000,'Profile angles'!Z43))","v":1000},{"$f":"IF('Profile angles'!AA43<0,1000,IF(EL13<0,1000,'Profile angles'!AA43))","v":1000},{"$f":"IF('Profile angles'!AB43<0,1000,IF(EM13<0,1000,'Profile angles'!AB43))","v":1000},null,10,{"$f":"EB13","v":34.130498638110296},40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,37.566870997040184,33.04159126014769,null,10,{"$f":"EP13","v":34.130498638110296},40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,37.566870997040184,33.04159126014769]
[null,11,{"$f":"('Solar Azimuth'!C13-('Input Data'!$F$9-90))","v":114.88507629301503},{"$f":"('Solar Azimuth'!D13-('Input Data'!$F$9-90))","v":121.63575223875733},{"$f":"('Solar Azimuth'!E13-('Input Data'!$F$9-90))","v":128.94106407984867},{"$f":"('Solar Azimuth'!F13-('Input Data'!$F$9-90))","v":143.64022289811948},{"$f":"('Solar Azimuth'!G13-('Input Data'!$F$9-90))","v":166.56128328990872},{"$f":"('Solar Azimuth'!H13-('Input Data'!$F$9-90))","v":178.98202668740043},{"$f":"('Solar Azimuth'!I13-('Input Data'!$F$9-90))","v":169.73218602655044},{"$f":"('Solar Azimuth'!J13-('Input Data'!$F$9-90))","v":145.67223338475344},{"$f":"('Solar Azimuth'!K13-('Input Data'!$F$9-90))","v":122.5023883084485},{"$f":"('Solar Azimuth'!L13-('Input Data'!$F$9-90))","v":111.13672353802934},{"$f":"('Solar Azimuth'!M13-('Input Data'!$F$9-90))","v":107.40927739240568},{"$f":"('Solar Azimuth'!N13-('Input Data'!$F$9-90))","v":109.53472056873984},null,11,{"$f":"('Solar Azimuth'!C13-('Input Data'!$F$9+180))","v":-155.11492370698497},{"$f":"('Solar Azimuth'!D13-('Input Data'!$F$9+180))","v":-148.36424776124267},{"$f":"('Solar Azimuth'!E13-('Input Data'!$F$9+180))","v":-141.05893592015133},{"$f":"('Solar Azimuth'!F13-('Input Data'!$F$9+180))","v":-126.35977710188054},{"$f":"('Solar Azimuth'!G13-('Input Data'!$F$9+180))","v":-103.43871671009128},{"$f":"('Solar Azimuth'!H13-('Input Data'!$F$9+180))","v":-91.01797331259958},{"$f":"('Solar Azimuth'!I13-('Input Data'!$F$9+180))","v":-100.26781397344958},{"$f":"('Solar Azimuth'!J13-('Input Data'!$F$9+180))","v":-124.32776661524655},{"$f":"('Solar Azimuth'!K13-('Input Data'!$F$9+180))","v":-147.4976116915515},{"$f":"('Solar Azimuth'!L13-('Input Data'!$F$9+180))","v":-158.86327646197066},{"$f":"('Solar Azimuth'!M13-('Input Data'!$F$9+180))","v":-162.59072260759433},{"$f":"('Solar Azimuth'!N13-('Input Data'!$F$9+180))","v":-160.46527943126014},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,4.3115714559620413,3.2464128143092861,2.4749954224766344,1.4723610680172359,0.47789560950652982,3.5537711429889846E-2,0.36230110926214038,1.3657282252450926,3.1390823947123012,5.1732462227384959,6.3783882651190664,5.6369674876386231,null,11,0.92773598694944548,1.2321291926797209,1.616164605265149,2.7167249167941021,8.3700287686893873,112.55648827841401,11.040540306780635,2.9288403988884109,1.2742577279073313,0.77320889588019126,0.62711767201041169,0.70960139627763608,null,11,0,0.18839679642267848,0.3812511443808414,0.63190973299569109,0.88052609762336753,0.99111557214252755,0.90942472268446495,0.65856794368872684,0.2152294013219247,0,0,0,null,11,0.76806600326263863,0.69196770183006984,0.59595884868371274,0.32081877080147447,0,0,0,0.26778990027789729,0.68143556802316718,0.80669777602995218,0.84322058199739702,0.82259965093059095,null,{"$f":"'Profile angles'!P15","v":11},{"$f":"IF('Profile angles'!Q15<0,1000,IF(EB14<0,1000,'Profile angles'!Q15))","v":1000},{"$f":"IF('Profile angles'!R15<0,1000,IF(EC14<0,1000,'Profile angles'!R15))","v":1000},{"$f":"IF('Profile angles'!S15<0,1000,IF(ED14<0,1000,'Profile angles'!S15))","v":1000},{"$f":"IF('Profile angles'!T15<0,1000,IF(EE14<0,1000,'Profile angles'!T15))","v":1000},{"$f":"IF('Profile angles'!U15<0,1000,IF(EF14<0,1000,'Profile angles'!U15))","v":1000},{"$f":"IF('Profile angles'!V15<0,1000,IF(EG14<0,1000,'Profile angles'!V15))","v":1000},{"$f":"IF('Profile angles'!W15<0,1000,IF(EH14<0,1000,'Profile angles'!W15))","v":1000},{"$f":"IF('Profile angles'!X15<0,1000,IF(EI14<0,1000,'Profile angles'!X15))","v":1000},{"$f":"IF('Profile angles'!Y15<0,1000,IF(EJ14<0,1000,'Profile angles'!Y15))","v":1000},{"$f":"IF('Profile angles'!Z15<0,1000,IF(EK14<0,1000,'Profile angles'!Z15))","v":1000},{"$f":"IF('Profile angles'!AA15<0,1000,IF(EL14<0,1000,'Profile angles'!AA15))","v":1000},{"$f":"IF('Profile angles'!AB15<0,1000,IF(EM14<0,1000,'Profile angles'!AB15))","v":1000},null,{"$f":"'Profile angles'!P44","v":11},{"$f":"IF('Profile angles'!Q44<0,1000,IF(EB14<0,1000,'Profile angles'!Q44))","v":1000},{"$f":"IF('Profile angles'!R44<0,1000,IF(EC14<0,1000,'Profile angles'!R44))","v":1000},{"$f":"IF('Profile angles'!S44<0,1000,IF(ED14<0,1000,'Profile angles'!S44))","v":1000},{"$f":"IF('Profile angles'!T44<0,1000,IF(EE14<0,1000,'Profile angles'!T44))","v":1000},{"$f":"IF('Profile angles'!U44<0,1000,IF(EF14<0,1000,'Profile angles'!U44))","v":1000},{"$f":"IF('Profile angles'!V44<0,1000,IF(EG14<0,1000,'Profile angles'!V44))","v":1000},{"$f":"IF('Profile angles'!W44<0,1000,IF(EH14<0,1000,'Profile angles'!W44))","v":1000},{"$f":"IF('Profile angles'!X44<0,1000,IF(EI14<0,1000,'Profile angles'!X44))","v":1000},{"$f":"IF('Profile angles'!Y44<0,1000,IF(EJ14<0,1000,'Profile angles'!Y44))","v":1000},{"$f":"IF('Profile angles'!Z44<0,1000,IF(EK14<0,1000,'Profile angles'!Z44))","v":1000},{"$f":"IF('Profile angles'!AA44<0,1000,IF(EL14<0,1000,'Profile angles'!AA44))","v":1000},{"$f":"IF('Profile angles'!AB44<0,1000,IF(EM14<0,1000,'Profile angles'!AB44))","v":1000},null,11,{"$f":"EB14","v":41.499338482119107},49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983,null,11,{"$f":"EP14","v":41.499338482119107},49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983]
[null,12,{"$f":"('Solar Azimuth'!C14-('Input Data'!$F$9-90))","v":96.118848947090342},{"$f":"('Solar Azimuth'!D14-('Input Data'!$F$9-90))","v":98.886713641915151},{"$f":"('Solar Azimuth'!E14-('Input Data'!$F$9-90))","v":98.699226152472818},{"$f":"('Solar Azimuth'!F14-('Input Data'!$F$9-90))","v":96.635494080327632},{"$f":"('Solar Azimuth'!G14-('Input Data'!$F$9-90))","v":101.56382585108686},{"$f":"('Solar Azimuth'!H14-('Input Data'!$F$9-90))","v":147.74787414376027},{"$f":"('Solar Azimuth'!I14-('Input Data'!$F$9-90))","v":126.88537657062238},{"$f":"('Solar Azimuth'!J14-('Input Data'!$F$9-90))","v":100.57531251683476},{"$f":"('Solar Azimuth'!K14-('Input Data'!$F$9-90))","v":90.219367121065503},{"$f":"('Solar Azimuth'!L14-('Input Data'!$F$9-90))","v":93.502097389140133},{"$f":"('Solar Azimuth'!M14-('Input Data'!$F$9-90))","v":92.231001794012499},{"$f":"('Solar Azimuth'!N14-('Input Data'!$F$9-90))","v":91.703294330187774},null,12,{"$f":"('Solar Azimuth'!C14-('Input Data'!$F$9+180))","v":-173.88115105290964},{"$f":"('Solar Azimuth'!D14-('Input Data'!$F$9+180))","v":-171.11328635808485},{"$f":"('Solar Azimuth'!E14-('Input Data'!$F$9+180))","v":-171.30077384752718},{"$f":"('Solar Azimuth'!F14-('Input Data'!$F$9+180))","v":-173.36450591967235},{"$f":"('Solar Azimuth'!G14-('Input Data'!$F$9+180))","v":-168.43617414891315},{"$f":"('Solar Azimuth'!H14-('Input Data'!$F$9+180))","v":-122.25212585623973},{"$f":"('Solar Azimuth'!I14-('Input Data'!$F$9+180))","v":-143.11462342937762},{"$f":"('Solar Azimuth'!J14-('Input Data'!$F$9+180))","v":-169.42468748316523},{"$f":"('Solar Azimuth'!K14-('Input Data'!$F$9+180))","v":-179.78063287893451},{"$f":"('Solar Azimuth'!L14-('Input Data'!$F$9+180))","v":-176.49790261085985},{"$f":"('Solar Azimuth'!M14-('Input Data'!$F$9+180))","v":-177.76899820598749},{"$f":"('Solar Azimuth'!N14-('Input Data'!$F$9+180))","v":-178.29670566981221},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,18.656383023553438,12.79113809888757,13.071239251417959,17.192207423425504,9.7745669836252009,1.2620097732659754,2.6651663281682172,10.712431284282641,522.37089380078942,32.680078435762979,51.337313650127932,67.256608489365263,null,12,0.21440383138307414,0.31271650490177111,0.3060153611346445,0.23266354933280711,0.40922528913055467,3.1695475619402993,1.5008444154962821,0.37339796110233386,7.6573944824825319E-3,0.12239872703679523,7.7916036418669316E-2,5.9473709570598547E-2,null,12,0,0,0,0,0,0.68449755668350609,0.3337084179579457,0,0,0,0,0,null,12,0.94639904215423143,0.92182087377455724,0.92349615971633892,0.94183411266679817,0.8976936777173613,0.20761310951492518,0.62478889612592947,0.90665050972441652,0.99808565137937932,0.9694003182408012,0.98052099089533262,0.9851315726073504,null,{"$f":"'Profile angles'!P16","v":12},{"$f":"IF('Profile angles'!Q16<0,1000,IF(EB15<0,1000,'Profile angles'!Q16))","v":1000},{"$f":"IF('Profile angles'!R16<0,1000,IF(EC15<0,1000,'Profile angles'!R16))","v":1000},{"$f":"IF('Profile angles'!S16<0,1000,IF(ED15<0,1000,'Profile angles'!S16))","v":1000},{"$f":"IF('Profile angles'!T16<0,1000,IF(EE15<0,1000,'Profile angles'!T16))","v":1000},{"$f":"IF('Profile angles'!U16<0,1000,IF(EF15<0,1000,'Profile angles'!U16))","v":1000},{"$f":"IF('Profile angles'!V16<0,1000,IF(EG15<0,1000,'Profile angles'!V16))","v":1000},{"$f":"IF('Profile angles'!W16<0,1000,IF(EH15<0,1000,'Profile angles'!W16))","v":1000},{"$f":"IF('Profile angles'!X16<0,1000,IF(EI15<0,1000,'Profile angles'!X16))","v":1000},{"$f":"IF('Profile angles'!Y16<0,1000,IF(EJ15<0,1000,'Profile angles'!Y16))","v":1000},{"$f":"IF('Profile angles'!Z16<0,1000,IF(EK15<0,1000,'Profile angles'!Z16))","v":1000},{"$f":"IF('Profile angles'!AA16<0,1000,IF(EL15<0,1000,'Profile angles'!AA16))","v":1000},{"$f":"IF('Profile angles'!AB16<0,1000,IF(EM15<0,1000,'Profile angles'!AB16))","v":1000},null,{"$f":"'Profile angles'!P45","v":12},{"$f":"IF('Profile angles'!Q45<0,1000,IF(EB15<0,1000,'Profile angles'!Q45))","v":1000},{"$f":"IF('Profile angles'!R45<0,1000,IF(EC15<0,1000,'Profile angles'!R45))","v":1000},{"$f":"IF('Profile angles'!S45<0,1000,IF(ED15<0,1000,'Profile angles'!S45))","v":1000},{"$f":"IF('Profile angles'!T45<0,1000,IF(EE15<0,1000,'Profile angles'!T45))","v":1000},{"$f":"IF('Profile angles'!U45<0,1000,IF(EF15<0,1000,'Profile angles'!U45))","v":1000},{"$f":"IF('Profile angles'!V45<0,1000,IF(EG15<0,1000,'Profile angles'!V45))","v":1000},{"$f":"IF('Profile angles'!W45<0,1000,IF(EH15<0,1000,'Profile angles'!W45))","v":1000},{"$f":"IF('Profile angles'!X45<0,1000,IF(EI15<0,1000,'Profile angles'!X45))","v":1000},{"$f":"IF('Profile angles'!Y45<0,1000,IF(EJ15<0,1000,'Profile angles'!Y45))","v":1000},{"$f":"IF('Profile angles'!Z45<0,1000,IF(EK15<0,1000,'Profile angles'!Z45))","v":1000},{"$f":"IF('Profile angles'!AA45<0,1000,IF(EL15<0,1000,'Profile angles'!AA45))","v":1000},{"$f":"IF('Profile angles'!AB45<0,1000,IF(EM15<0,1000,'Profile angles'!AB45))","v":1000},null,12,{"$f":"EB15","v":45.177523796213436},54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598,null,12,{"$f":"EP15","v":45.177523796213436},54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598]
[null,13,{"$f":"('Solar Azimuth'!C15-('Input Data'!$F$9-90))","v":76.267263470212924},{"$f":"('Solar Azimuth'!D15-('Input Data'!$F$9-90))","v":73.785569990240347},{"$f":"('Solar Azimuth'!E15-('Input Data'!$F$9-90))","v":64.359006518463914},{"$f":"('Solar Azimuth'!F15-('Input Data'!$F$9-90))","v":42.646391062228972},{"$f":"('Solar Azimuth'!G15-('Input Data'!$F$9-90))","v":15.943541177438121},{"$f":"('Solar Azimuth'!H15-('Input Data'!$F$9-90))","v":3.4145538937010258},{"$f":"('Solar Azimuth'!I15-('Input Data'!$F$9-90))","v":18.98171368746938},{"$f":"('Solar Azimuth'!J15-('Input Data'!$F$9-90))","v":44.280589087177873},{"$f":"('Solar Azimuth'!K15-('Input Data'!$F$9-90))","v":57.164389174203542},{"$f":"('Solar Azimuth'!L15-('Input Data'!$F$9-90))","v":62.802925250835528},{"$f":"('Solar Azimuth'!M15-('Input Data'!$F$9-90))","v":68.529351187883776},{"$f":"('Solar Azimuth'!N15-('Input Data'!$F$9-90))","v":73.605918482803006},null,13,{"$f":"('Solar Azimuth'!C15-('Input Data'!$F$9-180))","v":166.26726347021292},{"$f":"('Solar Azimuth'!D15-('Input Data'!$F$9-180))","v":163.78556999024033},{"$f":"('Solar Azimuth'!E15-('Input Data'!$F$9-180))","v":154.3590065184639},{"$f":"('Solar Azimuth'!F15-('Input Data'!$F$9-180))","v":132.64639106222899},{"$f":"('Solar Azimuth'!G15-('Input Data'!$F$9-180))","v":105.94354117743812},{"$f":"('Solar Azimuth'!H15-('Input Data'!$F$9-180))","v":93.414553893701026},{"$f":"('Solar Azimuth'!I15-('Input Data'!$F$9-180))","v":108.98171368746938},{"$f":"('Solar Azimuth'!J15-('Input Data'!$F$9-180))","v":134.28058908717787},{"$f":"('Solar Azimuth'!K15-('Input Data'!$F$9-180))","v":147.16438917420354},{"$f":"('Solar Azimuth'!L15-('Input Data'!$F$9-180))","v":152.80292525083553},{"$f":"('Solar Azimuth'!M15-('Input Data'!$F$9-180))","v":158.52935118788378},{"$f":"('Solar Azimuth'!N15-('Input Data'!$F$9-180))","v":163.60591848280299},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,8.1840052099578013,6.8775794323023725,4.1666689674939246,1.8420851286555417,0.57135854494679617,0.11933172172696038,0.68794131296942185,1.9503958706407938,3.0991605737448871,3.8920678746817532,5.0849332237373739,6.7980095603932806,null,13,0.48875824212978791,0.58159997123594775,0.95999946988969309,2.1714523057462736,7.000857929537875,33.520005763029964,5.8144494662407276,2.0508657038357132,1.2906720722658718,1.0277313060289504,0.78663766543231839,0.58840752788947148,null,13,0,0,0,0.53947871783611456,0.85716036376330096,0.97016706956825993,0.82801467175764454,0.51240103233980161,0.22520985656377823,2.6983031329561702E-2,0,0,null,13,0.87781043946755299,0.85460000719101303,0.7600001325275767,0.45713692356343161,0,0,0,0.4872835740410717,0.67733198193353206,0.74306717349276241,0.8033405836419204,0.85289811802763216,null,{"$f":"'Profile angles'!P17","v":13},{"$f":"IF('Profile angles'!Q17<0,1000,IF(EB16<0,1000,'Profile angles'!Q17))","v":76.310236007231225},{"$f":"IF('Profile angles'!R17<0,1000,IF(EC16<0,1000,'Profile angles'!R17))","v":78.301959925225134},{"$f":"IF('Profile angles'!S17<0,1000,IF(ED16<0,1000,'Profile angles'!S17))","v":77.550222553106053},{"$f":"IF('Profile angles'!T17<0,1000,IF(EE16<0,1000,'Profile angles'!T17))","v":76.496177068295182},{"$f":"IF('Profile angles'!U17<0,1000,IF(EF16<0,1000,'Profile angles'!U17))","v":76.818295906325034},{"$f":"IF('Profile angles'!V17<0,1000,IF(EG16<0,1000,'Profile angles'!V17))","v":78.211108618523411},{"$f":"IF('Profile angles'!W17<0,1000,IF(EH16<0,1000,'Profile angles'!W17))","v":79.058019787475942},{"$f":"IF('Profile angles'!X17<0,1000,IF(EI16<0,1000,'Profile angles'!X17))","v":77.387091031608094},{"$f":"IF('Profile angles'!Y17<0,1000,IF(EJ16<0,1000,'Profile angles'!Y17))","v":73.467983805952144},{"$f":"IF('Profile angles'!Z17<0,1000,IF(EK16<0,1000,'Profile angles'!Z17))","v":69.609222192948593},{"$f":"IF('Profile angles'!AA17<0,1000,IF(EL16<0,1000,'Profile angles'!AA17))","v":68.255417985347762},{"$f":"IF('Profile angles'!AB17<0,1000,IF(EM16<0,1000,'Profile angles'!AB17))","v":71.453363412613214},null,{"$f":"'Profile angles'!P46","v":13},{"$f":"IF('Profile angles'!Q46<0,1000,IF(EB16<0,1000,'Profile angles'!Q46))","v":1000},{"$f":"IF('Profile angles'!R46<0,1000,IF(EC16<0,1000,'Profile angles'!R46))","v":1000},{"$f":"IF('Profile angles'!S46<0,1000,IF(ED16<0,1000,'Profile angles'!S46))","v":1000},{"$f":"IF('Profile angles'!T46<0,1000,IF(EE16<0,1000,'Profile angles'!T46))","v":1000},{"$f":"IF('Profile angles'!U46<0,1000,IF(EF16<0,1000,'Profile angles'!U46))","v":1000},{"$f":"IF('Profile angles'!V46<0,1000,IF(EG16<0,1000,'Profile angles'!V46))","v":1000},{"$f":"IF('Profile angles'!W46<0,1000,IF(EH16<0,1000,'Profile angles'!W46))","v":1000},{"$f":"IF('Profile angles'!X46<0,1000,IF(EI16<0,1000,'Profile angles'!X46))","v":1000},{"$f":"IF('Profile angles'!Y46<0,1000,IF(EJ16<0,1000,'Profile angles'!Y46))","v":1000},{"$f":"IF('Profile angles'!Z46<0,1000,IF(EK16<0,1000,'Profile angles'!Z46))","v":1000},{"$f":"IF('Profile angles'!AA46<0,1000,IF(EL16<0,1000,'Profile angles'!AA46))","v":1000},{"$f":"IF('Profile angles'!AB46<0,1000,IF(EM16<0,1000,'Profile angles'!AB46))","v":1000},null,13,{"$f":"EB16","v":44.262516808487675},53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703,null,13,{"$f":"EP16","v":44.262516808487675},53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703]
[null,14,{"$f":"('Solar Azimuth'!C16-('Input Data'!$F$9-90))","v":58.71407429506786},{"$f":"('Solar Azimuth'!D16-('Input Data'!$F$9-90))","v":52.706794969524744},{"$f":"('Solar Azimuth'!E16-('Input Data'!$F$9-90))","v":40.162495230117166},{"$f":"('Solar Azimuth'!F16-('Input Data'!$F$9-90))","v":20.230865011389085},{"$f":"('Solar Azimuth'!G16-('Input Data'!$F$9-90))","v":3.4493002140159348},{"$f":"('Solar Azimuth'!H16-('Input Data'!$F$9-90))","v":-3.0222206260435485},{"$f":"('Solar Azimuth'!I16-('Input Data'!$F$9-90))","v":4.2996176141758582},{"$f":"('Solar Azimuth'!J16-('Input Data'!$F$9-90))","v":20.735608418876581},{"$f":"('Solar Azimuth'!K16-('Input Data'!$F$9-90))","v":35.795382130315581},{"$f":"('Solar Azimuth'!L16-('Input Data'!$F$9-90))","v":44.721962991616429},{"$f":"('Solar Azimuth'!M16-('Input Data'!$F$9-90))","v":52.514806498414103},{"$f":"('Solar Azimuth'!N16-('Input Data'!$F$9-90))","v":57.812052280891983},null,14,{"$f":"('Solar Azimuth'!C16-('Input Data'!$F$9-180))","v":148.71407429506786},{"$f":"('Solar Azimuth'!D16-('Input Data'!$F$9-180))","v":142.70679496952474},{"$f":"('Solar Azimuth'!E16-('Input Data'!$F$9-180))","v":130.16249523011717},{"$f":"('Solar Azimuth'!F16-('Input Data'!$F$9-180))","v":110.23086501138908},{"$f":"('Solar Azimuth'!G16-('Input Data'!$F$9-180))","v":93.449300214015935},{"$f":"('Solar Azimuth'!H16-('Input Data'!$F$9-180))","v":86.977779373956452},{"$f":"('Solar Azimuth'!I16-('Input Data'!$F$9-180))","v":94.299617614175858},{"$f":"('Solar Azimuth'!J16-('Input Data'!$F$9-180))","v":110.73560841887658},{"$f":"('Solar Azimuth'!K16-('Input Data'!$F$9-180))","v":125.79538213031557},{"$f":"('Solar Azimuth'!L16-('Input Data'!$F$9-180))","v":134.72196299161644},{"$f":"('Solar Azimuth'!M16-('Input Data'!$F$9-180))","v":142.51480649841409},{"$f":"('Solar Azimuth'!N16-('Input Data'!$F$9-180))","v":147.81205228089198},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,3.2912431090212055,2.6260212748937031,1.6878881954939748,0.73708020327204826,0.12054895915964677,0.10559335095693709,0.15036733216001172,0.75715780243783937,1.4422004657931577,1.9806829425528376,2.6078458663389363,3.1774281735384529,null,14,1.2153462589974324,1.5232169054540177,2.3698252115741383,5.4268178445753801,33.181539084901388,37.881173044989104,26.601522701376688,5.282914588109775,2.7735395285704247,2.0195054514098709,1.5338329813239544,1.25887975480041,null,14,0.17718922274469862,0.34349468127657423,0.57802795112650629,0.81572994918198793,0.96986276021008833,0.97360166226076572,0.96240816695999709,0.81071054939054021,0.63944988355171062,0.50482926436179065,0.34803853341526592,0.20564295661538678,null,14,0.69616343525064184,0.61919577363649558,0.40754369710646543,0,0,0,0,0,0.30661511785739382,0.49512363714753227,0.6165417546690114,0.68528006129989749,null,{"$f":"'Profile angles'!P18","v":14},{"$f":"IF('Profile angles'!Q18<0,1000,IF(EB17<0,1000,'Profile angles'!Q18))","v":57.329739937520216},{"$f":"IF('Profile angles'!R18<0,1000,IF(EC17<0,1000,'Profile angles'!R18))","v":60.7360775958551},{"$f":"IF('Profile angles'!S18<0,1000,IF(ED17<0,1000,'Profile angles'!S18))","v":61.409664244736106},{"$f":"IF('Profile angles'!T18<0,1000,IF(EE17<0,1000,'Profile angles'!T18))","v":61.715956668379413},{"$f":"IF('Profile angles'!U18<0,1000,IF(EF17<0,1000,'Profile angles'!U18))","v":62.905108672619058},{"$f":"IF('Profile angles'!V18<0,1000,IF(EG17<0,1000,'Profile angles'!V18))","v":64.600922398571711},{"$f":"IF('Profile angles'!W18<0,1000,IF(EH17<0,1000,'Profile angles'!W18))","v":65.128294922488053},{"$f":"IF('Profile angles'!X18<0,1000,IF(EI17<0,1000,'Profile angles'!X18))","v":62.607791450328726},{"$f":"IF('Profile angles'!Y18<0,1000,IF(EJ17<0,1000,'Profile angles'!Y18))","v":57.468525117430246},{"$f":"IF('Profile angles'!Z18<0,1000,IF(EK17<0,1000,'Profile angles'!Z18))","v":52.462028938168871},{"$f":"IF('Profile angles'!AA18<0,1000,IF(EL17<0,1000,'Profile angles'!AA18))","v":49.834295771439308},{"$f":"IF('Profile angles'!AB18<0,1000,IF(EM17<0,1000,'Profile angles'!AB18))","v":52.146583450749397},null,{"$f":"'Profile angles'!P47","v":14},{"$f":"IF('Profile angles'!Q47<0,1000,IF(EB17<0,1000,'Profile angles'!Q47))","v":1000},{"$f":"IF('Profile angles'!R47<0,1000,IF(EC17<0,1000,'Profile angles'!R47))","v":1000},{"$f":"IF('Profile angles'!S47<0,1000,IF(ED17<0,1000,'Profile angles'!S47))","v":1000},{"$f":"IF('Profile angles'!T47<0,1000,IF(EE17<0,1000,'Profile angles'!T47))","v":1000},{"$f":"IF('Profile angles'!U47<0,1000,IF(EF17<0,1000,'Profile angles'!U47))","v":1000},{"$f":"IF('Profile angles'!V47<0,1000,IF(EG17<0,1000,'Profile angles'!V47))","v":88.563972173918145},{"$f":"IF('Profile angles'!W47<0,1000,IF(EH17<0,1000,'Profile angles'!W47))","v":1000},{"$f":"IF('Profile angles'!X47<0,1000,IF(EI17<0,1000,'Profile angles'!X47))","v":1000},{"$f":"IF('Profile angles'!Y47<0,1000,IF(EJ17<0,1000,'Profile angles'!Y47))","v":1000},{"$f":"IF('Profile angles'!Z47<0,1000,IF(EK17<0,1000,'Profile angles'!Z47))","v":1000},{"$f":"IF('Profile angles'!AA47<0,1000,IF(EL17<0,1000,'Profile angles'!AA47))","v":1000},{"$f":"IF('Profile angles'!AB47<0,1000,IF(EM17<0,1000,'Profile angles'!AB47))","v":1000},null,14,{"$f":"EB17","v":39.001643714284292},47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348,null,14,{"$f":"EP17","v":39.001643714284292},47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348]
[null,15,{"$f":"('Solar Azimuth'!C17-('Input Data'!$F$9-90))","v":44.941480032338212},{"$f":"('Solar Azimuth'!D17-('Input Data'!$F$9-90))","v":37.542970727225381},{"$f":"('Solar Azimuth'!E17-('Input Data'!$F$9-90))","v":25.405430823072507},{"$f":"('Solar Azimuth'!F17-('Input Data'!$F$9-90))","v":9.2184273623364987},{"$f":"('Solar Azimuth'!G17-('Input Data'!$F$9-90))","v":-2.9389460763838144},{"$f":"('Solar Azimuth'!H17-('Input Data'!$F$9-90))","v":-7.3554695521591498},{"$f":"('Solar Azimuth'!I17-('Input Data'!$F$9-90))","v":-2.3704814782376644},{"$f":"('Solar Azimuth'!J17-('Input Data'!$F$9-90))","v":9.4534979551948197},{"$f":"('Solar Azimuth'!K17-('Input Data'!$F$9-90))","v":22.613296533239364},{"$f":"('Solar Azimuth'!L17-('Input Data'!$F$9-90))","v":31.932255396805935},{"$f":"('Solar Azimuth'!M17-('Input Data'!$F$9-90))","v":40.243846766776848},{"$f":"('Solar Azimuth'!N17-('Input Data'!$F$9-90))","v":45.280261294917132},null,15,{"$f":"('Solar Azimuth'!C17-('Input Data'!$F$9-180))","v":134.94148003233821},{"$f":"('Solar Azimuth'!D17-('Input Data'!$F$9-180))","v":127.54297072722538},{"$f":"('Solar Azimuth'!E17-('Input Data'!$F$9-180))","v":115.40543082307251},{"$f":"('Solar Azimuth'!F17-('Input Data'!$F$9-180))","v":99.218427362336499},{"$f":"('Solar Azimuth'!G17-('Input Data'!$F$9-180))","v":87.061053923616186},{"$f":"('Solar Azimuth'!H17-('Input Data'!$F$9-180))","v":82.64453044784085},{"$f":"('Solar Azimuth'!I17-('Input Data'!$F$9-180))","v":87.629518521762336},{"$f":"('Solar Azimuth'!J17-('Input Data'!$F$9-180))","v":99.45349795519482},{"$f":"('Solar Azimuth'!K17-('Input Data'!$F$9-180))","v":112.61329653323936},{"$f":"('Solar Azimuth'!L17-('Input Data'!$F$9-180))","v":121.93225539680594},{"$f":"('Solar Azimuth'!M17-('Input Data'!$F$9-180))","v":130.24384676677684},{"$f":"('Solar Azimuth'!N17-('Input Data'!$F$9-180))","v":135.28026129491712},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,1.9959187026242171,1.5370384732801039,0.94990214631444247,0.32458946067202182,0.10267863966010653,0.2581741808816963,8.2792657451236221E-2,0.33301676068799446,0.83306425953814989,1.246453059462763,1.6927562920917227,2.0196622638831019,null,15,2.004089642900202,2.6024072068045472,4.2109600610123223,12.323259023008637,38.956495851922647,15.49341605864503,48.313463091288583,12.011407449091205,4.8015503656555811,3.2091060065463282,2.3630099729579146,1.9805291565478897,null,15,0.50102032434394572,0.61574038167997402,0.76252446342138935,0.91885263483199453,0.97433034008497332,0.93545645477957595,0.97930183563719098,0.91674580982800136,0.79173393511546253,0.68838673513430926,0.57681092697706937,0.49508443402922453,null,15,0.49897758927494951,0.34939819829886321,0,0,0,0,0,0,0,0.19772349836341796,0.40924750676052135,0.50486771086302751,null,{"$f":"'Profile angles'!P19","v":15},{"$f":"IF('Profile angles'!Q19<0,1000,IF(EB18<0,1000,'Profile angles'!Q19))","v":39.812986834028628},{"$f":"IF('Profile angles'!R19<0,1000,IF(EC18<0,1000,'Profile angles'!R19))","v":44.138369778725988},{"$f":"IF('Profile angles'!S19<0,1000,IF(ED18<0,1000,'Profile angles'!S19))","v":45.919354280104962},{"$f":"IF('Profile angles'!T19<0,1000,IF(EE18<0,1000,'Profile angles'!T19))","v":47.350089337983867},{"$f":"IF('Profile angles'!U19<0,1000,IF(EF18<0,1000,'Profile angles'!U19))","v":49.279589339957219},{"$f":"IF('Profile angles'!V19<0,1000,IF(EG18<0,1000,'Profile angles'!V19))","v":51.233884049672319},{"$f":"IF('Profile angles'!W19<0,1000,IF(EH18<0,1000,'Profile angles'!W19))","v":51.471577651808317},{"$f":"IF('Profile angles'!X19<0,1000,IF(EI18<0,1000,'Profile angles'!X19))","v":48.232694478544275},{"$f":"IF('Profile angles'!Y19<0,1000,IF(EJ18<0,1000,'Profile angles'!Y19))","v":42.164171017516459},{"$f":"IF('Profile angles'!Z19<0,1000,IF(EK18<0,1000,'Profile angles'!Z19))","v":36.404340467875528},{"$f":"IF('Profile angles'!AA19<0,1000,IF(EL18<0,1000,'Profile angles'!AA19))","v":32.990491768082641},{"$f":"IF('Profile angles'!AB19<0,1000,IF(EM18<0,1000,'Profile angles'!AB19))","v":34.633273198345066},null,{"$f":"'Profile angles'!P48","v":15},{"$f":"IF('Profile angles'!Q48<0,1000,IF(EB18<0,1000,'Profile angles'!Q48))","v":1000},{"$f":"IF('Profile angles'!R48<0,1000,IF(EC18<0,1000,'Profile angles'!R48))","v":1000},{"$f":"IF('Profile angles'!S48<0,1000,IF(ED18<0,1000,'Profile angles'!S48))","v":1000},{"$f":"IF('Profile angles'!T48<0,1000,IF(EE18<0,1000,'Profile angles'!T48))","v":1000},{"$f":"IF('Profile angles'!U48<0,1000,IF(EF18<0,1000,'Profile angles'!U48))","v":87.46971071470432},{"$f":"IF('Profile angles'!V48<0,1000,IF(EG18<0,1000,'Profile angles'!V48))","v":84.081683557615165},{"$f":"IF('Profile angles'!W48<0,1000,IF(EH18<0,1000,'Profile angles'!W48))","v":88.112119041692722},{"$f":"IF('Profile angles'!X48<0,1000,IF(EI18<0,1000,'Profile angles'!X48))","v":1000},{"$f":"IF('Profile angles'!Y48<0,1000,IF(EJ18<0,1000,'Profile angles'!Y48))","v":1000},{"$f":"IF('Profile angles'!Z48<0,1000,IF(EK18<0,1000,'Profile angles'!Z48))","v":1000},{"$f":"IF('Profile angles'!AA48<0,1000,IF(EL18<0,1000,'Profile angles'!AA48))","v":1000},{"$f":"IF('Profile angles'!AB48<0,1000,IF(EM18<0,1000,'Profile angles'!AB48))","v":1000},null,15,{"$f":"EB18","v":30.541133571003865},37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655,null,15,{"$f":"EP18","v":30.541133571003865},37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655]
[null,16,{"$f":"('Solar Azimuth'!C18-('Input Data'!$F$9-90))","v":34.510352665517594},{"$f":"('Solar Azimuth'!D18-('Input Data'!$F$9-90))","v":26.731161680387615},{"$f":"('Solar Azimuth'!E18-('Input Data'!$F$9-90))","v":15.548899990516077},{"$f":"('Solar Azimuth'!F18-('Input Data'!$F$9-90))","v":1.8094767567827006},{"$f":"('Solar Azimuth'!G18-('Input Data'!$F$9-90))","v":-8.0387084231693819},{"$f":"('Solar Azimuth'!H18-('Input Data'!$F$9-90))","v":-11.470265617107984},{"$f":"('Solar Azimuth'!I18-('Input Data'!$F$9-90))","v":-7.5041471807779914},{"$f":"('Solar Azimuth'!J18-('Input Data'!$F$9-90))","v":1.9691283381029905},{"$f":"('Solar Azimuth'!K18-('Input Data'!$F$9-90))","v":13.515511233724098},{"$f":"('Solar Azimuth'!L18-('Input Data'!$F$9-90))","v":22.580592483252715},{"$f":"('Solar Azimuth'!M18-('Input Data'!$F$9-90))","v":30.919433907913337},{"$f":"('Solar Azimuth'!N18-('Input Data'!$F$9-90))","v":35.622464387417914},null,16,{"$f":"('Solar Azimuth'!C18-('Input Data'!$F$9-180))","v":124.51035266551759},{"$f":"('Solar Azimuth'!D18-('Input Data'!$F$9-180))","v":116.73116168038761},{"$f":"('Solar Azimuth'!E18-('Input Data'!$F$9-180))","v":105.54889999051608},{"$f":"('Solar Azimuth'!F18-('Input Data'!$F$9-180))","v":91.809476756782701},{"$f":"('Solar Azimuth'!G18-('Input Data'!$F$9-180))","v":81.961291576830618},{"$f":"('Solar Azimuth'!H18-('Input Data'!$F$9-180))","v":78.529734382892016},{"$f":"('Solar Azimuth'!I18-('Input Data'!$F$9-180))","v":82.495852819222009},{"$f":"('Solar Azimuth'!J18-('Input Data'!$F$9-180))","v":91.96912833810299},{"$f":"('Solar Azimuth'!K18-('Input Data'!$F$9-180))","v":103.5155112337241},{"$f":"('Solar Azimuth'!L18-('Input Data'!$F$9-180))","v":112.58059248325272},{"$f":"('Solar Azimuth'!M18-('Input Data'!$F$9-180))","v":120.91943390791334},{"$f":"('Solar Azimuth'!N18-('Input Data'!$F$9-180))","v":125.62246438741792},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,1.3750940573878732,1.007258480151463,0.55648773366940341,6.3183661730100898E-2,0.28245966743259326,0.40582382440484643,0.26345226960023205,6.8762620768522617E-2,0.48073020725317522,0.83172492695357625,1.1978968497768165,1.4330457771039471,null,16,2.9088919252537497,3.9711753028860222,7.1879392086947727,63.307505302346016,14.161313848302139,9.8564937774812194,15.183015906713132,58.171139425667086,8.3206753801793258,4.8092823364704387,3.3391856742467021,2.7912576582749709,null,16,0.65622648565303177,0.7481853799621343,0.8608780665826492,0.98420408456747477,0.92938508314185164,0.89854404389878839,0.93413693259994202,0.9828093448078693,0.87981744818670615,0.79206876826160588,0.70052578755579586,0.64173855572401317,null,16,0.27277701868656257,7.2061742784944594E-3,0,0,0,0,0,0,0,0,0.16520358143832448,0.30218558543125729,null,{"$f":"'Profile angles'!P20","v":16},{"$f":"IF('Profile angles'!Q20<0,1000,IF(EB19<0,1000,'Profile angles'!Q20))","v":23.875002480593196},{"$f":"IF('Profile angles'!R20<0,1000,IF(EC19<0,1000,'Profile angles'!R20))","v":28.656528802721059},{"$f":"IF('Profile angles'!S20<0,1000,IF(ED19<0,1000,'Profile angles'!S20))","v":31.171654482760921},{"$f":"IF('Profile angles'!T20<0,1000,IF(EE19<0,1000,'Profile angles'!T20))","v":33.432906045521179},{"$f":"IF('Profile angles'!U20<0,1000,IF(EF19<0,1000,'Profile angles'!U20))","v":35.951128585501792},{"$f":"IF('Profile angles'!V20<0,1000,IF(EG19<0,1000,'Profile angles'!V20))","v":38.121029600348642},{"$f":"IF('Profile angles'!W20<0,1000,IF(EH19<0,1000,'Profile angles'!W20))","v":38.115343474138719},{"$f":"IF('Profile angles'!X20<0,1000,IF(EI19<0,1000,'Profile angles'!X20))","v":34.304400656996243},{"$f":"IF('Profile angles'!Y20<0,1000,IF(EJ19<0,1000,'Profile angles'!Y20))","v":27.591172995772371},{"$f":"IF('Profile angles'!Z20<0,1000,IF(EK19<0,1000,'Profile angles'!Z20))","v":21.421982311981434},{"$f":"IF('Profile angles'!AA20<0,1000,IF(EL19<0,1000,'Profile angles'!AA20))","v":17.641166819660786},{"$f":"IF('Profile angles'!AB20<0,1000,IF(EM19<0,1000,'Profile angles'!AB20))","v":18.874041457280981},null,{"$f":"'Profile angles'!P49","v":16},{"$f":"IF('Profile angles'!Q49<0,1000,IF(EB19<0,1000,'Profile angles'!Q49))","v":1000},{"$f":"IF('Profile angles'!R49<0,1000,IF(EC19<0,1000,'Profile angles'!R49))","v":1000},{"$f":"IF('Profile angles'!S49<0,1000,IF(ED19<0,1000,'Profile angles'!S49))","v":1000},{"$f":"IF('Profile angles'!T49<0,1000,IF(EE19<0,1000,'Profile angles'!T49))","v":1000},{"$f":"IF('Profile angles'!U49<0,1000,IF(EF19<0,1000,'Profile angles'!U49))","v":78.980403720895197},{"$f":"IF('Profile angles'!V49<0,1000,IF(EG19<0,1000,'Profile angles'!V49))","v":75.501608463035367},{"$f":"IF('Profile angles'!W49<0,1000,IF(EH19<0,1000,'Profile angles'!W49))","v":80.468716677637929},{"$f":"IF('Profile angles'!X49<0,1000,IF(EI19<0,1000,'Profile angles'!X49))","v":1000},{"$f":"IF('Profile angles'!Y49<0,1000,IF(EJ19<0,1000,'Profile angles'!Y49))","v":1000},{"$f":"IF('Profile angles'!Z49<0,1000,IF(EK19<0,1000,'Profile angles'!Z49))","v":1000},{"$f":"IF('Profile angles'!AA49<0,1000,IF(EL19<0,1000,'Profile angles'!AA49))","v":1000},{"$f":"IF('Profile angles'!AB49<0,1000,IF(EM19<0,1000,'Profile angles'!AB49))","v":1000},null,16,{"$f":"EB19","v":20.038281727598083},26.016647471873153,30.233879108991232,33.419767540103443,35.682648220686666,37.56104623172925,37.876258416390314,34.288646107643089,26.935985833021654,19.913519068774189,15.259931573481456,15.530455637101428,null,16,{"$f":"EP19","v":20.038281727598083},26.016647471873153,30.233879108991232,33.419767540103443,35.682648220686666,37.56104623172925,37.876258416390314,34.288646107643089,26.935985833021654,19.913519068774189,15.259931573481456,15.530455637101428]
[null,17,{"$f":"('Solar Azimuth'!C19-('Input Data'!$F$9-90))","v":26.460723135338306},{"$f":"('Solar Azimuth'!D19-('Input Data'!$F$9-90))","v":18.544644404442906},{"$f":"('Solar Azimuth'!E19-('Input Data'!$F$9-90))","v":8.0315040139551144},{"$f":"('Solar Azimuth'!F19-('Input Data'!$F$9-90))","v":-4.3370103485486027},{"$f":"('Solar Azimuth'!G19-('Input Data'!$F$9-90))","v":-12.95522704697413},{"$f":"('Solar Azimuth'!H19-('Input Data'!$F$9-90))","v":-15.831771146861357},{"$f":"('Solar Azimuth'!I19-('Input Data'!$F$9-90))","v":-12.373216311793286},{"$f":"('Solar Azimuth'!J19-('Input Data'!$F$9-90))","v":-4.1905980785871009},{"$f":"('Solar Azimuth'!K19-('Input Data'!$F$9-90))","v":6.3481040051510007},{"$f":"('Solar Azimuth'!L19-('Input Data'!$F$9-90))","v":15.221283429308258},{"$f":"('Solar Azimuth'!M19-('Input Data'!$F$9-90))","v":23.606392816975699},{"$f":"('Solar Azimuth'!N19-('Input Data'!$F$9-90))","v":28.085268182094261},null,17,{"$f":"('Solar Azimuth'!C19-('Input Data'!$F$9-180))","v":116.4607231353383},{"$f":"('Solar Azimuth'!D19-('Input Data'!$F$9-180))","v":108.54464440444291},{"$f":"('Solar Azimuth'!E19-('Input Data'!$F$9-180))","v":98.031504013955114},{"$f":"('Solar Azimuth'!F19-('Input Data'!$F$9-180))","v":85.662989651451397},{"$f":"('Solar Azimuth'!G19-('Input Data'!$F$9-180))","v":77.04477295302587},{"$f":"('Solar Azimuth'!H19-('Input Data'!$F$9-180))","v":74.168228853138643},{"$f":"('Solar Azimuth'!I19-('Input Data'!$F$9-180))","v":77.626783688206714},{"$f":"('Solar Azimuth'!J19-('Input Data'!$F$9-180))","v":85.809401921412899},{"$f":"('Solar Azimuth'!K19-('Input Data'!$F$9-180))","v":96.348104005151001},{"$f":"('Solar Azimuth'!L19-('Input Data'!$F$9-180))","v":105.22128342930826},{"$f":"('Solar Azimuth'!M19-('Input Data'!$F$9-180))","v":113.6063928169757},{"$f":"('Solar Azimuth'!N19-('Input Data'!$F$9-180))","v":118.08526818209427},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,0.99545196608161113,0.67092394228366214,0.2822031746504749,0.15168002746829845,0.46009050674518565,0.56714096737101327,0.43874849774452335,0.14654086434487501,0.22250182621673806,0.54418582731168508,0.87404427285330133,1.0672397893131178,null,17,4.0182752521401577,5.9619276462022981,14.174184981987654,26.371303241199708,8.6939416079178979,7.0529202264157247,9.1168403323608391,27.296140348853431,17.977380536659584,7.350430311205038,4.5764272179738379,3.7479861977170326,null,17,0.75113700847959719,0.83226901442908452,0.92944920633738126,0.96207999313292536,0.88497737331370363,0.85821475815724668,0.89031287556386918,0.96336478391378122,0.94437454344581551,0.86395354317207873,0.78148893178667467,0.73319005267172055,null,17,0,0,0,0,0,0,0,0,0,0,0,6.3003450570741859E-2,null,{"$f":"'Profile angles'!P21","v":17},{"$f":"IF('Profile angles'!Q21<0,1000,IF(EB20<0,1000,'Profile angles'!Q21))","v":9.2385105897919768},{"$f":"IF('Profile angles'!R21<0,1000,IF(EC20<0,1000,'Profile angles'!R21))","v":14.141799097654047},{"$f":"IF('Profile angles'!S21<0,1000,IF(ED20<0,1000,'Profile angles'!S21))","v":17.054801329090424},{"$f":"IF('Profile angles'!T21<0,1000,IF(EE20<0,1000,'Profile angles'!T21))","v":19.854676249106344},{"$f":"IF('Profile angles'!U21<0,1000,IF(EF20<0,1000,'Profile angles'!U21))","v":22.809925103490791},{"$f":"IF('Profile angles'!V21<0,1000,IF(EG20<0,1000,'Profile angles'!V21))","v":25.161800037123339},{"$f":"IF('Profile angles'!W21<0,1000,IF(EH20<0,1000,'Profile angles'!W21))","v":24.96833403497148},{"$f":"IF('Profile angles'!X21<0,1000,IF(EI20<0,1000,'Profile angles'!X21))","v":20.721091695019812},{"$f":"IF('Profile angles'!Y21<0,1000,IF(EJ20<0,1000,'Profile angles'!Y21))","v":13.597367832295648},{"$f":"IF('Profile angles'!Z21<0,1000,IF(EK20<0,1000,'Profile angles'!Z21))","v":7.2728027816997747},{"$f":"IF('Profile angles'!AA21<0,1000,IF(EL20<0,1000,'Profile angles'!AA21))","v":3.4258822939894862},{"$f":"IF('Profile angles'!AB21<0,1000,IF(EM20<0,1000,'Profile angles'!AB21))","v":4.469701583642955},null,{"$f":"'Profile angles'!P50","v":17},{"$f":"IF('Profile angles'!Q50<0,1000,IF(EB20<0,1000,'Profile angles'!Q50))","v":1000},{"$f":"IF('Profile angles'!R50<0,1000,IF(EC20<0,1000,'Profile angles'!R50))","v":1000},{"$f":"IF('Profile angles'!S50<0,1000,IF(ED20<0,1000,'Profile angles'!S50))","v":1000},{"$f":"IF('Profile angles'!T50<0,1000,IF(EE20<0,1000,'Profile angles'!T50))","v":78.138866865290566},{"$f":"IF('Profile angles'!U50<0,1000,IF(EF20<0,1000,'Profile angles'!U50))","v":61.321747515833657},{"$f":"IF('Profile angles'!V50<0,1000,IF(EG20<0,1000,'Profile angles'!V50))","v":58.882202464658548},{"$f":"IF('Profile angles'!W50<0,1000,IF(EH20<0,1000,'Profile angles'!W50))","v":64.773504841898102},{"$f":"IF('Profile angles'!X50<0,1000,IF(EI20<0,1000,'Profile angles'!X50))","v":79.038177006237575},{"$f":"IF('Profile angles'!Y50<0,1000,IF(EJ20<0,1000,'Profile angles'!Y50))","v":1000},{"$f":"IF('Profile angles'!Z50<0,1000,IF(EK20<0,1000,'Profile angles'!Z50))","v":1000},{"$f":"IF('Profile angles'!AA50<0,1000,IF(EL20<0,1000,'Profile angles'!AA50))","v":1000},{"$f":"IF('Profile angles'!AB50<0,1000,IF(EM20<0,1000,'Profile angles'!AB50))","v":1000},null,17,{"$f":"EB20","v":8.2848854255444504},13.434807821200849,16.897092448538277,19.80224832363653,22.286756355186323,24.319689951925163,24.456964963286701,20.670382142796534,13.51706337533537,7.0202572324504446,3.1397975005302774,3.9451572875932328,null,17,{"$f":"EP20","v":8.2848854255444504},13.434807821200849,16.897092448538277,19.80224832363653,22.286756355186323,24.319689951925163,24.456964963286701,20.670382142796534,13.51706337533537,7.0202572324504446,3.1397975005302774,3.9451572875932328]
[null,18,{"$f":"('Solar Azimuth'!C20-('Input Data'!$F$9-90))","v":19.972606357545686},{"$f":"('Solar Azimuth'!D20-('Input Data'!$F$9-90))","v":11.815822621090689},{"$f":"('Solar Azimuth'!E20-('Input Data'!$F$9-90))","v":1.5304137753386726},{"$f":"('Solar Azimuth'!F20-('Input Data'!$F$9-90))","v":-10.232608427091932},{"$f":"('Solar Azimuth'!G20-('Input Data'!$F$9-90))","v":-18.21764026515396},{"$f":"('Solar Azimuth'!H20-('Input Data'!$F$9-90))","v":-20.746469283710354},{"$f":"('Solar Azimuth'!I20-('Input Data'!$F$9-90))","v":-17.532105861683178},{"$f":"('Solar Azimuth'!J20-('Input Data'!$F$9-90))","v":-10.067604893682898},{"$f":"('Solar Azimuth'!K20-('Input Data'!$F$9-90))","v":-3.8304508740267806E-2},{"$f":"('Solar Azimuth'!L20-('Input Data'!$F$9-90))","v":8.905662319897985},{"$f":"('Solar Azimuth'!M20-('Input Data'!$F$9-90))","v":17.58111073041492},{"$f":"('Solar Azimuth'!N20-('Input Data'!$F$9-90))","v":22.013185939328324},null,18,{"$f":"('Solar Azimuth'!C20-('Input Data'!$F$9-180))","v":109.97260635754569},{"$f":"('Solar Azimuth'!D20-('Input Data'!$F$9-180))","v":101.81582262109069},{"$f":"('Solar Azimuth'!E20-('Input Data'!$F$9-180))","v":91.530413775338673},{"$f":"('Solar Azimuth'!F20-('Input Data'!$F$9-180))","v":79.767391572908068},{"$f":"('Solar Azimuth'!G20-('Input Data'!$F$9-180))","v":71.78235973484604},{"$f":"('Solar Azimuth'!H20-('Input Data'!$F$9-180))","v":69.253530716289646},{"$f":"('Solar Azimuth'!I20-('Input Data'!$F$9-180))","v":72.467894138316822},{"$f":"('Solar Azimuth'!J20-('Input Data'!$F$9-180))","v":79.932395106317102},{"$f":"('Solar Azimuth'!K20-('Input Data'!$F$9-180))","v":89.961695491259732},{"$f":"('Solar Azimuth'!L20-('Input Data'!$F$9-180))","v":98.905662319897985},{"$f":"('Solar Azimuth'!M20-('Input Data'!$F$9-180))","v":107.58111073041492},{"$f":"('Solar Azimuth'!N20-('Input Data'!$F$9-180))","v":112.01318593932832},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,0.72685776394181012,0.41839822067212046,5.3434227010461501E-2,0.3610320177913261,0.65824893547366503,0.75759128486752114,0.63182991471601313,0.35508769562655074,1.3370797909538236E-3,0.31339414427234447,0.63371173727245422,0.80858791176007316,null,18,5.5031399517667214,9.560270102426216,74.858386165422942,11.0793497609178,6.0767283992972452,5.2798917832053389,6.3308176881714582,11.26482288534954,2991.5940896440793,12.763480342899888,6.3120181696749356,4.946895621149098,null,18,0.81828555901454747,0.8954004448319699,0.98664144324738468,0.9097419955521685,0.83543776613158371,0.81060217878311969,0.84204252132099677,0.91122807609336232,0.99966573005226156,0.92165146393191388,0.84157206568188647,0.79785302205998176,null,18,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$f":"'Profile angles'!P22","v":18},{"$f":"IF('Profile angles'!Q22<0,1000,IF(EB21<0,1000,'Profile angles'!Q22))","v":1000},{"$f":"IF('Profile angles'!R22<0,1000,IF(EC21<0,1000,'Profile angles'!R22))","v":0.2911309486956099},{"$f":"IF('Profile angles'!S22<0,1000,IF(ED21<0,1000,'Profile angles'!S22))","v":3.324414100544868},{"$f":"IF('Profile angles'!T22<0,1000,IF(EE21<0,1000,'Profile angles'!T22))","v":6.3911335111384062},{"$f":"IF('Profile angles'!U22<0,1000,IF(EF21<0,1000,'Profile angles'!U22))","v":9.6364921571497923},{"$f":"IF('Profile angles'!V22<0,1000,IF(EG21<0,1000,'Profile angles'!V22))","v":12.146410157593207},{"$f":"IF('Profile angles'!W22<0,1000,IF(EH21<0,1000,'Profile angles'!W22))","v":11.827587615885063},{"$f":"IF('Profile angles'!X22<0,1000,IF(EI21<0,1000,'Profile angles'!X22))","v":7.2645164628018666},{"$f":"IF('Profile angles'!Y22<0,1000,IF(EJ21<0,1000,'Profile angles'!Y22))","v":1000},{"$f":"IF('Profile angles'!Z22<0,1000,IF(EK21<0,1000,'Profile angles'!Z22))","v":1000},{"$f":"IF('Profile angles'!AA22<0,1000,IF(EL21<0,1000,'Profile angles'!AA22))","v":1000},{"$f":"IF('Profile angles'!AB22<0,1000,IF(EM21<0,1000,'Profile angles'!AB22))","v":1000},null,{"$f":"'Profile angles'!P51","v":18},{"$f":"IF('Profile angles'!Q51<0,1000,IF(EB21<0,1000,'Profile angles'!Q51))","v":1000},{"$f":"IF('Profile angles'!R51<0,1000,IF(EC21<0,1000,'Profile angles'!R51))","v":1000},{"$f":"IF('Profile angles'!S51<0,1000,IF(ED21<0,1000,'Profile angles'!S51))","v":1000},{"$f":"IF('Profile angles'!T51<0,1000,IF(EE21<0,1000,'Profile angles'!T51))","v":31.819852453718237},{"$f":"IF('Profile angles'!U51<0,1000,IF(EF21<0,1000,'Profile angles'!U51))","v":27.288827655179634},{"$f":"IF('Profile angles'!V51<0,1000,IF(EG21<0,1000,'Profile angles'!V51))","v":29.60490953504689},{"$f":"IF('Profile angles'!W51<0,1000,IF(EH21<0,1000,'Profile angles'!W51))","v":33.539568672346483},{"$f":"IF('Profile angles'!X51<0,1000,IF(EI21<0,1000,'Profile angles'!X51))","v":35.677719714065745},{"$f":"IF('Profile angles'!Y51<0,1000,IF(EJ21<0,1000,'Profile angles'!Y51))","v":1000},{"$f":"IF('Profile angles'!Z51<0,1000,IF(EK21<0,1000,'Profile angles'!Z51))","v":1000},{"$f":"IF('Profile angles'!AA51<0,1000,IF(EL21<0,1000,'Profile angles'!AA51))","v":1000},{"$f":"IF('Profile angles'!AB51<0,1000,IF(EM21<0,1000,'Profile angles'!AB51))","v":1000},null,18,{"$f":"EB21","v":-4.242067037456934},0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772,null,18,{"$f":"EP21","v":-4.242067037456934},0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772]
[null,19,{"$f":"('Solar Azimuth'!C21-('Input Data'!$F$9-90))","v":14.443608460207599},{"$f":"('Solar Azimuth'!D21-('Input Data'!$F$9-90))","v":5.7542728429225463},{"$f":"('Solar Azimuth'!E21-('Input Data'!$F$9-90))","v":-4.7909988948714499},{"$f":"('Solar Azimuth'!F21-('Input Data'!$F$9-90))","v":-16.548933940256234},{"$f":"('Solar Azimuth'!G21-('Input Data'!$F$9-90))","v":-24.271914122206482},{"$f":"('Solar Azimuth'!H21-('Input Data'!$F$9-90))","v":-26.550693724004134},{"$f":"('Solar Azimuth'!I21-('Input Data'!$F$9-90))","v":-23.418664534120552},{"$f":"('Solar Azimuth'!J21-('Input Data'!$F$9-90))","v":-16.336844142442843},{"$f":"('Solar Azimuth'!K21-('Input Data'!$F$9-90))","v":-6.429196681357439},{"$f":"('Solar Azimuth'!L21-('Input Data'!$F$9-90))","v":2.9358659497309247},{"$f":"('Solar Azimuth'!M21-('Input Data'!$F$9-90))","v":12.308806400416316},{"$f":"('Solar Azimuth'!N21-('Input Data'!$F$9-90))","v":16.923119162826197},null,19,{"$f":"('Solar Azimuth'!C21-('Input Data'!$F$9-180))","v":104.4436084602076},{"$f":"('Solar Azimuth'!D21-('Input Data'!$F$9-180))","v":95.754272842922546},{"$f":"('Solar Azimuth'!E21-('Input Data'!$F$9-180))","v":85.20900110512855},{"$f":"('Solar Azimuth'!F21-('Input Data'!$F$9-180))","v":73.451066059743766},{"$f":"('Solar Azimuth'!G21-('Input Data'!$F$9-180))","v":65.728085877793518},{"$f":"('Solar Azimuth'!H21-('Input Data'!$F$9-180))","v":63.449306275995866},{"$f":"('Solar Azimuth'!I21-('Input Data'!$F$9-180))","v":66.581335465879448},{"$f":"('Solar Azimuth'!J21-('Input Data'!$F$9-180))","v":73.663155857557157},{"$f":"('Solar Azimuth'!K21-('Input Data'!$F$9-180))","v":83.570803318642561},{"$f":"('Solar Azimuth'!L21-('Input Data'!$F$9-180))","v":92.935865949730925},{"$f":"('Solar Azimuth'!M21-('Input Data'!$F$9-180))","v":102.30880640041632},{"$f":"('Solar Azimuth'!N21-('Input Data'!$F$9-180))","v":106.9231191628262},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,0.51513561134924257,0.20154007415200931,0.16762828314829892,0.59428545160522017,0.90185463674408262,0.99937361639715461,0.86625091323332082,0.58623726847874758,0.22536798234507799,0.10257083987003481,0.43639254669010741,0.60852807313573087,null,19,7.7649456024273018,19.847169436799181,23.862321589616492,6.7307722058408617,4.4353045790627466,4.0025071048207312,4.61759974955734,6.8231758966463749,17.74875010362074,38.997438307693585,9.1660593892784643,6.5732382392616566,null,19,0.87121609716268933,0.94961498146199763,0.95809292921292522,0.85142863709869498,0.77453634081397937,0.75015659590071138,0.78343727169166977,0.85344068288031316,0.94365800441373049,0.97435729003249127,0.89090186332747312,0.84786798171606725,null,19,0,0,0,0,0,0,0,0,0,0,0,0,null,{"$f":"'Profile angles'!P23","v":19},{"$f":"IF('Profile angles'!Q23<0,1000,IF(EB22<0,1000,'Profile angles'!Q23))","v":1000},{"$f":"IF('Profile angles'!R23<0,1000,IF(EC22<0,1000,'Profile angles'!R23))","v":1000},{"$f":"IF('Profile angles'!S23<0,1000,IF(ED22<0,1000,'Profile angles'!S23))","v":1000},{"$f":"IF('Profile angles'!T23<0,1000,IF(EE22<0,1000,'Profile angles'!T23))","v":1000},{"$f":"IF('Profile angles'!U23<0,1000,IF(EF22<0,1000,'Profile angles'!U23))","v":1000},{"$f":"IF('Profile angles'!V23<0,1000,IF(EG22<0,1000,'Profile angles'!V23))","v":1000},{"$f":"IF('Profile angles'!W23<0,1000,IF(EH22<0,1000,'Profile angles'!W23))","v":1000},{"$f":"IF('Profile angles'!X23<0,1000,IF(EI22<0,1000,'Profile angles'!X23))","v":1000},{"$f":"IF('Profile angles'!Y23<0,1000,IF(EJ22<0,1000,'Profile angles'!Y23))","v":1000},{"$f":"IF('Profile angles'!Z23<0,1000,IF(EK22<0,1000,'Profile angles'!Z23))","v":1000},{"$f":"IF('Profile angles'!AA23<0,1000,IF(EL22<0,1000,'Profile angles'!AA23))","v":1000},{"$f":"IF('Profile angles'!AB23<0,1000,IF(EM22<0,1000,'Profile angles'!AB23))","v":1000},null,{"$f":"'Profile angles'!P52","v":19},{"$f":"IF('Profile angles'!Q52<0,1000,IF(EB22<0,1000,'Profile angles'!Q52))","v":1000},{"$f":"IF('Profile angles'!R52<0,1000,IF(EC22<0,1000,'Profile angles'!R52))","v":1000},{"$f":"IF('Profile angles'!S52<0,1000,IF(ED22<0,1000,'Profile angles'!S52))","v":1000},{"$f":"IF('Profile angles'!T52<0,1000,IF(EE22<0,1000,'Profile angles'!T52))","v":1000},{"$f":"IF('Profile angles'!U52<0,1000,IF(EF22<0,1000,'Profile angles'!U52))","v":1000},{"$f":"IF('Profile angles'!V52<0,1000,IF(EG22<0,1000,'Profile angles'!V52))","v":1000},{"$f":"IF('Profile angles'!W52<0,1000,IF(EH22<0,1000,'Profile angles'!W52))","v":1000},{"$f":"IF('Profile angles'!X52<0,1000,IF(EI22<0,1000,'Profile angles'!X52))","v":1000},{"$f":"IF('Profile angles'!Y52<0,1000,IF(EJ22<0,1000,'Profile angles'!Y52))","v":1000},{"$f":"IF('Profile angles'!Z52<0,1000,IF(EK22<0,1000,'Profile angles'!Z52))","v":1000},{"$f":"IF('Profile angles'!AA52<0,1000,IF(EL22<0,1000,'Profile angles'!AA52))","v":1000},{"$f":"IF('Profile angles'!AB52<0,1000,IF(EM22<0,1000,'Profile angles'!AB52))","v":1000},null,19,{"$f":"EB22","v":-17.258784755357599},-13.177535073458104,-10.292097151668569,-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176,null,19,{"$f":"EP22","v":-17.258784755357599},-13.177535073458104,-10.292097151668569,-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176]
[null,20,{"$f":"('Solar Azimuth'!C22-('Input Data'!$F$9-90))","v":9.4001345470871627},{"$f":"('Solar Azimuth'!D22-('Input Data'!$F$9-90))","v":-0.30699306227633372},{"$f":"('Solar Azimuth'!E22-('Input Data'!$F$9-90))","v":-11.689614465946548},{"$f":"('Solar Azimuth'!F22-('Input Data'!$F$9-90))","v":-23.971851617014863},{"$f":"('Solar Azimuth'!G22-('Input Data'!$F$9-90))","v":-31.650675732247308},{"$f":"('Solar Azimuth'!H22-('Input Data'!$F$9-90))","v":-33.692191921397452},{"$f":"('Solar Azimuth'!I22-('Input Data'!$F$9-90))","v":-30.539293657458373},{"$f":"('Solar Azimuth'!J22-('Input Data'!$F$9-90))","v":-23.673653885354412},{"$f":"('Solar Azimuth'!K22-('Input Data'!$F$9-90))","v":-13.612038341956506},{"$f":"('Solar Azimuth'!L22-('Input Data'!$F$9-90))","v":-3.389012330405194},{"$f":"('Solar Azimuth'!M22-('Input Data'!$F$9-90))","v":7.331416767230607},{"$f":"('Solar Azimuth'!N22-('Input Data'!$F$9-90))","v":12.458853223340071},null,20,{"$f":"('Solar Azimuth'!C22-('Input Data'!$F$9-180))","v":99.400134547087163},{"$f":"('Solar Azimuth'!D22-('Input Data'!$F$9-180))","v":89.693006937723666},{"$f":"('Solar Azimuth'!E22-('Input Data'!$F$9-180))","v":78.310385534053452},{"$f":"('Solar Azimuth'!F22-('Input Data'!$F$9-180))","v":66.028148382985137},{"$f":"('Solar Azimuth'!G22-('Input Data'!$F$9-180))","v":58.349324267752692},{"$f":"('Solar Azimuth'!H22-('Input Data'!$F$9-180))","v":56.307808078602548},{"$f":"('Solar Azimuth'!I22-('Input Data'!$F$9-180))","v":59.460706342541627},{"$f":"('Solar Azimuth'!J22-('Input Data'!$F$9-180))","v":66.326346114645588},{"$f":"('Solar Azimuth'!K22-('Input Data'!$F$9-180))","v":76.387961658043494},{"$f":"('Solar Azimuth'!L22-('Input Data'!$F$9-180))","v":86.610987669594806},{"$f":"('Solar Azimuth'!M22-('Input Data'!$F$9-180))","v":97.331416767230607},{"$f":"('Solar Azimuth'!N22-('Input Data'!$F$9-180))","v":102.45885322334007},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,0.33110267824263639,1.0716181984023916E-2,0.41380203222754969,0.88928029181005952,1.2328479470118929,1.3334404493212324,1.1799382993167944,0.87684197644852691,0.48429575640455508,0.11843700271620321,0.25732063583836029,0.44188267973752854,null,20,12.080844592470338,373.26727055992041,9.6664580849627146,4.498019394828054,3.2445201451606205,2.9997590083877683,3.3900077676231648,4.5618254000580585,8.2594157539109467,33.773228874971906,15.544808471997785,9.0521764790055546,null,20,0.91722433043934093,0.99732095450399405,0.89654949194311262,0.77767992704748512,0.69178801324702677,0.66663988766969196,0.7050154251708014,0.78078950588786822,0.87892606089886127,0.97039074932094915,0.93566984104040996,0.88952933006561785,null,20,0,0,0,0,0.18886996370984488,0.25006024790305792,0.1524980580942088,0,0,0,0,0,null,{"$f":"'Profile angles'!P24","v":20},{"$f":"IF('Profile angles'!Q24<0,1000,IF(EB23<0,1000,'Profile angles'!Q24))","v":1000},{"$f":"IF('Profile angles'!R24<0,1000,IF(EC23<0,1000,'Profile angles'!R24))","v":1000},{"$f":"IF('Profile angles'!S24<0,1000,IF(ED23<0,1000,'Profile angles'!S24))","v":1000},{"$f":"IF('Profile angles'!T24<0,1000,IF(EE23<0,1000,'Profile angles'!T24))","v":1000},{"$f":"IF('Profile angles'!U24<0,1000,IF(EF23<0,1000,'Profile angles'!U24))","v":1000},{"$f":"IF('Profile angles'!V24<0,1000,IF(EG23<0,1000,'Profile angles'!V24))","v":1000},{"$f":"IF('Profile angles'!W24<0,1000,IF(EH23<0,1000,'Profile angles'!W24))","v":1000},{"$f":"IF('Profile angles'!X24<0,1000,IF(EI23<0,1000,'Profile angles'!X24))","v":1000},{"$f":"IF('Profile angles'!Y24<0,1000,IF(EJ23<0,1000,'Profile angles'!Y24))","v":1000},{"$f":"IF('Profile angles'!Z24<0,1000,IF(EK23<0,1000,'Profile angles'!Z24))","v":1000},{"$f":"IF('Profile angles'!AA24<0,1000,IF(EL23<0,1000,'Profile angles'!AA24))","v":1000},{"$f":"IF('Profile angles'!AB24<0,1000,IF(EM23<0,1000,'Profile angles'!AB24))","v":1000},null,{"$f":"'Profile angles'!P53","v":20},{"$f":"IF('Profile angles'!Q53<0,1000,IF(EB23<0,1000,'Profile angles'!Q53))","v":1000},{"$f":"IF('Profile angles'!R53<0,1000,IF(EC23<0,1000,'Profile angles'!R53))","v":1000},{"$f":"IF('Profile angles'!S53<0,1000,IF(ED23<0,1000,'Profile angles'!S53))","v":1000},{"$f":"IF('Profile angles'!T53<0,1000,IF(EE23<0,1000,'Profile angles'!T53))","v":1000},{"$f":"IF('Profile angles'!U53<0,1000,IF(EF23<0,1000,'Profile angles'!U53))","v":1000},{"$f":"IF('Profile angles'!V53<0,1000,IF(EG23<0,1000,'Profile angles'!V53))","v":1000},{"$f":"IF('Profile angles'!W53<0,1000,IF(EH23<0,1000,'Profile angles'!W53))","v":1000},{"$f":"IF('Profile angles'!X53<0,1000,IF(EI23<0,1000,'Profile angles'!X53))","v":1000},{"$f":"IF('Profile angles'!Y53<0,1000,IF(EJ23<0,1000,'Profile angles'!Y53))","v":1000},{"$f":"IF('Profile angles'!Z53<0,1000,IF(EK23<0,1000,'Profile angles'!Z53))","v":1000},{"$f":"IF('Profile angles'!AA53<0,1000,IF(EL23<0,1000,'Profile angles'!AA53))","v":1000},{"$f":"IF('Profile angles'!AB53<0,1000,IF(EM23<0,1000,'Profile angles'!AB53))","v":1000},null,20,{"$f":"EB23","v":-30.589239677830651},-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,-12.902247652391463,-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299,null,20,{"$f":"EP23","v":-30.589239677830651},-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,-12.902247652391463,-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299]
[null,21,{"$f":"('Solar Azimuth'!C23-('Input Data'!$F$9-90))","v":4.353027976725528},{"$f":"('Solar Azimuth'!D23-('Input Data'!$F$9-90))","v":-7.1994155824302624},{"$f":"('Solar Azimuth'!E23-('Input Data'!$F$9-90))","v":-20.185646390817951},{"$f":"('Solar Azimuth'!F23-('Input Data'!$F$9-90))","v":-33.437801605317716},{"$f":"('Solar Azimuth'!G23-('Input Data'!$F$9-90))","v":-41.07652361833965},{"$f":"('Solar Azimuth'!H23-('Input Data'!$F$9-90))","v":-42.785358202845003},{"$f":"('Solar Azimuth'!I23-('Input Data'!$F$9-90))","v":-39.576345811315946},{"$f":"('Solar Azimuth'!J23-('Input Data'!$F$9-90))","v":-32.989142910631173},{"$f":"('Solar Azimuth'!K23-('Input Data'!$F$9-90))","v":-22.743737963249302},{"$f":"('Solar Azimuth'!L23-('Input Data'!$F$9-90))","v":-11.151822128155999},{"$f":"('Solar Azimuth'!M23-('Input Data'!$F$9-90))","v":2.0805334741474439},{"$f":"('Solar Azimuth'!N23-('Input Data'!$F$9-90))","v":8.3166558679225773},null,21,{"$f":"('Solar Azimuth'!C23-('Input Data'!$F$9-180))","v":94.353027976725528},{"$f":"('Solar Azimuth'!D23-('Input Data'!$F$9-180))","v":82.800584417569738},{"$f":"('Solar Azimuth'!E23-('Input Data'!$F$9-180))","v":69.814353609182049},{"$f":"('Solar Azimuth'!F23-('Input Data'!$F$9-180))","v":56.562198394682284},{"$f":"('Solar Azimuth'!G23-('Input Data'!$F$9-180))","v":48.92347638166035},{"$f":"('Solar Azimuth'!H23-('Input Data'!$F$9-180))","v":47.214641797154997},{"$f":"('Solar Azimuth'!I23-('Input Data'!$F$9-180))","v":50.423654188684054},{"$f":"('Solar Azimuth'!J23-('Input Data'!$F$9-180))","v":57.010857089368827},{"$f":"('Solar Azimuth'!K23-('Input Data'!$F$9-180))","v":67.256262036750698},{"$f":"('Solar Azimuth'!L23-('Input Data'!$F$9-180))","v":78.848177871844001},{"$f":"('Solar Azimuth'!M23-('Input Data'!$F$9-180))","v":92.080533474147444},{"$f":"('Solar Azimuth'!N23-('Input Data'!$F$9-180))","v":98.316655867922577},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,0.15224237600470544,0.2526380313310983,0.73528791168463403,1.3206510721162312,1.7432686087073683,1.8510711744896451,1.6531535970466797,1.2982764398021058,0.83841259239175447,0.39426329565524415,7.265625564143692E-2,0.29236224438348235,null,21,26.273893675151058,15.832928949472947,5.4400459145799278,3.0288091112441524,2.2945402561719939,2.1609109661074117,2.4196178789108926,3.0810079250993057,4.7709207093241872,10.1455043978979,55.053759166178963,13.681657179896751,null,21,0.96193940599882366,0.93684049216722542,0.81617802207884149,0.66983723197094225,0.56418284782315786,0.53723220637758873,0.58671160073833006,0.67543089004947354,0.79039685190206144,0.90143417608618892,0.98183593608964082,0.92690943890412947,null,21,0,0,0,0.2427977221889619,0.42636493595700153,0.45977225847314707,0.39509553027227684,0.22974801872517359,0,0,0,0,null,{"$f":"'Profile angles'!P25","v":21},{"$f":"IF('Profile angles'!Q25<0,1000,IF(EB24<0,1000,'Profile angles'!Q25))","v":1000},{"$f":"IF('Profile angles'!R25<0,1000,IF(EC24<0,1000,'Profile angles'!R25))","v":1000},{"$f":"IF('Profile angles'!S25<0,1000,IF(ED24<0,1000,'Profile angles'!S25))","v":1000},{"$f":"IF('Profile angles'!T25<0,1000,IF(EE24<0,1000,'Profile angles'!T25))","v":1000},{"$f":"IF('Profile angles'!U25<0,1000,IF(EF24<0,1000,'Profile angles'!U25))","v":1000},{"$f":"IF('Profile angles'!V25<0,1000,IF(EG24<0,1000,'Profile angles'!V25))","v":1000},{"$f":"IF('Profile angles'!W25<0,1000,IF(EH24<0,1000,'Profile angles'!W25))","v":1000},{"$f":"IF('Profile angles'!X25<0,1000,IF(EI24<0,1000,'Profile angles'!X25))","v":1000},{"$f":"IF('Profile angles'!Y25<0,1000,IF(EJ24<0,1000,'Profile angles'!Y25))","v":1000},{"$f":"IF('Profile angles'!Z25<0,1000,IF(EK24<0,1000,'Profile angles'!Z25))","v":1000},{"$f":"IF('Profile angles'!AA25<0,1000,IF(EL24<0,1000,'Profile angles'!AA25))","v":1000},{"$f":"IF('Profile angles'!AB25<0,1000,IF(EM24<0,1000,'Profile angles'!AB25))","v":1000},null,{"$f":"'Profile angles'!P54","v":21},{"$f":"IF('Profile angles'!Q54<0,1000,IF(EB24<0,1000,'Profile angles'!Q54))","v":1000},{"$f":"IF('Profile angles'!R54<0,1000,IF(EC24<0,1000,'Profile angles'!R54))","v":1000},{"$f":"IF('Profile angles'!S54<0,1000,IF(ED24<0,1000,'Profile angles'!S54))","v":1000},{"$f":"IF('Profile angles'!T54<0,1000,IF(EE24<0,1000,'Profile angles'!T54))","v":1000},{"$f":"IF('Profile angles'!U54<0,1000,IF(EF24<0,1000,'Profile angles'!U54))","v":1000},{"$f":"IF('Profile angles'!V54<0,1000,IF(EG24<0,1000,'Profile angles'!V54))","v":1000},{"$f":"IF('Profile angles'!W54<0,1000,IF(EH24<0,1000,'Profile angles'!W54))","v":1000},{"$f":"IF('Profile angles'!X54<0,1000,IF(EI24<0,1000,'Profile angles'!X54))","v":1000},{"$f":"IF('Profile angles'!Y54<0,1000,IF(EJ24<0,1000,'Profile angles'!Y54))","v":1000},{"$f":"IF('Profile angles'!Z54<0,1000,IF(EK24<0,1000,'Profile angles'!Z54))","v":1000},{"$f":"IF('Profile angles'!AA54<0,1000,IF(EL24<0,1000,'Profile angles'!AA54))","v":1000},{"$f":"IF('Profile angles'!AB54<0,1000,IF(EM24<0,1000,'Profile angles'!AB54))","v":1000},null,21,{"$f":"EB24","v":-44.11375465474292},-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762,null,21,{"$f":"EP24","v":-44.11375465474292},-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762]
[null,22,{"$f":"('Solar Azimuth'!C24-('Input Data'!$F$9-90))","v":-1.5294531692688622},{"$f":"('Solar Azimuth'!D24-('Input Data'!$F$9-90))","v":-16.517926475137585},{"$f":"('Solar Azimuth'!E24-('Input Data'!$F$9-90))","v":-32.110467294428858},{"$f":"('Solar Azimuth'!F24-('Input Data'!$F$9-90))","v":-46.342767114087906},{"$f":"('Solar Azimuth'!G24-('Input Data'!$F$9-90))","v":-53.469017215916779},{"$f":"('Solar Azimuth'!H24-('Input Data'!$F$9-90))","v":-54.581901944803064},{"$f":"('Solar Azimuth'!I24-('Input Data'!$F$9-90))","v":-51.41793606781556},{"$f":"('Solar Azimuth'!J24-('Input Data'!$F$9-90))","v":-45.638295063812194},{"$f":"('Solar Azimuth'!K24-('Input Data'!$F$9-90))","v":-35.996477230850189},{"$f":"('Solar Azimuth'!L24-('Input Data'!$F$9-90))","v":-22.86261366161574},{"$f":"('Solar Azimuth'!M24-('Input Data'!$F$9-90))","v":-4.6895142788941655},{"$f":"('Solar Azimuth'!N24-('Input Data'!$F$9-90))","v":4.1027929342693028},null,22,{"$f":"('Solar Azimuth'!C24-('Input Data'!$F$9-180))","v":88.470546830731138},{"$f":"('Solar Azimuth'!D24-('Input Data'!$F$9-180))","v":73.482073524862415},{"$f":"('Solar Azimuth'!E24-('Input Data'!$F$9-180))","v":57.889532705571142},{"$f":"('Solar Azimuth'!F24-('Input Data'!$F$9-180))","v":43.657232885912094},{"$f":"('Solar Azimuth'!G24-('Input Data'!$F$9-180))","v":36.530982784083221},{"$f":"('Solar Azimuth'!H24-('Input Data'!$F$9-180))","v":35.418098055196936},{"$f":"('Solar Azimuth'!I24-('Input Data'!$F$9-180))","v":38.58206393218444},{"$f":"('Solar Azimuth'!J24-('Input Data'!$F$9-180))","v":44.361704936187806},{"$f":"('Solar Azimuth'!K24-('Input Data'!$F$9-180))","v":54.003522769149811},{"$f":"('Solar Azimuth'!L24-('Input Data'!$F$9-180))","v":67.13738633838426},{"$f":"('Solar Azimuth'!M24-('Input Data'!$F$9-180))","v":85.310485721105835},{"$f":"('Solar Azimuth'!N24-('Input Data'!$F$9-180))","v":94.102792934269303},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,5.3400671613115326E-2,0.59310771006954255,1.2551068482009575,2.096010480421671,2.6997904092120111,2.8123916208152386,2.50696590302748,2.045065309521128,1.4528971862599469,0.84329560685835037,0.16406144229602443,0.14345977565397655,null,22,74.905424953823825,6.7441375859555013,3.1869796629135689,1.9083874042439368,1.4815964922134386,1.4222770294133171,1.595554209640224,1.9559277551564545,2.7531197925276558,4.7432951950286704,24.381109564931144,27.882380142904708,null,22,0.98664983209672119,0.85172307248261436,0.68622328794976062,0.47599737989458224,0.32505239769699723,0.29690209479619034,0.37325852424313,0.48873367261971801,0.63677570343501322,0.78917609828541235,0.95898463942599388,0.96413505608650585,null,22,0,0,0.20325508427160777,0.52290314893901579,0.62960087694664035,0.64443074264667066,0.60111144758994395,0.51101806121088633,0.31172005186808605,0,0,0,null,{"$f":"'Profile angles'!P26","v":22},{"$f":"IF('Profile angles'!Q26<0,1000,IF(EB25<0,1000,'Profile angles'!Q26))","v":1000},{"$f":"IF('Profile angles'!R26<0,1000,IF(EC25<0,1000,'Profile angles'!R26))","v":1000},{"$f":"IF('Profile angles'!S26<0,1000,IF(ED25<0,1000,'Profile angles'!S26))","v":1000},{"$f":"IF('Profile angles'!T26<0,1000,IF(EE25<0,1000,'Profile angles'!T26))","v":1000},{"$f":"IF('Profile angles'!U26<0,1000,IF(EF25<0,1000,'Profile angles'!U26))","v":1000},{"$f":"IF('Profile angles'!V26<0,1000,IF(EG25<0,1000,'Profile angles'!V26))","v":1000},{"$f":"IF('Profile angles'!W26<0,1000,IF(EH25<0,1000,'Profile angles'!W26))","v":1000},{"$f":"IF('Profile angles'!X26<0,1000,IF(EI25<0,1000,'Profile angles'!X26))","v":1000},{"$f":"IF('Profile angles'!Y26<0,1000,IF(EJ25<0,1000,'Profile angles'!Y26))","v":1000},{"$f":"IF('Profile angles'!Z26<0,1000,IF(EK25<0,1000,'Profile angles'!Z26))","v":1000},{"$f":"IF('Profile angles'!AA26<0,1000,IF(EL25<0,1000,'Profile angles'!AA26))","v":1000},{"$f":"IF('Profile angles'!AB26<0,1000,IF(EM25<0,1000,'Profile angles'!AB26))","v":1000},null,{"$f":"'Profile angles'!P55","v":22},{"$f":"IF('Profile angles'!Q55<0,1000,IF(EB25<0,1000,'Profile angles'!Q55))","v":1000},{"$f":"IF('Profile angles'!R55<0,1000,IF(EC25<0,1000,'Profile angles'!R55))","v":1000},{"$f":"IF('Profile angles'!S55<0,1000,IF(ED25<0,1000,'Profile angles'!S55))","v":1000},{"$f":"IF('Profile angles'!T55<0,1000,IF(EE25<0,1000,'Profile angles'!T55))","v":1000},{"$f":"IF('Profile angles'!U55<0,1000,IF(EF25<0,1000,'Profile angles'!U55))","v":1000},{"$f":"IF('Profile angles'!V55<0,1000,IF(EG25<0,1000,'Profile angles'!V55))","v":1000},{"$f":"IF('Profile angles'!W55<0,1000,IF(EH25<0,1000,'Profile angles'!W55))","v":1000},{"$f":"IF('Profile angles'!X55<0,1000,IF(EI25<0,1000,'Profile angles'!X55))","v":1000},{"$f":"IF('Profile angles'!Y55<0,1000,IF(EJ25<0,1000,'Profile angles'!Y55))","v":1000},{"$f":"IF('Profile angles'!Z55<0,1000,IF(EK25<0,1000,'Profile angles'!Z55))","v":1000},{"$f":"IF('Profile angles'!AA55<0,1000,IF(EL25<0,1000,'Profile angles'!AA55))","v":1000},{"$f":"IF('Profile angles'!AB55<0,1000,IF(EM25<0,1000,'Profile angles'!AB55))","v":1000},null,22,{"$f":"EB25","v":-57.730536859646747},-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132,null,22,{"$f":"EP25","v":-57.730536859646747},-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132]
[null,23,{"$f":"('Solar Azimuth'!C25-('Input Data'!$F$9-90))","v":-10.945348008769216},{"$f":"('Solar Azimuth'!D25-('Input Data'!$F$9-90))","v":-32.665388823399354},{"$f":"('Solar Azimuth'!E25-('Input Data'!$F$9-90))","v":-51.058935920151328},{"$f":"('Solar Azimuth'!F25-('Input Data'!$F$9-90))","v":-64.362976027003612},{"$f":"('Solar Azimuth'!G25-('Input Data'!$F$9-90))","v":-69.563069810063098},{"$f":"('Solar Azimuth'!H25-('Input Data'!$F$9-90))","v":-69.629861866663276},{"$f":"('Solar Azimuth'!I25-('Input Data'!$F$9-90))","v":-66.868968666705229},{"$f":"('Solar Azimuth'!J25-('Input Data'!$F$9-90))","v":-63.281586513777881},{"$f":"('Solar Azimuth'!K25-('Input Data'!$F$9-90))","v":-57.497611691551583},{"$f":"('Solar Azimuth'!L25-('Input Data'!$F$9-90))","v":-46.469388588491682},{"$f":"('Solar Azimuth'!M25-('Input Data'!$F$9-90))","v":-18.626157994443233},{"$f":"('Solar Azimuth'!N25-('Input Data'!$F$9-90))","v":-1.3834198698309024},null,23,{"$f":"('Solar Azimuth'!C25-('Input Data'!$F$9-180))","v":79.054651991230784},{"$f":"('Solar Azimuth'!D25-('Input Data'!$F$9-180))","v":57.334611176600646},{"$f":"('Solar Azimuth'!E25-('Input Data'!$F$9-180))","v":38.941064079848672},{"$f":"('Solar Azimuth'!F25-('Input Data'!$F$9-180))","v":25.637023972996388},{"$f":"('Solar Azimuth'!G25-('Input Data'!$F$9-180))","v":20.436930189936902},{"$f":"('Solar Azimuth'!H25-('Input Data'!$F$9-180))","v":20.370138133336724},{"$f":"('Solar Azimuth'!I25-('Input Data'!$F$9-180))","v":23.131031333294771},{"$f":"('Solar Azimuth'!J25-('Input Data'!$F$9-180))","v":26.718413486222119},{"$f":"('Solar Azimuth'!K25-('Input Data'!$F$9-180))","v":32.502388308448417},{"$f":"('Solar Azimuth'!L25-('Input Data'!$F$9-180))","v":43.530611411508318},{"$f":"('Solar Azimuth'!M25-('Input Data'!$F$9-180))","v":71.373842005556767},{"$f":"('Solar Azimuth'!N25-('Input Data'!$F$9-180))","v":88.616580130169098},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,0.38678118978700338,1.2822717419304539,2.474995422476634,4.167409034479415,5.3672465726824319,5.3864290251139968,4.6819062798557214,3.9733756933370392,3.1390823947123119,2.10530641663218,0.67409101893590262,4.8299849842381101E-2,null,23,10.341764557378712,3.1194635810799509,1.616164605265149,0.95982898892469126,0.74526108421377923,0.74260701874101875,0.8543528556328267,1.0067006768847979,1.2742577279073268,1.8999609597916518,5.9339167673740345,82.815992452427196,null,23,0.90330470255324913,0.67943206451738658,0.38125114438084151,0,0,0,0,6.656076665740196E-3,0.21522940132192203,0.473673395841955,0.8314772452660244,0.98792503753940475,null,23,0,0.22013410473001227,0.59595884868371274,0.76004275276882716,0.81368472894655519,0.81434824531474526,0.7864117860917933,0.74832483077880052,0.68143556802316829,0.5250097600520871,0,0,null,{"$f":"'Profile angles'!P27","v":23},{"$f":"IF('Profile angles'!Q27<0,1000,IF(EB26<0,1000,'Profile angles'!Q27))","v":1000},{"$f":"IF('Profile angles'!R27<0,1000,IF(EC26<0,1000,'Profile angles'!R27))","v":1000},{"$f":"IF('Profile angles'!S27<0,1000,IF(ED26<0,1000,'Profile angles'!S27))","v":1000},{"$f":"IF('Profile angles'!T27<0,1000,IF(EE26<0,1000,'Profile angles'!T27))","v":1000},{"$f":"IF('Profile angles'!U27<0,1000,IF(EF26<0,1000,'Profile angles'!U27))","v":1000},{"$f":"IF('Profile angles'!V27<0,1000,IF(EG26<0,1000,'Profile angles'!V27))","v":1000},{"$f":"IF('Profile angles'!W27<0,1000,IF(EH26<0,1000,'Profile angles'!W27))","v":1000},{"$f":"IF('Profile angles'!X27<0,1000,IF(EI26<0,1000,'Profile angles'!X27))","v":1000},{"$f":"IF('Profile angles'!Y27<0,1000,IF(EJ26<0,1000,'Profile angles'!Y27))","v":1000},{"$f":"IF('Profile angles'!Z27<0,1000,IF(EK26<0,1000,'Profile angles'!Z27))","v":1000},{"$f":"IF('Profile angles'!AA27<0,1000,IF(EL26<0,1000,'Profile angles'!AA27))","v":1000},{"$f":"IF('Profile angles'!AB27<0,1000,IF(EM26<0,1000,'Profile angles'!AB27))","v":1000},null,{"$f":"'Profile angles'!P56","v":23},{"$f":"IF('Profile angles'!Q56<0,1000,IF(EB26<0,1000,'Profile angles'!Q56))","v":1000},{"$f":"IF('Profile angles'!R56<0,1000,IF(EC26<0,1000,'Profile angles'!R56))","v":1000},{"$f":"IF('Profile angles'!S56<0,1000,IF(ED26<0,1000,'Profile angles'!S56))","v":1000},{"$f":"IF('Profile angles'!T56<0,1000,IF(EE26<0,1000,'Profile angles'!T56))","v":1000},{"$f":"IF('Profile angles'!U56<0,1000,IF(EF26<0,1000,'Profile angles'!U56))","v":1000},{"$f":"IF('Profile angles'!V56<0,1000,IF(EG26<0,1000,'Profile angles'!V56))","v":1000},{"$f":"IF('Profile angles'!W56<0,1000,IF(EH26<0,1000,'Profile angles'!W56))","v":1000},{"$f":"IF('Profile angles'!X56<0,1000,IF(EI26<0,1000,'Profile angles'!X56))","v":1000},{"$f":"IF('Profile angles'!Y56<0,1000,IF(EJ26<0,1000,'Profile angles'!Y56))","v":1000},{"$f":"IF('Profile angles'!Z56<0,1000,IF(EK26<0,1000,'Profile angles'!Z56))","v":1000},{"$f":"IF('Profile angles'!AA56<0,1000,IF(EL26<0,1000,'Profile angles'!AA56))","v":1000},{"$f":"IF('Profile angles'!AB56<0,1000,IF(EM26<0,1000,'Profile angles'!AB56))","v":1000},null,23,{"$f":"EB26","v":-71.276413671366612},-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272,null,23,{"$f":"EP26","v":-71.276413671366612},-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272]
[null,24,{"$f":"('Solar Azimuth'!C26-('Input Data'!$F$9-90))","v":-47.646886568528117},{"$f":"('Solar Azimuth'!D26-('Input Data'!$F$9-90))","v":-69.573834162038821},{"$f":"('Solar Azimuth'!E26-('Input Data'!$F$9-90))","v":-81.300773847527211},{"$f":"('Solar Azimuth'!F26-('Input Data'!$F$9-90))","v":-87.525798695816803},{"$f":"('Solar Azimuth'!G26-('Input Data'!$F$9-90))","v":-88.729059597475214},{"$f":"('Solar Azimuth'!H26-('Input Data'!$F$9-90))","v":-87.374107396965314},{"$f":"('Solar Azimuth'!I26-('Input Data'!$F$9-90))","v":-85.606821130538862},{"$f":"('Solar Azimuth'!J26-('Input Data'!$F$9-90))","v":-86.114489910663593},{"$f":"('Solar Azimuth'!K26-('Input Data'!$F$9-90))","v":-89.780632878936188},{"$f":"('Solar Azimuth'!L26-('Input Data'!$F$9-90))","v":-81.657828897458955},{"$f":"('Solar Azimuth'!M26-('Input Data'!$F$9-90))","v":-71.867642607529234},{"$f":"('Solar Azimuth'!N26-('Input Data'!$F$9-90))","v":-44.419458300077252},null,24,{"$f":"('Solar Azimuth'!C26-('Input Data'!$F$9-180))","v":42.353113431471883},{"$f":"('Solar Azimuth'!D26-('Input Data'!$F$9-180))","v":20.426165837961179},{"$f":"('Solar Azimuth'!E26-('Input Data'!$F$9-180))","v":8.6992261524727894},{"$f":"('Solar Azimuth'!F26-('Input Data'!$F$9-180))","v":2.4742013041831967},{"$f":"('Solar Azimuth'!G26-('Input Data'!$F$9-180))","v":1.2709404025247864},{"$f":"('Solar Azimuth'!H26-('Input Data'!$F$9-180))","v":2.6258926030346856},{"$f":"('Solar Azimuth'!I26-('Input Data'!$F$9-180))","v":4.3931788694611384},{"$f":"('Solar Azimuth'!J26-('Input Data'!$F$9-180))","v":3.8855100893364067},{"$f":"('Solar Azimuth'!K26-('Input Data'!$F$9-180))","v":0.21936712106381151},{"$f":"('Solar Azimuth'!L26-('Input Data'!$F$9-180))","v":8.3421711025410445},{"$f":"('Solar Azimuth'!M26-('Input Data'!$F$9-180))","v":18.132357392470766},{"$f":"('Solar Azimuth'!N26-('Input Data'!$F$9-180))","v":45.580541699922748},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,2.1938822423162123,5.3703299398878617,13.071239251418012,46.285773549133694,90.148022232326284,43.608530318103348,26.032835999148293,29.446800741319013,522.37089380483621,13.639216142221768,6.1073257646907972,1.9598757242104459,null,24,1.8232519151880093,0.74483319363493761,0.30601536113464295,8.6419642436220676E-2,4.4371467071027959E-2,9.1725173281968525E-2,0.15365210306440918,0.13583818612890242,7.6573944824242018E-3,0.29327198559582479,0.65495114459520132,2.0409457347666451,null,24,0.45152943942094692,0,0,0,0,0,0,0,0,0,0,0.51003106894738859,null,24,0.54418702120299767,0.81379170159126557,0.92349615971633925,0.97839508939094488,0.988907133232243,0.97706870667950785,0.96158697423389772,0.96604045346777445,0.99808565137939398,0.9266820036010438,0.8362622138511997,0.48976356630833873,null,{"$f":"'Profile angles'!P28","v":24},{"$f":"IF('Profile angles'!Q28<0,1000,IF(EB27<0,1000,'Profile angles'!Q28))","v":1000},{"$f":"IF('Profile angles'!R28<0,1000,IF(EC27<0,1000,'Profile angles'!R28))","v":1000},{"$f":"IF('Profile angles'!S28<0,1000,IF(ED27<0,1000,'Profile angles'!S28))","v":1000},{"$f":"IF('Profile angles'!T28<0,1000,IF(EE27<0,1000,'Profile angles'!T28))","v":1000},{"$f":"IF('Profile angles'!U28<0,1000,IF(EF27<0,1000,'Profile angles'!U28))","v":1000},{"$f":"IF('Profile angles'!V28<0,1000,IF(EG27<0,1000,'Profile angles'!V28))","v":1000},{"$f":"IF('Profile angles'!W28<0,1000,IF(EH27<0,1000,'Profile angles'!W28))","v":1000},{"$f":"IF('Profile angles'!X28<0,1000,IF(EI27<0,1000,'Profile angles'!X28))","v":1000},{"$f":"IF('Profile angles'!Y28<0,1000,IF(EJ27<0,1000,'Profile angles'!Y28))","v":1000},{"$f":"IF('Profile angles'!Z28<0,1000,IF(EK27<0,1000,'Profile angles'!Z28))","v":1000},{"$f":"IF('Profile angles'!AA28<0,1000,IF(EL27<0,1000,'Profile angles'!AA28))","v":1000},{"$f":"IF('Profile angles'!AB28<0,1000,IF(EM27<0,1000,'Profile angles'!AB28))","v":1000},null,{"$f":"'Profile angles'!P57","v":24},{"$f":"IF('Profile angles'!Q57<0,1000,IF(EB27<0,1000,'Profile angles'!Q57))","v":1000},{"$f":"IF('Profile angles'!R57<0,1000,IF(EC27<0,1000,'Profile angles'!R57))","v":1000},{"$f":"IF('Profile angles'!S57<0,1000,IF(ED27<0,1000,'Profile angles'!S57))","v":1000},{"$f":"IF('Profile angles'!T57<0,1000,IF(EE27<0,1000,'Profile angles'!T57))","v":1000},{"$f":"IF('Profile angles'!U57<0,1000,IF(EF27<0,1000,'Profile angles'!U57))","v":1000},{"$f":"IF('Profile angles'!V57<0,1000,IF(EG27<0,1000,'Profile angles'!V57))","v":1000},{"$f":"IF('Profile angles'!W57<0,1000,IF(EH27<0,1000,'Profile angles'!W57))","v":1000},{"$f":"IF('Profile angles'!X57<0,1000,IF(EI27<0,1000,'Profile angles'!X57))","v":1000},{"$f":"IF('Profile angles'!Y57<0,1000,IF(EJ27<0,1000,'Profile angles'!Y57))","v":1000},{"$f":"IF('Profile angles'!Z57<0,1000,IF(EK27<0,1000,'Profile angles'!Z57))","v":1000},{"$f":"IF('Profile angles'!AA57<0,1000,IF(EL27<0,1000,'Profile angles'!AA57))","v":1000},{"$f":"IF('Profile angles'!AB57<0,1000,IF(EM27<0,1000,'Profile angles'!AB57))","v":1000},null,24,{"$f":"EB27","v":-83.596484892158756},-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205,null,24,{"$f":"EP27","v":-83.596484892158756},-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205]
[null,null,null,null,null,null,null,null,"Horizontal Cutoff",null,null,null,null,{"$f":"'Operative BP'!AH29","v":55.007979801441337},null,null,null,null,null,null,null,null,"Horizontal Cutoff",null,null,null,null,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Horizontal Cutoff",null,null,null,null,{"$f":"'Operative BP'!CA29","v":0},null,null,null,null,null,null,null,null,"Horizontal Cutoff",null,null,null,null,90]
[]
[null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"RADIANS(C58)","v":3.5678561370339965},4.1018494424418792,4.26486922064948,4.3402911517184304,4.3961374348077085,4.4413791643363991,4.4486628705592075,4.3646149030012671,4.1392994595710499,3.8016498532242493,3.3857051024485769,3.1926628641442365,null,1,{"$f":"RADIANS(Q58)","v":5.138652463828894},5.6726457692367758,5.8356655474443766,5.9110874785133278,5.966933761602605,6.0121754911312957,6.0194591973541041,5.9354112297961636,5.7100957863659474,5.3724461800191463,4.9565014292434739,4.7634591909391331]
[null,2,{"$f":"RADIANS(C59)","v":3.2542239041025716},3.6056646369912788,3.8425604311718562,4.00568884444262,4.106974862539527,4.1630454338740499,4.1506560192893414,4.0253255656070337,3.7663399287733426,3.4726049454814891,3.1925569765268498,3.08472445598025,null,2,{"$f":"RADIANS(Q59)","v":-1.4581650762821186},{"$f":"RADIANS(R59)","v":-1.1067243433934106},-0.8698285492128337,-0.70670013594206949,-0.6054141178451623,-0.54934354651063955,-0.56173296109534809,-0.68706341477765587,-0.94604905161134711,-1.239784034903201,-1.5198320038578401,-1.6276645244044396]
[null,3,{"$f":"RADIANS(C60)","v":3.125040573171586},3.3739574459675068,3.5850010693400622,3.7647206854401913,3.8829103946213466,3.9415225139244487,3.9171467649010419,3.7798349002825429,3.5362691328246401,3.2946776053595426,3.083753594039095,3.0096292002931544,null,3,-1.5873484072131034,{"$f":"RADIANS(R60)","v":-1.3384315344171833},-1.1273879110446279,-0.94766829494449834,-0.8294785857633431,-0.77086646646024115,-0.79524221548364793,-0.9325540801021468,-1.1761198475600498,-1.4177113750251469,-1.6286353863455947,-1.7027597800915355]
[null,4,{"$f":"RADIANS(C61)","v":3.030678340383389},3.2285642451858769,3.4129721534876136,3.5896927068714009,3.7127217960535792,3.7707629642818374,3.7397240595282533,3.6017548182046668,3.3774828247085593,3.1688446022990888,2.9943416602329309,2.9377418639888528,null,4,-1.6817106400013011,{"$f":"RADIANS(R61)","v":-1.483824735198813},-1.299416826897076,-1.1226962735132888,-0.99966718433111057,-0.94162601610285235,-0.97266492085643641,-1.1106341621800229,-1.3349061556761304,-1.5435443780856013,-1.718047320151759,-1.7746471163958366]
[null,5,{"$f":"RADIANS(C62)","v":2.9438044891823614},3.1145939526678657,3.2817688425204503,3.4544925763875427,3.580159212214777,3.6376608738629606,3.6022810076480396,3.4647585535055607,3.252387969738717,3.0615913078312547,2.9070411914862584,2.8612603882487768,null,5,-1.7685844912023283,{"$f":"RADIANS(R62)","v":-1.5977950277168242},-1.4306201378642396,-1.257896403997147,-1.1322297681699127,-1.0747281065217291,-1.1101079727366501,-1.2476304268791292,-1.4600010106459729,-1.650797672553435,-1.8053477888984313,-1.8511285921359126]
[null,6,{"$f":"RADIANS(C63)","v":2.8534124758804911},3.0100729062929026,3.16830341288733,3.3414121427956855,3.4721111700052059,3.5306278139411602,3.4912064813534358,3.3508134314094731,3.140924113793917,2.9568676790220705,2.8128028480204481,2.7748571460557629,null,6,-1.8589765045041988,{"$f":"RADIANS(R63)","v":-1.7023160740917871},-1.5440855674973597,-1.3709768375890041,-1.2402778103794843,-1.1817611664435292,-1.2211824990312539,-1.3615755489752166,-1.5714648665907729,-1.7555213013626196,-1.8995861323642416,-1.9375318343289269]
[null,7,{"$f":"RADIANS(C64)","v":2.7514642416379758},2.9020327604853668,3.0579739484148769,3.2379228408154255,3.3789425715652799,3.4410938341621766,3.3964854026005575,3.2472523471095363,3.0293820032418135,2.842941742564848,2.7035441869113956,2.6725940451483035,null,7,-1.9609247387467139,{"$f":"RADIANS(R64)","v":-1.8103562198993228},-1.6544150319698128,-1.4744661395692642,-1.3334464088194098,-1.2712951462225131,-1.3159035777841321,-1.4651366332751539,-1.6830069771428762,-1.8694472378198419,-2.008844793473294,-2.0397949352363867]
[null,8,{"$f":"RADIANS(C65)","v":2.6290626341143808},2.7786437952935414,2.9375703928702674,3.1326237951598626,3.2928036927362276,3.3627586983432809,3.3102235292281534,3.1427927927896739,2.9040177666149423,2.7068619430810608,2.56934174726466,2.5465293845936596,null,8,-2.0833263462703093,{"$f":"RADIANS(R65)","v":-1.9337451850911487},-1.7748185875144222,-1.5797651852248271,-1.4195852876484623,-1.3496302820414088,-1.4021654511565365,-1.5695961875950157,-1.8083712137697474,-2.0055270373036289,-2.1430472331200296,-2.16585959579103]
[null,9,{"$f":"RADIANS(C66)","v":2.4743314349638355},2.6246206425269683,2.7892866624267101,3.0098348548621772,3.2049077700503501,3.2903154238152243,3.2242405160490257,3.0223534888194901,2.7446395419202636,2.5300773304817117,2.3966714166408631,2.3857849250131689,null,9,-2.2380575454208547,{"$f":"RADIANS(R66)","v":-2.0877683378577214},-1.9231023179579796,-1.7025541255225125,-1.5074812103343393,-1.4220735565694651,-1.4881484643356642,-1.6900354915651998,-1.9677494384644261,-2.182311649902978,-2.3157175637438265,-2.3266040553715208]
[null,10,{"$f":"RADIANS(C67)","v":2.2715117149530366},2.4167805984064219,2.5811592749480545,2.8361190900694075,3.0983257450741144,3.2170905128198126,3.124405258200472,2.8545262307109938,2.5133356067922863,2.2845804238382104,2.168812917493582,2.1772059277948954,null,10,-2.4408772654316535,{"$f":"RADIANS(R67)","v":-2.2956083819782678},-2.1312297054366351,-1.8762698903152821,-1.6140632353105755,-1.4952984675648771,-1.5879837221842179,-1.8578627496736959,-2.1990533735924034,-2.4278085565464798,-2.5435760628911077,-2.5351830525897938]
[null,11,{"$f":"RADIANS(C68)","v":2.0051228427179941},2.1229443647063793,2.2504461092183519,2.5069948278707361,2.9070427997559198,3.1238256675874974,2.9623854927708169,2.5424601012975514,2.1380700175390333,1.9397017456172936,1.8746455376853886,1.9117415191764662,null,11,-2.7072661376666955,{"$f":"RADIANS(R68)","v":-2.5894446156783104},-2.4619428711663378,-2.2053941525139535,-1.8053461806287698,-1.5885633127971928,-1.7500034876138733,-2.1699288790871383,-2.5743189628456564,-2.7726872347673961,-2.8377434426993013,-2.8006474612082233]
[null,12,{"$f":"RADIANS(C69)","v":1.6775903873538114},1.7258987395282124,1.7226264655311456,1.6866075459932068,1.7726231620235977,2.5786868666308145,2.2145675937902318,1.7553703496410313,1.5746250053281106,1.631919456960889,1.609734653718315,1.6005244209872247,null,12,-3.0347985930308781,{"$f":"RADIANS(R69)","v":-2.9864902408564773},-2.9897625148535441,-3.0257814343914826,-2.9397658183610922,-2.1337021137538752,-2.4978213865944578,-2.9570186307436583,-3.1377639750565796,-3.0804695234238006,-3.1026543266663746,-3.111864559397465]
[null,13,{"$f":"RADIANS(C70)","v":1.3311148590412119},1.2878011367904143,1.123276567059688,0.74431993812897757,0.27826728797358868,5.9595207931875366E-2,0.33129340151721459,0.77284207429392426,0.99770680598125416,1.0961178255109656,1.1960628124840591,1.2846656264794616,null,13,2.9019111858361084,{"$f":"RADIANS(R70)","v":2.8585974635853106},2.6940728938545844,2.3151162649238746,1.8490636147684854,1.6303915347267719,1.9020897283121112,2.3436384010888207,2.5685031327761507,2.6669141523058624,2.7668591392789557,2.8554619532743581]
[null,14,{"$f":"RADIANS(C71)","v":1.0247539137095028},0.91990711039179107,0.70096777758206219,0.35309520497525965,6.0201645624323126E-2,-5.2747700646144209E-2,7.5042483944111948E-2,0.36190463931365185,0.62474727518354878,0.78054550215875995,0.91655627944504048,1.0090106596366628,null,14,2.5955502405043993,{"$f":"RADIANS(R71)","v":2.4907034371866876},2.2717641043769587,1.9238915317701561,1.6309979724192196,1.5180486261487525,1.6458388107390085,1.9327009661085484,2.1955436019784451,2.3513418289536565,2.4873526062399369,2.5798069864315591]
[null,15,{"$f":"RADIANS(C72)","v":0.78437679728358944},0.65524845016993283,0.44340841575026824,0.16089190932870823,-5.1294285571466328E-2,-0.12837716171536995,-4.1372706652789554E-2,0.16499466514870098,0.39467647923484622,0.55732299426199194,0.70238762974833058,0.7902896457596551,null,15,2.3551731240784859,{"$f":"RADIANS(R72)","v":2.2260447769648293},2.0142047425451648,1.7316882361236048,1.5195020412234304,1.4424191650795266,1.529423620142107,1.7357909919435976,1.9654728060297428,2.1281193210568885,2.2731839565432268,2.3610859725545517]
[null,16,{"$f":"RADIANS(C73)","v":0.60231928003768342},0.466546784205704,0.27137949989782062,3.1581327144166761E-2,-0.14030192959210733,-0.20019390109683355,-0.13097207585882609,3.4367772894221299E-2,0.23589017111876637,0.39410568588384243,0.53964592454586491,0.62172929123486753,null,16,2.1731156068325799,{"$f":"RADIANS(R73)","v":2.0373431110006006},1.8421758266927173,1.6023776539390633,1.4304943972027893,1.3706024256980631,1.4398242509360706,1.6051640996891179,1.806686497913663,1.9649020126787391,2.1104422513407615,2.1925256180297641]
[null,17,{"$f":"RADIANS(C74)","v":0.46182674117029054},0.32366510346907168,0.14017618893065736,-7.5695110275239993E-2,-0.22611136731312065,-0.27631653293496938,-0.21595336370226212,-7.3139734099092996E-2,0.11079531614892403,0.26566151222068263,0.41200927917536512,0.4901804010831472,null,17,2.0326230679651869,{"$f":"RADIANS(R74)","v":1.8944614302639682},1.710972515725554,1.4951012165196567,1.344684959481776,1.2944797938599273,1.3548429630926344,1.4976565926958036,1.6815916429438207,1.8364578390155792,1.9828056059702617,2.0609767278780438]
[null,18,{"$f":"RADIANS(C75)","v":0.34858774114392405},0.20622500856965889,2.6710759297536635E-2,-0.17859270812007236,-0.31795780457082939,-0.36209419716461527,-0.30599297209456899,-0.17571285318466023,-6.6853979587661874E-4,0.15543312955301636,0.30684826840344553,0.38420257349499998,null,18,1.9193840679388205,{"$f":"RADIANS(R75)","v":1.7770213353645554},1.5975070860924332,1.3922036186748243,1.2528385222240672,1.2087021296302813,1.2648033547003277,1.3950834736102364,1.57012778699902,1.726229456347913,1.877644595198342,1.9549989002898966]
[null,19,{"$f":"RADIANS(C76)","v":0.25208852349953098},0.10043100716709291,-8.3618705174916472E-2,-0.28883338495250988,-0.42362481719381245,-0.46339702417246675,-0.40873280254042754,-0.28513171967077711,-0.11221065034798006,5.1240527219994968E-2,0.21482919867781625,0.29536414909866349,null,19,1.8228848502944275,{"$f":"RADIANS(R76)","v":1.6712273339619894},1.4871776216199801,1.2819629418423868,1.1471715096010842,1.1073993026224298,1.162063524254469,1.2856646071241196,1.4585856764469165,1.6220368540148915,1.7856255254727129,1.8661604758935602]
[null,20,{"$f":"RADIANS(C77)","v":0.16406329797713692},-5.3580397175020215E-3,-0.20402226071952581,-0.41838773851643613,-0.55240850200878278,-0.58803968124222006,-0.53301122555606995,-0.41318320627698268,-0.23757488697485082,-5.9149423556256568E-2,0.12795736142409281,0.21744800976999268,null,20,1.7348596247720336,{"$f":"RADIANS(R77)","v":1.5654382870773946},1.3667740660753707,1.1524085882784605,1.0183878247861138,0.9827566455526765,1.0377851012388266,1.1576131205179139,1.3332214398200457,1.5116469032386399,1.6987536882189893,1.7882443365648892]
[null,21,{"$f":"RADIANS(C78)","v":7.5974670625287552E-2},-0.1256535061327933,-0.35230599116308331,-0.58359973264143961,-0.71692058241324153,-0.74674537228480919,-0.69073754031532975,-0.57576916120145949,-0.3969531116695294,-0.19463601373308323,3.631215932182922E-2,0.14515302765055563,null,21,1.6467709974201841,{"$f":"RADIANS(R78)","v":1.4451428206621033},1.2184903356318133,0.98719659415345695,0.85387574438165503,0.82405095451008736,0.88005878647956681,0.99502716559343718,1.1738432151253673,1.3761603130618134,1.6071084861167257,1.7159493544454523]
[null,22,{"$f":"RADIANS(C79)","v":-2.6693993558803801E-2},-0.28829220259349214,-0.56043337864173903,-0.8088338706257846,-0.93321039822327956,-0.95263390093750977,-0.89741227896332787,-0.79653851386019836,-0.62825704679750671,-0.39902788400663136,-8.1847464485990812E-2,7.1607245230558628E-2,null,22,1.5441023332360928,{"$f":"RADIANS(R79)","v":1.2825041242014044},1.0103629481531575,0.76196245616911196,0.637585928571617,0.6181624258573869,0.67338404783156869,0.7742578129346982,0.94253927999738985,1.1717684427882653,1.4889488623089058,1.6424035720254553]
[null,23,{"$f":"RADIANS(C80)","v":-0.19103236052962799},-0.57011858641247526,-0.89114654437144125,-1.1233458480533918,-1.2141046059802676,-1.2152703472821191,-1.167083670646929,-1.104472040551064,-1.0035226360507614,-0.81104383225786025,-0.32508778399969807,-2.4145231666060616E-2,null,23,1.3797639662652685,{"$f":"RADIANS(R80)","v":1.0006777403824214},0.67964978242345542,0.44745047874150479,0.35669172081462902,0.35552597951277753,0.40371265614796764,0.46632428624383254,0.56727369074413514,0.75975249453703642,1.2457085427951986,1.5466510951288359]
[null,24,{"$f":"RADIANS(C81)","v":-0.83159504894507852},-1.2142924793640875,-1.4189661880586482,-1.5276133676797621,-1.5486142321742171,-1.5249658550681768,-1.4941208908937575,-1.5029813826165173,-1.5669676482617121,-1.4251979742908298,-1.254326989147948,-0.77526579928867145,null,24,0.73920127784981815,{"$f":"RADIANS(R81)","v":0.3565038474308091},0.15183013873624843,4.3182959115134534E-2,2.2182094620679573E-2,4.583047172671971E-2,7.6675435901139025E-2,6.7814944178379313E-2,3.8286785331845168E-3,0.14559835250406672,0.31646933764694851,0.7955305275062251]

{"sheet":"HVAC Dashboard","index":5,"n_rows":44,"n_cols":35,"rows_kept":44,"cut":false,"hidden":false,"merged":[[24,10,25,10],[1,1,1,24]]}
[]
[null,{"$f":"CONCATENATE(AE2,STAT!A2)","v":"     Laboratory Thermal Analysis ~  Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"     Laboratory Thermal Analysis ~ "]
[]
[null,null,"P","Skin Loads (Solar+ cond)",{"$f":"IF(C4=\"A\",(AC19*AD19+AC21*AD21+AC23*AD23+AC25*AD25)/1000,(AC19*AG19+AC21*AG21+AC23*AG23+AC25*AG25)/1000)","v":0.45969342121644979},"KBtu/h",{"$f":"E4/3.412","v":0.13472843529204273},{"$f":"G4*1000/$E$8","v":0.14969826143560303},null,null,"w/ft2","ACH"]
[]
[null,null,null,"Room Height",10,null,null,null,null,null,null,0,5,10,15,20,25,30,35,40]
[]
[null,null,null,"Room Area",{"$f":"'Operative BP'!P3*'Operative BP'!P6","v":900},null,null,null,null,null,null,{"$f":"(L6*$E$6*$E$8*0.018*$E$10)-($E$14*$E$8*3.412)-($H$12*250)","v":-5184.96},{"$f":"(M6*$E$6*$E$8*0.018*$E$10)-($E$14*$E$8*3.412)-($H$12*250)","v":11015.039999999997},{"$f":"(N6*$E$6*$E$8*0.018*$E$10)-($E$14*$E$8*3.412)-($H$12*250)","v":27215.039999999997},43415.040000000001,59615.039999999994,75815.039999999979,92015.039999999994,108215.03999999999,124415.03999999998]
[]
[null,null,null,"ΔT",20,null,null,null,null,null,null,{"$f":"(L8/3.412)/$E$8","v":-1.6884720593982023},{"$f":"(M8/3.412)/$E$8","v":3.5870261821023828},8.8625244236029683,14.138022665103557,19.413520906604138,24.689019148104723,29.964517389605312,35.240015631105898,40.515513872606476]
[]
[null,null,null,"Sq Ft/Person",165,null,null,{"$f":"ROUNDUP($E$8/$E$12,0)","v":6}]
[]
[null,null,null,"Lighting Power Density",{"$f":"(H14/10)","v":1.2},null,null,12]
[]
[]
[null,null,null,"Total Linear \nfeet of hoods","# of hoods","Operating Sash height","Face Velocity","Lab Exhaust",null,null,"Fumehood driven",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Orientations\n",null,null,"Average",null,null,"Peak"]
[null,null,null,8,{"$f":"IF(ISBLANK(E19),ROUNDUP(D18/6,0),E19)","v":2},18,60,{"$f":"IF(H19>H25,H19,H25)","v":900},null,null,"cfm"]
[null,null,null,{"$f":"E18*0.75","v":1.5},null,{"$f":"F18/12","v":1.5},null,{"$f":"(D18-D19)*F19*G18","v":585},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"North",false,{"$f":"IF(AB19,1,0)","v":0},{"$f":"'Operative BP'!BQ85/'Operative BP'!T9","v":2209.6447641509435},{"$f":"AD19/3.412","v":647.60983708996002},{"$f":"AE19/$E$8","v":0.71956648565551118},{"$f":"'Operative BP'!BQ34/'Operative BP'!T9","v":0},{"$f":"AG19/3.412","v":0},{"$f":"AH19/$E$8","v":0}]
[null,null,null,"Cooling Capacity of Air",{"$f":"E25*$E$6*$E$8*0.018*$E$10","v":19439.999999999996},"BTU/h"]
[null,null,null,"Internal Heat Gain",{"$f":"((E30+E14)*E8*3.412)+((E8/E12)*250)","v":17791.489784852813},"BTU/h",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"South",true,{"$f":"IF(AB21,1,0)","v":1},{"$f":"'Operative BP'!BC58/'Operative BP'!T9","v":1945.1771039161772},{"$f":"AD21/3.412","v":570.09879950649974},{"$f":"AE21/$E$8","v":0.63344311056277747},{"$f":"'Operative BP'!BC7/'Operative BP'!T9","v":459.69342121644979},{"$f":"AG21/3.412","v":134.72843529204272},{"$f":"AH21/$E$8","v":0.14969826143560303}]
[null,null,null,"Supplemental Cooling ",{"$f":"IF(E21>E20,(E21-E20)/1000,0)","v":0},"KBTU/h",{"$f":"E22/12","v":0}]
[null,null,null,"Reheat",{"$f":"IF(E20>E21,(E20-E21)/1000,0)","v":1.6485102151471838},"KBTU/h",{"$f":"E23/12","v":0.13737585126226531},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"East",false,{"$f":"IF(AB23,1,0)","v":0},{"$f":"'Operative BP'!BQ58/'Operative BP'!T9","v":2160.1100591743261},{"$f":"AD23/3.412","v":633.09204547899355},{"$f":"AE23/$E$8","v":0.70343560608777067},{"$f":"'Operative BP'!BQ7/'Operative BP'!T9","v":3826.0863600764724},{"$f":"AG23/3.412","v":1121.3617702451561},{"$f":"AH23/$E$8","v":1.2459575224946178}]
[]
[null,null,null,"Air Change",{"$f":"IF(H19>H25,(H19*60)/(E6*E8),F25/2)","v":6},12,null,{"$f":"F25/2*E8*E6/60","v":900},null,null,"Fumehood driven",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"West",false,{"$f":"IF(AB25,1,0)","v":0},{"$f":"'Operative BP'!BC85/'Operative BP'!T9","v":2780.5144498239301},{"$f":"AD25/3.412","v":814.92217169517301},{"$f":"AE25/$E$8","v":0.9054690796613033},{"$f":"'Operative BP'!BC34/'Operative BP'!T9","v":5622.3905501017762},{"$f":"AG25/3.412","v":1647.8284144495242},{"$f":"AH25/$E$8","v":1.8309204604994713}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(AD19:AD25)","v":9095.4463770653765}]
[]
[null,null,null,"Equipment Load (w/sf)",{"$f":"F28/2","v":4},8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,60,"N","A"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,80,"S","P"]
[null,null,null,"Equipment+Skin",{"$f":"E28+H4","v":4.1496982614356028},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,100,"E"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,null,"W"]
[null,null,null,"Lab Name","ACH","Equipmt \nW/SF","Orientation","Eqpmt \n+Skin","Average Skin Load","Peak Skin Load","Internal Gain BTU/h","Cooling","Ht Load",null,null,null,null,null,null,null,null,null,null,null,null,null,"Shades",null,null,null,null,0]
[null,null,"P",null,null,null,null,{"$f":"IF(C33=\"P\",F33+J33,F33+I33)","v":0},{"$f":"IF(G33=\"S\",$AF$21,IF(G33=\"N\",$AF$19,IF(G33=\"E\",$AF$23,IF(G33=\"W\",$AF$25,0))))","v":0},{"$f":"IF(G33=\"S\",$AI$21,IF(G33=\"N\",$AI$19,IF(G33=\"E\",$AI$23,IF(G33=\"W\",$AI$25,0))))","v":0},{"$f":"($H$12*250)+((H33+$E$14)*$E$8*3.412)","v":5184.96},{"$f":"E33*$E$6*$E$8*0.018*$E$10","v":0},{"$f":"K33-L33","v":5184.96}]
[null,null,"A",null,null,null,null,{"$f":"IF(C34=\"P\",F34+J34,F34+I34)","v":0},{"$f":"IF(G34=\"S\",$AF$21,IF(G34=\"N\",$AF$19,IF(G34=\"E\",$AF$23,IF(G34=\"W\",$AF$25,0))))","v":0},{"$f":"IF(G34=\"S\",$AI$21,IF(G34=\"N\",$AI$19,IF(G34=\"E\",$AI$23,IF(G34=\"W\",$AI$25,0))))","v":0},{"$f":"($H$12*250)+((H34+$E$14)*$E$8*3.412)","v":5184.96},{"$f":"E34*$E$6*$E$8*0.018*$E$10","v":0},{"$f":"K34-L34","v":5184.96},null,null,null,null,null,null,null,null,null,null,null,null,null,"South",true,{"$f":"IF(AB34,1,0)","v":1}]
[null,null,"P",null,null,null,null,0,0,0,5184.96,0,5184.96]
[null,null,"A",null,null,null,null,0,0,0,5184.96,0,5184.96,null,null,null,null,null,null,null,null,null,null,null,null,null,"East",true,{"$f":"IF(AB36,1,0)","v":1}]
[null,null,"P",null,null,null,null,0,0,0,5184.96,0,5184.96]
[null,null,"A",null,null,null,null,0,0,0,5184.96,0,5184.96,null,null,null,null,null,null,null,null,null,null,null,null,null,"West",true,{"$f":"IF(AB38,1,0)","v":1}]
[null,null,"P",null,null,null,null,0,0,0,5184.96,0,5184.96]
[null,null,"A",null,null,null,null,0,0,0,5184.96,0,5184.96]
[null,null,"P",null,null,null,null,0,0,0,{"$f":"($H$12*250)+((H41+$E$14)*$E$8*3.412)","v":5184.96},{"$f":"E41*$E$6*$E$8*0.018*$E$10","v":0},{"$f":"K41-L41","v":5184.96}]
[null,null,"A",null,null,null,null,0,0,0,5184.96,0,5184.96]
[null,null,"P",null,null,null,null,0,0,0,5184.96,0,5184.96]
[null,null,"A",null,null,null,null,0,0,0,5184.96,0,5184.96]

{"sheet":"Lab Data","index":6,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Lab Name","ACH","Equipment W/SF","Orientation"]
[null,"Lab 1 Day",6,6,"S"]
[null,"Lab 1 Setback",4,6,0]
[null,"Lab2 Day",6,6,"W"]
[null,"Lab2 Setback",4,4,0]
[null,"Lab3 Day",6,6,"E"]
[null,"Lab3 Setback",4,2,0]
[null,"Lab4 Day",15,5,"S"]
[null,"Lab4 Setback",8,5,0]
[null,"Lab5 Day",15,5,"W"]
[null,"Lab5 Setback",10,5,0]
[null,"Lab6 Day",15,5,"E"]
[null,"Lab6 Setback",15,2,0]

{"sheet":"Radiation","index":7,"n_rows":29,"n_cols":25,"rows_kept":29,"cut":false,"hidden":false,"merged":[[1,21,1,22],[1,23,1,24],[28,2,28,3],[1,1,1,3],[1,4,1,9],[1,10,1,13],[11,17,13,18],[2,17,4,18],[5,17,7,18],[8,17,10,18]]}
[]
[null,"Table 3",null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,"Solar Radiation\nBTU/ ft2",null,null,null,null,null,null,null,null,null,null,"June",null,"December"]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,"Very High - Strong Heat Source \nPossible Shading Needed",null,null,null,"eQUEST Weather File","Chhaya Data","eQUEST Weather File","Chhaya Data"]
[null,1,{"$f":"(3.412141/10.7639)*STAT!C398","v":0},{"$f":"(3.412141/10.7639)*STAT!D398","v":0},{"$f":"(3.412141/10.7639)*STAT!E398","v":0},{"$f":"(3.412141/10.7639)*STAT!F398","v":0},{"$f":"(3.412141/10.7639)*STAT!G398","v":0},{"$f":"(3.412141/10.7639)*STAT!H398","v":0},{"$f":"(3.412141/10.7639)*STAT!I398","v":0},{"$f":"(3.412141/10.7639)*STAT!J398","v":0},{"$f":"(3.412141/10.7639)*STAT!K398","v":0},{"$f":"(3.412141/10.7639)*STAT!L398","v":0},{"$f":"(3.412141/10.7639)*STAT!M398","v":0},{"$f":"(3.412141/10.7639)*STAT!N398","v":0},null,170,null,null,null,null,1,0,{"$f":"H4","v":0},0,{"$f":"N4","v":0}]
[null,2,{"$f":"(3.412141/10.7639)*STAT!C399","v":0},{"$f":"(3.412141/10.7639)*STAT!D399","v":0},{"$f":"(3.412141/10.7639)*STAT!E399","v":0},{"$f":"(3.412141/10.7639)*STAT!F399","v":0},{"$f":"(3.412141/10.7639)*STAT!G399","v":0},{"$f":"(3.412141/10.7639)*STAT!H399","v":0},{"$f":"(3.412141/10.7639)*STAT!I399","v":0},{"$f":"(3.412141/10.7639)*STAT!J399","v":0},{"$f":"(3.412141/10.7639)*STAT!K399","v":0},{"$f":"(3.412141/10.7639)*STAT!L399","v":0},{"$f":"(3.412141/10.7639)*STAT!M399","v":0},{"$f":"(3.412141/10.7639)*STAT!N399","v":0},null,null,null,null,null,null,2,0,{"$f":"H5","v":0},0,{"$f":"N5","v":0}]
[null,3,{"$f":"(3.412141/10.7639)*STAT!C400","v":0},{"$f":"(3.412141/10.7639)*STAT!D400","v":0},{"$f":"(3.412141/10.7639)*STAT!E400","v":0},{"$f":"(3.412141/10.7639)*STAT!F400","v":0},{"$f":"(3.412141/10.7639)*STAT!G400","v":0},{"$f":"(3.412141/10.7639)*STAT!H400","v":0},{"$f":"(3.412141/10.7639)*STAT!I400","v":0},{"$f":"(3.412141/10.7639)*STAT!J400","v":0},{"$f":"(3.412141/10.7639)*STAT!K400","v":0},{"$f":"(3.412141/10.7639)*STAT!L400","v":0},{"$f":"(3.412141/10.7639)*STAT!M400","v":0},{"$f":"(3.412141/10.7639)*STAT!N400","v":0},null,null,null,"Medium - Good Strong \nSource for Passive Solar",null,null,3,0,0,0,0]
[null,4,{"$f":"(3.412141/10.7639)*STAT!C401","v":0},{"$f":"(3.412141/10.7639)*STAT!D401","v":0},{"$f":"(3.412141/10.7639)*STAT!E401","v":0},{"$f":"(3.412141/10.7639)*STAT!F401","v":0},{"$f":"(3.412141/10.7639)*STAT!G401","v":0},{"$f":"(3.412141/10.7639)*STAT!H401","v":0},{"$f":"(3.412141/10.7639)*STAT!I401","v":0},{"$f":"(3.412141/10.7639)*STAT!J401","v":0},{"$f":"(3.412141/10.7639)*STAT!K401","v":0},{"$f":"(3.412141/10.7639)*STAT!L401","v":0},{"$f":"(3.412141/10.7639)*STAT!M401","v":0},{"$f":"(3.412141/10.7639)*STAT!N401","v":0},null,120,null,null,null,null,4,0,0,0,0]
[null,5,{"$f":"(3.412141/10.7639)*STAT!C402","v":0},{"$f":"(3.412141/10.7639)*STAT!D402","v":0},{"$f":"(3.412141/10.7639)*STAT!E402","v":0},{"$f":"(3.412141/10.7639)*STAT!F402","v":0},{"$f":"(3.412141/10.7639)*STAT!G402","v":0},{"$f":"(3.412141/10.7639)*STAT!H402","v":0},{"$f":"(3.412141/10.7639)*STAT!I402","v":0},{"$f":"(3.412141/10.7639)*STAT!J402","v":0},{"$f":"(3.412141/10.7639)*STAT!K402","v":0},{"$f":"(3.412141/10.7639)*STAT!L402","v":0},{"$f":"(3.412141/10.7639)*STAT!M402","v":0},{"$f":"(3.412141/10.7639)*STAT!N402","v":0},null,null,null,null,null,null,5,0,0,0,0]
[null,6,{"$f":"(3.412141/10.7639)*STAT!C403","v":0},{"$f":"(3.412141/10.7639)*STAT!D403","v":0},{"$f":"(3.412141/10.7639)*STAT!E403","v":0},{"$f":"(3.412141/10.7639)*STAT!F403","v":1.9019914714926747},{"$f":"(3.412141/10.7639)*STAT!G403","v":5.0719772573137991},{"$f":"(3.412141/10.7639)*STAT!H403","v":6.3399715716422484},{"$f":"(3.412141/10.7639)*STAT!I403","v":3.8039829429853493},{"$f":"(3.412141/10.7639)*STAT!J403","v":1.9019914714926747},{"$f":"(3.412141/10.7639)*STAT!K403","v":0.95099573574633733},{"$f":"(3.412141/10.7639)*STAT!L403","v":0},{"$f":"(3.412141/10.7639)*STAT!M403","v":0},{"$f":"(3.412141/10.7639)*STAT!N403","v":0},null,null,null,"Low - Not very Strong\nNot Useful for Passive Solar",null,null,6,4,6.3399715716422484,0,0]
[null,7,{"$f":"(3.412141/10.7639)*STAT!C404","v":1.5849928929105621},{"$f":"(3.412141/10.7639)*STAT!D404","v":3.8039829429853493},{"$f":"(3.412141/10.7639)*STAT!E404","v":10.777951671791824},{"$f":"(3.412141/10.7639)*STAT!F404","v":35.503840801196596},{"$f":"(3.412141/10.7639)*STAT!G404","v":51.987766887466442},{"$f":"(3.412141/10.7639)*STAT!H404","v":58.644737037690803},{"$f":"(3.412141/10.7639)*STAT!I404","v":45.64779531582419},{"$f":"(3.412141/10.7639)*STAT!J404","v":36.137837958360819},{"$f":"(3.412141/10.7639)*STAT!K404","v":29.480867808136459},{"$f":"(3.412141/10.7639)*STAT!L404","v":20.287909029255196},{"$f":"(3.412141/10.7639)*STAT!M404","v":6.3399715716422484},{"$f":"(3.412141/10.7639)*STAT!N404","v":2.5359886286568996},null,1,null,null,null,null,7,18,58.644737037690803,0,2.5359886286568996]
[null,8,{"$f":"(3.412141/10.7639)*STAT!C405","v":35.503840801196596},{"$f":"(3.412141/10.7639)*STAT!D405","v":46.915789630152645},{"$f":"(3.412141/10.7639)*STAT!E405","v":66.886700080825719},{"$f":"(3.412141/10.7639)*STAT!F405","v":103.65853519635077},{"$f":"(3.412141/10.7639)*STAT!G405","v":121.09345701836695},{"$f":"(3.412141/10.7639)*STAT!H405","v":133.77340016165144},{"$f":"(3.412141/10.7639)*STAT!I405","v":118.87446696829217},{"$f":"(3.412141/10.7639)*STAT!J405","v":109.04751103224667},{"$f":"(3.412141/10.7639)*STAT!K405","v":103.97553377493288},{"$f":"(3.412141/10.7639)*STAT!L405","v":90.978592053066265},{"$f":"(3.412141/10.7639)*STAT!M405","v":57.693741301944463},{"$f":"(3.412141/10.7639)*STAT!N405","v":35.18684222261448},null,null,null,null,null,null,8,52,133.77340016165144,2,35.18684222261448]
[null,9,{"$f":"(3.412141/10.7639)*STAT!C406","v":94.465576417469507},{"$f":"(3.412141/10.7639)*STAT!D406","v":107.46251813933611},{"$f":"(3.412141/10.7639)*STAT!E406","v":132.505405847323},{"$f":"(3.412141/10.7639)*STAT!F406","v":169.91123812001226},{"$f":"(3.412141/10.7639)*STAT!G406","v":186.39516420628212},{"$f":"(3.412141/10.7639)*STAT!H406","v":206.36607465695519},{"$f":"(3.412141/10.7639)*STAT!I406","v":193.05213435650649},{"$f":"(3.412141/10.7639)*STAT!J406","v":185.12716989195366},{"$f":"(3.412141/10.7639)*STAT!K406","v":181.32318694896833},{"$f":"(3.412141/10.7639)*STAT!L406","v":164.83926086269847},{"$f":"(3.412141/10.7639)*STAT!M406","v":124.58044138277019},{"$f":"(3.412141/10.7639)*STAT!N406","v":80.83463753843867},null,null,null,"Zero - Before Sunrise or\nAfter Sunset",null,null,9,74,206.36607465695519,27,80.83463753843867]
[null,10,{"$f":"(3.412141/10.7639)*STAT!C407","v":148.35533477642863},{"$f":"(3.412141/10.7639)*STAT!D407","v":164.20526370553424},{"$f":"(3.412141/10.7639)*STAT!E407","v":191.15014288501379},{"$f":"(3.412141/10.7639)*STAT!F407","v":226.01998652904618},{"$f":"(3.412141/10.7639)*STAT!G407","v":245.35689982255502},{"$f":"(3.412141/10.7639)*STAT!H407","v":266.59580458755659},{"$f":"(3.412141/10.7639)*STAT!I407","v":258.98783870158587},{"$f":"(3.412141/10.7639)*STAT!J407","v":250.11187850128672},{"$f":"(3.412141/10.7639)*STAT!K407","v":245.67389840113714},{"$f":"(3.412141/10.7639)*STAT!L407","v":224.75199221471772},{"$f":"(3.412141/10.7639)*STAT!M407","v":182.90817984187888},{"$f":"(3.412141/10.7639)*STAT!N407","v":127.75042716859132},null,null,null,null,null,null,10,100,266.59580458755659,55,127.75042716859132]
[null,11,{"$f":"(3.412141/10.7639)*STAT!C408","v":186.71216278486423},{"$f":"(3.412141/10.7639)*STAT!D408","v":205.73207749979099},{"$f":"(3.412141/10.7639)*STAT!E408","v":228.87297373628519},{"$f":"(3.412141/10.7639)*STAT!F408","v":262.15782448740697},{"$f":"(3.412141/10.7639)*STAT!G408","v":286.56671503822963},{"$f":"(3.412141/10.7639)*STAT!H408","v":308.75661553897754},{"$f":"(3.412141/10.7639)*STAT!I408","v":305.58662975315639},{"$f":"(3.412141/10.7639)*STAT!J408","v":296.71066955285727},{"$f":"(3.412141/10.7639)*STAT!K408","v":289.41970224546867},{"$f":"(3.412141/10.7639)*STAT!L408","v":264.69381311606389},{"$f":"(3.412141/10.7639)*STAT!M408","v":222.53300216464294},{"$f":"(3.412141/10.7639)*STAT!N408","v":161.35227649829523},null,null,null,null,null,null,11,134,308.75661553897754,96,161.35227649829523]
[null,12,{"$f":"(3.412141/10.7639)*STAT!C409","v":205.09808034262676},{"$f":"(3.412141/10.7639)*STAT!D409","v":227.28798084337461},{"$f":"(3.412141/10.7639)*STAT!E409","v":254.8668571800184},{"$f":"(3.412141/10.7639)*STAT!F409","v":273.56977331636301},{"$f":"(3.412141/10.7639)*STAT!G409","v":305.26963117457427},{"$f":"(3.412141/10.7639)*STAT!H409","v":329.67852172539693},{"$f":"(3.412141/10.7639)*STAT!I409","v":328.09352883248636},{"$f":"(3.412141/10.7639)*STAT!J409","v":320.4855629465157},{"$f":"(3.412141/10.7639)*STAT!K409","v":308.75661553897754},{"$f":"(3.412141/10.7639)*STAT!L409","v":281.81173635949796},{"$f":"(3.412141/10.7639)*STAT!M409","v":238.38293109374857},{"$f":"(3.412141/10.7639)*STAT!N409","v":176.88520684881874},null,null,null,null,null,null,12,130,329.67852172539693,136,176.88520684881874]
[null,13,{"$f":"(3.412141/10.7639)*STAT!C410","v":207.63406897128365},{"$f":"(3.412141/10.7639)*STAT!D410","v":238.06593251516645},{"$f":"(3.412141/10.7639)*STAT!E410","v":265.96180743039235},{"$f":"(3.412141/10.7639)*STAT!F410","v":269.76579037337768},{"$f":"(3.412141/10.7639)*STAT!G410","v":303.05064112449952},{"$f":"(3.412141/10.7639)*STAT!H410","v":327.45953167532218},{"$f":"(3.412141/10.7639)*STAT!I410","v":325.87453878241161},{"$f":"(3.412141/10.7639)*STAT!J410","v":318.90057005360512},{"$f":"(3.412141/10.7639)*STAT!K410","v":303.05064112449952},{"$f":"(3.412141/10.7639)*STAT!L410","v":273.25277473778095},{"$f":"(3.412141/10.7639)*STAT!M410","v":229.50697089344942},{"$f":"(3.412141/10.7639)*STAT!N410","v":181.00618837038621},null,null,null,null,null,null,13,153,327.45953167532218,151,181.00618837038621]
[null,14,{"$f":"(3.412141/10.7639)*STAT!C411","v":188.29715567777478},{"$f":"(3.412141/10.7639)*STAT!D411","v":224.4349936361356},{"$f":"(3.412141/10.7639)*STAT!E411","v":242.1869140367339},{"$f":"(3.412141/10.7639)*STAT!F411","v":244.72290266539082},{"$f":"(3.412141/10.7639)*STAT!G411","v":280.54374204516949},{"$f":"(3.412141/10.7639)*STAT!H411","v":301.14864965300683},{"$f":"(3.412141/10.7639)*STAT!I411","v":298.92965960293202},{"$f":"(3.412141/10.7639)*STAT!J411","v":290.68769655979713},{"$f":"(3.412141/10.7639)*STAT!K411","v":271.98478042345249},{"$f":"(3.412141/10.7639)*STAT!L411","v":239.96792398665912},{"$f":"(3.412141/10.7639)*STAT!M411","v":196.22212014232761},{"$f":"(3.412141/10.7639)*STAT!N411","v":161.98627365545946},null,null,null,null,null,null,14,142,301.14864965300683,167,161.98627365545946]
[null,15,{"$f":"(3.412141/10.7639)*STAT!C412","v":148.67233335501075},{"$f":"(3.412141/10.7639)*STAT!D412","v":187.02916136344635},{"$f":"(3.412141/10.7639)*STAT!E412","v":201.61109597822352},{"$f":"(3.412141/10.7639)*STAT!F412","v":200.66010024247717},{"$f":"(3.412141/10.7639)*STAT!G412","v":234.57894815076321},{"$f":"(3.412141/10.7639)*STAT!H412","v":253.28186428710785},{"$f":"(3.412141/10.7639)*STAT!I412","v":249.47788134412249},{"$f":"(3.412141/10.7639)*STAT!J412","v":239.650925408077},{"$f":"(3.412141/10.7639)*STAT!K412","v":218.41202064307546},{"$f":"(3.412141/10.7639)*STAT!L412","v":185.12716989195366},{"$f":"(3.412141/10.7639)*STAT!M412","v":142.64936036195061},{"$f":"(3.412141/10.7639)*STAT!N412","v":122.99544848985963},null,null,null,null,null,null,15,131,253.28186428710785,145,122.99544848985963]
[null,16,{"$f":"(3.412141/10.7639)*STAT!C413","v":98.586557939036965},{"$f":"(3.412141/10.7639)*STAT!D413","v":129.96941721866611},{"$f":"(3.412141/10.7639)*STAT!E413","v":143.91735467627905},{"$f":"(3.412141/10.7639)*STAT!F413","v":144.86835041202539},{"$f":"(3.412141/10.7639)*STAT!G413","v":174.66621679874396},{"$f":"(3.412141/10.7639)*STAT!H413","v":190.83314430643171},{"$f":"(3.412141/10.7639)*STAT!I413","v":188.29715567777478},{"$f":"(3.412141/10.7639)*STAT!J413","v":175.93421111307239},{"$f":"(3.412141/10.7639)*STAT!K413","v":149.30633051217495},{"$f":"(3.412141/10.7639)*STAT!L413","v":113.48549113239625},{"$f":"(3.412141/10.7639)*STAT!M413","v":76.396657438289097},{"$f":"(3.412141/10.7639)*STAT!N413","v":71.324680180975307},null,null,null,null,null,null,16,123,190.83314430643171,100,71.324680180975307]
[null,17,{"$f":"(3.412141/10.7639)*STAT!C414","v":38.356828008435606},{"$f":"(3.412141/10.7639)*STAT!D414","v":62.131721402094037},{"$f":"(3.412141/10.7639)*STAT!E414","v":76.713656016871212},{"$f":"(3.412141/10.7639)*STAT!F414","v":79.883641802692338},{"$f":"(3.412141/10.7639)*STAT!G414","v":98.90355651761908},{"$f":"(3.412141/10.7639)*STAT!H414","v":116.65547691821737},{"$f":"(3.412141/10.7639)*STAT!I414","v":114.75348544672471},{"$f":"(3.412141/10.7639)*STAT!J414","v":100.17155083194753},{"$f":"(3.412141/10.7639)*STAT!K414","v":71.007681602393191},{"$f":"(3.412141/10.7639)*STAT!L414","v":38.356828008435606},{"$f":"(3.412141/10.7639)*STAT!M414","v":14.898933193359285},{"$f":"(3.412141/10.7639)*STAT!N414","v":17.751920400598298},null,null,null,null,null,null,17,84,116.65547691821737,45,17.751920400598298]
[null,18,{"$f":"(3.412141/10.7639)*STAT!C415","v":2.2189900500747872},{"$f":"(3.412141/10.7639)*STAT!D415","v":7.6079658859706987},{"$f":"(3.412141/10.7639)*STAT!E415","v":13.947937457612948},{"$f":"(3.412141/10.7639)*STAT!F415","v":19.653911872090973},{"$f":"(3.412141/10.7639)*STAT!G415","v":30.748862122464907},{"$f":"(3.412141/10.7639)*STAT!H415","v":43.745803844331519},{"$f":"(3.412141/10.7639)*STAT!I415","v":42.477809530003064},{"$f":"(3.412141/10.7639)*STAT!J415","v":29.797866386718571},{"$f":"(3.412141/10.7639)*STAT!K415","v":10.143954514627598},{"$f":"(3.412141/10.7639)*STAT!L415","v":1.9019914714926747},{"$f":"(3.412141/10.7639)*STAT!M415","v":0},{"$f":"(3.412141/10.7639)*STAT!N415","v":0},null,null,null,null,null,null,18,63,43.745803844331519,8,0]
[null,19,{"$f":"(3.412141/10.7639)*STAT!C416","v":0},{"$f":"(3.412141/10.7639)*STAT!D416","v":0},{"$f":"(3.412141/10.7639)*STAT!E416","v":0},{"$f":"(3.412141/10.7639)*STAT!F416","v":0.31699857858211244},{"$f":"(3.412141/10.7639)*STAT!G416","v":1.5849928929105621},{"$f":"(3.412141/10.7639)*STAT!H416","v":3.486984364403237},{"$f":"(3.412141/10.7639)*STAT!I416","v":3.486984364403237},{"$f":"(3.412141/10.7639)*STAT!J416","v":1.2679943143284498},{"$f":"(3.412141/10.7639)*STAT!K416","v":0},{"$f":"(3.412141/10.7639)*STAT!L416","v":0},{"$f":"(3.412141/10.7639)*STAT!M416","v":0},{"$f":"(3.412141/10.7639)*STAT!N416","v":0},null,null,null,null,null,null,19,39,3.486984364403237,0,0]
[null,20,{"$f":"(3.412141/10.7639)*STAT!C417","v":0},{"$f":"(3.412141/10.7639)*STAT!D417","v":0},{"$f":"(3.412141/10.7639)*STAT!E417","v":0},{"$f":"(3.412141/10.7639)*STAT!F417","v":0},{"$f":"(3.412141/10.7639)*STAT!G417","v":0},{"$f":"(3.412141/10.7639)*STAT!H417","v":0},{"$f":"(3.412141/10.7639)*STAT!I417","v":0},{"$f":"(3.412141/10.7639)*STAT!J417","v":0},{"$f":"(3.412141/10.7639)*STAT!K417","v":0},{"$f":"(3.412141/10.7639)*STAT!L417","v":0},{"$f":"(3.412141/10.7639)*STAT!M417","v":0},{"$f":"(3.412141/10.7639)*STAT!N417","v":0},null,null,null,null,null,null,20,10,0,0,0]
[null,21,{"$f":"(3.412141/10.7639)*STAT!C418","v":0},{"$f":"(3.412141/10.7639)*STAT!D418","v":0},{"$f":"(3.412141/10.7639)*STAT!E418","v":0},{"$f":"(3.412141/10.7639)*STAT!F418","v":0},{"$f":"(3.412141/10.7639)*STAT!G418","v":0},{"$f":"(3.412141/10.7639)*STAT!H418","v":0},{"$f":"(3.412141/10.7639)*STAT!I418","v":0},{"$f":"(3.412141/10.7639)*STAT!J418","v":0},{"$f":"(3.412141/10.7639)*STAT!K418","v":0},{"$f":"(3.412141/10.7639)*STAT!L418","v":0},{"$f":"(3.412141/10.7639)*STAT!M418","v":0},{"$f":"(3.412141/10.7639)*STAT!N418","v":0},null,null,null,null,null,null,21,0,0,0,0]
[null,22,{"$f":"(3.412141/10.7639)*STAT!C419","v":0},{"$f":"(3.412141/10.7639)*STAT!D419","v":0},{"$f":"(3.412141/10.7639)*STAT!E419","v":0},{"$f":"(3.412141/10.7639)*STAT!F419","v":0},{"$f":"(3.412141/10.7639)*STAT!G419","v":0},{"$f":"(3.412141/10.7639)*STAT!H419","v":0},{"$f":"(3.412141/10.7639)*STAT!I419","v":0},{"$f":"(3.412141/10.7639)*STAT!J419","v":0},{"$f":"(3.412141/10.7639)*STAT!K419","v":0},{"$f":"(3.412141/10.7639)*STAT!L419","v":0},{"$f":"(3.412141/10.7639)*STAT!M419","v":0},{"$f":"(3.412141/10.7639)*STAT!N419","v":0},null,null,null,null,null,null,22,0,0,0,0]
[null,23,{"$f":"(3.412141/10.7639)*STAT!C420","v":0},{"$f":"(3.412141/10.7639)*STAT!D420","v":0},{"$f":"(3.412141/10.7639)*STAT!E420","v":0},{"$f":"(3.412141/10.7639)*STAT!F420","v":0},{"$f":"(3.412141/10.7639)*STAT!G420","v":0},{"$f":"(3.412141/10.7639)*STAT!H420","v":0},{"$f":"(3.412141/10.7639)*STAT!I420","v":0},{"$f":"(3.412141/10.7639)*STAT!J420","v":0},{"$f":"(3.412141/10.7639)*STAT!K420","v":0},{"$f":"(3.412141/10.7639)*STAT!L420","v":0},{"$f":"(3.412141/10.7639)*STAT!M420","v":0},{"$f":"(3.412141/10.7639)*STAT!N420","v":0},null,null,null,null,null,null,23,0,0,0,0]
[null,24,{"$f":"(3.412141/10.7639)*STAT!C421","v":0},{"$f":"(3.412141/10.7639)*STAT!D421","v":0},{"$f":"(3.412141/10.7639)*STAT!E421","v":0},{"$f":"(3.412141/10.7639)*STAT!F421","v":0},{"$f":"(3.412141/10.7639)*STAT!G421","v":0},{"$f":"(3.412141/10.7639)*STAT!H421","v":0},{"$f":"(3.412141/10.7639)*STAT!I421","v":0},{"$f":"(3.412141/10.7639)*STAT!J421","v":0},{"$f":"(3.412141/10.7639)*STAT!K421","v":0},{"$f":"(3.412141/10.7639)*STAT!L421","v":0},{"$f":"(3.412141/10.7639)*STAT!M421","v":0},{"$f":"(3.412141/10.7639)*STAT!N421","v":0},null,null,null,null,null,null,24,0,0,0,0]
[]
[null,null,"Home"]

{"sheet":"Dry Bulb","index":8,"n_rows":31,"n_cols":18,"rows_kept":31,"cut":false,"hidden":false,"merged":[[30,3,30,4],[2,11,2,14],[2,2,2,9]]}
[]
[]
[null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,null,null,null,"Dry Bulb Temperature"]
[null,null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,null,1,{"$f":"STAT!C127*9/5+32","v":52.879999999999995},{"$f":"STAT!D127*9/5+32","v":57.379999999999995},{"$f":"STAT!E127*9/5+32","v":64.22},{"$f":"STAT!F127*9/5+32","v":73.040000000000006},{"$f":"STAT!G127*9/5+32","v":84.56},{"$f":"STAT!H127*9/5+32","v":89.6},{"$f":"STAT!I127*9/5+32","v":90.86},{"$f":"STAT!J127*9/5+32","v":91.4},{"$f":"STAT!K127*9/5+32","v":85.82},{"$f":"STAT!L127*9/5+32","v":76.099999999999994},{"$f":"STAT!M127*9/5+32","v":65.12},{"$f":"STAT!N127*9/5+32","v":54.86},null,{"$f":"'Operative BP'!P15","v":75},"Hot - Cooling Needed"]
[null,null,2,{"$f":"STAT!C128*9/5+32","v":51.98},{"$f":"STAT!D128*9/5+32","v":56.3},{"$f":"STAT!E128*9/5+32","v":62.959999999999994},{"$f":"STAT!F128*9/5+32","v":71.959999999999994},{"$f":"STAT!G128*9/5+32","v":83.12},{"$f":"STAT!H128*9/5+32","v":87.8},{"$f":"STAT!I128*9/5+32","v":89.24},{"$f":"STAT!J128*9/5+32","v":89.78},{"$f":"STAT!K128*9/5+32","v":84.02},{"$f":"STAT!L128*9/5+32","v":74.84},{"$f":"STAT!M128*9/5+32","v":63.5},{"$f":"STAT!N128*9/5+32","v":54.14}]
[null,null,3,{"$f":"STAT!C129*9/5+32","v":51.44},{"$f":"STAT!D129*9/5+32","v":55.22},{"$f":"STAT!E129*9/5+32","v":61.7},{"$f":"STAT!F129*9/5+32","v":70.88},{"$f":"STAT!G129*9/5+32","v":82.04},{"$f":"STAT!H129*9/5+32","v":86.9},{"$f":"STAT!I129*9/5+32","v":88.16},{"$f":"STAT!J129*9/5+32","v":88.16},{"$f":"STAT!K129*9/5+32","v":82.4},{"$f":"STAT!L129*9/5+32","v":73.22},{"$f":"STAT!M129*9/5+32","v":62.24},{"$f":"STAT!N129*9/5+32","v":53.42},null,65,"Comfort Zone"]
[null,null,4,{"$f":"STAT!C130*9/5+32","v":50.54},{"$f":"STAT!D130*9/5+32","v":54.14},{"$f":"STAT!E130*9/5+32","v":60.8},{"$f":"STAT!F130*9/5+32","v":69.44},{"$f":"STAT!G130*9/5+32","v":81.5},{"$f":"STAT!H130*9/5+32","v":85.82},{"$f":"STAT!I130*9/5+32","v":86.72},{"$f":"STAT!J130*9/5+32","v":86.9},{"$f":"STAT!K130*9/5+32","v":80.959999999999994},{"$f":"STAT!L130*9/5+32","v":72.5},{"$f":"STAT!M130*9/5+32","v":60.980000000000004},{"$f":"STAT!N130*9/5+32","v":52.52}]
[null,null,5,{"$f":"STAT!C131*9/5+32","v":49.46},{"$f":"STAT!D131*9/5+32","v":53.42},{"$f":"STAT!E131*9/5+32","v":59.9},{"$f":"STAT!F131*9/5+32","v":68.36},{"$f":"STAT!G131*9/5+32","v":80.06},{"$f":"STAT!H131*9/5+32","v":84.56},{"$f":"STAT!I131*9/5+32","v":86},{"$f":"STAT!J131*9/5+32","v":85.82},{"$f":"STAT!K131*9/5+32","v":80.240000000000009},{"$f":"STAT!L131*9/5+32","v":71.06},{"$f":"STAT!M131*9/5+32","v":59.540000000000006},{"$f":"STAT!N131*9/5+32","v":51.620000000000005},null,50,"Cool - Passive Heating"]
[null,null,6,{"$f":"STAT!C132*9/5+32","v":48.92},{"$f":"STAT!D132*9/5+32","v":52.7},{"$f":"STAT!E132*9/5+32","v":59.36},{"$f":"STAT!F132*9/5+32","v":67.64},{"$f":"STAT!G132*9/5+32","v":78.8},{"$f":"STAT!H132*9/5+32","v":83.48},{"$f":"STAT!I132*9/5+32","v":85.28},{"$f":"STAT!J132*9/5+32","v":84.919999999999987},{"$f":"STAT!K132*9/5+32","v":79.7},{"$f":"STAT!L132*9/5+32","v":70.16},{"$f":"STAT!M132*9/5+32","v":59.18},{"$f":"STAT!N132*9/5+32","v":51.620000000000005}]
[null,null,7,{"$f":"STAT!C133*9/5+32","v":48.92},{"$f":"STAT!D133*9/5+32","v":52.7},{"$f":"STAT!E133*9/5+32","v":59.36},{"$f":"STAT!F133*9/5+32","v":69.44},{"$f":"STAT!G133*9/5+32","v":80.78},{"$f":"STAT!H133*9/5+32","v":86.36},{"$f":"STAT!I133*9/5+32","v":87.98},{"$f":"STAT!J133*9/5+32","v":87.44},{"$f":"STAT!K133*9/5+32","v":81.680000000000007},{"$f":"STAT!L133*9/5+32","v":71.06},{"$f":"STAT!M133*9/5+32","v":58.82},{"$f":"STAT!N133*9/5+32","v":51.26},null,null,"Cold - Mechanical Heating"]
[null,null,8,{"$f":"STAT!C134*9/5+32","v":51.26},{"$f":"STAT!D134*9/5+32","v":55.04},{"$f":"STAT!E134*9/5+32","v":62.42},{"$f":"STAT!F134*9/5+32","v":72.680000000000007},{"$f":"STAT!G134*9/5+32","v":84.38000000000001},{"$f":"STAT!H134*9/5+32","v":89.960000000000008},{"$f":"STAT!I134*9/5+32","v":91.580000000000013},{"$f":"STAT!J134*9/5+32","v":91.4},{"$f":"STAT!K134*9/5+32","v":86.18},{"$f":"STAT!L134*9/5+32","v":75.02},{"$f":"STAT!M134*9/5+32","v":63.68},{"$f":"STAT!N134*9/5+32","v":52.879999999999995}]
[null,null,9,{"$f":"STAT!C135*9/5+32","v":53.96},{"$f":"STAT!D135*9/5+32","v":57.92},{"$f":"STAT!E135*9/5+32","v":64.58},{"$f":"STAT!F135*9/5+32","v":77},{"$f":"STAT!G135*9/5+32","v":87.26},{"$f":"STAT!H135*9/5+32","v":93.38000000000001},{"$f":"STAT!I135*9/5+32","v":95.9},{"$f":"STAT!J135*9/5+32","v":96.080000000000013},{"$f":"STAT!K135*9/5+32","v":90.32},{"$f":"STAT!L135*9/5+32","v":79.16},{"$f":"STAT!M135*9/5+32","v":68.540000000000006},{"$f":"STAT!N135*9/5+32","v":55.76}]
[null,null,10,{"$f":"STAT!C136*9/5+32","v":56.84},{"$f":"STAT!D136*9/5+32","v":60.980000000000004},{"$f":"STAT!E136*9/5+32","v":67.459999999999994},{"$f":"STAT!F136*9/5+32","v":80.42},{"$f":"STAT!G136*9/5+32","v":90.32},{"$f":"STAT!H136*9/5+32","v":96.44},{"$f":"STAT!I136*9/5+32","v":99.68},{"$f":"STAT!J136*9/5+32","v":100.22},{"$f":"STAT!K136*9/5+32","v":93.919999999999987},{"$f":"STAT!L136*9/5+32","v":82.94},{"$f":"STAT!M136*9/5+32","v":72.5},{"$f":"STAT!N136*9/5+32","v":58.82}]
[null,null,11,{"$f":"STAT!C137*9/5+32","v":59.36},{"$f":"STAT!D137*9/5+32","v":64.400000000000006},{"$f":"STAT!E137*9/5+32","v":69.98},{"$f":"STAT!F137*9/5+32","v":83.3},{"$f":"STAT!G137*9/5+32","v":92.84},{"$f":"STAT!H137*9/5+32","v":99.14},{"$f":"STAT!I137*9/5+32","v":102.56},{"$f":"STAT!J137*9/5+32","v":103.64},{"$f":"STAT!K137*9/5+32","v":96.44},{"$f":"STAT!L137*9/5+32","v":86},{"$f":"STAT!M137*9/5+32","v":76.099999999999994},{"$f":"STAT!N137*9/5+32","v":61.88}]
[null,null,12,{"$f":"STAT!C138*9/5+32","v":61.88},{"$f":"STAT!D138*9/5+32","v":66.92},{"$f":"STAT!E138*9/5+32","v":71.599999999999994},{"$f":"STAT!F138*9/5+32","v":85.460000000000008},{"$f":"STAT!G138*9/5+32","v":94.82},{"$f":"STAT!H138*9/5+32","v":101.48},{"$f":"STAT!I138*9/5+32","v":104.36},{"$f":"STAT!J138*9/5+32","v":105.61999999999999},{"$f":"STAT!K138*9/5+32","v":98.24},{"$f":"STAT!L138*9/5+32","v":88.52},{"$f":"STAT!M138*9/5+32","v":78.62},{"$f":"STAT!N138*9/5+32","v":64.040000000000006}]
[null,null,13,{"$f":"STAT!C139*9/5+32","v":63.86},{"$f":"STAT!D139*9/5+32","v":69.62},{"$f":"STAT!E139*9/5+32","v":75.2},{"$f":"STAT!F139*9/5+32","v":86.72},{"$f":"STAT!G139*9/5+32","v":96.8},{"$f":"STAT!H139*9/5+32","v":102.74},{"$f":"STAT!I139*9/5+32","v":105.8},{"$f":"STAT!J139*9/5+32","v":107.6},{"$f":"STAT!K139*9/5+32","v":100.03999999999999},{"$f":"STAT!L139*9/5+32","v":90.32},{"$f":"STAT!M139*9/5+32","v":80.78},{"$f":"STAT!N139*9/5+32","v":66.2}]
[null,null,14,{"$f":"STAT!C140*9/5+32","v":65.48},{"$f":"STAT!D140*9/5+32","v":71.599999999999994},{"$f":"STAT!E140*9/5+32","v":76.819999999999993},{"$f":"STAT!F140*9/5+32","v":88.16},{"$f":"STAT!G140*9/5+32","v":98.24},{"$f":"STAT!H140*9/5+32","v":104.9},{"$f":"STAT!I140*9/5+32","v":107.41999999999999},{"$f":"STAT!J140*9/5+32","v":108.5},{"$f":"STAT!K140*9/5+32","v":101.11999999999999},{"$f":"STAT!L140*9/5+32","v":91.76},{"$f":"STAT!M140*9/5+32","v":81.680000000000007},{"$f":"STAT!N140*9/5+32","v":67.64}]
[null,null,15,{"$f":"STAT!C141*9/5+32","v":66.02},{"$f":"STAT!D141*9/5+32","v":72.680000000000007},{"$f":"STAT!E141*9/5+32","v":77.900000000000006},{"$f":"STAT!F141*9/5+32","v":89.06},{"$f":"STAT!G141*9/5+32","v":98.6},{"$f":"STAT!H141*9/5+32","v":105.61999999999999},{"$f":"STAT!I141*9/5+32","v":108.32},{"$f":"STAT!J141*9/5+32","v":108.86},{"$f":"STAT!K141*9/5+32","v":101.84},{"$f":"STAT!L141*9/5+32","v":92.66},{"$f":"STAT!M141*9/5+32","v":82.94},{"$f":"STAT!N141*9/5+32","v":68.36}]
[null,null,16,{"$f":"STAT!C142*9/5+32","v":66.2},{"$f":"STAT!D142*9/5+32","v":72.319999999999993},{"$f":"STAT!E142*9/5+32","v":78.259999999999991},{"$f":"STAT!F142*9/5+32","v":88.34},{"$f":"STAT!G142*9/5+32","v":98.78},{"$f":"STAT!H142*9/5+32","v":105.8},{"$f":"STAT!I142*9/5+32","v":108.14},{"$f":"STAT!J142*9/5+32","v":108.32},{"$f":"STAT!K142*9/5+32","v":101.66},{"$f":"STAT!L142*9/5+32","v":92.11999999999999},{"$f":"STAT!M142*9/5+32","v":82.04},{"$f":"STAT!N142*9/5+32","v":67.64}]
[null,null,17,{"$f":"STAT!C143*9/5+32","v":65.12},{"$f":"STAT!D143*9/5+32","v":70.88},{"$f":"STAT!E143*9/5+32","v":77.180000000000007},{"$f":"STAT!F143*9/5+32","v":86.72},{"$f":"STAT!G143*9/5+32","v":98.6},{"$f":"STAT!H143*9/5+32","v":105.08000000000001},{"$f":"STAT!I143*9/5+32","v":107.6},{"$f":"STAT!J143*9/5+32","v":107.06},{"$f":"STAT!K143*9/5+32","v":100.22},{"$f":"STAT!L143*9/5+32","v":91.039999999999992},{"$f":"STAT!M143*9/5+32","v":80.42},{"$f":"STAT!N143*9/5+32","v":65.66}]
[null,null,18,{"$f":"STAT!C144*9/5+32","v":63.32},{"$f":"STAT!D144*9/5+32","v":69.08},{"$f":"STAT!E144*9/5+32","v":75.92},{"$f":"STAT!F144*9/5+32","v":85.28},{"$f":"STAT!G144*9/5+32","v":97.34},{"$f":"STAT!H144*9/5+32","v":104.18},{"$f":"STAT!I144*9/5+32","v":106.16},{"$f":"STAT!J144*9/5+32","v":105.44},{"$f":"STAT!K144*9/5+32","v":99.14},{"$f":"STAT!L144*9/5+32","v":89.6},{"$f":"STAT!M144*9/5+32","v":77.900000000000006},{"$f":"STAT!N144*9/5+32","v":64.400000000000006}]
[null,null,19,{"$f":"STAT!C145*9/5+32","v":61.519999999999996},{"$f":"STAT!D145*9/5+32","v":67.28},{"$f":"STAT!E145*9/5+32","v":74.3},{"$f":"STAT!F145*9/5+32","v":82.759999999999991},{"$f":"STAT!G145*9/5+32","v":95.72},{"$f":"STAT!H145*9/5+32","v":102.2},{"$f":"STAT!I145*9/5+32","v":103.64},{"$f":"STAT!J145*9/5+32","v":103.1},{"$f":"STAT!K145*9/5+32","v":97.34},{"$f":"STAT!L145*9/5+32","v":87.61999999999999},{"$f":"STAT!M145*9/5+32","v":75.92},{"$f":"STAT!N145*9/5+32","v":61.88}]
[null,null,20,{"$f":"STAT!C146*9/5+32","v":59.540000000000006},{"$f":"STAT!D146*9/5+32","v":64.94},{"$f":"STAT!E146*9/5+32","v":71.78},{"$f":"STAT!F146*9/5+32","v":81.14},{"$f":"STAT!G146*9/5+32","v":93.38000000000001},{"$f":"STAT!H146*9/5+32","v":99.68},{"$f":"STAT!I146*9/5+32","v":100.03999999999999},{"$f":"STAT!J146*9/5+32","v":100.22},{"$f":"STAT!K146*9/5+32","v":95},{"$f":"STAT!L146*9/5+32","v":84.56},{"$f":"STAT!M146*9/5+32","v":73.400000000000006},{"$f":"STAT!N146*9/5+32","v":60.08}]
[null,null,21,{"$f":"STAT!C147*9/5+32","v":58.28},{"$f":"STAT!D147*9/5+32","v":63.14},{"$f":"STAT!E147*9/5+32","v":70.34},{"$f":"STAT!F147*9/5+32","v":79.52},{"$f":"STAT!G147*9/5+32","v":91.4},{"$f":"STAT!H147*9/5+32","v":96.98},{"$f":"STAT!I147*9/5+32","v":97.16},{"$f":"STAT!J147*9/5+32","v":98.24},{"$f":"STAT!K147*9/5+32","v":92.48},{"$f":"STAT!L147*9/5+32","v":82.58},{"$f":"STAT!M147*9/5+32","v":71.78},{"$f":"STAT!N147*9/5+32","v":58.82}]
[null,null,22,{"$f":"STAT!C148*9/5+32","v":56.84},{"$f":"STAT!D148*9/5+32","v":61.34},{"$f":"STAT!E148*9/5+32","v":68.72},{"$f":"STAT!F148*9/5+32","v":77.900000000000006},{"$f":"STAT!G148*9/5+32","v":89.6},{"$f":"STAT!H148*9/5+32","v":94.64},{"$f":"STAT!I148*9/5+32","v":94.460000000000008},{"$f":"STAT!J148*9/5+32","v":96.26},{"$f":"STAT!K148*9/5+32","v":90.68},{"$f":"STAT!L148*9/5+32","v":80.599999999999994},{"$f":"STAT!M148*9/5+32","v":69.8},{"$f":"STAT!N148*9/5+32","v":57.56}]
[null,null,23,{"$f":"STAT!C149*9/5+32","v":55.58},{"$f":"STAT!D149*9/5+32","v":59.9},{"$f":"STAT!E149*9/5+32","v":67.28},{"$f":"STAT!F149*9/5+32","v":75.740000000000009},{"$f":"STAT!G149*9/5+32","v":87.8},{"$f":"STAT!H149*9/5+32","v":92.84},{"$f":"STAT!I149*9/5+32","v":93.02},{"$f":"STAT!J149*9/5+32","v":94.64},{"$f":"STAT!K149*9/5+32","v":88.88000000000001},{"$f":"STAT!L149*9/5+32","v":78.98},{"$f":"STAT!M149*9/5+32","v":67.819999999999993},{"$f":"STAT!N149*9/5+32","v":56.66}]
[null,null,24,{"$f":"STAT!C150*9/5+32","v":54.68},{"$f":"STAT!D150*9/5+32","v":58.28},{"$f":"STAT!E150*9/5+32","v":65.84},{"$f":"STAT!F150*9/5+32","v":74.3},{"$f":"STAT!G150*9/5+32","v":86.18},{"$f":"STAT!H150*9/5+32","v":91.039999999999992},{"$f":"STAT!I150*9/5+32","v":91.76},{"$f":"STAT!J150*9/5+32","v":92.84},{"$f":"STAT!K150*9/5+32","v":87.26},{"$f":"STAT!L150*9/5+32","v":77.540000000000006},{"$f":"STAT!M150*9/5+32","v":66.56},{"$f":"STAT!N150*9/5+32","v":55.04}]
[]
[]
[null,null,null,"Home"]

{"sheet":"Profile angles","index":9,"n_rows":58,"n_cols":113,"rows_kept":58,"cut":false,"hidden":false,"merged":[[0,1,0,3],[0,7,0,8],[2,1,2,3],[2,26,2,27],[2,24,2,25],[2,15,2,17],[2,18,2,23],[2,4,2,9],[2,10,2,11],[58,95,58,98],[58,109,58,112],[31,100,31,103],[31,104,31,106],[31,107,31,109],[31,110,31,112],[2,104,2,106],[2,107,2,109],[2,110,2,112],[31,57,31,61],[2,57,2,61],[2,90,2,92],[31,86,31,89],[31,90,31,92],[2,86,2,89],[2,96,2,98],[29,109,29,112],[2,100,2,103],[29,95,29,98],[31,93,31,95],[31,96,31,98],[2,93,2,95],[31,71,31,75],[31,43,31,55],[2,71,2,75],[31,18,31,23],[2,29,2,41],[29,10,29,13],[2,12,2,13],[2,43,2,55],[31,29,31,41],[31,1,31,3],[31,4,31,9],[31,10,31,11],[31,12,31,13],[29,24,29,27],[58,10,58,13],[58,24,58,27],[31,24,31,25],[31,26,31,27],[31,15,31,17]]}
[null,"Control",null,null,30,null,null,"Home"]
[]
[null,"Table 1:",null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,"South",null," Profile",null,null,"Table 3:",null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,"West",null," Profile",null,null,"Balance pt",null,null,null,null,null,null,null,null,null,null,null,null,null,"Altitude",null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI3","v":"South Transmitted"},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BW3","v":"East Transmitted"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Table 5:",null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,"South",null,null," Profile",null,null,null,"Table 6:",null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,"West",null,null," Profile"]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$f":"'Operative BP'!B219","v":"HR"},{"$f":"'Operative BP'!C219","v":"Jan"},{"$f":"'Operative BP'!D219","v":"Feb"},{"$f":"'Operative BP'!E219","v":"Mar"},{"$f":"'Operative BP'!F219","v":"Apr"},{"$f":"'Operative BP'!G219","v":"May"},{"$f":"'Operative BP'!H219","v":"Jun"},{"$f":"'Operative BP'!I219","v":"Jul"},{"$f":"'Operative BP'!J219","v":"Aug"},{"$f":"'Operative BP'!K219","v":"Sep"},{"$f":"'Operative BP'!L219","v":"Oct"},{"$f":"'Operative BP'!M219","v":"Nov"},{"$f":"'Operative BP'!N219","v":"Dec"},null,{"$f":"'Solar Altitude'!B3","v":0},{"$f":"'Solar Altitude'!C3","v":"Jan"},{"$f":"'Solar Altitude'!D3","v":"Feb"},{"$f":"'Solar Altitude'!E3","v":"Mar"},{"$f":"'Solar Altitude'!F3","v":"Apr"},{"$f":"'Solar Altitude'!G3","v":"May"},{"$f":"'Solar Altitude'!H3","v":"Jun"},{"$f":"'Solar Altitude'!I3","v":"Jul"},{"$f":"'Solar Altitude'!J3","v":"Aug"},{"$f":"'Solar Altitude'!K3","v":"Sep"},{"$f":"'Solar Altitude'!L3","v":"Oct"},{"$f":"'Solar Altitude'!M3","v":"Nov"},{"$f":"'Solar Altitude'!N3","v":"Dec"},null,{"$f":"'Incident angle'!CK4","v":0},{"$f":"'Incident angle'!CL4","v":"Jan"},{"$f":"'Incident angle'!CM4","v":"Feb"},{"$f":"'Incident angle'!CN4","v":"Mar"},{"$f":"'Incident angle'!CO4","v":"Apr"},{"$f":"'Incident angle'!CP4","v":"May"},{"$f":"'Incident angle'!CQ4","v":"Jun"},{"$f":"'Incident angle'!CR4","v":"Jul"},{"$f":"'Incident angle'!CS4","v":"Aug"},{"$f":"'Incident angle'!CT4","v":"Sep"},{"$f":"'Incident angle'!CU4","v":"Oct"},{"$f":"'Incident angle'!CV4","v":"Nov"},{"$f":"'Incident angle'!CW4","v":"Dec"},null,{"$f":"'Incident angle'!CY4","v":0},{"$f":"'Incident angle'!CZ4","v":"Jan"},{"$f":"'Incident angle'!DA4","v":"Feb"},{"$f":"'Incident angle'!DB4","v":"Mar"},{"$f":"'Incident angle'!DC4","v":"Apr"},{"$f":"'Incident angle'!DD4","v":"May"},{"$f":"'Incident angle'!DE4","v":"Jun"},{"$f":"'Incident angle'!DF4","v":"Jul"},{"$f":"'Incident angle'!DG4","v":"Aug"},{"$f":"'Incident angle'!DH4","v":"Sep"},{"$f":"'Incident angle'!DI4","v":"Oct"},{"$f":"'Incident angle'!DJ4","v":"Nov"},{"$f":"'Incident angle'!DK4","v":"Dec"},null,null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"'Profile calcs'!C4","v":85.506692771390249},{"$f":"'Profile calcs'!D4","v":76.051491134901724},{"$f":"'Profile calcs'!E4","v":65.3},{"$f":"'Profile calcs'!F4","v":53.072313870844596},{"$f":"'Profile calcs'!G4","v":44.427911140068865},{"$f":"'Profile calcs'!H4","v":41.313454586896434},{"$f":"'Profile calcs'!I4","v":44.404551466519109},{"$f":"'Profile calcs'!J4","v":52.909735984441284},{"$f":"'Profile calcs'!K4","v":65.3},{"$f":"'Profile calcs'!L4","v":76.480736118519602},{"$f":"'Profile calcs'!M4","v":86.000045802283125},{"$f":"'Profile calcs'!N4","v":89.352163729921244},null,1,{"$f":"'Profile calcs'!AE4","v":80.182065177734387},{"$f":"'Profile calcs'!AF4","v":80.140892672943934},{"$f":"'Profile calcs'!AG4","v":77.550222553106011},{"$f":"'Profile calcs'!AH4","v":73.652297950713148},{"$f":"'Profile calcs'!AI4","v":71.539168870383392},{"$f":"'Profile calcs'!AJ4","v":72.45745912361852},{"$f":"'Profile calcs'!AK4","v":74.587173801009925},{"$f":"'Profile calcs'!AL4","v":74.673520776603795},{"$f":"'Profile calcs'!AM4","v":73.467983805952244},{"$f":"'Profile calcs'!AN4","v":72.789127866510924},{"$f":"'Profile calcs'!AO4","v":74.318586949653394},{"$f":"'Profile calcs'!AP4","v":77.526166860808985},null,{"$f":"'Operative BP'!B220","v":1},{"$f":"'Operative BP'!C220","v":62.979193205944796},{"$f":"'Operative BP'!D220","v":62.979193205944796},{"$f":"'Operative BP'!E220","v":69.979193205944796},{"$f":"'Operative BP'!F220","v":70.429443906581739},{"$f":"'Operative BP'!G220","v":69.979193205944796},{"$f":"'Operative BP'!H220","v":69.979193205944796},{"$f":"'Operative BP'!I220","v":69.979193205944796},{"$f":"'Operative BP'!J220","v":69.979193205944796},{"$f":"'Operative BP'!K220","v":69.979193205944796},{"$f":"'Operative BP'!L220","v":69.726501486199581},{"$f":"'Operative BP'!M220","v":72.248824288747343},{"$f":"'Operative BP'!N220","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B4","v":1},{"$f":"'Solar Altitude'!C4","v":-79.238745258454912},{"$f":"'Solar Altitude'!D4","v":-73.135890206899091},{"$f":"'Solar Altitude'!E4","v":-62.969753990761212},{"$f":"'Solar Altitude'!F4","v":-51.103815741194268},{"$f":"'Solar Altitude'!G4","v":-42.972420763986918},{"$f":"'Solar Altitude'!H4","v":-40.259838967181594},{"$f":"'Solar Altitude'!I4","v":-43.397326661656273},{"$f":"'Solar Altitude'!J4","v":-51.194813940312706},{"$f":"'Solar Altitude'!K4","v":-61.30334441705341},{"$f":"'Solar Altitude'!L4","v":-68.588756925018274},{"$f":"'Solar Altitude'!M4","v":-73.864057818332},{"$f":"'Solar Altitude'!N4","v":-77.510392918823513},null,{"$f":"'Incident angle'!CK5","v":1},{"$f":"'Incident angle'!CL5","v":0},{"$f":"'Incident angle'!CM5","v":0},{"$f":"'Incident angle'!CN5","v":0},{"$f":"'Incident angle'!CO5","v":0},{"$f":"'Incident angle'!CP5","v":0},{"$f":"'Incident angle'!CQ5","v":0},{"$f":"'Incident angle'!CR5","v":0},{"$f":"'Incident angle'!CS5","v":0},{"$f":"'Incident angle'!CT5","v":0},{"$f":"'Incident angle'!CU5","v":0},{"$f":"'Incident angle'!CV5","v":0},{"$f":"'Incident angle'!CW5","v":0},null,{"$f":"'Incident angle'!CY5","v":1},{"$f":"'Incident angle'!CZ5","v":0},{"$f":"'Incident angle'!DA5","v":0},{"$f":"'Incident angle'!DB5","v":0},{"$f":"'Incident angle'!DC5","v":0},{"$f":"'Incident angle'!DD5","v":0},{"$f":"'Incident angle'!DE5","v":0},{"$f":"'Incident angle'!DF5","v":0},{"$f":"'Incident angle'!DG5","v":0},{"$f":"'Incident angle'!DH5","v":0},{"$f":"'Incident angle'!DI5","v":0},{"$f":"'Incident angle'!DJ5","v":0},{"$f":"'Incident angle'!DK5","v":0},null,null,1,{"$f":"IF(BG5=0,1000,IF(AS5<0,1000,(IF(AE5>$E$1,1000,C5))))","v":1000},{"$f":"IF(BH5=0,1000,IF(AT5<0,1000,(IF(AF5>$E$1,1000,D5))))","v":1000},{"$f":"IF(BI5=0,1000,IF(AU5<0,1000,(IF(AG5>$E$1,1000,E5))))","v":1000},{"$f":"IF(BJ5=0,1000,IF(AV5<0,1000,(IF(AH5>$E$1,1000,F5))))","v":1000},{"$f":"IF(BK5=0,1000,IF(AW5<0,1000,(IF(AI5>$E$1,1000,G5))))","v":1000},{"$f":"IF(BL5=0,1000,IF(AX5<0,1000,(IF(AJ5>$E$1,1000,H5))))","v":1000},{"$f":"IF(BM5=0,1000,IF(AY5<0,1000,(IF(AK5>$E$1,1000,I5))))","v":1000},{"$f":"IF(BN5=0,1000,IF(AZ5<0,1000,(IF(AL5>$E$1,1000,J5))))","v":1000},{"$f":"IF(BO5=0,1000,IF(BA5<0,1000,(IF(AM5>$E$1,1000,K5))))","v":1000},{"$f":"IF(BP5=0,1000,IF(BB5<0,1000,(IF(AN5>$E$1,1000,L5))))","v":1000},{"$f":"IF(BQ5=0,1000,IF(BC5<0,1000,(IF(AO5>$E$1,1000,M5))))","v":1000},{"$f":"IF(BR5=0,1000,IF(BD5<0,1000,(IF(AP5>$E$1,1000,N5))))","v":1000},null,1,{"$f":"IF(BG34=0,1000,IF(AS5<0,1000,(IF(AE5>$E$1,1000,Q5))))","v":1000},{"$f":"IF(BH34=0,1000,IF(AT5<0,1000,(IF(AF5>$E$1,1000,R5))))","v":1000},{"$f":"IF(BI34=0,1000,IF(AU5<0,1000,(IF(AG5>$E$1,1000,S5))))","v":1000},{"$f":"IF(BJ34=0,1000,IF(AV5<0,1000,(IF(AH5>$E$1,1000,T5))))","v":1000},{"$f":"IF(BK34=0,1000,IF(AW5<0,1000,(IF(AI5>$E$1,1000,U5))))","v":1000},{"$f":"IF(BL34=0,1000,IF(AX5<0,1000,(IF(AJ5>$E$1,1000,V5))))","v":1000},{"$f":"IF(BM34=0,1000,IF(AY5<0,1000,(IF(AK5>$E$1,1000,W5))))","v":1000},{"$f":"IF(BN34=0,1000,IF(AZ5<0,1000,(IF(AL5>$E$1,1000,X5))))","v":1000},{"$f":"IF(BO34=0,1000,IF(BA5<0,1000,(IF(AM5>$E$1,1000,Y5))))","v":1000},{"$f":"IF(BP34=0,1000,IF(BB5<0,1000,(IF(AN5>$E$1,1000,Z5))))","v":1000},{"$f":"IF(BQ34=0,1000,IF(BC5<0,1000,(IF(AO5>$E$1,1000,AA5))))","v":1000},{"$f":"IF(BR34=0,1000,IF(BD5<0,1000,(IF(AP5>$E$1,1000,AB5))))","v":1000}]
[null,2,{"$f":"'Profile calcs'!C5","v":87.14026715835297},{"$f":"'Profile calcs'!D5","v":76.943421516331355},{"$f":"'Profile calcs'!E5","v":65.3},{"$f":"'Profile calcs'!F5","v":51.816577532022961},{"$f":"'Profile calcs'!G5","v":42.36628329809723},{"$f":"'Profile calcs'!H5","v":39.16397217391814},{"$f":"'Profile calcs'!I5","v":42.596177753639978},{"$f":"'Profile calcs'!J5","v":51.698849875501857},{"$f":"'Profile calcs'!K5","v":65.300000000000011},{"$f":"'Profile calcs'!L5","v":77.869647984236934},{"$f":"'Profile calcs'!M5","v":88.340906011691416},{"$f":"'Profile calcs'!N5","v":-88.404315155295123},null,2,{"$f":"'Profile calcs'!AE5","v":66.172099329250003},{"$f":"'Profile calcs'!AF5","v":65.140511421698719},{"$f":"'Profile calcs'!AG5","v":61.409664244736142},{"$f":"'Profile calcs'!AH5","v":56.119428429528277},{"$f":"'Profile calcs'!AI5","v":52.806644981683391},{"$f":"'Profile calcs'!AJ5","v":53.071524478923379},{"$f":"'Profile calcs'!AK5","v":55.607487949913931},{"$f":"'Profile calcs'!AL5","v":57.058845303129395},{"$f":"'Profile calcs'!AM5","v":57.468525117430296},{"$f":"'Profile calcs'!AN5","v":57.976591294307511},{"$f":"'Profile calcs'!AO5","v":60.410283592762973},{"$f":"'Profile calcs'!AP5","v":63.926268100735683},null,{"$f":"'Operative BP'!B221","v":2},{"$f":"'Operative BP'!C221","v":62.979193205944796},{"$f":"'Operative BP'!D221","v":62.979193205944796},{"$f":"'Operative BP'!E221","v":69.979193205944796},{"$f":"'Operative BP'!F221","v":70.677541231422509},{"$f":"'Operative BP'!G221","v":69.979193205944796},{"$f":"'Operative BP'!H221","v":69.979193205944796},{"$f":"'Operative BP'!I221","v":69.979193205944796},{"$f":"'Operative BP'!J221","v":69.979193205944796},{"$f":"'Operative BP'!K221","v":69.979193205944796},{"$f":"'Operative BP'!L221","v":70.015948365180463},{"$f":"'Operative BP'!M221","v":69.979193205944796},{"$f":"'Operative BP'!N221","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B5","v":2},{"$f":"'Solar Altitude'!C5","v":-66.037221876299029},{"$f":"'Solar Altitude'!D5","v":-62.610262119735701},{"$f":"'Solar Altitude'!E5","v":-54.505603493104644},{"$f":"'Solar Altitude'!F5","v":-44.039138424385058},{"$f":"'Solar Altitude'!G5","v":-36.867903866984811},{"$f":"'Solar Altitude'!H5","v":-34.787290206430924},{"$f":"'Solar Altitude'!I5","v":-37.887883453111968},{"$f":"'Solar Altitude'!J5","v":-44.388788539159933},{"$f":"'Solar Altitude'!K5","v":-51.819137025254065},{"$f":"'Solar Altitude'!L5","v":-56.521775308526607},{"$f":"'Solar Altitude'!M5","v":-60.378308807607461},{"$f":"'Solar Altitude'!N5","v":-63.889653492857697},null,{"$f":"'Incident angle'!CK6","v":2},{"$f":"'Incident angle'!CL6","v":0},{"$f":"'Incident angle'!CM6","v":0},{"$f":"'Incident angle'!CN6","v":0},{"$f":"'Incident angle'!CO6","v":0},{"$f":"'Incident angle'!CP6","v":0},{"$f":"'Incident angle'!CQ6","v":0},{"$f":"'Incident angle'!CR6","v":0},{"$f":"'Incident angle'!CS6","v":0},{"$f":"'Incident angle'!CT6","v":0},{"$f":"'Incident angle'!CU6","v":0},{"$f":"'Incident angle'!CV6","v":0},{"$f":"'Incident angle'!CW6","v":0},null,{"$f":"'Incident angle'!CY6","v":2},{"$f":"'Incident angle'!CZ6","v":0},{"$f":"'Incident angle'!DA6","v":0},{"$f":"'Incident angle'!DB6","v":0},{"$f":"'Incident angle'!DC6","v":0},{"$f":"'Incident angle'!DD6","v":0},{"$f":"'Incident angle'!DE6","v":0},{"$f":"'Incident angle'!DF6","v":0},{"$f":"'Incident angle'!DG6","v":0},{"$f":"'Incident angle'!DH6","v":0},{"$f":"'Incident angle'!DI6","v":0},{"$f":"'Incident angle'!DJ6","v":0},{"$f":"'Incident angle'!DK6","v":0},null,null,2,{"$f":"IF(BG6=0,1000,IF(AS6<0,1000,(IF(AE6>$E$1,1000,C6))))","v":1000},1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,2,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,3,{"$f":"'Profile calcs'!C6","v":-89.27056077739023},{"$f":"'Profile calcs'!D6","v":78.978814169951136},{"$f":"'Profile calcs'!E6","v":65.300000000000011},{"$f":"'Profile calcs'!F6","v":49.102677830512903},{"$f":"'Profile calcs'!G6","v":38.0697107147043},{"$f":"'Profile calcs'!H6","v":34.68168355761518},{"$f":"'Profile calcs'!I6","v":38.712119041692716},{"$f":"'Profile calcs'!J6","v":49.05817483751602},{"$f":"'Profile calcs'!K6","v":65.300000000000011},{"$f":"'Profile calcs'!L6","v":80.804155317269903},{"$f":"'Profile calcs'!M6","v":-86.888190980331871},{"$f":"'Profile calcs'!N6","v":-83.771615174618546},null,3,{"$f":"'Profile calcs'!AE6","v":52.435166723015541},{"$f":"'Profile calcs'!AF6","v":50.544173289630855},{"$f":"'Profile calcs'!AG6","v":45.91935428010499},{"$f":"'Profile calcs'!AH6","v":39.682535750671363},{"$f":"'Profile calcs'!AI6","v":35.643149417229338},{"$f":"'Profile calcs'!AJ6","v":35.46488164814032},{"$f":"'Profile calcs'!AK6","v":38.162804391158723},{"$f":"'Profile calcs'!AL6","v":40.534175714629335},{"$f":"'Profile calcs'!AM6","v":42.164171017516502},{"$f":"'Profile calcs'!AN6","v":43.623401532687332},{"$f":"'Profile calcs'!AO6","v":46.805449667898792},{"$f":"'Profile calcs'!AP6","v":50.572582527440368},null,{"$f":"'Operative BP'!B222","v":3},{"$f":"'Operative BP'!C222","v":62.979193205944796},{"$f":"'Operative BP'!D222","v":62.979193205944796},{"$f":"'Operative BP'!E222","v":69.979193205944796},{"$f":"'Operative BP'!F222","v":70.925638556263266},{"$f":"'Operative BP'!G222","v":69.979193205944796},{"$f":"'Operative BP'!H222","v":69.979193205944796},{"$f":"'Operative BP'!I222","v":69.979193205944796},{"$f":"'Operative BP'!J222","v":69.979193205944796},{"$f":"'Operative BP'!K222","v":69.979193205944796},{"$f":"'Operative BP'!L222","v":70.388094352441613},{"$f":"'Operative BP'!M222","v":69.979193205944796},{"$f":"'Operative BP'!N222","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B6","v":3},{"$f":"'Solar Altitude'!C6","v":-52.431373562484438},{"$f":"'Solar Altitude'!D6","v":-49.776364898184575},{"$f":"'Solar Altitude'!E6","v":-43.00744408924087},{"$f":"'Solar Altitude'!F6","v":-33.970697614512481},{"$f":"'Solar Altitude'!G6","v":-27.874166624770901},{"$f":"'Solar Altitude'!H6","v":-26.397406240900974},{"$f":"'Solar Altitude'!I6","v":-29.298461575777225},{"$f":"'Solar Altitude'!J6","v":-34.480458721023354},{"$f":"'Solar Altitude'!K6","v":-39.89507498863518},{"$f":"'Solar Altitude'!L6","v":-43.286892300779471},{"$f":"'Solar Altitude'!M6","v":-46.757596903257479},{"$f":"'Solar Altitude'!N6","v":-50.32692672055552},null,{"$f":"'Incident angle'!CK7","v":3},{"$f":"'Incident angle'!CL7","v":0},{"$f":"'Incident angle'!CM7","v":0},{"$f":"'Incident angle'!CN7","v":0},{"$f":"'Incident angle'!CO7","v":0},{"$f":"'Incident angle'!CP7","v":0},{"$f":"'Incident angle'!CQ7","v":0},{"$f":"'Incident angle'!CR7","v":0},{"$f":"'Incident angle'!CS7","v":0},{"$f":"'Incident angle'!CT7","v":0},{"$f":"'Incident angle'!CU7","v":0},{"$f":"'Incident angle'!CV7","v":0},{"$f":"'Incident angle'!CW7","v":0},null,{"$f":"'Incident angle'!CY7","v":3},{"$f":"'Incident angle'!CZ7","v":0},{"$f":"'Incident angle'!DA7","v":0},{"$f":"'Incident angle'!DB7","v":0},{"$f":"'Incident angle'!DC7","v":0},{"$f":"'Incident angle'!DD7","v":0},{"$f":"'Incident angle'!DE7","v":0},{"$f":"'Incident angle'!DF7","v":0},{"$f":"'Incident angle'!DG7","v":0},{"$f":"'Incident angle'!DH7","v":0},{"$f":"'Incident angle'!DI7","v":0},{"$f":"'Incident angle'!DJ7","v":0},{"$f":"'Incident angle'!DK7","v":0},null,null,3,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,3,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,4,{"$f":"'Profile calcs'!C7","v":-82.17192424427256},{"$f":"'Profile calcs'!D7","v":83.262329332993176},{"$f":"'Profile calcs'!E7","v":65.300000000000011},{"$f":"'Profile calcs'!F7","v":43.339610901243866},{"$f":"'Profile calcs'!G7","v":29.580403720895195},{"$f":"'Profile calcs'!H7","v":26.101608463035426},{"$f":"'Profile calcs'!I7","v":31.06871667763788},{"$f":"'Profile calcs'!J7","v":43.484854535342002},{"$f":"'Profile calcs'!K7","v":65.300000000000011},{"$f":"'Profile calcs'!L7","v":87.267222857858812},{"$f":"'Profile calcs'!M7","v":-77.36591787164663},{"$f":"'Profile calcs'!N7","v":-74.90694041138012},null,4,{"$f":"'Profile calcs'!AE7","v":39.010190181198872},{"$f":"'Profile calcs'!AF7","v":36.428743475161504},{"$f":"'Profile calcs'!AG7","v":31.171654482760939},{"$f":"'Profile calcs'!AH7","v":24.400458127908184},{"$f":"'Profile calcs'!AI7","v":20.038723532033892},{"$f":"'Profile calcs'!AJ7","v":19.625868131864095},{"$f":"'Profile calcs'!AK7","v":22.320002033579943},{"$f":"'Profile calcs'!AL7","v":25.178501666912496},{"$f":"'Profile calcs'!AM7","v":27.591172995772343},{"$f":"'Profile calcs'!AN7","v":29.729656317315495},{"$f":"'Profile calcs'!AO7","v":33.493277499644961},{"$f":"'Profile calcs'!AP7","v":37.470732683841966},null,{"$f":"'Operative BP'!B223","v":4},{"$f":"'Operative BP'!C223","v":62.979193205944796},{"$f":"'Operative BP'!D223","v":62.979193205944796},{"$f":"'Operative BP'!E223","v":69.979193205944796},{"$f":"'Operative BP'!F223","v":71.256434989384289},{"$f":"'Operative BP'!G223","v":69.979193205944796},{"$f":"'Operative BP'!H223","v":69.979193205944796},{"$f":"'Operative BP'!I223","v":69.979193205944796},{"$f":"'Operative BP'!J223","v":69.979193205944796},{"$f":"'Operative BP'!K223","v":69.979193205944796},{"$f":"'Operative BP'!L223","v":70.553492569002117},{"$f":"'Operative BP'!M223","v":69.979193205944796},{"$f":"'Operative BP'!N223","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B7","v":4},{"$f":"'Solar Altitude'!C7","v":-38.837571781392398},{"$f":"'Solar Altitude'!D7","v":-36.325136967893741},{"$f":"'Solar Altitude'!E7","v":-30.23387910899125},{"$f":"'Solar Altitude'!F7","v":-22.236891602714234},{"$f":"'Solar Altitude'!G7","v":-17.058579195686843},{"$f":"'Solar Altitude'!H7","v":-16.082853037589089},{"$f":"'Solar Altitude'!I7","v":-18.740224973134019},{"$f":"'Solar Altitude'!J7","v":-22.841111056638525},{"$f":"'Solar Altitude'!K7","v":-26.935985833021629},{"$f":"'Solar Altitude'!L7","v":-29.720493919992279},{"$f":"'Solar Altitude'!M7","v":-33.206986937806654},{"$f":"'Solar Altitude'!N7","v":-36.893522726896833},null,{"$f":"'Incident angle'!CK8","v":4},{"$f":"'Incident angle'!CL8","v":0},{"$f":"'Incident angle'!CM8","v":0},{"$f":"'Incident angle'!CN8","v":0},{"$f":"'Incident angle'!CO8","v":0},{"$f":"'Incident angle'!CP8","v":0},{"$f":"'Incident angle'!CQ8","v":0},{"$f":"'Incident angle'!CR8","v":0},{"$f":"'Incident angle'!CS8","v":0},{"$f":"'Incident angle'!CT8","v":0},{"$f":"'Incident angle'!CU8","v":0},{"$f":"'Incident angle'!CV8","v":0},{"$f":"'Incident angle'!CW8","v":0},null,{"$f":"'Incident angle'!CY8","v":4},{"$f":"'Incident angle'!CZ8","v":0},{"$f":"'Incident angle'!DA8","v":0},{"$f":"'Incident angle'!DB8","v":0},{"$f":"'Incident angle'!DC8","v":0},{"$f":"'Incident angle'!DD8","v":0},{"$f":"'Incident angle'!DE8","v":0},{"$f":"'Incident angle'!DF8","v":0},{"$f":"'Incident angle'!DG8","v":0},{"$f":"'Incident angle'!DH8","v":0},{"$f":"'Incident angle'!DI8","v":0},{"$f":"'Incident angle'!DJ8","v":0},{"$f":"'Incident angle'!DK8","v":0},null,null,4,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,4,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,5,{"$f":"'Profile calcs'!C8","v":-67.497147561415503},{"$f":"'Profile calcs'!D8","v":-86.309432298850382},{"$f":"'Profile calcs'!E8","v":65.300000000000011},{"$f":"'Profile calcs'!F8","v":28.738866865290532},{"$f":"'Profile calcs'!G8","v":11.921747515833621},{"$f":"'Profile calcs'!H8","v":9.482202464658485},{"$f":"'Profile calcs'!I8","v":15.373504841898113},{"$f":"'Profile calcs'!J8","v":29.638177006237576},{"$f":"'Profile calcs'!K8","v":65.300000000000011},{"$f":"'Profile calcs'!L8","v":-74.528119824042165},{"$f":"'Profile calcs'!M8","v":-57.19996124585586},{"$f":"'Profile calcs'!N8","v":-57.733947337338257},null,5,{"$f":"'Profile calcs'!AE8","v":25.815859178831762},{"$f":"'Profile calcs'!AF8","v":22.717824490126432},{"$f":"'Profile calcs'!AG8","v":17.054801329090406},{"$f":"'Profile calcs'!AH8","v":10.060267103118706},{"$f":"'Profile calcs'!AI8","v":5.6553451463568241},{"$f":"'Profile calcs'!AJ8","v":5.1651785422524581},{"$f":"'Profile calcs'!AK8","v":7.7705114298265903},{"$f":"'Profile calcs'!AL8","v":10.788309881886676},{"$f":"'Profile calcs'!AM8","v":13.597367832295642},{"$f":"'Profile calcs'!AN8","v":16.153367731431349},{"$f":"'Profile calcs'!AO8","v":20.343596801848918},{"$f":"'Profile calcs'!AP8","v":24.514554175011252},null,{"$f":"'Operative BP'!B224","v":5},{"$f":"'Operative BP'!C224","v":62.979193205944796},{"$f":"'Operative BP'!D224","v":62.979193205944796},{"$f":"'Operative BP'!E224","v":62.979193205944796},{"$f":"'Operative BP'!F224","v":71.50453231422506},{"$f":"'Operative BP'!G224","v":69.979193205944796},{"$f":"'Operative BP'!H224","v":69.979193205944796},{"$f":"'Operative BP'!I224","v":69.979193205944796},{"$f":"'Operative BP'!J224","v":69.979193205944796},{"$f":"'Operative BP'!K224","v":69.979193205944796},{"$f":"'Operative BP'!L224","v":70.88428900212314},{"$f":"'Operative BP'!M224","v":62.979193205944796},{"$f":"'Operative BP'!N224","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B8","v":5},{"$f":"'Solar Altitude'!C8","v":-25.376333918471747},{"$f":"'Solar Altitude'!D8","v":-22.7103856061896},{"$f":"'Solar Altitude'!E8","v":-16.897092448538263},{"$f":"'Solar Altitude'!F8","v":-9.5810693067706811},{"$f":"'Solar Altitude'!G8","v":-5.1231262317655331},{"$f":"'Solar Altitude'!H8","v":-4.54535827775074},{"$f":"'Solar Altitude'!I8","v":-6.9688312964780383},{"$f":"'Solar Altitude'!J8","v":-10.241982624949756},{"$f":"'Solar Altitude'!K8","v":-13.517063375335365},{"$f":"'Solar Altitude'!L8","v":-16.104385171900024},{"$f":"'Solar Altitude'!M8","v":-19.830528453312528},{"$f":"'Solar Altitude'!N8","v":-23.664530366970006},null,{"$f":"'Incident angle'!CK9","v":5},{"$f":"'Incident angle'!CL9","v":0},{"$f":"'Incident angle'!CM9","v":0},{"$f":"'Incident angle'!CN9","v":0},{"$f":"'Incident angle'!CO9","v":0},{"$f":"'Incident angle'!CP9","v":0},{"$f":"'Incident angle'!CQ9","v":0},{"$f":"'Incident angle'!CR9","v":0},{"$f":"'Incident angle'!CS9","v":0},{"$f":"'Incident angle'!CT9","v":0},{"$f":"'Incident angle'!CU9","v":0},{"$f":"'Incident angle'!CV9","v":0},{"$f":"'Incident angle'!CW9","v":0},null,{"$f":"'Incident angle'!CY9","v":5},{"$f":"'Incident angle'!CZ9","v":0},{"$f":"'Incident angle'!DA9","v":0},{"$f":"'Incident angle'!DB9","v":0},{"$f":"'Incident angle'!DC9","v":0},{"$f":"'Incident angle'!DD9","v":0},{"$f":"'Incident angle'!DE9","v":0},{"$f":"'Incident angle'!DF9","v":0},{"$f":"'Incident angle'!DG9","v":0},{"$f":"'Incident angle'!DH9","v":0},{"$f":"'Incident angle'!DI9","v":0},{"$f":"'Incident angle'!DJ9","v":0},{"$f":"'Incident angle'!DK9","v":0},null,null,5,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,5,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,6,{"$f":"'Profile calcs'!C9","v":-37.148186571308401},{"$f":"'Profile calcs'!D9","v":-50.791383654081223},{"$f":"'Profile calcs'!E9","v":65.300000000000054},{"$f":"'Profile calcs'!F9","v":-17.580147546281751},{"$f":"'Profile calcs'!G9","v":-22.111172344820318},{"$f":"'Profile calcs'!H9","v":-19.795090464953187},{"$f":"'Profile calcs'!I9","v":-15.860431327653474},{"$f":"'Profile calcs'!J9","v":-13.722280285934321},{"$f":"'Profile calcs'!K9","v":65.300000000001162},{"$f":"'Profile calcs'!L9","v":-13.894791408071965},{"$f":"'Profile calcs'!M9","v":-20.106401019882362},{"$f":"'Profile calcs'!N9","v":-27.88546048481528},null,6,{"$f":"'Profile calcs'!AE9","v":12.657580240548544},{"$f":"'Profile calcs'!AF9","v":9.2101030414712177},{"$f":"'Profile calcs'!AG9","v":3.3244141005449075},{"$f":"'Profile calcs'!AH9","v":-3.6714405326866673},{"$f":"'Profile calcs'!AI9","v":-7.9357874829851545},{"$f":"'Profile calcs'!AJ9","v":-8.3930552361023505},{"$f":"'Profile calcs'!AK9","v":-5.9138516774857015},{"$f":"'Profile calcs'!AL9","v":-2.9679829754440075},{"$f":"'Profile calcs'!AM9","v":-8.3279928680461496E-2},{"$f":"'Profile calcs'!AN9","v":2.64655398169262},{"$f":"'Profile calcs'!AO9","v":7.1190871836640657},{"$f":"'Profile calcs'!AP9","v":11.488991114943707},null,{"$f":"'Operative BP'!B225","v":6},{"$f":"'Operative BP'!C225","v":62.979193205944796},{"$f":"'Operative BP'!D225","v":62.979193205944796},{"$f":"'Operative BP'!E225","v":62.979193205944796},{"$f":"'Operative BP'!F225","v":71.508965671756357},{"$f":"'Operative BP'!G225","v":68.728733897373488},{"$f":"'Operative BP'!H225","v":69.528725672975227},{"$f":"'Operative BP'!I225","v":69.693163554430129},{"$f":"'Operative BP'!J225","v":69.817863494408968},{"$f":"'Operative BP'!K225","v":68.806892038234452},{"$f":"'Operative BP'!L225","v":71.091036772823784},{"$f":"'Operative BP'!M225","v":62.979193205944796},{"$f":"'Operative BP'!N225","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B9","v":6},{"$f":"'Solar Altitude'!C9","v":-12.151444093159176},{"$f":"'Solar Altitude'!D9","v":-9.1319080559186769},{"$f":"'Solar Altitude'!E9","v":-3.3232309033445411},{"$f":"'Solar Altitude'!F9","v":3.5985816694690373},{"$f":"'Solar Altitude'!G9","v":7.5112987220277185},{"$f":"'Solar Altitude'!H9","v":7.7738597839019823},{"$f":"'Solar Altitude'!I9","v":5.5584053941199079},{"$f":"'Solar Altitude'!J9","v":2.9033723023449274},{"$f":"'Solar Altitude'!K9","v":8.3279910069695443E-2},{"$f":"'Solar Altitude'!L9","v":-2.6015900354108483},{"$f":"'Solar Altitude'!M9","v":-6.7413522567651629},{"$f":"'Solar Altitude'!N9","v":-10.743396255327719},null,{"$f":"'Incident angle'!CK10","v":6},{"$f":"'Incident angle'!CL10","v":0},{"$f":"'Incident angle'!CM10","v":0},{"$f":"'Incident angle'!CN10","v":0},{"$f":"'Incident angle'!CO10","v":0},{"$f":"'Incident angle'!CP10","v":0},{"$f":"'Incident angle'!CQ10","v":0},{"$f":"'Incident angle'!CR10","v":0},{"$f":"'Incident angle'!CS10","v":0},{"$f":"'Incident angle'!CT10","v":0},{"$f":"'Incident angle'!CU10","v":0},{"$f":"'Incident angle'!CV10","v":0},{"$f":"'Incident angle'!CW10","v":0},null,{"$f":"'Incident angle'!CY10","v":6},{"$f":"'Incident angle'!CZ10","v":0},{"$f":"'Incident angle'!DA10","v":0},{"$f":"'Incident angle'!DB10","v":0},{"$f":"'Incident angle'!DC10","v":1},{"$f":"'Incident angle'!DD10","v":1},{"$f":"'Incident angle'!DE10","v":1},{"$f":"'Incident angle'!DF10","v":1},{"$f":"'Incident angle'!DG10","v":1},{"$f":"'Incident angle'!DH10","v":1},{"$f":"'Incident angle'!DI10","v":0},{"$f":"'Incident angle'!DJ10","v":0},{"$f":"'Incident angle'!DK10","v":0},null,null,6,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,6,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,7,{"$f":"'Profile calcs'!C10","v":1.8407058775768048},{"$f":"'Profile calcs'!D10","v":17.418156461309621},{"$f":"'Profile calcs'!E10","v":65.299999999999969},{"$f":"'Profile calcs'!F10","v":-72.609902347589838},{"$f":"'Profile calcs'!G10","v":-57.961158312930344},{"$f":"'Profile calcs'!H10","v":-51.874170400534652},{"$f":"'Profile calcs'!I10","v":-53.106981432720829},{"$f":"'Profile calcs'!J10","v":-70.235558391915404},{"$f":"'Profile calcs'!K10","v":65.3},{"$f":"'Profile calcs'!L10","v":32.525623758734746},{"$f":"'Profile calcs'!M10","v":13.689263813478037},{"$f":"'Profile calcs'!N10","v":3.7902225360911945},null,7,{"$f":"'Profile calcs'!AE10","v":-0.75712395765969032},{"$f":"'Profile calcs'!AF10","v":-4.3819211908166711},{"$f":"'Profile calcs'!AG10","v":-10.327408658619172},{"$f":"'Profile calcs'!AH10","v":-17.146626992599682},{"$f":"'Profile calcs'!AI10","v":-21.134165658355119},{"$f":"'Profile calcs'!AJ10","v":-21.477097073214686},{"$f":"'Profile calcs'!AK10","v":-19.142999224755304},{"$f":"'Profile calcs'!AL10","v":-16.444109273248728},{"$f":"'Profile calcs'!AM10","v":-13.765898970431955},{"$f":"'Profile calcs'!AN10","v":-11.107118463724456},{"$f":"'Profile calcs'!AO10","v":-6.5087495886135249},{"$f":"'Profile calcs'!AP10","v":-1.9226157929385757},null,{"$f":"'Operative BP'!B226","v":7},{"$f":"'Operative BP'!C226","v":62.856714294401563},{"$f":"'Operative BP'!D226","v":62.667031336996473},{"$f":"'Operative BP'!E226","v":62.078596779005807},{"$f":"'Operative BP'!F226","v":68.557294103745818},{"$f":"'Operative BP'!G226","v":66.537756321294182},{"$f":"'Operative BP'!H226","v":66.26545548330833},{"$f":"'Operative BP'!I226","v":66.89727868181231},{"$f":"'Operative BP'!J226","v":67.218672334952231},{"$f":"'Operative BP'!K226","v":67.653726998539284},{"$f":"'Operative BP'!L226","v":69.399567242025},{"$f":"'Operative BP'!M226","v":62.535788720614789},{"$f":"'Operative BP'!N226","v":62.794452031025394},null,{"$f":"'Solar Altitude'!B10","v":7},{"$f":"'Solar Altitude'!C10","v":0.70023973357815916},{"$f":"'Solar Altitude'!D10","v":4.2572512510716702},{"$f":"'Solar Altitude'!E10","v":10.292097151668541},{"$f":"'Solar Altitude'!F10","v":17.071764306110264},{"$f":"'Solar Altitude'!G10","v":20.59199880999245},{"$f":"'Solar Altitude'!H10","v":20.602944398333847},{"$f":"'Solar Altitude'!I10","v":18.567526961418682},{"$f":"'Solar Altitude'!J10","v":16.357318748220177},{"$f":"'Solar Altitude'!K10","v":13.682588857300253},{"$f":"'Solar Altitude'!L10","v":10.626902061270702},{"$f":"'Solar Altitude'!M10","v":5.8987575020687171},{"$f":"'Solar Altitude'!N10","v":1.7151458456731048},null,{"$f":"'Incident angle'!CK11","v":7},{"$f":"'Incident angle'!CL11","v":0},{"$f":"'Incident angle'!CM11","v":0},{"$f":"'Incident angle'!CN11","v":0},{"$f":"'Incident angle'!CO11","v":0},{"$f":"'Incident angle'!CP11","v":0},{"$f":"'Incident angle'!CQ11","v":0},{"$f":"'Incident angle'!CR11","v":0},{"$f":"'Incident angle'!CS11","v":0},{"$f":"'Incident angle'!CT11","v":0},{"$f":"'Incident angle'!CU11","v":0},{"$f":"'Incident angle'!CV11","v":0},{"$f":"'Incident angle'!CW11","v":1.5519142582101374E-2},null,{"$f":"'Incident angle'!CY11","v":7},{"$f":"'Incident angle'!CZ11","v":1},{"$f":"'Incident angle'!DA11","v":1},{"$f":"'Incident angle'!DB11","v":1},{"$f":"'Incident angle'!DC11","v":1},{"$f":"'Incident angle'!DD11","v":1},{"$f":"'Incident angle'!DE11","v":1},{"$f":"'Incident angle'!DF11","v":1},{"$f":"'Incident angle'!DG11","v":1},{"$f":"'Incident angle'!DH11","v":1},{"$f":"'Incident angle'!DI11","v":1},{"$f":"'Incident angle'!DJ11","v":1},{"$f":"'Incident angle'!DK11","v":0.9844808574178987},null,null,7,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,7,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,8,{"$f":"'Profile calcs'!C11","v":25.154979301423634},{"$f":"'Profile calcs'!D11","v":41.208162613283584},{"$f":"'Profile calcs'!E11","v":65.300000000000011},{"$f":"'Profile calcs'!F11","v":89.133910589679402},{"$f":"'Profile calcs'!G11","v":-77.392469719775818},{"$f":"'Profile calcs'!H11","v":-71.837796305169576},{"$f":"'Profile calcs'!I11","v":-74.903067121246494},{"$f":"'Profile calcs'!J11","v":-89.880701812612713},{"$f":"'Profile calcs'!K11","v":65.3},{"$f":"'Profile calcs'!L11","v":45.709102960920774},{"$f":"'Profile calcs'!M11","v":30.711991515210524},{"$f":"'Profile calcs'!N11","v":23.133349654536577},null,8,{"$f":"'Profile calcs'!AE11","v":-14.801512993977905},{"$f":"'Profile calcs'!AF11","v":-18.395161326018538},{"$f":"'Profile calcs'!AG11","v":-24.21988645529855},{"$f":"'Profile calcs'!AH11","v":-30.680730702005945},{"$f":"'Profile calcs'!AI11","v":-34.26512345162336},{"$f":"'Profile calcs'!AJ11","v":-34.426376431243654},{"$f":"'Profile calcs'!AK11","v":-32.256035415094608},{"$f":"'Profile calcs'!AL11","v":-29.958921059436694},{"$f":"'Profile calcs'!AM11","v":-27.765335603992927},{"$f":"'Profile calcs'!AN11","v":-25.454349023394595},{"$f":"'Profile calcs'!AO11","v":-20.939346821539349},{"$f":"'Profile calcs'!AP11","v":-16.129552534651118},null,{"$f":"'Operative BP'!B227","v":8},{"$f":"'Operative BP'!C227","v":60.636012287006743},{"$f":"'Operative BP'!D227","v":59.996852114891453},{"$f":"'Operative BP'!E227","v":65.687131489350378},{"$f":"'Operative BP'!F227","v":64.001054133397986},{"$f":"'Operative BP'!G227","v":63.505800104568934},{"$f":"'Operative BP'!H227","v":63.139041486907033},{"$f":"'Operative BP'!I227","v":63.362443210032374},{"$f":"'Operative BP'!J227","v":62.993641147864963},{"$f":"'Operative BP'!K227","v":63.853362851174566},{"$f":"'Operative BP'!L227","v":65.088569988960913},{"$f":"'Operative BP'!M227","v":66.344410694354679},{"$f":"'Operative BP'!N227","v":60.510075256014446},null,{"$f":"'Solar Altitude'!B11","v":8},{"$f":"'Solar Altitude'!C11","v":12.968359542715392},{"$f":"'Solar Altitude'!D11","v":17.270303982095768},{"$f":"'Solar Altitude'!E11","v":23.773745192987032},{"$f":"'Solar Altitude'!F11","v":30.67971943621767},{"$f":"'Solar Altitude'!G11","v":33.959814353189685},{"$f":"'Solar Altitude'!H11","v":33.770494749028082},{"$f":"'Solar Altitude'!I11","v":31.887744015481577},{"$f":"'Solar Altitude'!J11","v":29.958903207045175},{"$f":"'Solar Altitude'!K11","v":27.097900221004789},{"$f":"'Solar Altitude'!L11","v":23.350930400204959},{"$f":"'Solar Altitude'!M11","v":17.832347455280527},{"$f":"'Solar Altitude'!N11","v":13.467847656409182},null,{"$f":"'Incident angle'!CK12","v":8},{"$f":"'Incident angle'!CL12","v":0.10253062539393309},{"$f":"'Incident angle'!CM12","v":0},{"$f":"'Incident angle'!CN12","v":0},{"$f":"'Incident angle'!CO12","v":0},{"$f":"'Incident angle'!CP12","v":0},{"$f":"'Incident angle'!CQ12","v":0},{"$f":"'Incident angle'!CR12","v":0},{"$f":"'Incident angle'!CS12","v":0},{"$f":"'Incident angle'!CT12","v":0},{"$f":"'Incident angle'!CU12","v":0},{"$f":"'Incident angle'!CV12","v":0.18911868168998328},{"$f":"'Incident angle'!CW12","v":0.23774110917257671},null,{"$f":"'Incident angle'!CY12","v":8},{"$f":"'Incident angle'!CZ12","v":0.89746937460606691},{"$f":"'Incident angle'!DA12","v":1},{"$f":"'Incident angle'!DB12","v":1},{"$f":"'Incident angle'!DC12","v":1},{"$f":"'Incident angle'!DD12","v":1},{"$f":"'Incident angle'!DE12","v":1},{"$f":"'Incident angle'!DF12","v":1},{"$f":"'Incident angle'!DG12","v":1},{"$f":"'Incident angle'!DH12","v":1},{"$f":"'Incident angle'!DI12","v":1},{"$f":"'Incident angle'!DJ12","v":0.81088131831001664},{"$f":"'Incident angle'!DK12","v":0.76225889082742337},null,null,8,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,8,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,9,{"$f":"'Profile calcs'!C12","v":36.123628972409719},{"$f":"'Profile calcs'!D12","v":48.984103271498903},{"$f":"'Profile calcs'!E12","v":65.3},{"$f":"'Profile calcs'!F12","v":82.323917470741151},{"$f":"'Profile calcs'!G12","v":-86.682219236973438},{"$f":"'Profile calcs'!H12","v":-82.177260396790928},{"$f":"'Profile calcs'!I12","v":-85.346370921243249},{"$f":"'Profile calcs'!J12","v":82.868918499232819},{"$f":"'Profile calcs'!K12","v":65.300000000000011},{"$f":"'Profile calcs'!L12","v":50.828908694033096},{"$f":"'Profile calcs'!M12","v":38.841664176975662},{"$f":"'Profile calcs'!N12","v":33.137728896941795},null,9,{"$f":"'Profile calcs'!AE12","v":-29.897860503845664},{"$f":"'Profile calcs'!AF12","v":-33.171578582642681},{"$f":"'Profile calcs'!AG12","v":-38.635878844024361},{"$f":"'Profile calcs'!AH12","v":-44.516730121969097},{"$f":"'Profile calcs'!AI12","v":-47.561101053580373},{"$f":"'Profile calcs'!AJ12","v":-47.480410935356453},{"$f":"'Profile calcs'!AK12","v":-45.501067907501131},{"$f":"'Profile calcs'!AL12","v":-43.760303315048105},{"$f":"'Profile calcs'!AM12","v":-42.346663637257642},{"$f":"'Profile calcs'!AN12","v":-40.715743852069998},{"$f":"'Profile calcs'!AO12","v":-36.595216615504739},{"$f":"'Profile calcs'!AP12","v":-31.603785496296783},null,{"$f":"'Operative BP'!B228","v":9},{"$f":"'Operative BP'!C228","v":57.790747816331709},{"$f":"'Operative BP'!D228","v":58.189752038078609},{"$f":"'Operative BP'!E228","v":64.483529462678931},{"$f":"'Operative BP'!F228","v":63.177850689832482},{"$f":"'Operative BP'!G228","v":63.939107663566489},{"$f":"'Operative BP'!H228","v":63.556488212857914},{"$f":"'Operative BP'!I228","v":62.956925711956146},{"$f":"'Operative BP'!J228","v":62.758459334604439},{"$f":"'Operative BP'!K228","v":63.648996727151385},{"$f":"'Operative BP'!L228","v":63.384381281673647},{"$f":"'Operative BP'!M228","v":65.613423635929152},{"$f":"'Operative BP'!N228","v":58.544971452619734},null,{"$f":"'Solar Altitude'!B12","v":9},{"$f":"'Solar Altitude'!C12","v":24.306538235547787},{"$f":"'Solar Altitude'!D12","v":29.607456719563572},{"$f":"'Solar Altitude'!E12","v":36.877998514340362},{"$f":"'Solar Altitude'!F12","v":44.267398869292073},{"$f":"'Solar Altitude'!G12","v":47.503865138538167},{"$f":"'Solar Altitude'!H12","v":47.16345799134892},{"$f":"'Solar Altitude'!I12","v":45.403126432581416},{"$f":"'Solar Altitude'!J12","v":43.556385601632783},{"$f":"'Solar Altitude'!K12","v":40.048756889246128},{"$f":"'Solar Altitude'!L12","v":35.170537312656599},{"$f":"'Solar Altitude'!M12","v":28.628753160625717},{"$f":"'Solar Altitude'!N12","v":24.120985503613159},null,{"$f":"'Incident angle'!CK13","v":9},{"$f":"'Incident angle'!CL13","v":0.29516566816527884},{"$f":"'Incident angle'!CM13","v":4.6734913561712568E-2},{"$f":"'Incident angle'!CN13","v":0},{"$f":"'Incident angle'!CO13","v":0},{"$f":"'Incident angle'!CP13","v":0},{"$f":"'Incident angle'!CQ13","v":0},{"$f":"'Incident angle'!CR13","v":0},{"$f":"'Incident angle'!CS13","v":0},{"$f":"'Incident angle'!CT13","v":0},{"$f":"'Incident angle'!CU13","v":0.10656628908117825},{"$f":"'Incident angle'!CV13","v":0.38138128584091358},{"$f":"'Incident angle'!CW13","v":0.40841404978611101},null,{"$f":"'Incident angle'!CY13","v":9},{"$f":"'Incident angle'!CZ13","v":0.70483433183472122},{"$f":"'Incident angle'!DA13","v":0.95326508643828756},{"$f":"'Incident angle'!DB13","v":1},{"$f":"'Incident angle'!DC13","v":1},{"$f":"'Incident angle'!DD13","v":1},{"$f":"'Incident angle'!DE13","v":1},{"$f":"'Incident angle'!DF13","v":1},{"$f":"'Incident angle'!DG13","v":1},{"$f":"'Incident angle'!DH13","v":1},{"$f":"'Incident angle'!DI13","v":0.89343371091882173},{"$f":"'Incident angle'!DJ13","v":0.61861871415908642},{"$f":"'Incident angle'!DK13","v":0.59158595021388904},null,null,9,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,9,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,10,{"$f":"'Profile calcs'!C13","v":41.565533524141749},{"$f":"'Profile calcs'!D13","v":52.391449411165148},{"$f":"'Profile calcs'!E13","v":65.3},{"$f":"'Profile calcs'!F13","v":79.183835184665355},{"$f":"'Profile calcs'!G13","v":88.633552185609801},{"$f":"'Profile calcs'!H13","v":-87.576455047188773},{"$f":"'Profile calcs'!I13","v":89.408737808154712},{"$f":"'Profile calcs'!J13","v":79.54425546635963},{"$f":"'Profile calcs'!K13","v":65.3},{"$f":"'Profile calcs'!L13","v":53.228063715971984},{"$f":"'Profile calcs'!M13","v":42.944409695388977},{"$f":"'Profile calcs'!N13","v":38.364397938009645},null,10,{"$f":"'Profile calcs'!AE13","v":-46.432009669114628},{"$f":"'Profile calcs'!AF13","v":-48.98210838098047},{"$f":"'Profile calcs'!AG13","v":-53.761437623792659},{"$f":"'Profile calcs'!AH13","v":-58.790214649196756},{"$f":"'Profile calcs'!AI13","v":-61.14667544282198},{"$f":"'Profile calcs'!AJ13","v":-60.771492120895445},{"$f":"'Profile calcs'!AK13","v":-59.020595594487986},{"$f":"'Profile calcs'!AL13","v":-57.990814089298965},{"$f":"'Profile calcs'!AM13","v":-57.660184602658042},{"$f":"'Profile calcs'!AN13","v":-57.085561042213271},{"$f":"'Profile calcs'!AO13","v":-53.797693072162787},{"$f":"'Profile calcs'!AP13","v":-48.774894172678053},null,{"$f":"'Operative BP'!B229","v":10},{"$f":"'Operative BP'!C229","v":57.902045472522239},{"$f":"'Operative BP'!D229","v":66.559009996875588},{"$f":"'Operative BP'!E229","v":69.335027521318807},{"$f":"'Operative BP'!F229","v":69.795053985102271},{"$f":"'Operative BP'!G229","v":69.979193205944796},{"$f":"'Operative BP'!H229","v":69.979193205944796},{"$f":"'Operative BP'!I229","v":69.963287962183657},{"$f":"'Operative BP'!J229","v":69.122081637656436},{"$f":"'Operative BP'!K229","v":69.160968264645888},{"$f":"'Operative BP'!L229","v":68.55798942701972},{"$f":"'Operative BP'!M229","v":65.97149083553532},{"$f":"'Operative BP'!N229","v":58.56278759189361},null,{"$f":"'Solar Altitude'!B13","v":10},{"$f":"'Solar Altitude'!C13","v":34.130498638110296},{"$f":"'Solar Altitude'!D13","v":40.716949463115029},{"$f":"'Solar Altitude'!E13","v":49.130640449349286},{"$f":"'Solar Altitude'!F13","v":57.573642107854539},{"$f":"'Solar Altitude'!G13","v":61.123995517612983},{"$f":"'Solar Altitude'!H13","v":60.701791836412639},{"$f":"'Solar Altitude'!I13","v":59.016860616830343},{"$f":"'Solar Altitude'!J13","v":56.905164678924855},{"$f":"'Solar Altitude'!K13","v":51.954064465377563},{"$f":"'Solar Altitude'!L13","v":45.326184070335216},{"$f":"'Solar Altitude'!M13","v":37.566870997040184},{"$f":"'Solar Altitude'!N13","v":33.04159126014769},null,{"$f":"'Incident angle'!CK14","v":10},{"$f":"'Incident angle'!CL14","v":0.56002314416060595},{"$f":"'Incident angle'!CM14","v":0.17372244019094327},{"$f":"'Incident angle'!CN14","v":0},{"$f":"'Incident angle'!CO14","v":0},{"$f":"'Incident angle'!CP14","v":0},{"$f":"'Incident angle'!CQ14","v":0},{"$f":"'Incident angle'!CR14","v":0},{"$f":"'Incident angle'!CS14","v":0},{"$f":"'Incident angle'!CT14","v":0},{"$f":"'Incident angle'!CU14","v":0.51768444424225513},{"$f":"'Incident angle'!CV14","v":0.81214878868617979},{"$f":"'Incident angle'!CW14","v":0.74703498311093197},null,{"$f":"'Incident angle'!CY14","v":10},{"$f":"'Incident angle'!CZ14","v":0.439976855839394},{"$f":"'Incident angle'!DA14","v":0.82627755980905682},{"$f":"'Incident angle'!DB14","v":1},{"$f":"'Incident angle'!DC14","v":1},{"$f":"'Incident angle'!DD14","v":0},{"$f":"'Incident angle'!DE14","v":0},{"$f":"'Incident angle'!DF14","v":1},{"$f":"'Incident angle'!DG14","v":1},{"$f":"'Incident angle'!DH14","v":1},{"$f":"'Incident angle'!DI14","v":0.48231555575774493},{"$f":"'Incident angle'!DJ14","v":0.18785121131382015},{"$f":"'Incident angle'!DK14","v":0.25296501688906803},null,null,10,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,10,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,11,{"$f":"'Profile calcs'!C14","v":44.282217904128672},{"$f":"'Profile calcs'!D14","v":54.018451059115115},{"$f":"'Profile calcs'!E14","v":65.300000000000011},{"$f":"'Profile calcs'!F14","v":77.69612062717222},{"$f":"'Profile calcs'!G14","v":86.343646743656691},{"$f":"'Profile calcs'!H14","v":89.714212091310287},{"$f":"'Profile calcs'!I14","v":86.798330968762983},{"$f":"'Profile calcs'!J14","v":77.960826272965903},{"$f":"'Profile calcs'!K14","v":65.300000000000011},{"$f":"'Profile calcs'!L14","v":54.328164209664372},{"$f":"'Profile calcs'!M14","v":44.893647845797645},{"$f":"'Profile calcs'!N14","v":40.97067975660989},null,11,{"$f":"'Profile calcs'!AE14","v":-64.562443951008902},{"$f":"'Profile calcs'!AF14","v":-65.901314539685401},{"$f":"'Profile calcs'!AG14","v":-69.61109114186894},{"$f":"'Profile calcs'!AH14","v":-73.497168133288227},{"$f":"'Profile calcs'!AI14","v":-75.027677809677201},{"$f":"'Profile calcs'!AJ14","v":-74.319781349482838},{"$f":"'Profile calcs'!AK14","v":-72.839713407261911},{"$f":"'Profile calcs'!AL14","v":-72.655436766674285},{"$f":"'Profile calcs'!AM14","v":-73.666960034724269},{"$f":"'Profile calcs'!AN14","v":-74.489845422408848},{"$f":"'Profile calcs'!AO14","v":-72.529904986775534},{"$f":"'Profile calcs'!AP14","v":-67.776371428052769},null,{"$f":"'Operative BP'!B230","v":11},{"$f":"'Operative BP'!C230","v":58.94591794194146},{"$f":"'Operative BP'!D230","v":69.514570358791829},{"$f":"'Operative BP'!E230","v":71.132386326963911},{"$f":"'Operative BP'!F230","v":69.979193205944796},{"$f":"'Operative BP'!G230","v":69.979193205944796},{"$f":"'Operative BP'!H230","v":69.979193205944796},{"$f":"'Operative BP'!I230","v":69.979193205944796},{"$f":"'Operative BP'!J230","v":69.979193205944796},{"$f":"'Operative BP'!K230","v":69.979193205944796},{"$f":"'Operative BP'!L230","v":69.49871550800458},{"$f":"'Operative BP'!M230","v":64.691347545134462},{"$f":"'Operative BP'!N230","v":65.356538962096309},null,{"$f":"'Solar Altitude'!B14","v":11},{"$f":"'Solar Altitude'!C14","v":41.499338482119107},{"$f":"'Solar Altitude'!D14","v":49.543356395157261},{"$f":"'Solar Altitude'!E14","v":59.402009530792824},{"$f":"'Solar Altitude'!F14","v":69.801829865076741},{"$f":"'Solar Altitude'!G14","v":74.625870049112294},{"$f":"'Solar Altitude'!H14","v":74.317427946135254},{"$f":"'Solar Altitude'!I14","v":72.577202871970812},{"$f":"'Solar Altitude'!J14","v":69.283885987295108},{"$f":"'Solar Altitude'!K14","v":61.393251168859464},{"$f":"'Solar Altitude'!L14","v":52.417946997507137},{"$f":"'Solar Altitude'!M14","v":43.550952586854685},{"$f":"'Solar Altitude'!N14","v":39.297011346471983},null,{"$f":"'Incident angle'!CK15","v":11},{"$f":"'Incident angle'!CL15","v":1},{"$f":"'Incident angle'!CM15","v":1},{"$f":"'Incident angle'!CN15","v":0},{"$f":"'Incident angle'!CO15","v":0},{"$f":"'Incident angle'!CP15","v":0},{"$f":"'Incident angle'!CQ15","v":0},{"$f":"'Incident angle'!CR15","v":0},{"$f":"'Incident angle'!CS15","v":0},{"$f":"'Incident angle'!CT15","v":0},{"$f":"'Incident angle'!CU15","v":1},{"$f":"'Incident angle'!CV15","v":1},{"$f":"'Incident angle'!CW15","v":1},null,{"$f":"'Incident angle'!CY15","v":11},{"$f":"'Incident angle'!CZ15","v":0},{"$f":"'Incident angle'!DA15","v":0},{"$f":"'Incident angle'!DB15","v":0},{"$f":"'Incident angle'!DC15","v":0},{"$f":"'Incident angle'!DD15","v":0},{"$f":"'Incident angle'!DE15","v":0},{"$f":"'Incident angle'!DF15","v":0},{"$f":"'Incident angle'!DG15","v":0},{"$f":"'Incident angle'!DH15","v":0},{"$f":"'Incident angle'!DI15","v":0},{"$f":"'Incident angle'!DJ15","v":0},{"$f":"'Incident angle'!DK15","v":0},null,null,11,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,11,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,12,{"$f":"'Profile calcs'!C15","v":45.341192522261665},{"$f":"'Profile calcs'!D15","v":54.65622400407787},{"$f":"'Profile calcs'!E15","v":65.300000000000011},{"$f":"'Profile calcs'!F15","v":77.204007036944958},{"$f":"'Profile calcs'!G15","v":85.602608099870324},{"$f":"'Profile calcs'!H15","v":88.764506326073786},{"$f":"'Profile calcs'!I15","v":85.831844934745362},{"$f":"'Profile calcs'!J15","v":77.410166839433359},{"$f":"'Profile calcs'!K15","v":65.3},{"$f":"'Profile calcs'!L15","v":54.593196533889113},{"$f":"'Profile calcs'!M15","v":45.392239295822165},{"$f":"'Profile calcs'!N15","v":41.843902161818413},null,12,{"$f":"'Profile calcs'!AE15","v":-83.95305525324396},{"$f":"'Profile calcs'!AF15","v":-83.672477687445479},{"$f":"'Profile calcs'!AG15","v":-85.9744082667399},{"$f":"'Profile calcs'!AH15","v":-88.486518830478445},{"$f":"'Profile calcs'!AI15","v":-89.098541577633242},{"$f":"'Profile calcs'!AJ15","v":-88.042480487312574},{"$f":"'Profile calcs'!AK15","v":-86.869712514125027},{"$f":"'Profile calcs'!AL15","v":-87.612299057311645},{"$f":"'Profile calcs'!AM15","v":-89.899102008780474},{"$f":"'Profile calcs'!AN15","v":-87.509028766495277},{"$f":"'Profile calcs'!AO15","v":-87.799307231125709},{"$f":"'Profile calcs'!AP15","v":-88.098042556805254},null,{"$f":"'Operative BP'!B231","v":12},{"$f":"'Operative BP'!C231","v":64.957687352607891},{"$f":"'Operative BP'!D231","v":71.590002591314217},{"$f":"'Operative BP'!E231","v":70.760240339702762},{"$f":"'Operative BP'!F231","v":69.979193205944796},{"$f":"'Operative BP'!G231","v":69.979193205944796},{"$f":"'Operative BP'!H231","v":69.979193205944796},{"$f":"'Operative BP'!I231","v":69.979193205944796},{"$f":"'Operative BP'!J231","v":69.979193205944796},{"$f":"'Operative BP'!K231","v":69.979193205944796},{"$f":"'Operative BP'!L231","v":69.602986212581641},{"$f":"'Operative BP'!M231","v":63.12666519334234},{"$f":"'Operative BP'!N231","v":64.200289988632846},null,{"$f":"'Solar Altitude'!B15","v":12},{"$f":"'Solar Altitude'!C15","v":45.177523796213436},{"$f":"'Solar Altitude'!D15","v":54.329068465075267},{"$f":"'Solar Altitude'!E15","v":65.047371814417531},{"$f":"'Solar Altitude'!F15","v":77.120581963762746},{"$f":"'Solar Altitude'!G15","v":85.511869047796154},{"$f":"'Solar Altitude'!H15","v":87.685706703910299},{"$f":"'Solar Altitude'!I15","v":84.793912346691229},{"$f":"'Solar Altitude'!J15","v":77.199736149013034},{"$f":"'Solar Altitude'!K15","v":65.299840573859427},{"$f":"'Solar Altitude'!L15","v":54.542607240756659},{"$f":"'Solar Altitude'!M15","v":45.370517861678998},{"$f":"'Solar Altitude'!N15","v":41.831318434437598},null,{"$f":"'Incident angle'!CK16","v":12},{"$f":"'Incident angle'!CL16","v":1},{"$f":"'Incident angle'!CM16","v":1},{"$f":"'Incident angle'!CN16","v":0},{"$f":"'Incident angle'!CO16","v":0},{"$f":"'Incident angle'!CP16","v":0},{"$f":"'Incident angle'!CQ16","v":0},{"$f":"'Incident angle'!CR16","v":0},{"$f":"'Incident angle'!CS16","v":0},{"$f":"'Incident angle'!CT16","v":0},{"$f":"'Incident angle'!CU16","v":1},{"$f":"'Incident angle'!CV16","v":1},{"$f":"'Incident angle'!CW16","v":1},null,{"$f":"'Incident angle'!CY16","v":12},{"$f":"'Incident angle'!CZ16","v":0},{"$f":"'Incident angle'!DA16","v":0},{"$f":"'Incident angle'!DB16","v":0},{"$f":"'Incident angle'!DC16","v":0},{"$f":"'Incident angle'!DD16","v":0},{"$f":"'Incident angle'!DE16","v":0},{"$f":"'Incident angle'!DF16","v":0},{"$f":"'Incident angle'!DG16","v":0},{"$f":"'Incident angle'!DH16","v":0},{"$f":"'Incident angle'!DI16","v":0},{"$f":"'Incident angle'!DJ16","v":0},{"$f":"'Incident angle'!DK16","v":0},null,null,12,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,12,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,13,{"$f":"'Profile calcs'!C16","v":45.093307228609767},{"$f":"'Profile calcs'!D16","v":54.548508865098285},{"$f":"'Profile calcs'!E16","v":65.300000000000011},{"$f":"'Profile calcs'!F16","v":77.527686129155398},{"$f":"'Profile calcs'!G16","v":86.172088859931137},{"$f":"'Profile calcs'!H16","v":89.286545413103582},{"$f":"'Profile calcs'!I16","v":86.195448533480899},{"$f":"'Profile calcs'!J16","v":77.690264015558725},{"$f":"'Profile calcs'!K16","v":65.300000000000011},{"$f":"'Profile calcs'!L16","v":54.1192638814804},{"$f":"'Profile calcs'!M16","v":44.599954197716883},{"$f":"'Profile calcs'!N16","v":41.247836270078757},null,13,{"$f":"'Profile calcs'!AE16","v":76.310236007231225},{"$f":"'Profile calcs'!AF16","v":78.301959925225134},{"$f":"'Profile calcs'!AG16","v":77.550222553106053},{"$f":"'Profile calcs'!AH16","v":76.496177068295182},{"$f":"'Profile calcs'!AI16","v":76.818295906325034},{"$f":"'Profile calcs'!AJ16","v":78.211108618523411},{"$f":"'Profile calcs'!AK16","v":79.058019787475942},{"$f":"'Profile calcs'!AL16","v":77.387091031608094},{"$f":"'Profile calcs'!AM16","v":73.467983805952144},{"$f":"'Profile calcs'!AN16","v":69.609222192948593},{"$f":"'Profile calcs'!AO16","v":68.255417985347762},{"$f":"'Profile calcs'!AP16","v":71.453363412613214},null,{"$f":"'Operative BP'!B232","v":13},{"$f":"'Operative BP'!C232","v":65.166410679679444},{"$f":"'Operative BP'!D232","v":70.904294053726574},{"$f":"'Operative BP'!E232","v":69.933249256900211},{"$f":"'Operative BP'!F232","v":69.979193205944796},{"$f":"'Operative BP'!G232","v":69.979193205944796},{"$f":"'Operative BP'!H232","v":69.979193205944796},{"$f":"'Operative BP'!I232","v":69.979193205944796},{"$f":"'Operative BP'!J232","v":69.979193205944796},{"$f":"'Operative BP'!K232","v":69.979193205944796},{"$f":"'Operative BP'!L232","v":69.383683665255802},{"$f":"'Operative BP'!M232","v":64.916844657285395},{"$f":"'Operative BP'!N232","v":66.704775751867658},null,{"$f":"'Solar Altitude'!B16","v":13},{"$f":"'Solar Altitude'!C16","v":44.262516808487675},{"$f":"'Solar Altitude'!D16","v":53.442649547558034},{"$f":"'Solar Altitude'!E16","v":62.96975399076122},{"$f":"'Solar Altitude'!F16","v":71.918657174425832},{"$f":"'Solar Altitude'!G16","v":76.310429689037434},{"$f":"'Solar Altitude'!H16","v":78.190731192893594},{"$f":"'Solar Altitude'!I16","v":78.445286814888803},{"$f":"'Solar Altitude'!J16","v":72.64341275146262},{"$f":"'Solar Altitude'!K16","v":61.303344417053367},{"$f":"'Solar Altitude'!L16","v":50.879096974273239},{"$f":"'Solar Altitude'!M16","v":42.542599664242438},{"$f":"'Solar Altitude'!N16","v":40.072467904514703},null,{"$f":"'Incident angle'!CK17","v":13},{"$f":"'Incident angle'!CL17","v":1},{"$f":"'Incident angle'!CM17","v":1},{"$f":"'Incident angle'!CN17","v":0},{"$f":"'Incident angle'!CO17","v":0},{"$f":"'Incident angle'!CP17","v":0},{"$f":"'Incident angle'!CQ17","v":0},{"$f":"'Incident angle'!CR17","v":0},{"$f":"'Incident angle'!CS17","v":0},{"$f":"'Incident angle'!CT17","v":0},{"$f":"'Incident angle'!CU17","v":1},{"$f":"'Incident angle'!CV17","v":1},{"$f":"'Incident angle'!CW17","v":1},null,{"$f":"'Incident angle'!CY17","v":13},{"$f":"'Incident angle'!CZ17","v":0},{"$f":"'Incident angle'!DA17","v":0},{"$f":"'Incident angle'!DB17","v":0},{"$f":"'Incident angle'!DC17","v":0},{"$f":"'Incident angle'!DD17","v":0},{"$f":"'Incident angle'!DE17","v":0},{"$f":"'Incident angle'!DF17","v":0},{"$f":"'Incident angle'!DG17","v":0},{"$f":"'Incident angle'!DH17","v":0},{"$f":"'Incident angle'!DI17","v":0},{"$f":"'Incident angle'!DJ17","v":0},{"$f":"'Incident angle'!DK17","v":0},null,null,13,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,13,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,14,{"$f":"'Profile calcs'!C17","v":43.459732841647039},{"$f":"'Profile calcs'!D17","v":53.656578483668653},{"$f":"'Profile calcs'!E17","v":65.3},{"$f":"'Profile calcs'!F17","v":78.783422467977019},{"$f":"'Profile calcs'!G17","v":88.233716701902779},{"$f":"'Profile calcs'!H17","v":-88.563972173918131},{"$f":"'Profile calcs'!I17","v":88.003822246360016},{"$f":"'Profile calcs'!J17","v":78.90115012449813},{"$f":"'Profile calcs'!K17","v":65.3},{"$f":"'Profile calcs'!L17","v":52.730352015763074},{"$f":"'Profile calcs'!M17","v":42.259093988308607},{"$f":"'Profile calcs'!N17","v":39.004315155295124},null,14,{"$f":"'Profile calcs'!AE17","v":57.329739937520216},{"$f":"'Profile calcs'!AF17","v":60.7360775958551},{"$f":"'Profile calcs'!AG17","v":61.409664244736106},{"$f":"'Profile calcs'!AH17","v":61.715956668379413},{"$f":"'Profile calcs'!AI17","v":62.905108672619058},{"$f":"'Profile calcs'!AJ17","v":64.600922398571711},{"$f":"'Profile calcs'!AK17","v":65.128294922488053},{"$f":"'Profile calcs'!AL17","v":62.607791450328726},{"$f":"'Profile calcs'!AM17","v":57.468525117430246},{"$f":"'Profile calcs'!AN17","v":52.462028938168871},{"$f":"'Profile calcs'!AO17","v":49.834295771439308},{"$f":"'Profile calcs'!AP17","v":52.146583450749397},null,{"$f":"'Operative BP'!B233","v":14},{"$f":"'Operative BP'!C233","v":68.2574307486706},{"$f":"'Operative BP'!D233","v":70.145131161436467},{"$f":"'Operative BP'!E233","v":69.561103269639062},{"$f":"'Operative BP'!F233","v":69.979193205944796},{"$f":"'Operative BP'!G233","v":69.979193205944796},{"$f":"'Operative BP'!H233","v":69.979193205944796},{"$f":"'Operative BP'!I233","v":69.979193205944796},{"$f":"'Operative BP'!J233","v":69.979193205944796},{"$f":"'Operative BP'!K233","v":69.979193205944796},{"$f":"'Operative BP'!L233","v":67.816007712166055},{"$f":"'Operative BP'!M233","v":64.687147940806668},{"$f":"'Operative BP'!N233","v":67.017655064117022},null,{"$f":"'Solar Altitude'!B17","v":14},{"$f":"'Solar Altitude'!C17","v":39.001643714284292},{"$f":"'Solar Altitude'!D17","v":47.236569251778789},{"$f":"'Solar Altitude'!E17","v":54.505603493104616},{"$f":"'Solar Altitude'!F17","v":60.167275430762508},{"$f":"'Solar Altitude'!G17","v":62.862961225627508},{"$f":"'Solar Altitude'!H17","v":64.570010808670432},{"$f":"'Solar Altitude'!I17","v":65.066621957768987},{"$f":"'Solar Altitude'!J17","v":61.010544197086858},{"$f":"'Solar Altitude'!K17","v":51.819137025254037},{"$f":"'Solar Altitude'!L17","v":42.759898297268641},{"$f":"'Solar Altitude'!M17","v":35.791762146841563},{"$f":"'Solar Altitude'!N17","v":34.427909280399348},null,{"$f":"'Incident angle'!CK18","v":14},{"$f":"'Incident angle'!CL18","v":1},{"$f":"'Incident angle'!CM18","v":1},{"$f":"'Incident angle'!CN18","v":0},{"$f":"'Incident angle'!CO18","v":0},{"$f":"'Incident angle'!CP18","v":0},{"$f":"'Incident angle'!CQ18","v":0},{"$f":"'Incident angle'!CR18","v":0},{"$f":"'Incident angle'!CS18","v":0},{"$f":"'Incident angle'!CT18","v":0},{"$f":"'Incident angle'!CU18","v":0.40105237912950042},{"$f":"'Incident angle'!CV18","v":0.73623397042051142},{"$f":"'Incident angle'!CW18","v":0.9165824100126917},null,{"$f":"'Incident angle'!CY18","v":14},{"$f":"'Incident angle'!CZ18","v":0},{"$f":"'Incident angle'!DA18","v":0},{"$f":"'Incident angle'!DB18","v":0},{"$f":"'Incident angle'!DC18","v":0},{"$f":"'Incident angle'!DD18","v":0},{"$f":"'Incident angle'!DE18","v":0},{"$f":"'Incident angle'!DF18","v":0},{"$f":"'Incident angle'!DG18","v":0},{"$f":"'Incident angle'!DH18","v":0},{"$f":"'Incident angle'!DI18","v":0},{"$f":"'Incident angle'!DJ18","v":0},{"$f":"'Incident angle'!DK18","v":0},null,null,14,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,14,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,15,{"$f":"'Profile calcs'!C18","v":39.870560777390224},{"$f":"'Profile calcs'!D18","v":51.621185830048873},{"$f":"'Profile calcs'!E18","v":65.300000000000011},{"$f":"'Profile calcs'!F18","v":81.497322169487106},{"$f":"'Profile calcs'!G18","v":-87.46971071470432},{"$f":"'Profile calcs'!H18","v":-84.081683557615165},{"$f":"'Profile calcs'!I18","v":-88.112119041692736},{"$f":"'Profile calcs'!J18","v":81.541825162483974},{"$f":"'Profile calcs'!K18","v":65.3},{"$f":"'Profile calcs'!L18","v":49.795844682730099},{"$f":"'Profile calcs'!M18","v":37.488190980331879},{"$f":"'Profile calcs'!N18","v":34.371615174618547},null,15,{"$f":"'Profile calcs'!AE18","v":39.812986834028628},{"$f":"'Profile calcs'!AF18","v":44.138369778725988},{"$f":"'Profile calcs'!AG18","v":45.919354280104962},{"$f":"'Profile calcs'!AH18","v":47.350089337983867},{"$f":"'Profile calcs'!AI18","v":49.279589339957219},{"$f":"'Profile calcs'!AJ18","v":51.233884049672319},{"$f":"'Profile calcs'!AK18","v":51.471577651808317},{"$f":"'Profile calcs'!AL18","v":48.232694478544275},{"$f":"'Profile calcs'!AM18","v":42.164171017516459},{"$f":"'Profile calcs'!AN18","v":36.404340467875528},{"$f":"'Profile calcs'!AO18","v":32.990491768082641},{"$f":"'Profile calcs'!AP18","v":34.633273198345066},null,{"$f":"'Operative BP'!B234","v":15},{"$f":"'Operative BP'!C234","v":65.664876920979196},{"$f":"'Operative BP'!D234","v":65.553918997933678},{"$f":"'Operative BP'!E234","v":64.339058651911216},{"$f":"'Operative BP'!F234","v":64.808867966145158},{"$f":"'Operative BP'!G234","v":64.998379691108426},{"$f":"'Operative BP'!H234","v":66.4521783633014},{"$f":"'Operative BP'!I234","v":66.549650931585234},{"$f":"'Operative BP'!J234","v":64.434341743781175},{"$f":"'Operative BP'!K234","v":62.574143771292157},{"$f":"'Operative BP'!L234","v":62.200862432331924},{"$f":"'Operative BP'!M234","v":62.292280927031598},{"$f":"'Operative BP'!N234","v":65.06921752565755},null,{"$f":"'Solar Altitude'!B18","v":15},{"$f":"'Solar Altitude'!C18","v":30.541133571003865},{"$f":"'Solar Altitude'!D18","v":37.574701882546435},{"$f":"'Solar Altitude'!E18","v":43.007444089240849},{"$f":"'Solar Altitude'!F18","v":46.978750874484376},{"$f":"'Solar Altitude'!G18","v":49.242301300948341},{"$f":"'Solar Altitude'!H18","v":51.002542825705397},{"$f":"'Solar Altitude'!I18","v":51.447673176445399},{"$f":"'Solar Altitude'!J18","v":47.843171633901541},{"$f":"'Solar Altitude'!K18","v":39.895074988635152},{"$f":"'Solar Altitude'!L18","v":32.038156511029932},{"$f":"'Solar Altitude'!M18","v":26.359057025099464},{"$f":"'Solar Altitude'!N18","v":25.920295493187655},null,{"$f":"'Incident angle'!CK19","v":15},{"$f":"'Incident angle'!CL19","v":0.42985970538426138},{"$f":"'Incident angle'!CM19","v":0.1387240028188502},{"$f":"'Incident angle'!CN19","v":0},{"$f":"'Incident angle'!CO19","v":0},{"$f":"'Incident angle'!CP19","v":0},{"$f":"'Incident angle'!CQ19","v":0},{"$f":"'Incident angle'!CR19","v":0},{"$f":"'Incident angle'!CS19","v":0},{"$f":"'Incident angle'!CT19","v":0},{"$f":"'Incident angle'!CU19","v":7.2286194092559944E-2},{"$f":"'Incident angle'!CV19","v":0.31757112208291405},{"$f":"'Incident angle'!CW19","v":0.43705225732244574},null,{"$f":"'Incident angle'!CY19","v":15},{"$f":"'Incident angle'!CZ19","v":0},{"$f":"'Incident angle'!DA19","v":0},{"$f":"'Incident angle'!DB19","v":0},{"$f":"'Incident angle'!DC19","v":0},{"$f":"'Incident angle'!DD19","v":0},{"$f":"'Incident angle'!DE19","v":0},{"$f":"'Incident angle'!DF19","v":0},{"$f":"'Incident angle'!DG19","v":0},{"$f":"'Incident angle'!DH19","v":0},{"$f":"'Incident angle'!DI19","v":0},{"$f":"'Incident angle'!DJ19","v":0},{"$f":"'Incident angle'!DK19","v":0},null,null,15,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,15,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,16,{"$f":"'Profile calcs'!C19","v":32.771924244272569},{"$f":"'Profile calcs'!D19","v":47.337670667006847},{"$f":"'Profile calcs'!E19","v":65.3},{"$f":"'Profile calcs'!F19","v":87.260389098756136},{"$f":"'Profile calcs'!G19","v":-78.980403720895211},{"$f":"'Profile calcs'!H19","v":-75.501608463035367},{"$f":"'Profile calcs'!I19","v":-80.468716677637914},{"$f":"'Profile calcs'!J19","v":87.115145464657985},{"$f":"'Profile calcs'!K19","v":65.300000000000011},{"$f":"'Profile calcs'!L19","v":43.332777142141182},{"$f":"'Profile calcs'!M19","v":27.965917871646649},{"$f":"'Profile calcs'!N19","v":25.506940411380103},null,16,{"$f":"'Profile calcs'!AE19","v":23.875002480593196},{"$f":"'Profile calcs'!AF19","v":28.656528802721059},{"$f":"'Profile calcs'!AG19","v":31.171654482760921},{"$f":"'Profile calcs'!AH19","v":33.432906045521179},{"$f":"'Profile calcs'!AI19","v":35.951128585501792},{"$f":"'Profile calcs'!AJ19","v":38.121029600348642},{"$f":"'Profile calcs'!AK19","v":38.115343474138719},{"$f":"'Profile calcs'!AL19","v":34.304400656996243},{"$f":"'Profile calcs'!AM19","v":27.591172995772371},{"$f":"'Profile calcs'!AN19","v":21.421982311981434},{"$f":"'Profile calcs'!AO19","v":17.641166819660786},{"$f":"'Profile calcs'!AP19","v":18.874041457280981},null,{"$f":"'Operative BP'!B235","v":16},{"$f":"'Operative BP'!C235","v":65.417496592038944},{"$f":"'Operative BP'!D235","v":63.527205526822272},{"$f":"'Operative BP'!E235","v":60.838120810021991},{"$f":"'Operative BP'!F235","v":60.968870215774587},{"$f":"'Operative BP'!G235","v":60.597068385282491},{"$f":"'Operative BP'!H235","v":60.914738351398519},{"$f":"'Operative BP'!I235","v":60.676771800160417},{"$f":"'Operative BP'!J235","v":59.36840660513937},{"$f":"'Operative BP'!K235","v":60.183567132662454},{"$f":"'Operative BP'!L235","v":62.312384489714823},{"$f":"'Operative BP'!M235","v":64.370966662544703},{"$f":"'Operative BP'!N235","v":66.282037574210577},null,{"$f":"'Solar Altitude'!B19","v":16},{"$f":"'Solar Altitude'!C19","v":20.038281727598083},{"$f":"'Solar Altitude'!D19","v":26.016647471873153},{"$f":"'Solar Altitude'!E19","v":30.233879108991232},{"$f":"'Solar Altitude'!F19","v":33.419767540103443},{"$f":"'Solar Altitude'!G19","v":35.682648220686666},{"$f":"'Solar Altitude'!H19","v":37.56104623172925},{"$f":"'Solar Altitude'!I19","v":37.876258416390314},{"$f":"'Solar Altitude'!J19","v":34.288646107643089},{"$f":"'Solar Altitude'!K19","v":26.935985833021654},{"$f":"'Solar Altitude'!L19","v":19.913519068774189},{"$f":"'Solar Altitude'!M19","v":15.259931573481456},{"$f":"'Solar Altitude'!N19","v":15.530455637101428},null,{"$f":"'Incident angle'!CK20","v":16},{"$f":"'Incident angle'!CL20","v":0.20458732498358867},{"$f":"'Incident angle'!CM20","v":2.7708256806850172E-3},{"$f":"'Incident angle'!CN20","v":0},{"$f":"'Incident angle'!CO20","v":0},{"$f":"'Incident angle'!CP20","v":0},{"$f":"'Incident angle'!CQ20","v":0},{"$f":"'Incident angle'!CR20","v":0},{"$f":"'Incident angle'!CS20","v":0},{"$f":"'Incident angle'!CT20","v":0},{"$f":"'Incident angle'!CU20","v":0},{"$f":"'Incident angle'!CV20","v":0.12853419638545177},{"$f":"'Incident angle'!CW20","v":0.24189764271439126},null,{"$f":"'Incident angle'!CY20","v":16},{"$f":"'Incident angle'!CZ20","v":0},{"$f":"'Incident angle'!DA20","v":0},{"$f":"'Incident angle'!DB20","v":0},{"$f":"'Incident angle'!DC20","v":0},{"$f":"'Incident angle'!DD20","v":0},{"$f":"'Incident angle'!DE20","v":0},{"$f":"'Incident angle'!DF20","v":0},{"$f":"'Incident angle'!DG20","v":0},{"$f":"'Incident angle'!DH20","v":0},{"$f":"'Incident angle'!DI20","v":0},{"$f":"'Incident angle'!DJ20","v":0},{"$f":"'Incident angle'!DK20","v":0},null,null,16,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,16,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,17,{"$f":"'Profile calcs'!C20","v":18.097147561415554},{"$f":"'Profile calcs'!D20","v":36.90943229885039},{"$f":"'Profile calcs'!E20","v":65.299999999999983},{"$f":"'Profile calcs'!F20","v":-78.138866865290538},{"$f":"'Profile calcs'!G20","v":-61.321747515833643},{"$f":"'Profile calcs'!H20","v":-58.88220246465854},{"$f":"'Profile calcs'!I20","v":-64.773504841898102},{"$f":"'Profile calcs'!J20","v":-79.038177006237561},{"$f":"'Profile calcs'!K20","v":65.3},{"$f":"'Profile calcs'!L20","v":25.128119824042169},{"$f":"'Profile calcs'!M20","v":7.7999612458558687},{"$f":"'Profile calcs'!N20","v":8.333947337338298},null,17,{"$f":"'Profile calcs'!AE20","v":9.2385105897919768},{"$f":"'Profile calcs'!AF20","v":14.141799097654047},{"$f":"'Profile calcs'!AG20","v":17.054801329090424},{"$f":"'Profile calcs'!AH20","v":19.854676249106344},{"$f":"'Profile calcs'!AI20","v":22.809925103490791},{"$f":"'Profile calcs'!AJ20","v":25.161800037123339},{"$f":"'Profile calcs'!AK20","v":24.96833403497148},{"$f":"'Profile calcs'!AL20","v":20.721091695019812},{"$f":"'Profile calcs'!AM20","v":13.597367832295648},{"$f":"'Profile calcs'!AN20","v":7.2728027816997747},{"$f":"'Profile calcs'!AO20","v":3.4258822939894862},{"$f":"'Profile calcs'!AP20","v":4.469701583642955},null,{"$f":"'Operative BP'!B236","v":17},{"$f":"'Operative BP'!C236","v":69.245820757135903},{"$f":"'Operative BP'!D236","v":65.914433734289005},{"$f":"'Operative BP'!E236","v":62.891488365592302},{"$f":"'Operative BP'!F236","v":63.22242767039549},{"$f":"'Operative BP'!G236","v":62.713388756476277},{"$f":"'Operative BP'!H236","v":62.076737417212001},{"$f":"'Operative BP'!I236","v":61.878623985300159},{"$f":"'Operative BP'!J236","v":61.631481149056903},{"$f":"'Operative BP'!K236","v":63.428930949400382},{"$f":"'Operative BP'!L236","v":66.429600408882862},{"$f":"'Operative BP'!M236","v":68.666663721759676},{"$f":"'Operative BP'!N236","v":70.58718209572443},null,{"$f":"'Solar Altitude'!B20","v":17},{"$f":"'Solar Altitude'!C20","v":8.2848854255444504},{"$f":"'Solar Altitude'!D20","v":13.434807821200849},{"$f":"'Solar Altitude'!E20","v":16.897092448538277},{"$f":"'Solar Altitude'!F20","v":19.80224832363653},{"$f":"'Solar Altitude'!G20","v":22.286756355186323},{"$f":"'Solar Altitude'!H20","v":24.319689951925163},{"$f":"'Solar Altitude'!I20","v":24.456964963286701},{"$f":"'Solar Altitude'!J20","v":20.670382142796534},{"$f":"'Solar Altitude'!K20","v":13.51706337533537},{"$f":"'Solar Altitude'!L20","v":7.0202572324504446},{"$f":"'Solar Altitude'!M20","v":3.1397975005302774},{"$f":"'Solar Altitude'!N20","v":3.9451572875932328},null,{"$f":"'Incident angle'!CK21","v":17},{"$f":"'Incident angle'!CL21","v":0},{"$f":"'Incident angle'!CM21","v":0},{"$f":"'Incident angle'!CN21","v":0},{"$f":"'Incident angle'!CO21","v":0},{"$f":"'Incident angle'!CP21","v":0},{"$f":"'Incident angle'!CQ21","v":0},{"$f":"'Incident angle'!CR21","v":0},{"$f":"'Incident angle'!CS21","v":0},{"$f":"'Incident angle'!CT21","v":0},{"$f":"'Incident angle'!CU21","v":0},{"$f":"'Incident angle'!CV21","v":0},{"$f":"'Incident angle'!CW21","v":5.8907157351308172E-2},null,{"$f":"'Incident angle'!CY21","v":17},{"$f":"'Incident angle'!CZ21","v":0},{"$f":"'Incident angle'!DA21","v":0},{"$f":"'Incident angle'!DB21","v":0},{"$f":"'Incident angle'!DC21","v":0},{"$f":"'Incident angle'!DD21","v":0},{"$f":"'Incident angle'!DE21","v":0},{"$f":"'Incident angle'!DF21","v":0},{"$f":"'Incident angle'!DG21","v":0},{"$f":"'Incident angle'!DH21","v":0},{"$f":"'Incident angle'!DI21","v":0},{"$f":"'Incident angle'!DJ21","v":0},{"$f":"'Incident angle'!DK21","v":0},null,null,17,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,17,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,18,{"$f":"'Profile calcs'!C21","v":-12.251813428691667},{"$f":"'Profile calcs'!D21","v":1.391383654081259},{"$f":"'Profile calcs'!E21","v":65.299999999999883},{"$f":"'Profile calcs'!F21","v":-31.81985245371823},{"$f":"'Profile calcs'!G21","v":-27.288827655179645},{"$f":"'Profile calcs'!H21","v":-29.604909535046897},{"$f":"'Profile calcs'!I21","v":-33.539568672346476},{"$f":"'Profile calcs'!J21","v":-35.677719714065731},{"$f":"'Profile calcs'!K21","v":65.300000000005312},{"$f":"'Profile calcs'!L21","v":-35.505208591928351},{"$f":"'Profile calcs'!M21","v":-29.293598980117586},{"$f":"'Profile calcs'!N21","v":-21.514539515184669},null,18,{"$f":"'Profile calcs'!AE21","v":-4.5124409084911488},{"$f":"'Profile calcs'!AF21","v":0.2911309486956099},{"$f":"'Profile calcs'!AG21","v":3.324414100544868},{"$f":"'Profile calcs'!AH21","v":6.3911335111384062},{"$f":"'Profile calcs'!AI21","v":9.6364921571497923},{"$f":"'Profile calcs'!AJ21","v":12.146410157593207},{"$f":"'Profile calcs'!AK21","v":11.827587615885063},{"$f":"'Profile calcs'!AL21","v":7.2645164628018666},{"$f":"'Profile calcs'!AM21","v":-8.3279928680489793E-2},{"$f":"'Profile calcs'!AN21","v":-6.3787494503651301},{"$f":"'Profile calcs'!AO21","v":-10.079870372411357},{"$f":"'Profile calcs'!AP21","v":-9.055310015770992},null,{"$f":"'Operative BP'!B237","v":18},{"$f":"'Operative BP'!C237","v":69.979193205944796},{"$f":"'Operative BP'!D237","v":70.541430493762959},{"$f":"'Operative BP'!E237","v":68.220527259173267},{"$f":"'Operative BP'!F237","v":68.042651415341922},{"$f":"'Operative BP'!G237","v":67.315969428642248},{"$f":"'Operative BP'!H237","v":66.435534677794081},{"$f":"'Operative BP'!I237","v":66.387672432916617},{"$f":"'Operative BP'!J237","v":67.072666601956769},{"$f":"'Operative BP'!K237","v":69.979193205944796},{"$f":"'Operative BP'!L237","v":69.979193205944796},{"$f":"'Operative BP'!M237","v":69.313005944798306},{"$f":"'Operative BP'!N237","v":69.979193205944796},null,{"$f":"'Solar Altitude'!B21","v":18},{"$f":"'Solar Altitude'!C21","v":-4.242067037456934},{"$f":"'Solar Altitude'!D21","v":0.28496224246637836},{"$f":"'Solar Altitude'!E21","v":3.3232309033445016},{"$f":"'Solar Altitude'!F21","v":6.2903017477886056},{"$f":"'Solar Altitude'!G21","v":9.1618728727979484},{"$f":"'Solar Altitude'!H21","v":11.380032986011807},{"$f":"'Solar Altitude'!I21","v":11.292623329902437},{"$f":"'Solar Altitude'!J21","v":7.1538265372891177},{"$f":"'Solar Altitude'!K21","v":-8.3279910069723753E-2},{"$f":"'Solar Altitude'!L21","v":-6.3024734223343577},{"$f":"'Solar Altitude'!M21","v":-9.6180467382750852},{"$f":"'Solar Altitude'!N21","v":-8.4049479592926772},null,{"$f":"'Incident angle'!CK22","v":18},{"$f":"'Incident angle'!CL22","v":0},{"$f":"'Incident angle'!CM22","v":0},{"$f":"'Incident angle'!CN22","v":0},{"$f":"'Incident angle'!CO22","v":0},{"$f":"'Incident angle'!CP22","v":0},{"$f":"'Incident angle'!CQ22","v":0},{"$f":"'Incident angle'!CR22","v":0},{"$f":"'Incident angle'!CS22","v":0},{"$f":"'Incident angle'!CT22","v":0},{"$f":"'Incident angle'!CU22","v":0},{"$f":"'Incident angle'!CV22","v":0},{"$f":"'Incident angle'!CW22","v":0},null,{"$f":"'Incident angle'!CY22","v":18},{"$f":"'Incident angle'!CZ22","v":0},{"$f":"'Incident angle'!DA22","v":0},{"$f":"'Incident angle'!DB22","v":0},{"$f":"'Incident angle'!DC22","v":0},{"$f":"'Incident angle'!DD22","v":0},{"$f":"'Incident angle'!DE22","v":0},{"$f":"'Incident angle'!DF22","v":0},{"$f":"'Incident angle'!DG22","v":0},{"$f":"'Incident angle'!DH22","v":0},{"$f":"'Incident angle'!DI22","v":0},{"$f":"'Incident angle'!DJ22","v":0},{"$f":"'Incident angle'!DK22","v":0},null,null,18,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,18,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,19,{"$f":"'Profile calcs'!C22","v":-51.240705877576872},{"$f":"'Profile calcs'!D22","v":-66.818156461309627},{"$f":"'Profile calcs'!E22","v":65.300000000000011},{"$f":"'Profile calcs'!F22","v":23.209902347589786},{"$f":"'Profile calcs'!G22","v":8.5611583129303881},{"$f":"'Profile calcs'!H22","v":2.4741704005345873},{"$f":"'Profile calcs'!I22","v":3.7069814327208346},{"$f":"'Profile calcs'!J22","v":20.835558391915374},{"$f":"'Profile calcs'!K22","v":65.300000000000011},{"$f":"'Profile calcs'!L22","v":-81.925623758734844},{"$f":"'Profile calcs'!M22","v":-63.089263813477999},{"$f":"'Profile calcs'!N22","v":-53.190222536091191},null,19,{"$f":"'Profile calcs'!AE22","v":-17.787083138469381},{"$f":"'Profile calcs'!AF22","v":-13.241926751478145},{"$f":"'Profile calcs'!AG22","v":-10.3274086586192},{"$f":"'Profile calcs'!AH22","v":-7.2612910314068433},{"$f":"'Profile calcs'!AI22","v":-3.8834912247576012},{"$f":"'Profile calcs'!AJ22","v":-1.2368871636337018},{"$f":"'Profile calcs'!AK22","v":-1.6074102522073654},{"$f":"'Profile calcs'!AL22","v":-6.3652304276825138},{"$f":"'Profile calcs'!AM22","v":-13.765898970431998},{"$f":"'Profile calcs'!AN22","v":-19.875382193162707},{"$f":"'Profile calcs'!AO22","v":-23.262321940359538},{"$f":"'Profile calcs'!AP22","v":-22.125354369783608},null,{"$f":"'Operative BP'!B238","v":19},{"$f":"'Operative BP'!C238","v":69.979193205944796},{"$f":"'Operative BP'!D238","v":71.752629639065816},{"$f":"'Operative BP'!E238","v":70.139997027600856},{"$f":"'Operative BP'!F238","v":69.979193205944796},{"$f":"'Operative BP'!G238","v":69.979193205944796},{"$f":"'Operative BP'!H238","v":69.979193205944796},{"$f":"'Operative BP'!I238","v":69.979193205944796},{"$f":"'Operative BP'!J238","v":69.979193205944796},{"$f":"'Operative BP'!K238","v":69.979193205944796},{"$f":"'Operative BP'!L238","v":69.979193205944796},{"$f":"'Operative BP'!M238","v":69.767851040339707},{"$f":"'Operative BP'!N238","v":69.979193205944796},null,{"$f":"'Solar Altitude'!B22","v":19},{"$f":"'Solar Altitude'!C22","v":-17.258784755357599},{"$f":"'Solar Altitude'!D22","v":-13.177535073458104},{"$f":"'Solar Altitude'!E22","v":-10.292097151668569},{"$f":"'Solar Altitude'!F22","v":-6.9635212465343193},{"$f":"'Solar Altitude'!G22","v":-3.5411252469823715},{"$f":"'Solar Altitude'!H22","v":-1.1064784283971907},{"$f":"'Solar Altitude'!I22","v":-1.4750612815819091},{"$f":"'Solar Altitude'!J22","v":-6.1102162570653853},{"$f":"'Solar Altitude'!K22","v":-13.682588857300294},{"$f":"'Solar Altitude'!L22","v":-19.851334869589788},{"$f":"'Solar Altitude'!M22","v":-22.782734775346487},{"$f":"'Solar Altitude'!N22","v":-21.2544074674176},null,{"$f":"'Incident angle'!CK23","v":19},{"$f":"'Incident angle'!CL23","v":0},{"$f":"'Incident angle'!CM23","v":0},{"$f":"'Incident angle'!CN23","v":0},{"$f":"'Incident angle'!CO23","v":0},{"$f":"'Incident angle'!CP23","v":0},{"$f":"'Incident angle'!CQ23","v":0},{"$f":"'Incident angle'!CR23","v":0},{"$f":"'Incident angle'!CS23","v":0},{"$f":"'Incident angle'!CT23","v":0},{"$f":"'Incident angle'!CU23","v":0},{"$f":"'Incident angle'!CV23","v":0},{"$f":"'Incident angle'!CW23","v":0},null,{"$f":"'Incident angle'!CY23","v":19},{"$f":"'Incident angle'!CZ23","v":0},{"$f":"'Incident angle'!DA23","v":0},{"$f":"'Incident angle'!DB23","v":0},{"$f":"'Incident angle'!DC23","v":0},{"$f":"'Incident angle'!DD23","v":0},{"$f":"'Incident angle'!DE23","v":0},{"$f":"'Incident angle'!DF23","v":0},{"$f":"'Incident angle'!DG23","v":0},{"$f":"'Incident angle'!DH23","v":0},{"$f":"'Incident angle'!DI23","v":0},{"$f":"'Incident angle'!DJ23","v":0},{"$f":"'Incident angle'!DK23","v":0},null,null,19,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,19,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,20,{"$f":"'Profile calcs'!C23","v":-74.554979301423643},{"$f":"'Profile calcs'!D23","v":89.391837386716404},{"$f":"'Profile calcs'!E23","v":65.300000000000011},{"$f":"'Profile calcs'!F23","v":41.466089410320606},{"$f":"'Profile calcs'!G23","v":27.99246971977583},{"$f":"'Profile calcs'!H23","v":22.437796305169524},{"$f":"'Profile calcs'!I23","v":25.503067121246531},{"$f":"'Profile calcs'!J23","v":40.480701812612722},{"$f":"'Profile calcs'!K23","v":65.300000000000011},{"$f":"'Profile calcs'!L23","v":84.890897039079221},{"$f":"'Profile calcs'!M23","v":-80.111991515210519},{"$f":"'Profile calcs'!N23","v":-72.533349654536536},null,20,{"$f":"'Profile calcs'!AE23","v":-30.929660168946619},{"$f":"'Profile calcs'!AF23","v":-26.783441749367146},{"$f":"'Profile calcs'!AG23","v":-24.219886455298596},{"$f":"'Profile calcs'!AH23","v":-21.450631303008365},{"$f":"'Profile calcs'!AI23","v":-18.141617234558211},{"$f":"'Profile calcs'!AJ23","v":-15.393131364902047},{"$f":"'Profile calcs'!AK23","v":-15.718705218374629},{"$f":"'Profile calcs'!AL23","v":-20.515426310682397},{"$f":"'Profile calcs'!AM23","v":-27.765335603992941},{"$f":"'Profile calcs'!AN23","v":-33.518173513343072},{"$f":"'Profile calcs'!AO23","v":-36.431124914543311},{"$f":"'Profile calcs'!AP23","v":-35.075043189143301},null,{"$f":"'Operative BP'!B239","v":20},{"$f":"'Operative BP'!C239","v":62.979193205944796},{"$f":"'Operative BP'!D239","v":69.979193205944796},{"$f":"'Operative BP'!E239","v":70.718890785562635},{"$f":"'Operative BP'!F239","v":69.979193205944796},{"$f":"'Operative BP'!G239","v":69.979193205944796},{"$f":"'Operative BP'!H239","v":69.979193205944796},{"$f":"'Operative BP'!I239","v":69.979193205944796},{"$f":"'Operative BP'!J239","v":69.979193205944796},{"$f":"'Operative BP'!K239","v":69.979193205944796},{"$f":"'Operative BP'!L239","v":69.979193205944796},{"$f":"'Operative BP'!M239","v":70.346744798301486},{"$f":"'Operative BP'!N239","v":69.979193205944796},null,{"$f":"'Solar Altitude'!B23","v":20},{"$f":"'Solar Altitude'!C23","v":-30.589239677830651},{"$f":"'Solar Altitude'!D23","v":-26.783110901661868},{"$f":"'Solar Altitude'!E23","v":-23.773745192987072},{"$f":"'Solar Altitude'!F23","v":-19.749387170381588},{"$f":"'Solar Altitude'!G23","v":-15.584861719885295},{"$f":"'Solar Altitude'!H23","v":-12.902247652391463},{"$f":"'Solar Altitude'!I23","v":-13.625605199002544},{"$f":"'Solar Altitude'!J23","v":-18.916708643772196},{"$f":"'Solar Altitude'!K23","v":-27.097900221004799},{"$f":"'Solar Altitude'!L23","v":-33.472019280706604},{"$f":"'Solar Altitude'!M23","v":-36.206670576844481},{"$f":"'Solar Altitude'!N23","v":-34.435555539572299},null,{"$f":"'Incident angle'!CK24","v":20},{"$f":"'Incident angle'!CL24","v":0},{"$f":"'Incident angle'!CM24","v":0},{"$f":"'Incident angle'!CN24","v":0},{"$f":"'Incident angle'!CO24","v":0},{"$f":"'Incident angle'!CP24","v":0},{"$f":"'Incident angle'!CQ24","v":0},{"$f":"'Incident angle'!CR24","v":0},{"$f":"'Incident angle'!CS24","v":0},{"$f":"'Incident angle'!CT24","v":0},{"$f":"'Incident angle'!CU24","v":0},{"$f":"'Incident angle'!CV24","v":0},{"$f":"'Incident angle'!CW24","v":0},null,{"$f":"'Incident angle'!CY24","v":20},{"$f":"'Incident angle'!CZ24","v":0},{"$f":"'Incident angle'!DA24","v":0},{"$f":"'Incident angle'!DB24","v":0},{"$f":"'Incident angle'!DC24","v":0},{"$f":"'Incident angle'!DD24","v":0},{"$f":"'Incident angle'!DE24","v":0},{"$f":"'Incident angle'!DF24","v":0},{"$f":"'Incident angle'!DG24","v":0},{"$f":"'Incident angle'!DH24","v":0},{"$f":"'Incident angle'!DI24","v":0},{"$f":"'Incident angle'!DJ24","v":0},{"$f":"'Incident angle'!DK24","v":0},null,null,20,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,20,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,21,{"$f":"'Profile calcs'!C24","v":-85.523628972409725},{"$f":"'Profile calcs'!D24","v":81.615896728501113},{"$f":"'Profile calcs'!E24","v":65.300000000000011},{"$f":"'Profile calcs'!F24","v":48.276082529258858},{"$f":"'Profile calcs'!G24","v":37.282219236973447},{"$f":"'Profile calcs'!H24","v":32.777260396790922},{"$f":"'Profile calcs'!I24","v":35.946370921243286},{"$f":"'Profile calcs'!J24","v":47.731081500767182},{"$f":"'Profile calcs'!K24","v":65.3},{"$f":"'Profile calcs'!L24","v":79.771091305966891},{"$f":"'Profile calcs'!M24","v":-88.241664176975647},{"$f":"'Profile calcs'!N24","v":-82.5377288969418},null,21,{"$f":"'Profile calcs'!AE24","v":-44.196478266846057},{"$f":"'Profile calcs'!AF24","v":-40.599089566496509},{"$f":"'Profile calcs'!AG24","v":-38.635878844024383},{"$f":"'Profile calcs'!AH24","v":-36.520338007765027},{"$f":"'Profile calcs'!AI24","v":-33.567457399080453},{"$f":"'Profile calcs'!AJ24","v":-30.792711025689055},{"$f":"'Profile calcs'!AK24","v":-30.936867265726114},{"$f":"'Profile calcs'!AL24","v":-35.533344323926308},{"$f":"'Profile calcs'!AM24","v":-42.346663637257642},{"$f":"'Profile calcs'!AN24","v":-47.52980172868061},{"$f":"'Profile calcs'!AO24","v":-49.801160168555157},{"$f":"'Profile calcs'!AP24","v":-48.138711526458181},null,{"$f":"'Operative BP'!B240","v":21},{"$f":"'Operative BP'!C240","v":62.979193205944796},{"$f":"'Operative BP'!D240","v":69.979193205944796},{"$f":"'Operative BP'!E240","v":71.049687218683658},{"$f":"'Operative BP'!F240","v":68.940859957537157},{"$f":"'Operative BP'!G240","v":69.979193205944796},{"$f":"'Operative BP'!H240","v":69.979193205944796},{"$f":"'Operative BP'!I240","v":69.979193205944796},{"$f":"'Operative BP'!J240","v":69.979193205944796},{"$f":"'Operative BP'!K240","v":69.979193205944796},{"$f":"'Operative BP'!L240","v":69.979193205944796},{"$f":"'Operative BP'!M240","v":70.718890785562635},{"$f":"'Operative BP'!N240","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B24","v":21},{"$f":"'Solar Altitude'!C24","v":-44.11375465474292},{"$f":"'Solar Altitude'!D24","v":-40.375142281624065},{"$f":"'Solar Altitude'!E24","v":-36.877998514340369},{"$f":"'Solar Altitude'!F24","v":-31.713766855869693},{"$f":"'Solar Altitude'!G24","v":-26.575515215416551},{"$f":"'Solar Altitude'!H24","v":-23.623016903493113},{"$f":"'Solar Altitude'!I24","v":-24.79570873532365},{"$f":"'Solar Altitude'!J24","v":-30.92280247893752},{"$f":"'Solar Altitude'!K24","v":-40.048756889246128},{"$f":"'Solar Altitude'!L24","v":-46.985407153208357},{"$f":"'Solar Altitude'!M24","v":-49.782532508401836},{"$f":"'Solar Altitude'!N24","v":-47.837496220337762},null,{"$f":"'Incident angle'!CK25","v":21},{"$f":"'Incident angle'!CL25","v":0},{"$f":"'Incident angle'!CM25","v":0},{"$f":"'Incident angle'!CN25","v":0},{"$f":"'Incident angle'!CO25","v":0},{"$f":"'Incident angle'!CP25","v":0},{"$f":"'Incident angle'!CQ25","v":0},{"$f":"'Incident angle'!CR25","v":0},{"$f":"'Incident angle'!CS25","v":0},{"$f":"'Incident angle'!CT25","v":0},{"$f":"'Incident angle'!CU25","v":0},{"$f":"'Incident angle'!CV25","v":0},{"$f":"'Incident angle'!CW25","v":0},null,{"$f":"'Incident angle'!CY25","v":21},{"$f":"'Incident angle'!CZ25","v":0},{"$f":"'Incident angle'!DA25","v":0},{"$f":"'Incident angle'!DB25","v":0},{"$f":"'Incident angle'!DC25","v":0},{"$f":"'Incident angle'!DD25","v":0},{"$f":"'Incident angle'!DE25","v":0},{"$f":"'Incident angle'!DF25","v":0},{"$f":"'Incident angle'!DG25","v":0},{"$f":"'Incident angle'!DH25","v":0},{"$f":"'Incident angle'!DI25","v":0},{"$f":"'Incident angle'!DJ25","v":0},{"$f":"'Incident angle'!DK25","v":0},null,null,21,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,21,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,22,{"$f":"'Profile calcs'!C25","v":89.034466475858267},{"$f":"'Profile calcs'!D25","v":78.208550588834868},{"$f":"'Profile calcs'!E25","v":65.300000000000011},{"$f":"'Profile calcs'!F25","v":51.41616481533466},{"$f":"'Profile calcs'!G25","v":41.966447814390222},{"$f":"'Profile calcs'!H25","v":38.176455047188753},{"$f":"'Profile calcs'!I25","v":41.191262191845297},{"$f":"'Profile calcs'!J25","v":51.055744533640386},{"$f":"'Profile calcs'!K25","v":65.3},{"$f":"'Profile calcs'!L25","v":77.37193628402801},{"$f":"'Profile calcs'!M25","v":87.655590304611039},{"$f":"'Profile calcs'!N25","v":-87.764397938009651},null,22,{"$f":"'Profile calcs'!AE25","v":-57.739752741902734},{"$f":"'Profile calcs'!AF25","v":-54.856879804295147},{"$f":"'Profile calcs'!AG25","v":-53.761437623792688},{"$f":"'Profile calcs'!AH25","v":-52.718628788708926},{"$f":"'Profile calcs'!AI25","v":-50.521398141456487},{"$f":"'Profile calcs'!AJ25","v":-47.871905572894391},{"$f":"'Profile calcs'!AK25","v":-47.648515276704565},{"$f":"'Profile calcs'!AL25","v":-51.678377748209428},{"$f":"'Profile calcs'!AM25","v":-57.660184602658042},{"$f":"'Profile calcs'!AN25","v":-62.016242169118094},{"$f":"'Profile calcs'!AO25","v":-63.476783571899695},{"$f":"'Profile calcs'!AP25","v":-61.443103356413083},null,{"$f":"'Operative BP'!B241","v":22},{"$f":"'Operative BP'!C241","v":62.979193205944796},{"$f":"'Operative BP'!D241","v":69.979193205944796},{"$f":"'Operative BP'!E241","v":71.421833205944793},{"$f":"'Operative BP'!F241","v":69.313005944798306},{"$f":"'Operative BP'!G241","v":69.979193205944796},{"$f":"'Operative BP'!H241","v":69.979193205944796},{"$f":"'Operative BP'!I241","v":69.979193205944796},{"$f":"'Operative BP'!J241","v":69.979193205944796},{"$f":"'Operative BP'!K241","v":69.979193205944796},{"$f":"'Operative BP'!L241","v":69.979193205944796},{"$f":"'Operative BP'!M241","v":71.173735881104037},{"$f":"'Operative BP'!N241","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B25","v":22},{"$f":"'Solar Altitude'!C25","v":-57.730536859646747},{"$f":"'Solar Altitude'!D25","v":-53.7124665497957},{"$f":"'Solar Altitude'!E25","v":-49.130640449349315},{"$f":"'Solar Altitude'!F25","v":-42.202232941267965},{"$f":"'Solar Altitude'!G25","v":-35.853933091501311},{"$f":"'Solar Altitude'!H25","v":-32.649969945256942},{"$f":"'Solar Altitude'!I25","v":-34.377195915482893},{"$f":"'Solar Altitude'!J25","v":-41.497131280000914},{"$f":"'Solar Altitude'!K25","v":-51.954064465377563},{"$f":"'Solar Altitude'!L25","v":-60.030194510304511},{"$f":"'Solar Altitude'!M25","v":-63.399939655490947},{"$f":"'Solar Altitude'!N25","v":-61.381330079855132},null,{"$f":"'Incident angle'!CK26","v":22},{"$f":"'Incident angle'!CL26","v":0},{"$f":"'Incident angle'!CM26","v":0},{"$f":"'Incident angle'!CN26","v":0},{"$f":"'Incident angle'!CO26","v":0},{"$f":"'Incident angle'!CP26","v":0},{"$f":"'Incident angle'!CQ26","v":0},{"$f":"'Incident angle'!CR26","v":0},{"$f":"'Incident angle'!CS26","v":0},{"$f":"'Incident angle'!CT26","v":0},{"$f":"'Incident angle'!CU26","v":0},{"$f":"'Incident angle'!CV26","v":0},{"$f":"'Incident angle'!CW26","v":0},null,{"$f":"'Incident angle'!CY26","v":22},{"$f":"'Incident angle'!CZ26","v":0},{"$f":"'Incident angle'!DA26","v":0},{"$f":"'Incident angle'!DB26","v":0},{"$f":"'Incident angle'!DC26","v":0},{"$f":"'Incident angle'!DD26","v":0},{"$f":"'Incident angle'!DE26","v":0},{"$f":"'Incident angle'!DF26","v":0},{"$f":"'Incident angle'!DG26","v":0},{"$f":"'Incident angle'!DH26","v":0},{"$f":"'Incident angle'!DI26","v":0},{"$f":"'Incident angle'!DJ26","v":0},{"$f":"'Incident angle'!DK26","v":0},null,null,22,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,22,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,23,{"$f":"'Profile calcs'!C26","v":86.317782095871337},{"$f":"'Profile calcs'!D26","v":76.581548940884886},{"$f":"'Profile calcs'!E26","v":65.300000000000011},{"$f":"'Profile calcs'!F26","v":52.903879372827781},{"$f":"'Profile calcs'!G26","v":44.256353256343338},{"$f":"'Profile calcs'!H26","v":40.885787908689707},{"$f":"'Profile calcs'!I26","v":43.801669031237033},{"$f":"'Profile calcs'!J26","v":52.639173727034112},{"$f":"'Profile calcs'!K26","v":65.300000000000011},{"$f":"'Profile calcs'!L26","v":76.271835790335643},{"$f":"'Profile calcs'!M26","v":85.706352154202364},{"$f":"'Profile calcs'!N26","v":89.629320243390126},null,23,{"$f":"'Profile calcs'!AE26","v":-71.593874807745053},{"$f":"'Profile calcs'!AF26","v":-69.589194473644923},{"$f":"'Profile calcs'!AG26","v":-69.61109114186894},{"$f":"'Profile calcs'!AH26","v":-70.053891850109679},{"$f":"'Profile calcs'!AI26","v":-69.071591312252522},{"$f":"'Profile calcs'!AJ26","v":-66.787471568061889},{"$f":"'Profile calcs'!AK26","v":-65.990399025379276},{"$f":"'Profile calcs'!AL26","v":-68.978463775005906},{"$f":"'Profile calcs'!AM26","v":-73.666960034724326},{"$f":"'Profile calcs'!AN26","v":-76.93436810343789},{"$f":"'Profile calcs'!AO26","v":-77.442055417846433},{"$f":"'Profile calcs'!AP26","v":-75.002834283541929},null,{"$f":"'Operative BP'!B242","v":23},{"$f":"'Operative BP'!C242","v":62.979193205944796},{"$f":"'Operative BP'!D242","v":62.979193205944796},{"$f":"'Operative BP'!E242","v":71.752629639065816},{"$f":"'Operative BP'!F242","v":69.809200594479833},{"$f":"'Operative BP'!G242","v":69.979193205944796},{"$f":"'Operative BP'!H242","v":69.979193205944796},{"$f":"'Operative BP'!I242","v":69.979193205944796},{"$f":"'Operative BP'!J242","v":69.979193205944796},{"$f":"'Operative BP'!K242","v":69.979193205944796},{"$f":"'Operative BP'!L242","v":69.064908619957535},{"$f":"'Operative BP'!M242","v":71.628580976645438},{"$f":"'Operative BP'!N242","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B26","v":23},{"$f":"'Solar Altitude'!C26","v":-71.276413671366612},{"$f":"'Solar Altitude'!D26","v":-66.153465993410151},{"$f":"'Solar Altitude'!E26","v":-59.402009530792824},{"$f":"'Solar Altitude'!F26","v":-50.011386554405469},{"$f":"'Solar Altitude'!G26","v":-42.39742803240717},{"$f":"'Solar Altitude'!H26","v":-39.064492418979341},{"$f":"'Solar Altitude'!I26","v":-41.409864595350896},{"$f":"'Solar Altitude'!J26","v":-49.478233796277678},{"$f":"'Solar Altitude'!K26","v":-61.393251168859493},{"$f":"'Solar Altitude'!L26","v":-71.378499679687209},{"$f":"'Solar Altitude'!M26","v":-76.771747562226409},{"$f":"'Solar Altitude'!N26","v":-74.998658692112272},null,{"$f":"'Incident angle'!CK27","v":23},{"$f":"'Incident angle'!CL27","v":0},{"$f":"'Incident angle'!CM27","v":0},{"$f":"'Incident angle'!CN27","v":0},{"$f":"'Incident angle'!CO27","v":0},{"$f":"'Incident angle'!CP27","v":0},{"$f":"'Incident angle'!CQ27","v":0},{"$f":"'Incident angle'!CR27","v":0},{"$f":"'Incident angle'!CS27","v":0},{"$f":"'Incident angle'!CT27","v":0},{"$f":"'Incident angle'!CU27","v":0},{"$f":"'Incident angle'!CV27","v":0},{"$f":"'Incident angle'!CW27","v":0},null,{"$f":"'Incident angle'!CY27","v":23},{"$f":"'Incident angle'!CZ27","v":0},{"$f":"'Incident angle'!DA27","v":0},{"$f":"'Incident angle'!DB27","v":0},{"$f":"'Incident angle'!DC27","v":0},{"$f":"'Incident angle'!DD27","v":0},{"$f":"'Incident angle'!DE27","v":0},{"$f":"'Incident angle'!DF27","v":0},{"$f":"'Incident angle'!DG27","v":0},{"$f":"'Incident angle'!DH27","v":0},{"$f":"'Incident angle'!DI27","v":0},{"$f":"'Incident angle'!DJ27","v":0},{"$f":"'Incident angle'!DK27","v":0},null,null,23,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,23,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,24,{"$f":"'Profile calcs'!C27","v":85.258807477738344},{"$f":"'Profile calcs'!D27","v":75.943775995922138},{"$f":"'Profile calcs'!E27","v":65.3},{"$f":"'Profile calcs'!F27","v":53.395992963055065},{"$f":"'Profile calcs'!G27","v":44.997391900129685},{"$f":"'Profile calcs'!H27","v":41.835493673926223},{"$f":"'Profile calcs'!I27","v":44.768155065254646},{"$f":"'Profile calcs'!J27","v":53.189833160566664},{"$f":"'Profile calcs'!K27","v":65.3},{"$f":"'Profile calcs'!L27","v":76.006803466110895},{"$f":"'Profile calcs'!M27","v":85.207760704177844},{"$f":"'Profile calcs'!N27","v":88.756097838181603},null,24,{"$f":"'Profile calcs'!AE27","v":-85.676140318453747},{"$f":"'Profile calcs'!AF27","v":-84.673020487038187},{"$f":"'Profile calcs'!AG27","v":-85.974408266739914},{"$f":"'Profile calcs'!AH27","v":-88.161715299139871},{"$f":"'Profile calcs'!AI27","v":-88.728943923930075},{"$f":"'Profile calcs'!AJ27","v":-87.067266457680958},{"$f":"'Profile calcs'!AK27","v":-85.571264313099363},{"$f":"'Profile calcs'!AL27","v":-87.09022999649082},{"$f":"'Profile calcs'!AM27","v":-89.899102008781256},{"$f":"'Profile calcs'!AN27","v":-87.907230778803338},{"$f":"'Profile calcs'!AO27","v":-88.427383905065867},{"$f":"'Profile calcs'!AP27","v":-88.730639842766692},null,{"$f":"'Operative BP'!B243","v":24},{"$f":"'Operative BP'!C243","v":62.979193205944796},{"$f":"'Operative BP'!D243","v":62.979193205944796},{"$f":"'Operative BP'!E243","v":72.083426072186839},{"$f":"'Operative BP'!F243","v":70.139997027600856},{"$f":"'Operative BP'!G243","v":69.979193205944796},{"$f":"'Operative BP'!H243","v":69.979193205944796},{"$f":"'Operative BP'!I243","v":69.979193205944796},{"$f":"'Operative BP'!J243","v":69.979193205944796},{"$f":"'Operative BP'!K243","v":69.979193205944796},{"$f":"'Operative BP'!L243","v":69.395705053078558},{"$f":"'Operative BP'!M243","v":71.91802785562632},{"$f":"'Operative BP'!N243","v":62.979193205944796},null,{"$f":"'Solar Altitude'!B27","v":24},{"$f":"'Solar Altitude'!C27","v":-83.596484892158756},{"$f":"'Solar Altitude'!D27","v":-75.041691580826409},{"$f":"'Solar Altitude'!E27","v":-65.047371814417531},{"$f":"'Solar Altitude'!F27","v":-53.370409687127484},{"$f":"'Solar Altitude'!G27","v":-44.990343292174892},{"$f":"'Solar Altitude'!H27","v":-41.805581832384377},{"$f":"'Solar Altitude'!I27","v":-44.683864079458822},{"$f":"'Solar Altitude'!J27","v":-53.126563822663151},{"$f":"'Solar Altitude'!K27","v":-65.299840573859427},{"$f":"'Solar Altitude'!L27","v":-75.863131931954825},{"$f":"'Solar Altitude'!M27","v":-84.958601709687045},{"$f":"'Solar Altitude'!N27","v":-88.223048770244205},null,{"$f":"'Incident angle'!CK28","v":24},{"$f":"'Incident angle'!CL28","v":0},{"$f":"'Incident angle'!CM28","v":0},{"$f":"'Incident angle'!CN28","v":0},{"$f":"'Incident angle'!CO28","v":0},{"$f":"'Incident angle'!CP28","v":0},{"$f":"'Incident angle'!CQ28","v":0},{"$f":"'Incident angle'!CR28","v":0},{"$f":"'Incident angle'!CS28","v":0},{"$f":"'Incident angle'!CT28","v":0},{"$f":"'Incident angle'!CU28","v":0},{"$f":"'Incident angle'!CV28","v":0},{"$f":"'Incident angle'!CW28","v":0},null,{"$f":"'Incident angle'!CY28","v":24},{"$f":"'Incident angle'!CZ28","v":0},{"$f":"'Incident angle'!DA28","v":0},{"$f":"'Incident angle'!DB28","v":0},{"$f":"'Incident angle'!DC28","v":0},{"$f":"'Incident angle'!DD28","v":0},{"$f":"'Incident angle'!DE28","v":0},{"$f":"'Incident angle'!DF28","v":0},{"$f":"'Incident angle'!DG28","v":0},{"$f":"'Incident angle'!DH28","v":0},{"$f":"'Incident angle'!DI28","v":0},{"$f":"'Incident angle'!DJ28","v":0},{"$f":"'Incident angle'!DK28","v":0},null,null,24,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,24,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,null,null,null,null,null,null,null,{"$f":"CP29","v":"Heat Cutoff"},null,null,{"$f":"CS29","v":1000},{"$f":"CT29","v":"-"},{"$f":"CU29","v":1010},null,null,null,null,null,null,null,null,{"$f":"DD29","v":"Heat Cutoff"},null,null,{"$f":"IF(DG29=1000,\"-\",DG29)","v":"-"},{"$f":"DH29","v":"-"},{"$f":"IF(DI29=1010,\"-\",DI29)","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heat Cutoff",null,null,{"$f":"MIN(CJ13:CU21)","v":1000},"-",{"$f":"CS29+10","v":1010},null,null,null,null,null,null,null,null,"Heat Cutoff",null,null,{"$f":"MIN(CX13:DI21)","v":1000},"-",{"$f":"DG29+10","v":1010}]
[]
[]
[null,"Table 2:",null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,"East",null,"East"," Profile"," Profile",null,null,"Table 4:",null,null,{"$f":"STAT!A2","v":" Statistics for SAU_Riyadh.404380_IWEC"},{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,"North",null,"North"," Profile"," Profile",null,null,"Dry Bulb Temp",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BI58","v":"West Transmitted "},null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!BW58","v":"North Transmitted"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Table 7:",null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,"East",null,null," Profile",null,null,null,"Table 8:",null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,"North",null,null," Profile"]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$f":"'Dry Bulb'!C4","v":"HR"},{"$f":"'Dry Bulb'!D4","v":"Jan"},{"$f":"'Dry Bulb'!E4","v":"Feb"},{"$f":"'Dry Bulb'!F4","v":"Mar"},{"$f":"'Dry Bulb'!G4","v":"Apr"},{"$f":"'Dry Bulb'!H4","v":"May"},{"$f":"'Dry Bulb'!I4","v":"Jun"},{"$f":"'Dry Bulb'!J4","v":"Jul"},{"$f":"'Dry Bulb'!K4","v":"Aug"},{"$f":"'Dry Bulb'!L4","v":"Sep"},{"$f":"'Dry Bulb'!M4","v":"Oct"},{"$f":"'Dry Bulb'!N4","v":"Nov"},{"$f":"'Dry Bulb'!O4","v":"Dec"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK59","v":0},{"$f":"'Incident angle'!CL59","v":"Jan"},{"$f":"'Incident angle'!CM59","v":"Feb"},{"$f":"'Incident angle'!CN59","v":"Mar"},{"$f":"'Incident angle'!CO59","v":"Apr"},{"$f":"'Incident angle'!CP59","v":"May"},{"$f":"'Incident angle'!CQ59","v":"Jun"},{"$f":"'Incident angle'!CR59","v":"Jul"},{"$f":"'Incident angle'!CS59","v":"Aug"},{"$f":"'Incident angle'!CT59","v":"Sep"},{"$f":"'Incident angle'!CU59","v":"Oct"},{"$f":"'Incident angle'!CV59","v":"Nov"},{"$f":"'Incident angle'!CW59","v":"Dec"},null,{"$f":"'Incident angle'!CY59","v":0},{"$f":"'Incident angle'!CZ59","v":"Jan"},{"$f":"'Incident angle'!DA59","v":"Feb"},{"$f":"'Incident angle'!DB59","v":"Mar"},{"$f":"'Incident angle'!DC59","v":"Apr"},{"$f":"'Incident angle'!DD59","v":"May"},{"$f":"'Incident angle'!DE59","v":"Jun"},{"$f":"'Incident angle'!DF59","v":"Jul"},{"$f":"'Incident angle'!DG59","v":"Aug"},{"$f":"'Incident angle'!DH59","v":"Sep"},{"$f":"'Incident angle'!DI59","v":"Oct"},{"$f":"'Incident angle'!DJ59","v":"Nov"},{"$f":"'Incident angle'!DK59","v":"Dec"},null,null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"'Profile calcs'!Q4","v":-80.182065177734387},{"$f":"'Profile calcs'!R4","v":-80.140892672943934},{"$f":"'Profile calcs'!S4","v":-77.550222553105996},{"$f":"'Profile calcs'!T4","v":-73.652297950713162},{"$f":"'Profile calcs'!U4","v":-71.539168870383421},{"$f":"'Profile calcs'!V4","v":-72.457459123618534},{"$f":"'Profile calcs'!W4","v":-74.587173801009939},{"$f":"'Profile calcs'!X4","v":-74.673520776603795},{"$f":"'Profile calcs'!Y4","v":-73.467983805952244},{"$f":"'Profile calcs'!Z4","v":-72.789127866510924},{"$f":"'Profile calcs'!AA4","v":-74.318586949653394},{"$f":"'Profile calcs'!AB4","v":-77.526166860808985},null,1,{"$f":"'Profile calcs'!AS4","v":-85.506692771390249},{"$f":"'Profile calcs'!AT4","v":-76.051491134901724},{"$f":"'Profile calcs'!AU4","v":-65.300000000000011},{"$f":"'Profile calcs'!AV4","v":-53.072313870844596},{"$f":"'Profile calcs'!AW4","v":-44.427911140068865},{"$f":"'Profile calcs'!AX4","v":-41.313454586896434},{"$f":"'Profile calcs'!AY4","v":-44.404551466519116},{"$f":"'Profile calcs'!AZ4","v":-52.909735984441276},{"$f":"'Profile calcs'!BA4","v":-65.3},{"$f":"'Profile calcs'!BB4","v":-76.480736118519602},{"$f":"'Profile calcs'!BC4","v":-86.000045802283125},{"$f":"'Profile calcs'!BD4","v":-89.352163729921244},null,{"$f":"'Dry Bulb'!C5","v":1},{"$f":"'Dry Bulb'!D5","v":52.879999999999995},{"$f":"'Dry Bulb'!E5","v":57.379999999999995},{"$f":"'Dry Bulb'!F5","v":64.22},{"$f":"'Dry Bulb'!G5","v":73.040000000000006},{"$f":"'Dry Bulb'!H5","v":84.56},{"$f":"'Dry Bulb'!I5","v":89.6},{"$f":"'Dry Bulb'!J5","v":90.86},{"$f":"'Dry Bulb'!K5","v":91.4},{"$f":"'Dry Bulb'!L5","v":85.82},{"$f":"'Dry Bulb'!M5","v":76.099999999999994},{"$f":"'Dry Bulb'!N5","v":65.12},{"$f":"'Dry Bulb'!O5","v":54.86},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK60","v":1},{"$f":"'Incident angle'!CL60","v":0},{"$f":"'Incident angle'!CM60","v":0},{"$f":"'Incident angle'!CN60","v":0},{"$f":"'Incident angle'!CO60","v":0},{"$f":"'Incident angle'!CP60","v":0},{"$f":"'Incident angle'!CQ60","v":0},{"$f":"'Incident angle'!CR60","v":0},{"$f":"'Incident angle'!CS60","v":0},{"$f":"'Incident angle'!CT60","v":0},{"$f":"'Incident angle'!CU60","v":0},{"$f":"'Incident angle'!CV60","v":0},{"$f":"'Incident angle'!CW60","v":0},null,{"$f":"'Incident angle'!CY60","v":1},{"$f":"'Incident angle'!CZ60","v":0},{"$f":"'Incident angle'!DA60","v":0},{"$f":"'Incident angle'!DB60","v":0},{"$f":"'Incident angle'!DC60","v":0},{"$f":"'Incident angle'!DD60","v":0},{"$f":"'Incident angle'!DE60","v":0},{"$f":"'Incident angle'!DF60","v":0},{"$f":"'Incident angle'!DG60","v":0},{"$f":"'Incident angle'!DH60","v":0},{"$f":"'Incident angle'!DI60","v":0},{"$f":"'Incident angle'!DJ60","v":0},{"$f":"'Incident angle'!DK60","v":0},null,null,1,{"$f":"IF(BU5=0,1000,IF(AS5<0,1000,(IF(AE5>$E$1,1000,C34))))","v":1000},{"$f":"IF(BV5=0,1000,IF(AT5<0,1000,(IF(AF5>$E$1,1000,D34))))","v":1000},{"$f":"IF(BW5=0,1000,IF(AU5<0,1000,(IF(AG5>$E$1,1000,E34))))","v":1000},{"$f":"IF(BX5=0,1000,IF(AV5<0,1000,(IF(AH5>$E$1,1000,F34))))","v":1000},{"$f":"IF(BY5=0,1000,IF(AW5<0,1000,(IF(AI5>$E$1,1000,G34))))","v":1000},{"$f":"IF(BZ5=0,1000,IF(AX5<0,1000,(IF(AJ5>$E$1,1000,H34))))","v":1000},{"$f":"IF(CA5=0,1000,IF(AY5<0,1000,(IF(AK5>$E$1,1000,I34))))","v":1000},{"$f":"IF(CB5=0,1000,IF(AZ5<0,1000,(IF(AL5>$E$1,1000,J34))))","v":1000},{"$f":"IF(CC5=0,1000,IF(BA5<0,1000,(IF(AM5>$E$1,1000,K34))))","v":1000},{"$f":"IF(CD5=0,1000,IF(BB5<0,1000,(IF(AN5>$E$1,1000,L34))))","v":1000},{"$f":"IF(CE5=0,1000,IF(BC5<0,1000,(IF(AO5>$E$1,1000,M34))))","v":1000},{"$f":"IF(CF5=0,1000,IF(BD5<0,1000,(IF(AP5>$E$1,1000,N34))))","v":1000},null,1,{"$f":"IF(BU34=0,1000,IF(AS5<0,1000,(IF(AE5>$E$1,1000,Q34))))","v":1000},{"$f":"IF(BV34=0,1000,IF(AT5<0,1000,(IF(AF5>$E$1,1000,R34))))","v":1000},{"$f":"IF(BW34=0,1000,IF(AU5<0,1000,(IF(AG5>$E$1,1000,S34))))","v":1000},{"$f":"IF(BX34=0,1000,IF(AV5<0,1000,(IF(AH5>$E$1,1000,T34))))","v":1000},{"$f":"IF(BY34=0,1000,IF(AW5<0,1000,(IF(AI5>$E$1,1000,U34))))","v":1000},{"$f":"IF(BZ34=0,1000,IF(AX5<0,1000,(IF(AJ5>$E$1,1000,V34))))","v":1000},{"$f":"IF(CA34=0,1000,IF(AY5<0,1000,(IF(AK5>$E$1,1000,W34))))","v":1000},{"$f":"IF(CB34=0,1000,IF(AZ5<0,1000,(IF(AL5>$E$1,1000,X34))))","v":1000},{"$f":"IF(CC34=0,1000,IF(BA5<0,1000,(IF(AM5>$E$1,1000,Y34))))","v":1000},{"$f":"IF(CD34=0,1000,IF(BB5<0,1000,(IF(AN5>$E$1,1000,Z34))))","v":1000},{"$f":"IF(CE34=0,1000,IF(BC5<0,1000,(IF(AO5>$E$1,1000,AA34))))","v":1000},{"$f":"IF(CF34=0,1000,IF(BD5<0,1000,(IF(AP5>$E$1,1000,AB34))))","v":1000}]
[null,2,{"$f":"'Profile calcs'!Q5","v":-66.172099329250003},{"$f":"'Profile calcs'!R5","v":-65.140511421698733},{"$f":"'Profile calcs'!S5","v":-61.409664244736128},{"$f":"'Profile calcs'!T5","v":-56.119428429528291},{"$f":"'Profile calcs'!U5","v":-52.806644981683412},{"$f":"'Profile calcs'!V5","v":-53.071524478923401},{"$f":"'Profile calcs'!W5","v":-55.607487949913953},{"$f":"'Profile calcs'!X5","v":-57.058845303129402},{"$f":"'Profile calcs'!Y5","v":-57.468525117430296},{"$f":"'Profile calcs'!Z5","v":-57.976591294307511},{"$f":"'Profile calcs'!AA5","v":-60.410283592762973},{"$f":"'Profile calcs'!AB5","v":-63.926268100735683},null,2,{"$f":"'Profile calcs'!AS5","v":-87.14026715835297},{"$f":"'Profile calcs'!AT5","v":-76.94342151633137},{"$f":"'Profile calcs'!AU5","v":-65.300000000000011},{"$f":"'Profile calcs'!AV5","v":-51.816577532022968},{"$f":"'Profile calcs'!AW5","v":-42.36628329809723},{"$f":"'Profile calcs'!AX5","v":-39.16397217391814},{"$f":"'Profile calcs'!AY5","v":-42.596177753639978},{"$f":"'Profile calcs'!AZ5","v":-51.698849875501864},{"$f":"'Profile calcs'!BA5","v":-65.3},{"$f":"'Profile calcs'!BB5","v":-77.869647984236934},{"$f":"'Profile calcs'!BC5","v":-88.340906011691416},{"$f":"'Profile calcs'!BD5","v":88.404315155295109},null,{"$f":"'Dry Bulb'!C6","v":2},{"$f":"'Dry Bulb'!D6","v":51.98},{"$f":"'Dry Bulb'!E6","v":56.3},{"$f":"'Dry Bulb'!F6","v":62.959999999999994},{"$f":"'Dry Bulb'!G6","v":71.959999999999994},{"$f":"'Dry Bulb'!H6","v":83.12},{"$f":"'Dry Bulb'!I6","v":87.8},{"$f":"'Dry Bulb'!J6","v":89.24},{"$f":"'Dry Bulb'!K6","v":89.78},{"$f":"'Dry Bulb'!L6","v":84.02},{"$f":"'Dry Bulb'!M6","v":74.84},{"$f":"'Dry Bulb'!N6","v":63.5},{"$f":"'Dry Bulb'!O6","v":54.14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK61","v":2},{"$f":"'Incident angle'!CL61","v":0},{"$f":"'Incident angle'!CM61","v":0},{"$f":"'Incident angle'!CN61","v":0},{"$f":"'Incident angle'!CO61","v":0},{"$f":"'Incident angle'!CP61","v":0},{"$f":"'Incident angle'!CQ61","v":0},{"$f":"'Incident angle'!CR61","v":0},{"$f":"'Incident angle'!CS61","v":0},{"$f":"'Incident angle'!CT61","v":0},{"$f":"'Incident angle'!CU61","v":0},{"$f":"'Incident angle'!CV61","v":0},{"$f":"'Incident angle'!CW61","v":0},null,{"$f":"'Incident angle'!CY61","v":2},{"$f":"'Incident angle'!CZ61","v":0},{"$f":"'Incident angle'!DA61","v":0},{"$f":"'Incident angle'!DB61","v":0},{"$f":"'Incident angle'!DC61","v":0},{"$f":"'Incident angle'!DD61","v":0},{"$f":"'Incident angle'!DE61","v":0},{"$f":"'Incident angle'!DF61","v":0},{"$f":"'Incident angle'!DG61","v":0},{"$f":"'Incident angle'!DH61","v":0},{"$f":"'Incident angle'!DI61","v":0},{"$f":"'Incident angle'!DJ61","v":0},{"$f":"'Incident angle'!DK61","v":0},null,null,2,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,2,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,3,{"$f":"'Profile calcs'!Q6","v":-52.435166723015541},{"$f":"'Profile calcs'!R6","v":-50.544173289630855},{"$f":"'Profile calcs'!S6","v":-45.91935428010499},{"$f":"'Profile calcs'!T6","v":-39.682535750671363},{"$f":"'Profile calcs'!U6","v":-35.643149417229338},{"$f":"'Profile calcs'!V6","v":-35.46488164814032},{"$f":"'Profile calcs'!W6","v":-38.162804391158723},{"$f":"'Profile calcs'!X6","v":-40.534175714629342},{"$f":"'Profile calcs'!Y6","v":-42.164171017516495},{"$f":"'Profile calcs'!Z6","v":-43.623401532687339},{"$f":"'Profile calcs'!AA6","v":-46.805449667898792},{"$f":"'Profile calcs'!AB6","v":-50.572582527440368},null,3,{"$f":"'Profile calcs'!AS6","v":89.27056077739023},{"$f":"'Profile calcs'!AT6","v":-78.978814169951136},{"$f":"'Profile calcs'!AU6","v":-65.300000000000011},{"$f":"'Profile calcs'!AV6","v":-49.102677830512903},{"$f":"'Profile calcs'!AW6","v":-38.069710714704293},{"$f":"'Profile calcs'!AX6","v":-34.68168355761518},{"$f":"'Profile calcs'!AY6","v":-38.712119041692716},{"$f":"'Profile calcs'!AZ6","v":-49.058174837516013},{"$f":"'Profile calcs'!BA6","v":-65.300000000000011},{"$f":"'Profile calcs'!BB6","v":-80.804155317269903},{"$f":"'Profile calcs'!BC6","v":86.888190980331885},{"$f":"'Profile calcs'!BD6","v":83.771615174618546},null,{"$f":"'Dry Bulb'!C7","v":3},{"$f":"'Dry Bulb'!D7","v":51.44},{"$f":"'Dry Bulb'!E7","v":55.22},{"$f":"'Dry Bulb'!F7","v":61.7},{"$f":"'Dry Bulb'!G7","v":70.88},{"$f":"'Dry Bulb'!H7","v":82.04},{"$f":"'Dry Bulb'!I7","v":86.9},{"$f":"'Dry Bulb'!J7","v":88.16},{"$f":"'Dry Bulb'!K7","v":88.16},{"$f":"'Dry Bulb'!L7","v":82.4},{"$f":"'Dry Bulb'!M7","v":73.22},{"$f":"'Dry Bulb'!N7","v":62.24},{"$f":"'Dry Bulb'!O7","v":53.42},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK62","v":3},{"$f":"'Incident angle'!CL62","v":0},{"$f":"'Incident angle'!CM62","v":0},{"$f":"'Incident angle'!CN62","v":0},{"$f":"'Incident angle'!CO62","v":0},{"$f":"'Incident angle'!CP62","v":0},{"$f":"'Incident angle'!CQ62","v":0},{"$f":"'Incident angle'!CR62","v":0},{"$f":"'Incident angle'!CS62","v":0},{"$f":"'Incident angle'!CT62","v":0},{"$f":"'Incident angle'!CU62","v":0},{"$f":"'Incident angle'!CV62","v":0},{"$f":"'Incident angle'!CW62","v":0},null,{"$f":"'Incident angle'!CY62","v":3},{"$f":"'Incident angle'!CZ62","v":0},{"$f":"'Incident angle'!DA62","v":0},{"$f":"'Incident angle'!DB62","v":0},{"$f":"'Incident angle'!DC62","v":0},{"$f":"'Incident angle'!DD62","v":0},{"$f":"'Incident angle'!DE62","v":0},{"$f":"'Incident angle'!DF62","v":0},{"$f":"'Incident angle'!DG62","v":0},{"$f":"'Incident angle'!DH62","v":0},{"$f":"'Incident angle'!DI62","v":0},{"$f":"'Incident angle'!DJ62","v":0},{"$f":"'Incident angle'!DK62","v":0},null,null,3,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,3,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,4,{"$f":"'Profile calcs'!Q7","v":-39.010190181198872},{"$f":"'Profile calcs'!R7","v":-36.428743475161504},{"$f":"'Profile calcs'!S7","v":-31.171654482760939},{"$f":"'Profile calcs'!T7","v":-24.400458127908184},{"$f":"'Profile calcs'!U7","v":-20.038723532033892},{"$f":"'Profile calcs'!V7","v":-19.625868131864095},{"$f":"'Profile calcs'!W7","v":-22.32000203357995},{"$f":"'Profile calcs'!X7","v":-25.178501666912496},{"$f":"'Profile calcs'!Y7","v":-27.591172995772343},{"$f":"'Profile calcs'!Z7","v":-29.729656317315495},{"$f":"'Profile calcs'!AA7","v":-33.493277499644961},{"$f":"'Profile calcs'!AB7","v":-37.470732683841966},null,4,{"$f":"'Profile calcs'!AS7","v":82.17192424427256},{"$f":"'Profile calcs'!AT7","v":-83.262329332993176},{"$f":"'Profile calcs'!AU7","v":-65.300000000000026},{"$f":"'Profile calcs'!AV7","v":-43.339610901243866},{"$f":"'Profile calcs'!AW7","v":-29.580403720895195},{"$f":"'Profile calcs'!AX7","v":-26.101608463035426},{"$f":"'Profile calcs'!AY7","v":-31.06871667763788},{"$f":"'Profile calcs'!AZ7","v":-43.484854535341988},{"$f":"'Profile calcs'!BA7","v":-65.3},{"$f":"'Profile calcs'!BB7","v":-87.267222857858798},{"$f":"'Profile calcs'!BC7","v":77.365917871646644},{"$f":"'Profile calcs'!BD7","v":74.906940411380106},null,{"$f":"'Dry Bulb'!C8","v":4},{"$f":"'Dry Bulb'!D8","v":50.54},{"$f":"'Dry Bulb'!E8","v":54.14},{"$f":"'Dry Bulb'!F8","v":60.8},{"$f":"'Dry Bulb'!G8","v":69.44},{"$f":"'Dry Bulb'!H8","v":81.5},{"$f":"'Dry Bulb'!I8","v":85.82},{"$f":"'Dry Bulb'!J8","v":86.72},{"$f":"'Dry Bulb'!K8","v":86.9},{"$f":"'Dry Bulb'!L8","v":80.959999999999994},{"$f":"'Dry Bulb'!M8","v":72.5},{"$f":"'Dry Bulb'!N8","v":60.980000000000004},{"$f":"'Dry Bulb'!O8","v":52.52},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK63","v":4},{"$f":"'Incident angle'!CL63","v":0},{"$f":"'Incident angle'!CM63","v":0},{"$f":"'Incident angle'!CN63","v":0},{"$f":"'Incident angle'!CO63","v":0},{"$f":"'Incident angle'!CP63","v":0},{"$f":"'Incident angle'!CQ63","v":0},{"$f":"'Incident angle'!CR63","v":0},{"$f":"'Incident angle'!CS63","v":0},{"$f":"'Incident angle'!CT63","v":0},{"$f":"'Incident angle'!CU63","v":0},{"$f":"'Incident angle'!CV63","v":0},{"$f":"'Incident angle'!CW63","v":0},null,{"$f":"'Incident angle'!CY63","v":4},{"$f":"'Incident angle'!CZ63","v":0},{"$f":"'Incident angle'!DA63","v":0},{"$f":"'Incident angle'!DB63","v":0},{"$f":"'Incident angle'!DC63","v":0},{"$f":"'Incident angle'!DD63","v":0},{"$f":"'Incident angle'!DE63","v":0},{"$f":"'Incident angle'!DF63","v":0},{"$f":"'Incident angle'!DG63","v":0},{"$f":"'Incident angle'!DH63","v":0},{"$f":"'Incident angle'!DI63","v":0},{"$f":"'Incident angle'!DJ63","v":0},{"$f":"'Incident angle'!DK63","v":0},null,null,4,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,4,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,5,{"$f":"'Profile calcs'!Q8","v":-25.815859178831762},{"$f":"'Profile calcs'!R8","v":-22.717824490126432},{"$f":"'Profile calcs'!S8","v":-17.054801329090406},{"$f":"'Profile calcs'!T8","v":-10.060267103118708},{"$f":"'Profile calcs'!U8","v":-5.6553451463568249},{"$f":"'Profile calcs'!V8","v":-5.1651785422524581},{"$f":"'Profile calcs'!W8","v":-7.7705114298265903},{"$f":"'Profile calcs'!X8","v":-10.788309881886676},{"$f":"'Profile calcs'!Y8","v":-13.597367832295642},{"$f":"'Profile calcs'!Z8","v":-16.153367731431349},{"$f":"'Profile calcs'!AA8","v":-20.343596801848918},{"$f":"'Profile calcs'!AB8","v":-24.514554175011249},null,5,{"$f":"'Profile calcs'!AS8","v":67.497147561415517},{"$f":"'Profile calcs'!AT8","v":86.309432298850368},{"$f":"'Profile calcs'!AU8","v":-65.300000000000026},{"$f":"'Profile calcs'!AV8","v":-28.738866865290543},{"$f":"'Profile calcs'!AW8","v":-11.921747515833617},{"$f":"'Profile calcs'!AX8","v":-9.4822024646584833},{"$f":"'Profile calcs'!AY8","v":-15.373504841898106},{"$f":"'Profile calcs'!AZ8","v":-29.638177006237569},{"$f":"'Profile calcs'!BA8","v":-65.30000000000004},{"$f":"'Profile calcs'!BB8","v":74.528119824042179},{"$f":"'Profile calcs'!BC8","v":57.199961245855874},{"$f":"'Profile calcs'!BD8","v":57.733947337338272},null,{"$f":"'Dry Bulb'!C9","v":5},{"$f":"'Dry Bulb'!D9","v":49.46},{"$f":"'Dry Bulb'!E9","v":53.42},{"$f":"'Dry Bulb'!F9","v":59.9},{"$f":"'Dry Bulb'!G9","v":68.36},{"$f":"'Dry Bulb'!H9","v":80.06},{"$f":"'Dry Bulb'!I9","v":84.56},{"$f":"'Dry Bulb'!J9","v":86},{"$f":"'Dry Bulb'!K9","v":85.82},{"$f":"'Dry Bulb'!L9","v":80.240000000000009},{"$f":"'Dry Bulb'!M9","v":71.06},{"$f":"'Dry Bulb'!N9","v":59.540000000000006},{"$f":"'Dry Bulb'!O9","v":51.620000000000005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK64","v":5},{"$f":"'Incident angle'!CL64","v":0},{"$f":"'Incident angle'!CM64","v":0},{"$f":"'Incident angle'!CN64","v":0},{"$f":"'Incident angle'!CO64","v":0},{"$f":"'Incident angle'!CP64","v":0},{"$f":"'Incident angle'!CQ64","v":0},{"$f":"'Incident angle'!CR64","v":0},{"$f":"'Incident angle'!CS64","v":0},{"$f":"'Incident angle'!CT64","v":0},{"$f":"'Incident angle'!CU64","v":0},{"$f":"'Incident angle'!CV64","v":0},{"$f":"'Incident angle'!CW64","v":0},null,{"$f":"'Incident angle'!CY64","v":5},{"$f":"'Incident angle'!CZ64","v":0},{"$f":"'Incident angle'!DA64","v":0},{"$f":"'Incident angle'!DB64","v":0},{"$f":"'Incident angle'!DC64","v":0},{"$f":"'Incident angle'!DD64","v":0},{"$f":"'Incident angle'!DE64","v":0},{"$f":"'Incident angle'!DF64","v":0},{"$f":"'Incident angle'!DG64","v":0},{"$f":"'Incident angle'!DH64","v":0},{"$f":"'Incident angle'!DI64","v":0},{"$f":"'Incident angle'!DJ64","v":0},{"$f":"'Incident angle'!DK64","v":0},null,null,5,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,5,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,6,{"$f":"'Profile calcs'!Q9","v":-12.657580240548544},{"$f":"'Profile calcs'!R9","v":-9.2101030414712177},{"$f":"'Profile calcs'!S9","v":-3.3244141005449075},{"$f":"'Profile calcs'!T9","v":3.6714405326866673},{"$f":"'Profile calcs'!U9","v":7.9357874829851527},{"$f":"'Profile calcs'!V9","v":8.3930552361023523},{"$f":"'Profile calcs'!W9","v":5.9138516774857015},{"$f":"'Profile calcs'!X9","v":2.9679829754440079},{"$f":"'Profile calcs'!Y9","v":8.3279928680461496E-2},{"$f":"'Profile calcs'!Z9","v":-2.6465539816926205},{"$f":"'Profile calcs'!AA9","v":-7.1190871836640657},{"$f":"'Profile calcs'!AB9","v":-11.488991114943707},null,6,{"$f":"'Profile calcs'!AS9","v":37.148186571308415},{"$f":"'Profile calcs'!AT9","v":50.791383654081251},{"$f":"'Profile calcs'!AU9","v":-65.299999999999955},{"$f":"'Profile calcs'!AV9","v":17.58014754628174},{"$f":"'Profile calcs'!AW9","v":22.111172344820307},{"$f":"'Profile calcs'!AX9","v":19.79509046495318},{"$f":"'Profile calcs'!AY9","v":15.860431327653469},{"$f":"'Profile calcs'!AZ9","v":13.722280285934318},{"$f":"'Profile calcs'!BA9","v":-65.300000000005156},{"$f":"'Profile calcs'!BB9","v":13.894791408071976},{"$f":"'Profile calcs'!BC9","v":20.106401019882369},{"$f":"'Profile calcs'!BD9","v":27.885460484815273},null,{"$f":"'Dry Bulb'!C10","v":6},{"$f":"'Dry Bulb'!D10","v":48.92},{"$f":"'Dry Bulb'!E10","v":52.7},{"$f":"'Dry Bulb'!F10","v":59.36},{"$f":"'Dry Bulb'!G10","v":67.64},{"$f":"'Dry Bulb'!H10","v":78.8},{"$f":"'Dry Bulb'!I10","v":83.48},{"$f":"'Dry Bulb'!J10","v":85.28},{"$f":"'Dry Bulb'!K10","v":84.919999999999987},{"$f":"'Dry Bulb'!L10","v":79.7},{"$f":"'Dry Bulb'!M10","v":70.16},{"$f":"'Dry Bulb'!N10","v":59.18},{"$f":"'Dry Bulb'!O10","v":51.620000000000005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK65","v":6},{"$f":"'Incident angle'!CL65","v":0},{"$f":"'Incident angle'!CM65","v":0},{"$f":"'Incident angle'!CN65","v":0},{"$f":"'Incident angle'!CO65","v":0},{"$f":"'Incident angle'!CP65","v":0},{"$f":"'Incident angle'!CQ65","v":0},{"$f":"'Incident angle'!CR65","v":0},{"$f":"'Incident angle'!CS65","v":0},{"$f":"'Incident angle'!CT65","v":0},{"$f":"'Incident angle'!CU65","v":0},{"$f":"'Incident angle'!CV65","v":0},{"$f":"'Incident angle'!CW65","v":0},null,{"$f":"'Incident angle'!CY65","v":6},{"$f":"'Incident angle'!CZ65","v":0},{"$f":"'Incident angle'!DA65","v":0},{"$f":"'Incident angle'!DB65","v":0},{"$f":"'Incident angle'!DC65","v":0},{"$f":"'Incident angle'!DD65","v":0},{"$f":"'Incident angle'!DE65","v":0},{"$f":"'Incident angle'!DF65","v":0},{"$f":"'Incident angle'!DG65","v":0},{"$f":"'Incident angle'!DH65","v":0},{"$f":"'Incident angle'!DI65","v":0},{"$f":"'Incident angle'!DJ65","v":0},{"$f":"'Incident angle'!DK65","v":0},null,null,6,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,6,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,7,{"$f":"'Profile calcs'!Q10","v":0.75712395765969032},{"$f":"'Profile calcs'!R10","v":4.3819211908166711},{"$f":"'Profile calcs'!S10","v":10.327408658619172},{"$f":"'Profile calcs'!T10","v":17.146626992599682},{"$f":"'Profile calcs'!U10","v":21.134165658355119},{"$f":"'Profile calcs'!V10","v":21.477097073214686},{"$f":"'Profile calcs'!W10","v":19.142999224755304},{"$f":"'Profile calcs'!X10","v":16.444109273248728},{"$f":"'Profile calcs'!Y10","v":13.765898970431955},{"$f":"'Profile calcs'!Z10","v":11.107118463724456},{"$f":"'Profile calcs'!AA10","v":6.5087495886135249},{"$f":"'Profile calcs'!AB10","v":1.9226157929385757},null,7,{"$f":"'Profile calcs'!AS10","v":-1.8407058775768053},{"$f":"'Profile calcs'!AT10","v":-17.418156461309618},{"$f":"'Profile calcs'!AU10","v":-65.300000000000011},{"$f":"'Profile calcs'!AV10","v":72.609902347589809},{"$f":"'Profile calcs'!AW10","v":57.96115831293033},{"$f":"'Profile calcs'!AX10","v":51.874170400534645},{"$f":"'Profile calcs'!AY10","v":53.106981432720829},{"$f":"'Profile calcs'!AZ10","v":70.235558391915376},{"$f":"'Profile calcs'!BA10","v":-65.300000000000026},{"$f":"'Profile calcs'!BB10","v":-32.525623758734753},{"$f":"'Profile calcs'!BC10","v":-13.689263813478044},{"$f":"'Profile calcs'!BD10","v":-3.7902225360911941},null,{"$f":"'Dry Bulb'!C11","v":7},{"$f":"'Dry Bulb'!D11","v":48.92},{"$f":"'Dry Bulb'!E11","v":52.7},{"$f":"'Dry Bulb'!F11","v":59.36},{"$f":"'Dry Bulb'!G11","v":69.44},{"$f":"'Dry Bulb'!H11","v":80.78},{"$f":"'Dry Bulb'!I11","v":86.36},{"$f":"'Dry Bulb'!J11","v":87.98},{"$f":"'Dry Bulb'!K11","v":87.44},{"$f":"'Dry Bulb'!L11","v":81.680000000000007},{"$f":"'Dry Bulb'!M11","v":71.06},{"$f":"'Dry Bulb'!N11","v":58.82},{"$f":"'Dry Bulb'!O11","v":51.26},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK66","v":7},{"$f":"'Incident angle'!CL66","v":0},{"$f":"'Incident angle'!CM66","v":0},{"$f":"'Incident angle'!CN66","v":0},{"$f":"'Incident angle'!CO66","v":0},{"$f":"'Incident angle'!CP66","v":0},{"$f":"'Incident angle'!CQ66","v":0},{"$f":"'Incident angle'!CR66","v":0},{"$f":"'Incident angle'!CS66","v":0},{"$f":"'Incident angle'!CT66","v":0},{"$f":"'Incident angle'!CU66","v":0},{"$f":"'Incident angle'!CV66","v":0},{"$f":"'Incident angle'!CW66","v":0},null,{"$f":"'Incident angle'!CY66","v":7},{"$f":"'Incident angle'!CZ66","v":0},{"$f":"'Incident angle'!DA66","v":0},{"$f":"'Incident angle'!DB66","v":0},{"$f":"'Incident angle'!DC66","v":0},{"$f":"'Incident angle'!DD66","v":0},{"$f":"'Incident angle'!DE66","v":0},{"$f":"'Incident angle'!DF66","v":0},{"$f":"'Incident angle'!DG66","v":0},{"$f":"'Incident angle'!DH66","v":0},{"$f":"'Incident angle'!DI66","v":0},{"$f":"'Incident angle'!DJ66","v":0},{"$f":"'Incident angle'!DK66","v":0},null,null,7,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,7,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,8,{"$f":"'Profile calcs'!Q11","v":14.801512993977905},{"$f":"'Profile calcs'!R11","v":18.395161326018542},{"$f":"'Profile calcs'!S11","v":24.21988645529855},{"$f":"'Profile calcs'!T11","v":30.680730702005945},{"$f":"'Profile calcs'!U11","v":34.26512345162336},{"$f":"'Profile calcs'!V11","v":34.426376431243654},{"$f":"'Profile calcs'!W11","v":32.256035415094608},{"$f":"'Profile calcs'!X11","v":29.958921059436694},{"$f":"'Profile calcs'!Y11","v":27.765335603992927},{"$f":"'Profile calcs'!Z11","v":25.454349023394592},{"$f":"'Profile calcs'!AA11","v":20.939346821539349},{"$f":"'Profile calcs'!AB11","v":16.129552534651118},null,8,{"$f":"'Profile calcs'!AS11","v":-25.15497930142363},{"$f":"'Profile calcs'!AT11","v":-41.208162613283591},{"$f":"'Profile calcs'!AU11","v":-65.3},{"$f":"'Profile calcs'!AV11","v":-89.133910589679402},{"$f":"'Profile calcs'!AW11","v":77.392469719775818},{"$f":"'Profile calcs'!AX11","v":71.837796305169562},{"$f":"'Profile calcs'!AY11","v":74.90306712124648},{"$f":"'Profile calcs'!AZ11","v":89.880701812612699},{"$f":"'Profile calcs'!BA11","v":-65.300000000000011},{"$f":"'Profile calcs'!BB11","v":-45.709102960920774},{"$f":"'Profile calcs'!BC11","v":-30.711991515210528},{"$f":"'Profile calcs'!BD11","v":-23.133349654536577},null,{"$f":"'Dry Bulb'!C12","v":8},{"$f":"'Dry Bulb'!D12","v":51.26},{"$f":"'Dry Bulb'!E12","v":55.04},{"$f":"'Dry Bulb'!F12","v":62.42},{"$f":"'Dry Bulb'!G12","v":72.680000000000007},{"$f":"'Dry Bulb'!H12","v":84.38000000000001},{"$f":"'Dry Bulb'!I12","v":89.960000000000008},{"$f":"'Dry Bulb'!J12","v":91.580000000000013},{"$f":"'Dry Bulb'!K12","v":91.4},{"$f":"'Dry Bulb'!L12","v":86.18},{"$f":"'Dry Bulb'!M12","v":75.02},{"$f":"'Dry Bulb'!N12","v":63.68},{"$f":"'Dry Bulb'!O12","v":52.879999999999995},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK67","v":8},{"$f":"'Incident angle'!CL67","v":0},{"$f":"'Incident angle'!CM67","v":0},{"$f":"'Incident angle'!CN67","v":0},{"$f":"'Incident angle'!CO67","v":0},{"$f":"'Incident angle'!CP67","v":0},{"$f":"'Incident angle'!CQ67","v":0},{"$f":"'Incident angle'!CR67","v":0},{"$f":"'Incident angle'!CS67","v":0},{"$f":"'Incident angle'!CT67","v":0},{"$f":"'Incident angle'!CU67","v":0},{"$f":"'Incident angle'!CV67","v":0},{"$f":"'Incident angle'!CW67","v":0},null,{"$f":"'Incident angle'!CY67","v":8},{"$f":"'Incident angle'!CZ67","v":0},{"$f":"'Incident angle'!DA67","v":0},{"$f":"'Incident angle'!DB67","v":0},{"$f":"'Incident angle'!DC67","v":0},{"$f":"'Incident angle'!DD67","v":0},{"$f":"'Incident angle'!DE67","v":0},{"$f":"'Incident angle'!DF67","v":0},{"$f":"'Incident angle'!DG67","v":0},{"$f":"'Incident angle'!DH67","v":0},{"$f":"'Incident angle'!DI67","v":0},{"$f":"'Incident angle'!DJ67","v":0},{"$f":"'Incident angle'!DK67","v":0},null,null,8,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,8,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,9,{"$f":"'Profile calcs'!Q12","v":29.897860503845664},{"$f":"'Profile calcs'!R12","v":33.171578582642681},{"$f":"'Profile calcs'!S12","v":38.635878844024361},{"$f":"'Profile calcs'!T12","v":44.516730121969097},{"$f":"'Profile calcs'!U12","v":47.561101053580373},{"$f":"'Profile calcs'!V12","v":47.480410935356453},{"$f":"'Profile calcs'!W12","v":45.501067907501131},{"$f":"'Profile calcs'!X12","v":43.760303315048105},{"$f":"'Profile calcs'!Y12","v":42.346663637257642},{"$f":"'Profile calcs'!Z12","v":40.715743852069998},{"$f":"'Profile calcs'!AA12","v":36.595216615504739},{"$f":"'Profile calcs'!AB12","v":31.603785496296783},null,9,{"$f":"'Profile calcs'!AS12","v":-36.123628972409719},{"$f":"'Profile calcs'!AT12","v":-48.984103271498903},{"$f":"'Profile calcs'!AU12","v":-65.300000000000011},{"$f":"'Profile calcs'!AV12","v":-82.323917470741165},{"$f":"'Profile calcs'!AW12","v":86.682219236973438},{"$f":"'Profile calcs'!AX12","v":82.177260396790942},{"$f":"'Profile calcs'!AY12","v":85.346370921243249},{"$f":"'Profile calcs'!AZ12","v":-82.868918499232805},{"$f":"'Profile calcs'!BA12","v":-65.3},{"$f":"'Profile calcs'!BB12","v":-50.828908694033096},{"$f":"'Profile calcs'!BC12","v":-38.841664176975669},{"$f":"'Profile calcs'!BD12","v":-33.137728896941802},null,{"$f":"'Dry Bulb'!C13","v":9},{"$f":"'Dry Bulb'!D13","v":53.96},{"$f":"'Dry Bulb'!E13","v":57.92},{"$f":"'Dry Bulb'!F13","v":64.58},{"$f":"'Dry Bulb'!G13","v":77},{"$f":"'Dry Bulb'!H13","v":87.26},{"$f":"'Dry Bulb'!I13","v":93.38000000000001},{"$f":"'Dry Bulb'!J13","v":95.9},{"$f":"'Dry Bulb'!K13","v":96.080000000000013},{"$f":"'Dry Bulb'!L13","v":90.32},{"$f":"'Dry Bulb'!M13","v":79.16},{"$f":"'Dry Bulb'!N13","v":68.540000000000006},{"$f":"'Dry Bulb'!O13","v":55.76},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK68","v":9},{"$f":"'Incident angle'!CL68","v":0},{"$f":"'Incident angle'!CM68","v":0},{"$f":"'Incident angle'!CN68","v":0},{"$f":"'Incident angle'!CO68","v":0},{"$f":"'Incident angle'!CP68","v":0},{"$f":"'Incident angle'!CQ68","v":0},{"$f":"'Incident angle'!CR68","v":0},{"$f":"'Incident angle'!CS68","v":0},{"$f":"'Incident angle'!CT68","v":0},{"$f":"'Incident angle'!CU68","v":0},{"$f":"'Incident angle'!CV68","v":0},{"$f":"'Incident angle'!CW68","v":0},null,{"$f":"'Incident angle'!CY68","v":9},{"$f":"'Incident angle'!CZ68","v":0},{"$f":"'Incident angle'!DA68","v":0},{"$f":"'Incident angle'!DB68","v":0},{"$f":"'Incident angle'!DC68","v":0},{"$f":"'Incident angle'!DD68","v":0},{"$f":"'Incident angle'!DE68","v":0},{"$f":"'Incident angle'!DF68","v":0},{"$f":"'Incident angle'!DG68","v":0},{"$f":"'Incident angle'!DH68","v":0},{"$f":"'Incident angle'!DI68","v":0},{"$f":"'Incident angle'!DJ68","v":0},{"$f":"'Incident angle'!DK68","v":0},null,null,9,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,9,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,10,{"$f":"'Profile calcs'!Q13","v":46.432009669114628},{"$f":"'Profile calcs'!R13","v":48.982108380980456},{"$f":"'Profile calcs'!S13","v":53.761437623792659},{"$f":"'Profile calcs'!T13","v":58.790214649196741},{"$f":"'Profile calcs'!U13","v":61.14667544282198},{"$f":"'Profile calcs'!V13","v":60.771492120895445},{"$f":"'Profile calcs'!W13","v":59.020595594487986},{"$f":"'Profile calcs'!X13","v":57.990814089298965},{"$f":"'Profile calcs'!Y13","v":57.660184602658042},{"$f":"'Profile calcs'!Z13","v":57.085561042213271},{"$f":"'Profile calcs'!AA13","v":53.797693072162787},{"$f":"'Profile calcs'!AB13","v":48.774894172678039},null,10,{"$f":"'Profile calcs'!AS13","v":-41.565533524141735},{"$f":"'Profile calcs'!AT13","v":-52.391449411165141},{"$f":"'Profile calcs'!AU13","v":-65.300000000000011},{"$f":"'Profile calcs'!AV13","v":-79.183835184665355},{"$f":"'Profile calcs'!AW13","v":-88.633552185609801},{"$f":"'Profile calcs'!AX13","v":87.576455047188773},{"$f":"'Profile calcs'!AY13","v":-89.408737808154712},{"$f":"'Profile calcs'!AZ13","v":-79.54425546635963},{"$f":"'Profile calcs'!BA13","v":-65.3},{"$f":"'Profile calcs'!BB13","v":-53.228063715971977},{"$f":"'Profile calcs'!BC13","v":-42.944409695388977},{"$f":"'Profile calcs'!BD13","v":-38.364397938009652},null,{"$f":"'Dry Bulb'!C14","v":10},{"$f":"'Dry Bulb'!D14","v":56.84},{"$f":"'Dry Bulb'!E14","v":60.980000000000004},{"$f":"'Dry Bulb'!F14","v":67.459999999999994},{"$f":"'Dry Bulb'!G14","v":80.42},{"$f":"'Dry Bulb'!H14","v":90.32},{"$f":"'Dry Bulb'!I14","v":96.44},{"$f":"'Dry Bulb'!J14","v":99.68},{"$f":"'Dry Bulb'!K14","v":100.22},{"$f":"'Dry Bulb'!L14","v":93.919999999999987},{"$f":"'Dry Bulb'!M14","v":82.94},{"$f":"'Dry Bulb'!N14","v":72.5},{"$f":"'Dry Bulb'!O14","v":58.82},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK69","v":10},{"$f":"'Incident angle'!CL69","v":0},{"$f":"'Incident angle'!CM69","v":0},{"$f":"'Incident angle'!CN69","v":0},{"$f":"'Incident angle'!CO69","v":0},{"$f":"'Incident angle'!CP69","v":0},{"$f":"'Incident angle'!CQ69","v":0},{"$f":"'Incident angle'!CR69","v":0},{"$f":"'Incident angle'!CS69","v":0},{"$f":"'Incident angle'!CT69","v":0},{"$f":"'Incident angle'!CU69","v":0},{"$f":"'Incident angle'!CV69","v":0},{"$f":"'Incident angle'!CW69","v":0},null,{"$f":"'Incident angle'!CY69","v":10},{"$f":"'Incident angle'!CZ69","v":0},{"$f":"'Incident angle'!DA69","v":0},{"$f":"'Incident angle'!DB69","v":0},{"$f":"'Incident angle'!DC69","v":0},{"$f":"'Incident angle'!DD69","v":0},{"$f":"'Incident angle'!DE69","v":0},{"$f":"'Incident angle'!DF69","v":0},{"$f":"'Incident angle'!DG69","v":0},{"$f":"'Incident angle'!DH69","v":0},{"$f":"'Incident angle'!DI69","v":0},{"$f":"'Incident angle'!DJ69","v":0},{"$f":"'Incident angle'!DK69","v":0},null,null,10,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,10,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,11,{"$f":"'Profile calcs'!Q14","v":64.562443951008888},{"$f":"'Profile calcs'!R14","v":65.901314539685401},{"$f":"'Profile calcs'!S14","v":69.61109114186894},{"$f":"'Profile calcs'!T14","v":73.497168133288227},{"$f":"'Profile calcs'!U14","v":75.027677809677201},{"$f":"'Profile calcs'!V14","v":74.319781349482838},{"$f":"'Profile calcs'!W14","v":72.839713407261911},{"$f":"'Profile calcs'!X14","v":72.655436766674285},{"$f":"'Profile calcs'!Y14","v":73.666960034724283},{"$f":"'Profile calcs'!Z14","v":74.489845422408862},{"$f":"'Profile calcs'!AA14","v":72.52990498677552},{"$f":"'Profile calcs'!AB14","v":67.776371428052769},null,11,{"$f":"'Profile calcs'!AS14","v":-44.282217904128672},{"$f":"'Profile calcs'!AT14","v":-54.018451059115115},{"$f":"'Profile calcs'!AU14","v":-65.300000000000011},{"$f":"'Profile calcs'!AV14","v":-77.69612062717222},{"$f":"'Profile calcs'!AW14","v":-86.343646743656691},{"$f":"'Profile calcs'!AX14","v":-89.714212091310301},{"$f":"'Profile calcs'!AY14","v":-86.798330968762997},{"$f":"'Profile calcs'!AZ14","v":-77.960826272965903},{"$f":"'Profile calcs'!BA14","v":-65.300000000000011},{"$f":"'Profile calcs'!BB14","v":-54.328164209664372},{"$f":"'Profile calcs'!BC14","v":-44.893647845797645},{"$f":"'Profile calcs'!BD14","v":-40.97067975660989},null,{"$f":"'Dry Bulb'!C15","v":11},{"$f":"'Dry Bulb'!D15","v":59.36},{"$f":"'Dry Bulb'!E15","v":64.400000000000006},{"$f":"'Dry Bulb'!F15","v":69.98},{"$f":"'Dry Bulb'!G15","v":83.3},{"$f":"'Dry Bulb'!H15","v":92.84},{"$f":"'Dry Bulb'!I15","v":99.14},{"$f":"'Dry Bulb'!J15","v":102.56},{"$f":"'Dry Bulb'!K15","v":103.64},{"$f":"'Dry Bulb'!L15","v":96.44},{"$f":"'Dry Bulb'!M15","v":86},{"$f":"'Dry Bulb'!N15","v":76.099999999999994},{"$f":"'Dry Bulb'!O15","v":61.88},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK70","v":11},{"$f":"'Incident angle'!CL70","v":0},{"$f":"'Incident angle'!CM70","v":0},{"$f":"'Incident angle'!CN70","v":0},{"$f":"'Incident angle'!CO70","v":0},{"$f":"'Incident angle'!CP70","v":0},{"$f":"'Incident angle'!CQ70","v":0},{"$f":"'Incident angle'!CR70","v":0},{"$f":"'Incident angle'!CS70","v":0},{"$f":"'Incident angle'!CT70","v":0},{"$f":"'Incident angle'!CU70","v":0},{"$f":"'Incident angle'!CV70","v":0},{"$f":"'Incident angle'!CW70","v":0},null,{"$f":"'Incident angle'!CY70","v":11},{"$f":"'Incident angle'!CZ70","v":0},{"$f":"'Incident angle'!DA70","v":0},{"$f":"'Incident angle'!DB70","v":0},{"$f":"'Incident angle'!DC70","v":0},{"$f":"'Incident angle'!DD70","v":0},{"$f":"'Incident angle'!DE70","v":0},{"$f":"'Incident angle'!DF70","v":0},{"$f":"'Incident angle'!DG70","v":0},{"$f":"'Incident angle'!DH70","v":0},{"$f":"'Incident angle'!DI70","v":0},{"$f":"'Incident angle'!DJ70","v":0},{"$f":"'Incident angle'!DK70","v":0},null,null,11,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,11,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,12,{"$f":"'Profile calcs'!Q15","v":83.953055253243946},{"$f":"'Profile calcs'!R15","v":83.672477687445479},{"$f":"'Profile calcs'!S15","v":85.9744082667399},{"$f":"'Profile calcs'!T15","v":88.486518830478445},{"$f":"'Profile calcs'!U15","v":89.098541577633242},{"$f":"'Profile calcs'!V15","v":88.042480487312574},{"$f":"'Profile calcs'!W15","v":86.869712514125027},{"$f":"'Profile calcs'!X15","v":87.612299057311645},{"$f":"'Profile calcs'!Y15","v":89.899102008780474},{"$f":"'Profile calcs'!Z15","v":87.509028766495277},{"$f":"'Profile calcs'!AA15","v":87.799307231125709},{"$f":"'Profile calcs'!AB15","v":88.09804255680524},null,12,{"$f":"'Profile calcs'!AS15","v":-45.341192522261665},{"$f":"'Profile calcs'!AT15","v":-54.65622400407787},{"$f":"'Profile calcs'!AU15","v":-65.300000000000011},{"$f":"'Profile calcs'!AV15","v":-77.204007036944958},{"$f":"'Profile calcs'!AW15","v":-85.602608099870324},{"$f":"'Profile calcs'!AX15","v":-88.764506326073786},{"$f":"'Profile calcs'!AY15","v":-85.831844934745362},{"$f":"'Profile calcs'!AZ15","v":-77.410166839433359},{"$f":"'Profile calcs'!BA15","v":-65.3},{"$f":"'Profile calcs'!BB15","v":-54.593196533889113},{"$f":"'Profile calcs'!BC15","v":-45.392239295822165},{"$f":"'Profile calcs'!BD15","v":-41.843902161818413},null,{"$f":"'Dry Bulb'!C16","v":12},{"$f":"'Dry Bulb'!D16","v":61.88},{"$f":"'Dry Bulb'!E16","v":66.92},{"$f":"'Dry Bulb'!F16","v":71.599999999999994},{"$f":"'Dry Bulb'!G16","v":85.460000000000008},{"$f":"'Dry Bulb'!H16","v":94.82},{"$f":"'Dry Bulb'!I16","v":101.48},{"$f":"'Dry Bulb'!J16","v":104.36},{"$f":"'Dry Bulb'!K16","v":105.61999999999999},{"$f":"'Dry Bulb'!L16","v":98.24},{"$f":"'Dry Bulb'!M16","v":88.52},{"$f":"'Dry Bulb'!N16","v":78.62},{"$f":"'Dry Bulb'!O16","v":64.040000000000006},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK71","v":12},{"$f":"'Incident angle'!CL71","v":0},{"$f":"'Incident angle'!CM71","v":0},{"$f":"'Incident angle'!CN71","v":0},{"$f":"'Incident angle'!CO71","v":0},{"$f":"'Incident angle'!CP71","v":0},{"$f":"'Incident angle'!CQ71","v":0},{"$f":"'Incident angle'!CR71","v":0},{"$f":"'Incident angle'!CS71","v":0},{"$f":"'Incident angle'!CT71","v":0},{"$f":"'Incident angle'!CU71","v":0},{"$f":"'Incident angle'!CV71","v":0},{"$f":"'Incident angle'!CW71","v":0},null,{"$f":"'Incident angle'!CY71","v":12},{"$f":"'Incident angle'!CZ71","v":0},{"$f":"'Incident angle'!DA71","v":0},{"$f":"'Incident angle'!DB71","v":0},{"$f":"'Incident angle'!DC71","v":0},{"$f":"'Incident angle'!DD71","v":0},{"$f":"'Incident angle'!DE71","v":0},{"$f":"'Incident angle'!DF71","v":0},{"$f":"'Incident angle'!DG71","v":0},{"$f":"'Incident angle'!DH71","v":0},{"$f":"'Incident angle'!DI71","v":0},{"$f":"'Incident angle'!DJ71","v":0},{"$f":"'Incident angle'!DK71","v":0},null,null,12,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,12,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,13,{"$f":"'Profile calcs'!Q16","v":-76.310236007231211},{"$f":"'Profile calcs'!R16","v":-78.301959925225134},{"$f":"'Profile calcs'!S16","v":-77.550222553106039},{"$f":"'Profile calcs'!T16","v":-76.496177068295182},{"$f":"'Profile calcs'!U16","v":-76.818295906325048},{"$f":"'Profile calcs'!V16","v":-78.211108618523411},{"$f":"'Profile calcs'!W16","v":-79.058019787475942},{"$f":"'Profile calcs'!X16","v":-77.387091031608094},{"$f":"'Profile calcs'!Y16","v":-73.467983805952144},{"$f":"'Profile calcs'!Z16","v":-69.609222192948593},{"$f":"'Profile calcs'!AA16","v":-68.255417985347776},{"$f":"'Profile calcs'!AB16","v":-71.453363412613228},null,13,{"$f":"'Profile calcs'!AS16","v":-45.093307228609767},{"$f":"'Profile calcs'!AT16","v":-54.548508865098285},{"$f":"'Profile calcs'!AU16","v":-65.300000000000011},{"$f":"'Profile calcs'!AV16","v":-77.527686129155384},{"$f":"'Profile calcs'!AW16","v":-86.172088859931137},{"$f":"'Profile calcs'!AX16","v":-89.286545413103582},{"$f":"'Profile calcs'!AY16","v":-86.195448533480899},{"$f":"'Profile calcs'!AZ16","v":-77.690264015558725},{"$f":"'Profile calcs'!BA16","v":-65.300000000000011},{"$f":"'Profile calcs'!BB16","v":-54.1192638814804},{"$f":"'Profile calcs'!BC16","v":-44.599954197716883},{"$f":"'Profile calcs'!BD16","v":-41.247836270078757},null,{"$f":"'Dry Bulb'!C17","v":13},{"$f":"'Dry Bulb'!D17","v":63.86},{"$f":"'Dry Bulb'!E17","v":69.62},{"$f":"'Dry Bulb'!F17","v":75.2},{"$f":"'Dry Bulb'!G17","v":86.72},{"$f":"'Dry Bulb'!H17","v":96.8},{"$f":"'Dry Bulb'!I17","v":102.74},{"$f":"'Dry Bulb'!J17","v":105.8},{"$f":"'Dry Bulb'!K17","v":107.6},{"$f":"'Dry Bulb'!L17","v":100.03999999999999},{"$f":"'Dry Bulb'!M17","v":90.32},{"$f":"'Dry Bulb'!N17","v":80.78},{"$f":"'Dry Bulb'!O17","v":66.2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK72","v":13},{"$f":"'Incident angle'!CL72","v":0},{"$f":"'Incident angle'!CM72","v":0},{"$f":"'Incident angle'!CN72","v":0},{"$f":"'Incident angle'!CO72","v":0},{"$f":"'Incident angle'!CP72","v":0},{"$f":"'Incident angle'!CQ72","v":0},{"$f":"'Incident angle'!CR72","v":0},{"$f":"'Incident angle'!CS72","v":0},{"$f":"'Incident angle'!CT72","v":0},{"$f":"'Incident angle'!CU72","v":0},{"$f":"'Incident angle'!CV72","v":0},{"$f":"'Incident angle'!CW72","v":0},null,{"$f":"'Incident angle'!CY72","v":13},{"$f":"'Incident angle'!CZ72","v":0},{"$f":"'Incident angle'!DA72","v":0},{"$f":"'Incident angle'!DB72","v":0},{"$f":"'Incident angle'!DC72","v":0},{"$f":"'Incident angle'!DD72","v":0},{"$f":"'Incident angle'!DE72","v":0},{"$f":"'Incident angle'!DF72","v":0},{"$f":"'Incident angle'!DG72","v":0},{"$f":"'Incident angle'!DH72","v":0},{"$f":"'Incident angle'!DI72","v":0},{"$f":"'Incident angle'!DJ72","v":0},{"$f":"'Incident angle'!DK72","v":0},null,null,13,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,13,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,14,{"$f":"'Profile calcs'!Q17","v":-57.32973993752023},{"$f":"'Profile calcs'!R17","v":-60.7360775958551},{"$f":"'Profile calcs'!S17","v":-61.409664244736106},{"$f":"'Profile calcs'!T17","v":-61.715956668379413},{"$f":"'Profile calcs'!U17","v":-62.905108672619058},{"$f":"'Profile calcs'!V17","v":-64.600922398571711},{"$f":"'Profile calcs'!W17","v":-65.128294922488053},{"$f":"'Profile calcs'!X17","v":-62.607791450328726},{"$f":"'Profile calcs'!Y17","v":-57.468525117430246},{"$f":"'Profile calcs'!Z17","v":-52.462028938168871},{"$f":"'Profile calcs'!AA17","v":-49.834295771439308},{"$f":"'Profile calcs'!AB17","v":-52.146583450749397},null,14,{"$f":"'Profile calcs'!AS17","v":-43.459732841647046},{"$f":"'Profile calcs'!AT17","v":-53.656578483668653},{"$f":"'Profile calcs'!AU17","v":-65.3},{"$f":"'Profile calcs'!AV17","v":-78.783422467977033},{"$f":"'Profile calcs'!AW17","v":-88.233716701902779},{"$f":"'Profile calcs'!AX17","v":88.563972173918145},{"$f":"'Profile calcs'!AY17","v":-88.003822246360016},{"$f":"'Profile calcs'!AZ17","v":-78.901150124498145},{"$f":"'Profile calcs'!BA17","v":-65.300000000000011},{"$f":"'Profile calcs'!BB17","v":-52.730352015763074},{"$f":"'Profile calcs'!BC17","v":-42.259093988308607},{"$f":"'Profile calcs'!BD17","v":-39.004315155295124},null,{"$f":"'Dry Bulb'!C18","v":14},{"$f":"'Dry Bulb'!D18","v":65.48},{"$f":"'Dry Bulb'!E18","v":71.599999999999994},{"$f":"'Dry Bulb'!F18","v":76.819999999999993},{"$f":"'Dry Bulb'!G18","v":88.16},{"$f":"'Dry Bulb'!H18","v":98.24},{"$f":"'Dry Bulb'!I18","v":104.9},{"$f":"'Dry Bulb'!J18","v":107.41999999999999},{"$f":"'Dry Bulb'!K18","v":108.5},{"$f":"'Dry Bulb'!L18","v":101.11999999999999},{"$f":"'Dry Bulb'!M18","v":91.76},{"$f":"'Dry Bulb'!N18","v":81.680000000000007},{"$f":"'Dry Bulb'!O18","v":67.64},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK73","v":14},{"$f":"'Incident angle'!CL73","v":0},{"$f":"'Incident angle'!CM73","v":0},{"$f":"'Incident angle'!CN73","v":0},{"$f":"'Incident angle'!CO73","v":0},{"$f":"'Incident angle'!CP73","v":0},{"$f":"'Incident angle'!CQ73","v":0},{"$f":"'Incident angle'!CR73","v":0},{"$f":"'Incident angle'!CS73","v":0},{"$f":"'Incident angle'!CT73","v":0},{"$f":"'Incident angle'!CU73","v":0.59894762087049969},{"$f":"'Incident angle'!CV73","v":0.26376602957948858},{"$f":"'Incident angle'!CW73","v":8.3417589987308416E-2},null,{"$f":"'Incident angle'!CY73","v":14},{"$f":"'Incident angle'!CZ73","v":0},{"$f":"'Incident angle'!DA73","v":0},{"$f":"'Incident angle'!DB73","v":0},{"$f":"'Incident angle'!DC73","v":0},{"$f":"'Incident angle'!DD73","v":0},{"$f":"'Incident angle'!DE73","v":0},{"$f":"'Incident angle'!DF73","v":0},{"$f":"'Incident angle'!DG73","v":0},{"$f":"'Incident angle'!DH73","v":0},{"$f":"'Incident angle'!DI73","v":0},{"$f":"'Incident angle'!DJ73","v":0},{"$f":"'Incident angle'!DK73","v":0},null,null,14,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,14,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,15,{"$f":"'Profile calcs'!Q18","v":-39.812986834028628},{"$f":"'Profile calcs'!R18","v":-44.138369778725995},{"$f":"'Profile calcs'!S18","v":-45.919354280104955},{"$f":"'Profile calcs'!T18","v":-47.350089337983867},{"$f":"'Profile calcs'!U18","v":-49.279589339957219},{"$f":"'Profile calcs'!V18","v":-51.233884049672319},{"$f":"'Profile calcs'!W18","v":-51.471577651808317},{"$f":"'Profile calcs'!X18","v":-48.232694478544275},{"$f":"'Profile calcs'!Y18","v":-42.164171017516459},{"$f":"'Profile calcs'!Z18","v":-36.404340467875535},{"$f":"'Profile calcs'!AA18","v":-32.990491768082641},{"$f":"'Profile calcs'!AB18","v":-34.633273198345073},null,15,{"$f":"'Profile calcs'!AS18","v":-39.870560777390232},{"$f":"'Profile calcs'!AT18","v":-51.621185830048873},{"$f":"'Profile calcs'!AU18","v":-65.300000000000011},{"$f":"'Profile calcs'!AV18","v":-81.497322169487106},{"$f":"'Profile calcs'!AW18","v":87.46971071470432},{"$f":"'Profile calcs'!AX18","v":84.081683557615165},{"$f":"'Profile calcs'!AY18","v":88.112119041692722},{"$f":"'Profile calcs'!AZ18","v":-81.541825162483974},{"$f":"'Profile calcs'!BA18","v":-65.300000000000011},{"$f":"'Profile calcs'!BB18","v":-49.795844682730106},{"$f":"'Profile calcs'!BC18","v":-37.488190980331893},{"$f":"'Profile calcs'!BD18","v":-34.371615174618547},null,{"$f":"'Dry Bulb'!C19","v":15},{"$f":"'Dry Bulb'!D19","v":66.02},{"$f":"'Dry Bulb'!E19","v":72.680000000000007},{"$f":"'Dry Bulb'!F19","v":77.900000000000006},{"$f":"'Dry Bulb'!G19","v":89.06},{"$f":"'Dry Bulb'!H19","v":98.6},{"$f":"'Dry Bulb'!I19","v":105.61999999999999},{"$f":"'Dry Bulb'!J19","v":108.32},{"$f":"'Dry Bulb'!K19","v":108.86},{"$f":"'Dry Bulb'!L19","v":101.84},{"$f":"'Dry Bulb'!M19","v":92.66},{"$f":"'Dry Bulb'!N19","v":82.94},{"$f":"'Dry Bulb'!O19","v":68.36},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK74","v":15},{"$f":"'Incident angle'!CL74","v":0.57014029461573867},{"$f":"'Incident angle'!CM74","v":0.86127599718114978},{"$f":"'Incident angle'!CN74","v":1},{"$f":"'Incident angle'!CO74","v":1},{"$f":"'Incident angle'!CP74","v":1},{"$f":"'Incident angle'!CQ74","v":1},{"$f":"'Incident angle'!CR74","v":1},{"$f":"'Incident angle'!CS74","v":1},{"$f":"'Incident angle'!CT74","v":1},{"$f":"'Incident angle'!CU74","v":0.92771380590744001},{"$f":"'Incident angle'!CV74","v":0.68242887791708595},{"$f":"'Incident angle'!CW74","v":0.56294774267755432},null,{"$f":"'Incident angle'!CY74","v":15},{"$f":"'Incident angle'!CZ74","v":0},{"$f":"'Incident angle'!DA74","v":0},{"$f":"'Incident angle'!DB74","v":0},{"$f":"'Incident angle'!DC74","v":0},{"$f":"'Incident angle'!DD74","v":0},{"$f":"'Incident angle'!DE74","v":0},{"$f":"'Incident angle'!DF74","v":0},{"$f":"'Incident angle'!DG74","v":0},{"$f":"'Incident angle'!DH74","v":0},{"$f":"'Incident angle'!DI74","v":0},{"$f":"'Incident angle'!DJ74","v":0},{"$f":"'Incident angle'!DK74","v":0},null,null,15,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,15,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,16,{"$f":"'Profile calcs'!Q19","v":-23.875002480593199},{"$f":"'Profile calcs'!R19","v":-28.656528802721059},{"$f":"'Profile calcs'!S19","v":-31.171654482760921},{"$f":"'Profile calcs'!T19","v":-33.432906045521179},{"$f":"'Profile calcs'!U19","v":-35.951128585501792},{"$f":"'Profile calcs'!V19","v":-38.121029600348642},{"$f":"'Profile calcs'!W19","v":-38.115343474138719},{"$f":"'Profile calcs'!X19","v":-34.304400656996243},{"$f":"'Profile calcs'!Y19","v":-27.591172995772371},{"$f":"'Profile calcs'!Z19","v":-21.421982311981434},{"$f":"'Profile calcs'!AA19","v":-17.641166819660786},{"$f":"'Profile calcs'!AB19","v":-18.874041457280981},null,16,{"$f":"'Profile calcs'!AS19","v":-32.771924244272576},{"$f":"'Profile calcs'!AT19","v":-47.337670667006861},{"$f":"'Profile calcs'!AU19","v":-65.3},{"$f":"'Profile calcs'!AV19","v":-87.26038909875615},{"$f":"'Profile calcs'!AW19","v":78.980403720895197},{"$f":"'Profile calcs'!AX19","v":75.501608463035367},{"$f":"'Profile calcs'!AY19","v":80.468716677637929},{"$f":"'Profile calcs'!AZ19","v":-87.115145464657999},{"$f":"'Profile calcs'!BA19","v":-65.300000000000011},{"$f":"'Profile calcs'!BB19","v":-43.332777142141182},{"$f":"'Profile calcs'!BC19","v":-27.965917871646653},{"$f":"'Profile calcs'!BD19","v":-25.506940411380103},null,{"$f":"'Dry Bulb'!C20","v":16},{"$f":"'Dry Bulb'!D20","v":66.2},{"$f":"'Dry Bulb'!E20","v":72.319999999999993},{"$f":"'Dry Bulb'!F20","v":78.259999999999991},{"$f":"'Dry Bulb'!G20","v":88.34},{"$f":"'Dry Bulb'!H20","v":98.78},{"$f":"'Dry Bulb'!I20","v":105.8},{"$f":"'Dry Bulb'!J20","v":108.14},{"$f":"'Dry Bulb'!K20","v":108.32},{"$f":"'Dry Bulb'!L20","v":101.66},{"$f":"'Dry Bulb'!M20","v":92.11999999999999},{"$f":"'Dry Bulb'!N20","v":82.04},{"$f":"'Dry Bulb'!O20","v":67.64},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK75","v":16},{"$f":"'Incident angle'!CL75","v":0.79541267501641133},{"$f":"'Incident angle'!CM75","v":0.99722917431931501},{"$f":"'Incident angle'!CN75","v":1},{"$f":"'Incident angle'!CO75","v":1},{"$f":"'Incident angle'!CP75","v":1},{"$f":"'Incident angle'!CQ75","v":1},{"$f":"'Incident angle'!CR75","v":1},{"$f":"'Incident angle'!CS75","v":1},{"$f":"'Incident angle'!CT75","v":1},{"$f":"'Incident angle'!CU75","v":1},{"$f":"'Incident angle'!CV75","v":0.87146580361454828},{"$f":"'Incident angle'!CW75","v":0.75810235728560871},null,{"$f":"'Incident angle'!CY75","v":16},{"$f":"'Incident angle'!CZ75","v":0},{"$f":"'Incident angle'!DA75","v":0},{"$f":"'Incident angle'!DB75","v":0},{"$f":"'Incident angle'!DC75","v":0},{"$f":"'Incident angle'!DD75","v":0},{"$f":"'Incident angle'!DE75","v":0},{"$f":"'Incident angle'!DF75","v":0},{"$f":"'Incident angle'!DG75","v":0},{"$f":"'Incident angle'!DH75","v":0},{"$f":"'Incident angle'!DI75","v":0},{"$f":"'Incident angle'!DJ75","v":0},{"$f":"'Incident angle'!DK75","v":0},null,null,16,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,16,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,17,{"$f":"'Profile calcs'!Q20","v":-9.2385105897919768},{"$f":"'Profile calcs'!R20","v":-14.141799097654047},{"$f":"'Profile calcs'!S20","v":-17.05480132909042},{"$f":"'Profile calcs'!T20","v":-19.854676249106344},{"$f":"'Profile calcs'!U20","v":-22.809925103490791},{"$f":"'Profile calcs'!V20","v":-25.161800037123335},{"$f":"'Profile calcs'!W20","v":-24.96833403497148},{"$f":"'Profile calcs'!X20","v":-20.721091695019808},{"$f":"'Profile calcs'!Y20","v":-13.597367832295648},{"$f":"'Profile calcs'!Z20","v":-7.2728027816997747},{"$f":"'Profile calcs'!AA20","v":-3.4258822939894862},{"$f":"'Profile calcs'!AB20","v":-4.469701583642955},null,17,{"$f":"'Profile calcs'!AS20","v":-18.097147561415564},{"$f":"'Profile calcs'!AT20","v":-36.909432298850398},{"$f":"'Profile calcs'!AU20","v":-65.300000000000011},{"$f":"'Profile calcs'!AV20","v":78.138866865290566},{"$f":"'Profile calcs'!AW20","v":61.321747515833657},{"$f":"'Profile calcs'!AX20","v":58.882202464658548},{"$f":"'Profile calcs'!AY20","v":64.773504841898102},{"$f":"'Profile calcs'!AZ20","v":79.038177006237575},{"$f":"'Profile calcs'!BA20","v":-65.299999999999983},{"$f":"'Profile calcs'!BB20","v":-25.128119824042177},{"$f":"'Profile calcs'!BC20","v":-7.7999612458558714},{"$f":"'Profile calcs'!BD20","v":-8.3339473373382997},null,{"$f":"'Dry Bulb'!C21","v":17},{"$f":"'Dry Bulb'!D21","v":65.12},{"$f":"'Dry Bulb'!E21","v":70.88},{"$f":"'Dry Bulb'!F21","v":77.180000000000007},{"$f":"'Dry Bulb'!G21","v":86.72},{"$f":"'Dry Bulb'!H21","v":98.6},{"$f":"'Dry Bulb'!I21","v":105.08000000000001},{"$f":"'Dry Bulb'!J21","v":107.6},{"$f":"'Dry Bulb'!K21","v":107.06},{"$f":"'Dry Bulb'!L21","v":100.22},{"$f":"'Dry Bulb'!M21","v":91.039999999999992},{"$f":"'Dry Bulb'!N21","v":80.42},{"$f":"'Dry Bulb'!O21","v":65.66},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK76","v":17},{"$f":"'Incident angle'!CL76","v":1},{"$f":"'Incident angle'!CM76","v":1},{"$f":"'Incident angle'!CN76","v":1},{"$f":"'Incident angle'!CO76","v":1},{"$f":"'Incident angle'!CP76","v":1},{"$f":"'Incident angle'!CQ76","v":1},{"$f":"'Incident angle'!CR76","v":1},{"$f":"'Incident angle'!CS76","v":1},{"$f":"'Incident angle'!CT76","v":1},{"$f":"'Incident angle'!CU76","v":1},{"$f":"'Incident angle'!CV76","v":1},{"$f":"'Incident angle'!CW76","v":0.94109284264869175},null,{"$f":"'Incident angle'!CY76","v":17},{"$f":"'Incident angle'!CZ76","v":0},{"$f":"'Incident angle'!DA76","v":0},{"$f":"'Incident angle'!DB76","v":0},{"$f":"'Incident angle'!DC76","v":0},{"$f":"'Incident angle'!DD76","v":0},{"$f":"'Incident angle'!DE76","v":0},{"$f":"'Incident angle'!DF76","v":0},{"$f":"'Incident angle'!DG76","v":0},{"$f":"'Incident angle'!DH76","v":0},{"$f":"'Incident angle'!DI76","v":0},{"$f":"'Incident angle'!DJ76","v":0},{"$f":"'Incident angle'!DK76","v":0},null,null,17,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,17,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,18,{"$f":"'Profile calcs'!Q21","v":4.5124409084911488},{"$f":"'Profile calcs'!R21","v":-0.2911309486956099},{"$f":"'Profile calcs'!S21","v":-3.324414100544868},{"$f":"'Profile calcs'!T21","v":-6.3911335111384062},{"$f":"'Profile calcs'!U21","v":-9.6364921571497923},{"$f":"'Profile calcs'!V21","v":-12.146410157593207},{"$f":"'Profile calcs'!W21","v":-11.827587615885065},{"$f":"'Profile calcs'!X21","v":-7.2645164628018666},{"$f":"'Profile calcs'!Y21","v":8.3279928680489793E-2},{"$f":"'Profile calcs'!Z21","v":6.378749450365131},{"$f":"'Profile calcs'!AA21","v":10.079870372411358},{"$f":"'Profile calcs'!AB21","v":9.055310015770992},null,18,{"$f":"'Profile calcs'!AS21","v":12.251813428691671},{"$f":"'Profile calcs'!AT21","v":-1.3913836540812599},{"$f":"'Profile calcs'!AU21","v":-65.299999999999983},{"$f":"'Profile calcs'!AV21","v":31.819852453718237},{"$f":"'Profile calcs'!AW21","v":27.288827655179634},{"$f":"'Profile calcs'!AX21","v":29.60490953504689},{"$f":"'Profile calcs'!AY21","v":33.539568672346483},{"$f":"'Profile calcs'!AZ21","v":35.677719714065745},{"$f":"'Profile calcs'!BA21","v":-65.300000000001333},{"$f":"'Profile calcs'!BB21","v":35.505208591928337},{"$f":"'Profile calcs'!BC21","v":29.293598980117594},{"$f":"'Profile calcs'!BD21","v":21.514539515184662},null,{"$f":"'Dry Bulb'!C22","v":18},{"$f":"'Dry Bulb'!D22","v":63.32},{"$f":"'Dry Bulb'!E22","v":69.08},{"$f":"'Dry Bulb'!F22","v":75.92},{"$f":"'Dry Bulb'!G22","v":85.28},{"$f":"'Dry Bulb'!H22","v":97.34},{"$f":"'Dry Bulb'!I22","v":104.18},{"$f":"'Dry Bulb'!J22","v":106.16},{"$f":"'Dry Bulb'!K22","v":105.44},{"$f":"'Dry Bulb'!L22","v":99.14},{"$f":"'Dry Bulb'!M22","v":89.6},{"$f":"'Dry Bulb'!N22","v":77.900000000000006},{"$f":"'Dry Bulb'!O22","v":64.400000000000006},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK77","v":18},{"$f":"'Incident angle'!CL77","v":0},{"$f":"'Incident angle'!CM77","v":1},{"$f":"'Incident angle'!CN77","v":1},{"$f":"'Incident angle'!CO77","v":1},{"$f":"'Incident angle'!CP77","v":1},{"$f":"'Incident angle'!CQ77","v":1},{"$f":"'Incident angle'!CR77","v":1},{"$f":"'Incident angle'!CS77","v":1},{"$f":"'Incident angle'!CT77","v":0},{"$f":"'Incident angle'!CU77","v":0},{"$f":"'Incident angle'!CV77","v":0},{"$f":"'Incident angle'!CW77","v":0},null,{"$f":"'Incident angle'!CY77","v":18},{"$f":"'Incident angle'!CZ77","v":0},{"$f":"'Incident angle'!DA77","v":0},{"$f":"'Incident angle'!DB77","v":0},{"$f":"'Incident angle'!DC77","v":0},{"$f":"'Incident angle'!DD77","v":0},{"$f":"'Incident angle'!DE77","v":0},{"$f":"'Incident angle'!DF77","v":0},{"$f":"'Incident angle'!DG77","v":0},{"$f":"'Incident angle'!DH77","v":0},{"$f":"'Incident angle'!DI77","v":0},{"$f":"'Incident angle'!DJ77","v":0},{"$f":"'Incident angle'!DK77","v":0},null,null,18,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,18,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,19,{"$f":"'Profile calcs'!Q22","v":17.787083138469381},{"$f":"'Profile calcs'!R22","v":13.241926751478145},{"$f":"'Profile calcs'!S22","v":10.3274086586192},{"$f":"'Profile calcs'!T22","v":7.2612910314068415},{"$f":"'Profile calcs'!U22","v":3.8834912247576012},{"$f":"'Profile calcs'!V22","v":1.2368871636337018},{"$f":"'Profile calcs'!W22","v":1.6074102522073654},{"$f":"'Profile calcs'!X22","v":6.3652304276825138},{"$f":"'Profile calcs'!Y22","v":13.765898970431998},{"$f":"'Profile calcs'!Z22","v":19.875382193162707},{"$f":"'Profile calcs'!AA22","v":23.262321940359538},{"$f":"'Profile calcs'!AB22","v":22.125354369783608},null,19,{"$f":"'Profile calcs'!AS22","v":51.240705877576879},{"$f":"'Profile calcs'!AT22","v":66.818156461309655},{"$f":"'Profile calcs'!AU22","v":-65.299999999999969},{"$f":"'Profile calcs'!AV22","v":-23.209902347589793},{"$f":"'Profile calcs'!AW22","v":-8.5611583129303863},{"$f":"'Profile calcs'!AX22","v":-2.4741704005345868},{"$f":"'Profile calcs'!AY22","v":-3.7069814327208337},{"$f":"'Profile calcs'!AZ22","v":-20.835558391915377},{"$f":"'Profile calcs'!BA22","v":-65.299999999999983},{"$f":"'Profile calcs'!BB22","v":81.925623758734872},{"$f":"'Profile calcs'!BC22","v":63.089263813477984},{"$f":"'Profile calcs'!BD22","v":53.190222536091184},null,{"$f":"'Dry Bulb'!C23","v":19},{"$f":"'Dry Bulb'!D23","v":61.519999999999996},{"$f":"'Dry Bulb'!E23","v":67.28},{"$f":"'Dry Bulb'!F23","v":74.3},{"$f":"'Dry Bulb'!G23","v":82.759999999999991},{"$f":"'Dry Bulb'!H23","v":95.72},{"$f":"'Dry Bulb'!I23","v":102.2},{"$f":"'Dry Bulb'!J23","v":103.64},{"$f":"'Dry Bulb'!K23","v":103.1},{"$f":"'Dry Bulb'!L23","v":97.34},{"$f":"'Dry Bulb'!M23","v":87.61999999999999},{"$f":"'Dry Bulb'!N23","v":75.92},{"$f":"'Dry Bulb'!O23","v":61.88},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK78","v":19},{"$f":"'Incident angle'!CL78","v":0},{"$f":"'Incident angle'!CM78","v":0},{"$f":"'Incident angle'!CN78","v":0},{"$f":"'Incident angle'!CO78","v":0},{"$f":"'Incident angle'!CP78","v":0},{"$f":"'Incident angle'!CQ78","v":0},{"$f":"'Incident angle'!CR78","v":0},{"$f":"'Incident angle'!CS78","v":0},{"$f":"'Incident angle'!CT78","v":0},{"$f":"'Incident angle'!CU78","v":0},{"$f":"'Incident angle'!CV78","v":0},{"$f":"'Incident angle'!CW78","v":0},null,{"$f":"'Incident angle'!CY78","v":19},{"$f":"'Incident angle'!CZ78","v":0},{"$f":"'Incident angle'!DA78","v":0},{"$f":"'Incident angle'!DB78","v":0},{"$f":"'Incident angle'!DC78","v":0},{"$f":"'Incident angle'!DD78","v":0},{"$f":"'Incident angle'!DE78","v":0},{"$f":"'Incident angle'!DF78","v":0},{"$f":"'Incident angle'!DG78","v":0},{"$f":"'Incident angle'!DH78","v":0},{"$f":"'Incident angle'!DI78","v":0},{"$f":"'Incident angle'!DJ78","v":0},{"$f":"'Incident angle'!DK78","v":0},null,null,19,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,19,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,20,{"$f":"'Profile calcs'!Q23","v":30.929660168946619},{"$f":"'Profile calcs'!R23","v":26.783441749367146},{"$f":"'Profile calcs'!S23","v":24.219886455298596},{"$f":"'Profile calcs'!T23","v":21.450631303008365},{"$f":"'Profile calcs'!U23","v":18.141617234558208},{"$f":"'Profile calcs'!V23","v":15.393131364902054},{"$f":"'Profile calcs'!W23","v":15.718705218374629},{"$f":"'Profile calcs'!X23","v":20.515426310682393},{"$f":"'Profile calcs'!Y23","v":27.765335603992941},{"$f":"'Profile calcs'!Z23","v":33.518173513343072},{"$f":"'Profile calcs'!AA23","v":36.431124914543311},{"$f":"'Profile calcs'!AB23","v":35.075043189143301},null,20,{"$f":"'Profile calcs'!AS23","v":74.554979301423629},{"$f":"'Profile calcs'!AT23","v":-89.391837386716418},{"$f":"'Profile calcs'!AU23","v":-65.3},{"$f":"'Profile calcs'!AV23","v":-41.466089410320599},{"$f":"'Profile calcs'!AW23","v":-27.992469719775826},{"$f":"'Profile calcs'!AX23","v":-22.437796305169524},{"$f":"'Profile calcs'!AY23","v":-25.503067121246527},{"$f":"'Profile calcs'!AZ23","v":-40.480701812612715},{"$f":"'Profile calcs'!BA23","v":-65.3},{"$f":"'Profile calcs'!BB23","v":-84.890897039079206},{"$f":"'Profile calcs'!BC23","v":80.111991515210534},{"$f":"'Profile calcs'!BD23","v":72.533349654536536},null,{"$f":"'Dry Bulb'!C24","v":20},{"$f":"'Dry Bulb'!D24","v":59.540000000000006},{"$f":"'Dry Bulb'!E24","v":64.94},{"$f":"'Dry Bulb'!F24","v":71.78},{"$f":"'Dry Bulb'!G24","v":81.14},{"$f":"'Dry Bulb'!H24","v":93.38000000000001},{"$f":"'Dry Bulb'!I24","v":99.68},{"$f":"'Dry Bulb'!J24","v":100.03999999999999},{"$f":"'Dry Bulb'!K24","v":100.22},{"$f":"'Dry Bulb'!L24","v":95},{"$f":"'Dry Bulb'!M24","v":84.56},{"$f":"'Dry Bulb'!N24","v":73.400000000000006},{"$f":"'Dry Bulb'!O24","v":60.08},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK79","v":20},{"$f":"'Incident angle'!CL79","v":0},{"$f":"'Incident angle'!CM79","v":0},{"$f":"'Incident angle'!CN79","v":0},{"$f":"'Incident angle'!CO79","v":0},{"$f":"'Incident angle'!CP79","v":0},{"$f":"'Incident angle'!CQ79","v":0},{"$f":"'Incident angle'!CR79","v":0},{"$f":"'Incident angle'!CS79","v":0},{"$f":"'Incident angle'!CT79","v":0},{"$f":"'Incident angle'!CU79","v":0},{"$f":"'Incident angle'!CV79","v":0},{"$f":"'Incident angle'!CW79","v":0},null,{"$f":"'Incident angle'!CY79","v":20},{"$f":"'Incident angle'!CZ79","v":0},{"$f":"'Incident angle'!DA79","v":0},{"$f":"'Incident angle'!DB79","v":0},{"$f":"'Incident angle'!DC79","v":0},{"$f":"'Incident angle'!DD79","v":0},{"$f":"'Incident angle'!DE79","v":0},{"$f":"'Incident angle'!DF79","v":0},{"$f":"'Incident angle'!DG79","v":0},{"$f":"'Incident angle'!DH79","v":0},{"$f":"'Incident angle'!DI79","v":0},{"$f":"'Incident angle'!DJ79","v":0},{"$f":"'Incident angle'!DK79","v":0},null,null,20,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,20,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,21,{"$f":"'Profile calcs'!Q24","v":44.196478266846057},{"$f":"'Profile calcs'!R24","v":40.599089566496509},{"$f":"'Profile calcs'!S24","v":38.635878844024383},{"$f":"'Profile calcs'!T24","v":36.520338007765019},{"$f":"'Profile calcs'!U24","v":33.567457399080453},{"$f":"'Profile calcs'!V24","v":30.792711025689055},{"$f":"'Profile calcs'!W24","v":30.936867265726114},{"$f":"'Profile calcs'!X24","v":35.533344323926315},{"$f":"'Profile calcs'!Y24","v":42.346663637257642},{"$f":"'Profile calcs'!Z24","v":47.52980172868061},{"$f":"'Profile calcs'!AA24","v":49.801160168555157},{"$f":"'Profile calcs'!AB24","v":48.138711526458181},null,21,{"$f":"'Profile calcs'!AS24","v":85.523628972409725},{"$f":"'Profile calcs'!AT24","v":-81.615896728501099},{"$f":"'Profile calcs'!AU24","v":-65.3},{"$f":"'Profile calcs'!AV24","v":-48.276082529258844},{"$f":"'Profile calcs'!AW24","v":-37.282219236973447},{"$f":"'Profile calcs'!AX24","v":-32.777260396790929},{"$f":"'Profile calcs'!AY24","v":-35.946370921243279},{"$f":"'Profile calcs'!AZ24","v":-47.731081500767182},{"$f":"'Profile calcs'!BA24","v":-65.300000000000011},{"$f":"'Profile calcs'!BB24","v":-79.771091305966891},{"$f":"'Profile calcs'!BC24","v":88.241664176975661},{"$f":"'Profile calcs'!BD24","v":82.537728896941786},null,{"$f":"'Dry Bulb'!C25","v":21},{"$f":"'Dry Bulb'!D25","v":58.28},{"$f":"'Dry Bulb'!E25","v":63.14},{"$f":"'Dry Bulb'!F25","v":70.34},{"$f":"'Dry Bulb'!G25","v":79.52},{"$f":"'Dry Bulb'!H25","v":91.4},{"$f":"'Dry Bulb'!I25","v":96.98},{"$f":"'Dry Bulb'!J25","v":97.16},{"$f":"'Dry Bulb'!K25","v":98.24},{"$f":"'Dry Bulb'!L25","v":92.48},{"$f":"'Dry Bulb'!M25","v":82.58},{"$f":"'Dry Bulb'!N25","v":71.78},{"$f":"'Dry Bulb'!O25","v":58.82},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK80","v":21},{"$f":"'Incident angle'!CL80","v":0},{"$f":"'Incident angle'!CM80","v":0},{"$f":"'Incident angle'!CN80","v":0},{"$f":"'Incident angle'!CO80","v":0},{"$f":"'Incident angle'!CP80","v":0},{"$f":"'Incident angle'!CQ80","v":0},{"$f":"'Incident angle'!CR80","v":0},{"$f":"'Incident angle'!CS80","v":0},{"$f":"'Incident angle'!CT80","v":0},{"$f":"'Incident angle'!CU80","v":0},{"$f":"'Incident angle'!CV80","v":0},{"$f":"'Incident angle'!CW80","v":0},null,{"$f":"'Incident angle'!CY80","v":21},{"$f":"'Incident angle'!CZ80","v":0},{"$f":"'Incident angle'!DA80","v":0},{"$f":"'Incident angle'!DB80","v":0},{"$f":"'Incident angle'!DC80","v":0},{"$f":"'Incident angle'!DD80","v":0},{"$f":"'Incident angle'!DE80","v":0},{"$f":"'Incident angle'!DF80","v":0},{"$f":"'Incident angle'!DG80","v":0},{"$f":"'Incident angle'!DH80","v":0},{"$f":"'Incident angle'!DI80","v":0},{"$f":"'Incident angle'!DJ80","v":0},{"$f":"'Incident angle'!DK80","v":0},null,null,21,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,21,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,22,{"$f":"'Profile calcs'!Q25","v":57.739752741902734},{"$f":"'Profile calcs'!R25","v":54.856879804295147},{"$f":"'Profile calcs'!S25","v":53.761437623792695},{"$f":"'Profile calcs'!T25","v":52.718628788708926},{"$f":"'Profile calcs'!U25","v":50.521398141456501},{"$f":"'Profile calcs'!V25","v":47.871905572894399},{"$f":"'Profile calcs'!W25","v":47.648515276704565},{"$f":"'Profile calcs'!X25","v":51.678377748209421},{"$f":"'Profile calcs'!Y25","v":57.660184602658042},{"$f":"'Profile calcs'!Z25","v":62.016242169118094},{"$f":"'Profile calcs'!AA25","v":63.476783571899695},{"$f":"'Profile calcs'!AB25","v":61.443103356413083},null,22,{"$f":"'Profile calcs'!AS25","v":-89.034466475858252},{"$f":"'Profile calcs'!AT25","v":-78.208550588834868},{"$f":"'Profile calcs'!AU25","v":-65.300000000000011},{"$f":"'Profile calcs'!AV25","v":-51.41616481533466},{"$f":"'Profile calcs'!AW25","v":-41.966447814390222},{"$f":"'Profile calcs'!AX25","v":-38.17645504718876},{"$f":"'Profile calcs'!AY25","v":-41.191262191845297},{"$f":"'Profile calcs'!AZ25","v":-51.055744533640386},{"$f":"'Profile calcs'!BA25","v":-65.3},{"$f":"'Profile calcs'!BB25","v":-77.37193628402801},{"$f":"'Profile calcs'!BC25","v":-87.655590304611039},{"$f":"'Profile calcs'!BD25","v":87.764397938009637},null,{"$f":"'Dry Bulb'!C26","v":22},{"$f":"'Dry Bulb'!D26","v":56.84},{"$f":"'Dry Bulb'!E26","v":61.34},{"$f":"'Dry Bulb'!F26","v":68.72},{"$f":"'Dry Bulb'!G26","v":77.900000000000006},{"$f":"'Dry Bulb'!H26","v":89.6},{"$f":"'Dry Bulb'!I26","v":94.64},{"$f":"'Dry Bulb'!J26","v":94.460000000000008},{"$f":"'Dry Bulb'!K26","v":96.26},{"$f":"'Dry Bulb'!L26","v":90.68},{"$f":"'Dry Bulb'!M26","v":80.599999999999994},{"$f":"'Dry Bulb'!N26","v":69.8},{"$f":"'Dry Bulb'!O26","v":57.56},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK81","v":22},{"$f":"'Incident angle'!CL81","v":0},{"$f":"'Incident angle'!CM81","v":0},{"$f":"'Incident angle'!CN81","v":0},{"$f":"'Incident angle'!CO81","v":0},{"$f":"'Incident angle'!CP81","v":0},{"$f":"'Incident angle'!CQ81","v":0},{"$f":"'Incident angle'!CR81","v":0},{"$f":"'Incident angle'!CS81","v":0},{"$f":"'Incident angle'!CT81","v":0},{"$f":"'Incident angle'!CU81","v":0},{"$f":"'Incident angle'!CV81","v":0},{"$f":"'Incident angle'!CW81","v":0},null,{"$f":"'Incident angle'!CY81","v":22},{"$f":"'Incident angle'!CZ81","v":0},{"$f":"'Incident angle'!DA81","v":0},{"$f":"'Incident angle'!DB81","v":0},{"$f":"'Incident angle'!DC81","v":0},{"$f":"'Incident angle'!DD81","v":0},{"$f":"'Incident angle'!DE81","v":0},{"$f":"'Incident angle'!DF81","v":0},{"$f":"'Incident angle'!DG81","v":0},{"$f":"'Incident angle'!DH81","v":0},{"$f":"'Incident angle'!DI81","v":0},{"$f":"'Incident angle'!DJ81","v":0},{"$f":"'Incident angle'!DK81","v":0},null,null,22,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,22,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,23,{"$f":"'Profile calcs'!Q26","v":71.593874807745053},{"$f":"'Profile calcs'!R26","v":69.589194473644923},{"$f":"'Profile calcs'!S26","v":69.61109114186894},{"$f":"'Profile calcs'!T26","v":70.053891850109665},{"$f":"'Profile calcs'!U26","v":69.071591312252522},{"$f":"'Profile calcs'!V26","v":66.787471568061861},{"$f":"'Profile calcs'!W26","v":65.990399025379261},{"$f":"'Profile calcs'!X26","v":68.97846377500592},{"$f":"'Profile calcs'!Y26","v":73.666960034724326},{"$f":"'Profile calcs'!Z26","v":76.934368103437876},{"$f":"'Profile calcs'!AA26","v":77.442055417846433},{"$f":"'Profile calcs'!AB26","v":75.002834283541929},null,23,{"$f":"'Profile calcs'!AS26","v":-86.317782095871323},{"$f":"'Profile calcs'!AT26","v":-76.581548940884886},{"$f":"'Profile calcs'!AU26","v":-65.300000000000011},{"$f":"'Profile calcs'!AV26","v":-52.903879372827781},{"$f":"'Profile calcs'!AW26","v":-44.256353256343338},{"$f":"'Profile calcs'!AX26","v":-40.885787908689707},{"$f":"'Profile calcs'!AY26","v":-43.801669031237026},{"$f":"'Profile calcs'!AZ26","v":-52.639173727034112},{"$f":"'Profile calcs'!BA26","v":-65.300000000000011},{"$f":"'Profile calcs'!BB26","v":-76.271835790335643},{"$f":"'Profile calcs'!BC26","v":-85.706352154202364},{"$f":"'Profile calcs'!BD26","v":-89.629320243390126},null,{"$f":"'Dry Bulb'!C27","v":23},{"$f":"'Dry Bulb'!D27","v":55.58},{"$f":"'Dry Bulb'!E27","v":59.9},{"$f":"'Dry Bulb'!F27","v":67.28},{"$f":"'Dry Bulb'!G27","v":75.740000000000009},{"$f":"'Dry Bulb'!H27","v":87.8},{"$f":"'Dry Bulb'!I27","v":92.84},{"$f":"'Dry Bulb'!J27","v":93.02},{"$f":"'Dry Bulb'!K27","v":94.64},{"$f":"'Dry Bulb'!L27","v":88.88000000000001},{"$f":"'Dry Bulb'!M27","v":78.98},{"$f":"'Dry Bulb'!N27","v":67.819999999999993},{"$f":"'Dry Bulb'!O27","v":56.66},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK82","v":23},{"$f":"'Incident angle'!CL82","v":0},{"$f":"'Incident angle'!CM82","v":0},{"$f":"'Incident angle'!CN82","v":0},{"$f":"'Incident angle'!CO82","v":0},{"$f":"'Incident angle'!CP82","v":0},{"$f":"'Incident angle'!CQ82","v":0},{"$f":"'Incident angle'!CR82","v":0},{"$f":"'Incident angle'!CS82","v":0},{"$f":"'Incident angle'!CT82","v":0},{"$f":"'Incident angle'!CU82","v":0},{"$f":"'Incident angle'!CV82","v":0},{"$f":"'Incident angle'!CW82","v":0},null,{"$f":"'Incident angle'!CY82","v":23},{"$f":"'Incident angle'!CZ82","v":0},{"$f":"'Incident angle'!DA82","v":0},{"$f":"'Incident angle'!DB82","v":0},{"$f":"'Incident angle'!DC82","v":0},{"$f":"'Incident angle'!DD82","v":0},{"$f":"'Incident angle'!DE82","v":0},{"$f":"'Incident angle'!DF82","v":0},{"$f":"'Incident angle'!DG82","v":0},{"$f":"'Incident angle'!DH82","v":0},{"$f":"'Incident angle'!DI82","v":0},{"$f":"'Incident angle'!DJ82","v":0},{"$f":"'Incident angle'!DK82","v":0},null,null,23,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,23,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,24,{"$f":"'Profile calcs'!Q27","v":85.676140318453747},{"$f":"'Profile calcs'!R27","v":84.673020487038187},{"$f":"'Profile calcs'!S27","v":85.974408266739928},{"$f":"'Profile calcs'!T27","v":88.161715299139843},{"$f":"'Profile calcs'!U27","v":88.728943923930075},{"$f":"'Profile calcs'!V27","v":87.067266457680972},{"$f":"'Profile calcs'!W27","v":85.571264313099348},{"$f":"'Profile calcs'!X27","v":87.09022999649082},{"$f":"'Profile calcs'!Y27","v":89.899102008781256},{"$f":"'Profile calcs'!Z27","v":87.907230778803338},{"$f":"'Profile calcs'!AA27","v":88.427383905065867},{"$f":"'Profile calcs'!AB27","v":88.730639842766692},null,24,{"$f":"'Profile calcs'!AS27","v":-85.258807477738344},{"$f":"'Profile calcs'!AT27","v":-75.943775995922138},{"$f":"'Profile calcs'!AU27","v":-65.3},{"$f":"'Profile calcs'!AV27","v":-53.395992963055065},{"$f":"'Profile calcs'!AW27","v":-44.997391900129685},{"$f":"'Profile calcs'!AX27","v":-41.835493673926223},{"$f":"'Profile calcs'!AY27","v":-44.768155065254646},{"$f":"'Profile calcs'!AZ27","v":-53.189833160566664},{"$f":"'Profile calcs'!BA27","v":-65.3},{"$f":"'Profile calcs'!BB27","v":-76.006803466110895},{"$f":"'Profile calcs'!BC27","v":-85.207760704177844},{"$f":"'Profile calcs'!BD27","v":-88.756097838181603},null,{"$f":"'Dry Bulb'!C28","v":24},{"$f":"'Dry Bulb'!D28","v":54.68},{"$f":"'Dry Bulb'!E28","v":58.28},{"$f":"'Dry Bulb'!F28","v":65.84},{"$f":"'Dry Bulb'!G28","v":74.3},{"$f":"'Dry Bulb'!H28","v":86.18},{"$f":"'Dry Bulb'!I28","v":91.039999999999992},{"$f":"'Dry Bulb'!J28","v":91.76},{"$f":"'Dry Bulb'!K28","v":92.84},{"$f":"'Dry Bulb'!L28","v":87.26},{"$f":"'Dry Bulb'!M28","v":77.540000000000006},{"$f":"'Dry Bulb'!N28","v":66.56},{"$f":"'Dry Bulb'!O28","v":55.04},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"'Incident angle'!CK83","v":24},{"$f":"'Incident angle'!CL83","v":0},{"$f":"'Incident angle'!CM83","v":0},{"$f":"'Incident angle'!CN83","v":0},{"$f":"'Incident angle'!CO83","v":0},{"$f":"'Incident angle'!CP83","v":0},{"$f":"'Incident angle'!CQ83","v":0},{"$f":"'Incident angle'!CR83","v":0},{"$f":"'Incident angle'!CS83","v":0},{"$f":"'Incident angle'!CT83","v":0},{"$f":"'Incident angle'!CU83","v":0},{"$f":"'Incident angle'!CV83","v":0},{"$f":"'Incident angle'!CW83","v":0},null,{"$f":"'Incident angle'!CY83","v":24},{"$f":"'Incident angle'!CZ83","v":0},{"$f":"'Incident angle'!DA83","v":0},{"$f":"'Incident angle'!DB83","v":0},{"$f":"'Incident angle'!DC83","v":0},{"$f":"'Incident angle'!DD83","v":0},{"$f":"'Incident angle'!DE83","v":0},{"$f":"'Incident angle'!DF83","v":0},{"$f":"'Incident angle'!DG83","v":0},{"$f":"'Incident angle'!DH83","v":0},{"$f":"'Incident angle'!DI83","v":0},{"$f":"'Incident angle'!DJ83","v":0},{"$f":"'Incident angle'!DK83","v":0},null,null,24,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,null,24,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000,1000]
[null,null,null,null,null,null,null,null,{"$f":"CP58","v":"Heat Cutoff"},null,null,{"$f":"IF(CS58=1000,\"-\",CS58)","v":"-"},{"$f":"CT58","v":"-"},{"$f":"IF(CU58=1010,\"-\",CU58)","v":"-"},null,null,null,null,null,null,null,null,{"$f":"DD58","v":"Heat Cutoff"},null,null,{"$f":"IF(DG58=1000,\"-\",DG58)","v":"-"},{"$f":"DH58","v":"-"},{"$f":"IF(DI58=1010,\"-\",DI58)","v":"-"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heat Cutoff",null,null,{"$f":"MIN(CJ42:CU50)","v":1000},"-",{"$f":"CS58+10","v":1010},null,null,null,null,null,null,null,null,"Heat Cutoff",null,null,{"$f":"MIN(CX42:DI50)","v":1000},"-",{"$f":"DG58+10","v":1010}]

{"sheet":"Solar Altitude","index":10,"n_rows":80,"n_cols":16,"rows_kept":80,"cut":false,"hidden":true,"merged":[[1,1,1,13],[2,15,2,16]]}
[]
[null,"Solar Altitude"]
[null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Home"]
[null,1,{"$f":"DEGREES(C31)","v":-79.238745258454912},-73.135890206899091,-62.969753990761212,-51.103815741194268,-42.972420763986918,-40.259838967181594,-43.397326661656273,-51.194813940312706,-61.30334441705341,-68.588756925018274,-73.864057818332,-77.510392918823513]
[null,2,{"$f":"DEGREES(C32)","v":-66.037221876299029},-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697]
[null,3,{"$f":"DEGREES(C33)","v":-52.431373562484438},-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552]
[null,4,{"$f":"DEGREES(C34)","v":-38.837571781392398},-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833]
[null,5,{"$f":"DEGREES(C35)","v":-25.376333918471747},-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006]
[null,6,{"$f":"DEGREES(C36)","v":-12.151444093159176},-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719]
[null,7,{"$f":"DEGREES(C37)","v":0.70023973357815916},4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048]
[null,8,{"$f":"DEGREES(C38)","v":12.968359542715392},17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182]
[null,9,{"$f":"DEGREES(C39)","v":24.306538235547787},29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159]
[null,10,{"$f":"DEGREES(C40)","v":34.130498638110296},40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,37.566870997040184,33.04159126014769]
[null,11,{"$f":"DEGREES(C41)","v":41.499338482119107},49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983]
[null,12,{"$f":"DEGREES(C42)","v":45.177523796213436},54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598]
[null,13,{"$f":"DEGREES(C43)","v":44.262516808487675},53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703]
[null,14,{"$f":"DEGREES(C44)","v":39.001643714284292},47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348]
[null,15,{"$f":"DEGREES(C45)","v":30.541133571003865},37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655]
[null,16,{"$f":"DEGREES(C46)","v":20.038281727598083},26.016647471873153,30.233879108991232,33.419767540103443,35.682648220686666,37.56104623172925,37.876258416390314,34.288646107643089,26.935985833021654,19.913519068774189,15.259931573481456,15.530455637101428]
[null,17,{"$f":"DEGREES(C47)","v":8.2848854255444504},13.434807821200849,16.897092448538277,19.80224832363653,22.286756355186323,24.319689951925163,24.456964963286701,20.670382142796534,13.51706337533537,7.0202572324504446,3.1397975005302774,3.9451572875932328]
[null,18,{"$f":"DEGREES(C48)","v":-4.242067037456934},0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772]
[null,19,{"$f":"DEGREES(C49)","v":-17.258784755357599},-13.177535073458104,-10.292097151668569,-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176]
[null,20,{"$f":"DEGREES(C50)","v":-30.589239677830651},-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,-12.902247652391463,-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299]
[null,21,{"$f":"DEGREES(C51)","v":-44.11375465474292},-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762]
[null,22,{"$f":"DEGREES(C52)","v":-57.730536859646747},-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132]
[null,23,{"$f":"DEGREES(C53)","v":-71.276413671366612},-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272]
[null,24,{"$f":"DEGREES(C54)","v":-83.596484892158756},-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205]
[]
[]
[null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-1.3829769999090833},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-1.276462085487466},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-1.0990295363096221},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.89192984501634631},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-0.75001022988394883},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-0.70266674630003212},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.75742623680942112},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.89351806320434846},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-1.0699452025616658},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-1.1970996381916303},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-1.2891710078133529},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N57))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-1.3528115609479683}]
[null,2,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-1.1525669506114455},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-1.0927552195260721},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-0.95130224174119837},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.76862796524706711},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-0.6434663107876345},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-0.60715275194899754},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.66126831286868248},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.77473051097986467},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-0.90441455663278347},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-0.98649107820622306},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-1.0538002854786417},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N58))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-1.1150848114086622}]
[null,3,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-0.91510010000846231},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-0.8687614571474529},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-0.7506215022246272},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.59290052257262627},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-0.48649598385176701},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-0.46072165289022143},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.51135462026635869},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.60179753227985044},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-0.69630041388172326},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-0.75549879360478533},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-0.8160740162821476},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N59))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-0.87837057368360594}]
[null,4,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-0.67784350106493674},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-0.63399324132765555},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-0.52768073610182686},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.38810697387644222},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-0.29772837267694147},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-0.28069873862030092},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.32707862834565449},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.39865259275202325},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-0.47012164005677498},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-0.51872047422282141},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-0.57957125673147558},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N60))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-0.64391344424370645}]
[null,5,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-0.44290057896284629},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-0.39637100322553681},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-0.29490989724086319},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.16722120526491902},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-8.9415420739598656E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-7.9331467629529334E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.12162905113956689},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.17875631873742479},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-0.2359172611003402},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-0.28107454525900838},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-0.34610801392072221},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N61))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-0.41302397084180853}]
[null,6,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-0.2120827082976442},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-0.15938186256517536},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-5.800132106738768E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":6.2807098534149008E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":0.13109689380022602},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":0.13567944881746447},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":9.7012475288005454E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":5.0673406087127268E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":1.4535086314809659E-3},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-4.5406311904995174E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-0.11765879291730227},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N62))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-0.18750763750189808}]
[null,7,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":1.2221488904226771E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":7.430305141584842E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":0.17963098223174623},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":0.29795849626606924},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":0.35939817880112246},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":0.35958921535624772},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":0.32406447942957417},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":0.28548906895463944},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":0.23880622575657798},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.18547443025614593},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.10295274018781533},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N63))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":2.9934942158898217E-2}]
[null,8,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.22634057260280982},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.30142366730785897},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":0.41493012914779842},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":0.53546211775009678},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":0.59271057382918846},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":0.58940632339799615},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":0.5565461241032712},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":0.52288150124922672},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":0.47294757923343267},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.40755061888761374},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.31123317645427745},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N64))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":0.23505828476134222}]
[null,9,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.42422912197220192},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.51674760289810373},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":0.64364249562081655},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":0.77261186156276163},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":0.82909885409084327},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":0.82315762857506991},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":0.79243404694781294},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":0.76020233901674328},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":0.69898266904810691},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.61384167580137594},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.4996660033936518},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N65))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":0.42099061586387221}]
[null,10,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.59568957658246524},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.7106448294994947},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":0.85749143945465145},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":1.0048496171469099},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":1.0668149737566022},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":1.0594461294056157},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":1.0300385319542611},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":0.99318248503682061},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":0.90676948471422592},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.79109114939235459},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.6556655885703162},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N66))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":0.57668455758775938}]
[null,11,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.72430009391256434},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.86469469158448298},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":1.0367606486133867},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":1.2182717550624984},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":1.3024671395224319},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":1.2970838092737071},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":1.2667111520037753},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":1.2092319290546618},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":1.0715143714004549},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.91486576224237537},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.76010751502055596},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N67))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":0.6858622341895062}]
[null,12,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.78849653814201215},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.94822112425698535},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":1.1352908079305437},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":1.3460080763218141},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":1.4924636644182712},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":1.5304042889212992},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":1.4799329560972334},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":1.3473895774711653},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":1.1396972190412304},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.95194807897330325},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.79186492002119568},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N68))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":0.73009423713113575}]
[null,13,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.77252665352744232},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.93275019559434558},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":1.0990295363096223},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":1.2552173613067725},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":1.3318682516853357},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":1.3646857038578266},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":1.3691285375911051},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":1.267866732398256},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":1.0699452025616651},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.88800776264255266},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.74250843649886467},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N69))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":0.69939650433353429}]
[null,14,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.68070709650401151},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.82443366078985414},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":0.95130224174119793},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":1.0501170582210952},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":1.0971656509407299},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":1.1269592866596254},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":1.1356267863135077},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":1.0648348746726859},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":0.90441455663278292},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.74630101310525476},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.6246840945530594},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N70))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":0.60088037152088025}]
[null,15,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.53304333810539084},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.65580226330574698},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":0.75062150222462676},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":0.81993388123391775},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":0.85944028896063562},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":0.89016229919797163},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":0.89793128941894174},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":0.83502086960833699},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":0.6963004138817227},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.55917131738673131},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.46005233280892727},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N71))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":0.45239449944597204}]
[null,16,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.34973399258880405},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.45407615871484536},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":0.52768073610182653},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":0.58328497882593111},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":0.62277969728187854},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":0.65556392723748436},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":0.66106541770222438},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":0.59844977062950988},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":0.47012164005677542},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.34755647340878471},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":0.26633604958629042},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N72))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":0.27105758520233353}]
[null,17,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":0.14459852882624219},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":0.23448163085264045},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":0.29490989724086347},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":0.34561443254498508},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":0.38897727798777215},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":0.42445866272527555},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":0.42685456365424701},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":0.36076622603724018},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":0.23591726110034028},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":0.12252660304320516},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":5.4799804230141747E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N73))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":6.8855984177550747E-2}]
[null,18,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-7.4038036893945114E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":4.9735293749047088E-3},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":5.8001321067386986E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":0.10978647644286511},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":0.15990484727947582},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":0.19861904459146784},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":0.19709345829432334},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":0.12485782719224001},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-1.4535086314814598E-3},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-0.10999891223916966},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-0.16786658319360157},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N74))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-0.14669401534843554}]
[null,19,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-0.30122261887399415},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-0.22999137432887676},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-0.17963098223174673},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.12153637328460365},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-6.1804294785339775E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-1.93116916778233E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-2.5744676032291504E-2},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.10664339169467521},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-0.2388062257565787},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-0.34647115439030096},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-0.39763373443840683},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N75))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-0.37095939086690655}]
[null,20,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-0.53388294805983438},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-0.46745346916078678},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-0.41493012914779914},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.34469183137428505},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-0.27200715048002461},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-0.22518670244193986},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.23781167329945158},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.33015884947429597},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-0.47294757923343284},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-0.58419694373935427},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-0.63192561275089076},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N76))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-0.60101382391890912}]
[null,21,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-0.76993026414223831},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-0.70467916877551551},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-0.64364249562081677},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.55350964984477613},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-0.46383024092286895},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-0.41229942422023036},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.43276675779691687},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.53970471720132418},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-0.69898266904810691},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-0.82005005521358165},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-0.86886910225272374},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N77))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-0.83492181495523676}]
[null,22,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-1.0075879471447833},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-0.93745939066125372},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-0.85749143945465189},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.73656791651873665},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-0.62576918223644717},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-0.56984947622192639},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.59999525632832273},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.72426157096834487},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-0.90676948471422592},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-1.0477245448174388},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-1.1065376925540364},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N78))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-1.0713063091469059}]
[null,23,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-1.244008097578847},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-1.1545957931911086},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-1.0367606486133867},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.87286335886199762},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-0.73997471354284627},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-0.68180401333155372},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.72273847999390251},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.86355808781657872},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-1.0715143714004554},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-1.2457898345442597},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-1.339919767470781},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N79))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-1.3089735287568234}]
[null,24,{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!C$5)*COS(C80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!C$5)))","v":-1.459033904461867},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!D$5)*COS(D80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!D$5)))","v":-1.3097245943515294},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!E$5)*COS(E80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!E$5)))","v":-1.1352908079305437},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!F$5)*COS(F80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!F$5)))","v":-0.93148937217865124},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!G$5)*COS(G80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!G$5)))","v":-0.785229622050997},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!H$5)*COS(H80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!H$5)))","v":-0.72964504868703162},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!I$5)*COS(I80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!I$5)))","v":-0.77988055070018159},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!J$5)*COS(J80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!J$5)))","v":-0.92723345897637688},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!K$5)*COS(K80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!K$5)))","v":-1.1396972190412304},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!L$5)*COS(L80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!L$5)))","v":-1.3240614330874585},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!M$5)*COS(M80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!M$5)))","v":-1.4828073277245226},{"$f":"ASIN((COS('Input Data'!$G$3)*COS('eq of time'!N$5)*COS(N80))+(SIN('Input Data'!$G$3)*SIN('eq of time'!N$5)))","v":-1.5397826771882956}]
[]
[null,"H","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"RADIANS(15*(12-AST!B2))","v":2.9597875231737172},{"$f":"RADIANS(15*(12-AST!C2))","v":2.9715684956246786},{"$f":"RADIANS(15*(12-AST!D2))","v":2.9436432275927698},{"$f":"RADIANS(15*(12-AST!E2))","v":2.9061186486748913},{"$f":"RADIANS(15*(12-AST!F2))","v":2.8965193377889222},{"$f":"RADIANS(15*(12-AST!G2))","v":2.9170269564998561},{"$f":"RADIANS(15*(12-AST!H2))","v":2.9379709075237876},{"$f":"RADIANS(15*(12-AST!I2))","v":2.9213902796298417},{"$f":"RADIANS(15*(12-AST!J2))","v":2.8781933806429829},{"$f":"RADIANS(15*(12-AST!K2))","v":2.8437231279160944},{"$f":"RADIANS(15*(12-AST!L2))","v":2.8507044449240717},{"$f":"RADIANS(15*(12-AST!M2))","v":2.9039369871098986}]
[null,2,{"$f":"RADIANS(15*(12-AST!B3))","v":2.6979881353745681},{"$f":"RADIANS(15*(12-AST!C3))","v":2.7097691078255295},{"$f":"RADIANS(15*(12-AST!D3))","v":2.6818438397936206},{"$f":"RADIANS(15*(12-AST!E3))","v":2.6443192608757422},{"$f":"RADIANS(15*(12-AST!F3))","v":2.6347199499897731},{"$f":"RADIANS(15*(12-AST!G3))","v":2.655227568700707},{"$f":"RADIANS(15*(12-AST!H3))","v":2.6761715197246385},{"$f":"RADIANS(15*(12-AST!I3))","v":2.6595908918306925},{"$f":"RADIANS(15*(12-AST!J3))","v":2.6163939928438333},{"$f":"RADIANS(15*(12-AST!K3))","v":2.5819237401169448},{"$f":"RADIANS(15*(12-AST!L3))","v":2.5889050571249221},{"$f":"RADIANS(15*(12-AST!M3))","v":2.642137599310749}]
[null,3,{"$f":"RADIANS(15*(12-AST!B4))","v":2.4361887475754185},{"$f":"RADIANS(15*(12-AST!C4))","v":2.4479697200263799},{"$f":"RADIANS(15*(12-AST!D4))","v":2.420044451994471},{"$f":"RADIANS(15*(12-AST!E4))","v":2.3825198730765926},{"$f":"RADIANS(15*(12-AST!F4))","v":2.3729205621906235},{"$f":"RADIANS(15*(12-AST!G4))","v":2.3934281809015574},{"$f":"RADIANS(15*(12-AST!H4))","v":2.4143721319254889},{"$f":"RADIANS(15*(12-AST!I4))","v":2.397791504031543},{"$f":"RADIANS(15*(12-AST!J4))","v":2.3545946050446838},{"$f":"RADIANS(15*(12-AST!K4))","v":2.3201243523177957},{"$f":"RADIANS(15*(12-AST!L4))","v":2.327105669325773},{"$f":"RADIANS(15*(12-AST!M4))","v":2.3803382115115999}]
[null,4,{"$f":"RADIANS(15*(12-AST!B5))","v":2.1743893597762689},{"$f":"RADIANS(15*(12-AST!C5))","v":2.1861703322272303},{"$f":"RADIANS(15*(12-AST!D5))","v":2.1582450641953215},{"$f":"RADIANS(15*(12-AST!E5))","v":2.1207204852774431},{"$f":"RADIANS(15*(12-AST!F5))","v":2.1111211743914744},{"$f":"RADIANS(15*(12-AST!G5))","v":2.1316287931024083},{"$f":"RADIANS(15*(12-AST!H5))","v":2.1525727441263394},{"$f":"RADIANS(15*(12-AST!I5))","v":2.1359921162323934},{"$f":"RADIANS(15*(12-AST!J5))","v":2.0927952172455337},{"$f":"RADIANS(15*(12-AST!K5))","v":2.0583249645186461},{"$f":"RADIANS(15*(12-AST!L5))","v":2.0653062815266234},{"$f":"RADIANS(15*(12-AST!M5))","v":2.1185388237124503}]
[null,5,{"$f":"RADIANS(15*(12-AST!B6))","v":1.9125899719771193},{"$f":"RADIANS(15*(12-AST!C6))","v":1.924370944428081},{"$f":"RADIANS(15*(12-AST!D6))","v":1.8964456763961719},{"$f":"RADIANS(15*(12-AST!E6))","v":1.8589210974782937},{"$f":"RADIANS(15*(12-AST!F6))","v":1.8493217865923248},{"$f":"RADIANS(15*(12-AST!G6))","v":1.8698294053032583},{"$f":"RADIANS(15*(12-AST!H6))","v":1.8907733563271902},{"$f":"RADIANS(15*(12-AST!I6))","v":1.874192728433244},{"$f":"RADIANS(15*(12-AST!J6))","v":1.8309958294463846},{"$f":"RADIANS(15*(12-AST!K6))","v":1.7965255767194965},{"$f":"RADIANS(15*(12-AST!L6))","v":1.8035068937274739},{"$f":"RADIANS(15*(12-AST!M6))","v":1.8567394359133007}]
[null,6,{"$f":"RADIANS(15*(12-AST!B7))","v":1.65079058417797},{"$f":"RADIANS(15*(12-AST!C7))","v":1.6625715566289316},{"$f":"RADIANS(15*(12-AST!D7))","v":1.6346462885970225},{"$f":"RADIANS(15*(12-AST!E7))","v":1.5971217096791444},{"$f":"RADIANS(15*(12-AST!F7))","v":1.5875223987931755},{"$f":"RADIANS(15*(12-AST!G7))","v":1.6080300175041089},{"$f":"RADIANS(15*(12-AST!H7))","v":1.6289739685280409},{"$f":"RADIANS(15*(12-AST!I7))","v":1.6123933406340947},{"$f":"RADIANS(15*(12-AST!J7))","v":1.569196441647235},{"$f":"RADIANS(15*(12-AST!K7))","v":1.5347261889203472},{"$f":"RADIANS(15*(12-AST!L7))","v":1.5417075059283243},{"$f":"RADIANS(15*(12-AST!M7))","v":1.5949400481141514}]
[null,7,{"$f":"RADIANS(15*(12-AST!B8))","v":1.3889911963788206},{"$f":"RADIANS(15*(12-AST!C8))","v":1.4007721688297823},{"$f":"RADIANS(15*(12-AST!D8))","v":1.372846900797873},{"$f":"RADIANS(15*(12-AST!E8))","v":1.3353223218799948},{"$f":"RADIANS(15*(12-AST!F8))","v":1.3257230109940261},{"$f":"RADIANS(15*(12-AST!G8))","v":1.3462306297049593},{"$f":"RADIANS(15*(12-AST!H8))","v":1.3671745807288913},{"$f":"RADIANS(15*(12-AST!I8))","v":1.3505939528349453},{"$f":"RADIANS(15*(12-AST!J8))","v":1.3073970538480857},{"$f":"RADIANS(15*(12-AST!K8))","v":1.2729268011211978},{"$f":"RADIANS(15*(12-AST!L8))","v":1.2799081181291749},{"$f":"RADIANS(15*(12-AST!M8))","v":1.333140660315002}]
[null,8,{"$f":"RADIANS(15*(12-AST!B9))","v":1.1271918085796711},{"$f":"RADIANS(15*(12-AST!C9))","v":1.1389727810306327},{"$f":"RADIANS(15*(12-AST!D9))","v":1.1110475129987236},{"$f":"RADIANS(15*(12-AST!E9))","v":1.0735229340808454},{"$f":"RADIANS(15*(12-AST!F9))","v":1.0639236231948765},{"$f":"RADIANS(15*(12-AST!G9))","v":1.0844312419058098},{"$f":"RADIANS(15*(12-AST!H9))","v":1.1053751929297422},{"$f":"RADIANS(15*(12-AST!I9))","v":1.0887945650357957},{"$f":"RADIANS(15*(12-AST!J9))","v":1.0455976660489359},{"$f":"RADIANS(15*(12-AST!K9))","v":1.0111274133220483},{"$f":"RADIANS(15*(12-AST!L9))","v":1.0181087303300258},{"$f":"RADIANS(15*(12-AST!M9))","v":1.0713412725158524}]
[null,9,{"$f":"RADIANS(15*(12-AST!B10))","v":0.8653924207805217},{"$f":"RADIANS(15*(12-AST!C10))","v":0.87717339323148336},{"$f":"RADIANS(15*(12-AST!D10))","v":0.84924812519957393},{"$f":"RADIANS(15*(12-AST!E10))","v":0.81172354628169596},{"$f":"RADIANS(15*(12-AST!F10))","v":0.80212423539572753},{"$f":"RADIANS(15*(12-AST!G10))","v":0.8226318541066604},{"$f":"RADIANS(15*(12-AST!H10))","v":0.84357580513059294},{"$f":"RADIANS(15*(12-AST!I10))","v":0.82699517723664651},{"$f":"RADIANS(15*(12-AST!J10))","v":0.78379827824978654},{"$f":"RADIANS(15*(12-AST!K10))","v":0.74932802552289879},{"$f":"RADIANS(15*(12-AST!L10))","v":0.75630934253087634},{"$f":"RADIANS(15*(12-AST!M10))","v":0.8095418847167033}]
[null,10,{"$f":"RADIANS(15*(12-AST!B11))","v":0.60359303298137224},{"$f":"RADIANS(15*(12-AST!C11))","v":0.61537400543233389},{"$f":"RADIANS(15*(12-AST!D11))","v":0.58744873740042447},{"$f":"RADIANS(15*(12-AST!E11))","v":0.54992415848254661},{"$f":"RADIANS(15*(12-AST!F11))","v":0.54032484759657817},{"$f":"RADIANS(15*(12-AST!G11))","v":0.56083246630751094},{"$f":"RADIANS(15*(12-AST!H11))","v":0.58177641733144347},{"$f":"RADIANS(15*(12-AST!I11))","v":0.56519578943749704},{"$f":"RADIANS(15*(12-AST!J11))","v":0.52199889045063708},{"$f":"RADIANS(15*(12-AST!K11))","v":0.48752863772374933},{"$f":"RADIANS(15*(12-AST!L11))","v":0.49450995473172682},{"$f":"RADIANS(15*(12-AST!M11))","v":0.54774249691755383}]
[null,11,{"$f":"RADIANS(15*(12-AST!B12))","v":0.34179364518222277},{"$f":"RADIANS(15*(12-AST!C12))","v":0.35357461763318454},{"$f":"RADIANS(15*(12-AST!D12))","v":0.32564934960127506},{"$f":"RADIANS(15*(12-AST!E12))","v":0.28812477068339715},{"$f":"RADIANS(15*(12-AST!F12))","v":0.27852545979742871},{"$f":"RADIANS(15*(12-AST!G12))","v":0.29903307850836153},{"$f":"RADIANS(15*(12-AST!H12))","v":0.31997702953229407},{"$f":"RADIANS(15*(12-AST!I12))","v":0.30339640163834763},{"$f":"RADIANS(15*(12-AST!J12))","v":0.26019950265148772},{"$f":"RADIANS(15*(12-AST!K12))","v":0.22572924992459989},{"$f":"RADIANS(15*(12-AST!L12))","v":0.23271056693257738},{"$f":"RADIANS(15*(12-AST!M12))","v":0.28594310911840437}]
[null,12,{"$f":"RADIANS(15*(12-AST!B13))","v":7.9994257383073392E-2},{"$f":"RADIANS(15*(12-AST!C13))","v":9.1775229834035091E-2},{"$f":"RADIANS(15*(12-AST!D13))","v":6.384996180212564E-2},{"$f":"RADIANS(15*(12-AST!E13))","v":2.6325382884247735E-2},{"$f":"RADIANS(15*(12-AST!F13))","v":1.6726071998279281E-2},{"$f":"RADIANS(15*(12-AST!G13))","v":3.723369070921214E-2},{"$f":"RADIANS(15*(12-AST!H13))","v":5.8177641733144575E-2},{"$f":"RADIANS(15*(12-AST!I13))","v":4.1597013839198178E-2},{"$f":"RADIANS(15*(12-AST!J13))","v":-1.5998851476617189E-3},{"$f":"RADIANS(15*(12-AST!K13))","v":-3.6070137874549532E-2},{"$f":"RADIANS(15*(12-AST!L13))","v":-2.9088820866572055E-2},{"$f":"RADIANS(15*(12-AST!M13))","v":2.4143721319254945E-2}]
[null,13,{"$f":"RADIANS(15*(12-AST!B14))","v":-0.18180513041607604},{"$f":"RADIANS(15*(12-AST!C14))","v":-0.17002415796511433},{"$f":"RADIANS(15*(12-AST!D14))","v":-0.19794942599702378},{"$f":"RADIANS(15*(12-AST!E14))","v":-0.2354740049149017},{"$f":"RADIANS(15*(12-AST!F14))","v":-0.24507331580087016},{"$f":"RADIANS(15*(12-AST!G14))","v":-0.22456569708993729},{"$f":"RADIANS(15*(12-AST!H14))","v":-0.20362174606600486},{"$f":"RADIANS(15*(12-AST!I14))","v":-0.22020237395995126},{"$f":"RADIANS(15*(12-AST!J14))","v":-0.26339927294681115},{"$f":"RADIANS(15*(12-AST!K14))","v":-0.29786952567369895},{"$f":"RADIANS(15*(12-AST!L14))","v":-0.29088820866572151},{"$f":"RADIANS(15*(12-AST!M14))","v":-0.23765566647989447}]
[null,14,{"$f":"RADIANS(15*(12-AST!B15))","v":-0.44360451821522551},{"$f":"RADIANS(15*(12-AST!C15))","v":-0.43182354576426379},{"$f":"RADIANS(15*(12-AST!D15))","v":-0.45974881379617327},{"$f":"RADIANS(15*(12-AST!E15))","v":-0.49727339271405113},{"$f":"RADIANS(15*(12-AST!F15))","v":-0.50687270360001957},{"$f":"RADIANS(15*(12-AST!G15))","v":-0.48636508488908675},{"$f":"RADIANS(15*(12-AST!H15))","v":-0.46542113386515427},{"$f":"RADIANS(15*(12-AST!I15))","v":-0.4820017617591007},{"$f":"RADIANS(15*(12-AST!J15))","v":-0.52519866074596067},{"$f":"RADIANS(15*(12-AST!K15))","v":-0.55966891347284842},{"$f":"RADIANS(15*(12-AST!L15))","v":-0.55268759646487087},{"$f":"RADIANS(15*(12-AST!M15))","v":-0.49945505427904391}]
[null,15,{"$f":"RADIANS(15*(12-AST!B16))","v":-0.70540390601437497},{"$f":"RADIANS(15*(12-AST!C16))","v":-0.69362293356341331},{"$f":"RADIANS(15*(12-AST!D16))","v":-0.72154820159532274},{"$f":"RADIANS(15*(12-AST!E16))","v":-0.7590727805132006},{"$f":"RADIANS(15*(12-AST!F16))","v":-0.76867209139916903},{"$f":"RADIANS(15*(12-AST!G16))","v":-0.74816447268823616},{"$f":"RADIANS(15*(12-AST!H16))","v":-0.72722052166430373},{"$f":"RADIANS(15*(12-AST!I16))","v":-0.74380114955825016},{"$f":"RADIANS(15*(12-AST!J16))","v":-0.78699804854511002},{"$f":"RADIANS(15*(12-AST!K16))","v":-0.82146830127199788},{"$f":"RADIANS(15*(12-AST!L16))","v":-0.81448698426402033},{"$f":"RADIANS(15*(12-AST!M16))","v":-0.76125444207819326}]
[null,16,{"$f":"RADIANS(15*(12-AST!B17))","v":-0.96720329381352432},{"$f":"RADIANS(15*(12-AST!C17))","v":-0.95542232136256267},{"$f":"RADIANS(15*(12-AST!D17))","v":-0.98334758939447209},{"$f":"RADIANS(15*(12-AST!E17))","v":-1.0208721683123501},{"$f":"RADIANS(15*(12-AST!F17))","v":-1.0304714791983185},{"$f":"RADIANS(15*(12-AST!G17))","v":-1.0099638604873855},{"$f":"RADIANS(15*(12-AST!H17))","v":-0.98901990946345308},{"$f":"RADIANS(15*(12-AST!I17))","v":-1.0056005373573995},{"$f":"RADIANS(15*(12-AST!J17))","v":-1.0487974363442589},{"$f":"RADIANS(15*(12-AST!K17))","v":-1.0832676890711472},{"$f":"RADIANS(15*(12-AST!L17))","v":-1.0762863720631697},{"$f":"RADIANS(15*(12-AST!M17))","v":-1.0230538298773426}]
[null,17,{"$f":"RADIANS(15*(12-AST!B18))","v":-1.2290026816126733},{"$f":"RADIANS(15*(12-AST!C18))","v":-1.2172217091617121},{"$f":"RADIANS(15*(12-AST!D18))","v":-1.245146977193621},{"$f":"RADIANS(15*(12-AST!E18))","v":-1.2826715561114994},{"$f":"RADIANS(15*(12-AST!F18))","v":-1.2922708669974681},{"$f":"RADIANS(15*(12-AST!G18))","v":-1.2717632482865344},{"$f":"RADIANS(15*(12-AST!H18))","v":-1.2508192972626031},{"$f":"RADIANS(15*(12-AST!I18))","v":-1.2673999251565491},{"$f":"RADIANS(15*(12-AST!J18))","v":-1.3105968241434085},{"$f":"RADIANS(15*(12-AST!K18))","v":-1.3450670768702966},{"$f":"RADIANS(15*(12-AST!L18))","v":-1.3380857598623193},{"$f":"RADIANS(15*(12-AST!M18))","v":-1.2848532176764922}]
[null,18,{"$f":"RADIANS(15*(12-AST!B19))","v":-1.4908020694118238},{"$f":"RADIANS(15*(12-AST!C19))","v":-1.4790210969608615},{"$f":"RADIANS(15*(12-AST!D19))","v":-1.5069463649927715},{"$f":"RADIANS(15*(12-AST!E19))","v":-1.544470943910649},{"$f":"RADIANS(15*(12-AST!F19))","v":-1.5540702547966181},{"$f":"RADIANS(15*(12-AST!G19))","v":-1.5335626360856838},{"$f":"RADIANS(15*(12-AST!H19))","v":-1.5126186850617527},{"$f":"RADIANS(15*(12-AST!I19))","v":-1.5291993129556984},{"$f":"RADIANS(15*(12-AST!J19))","v":-1.5723962119425587},{"$f":"RADIANS(15*(12-AST!K19))","v":-1.606866464669447},{"$f":"RADIANS(15*(12-AST!L19))","v":-1.5998851476614686},{"$f":"RADIANS(15*(12-AST!M19))","v":-1.5466526054756415}]
[null,19,{"$f":"RADIANS(15*(12-AST!B20))","v":-1.7526014572109732},{"$f":"RADIANS(15*(12-AST!C20))","v":-1.7408204847600111},{"$f":"RADIANS(15*(12-AST!D20))","v":-1.7687457527919208},{"$f":"RADIANS(15*(12-AST!E20))","v":-1.8062703317097983},{"$f":"RADIANS(15*(12-AST!F20))","v":-1.8158696425957677},{"$f":"RADIANS(15*(12-AST!G20))","v":-1.7953620238848333},{"$f":"RADIANS(15*(12-AST!H20))","v":-1.774418072860902},{"$f":"RADIANS(15*(12-AST!I20))","v":-1.790998700754848},{"$f":"RADIANS(15*(12-AST!J20))","v":-1.8341955997417083},{"$f":"RADIANS(15*(12-AST!K20))","v":-1.8686658524685964},{"$f":"RADIANS(15*(12-AST!L20))","v":-1.861684535460618},{"$f":"RADIANS(15*(12-AST!M20))","v":-1.8084519932747911}]
[null,20,{"$f":"RADIANS(15*(12-AST!B21))","v":-2.0144008450101225},{"$f":"RADIANS(15*(12-AST!C21))","v":-2.0026198725591606},{"$f":"RADIANS(15*(12-AST!D21))","v":-2.0305451405910704},{"$f":"RADIANS(15*(12-AST!E21))","v":-2.0680697195089479},{"$f":"RADIANS(15*(12-AST!F21))","v":-2.077669030394917},{"$f":"RADIANS(15*(12-AST!G21))","v":-2.0571614116839827},{"$f":"RADIANS(15*(12-AST!H21))","v":-2.0362174606600516},{"$f":"RADIANS(15*(12-AST!I21))","v":-2.0527980885539976},{"$f":"RADIANS(15*(12-AST!J21))","v":-2.0959949875408577},{"$f":"RADIANS(15*(12-AST!K21))","v":-2.1304652402677458},{"$f":"RADIANS(15*(12-AST!L21))","v":-2.1234839232597675},{"$f":"RADIANS(15*(12-AST!M21))","v":-2.0702513810739402}]
[null,21,{"$f":"RADIANS(15*(12-AST!B22))","v":-2.2762002328092716},{"$f":"RADIANS(15*(12-AST!C22))","v":-2.2644192603583098},{"$f":"RADIANS(15*(12-AST!D22))","v":-2.2923445283902195},{"$f":"RADIANS(15*(12-AST!E22))","v":-2.329869107308097},{"$f":"RADIANS(15*(12-AST!F22))","v":-2.3394684181940666},{"$f":"RADIANS(15*(12-AST!G22))","v":-2.3189607994831323},{"$f":"RADIANS(15*(12-AST!H22))","v":-2.2980168484592007},{"$f":"RADIANS(15*(12-AST!I22))","v":-2.3145974763531467},{"$f":"RADIANS(15*(12-AST!J22))","v":-2.3577943753400068},{"$f":"RADIANS(15*(12-AST!K22))","v":-2.3922646280668953},{"$f":"RADIANS(15*(12-AST!L22))","v":-2.3852833110589167},{"$f":"RADIANS(15*(12-AST!M22))","v":-2.3320507688730903}]
[null,22,{"$f":"RADIANS(15*(12-AST!B23))","v":-2.5379996206084212},{"$f":"RADIANS(15*(12-AST!C23))","v":-2.5262186481574593},{"$f":"RADIANS(15*(12-AST!D23))","v":-2.5541439161893691},{"$f":"RADIANS(15*(12-AST!E23))","v":-2.5916684951072466},{"$f":"RADIANS(15*(12-AST!F23))","v":-2.6012678059932162},{"$f":"RADIANS(15*(12-AST!G23))","v":-2.5807601872822814},{"$f":"RADIANS(15*(12-AST!H23))","v":-2.5598162362583503},{"$f":"RADIANS(15*(12-AST!I23))","v":-2.5763968641522963},{"$f":"RADIANS(15*(12-AST!J23))","v":-2.6195937631391564},{"$f":"RADIANS(15*(12-AST!K23))","v":-2.6540640158660449},{"$f":"RADIANS(15*(12-AST!L23))","v":-2.6470826988580662},{"$f":"RADIANS(15*(12-AST!M23))","v":-2.5938501566722394}]
[null,23,{"$f":"RADIANS(15*(12-AST!B24))","v":-2.7997990084075708},{"$f":"RADIANS(15*(12-AST!C24))","v":-2.7880180359566089},{"$f":"RADIANS(15*(12-AST!D24))","v":-2.8159433039885182},{"$f":"RADIANS(15*(12-AST!E24))","v":-2.8534678829063962},{"$f":"RADIANS(15*(12-AST!F24))","v":-2.8630671937923657},{"$f":"RADIANS(15*(12-AST!G24))","v":-2.842559575081431},{"$f":"RADIANS(15*(12-AST!H24))","v":-2.8216156240574999},{"$f":"RADIANS(15*(12-AST!I24))","v":-2.8381962519514459},{"$f":"RADIANS(15*(12-AST!J24))","v":-2.8813931509383059},{"$f":"RADIANS(15*(12-AST!K24))","v":-2.915863403665194},{"$f":"RADIANS(15*(12-AST!L24))","v":-2.9088820866572158},{"$f":"RADIANS(15*(12-AST!M24))","v":-2.855649544471389}]
[null,24,{"$f":"RADIANS(15*(12-AST!B25))","v":-3.0615983962067199},{"$f":"RADIANS(15*(12-AST!C25))","v":-3.049817423755758},{"$f":"RADIANS(15*(12-AST!D25))","v":-3.0777426917876678},{"$f":"RADIANS(15*(12-AST!E25))","v":-3.1152672707055453},{"$f":"RADIANS(15*(12-AST!F25))","v":-3.1248665815915149},{"$f":"RADIANS(15*(12-AST!G25))","v":-3.1043589628805806},{"$f":"RADIANS(15*(12-AST!H25))","v":-3.083415011856649},{"$f":"RADIANS(15*(12-AST!I25))","v":-3.099995639750595},{"$f":"RADIANS(15*(12-AST!J25))","v":-3.1431925387374551},{"$f":"RADIANS(15*(12-AST!K25))","v":-3.1776627914643436},{"$f":"RADIANS(15*(12-AST!L25))","v":-3.1706814744563654},{"$f":"RADIANS(15*(12-AST!M25))","v":-3.1174489322705385}]

{"sheet":"Incident angle","index":11,"n_rows":180,"n_cols":144,"rows_kept":180,"cut":false,"hidden":true,"merged":[[57,102,57,114],[2,15,2,27],[1,1,1,2],[1,88,1,114],[2,88,2,100],[2,102,2,114],[1,31,1,57],[57,31,57,43],[2,1,2,13],[57,88,57,100],[57,1,57,13],[57,15,57,27],[2,31,2,43],[2,45,2,57],[57,45,57,57],[141,60,141,67],[141,69,141,76],[112,76,112,88],[2,74,2,86],[1,60,1,86],[2,60,2,72],[57,60,57,72],[57,74,57,86],[112,60,112,72]]}
[]
[null,"Home",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Transmitted per sq ft",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Transmitted total BTU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Percentage of total"]
[null,"South Incident Angle",null,null,null,null,null,null,null,null,null,null,null,null,null,"East Incident Angle",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"South Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,"East Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"South Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,"East Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,"South Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,"East Transmitted"]
[null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,{"$f":"'Solar Altitude'!B3","v":0},{"$f":"'Solar Altitude'!C3","v":"Jan"},{"$f":"'Solar Altitude'!D3","v":"Feb"},{"$f":"'Solar Altitude'!E3","v":"Mar"},{"$f":"'Solar Altitude'!F3","v":"Apr"},{"$f":"'Solar Altitude'!G3","v":"May"},{"$f":"'Solar Altitude'!H3","v":"Jun"},{"$f":"'Solar Altitude'!I3","v":"Jul"},{"$f":"'Solar Altitude'!J3","v":"Aug"},{"$f":"'Solar Altitude'!K3","v":"Sep"},{"$f":"'Solar Altitude'!L3","v":"Oct"},{"$f":"'Solar Altitude'!M3","v":"Nov"},{"$f":"'Solar Altitude'!N3","v":"Dec"},null,{"$f":"DN4","v":0},{"$f":"DO4","v":"Jan"},"Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"DEGREES(C33)","v":94.427764435439073},103.75038818007532,114.18642562804527,125.7988349057802,134.05880106841792,137.32989830871489,134.54623242799599,126.0972547614585,113.79434888072159,102.93471141481059,93.851530539011748,90.632545192343642,null,1,{"$f":"DEGREES(Q33)","v":80.211656093594883},80.42615014541947,78.658333333333303,76.803582365113826,76.846679965820812,78.211996998901228,79.081553542746022,77.668097760060832,74.908333333333402,73.238925529430162,74.354912487115016,77.526939258767655,null,null,null,1,{"$f":"IF(DO5<0,0,IF(0>C5,0,IF(50>C5,((-0.000009*C5^2 + 0.0004*C5 + 0.7918)*Radiation!C4),IF(90>C5,(( -0.0006*C5^2 + 0.0699*C5 - 1.2225)*Radiation!C4),0))))","v":0},{"$f":"IF(DP5<0,0,IF(0>D5,0,IF(50>D5,((-0.000009*D5^2 + 0.0004*D5 + 0.7918)*Radiation!D4),IF(90>D5,(( -0.0006*D5^2 + 0.0699*D5 - 1.2225)*Radiation!D4),0))))","v":0},{"$f":"IF(DQ5<0,0,IF(0>E5,0,IF(50>E5,((-0.000009*E5^2 + 0.0004*E5 + 0.7918)*Radiation!E4),IF(90>E5,(( -0.0006*E5^2 + 0.0699*E5 - 1.2225)*Radiation!E4),0))))","v":0},{"$f":"IF(DR5<0,0,IF(0>F5,0,IF(50>F5,((-0.000009*F5^2 + 0.0004*F5 + 0.7918)*Radiation!F4),IF(90>F5,(( -0.0006*F5^2 + 0.0699*F5 - 1.2225)*Radiation!F4),0))))","v":0},{"$f":"IF(DS5<0,0,IF(0>G5,0,IF(50>G5,((-0.000009*G5^2 + 0.0004*G5 + 0.7918)*Radiation!G4),IF(90>G5,(( -0.0006*G5^2 + 0.0699*G5 - 1.2225)*Radiation!G4),0))))","v":0},{"$f":"IF(DT5<0,0,IF(0>H5,0,IF(50>H5,((-0.000009*H5^2 + 0.0004*H5 + 0.7918)*Radiation!H4),IF(90>H5,(( -0.0006*H5^2 + 0.0699*H5 - 1.2225)*Radiation!H4),0))))","v":0},{"$f":"IF(DU5<0,0,IF(0>I5,0,IF(50>I5,((-0.000009*I5^2 + 0.0004*I5 + 0.7918)*Radiation!I4),IF(90>I5,(( -0.0006*I5^2 + 0.0699*I5 - 1.2225)*Radiation!I4),0))))","v":0},{"$f":"IF(DV5<0,0,IF(0>J5,0,IF(50>J5,((-0.000009*J5^2 + 0.0004*J5 + 0.7918)*Radiation!J4),IF(90>J5,(( -0.0006*J5^2 + 0.0699*J5 - 1.2225)*Radiation!J4),0))))","v":0},{"$f":"IF(DW5<0,0,IF(0>K5,0,IF(50>K5,((-0.000009*K5^2 + 0.0004*K5 + 0.7918)*Radiation!K4),IF(90>K5,(( -0.0006*K5^2 + 0.0699*K5 - 1.2225)*Radiation!K4),0))))","v":0},{"$f":"IF(DX5<0,0,IF(0>L5,0,IF(50>L5,((-0.000009*L5^2 + 0.0004*L5 + 0.7918)*Radiation!L4),IF(90>L5,(( -0.0006*L5^2 + 0.0699*L5 - 1.2225)*Radiation!L4),0))))","v":0},{"$f":"IF(DY5<0,0,IF(0>M5,0,IF(50>M5,((-0.000009*M5^2 + 0.0004*M5 + 0.7918)*Radiation!M4),IF(90>M5,(( -0.0006*M5^2 + 0.0699*M5 - 1.2225)*Radiation!M4),0))))","v":0},{"$f":"IF(DZ5<0,0,IF(0>N5,0,IF(50>N5,((-0.000009*N5^2 + 0.0004*N5 + 0.7918)*Radiation!N4),IF(90>N5,(( -0.0006*N5^2 + 0.0699*N5 - 1.2225)*Radiation!N4),0))))","v":0},null,1,{"$f":"IF(EC5<0,0,IF(0>Q5,0,IF(50>Q5,(( -0.000009*Q5^2 + 0.0004*Q5 + 0.7918)*Radiation!C4),IF(90>Q5,((-0.0006*Q5^2 + 0.0699*Q5 - 1.2225)*Radiation!C4),0))))","v":0},{"$f":"IF(ED5<0,0,IF(0>R5,0,IF(50>R5,(( -0.000009*R5^2 + 0.0004*R5 + 0.7918)*Radiation!D4),IF(90>R5,((-0.0006*R5^2 + 0.0699*R5 - 1.2225)*Radiation!D4),0))))","v":0},{"$f":"IF(EE5<0,0,IF(0>S5,0,IF(50>S5,(( -0.000009*S5^2 + 0.0004*S5 + 0.7918)*Radiation!E4),IF(90>S5,((-0.0006*S5^2 + 0.0699*S5 - 1.2225)*Radiation!E4),0))))","v":0},{"$f":"IF(EF5<0,0,IF(0>T5,0,IF(50>T5,(( -0.000009*T5^2 + 0.0004*T5 + 0.7918)*Radiation!F4),IF(90>T5,((-0.0006*T5^2 + 0.0699*T5 - 1.2225)*Radiation!F4),0))))","v":0},{"$f":"IF(EG5<0,0,IF(0>U5,0,IF(50>U5,(( -0.000009*U5^2 + 0.0004*U5 + 0.7918)*Radiation!G4),IF(90>U5,((-0.0006*U5^2 + 0.0699*U5 - 1.2225)*Radiation!G4),0))))","v":0},{"$f":"IF(EH5<0,0,IF(0>V5,0,IF(50>V5,(( -0.000009*V5^2 + 0.0004*V5 + 0.7918)*Radiation!H4),IF(90>V5,((-0.0006*V5^2 + 0.0699*V5 - 1.2225)*Radiation!H4),0))))","v":0},{"$f":"IF(EI5<0,0,IF(0>W5,0,IF(50>W5,(( -0.000009*W5^2 + 0.0004*W5 + 0.7918)*Radiation!I4),IF(90>W5,((-0.0006*W5^2 + 0.0699*W5 - 1.2225)*Radiation!I4),0))))","v":0},{"$f":"IF(EJ5<0,0,IF(0>X5,0,IF(50>X5,(( -0.000009*X5^2 + 0.0004*X5 + 0.7918)*Radiation!J4),IF(90>X5,((-0.0006*X5^2 + 0.0699*X5 - 1.2225)*Radiation!J4),0))))","v":0},{"$f":"IF(EK5<0,0,IF(0>Y5,0,IF(50>Y5,(( -0.000009*Y5^2 + 0.0004*Y5 + 0.7918)*Radiation!K4),IF(90>Y5,((-0.0006*Y5^2 + 0.0699*Y5 - 1.2225)*Radiation!K4),0))))","v":0},{"$f":"IF(EL5<0,0,IF(0>Z5,0,IF(50>Z5,(( -0.000009*Z5^2 + 0.0004*Z5 + 0.7918)*Radiation!L4),IF(90>Z5,((-0.0006*Z5^2 + 0.0699*Z5 - 1.2225)*Radiation!L4),0))))","v":0},{"$f":"IF(EM5<0,0,IF(0>AA5,0,IF(50>AA5,(( -0.000009*AA5^2 + 0.0004*AA5 + 0.7918)*Radiation!M4),IF(90>AA5,((-0.0006*AA5^2 + 0.0699*AA5 - 1.2225)*Radiation!M4),0))))","v":0},{"$f":"IF(EN5<0,0,IF(0>AB5,0,IF(50>AB5,(( -0.000009*AB5^2 + 0.0004*AB5 + 0.7918)*Radiation!N4),IF(90>AB5,((-0.0006*AB5^2 + 0.0699*AB5 - 1.2225)*Radiation!N4),0))))","v":0},null,null,1,{"$f":"AG5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU5","v":0},{"$f":"AH5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV5","v":0},{"$f":"AI5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW5","v":0},{"$f":"AJ5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX5","v":0},{"$f":"AK5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY5","v":0},{"$f":"AL5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ5","v":0},{"$f":"AM5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA5","v":0},{"$f":"AN5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB5","v":0},{"$f":"AO5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC5","v":0},{"$f":"AP5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD5","v":0},{"$f":"AQ5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE5","v":0},{"$f":"AR5*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF5","v":0},null,1,{"$f":"AU5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI5","v":0},{"$f":"AV5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ5","v":0},{"$f":"AW5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK5","v":0},{"$f":"AX5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL5","v":0},{"$f":"AY5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM5","v":0},{"$f":"AZ5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN5","v":0},{"$f":"BA5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO5","v":0},{"$f":"BB5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP5","v":0},{"$f":"BC5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ5","v":0},{"$f":"BD5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR5","v":0},{"$f":"BE5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS5","v":0},{"$f":"BF5*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT5","v":0},null,1,{"$f":"IF(BJ115=0,0,BJ5/BJ115)","v":0},{"$f":"IF(BK115=0,0,BK5/BK115)","v":0},{"$f":"IF(BL115=0,0,BL5/BL115)","v":0},{"$f":"IF(BM115=0,0,BM5/BM115)","v":0},{"$f":"IF(BN115=0,0,BN5/BN115)","v":0},{"$f":"IF(BO115=0,0,BO5/BO115)","v":0},{"$f":"IF(BP115=0,0,BP5/BP115)","v":0},{"$f":"IF(BQ115=0,0,BQ5/BQ115)","v":0},{"$f":"IF(BR115=0,0,BR5/BR115)","v":0},{"$f":"IF(BS115=0,0,BS5/BS115)","v":0},{"$f":"IF(BT115=0,0,BT5/BT115)","v":0},{"$f":"IF(BU115=0,0,BU5/BU115)","v":0},null,1,{"$f":"IF(BJ115=0,0,BX5/BJ115)","v":0},{"$f":"IF(BK115=0,0,BY5/BK115)","v":0},0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B4","v":1},{"$f":"'Solar Altitude'!C4","v":-79.238745258454912},{"$f":"'Solar Altitude'!D4","v":-73.135890206899091},{"$f":"'Solar Altitude'!E4","v":-62.969753990761212},{"$f":"'Solar Altitude'!F4","v":-51.103815741194268},{"$f":"'Solar Altitude'!G4","v":-42.972420763986918},{"$f":"'Solar Altitude'!H4","v":-40.259838967181594},{"$f":"'Solar Altitude'!I4","v":-43.397326661656273},{"$f":"'Solar Altitude'!J4","v":-51.194813940312706},{"$f":"'Solar Altitude'!K4","v":-61.30334441705341},{"$f":"'Solar Altitude'!L4","v":-68.588756925018274},{"$f":"'Solar Altitude'!M4","v":-73.864057818332},{"$f":"'Solar Altitude'!N4","v":-77.510392918823513},null,{"$f":"DN5","v":1},-79.238745258454912,-73.135890206899091,-62.969753990761212,-51.103815741194268,-42.972420763986918,-40.259838967181594,-43.397326661656273,-51.194813940312706,-61.30334441705341,-68.588756925018274,-73.864057818332,-77.510392918823513]
[null,2,{"$f":"DEGREES(C34)","v":92.616332381779301},101.88283821271202,111.99201796307231,123.14112991180887,131.13461300040669,134.46226733550131,131.90812336363038,123.53685005039152,111.1953417112037,100.32763845235745,91.442819186409352,88.566637731271925,null,2,{"$f":"DEGREES(Q34)","v":66.198473357653086},65.70809290001776,63.65833333333336,62.17457951558481,62.916148077749689,64.607895157234339,65.141563764751211,63.047277265987553,59.908333333333367,58.555346461938157,60.42059821472575,63.935040516289604,null,null,null,2,{"$f":"IF(DO6<0,0,IF(0>C6,0,IF(50>C6,((-0.000009*C6^2 + 0.0004*C6 + 0.7918)*Radiation!C5),IF(90>C6,(( -0.0006*C6^2 + 0.0699*C6 - 1.2225)*Radiation!C5),0))))","v":0},{"$f":"IF(DP6<0,0,IF(0>D6,0,IF(50>D6,((-0.000009*D6^2 + 0.0004*D6 + 0.7918)*Radiation!D5),IF(90>D6,(( -0.0006*D6^2 + 0.0699*D6 - 1.2225)*Radiation!D5),0))))","v":0},{"$f":"IF(DQ6<0,0,IF(0>E6,0,IF(50>E6,((-0.000009*E6^2 + 0.0004*E6 + 0.7918)*Radiation!E5),IF(90>E6,(( -0.0006*E6^2 + 0.0699*E6 - 1.2225)*Radiation!E5),0))))","v":0},{"$f":"IF(DR6<0,0,IF(0>F6,0,IF(50>F6,((-0.000009*F6^2 + 0.0004*F6 + 0.7918)*Radiation!F5),IF(90>F6,(( -0.0006*F6^2 + 0.0699*F6 - 1.2225)*Radiation!F5),0))))","v":0},{"$f":"IF(DS6<0,0,IF(0>G6,0,IF(50>G6,((-0.000009*G6^2 + 0.0004*G6 + 0.7918)*Radiation!G5),IF(90>G6,(( -0.0006*G6^2 + 0.0699*G6 - 1.2225)*Radiation!G5),0))))","v":0},{"$f":"IF(DT6<0,0,IF(0>H6,0,IF(50>H6,((-0.000009*H6^2 + 0.0004*H6 + 0.7918)*Radiation!H5),IF(90>H6,(( -0.0006*H6^2 + 0.0699*H6 - 1.2225)*Radiation!H5),0))))","v":0},{"$f":"IF(DU6<0,0,IF(0>I6,0,IF(50>I6,((-0.000009*I6^2 + 0.0004*I6 + 0.7918)*Radiation!I5),IF(90>I6,(( -0.0006*I6^2 + 0.0699*I6 - 1.2225)*Radiation!I5),0))))","v":0},{"$f":"IF(DV6<0,0,IF(0>J6,0,IF(50>J6,((-0.000009*J6^2 + 0.0004*J6 + 0.7918)*Radiation!J5),IF(90>J6,(( -0.0006*J6^2 + 0.0699*J6 - 1.2225)*Radiation!J5),0))))","v":0},{"$f":"IF(DW6<0,0,IF(0>K6,0,IF(50>K6,((-0.000009*K6^2 + 0.0004*K6 + 0.7918)*Radiation!K5),IF(90>K6,(( -0.0006*K6^2 + 0.0699*K6 - 1.2225)*Radiation!K5),0))))","v":0},{"$f":"IF(DX6<0,0,IF(0>L6,0,IF(50>L6,((-0.000009*L6^2 + 0.0004*L6 + 0.7918)*Radiation!L5),IF(90>L6,(( -0.0006*L6^2 + 0.0699*L6 - 1.2225)*Radiation!L5),0))))","v":0},{"$f":"IF(DY6<0,0,IF(0>M6,0,IF(50>M6,((-0.000009*M6^2 + 0.0004*M6 + 0.7918)*Radiation!M5),IF(90>M6,(( -0.0006*M6^2 + 0.0699*M6 - 1.2225)*Radiation!M5),0))))","v":0},{"$f":"IF(DZ6<0,0,IF(0>N6,0,IF(50>N6,((-0.000009*N6^2 + 0.0004*N6 + 0.7918)*Radiation!N5),IF(90>N6,(( -0.0006*N6^2 + 0.0699*N6 - 1.2225)*Radiation!N5),0))))","v":0},null,2,{"$f":"IF(EC6<0,0,IF(0>Q6,0,IF(50>Q6,(( -0.000009*Q6^2 + 0.0004*Q6 + 0.7918)*Radiation!C5),IF(90>Q6,((-0.0006*Q6^2 + 0.0699*Q6 - 1.2225)*Radiation!C5),0))))","v":0},{"$f":"IF(ED6<0,0,IF(0>R6,0,IF(50>R6,(( -0.000009*R6^2 + 0.0004*R6 + 0.7918)*Radiation!D5),IF(90>R6,((-0.0006*R6^2 + 0.0699*R6 - 1.2225)*Radiation!D5),0))))","v":0},{"$f":"IF(EE6<0,0,IF(0>S6,0,IF(50>S6,(( -0.000009*S6^2 + 0.0004*S6 + 0.7918)*Radiation!E5),IF(90>S6,((-0.0006*S6^2 + 0.0699*S6 - 1.2225)*Radiation!E5),0))))","v":0},{"$f":"IF(EF6<0,0,IF(0>T6,0,IF(50>T6,(( -0.000009*T6^2 + 0.0004*T6 + 0.7918)*Radiation!F5),IF(90>T6,((-0.0006*T6^2 + 0.0699*T6 - 1.2225)*Radiation!F5),0))))","v":0},{"$f":"IF(EG6<0,0,IF(0>U6,0,IF(50>U6,(( -0.000009*U6^2 + 0.0004*U6 + 0.7918)*Radiation!G5),IF(90>U6,((-0.0006*U6^2 + 0.0699*U6 - 1.2225)*Radiation!G5),0))))","v":0},{"$f":"IF(EH6<0,0,IF(0>V6,0,IF(50>V6,(( -0.000009*V6^2 + 0.0004*V6 + 0.7918)*Radiation!H5),IF(90>V6,((-0.0006*V6^2 + 0.0699*V6 - 1.2225)*Radiation!H5),0))))","v":0},{"$f":"IF(EI6<0,0,IF(0>W6,0,IF(50>W6,(( -0.000009*W6^2 + 0.0004*W6 + 0.7918)*Radiation!I5),IF(90>W6,((-0.0006*W6^2 + 0.0699*W6 - 1.2225)*Radiation!I5),0))))","v":0},{"$f":"IF(EJ6<0,0,IF(0>X6,0,IF(50>X6,(( -0.000009*X6^2 + 0.0004*X6 + 0.7918)*Radiation!J5),IF(90>X6,((-0.0006*X6^2 + 0.0699*X6 - 1.2225)*Radiation!J5),0))))","v":0},{"$f":"IF(EK6<0,0,IF(0>Y6,0,IF(50>Y6,(( -0.000009*Y6^2 + 0.0004*Y6 + 0.7918)*Radiation!K5),IF(90>Y6,((-0.0006*Y6^2 + 0.0699*Y6 - 1.2225)*Radiation!K5),0))))","v":0},{"$f":"IF(EL6<0,0,IF(0>Z6,0,IF(50>Z6,(( -0.000009*Z6^2 + 0.0004*Z6 + 0.7918)*Radiation!L5),IF(90>Z6,((-0.0006*Z6^2 + 0.0699*Z6 - 1.2225)*Radiation!L5),0))))","v":0},{"$f":"IF(EM6<0,0,IF(0>AA6,0,IF(50>AA6,(( -0.000009*AA6^2 + 0.0004*AA6 + 0.7918)*Radiation!M5),IF(90>AA6,((-0.0006*AA6^2 + 0.0699*AA6 - 1.2225)*Radiation!M5),0))))","v":0},{"$f":"IF(EN6<0,0,IF(0>AB6,0,IF(50>AB6,(( -0.000009*AB6^2 + 0.0004*AB6 + 0.7918)*Radiation!N5),IF(90>AB6,((-0.0006*AB6^2 + 0.0699*AB6 - 1.2225)*Radiation!N5),0))))","v":0},null,null,2,{"$f":"AG6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU6","v":0},{"$f":"AH6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV6","v":0},{"$f":"AI6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW6","v":0},{"$f":"AJ6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX6","v":0},{"$f":"AK6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY6","v":0},{"$f":"AL6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ6","v":0},{"$f":"AM6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA6","v":0},{"$f":"AN6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB6","v":0},{"$f":"AO6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC6","v":0},{"$f":"AP6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD6","v":0},{"$f":"AQ6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE6","v":0},{"$f":"AR6*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF6","v":0},null,2,{"$f":"AU6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI6","v":0},{"$f":"AV6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ6","v":0},{"$f":"AW6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK6","v":0},{"$f":"AX6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL6","v":0},{"$f":"AY6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM6","v":0},{"$f":"AZ6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN6","v":0},{"$f":"BA6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO6","v":0},{"$f":"BB6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP6","v":0},{"$f":"BC6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ6","v":0},{"$f":"BD6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR6","v":0},{"$f":"BE6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS6","v":0},{"$f":"BF6*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT6","v":0},null,2,0,0,0,0,0,0,0,0,0,0,0,0,null,2,0,{"$f":"IF(BK116=0,0,BY6/BK116)","v":0},{"$f":"IF(BL116=0,0,BZ6/BL116)","v":0},{"$f":"IF(BM116=0,0,CA6/BM116)","v":0},{"$f":"IF(BN116=0,0,CB6/BN116)","v":0},{"$f":"IF(BO116=0,0,CC6/BO116)","v":0},{"$f":"IF(BP116=0,0,CD6/BP116)","v":0},{"$f":"IF(BQ116=0,0,CE6/BQ116)","v":0},{"$f":"IF(BR116=0,0,CF6/BR116)","v":0},{"$f":"IF(BS116=0,0,CG6/BS116)","v":0},{"$f":"IF(BT116=0,0,CH6/BT116)","v":0},{"$f":"IF(BU116=0,0,CI6/BU116)","v":0},null,null,{"$f":"'Solar Altitude'!B5","v":2},{"$f":"'Solar Altitude'!C5","v":-66.037221876299029},{"$f":"'Solar Altitude'!D5","v":-62.610262119735701},{"$f":"'Solar Altitude'!E5","v":-54.505603493104644},{"$f":"'Solar Altitude'!F5","v":-44.039138424385058},{"$f":"'Solar Altitude'!G5","v":-36.867903866984811},{"$f":"'Solar Altitude'!H5","v":-34.787290206430924},{"$f":"'Solar Altitude'!I5","v":-37.887883453111968},{"$f":"'Solar Altitude'!J5","v":-44.388788539159933},{"$f":"'Solar Altitude'!K5","v":-51.819137025254065},{"$f":"'Solar Altitude'!L5","v":-56.521775308526607},{"$f":"'Solar Altitude'!M5","v":-60.378308807607461},{"$f":"'Solar Altitude'!N5","v":-63.889653492857697},null,2,-66.037221876299029,-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697]
[null,3,{"$f":"DEGREES(C35)","v":89.421788187374304},98.552069571944557,108.28403534265583,118.9453419490403,126.64922385135311,129.97960982634706,127.62965977915214,119.41401094029339,107.15774933833094,96.372983751631963,87.730340945568003,85.181362802707582,null,3,{"$f":"DEGREES(Q35)","v":52.437410650188276},51.066551624009087,48.658333333333339,47.665488828500578,49.307220768285362,51.383290954296264,51.486735653262421,48.543799917354953,44.908333333333346,43.993651713190367,46.847636168318587,50.738887712860532,null,null,null,3,{"$f":"IF(DO7<0,0,IF(0>C7,0,IF(50>C7,((-0.000009*C7^2 + 0.0004*C7 + 0.7918)*Radiation!C6),IF(90>C7,(( -0.0006*C7^2 + 0.0699*C7 - 1.2225)*Radiation!C6),0))))","v":0},{"$f":"IF(DP7<0,0,IF(0>D7,0,IF(50>D7,((-0.000009*D7^2 + 0.0004*D7 + 0.7918)*Radiation!D6),IF(90>D7,(( -0.0006*D7^2 + 0.0699*D7 - 1.2225)*Radiation!D6),0))))","v":0},{"$f":"IF(DQ7<0,0,IF(0>E7,0,IF(50>E7,((-0.000009*E7^2 + 0.0004*E7 + 0.7918)*Radiation!E6),IF(90>E7,(( -0.0006*E7^2 + 0.0699*E7 - 1.2225)*Radiation!E6),0))))","v":0},{"$f":"IF(DR7<0,0,IF(0>F7,0,IF(50>F7,((-0.000009*F7^2 + 0.0004*F7 + 0.7918)*Radiation!F6),IF(90>F7,(( -0.0006*F7^2 + 0.0699*F7 - 1.2225)*Radiation!F6),0))))","v":0},{"$f":"IF(DS7<0,0,IF(0>G7,0,IF(50>G7,((-0.000009*G7^2 + 0.0004*G7 + 0.7918)*Radiation!G6),IF(90>G7,(( -0.0006*G7^2 + 0.0699*G7 - 1.2225)*Radiation!G6),0))))","v":0},{"$f":"IF(DT7<0,0,IF(0>H7,0,IF(50>H7,((-0.000009*H7^2 + 0.0004*H7 + 0.7918)*Radiation!H6),IF(90>H7,(( -0.0006*H7^2 + 0.0699*H7 - 1.2225)*Radiation!H6),0))))","v":0},{"$f":"IF(DU7<0,0,IF(0>I7,0,IF(50>I7,((-0.000009*I7^2 + 0.0004*I7 + 0.7918)*Radiation!I6),IF(90>I7,(( -0.0006*I7^2 + 0.0699*I7 - 1.2225)*Radiation!I6),0))))","v":0},{"$f":"IF(DV7<0,0,IF(0>J7,0,IF(50>J7,((-0.000009*J7^2 + 0.0004*J7 + 0.7918)*Radiation!J6),IF(90>J7,(( -0.0006*J7^2 + 0.0699*J7 - 1.2225)*Radiation!J6),0))))","v":0},{"$f":"IF(DW7<0,0,IF(0>K7,0,IF(50>K7,((-0.000009*K7^2 + 0.0004*K7 + 0.7918)*Radiation!K6),IF(90>K7,(( -0.0006*K7^2 + 0.0699*K7 - 1.2225)*Radiation!K6),0))))","v":0},{"$f":"IF(DX7<0,0,IF(0>L7,0,IF(50>L7,((-0.000009*L7^2 + 0.0004*L7 + 0.7918)*Radiation!L6),IF(90>L7,(( -0.0006*L7^2 + 0.0699*L7 - 1.2225)*Radiation!L6),0))))","v":0},{"$f":"IF(DY7<0,0,IF(0>M7,0,IF(50>M7,((-0.000009*M7^2 + 0.0004*M7 + 0.7918)*Radiation!M6),IF(90>M7,(( -0.0006*M7^2 + 0.0699*M7 - 1.2225)*Radiation!M6),0))))","v":0},{"$f":"IF(DZ7<0,0,IF(0>N7,0,IF(50>N7,((-0.000009*N7^2 + 0.0004*N7 + 0.7918)*Radiation!N6),IF(90>N7,(( -0.0006*N7^2 + 0.0699*N7 - 1.2225)*Radiation!N6),0))))","v":0},null,3,{"$f":"IF(EC7<0,0,IF(0>Q7,0,IF(50>Q7,(( -0.000009*Q7^2 + 0.0004*Q7 + 0.7918)*Radiation!C6),IF(90>Q7,((-0.0006*Q7^2 + 0.0699*Q7 - 1.2225)*Radiation!C6),0))))","v":0},{"$f":"IF(ED7<0,0,IF(0>R7,0,IF(50>R7,(( -0.000009*R7^2 + 0.0004*R7 + 0.7918)*Radiation!D6),IF(90>R7,((-0.0006*R7^2 + 0.0699*R7 - 1.2225)*Radiation!D6),0))))","v":0},{"$f":"IF(EE7<0,0,IF(0>S7,0,IF(50>S7,(( -0.000009*S7^2 + 0.0004*S7 + 0.7918)*Radiation!E6),IF(90>S7,((-0.0006*S7^2 + 0.0699*S7 - 1.2225)*Radiation!E6),0))))","v":0},{"$f":"IF(EF7<0,0,IF(0>T7,0,IF(50>T7,(( -0.000009*T7^2 + 0.0004*T7 + 0.7918)*Radiation!F6),IF(90>T7,((-0.0006*T7^2 + 0.0699*T7 - 1.2225)*Radiation!F6),0))))","v":0},{"$f":"IF(EG7<0,0,IF(0>U7,0,IF(50>U7,(( -0.000009*U7^2 + 0.0004*U7 + 0.7918)*Radiation!G6),IF(90>U7,((-0.0006*U7^2 + 0.0699*U7 - 1.2225)*Radiation!G6),0))))","v":0},{"$f":"IF(EH7<0,0,IF(0>V7,0,IF(50>V7,(( -0.000009*V7^2 + 0.0004*V7 + 0.7918)*Radiation!H6),IF(90>V7,((-0.0006*V7^2 + 0.0699*V7 - 1.2225)*Radiation!H6),0))))","v":0},{"$f":"IF(EI7<0,0,IF(0>W7,0,IF(50>W7,(( -0.000009*W7^2 + 0.0004*W7 + 0.7918)*Radiation!I6),IF(90>W7,((-0.0006*W7^2 + 0.0699*W7 - 1.2225)*Radiation!I6),0))))","v":0},{"$f":"IF(EJ7<0,0,IF(0>X7,0,IF(50>X7,(( -0.000009*X7^2 + 0.0004*X7 + 0.7918)*Radiation!J6),IF(90>X7,((-0.0006*X7^2 + 0.0699*X7 - 1.2225)*Radiation!J6),0))))","v":0},{"$f":"IF(EK7<0,0,IF(0>Y7,0,IF(50>Y7,(( -0.000009*Y7^2 + 0.0004*Y7 + 0.7918)*Radiation!K6),IF(90>Y7,((-0.0006*Y7^2 + 0.0699*Y7 - 1.2225)*Radiation!K6),0))))","v":0},{"$f":"IF(EL7<0,0,IF(0>Z7,0,IF(50>Z7,(( -0.000009*Z7^2 + 0.0004*Z7 + 0.7918)*Radiation!L6),IF(90>Z7,((-0.0006*Z7^2 + 0.0699*Z7 - 1.2225)*Radiation!L6),0))))","v":0},{"$f":"IF(EM7<0,0,IF(0>AA7,0,IF(50>AA7,(( -0.000009*AA7^2 + 0.0004*AA7 + 0.7918)*Radiation!M6),IF(90>AA7,((-0.0006*AA7^2 + 0.0699*AA7 - 1.2225)*Radiation!M6),0))))","v":0},{"$f":"IF(EN7<0,0,IF(0>AB7,0,IF(50>AB7,(( -0.000009*AB7^2 + 0.0004*AB7 + 0.7918)*Radiation!N6),IF(90>AB7,((-0.0006*AB7^2 + 0.0699*AB7 - 1.2225)*Radiation!N6),0))))","v":0},null,null,3,{"$f":"AG7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU7","v":0},{"$f":"AH7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV7","v":0},{"$f":"AI7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW7","v":0},{"$f":"AJ7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX7","v":0},{"$f":"AK7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY7","v":0},{"$f":"AL7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ7","v":0},{"$f":"AM7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA7","v":0},{"$f":"AN7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB7","v":0},{"$f":"AO7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC7","v":0},{"$f":"AP7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD7","v":0},{"$f":"AQ7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE7","v":0},{"$f":"AR7*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF7","v":0},null,3,{"$f":"AU7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI7","v":0},{"$f":"AV7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ7","v":0},{"$f":"AW7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK7","v":0},{"$f":"AX7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL7","v":0},{"$f":"AY7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM7","v":0},{"$f":"AZ7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN7","v":0},{"$f":"BA7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO7","v":0},{"$f":"BB7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP7","v":0},{"$f":"BC7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ7","v":0},{"$f":"BD7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR7","v":0},{"$f":"BE7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS7","v":0},{"$f":"BF7*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT7","v":0},null,3,0,0,0,0,0,0,0,0,0,0,0,0,null,3,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B6","v":3},{"$f":"'Solar Altitude'!C6","v":-52.431373562484438},{"$f":"'Solar Altitude'!D6","v":-49.776364898184575},{"$f":"'Solar Altitude'!E6","v":-43.00744408924087},{"$f":"'Solar Altitude'!F6","v":-33.970697614512481},{"$f":"'Solar Altitude'!G6","v":-27.874166624770901},{"$f":"'Solar Altitude'!H6","v":-26.397406240900974},{"$f":"'Solar Altitude'!I6","v":-29.298461575777225},{"$f":"'Solar Altitude'!J6","v":-34.480458721023354},{"$f":"'Solar Altitude'!K6","v":-39.89507498863518},{"$f":"'Solar Altitude'!L6","v":-43.286892300779471},{"$f":"'Solar Altitude'!M6","v":-46.757596903257479},{"$f":"'Solar Altitude'!N6","v":-50.32692672055552},null,3,-52.431373562484438,-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552]
[null,4,{"$f":"DEGREES(C36)","v":85.053982641414919},94.012951465702486,103.39119101462578,113.64268461471413,121.11781827838766,124.43302516792059,122.22507392798765,114.15897074163232,102.02592730130129,91.355981984453905,82.948595311363079,80.68260606153396,null,4,{"$f":"DEGREES(Q36)","v":39.272815363784119},36.618652439227098,33.658333333333339,33.463039652764039,36.459337884487461,39.024897587328631,38.502757361484051,34.338234473859956,29.908333333333321,29.757740035869418,34.142635467633298,38.446132425353888,null,null,null,4,{"$f":"IF(DO8<0,0,IF(0>C8,0,IF(50>C8,((-0.000009*C8^2 + 0.0004*C8 + 0.7918)*Radiation!C7),IF(90>C8,(( -0.0006*C8^2 + 0.0699*C8 - 1.2225)*Radiation!C7),0))))","v":0},{"$f":"IF(DP8<0,0,IF(0>D8,0,IF(50>D8,((-0.000009*D8^2 + 0.0004*D8 + 0.7918)*Radiation!D7),IF(90>D8,(( -0.0006*D8^2 + 0.0699*D8 - 1.2225)*Radiation!D7),0))))","v":0},{"$f":"IF(DQ8<0,0,IF(0>E8,0,IF(50>E8,((-0.000009*E8^2 + 0.0004*E8 + 0.7918)*Radiation!E7),IF(90>E8,(( -0.0006*E8^2 + 0.0699*E8 - 1.2225)*Radiation!E7),0))))","v":0},{"$f":"IF(DR8<0,0,IF(0>F8,0,IF(50>F8,((-0.000009*F8^2 + 0.0004*F8 + 0.7918)*Radiation!F7),IF(90>F8,(( -0.0006*F8^2 + 0.0699*F8 - 1.2225)*Radiation!F7),0))))","v":0},{"$f":"IF(DS8<0,0,IF(0>G8,0,IF(50>G8,((-0.000009*G8^2 + 0.0004*G8 + 0.7918)*Radiation!G7),IF(90>G8,(( -0.0006*G8^2 + 0.0699*G8 - 1.2225)*Radiation!G7),0))))","v":0},{"$f":"IF(DT8<0,0,IF(0>H8,0,IF(50>H8,((-0.000009*H8^2 + 0.0004*H8 + 0.7918)*Radiation!H7),IF(90>H8,(( -0.0006*H8^2 + 0.0699*H8 - 1.2225)*Radiation!H7),0))))","v":0},{"$f":"IF(DU8<0,0,IF(0>I8,0,IF(50>I8,((-0.000009*I8^2 + 0.0004*I8 + 0.7918)*Radiation!I7),IF(90>I8,(( -0.0006*I8^2 + 0.0699*I8 - 1.2225)*Radiation!I7),0))))","v":0},{"$f":"IF(DV8<0,0,IF(0>J8,0,IF(50>J8,((-0.000009*J8^2 + 0.0004*J8 + 0.7918)*Radiation!J7),IF(90>J8,(( -0.0006*J8^2 + 0.0699*J8 - 1.2225)*Radiation!J7),0))))","v":0},{"$f":"IF(DW8<0,0,IF(0>K8,0,IF(50>K8,((-0.000009*K8^2 + 0.0004*K8 + 0.7918)*Radiation!K7),IF(90>K8,(( -0.0006*K8^2 + 0.0699*K8 - 1.2225)*Radiation!K7),0))))","v":0},{"$f":"IF(DX8<0,0,IF(0>L8,0,IF(50>L8,((-0.000009*L8^2 + 0.0004*L8 + 0.7918)*Radiation!L7),IF(90>L8,(( -0.0006*L8^2 + 0.0699*L8 - 1.2225)*Radiation!L7),0))))","v":0},{"$f":"IF(DY8<0,0,IF(0>M8,0,IF(50>M8,((-0.000009*M8^2 + 0.0004*M8 + 0.7918)*Radiation!M7),IF(90>M8,(( -0.0006*M8^2 + 0.0699*M8 - 1.2225)*Radiation!M7),0))))","v":0},{"$f":"IF(DZ8<0,0,IF(0>N8,0,IF(50>N8,((-0.000009*N8^2 + 0.0004*N8 + 0.7918)*Radiation!N7),IF(90>N8,(( -0.0006*N8^2 + 0.0699*N8 - 1.2225)*Radiation!N7),0))))","v":0},null,4,{"$f":"IF(EC8<0,0,IF(0>Q8,0,IF(50>Q8,(( -0.000009*Q8^2 + 0.0004*Q8 + 0.7918)*Radiation!C7),IF(90>Q8,((-0.0006*Q8^2 + 0.0699*Q8 - 1.2225)*Radiation!C7),0))))","v":0},{"$f":"IF(ED8<0,0,IF(0>R8,0,IF(50>R8,(( -0.000009*R8^2 + 0.0004*R8 + 0.7918)*Radiation!D7),IF(90>R8,((-0.0006*R8^2 + 0.0699*R8 - 1.2225)*Radiation!D7),0))))","v":0},{"$f":"IF(EE8<0,0,IF(0>S8,0,IF(50>S8,(( -0.000009*S8^2 + 0.0004*S8 + 0.7918)*Radiation!E7),IF(90>S8,((-0.0006*S8^2 + 0.0699*S8 - 1.2225)*Radiation!E7),0))))","v":0},{"$f":"IF(EF8<0,0,IF(0>T8,0,IF(50>T8,(( -0.000009*T8^2 + 0.0004*T8 + 0.7918)*Radiation!F7),IF(90>T8,((-0.0006*T8^2 + 0.0699*T8 - 1.2225)*Radiation!F7),0))))","v":0},{"$f":"IF(EG8<0,0,IF(0>U8,0,IF(50>U8,(( -0.000009*U8^2 + 0.0004*U8 + 0.7918)*Radiation!G7),IF(90>U8,((-0.0006*U8^2 + 0.0699*U8 - 1.2225)*Radiation!G7),0))))","v":0},{"$f":"IF(EH8<0,0,IF(0>V8,0,IF(50>V8,(( -0.000009*V8^2 + 0.0004*V8 + 0.7918)*Radiation!H7),IF(90>V8,((-0.0006*V8^2 + 0.0699*V8 - 1.2225)*Radiation!H7),0))))","v":0},{"$f":"IF(EI8<0,0,IF(0>W8,0,IF(50>W8,(( -0.000009*W8^2 + 0.0004*W8 + 0.7918)*Radiation!I7),IF(90>W8,((-0.0006*W8^2 + 0.0699*W8 - 1.2225)*Radiation!I7),0))))","v":0},{"$f":"IF(EJ8<0,0,IF(0>X8,0,IF(50>X8,(( -0.000009*X8^2 + 0.0004*X8 + 0.7918)*Radiation!J7),IF(90>X8,((-0.0006*X8^2 + 0.0699*X8 - 1.2225)*Radiation!J7),0))))","v":0},{"$f":"IF(EK8<0,0,IF(0>Y8,0,IF(50>Y8,(( -0.000009*Y8^2 + 0.0004*Y8 + 0.7918)*Radiation!K7),IF(90>Y8,((-0.0006*Y8^2 + 0.0699*Y8 - 1.2225)*Radiation!K7),0))))","v":0},{"$f":"IF(EL8<0,0,IF(0>Z8,0,IF(50>Z8,(( -0.000009*Z8^2 + 0.0004*Z8 + 0.7918)*Radiation!L7),IF(90>Z8,((-0.0006*Z8^2 + 0.0699*Z8 - 1.2225)*Radiation!L7),0))))","v":0},{"$f":"IF(EM8<0,0,IF(0>AA8,0,IF(50>AA8,(( -0.000009*AA8^2 + 0.0004*AA8 + 0.7918)*Radiation!M7),IF(90>AA8,((-0.0006*AA8^2 + 0.0699*AA8 - 1.2225)*Radiation!M7),0))))","v":0},{"$f":"IF(EN8<0,0,IF(0>AB8,0,IF(50>AB8,(( -0.000009*AB8^2 + 0.0004*AB8 + 0.7918)*Radiation!N7),IF(90>AB8,((-0.0006*AB8^2 + 0.0699*AB8 - 1.2225)*Radiation!N7),0))))","v":0},null,null,4,{"$f":"AG8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU8","v":0},{"$f":"AH8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV8","v":0},{"$f":"AI8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW8","v":0},{"$f":"AJ8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX8","v":0},{"$f":"AK8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY8","v":0},{"$f":"AL8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ8","v":0},{"$f":"AM8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA8","v":0},{"$f":"AN8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB8","v":0},{"$f":"AO8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC8","v":0},{"$f":"AP8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD8","v":0},{"$f":"AQ8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE8","v":0},{"$f":"AR8*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF8","v":0},null,4,{"$f":"AU8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI8","v":0},{"$f":"AV8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ8","v":0},{"$f":"AW8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK8","v":0},{"$f":"AX8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL8","v":0},{"$f":"AY8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM8","v":0},{"$f":"AZ8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN8","v":0},{"$f":"BA8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO8","v":0},{"$f":"BB8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP8","v":0},{"$f":"BC8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ8","v":0},{"$f":"BD8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR8","v":0},{"$f":"BE8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS8","v":0},{"$f":"BF8*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT8","v":0},null,4,0,0,0,0,0,0,0,0,0,0,0,0,null,4,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B7","v":4},{"$f":"'Solar Altitude'!C7","v":-38.837571781392398},{"$f":"'Solar Altitude'!D7","v":-36.325136967893741},{"$f":"'Solar Altitude'!E7","v":-30.23387910899125},{"$f":"'Solar Altitude'!F7","v":-22.236891602714234},{"$f":"'Solar Altitude'!G7","v":-17.058579195686843},{"$f":"'Solar Altitude'!H7","v":-16.082853037589089},{"$f":"'Solar Altitude'!I7","v":-18.740224973134019},{"$f":"'Solar Altitude'!J7","v":-22.841111056638525},{"$f":"'Solar Altitude'!K7","v":-26.935985833021629},{"$f":"'Solar Altitude'!L7","v":-29.720493919992279},{"$f":"'Solar Altitude'!M7","v":-33.206986937806654},{"$f":"'Solar Altitude'!N7","v":-36.893522726896833},null,4,-38.837571781392398,-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833]
[null,5,{"$f":"DEGREES(C37)","v":79.773426955763838},88.573049190838788,97.682629304268744,107.66946451033002,115.02070318899732,118.32513425230428,116.18561015543018,108.21055216160548,96.171570684789046,85.596498273320066,77.371710623561214,75.320626771769952,null,5,{"$f":"DEGREES(Q37)","v":27.637871812062123},22.760226129815841,18.658333333333335,20.252986237488916,25.611674241310439,28.753808102271933,27.23597615871239,21.072659509379324,14.908333333333326,16.727385306572234,23.80243187548535,28.338651450576869,null,null,null,5,{"$f":"IF(DO9<0,0,IF(0>C9,0,IF(50>C9,((-0.000009*C9^2 + 0.0004*C9 + 0.7918)*Radiation!C8),IF(90>C9,(( -0.0006*C9^2 + 0.0699*C9 - 1.2225)*Radiation!C8),0))))","v":0},{"$f":"IF(DP9<0,0,IF(0>D9,0,IF(50>D9,((-0.000009*D9^2 + 0.0004*D9 + 0.7918)*Radiation!D8),IF(90>D9,(( -0.0006*D9^2 + 0.0699*D9 - 1.2225)*Radiation!D8),0))))","v":0},{"$f":"IF(DQ9<0,0,IF(0>E9,0,IF(50>E9,((-0.000009*E9^2 + 0.0004*E9 + 0.7918)*Radiation!E8),IF(90>E9,(( -0.0006*E9^2 + 0.0699*E9 - 1.2225)*Radiation!E8),0))))","v":0},{"$f":"IF(DR9<0,0,IF(0>F9,0,IF(50>F9,((-0.000009*F9^2 + 0.0004*F9 + 0.7918)*Radiation!F8),IF(90>F9,(( -0.0006*F9^2 + 0.0699*F9 - 1.2225)*Radiation!F8),0))))","v":0},{"$f":"IF(DS9<0,0,IF(0>G9,0,IF(50>G9,((-0.000009*G9^2 + 0.0004*G9 + 0.7918)*Radiation!G8),IF(90>G9,(( -0.0006*G9^2 + 0.0699*G9 - 1.2225)*Radiation!G8),0))))","v":0},{"$f":"IF(DT9<0,0,IF(0>H9,0,IF(50>H9,((-0.000009*H9^2 + 0.0004*H9 + 0.7918)*Radiation!H8),IF(90>H9,(( -0.0006*H9^2 + 0.0699*H9 - 1.2225)*Radiation!H8),0))))","v":0},{"$f":"IF(DU9<0,0,IF(0>I9,0,IF(50>I9,((-0.000009*I9^2 + 0.0004*I9 + 0.7918)*Radiation!I8),IF(90>I9,(( -0.0006*I9^2 + 0.0699*I9 - 1.2225)*Radiation!I8),0))))","v":0},{"$f":"IF(DV9<0,0,IF(0>J9,0,IF(50>J9,((-0.000009*J9^2 + 0.0004*J9 + 0.7918)*Radiation!J8),IF(90>J9,(( -0.0006*J9^2 + 0.0699*J9 - 1.2225)*Radiation!J8),0))))","v":0},{"$f":"IF(DW9<0,0,IF(0>K9,0,IF(50>K9,((-0.000009*K9^2 + 0.0004*K9 + 0.7918)*Radiation!K8),IF(90>K9,(( -0.0006*K9^2 + 0.0699*K9 - 1.2225)*Radiation!K8),0))))","v":0},{"$f":"IF(DX9<0,0,IF(0>L9,0,IF(50>L9,((-0.000009*L9^2 + 0.0004*L9 + 0.7918)*Radiation!L8),IF(90>L9,(( -0.0006*L9^2 + 0.0699*L9 - 1.2225)*Radiation!L8),0))))","v":0},{"$f":"IF(DY9<0,0,IF(0>M9,0,IF(50>M9,((-0.000009*M9^2 + 0.0004*M9 + 0.7918)*Radiation!M8),IF(90>M9,(( -0.0006*M9^2 + 0.0699*M9 - 1.2225)*Radiation!M8),0))))","v":0},{"$f":"IF(DZ9<0,0,IF(0>N9,0,IF(50>N9,((-0.000009*N9^2 + 0.0004*N9 + 0.7918)*Radiation!N8),IF(90>N9,(( -0.0006*N9^2 + 0.0699*N9 - 1.2225)*Radiation!N8),0))))","v":0},null,5,{"$f":"IF(EC9<0,0,IF(0>Q9,0,IF(50>Q9,(( -0.000009*Q9^2 + 0.0004*Q9 + 0.7918)*Radiation!C8),IF(90>Q9,((-0.0006*Q9^2 + 0.0699*Q9 - 1.2225)*Radiation!C8),0))))","v":0},{"$f":"IF(ED9<0,0,IF(0>R9,0,IF(50>R9,(( -0.000009*R9^2 + 0.0004*R9 + 0.7918)*Radiation!D8),IF(90>R9,((-0.0006*R9^2 + 0.0699*R9 - 1.2225)*Radiation!D8),0))))","v":0},{"$f":"IF(EE9<0,0,IF(0>S9,0,IF(50>S9,(( -0.000009*S9^2 + 0.0004*S9 + 0.7918)*Radiation!E8),IF(90>S9,((-0.0006*S9^2 + 0.0699*S9 - 1.2225)*Radiation!E8),0))))","v":0},{"$f":"IF(EF9<0,0,IF(0>T9,0,IF(50>T9,(( -0.000009*T9^2 + 0.0004*T9 + 0.7918)*Radiation!F8),IF(90>T9,((-0.0006*T9^2 + 0.0699*T9 - 1.2225)*Radiation!F8),0))))","v":0},{"$f":"IF(EG9<0,0,IF(0>U9,0,IF(50>U9,(( -0.000009*U9^2 + 0.0004*U9 + 0.7918)*Radiation!G8),IF(90>U9,((-0.0006*U9^2 + 0.0699*U9 - 1.2225)*Radiation!G8),0))))","v":0},{"$f":"IF(EH9<0,0,IF(0>V9,0,IF(50>V9,(( -0.000009*V9^2 + 0.0004*V9 + 0.7918)*Radiation!H8),IF(90>V9,((-0.0006*V9^2 + 0.0699*V9 - 1.2225)*Radiation!H8),0))))","v":0},{"$f":"IF(EI9<0,0,IF(0>W9,0,IF(50>W9,(( -0.000009*W9^2 + 0.0004*W9 + 0.7918)*Radiation!I8),IF(90>W9,((-0.0006*W9^2 + 0.0699*W9 - 1.2225)*Radiation!I8),0))))","v":0},{"$f":"IF(EJ9<0,0,IF(0>X9,0,IF(50>X9,(( -0.000009*X9^2 + 0.0004*X9 + 0.7918)*Radiation!J8),IF(90>X9,((-0.0006*X9^2 + 0.0699*X9 - 1.2225)*Radiation!J8),0))))","v":0},{"$f":"IF(EK9<0,0,IF(0>Y9,0,IF(50>Y9,(( -0.000009*Y9^2 + 0.0004*Y9 + 0.7918)*Radiation!K8),IF(90>Y9,((-0.0006*Y9^2 + 0.0699*Y9 - 1.2225)*Radiation!K8),0))))","v":0},{"$f":"IF(EL9<0,0,IF(0>Z9,0,IF(50>Z9,(( -0.000009*Z9^2 + 0.0004*Z9 + 0.7918)*Radiation!L8),IF(90>Z9,((-0.0006*Z9^2 + 0.0699*Z9 - 1.2225)*Radiation!L8),0))))","v":0},{"$f":"IF(EM9<0,0,IF(0>AA9,0,IF(50>AA9,(( -0.000009*AA9^2 + 0.0004*AA9 + 0.7918)*Radiation!M8),IF(90>AA9,((-0.0006*AA9^2 + 0.0699*AA9 - 1.2225)*Radiation!M8),0))))","v":0},{"$f":"IF(EN9<0,0,IF(0>AB9,0,IF(50>AB9,(( -0.000009*AB9^2 + 0.0004*AB9 + 0.7918)*Radiation!N8),IF(90>AB9,((-0.0006*AB9^2 + 0.0699*AB9 - 1.2225)*Radiation!N8),0))))","v":0},null,null,5,{"$f":"AG9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU9","v":0},{"$f":"AH9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV9","v":0},{"$f":"AI9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW9","v":0},{"$f":"AJ9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX9","v":0},{"$f":"AK9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY9","v":0},{"$f":"AL9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ9","v":0},{"$f":"AM9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA9","v":0},{"$f":"AN9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB9","v":0},{"$f":"AO9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC9","v":0},{"$f":"AP9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD9","v":0},{"$f":"AQ9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE9","v":0},{"$f":"AR9*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF9","v":0},null,5,{"$f":"AU9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI9","v":0},{"$f":"AV9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ9","v":0},{"$f":"AW9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK9","v":0},{"$f":"AX9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL9","v":0},{"$f":"AY9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM9","v":0},{"$f":"AZ9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN9","v":0},{"$f":"BA9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO9","v":0},{"$f":"BB9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP9","v":0},{"$f":"BC9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ9","v":0},{"$f":"BD9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR9","v":0},{"$f":"BE9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS9","v":0},{"$f":"BF9*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT9","v":0},null,5,0,0,0,0,0,0,0,0,0,0,0,0,null,5,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B8","v":5},{"$f":"'Solar Altitude'!C8","v":-25.376333918471747},{"$f":"'Solar Altitude'!D8","v":-22.7103856061896},{"$f":"'Solar Altitude'!E8","v":-16.897092448538263},{"$f":"'Solar Altitude'!F8","v":-9.5810693067706811},{"$f":"'Solar Altitude'!G8","v":-5.1231262317655331},{"$f":"'Solar Altitude'!H8","v":-4.54535827775074},{"$f":"'Solar Altitude'!I8","v":-6.9688312964780383},{"$f":"'Solar Altitude'!J8","v":-10.241982624949756},{"$f":"'Solar Altitude'!K8","v":-13.517063375335365},{"$f":"'Solar Altitude'!L8","v":-16.104385171900024},{"$f":"'Solar Altitude'!M8","v":-19.830528453312528},{"$f":"'Solar Altitude'!N8","v":-23.664530366970006},null,5,-25.376333918471747,-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006]
[null,6,{"$f":"DEGREES(C38)","v":73.868660509051566},82.560525935307453,91.527839613033848,101.42593517586506,108.76871394003487,112.07438399392458,109.93320445619683,101.97185210497935,89.961695531722469,79.427072964371703,71.296827350986064,69.372867490370865,null,6,{"$f":"DEGREES(Q38)","v":20.400123044346774},11.819209502025943,3.6583333333333772,11.99384260169014,20.321654647600202,23.541380287535347,20.757716132520656,12.329053937677804,9.1666666666745777E-2,10.895473299208135,19.966851705660439,23.488466210529037,null,null,null,6,{"$f":"IF(DO10<0,0,IF(0>C10,0,IF(50>C10,((-0.000009*C10^2 + 0.0004*C10 + 0.7918)*Radiation!C9),IF(90>C10,(( -0.0006*C10^2 + 0.0699*C10 - 1.2225)*Radiation!C9),0))))","v":0},{"$f":"IF(DP10<0,0,IF(0>D10,0,IF(50>D10,((-0.000009*D10^2 + 0.0004*D10 + 0.7918)*Radiation!D9),IF(90>D10,(( -0.0006*D10^2 + 0.0699*D10 - 1.2225)*Radiation!D9),0))))","v":0},{"$f":"IF(DQ10<0,0,IF(0>E10,0,IF(50>E10,((-0.000009*E10^2 + 0.0004*E10 + 0.7918)*Radiation!E9),IF(90>E10,(( -0.0006*E10^2 + 0.0699*E10 - 1.2225)*Radiation!E9),0))))","v":0},{"$f":"IF(DR10<0,0,IF(0>F10,0,IF(50>F10,((-0.000009*F10^2 + 0.0004*F10 + 0.7918)*Radiation!F9),IF(90>F10,(( -0.0006*F10^2 + 0.0699*F10 - 1.2225)*Radiation!F9),0))))","v":0},{"$f":"IF(DS10<0,0,IF(0>G10,0,IF(50>G10,((-0.000009*G10^2 + 0.0004*G10 + 0.7918)*Radiation!G9),IF(90>G10,(( -0.0006*G10^2 + 0.0699*G10 - 1.2225)*Radiation!G9),0))))","v":0},{"$f":"IF(DT10<0,0,IF(0>H10,0,IF(50>H10,((-0.000009*H10^2 + 0.0004*H10 + 0.7918)*Radiation!H9),IF(90>H10,(( -0.0006*H10^2 + 0.0699*H10 - 1.2225)*Radiation!H9),0))))","v":0},{"$f":"IF(DU10<0,0,IF(0>I10,0,IF(50>I10,((-0.000009*I10^2 + 0.0004*I10 + 0.7918)*Radiation!I9),IF(90>I10,(( -0.0006*I10^2 + 0.0699*I10 - 1.2225)*Radiation!I9),0))))","v":0},{"$f":"IF(DV10<0,0,IF(0>J10,0,IF(50>J10,((-0.000009*J10^2 + 0.0004*J10 + 0.7918)*Radiation!J9),IF(90>J10,(( -0.0006*J10^2 + 0.0699*J10 - 1.2225)*Radiation!J9),0))))","v":0},{"$f":"IF(DW10<0,0,IF(0>K10,0,IF(50>K10,((-0.000009*K10^2 + 0.0004*K10 + 0.7918)*Radiation!K9),IF(90>K10,(( -0.0006*K10^2 + 0.0699*K10 - 1.2225)*Radiation!K9),0))))","v":0.19966965711041554},{"$f":"IF(DX10<0,0,IF(0>L10,0,IF(50>L10,((-0.000009*L10^2 + 0.0004*L10 + 0.7918)*Radiation!L9),IF(90>L10,(( -0.0006*L10^2 + 0.0699*L10 - 1.2225)*Radiation!L9),0))))","v":0},{"$f":"IF(DY10<0,0,IF(0>M10,0,IF(50>M10,((-0.000009*M10^2 + 0.0004*M10 + 0.7918)*Radiation!M9),IF(90>M10,(( -0.0006*M10^2 + 0.0699*M10 - 1.2225)*Radiation!M9),0))))","v":0},{"$f":"IF(DZ10<0,0,IF(0>N10,0,IF(50>N10,((-0.000009*N10^2 + 0.0004*N10 + 0.7918)*Radiation!N9),IF(90>N10,(( -0.0006*N10^2 + 0.0699*N10 - 1.2225)*Radiation!N9),0))))","v":0},null,6,{"$f":"IF(EC10<0,0,IF(0>Q10,0,IF(50>Q10,(( -0.000009*Q10^2 + 0.0004*Q10 + 0.7918)*Radiation!C9),IF(90>Q10,((-0.0006*Q10^2 + 0.0699*Q10 - 1.2225)*Radiation!C9),0))))","v":0},{"$f":"IF(ED10<0,0,IF(0>R10,0,IF(50>R10,(( -0.000009*R10^2 + 0.0004*R10 + 0.7918)*Radiation!D9),IF(90>R10,((-0.0006*R10^2 + 0.0699*R10 - 1.2225)*Radiation!D9),0))))","v":0},{"$f":"IF(EE10<0,0,IF(0>S10,0,IF(50>S10,(( -0.000009*S10^2 + 0.0004*S10 + 0.7918)*Radiation!E9),IF(90>S10,((-0.0006*S10^2 + 0.0699*S10 - 1.2225)*Radiation!E9),0))))","v":0},{"$f":"IF(EF10<0,0,IF(0>T10,0,IF(50>T10,(( -0.000009*T10^2 + 0.0004*T10 + 0.7918)*Radiation!F9),IF(90>T10,((-0.0006*T10^2 + 0.0699*T10 - 1.2225)*Radiation!F9),0))))","v":1.5126592697122996},{"$f":"IF(EG10<0,0,IF(0>U10,0,IF(50>U10,(( -0.000009*U10^2 + 0.0004*U10 + 0.7918)*Radiation!G9),IF(90>U10,((-0.0006*U10^2 + 0.0699*U10 - 1.2225)*Radiation!G9),0))))","v":4.0383688264764732},{"$f":"IF(EH10<0,0,IF(0>V10,0,IF(50>V10,(( -0.000009*V10^2 + 0.0004*V10 + 0.7918)*Radiation!H9),IF(90>V10,((-0.0006*V10^2 + 0.0699*V10 - 1.2225)*Radiation!H9),0))))","v":5.048067847744333},{"$f":"IF(EI10<0,0,IF(0>W10,0,IF(50>W10,(( -0.000009*W10^2 + 0.0004*W10 + 0.7918)*Radiation!I9),IF(90>W10,((-0.0006*W10^2 + 0.0699*W10 - 1.2225)*Radiation!I9),0))))","v":3.028826856820185},{"$f":"IF(EJ10<0,0,IF(0>X10,0,IF(50>X10,(( -0.000009*X10^2 + 0.0004*X10 + 0.7918)*Radiation!J9),IF(90>X10,((-0.0006*X10^2 + 0.0699*X10 - 1.2225)*Radiation!J9),0))))","v":1.5127747296073932},{"$f":"IF(EK10<0,0,IF(0>Y10,0,IF(50>Y10,(( -0.000009*Y10^2 + 0.0004*Y10 + 0.7918)*Radiation!K9),IF(90>Y10,((-0.0006*Y10^2 + 0.0699*Y10 - 1.2225)*Radiation!K9),0))))","v":0.75303322148854135},{"$f":"IF(EL10<0,0,IF(0>Z10,0,IF(50>Z10,(( -0.000009*Z10^2 + 0.0004*Z10 + 0.7918)*Radiation!L9),IF(90>Z10,((-0.0006*Z10^2 + 0.0699*Z10 - 1.2225)*Radiation!L9),0))))","v":0},{"$f":"IF(EM10<0,0,IF(0>AA10,0,IF(50>AA10,(( -0.000009*AA10^2 + 0.0004*AA10 + 0.7918)*Radiation!M9),IF(90>AA10,((-0.0006*AA10^2 + 0.0699*AA10 - 1.2225)*Radiation!M9),0))))","v":0},{"$f":"IF(EN10<0,0,IF(0>AB10,0,IF(50>AB10,(( -0.000009*AB10^2 + 0.0004*AB10 + 0.7918)*Radiation!N9),IF(90>AB10,((-0.0006*AB10^2 + 0.0699*AB10 - 1.2225)*Radiation!N9),0))))","v":0},null,null,6,{"$f":"AG10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU10","v":0},{"$f":"AH10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV10","v":0},{"$f":"AI10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW10","v":0},{"$f":"AJ10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX10","v":0},{"$f":"AK10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY10","v":0},{"$f":"AL10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ10","v":0},{"$f":"AM10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA10","v":0},{"$f":"AN10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB10","v":0},{"$f":"AO10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC10","v":0},{"$f":"AP10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD10","v":0},{"$f":"AQ10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE10","v":0},{"$f":"AR10*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF10","v":0},null,6,{"$f":"AU10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI10","v":0},{"$f":"AV10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ10","v":0},{"$f":"AW10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK10","v":0},{"$f":"AX10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL10","v":85.291254678098866},{"$f":"AY10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM10","v":200.04067612922577},{"$f":"AZ10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN10","v":238.69148403224921},{"$f":"BA10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO10","v":151.55996159633474},{"$f":"BB10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP10","v":85.484580900045813},{"$f":"BC10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ10","v":49.076156240520959},{"$f":"BD10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR10","v":0},{"$f":"BE10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS10","v":0},{"$f":"BF10*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT10","v":0},null,6,0,0,0,0,0,0,0,0,0,0,0,0,null,6,0,0,0,1,1,1,1,1,1,0,0,0,null,null,{"$f":"'Solar Altitude'!B9","v":6},{"$f":"'Solar Altitude'!C9","v":-12.151444093159176},{"$f":"'Solar Altitude'!D9","v":-9.1319080559186769},{"$f":"'Solar Altitude'!E9","v":-3.3232309033445411},{"$f":"'Solar Altitude'!F9","v":3.5985816694690373},{"$f":"'Solar Altitude'!G9","v":7.5112987220277185},{"$f":"'Solar Altitude'!H9","v":7.7738597839019823},{"$f":"'Solar Altitude'!I9","v":5.5584053941199079},{"$f":"'Solar Altitude'!J9","v":2.9033723023449274},{"$f":"'Solar Altitude'!K9","v":8.3279910069695443E-2},{"$f":"'Solar Altitude'!L9","v":-2.6015900354108483},{"$f":"'Solar Altitude'!M9","v":-6.7413522567651629},{"$f":"'Solar Altitude'!N9","v":-10.743396255327719},null,6,-12.151444093159176,-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719]
[null,7,{"$f":"DEGREES(C39)","v":67.649048034613585},76.312839690849742,85.286265589431679,95.275414492062694,102.71520302049352,106.03193354336621,103.82855429080293,95.807958143509993,83.753994157338383,73.190847998989256,65.043691426582853,63.141365289312155,null,7,{"$f":"DEGREES(Q39)","v":22.363115013737691},14.358718721607596,11.341666666666669,17.916487823059342,24.513383283898659,26.572066445658269,23.462461777687516,17.412902231087408,15.091666666666665,20.058590682931534,25.738401798789798,26.922256182529942,null,null,null,7,{"$f":"IF(DO11<0,0,IF(0>C11,0,IF(50>C11,((-0.000009*C11^2 + 0.0004*C11 + 0.7918)*Radiation!C10),IF(90>C11,(( -0.0006*C11^2 + 0.0699*C11 - 1.2225)*Radiation!C10),0))))","v":1.2051211928877039},{"$f":"IF(DP11<0,0,IF(0>D11,0,IF(50>D11,((-0.000009*D11^2 + 0.0004*D11 + 0.7918)*Radiation!D10),IF(90>D11,(( -0.0006*D11^2 + 0.0699*D11 - 1.2225)*Radiation!D10),0))))","v":2.3492553919901336},{"$f":"IF(DQ11<0,0,IF(0>E11,0,IF(50>E11,((-0.000009*E11^2 + 0.0004*E11 + 0.7918)*Radiation!E10),IF(90>E11,(( -0.0006*E11^2 + 0.0699*E11 - 1.2225)*Radiation!E10),0))))","v":4.0391635534065422},{"$f":"IF(DR11<0,0,IF(0>F11,0,IF(50>F11,((-0.000009*F11^2 + 0.0004*F11 + 0.7918)*Radiation!F10),IF(90>F11,(( -0.0006*F11^2 + 0.0699*F11 - 1.2225)*Radiation!F10),0))))","v":0},{"$f":"IF(DS11<0,0,IF(0>G11,0,IF(50>G11,((-0.000009*G11^2 + 0.0004*G11 + 0.7918)*Radiation!G10),IF(90>G11,(( -0.0006*G11^2 + 0.0699*G11 - 1.2225)*Radiation!G10),0))))","v":0},{"$f":"IF(DT11<0,0,IF(0>H11,0,IF(50>H11,((-0.000009*H11^2 + 0.0004*H11 + 0.7918)*Radiation!H10),IF(90>H11,(( -0.0006*H11^2 + 0.0699*H11 - 1.2225)*Radiation!H10),0))))","v":0},{"$f":"IF(DU11<0,0,IF(0>I11,0,IF(50>I11,((-0.000009*I11^2 + 0.0004*I11 + 0.7918)*Radiation!I10),IF(90>I11,(( -0.0006*I11^2 + 0.0699*I11 - 1.2225)*Radiation!I10),0))))","v":0},{"$f":"IF(DV11<0,0,IF(0>J11,0,IF(50>J11,((-0.000009*J11^2 + 0.0004*J11 + 0.7918)*Radiation!J10),IF(90>J11,(( -0.0006*J11^2 + 0.0699*J11 - 1.2225)*Radiation!J10),0))))","v":0},{"$f":"IF(DW11<0,0,IF(0>K11,0,IF(50>K11,((-0.000009*K11^2 + 0.0004*K11 + 0.7918)*Radiation!K10),IF(90>K11,(( -0.0006*K11^2 + 0.0699*K11 - 1.2225)*Radiation!K10),0))))","v":12.472331275895991},{"$f":"IF(DX11<0,0,IF(0>L11,0,IF(50>L11,((-0.000009*L11^2 + 0.0004*L11 + 0.7918)*Radiation!L10),IF(90>L11,(( -0.0006*L11^2 + 0.0699*L11 - 1.2225)*Radiation!L10),0))))","v":13.783608166669842},{"$f":"IF(DY11<0,0,IF(0>M11,0,IF(50>M11,((-0.000009*M11^2 + 0.0004*M11 + 0.7918)*Radiation!M10),IF(90>M11,(( -0.0006*M11^2 + 0.0699*M11 - 1.2225)*Radiation!M10),0))))","v":4.9809666742728052},{"$f":"IF(DZ11<0,0,IF(0>N11,0,IF(50>N11,((-0.000009*N11^2 + 0.0004*N11 + 0.7918)*Radiation!N10),IF(90>N11,(( -0.0006*N11^2 + 0.0699*N11 - 1.2225)*Radiation!N10),0))))","v":2.0262098430938309},null,7,{"$f":"IF(EC11<0,0,IF(0>Q11,0,IF(50>Q11,(( -0.000009*Q11^2 + 0.0004*Q11 + 0.7918)*Radiation!C10),IF(90>Q11,((-0.0006*Q11^2 + 0.0699*Q11 - 1.2225)*Radiation!C10),0))))","v":1.2620415022938749},{"$f":"IF(ED11<0,0,IF(0>R11,0,IF(50>R11,(( -0.000009*R11^2 + 0.0004*R11 + 0.7918)*Radiation!D10),IF(90>R11,((-0.0006*R11^2 + 0.0699*R11 - 1.2225)*Radiation!D10),0))))","v":3.0267833222514029},{"$f":"IF(EE11<0,0,IF(0>S11,0,IF(50>S11,(( -0.000009*S11^2 + 0.0004*S11 + 0.7918)*Radiation!E10),IF(90>S11,((-0.0006*S11^2 + 0.0699*S11 - 1.2225)*Radiation!E10),0))))","v":8.5704004664224751},{"$f":"IF(EF11<0,0,IF(0>T11,0,IF(50>T11,(( -0.000009*T11^2 + 0.0004*T11 + 0.7918)*Radiation!F10),IF(90>T11,((-0.0006*T11^2 + 0.0699*T11 - 1.2225)*Radiation!F10),0))))","v":28.263812031624404},{"$f":"IF(EG11<0,0,IF(0>U11,0,IF(50>U11,(( -0.000009*U11^2 + 0.0004*U11 + 0.7918)*Radiation!G10),IF(90>U11,((-0.0006*U11^2 + 0.0699*U11 - 1.2225)*Radiation!G10),0))))","v":41.392514413071673},{"$f":"IF(EH11<0,0,IF(0>V11,0,IF(50>V11,(( -0.000009*V11^2 + 0.0004*V11 + 0.7918)*Radiation!H10),IF(90>V11,((-0.0006*V11^2 + 0.0699*V11 - 1.2225)*Radiation!H10),0))))","v":46.685559432132216},{"$f":"IF(EI11<0,0,IF(0>W11,0,IF(50>W11,(( -0.000009*W11^2 + 0.0004*W11 + 0.7918)*Radiation!I10),IF(90>W11,((-0.0006*W11^2 + 0.0699*W11 - 1.2225)*Radiation!I10),0))))","v":36.346171484814676},{"$f":"IF(EJ11<0,0,IF(0>X11,0,IF(50>X11,(( -0.000009*X11^2 + 0.0004*X11 + 0.7918)*Radiation!J10),IF(90>X11,((-0.0006*X11^2 + 0.0699*X11 - 1.2225)*Radiation!J10),0))))","v":28.76703003835414},{"$f":"IF(EK11<0,0,IF(0>Y11,0,IF(50>Y11,(( -0.000009*Y11^2 + 0.0004*Y11 + 0.7918)*Radiation!K10),IF(90>Y11,((-0.0006*Y11^2 + 0.0699*Y11 - 1.2225)*Radiation!K10),0))))","v":23.460486664203877},{"$f":"IF(EL11<0,0,IF(0>Z11,0,IF(50>Z11,(( -0.000009*Z11^2 + 0.0004*Z11 + 0.7918)*Radiation!L10),IF(90>Z11,((-0.0006*Z11^2 + 0.0699*Z11 - 1.2225)*Radiation!L10),0))))","v":16.153280089579351},{"$f":"IF(EM11<0,0,IF(0>AA11,0,IF(50>AA11,(( -0.000009*AA11^2 + 0.0004*AA11 + 0.7918)*Radiation!M10),IF(90>AA11,((-0.0006*AA11^2 + 0.0699*AA11 - 1.2225)*Radiation!M10),0))))","v":5.0474616826355589},{"$f":"IF(EN11<0,0,IF(0>AB11,0,IF(50>AB11,(( -0.000009*AB11^2 + 0.0004*AB11 + 0.7918)*Radiation!N10),IF(90>AB11,((-0.0006*AB11^2 + 0.0699*AB11 - 1.2225)*Radiation!N10),0))))","v":2.01876266955705},null,null,7,{"$f":"AG11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU11","v":0},{"$f":"AH11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV11","v":0},{"$f":"AI11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW11","v":0},{"$f":"AJ11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX11","v":0},{"$f":"AK11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY11","v":0},{"$f":"AL11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ11","v":0},{"$f":"AM11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA11","v":0},{"$f":"AN11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB11","v":0},{"$f":"AO11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC11","v":0},{"$f":"AP11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD11","v":0},{"$f":"AQ11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE11","v":0},{"$f":"AR11*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF11","v":1.519164678131067},null,7,{"$f":"AU11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI11","v":64.898513253972396},{"$f":"AV11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ11","v":165.40677030899579},{"$f":"AW11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK11","v":477.20353172430015},{"$f":"AX11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL11","v":1430.2072767776865},{"$f":"AY11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM11","v":1823.5313692542443},{"$f":"AZ11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN11","v":1967.8167757820027},{"$f":"BA11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO11","v":1633.0294584747032},{"$f":"BB11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP11","v":1462.7309965171892},{"$f":"BC11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ11","v":1232.2064066489952},{"$f":"BD11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR11","v":786.71694263200231},{"$f":"BE11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS11","v":234.94895166423882},{"$f":"BF11*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT11","v":96.370565382288561},null,7,0,0,0,0,0,0,0,0,0,0,0,1.5519142582101374E-2,null,7,1,1,1,1,1,1,1,1,1,1,1,0.9844808574178987,null,null,{"$f":"'Solar Altitude'!B10","v":7},{"$f":"'Solar Altitude'!C10","v":0.70023973357815916},{"$f":"'Solar Altitude'!D10","v":4.2572512510716702},{"$f":"'Solar Altitude'!E10","v":10.292097151668541},{"$f":"'Solar Altitude'!F10","v":17.071764306110264},{"$f":"'Solar Altitude'!G10","v":20.59199880999245},{"$f":"'Solar Altitude'!H10","v":20.602944398333847},{"$f":"'Solar Altitude'!I10","v":18.567526961418682},{"$f":"'Solar Altitude'!J10","v":16.357318748220177},{"$f":"'Solar Altitude'!K10","v":13.682588857300253},{"$f":"'Solar Altitude'!L10","v":10.626902061270702},{"$f":"'Solar Altitude'!M10","v":5.8987575020687171},{"$f":"'Solar Altitude'!N10","v":1.7151458456731048},null,7,0.70023973357815916,4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048]
[null,8,{"$f":"DEGREES(C40)","v":61.453222639747757},70.182467614205279,79.314540713478877,89.55804976800853,97.177377926252248,100.50688821263151,98.19278334216709,90.05957506979675,77.90623012154407,67.252525369320495,58.968515794713213,56.965348514634712,null,8,{"$f":"DEGREES(Q40)","v":31.866762607805029},26.784740200575246,26.341666666666665,30.683603452863519,34.918683399762614,35.803997711168762,33.171053544895116,29.958974794295194,30.091666666666686,33.623263740320041,36.841727364302294,36.356841900499546,null,null,null,8,{"$f":"IF(DO12<0,0,IF(0>C12,0,IF(50>C12,((-0.000009*C12^2 + 0.0004*C12 + 0.7918)*Radiation!C11),IF(90>C12,(( -0.0006*C12^2 + 0.0699*C12 - 1.2225)*Radiation!C11),0))))","v":28.658029940747507},{"$f":"IF(DP12<0,0,IF(0>D12,0,IF(50>D12,((-0.000009*D12^2 + 0.0004*D12 + 0.7918)*Radiation!D11),IF(90>D12,(( -0.0006*D12^2 + 0.0699*D12 - 1.2225)*Radiation!D11),0))))","v":34.150342472082272},{"$f":"IF(DQ12<0,0,IF(0>E12,0,IF(50>E12,((-0.000009*E12^2 + 0.0004*E12 + 0.7918)*Radiation!E11),IF(90>E12,(( -0.0006*E12^2 + 0.0699*E12 - 1.2225)*Radiation!E11),0))))","v":36.594287148818601},{"$f":"IF(DR12<0,0,IF(0>F12,0,IF(50>F12,((-0.000009*F12^2 + 0.0004*F12 + 0.7918)*Radiation!F11),IF(90>F12,(( -0.0006*F12^2 + 0.0699*F12 - 1.2225)*Radiation!F11),0))))","v":23.346090548041335},{"$f":"IF(DS12<0,0,IF(0>G12,0,IF(50>G12,((-0.000009*G12^2 + 0.0004*G12 + 0.7918)*Radiation!G11),IF(90>G12,(( -0.0006*G12^2 + 0.0699*G12 - 1.2225)*Radiation!G11),0))))","v":0},{"$f":"IF(DT12<0,0,IF(0>H12,0,IF(50>H12,((-0.000009*H12^2 + 0.0004*H12 + 0.7918)*Radiation!H11),IF(90>H12,(( -0.0006*H12^2 + 0.0699*H12 - 1.2225)*Radiation!H11),0))))","v":0},{"$f":"IF(DU12<0,0,IF(0>I12,0,IF(50>I12,((-0.000009*I12^2 + 0.0004*I12 + 0.7918)*Radiation!I11),IF(90>I12,(( -0.0006*I12^2 + 0.0699*I12 - 1.2225)*Radiation!I11),0))))","v":0},{"$f":"IF(DV12<0,0,IF(0>J12,0,IF(50>J12,((-0.000009*J12^2 + 0.0004*J12 + 0.7918)*Radiation!J11),IF(90>J12,(( -0.0006*J12^2 + 0.0699*J12 - 1.2225)*Radiation!J11),0))))","v":0},{"$f":"IF(DW12<0,0,IF(0>K12,0,IF(50>K12,((-0.000009*K12^2 + 0.0004*K12 + 0.7918)*Radiation!K11),IF(90>K12,(( -0.0006*K12^2 + 0.0699*K12 - 1.2225)*Radiation!K11),0))))","v":60.463547798789783},{"$f":"IF(DX12<0,0,IF(0>L12,0,IF(50>L12,((-0.000009*L12^2 + 0.0004*L12 + 0.7918)*Radiation!L11),IF(90>L12,(( -0.0006*L12^2 + 0.0699*L12 - 1.2225)*Radiation!L11),0))))","v":69.572259342964671},{"$f":"IF(DY12<0,0,IF(0>M12,0,IF(50>M12,((-0.000009*M12^2 + 0.0004*M12 + 0.7918)*Radiation!M11),IF(90>M12,(( -0.0006*M12^2 + 0.0699*M12 - 1.2225)*Radiation!M11),0))))","v":46.906612162384235},{"$f":"IF(DZ12<0,0,IF(0>N12,0,IF(50>N12,((-0.000009*N12^2 + 0.0004*N12 + 0.7918)*Radiation!N11),IF(90>N12,(( -0.0006*N12^2 + 0.0699*N12 - 1.2225)*Radiation!N11),0))))","v":28.583936357287616},null,8,{"$f":"IF(EC12<0,0,IF(0>Q12,0,IF(50>Q12,(( -0.000009*Q12^2 + 0.0004*Q12 + 0.7918)*Radiation!C11),IF(90>Q12,((-0.0006*Q12^2 + 0.0699*Q12 - 1.2225)*Radiation!C11),0))))","v":28.240013796668933},{"$f":"IF(ED12<0,0,IF(0>R12,0,IF(50>R12,(( -0.000009*R12^2 + 0.0004*R12 + 0.7918)*Radiation!D11),IF(90>R12,((-0.0006*R12^2 + 0.0699*R12 - 1.2225)*Radiation!D11),0))))","v":37.347647217234993},{"$f":"IF(EE12<0,0,IF(0>S12,0,IF(50>S12,(( -0.000009*S12^2 + 0.0004*S12 + 0.7918)*Radiation!E11),IF(90>S12,((-0.0006*S12^2 + 0.0699*S12 - 1.2225)*Radiation!E11),0))))","v":53.247947847708829},{"$f":"IF(EF12<0,0,IF(0>T12,0,IF(50>T12,(( -0.000009*T12^2 + 0.0004*T12 + 0.7918)*Radiation!F11),IF(90>T12,((-0.0006*T12^2 + 0.0699*T12 - 1.2225)*Radiation!F11),0))))","v":82.470739899710608},{"$f":"IF(EG12<0,0,IF(0>U12,0,IF(50>U12,(( -0.000009*U12^2 + 0.0004*U12 + 0.7918)*Radiation!G11),IF(90>U12,((-0.0006*U12^2 + 0.0699*U12 - 1.2225)*Radiation!G11),0))))","v":96.244309884212896},{"$f":"IF(EH12<0,0,IF(0>V12,0,IF(50>V12,(( -0.000009*V12^2 + 0.0004*V12 + 0.7918)*Radiation!H11),IF(90>V12,((-0.0006*V12^2 + 0.0699*V12 - 1.2225)*Radiation!H11),0))))","v":106.29423855177606},{"$f":"IF(EI12<0,0,IF(0>W12,0,IF(50>W12,(( -0.000009*W12^2 + 0.0004*W12 + 0.7918)*Radiation!I11),IF(90>W12,((-0.0006*W12^2 + 0.0699*W12 - 1.2225)*Radiation!I11),0))))","v":94.524881178648798},{"$f":"IF(EJ12<0,0,IF(0>X12,0,IF(50>X12,(( -0.000009*X12^2 + 0.0004*X12 + 0.7918)*Radiation!J11),IF(90>X12,((-0.0006*X12^2 + 0.0699*X12 - 1.2225)*Radiation!J11),0))))","v":86.769729194069811},{"$f":"IF(EK12<0,0,IF(0>Y12,0,IF(50>Y12,(( -0.000009*Y12^2 + 0.0004*Y12 + 0.7918)*Radiation!K11),IF(90>Y12,((-0.0006*Y12^2 + 0.0699*Y12 - 1.2225)*Radiation!K11),0))))","v":82.731990008880899},{"$f":"IF(EL12<0,0,IF(0>Z12,0,IF(50>Z12,(( -0.000009*Z12^2 + 0.0004*Z12 + 0.7918)*Radiation!L11),IF(90>Z12,((-0.0006*Z12^2 + 0.0699*Z12 - 1.2225)*Radiation!L11),0))))","v":72.334766840433886},{"$f":"IF(EM12<0,0,IF(0>AA12,0,IF(50>AA12,(( -0.000009*AA12^2 + 0.0004*AA12 + 0.7918)*Radiation!M11),IF(90>AA12,((-0.0006*AA12^2 + 0.0699*AA12 - 1.2225)*Radiation!M11),0))))","v":45.827343076967956},{"$f":"IF(EN12<0,0,IF(0>AB12,0,IF(50>AB12,(( -0.000009*AB12^2 + 0.0004*AB12 + 0.7918)*Radiation!N11),IF(90>AB12,((-0.0006*AB12^2 + 0.0699*AB12 - 1.2225)*Radiation!N11),0))))","v":27.95405862454307},null,null,8,{"$f":"AG12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU12","v":127.30130569019155},{"$f":"AH12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV12","v":0},{"$f":"AI12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW12","v":0},{"$f":"AJ12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX12","v":0},{"$f":"AK12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY12","v":0},{"$f":"AL12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ12","v":0},{"$f":"AM12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA12","v":0},{"$f":"AN12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB12","v":0},{"$f":"AO12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC12","v":0},{"$f":"AP12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD12","v":0},{"$f":"AQ12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE12","v":364.2388710559141},{"$f":"AR12*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF12","v":311.04236889499981},null,8,{"$f":"AU12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI12","v":1114.2916837321102},{"$f":"AV12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ12","v":1580.2679856218936},{"$f":"AW12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK12","v":2274.2562020804671},{"$f":"AX12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL12","v":3450.0632210657404},{"$f":"AY12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM12","v":3430.0891695915338},{"$f":"AZ12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN12","v":3624.4253921251366},{"$f":"BA12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO12","v":3506.0504040840974},{"$f":"BB12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP12","v":3701.4693967750522},{"$f":"BC12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ12","v":3245.9243592338794},{"$f":"BD12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR12","v":2588.9845220993402},{"$f":"BE12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS12","v":1561.7415122729005},{"$f":"BF12*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT12","v":997.28150482434762},null,8,0.10253062539393309,0,0,0,0,0,0,0,0,0,0.18911868168998328,0.23774110917257671,null,8,0.89746937460606691,1,1,1,1,1,1,1,1,1,0.81088131831001664,0.76225889082742337,null,null,{"$f":"'Solar Altitude'!B11","v":8},{"$f":"'Solar Altitude'!C11","v":12.968359542715392},{"$f":"'Solar Altitude'!D11","v":17.270303982095768},{"$f":"'Solar Altitude'!E11","v":23.773745192987032},{"$f":"'Solar Altitude'!F11","v":30.67971943621767},{"$f":"'Solar Altitude'!G11","v":33.959814353189685},{"$f":"'Solar Altitude'!H11","v":33.770494749028082},{"$f":"'Solar Altitude'!I11","v":31.887744015481577},{"$f":"'Solar Altitude'!J11","v":29.958903207045175},{"$f":"'Solar Altitude'!K11","v":27.097900221004789},{"$f":"'Solar Altitude'!L11","v":23.350930400204959},{"$f":"'Solar Altitude'!M11","v":17.832347455280527},{"$f":"'Solar Altitude'!N11","v":13.467847656409182},null,8,12.968359542715392,17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182]
[null,9,{"$f":"DEGREES(C41)","v":55.66844310193531},64.550449494020668,73.977120459924436,84.601762309780682,92.449760000438687,95.782108081289778,93.322851696666291,85.054530114355757,72.785548204204289,62.011118374738004,53.484947987297886,51.245180956281459,null,9,{"$f":"DEGREES(Q41)","v":44.283968367372353},40.903521848191559,41.341666666666676,44.774579106628146,47.608962417547808,47.747144287511269,45.595647887719679,43.982590510226871,45.091666666666676,47.986654037396633,49.814463007257963,48.380798902239178,null,null,null,9,{"$f":"IF(DO13<0,0,IF(0>C13,0,IF(50>C13,((-0.000009*C13^2 + 0.0004*C13 + 0.7918)*Radiation!C12),IF(90>C13,(( -0.0006*C13^2 + 0.0699*C13 - 1.2225)*Radiation!C12),0))))","v":76.454659885484119},{"$f":"IF(DP13<0,0,IF(0>D13,0,IF(50>D13,((-0.000009*D13^2 + 0.0004*D13 + 0.7918)*Radiation!D12),IF(90>D13,(( -0.0006*D13^2 + 0.0699*D13 - 1.2225)*Radiation!D12),0))))","v":84.843818250734117},{"$f":"IF(DQ13<0,0,IF(0>E13,0,IF(50>E13,((-0.000009*E13^2 + 0.0004*E13 + 0.7918)*Radiation!E12),IF(90>E13,(( -0.0006*E13^2 + 0.0699*E13 - 1.2225)*Radiation!E12),0))))","v":88.10709899356533},{"$f":"IF(DR13<0,0,IF(0>F13,0,IF(50>F13,((-0.000009*F13^2 + 0.0004*F13 + 0.7918)*Radiation!F12),IF(90>F13,(( -0.0006*F13^2 + 0.0699*F13 - 1.2225)*Radiation!F12),0))))","v":67.401795766259411},{"$f":"IF(DS13<0,0,IF(0>G13,0,IF(50>G13,((-0.000009*G13^2 + 0.0004*G13 + 0.7918)*Radiation!G12),IF(90>G13,(( -0.0006*G13^2 + 0.0699*G13 - 1.2225)*Radiation!G12),0))))","v":0},{"$f":"IF(DT13<0,0,IF(0>H13,0,IF(50>H13,((-0.000009*H13^2 + 0.0004*H13 + 0.7918)*Radiation!H12),IF(90>H13,(( -0.0006*H13^2 + 0.0699*H13 - 1.2225)*Radiation!H12),0))))","v":0},{"$f":"IF(DU13<0,0,IF(0>I13,0,IF(50>I13,((-0.000009*I13^2 + 0.0004*I13 + 0.7918)*Radiation!I12),IF(90>I13,(( -0.0006*I13^2 + 0.0699*I13 - 1.2225)*Radiation!I12),0))))","v":0},{"$f":"IF(DV13<0,0,IF(0>J13,0,IF(50>J13,((-0.000009*J13^2 + 0.0004*J13 + 0.7918)*Radiation!J12),IF(90>J13,(( -0.0006*J13^2 + 0.0699*J13 - 1.2225)*Radiation!J12),0))))","v":70.764453265019213},{"$f":"IF(DW13<0,0,IF(0>K13,0,IF(50>K13,((-0.000009*K13^2 + 0.0004*K13 + 0.7918)*Radiation!K12),IF(90>K13,(( -0.0006*K13^2 + 0.0699*K13 - 1.2225)*Radiation!K12),0))))","v":124.49073463339323},{"$f":"IF(DX13<0,0,IF(0>L13,0,IF(50>L13,((-0.000009*L13^2 + 0.0004*L13 + 0.7918)*Radiation!L12),IF(90>L13,(( -0.0006*L13^2 + 0.0699*L13 - 1.2225)*Radiation!L12),0))))","v":132.67086149106868},{"$f":"IF(DY13<0,0,IF(0>M13,0,IF(50>M13,((-0.000009*M13^2 + 0.0004*M13 + 0.7918)*Radiation!M12),IF(90>M13,(( -0.0006*M13^2 + 0.0699*M13 - 1.2225)*Radiation!M12),0))))","v":99.628731520341105},{"$f":"IF(DZ13<0,0,IF(0>N13,0,IF(50>N13,((-0.000009*N13^2 + 0.0004*N13 + 0.7918)*Radiation!N12),IF(90>N13,(( -0.0006*N13^2 + 0.0699*N13 - 1.2225)*Radiation!N12),0))))","v":63.366030355468233},null,9,{"$f":"IF(EC13<0,0,IF(0>Q13,0,IF(50>Q13,(( -0.000009*Q13^2 + 0.0004*Q13 + 0.7918)*Radiation!C12),IF(90>Q13,((-0.0006*Q13^2 + 0.0699*Q13 - 1.2225)*Radiation!C12),0))))","v":74.803885298817647},{"$f":"IF(ED13<0,0,IF(0>R13,0,IF(50>R13,(( -0.000009*R13^2 + 0.0004*R13 + 0.7918)*Radiation!D12),IF(90>R13,((-0.0006*R13^2 + 0.0699*R13 - 1.2225)*Radiation!D12),0))))","v":85.228902032275599},{"$f":"IF(EE13<0,0,IF(0>S13,0,IF(50>S13,(( -0.000009*S13^2 + 0.0004*S13 + 0.7918)*Radiation!E12),IF(90>S13,((-0.0006*S13^2 + 0.0699*S13 - 1.2225)*Radiation!E12),0))))","v":105.07075334129834},{"$f":"IF(EF13<0,0,IF(0>T13,0,IF(50>T13,(( -0.000009*T13^2 + 0.0004*T13 + 0.7918)*Radiation!F12),IF(90>T13,((-0.0006*T13^2 + 0.0699*T13 - 1.2225)*Radiation!F12),0))))","v":134.51311424180341},{"$f":"IF(EG13<0,0,IF(0>U13,0,IF(50>U13,(( -0.000009*U13^2 + 0.0004*U13 + 0.7918)*Radiation!G12),IF(90>U13,((-0.0006*U13^2 + 0.0699*U13 - 1.2225)*Radiation!G12),0))))","v":147.33495133717443},{"$f":"IF(EH13<0,0,IF(0>V13,0,IF(50>V13,(( -0.000009*V13^2 + 0.0004*V13 + 0.7918)*Radiation!H12),IF(90>V13,((-0.0006*V13^2 + 0.0699*V13 - 1.2225)*Radiation!H12),0))))","v":163.10777278484099},{"$f":"IF(EI13<0,0,IF(0>W13,0,IF(50>W13,(( -0.000009*W13^2 + 0.0004*W13 + 0.7918)*Radiation!I12),IF(90>W13,((-0.0006*W13^2 + 0.0699*W13 - 1.2225)*Radiation!I12),0))))","v":152.7674804560402},{"$f":"IF(EJ13<0,0,IF(0>X13,0,IF(50>X13,(( -0.000009*X13^2 + 0.0004*X13 + 0.7918)*Radiation!J12),IF(90>X13,((-0.0006*X13^2 + 0.0699*X13 - 1.2225)*Radiation!J12),0))))","v":146.61753840142941},{"$f":"IF(EK13<0,0,IF(0>Y13,0,IF(50>Y13,(( -0.000009*Y13^2 + 0.0004*Y13 + 0.7918)*Radiation!K12),IF(90>Y13,((-0.0006*Y13^2 + 0.0699*Y13 - 1.2225)*Radiation!K12),0))))","v":143.52407326678741},{"$f":"IF(EL13<0,0,IF(0>Z13,0,IF(50>Z13,(( -0.000009*Z13^2 + 0.0004*Z13 + 0.7918)*Radiation!L12),IF(90>Z13,((-0.0006*Z13^2 + 0.0699*Z13 - 1.2225)*Radiation!L12),0))))","v":130.26755415367236},{"$f":"IF(EM13<0,0,IF(0>AA13,0,IF(50>AA13,(( -0.000009*AA13^2 + 0.0004*AA13 + 0.7918)*Radiation!M12),IF(90>AA13,((-0.0006*AA13^2 + 0.0699*AA13 - 1.2225)*Radiation!M12),0))))","v":98.342860926658076},{"$f":"IF(EN13<0,0,IF(0>AB13,0,IF(50>AB13,(( -0.000009*AB13^2 + 0.0004*AB13 + 0.7918)*Radiation!N12),IF(90>AB13,((-0.0006*AB13^2 + 0.0699*AB13 - 1.2225)*Radiation!N12),0))))","v":63.866315776863026},null,null,9,{"$f":"AG13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU13","v":811.47757221825918},{"$f":"AH13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV13","v":118.60410379936748},{"$f":"AI13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW13","v":0},{"$f":"AJ13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX13","v":0},{"$f":"AK13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY13","v":0},{"$f":"AL13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ13","v":0},{"$f":"AM13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA13","v":0},{"$f":"AN13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB13","v":0},{"$f":"AO13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC13","v":0},{"$f":"AP13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD13","v":318.42639417912727},{"$f":"AQ13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE13","v":1182.1451144318978},{"$f":"AR13*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF13","v":959.6028110723438},null,9,{"$f":"AU13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI13","v":1937.7499286029749},{"$f":"AV13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ13","v":2419.2010350237315},{"$f":"AW13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK13","v":2912.014825963},{"$f":"AX13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL13","v":3360.4158657250155},{"$f":"AY13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM13","v":3200.4903267677082},{"$f":"AZ13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN13","v":3403.2308082119139},{"$f":"BA13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO13","v":3720.9239883772384},{"$f":"BB13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP13","v":3826.0863600764724},{"$f":"BC13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ13","v":3354.2128592006602},{"$f":"BD13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR13","v":2669.6329341940491},{"$f":"BE13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS13","v":1917.4960014801416},{"$f":"BF13*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT13","v":1389.9804404707747},null,9,0.29516566816527884,4.6734913561712568E-2,0,0,0,0,0,0,0,0.10656628908117825,0.38138128584091358,0.40841404978611101,null,9,0.70483433183472122,0.95326508643828756,1,1,1,1,1,1,1,0.89343371091882173,0.61861871415908642,0.59158595021388904,null,null,{"$f":"'Solar Altitude'!B12","v":9},{"$f":"'Solar Altitude'!C12","v":24.306538235547787},{"$f":"'Solar Altitude'!D12","v":29.607456719563572},{"$f":"'Solar Altitude'!E12","v":36.877998514340362},{"$f":"'Solar Altitude'!F12","v":44.267398869292073},{"$f":"'Solar Altitude'!G12","v":47.503865138538167},{"$f":"'Solar Altitude'!H12","v":47.16345799134892},{"$f":"'Solar Altitude'!I12","v":45.403126432581416},{"$f":"'Solar Altitude'!J12","v":43.556385601632783},{"$f":"'Solar Altitude'!K12","v":40.048756889246128},{"$f":"'Solar Altitude'!L12","v":35.170537312656599},{"$f":"'Solar Altitude'!M12","v":28.628753160625717},{"$f":"'Solar Altitude'!N12","v":24.120985503613159},null,9,24.306538235547787,29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159]
[null,10,{"$f":"DEGREES(C42)","v":50.748508450174889},59.83372278752379,69.646286446366432,80.719732227983556,88.803132996838229,92.115278065266637,89.493075184303351,81.106292527820685,68.763568929500451,57.896973750363728,49.074107135865901,46.464001605242331,null,10,{"$f":"DEGREES(Q42)","v":57.743424902720641},55.429966762771883,56.341666666666683,59.243479873249626,61.153562517113578,60.793335174423419,59.021941915541937,58.420422229010185,60.091666666666704,62.593599483994453,63.49594861892195,61.461417100099787,null,null,null,10,{"$f":"IF(DO14<0,0,IF(0>C14,0,IF(50>C14,((-0.000009*C14^2 + 0.0004*C14 + 0.7918)*Radiation!C13),IF(90>C14,(( -0.0006*C14^2 + 0.0699*C14 - 1.2225)*Radiation!C13),0))))","v":115.6539728376268},{"$f":"IF(DP14<0,0,IF(0>D14,0,IF(50>D14,((-0.000009*D14^2 + 0.0004*D14 + 0.7918)*Radiation!D13),IF(90>D14,(( -0.0006*D14^2 + 0.0699*D14 - 1.2225)*Radiation!D13),0))))","v":133.3071850641862},{"$f":"IF(DQ14<0,0,IF(0>E14,0,IF(50>E14,((-0.000009*E14^2 + 0.0004*E14 + 0.7918)*Radiation!E13),IF(90>E14,(( -0.0006*E14^2 + 0.0699*E14 - 1.2225)*Radiation!E13),0))))","v":140.57416491299557},{"$f":"IF(DR14<0,0,IF(0>F14,0,IF(50>F14,((-0.000009*F14^2 + 0.0004*F14 + 0.7918)*Radiation!F13),IF(90>F14,(( -0.0006*F14^2 + 0.0699*F14 - 1.2225)*Radiation!F13),0))))","v":115.3615459245006},{"$f":"IF(DS14<0,0,IF(0>G14,0,IF(50>G14,((-0.000009*G14^2 + 0.0004*G14 + 0.7918)*Radiation!G13),IF(90>G14,(( -0.0006*G14^2 + 0.0699*G14 - 1.2225)*Radiation!G13),0))))","v":62.134460636770051},{"$f":"IF(DT14<0,0,IF(0>H14,0,IF(50>H14,((-0.000009*H14^2 + 0.0004*H14 + 0.7918)*Radiation!H13),IF(90>H14,(( -0.0006*H14^2 + 0.0699*H14 - 1.2225)*Radiation!H13),0))))","v":0},{"$f":"IF(DU14<0,0,IF(0>I14,0,IF(50>I14,((-0.000009*I14^2 + 0.0004*I14 + 0.7918)*Radiation!I13),IF(90>I14,(( -0.0006*I14^2 + 0.0699*I14 - 1.2225)*Radiation!I13),0))))","v":58.961081183583978},{"$f":"IF(DV14<0,0,IF(0>J14,0,IF(50>J14,((-0.000009*J14^2 + 0.0004*J14 + 0.7918)*Radiation!J13),IF(90>J14,(( -0.0006*J14^2 + 0.0699*J14 - 1.2225)*Radiation!J13),0))))","v":125.0287858869717},{"$f":"IF(DW14<0,0,IF(0>K14,0,IF(50>K14,((-0.000009*K14^2 + 0.0004*K14 + 0.7918)*Radiation!K13),IF(90>K14,(( -0.0006*K14^2 + 0.0699*K14 - 1.2225)*Radiation!K13),0))))","v":183.52243632135037},{"$f":"IF(DX14<0,0,IF(0>L14,0,IF(50>L14,((-0.000009*L14^2 + 0.0004*L14 + 0.7918)*Radiation!L13),IF(90>L14,(( -0.0006*L14^2 + 0.0699*L14 - 1.2225)*Radiation!L13),0))))","v":182.78241729615141},{"$f":"IF(DY14<0,0,IF(0>M14,0,IF(50>M14,((-0.000009*M14^2 + 0.0004*M14 + 0.7918)*Radiation!M13),IF(90>M14,(( -0.0006*M14^2 + 0.0699*M14 - 1.2225)*Radiation!M13),0))))","v":144.45269181068656},{"$f":"IF(DZ14<0,0,IF(0>N14,0,IF(50>N14,((-0.000009*N14^2 + 0.0004*N14 + 0.7918)*Radiation!N13),IF(90>N14,(( -0.0006*N14^2 + 0.0699*N14 - 1.2225)*Radiation!N13),0))))","v":101.04489911727516},null,10,{"$f":"IF(EC14<0,0,IF(0>Q14,0,IF(50>Q14,(( -0.000009*Q14^2 + 0.0004*Q14 + 0.7918)*Radiation!C13),IF(90>Q14,((-0.0006*Q14^2 + 0.0699*Q14 - 1.2225)*Radiation!C13),0))))","v":120.64011467984207},{"$f":"IF(ED14<0,0,IF(0>R14,0,IF(50>R14,(( -0.000009*R14^2 + 0.0004*R14 + 0.7918)*Radiation!D13),IF(90>R14,((-0.0006*R14^2 + 0.0699*R14 - 1.2225)*Radiation!D13),0))))","v":132.77078463658518},{"$f":"IF(EE14<0,0,IF(0>S14,0,IF(50>S14,(( -0.000009*S14^2 + 0.0004*S14 + 0.7918)*Radiation!E13),IF(90>S14,((-0.0006*S14^2 + 0.0699*S14 - 1.2225)*Radiation!E13),0))))","v":155.05190831194699},{"$f":"IF(EF14<0,0,IF(0>T14,0,IF(50>T14,(( -0.000009*T14^2 + 0.0004*T14 + 0.7918)*Radiation!F13),IF(90>T14,((-0.0006*T14^2 + 0.0699*T14 - 1.2225)*Radiation!F13),0))))","v":183.69668145125894},{"$f":"IF(EG14<0,0,IF(0>U14,0,IF(50>U14,(( -0.000009*U14^2 + 0.0004*U14 + 0.7918)*Radiation!G13),IF(90>U14,((-0.0006*U14^2 + 0.0699*U14 - 1.2225)*Radiation!G13),0))))","v":198.31685289777261},{"$f":"IF(EH14<0,0,IF(0>V14,0,IF(50>V14,(( -0.000009*V14^2 + 0.0004*V14 + 0.7918)*Radiation!H13),IF(90>V14,((-0.0006*V14^2 + 0.0699*V14 - 1.2225)*Radiation!H13),0))))","v":215.79767162932151},{"$f":"IF(EI14<0,0,IF(0>W14,0,IF(50>W14,(( -0.000009*W14^2 + 0.0004*W14 + 0.7918)*Radiation!I13),IF(90>W14,((-0.0006*W14^2 + 0.0699*W14 - 1.2225)*Radiation!I13),0))))","v":210.55192363058165},{"$f":"IF(EJ14<0,0,IF(0>X14,0,IF(50>X14,(( -0.000009*X14^2 + 0.0004*X14 + 0.7918)*Radiation!J13),IF(90>X14,((-0.0006*X14^2 + 0.0699*X14 - 1.2225)*Radiation!J13),0))))","v":203.42101147049743},{"$f":"IF(EK14<0,0,IF(0>Y14,0,IF(50>Y14,(( -0.000009*Y14^2 + 0.0004*Y14 + 0.7918)*Radiation!K13),IF(90>Y14,((-0.0006*Y14^2 + 0.0699*Y14 - 1.2225)*Radiation!K13),0))))","v":199.31583772117622},{"$f":"IF(EL14<0,0,IF(0>Z14,0,IF(50>Z14,(( -0.000009*Z14^2 + 0.0004*Z14 + 0.7918)*Radiation!L13),IF(90>Z14,((-0.0006*Z14^2 + 0.0699*Z14 - 1.2225)*Radiation!L13),0))))","v":180.25500531986901},{"$f":"IF(EM14<0,0,IF(0>AA14,0,IF(50>AA14,(( -0.000009*AA14^2 + 0.0004*AA14 + 0.7918)*Radiation!M13),IF(90>AA14,((-0.0006*AA14^2 + 0.0699*AA14 - 1.2225)*Radiation!M13),0))))","v":145.74590439034509},{"$f":"IF(EN14<0,0,IF(0>AB14,0,IF(50>AB14,(( -0.000009*AB14^2 + 0.0004*AB14 + 0.7918)*Radiation!N13),IF(90>AB14,((-0.0006*AB14^2 + 0.0699*AB14 - 1.2225)*Radiation!N13),0))))","v":103.11370364998336},null,null,10,{"$f":"AG14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU14","v":1506.6043106011446},{"$f":"AH14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV14","v":314.83189335756248},{"$f":"AI14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW14","v":0},{"$f":"AJ14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX14","v":0},{"$f":"AK14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY14","v":0},{"$f":"AL14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ14","v":0},{"$f":"AM14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA14","v":0},{"$f":"AN14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB14","v":0},{"$f":"AO14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC14","v":0},{"$f":"AP14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD14","v":389.84762999128924},{"$f":"AQ14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE14","v":1971.8064351296152},{"$f":"AR14*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF14","v":1748.1686302643286},null,10,{"$f":"AU14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI14","v":1183.6493446461352},{"$f":"AV14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ14","v":1497.4376845479851},{"$f":"AW14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK14","v":1259.1168271411946},{"$f":"AX14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL14","v":97.570769643937751},{"$f":"AY14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM14","v":0},{"$f":"AZ14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN14","v":0},{"$f":"BA14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO14","v":8.4277910379317671},{"$f":"BB14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP14","v":454.16199224679519},{"$f":"BC14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ14","v":433.5569407707585},{"$f":"BD14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR14","v":363.21272236663583},{"$f":"BE14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS14","v":456.08173339111073},{"$f":"BF14*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT14","v":591.97429448104697},null,10,0.56002314416060595,0.17372244019094327,0,0,0,0,0,0,0,0.51768444424225513,0.81214878868617979,0.74703498311093197,null,10,0.439976855839394,0.82627755980905682,1,1,0,0,1,1,1,0.48231555575774493,0.18785121131382015,0.25296501688906803,null,null,{"$f":"'Solar Altitude'!B13","v":10},{"$f":"'Solar Altitude'!C13","v":34.130498638110296},{"$f":"'Solar Altitude'!D13","v":40.716949463115029},{"$f":"'Solar Altitude'!E13","v":49.130640449349286},{"$f":"'Solar Altitude'!F13","v":57.573642107854539},{"$f":"'Solar Altitude'!G13","v":61.123995517612983},{"$f":"'Solar Altitude'!H13","v":60.701791836412639},{"$f":"'Solar Altitude'!I13","v":59.016860616830343},{"$f":"'Solar Altitude'!J13","v":56.905164678924855},{"$f":"'Solar Altitude'!K13","v":51.954064465377563},{"$f":"'Solar Altitude'!L13","v":45.326184070335216},{"$f":"'Solar Altitude'!M13","v":37.566870997040184},{"$f":"'Solar Altitude'!N13","v":33.04159126014769},null,10,34.130498638110296,40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,37.566870997040184,33.04159126014769]
[null,11,{"$f":"DEGREES(C43)","v":47.201284429179303},56.464752113501987,66.677552060174634,78.188440183669442,86.467457396769547,89.724847489139563,86.940582305560554,78.493323336461458,66.183979517129771,55.328905491358782,46.246120441073181,43.169882706520688,null,11,{"$f":"DEGREES(Q43)","v":71.629318930407436},70.102116697385554,71.341666666666683,73.856260987432108,75.056789518420786,74.31996681307163,72.864928393304083,73.014741414299039,75.091666666666654,77.29533586259403,77.476186623630454,75.00313399944207,null,null,null,11,{"$f":"IF(DO15<0,0,IF(0>C15,0,IF(50>C15,((-0.000009*C15^2 + 0.0004*C15 + 0.7918)*Radiation!C14),IF(90>C15,(( -0.0006*C15^2 + 0.0699*C15 - 1.2225)*Radiation!C14),0))))","v":147.62002487859368},{"$f":"IF(DP15<0,0,IF(0>D15,0,IF(50>D15,((-0.000009*D15^2 + 0.0004*D15 + 0.7918)*Radiation!D14),IF(90>D15,(( -0.0006*D15^2 + 0.0699*D15 - 1.2225)*Radiation!D14),0))))","v":166.93619912456876},{"$f":"IF(DQ15<0,0,IF(0>E15,0,IF(50>E15,((-0.000009*E15^2 + 0.0004*E15 + 0.7918)*Radiation!E14),IF(90>E15,(( -0.0006*E15^2 + 0.0699*E15 - 1.2225)*Radiation!E14),0))))","v":176.39773812224922},{"$f":"IF(DR15<0,0,IF(0>F15,0,IF(50>F15,((-0.000009*F15^2 + 0.0004*F15 + 0.7918)*Radiation!F14),IF(90>F15,(( -0.0006*F15^2 + 0.0699*F15 - 1.2225)*Radiation!F14),0))))","v":150.69163691194723},{"$f":"IF(DS15<0,0,IF(0>G15,0,IF(50>G15,((-0.000009*G15^2 + 0.0004*G15 + 0.7918)*Radiation!G14),IF(90>G15,(( -0.0006*G15^2 + 0.0699*G15 - 1.2225)*Radiation!G14),0))))","v":96.172522844314187},{"$f":"IF(DT15<0,0,IF(0>H15,0,IF(50>H15,((-0.000009*H15^2 + 0.0004*H15 + 0.7918)*Radiation!H14),IF(90>H15,(( -0.0006*H15^2 + 0.0699*H15 - 1.2225)*Radiation!H14),0))))","v":67.598520485047956},{"$f":"IF(DU15<0,0,IF(0>I15,0,IF(50>I15,((-0.000009*I15^2 + 0.0004*I15 + 0.7918)*Radiation!I14),IF(90>I15,(( -0.0006*I15^2 + 0.0699*I15 - 1.2225)*Radiation!I14),0))))","v":97.618974194591217},{"$f":"IF(DV15<0,0,IF(0>J15,0,IF(50>J15,((-0.000009*J15^2 + 0.0004*J15 + 0.7918)*Radiation!J14),IF(90>J15,(( -0.0006*J15^2 + 0.0699*J15 - 1.2225)*Radiation!J14),0))))","v":168.37209410791075},{"$f":"IF(DW15<0,0,IF(0>K15,0,IF(50>K15,((-0.000009*K15^2 + 0.0004*K15 + 0.7918)*Radiation!K14),IF(90>K15,(( -0.0006*K15^2 + 0.0699*K15 - 1.2225)*Radiation!K14),0))))","v":224.46485684547838},{"$f":"IF(DX15<0,0,IF(0>L15,0,IF(50>L15,((-0.000009*L15^2 + 0.0004*L15 + 0.7918)*Radiation!L14),IF(90>L15,(( -0.0006*L15^2 + 0.0699*L15 - 1.2225)*Radiation!L14),0))))","v":213.93025769547253},{"$f":"IF(DY15<0,0,IF(0>M15,0,IF(50>M15,((-0.000009*M15^2 + 0.0004*M15 + 0.7918)*Radiation!M14),IF(90>M15,(( -0.0006*M15^2 + 0.0699*M15 - 1.2225)*Radiation!M14),0))))","v":176.03475701456045},{"$f":"IF(DZ15<0,0,IF(0>N15,0,IF(50>N15,((-0.000009*N15^2 + 0.0004*N15 + 0.7918)*Radiation!N14),IF(90>N15,(( -0.0006*N15^2 + 0.0699*N15 - 1.2225)*Radiation!N14),0))))","v":127.83863484450123},null,11,{"$f":"IF(EC15<0,0,IF(0>Q15,0,IF(50>Q15,(( -0.000009*Q15^2 + 0.0004*Q15 + 0.7918)*Radiation!C14),IF(90>Q15,((-0.0006*Q15^2 + 0.0699*Q15 - 1.2225)*Radiation!C14),0))))","v":131.80642564272131},{"$f":"IF(ED15<0,0,IF(0>R15,0,IF(50>R15,(( -0.000009*R15^2 + 0.0004*R15 + 0.7918)*Radiation!D14),IF(90>R15,((-0.0006*R15^2 + 0.0699*R15 - 1.2225)*Radiation!D14),0))))","v":149.98977301913047},{"$f":"IF(EE15<0,0,IF(0>S15,0,IF(50>S15,(( -0.000009*S15^2 + 0.0004*S15 + 0.7918)*Radiation!E14),IF(90>S15,((-0.0006*S15^2 + 0.0699*S15 - 1.2225)*Radiation!E14),0))))","v":162.61481048569104},{"$f":"IF(EF15<0,0,IF(0>T15,0,IF(50>T15,(( -0.000009*T15^2 + 0.0004*T15 + 0.7918)*Radiation!F14),IF(90>T15,((-0.0006*T15^2 + 0.0699*T15 - 1.2225)*Radiation!F14),0))))","v":174.91282012040077},{"$f":"IF(EG15<0,0,IF(0>U15,0,IF(50>U15,(( -0.000009*U15^2 + 0.0004*U15 + 0.7918)*Radiation!G14),IF(90>U15,((-0.0006*U15^2 + 0.0699*U15 - 1.2225)*Radiation!G14),0))))","v":184.50786957114738},{"$f":"IF(EH15<0,0,IF(0>V15,0,IF(50>V15,(( -0.000009*V15^2 + 0.0004*V15 + 0.7918)*Radiation!H14),IF(90>V15,((-0.0006*V15^2 + 0.0699*V15 - 1.2225)*Radiation!H14),0))))","v":203.28263860525661},{"$f":"IF(EI15<0,0,IF(0>W15,0,IF(50>W15,(( -0.000009*W15^2 + 0.0004*W15 + 0.7918)*Radiation!I14),IF(90>W15,((-0.0006*W15^2 + 0.0699*W15 - 1.2225)*Radiation!I14),0))))","v":209.38179222388706},{"$f":"IF(EJ15<0,0,IF(0>X15,0,IF(50>X15,(( -0.000009*X15^2 + 0.0004*X15 + 0.7918)*Radiation!J14),IF(90>X15,((-0.0006*X15^2 + 0.0699*X15 - 1.2225)*Radiation!J14),0))))","v":202.51658783604833},{"$f":"IF(EK15<0,0,IF(0>Y15,0,IF(50>Y15,(( -0.000009*Y15^2 + 0.0004*Y15 + 0.7918)*Radiation!K14),IF(90>Y15,((-0.0006*Y15^2 + 0.0699*Y15 - 1.2225)*Radiation!K14),0))))","v":186.14099298927496},{"$f":"IF(EL15<0,0,IF(0>Z15,0,IF(50>Z15,(( -0.000009*Z15^2 + 0.0004*Z15 + 0.7918)*Radiation!L14),IF(90>Z15,((-0.0006*Z15^2 + 0.0699*Z15 - 1.2225)*Radiation!L14),0))))","v":157.67879509343589},{"$f":"IF(EM15<0,0,IF(0>AA15,0,IF(50>AA15,(( -0.000009*AA15^2 + 0.0004*AA15 + 0.7918)*Radiation!M14),IF(90>AA15,((-0.0006*AA15^2 + 0.0699*AA15 - 1.2225)*Radiation!M14),0))))","v":131.63934151863276},{"$f":"IF(EN15<0,0,IF(0>AB15,0,IF(50>AB15,(( -0.000009*AB15^2 + 0.0004*AB15 + 0.7918)*Radiation!N14),IF(90>AB15,((-0.0006*AB15^2 + 0.0699*AB15 - 1.2225)*Radiation!N14),0))))","v":104.06205326383902},null,null,11,{"$f":"AG15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU15","v":2137.1317305137704},{"$f":"AH15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV15","v":246.19203113518182},{"$f":"AI15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW15","v":0},{"$f":"AJ15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX15","v":0},{"$f":"AK15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY15","v":0},{"$f":"AL15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ15","v":0},{"$f":"AM15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA15","v":0},{"$f":"AN15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB15","v":0},{"$f":"AO15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC15","v":0},{"$f":"AP15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD15","v":254.59312019607125},{"$f":"AQ15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE15","v":2668.0021945218805},{"$f":"AR15*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF15","v":2449.42891745922},null,11,{"$f":"AU15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI15","v":0},{"$f":"AV15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ15","v":0},{"$f":"AW15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK15","v":0},{"$f":"AX15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL15","v":0},{"$f":"AY15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM15","v":0},{"$f":"AZ15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN15","v":0},{"$f":"BA15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO15","v":0},{"$f":"BB15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP15","v":0},{"$f":"BC15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ15","v":0},{"$f":"BD15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR15","v":0},{"$f":"BE15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS15","v":0},{"$f":"BF15*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT15","v":0},null,11,1,1,0,0,0,0,0,0,0,1,1,1,null,11,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B14","v":11},{"$f":"'Solar Altitude'!C14","v":41.499338482119107},{"$f":"'Solar Altitude'!D14","v":49.543356395157261},{"$f":"'Solar Altitude'!E14","v":59.402009530792824},{"$f":"'Solar Altitude'!F14","v":69.801829865076741},{"$f":"'Solar Altitude'!G14","v":74.625870049112294},{"$f":"'Solar Altitude'!H14","v":74.317427946135254},{"$f":"'Solar Altitude'!I14","v":72.577202871970812},{"$f":"'Solar Altitude'!J14","v":69.283885987295108},{"$f":"'Solar Altitude'!K14","v":61.393251168859464},{"$f":"'Solar Altitude'!L14","v":52.417946997507137},{"$f":"'Solar Altitude'!M14","v":43.550952586854685},{"$f":"'Solar Altitude'!N14","v":39.297011346471983},null,11,41.499338482119107,49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983]
[null,12,{"$f":"DEGREES(C44)","v":45.501019385071835},54.821258873968112,65.353688610771755,77.208324182904803,85.603150220435197,88.765227102715201,85.838042185897848,77.42074936054216,65.300033727131805,54.618770916281782,45.413374190147707,41.859593897633104,null,12,{"$f":"DEGREES(Q44)","v":85.690879792171273},84.831644602709204,86.341666666666811,88.524089531337211,89.101194815804078,88.042935221045823,86.877975633580263,87.669646168258964,89.908333333335293,87.96928207449848,88.432878734944666,88.730938878386141,null,null,null,12,{"$f":"IF(DO16<0,0,IF(0>C16,0,IF(50>C16,((-0.000009*C16^2 + 0.0004*C16 + 0.7918)*Radiation!C15),IF(90>C16,(( -0.0006*C16^2 + 0.0699*C16 - 1.2225)*Radiation!C15),0))))","v":162.30791876617258},{"$f":"IF(DP16<0,0,IF(0>D16,0,IF(50>D16,((-0.000009*D16^2 + 0.0004*D16 + 0.7918)*Radiation!D15),IF(90>D16,(( -0.0006*D16^2 + 0.0699*D16 - 1.2225)*Radiation!D15),0))))","v":183.2586033819974},{"$f":"IF(DQ16<0,0,IF(0>E16,0,IF(50>E16,((-0.000009*E16^2 + 0.0004*E16 + 0.7918)*Radiation!E15),IF(90>E16,(( -0.0006*E16^2 + 0.0699*E16 - 1.2225)*Radiation!E15),0))))","v":199.57605771729038},{"$f":"IF(DR16<0,0,IF(0>F16,0,IF(50>F16,((-0.000009*F16^2 + 0.0004*F16 + 0.7918)*Radiation!F15),IF(90>F16,(( -0.0006*F16^2 + 0.0699*F16 - 1.2225)*Radiation!F15),0))))","v":163.50900587013135},{"$f":"IF(DS16<0,0,IF(0>G16,0,IF(50>G16,((-0.000009*G16^2 + 0.0004*G16 + 0.7918)*Radiation!G15),IF(90>G16,(( -0.0006*G16^2 + 0.0699*G16 - 1.2225)*Radiation!G15),0))))","v":111.2465433177949},{"$f":"IF(DT16<0,0,IF(0>H16,0,IF(50>H16,((-0.000009*H16^2 + 0.0004*H16 + 0.7918)*Radiation!H15),IF(90>H16,(( -0.0006*H16^2 + 0.0699*H16 - 1.2225)*Radiation!H15),0))))","v":83.946058115414729},{"$f":"IF(DU16<0,0,IF(0>I16,0,IF(50>I16,((-0.000009*I16^2 + 0.0004*I16 + 0.7918)*Radiation!I15),IF(90>I16,(( -0.0006*I16^2 + 0.0699*I16 - 1.2225)*Radiation!I15),0))))","v":117.02356552523561},{"$f":"IF(DV16<0,0,IF(0>J16,0,IF(50>J16,((-0.000009*J16^2 + 0.0004*J16 + 0.7918)*Radiation!J15),IF(90>J16,(( -0.0006*J16^2 + 0.0699*J16 - 1.2225)*Radiation!J15),0))))","v":189.99246962612807},{"$f":"IF(DW16<0,0,IF(0>K16,0,IF(50>K16,((-0.000009*K16^2 + 0.0004*K16 + 0.7918)*Radiation!K15),IF(90>K16,(( -0.0006*K16^2 + 0.0699*K16 - 1.2225)*Radiation!K15),0))))","v":241.91566028242801},{"$f":"IF(DX16<0,0,IF(0>L16,0,IF(50>L16,((-0.000009*L16^2 + 0.0004*L16 + 0.7918)*Radiation!L15),IF(90>L16,(( -0.0006*L16^2 + 0.0699*L16 - 1.2225)*Radiation!L15),0))))","v":226.97850103589707},{"$f":"IF(DY16<0,0,IF(0>M16,0,IF(50>M16,((-0.000009*M16^2 + 0.0004*M16 + 0.7918)*Radiation!M15),IF(90>M16,(( -0.0006*M16^2 + 0.0699*M16 - 1.2225)*Radiation!M15),0))))","v":188.65720011652797},{"$f":"IF(DZ16<0,0,IF(0>N16,0,IF(50>N16,((-0.000009*N16^2 + 0.0004*N16 + 0.7918)*Radiation!N15),IF(90>N16,(( -0.0006*N16^2 + 0.0699*N16 - 1.2225)*Radiation!N15),0))))","v":140.22995886162528},null,12,{"$f":"IF(EC16<0,0,IF(0>Q16,0,IF(50>Q16,(( -0.000009*Q16^2 + 0.0004*Q16 + 0.7918)*Radiation!C15),IF(90>Q16,((-0.0006*Q16^2 + 0.0699*Q16 - 1.2225)*Radiation!C15),0))))","v":74.150415407503871},{"$f":"IF(ED16<0,0,IF(0>R16,0,IF(50>R16,(( -0.000009*R16^2 + 0.0004*R16 + 0.7918)*Radiation!D15),IF(90>R16,((-0.0006*R16^2 + 0.0699*R16 - 1.2225)*Radiation!D15),0))))","v":88.503030938186953},{"$f":"IF(EE16<0,0,IF(0>S16,0,IF(50>S16,(( -0.000009*S16^2 + 0.0004*S16 + 0.7918)*Radiation!E15),IF(90>S16,((-0.0006*S16^2 + 0.0699*S16 - 1.2225)*Radiation!E15),0))))","v":86.617127960318797},{"$f":"IF(EF16<0,0,IF(0>T16,0,IF(50>T16,(( -0.000009*T16^2 + 0.0004*T16 + 0.7918)*Radiation!F15),IF(90>T16,((-0.0006*T16^2 + 0.0699*T16 - 1.2225)*Radiation!F15),0))))","v":72.065172750217215},{"$f":"IF(EG16<0,0,IF(0>U16,0,IF(50>U16,(( -0.000009*U16^2 + 0.0004*U16 + 0.7918)*Radiation!G15),IF(90>U16,((-0.0006*U16^2 + 0.0699*U16 - 1.2225)*Radiation!G15),0))))","v":73.954549739572059},{"$f":"IF(EH16<0,0,IF(0>V16,0,IF(50>V16,(( -0.000009*V16^2 + 0.0004*V16 + 0.7918)*Radiation!H15),IF(90>V16,((-0.0006*V16^2 + 0.0699*V16 - 1.2225)*Radiation!H15),0))))","v":92.562554957584368},{"$f":"IF(EI16<0,0,IF(0>W16,0,IF(50>W16,(( -0.000009*W16^2 + 0.0004*W16 + 0.7918)*Radiation!I15),IF(90>W16,((-0.0006*W16^2 + 0.0699*W16 - 1.2225)*Radiation!I15),0))))","v":105.51517634636079},{"$f":"IF(EJ16<0,0,IF(0>X16,0,IF(50>X16,(( -0.000009*X16^2 + 0.0004*X16 + 0.7918)*Radiation!J15),IF(90>X16,((-0.0006*X16^2 + 0.0699*X16 - 1.2225)*Radiation!J15),0))))","v":94.231777687863612},{"$f":"IF(EK16<0,0,IF(0>Y16,0,IF(50>Y16,(( -0.000009*Y16^2 + 0.0004*Y16 + 0.7918)*Radiation!K15),IF(90>Y16,((-0.0006*Y16^2 + 0.0699*Y16 - 1.2225)*Radiation!K15),0))))","v":65.452530171687158},{"$f":"IF(EL16<0,0,IF(0>Z16,0,IF(50>Z16,(( -0.000009*Z16^2 + 0.0004*Z16 + 0.7918)*Radiation!L15),IF(90>Z16,((-0.0006*Z16^2 + 0.0699*Z16 - 1.2225)*Radiation!L15),0))))","v":79.864336812933772},{"$f":"IF(EM16<0,0,IF(0>AA16,0,IF(50>AA16,(( -0.000009*AA16^2 + 0.0004*AA16 + 0.7918)*Radiation!M15),IF(90>AA16,((-0.0006*AA16^2 + 0.0699*AA16 - 1.2225)*Radiation!M15),0))))","v":63.58478477088817},{"$f":"IF(EN16<0,0,IF(0>AB16,0,IF(50>AB16,(( -0.000009*AB16^2 + 0.0004*AB16 + 0.7918)*Radiation!N15),IF(90>AB16,((-0.0006*AB16^2 + 0.0699*AB16 - 1.2225)*Radiation!N15),0))))","v":45.262256836581749},null,null,12,{"$f":"AG16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU16","v":2660.7704140368955},{"$f":"AH16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV16","v":129.99219692738231},{"$f":"AI16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW16","v":0},{"$f":"AJ16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX16","v":0},{"$f":"AK16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY16","v":0},{"$f":"AL16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ16","v":0},{"$f":"AM16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA16","v":0},{"$f":"AN16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB16","v":0},{"$f":"AO16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC16","v":0},{"$f":"AP16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD16","v":199.34268060830314},{"$f":"AQ16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE16","v":3190.3469256777284},{"$f":"AR16*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF16","v":3062.0963422731697},null,12,{"$f":"AU16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI16","v":0},{"$f":"AV16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ16","v":0},{"$f":"AW16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK16","v":0},{"$f":"AX16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL16","v":0},{"$f":"AY16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM16","v":0},{"$f":"AZ16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN16","v":0},{"$f":"BA16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO16","v":0},{"$f":"BB16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP16","v":0},{"$f":"BC16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ16","v":0},{"$f":"BD16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR16","v":0},{"$f":"BE16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS16","v":0},{"$f":"BF16*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT16","v":0},null,12,1,1,0,0,0,0,0,0,0,1,1,1,null,12,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B15","v":12},{"$f":"'Solar Altitude'!C15","v":45.177523796213436},{"$f":"'Solar Altitude'!D15","v":54.329068465075267},{"$f":"'Solar Altitude'!E15","v":65.047371814417531},{"$f":"'Solar Altitude'!F15","v":77.120581963762746},{"$f":"'Solar Altitude'!G15","v":85.511869047796154},{"$f":"'Solar Altitude'!H15","v":87.685706703910299},{"$f":"'Solar Altitude'!I15","v":84.793912346691229},{"$f":"'Solar Altitude'!J15","v":77.199736149013034},{"$f":"'Solar Altitude'!K15","v":65.299840573859427},{"$f":"'Solar Altitude'!L15","v":54.542607240756659},{"$f":"'Solar Altitude'!M15","v":45.370517861678998},{"$f":"'Solar Altitude'!N15","v":41.831318434437598},null,12,45.177523796213436,54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598]
[null,13,{"$f":"DEGREES(C45)","v":45.918779643114902},55.114724298725349,65.813574371954715,77.862129073667887,86.272659389691,89.301592790838612,86.264418009743196,77.978584119532357,66.205651119278428,55.861181201924744,46.713529364890427,42.767179671443238,null,13,{"$f":"DEGREES(Q45)","v":99.788343906405061},99.573849854580416,101.34166666666665,103.19641763488615,103.15332003417913,101.78800300109876,100.91844645725392,102.33190223993921,105.09166666666668,106.76107447056987,105.64508751288498,102.47306074123237,null,null,null,13,{"$f":"IF(DO17<0,0,IF(0>C17,0,IF(50>C17,((-0.000009*C17^2 + 0.0004*C17 + 0.7918)*Radiation!C16),IF(90>C17,(( -0.0006*C17^2 + 0.0699*C17 - 1.2225)*Radiation!C16),0))))","v":164.27814498410373},{"$f":"IF(DP17<0,0,IF(0>D17,0,IF(50>D17,((-0.000009*D17^2 + 0.0004*D17 + 0.7918)*Radiation!D16),IF(90>D17,(( -0.0006*D17^2 + 0.0699*D17 - 1.2225)*Radiation!D16),0))))","v":192.22384412726569},{"$f":"IF(DQ17<0,0,IF(0>E17,0,IF(50>E17,((-0.000009*E17^2 + 0.0004*E17 + 0.7918)*Radiation!E16),IF(90>E17,(( -0.0006*E17^2 + 0.0699*E17 - 1.2225)*Radiation!E16),0))))","v":207.18768039347401},{"$f":"IF(DR17<0,0,IF(0>F17,0,IF(50>F17,((-0.000009*F17^2 + 0.0004*F17 + 0.7918)*Radiation!F16),IF(90>F17,(( -0.0006*F17^2 + 0.0699*F17 - 1.2225)*Radiation!F16),0))))","v":157.15371644296221},{"$f":"IF(DS17<0,0,IF(0>G17,0,IF(50>G17,((-0.000009*G17^2 + 0.0004*G17 + 0.7918)*Radiation!G16),IF(90>G17,(( -0.0006*G17^2 + 0.0699*G17 - 1.2225)*Radiation!G16),0))))","v":103.69660660973207},{"$f":"IF(DT17<0,0,IF(0>H17,0,IF(50>H17,((-0.000009*H17^2 + 0.0004*H17 + 0.7918)*Radiation!H16),IF(90>H17,(( -0.0006*H17^2 + 0.0699*H17 - 1.2225)*Radiation!H16),0))))","v":76.892950595880322},{"$f":"IF(DU17<0,0,IF(0>I17,0,IF(50>I17,((-0.000009*I17^2 + 0.0004*I17 + 0.7918)*Radiation!I16),IF(90>I17,(( -0.0006*I17^2 + 0.0699*I17 - 1.2225)*Radiation!I16),0))))","v":111.59669066576113},{"$f":"IF(DV17<0,0,IF(0>J17,0,IF(50>J17,((-0.000009*J17^2 + 0.0004*J17 + 0.7918)*Radiation!J16),IF(90>J17,(( -0.0006*J17^2 + 0.0699*J17 - 1.2225)*Radiation!J16),0))))","v":184.90087249052854},{"$f":"IF(DW17<0,0,IF(0>K17,0,IF(50>K17,((-0.000009*K17^2 + 0.0004*K17 + 0.7918)*Radiation!K16),IF(90>K17,(( -0.0006*K17^2 + 0.0699*K17 - 1.2225)*Radiation!K16),0))))","v":234.97397216285816},{"$f":"IF(DX17<0,0,IF(0>L17,0,IF(50>L17,((-0.000009*L17^2 + 0.0004*L17 + 0.7918)*Radiation!L16),IF(90>L17,(( -0.0006*L17^2 + 0.0699*L17 - 1.2225)*Radiation!L16),0))))","v":221.31114583469616},{"$f":"IF(DY17<0,0,IF(0>M17,0,IF(50>M17,((-0.000009*M17^2 + 0.0004*M17 + 0.7918)*Radiation!M16),IF(90>M17,(( -0.0006*M17^2 + 0.0699*M17 - 1.2225)*Radiation!M16),0))))","v":181.5046761720543},{"$f":"IF(DZ17<0,0,IF(0>N17,0,IF(50>N17,((-0.000009*N17^2 + 0.0004*N17 + 0.7918)*Radiation!N16),IF(90>N17,(( -0.0006*N17^2 + 0.0699*N17 - 1.2225)*Radiation!N16),0))))","v":143.43755518568184},null,13,{"$f":"IF(EC17<0,0,IF(0>Q17,0,IF(50>Q17,(( -0.000009*Q17^2 + 0.0004*Q17 + 0.7918)*Radiation!C16),IF(90>Q17,((-0.0006*Q17^2 + 0.0699*Q17 - 1.2225)*Radiation!C16),0))))","v":0},{"$f":"IF(ED17<0,0,IF(0>R17,0,IF(50>R17,(( -0.000009*R17^2 + 0.0004*R17 + 0.7918)*Radiation!D16),IF(90>R17,((-0.0006*R17^2 + 0.0699*R17 - 1.2225)*Radiation!D16),0))))","v":0},{"$f":"IF(EE17<0,0,IF(0>S17,0,IF(50>S17,(( -0.000009*S17^2 + 0.0004*S17 + 0.7918)*Radiation!E16),IF(90>S17,((-0.0006*S17^2 + 0.0699*S17 - 1.2225)*Radiation!E16),0))))","v":0},{"$f":"IF(EF17<0,0,IF(0>T17,0,IF(50>T17,(( -0.000009*T17^2 + 0.0004*T17 + 0.7918)*Radiation!F16),IF(90>T17,((-0.0006*T17^2 + 0.0699*T17 - 1.2225)*Radiation!F16),0))))","v":0},{"$f":"IF(EG17<0,0,IF(0>U17,0,IF(50>U17,(( -0.000009*U17^2 + 0.0004*U17 + 0.7918)*Radiation!G16),IF(90>U17,((-0.0006*U17^2 + 0.0699*U17 - 1.2225)*Radiation!G16),0))))","v":0},{"$f":"IF(EH17<0,0,IF(0>V17,0,IF(50>V17,(( -0.000009*V17^2 + 0.0004*V17 + 0.7918)*Radiation!H16),IF(90>V17,((-0.0006*V17^2 + 0.0699*V17 - 1.2225)*Radiation!H16),0))))","v":0},{"$f":"IF(EI17<0,0,IF(0>W17,0,IF(50>W17,(( -0.000009*W17^2 + 0.0004*W17 + 0.7918)*Radiation!I16),IF(90>W17,((-0.0006*W17^2 + 0.0699*W17 - 1.2225)*Radiation!I16),0))))","v":0},{"$f":"IF(EJ17<0,0,IF(0>X17,0,IF(50>X17,(( -0.000009*X17^2 + 0.0004*X17 + 0.7918)*Radiation!J16),IF(90>X17,((-0.0006*X17^2 + 0.0699*X17 - 1.2225)*Radiation!J16),0))))","v":0},{"$f":"IF(EK17<0,0,IF(0>Y17,0,IF(50>Y17,(( -0.000009*Y17^2 + 0.0004*Y17 + 0.7918)*Radiation!K16),IF(90>Y17,((-0.0006*Y17^2 + 0.0699*Y17 - 1.2225)*Radiation!K16),0))))","v":0},{"$f":"IF(EL17<0,0,IF(0>Z17,0,IF(50>Z17,(( -0.000009*Z17^2 + 0.0004*Z17 + 0.7918)*Radiation!L16),IF(90>Z17,((-0.0006*Z17^2 + 0.0699*Z17 - 1.2225)*Radiation!L16),0))))","v":0},{"$f":"IF(EM17<0,0,IF(0>AA17,0,IF(50>AA17,(( -0.000009*AA17^2 + 0.0004*AA17 + 0.7918)*Radiation!M16),IF(90>AA17,((-0.0006*AA17^2 + 0.0699*AA17 - 1.2225)*Radiation!M16),0))))","v":0},{"$f":"IF(EN17<0,0,IF(0>AB17,0,IF(50>AB17,(( -0.000009*AB17^2 + 0.0004*AB17 + 0.7918)*Radiation!N16),IF(90>AB17,((-0.0006*AB17^2 + 0.0699*AB17 - 1.2225)*Radiation!N16),0))))","v":0},null,null,13,{"$f":"AG17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU17","v":2550.173141104859},{"$f":"AH17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV17","v":164.68058328163184},{"$f":"AI17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW17","v":0},{"$f":"AJ17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX17","v":0},{"$f":"AK17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY17","v":0},{"$f":"AL17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ17","v":0},{"$f":"AM17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA17","v":0},{"$f":"AN17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB17","v":0},{"$f":"AO17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC17","v":0},{"$f":"AP17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD17","v":315.54561787258626},{"$f":"AQ17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE17","v":2682.4119372208993},{"$f":"AR17*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF17","v":2806.1921484791264},null,13,{"$f":"AU17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI17","v":0},{"$f":"AV17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ17","v":0},{"$f":"AW17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK17","v":0},{"$f":"AX17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL17","v":0},{"$f":"AY17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM17","v":0},{"$f":"AZ17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN17","v":0},{"$f":"BA17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO17","v":0},{"$f":"BB17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP17","v":0},{"$f":"BC17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ17","v":0},{"$f":"BD17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR17","v":0},{"$f":"BE17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS17","v":0},{"$f":"BF17*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT17","v":0},null,13,1,1,0,0,0,0,0,0,0,1,1,1,null,13,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B16","v":13},{"$f":"'Solar Altitude'!C16","v":44.262516808487675},{"$f":"'Solar Altitude'!D16","v":53.442649547558034},{"$f":"'Solar Altitude'!E16","v":62.96975399076122},{"$f":"'Solar Altitude'!F16","v":71.918657174425832},{"$f":"'Solar Altitude'!G16","v":76.310429689037434},{"$f":"'Solar Altitude'!H16","v":78.190731192893594},{"$f":"'Solar Altitude'!I16","v":78.445286814888803},{"$f":"'Solar Altitude'!J16","v":72.64341275146262},{"$f":"'Solar Altitude'!K16","v":61.303344417053367},{"$f":"'Solar Altitude'!L16","v":50.879096974273239},{"$f":"'Solar Altitude'!M16","v":42.542599664242438},{"$f":"'Solar Altitude'!N16","v":40.072467904514703},null,13,44.262516808487675,53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703]
[null,14,{"$f":"DEGREES(C46)","v":48.384923871764663},57.30589777180974,68.0079820369277,80.094317479627279,88.427456929501062,91.297274502331859,88.188834479024777,80.119557426128281,68.804658288796318,58.893124354771295,49.935131171639902,45.72804470108909,null,14,{"$f":"DEGREES(Q46)","v":113.80152664234694},114.29190709998221,116.34166666666667,117.8254204844152,117.08385192225026,115.39210484276566,114.85843623524879,116.95272273401245,120.09166666666668,121.44465353806184,119.57940178527421,116.06495948371041,null,null,null,14,{"$f":"IF(DO18<0,0,IF(0>C18,0,IF(50>C18,((-0.000009*C18^2 + 0.0004*C18 + 0.7918)*Radiation!C17),IF(90>C18,(( -0.0006*C18^2 + 0.0699*C18 - 1.2225)*Radiation!C17),0))))","v":148.77058158818227},{"$f":"IF(DP18<0,0,IF(0>D18,0,IF(50>D18,((-0.000009*D18^2 + 0.0004*D18 + 0.7918)*Radiation!D17),IF(90>D18,(( -0.0006*D18^2 + 0.0699*D18 - 1.2225)*Radiation!D17),0))))","v":182.4213693831388},{"$f":"IF(DQ18<0,0,IF(0>E18,0,IF(50>E18,((-0.000009*E18^2 + 0.0004*E18 + 0.7918)*Radiation!E17),IF(90>E18,(( -0.0006*E18^2 + 0.0699*E18 - 1.2225)*Radiation!E17),0))))","v":183.14333603249401},{"$f":"IF(DR18<0,0,IF(0>F18,0,IF(50>F18,((-0.000009*F18^2 + 0.0004*F18 + 0.7918)*Radiation!F17),IF(90>F18,(( -0.0006*F18^2 + 0.0699*F18 - 1.2225)*Radiation!F17),0))))","v":128.97703976285345},{"$f":"IF(DS18<0,0,IF(0>G18,0,IF(50>G18,((-0.000009*G18^2 + 0.0004*G18 + 0.7918)*Radiation!G17),IF(90>G18,(( -0.0006*G18^2 + 0.0699*G18 - 1.2225)*Radiation!G17),0))))","v":74.885584817961842},{"$f":"IF(DT18<0,0,IF(0>H18,0,IF(50>H18,((-0.000009*H18^2 + 0.0004*H18 + 0.7918)*Radiation!H17),IF(90>H18,(( -0.0006*H18^2 + 0.0699*H18 - 1.2225)*Radiation!H17),0))))","v":0},{"$f":"IF(DU18<0,0,IF(0>I18,0,IF(50>I18,((-0.000009*I18^2 + 0.0004*I18 + 0.7918)*Radiation!I17),IF(90>I18,(( -0.0006*I18^2 + 0.0699*I18 - 1.2225)*Radiation!I17),0))))","v":82.366245595696597},{"$f":"IF(DV18<0,0,IF(0>J18,0,IF(50>J18,((-0.000009*J18^2 + 0.0004*J18 + 0.7918)*Radiation!J17),IF(90>J18,(( -0.0006*J18^2 + 0.0699*J18 - 1.2225)*Radiation!J17),0))))","v":153.00956619797941},{"$f":"IF(DW18<0,0,IF(0>K18,0,IF(50>K18,((-0.000009*K18^2 + 0.0004*K18 + 0.7918)*Radiation!K17),IF(90>K18,(( -0.0006*K18^2 + 0.0699*K18 - 1.2225)*Radiation!K17),0))))","v":203.03582617954794},{"$f":"IF(DX18<0,0,IF(0>L18,0,IF(50>L18,((-0.000009*L18^2 + 0.0004*L18 + 0.7918)*Radiation!L17),IF(90>L18,(( -0.0006*L18^2 + 0.0699*L18 - 1.2225)*Radiation!L17),0))))","v":195.11535964891399},{"$f":"IF(DY18<0,0,IF(0>M18,0,IF(50>M18,((-0.000009*M18^2 + 0.0004*M18 + 0.7918)*Radiation!M17),IF(90>M18,(( -0.0006*M18^2 + 0.0699*M18 - 1.2225)*Radiation!M17),0))))","v":154.88447634659303},{"$f":"IF(DZ18<0,0,IF(0>N18,0,IF(50>N18,((-0.000009*N18^2 + 0.0004*N18 + 0.7918)*Radiation!N17),IF(90>N18,(( -0.0006*N18^2 + 0.0699*N18 - 1.2225)*Radiation!N17),0))))","v":128.17515919097704},null,14,{"$f":"IF(EC18<0,0,IF(0>Q18,0,IF(50>Q18,(( -0.000009*Q18^2 + 0.0004*Q18 + 0.7918)*Radiation!C17),IF(90>Q18,((-0.0006*Q18^2 + 0.0699*Q18 - 1.2225)*Radiation!C17),0))))","v":0},{"$f":"IF(ED18<0,0,IF(0>R18,0,IF(50>R18,(( -0.000009*R18^2 + 0.0004*R18 + 0.7918)*Radiation!D17),IF(90>R18,((-0.0006*R18^2 + 0.0699*R18 - 1.2225)*Radiation!D17),0))))","v":0},{"$f":"IF(EE18<0,0,IF(0>S18,0,IF(50>S18,(( -0.000009*S18^2 + 0.0004*S18 + 0.7918)*Radiation!E17),IF(90>S18,((-0.0006*S18^2 + 0.0699*S18 - 1.2225)*Radiation!E17),0))))","v":0},{"$f":"IF(EF18<0,0,IF(0>T18,0,IF(50>T18,(( -0.000009*T18^2 + 0.0004*T18 + 0.7918)*Radiation!F17),IF(90>T18,((-0.0006*T18^2 + 0.0699*T18 - 1.2225)*Radiation!F17),0))))","v":0},{"$f":"IF(EG18<0,0,IF(0>U18,0,IF(50>U18,(( -0.000009*U18^2 + 0.0004*U18 + 0.7918)*Radiation!G17),IF(90>U18,((-0.0006*U18^2 + 0.0699*U18 - 1.2225)*Radiation!G17),0))))","v":0},{"$f":"IF(EH18<0,0,IF(0>V18,0,IF(50>V18,(( -0.000009*V18^2 + 0.0004*V18 + 0.7918)*Radiation!H17),IF(90>V18,((-0.0006*V18^2 + 0.0699*V18 - 1.2225)*Radiation!H17),0))))","v":0},{"$f":"IF(EI18<0,0,IF(0>W18,0,IF(50>W18,(( -0.000009*W18^2 + 0.0004*W18 + 0.7918)*Radiation!I17),IF(90>W18,((-0.0006*W18^2 + 0.0699*W18 - 1.2225)*Radiation!I17),0))))","v":0},{"$f":"IF(EJ18<0,0,IF(0>X18,0,IF(50>X18,(( -0.000009*X18^2 + 0.0004*X18 + 0.7918)*Radiation!J17),IF(90>X18,((-0.0006*X18^2 + 0.0699*X18 - 1.2225)*Radiation!J17),0))))","v":0},{"$f":"IF(EK18<0,0,IF(0>Y18,0,IF(50>Y18,(( -0.000009*Y18^2 + 0.0004*Y18 + 0.7918)*Radiation!K17),IF(90>Y18,((-0.0006*Y18^2 + 0.0699*Y18 - 1.2225)*Radiation!K17),0))))","v":0},{"$f":"IF(EL18<0,0,IF(0>Z18,0,IF(50>Z18,(( -0.000009*Z18^2 + 0.0004*Z18 + 0.7918)*Radiation!L17),IF(90>Z18,((-0.0006*Z18^2 + 0.0699*Z18 - 1.2225)*Radiation!L17),0))))","v":0},{"$f":"IF(EM18<0,0,IF(0>AA18,0,IF(50>AA18,(( -0.000009*AA18^2 + 0.0004*AA18 + 0.7918)*Radiation!M17),IF(90>AA18,((-0.0006*AA18^2 + 0.0699*AA18 - 1.2225)*Radiation!M17),0))))","v":0},{"$f":"IF(EN18<0,0,IF(0>AB18,0,IF(50>AB18,(( -0.000009*AB18^2 + 0.0004*AB18 + 0.7918)*Radiation!N17),IF(90>AB18,((-0.0006*AB18^2 + 0.0699*AB18 - 1.2225)*Radiation!N17),0))))","v":0},null,null,14,{"$f":"AG18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU18","v":2071.1194620481665},{"$f":"AH18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV18","v":325.93097583385139},{"$f":"AI18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW18","v":0},{"$f":"AJ18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX18","v":0},{"$f":"AK18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY18","v":0},{"$f":"AL18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ18","v":0},{"$f":"AM18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA18","v":0},{"$f":"AN18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB18","v":0},{"$f":"AO18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC18","v":0},{"$f":"AP18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD18","v":459.69342121644979},{"$f":"AQ18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE18","v":2064.4902305776382},{"$f":"AR18*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF18","v":2259.4897211870334},null,14,{"$f":"AU18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI18","v":0},{"$f":"AV18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ18","v":0},{"$f":"AW18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK18","v":0},{"$f":"AX18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL18","v":0},{"$f":"AY18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM18","v":0},{"$f":"AZ18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN18","v":0},{"$f":"BA18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO18","v":0},{"$f":"BB18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP18","v":0},{"$f":"BC18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ18","v":0},{"$f":"BD18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR18","v":0},{"$f":"BE18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS18","v":0},{"$f":"BF18*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT18","v":0},null,14,1,1,0,0,0,0,0,0,0,0.40105237912950042,0.73623397042051142,0.9165824100126917,null,14,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B17","v":14},{"$f":"'Solar Altitude'!C17","v":39.001643714284292},{"$f":"'Solar Altitude'!D17","v":47.236569251778789},{"$f":"'Solar Altitude'!E17","v":54.505603493104616},{"$f":"'Solar Altitude'!F17","v":60.167275430762508},{"$f":"'Solar Altitude'!G17","v":62.862961225627508},{"$f":"'Solar Altitude'!H17","v":64.570010808670432},{"$f":"'Solar Altitude'!I17","v":65.066621957768987},{"$f":"'Solar Altitude'!J17","v":61.010544197086858},{"$f":"'Solar Altitude'!K17","v":51.819137025254037},{"$f":"'Solar Altitude'!L17","v":42.759898297268641},{"$f":"'Solar Altitude'!M17","v":35.791762146841563},{"$f":"'Solar Altitude'!N17","v":34.427909280399348},null,14,39.001643714284292,47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348]
[null,15,{"$f":"DEGREES(C47)","v":52.527275882085547},61.121700815529152,71.715964657344173,83.725111578584958,91.918241909554226,94.620997796705083,91.477095254085199,83.671055341179695,72.842250661669055,63.361512984487817,54.628717489789388,50.276957524957531,null,15,{"$f":"DEGREES(Q47)","v":127.56258934981172},128.93344837599088,131.3416666666667,132.33451117149943,130.69277923171461,128.61670904570374,128.51326434673757,131.45620008264507,135.0916666666667,136.00634828680964,133.15236383168141,129.26111228713944,null,null,null,15,{"$f":"IF(DO19<0,0,IF(0>C19,0,IF(50>C19,((-0.000009*C19^2 + 0.0004*C19 + 0.7918)*Radiation!C18),IF(90>C19,(( -0.0006*C19^2 + 0.0699*C19 - 1.2225)*Radiation!C18),0))))","v":117.99941081854807},{"$f":"IF(DP19<0,0,IF(0>D19,0,IF(50>D19,((-0.000009*D19^2 + 0.0004*D19 + 0.7918)*Radiation!D18),IF(90>D19,(( -0.0006*D19^2 + 0.0699*D19 - 1.2225)*Radiation!D18),0))))","v":151.19241036264214},{"$f":"IF(DQ19<0,0,IF(0>E19,0,IF(50>E19,((-0.000009*E19^2 + 0.0004*E19 + 0.7918)*Radiation!E18),IF(90>E19,(( -0.0006*E19^2 + 0.0699*E19 - 1.2225)*Radiation!E18),0))))","v":142.0427141259475},{"$f":"IF(DR19<0,0,IF(0>F19,0,IF(50>F19,((-0.000009*F19^2 + 0.0004*F19 + 0.7918)*Radiation!F18),IF(90>F19,(( -0.0006*F19^2 + 0.0699*F19 - 1.2225)*Radiation!F18),0))))","v":85.069591455970269},{"$f":"IF(DS19<0,0,IF(0>G19,0,IF(50>G19,((-0.000009*G19^2 + 0.0004*G19 + 0.7918)*Radiation!G18),IF(90>G19,(( -0.0006*G19^2 + 0.0699*G19 - 1.2225)*Radiation!G18),0))))","v":0},{"$f":"IF(DT19<0,0,IF(0>H19,0,IF(50>H19,((-0.000009*H19^2 + 0.0004*H19 + 0.7918)*Radiation!H18),IF(90>H19,(( -0.0006*H19^2 + 0.0699*H19 - 1.2225)*Radiation!H18),0))))","v":0},{"$f":"IF(DU19<0,0,IF(0>I19,0,IF(50>I19,((-0.000009*I19^2 + 0.0004*I19 + 0.7918)*Radiation!I18),IF(90>I19,(( -0.0006*I19^2 + 0.0699*I19 - 1.2225)*Radiation!I18),0))))","v":0},{"$f":"IF(DV19<0,0,IF(0>J19,0,IF(50>J19,((-0.000009*J19^2 + 0.0004*J19 + 0.7918)*Radiation!J18),IF(90>J19,(( -0.0006*J19^2 + 0.0699*J19 - 1.2225)*Radiation!J18),0))))","v":101.99530616872087},{"$f":"IF(DW19<0,0,IF(0>K19,0,IF(50>K19,((-0.000009*K19^2 + 0.0004*K19 + 0.7918)*Radiation!K18),IF(90>K19,(( -0.0006*K19^2 + 0.0699*K19 - 1.2225)*Radiation!K18),0))))","v":149.73830863017571},{"$f":"IF(DX19<0,0,IF(0>L19,0,IF(50>L19,((-0.000009*L19^2 + 0.0004*L19 + 0.7918)*Radiation!L18),IF(90>L19,(( -0.0006*L19^2 + 0.0699*L19 - 1.2225)*Radiation!L18),0))))","v":147.66871624427156},{"$f":"IF(DY19<0,0,IF(0>M19,0,IF(50>M19,((-0.000009*M19^2 + 0.0004*M19 + 0.7918)*Radiation!M18),IF(90>M19,(( -0.0006*M19^2 + 0.0699*M19 - 1.2225)*Radiation!M18),0))))","v":114.89967869426059},{"$f":"IF(DZ19<0,0,IF(0>N19,0,IF(50>N19,((-0.000009*N19^2 + 0.0004*N19 + 0.7918)*Radiation!N18),IF(90>N19,(( -0.0006*N19^2 + 0.0699*N19 - 1.2225)*Radiation!N18),0))))","v":95.345562002607963},null,15,{"$f":"IF(EC19<0,0,IF(0>Q19,0,IF(50>Q19,(( -0.000009*Q19^2 + 0.0004*Q19 + 0.7918)*Radiation!C18),IF(90>Q19,((-0.0006*Q19^2 + 0.0699*Q19 - 1.2225)*Radiation!C18),0))))","v":0},{"$f":"IF(ED19<0,0,IF(0>R19,0,IF(50>R19,(( -0.000009*R19^2 + 0.0004*R19 + 0.7918)*Radiation!D18),IF(90>R19,((-0.0006*R19^2 + 0.0699*R19 - 1.2225)*Radiation!D18),0))))","v":0},{"$f":"IF(EE19<0,0,IF(0>S19,0,IF(50>S19,(( -0.000009*S19^2 + 0.0004*S19 + 0.7918)*Radiation!E18),IF(90>S19,((-0.0006*S19^2 + 0.0699*S19 - 1.2225)*Radiation!E18),0))))","v":0},{"$f":"IF(EF19<0,0,IF(0>T19,0,IF(50>T19,(( -0.000009*T19^2 + 0.0004*T19 + 0.7918)*Radiation!F18),IF(90>T19,((-0.0006*T19^2 + 0.0699*T19 - 1.2225)*Radiation!F18),0))))","v":0},{"$f":"IF(EG19<0,0,IF(0>U19,0,IF(50>U19,(( -0.000009*U19^2 + 0.0004*U19 + 0.7918)*Radiation!G18),IF(90>U19,((-0.0006*U19^2 + 0.0699*U19 - 1.2225)*Radiation!G18),0))))","v":0},{"$f":"IF(EH19<0,0,IF(0>V19,0,IF(50>V19,(( -0.000009*V19^2 + 0.0004*V19 + 0.7918)*Radiation!H18),IF(90>V19,((-0.0006*V19^2 + 0.0699*V19 - 1.2225)*Radiation!H18),0))))","v":0},{"$f":"IF(EI19<0,0,IF(0>W19,0,IF(50>W19,(( -0.000009*W19^2 + 0.0004*W19 + 0.7918)*Radiation!I18),IF(90>W19,((-0.0006*W19^2 + 0.0699*W19 - 1.2225)*Radiation!I18),0))))","v":0},{"$f":"IF(EJ19<0,0,IF(0>X19,0,IF(50>X19,(( -0.000009*X19^2 + 0.0004*X19 + 0.7918)*Radiation!J18),IF(90>X19,((-0.0006*X19^2 + 0.0699*X19 - 1.2225)*Radiation!J18),0))))","v":0},{"$f":"IF(EK19<0,0,IF(0>Y19,0,IF(50>Y19,(( -0.000009*Y19^2 + 0.0004*Y19 + 0.7918)*Radiation!K18),IF(90>Y19,((-0.0006*Y19^2 + 0.0699*Y19 - 1.2225)*Radiation!K18),0))))","v":0},{"$f":"IF(EL19<0,0,IF(0>Z19,0,IF(50>Z19,(( -0.000009*Z19^2 + 0.0004*Z19 + 0.7918)*Radiation!L18),IF(90>Z19,((-0.0006*Z19^2 + 0.0699*Z19 - 1.2225)*Radiation!L18),0))))","v":0},{"$f":"IF(EM19<0,0,IF(0>AA19,0,IF(50>AA19,(( -0.000009*AA19^2 + 0.0004*AA19 + 0.7918)*Radiation!M18),IF(90>AA19,((-0.0006*AA19^2 + 0.0699*AA19 - 1.2225)*Radiation!M18),0))))","v":0},{"$f":"IF(EN19<0,0,IF(0>AB19,0,IF(50>AB19,(( -0.000009*AB19^2 + 0.0004*AB19 + 0.7918)*Radiation!N18),IF(90>AB19,((-0.0006*AB19^2 + 0.0699*AB19 - 1.2225)*Radiation!N18),0))))","v":0},null,null,15,{"$f":"AG19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU19","v":1452.546941542701},{"$f":"AH19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV19","v":364.46110364013998},{"$f":"AI19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW19","v":0},{"$f":"AJ19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX19","v":0},{"$f":"AK19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY19","v":0},{"$f":"AL19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ19","v":0},{"$f":"AM19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA19","v":0},{"$f":"AN19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB19","v":0},{"$f":"AO19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC19","v":0},{"$f":"AP19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD19","v":297.93065860827932},{"$f":"AQ19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE19","v":1293.4997769469985},{"$f":"AR19*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF19","v":1490.3099220028244},null,15,{"$f":"AU19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI19","v":0},{"$f":"AV19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ19","v":0},{"$f":"AW19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK19","v":0},{"$f":"AX19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL19","v":0},{"$f":"AY19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM19","v":0},{"$f":"AZ19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN19","v":0},{"$f":"BA19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO19","v":0},{"$f":"BB19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP19","v":0},{"$f":"BC19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ19","v":0},{"$f":"BD19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR19","v":0},{"$f":"BE19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS19","v":0},{"$f":"BF19*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT19","v":0},null,15,0.42985970538426138,0.1387240028188502,0,0,0,0,0,0,0,7.2286194092559944E-2,0.31757112208291405,0.43705225732244574,null,15,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B18","v":15},{"$f":"'Solar Altitude'!C18","v":30.541133571003865},{"$f":"'Solar Altitude'!D18","v":37.574701882546435},{"$f":"'Solar Altitude'!E18","v":43.007444089240849},{"$f":"'Solar Altitude'!F18","v":46.978750874484376},{"$f":"'Solar Altitude'!G18","v":49.242301300948341},{"$f":"'Solar Altitude'!H18","v":51.002542825705397},{"$f":"'Solar Altitude'!I18","v":51.447673176445399},{"$f":"'Solar Altitude'!J18","v":47.843171633901541},{"$f":"'Solar Altitude'!K18","v":39.895074988635152},{"$f":"'Solar Altitude'!L18","v":32.038156511029932},{"$f":"'Solar Altitude'!M18","v":26.359057025099464},{"$f":"'Solar Altitude'!N18","v":25.920295493187655},null,15,30.541133571003865,37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655]
[null,16,{"$f":"DEGREES(C48)","v":57.841847447541205},66.157455563706563,76.608808985374225,88.489782119801262,96.522199020907905,99.06974652673415,95.916904068398793,88.373188255008557,77.974072698698691,68.836939082031861,60.283062869381794,55.862851093401424,null,16,{"$f":"DEGREES(Q48)","v":140.72718463621587},143.38134756077289,146.34166666666667,146.53696034723595,143.54066211551253,140.97510241267139,141.4972426385159,145.66176552614004,150.09166666666664,150.24225996413057,145.85736453236672,141.55386757464609,null,null,null,16,{"$f":"IF(DO20<0,0,IF(0>C20,0,IF(50>C20,((-0.000009*C20^2 + 0.0004*C20 + 0.7918)*Radiation!C19),IF(90>C20,(( -0.0006*C20^2 + 0.0699*C20 - 1.2225)*Radiation!C19),0))))","v":80.174290535297629},{"$f":"IF(DP20<0,0,IF(0>D20,0,IF(50>D20,((-0.000009*D20^2 + 0.0004*D20 + 0.7918)*Radiation!D19),IF(90>D20,(( -0.0006*D20^2 + 0.0699*D20 - 1.2225)*Radiation!D19),0))))","v":100.83297567011383},{"$f":"IF(DQ20<0,0,IF(0>E20,0,IF(50>E20,((-0.000009*E20^2 + 0.0004*E20 + 0.7918)*Radiation!E19),IF(90>E20,(( -0.0006*E20^2 + 0.0699*E20 - 1.2225)*Radiation!E19),0))))","v":87.949331677878433},{"$f":"IF(DR20<0,0,IF(0>F20,0,IF(50>F20,((-0.000009*F20^2 + 0.0004*F20 + 0.7918)*Radiation!F19),IF(90>F20,(( -0.0006*F20^2 + 0.0699*F20 - 1.2225)*Radiation!F19),0))))","v":38.342428921306023},{"$f":"IF(DS20<0,0,IF(0>G20,0,IF(50>G20,((-0.000009*G20^2 + 0.0004*G20 + 0.7918)*Radiation!G19),IF(90>G20,(( -0.0006*G20^2 + 0.0699*G20 - 1.2225)*Radiation!G19),0))))","v":0},{"$f":"IF(DT20<0,0,IF(0>H20,0,IF(50>H20,((-0.000009*H20^2 + 0.0004*H20 + 0.7918)*Radiation!H19),IF(90>H20,(( -0.0006*H20^2 + 0.0699*H20 - 1.2225)*Radiation!H19),0))))","v":0},{"$f":"IF(DU20<0,0,IF(0>I20,0,IF(50>I20,((-0.000009*I20^2 + 0.0004*I20 + 0.7918)*Radiation!I19),IF(90>I20,(( -0.0006*I20^2 + 0.0699*I20 - 1.2225)*Radiation!I19),0))))","v":0},{"$f":"IF(DV20<0,0,IF(0>J20,0,IF(50>J20,((-0.000009*J20^2 + 0.0004*J20 + 0.7918)*Radiation!J19),IF(90>J20,(( -0.0006*J20^2 + 0.0699*J20 - 1.2225)*Radiation!J19),0))))","v":47.307586487905539},{"$f":"IF(DW20<0,0,IF(0>K20,0,IF(50>K20,((-0.000009*K20^2 + 0.0004*K20 + 0.7918)*Radiation!K19),IF(90>K20,(( -0.0006*K20^2 + 0.0699*K20 - 1.2225)*Radiation!K19),0))))","v":86.584842357390428},{"$f":"IF(DX20<0,0,IF(0>L20,0,IF(50>L20,((-0.000009*L20^2 + 0.0004*L20 + 0.7918)*Radiation!L19),IF(90>L20,(( -0.0006*L20^2 + 0.0699*L20 - 1.2225)*Radiation!L19),0))))","v":84.670110056244752},{"$f":"IF(DY20<0,0,IF(0>M20,0,IF(50>M20,((-0.000009*M20^2 + 0.0004*M20 + 0.7918)*Radiation!M19),IF(90>M20,(( -0.0006*M20^2 + 0.0699*M20 - 1.2225)*Radiation!M19),0))))","v":61.946802140911593},{"$f":"IF(DZ20<0,0,IF(0>N20,0,IF(50>N20,((-0.000009*N20^2 + 0.0004*N20 + 0.7918)*Radiation!N19),IF(90>N20,(( -0.0006*N20^2 + 0.0699*N20 - 1.2225)*Radiation!N19),0))))","v":57.767171712765524},null,16,{"$f":"IF(EC20<0,0,IF(0>Q20,0,IF(50>Q20,(( -0.000009*Q20^2 + 0.0004*Q20 + 0.7918)*Radiation!C19),IF(90>Q20,((-0.0006*Q20^2 + 0.0699*Q20 - 1.2225)*Radiation!C19),0))))","v":0},{"$f":"IF(ED20<0,0,IF(0>R20,0,IF(50>R20,(( -0.000009*R20^2 + 0.0004*R20 + 0.7918)*Radiation!D19),IF(90>R20,((-0.0006*R20^2 + 0.0699*R20 - 1.2225)*Radiation!D19),0))))","v":0},{"$f":"IF(EE20<0,0,IF(0>S20,0,IF(50>S20,(( -0.000009*S20^2 + 0.0004*S20 + 0.7918)*Radiation!E19),IF(90>S20,((-0.0006*S20^2 + 0.0699*S20 - 1.2225)*Radiation!E19),0))))","v":0},{"$f":"IF(EF20<0,0,IF(0>T20,0,IF(50>T20,(( -0.000009*T20^2 + 0.0004*T20 + 0.7918)*Radiation!F19),IF(90>T20,((-0.0006*T20^2 + 0.0699*T20 - 1.2225)*Radiation!F19),0))))","v":0},{"$f":"IF(EG20<0,0,IF(0>U20,0,IF(50>U20,(( -0.000009*U20^2 + 0.0004*U20 + 0.7918)*Radiation!G19),IF(90>U20,((-0.0006*U20^2 + 0.0699*U20 - 1.2225)*Radiation!G19),0))))","v":0},{"$f":"IF(EH20<0,0,IF(0>V20,0,IF(50>V20,(( -0.000009*V20^2 + 0.0004*V20 + 0.7918)*Radiation!H19),IF(90>V20,((-0.0006*V20^2 + 0.0699*V20 - 1.2225)*Radiation!H19),0))))","v":0},{"$f":"IF(EI20<0,0,IF(0>W20,0,IF(50>W20,(( -0.000009*W20^2 + 0.0004*W20 + 0.7918)*Radiation!I19),IF(90>W20,((-0.0006*W20^2 + 0.0699*W20 - 1.2225)*Radiation!I19),0))))","v":0},{"$f":"IF(EJ20<0,0,IF(0>X20,0,IF(50>X20,(( -0.000009*X20^2 + 0.0004*X20 + 0.7918)*Radiation!J19),IF(90>X20,((-0.0006*X20^2 + 0.0699*X20 - 1.2225)*Radiation!J19),0))))","v":0},{"$f":"IF(EK20<0,0,IF(0>Y20,0,IF(50>Y20,(( -0.000009*Y20^2 + 0.0004*Y20 + 0.7918)*Radiation!K19),IF(90>Y20,((-0.0006*Y20^2 + 0.0699*Y20 - 1.2225)*Radiation!K19),0))))","v":0},{"$f":"IF(EL20<0,0,IF(0>Z20,0,IF(50>Z20,(( -0.000009*Z20^2 + 0.0004*Z20 + 0.7918)*Radiation!L19),IF(90>Z20,((-0.0006*Z20^2 + 0.0699*Z20 - 1.2225)*Radiation!L19),0))))","v":0},{"$f":"IF(EM20<0,0,IF(0>AA20,0,IF(50>AA20,(( -0.000009*AA20^2 + 0.0004*AA20 + 0.7918)*Radiation!M19),IF(90>AA20,((-0.0006*AA20^2 + 0.0699*AA20 - 1.2225)*Radiation!M19),0))))","v":0},{"$f":"IF(EN20<0,0,IF(0>AB20,0,IF(50>AB20,(( -0.000009*AB20^2 + 0.0004*AB20 + 0.7918)*Radiation!N19),IF(90>AB20,((-0.0006*AB20^2 + 0.0699*AB20 - 1.2225)*Radiation!N19),0))))","v":0},null,null,16,{"$f":"AG20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU20","v":713.65975482504973},{"$f":"AH20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV20","v":10.376642262278452},{"$f":"AI20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW20","v":0},{"$f":"AJ20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX20","v":0},{"$f":"AK20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY20","v":0},{"$f":"AL20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ20","v":0},{"$f":"AM20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA20","v":0},{"$f":"AN20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB20","v":0},{"$f":"AO20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC20","v":0},{"$f":"AP20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD20","v":0},{"$f":"AQ20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE20","v":381.95980659736199},{"$f":"AR20*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF20","v":690.59594603259609},null,16,{"$f":"AU20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI20","v":0},{"$f":"AV20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ20","v":0},{"$f":"AW20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK20","v":0},{"$f":"AX20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL20","v":0},{"$f":"AY20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM20","v":0},{"$f":"AZ20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN20","v":0},{"$f":"BA20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO20","v":0},{"$f":"BB20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP20","v":0},{"$f":"BC20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ20","v":0},{"$f":"BD20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR20","v":0},{"$f":"BE20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS20","v":0},{"$f":"BF20*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT20","v":0},null,16,0.20458732498358867,2.7708256806850172E-3,0,0,0,0,0,0,0,0,0.12853419638545177,0.24189764271439126,null,16,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B19","v":16},{"$f":"'Solar Altitude'!C19","v":20.038281727598083},{"$f":"'Solar Altitude'!D19","v":26.016647471873153},{"$f":"'Solar Altitude'!E19","v":30.233879108991232},{"$f":"'Solar Altitude'!F19","v":33.419767540103443},{"$f":"'Solar Altitude'!G19","v":35.682648220686666},{"$f":"'Solar Altitude'!H19","v":37.56104623172925},{"$f":"'Solar Altitude'!I19","v":37.876258416390314},{"$f":"'Solar Altitude'!J19","v":34.288646107643089},{"$f":"'Solar Altitude'!K19","v":26.935985833021654},{"$f":"'Solar Altitude'!L19","v":19.913519068774189},{"$f":"'Solar Altitude'!M19","v":15.259931573481456},{"$f":"'Solar Altitude'!N19","v":15.530455637101428},null,16,{"$f":"DO20","v":20.038281727598083},{"$f":"DP20","v":26.016647471873153},{"$f":"DQ20","v":30.233879108991232},{"$f":"DR20","v":33.419767540103443},{"$f":"DS20","v":35.682648220686666},{"$f":"DT20","v":37.56104623172925},{"$f":"DU20","v":37.876258416390314},{"$f":"DV20","v":34.288646107643089},{"$f":"DW20","v":26.935985833021654},{"$f":"DX20","v":19.913519068774189},{"$f":"DY20","v":15.259931573481456},{"$f":"DZ20","v":15.530455637101428}]
[null,17,{"$f":"DEGREES(C49)","v":63.836508807009714},71.980527779765922,82.317370695731228,94.080103860845398,101.97249092127181,104.39496468219401,101.24776405592698,93.920398769784754,83.828429315210954,74.895560749988377,66.431189468708737,61.987157084725183,null,17,{"$f":"DEGREES(Q49)","v":152.36212818793786},157.23977387018414,161.34166666666664,159.74701376251107,154.38832575868955,151.24619189772807,152.76402384128761,158.92734049062068,165.09166666666667,163.27261469342773,156.19756812451465,151.66134854942314,null,null,null,17,{"$f":"IF(DO21<0,0,IF(0>C21,0,IF(50>C21,((-0.000009*C21^2 + 0.0004*C21 + 0.7918)*Radiation!C20),IF(90>C21,(( -0.0006*C21^2 + 0.0699*C21 - 1.2225)*Radiation!C20),0))))","v":30.478797797016597},{"$f":"IF(DP21<0,0,IF(0>D21,0,IF(50>D21,((-0.000009*D21^2 + 0.0004*D21 + 0.7918)*Radiation!D20),IF(90>D21,(( -0.0006*D21^2 + 0.0699*D21 - 1.2225)*Radiation!D20),0))))","v":43.505940076617108},{"$f":"IF(DQ21<0,0,IF(0>E21,0,IF(50>E21,((-0.000009*E21^2 + 0.0004*E21 + 0.7918)*Radiation!E20),IF(90>E21,(( -0.0006*E21^2 + 0.0699*E21 - 1.2225)*Radiation!E20),0))))","v":35.732799099451555},{"$f":"IF(DR21<0,0,IF(0>F21,0,IF(50>F21,((-0.000009*F21^2 + 0.0004*F21 + 0.7918)*Radiation!F20),IF(90>F21,(( -0.0006*F21^2 + 0.0699*F21 - 1.2225)*Radiation!F20),0))))","v":0},{"$f":"IF(DS21<0,0,IF(0>G21,0,IF(50>G21,((-0.000009*G21^2 + 0.0004*G21 + 0.7918)*Radiation!G20),IF(90>G21,(( -0.0006*G21^2 + 0.0699*G21 - 1.2225)*Radiation!G20),0))))","v":0},{"$f":"IF(DT21<0,0,IF(0>H21,0,IF(50>H21,((-0.000009*H21^2 + 0.0004*H21 + 0.7918)*Radiation!H20),IF(90>H21,(( -0.0006*H21^2 + 0.0699*H21 - 1.2225)*Radiation!H20),0))))","v":0},{"$f":"IF(DU21<0,0,IF(0>I21,0,IF(50>I21,((-0.000009*I21^2 + 0.0004*I21 + 0.7918)*Radiation!I20),IF(90>I21,(( -0.0006*I21^2 + 0.0699*I21 - 1.2225)*Radiation!I20),0))))","v":0},{"$f":"IF(DV21<0,0,IF(0>J21,0,IF(50>J21,((-0.000009*J21^2 + 0.0004*J21 + 0.7918)*Radiation!J20),IF(90>J21,(( -0.0006*J21^2 + 0.0699*J21 - 1.2225)*Radiation!J20),0))))","v":0},{"$f":"IF(DW21<0,0,IF(0>K21,0,IF(50>K21,((-0.000009*K21^2 + 0.0004*K21 + 0.7918)*Radiation!K20),IF(90>K21,(( -0.0006*K21^2 + 0.0699*K21 - 1.2225)*Radiation!K20),0))))","v":29.878887224864119},{"$f":"IF(DX21<0,0,IF(0>L21,0,IF(50>L21,((-0.000009*L21^2 + 0.0004*L21 + 0.7918)*Radiation!L20),IF(90>L21,(( -0.0006*L21^2 + 0.0699*L21 - 1.2225)*Radiation!L20),0))))","v":24.820422800705128},{"$f":"IF(DY21<0,0,IF(0>M21,0,IF(50>M21,((-0.000009*M21^2 + 0.0004*M21 + 0.7918)*Radiation!M20),IF(90>M21,(( -0.0006*M21^2 + 0.0699*M21 - 1.2225)*Radiation!M20),0))))","v":11.519533079727399},{"$f":"IF(DZ21<0,0,IF(0>N21,0,IF(50>N21,((-0.000009*N21^2 + 0.0004*N21 + 0.7918)*Radiation!N20),IF(90>N21,(( -0.0006*N21^2 + 0.0699*N21 - 1.2225)*Radiation!N20),0))))","v":14.289544912479011},null,17,{"$f":"IF(EC21<0,0,IF(0>Q21,0,IF(50>Q21,(( -0.000009*Q21^2 + 0.0004*Q21 + 0.7918)*Radiation!C20),IF(90>Q21,((-0.0006*Q21^2 + 0.0699*Q21 - 1.2225)*Radiation!C20),0))))","v":0},{"$f":"IF(ED21<0,0,IF(0>R21,0,IF(50>R21,(( -0.000009*R21^2 + 0.0004*R21 + 0.7918)*Radiation!D20),IF(90>R21,((-0.0006*R21^2 + 0.0699*R21 - 1.2225)*Radiation!D20),0))))","v":0},{"$f":"IF(EE21<0,0,IF(0>S21,0,IF(50>S21,(( -0.000009*S21^2 + 0.0004*S21 + 0.7918)*Radiation!E20),IF(90>S21,((-0.0006*S21^2 + 0.0699*S21 - 1.2225)*Radiation!E20),0))))","v":0},{"$f":"IF(EF21<0,0,IF(0>T21,0,IF(50>T21,(( -0.000009*T21^2 + 0.0004*T21 + 0.7918)*Radiation!F20),IF(90>T21,((-0.0006*T21^2 + 0.0699*T21 - 1.2225)*Radiation!F20),0))))","v":0},{"$f":"IF(EG21<0,0,IF(0>U21,0,IF(50>U21,(( -0.000009*U21^2 + 0.0004*U21 + 0.7918)*Radiation!G20),IF(90>U21,((-0.0006*U21^2 + 0.0699*U21 - 1.2225)*Radiation!G20),0))))","v":0},{"$f":"IF(EH21<0,0,IF(0>V21,0,IF(50>V21,(( -0.000009*V21^2 + 0.0004*V21 + 0.7918)*Radiation!H20),IF(90>V21,((-0.0006*V21^2 + 0.0699*V21 - 1.2225)*Radiation!H20),0))))","v":0},{"$f":"IF(EI21<0,0,IF(0>W21,0,IF(50>W21,(( -0.000009*W21^2 + 0.0004*W21 + 0.7918)*Radiation!I20),IF(90>W21,((-0.0006*W21^2 + 0.0699*W21 - 1.2225)*Radiation!I20),0))))","v":0},{"$f":"IF(EJ21<0,0,IF(0>X21,0,IF(50>X21,(( -0.000009*X21^2 + 0.0004*X21 + 0.7918)*Radiation!J20),IF(90>X21,((-0.0006*X21^2 + 0.0699*X21 - 1.2225)*Radiation!J20),0))))","v":0},{"$f":"IF(EK21<0,0,IF(0>Y21,0,IF(50>Y21,(( -0.000009*Y21^2 + 0.0004*Y21 + 0.7918)*Radiation!K20),IF(90>Y21,((-0.0006*Y21^2 + 0.0699*Y21 - 1.2225)*Radiation!K20),0))))","v":0},{"$f":"IF(EL21<0,0,IF(0>Z21,0,IF(50>Z21,(( -0.000009*Z21^2 + 0.0004*Z21 + 0.7918)*Radiation!L20),IF(90>Z21,((-0.0006*Z21^2 + 0.0699*Z21 - 1.2225)*Radiation!L20),0))))","v":0},{"$f":"IF(EM21<0,0,IF(0>AA21,0,IF(50>AA21,(( -0.000009*AA21^2 + 0.0004*AA21 + 0.7918)*Radiation!M20),IF(90>AA21,((-0.0006*AA21^2 + 0.0699*AA21 - 1.2225)*Radiation!M20),0))))","v":0},{"$f":"IF(EN21<0,0,IF(0>AB21,0,IF(50>AB21,(( -0.000009*AB21^2 + 0.0004*AB21 + 0.7918)*Radiation!N20),IF(90>AB21,((-0.0006*AB21^2 + 0.0699*AB21 - 1.2225)*Radiation!N20),0))))","v":0},null,null,17,{"$f":"AG21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU21","v":0},{"$f":"AH21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV21","v":0},{"$f":"AI21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW21","v":0},{"$f":"AJ21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX21","v":0},{"$f":"AK21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY21","v":0},{"$f":"AL21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ21","v":0},{"$f":"AM21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA21","v":0},{"$f":"AN21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB21","v":0},{"$f":"AO21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC21","v":0},{"$f":"AP21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD21","v":0},{"$f":"AQ21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE21","v":0},{"$f":"AR21*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF21","v":47.993568038259191},null,17,{"$f":"AU21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI21","v":0},{"$f":"AV21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ21","v":0},{"$f":"AW21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK21","v":0},{"$f":"AX21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL21","v":0},{"$f":"AY21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM21","v":0},{"$f":"AZ21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN21","v":0},{"$f":"BA21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO21","v":0},{"$f":"BB21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP21","v":0},{"$f":"BC21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ21","v":0},{"$f":"BD21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR21","v":0},{"$f":"BE21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS21","v":0},{"$f":"BF21*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT21","v":0},null,17,0,0,0,0,0,0,0,0,0,0,0,5.8907157351308172E-2,null,17,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B20","v":17},{"$f":"'Solar Altitude'!C20","v":8.2848854255444504},{"$f":"'Solar Altitude'!D20","v":13.434807821200849},{"$f":"'Solar Altitude'!E20","v":16.897092448538277},{"$f":"'Solar Altitude'!F20","v":19.80224832363653},{"$f":"'Solar Altitude'!G20","v":22.286756355186323},{"$f":"'Solar Altitude'!H20","v":24.319689951925163},{"$f":"'Solar Altitude'!I20","v":24.456964963286701},{"$f":"'Solar Altitude'!J20","v":20.670382142796534},{"$f":"'Solar Altitude'!K20","v":13.51706337533537},{"$f":"'Solar Altitude'!L20","v":7.0202572324504446},{"$f":"'Solar Altitude'!M20","v":3.1397975005302774},{"$f":"'Solar Altitude'!N20","v":3.9451572875932328},null,17,8.2848854255444504,13.434807821200849,16.897092448538277,19.80224832363653,22.286756355186323,24.319689951925163,24.456964963286701,20.670382142796534,13.51706337533537,7.0202572324504446,3.1397975005302774,3.9451572875932328]
[null,18,{"$f":"DEGREES(C50)","v":70.084429107723579},78.184325624174704,88.472160386966166,100.17034582236116,107.97723057216724,110.320376753952,107.18201187677536,99.98842545866934,90.038304468277545,81.148595232008844,72.673899805332141,68.235388452942999,null,18,{"$f":"DEGREES(Q50)","v":159.59987695565323},168.1807904979741,176.34166666666673,168.00615739830985,159.67834535239979,156.45861971246464,159.2422838674793,167.67094606232226,179.90833333333325,169.10452670079181,160.03314829433953,156.51153378947097,null,null,null,18,{"$f":"IF(DO22<0,0,IF(0>C22,0,IF(50>C22,((-0.000009*C22^2 + 0.0004*C22 + 0.7918)*Radiation!C21),IF(90>C22,(( -0.0006*C22^2 + 0.0699*C22 - 1.2225)*Radiation!C21),0))))","v":0},{"$f":"IF(DP22<0,0,IF(0>D22,0,IF(50>D22,((-0.000009*D22^2 + 0.0004*D22 + 0.7918)*Radiation!D21),IF(90>D22,(( -0.0006*D22^2 + 0.0699*D22 - 1.2225)*Radiation!D21),0))))","v":4.3739040145498933},{"$f":"IF(DQ22<0,0,IF(0>E22,0,IF(50>E22,((-0.000009*E22^2 + 0.0004*E22 + 0.7918)*Radiation!E21),IF(90>E22,(( -0.0006*E22^2 + 0.0699*E22 - 1.2225)*Radiation!E21),0))))","v":3.7005288619737864},{"$f":"IF(DR22<0,0,IF(0>F22,0,IF(50>F22,((-0.000009*F22^2 + 0.0004*F22 + 0.7918)*Radiation!F21),IF(90>F22,(( -0.0006*F22^2 + 0.0699*F22 - 1.2225)*Radiation!F21),0))))","v":0},{"$f":"IF(DS22<0,0,IF(0>G22,0,IF(50>G22,((-0.000009*G22^2 + 0.0004*G22 + 0.7918)*Radiation!G21),IF(90>G22,(( -0.0006*G22^2 + 0.0699*G22 - 1.2225)*Radiation!G21),0))))","v":0},{"$f":"IF(DT22<0,0,IF(0>H22,0,IF(50>H22,((-0.000009*H22^2 + 0.0004*H22 + 0.7918)*Radiation!H21),IF(90>H22,(( -0.0006*H22^2 + 0.0699*H22 - 1.2225)*Radiation!H21),0))))","v":0},{"$f":"IF(DU22<0,0,IF(0>I22,0,IF(50>I22,((-0.000009*I22^2 + 0.0004*I22 + 0.7918)*Radiation!I21),IF(90>I22,(( -0.0006*I22^2 + 0.0699*I22 - 1.2225)*Radiation!I21),0))))","v":0},{"$f":"IF(DV22<0,0,IF(0>J22,0,IF(50>J22,((-0.000009*J22^2 + 0.0004*J22 + 0.7918)*Radiation!J21),IF(90>J22,(( -0.0006*J22^2 + 0.0699*J22 - 1.2225)*Radiation!J21),0))))","v":0},{"$f":"IF(DW22<0,0,IF(0>K22,0,IF(50>K22,((-0.000009*K22^2 + 0.0004*K22 + 0.7918)*Radiation!K21),IF(90>K22,(( -0.0006*K22^2 + 0.0699*K22 - 1.2225)*Radiation!K21),0))))","v":0},{"$f":"IF(DX22<0,0,IF(0>L22,0,IF(50>L22,((-0.000009*L22^2 + 0.0004*L22 + 0.7918)*Radiation!L21),IF(90>L22,(( -0.0006*L22^2 + 0.0699*L22 - 1.2225)*Radiation!L21),0))))","v":0},{"$f":"IF(DY22<0,0,IF(0>M22,0,IF(50>M22,((-0.000009*M22^2 + 0.0004*M22 + 0.7918)*Radiation!M21),IF(90>M22,(( -0.0006*M22^2 + 0.0699*M22 - 1.2225)*Radiation!M21),0))))","v":0},{"$f":"IF(DZ22<0,0,IF(0>N22,0,IF(50>N22,((-0.000009*N22^2 + 0.0004*N22 + 0.7918)*Radiation!N21),IF(90>N22,(( -0.0006*N22^2 + 0.0699*N22 - 1.2225)*Radiation!N21),0))))","v":0},null,18,{"$f":"IF(EC22<0,0,IF(0>Q22,0,IF(50>Q22,(( -0.000009*Q22^2 + 0.0004*Q22 + 0.7918)*Radiation!C21),IF(90>Q22,((-0.0006*Q22^2 + 0.0699*Q22 - 1.2225)*Radiation!C21),0))))","v":0},{"$f":"IF(ED22<0,0,IF(0>R22,0,IF(50>R22,(( -0.000009*R22^2 + 0.0004*R22 + 0.7918)*Radiation!D21),IF(90>R22,((-0.0006*R22^2 + 0.0699*R22 - 1.2225)*Radiation!D21),0))))","v":0},{"$f":"IF(EE22<0,0,IF(0>S22,0,IF(50>S22,(( -0.000009*S22^2 + 0.0004*S22 + 0.7918)*Radiation!E21),IF(90>S22,((-0.0006*S22^2 + 0.0699*S22 - 1.2225)*Radiation!E21),0))))","v":0},{"$f":"IF(EF22<0,0,IF(0>T22,0,IF(50>T22,(( -0.000009*T22^2 + 0.0004*T22 + 0.7918)*Radiation!F21),IF(90>T22,((-0.0006*T22^2 + 0.0699*T22 - 1.2225)*Radiation!F21),0))))","v":0},{"$f":"IF(EG22<0,0,IF(0>U22,0,IF(50>U22,(( -0.000009*U22^2 + 0.0004*U22 + 0.7918)*Radiation!G21),IF(90>U22,((-0.0006*U22^2 + 0.0699*U22 - 1.2225)*Radiation!G21),0))))","v":0},{"$f":"IF(EH22<0,0,IF(0>V22,0,IF(50>V22,(( -0.000009*V22^2 + 0.0004*V22 + 0.7918)*Radiation!H21),IF(90>V22,((-0.0006*V22^2 + 0.0699*V22 - 1.2225)*Radiation!H21),0))))","v":0},{"$f":"IF(EI22<0,0,IF(0>W22,0,IF(50>W22,(( -0.000009*W22^2 + 0.0004*W22 + 0.7918)*Radiation!I21),IF(90>W22,((-0.0006*W22^2 + 0.0699*W22 - 1.2225)*Radiation!I21),0))))","v":0},{"$f":"IF(EJ22<0,0,IF(0>X22,0,IF(50>X22,(( -0.000009*X22^2 + 0.0004*X22 + 0.7918)*Radiation!J21),IF(90>X22,((-0.0006*X22^2 + 0.0699*X22 - 1.2225)*Radiation!J21),0))))","v":0},{"$f":"IF(EK22<0,0,IF(0>Y22,0,IF(50>Y22,(( -0.000009*Y22^2 + 0.0004*Y22 + 0.7918)*Radiation!K21),IF(90>Y22,((-0.0006*Y22^2 + 0.0699*Y22 - 1.2225)*Radiation!K21),0))))","v":0},{"$f":"IF(EL22<0,0,IF(0>Z22,0,IF(50>Z22,(( -0.000009*Z22^2 + 0.0004*Z22 + 0.7918)*Radiation!L21),IF(90>Z22,((-0.0006*Z22^2 + 0.0699*Z22 - 1.2225)*Radiation!L21),0))))","v":0},{"$f":"IF(EM22<0,0,IF(0>AA22,0,IF(50>AA22,(( -0.000009*AA22^2 + 0.0004*AA22 + 0.7918)*Radiation!M21),IF(90>AA22,((-0.0006*AA22^2 + 0.0699*AA22 - 1.2225)*Radiation!M21),0))))","v":0},{"$f":"IF(EN22<0,0,IF(0>AB22,0,IF(50>AB22,(( -0.000009*AB22^2 + 0.0004*AB22 + 0.7918)*Radiation!N21),IF(90>AB22,((-0.0006*AB22^2 + 0.0699*AB22 - 1.2225)*Radiation!N21),0))))","v":0},null,null,18,{"$f":"AG22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU22","v":0},{"$f":"AH22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV22","v":0},{"$f":"AI22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW22","v":0},{"$f":"AJ22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX22","v":0},{"$f":"AK22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY22","v":0},{"$f":"AL22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ22","v":0},{"$f":"AM22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA22","v":0},{"$f":"AN22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB22","v":0},{"$f":"AO22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC22","v":0},{"$f":"AP22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD22","v":0},{"$f":"AQ22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE22","v":0},{"$f":"AR22*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF22","v":0},null,18,{"$f":"AU22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI22","v":0},{"$f":"AV22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ22","v":0},{"$f":"AW22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK22","v":0},{"$f":"AX22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL22","v":0},{"$f":"AY22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM22","v":0},{"$f":"AZ22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN22","v":0},{"$f":"BA22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO22","v":0},{"$f":"BB22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP22","v":0},{"$f":"BC22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ22","v":0},{"$f":"BD22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR22","v":0},{"$f":"BE22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS22","v":0},{"$f":"BF22*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT22","v":0},null,18,0,0,0,0,0,0,0,0,0,0,0,0,null,18,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B21","v":18},{"$f":"'Solar Altitude'!C21","v":-4.242067037456934},{"$f":"'Solar Altitude'!D21","v":0.28496224246637836},{"$f":"'Solar Altitude'!E21","v":3.3232309033445016},{"$f":"'Solar Altitude'!F21","v":6.2903017477886056},{"$f":"'Solar Altitude'!G21","v":9.1618728727979484},{"$f":"'Solar Altitude'!H21","v":11.380032986011807},{"$f":"'Solar Altitude'!I21","v":11.292623329902437},{"$f":"'Solar Altitude'!J21","v":7.1538265372891177},{"$f":"'Solar Altitude'!K21","v":-8.3279910069723753E-2},{"$f":"'Solar Altitude'!L21","v":-6.3024734223343577},{"$f":"'Solar Altitude'!M21","v":-9.6180467382750852},{"$f":"'Solar Altitude'!N21","v":-8.4049479592926772},null,18,-4.242067037456934,0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772]
[null,19,{"$f":"DEGREES(C51)","v":76.219883371952747},84.39773793961092,94.713734410568335,106.42339032670239,114.22259514924912,116.54535536775172,113.41044127974908,106.24145771637895,96.246005842661631,87.238731794104538,78.664821592443701,74.259050105874195,null,19,{"$f":"DEGREES(Q51)","v":157.63688498626229},165.64128127839234,168.65833333333327,162.08351217694067,155.48661671610134,153.42793355434173,156.53753822231249,162.58709776891263,164.9083333333333,159.94140931706841,154.26159820121021,153.07774381747009,null,null,null,19,{"$f":"IF(DO23<0,0,IF(0>C23,0,IF(50>C23,((-0.000009*C23^2 + 0.0004*C23 + 0.7918)*Radiation!C22),IF(90>C23,(( -0.0006*C23^2 + 0.0699*C23 - 1.2225)*Radiation!C22),0))))","v":0},{"$f":"IF(DP23<0,0,IF(0>D23,0,IF(50>D23,((-0.000009*D23^2 + 0.0004*D23 + 0.7918)*Radiation!D22),IF(90>D23,(( -0.0006*D23^2 + 0.0699*D23 - 1.2225)*Radiation!D22),0))))","v":0},{"$f":"IF(DQ23<0,0,IF(0>E23,0,IF(50>E23,((-0.000009*E23^2 + 0.0004*E23 + 0.7918)*Radiation!E22),IF(90>E23,(( -0.0006*E23^2 + 0.0699*E23 - 1.2225)*Radiation!E22),0))))","v":0},{"$f":"IF(DR23<0,0,IF(0>F23,0,IF(50>F23,((-0.000009*F23^2 + 0.0004*F23 + 0.7918)*Radiation!F22),IF(90>F23,(( -0.0006*F23^2 + 0.0699*F23 - 1.2225)*Radiation!F22),0))))","v":0},{"$f":"IF(DS23<0,0,IF(0>G23,0,IF(50>G23,((-0.000009*G23^2 + 0.0004*G23 + 0.7918)*Radiation!G22),IF(90>G23,(( -0.0006*G23^2 + 0.0699*G23 - 1.2225)*Radiation!G22),0))))","v":0},{"$f":"IF(DT23<0,0,IF(0>H23,0,IF(50>H23,((-0.000009*H23^2 + 0.0004*H23 + 0.7918)*Radiation!H22),IF(90>H23,(( -0.0006*H23^2 + 0.0699*H23 - 1.2225)*Radiation!H22),0))))","v":0},{"$f":"IF(DU23<0,0,IF(0>I23,0,IF(50>I23,((-0.000009*I23^2 + 0.0004*I23 + 0.7918)*Radiation!I22),IF(90>I23,(( -0.0006*I23^2 + 0.0699*I23 - 1.2225)*Radiation!I22),0))))","v":0},{"$f":"IF(DV23<0,0,IF(0>J23,0,IF(50>J23,((-0.000009*J23^2 + 0.0004*J23 + 0.7918)*Radiation!J22),IF(90>J23,(( -0.0006*J23^2 + 0.0699*J23 - 1.2225)*Radiation!J22),0))))","v":0},{"$f":"IF(DW23<0,0,IF(0>K23,0,IF(50>K23,((-0.000009*K23^2 + 0.0004*K23 + 0.7918)*Radiation!K22),IF(90>K23,(( -0.0006*K23^2 + 0.0699*K23 - 1.2225)*Radiation!K22),0))))","v":0},{"$f":"IF(DX23<0,0,IF(0>L23,0,IF(50>L23,((-0.000009*L23^2 + 0.0004*L23 + 0.7918)*Radiation!L22),IF(90>L23,(( -0.0006*L23^2 + 0.0699*L23 - 1.2225)*Radiation!L22),0))))","v":0},{"$f":"IF(DY23<0,0,IF(0>M23,0,IF(50>M23,((-0.000009*M23^2 + 0.0004*M23 + 0.7918)*Radiation!M22),IF(90>M23,(( -0.0006*M23^2 + 0.0699*M23 - 1.2225)*Radiation!M22),0))))","v":0},{"$f":"IF(DZ23<0,0,IF(0>N23,0,IF(50>N23,((-0.000009*N23^2 + 0.0004*N23 + 0.7918)*Radiation!N22),IF(90>N23,(( -0.0006*N23^2 + 0.0699*N23 - 1.2225)*Radiation!N22),0))))","v":0},null,19,{"$f":"IF(EC23<0,0,IF(0>Q23,0,IF(50>Q23,(( -0.000009*Q23^2 + 0.0004*Q23 + 0.7918)*Radiation!C22),IF(90>Q23,((-0.0006*Q23^2 + 0.0699*Q23 - 1.2225)*Radiation!C22),0))))","v":0},{"$f":"IF(ED23<0,0,IF(0>R23,0,IF(50>R23,(( -0.000009*R23^2 + 0.0004*R23 + 0.7918)*Radiation!D22),IF(90>R23,((-0.0006*R23^2 + 0.0699*R23 - 1.2225)*Radiation!D22),0))))","v":0},{"$f":"IF(EE23<0,0,IF(0>S23,0,IF(50>S23,(( -0.000009*S23^2 + 0.0004*S23 + 0.7918)*Radiation!E22),IF(90>S23,((-0.0006*S23^2 + 0.0699*S23 - 1.2225)*Radiation!E22),0))))","v":0},{"$f":"IF(EF23<0,0,IF(0>T23,0,IF(50>T23,(( -0.000009*T23^2 + 0.0004*T23 + 0.7918)*Radiation!F22),IF(90>T23,((-0.0006*T23^2 + 0.0699*T23 - 1.2225)*Radiation!F22),0))))","v":0},{"$f":"IF(EG23<0,0,IF(0>U23,0,IF(50>U23,(( -0.000009*U23^2 + 0.0004*U23 + 0.7918)*Radiation!G22),IF(90>U23,((-0.0006*U23^2 + 0.0699*U23 - 1.2225)*Radiation!G22),0))))","v":0},{"$f":"IF(EH23<0,0,IF(0>V23,0,IF(50>V23,(( -0.000009*V23^2 + 0.0004*V23 + 0.7918)*Radiation!H22),IF(90>V23,((-0.0006*V23^2 + 0.0699*V23 - 1.2225)*Radiation!H22),0))))","v":0},{"$f":"IF(EI23<0,0,IF(0>W23,0,IF(50>W23,(( -0.000009*W23^2 + 0.0004*W23 + 0.7918)*Radiation!I22),IF(90>W23,((-0.0006*W23^2 + 0.0699*W23 - 1.2225)*Radiation!I22),0))))","v":0},{"$f":"IF(EJ23<0,0,IF(0>X23,0,IF(50>X23,(( -0.000009*X23^2 + 0.0004*X23 + 0.7918)*Radiation!J22),IF(90>X23,((-0.0006*X23^2 + 0.0699*X23 - 1.2225)*Radiation!J22),0))))","v":0},{"$f":"IF(EK23<0,0,IF(0>Y23,0,IF(50>Y23,(( -0.000009*Y23^2 + 0.0004*Y23 + 0.7918)*Radiation!K22),IF(90>Y23,((-0.0006*Y23^2 + 0.0699*Y23 - 1.2225)*Radiation!K22),0))))","v":0},{"$f":"IF(EL23<0,0,IF(0>Z23,0,IF(50>Z23,(( -0.000009*Z23^2 + 0.0004*Z23 + 0.7918)*Radiation!L22),IF(90>Z23,((-0.0006*Z23^2 + 0.0699*Z23 - 1.2225)*Radiation!L22),0))))","v":0},{"$f":"IF(EM23<0,0,IF(0>AA23,0,IF(50>AA23,(( -0.000009*AA23^2 + 0.0004*AA23 + 0.7918)*Radiation!M22),IF(90>AA23,((-0.0006*AA23^2 + 0.0699*AA23 - 1.2225)*Radiation!M22),0))))","v":0},{"$f":"IF(EN23<0,0,IF(0>AB23,0,IF(50>AB23,(( -0.000009*AB23^2 + 0.0004*AB23 + 0.7918)*Radiation!N22),IF(90>AB23,((-0.0006*AB23^2 + 0.0699*AB23 - 1.2225)*Radiation!N22),0))))","v":0},null,null,19,{"$f":"AG23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU23","v":0},{"$f":"AH23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV23","v":0},{"$f":"AI23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW23","v":0},{"$f":"AJ23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX23","v":0},{"$f":"AK23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY23","v":0},{"$f":"AL23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ23","v":0},{"$f":"AM23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA23","v":0},{"$f":"AN23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB23","v":0},{"$f":"AO23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC23","v":0},{"$f":"AP23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD23","v":0},{"$f":"AQ23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE23","v":0},{"$f":"AR23*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF23","v":0},null,19,{"$f":"AU23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI23","v":0},{"$f":"AV23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ23","v":0},{"$f":"AW23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK23","v":0},{"$f":"AX23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL23","v":0},{"$f":"AY23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM23","v":0},{"$f":"AZ23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN23","v":0},{"$f":"BA23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO23","v":0},{"$f":"BB23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP23","v":0},{"$f":"BC23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ23","v":0},{"$f":"BD23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR23","v":0},{"$f":"BE23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS23","v":0},{"$f":"BF23*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT23","v":0},null,19,0,0,0,0,0,0,0,0,0,0,0,0,null,19,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B22","v":19},{"$f":"'Solar Altitude'!C22","v":-17.258784755357599},{"$f":"'Solar Altitude'!D22","v":-13.177535073458104},{"$f":"'Solar Altitude'!E22","v":-10.292097151668569},{"$f":"'Solar Altitude'!F22","v":-6.9635212465343193},{"$f":"'Solar Altitude'!G22","v":-3.5411252469823715},{"$f":"'Solar Altitude'!H22","v":-1.1064784283971907},{"$f":"'Solar Altitude'!I22","v":-1.4750612815819091},{"$f":"'Solar Altitude'!J22","v":-6.1102162570653853},{"$f":"'Solar Altitude'!K22","v":-13.682588857300294},{"$f":"'Solar Altitude'!L22","v":-19.851334869589788},{"$f":"'Solar Altitude'!M22","v":-22.782734775346487},{"$f":"'Solar Altitude'!N22","v":-21.2544074674176},null,19,-17.258784755357599,-13.177535073458104,-10.292097151668569,-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176]
[null,20,{"$f":"DEGREES(C52)","v":81.917483465874284},90.274058176596213,100.68545928652114,112.48179037227587,120.36097961903782,122.7330362532708,119.59251501071874,112.32380793152561,102.09376987845592,92.826460586959826,84.089996953970044,79.750612677212175,null,20,{"$f":"DEGREES(Q52)","v":148.13323739219496},153.21525979942476,153.65833333333327,149.31639654713646,145.08131660023744,144.19600228883124,146.82894645510487,150.04102520570484,149.9083333333333,146.37673625967992,143.1582726356977,143.64315809950045,null,null,null,20,{"$f":"IF(DO24<0,0,IF(0>C24,0,IF(50>C24,((-0.000009*C24^2 + 0.0004*C24 + 0.7918)*Radiation!C23),IF(90>C24,(( -0.0006*C24^2 + 0.0699*C24 - 1.2225)*Radiation!C23),0))))","v":0},{"$f":"IF(DP24<0,0,IF(0>D24,0,IF(50>D24,((-0.000009*D24^2 + 0.0004*D24 + 0.7918)*Radiation!D23),IF(90>D24,(( -0.0006*D24^2 + 0.0699*D24 - 1.2225)*Radiation!D23),0))))","v":0},{"$f":"IF(DQ24<0,0,IF(0>E24,0,IF(50>E24,((-0.000009*E24^2 + 0.0004*E24 + 0.7918)*Radiation!E23),IF(90>E24,(( -0.0006*E24^2 + 0.0699*E24 - 1.2225)*Radiation!E23),0))))","v":0},{"$f":"IF(DR24<0,0,IF(0>F24,0,IF(50>F24,((-0.000009*F24^2 + 0.0004*F24 + 0.7918)*Radiation!F23),IF(90>F24,(( -0.0006*F24^2 + 0.0699*F24 - 1.2225)*Radiation!F23),0))))","v":0},{"$f":"IF(DS24<0,0,IF(0>G24,0,IF(50>G24,((-0.000009*G24^2 + 0.0004*G24 + 0.7918)*Radiation!G23),IF(90>G24,(( -0.0006*G24^2 + 0.0699*G24 - 1.2225)*Radiation!G23),0))))","v":0},{"$f":"IF(DT24<0,0,IF(0>H24,0,IF(50>H24,((-0.000009*H24^2 + 0.0004*H24 + 0.7918)*Radiation!H23),IF(90>H24,(( -0.0006*H24^2 + 0.0699*H24 - 1.2225)*Radiation!H23),0))))","v":0},{"$f":"IF(DU24<0,0,IF(0>I24,0,IF(50>I24,((-0.000009*I24^2 + 0.0004*I24 + 0.7918)*Radiation!I23),IF(90>I24,(( -0.0006*I24^2 + 0.0699*I24 - 1.2225)*Radiation!I23),0))))","v":0},{"$f":"IF(DV24<0,0,IF(0>J24,0,IF(50>J24,((-0.000009*J24^2 + 0.0004*J24 + 0.7918)*Radiation!J23),IF(90>J24,(( -0.0006*J24^2 + 0.0699*J24 - 1.2225)*Radiation!J23),0))))","v":0},{"$f":"IF(DW24<0,0,IF(0>K24,0,IF(50>K24,((-0.000009*K24^2 + 0.0004*K24 + 0.7918)*Radiation!K23),IF(90>K24,(( -0.0006*K24^2 + 0.0699*K24 - 1.2225)*Radiation!K23),0))))","v":0},{"$f":"IF(DX24<0,0,IF(0>L24,0,IF(50>L24,((-0.000009*L24^2 + 0.0004*L24 + 0.7918)*Radiation!L23),IF(90>L24,(( -0.0006*L24^2 + 0.0699*L24 - 1.2225)*Radiation!L23),0))))","v":0},{"$f":"IF(DY24<0,0,IF(0>M24,0,IF(50>M24,((-0.000009*M24^2 + 0.0004*M24 + 0.7918)*Radiation!M23),IF(90>M24,(( -0.0006*M24^2 + 0.0699*M24 - 1.2225)*Radiation!M23),0))))","v":0},{"$f":"IF(DZ24<0,0,IF(0>N24,0,IF(50>N24,((-0.000009*N24^2 + 0.0004*N24 + 0.7918)*Radiation!N23),IF(90>N24,(( -0.0006*N24^2 + 0.0699*N24 - 1.2225)*Radiation!N23),0))))","v":0},null,20,{"$f":"IF(EC24<0,0,IF(0>Q24,0,IF(50>Q24,(( -0.000009*Q24^2 + 0.0004*Q24 + 0.7918)*Radiation!C23),IF(90>Q24,((-0.0006*Q24^2 + 0.0699*Q24 - 1.2225)*Radiation!C23),0))))","v":0},{"$f":"IF(ED24<0,0,IF(0>R24,0,IF(50>R24,(( -0.000009*R24^2 + 0.0004*R24 + 0.7918)*Radiation!D23),IF(90>R24,((-0.0006*R24^2 + 0.0699*R24 - 1.2225)*Radiation!D23),0))))","v":0},{"$f":"IF(EE24<0,0,IF(0>S24,0,IF(50>S24,(( -0.000009*S24^2 + 0.0004*S24 + 0.7918)*Radiation!E23),IF(90>S24,((-0.0006*S24^2 + 0.0699*S24 - 1.2225)*Radiation!E23),0))))","v":0},{"$f":"IF(EF24<0,0,IF(0>T24,0,IF(50>T24,(( -0.000009*T24^2 + 0.0004*T24 + 0.7918)*Radiation!F23),IF(90>T24,((-0.0006*T24^2 + 0.0699*T24 - 1.2225)*Radiation!F23),0))))","v":0},{"$f":"IF(EG24<0,0,IF(0>U24,0,IF(50>U24,(( -0.000009*U24^2 + 0.0004*U24 + 0.7918)*Radiation!G23),IF(90>U24,((-0.0006*U24^2 + 0.0699*U24 - 1.2225)*Radiation!G23),0))))","v":0},{"$f":"IF(EH24<0,0,IF(0>V24,0,IF(50>V24,(( -0.000009*V24^2 + 0.0004*V24 + 0.7918)*Radiation!H23),IF(90>V24,((-0.0006*V24^2 + 0.0699*V24 - 1.2225)*Radiation!H23),0))))","v":0},{"$f":"IF(EI24<0,0,IF(0>W24,0,IF(50>W24,(( -0.000009*W24^2 + 0.0004*W24 + 0.7918)*Radiation!I23),IF(90>W24,((-0.0006*W24^2 + 0.0699*W24 - 1.2225)*Radiation!I23),0))))","v":0},{"$f":"IF(EJ24<0,0,IF(0>X24,0,IF(50>X24,(( -0.000009*X24^2 + 0.0004*X24 + 0.7918)*Radiation!J23),IF(90>X24,((-0.0006*X24^2 + 0.0699*X24 - 1.2225)*Radiation!J23),0))))","v":0},{"$f":"IF(EK24<0,0,IF(0>Y24,0,IF(50>Y24,(( -0.000009*Y24^2 + 0.0004*Y24 + 0.7918)*Radiation!K23),IF(90>Y24,((-0.0006*Y24^2 + 0.0699*Y24 - 1.2225)*Radiation!K23),0))))","v":0},{"$f":"IF(EL24<0,0,IF(0>Z24,0,IF(50>Z24,(( -0.000009*Z24^2 + 0.0004*Z24 + 0.7918)*Radiation!L23),IF(90>Z24,((-0.0006*Z24^2 + 0.0699*Z24 - 1.2225)*Radiation!L23),0))))","v":0},{"$f":"IF(EM24<0,0,IF(0>AA24,0,IF(50>AA24,(( -0.000009*AA24^2 + 0.0004*AA24 + 0.7918)*Radiation!M23),IF(90>AA24,((-0.0006*AA24^2 + 0.0699*AA24 - 1.2225)*Radiation!M23),0))))","v":0},{"$f":"IF(EN24<0,0,IF(0>AB24,0,IF(50>AB24,(( -0.000009*AB24^2 + 0.0004*AB24 + 0.7918)*Radiation!N23),IF(90>AB24,((-0.0006*AB24^2 + 0.0699*AB24 - 1.2225)*Radiation!N23),0))))","v":0},null,null,20,{"$f":"AG24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU24","v":0},{"$f":"AH24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV24","v":0},{"$f":"AI24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW24","v":0},{"$f":"AJ24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX24","v":0},{"$f":"AK24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY24","v":0},{"$f":"AL24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ24","v":0},{"$f":"AM24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA24","v":0},{"$f":"AN24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB24","v":0},{"$f":"AO24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC24","v":0},{"$f":"AP24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD24","v":0},{"$f":"AQ24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE24","v":0},{"$f":"AR24*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF24","v":0},null,20,{"$f":"AU24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI24","v":0},{"$f":"AV24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ24","v":0},{"$f":"AW24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK24","v":0},{"$f":"AX24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL24","v":0},{"$f":"AY24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM24","v":0},{"$f":"AZ24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN24","v":0},{"$f":"BA24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO24","v":0},{"$f":"BB24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP24","v":0},{"$f":"BC24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ24","v":0},{"$f":"BD24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR24","v":0},{"$f":"BE24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS24","v":0},{"$f":"BF24*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT24","v":0},null,20,0,0,0,0,0,0,0,0,0,0,0,0,null,20,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B23","v":20},{"$f":"'Solar Altitude'!C23","v":-30.589239677830651},{"$f":"'Solar Altitude'!D23","v":-26.783110901661868},{"$f":"'Solar Altitude'!E23","v":-23.773745192987072},{"$f":"'Solar Altitude'!F23","v":-19.749387170381588},{"$f":"'Solar Altitude'!G23","v":-15.584861719885295},{"$f":"'Solar Altitude'!H23","v":-12.902247652391463},{"$f":"'Solar Altitude'!I23","v":-13.625605199002544},{"$f":"'Solar Altitude'!J23","v":-18.916708643772196},{"$f":"'Solar Altitude'!K23","v":-27.097900221004799},{"$f":"'Solar Altitude'!L23","v":-33.472019280706604},{"$f":"'Solar Altitude'!M23","v":-36.206670576844481},{"$f":"'Solar Altitude'!N23","v":-34.435555539572299},null,20,-30.589239677830651,-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,-12.902247652391463,-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299]
[null,21,{"$f":"DEGREES(C53)","v":86.876161796875635},95.478577975373568,106.02287954007556,117.95345081372363,125.99002534742664,128.48674388860007,125.33600255518053,117.84543463198899,107.21445179579572,97.581766197424642,88.656791446324078,84.428369662526421,null,21,{"$f":"DEGREES(Q53)","v":135.71603163262762},139.09647815180844,138.6583333333333,135.2254208933719,132.39103758245213,132.25285571248878,134.40435211228029,136.01740948977312,134.90833333333333,132.0133459626033,130.18553699274204,131.61920109776079,null,null,null,21,{"$f":"IF(DO25<0,0,IF(0>C25,0,IF(50>C25,((-0.000009*C25^2 + 0.0004*C25 + 0.7918)*Radiation!C24),IF(90>C25,(( -0.0006*C25^2 + 0.0699*C25 - 1.2225)*Radiation!C24),0))))","v":0},{"$f":"IF(DP25<0,0,IF(0>D25,0,IF(50>D25,((-0.000009*D25^2 + 0.0004*D25 + 0.7918)*Radiation!D24),IF(90>D25,(( -0.0006*D25^2 + 0.0699*D25 - 1.2225)*Radiation!D24),0))))","v":0},{"$f":"IF(DQ25<0,0,IF(0>E25,0,IF(50>E25,((-0.000009*E25^2 + 0.0004*E25 + 0.7918)*Radiation!E24),IF(90>E25,(( -0.0006*E25^2 + 0.0699*E25 - 1.2225)*Radiation!E24),0))))","v":0},{"$f":"IF(DR25<0,0,IF(0>F25,0,IF(50>F25,((-0.000009*F25^2 + 0.0004*F25 + 0.7918)*Radiation!F24),IF(90>F25,(( -0.0006*F25^2 + 0.0699*F25 - 1.2225)*Radiation!F24),0))))","v":0},{"$f":"IF(DS25<0,0,IF(0>G25,0,IF(50>G25,((-0.000009*G25^2 + 0.0004*G25 + 0.7918)*Radiation!G24),IF(90>G25,(( -0.0006*G25^2 + 0.0699*G25 - 1.2225)*Radiation!G24),0))))","v":0},{"$f":"IF(DT25<0,0,IF(0>H25,0,IF(50>H25,((-0.000009*H25^2 + 0.0004*H25 + 0.7918)*Radiation!H24),IF(90>H25,(( -0.0006*H25^2 + 0.0699*H25 - 1.2225)*Radiation!H24),0))))","v":0},{"$f":"IF(DU25<0,0,IF(0>I25,0,IF(50>I25,((-0.000009*I25^2 + 0.0004*I25 + 0.7918)*Radiation!I24),IF(90>I25,(( -0.0006*I25^2 + 0.0699*I25 - 1.2225)*Radiation!I24),0))))","v":0},{"$f":"IF(DV25<0,0,IF(0>J25,0,IF(50>J25,((-0.000009*J25^2 + 0.0004*J25 + 0.7918)*Radiation!J24),IF(90>J25,(( -0.0006*J25^2 + 0.0699*J25 - 1.2225)*Radiation!J24),0))))","v":0},{"$f":"IF(DW25<0,0,IF(0>K25,0,IF(50>K25,((-0.000009*K25^2 + 0.0004*K25 + 0.7918)*Radiation!K24),IF(90>K25,(( -0.0006*K25^2 + 0.0699*K25 - 1.2225)*Radiation!K24),0))))","v":0},{"$f":"IF(DX25<0,0,IF(0>L25,0,IF(50>L25,((-0.000009*L25^2 + 0.0004*L25 + 0.7918)*Radiation!L24),IF(90>L25,(( -0.0006*L25^2 + 0.0699*L25 - 1.2225)*Radiation!L24),0))))","v":0},{"$f":"IF(DY25<0,0,IF(0>M25,0,IF(50>M25,((-0.000009*M25^2 + 0.0004*M25 + 0.7918)*Radiation!M24),IF(90>M25,(( -0.0006*M25^2 + 0.0699*M25 - 1.2225)*Radiation!M24),0))))","v":0},{"$f":"IF(DZ25<0,0,IF(0>N25,0,IF(50>N25,((-0.000009*N25^2 + 0.0004*N25 + 0.7918)*Radiation!N24),IF(90>N25,(( -0.0006*N25^2 + 0.0699*N25 - 1.2225)*Radiation!N24),0))))","v":0},null,21,{"$f":"IF(EC25<0,0,IF(0>Q25,0,IF(50>Q25,(( -0.000009*Q25^2 + 0.0004*Q25 + 0.7918)*Radiation!C24),IF(90>Q25,((-0.0006*Q25^2 + 0.0699*Q25 - 1.2225)*Radiation!C24),0))))","v":0},{"$f":"IF(ED25<0,0,IF(0>R25,0,IF(50>R25,(( -0.000009*R25^2 + 0.0004*R25 + 0.7918)*Radiation!D24),IF(90>R25,((-0.0006*R25^2 + 0.0699*R25 - 1.2225)*Radiation!D24),0))))","v":0},{"$f":"IF(EE25<0,0,IF(0>S25,0,IF(50>S25,(( -0.000009*S25^2 + 0.0004*S25 + 0.7918)*Radiation!E24),IF(90>S25,((-0.0006*S25^2 + 0.0699*S25 - 1.2225)*Radiation!E24),0))))","v":0},{"$f":"IF(EF25<0,0,IF(0>T25,0,IF(50>T25,(( -0.000009*T25^2 + 0.0004*T25 + 0.7918)*Radiation!F24),IF(90>T25,((-0.0006*T25^2 + 0.0699*T25 - 1.2225)*Radiation!F24),0))))","v":0},{"$f":"IF(EG25<0,0,IF(0>U25,0,IF(50>U25,(( -0.000009*U25^2 + 0.0004*U25 + 0.7918)*Radiation!G24),IF(90>U25,((-0.0006*U25^2 + 0.0699*U25 - 1.2225)*Radiation!G24),0))))","v":0},{"$f":"IF(EH25<0,0,IF(0>V25,0,IF(50>V25,(( -0.000009*V25^2 + 0.0004*V25 + 0.7918)*Radiation!H24),IF(90>V25,((-0.0006*V25^2 + 0.0699*V25 - 1.2225)*Radiation!H24),0))))","v":0},{"$f":"IF(EI25<0,0,IF(0>W25,0,IF(50>W25,(( -0.000009*W25^2 + 0.0004*W25 + 0.7918)*Radiation!I24),IF(90>W25,((-0.0006*W25^2 + 0.0699*W25 - 1.2225)*Radiation!I24),0))))","v":0},{"$f":"IF(EJ25<0,0,IF(0>X25,0,IF(50>X25,(( -0.000009*X25^2 + 0.0004*X25 + 0.7918)*Radiation!J24),IF(90>X25,((-0.0006*X25^2 + 0.0699*X25 - 1.2225)*Radiation!J24),0))))","v":0},{"$f":"IF(EK25<0,0,IF(0>Y25,0,IF(50>Y25,(( -0.000009*Y25^2 + 0.0004*Y25 + 0.7918)*Radiation!K24),IF(90>Y25,((-0.0006*Y25^2 + 0.0699*Y25 - 1.2225)*Radiation!K24),0))))","v":0},{"$f":"IF(EL25<0,0,IF(0>Z25,0,IF(50>Z25,(( -0.000009*Z25^2 + 0.0004*Z25 + 0.7918)*Radiation!L24),IF(90>Z25,((-0.0006*Z25^2 + 0.0699*Z25 - 1.2225)*Radiation!L24),0))))","v":0},{"$f":"IF(EM25<0,0,IF(0>AA25,0,IF(50>AA25,(( -0.000009*AA25^2 + 0.0004*AA25 + 0.7918)*Radiation!M24),IF(90>AA25,((-0.0006*AA25^2 + 0.0699*AA25 - 1.2225)*Radiation!M24),0))))","v":0},{"$f":"IF(EN25<0,0,IF(0>AB25,0,IF(50>AB25,(( -0.000009*AB25^2 + 0.0004*AB25 + 0.7918)*Radiation!N24),IF(90>AB25,((-0.0006*AB25^2 + 0.0699*AB25 - 1.2225)*Radiation!N24),0))))","v":0},null,null,21,{"$f":"AG25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU25","v":0},{"$f":"AH25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV25","v":0},{"$f":"AI25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW25","v":0},{"$f":"AJ25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX25","v":0},{"$f":"AK25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY25","v":0},{"$f":"AL25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ25","v":0},{"$f":"AM25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA25","v":0},{"$f":"AN25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB25","v":0},{"$f":"AO25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC25","v":0},{"$f":"AP25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD25","v":0},{"$f":"AQ25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE25","v":0},{"$f":"AR25*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF25","v":0},null,21,{"$f":"AU25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI25","v":0},{"$f":"AV25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ25","v":0},{"$f":"AW25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK25","v":0},{"$f":"AX25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL25","v":0},{"$f":"AY25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM25","v":0},{"$f":"AZ25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN25","v":0},{"$f":"BA25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO25","v":0},{"$f":"BB25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP25","v":0},{"$f":"BC25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ25","v":0},{"$f":"BD25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR25","v":0},{"$f":"BE25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS25","v":0},{"$f":"BF25*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT25","v":0},null,21,0,0,0,0,0,0,0,0,0,0,0,0,null,21,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B24","v":21},{"$f":"'Solar Altitude'!C24","v":-44.11375465474292},{"$f":"'Solar Altitude'!D24","v":-40.375142281624065},{"$f":"'Solar Altitude'!E24","v":-36.877998514340369},{"$f":"'Solar Altitude'!F24","v":-31.713766855869693},{"$f":"'Solar Altitude'!G24","v":-26.575515215416551},{"$f":"'Solar Altitude'!H24","v":-23.623016903493113},{"$f":"'Solar Altitude'!I24","v":-24.79570873532365},{"$f":"'Solar Altitude'!J24","v":-30.92280247893752},{"$f":"'Solar Altitude'!K24","v":-40.048756889246128},{"$f":"'Solar Altitude'!L24","v":-46.985407153208357},{"$f":"'Solar Altitude'!M24","v":-49.782532508401836},{"$f":"'Solar Altitude'!N24","v":-47.837496220337762},null,21,-44.11375465474292,-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762]
[null,22,{"$f":"DEGREES(C54)","v":90.81650842422502},99.687164569818719,110.35371355363357,122.40770431955607,130.63783856344438,133.32761112969368,130.17916742311377,122.37662161719899,111.23643107049956,101.19122104399018,92.097902171541335,88.036147231117496,null,22,{"$f":"DEGREES(Q54)","v":122.25657509727932},124.5700332372281,123.65833333333329,120.7565201267504,118.84643748288636,119.20666482557664,120.97805808445801,121.57957777098981,119.9083333333333,117.40640051600549,116.5040513810781,118.53858289990021,null,null,null,22,{"$f":"IF(DO26<0,0,IF(0>C26,0,IF(50>C26,((-0.000009*C26^2 + 0.0004*C26 + 0.7918)*Radiation!C25),IF(90>C26,(( -0.0006*C26^2 + 0.0699*C26 - 1.2225)*Radiation!C25),0))))","v":0},{"$f":"IF(DP26<0,0,IF(0>D26,0,IF(50>D26,((-0.000009*D26^2 + 0.0004*D26 + 0.7918)*Radiation!D25),IF(90>D26,(( -0.0006*D26^2 + 0.0699*D26 - 1.2225)*Radiation!D25),0))))","v":0},{"$f":"IF(DQ26<0,0,IF(0>E26,0,IF(50>E26,((-0.000009*E26^2 + 0.0004*E26 + 0.7918)*Radiation!E25),IF(90>E26,(( -0.0006*E26^2 + 0.0699*E26 - 1.2225)*Radiation!E25),0))))","v":0},{"$f":"IF(DR26<0,0,IF(0>F26,0,IF(50>F26,((-0.000009*F26^2 + 0.0004*F26 + 0.7918)*Radiation!F25),IF(90>F26,(( -0.0006*F26^2 + 0.0699*F26 - 1.2225)*Radiation!F25),0))))","v":0},{"$f":"IF(DS26<0,0,IF(0>G26,0,IF(50>G26,((-0.000009*G26^2 + 0.0004*G26 + 0.7918)*Radiation!G25),IF(90>G26,(( -0.0006*G26^2 + 0.0699*G26 - 1.2225)*Radiation!G25),0))))","v":0},{"$f":"IF(DT26<0,0,IF(0>H26,0,IF(50>H26,((-0.000009*H26^2 + 0.0004*H26 + 0.7918)*Radiation!H25),IF(90>H26,(( -0.0006*H26^2 + 0.0699*H26 - 1.2225)*Radiation!H25),0))))","v":0},{"$f":"IF(DU26<0,0,IF(0>I26,0,IF(50>I26,((-0.000009*I26^2 + 0.0004*I26 + 0.7918)*Radiation!I25),IF(90>I26,(( -0.0006*I26^2 + 0.0699*I26 - 1.2225)*Radiation!I25),0))))","v":0},{"$f":"IF(DV26<0,0,IF(0>J26,0,IF(50>J26,((-0.000009*J26^2 + 0.0004*J26 + 0.7918)*Radiation!J25),IF(90>J26,(( -0.0006*J26^2 + 0.0699*J26 - 1.2225)*Radiation!J25),0))))","v":0},{"$f":"IF(DW26<0,0,IF(0>K26,0,IF(50>K26,((-0.000009*K26^2 + 0.0004*K26 + 0.7918)*Radiation!K25),IF(90>K26,(( -0.0006*K26^2 + 0.0699*K26 - 1.2225)*Radiation!K25),0))))","v":0},{"$f":"IF(DX26<0,0,IF(0>L26,0,IF(50>L26,((-0.000009*L26^2 + 0.0004*L26 + 0.7918)*Radiation!L25),IF(90>L26,(( -0.0006*L26^2 + 0.0699*L26 - 1.2225)*Radiation!L25),0))))","v":0},{"$f":"IF(DY26<0,0,IF(0>M26,0,IF(50>M26,((-0.000009*M26^2 + 0.0004*M26 + 0.7918)*Radiation!M25),IF(90>M26,(( -0.0006*M26^2 + 0.0699*M26 - 1.2225)*Radiation!M25),0))))","v":0},{"$f":"IF(DZ26<0,0,IF(0>N26,0,IF(50>N26,((-0.000009*N26^2 + 0.0004*N26 + 0.7918)*Radiation!N25),IF(90>N26,(( -0.0006*N26^2 + 0.0699*N26 - 1.2225)*Radiation!N25),0))))","v":0},null,22,{"$f":"IF(EC26<0,0,IF(0>Q26,0,IF(50>Q26,(( -0.000009*Q26^2 + 0.0004*Q26 + 0.7918)*Radiation!C25),IF(90>Q26,((-0.0006*Q26^2 + 0.0699*Q26 - 1.2225)*Radiation!C25),0))))","v":0},{"$f":"IF(ED26<0,0,IF(0>R26,0,IF(50>R26,(( -0.000009*R26^2 + 0.0004*R26 + 0.7918)*Radiation!D25),IF(90>R26,((-0.0006*R26^2 + 0.0699*R26 - 1.2225)*Radiation!D25),0))))","v":0},{"$f":"IF(EE26<0,0,IF(0>S26,0,IF(50>S26,(( -0.000009*S26^2 + 0.0004*S26 + 0.7918)*Radiation!E25),IF(90>S26,((-0.0006*S26^2 + 0.0699*S26 - 1.2225)*Radiation!E25),0))))","v":0},{"$f":"IF(EF26<0,0,IF(0>T26,0,IF(50>T26,(( -0.000009*T26^2 + 0.0004*T26 + 0.7918)*Radiation!F25),IF(90>T26,((-0.0006*T26^2 + 0.0699*T26 - 1.2225)*Radiation!F25),0))))","v":0},{"$f":"IF(EG26<0,0,IF(0>U26,0,IF(50>U26,(( -0.000009*U26^2 + 0.0004*U26 + 0.7918)*Radiation!G25),IF(90>U26,((-0.0006*U26^2 + 0.0699*U26 - 1.2225)*Radiation!G25),0))))","v":0},{"$f":"IF(EH26<0,0,IF(0>V26,0,IF(50>V26,(( -0.000009*V26^2 + 0.0004*V26 + 0.7918)*Radiation!H25),IF(90>V26,((-0.0006*V26^2 + 0.0699*V26 - 1.2225)*Radiation!H25),0))))","v":0},{"$f":"IF(EI26<0,0,IF(0>W26,0,IF(50>W26,(( -0.000009*W26^2 + 0.0004*W26 + 0.7918)*Radiation!I25),IF(90>W26,((-0.0006*W26^2 + 0.0699*W26 - 1.2225)*Radiation!I25),0))))","v":0},{"$f":"IF(EJ26<0,0,IF(0>X26,0,IF(50>X26,(( -0.000009*X26^2 + 0.0004*X26 + 0.7918)*Radiation!J25),IF(90>X26,((-0.0006*X26^2 + 0.0699*X26 - 1.2225)*Radiation!J25),0))))","v":0},{"$f":"IF(EK26<0,0,IF(0>Y26,0,IF(50>Y26,(( -0.000009*Y26^2 + 0.0004*Y26 + 0.7918)*Radiation!K25),IF(90>Y26,((-0.0006*Y26^2 + 0.0699*Y26 - 1.2225)*Radiation!K25),0))))","v":0},{"$f":"IF(EL26<0,0,IF(0>Z26,0,IF(50>Z26,(( -0.000009*Z26^2 + 0.0004*Z26 + 0.7918)*Radiation!L25),IF(90>Z26,((-0.0006*Z26^2 + 0.0699*Z26 - 1.2225)*Radiation!L25),0))))","v":0},{"$f":"IF(EM26<0,0,IF(0>AA26,0,IF(50>AA26,(( -0.000009*AA26^2 + 0.0004*AA26 + 0.7918)*Radiation!M25),IF(90>AA26,((-0.0006*AA26^2 + 0.0699*AA26 - 1.2225)*Radiation!M25),0))))","v":0},{"$f":"IF(EN26<0,0,IF(0>AB26,0,IF(50>AB26,(( -0.000009*AB26^2 + 0.0004*AB26 + 0.7918)*Radiation!N25),IF(90>AB26,((-0.0006*AB26^2 + 0.0699*AB26 - 1.2225)*Radiation!N25),0))))","v":0},null,null,22,{"$f":"AG26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU26","v":0},{"$f":"AH26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV26","v":0},{"$f":"AI26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW26","v":0},{"$f":"AJ26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX26","v":0},{"$f":"AK26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY26","v":0},{"$f":"AL26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ26","v":0},{"$f":"AM26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA26","v":0},{"$f":"AN26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB26","v":0},{"$f":"AO26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC26","v":0},{"$f":"AP26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD26","v":0},{"$f":"AQ26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE26","v":0},{"$f":"AR26*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF26","v":0},null,22,{"$f":"AU26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI26","v":0},{"$f":"AV26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ26","v":0},{"$f":"AW26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK26","v":0},{"$f":"AX26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL26","v":0},{"$f":"AY26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM26","v":0},{"$f":"AZ26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN26","v":0},{"$f":"BA26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO26","v":0},{"$f":"BB26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP26","v":0},{"$f":"BC26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ26","v":0},{"$f":"BD26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR26","v":0},{"$f":"BE26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS26","v":0},{"$f":"BF26*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT26","v":0},null,22,0,0,0,0,0,0,0,0,0,0,0,0,null,22,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B25","v":22},{"$f":"'Solar Altitude'!C25","v":-57.730536859646747},{"$f":"'Solar Altitude'!D25","v":-53.7124665497957},{"$f":"'Solar Altitude'!E25","v":-49.130640449349315},{"$f":"'Solar Altitude'!F25","v":-42.202232941267965},{"$f":"'Solar Altitude'!G25","v":-35.853933091501311},{"$f":"'Solar Altitude'!H25","v":-32.649969945256942},{"$f":"'Solar Altitude'!I25","v":-34.377195915482893},{"$f":"'Solar Altitude'!J25","v":-41.497131280000914},{"$f":"'Solar Altitude'!K25","v":-51.954064465377563},{"$f":"'Solar Altitude'!L25","v":-60.030194510304511},{"$f":"'Solar Altitude'!M25","v":-63.399939655490947},{"$f":"'Solar Altitude'!N25","v":-61.381330079855132},null,22,-57.730536859646747,-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132]
[null,23,{"$f":"DEGREES(C55)","v":93.494323248157158},102.6037590015965,113.32244793982535,125.40623823849923,133.78888934433641,136.70908302162255,133.60668883962251,125.47604163089012,113.81602048287024,103.38571749406297,94.191299779240623,90.358054230132893,null,23,{"$f":"DEGREES(Q55)","v":108.37068106959256},109.89788330261445,108.65833333333332,106.14373901256786,104.94321048157917,105.68003318692838,107.13507160669592,106.98525858570093,104.90833333333329,102.70466413740596,102.52381337636956,104.99686600055787,null,null,null,23,{"$f":"IF(DO27<0,0,IF(0>C27,0,IF(50>C27,((-0.000009*C27^2 + 0.0004*C27 + 0.7918)*Radiation!C26),IF(90>C27,(( -0.0006*C27^2 + 0.0699*C27 - 1.2225)*Radiation!C26),0))))","v":0},{"$f":"IF(DP27<0,0,IF(0>D27,0,IF(50>D27,((-0.000009*D27^2 + 0.0004*D27 + 0.7918)*Radiation!D26),IF(90>D27,(( -0.0006*D27^2 + 0.0699*D27 - 1.2225)*Radiation!D26),0))))","v":0},{"$f":"IF(DQ27<0,0,IF(0>E27,0,IF(50>E27,((-0.000009*E27^2 + 0.0004*E27 + 0.7918)*Radiation!E26),IF(90>E27,(( -0.0006*E27^2 + 0.0699*E27 - 1.2225)*Radiation!E26),0))))","v":0},{"$f":"IF(DR27<0,0,IF(0>F27,0,IF(50>F27,((-0.000009*F27^2 + 0.0004*F27 + 0.7918)*Radiation!F26),IF(90>F27,(( -0.0006*F27^2 + 0.0699*F27 - 1.2225)*Radiation!F26),0))))","v":0},{"$f":"IF(DS27<0,0,IF(0>G27,0,IF(50>G27,((-0.000009*G27^2 + 0.0004*G27 + 0.7918)*Radiation!G26),IF(90>G27,(( -0.0006*G27^2 + 0.0699*G27 - 1.2225)*Radiation!G26),0))))","v":0},{"$f":"IF(DT27<0,0,IF(0>H27,0,IF(50>H27,((-0.000009*H27^2 + 0.0004*H27 + 0.7918)*Radiation!H26),IF(90>H27,(( -0.0006*H27^2 + 0.0699*H27 - 1.2225)*Radiation!H26),0))))","v":0},{"$f":"IF(DU27<0,0,IF(0>I27,0,IF(50>I27,((-0.000009*I27^2 + 0.0004*I27 + 0.7918)*Radiation!I26),IF(90>I27,(( -0.0006*I27^2 + 0.0699*I27 - 1.2225)*Radiation!I26),0))))","v":0},{"$f":"IF(DV27<0,0,IF(0>J27,0,IF(50>J27,((-0.000009*J27^2 + 0.0004*J27 + 0.7918)*Radiation!J26),IF(90>J27,(( -0.0006*J27^2 + 0.0699*J27 - 1.2225)*Radiation!J26),0))))","v":0},{"$f":"IF(DW27<0,0,IF(0>K27,0,IF(50>K27,((-0.000009*K27^2 + 0.0004*K27 + 0.7918)*Radiation!K26),IF(90>K27,(( -0.0006*K27^2 + 0.0699*K27 - 1.2225)*Radiation!K26),0))))","v":0},{"$f":"IF(DX27<0,0,IF(0>L27,0,IF(50>L27,((-0.000009*L27^2 + 0.0004*L27 + 0.7918)*Radiation!L26),IF(90>L27,(( -0.0006*L27^2 + 0.0699*L27 - 1.2225)*Radiation!L26),0))))","v":0},{"$f":"IF(DY27<0,0,IF(0>M27,0,IF(50>M27,((-0.000009*M27^2 + 0.0004*M27 + 0.7918)*Radiation!M26),IF(90>M27,(( -0.0006*M27^2 + 0.0699*M27 - 1.2225)*Radiation!M26),0))))","v":0},{"$f":"IF(DZ27<0,0,IF(0>N27,0,IF(50>N27,((-0.000009*N27^2 + 0.0004*N27 + 0.7918)*Radiation!N26),IF(90>N27,(( -0.0006*N27^2 + 0.0699*N27 - 1.2225)*Radiation!N26),0))))","v":0},null,23,{"$f":"IF(EC27<0,0,IF(0>Q27,0,IF(50>Q27,(( -0.000009*Q27^2 + 0.0004*Q27 + 0.7918)*Radiation!C26),IF(90>Q27,((-0.0006*Q27^2 + 0.0699*Q27 - 1.2225)*Radiation!C26),0))))","v":0},{"$f":"IF(ED27<0,0,IF(0>R27,0,IF(50>R27,(( -0.000009*R27^2 + 0.0004*R27 + 0.7918)*Radiation!D26),IF(90>R27,((-0.0006*R27^2 + 0.0699*R27 - 1.2225)*Radiation!D26),0))))","v":0},{"$f":"IF(EE27<0,0,IF(0>S27,0,IF(50>S27,(( -0.000009*S27^2 + 0.0004*S27 + 0.7918)*Radiation!E26),IF(90>S27,((-0.0006*S27^2 + 0.0699*S27 - 1.2225)*Radiation!E26),0))))","v":0},{"$f":"IF(EF27<0,0,IF(0>T27,0,IF(50>T27,(( -0.000009*T27^2 + 0.0004*T27 + 0.7918)*Radiation!F26),IF(90>T27,((-0.0006*T27^2 + 0.0699*T27 - 1.2225)*Radiation!F26),0))))","v":0},{"$f":"IF(EG27<0,0,IF(0>U27,0,IF(50>U27,(( -0.000009*U27^2 + 0.0004*U27 + 0.7918)*Radiation!G26),IF(90>U27,((-0.0006*U27^2 + 0.0699*U27 - 1.2225)*Radiation!G26),0))))","v":0},{"$f":"IF(EH27<0,0,IF(0>V27,0,IF(50>V27,(( -0.000009*V27^2 + 0.0004*V27 + 0.7918)*Radiation!H26),IF(90>V27,((-0.0006*V27^2 + 0.0699*V27 - 1.2225)*Radiation!H26),0))))","v":0},{"$f":"IF(EI27<0,0,IF(0>W27,0,IF(50>W27,(( -0.000009*W27^2 + 0.0004*W27 + 0.7918)*Radiation!I26),IF(90>W27,((-0.0006*W27^2 + 0.0699*W27 - 1.2225)*Radiation!I26),0))))","v":0},{"$f":"IF(EJ27<0,0,IF(0>X27,0,IF(50>X27,(( -0.000009*X27^2 + 0.0004*X27 + 0.7918)*Radiation!J26),IF(90>X27,((-0.0006*X27^2 + 0.0699*X27 - 1.2225)*Radiation!J26),0))))","v":0},{"$f":"IF(EK27<0,0,IF(0>Y27,0,IF(50>Y27,(( -0.000009*Y27^2 + 0.0004*Y27 + 0.7918)*Radiation!K26),IF(90>Y27,((-0.0006*Y27^2 + 0.0699*Y27 - 1.2225)*Radiation!K26),0))))","v":0},{"$f":"IF(EL27<0,0,IF(0>Z27,0,IF(50>Z27,(( -0.000009*Z27^2 + 0.0004*Z27 + 0.7918)*Radiation!L26),IF(90>Z27,((-0.0006*Z27^2 + 0.0699*Z27 - 1.2225)*Radiation!L26),0))))","v":0},{"$f":"IF(EM27<0,0,IF(0>AA27,0,IF(50>AA27,(( -0.000009*AA27^2 + 0.0004*AA27 + 0.7918)*Radiation!M26),IF(90>AA27,((-0.0006*AA27^2 + 0.0699*AA27 - 1.2225)*Radiation!M26),0))))","v":0},{"$f":"IF(EN27<0,0,IF(0>AB27,0,IF(50>AB27,(( -0.000009*AB27^2 + 0.0004*AB27 + 0.7918)*Radiation!N26),IF(90>AB27,((-0.0006*AB27^2 + 0.0699*AB27 - 1.2225)*Radiation!N26),0))))","v":0},null,null,23,{"$f":"AG27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU27","v":0},{"$f":"AH27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV27","v":0},{"$f":"AI27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW27","v":0},{"$f":"AJ27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX27","v":0},{"$f":"AK27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY27","v":0},{"$f":"AL27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ27","v":0},{"$f":"AM27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA27","v":0},{"$f":"AN27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB27","v":0},{"$f":"AO27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC27","v":0},{"$f":"AP27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD27","v":0},{"$f":"AQ27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE27","v":0},{"$f":"AR27*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF27","v":0},null,23,{"$f":"AU27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI27","v":0},{"$f":"AV27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ27","v":0},{"$f":"AW27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK27","v":0},{"$f":"AX27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL27","v":0},{"$f":"AY27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM27","v":0},{"$f":"AZ27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN27","v":0},{"$f":"BA27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO27","v":0},{"$f":"BB27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP27","v":0},{"$f":"BC27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ27","v":0},{"$f":"BD27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR27","v":0},{"$f":"BE27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS27","v":0},{"$f":"BF27*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT27","v":0},null,23,0,0,0,0,0,0,0,0,0,0,0,0,null,23,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B26","v":23},{"$f":"'Solar Altitude'!C26","v":-71.276413671366612},{"$f":"'Solar Altitude'!D26","v":-66.153465993410151},{"$f":"'Solar Altitude'!E26","v":-59.402009530792824},{"$f":"'Solar Altitude'!F26","v":-50.011386554405469},{"$f":"'Solar Altitude'!G26","v":-42.39742803240717},{"$f":"'Solar Altitude'!H26","v":-39.064492418979341},{"$f":"'Solar Altitude'!I26","v":-41.409864595350896},{"$f":"'Solar Altitude'!J26","v":-49.478233796277678},{"$f":"'Solar Altitude'!K26","v":-61.393251168859493},{"$f":"'Solar Altitude'!L26","v":-71.378499679687209},{"$f":"'Solar Altitude'!M26","v":-76.771747562226409},{"$f":"'Solar Altitude'!N26","v":-74.998658692112272},null,23,-71.276413671366612,-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272]
[null,24,{"$f":"DEGREES(C56)","v":94.727759508116819},103.99790828964116,114.64631138922826,126.58988945315083,134.99555820854803,138.1271874495383,135.14618056558032,126.77471420878038,114.6999662728682,103.98422960007085,94.790442680138753,91.24359700259528,null,24,{"$f":"DEGREES(Q56)","v":94.30912020782884},95.168355397290895,93.658333333333161,91.475910468663045,90.89880518419568,91.957064778954219,93.12202436641951,92.330353831740936,90.091666666663983,92.030717925501492,91.567121265055405,91.269061121613731,null,null,null,24,{"$f":"IF(DO28<0,0,IF(0>C28,0,IF(50>C28,((-0.000009*C28^2 + 0.0004*C28 + 0.7918)*Radiation!C27),IF(90>C28,(( -0.0006*C28^2 + 0.0699*C28 - 1.2225)*Radiation!C27),0))))","v":0},{"$f":"IF(DP28<0,0,IF(0>D28,0,IF(50>D28,((-0.000009*D28^2 + 0.0004*D28 + 0.7918)*Radiation!D27),IF(90>D28,(( -0.0006*D28^2 + 0.0699*D28 - 1.2225)*Radiation!D27),0))))","v":0},{"$f":"IF(DQ28<0,0,IF(0>E28,0,IF(50>E28,((-0.000009*E28^2 + 0.0004*E28 + 0.7918)*Radiation!E27),IF(90>E28,(( -0.0006*E28^2 + 0.0699*E28 - 1.2225)*Radiation!E27),0))))","v":0},{"$f":"IF(DR28<0,0,IF(0>F28,0,IF(50>F28,((-0.000009*F28^2 + 0.0004*F28 + 0.7918)*Radiation!F27),IF(90>F28,(( -0.0006*F28^2 + 0.0699*F28 - 1.2225)*Radiation!F27),0))))","v":0},{"$f":"IF(DS28<0,0,IF(0>G28,0,IF(50>G28,((-0.000009*G28^2 + 0.0004*G28 + 0.7918)*Radiation!G27),IF(90>G28,(( -0.0006*G28^2 + 0.0699*G28 - 1.2225)*Radiation!G27),0))))","v":0},{"$f":"IF(DT28<0,0,IF(0>H28,0,IF(50>H28,((-0.000009*H28^2 + 0.0004*H28 + 0.7918)*Radiation!H27),IF(90>H28,(( -0.0006*H28^2 + 0.0699*H28 - 1.2225)*Radiation!H27),0))))","v":0},{"$f":"IF(DU28<0,0,IF(0>I28,0,IF(50>I28,((-0.000009*I28^2 + 0.0004*I28 + 0.7918)*Radiation!I27),IF(90>I28,(( -0.0006*I28^2 + 0.0699*I28 - 1.2225)*Radiation!I27),0))))","v":0},{"$f":"IF(DV28<0,0,IF(0>J28,0,IF(50>J28,((-0.000009*J28^2 + 0.0004*J28 + 0.7918)*Radiation!J27),IF(90>J28,(( -0.0006*J28^2 + 0.0699*J28 - 1.2225)*Radiation!J27),0))))","v":0},{"$f":"IF(DW28<0,0,IF(0>K28,0,IF(50>K28,((-0.000009*K28^2 + 0.0004*K28 + 0.7918)*Radiation!K27),IF(90>K28,(( -0.0006*K28^2 + 0.0699*K28 - 1.2225)*Radiation!K27),0))))","v":0},{"$f":"IF(DX28<0,0,IF(0>L28,0,IF(50>L28,((-0.000009*L28^2 + 0.0004*L28 + 0.7918)*Radiation!L27),IF(90>L28,(( -0.0006*L28^2 + 0.0699*L28 - 1.2225)*Radiation!L27),0))))","v":0},{"$f":"IF(DY28<0,0,IF(0>M28,0,IF(50>M28,((-0.000009*M28^2 + 0.0004*M28 + 0.7918)*Radiation!M27),IF(90>M28,(( -0.0006*M28^2 + 0.0699*M28 - 1.2225)*Radiation!M27),0))))","v":0},{"$f":"IF(DZ28<0,0,IF(0>N28,0,IF(50>N28,((-0.000009*N28^2 + 0.0004*N28 + 0.7918)*Radiation!N27),IF(90>N28,(( -0.0006*N28^2 + 0.0699*N28 - 1.2225)*Radiation!N27),0))))","v":0},null,24,{"$f":"IF(EC28<0,0,IF(0>Q28,0,IF(50>Q28,(( -0.000009*Q28^2 + 0.0004*Q28 + 0.7918)*Radiation!C27),IF(90>Q28,((-0.0006*Q28^2 + 0.0699*Q28 - 1.2225)*Radiation!C27),0))))","v":0},{"$f":"IF(ED28<0,0,IF(0>R28,0,IF(50>R28,(( -0.000009*R28^2 + 0.0004*R28 + 0.7918)*Radiation!D27),IF(90>R28,((-0.0006*R28^2 + 0.0699*R28 - 1.2225)*Radiation!D27),0))))","v":0},{"$f":"IF(EE28<0,0,IF(0>S28,0,IF(50>S28,(( -0.000009*S28^2 + 0.0004*S28 + 0.7918)*Radiation!E27),IF(90>S28,((-0.0006*S28^2 + 0.0699*S28 - 1.2225)*Radiation!E27),0))))","v":0},{"$f":"IF(EF28<0,0,IF(0>T28,0,IF(50>T28,(( -0.000009*T28^2 + 0.0004*T28 + 0.7918)*Radiation!F27),IF(90>T28,((-0.0006*T28^2 + 0.0699*T28 - 1.2225)*Radiation!F27),0))))","v":0},{"$f":"IF(EG28<0,0,IF(0>U28,0,IF(50>U28,(( -0.000009*U28^2 + 0.0004*U28 + 0.7918)*Radiation!G27),IF(90>U28,((-0.0006*U28^2 + 0.0699*U28 - 1.2225)*Radiation!G27),0))))","v":0},{"$f":"IF(EH28<0,0,IF(0>V28,0,IF(50>V28,(( -0.000009*V28^2 + 0.0004*V28 + 0.7918)*Radiation!H27),IF(90>V28,((-0.0006*V28^2 + 0.0699*V28 - 1.2225)*Radiation!H27),0))))","v":0},{"$f":"IF(EI28<0,0,IF(0>W28,0,IF(50>W28,(( -0.000009*W28^2 + 0.0004*W28 + 0.7918)*Radiation!I27),IF(90>W28,((-0.0006*W28^2 + 0.0699*W28 - 1.2225)*Radiation!I27),0))))","v":0},{"$f":"IF(EJ28<0,0,IF(0>X28,0,IF(50>X28,(( -0.000009*X28^2 + 0.0004*X28 + 0.7918)*Radiation!J27),IF(90>X28,((-0.0006*X28^2 + 0.0699*X28 - 1.2225)*Radiation!J27),0))))","v":0},{"$f":"IF(EK28<0,0,IF(0>Y28,0,IF(50>Y28,(( -0.000009*Y28^2 + 0.0004*Y28 + 0.7918)*Radiation!K27),IF(90>Y28,((-0.0006*Y28^2 + 0.0699*Y28 - 1.2225)*Radiation!K27),0))))","v":0},{"$f":"IF(EL28<0,0,IF(0>Z28,0,IF(50>Z28,(( -0.000009*Z28^2 + 0.0004*Z28 + 0.7918)*Radiation!L27),IF(90>Z28,((-0.0006*Z28^2 + 0.0699*Z28 - 1.2225)*Radiation!L27),0))))","v":0},{"$f":"IF(EM28<0,0,IF(0>AA28,0,IF(50>AA28,(( -0.000009*AA28^2 + 0.0004*AA28 + 0.7918)*Radiation!M27),IF(90>AA28,((-0.0006*AA28^2 + 0.0699*AA28 - 1.2225)*Radiation!M27),0))))","v":0},{"$f":"IF(EN28<0,0,IF(0>AB28,0,IF(50>AB28,(( -0.000009*AB28^2 + 0.0004*AB28 + 0.7918)*Radiation!N27),IF(90>AB28,((-0.0006*AB28^2 + 0.0699*AB28 - 1.2225)*Radiation!N27),0))))","v":0},null,null,24,{"$f":"AG28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CU28","v":0},{"$f":"AH28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CV28","v":0},{"$f":"AI28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CW28","v":0},{"$f":"AJ28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CX28","v":0},{"$f":"AK28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CY28","v":0},{"$f":"AL28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!CZ28","v":0},{"$f":"AM28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DA28","v":0},{"$f":"AN28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DB28","v":0},{"$f":"AO28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DC28","v":0},{"$f":"AP28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DD28","v":0},{"$f":"AQ28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DE28","v":0},{"$f":"AR28*'Input Data'!$F$32*'Input Data'!$F$33*'Operative BP'!DF28","v":0},null,24,{"$f":"AU28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DI28","v":0},{"$f":"AV28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DJ28","v":0},{"$f":"AW28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DK28","v":0},{"$f":"AX28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DL28","v":0},{"$f":"AY28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DM28","v":0},{"$f":"AZ28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DN28","v":0},{"$f":"BA28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DO28","v":0},{"$f":"BB28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DP28","v":0},{"$f":"BC28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DQ28","v":0},{"$f":"BD28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DR28","v":0},{"$f":"BE28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DS28","v":0},{"$f":"BF28*'Input Data'!$F$35*'Input Data'!$F$36*'Operative BP'!DT28","v":0},null,24,0,0,0,0,0,0,0,0,0,0,0,0,null,24,0,0,0,0,0,0,0,0,0,0,0,0,null,null,{"$f":"'Solar Altitude'!B27","v":24},{"$f":"'Solar Altitude'!C27","v":-83.596484892158756},{"$f":"'Solar Altitude'!D27","v":-75.041691580826409},{"$f":"'Solar Altitude'!E27","v":-65.047371814417531},{"$f":"'Solar Altitude'!F27","v":-53.370409687127484},{"$f":"'Solar Altitude'!G27","v":-44.990343292174892},{"$f":"'Solar Altitude'!H27","v":-41.805581832384377},{"$f":"'Solar Altitude'!I27","v":-44.683864079458822},{"$f":"'Solar Altitude'!J27","v":-53.126563822663151},{"$f":"'Solar Altitude'!K27","v":-65.299840573859427},{"$f":"'Solar Altitude'!L27","v":-75.863131931954825},{"$f":"'Solar Altitude'!M27","v":-84.958601709687045},{"$f":"'Solar Altitude'!N27","v":-88.223048770244205},null,24,-83.596484892158756,-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T",{"$f":"SUM(BJ5:BJ28)","v":14030.784632581037},{"$f":"SUM(BK5:BK28)","v":1675.0695302373958},0,0,0,0,0,0,0,2235.3795226721063,15798.901292159933,15826.439540382029,null,"T",{"$f":"SUM(BX5:BX28)","v":4300.5894702351925},5662.3134755026058,6922.5913869089618,8423.5483878904797,8654.1515417427108,9234.1644601513017,9019.9916035703045,9529.9333265155547,8314.9767220948142,6408.5471212920274,4170.2681988083914,3075.606805158458,null,"T",0.56980601464531988,0.10205908169977175,0,0,0,0,0,0,0,0.11705179123884379,0.59009295928329553,0.66058174450513618,null,"T",0.17465179680472082,0.34499494091098332,0.37797177352405409,0.4100270297811936,0.4020351622475849,0.42028724845204973,0.41071487748210944,0.39619338327316861,0.39784568347211025,0.33557251114525838,0.15576057201275353,0.12837313810092754]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max Tons",{"$f":"(MAX(BJ5:BJ28))*0.000083333","v":0.22172998091293661},{"$f":"(MAX(BK5:BK28))*0.000083333","v":3.0371637149643783E-2},0,0,0,0,0,0,0,3.830763187023041E-2,0.26586118035750211,0.25517367449065004,null,"Max Tons",{"$f":"(MAX(BX5:BX28))*0.000083333","v":0.1614785148002717},{"$f":"(MAX(BY5:BY28))*0.000083333","v":0.20159927985163262},0.24266693149197466,0.28750411840107132,0.28583962076957126,0.30203424120196398,0.3100757587234404,0.31883925464425267,0.27951662019576862,0.22246852130519268,0.15979069429134463,0.11583124004575107]
[]
[null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"ACOS((COS('Solar Altitude'!C31)*COS('Surface Solar Azimuth Angles'!C30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C31)*COS('Input Data'!$G$14)))","v":1.6480753946960163},{"$f":"ACOS((COS('Solar Altitude'!D31)*COS('Surface Solar Azimuth Angles'!D30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D31)*COS('Input Data'!$G$14)))","v":1.8107858739645217},{"$f":"ACOS((COS('Solar Altitude'!E31)*COS('Surface Solar Azimuth Angles'!E30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E31)*COS('Input Data'!$G$14)))","v":1.992929088293024},{"$f":"ACOS((COS('Solar Altitude'!F31)*COS('Surface Solar Azimuth Angles'!F30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F31)*COS('Input Data'!$G$14)))","v":2.1956038642786351},{"$f":"ACOS((COS('Solar Altitude'!G31)*COS('Surface Solar Azimuth Angles'!G30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G31)*COS('Input Data'!$G$14)))","v":2.3397674699199849},{"$f":"ACOS((COS('Solar Altitude'!H31)*COS('Surface Solar Azimuth Angles'!H30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H31)*COS('Input Data'!$G$14)))","v":2.3968588869160667},{"$f":"ACOS((COS('Solar Altitude'!I31)*COS('Surface Solar Azimuth Angles'!I30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I31)*COS('Input Data'!$G$14)))","v":2.3482747520220943},{"$f":"ACOS((COS('Solar Altitude'!J31)*COS('Surface Solar Azimuth Angles'!J30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J31)*COS('Input Data'!$G$14)))","v":2.2008122733135478},{"$f":"ACOS((COS('Solar Altitude'!K31)*COS('Surface Solar Azimuth Angles'!K30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K31)*COS('Input Data'!$G$14)))","v":1.9860860581317157},{"$f":"ACOS((COS('Solar Altitude'!L31)*COS('Surface Solar Azimuth Angles'!L30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L31)*COS('Input Data'!$G$14)))","v":1.7965496287786353},{"$f":"ACOS((COS('Solar Altitude'!M31)*COS('Surface Solar Azimuth Angles'!M30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M31)*COS('Input Data'!$G$14)))","v":1.6380182159417636},{"$f":"ACOS((COS('Solar Altitude'!N31)*COS('Surface Solar Azimuth Angles'!N30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N31)*COS('Input Data'!$G$14)))","v":1.5818363230689541},null,1,{"$f":"ACOS((COS('Solar Altitude'!C31)*COS('Surface Solar Azimuth Angles'!Q30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C31)*COS('Input Data'!$G$14)))","v":1.3999574973106035},{"$f":"ACOS((COS('Solar Altitude'!D31)*COS('Surface Solar Azimuth Angles'!R30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D31)*COS('Input Data'!$G$14)))","v":1.4037011247408859},{"$f":"ACOS((COS('Solar Altitude'!E31)*COS('Surface Solar Azimuth Angles'!S30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E31)*COS('Input Data'!$G$14)))","v":1.3728469007978725},{"$f":"ACOS((COS('Solar Altitude'!F31)*COS('Surface Solar Azimuth Angles'!T30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F31)*COS('Input Data'!$G$14)))","v":1.34047538959789},{"$f":"ACOS((COS('Solar Altitude'!G31)*COS('Surface Solar Azimuth Angles'!U30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G31)*COS('Input Data'!$G$14)))","v":1.3412275846299366},{"$f":"ACOS((COS('Solar Altitude'!H31)*COS('Surface Solar Azimuth Angles'!V30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H31)*COS('Input Data'!$G$14)))","v":1.3650568621907502},{"$f":"ACOS((COS('Solar Altitude'!I31)*COS('Surface Solar Azimuth Angles'!W30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I31)*COS('Input Data'!$G$14)))","v":1.3802334869131043},{"$f":"ACOS((COS('Solar Altitude'!J31)*COS('Surface Solar Azimuth Angles'!X30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J31)*COS('Input Data'!$G$14)))","v":1.3555640296738942},{"$f":"ACOS((COS('Solar Altitude'!K31)*COS('Surface Solar Azimuth Angles'!Y30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K31)*COS('Input Data'!$G$14)))","v":1.3073970538480868},{"$f":"ACOS((COS('Solar Altitude'!L31)*COS('Surface Solar Azimuth Angles'!Z30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L31)*COS('Input Data'!$G$14)))","v":1.2782603911114874},{"$f":"ACOS((COS('Solar Altitude'!M31)*COS('Surface Solar Azimuth Angles'!AA30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M31)*COS('Input Data'!$G$14)))","v":1.2977380379324028},{"$f":"ACOS((COS('Solar Altitude'!N31)*COS('Surface Solar Azimuth Angles'!AB30)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N31)*COS('Input Data'!$G$14)))","v":1.3531003490591478}]
[null,2,{"$f":"ACOS((COS('Solar Altitude'!C32)*COS('Surface Solar Azimuth Angles'!C31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C32)*COS('Input Data'!$G$14)))","v":1.6164599411834906},{"$f":"ACOS((COS('Solar Altitude'!D32)*COS('Surface Solar Azimuth Angles'!D31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D32)*COS('Input Data'!$G$14)))","v":1.7781909780885197},{"$f":"ACOS((COS('Solar Altitude'!E32)*COS('Surface Solar Azimuth Angles'!E31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E32)*COS('Input Data'!$G$14)))","v":1.9546294494082452},{"$f":"ACOS((COS('Solar Altitude'!F32)*COS('Surface Solar Azimuth Angles'!F31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F32)*COS('Input Data'!$G$14)))","v":2.1492181615871395},{"$f":"ACOS((COS('Solar Altitude'!G32)*COS('Surface Solar Azimuth Angles'!G31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G32)*COS('Input Data'!$G$14)))","v":2.2887307601856568},{"$f":"ACOS((COS('Solar Altitude'!H32)*COS('Surface Solar Azimuth Angles'!H31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H32)*COS('Input Data'!$G$14)))","v":2.3468092847013207},{"$f":"ACOS((COS('Solar Altitude'!I32)*COS('Surface Solar Azimuth Angles'!I31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I32)*COS('Input Data'!$G$14)))","v":2.3022310628222074},{"$f":"ACOS((COS('Solar Altitude'!J32)*COS('Surface Solar Azimuth Angles'!J31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J32)*COS('Input Data'!$G$14)))","v":2.1561247809218549},{"$f":"ACOS((COS('Solar Altitude'!K32)*COS('Surface Solar Azimuth Angles'!K31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K32)*COS('Input Data'!$G$14)))","v":1.9407248257406902},{"$f":"ACOS((COS('Solar Altitude'!L32)*COS('Surface Solar Azimuth Angles'!L31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L32)*COS('Input Data'!$G$14)))","v":1.7510476217441056},{"$f":"ACOS((COS('Solar Altitude'!M32)*COS('Surface Solar Azimuth Angles'!M31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M32)*COS('Input Data'!$G$14)))","v":1.5959782721086855},{"$f":"ACOS((COS('Solar Altitude'!N32)*COS('Surface Solar Azimuth Angles'!N31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N32)*COS('Input Data'!$G$14)))","v":1.5457794358317358},null,2,{"$f":"ACOS((COS('Solar Altitude'!C32)*COS('Surface Solar Azimuth Angles'!Q31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C32)*COS('Input Data'!$G$14)))","v":1.1553813198847922},{"$f":"ACOS((COS('Solar Altitude'!D32)*COS('Surface Solar Azimuth Angles'!R31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D32)*COS('Input Data'!$G$14)))","v":1.1468225663116192},{"$f":"ACOS((COS('Solar Altitude'!E32)*COS('Surface Solar Azimuth Angles'!S31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E32)*COS('Input Data'!$G$14)))","v":1.1110475129987241},{"$f":"ACOS((COS('Solar Altitude'!F32)*COS('Surface Solar Azimuth Angles'!T31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F32)*COS('Input Data'!$G$14)))","v":1.085151123589976},{"$f":"ACOS((COS('Solar Altitude'!G32)*COS('Surface Solar Azimuth Angles'!U31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G32)*COS('Input Data'!$G$14)))","v":1.0980939366290334},{"$f":"ACOS((COS('Solar Altitude'!H32)*COS('Surface Solar Azimuth Angles'!V31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H32)*COS('Input Data'!$G$14)))","v":1.1276204932770386},{"$f":"ACOS((COS('Solar Altitude'!I32)*COS('Surface Solar Azimuth Angles'!W31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I32)*COS('Input Data'!$G$14)))","v":1.1369347675927415},{"$f":"ACOS((COS('Solar Altitude'!J32)*COS('Surface Solar Azimuth Angles'!X31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J32)*COS('Input Data'!$G$14)))","v":1.1003825727092515},{"$f":"ACOS((COS('Solar Altitude'!K32)*COS('Surface Solar Azimuth Angles'!Y31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K32)*COS('Input Data'!$G$14)))","v":1.0455976660489368},{"$f":"ACOS((COS('Solar Altitude'!L32)*COS('Surface Solar Azimuth Angles'!Z31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L32)*COS('Input Data'!$G$14)))","v":1.0219835904068333},{"$f":"ACOS((COS('Solar Altitude'!M32)*COS('Surface Solar Azimuth Angles'!AA31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M32)*COS('Input Data'!$G$14)))","v":1.0545383748715722},{"$f":"ACOS((COS('Solar Altitude'!N32)*COS('Surface Solar Azimuth Angles'!AB31)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N32)*COS('Input Data'!$G$14)))","v":1.1158769644052289}]
[null,3,{"$f":"ACOS((COS('Solar Altitude'!C33)*COS('Surface Solar Azimuth Angles'!C32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C33)*COS('Input Data'!$G$14)))","v":1.5607046268906537},{"$f":"ACOS((COS('Solar Altitude'!D33)*COS('Surface Solar Azimuth Angles'!D32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D33)*COS('Input Data'!$G$14)))","v":1.7200580986849512},{"$f":"ACOS((COS('Solar Altitude'!E33)*COS('Surface Solar Azimuth Angles'!E32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E33)*COS('Input Data'!$G$14)))","v":1.8899129440752505},{"$f":"ACOS((COS('Solar Altitude'!F33)*COS('Surface Solar Azimuth Angles'!F32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F33)*COS('Input Data'!$G$14)))","v":2.0759878469212825},{"$f":"ACOS((COS('Solar Altitude'!G33)*COS('Surface Solar Azimuth Angles'!G32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G33)*COS('Input Data'!$G$14)))","v":2.2104459513014452},{"$f":"ACOS((COS('Solar Altitude'!H33)*COS('Surface Solar Azimuth Angles'!H32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H33)*COS('Input Data'!$G$14)))","v":2.268572151927331},{"$f":"ACOS((COS('Solar Altitude'!I33)*COS('Surface Solar Azimuth Angles'!I32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I33)*COS('Input Data'!$G$14)))","v":2.2275577863463836},{"$f":"ACOS((COS('Solar Altitude'!J33)*COS('Surface Solar Azimuth Angles'!J32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J33)*COS('Input Data'!$G$14)))","v":2.0841676639206494},{"$f":"ACOS((COS('Solar Altitude'!K33)*COS('Surface Solar Azimuth Angles'!K32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K33)*COS('Input Data'!$G$14)))","v":1.8702555449806502},{"$f":"ACOS((COS('Solar Altitude'!L33)*COS('Surface Solar Azimuth Angles'!L32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L33)*COS('Input Data'!$G$14)))","v":1.6820258764369749},{"$f":"ACOS((COS('Solar Altitude'!M33)*COS('Surface Solar Azimuth Angles'!M32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M33)*COS('Input Data'!$G$14)))","v":1.531183303397357},{"$f":"ACOS((COS('Solar Altitude'!N33)*COS('Surface Solar Azimuth Angles'!N32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N33)*COS('Input Data'!$G$14)))","v":1.4866952422430724},null,3,{"$f":"ACOS((COS('Solar Altitude'!C33)*COS('Surface Solar Azimuth Angles'!Q32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C33)*COS('Input Data'!$G$14)))","v":0.91520546706612593},{"$f":"ACOS((COS('Solar Altitude'!D33)*COS('Surface Solar Azimuth Angles'!R32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D33)*COS('Input Data'!$G$14)))","v":0.89127946347861597},{"$f":"ACOS((COS('Solar Altitude'!E33)*COS('Surface Solar Azimuth Angles'!S32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E33)*COS('Input Data'!$G$14)))","v":0.84924812519957427},{"$f":"ACOS((COS('Solar Altitude'!F33)*COS('Surface Solar Azimuth Angles'!T32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F33)*COS('Input Data'!$G$14)))","v":0.83191971962990985},{"$f":"ACOS((COS('Solar Altitude'!G33)*COS('Surface Solar Azimuth Angles'!U32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G33)*COS('Input Data'!$G$14)))","v":0.86057334741430758},{"$f":"ACOS((COS('Solar Altitude'!H33)*COS('Surface Solar Azimuth Angles'!V32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H33)*COS('Input Data'!$G$14)))","v":0.89680760766268897},{"$f":"ACOS((COS('Solar Altitude'!I33)*COS('Surface Solar Azimuth Angles'!W32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I33)*COS('Input Data'!$G$14)))","v":0.89861305825338278},{"$f":"ACOS((COS('Solar Altitude'!J33)*COS('Surface Solar Azimuth Angles'!X32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J33)*COS('Input Data'!$G$14)))","v":0.84724913998719509},{"$f":"ACOS((COS('Solar Altitude'!K33)*COS('Surface Solar Azimuth Angles'!Y32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K33)*COS('Input Data'!$G$14)))","v":0.78379827824978698},{"$f":"ACOS((COS('Solar Altitude'!L33)*COS('Surface Solar Azimuth Angles'!Z32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L33)*COS('Input Data'!$G$14)))","v":0.76783407237081602},{"$f":"ACOS((COS('Solar Altitude'!M33)*COS('Surface Solar Azimuth Angles'!AA32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M33)*COS('Input Data'!$G$14)))","v":0.8176454979135398},{"$f":"ACOS((COS('Solar Altitude'!N33)*COS('Surface Solar Azimuth Angles'!AB32)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N33)*COS('Input Data'!$G$14)))","v":0.8855606493891115}]
[null,4,{"$f":"ACOS((COS('Solar Altitude'!C34)*COS('Surface Solar Azimuth Angles'!C33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C34)*COS('Input Data'!$G$14)))","v":1.4844720390267938},{"$f":"ACOS((COS('Solar Altitude'!D34)*COS('Surface Solar Azimuth Angles'!D33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D34)*COS('Input Data'!$G$14)))","v":1.6408355425941372},{"$f":"ACOS((COS('Solar Altitude'!E34)*COS('Surface Solar Azimuth Angles'!E33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E34)*COS('Input Data'!$G$14)))","v":1.8045167007635965},{"$f":"ACOS((COS('Solar Altitude'!F34)*COS('Surface Solar Azimuth Angles'!F33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F34)*COS('Input Data'!$G$14)))","v":1.9834390173322651},{"$f":"ACOS((COS('Solar Altitude'!G34)*COS('Surface Solar Azimuth Angles'!G33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G34)*COS('Input Data'!$G$14)))","v":2.1139047117900347},{"$f":"ACOS((COS('Solar Altitude'!H34)*COS('Surface Solar Azimuth Angles'!H33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H34)*COS('Input Data'!$G$14)))","v":2.1717659873971842},{"$f":"ACOS((COS('Solar Altitude'!I34)*COS('Surface Solar Azimuth Angles'!I33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I34)*COS('Input Data'!$G$14)))","v":2.1332299685368632},{"$f":"ACOS((COS('Solar Altitude'!J34)*COS('Surface Solar Azimuth Angles'!J33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J34)*COS('Input Data'!$G$14)))","v":1.9924499101293567},{"$f":"ACOS((COS('Solar Altitude'!K34)*COS('Surface Solar Azimuth Angles'!K33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K34)*COS('Input Data'!$G$14)))","v":1.7806883538080802},{"$f":"ACOS((COS('Solar Altitude'!L34)*COS('Surface Solar Azimuth Angles'!L33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L34)*COS('Input Data'!$G$14)))","v":1.5944626770213437},{"$f":"ACOS((COS('Solar Altitude'!M34)*COS('Surface Solar Azimuth Angles'!M33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M34)*COS('Input Data'!$G$14)))","v":1.4477260980876168},{"$f":"ACOS((COS('Solar Altitude'!N34)*COS('Surface Solar Azimuth Angles'!N33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N34)*COS('Input Data'!$G$14)))","v":1.4081771248633022},null,4,{"$f":"ACOS((COS('Solar Altitude'!C34)*COS('Surface Solar Azimuth Angles'!Q33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C34)*COS('Input Data'!$G$14)))","v":0.68543993462584751},{"$f":"ACOS((COS('Solar Altitude'!D34)*COS('Surface Solar Azimuth Angles'!R33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D34)*COS('Input Data'!$G$14)))","v":0.63911605270796557},{"$f":"ACOS((COS('Solar Altitude'!E34)*COS('Surface Solar Azimuth Angles'!S33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E34)*COS('Input Data'!$G$14)))","v":0.5874487374004248},{"$f":"ACOS((COS('Solar Altitude'!F34)*COS('Surface Solar Azimuth Angles'!T33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F34)*COS('Input Data'!$G$14)))","v":0.58404021966615249},{"$f":"ACOS((COS('Solar Altitude'!G34)*COS('Surface Solar Azimuth Angles'!U33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G34)*COS('Input Data'!$G$14)))","v":0.63633548918141025},{"$f":"ACOS((COS('Solar Altitude'!H34)*COS('Surface Solar Azimuth Angles'!V33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H34)*COS('Input Data'!$G$14)))","v":0.68111295315247589},{"$f":"ACOS((COS('Solar Altitude'!I34)*COS('Surface Solar Azimuth Angles'!W33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I34)*COS('Input Data'!$G$14)))","v":0.67199988705438118},{"$f":"ACOS((COS('Solar Altitude'!J34)*COS('Surface Solar Azimuth Angles'!X33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J34)*COS('Input Data'!$G$14)))","v":0.59931525089067894},{"$f":"ACOS((COS('Solar Altitude'!K34)*COS('Surface Solar Azimuth Angles'!Y33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K34)*COS('Input Data'!$G$14)))","v":0.52199889045063719},{"$f":"ACOS((COS('Solar Altitude'!L34)*COS('Surface Solar Azimuth Angles'!Z33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L34)*COS('Input Data'!$G$14)))","v":0.51937054157845686},{"$f":"ACOS((COS('Solar Altitude'!M34)*COS('Surface Solar Azimuth Angles'!AA33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M34)*COS('Input Data'!$G$14)))","v":0.59590140421839488},{"$f":"ACOS((COS('Solar Altitude'!N34)*COS('Surface Solar Azimuth Angles'!AB33)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N34)*COS('Input Data'!$G$14)))","v":0.67101159548017841}]
[null,5,{"$f":"ACOS((COS('Solar Altitude'!C35)*COS('Surface Solar Azimuth Angles'!C34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C35)*COS('Input Data'!$G$14)))","v":1.3923089559772759},{"$f":"ACOS((COS('Solar Altitude'!D35)*COS('Surface Solar Azimuth Angles'!D34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D35)*COS('Input Data'!$G$14)))","v":1.5458913369110361},{"$f":"ACOS((COS('Solar Altitude'!E35)*COS('Surface Solar Azimuth Angles'!E34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E35)*COS('Input Data'!$G$14)))","v":1.7048835033645875},{"$f":"ACOS((COS('Solar Altitude'!F35)*COS('Surface Solar Azimuth Angles'!F34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F35)*COS('Input Data'!$G$14)))","v":1.8791866595644429},{"$f":"ACOS((COS('Solar Altitude'!G35)*COS('Surface Solar Azimuth Angles'!G34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G35)*COS('Input Data'!$G$14)))","v":2.0074899786071447},{"$f":"ACOS((COS('Solar Altitude'!H35)*COS('Surface Solar Azimuth Angles'!H34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H35)*COS('Input Data'!$G$14)))","v":2.0651631805670285},{"$f":"ACOS((COS('Solar Altitude'!I35)*COS('Surface Solar Azimuth Angles'!I34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I35)*COS('Input Data'!$G$14)))","v":2.0278214406508175},{"$f":"ACOS((COS('Solar Altitude'!J35)*COS('Surface Solar Azimuth Angles'!J34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J35)*COS('Input Data'!$G$14)))","v":1.8886304206210827},{"$f":"ACOS((COS('Solar Altitude'!K35)*COS('Surface Solar Azimuth Angles'!K34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K35)*COS('Input Data'!$G$14)))","v":1.6785105552640265},{"$f":"ACOS((COS('Solar Altitude'!L35)*COS('Surface Solar Azimuth Angles'!L34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L35)*COS('Input Data'!$G$14)))","v":1.4939407230470763},{"$f":"ACOS((COS('Solar Altitude'!M35)*COS('Surface Solar Azimuth Angles'!M34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M35)*COS('Input Data'!$G$14)))","v":1.3503910982814182},{"$f":"ACOS((COS('Solar Altitude'!N35)*COS('Surface Solar Azimuth Angles'!N34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N35)*COS('Input Data'!$G$14)))","v":1.3145929318331733},null,5,{"$f":"ACOS((COS('Solar Altitude'!C35)*COS('Surface Solar Azimuth Angles'!Q34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C35)*COS('Input Data'!$G$14)))","v":0.48237186136461552},{"$f":"ACOS((COS('Solar Altitude'!D35)*COS('Surface Solar Azimuth Angles'!R34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D35)*COS('Input Data'!$G$14)))","v":0.39724088446373274},{"$f":"ACOS((COS('Solar Altitude'!E35)*COS('Surface Solar Azimuth Angles'!S34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E35)*COS('Input Data'!$G$14)))","v":0.32564934960127534},{"$f":"ACOS((COS('Solar Altitude'!F35)*COS('Surface Solar Azimuth Angles'!T34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F35)*COS('Input Data'!$G$14)))","v":0.35348129320527977},{"$f":"ACOS((COS('Solar Altitude'!G35)*COS('Surface Solar Azimuth Angles'!U34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G35)*COS('Input Data'!$G$14)))","v":0.44700804245908787},{"$f":"ACOS((COS('Solar Altitude'!H35)*COS('Surface Solar Azimuth Angles'!V34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H35)*COS('Input Data'!$G$14)))","v":0.50184862387126761},{"$f":"ACOS((COS('Solar Altitude'!I35)*COS('Surface Solar Azimuth Angles'!W34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I35)*COS('Input Data'!$G$14)))","v":0.47535745896420889},{"$f":"ACOS((COS('Solar Altitude'!J35)*COS('Surface Solar Azimuth Angles'!X34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J35)*COS('Input Data'!$G$14)))","v":0.36778729059036208},{"$f":"ACOS((COS('Solar Altitude'!K35)*COS('Surface Solar Azimuth Angles'!Y34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K35)*COS('Input Data'!$G$14)))","v":0.26019950265148784},{"$f":"ACOS((COS('Solar Altitude'!L35)*COS('Surface Solar Azimuth Angles'!Z34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L35)*COS('Input Data'!$G$14)))","v":0.29194794884940656},{"$f":"ACOS((COS('Solar Altitude'!M35)*COS('Surface Solar Azimuth Angles'!AA34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M35)*COS('Input Data'!$G$14)))","v":0.4154308062088683},{"$f":"ACOS((COS('Solar Altitude'!N35)*COS('Surface Solar Azimuth Angles'!AB34)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N35)*COS('Input Data'!$G$14)))","v":0.49460277338763348}]
[null,6,{"$f":"ACOS((COS('Solar Altitude'!C36)*COS('Surface Solar Azimuth Angles'!C35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C36)*COS('Input Data'!$G$14)))","v":1.2892513399208603},{"$f":"ACOS((COS('Solar Altitude'!D36)*COS('Surface Solar Azimuth Angles'!D35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D36)*COS('Input Data'!$G$14)))","v":1.440953009749286},{"$f":"ACOS((COS('Solar Altitude'!E36)*COS('Surface Solar Azimuth Angles'!E35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E36)*COS('Input Data'!$G$14)))","v":1.5974621584847333},{"$f":"ACOS((COS('Solar Altitude'!F36)*COS('Surface Solar Azimuth Angles'!F35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F36)*COS('Input Data'!$G$14)))","v":1.7702165157331793},{"$f":"ACOS((COS('Solar Altitude'!G36)*COS('Surface Solar Azimuth Angles'!G35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G36)*COS('Input Data'!$G$14)))","v":1.8983721814134626},{"$f":"ACOS((COS('Solar Altitude'!H36)*COS('Surface Solar Azimuth Angles'!H35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H36)*COS('Input Data'!$G$14)))","v":1.9560670078384166},{"$f":"ACOS((COS('Solar Altitude'!I36)*COS('Surface Solar Azimuth Angles'!I35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I36)*COS('Input Data'!$G$14)))","v":1.9186963750287371},{"$f":"ACOS((COS('Solar Altitude'!J36)*COS('Surface Solar Azimuth Angles'!J35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J36)*COS('Input Data'!$G$14)))","v":1.7797445635886},{"$f":"ACOS((COS('Solar Altitude'!K36)*COS('Surface Solar Azimuth Angles'!K35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K36)*COS('Input Data'!$G$14)))","v":1.570127787705228},{"$f":"ACOS((COS('Solar Altitude'!L36)*COS('Surface Solar Azimuth Angles'!L35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L36)*COS('Input Data'!$G$14)))","v":1.386263938450059},{"$f":"ACOS((COS('Solar Altitude'!M36)*COS('Surface Solar Azimuth Angles'!M35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M36)*COS('Input Data'!$G$14)))","v":1.2443643835006537},{"$f":"ACOS((COS('Solar Altitude'!N36)*COS('Surface Solar Azimuth Angles'!N35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N36)*COS('Input Data'!$G$14)))","v":1.2107849492567073},null,6,{"$f":"ACOS((COS('Solar Altitude'!C36)*COS('Surface Solar Azimuth Angles'!Q35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C36)*COS('Input Data'!$G$14)))","v":0.35604931493582037},{"$f":"ACOS((COS('Solar Altitude'!D36)*COS('Surface Solar Azimuth Angles'!R35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D36)*COS('Input Data'!$G$14)))","v":0.20628412079335212},{"$f":"ACOS((COS('Solar Altitude'!E36)*COS('Surface Solar Azimuth Angles'!S35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E36)*COS('Input Data'!$G$14)))","v":6.3849961802126654E-2},{"$f":"ACOS((COS('Solar Altitude'!F36)*COS('Surface Solar Azimuth Angles'!T35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F36)*COS('Input Data'!$G$14)))","v":0.20933204336545574},{"$f":"ACOS((COS('Solar Altitude'!G36)*COS('Surface Solar Azimuth Angles'!U35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G36)*COS('Input Data'!$G$14)))","v":0.35467978305383152},{"$f":"ACOS((COS('Solar Altitude'!H36)*COS('Surface Solar Azimuth Angles'!V35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H36)*COS('Input Data'!$G$14)))","v":0.4108745964815812},{"$f":"ACOS((COS('Solar Altitude'!I36)*COS('Surface Solar Azimuth Angles'!W35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I36)*COS('Input Data'!$G$14)))","v":0.36229049170682903},{"$f":"ACOS((COS('Solar Altitude'!J36)*COS('Surface Solar Azimuth Angles'!X35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J36)*COS('Input Data'!$G$14)))","v":0.21518258486844943},{"$f":"ACOS((COS('Solar Altitude'!K36)*COS('Surface Solar Azimuth Angles'!Y35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K36)*COS('Input Data'!$G$14)))","v":1.5998851476628495E-3},{"$f":"ACOS((COS('Solar Altitude'!L36)*COS('Surface Solar Azimuth Angles'!Z35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L36)*COS('Input Data'!$G$14)))","v":0.19016188263431122},{"$f":"ACOS((COS('Solar Altitude'!M36)*COS('Surface Solar Azimuth Angles'!AA35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M36)*COS('Input Data'!$G$14)))","v":0.34848730352122037},{"$f":"ACOS((COS('Solar Altitude'!N36)*COS('Surface Solar Azimuth Angles'!AB35)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N36)*COS('Input Data'!$G$14)))","v":0.40995107161716726}]
[null,7,{"$f":"ACOS((COS('Solar Altitude'!C37)*COS('Surface Solar Azimuth Angles'!C36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C37)*COS('Input Data'!$G$14)))","v":1.180698624043806},{"$f":"ACOS((COS('Solar Altitude'!D37)*COS('Surface Solar Azimuth Angles'!D36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D37)*COS('Input Data'!$G$14)))","v":1.3319103141519397},{"$f":"ACOS((COS('Solar Altitude'!E37)*COS('Surface Solar Azimuth Angles'!E36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E37)*COS('Input Data'!$G$14)))","v":1.4885261412659252},{"$f":"ACOS((COS('Solar Altitude'!F37)*COS('Surface Solar Azimuth Angles'!F36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F37)*COS('Input Data'!$G$14)))","v":1.6628696790888149},{"$f":"ACOS((COS('Solar Altitude'!G37)*COS('Surface Solar Azimuth Angles'!G36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G37)*COS('Input Data'!$G$14)))","v":1.7927184845620365},{"$f":"ACOS((COS('Solar Altitude'!H37)*COS('Surface Solar Azimuth Angles'!H36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H37)*COS('Input Data'!$G$14)))","v":1.850606352587558},{"$f":"ACOS((COS('Solar Altitude'!I37)*COS('Surface Solar Azimuth Angles'!I36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I37)*COS('Input Data'!$G$14)))","v":1.812150129960197},{"$f":"ACOS((COS('Solar Altitude'!J37)*COS('Surface Solar Azimuth Angles'!J36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J37)*COS('Input Data'!$G$14)))","v":1.6721643192171634},{"$f":"ACOS((COS('Solar Altitude'!K37)*COS('Surface Solar Azimuth Angles'!K36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K37)*COS('Input Data'!$G$14)))","v":1.4617829597416485},{"$f":"ACOS((COS('Solar Altitude'!L37)*COS('Surface Solar Azimuth Angles'!L36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L37)*COS('Input Data'!$G$14)))","v":1.2774212799090658},{"$f":"ACOS((COS('Solar Altitude'!M37)*COS('Surface Solar Azimuth Angles'!M36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M37)*COS('Input Data'!$G$14)))","v":1.1352265730450783},{"$f":"ACOS((COS('Solar Altitude'!N37)*COS('Surface Solar Azimuth Angles'!N36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N37)*COS('Input Data'!$G$14)))","v":1.102024718502959},null,7,{"$f":"ACOS((COS('Solar Altitude'!C37)*COS('Surface Solar Azimuth Angles'!Q36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C37)*COS('Input Data'!$G$14)))","v":0.39030998799189964},{"$f":"ACOS((COS('Solar Altitude'!D37)*COS('Surface Solar Azimuth Angles'!R36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D37)*COS('Input Data'!$G$14)))","v":0.25060691805980362},{"$f":"ACOS((COS('Solar Altitude'!E37)*COS('Surface Solar Azimuth Angles'!S36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E37)*COS('Input Data'!$G$14)))","v":0.19794942599702359},{"$f":"ACOS((COS('Solar Altitude'!F37)*COS('Surface Solar Azimuth Angles'!T36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F37)*COS('Input Data'!$G$14)))","v":0.31270170290585675},{"$f":"ACOS((COS('Solar Altitude'!G37)*COS('Surface Solar Azimuth Angles'!U36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G37)*COS('Input Data'!$G$14)))","v":0.42783924910737148},{"$f":"ACOS((COS('Solar Altitude'!H37)*COS('Surface Solar Azimuth Angles'!V36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H37)*COS('Input Data'!$G$14)))","v":0.46377004853544368},{"$f":"ACOS((COS('Solar Altitude'!I37)*COS('Surface Solar Azimuth Angles'!W36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I37)*COS('Input Data'!$G$14)))","v":0.40949720864396899},{"$f":"ACOS((COS('Solar Altitude'!J37)*COS('Surface Solar Azimuth Angles'!X36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J37)*COS('Input Data'!$G$14)))","v":0.30391247626034179},{"$f":"ACOS((COS('Solar Altitude'!K37)*COS('Surface Solar Azimuth Angles'!Y36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K37)*COS('Input Data'!$G$14)))","v":0.26339927294681087},{"$f":"ACOS((COS('Solar Altitude'!L37)*COS('Surface Solar Azimuth Angles'!Z36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L37)*COS('Input Data'!$G$14)))","v":0.35008845072701322},{"$f":"ACOS((COS('Solar Altitude'!M37)*COS('Surface Solar Azimuth Angles'!AA36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M37)*COS('Input Data'!$G$14)))","v":0.44921985559011302},{"$f":"ACOS((COS('Solar Altitude'!N37)*COS('Surface Solar Azimuth Angles'!AB36)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N37)*COS('Input Data'!$G$14)))","v":0.46988201245054695}]
[null,8,{"$f":"ACOS((COS('Solar Altitude'!C38)*COS('Surface Solar Azimuth Angles'!C37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C38)*COS('Input Data'!$G$14)))","v":1.0725610710247195},{"$f":"ACOS((COS('Solar Altitude'!D38)*COS('Surface Solar Azimuth Angles'!D37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D38)*COS('Input Data'!$G$14)))","v":1.2249151370421716},{"$f":"ACOS((COS('Solar Altitude'!E38)*COS('Surface Solar Azimuth Angles'!E37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E38)*COS('Input Data'!$G$14)))","v":1.3842998801572988},{"$f":"ACOS((COS('Solar Altitude'!F38)*COS('Surface Solar Azimuth Angles'!F37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F38)*COS('Input Data'!$G$14)))","v":1.5630828401166925},{"$f":"ACOS((COS('Solar Altitude'!G38)*COS('Surface Solar Azimuth Angles'!G37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G38)*COS('Input Data'!$G$14)))","v":1.6960652032679611},{"$f":"ACOS((COS('Solar Altitude'!H38)*COS('Surface Solar Azimuth Angles'!H37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H38)*COS('Input Data'!$G$14)))","v":1.7541761202442985},{"$f":"ACOS((COS('Solar Altitude'!I38)*COS('Surface Solar Azimuth Angles'!I37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I38)*COS('Input Data'!$G$14)))","v":1.7137873710182574},{"$f":"ACOS((COS('Solar Altitude'!J38)*COS('Surface Solar Azimuth Angles'!J37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J38)*COS('Input Data'!$G$14)))","v":1.5718361079149552},{"$f":"ACOS((COS('Solar Altitude'!K38)*COS('Surface Solar Azimuth Angles'!K37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K38)*COS('Input Data'!$G$14)))","v":1.3597202234373262},{"$f":"ACOS((COS('Solar Altitude'!L38)*COS('Surface Solar Azimuth Angles'!L37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L38)*COS('Input Data'!$G$14)))","v":1.173777997975658},{"$f":"ACOS((COS('Solar Altitude'!M38)*COS('Surface Solar Azimuth Angles'!M37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M38)*COS('Input Data'!$G$14)))","v":1.0291947556320262},{"$f":"ACOS((COS('Solar Altitude'!N38)*COS('Surface Solar Azimuth Angles'!N37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N38)*COS('Input Data'!$G$14)))","v":0.99423289112643698},null,8,{"$f":"ACOS((COS('Solar Altitude'!C38)*COS('Surface Solar Azimuth Angles'!Q37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C38)*COS('Input Data'!$G$14)))","v":0.55617992945761219},{"$f":"ACOS((COS('Solar Altitude'!D38)*COS('Surface Solar Azimuth Angles'!R37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D38)*COS('Input Data'!$G$14)))","v":0.46748190579132443},{"$f":"ACOS((COS('Solar Altitude'!E38)*COS('Surface Solar Azimuth Angles'!S37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E38)*COS('Input Data'!$G$14)))","v":0.45974881379617294},{"$f":"ACOS((COS('Solar Altitude'!F38)*COS('Surface Solar Azimuth Angles'!T37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F38)*COS('Input Data'!$G$14)))","v":0.53552990662876909},{"$f":"ACOS((COS('Solar Altitude'!G38)*COS('Surface Solar Azimuth Angles'!U37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G38)*COS('Input Data'!$G$14)))","v":0.60944599578734493},{"$f":"ACOS((COS('Solar Altitude'!H38)*COS('Surface Solar Azimuth Angles'!V37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H38)*COS('Input Data'!$G$14)))","v":0.62489764543640858},{"$f":"ACOS((COS('Solar Altitude'!I38)*COS('Surface Solar Azimuth Angles'!W37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I38)*COS('Input Data'!$G$14)))","v":0.57894410071375646},{"$f":"ACOS((COS('Solar Altitude'!J38)*COS('Surface Solar Azimuth Angles'!X37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J38)*COS('Input Data'!$G$14)))","v":0.52288275068244205},{"$f":"ACOS((COS('Solar Altitude'!K38)*COS('Surface Solar Azimuth Angles'!Y37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K38)*COS('Input Data'!$G$14)))","v":0.52519866074596067},{"$f":"ACOS((COS('Solar Altitude'!L38)*COS('Surface Solar Azimuth Angles'!Z37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L38)*COS('Input Data'!$G$14)))","v":0.58683665753500835},{"$f":"ACOS((COS('Solar Altitude'!M38)*COS('Surface Solar Azimuth Angles'!AA37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M38)*COS('Input Data'!$G$14)))","v":0.64300944462916743},{"$f":"ACOS((COS('Solar Altitude'!N38)*COS('Surface Solar Azimuth Angles'!AB37)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N38)*COS('Input Data'!$G$14)))","v":0.63454659679074965}]
[null,9,{"$f":"ACOS((COS('Solar Altitude'!C39)*COS('Surface Solar Azimuth Angles'!C38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C39)*COS('Input Data'!$G$14)))","v":0.97159762158789653},{"$f":"ACOS((COS('Solar Altitude'!D39)*COS('Surface Solar Azimuth Angles'!D38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D39)*COS('Input Data'!$G$14)))","v":1.1266178773129685},{"$f":"ACOS((COS('Solar Altitude'!E39)*COS('Surface Solar Azimuth Angles'!E38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E39)*COS('Input Data'!$G$14)))","v":1.2911443231701432},{"$f":"ACOS((COS('Solar Altitude'!F39)*COS('Surface Solar Azimuth Angles'!F38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F39)*COS('Input Data'!$G$14)))","v":1.4765793052953158},{"$f":"ACOS((COS('Solar Altitude'!G39)*COS('Surface Solar Azimuth Angles'!G38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G39)*COS('Input Data'!$G$14)))","v":1.6135527046862093},{"$f":"ACOS((COS('Solar Altitude'!H39)*COS('Surface Solar Azimuth Angles'!H38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H39)*COS('Input Data'!$G$14)))","v":1.671713150519575},{"$f":"ACOS((COS('Solar Altitude'!I39)*COS('Surface Solar Azimuth Angles'!I38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I39)*COS('Input Data'!$G$14)))","v":1.6287910294572032},{"$f":"ACOS((COS('Solar Altitude'!J39)*COS('Surface Solar Azimuth Angles'!J38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J39)*COS('Input Data'!$G$14)))","v":1.484481594232177},{"$f":"ACOS((COS('Solar Altitude'!K39)*COS('Surface Solar Azimuth Angles'!K38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K39)*COS('Input Data'!$G$14)))","v":1.2703474640324108},{"$f":"ACOS((COS('Solar Altitude'!L39)*COS('Surface Solar Azimuth Angles'!L38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L39)*COS('Input Data'!$G$14)))","v":1.0822981884831331},{"$f":"ACOS((COS('Solar Altitude'!M39)*COS('Surface Solar Azimuth Angles'!M38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M39)*COS('Input Data'!$G$14)))","v":0.93348844263626241},{"$f":"ACOS((COS('Solar Altitude'!N39)*COS('Surface Solar Azimuth Angles'!N38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N39)*COS('Input Data'!$G$14)))","v":0.89439713346740779},null,9,{"$f":"ACOS((COS('Solar Altitude'!C39)*COS('Surface Solar Azimuth Angles'!Q38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C39)*COS('Input Data'!$G$14)))","v":0.77290105385966534},{"$f":"ACOS((COS('Solar Altitude'!D39)*COS('Surface Solar Azimuth Angles'!R38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D39)*COS('Input Data'!$G$14)))","v":0.71390113191237892},{"$f":"ACOS((COS('Solar Altitude'!E39)*COS('Surface Solar Azimuth Angles'!S38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E39)*COS('Input Data'!$G$14)))","v":0.72154820159532251},{"$f":"ACOS((COS('Solar Altitude'!F39)*COS('Surface Solar Azimuth Angles'!T38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F39)*COS('Input Data'!$G$14)))","v":0.78146382660532232},{"$f":"ACOS((COS('Solar Altitude'!G39)*COS('Surface Solar Azimuth Angles'!U38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G39)*COS('Input Data'!$G$14)))","v":0.83093314764444859},{"$f":"ACOS((COS('Solar Altitude'!H39)*COS('Surface Solar Azimuth Angles'!V38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H39)*COS('Input Data'!$G$14)))","v":0.8333448762418737},{"$f":"ACOS((COS('Solar Altitude'!I39)*COS('Surface Solar Azimuth Angles'!W38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I39)*COS('Input Data'!$G$14)))","v":0.79579418022070614},{"$f":"ACOS((COS('Solar Altitude'!J39)*COS('Surface Solar Azimuth Angles'!X38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J39)*COS('Input Data'!$G$14)))","v":0.76764101795987161},{"$f":"ACOS((COS('Solar Altitude'!K39)*COS('Surface Solar Azimuth Angles'!Y38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K39)*COS('Input Data'!$G$14)))","v":0.78699804854510991},{"$f":"ACOS((COS('Solar Altitude'!L39)*COS('Surface Solar Azimuth Angles'!Z38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L39)*COS('Input Data'!$G$14)))","v":0.83752510996800134},{"$f":"ACOS((COS('Solar Altitude'!M39)*COS('Surface Solar Azimuth Angles'!AA38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M39)*COS('Input Data'!$G$14)))","v":0.86942639458956739},{"$f":"ACOS((COS('Solar Altitude'!N39)*COS('Surface Solar Azimuth Angles'!AB38)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N39)*COS('Input Data'!$G$14)))","v":0.84440423558933186}]
[null,10,{"$f":"ACOS((COS('Solar Altitude'!C40)*COS('Surface Solar Azimuth Angles'!C39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C40)*COS('Input Data'!$G$14)))","v":0.88572856293171653},{"$f":"ACOS((COS('Solar Altitude'!D40)*COS('Surface Solar Azimuth Angles'!D39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D40)*COS('Input Data'!$G$14)))","v":1.0442954663678496},{"$f":"ACOS((COS('Solar Altitude'!E40)*COS('Surface Solar Azimuth Angles'!E39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E40)*COS('Input Data'!$G$14)))","v":1.2155570102761952},{"$f":"ACOS((COS('Solar Altitude'!F40)*COS('Surface Solar Azimuth Angles'!F39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F40)*COS('Input Data'!$G$14)))","v":1.4088250987064912},{"$f":"ACOS((COS('Solar Altitude'!G40)*COS('Surface Solar Azimuth Angles'!G39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G40)*COS('Input Data'!$G$14)))","v":1.5499070568812463},{"$f":"ACOS((COS('Solar Altitude'!H40)*COS('Surface Solar Azimuth Angles'!H39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H40)*COS('Input Data'!$G$14)))","v":1.6077148936290149},{"$f":"ACOS((COS('Solar Altitude'!I40)*COS('Surface Solar Azimuth Angles'!I39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I40)*COS('Input Data'!$G$14)))","v":1.5619488197009246},{"$f":"ACOS((COS('Solar Altitude'!J40)*COS('Surface Solar Azimuth Angles'!J39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J40)*COS('Input Data'!$G$14)))","v":1.4155718486961455},{"$f":"ACOS((COS('Solar Altitude'!K40)*COS('Surface Solar Azimuth Angles'!K39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K40)*COS('Input Data'!$G$14)))","v":1.2001506832418554},{"$f":"ACOS((COS('Solar Altitude'!L40)*COS('Surface Solar Azimuth Angles'!L39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L40)*COS('Input Data'!$G$14)))","v":1.0104928188845765},{"$f":"ACOS((COS('Solar Altitude'!M40)*COS('Surface Solar Azimuth Angles'!M39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M40)*COS('Input Data'!$G$14)))","v":0.85650474699730428},{"$f":"ACOS((COS('Solar Altitude'!N40)*COS('Surface Solar Azimuth Angles'!N39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N40)*COS('Input Data'!$G$14)))","v":0.81094981166340918},null,10,{"$f":"ACOS((COS('Solar Altitude'!C40)*COS('Surface Solar Azimuth Angles'!Q39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C40)*COS('Input Data'!$G$14)))","v":1.0078128859305615},{"$f":"ACOS((COS('Solar Altitude'!D40)*COS('Surface Solar Azimuth Angles'!R39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D40)*COS('Input Data'!$G$14)))","v":0.96743542428139195},{"$f":"ACOS((COS('Solar Altitude'!E40)*COS('Surface Solar Azimuth Angles'!S39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E40)*COS('Input Data'!$G$14)))","v":0.98334758939447209},{"$f":"ACOS((COS('Solar Altitude'!F40)*COS('Surface Solar Azimuth Angles'!T39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F40)*COS('Input Data'!$G$14)))","v":1.0339937841271989},{"$f":"ACOS((COS('Solar Altitude'!G40)*COS('Surface Solar Azimuth Angles'!U39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G40)*COS('Input Data'!$G$14)))","v":1.067331015247823},{"$f":"ACOS((COS('Solar Altitude'!H40)*COS('Surface Solar Azimuth Angles'!V39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H40)*COS('Input Data'!$G$14)))","v":1.0610438620621698},{"$f":"ACOS((COS('Solar Altitude'!I40)*COS('Surface Solar Azimuth Angles'!W39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I40)*COS('Input Data'!$G$14)))","v":1.0301272173470557},{"$f":"ACOS((COS('Solar Altitude'!J40)*COS('Surface Solar Azimuth Angles'!X39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J40)*COS('Input Data'!$G$14)))","v":1.0196287183015125},{"$f":"ACOS((COS('Solar Altitude'!K40)*COS('Surface Solar Azimuth Angles'!Y39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K40)*COS('Input Data'!$G$14)))","v":1.0487974363442598},{"$f":"ACOS((COS('Solar Altitude'!L40)*COS('Surface Solar Azimuth Angles'!Z39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L40)*COS('Input Data'!$G$14)))","v":1.0924644016703269},{"$f":"ACOS((COS('Solar Altitude'!M40)*COS('Surface Solar Azimuth Angles'!AA39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M40)*COS('Input Data'!$G$14)))","v":1.1082133650773343},{"$f":"ACOS((COS('Solar Altitude'!N40)*COS('Surface Solar Azimuth Angles'!AB39)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N40)*COS('Input Data'!$G$14)))","v":1.0727040913382866}]
[null,11,{"$f":"ACOS((COS('Solar Altitude'!C41)*COS('Surface Solar Azimuth Angles'!C40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C41)*COS('Input Data'!$G$14)))","v":0.82381782445951102},{"$f":"ACOS((COS('Solar Altitude'!D41)*COS('Surface Solar Azimuth Angles'!D40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D41)*COS('Input Data'!$G$14)))","v":0.98549583570303656},{"$f":"ACOS((COS('Solar Altitude'!E41)*COS('Surface Solar Azimuth Angles'!E40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E41)*COS('Input Data'!$G$14)))","v":1.1637428206199756},{"$f":"ACOS((COS('Solar Altitude'!F41)*COS('Surface Solar Azimuth Angles'!F40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F41)*COS('Input Data'!$G$14)))","v":1.3646457182036715},{"$f":"ACOS((COS('Solar Altitude'!G41)*COS('Surface Solar Azimuth Angles'!G40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G41)*COS('Input Data'!$G$14)))","v":1.5091418274015536},{"$f":"ACOS((COS('Solar Altitude'!H41)*COS('Surface Solar Azimuth Angles'!H40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H41)*COS('Input Data'!$G$14)))","v":1.5659940095352525},{"$f":"ACOS((COS('Solar Altitude'!I41)*COS('Surface Solar Azimuth Angles'!I40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I41)*COS('Input Data'!$G$14)))","v":1.5173994148331544},{"$f":"ACOS((COS('Solar Altitude'!J41)*COS('Surface Solar Azimuth Angles'!J40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J41)*COS('Input Data'!$G$14)))","v":1.3699669330537532},{"$f":"ACOS((COS('Solar Altitude'!K41)*COS('Surface Solar Azimuth Angles'!K40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K41)*COS('Input Data'!$G$14)))","v":1.1551283546464013},{"$f":"ACOS((COS('Solar Altitude'!L41)*COS('Surface Solar Azimuth Angles'!L40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L41)*COS('Input Data'!$G$14)))","v":0.96567157234898171},{"$f":"ACOS((COS('Solar Altitude'!M41)*COS('Surface Solar Azimuth Angles'!M40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M41)*COS('Input Data'!$G$14)))","v":0.80714706797057922},{"$f":"ACOS((COS('Solar Altitude'!N41)*COS('Surface Solar Azimuth Angles'!N40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N41)*COS('Input Data'!$G$14)))","v":0.75345659092854689},null,11,{"$f":"ACOS((COS('Solar Altitude'!C41)*COS('Surface Solar Azimuth Angles'!Q40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C41)*COS('Input Data'!$G$14)))","v":1.2501674562967127},{"$f":"ACOS((COS('Solar Altitude'!D41)*COS('Surface Solar Azimuth Angles'!R40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D41)*COS('Input Data'!$G$14)))","v":1.2235127489866713},{"$f":"ACOS((COS('Solar Altitude'!E41)*COS('Surface Solar Azimuth Angles'!S40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E41)*COS('Input Data'!$G$14)))","v":1.2451469771936214},{"$f":"ACOS((COS('Solar Altitude'!F41)*COS('Surface Solar Azimuth Angles'!T40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F41)*COS('Input Data'!$G$14)))","v":1.2890349274429287},{"$f":"ACOS((COS('Solar Altitude'!G41)*COS('Surface Solar Azimuth Angles'!U40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G41)*COS('Input Data'!$G$14)))","v":1.3099881030728118},{"$f":"ACOS((COS('Solar Altitude'!H41)*COS('Surface Solar Azimuth Angles'!V40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H41)*COS('Input Data'!$G$14)))","v":1.297128120861017},{"$f":"ACOS((COS('Solar Altitude'!I41)*COS('Surface Solar Azimuth Angles'!W40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I41)*COS('Input Data'!$G$14)))","v":1.2717329096930581},{"$f":"ACOS((COS('Solar Altitude'!J41)*COS('Surface Solar Azimuth Angles'!X40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J41)*COS('Input Data'!$G$14)))","v":1.2743476401717793},{"$f":"ACOS((COS('Solar Altitude'!K41)*COS('Surface Solar Azimuth Angles'!Y40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K41)*COS('Input Data'!$G$14)))","v":1.3105968241434085},{"$f":"ACOS((COS('Solar Altitude'!L41)*COS('Surface Solar Azimuth Angles'!Z40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L41)*COS('Input Data'!$G$14)))","v":1.3490581072371171},{"$f":"ACOS((COS('Solar Altitude'!M41)*COS('Surface Solar Azimuth Angles'!AA40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M41)*COS('Input Data'!$G$14)))","v":1.3522145484719401},{"$f":"ACOS((COS('Solar Altitude'!N41)*COS('Surface Solar Azimuth Angles'!AB40)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N41)*COS('Input Data'!$G$14)))","v":1.3090516376047669}]
[null,12,{"$f":"ACOS((COS('Solar Altitude'!C42)*COS('Surface Solar Azimuth Angles'!C41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C42)*COS('Input Data'!$G$14)))","v":0.79414260128326908},{"$f":"ACOS((COS('Solar Altitude'!D42)*COS('Surface Solar Azimuth Angles'!D41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D42)*COS('Input Data'!$G$14)))","v":0.95681146743890266},{"$f":"ACOS((COS('Solar Altitude'!E42)*COS('Surface Solar Azimuth Angles'!E41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E42)*COS('Input Data'!$G$14)))","v":1.1406370445810861},{"$f":"ACOS((COS('Solar Altitude'!F42)*COS('Surface Solar Azimuth Angles'!F41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F42)*COS('Input Data'!$G$14)))","v":1.3475394669388494},{"$f":"ACOS((COS('Solar Altitude'!G42)*COS('Surface Solar Azimuth Angles'!G41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G42)*COS('Input Data'!$G$14)))","v":1.4940568214259038},{"$f":"ACOS((COS('Solar Altitude'!H42)*COS('Surface Solar Azimuth Angles'!H41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H42)*COS('Input Data'!$G$14)))","v":1.5492454742228872},{"$f":"ACOS((COS('Solar Altitude'!I42)*COS('Surface Solar Azimuth Angles'!I41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I42)*COS('Input Data'!$G$14)))","v":1.4981564596097079},{"$f":"ACOS((COS('Solar Altitude'!J42)*COS('Surface Solar Azimuth Angles'!J41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J42)*COS('Input Data'!$G$14)))","v":1.3512469857027551},{"$f":"ACOS((COS('Solar Altitude'!K42)*COS('Surface Solar Azimuth Angles'!K41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K42)*COS('Input Data'!$G$14)))","v":1.1397005902017945},{"$f":"ACOS((COS('Solar Altitude'!L42)*COS('Surface Solar Azimuth Angles'!L41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L42)*COS('Input Data'!$G$14)))","v":0.95327738588163724},{"$f":"ACOS((COS('Solar Altitude'!M42)*COS('Surface Solar Azimuth Angles'!M41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M42)*COS('Input Data'!$G$14)))","v":0.79261290405829088},{"$f":"ACOS((COS('Solar Altitude'!N42)*COS('Surface Solar Azimuth Angles'!N41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N42)*COS('Input Data'!$G$14)))","v":0.73058773706142388},null,12,{"$f":"ACOS((COS('Solar Altitude'!C42)*COS('Surface Solar Azimuth Angles'!Q41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C42)*COS('Input Data'!$G$14)))","v":1.4955879913040631},{"$f":"ACOS((COS('Solar Altitude'!D42)*COS('Surface Solar Azimuth Angles'!R41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D42)*COS('Input Data'!$G$14)))","v":1.4805915081989525},{"$f":"ACOS((COS('Solar Altitude'!E42)*COS('Surface Solar Azimuth Angles'!S41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E42)*COS('Input Data'!$G$14)))","v":1.5069463649927732},{"$f":"ACOS((COS('Solar Altitude'!F42)*COS('Surface Solar Azimuth Angles'!T41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F42)*COS('Input Data'!$G$14)))","v":1.5450368296520782},{"$f":"ACOS((COS('Solar Altitude'!G42)*COS('Surface Solar Azimuth Angles'!U41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G42)*COS('Input Data'!$G$14)))","v":1.5551092169966836},{"$f":"ACOS((COS('Solar Altitude'!H42)*COS('Surface Solar Azimuth Angles'!V41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H42)*COS('Input Data'!$G$14)))","v":1.5366391027273312},{"$f":"ACOS((COS('Solar Altitude'!I42)*COS('Surface Solar Azimuth Angles'!W41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I42)*COS('Input Data'!$G$14)))","v":1.5163067222733824},{"$f":"ACOS((COS('Solar Altitude'!J42)*COS('Surface Solar Azimuth Angles'!X41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J42)*COS('Input Data'!$G$14)))","v":1.5301239796945496},{"$f":"ACOS((COS('Solar Altitude'!K42)*COS('Surface Solar Azimuth Angles'!Y41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K42)*COS('Input Data'!$G$14)))","v":1.5691964416472692},{"$f":"ACOS((COS('Solar Altitude'!L42)*COS('Surface Solar Azimuth Angles'!Z41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L42)*COS('Input Data'!$G$14)))","v":1.5353536128156262},{"$f":"ACOS((COS('Solar Altitude'!M42)*COS('Surface Solar Azimuth Angles'!AA41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M42)*COS('Input Data'!$G$14)))","v":1.5434449009416622},{"$f":"ACOS((COS('Solar Altitude'!N42)*COS('Surface Solar Azimuth Angles'!AB41)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N42)*COS('Input Data'!$G$14)))","v":1.5486470318136825}]
[null,13,{"$f":"ACOS((COS('Solar Altitude'!C43)*COS('Surface Solar Azimuth Angles'!C42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C43)*COS('Input Data'!$G$14)))","v":0.80143389327010173},{"$f":"ACOS((COS('Solar Altitude'!D43)*COS('Surface Solar Azimuth Angles'!D42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D43)*COS('Input Data'!$G$14)))","v":0.96193340534168015},{"$f":"ACOS((COS('Solar Altitude'!E43)*COS('Surface Solar Azimuth Angles'!E42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E43)*COS('Input Data'!$G$14)))","v":1.1486635652967689},{"$f":"ACOS((COS('Solar Altitude'!F43)*COS('Surface Solar Azimuth Angles'!F42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F43)*COS('Input Data'!$G$14)))","v":1.358950514948307},{"$f":"ACOS((COS('Solar Altitude'!G43)*COS('Surface Solar Azimuth Angles'!G42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G43)*COS('Input Data'!$G$14)))","v":1.5057419608017095},{"$f":"ACOS((COS('Solar Altitude'!H43)*COS('Surface Solar Azimuth Angles'!H42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H43)*COS('Input Data'!$G$14)))","v":1.5586068214753657},{"$f":"ACOS((COS('Solar Altitude'!I43)*COS('Surface Solar Azimuth Angles'!I42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I43)*COS('Input Data'!$G$14)))","v":1.5055981215867127},{"$f":"ACOS((COS('Solar Altitude'!J43)*COS('Surface Solar Azimuth Angles'!J42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J43)*COS('Input Data'!$G$14)))","v":1.360983038929203},{"$f":"ACOS((COS('Solar Altitude'!K43)*COS('Surface Solar Azimuth Angles'!K42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K43)*COS('Input Data'!$G$14)))","v":1.1555065954580777},{"$f":"ACOS((COS('Solar Altitude'!L43)*COS('Surface Solar Azimuth Angles'!L42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L43)*COS('Input Data'!$G$14)))","v":0.97496153602675018},{"$f":"ACOS((COS('Solar Altitude'!M43)*COS('Surface Solar Azimuth Angles'!M42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M43)*COS('Input Data'!$G$14)))","v":0.81530489264439354},{"$f":"ACOS((COS('Solar Altitude'!N43)*COS('Surface Solar Azimuth Angles'!N42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N43)*COS('Input Data'!$G$14)))","v":0.74642809705867119},null,13,{"$f":"ACOS((COS('Solar Altitude'!C43)*COS('Surface Solar Azimuth Angles'!Q42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C43)*COS('Input Data'!$G$14)))","v":1.7416351562791885},{"$f":"ACOS((COS('Solar Altitude'!D43)*COS('Surface Solar Azimuth Angles'!R42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D43)*COS('Input Data'!$G$14)))","v":1.7378915288489052},{"$f":"ACOS((COS('Solar Altitude'!E43)*COS('Surface Solar Azimuth Angles'!S42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E43)*COS('Input Data'!$G$14)))","v":1.7687457527919199},{"$f":"ACOS((COS('Solar Altitude'!F43)*COS('Surface Solar Azimuth Angles'!T42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F43)*COS('Input Data'!$G$14)))","v":1.8011172639919026},{"$f":"ACOS((COS('Solar Altitude'!G43)*COS('Surface Solar Azimuth Angles'!U42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G43)*COS('Input Data'!$G$14)))","v":1.8003650689598554},{"$f":"ACOS((COS('Solar Altitude'!H43)*COS('Surface Solar Azimuth Angles'!V42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H43)*COS('Input Data'!$G$14)))","v":1.7765357913990427},{"$f":"ACOS((COS('Solar Altitude'!I43)*COS('Surface Solar Azimuth Angles'!W42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I43)*COS('Input Data'!$G$14)))","v":1.7613591666766877},{"$f":"ACOS((COS('Solar Altitude'!J43)*COS('Surface Solar Azimuth Angles'!X42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J43)*COS('Input Data'!$G$14)))","v":1.7860286239158996},{"$f":"ACOS((COS('Solar Altitude'!K43)*COS('Surface Solar Azimuth Angles'!Y42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K43)*COS('Input Data'!$G$14)))","v":1.8341955997417076},{"$f":"ACOS((COS('Solar Altitude'!L43)*COS('Surface Solar Azimuth Angles'!Z42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L43)*COS('Input Data'!$G$14)))","v":1.8633322624783062},{"$f":"ACOS((COS('Solar Altitude'!M43)*COS('Surface Solar Azimuth Angles'!AA42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M43)*COS('Input Data'!$G$14)))","v":1.8438546156573903},{"$f":"ACOS((COS('Solar Altitude'!N43)*COS('Surface Solar Azimuth Angles'!AB42)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N43)*COS('Input Data'!$G$14)))","v":1.788492304530646}]
[null,14,{"$f":"ACOS((COS('Solar Altitude'!C44)*COS('Surface Solar Azimuth Angles'!C43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C44)*COS('Input Data'!$G$14)))","v":0.84447622988909599},{"$f":"ACOS((COS('Solar Altitude'!D44)*COS('Surface Solar Azimuth Angles'!D43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D44)*COS('Input Data'!$G$14)))","v":1.0001765969293621},{"$f":"ACOS((COS('Solar Altitude'!E44)*COS('Surface Solar Azimuth Angles'!E43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E44)*COS('Input Data'!$G$14)))","v":1.1869632041815481},{"$f":"ACOS((COS('Solar Altitude'!F44)*COS('Surface Solar Azimuth Angles'!F43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F44)*COS('Input Data'!$G$14)))","v":1.3979095521571423},{"$f":"ACOS((COS('Solar Altitude'!G44)*COS('Surface Solar Azimuth Angles'!G43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G44)*COS('Input Data'!$G$14)))","v":1.5433502725852688},{"$f":"ACOS((COS('Solar Altitude'!H44)*COS('Surface Solar Azimuth Angles'!H43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H44)*COS('Input Data'!$G$14)))","v":1.5934380381627584},{"$f":"ACOS((COS('Solar Altitude'!I44)*COS('Surface Solar Azimuth Angles'!I43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I44)*COS('Input Data'!$G$14)))","v":1.5391855251552806},{"$f":"ACOS((COS('Solar Altitude'!J44)*COS('Surface Solar Azimuth Angles'!J43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J44)*COS('Input Data'!$G$14)))","v":1.398350072326612},{"$f":"ACOS((COS('Solar Altitude'!K44)*COS('Surface Solar Azimuth Angles'!K43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K44)*COS('Input Data'!$G$14)))","v":1.2008678278491032},{"$f":"ACOS((COS('Solar Altitude'!L44)*COS('Surface Solar Azimuth Angles'!L43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L44)*COS('Input Data'!$G$14)))","v":1.0278789267772201},{"$f":"ACOS((COS('Solar Altitude'!M44)*COS('Surface Solar Azimuth Angles'!M43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M44)*COS('Input Data'!$G$14)))","v":0.87153245136036994},{"$f":"ACOS((COS('Solar Altitude'!N44)*COS('Surface Solar Azimuth Angles'!N43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N44)*COS('Input Data'!$G$14)))","v":0.79810494053315084},null,14,{"$f":"ACOS((COS('Solar Altitude'!C44)*COS('Surface Solar Azimuth Angles'!Q43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C44)*COS('Input Data'!$G$14)))","v":1.9862113337050016},{"$f":"ACOS((COS('Solar Altitude'!D44)*COS('Surface Solar Azimuth Angles'!R43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D44)*COS('Input Data'!$G$14)))","v":1.9947700872781735},{"$f":"ACOS((COS('Solar Altitude'!E44)*COS('Surface Solar Azimuth Angles'!S43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E44)*COS('Input Data'!$G$14)))","v":2.0305451405910695},{"$f":"ACOS((COS('Solar Altitude'!F44)*COS('Surface Solar Azimuth Angles'!T43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F44)*COS('Input Data'!$G$14)))","v":2.0564415299998173},{"$f":"ACOS((COS('Solar Altitude'!G44)*COS('Surface Solar Azimuth Angles'!U43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G44)*COS('Input Data'!$G$14)))","v":2.0434987169607588},{"$f":"ACOS((COS('Solar Altitude'!H44)*COS('Surface Solar Azimuth Angles'!V43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H44)*COS('Input Data'!$G$14)))","v":2.0139721603127545},{"$f":"ACOS((COS('Solar Altitude'!I44)*COS('Surface Solar Azimuth Angles'!W43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I44)*COS('Input Data'!$G$14)))","v":2.0046578859970516},{"$f":"ACOS((COS('Solar Altitude'!J44)*COS('Surface Solar Azimuth Angles'!X43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J44)*COS('Input Data'!$G$14)))","v":2.0412100808805418},{"$f":"ACOS((COS('Solar Altitude'!K44)*COS('Surface Solar Azimuth Angles'!Y43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K44)*COS('Input Data'!$G$14)))","v":2.0959949875408572},{"$f":"ACOS((COS('Solar Altitude'!L44)*COS('Surface Solar Azimuth Angles'!Z43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L44)*COS('Input Data'!$G$14)))","v":2.1196090631829598},{"$f":"ACOS((COS('Solar Altitude'!M44)*COS('Surface Solar Azimuth Angles'!AA43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M44)*COS('Input Data'!$G$14)))","v":2.0870542787182202},{"$f":"ACOS((COS('Solar Altitude'!N44)*COS('Surface Solar Azimuth Angles'!AB43)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N44)*COS('Input Data'!$G$14)))","v":2.0257156891845645}]
[null,15,{"$f":"ACOS((COS('Solar Altitude'!C45)*COS('Surface Solar Azimuth Angles'!C44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C45)*COS('Input Data'!$G$14)))","v":0.91677391124580154},{"$f":"ACOS((COS('Solar Altitude'!D45)*COS('Surface Solar Azimuth Angles'!D44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D45)*COS('Input Data'!$G$14)))","v":1.0667749236498869},{"$f":"ACOS((COS('Solar Altitude'!E45)*COS('Surface Solar Azimuth Angles'!E44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E45)*COS('Input Data'!$G$14)))","v":1.2516797095145429},{"$f":"ACOS((COS('Solar Altitude'!F45)*COS('Surface Solar Azimuth Angles'!F44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F45)*COS('Input Data'!$G$14)))","v":1.4612788636459346},{"$f":"ACOS((COS('Solar Altitude'!G45)*COS('Surface Solar Azimuth Angles'!G44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G45)*COS('Input Data'!$G$14)))","v":1.6042759639663611},{"$f":"ACOS((COS('Solar Altitude'!H45)*COS('Surface Solar Azimuth Angles'!H44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H45)*COS('Input Data'!$G$14)))","v":1.6514479530748039},{"$f":"ACOS((COS('Solar Altitude'!I45)*COS('Surface Solar Azimuth Angles'!I44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I45)*COS('Input Data'!$G$14)))","v":1.5965765023442655},{"$f":"ACOS((COS('Solar Altitude'!J45)*COS('Surface Solar Azimuth Angles'!J44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J45)*COS('Input Data'!$G$14)))","v":1.460335404321973},{"$f":"ACOS((COS('Solar Altitude'!K45)*COS('Surface Solar Azimuth Angles'!K44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K45)*COS('Input Data'!$G$14)))","v":1.271337108609143},{"$f":"ACOS((COS('Solar Altitude'!L45)*COS('Surface Solar Azimuth Angles'!L44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L45)*COS('Input Data'!$G$14)))","v":1.1058670206244512},{"$f":"ACOS((COS('Solar Altitude'!M45)*COS('Surface Solar Azimuth Angles'!M44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M45)*COS('Input Data'!$G$14)))","v":0.95345098633863656},{"$f":"ACOS((COS('Solar Altitude'!N45)*COS('Surface Solar Azimuth Angles'!N44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N45)*COS('Input Data'!$G$14)))","v":0.87749844669584809},null,15,{"$f":"ACOS((COS('Solar Altitude'!C45)*COS('Surface Solar Azimuth Angles'!Q44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C45)*COS('Input Data'!$G$14)))","v":2.2263871865236671},{"$f":"ACOS((COS('Solar Altitude'!D45)*COS('Surface Solar Azimuth Angles'!R44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D45)*COS('Input Data'!$G$14)))","v":2.2503131901111768},{"$f":"ACOS((COS('Solar Altitude'!E45)*COS('Surface Solar Azimuth Angles'!S44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E45)*COS('Input Data'!$G$14)))","v":2.2923445283902195},{"$f":"ACOS((COS('Solar Altitude'!F45)*COS('Surface Solar Azimuth Angles'!T44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F45)*COS('Input Data'!$G$14)))","v":2.3096729339598836},{"$f":"ACOS((COS('Solar Altitude'!G45)*COS('Surface Solar Azimuth Angles'!U44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G45)*COS('Input Data'!$G$14)))","v":2.2810193061754851},{"$f":"ACOS((COS('Solar Altitude'!H45)*COS('Surface Solar Azimuth Angles'!V44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H45)*COS('Input Data'!$G$14)))","v":2.2447850459271042},{"$f":"ACOS((COS('Solar Altitude'!I45)*COS('Surface Solar Azimuth Angles'!W44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I45)*COS('Input Data'!$G$14)))","v":2.2429795953364104},{"$f":"ACOS((COS('Solar Altitude'!J45)*COS('Surface Solar Azimuth Angles'!X44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J45)*COS('Input Data'!$G$14)))","v":2.2943435136025983},{"$f":"ACOS((COS('Solar Altitude'!K45)*COS('Surface Solar Azimuth Angles'!Y44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K45)*COS('Input Data'!$G$14)))","v":2.3577943753400068},{"$f":"ACOS((COS('Solar Altitude'!L45)*COS('Surface Solar Azimuth Angles'!Z44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L45)*COS('Input Data'!$G$14)))","v":2.3737585812189774},{"$f":"ACOS((COS('Solar Altitude'!M45)*COS('Surface Solar Azimuth Angles'!AA44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M45)*COS('Input Data'!$G$14)))","v":2.3239471556762532},{"$f":"ACOS((COS('Solar Altitude'!N45)*COS('Surface Solar Azimuth Angles'!AB44)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N45)*COS('Input Data'!$G$14)))","v":2.256032004200681}]
[null,16,{"$f":"ACOS((COS('Solar Altitude'!C46)*COS('Surface Solar Azimuth Angles'!C45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C46)*COS('Input Data'!$G$14)))","v":1.0095306833958722},{"$f":"ACOS((COS('Solar Altitude'!D46)*COS('Surface Solar Azimuth Angles'!D45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D46)*COS('Input Data'!$G$14)))","v":1.1546654243285206},{"$f":"ACOS((COS('Solar Altitude'!E46)*COS('Surface Solar Azimuth Angles'!E45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E46)*COS('Input Data'!$G$14)))","v":1.3370759528261966},{"$f":"ACOS((COS('Solar Altitude'!F46)*COS('Surface Solar Azimuth Angles'!F45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F46)*COS('Input Data'!$G$14)))","v":1.5444380523629393},{"$f":"ACOS((COS('Solar Altitude'!G46)*COS('Surface Solar Azimuth Angles'!G45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G46)*COS('Input Data'!$G$14)))","v":1.68463017418009},{"$f":"ACOS((COS('Solar Altitude'!H46)*COS('Surface Solar Azimuth Angles'!H45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H46)*COS('Input Data'!$G$14)))","v":1.7290932660077274},{"$f":"ACOS((COS('Solar Altitude'!I46)*COS('Surface Solar Azimuth Angles'!I45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I46)*COS('Input Data'!$G$14)))","v":1.6740657843131033},{"$f":"ACOS((COS('Solar Altitude'!J46)*COS('Surface Solar Azimuth Angles'!J45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J46)*COS('Input Data'!$G$14)))","v":1.5424031055346816},{"$f":"ACOS((COS('Solar Altitude'!K46)*COS('Surface Solar Azimuth Angles'!K45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K46)*COS('Input Data'!$G$14)))","v":1.3609042997817127},{"$f":"ACOS((COS('Solar Altitude'!L46)*COS('Surface Solar Azimuth Angles'!L45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L46)*COS('Input Data'!$G$14)))","v":1.201431233976219},{"$f":"ACOS((COS('Solar Altitude'!M46)*COS('Surface Solar Azimuth Angles'!M45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M46)*COS('Input Data'!$G$14)))","v":1.0521379302574527},{"$f":"ACOS((COS('Solar Altitude'!N46)*COS('Surface Solar Azimuth Angles'!N45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N46)*COS('Input Data'!$G$14)))","v":0.97499068113116927},null,16,{"$f":"ACOS((COS('Solar Altitude'!C46)*COS('Surface Solar Azimuth Angles'!Q45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C46)*COS('Input Data'!$G$14)))","v":2.4561527189639456},{"$f":"ACOS((COS('Solar Altitude'!D46)*COS('Surface Solar Azimuth Angles'!R45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D46)*COS('Input Data'!$G$14)))","v":2.5024766008818276},{"$f":"ACOS((COS('Solar Altitude'!E46)*COS('Surface Solar Azimuth Angles'!S45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E46)*COS('Input Data'!$G$14)))","v":2.5541439161893686},{"$f":"ACOS((COS('Solar Altitude'!F46)*COS('Surface Solar Azimuth Angles'!T45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F46)*COS('Input Data'!$G$14)))","v":2.5575524339236404},{"$f":"ACOS((COS('Solar Altitude'!G46)*COS('Surface Solar Azimuth Angles'!U45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G46)*COS('Input Data'!$G$14)))","v":2.5052571644083828},{"$f":"ACOS((COS('Solar Altitude'!H46)*COS('Surface Solar Azimuth Angles'!V45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H46)*COS('Input Data'!$G$14)))","v":2.4604797004373173},{"$f":"ACOS((COS('Solar Altitude'!I46)*COS('Surface Solar Azimuth Angles'!W45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I46)*COS('Input Data'!$G$14)))","v":2.4695927665354112},{"$f":"ACOS((COS('Solar Altitude'!J46)*COS('Surface Solar Azimuth Angles'!X45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J46)*COS('Input Data'!$G$14)))","v":2.542277402699114},{"$f":"ACOS((COS('Solar Altitude'!K46)*COS('Surface Solar Azimuth Angles'!Y45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K46)*COS('Input Data'!$G$14)))","v":2.6195937631391555},{"$f":"ACOS((COS('Solar Altitude'!L46)*COS('Surface Solar Azimuth Angles'!Z45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L46)*COS('Input Data'!$G$14)))","v":2.622222112011336},{"$f":"ACOS((COS('Solar Altitude'!M46)*COS('Surface Solar Azimuth Angles'!AA45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M46)*COS('Input Data'!$G$14)))","v":2.5456912493713983},{"$f":"ACOS((COS('Solar Altitude'!N46)*COS('Surface Solar Azimuth Angles'!AB45)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N46)*COS('Input Data'!$G$14)))","v":2.4705810581096146}]
[null,17,{"$f":"ACOS((COS('Solar Altitude'!C47)*COS('Surface Solar Azimuth Angles'!C46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C47)*COS('Input Data'!$G$14)))","v":1.114157261660677},{"$f":"ACOS((COS('Solar Altitude'!D47)*COS('Surface Solar Azimuth Angles'!D46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D47)*COS('Input Data'!$G$14)))","v":1.2562972070801592},{"$f":"ACOS((COS('Solar Altitude'!E47)*COS('Surface Solar Azimuth Angles'!E46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E47)*COS('Input Data'!$G$14)))","v":1.4367091502252052},{"$f":"ACOS((COS('Solar Altitude'!F47)*COS('Surface Solar Azimuth Angles'!F46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F47)*COS('Input Data'!$G$14)))","v":1.6420075729899812},{"$f":"ACOS((COS('Solar Altitude'!G47)*COS('Surface Solar Azimuth Angles'!G46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G47)*COS('Input Data'!$G$14)))","v":1.7797557130362189},{"$f":"ACOS((COS('Solar Altitude'!H47)*COS('Surface Solar Azimuth Angles'!H46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H47)*COS('Input Data'!$G$14)))","v":1.8220358562074812},{"$f":"ACOS((COS('Solar Altitude'!I47)*COS('Surface Solar Azimuth Angles'!I46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I47)*COS('Input Data'!$G$14)))","v":1.7671068430582939},{"$f":"ACOS((COS('Solar Altitude'!J47)*COS('Surface Solar Azimuth Angles'!J46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J47)*COS('Input Data'!$G$14)))","v":1.6392201933187758},{"$f":"ACOS((COS('Solar Altitude'!K47)*COS('Surface Solar Azimuth Angles'!K46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K47)*COS('Input Data'!$G$14)))","v":1.4630820983257666},{"$f":"ACOS((COS('Solar Altitude'!L47)*COS('Surface Solar Azimuth Angles'!L46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L47)*COS('Input Data'!$G$14)))","v":1.3071741302147308},{"$f":"ACOS((COS('Solar Altitude'!M47)*COS('Surface Solar Azimuth Angles'!M46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M47)*COS('Input Data'!$G$14)))","v":1.15944298224515},{"$f":"ACOS((COS('Solar Altitude'!N47)*COS('Surface Solar Azimuth Angles'!N46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N47)*COS('Input Data'!$G$14)))","v":1.0818799850793841},null,17,{"$f":"ACOS((COS('Solar Altitude'!C47)*COS('Surface Solar Azimuth Angles'!Q46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C47)*COS('Input Data'!$G$14)))","v":2.6592207922251774},{"$f":"ACOS((COS('Solar Altitude'!D47)*COS('Surface Solar Azimuth Angles'!R46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D47)*COS('Input Data'!$G$14)))","v":2.7443517691260602},{"$f":"ACOS((COS('Solar Altitude'!E47)*COS('Surface Solar Azimuth Angles'!S46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E47)*COS('Input Data'!$G$14)))","v":2.8159433039885173},{"$f":"ACOS((COS('Solar Altitude'!F47)*COS('Surface Solar Azimuth Angles'!T46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F47)*COS('Input Data'!$G$14)))","v":2.7881113603845131},{"$f":"ACOS((COS('Solar Altitude'!G47)*COS('Surface Solar Azimuth Angles'!U46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G47)*COS('Input Data'!$G$14)))","v":2.694584611130705},{"$f":"ACOS((COS('Solar Altitude'!H47)*COS('Surface Solar Azimuth Angles'!V46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H47)*COS('Input Data'!$G$14)))","v":2.6397440297185253},{"$f":"ACOS((COS('Solar Altitude'!I47)*COS('Surface Solar Azimuth Angles'!W46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I47)*COS('Input Data'!$G$14)))","v":2.6662351946255844},{"$f":"ACOS((COS('Solar Altitude'!J47)*COS('Surface Solar Azimuth Angles'!X46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J47)*COS('Input Data'!$G$14)))","v":2.7738053629994313},{"$f":"ACOS((COS('Solar Altitude'!K47)*COS('Surface Solar Azimuth Angles'!Y46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K47)*COS('Input Data'!$G$14)))","v":2.8813931509383051},{"$f":"ACOS((COS('Solar Altitude'!L47)*COS('Surface Solar Azimuth Angles'!Z46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L47)*COS('Input Data'!$G$14)))","v":2.8496447047403861},{"$f":"ACOS((COS('Solar Altitude'!M47)*COS('Surface Solar Azimuth Angles'!AA46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M47)*COS('Input Data'!$G$14)))","v":2.7261618473809248},{"$f":"ACOS((COS('Solar Altitude'!N47)*COS('Surface Solar Azimuth Angles'!AB46)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N47)*COS('Input Data'!$G$14)))","v":2.6469898802021596}]
[null,18,{"$f":"ACOS((COS('Solar Altitude'!C48)*COS('Surface Solar Azimuth Angles'!C47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C48)*COS('Input Data'!$G$14)))","v":1.2232040423103281},{"$f":"ACOS((COS('Solar Altitude'!D48)*COS('Surface Solar Azimuth Angles'!D47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D48)*COS('Input Data'!$G$14)))","v":1.3645739055932193},{"$f":"ACOS((COS('Solar Altitude'!E48)*COS('Surface Solar Azimuth Angles'!E47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E48)*COS('Input Data'!$G$14)))","v":1.5441304951050601},{"$f":"ACOS((COS('Solar Altitude'!F48)*COS('Surface Solar Azimuth Angles'!F47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F48)*COS('Input Data'!$G$14)))","v":1.7483023474615491},{"$f":"ACOS((COS('Solar Altitude'!G48)*COS('Surface Solar Azimuth Angles'!G47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G48)*COS('Input Data'!$G$14)))","v":1.8845581906693991},{"$f":"ACOS((COS('Solar Altitude'!H48)*COS('Surface Solar Azimuth Angles'!H47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H48)*COS('Input Data'!$G$14)))","v":1.9254538063970768},{"$f":"ACOS((COS('Solar Altitude'!I48)*COS('Surface Solar Azimuth Angles'!I47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I48)*COS('Input Data'!$G$14)))","v":1.8706790061613969},{"$f":"ACOS((COS('Solar Altitude'!J48)*COS('Surface Solar Azimuth Angles'!J47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J48)*COS('Input Data'!$G$14)))","v":1.7451272381387013},{"$f":"ACOS((COS('Solar Altitude'!K48)*COS('Surface Solar Azimuth Angles'!K47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K48)*COS('Input Data'!$G$14)))","v":1.5714648658845654},{"$f":"ACOS((COS('Solar Altitude'!L48)*COS('Surface Solar Azimuth Angles'!L47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L48)*COS('Input Data'!$G$14)))","v":1.416310170166726},{"$f":"ACOS((COS('Solar Altitude'!M48)*COS('Surface Solar Azimuth Angles'!M47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M48)*COS('Input Data'!$G$14)))","v":1.2683988318675119},{"$f":"ACOS((COS('Solar Altitude'!N48)*COS('Surface Solar Azimuth Angles'!N47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N48)*COS('Input Data'!$G$14)))","v":1.1909321948811751},null,18,{"$f":"ACOS((COS('Solar Altitude'!C48)*COS('Surface Solar Azimuth Angles'!Q47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C48)*COS('Input Data'!$G$14)))","v":2.785543338653973},{"$f":"ACOS((COS('Solar Altitude'!D48)*COS('Surface Solar Azimuth Angles'!R47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D48)*COS('Input Data'!$G$14)))","v":2.9353085327964417},{"$f":"ACOS((COS('Solar Altitude'!E48)*COS('Surface Solar Azimuth Angles'!S47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E48)*COS('Input Data'!$G$14)))","v":3.0777426917876682},{"$f":"ACOS((COS('Solar Altitude'!F48)*COS('Surface Solar Azimuth Angles'!T47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F48)*COS('Input Data'!$G$14)))","v":2.9322606102243371},{"$f":"ACOS((COS('Solar Altitude'!G48)*COS('Surface Solar Azimuth Angles'!U47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G48)*COS('Input Data'!$G$14)))","v":2.7869128705359616},{"$f":"ACOS((COS('Solar Altitude'!H48)*COS('Surface Solar Azimuth Angles'!V47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H48)*COS('Input Data'!$G$14)))","v":2.7307180571082115},{"$f":"ACOS((COS('Solar Altitude'!I48)*COS('Surface Solar Azimuth Angles'!W47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I48)*COS('Input Data'!$G$14)))","v":2.7793021618829634},{"$f":"ACOS((COS('Solar Altitude'!J48)*COS('Surface Solar Azimuth Angles'!X47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J48)*COS('Input Data'!$G$14)))","v":2.9264100687213448},{"$f":"ACOS((COS('Solar Altitude'!K48)*COS('Surface Solar Azimuth Angles'!Y47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K48)*COS('Input Data'!$G$14)))","v":3.1399927684421303},{"$f":"ACOS((COS('Solar Altitude'!L48)*COS('Surface Solar Azimuth Angles'!Z47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L48)*COS('Input Data'!$G$14)))","v":2.951430770955481},{"$f":"ACOS((COS('Solar Altitude'!M48)*COS('Surface Solar Azimuth Angles'!AA47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M48)*COS('Input Data'!$G$14)))","v":2.7931053500685721},{"$f":"ACOS((COS('Solar Altitude'!N48)*COS('Surface Solar Azimuth Angles'!AB47)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N48)*COS('Input Data'!$G$14)))","v":2.7316415819726259}]
[null,19,{"$f":"ACOS((COS('Solar Altitude'!C49)*COS('Surface Solar Azimuth Angles'!C48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C49)*COS('Input Data'!$G$14)))","v":1.3302879203266533},{"$f":"ACOS((COS('Solar Altitude'!D49)*COS('Surface Solar Azimuth Angles'!D48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D49)*COS('Input Data'!$G$14)))","v":1.4730184082815458},{"$f":"ACOS((COS('Solar Altitude'!E49)*COS('Surface Solar Azimuth Angles'!E48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E49)*COS('Input Data'!$G$14)))","v":1.6530665123238681},{"$f":"ACOS((COS('Solar Altitude'!F49)*COS('Surface Solar Azimuth Angles'!F48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F49)*COS('Input Data'!$G$14)))","v":1.8574385623360405},{"$f":"ACOS((COS('Solar Altitude'!G49)*COS('Surface Solar Azimuth Angles'!G48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G49)*COS('Input Data'!$G$14)))","v":1.993560365526901},{"$f":"ACOS((COS('Solar Altitude'!H49)*COS('Surface Solar Azimuth Angles'!H48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H49)*COS('Input Data'!$G$14)))","v":2.0341001790741142},{"$f":"ACOS((COS('Solar Altitude'!I49)*COS('Surface Solar Azimuth Angles'!I48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I49)*COS('Input Data'!$G$14)))","v":1.9793856064713129},{"$f":"ACOS((COS('Solar Altitude'!J49)*COS('Surface Solar Azimuth Angles'!J48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J49)*COS('Input Data'!$G$14)))","v":1.8542632392691485},{"$f":"ACOS((COS('Solar Altitude'!K49)*COS('Surface Solar Azimuth Angles'!K48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K49)*COS('Input Data'!$G$14)))","v":1.6798096938481448},{"$f":"ACOS((COS('Solar Altitude'!L49)*COS('Surface Solar Azimuth Angles'!L48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L49)*COS('Input Data'!$G$14)))","v":1.522603105071384},{"$f":"ACOS((COS('Solar Altitude'!M49)*COS('Surface Solar Azimuth Angles'!M48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M49)*COS('Input Data'!$G$14)))","v":1.3729601422820714},{"$f":"ACOS((COS('Solar Altitude'!N49)*COS('Surface Solar Azimuth Angles'!N48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N49)*COS('Input Data'!$G$14)))","v":1.2960649237509485},null,19,{"$f":"ACOS((COS('Solar Altitude'!C49)*COS('Surface Solar Azimuth Angles'!Q48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C49)*COS('Input Data'!$G$14)))","v":2.751282665597893},{"$f":"ACOS((COS('Solar Altitude'!D49)*COS('Surface Solar Azimuth Angles'!R48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D49)*COS('Input Data'!$G$14)))","v":2.8909857355299886},{"$f":"ACOS((COS('Solar Altitude'!E49)*COS('Surface Solar Azimuth Angles'!S48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E49)*COS('Input Data'!$G$14)))","v":2.9436432275927684},{"$f":"ACOS((COS('Solar Altitude'!F49)*COS('Surface Solar Azimuth Angles'!T48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F49)*COS('Input Data'!$G$14)))","v":2.8288909506839368},{"$f":"ACOS((COS('Solar Altitude'!G49)*COS('Surface Solar Azimuth Angles'!U48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G49)*COS('Input Data'!$G$14)))","v":2.7137534044824214},{"$f":"ACOS((COS('Solar Altitude'!H49)*COS('Surface Solar Azimuth Angles'!V48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H49)*COS('Input Data'!$G$14)))","v":2.6778226050543497},{"$f":"ACOS((COS('Solar Altitude'!I49)*COS('Surface Solar Azimuth Angles'!W48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I49)*COS('Input Data'!$G$14)))","v":2.7320954449458243},{"$f":"ACOS((COS('Solar Altitude'!J49)*COS('Surface Solar Azimuth Angles'!X48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J49)*COS('Input Data'!$G$14)))","v":2.8376801773294518},{"$f":"ACOS((COS('Solar Altitude'!K49)*COS('Surface Solar Azimuth Angles'!Y48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K49)*COS('Input Data'!$G$14)))","v":2.8781933806429816},{"$f":"ACOS((COS('Solar Altitude'!L49)*COS('Surface Solar Azimuth Angles'!Z48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L49)*COS('Input Data'!$G$14)))","v":2.7915042028627788},{"$f":"ACOS((COS('Solar Altitude'!M49)*COS('Surface Solar Azimuth Angles'!AA48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M49)*COS('Input Data'!$G$14)))","v":2.6923727979996803},{"$f":"ACOS((COS('Solar Altitude'!N49)*COS('Surface Solar Azimuth Angles'!AB48)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N49)*COS('Input Data'!$G$14)))","v":2.6717106411392466}]
[null,20,{"$f":"ACOS((COS('Solar Altitude'!C50)*COS('Surface Solar Azimuth Angles'!C49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C50)*COS('Input Data'!$G$14)))","v":1.4297298014275222},{"$f":"ACOS((COS('Solar Altitude'!D50)*COS('Surface Solar Azimuth Angles'!D49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D50)*COS('Input Data'!$G$14)))","v":1.5755795443185125},{"$f":"ACOS((COS('Solar Altitude'!E50)*COS('Surface Solar Azimuth Angles'!E49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E50)*COS('Input Data'!$G$14)))","v":1.7572927734324946},{"$f":"ACOS((COS('Solar Altitude'!F50)*COS('Surface Solar Azimuth Angles'!F49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F50)*COS('Input Data'!$G$14)))","v":1.9631775905342721},{"$f":"ACOS((COS('Solar Altitude'!G50)*COS('Surface Solar Azimuth Angles'!G49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G50)*COS('Input Data'!$G$14)))","v":2.1006953852780001},{"$f":"ACOS((COS('Solar Altitude'!H50)*COS('Surface Solar Azimuth Angles'!H49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H50)*COS('Input Data'!$G$14)))","v":2.1420955835891404},{"$f":"ACOS((COS('Solar Altitude'!I50)*COS('Surface Solar Azimuth Angles'!I49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I50)*COS('Input Data'!$G$14)))","v":2.0872831476777836},{"$f":"ACOS((COS('Solar Altitude'!J50)*COS('Surface Solar Azimuth Angles'!J49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J50)*COS('Input Data'!$G$14)))","v":1.9604202767828434},{"$f":"ACOS((COS('Solar Altitude'!K50)*COS('Surface Solar Azimuth Angles'!K49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K50)*COS('Input Data'!$G$14)))","v":1.7818724301524667},{"$f":"ACOS((COS('Solar Altitude'!L50)*COS('Surface Solar Azimuth Angles'!L49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L50)*COS('Input Data'!$G$14)))","v":1.620127370215197},{"$f":"ACOS((COS('Solar Altitude'!M50)*COS('Surface Solar Azimuth Angles'!M49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M50)*COS('Input Data'!$G$14)))","v":1.4676473148387799},{"$f":"ACOS((COS('Solar Altitude'!N50)*COS('Surface Solar Azimuth Angles'!N49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N50)*COS('Input Data'!$G$14)))","v":1.3919107717000823},null,20,{"$f":"ACOS((COS('Solar Altitude'!C50)*COS('Surface Solar Azimuth Angles'!Q49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C50)*COS('Input Data'!$G$14)))","v":2.5854127241321807},{"$f":"ACOS((COS('Solar Altitude'!D50)*COS('Surface Solar Azimuth Angles'!R49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D50)*COS('Input Data'!$G$14)))","v":2.6741107477984687},{"$f":"ACOS((COS('Solar Altitude'!E50)*COS('Surface Solar Azimuth Angles'!S49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E50)*COS('Input Data'!$G$14)))","v":2.6818438397936193},{"$f":"ACOS((COS('Solar Altitude'!F50)*COS('Surface Solar Azimuth Angles'!T49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F50)*COS('Input Data'!$G$14)))","v":2.6060627469610238},{"$f":"ACOS((COS('Solar Altitude'!G50)*COS('Surface Solar Azimuth Angles'!U49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G50)*COS('Input Data'!$G$14)))","v":2.532146657802449},{"$f":"ACOS((COS('Solar Altitude'!H50)*COS('Surface Solar Azimuth Angles'!V49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H50)*COS('Input Data'!$G$14)))","v":2.5166950081533845},{"$f":"ACOS((COS('Solar Altitude'!I50)*COS('Surface Solar Azimuth Angles'!W49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I50)*COS('Input Data'!$G$14)))","v":2.5626485528760363},{"$f":"ACOS((COS('Solar Altitude'!J50)*COS('Surface Solar Azimuth Angles'!X49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J50)*COS('Input Data'!$G$14)))","v":2.6187099029073515},{"$f":"ACOS((COS('Solar Altitude'!K50)*COS('Surface Solar Azimuth Angles'!Y49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K50)*COS('Input Data'!$G$14)))","v":2.6163939928438325},{"$f":"ACOS((COS('Solar Altitude'!L50)*COS('Surface Solar Azimuth Angles'!Z49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L50)*COS('Input Data'!$G$14)))","v":2.5547559960547841},{"$f":"ACOS((COS('Solar Altitude'!M50)*COS('Surface Solar Azimuth Angles'!AA49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M50)*COS('Input Data'!$G$14)))","v":2.4985832089606257},{"$f":"ACOS((COS('Solar Altitude'!N50)*COS('Surface Solar Azimuth Angles'!AB49)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N50)*COS('Input Data'!$G$14)))","v":2.5070460567990436}]
[null,21,{"$f":"ACOS((COS('Solar Altitude'!C51)*COS('Surface Solar Azimuth Angles'!C50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C51)*COS('Input Data'!$G$14)))","v":1.516275064850793},{"$f":"ACOS((COS('Solar Altitude'!D51)*COS('Surface Solar Azimuth Angles'!D50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D51)*COS('Input Data'!$G$14)))","v":1.6664155507924101},{"$f":"ACOS((COS('Solar Altitude'!E51)*COS('Surface Solar Azimuth Angles'!E50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E51)*COS('Input Data'!$G$14)))","v":1.85044833041965},{"$f":"ACOS((COS('Solar Altitude'!F51)*COS('Surface Solar Azimuth Angles'!F50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F51)*COS('Input Data'!$G$14)))","v":2.0586760807886622},{"$f":"ACOS((COS('Solar Altitude'!G51)*COS('Surface Solar Azimuth Angles'!G50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G51)*COS('Input Data'!$G$14)))","v":2.1989407669837076},{"$f":"ACOS((COS('Solar Altitude'!H51)*COS('Surface Solar Azimuth Angles'!H50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H51)*COS('Input Data'!$G$14)))","v":2.2425167260227736},{"$f":"ACOS((COS('Solar Altitude'!I51)*COS('Surface Solar Azimuth Angles'!I50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I51)*COS('Input Data'!$G$14)))","v":2.1875259158759262},{"$f":"ACOS((COS('Solar Altitude'!J51)*COS('Surface Solar Azimuth Angles'!J50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J51)*COS('Input Data'!$G$14)))","v":2.0567908427719601},{"$f":"ACOS((COS('Solar Altitude'!K51)*COS('Surface Solar Azimuth Angles'!K50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K51)*COS('Input Data'!$G$14)))","v":1.8712451895573825},{"$f":"ACOS((COS('Solar Altitude'!L51)*COS('Surface Solar Azimuth Angles'!L50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L51)*COS('Input Data'!$G$14)))","v":1.7031231100563671},{"$f":"ACOS((COS('Solar Altitude'!M51)*COS('Surface Solar Azimuth Angles'!M50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M51)*COS('Input Data'!$G$14)))","v":1.5473529149923007},{"$f":"ACOS((COS('Solar Altitude'!N51)*COS('Surface Solar Azimuth Angles'!N50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N51)*COS('Input Data'!$G$14)))","v":1.4735530327019799},null,21,{"$f":"ACOS((COS('Solar Altitude'!C51)*COS('Surface Solar Azimuth Angles'!Q50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C51)*COS('Input Data'!$G$14)))","v":2.3686915997301274},{"$f":"ACOS((COS('Solar Altitude'!D51)*COS('Surface Solar Azimuth Angles'!R50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D51)*COS('Input Data'!$G$14)))","v":2.4276915216774144},{"$f":"ACOS((COS('Solar Altitude'!E51)*COS('Surface Solar Azimuth Angles'!S50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E51)*COS('Input Data'!$G$14)))","v":2.4200444519944702},{"$f":"ACOS((COS('Solar Altitude'!F51)*COS('Surface Solar Azimuth Angles'!T50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F51)*COS('Input Data'!$G$14)))","v":2.3601288269844716},{"$f":"ACOS((COS('Solar Altitude'!G51)*COS('Surface Solar Azimuth Angles'!U50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G51)*COS('Input Data'!$G$14)))","v":2.3106595059453436},{"$f":"ACOS((COS('Solar Altitude'!H51)*COS('Surface Solar Azimuth Angles'!V50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H51)*COS('Input Data'!$G$14)))","v":2.3082477773479204},{"$f":"ACOS((COS('Solar Altitude'!I51)*COS('Surface Solar Azimuth Angles'!W50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I51)*COS('Input Data'!$G$14)))","v":2.3457984733690864},{"$f":"ACOS((COS('Solar Altitude'!J51)*COS('Surface Solar Azimuth Angles'!X50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J51)*COS('Input Data'!$G$14)))","v":2.3739516356299211},{"$f":"ACOS((COS('Solar Altitude'!K51)*COS('Surface Solar Azimuth Angles'!Y50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K51)*COS('Input Data'!$G$14)))","v":2.3545946050446833},{"$f":"ACOS((COS('Solar Altitude'!L51)*COS('Surface Solar Azimuth Angles'!Z50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L51)*COS('Input Data'!$G$14)))","v":2.3040675436217906},{"$f":"ACOS((COS('Solar Altitude'!M51)*COS('Surface Solar Azimuth Angles'!AA50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M51)*COS('Input Data'!$G$14)))","v":2.2721662590002261},{"$f":"ACOS((COS('Solar Altitude'!N51)*COS('Surface Solar Azimuth Angles'!AB50)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N51)*COS('Input Data'!$G$14)))","v":2.2971884180004607}]
[null,22,{"$f":"ACOS((COS('Solar Altitude'!C52)*COS('Surface Solar Azimuth Angles'!C51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C52)*COS('Input Data'!$G$14)))","v":1.5850470871678939},{"$f":"ACOS((COS('Solar Altitude'!D52)*COS('Surface Solar Azimuth Angles'!D51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D52)*COS('Input Data'!$G$14)))","v":1.7398692437207732},{"$f":"ACOS((COS('Solar Altitude'!E52)*COS('Surface Solar Azimuth Angles'!E51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E52)*COS('Input Data'!$G$14)))","v":1.9260356433135979},{"$f":"ACOS((COS('Solar Altitude'!F52)*COS('Surface Solar Azimuth Angles'!F51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F52)*COS('Input Data'!$G$14)))","v":2.1364174701839387},{"$f":"ACOS((COS('Solar Altitude'!G52)*COS('Surface Solar Azimuth Angles'!G51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G52)*COS('Input Data'!$G$14)))","v":2.2800604106209237},{"$f":"ACOS((COS('Solar Altitude'!H52)*COS('Surface Solar Azimuth Angles'!H51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H52)*COS('Input Data'!$G$14)))","v":2.3270057980317911},{"$f":"ACOS((COS('Solar Altitude'!I52)*COS('Surface Solar Azimuth Angles'!I51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I52)*COS('Input Data'!$G$14)))","v":2.2720550890382776},{"$f":"ACOS((COS('Solar Altitude'!J52)*COS('Surface Solar Azimuth Angles'!J51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J52)*COS('Input Data'!$G$14)))","v":2.1358749746873902},{"$f":"ACOS((COS('Solar Altitude'!K52)*COS('Surface Solar Azimuth Angles'!K51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K52)*COS('Input Data'!$G$14)))","v":1.941441970347938},{"$f":"ACOS((COS('Solar Altitude'!L52)*COS('Surface Solar Azimuth Angles'!L51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L52)*COS('Input Data'!$G$14)))","v":1.7661199813310025},{"$f":"ACOS((COS('Solar Altitude'!M52)*COS('Surface Solar Azimuth Angles'!M51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M52)*COS('Input Data'!$G$14)))","v":1.6074116270730319},{"$f":"ACOS((COS('Solar Altitude'!N52)*COS('Surface Solar Azimuth Angles'!N51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N52)*COS('Input Data'!$G$14)))","v":1.5365206299534897},null,22,{"$f":"ACOS((COS('Solar Altitude'!C52)*COS('Surface Solar Azimuth Angles'!Q51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C52)*COS('Input Data'!$G$14)))","v":2.1337797676592309},{"$f":"ACOS((COS('Solar Altitude'!D52)*COS('Surface Solar Azimuth Angles'!R51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D52)*COS('Input Data'!$G$14)))","v":2.1741572293084008},{"$f":"ACOS((COS('Solar Altitude'!E52)*COS('Surface Solar Azimuth Angles'!S51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E52)*COS('Input Data'!$G$14)))","v":2.1582450641953206},{"$f":"ACOS((COS('Solar Altitude'!F52)*COS('Surface Solar Azimuth Angles'!T51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F52)*COS('Input Data'!$G$14)))","v":2.1075988694625947},{"$f":"ACOS((COS('Solar Altitude'!G52)*COS('Surface Solar Azimuth Angles'!U51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G52)*COS('Input Data'!$G$14)))","v":2.074261638341969},{"$f":"ACOS((COS('Solar Altitude'!H52)*COS('Surface Solar Azimuth Angles'!V51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H52)*COS('Input Data'!$G$14)))","v":2.0805487915276242},{"$f":"ACOS((COS('Solar Altitude'!I52)*COS('Surface Solar Azimuth Angles'!W51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I52)*COS('Input Data'!$G$14)))","v":2.1114654362427365},{"$f":"ACOS((COS('Solar Altitude'!J52)*COS('Surface Solar Azimuth Angles'!X51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J52)*COS('Input Data'!$G$14)))","v":2.1219639352882806},{"$f":"ACOS((COS('Solar Altitude'!K52)*COS('Surface Solar Azimuth Angles'!Y51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K52)*COS('Input Data'!$G$14)))","v":2.0927952172455333},{"$f":"ACOS((COS('Solar Altitude'!L52)*COS('Surface Solar Azimuth Angles'!Z51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L52)*COS('Input Data'!$G$14)))","v":2.0491282519194653},{"$f":"ACOS((COS('Solar Altitude'!M52)*COS('Surface Solar Azimuth Angles'!AA51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M52)*COS('Input Data'!$G$14)))","v":2.0333792885124597},{"$f":"ACOS((COS('Solar Altitude'!N52)*COS('Surface Solar Azimuth Angles'!AB51)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N52)*COS('Input Data'!$G$14)))","v":2.0688885622515065}]
[null,23,{"$f":"ACOS((COS('Solar Altitude'!C53)*COS('Surface Solar Azimuth Angles'!C52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C53)*COS('Input Data'!$G$14)))","v":1.6317837726042219},{"$f":"ACOS((COS('Solar Altitude'!D53)*COS('Surface Solar Azimuth Angles'!D52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D53)*COS('Input Data'!$G$14)))","v":1.7907734195006288},{"$f":"ACOS((COS('Solar Altitude'!E53)*COS('Surface Solar Azimuth Angles'!E52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E53)*COS('Input Data'!$G$14)))","v":1.9778498329698173},{"$f":"ACOS((COS('Solar Altitude'!F53)*COS('Surface Solar Azimuth Angles'!F52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F53)*COS('Input Data'!$G$14)))","v":2.1887517598022255},{"$f":"ACOS((COS('Solar Altitude'!G53)*COS('Surface Solar Azimuth Angles'!G52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G53)*COS('Input Data'!$G$14)))","v":2.3350566216450277},{"$f":"ACOS((COS('Solar Altitude'!H53)*COS('Surface Solar Azimuth Angles'!H52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H53)*COS('Input Data'!$G$14)))","v":2.3860236161095916},{"$f":"ACOS((COS('Solar Altitude'!I53)*COS('Surface Solar Azimuth Angles'!I52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I53)*COS('Input Data'!$G$14)))","v":2.3318766229389749},{"$f":"ACOS((COS('Solar Altitude'!J53)*COS('Surface Solar Azimuth Angles'!J52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J53)*COS('Input Data'!$G$14)))","v":2.189970058828508},{"$f":"ACOS((COS('Solar Altitude'!K53)*COS('Surface Solar Azimuth Angles'!K52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K53)*COS('Input Data'!$G$14)))","v":1.986464298943392},{"$f":"ACOS((COS('Solar Altitude'!L53)*COS('Surface Solar Azimuth Angles'!L52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L53)*COS('Input Data'!$G$14)))","v":1.8044211698081001},{"$f":"ACOS((COS('Solar Altitude'!M53)*COS('Surface Solar Azimuth Angles'!M52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M53)*COS('Input Data'!$G$14)))","v":1.6439483078807569},{"$f":"ACOS((COS('Solar Altitude'!N53)*COS('Surface Solar Azimuth Angles'!N52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N53)*COS('Input Data'!$G$14)))","v":1.5770455520114091},null,23,{"$f":"ACOS((COS('Solar Altitude'!C53)*COS('Surface Solar Azimuth Angles'!Q52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C53)*COS('Input Data'!$G$14)))","v":1.8914251972930805},{"$f":"ACOS((COS('Solar Altitude'!D53)*COS('Surface Solar Azimuth Angles'!R52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D53)*COS('Input Data'!$G$14)))","v":1.9180799046031218},{"$f":"ACOS((COS('Solar Altitude'!E53)*COS('Surface Solar Azimuth Angles'!S52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E53)*COS('Input Data'!$G$14)))","v":1.8964456763961717},{"$f":"ACOS((COS('Solar Altitude'!F53)*COS('Surface Solar Azimuth Angles'!T52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F53)*COS('Input Data'!$G$14)))","v":1.852557726146864},{"$f":"ACOS((COS('Solar Altitude'!G53)*COS('Surface Solar Azimuth Angles'!U52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G53)*COS('Input Data'!$G$14)))","v":1.8316045505169805},{"$f":"ACOS((COS('Solar Altitude'!H53)*COS('Surface Solar Azimuth Angles'!V52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H53)*COS('Input Data'!$G$14)))","v":1.8444645327287763},{"$f":"ACOS((COS('Solar Altitude'!I53)*COS('Surface Solar Azimuth Angles'!W52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I53)*COS('Input Data'!$G$14)))","v":1.869859743896735},{"$f":"ACOS((COS('Solar Altitude'!J53)*COS('Surface Solar Azimuth Angles'!X52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J53)*COS('Input Data'!$G$14)))","v":1.8672450134180134},{"$f":"ACOS((COS('Solar Altitude'!K53)*COS('Surface Solar Azimuth Angles'!Y52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K53)*COS('Input Data'!$G$14)))","v":1.8309958294463837},{"$f":"ACOS((COS('Solar Altitude'!L53)*COS('Surface Solar Azimuth Angles'!Z52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L53)*COS('Input Data'!$G$14)))","v":1.7925345463526758},{"$f":"ACOS((COS('Solar Altitude'!M53)*COS('Surface Solar Azimuth Angles'!AA52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M53)*COS('Input Data'!$G$14)))","v":1.7893781051178532},{"$f":"ACOS((COS('Solar Altitude'!N53)*COS('Surface Solar Azimuth Angles'!AB52)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N53)*COS('Input Data'!$G$14)))","v":1.8325410159850253}]
[null,24,{"$f":"ACOS((COS('Solar Altitude'!C54)*COS('Surface Solar Azimuth Angles'!C53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C54)*COS('Input Data'!$G$14)))","v":1.6533112964540027},{"$f":"ACOS((COS('Solar Altitude'!D54)*COS('Surface Solar Azimuth Angles'!D53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D54)*COS('Input Data'!$G$14)))","v":1.8151059148413429},{"$f":"ACOS((COS('Solar Altitude'!E54)*COS('Surface Solar Azimuth Angles'!E53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E54)*COS('Input Data'!$G$14)))","v":2.0009556090087073},{"$f":"ACOS((COS('Solar Altitude'!F54)*COS('Surface Solar Azimuth Angles'!F53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F54)*COS('Input Data'!$G$14)))","v":2.2094103706931261},{"$f":"ACOS((COS('Solar Altitude'!G54)*COS('Surface Solar Azimuth Angles'!G53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G54)*COS('Input Data'!$G$14)))","v":2.3561169663068209},{"$f":"ACOS((COS('Solar Altitude'!H54)*COS('Surface Solar Azimuth Angles'!H53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H54)*COS('Input Data'!$G$14)))","v":2.4107742075138323},{"$f":"ACOS((COS('Solar Altitude'!I54)*COS('Surface Solar Azimuth Angles'!I53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I54)*COS('Input Data'!$G$14)))","v":2.3587458223641491},{"$f":"ACOS((COS('Solar Altitude'!J54)*COS('Surface Solar Azimuth Angles'!J53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J54)*COS('Input Data'!$G$14)))","v":2.2126361712180556},{"$f":"ACOS((COS('Solar Altitude'!K54)*COS('Surface Solar Azimuth Angles'!K53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K54)*COS('Input Data'!$G$14)))","v":2.0018920633879986},{"$f":"ACOS((COS('Solar Altitude'!L54)*COS('Surface Solar Azimuth Angles'!L53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L54)*COS('Input Data'!$G$14)))","v":1.8148671766709827},{"$f":"ACOS((COS('Solar Altitude'!M54)*COS('Surface Solar Azimuth Angles'!M53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M54)*COS('Input Data'!$G$14)))","v":1.6544053241913794},{"$f":"ACOS((COS('Solar Altitude'!N54)*COS('Surface Solar Azimuth Angles'!N53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N54)*COS('Input Data'!$G$14)))","v":1.5925011890581167},null,24,{"$f":"ACOS((COS('Solar Altitude'!C54)*COS('Surface Solar Azimuth Angles'!Q53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C54)*COS('Input Data'!$G$14)))","v":1.6460046622857321},{"$f":"ACOS((COS('Solar Altitude'!D54)*COS('Surface Solar Azimuth Angles'!R53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D54)*COS('Input Data'!$G$14)))","v":1.6610011453908424},{"$f":"ACOS((COS('Solar Altitude'!E54)*COS('Surface Solar Azimuth Angles'!S53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E54)*COS('Input Data'!$G$14)))","v":1.6346462885970194},{"$f":"ACOS((COS('Solar Altitude'!F54)*COS('Surface Solar Azimuth Angles'!T53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F54)*COS('Input Data'!$G$14)))","v":1.5965558239377193},{"$f":"ACOS((COS('Solar Altitude'!G54)*COS('Surface Solar Azimuth Angles'!U53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G54)*COS('Input Data'!$G$14)))","v":1.5864834365931053},{"$f":"ACOS((COS('Solar Altitude'!H54)*COS('Surface Solar Azimuth Angles'!V53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H54)*COS('Input Data'!$G$14)))","v":1.6049535508624626},{"$f":"ACOS((COS('Solar Altitude'!I54)*COS('Surface Solar Azimuth Angles'!W53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I54)*COS('Input Data'!$G$14)))","v":1.625285931316407},{"$f":"ACOS((COS('Solar Altitude'!J54)*COS('Surface Solar Azimuth Angles'!X53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J54)*COS('Input Data'!$G$14)))","v":1.6114686738952417},{"$f":"ACOS((COS('Solar Altitude'!K54)*COS('Surface Solar Azimuth Angles'!Y53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K54)*COS('Input Data'!$G$14)))","v":1.5723962119425112},{"$f":"ACOS((COS('Solar Altitude'!L54)*COS('Surface Solar Azimuth Angles'!Z53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L54)*COS('Input Data'!$G$14)))","v":1.6062390407741665},{"$f":"ACOS((COS('Solar Altitude'!M54)*COS('Surface Solar Azimuth Angles'!AA53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M54)*COS('Input Data'!$G$14)))","v":1.598147752648132},{"$f":"ACOS((COS('Solar Altitude'!N54)*COS('Surface Solar Azimuth Angles'!AB53)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N54)*COS('Input Data'!$G$14)))","v":1.5929456217761084}]
[]
[null,"West Incident Angle",null,null,null,null,null,null,null,null,null,null,null,null,null,"North Incident Angle",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"West Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,"North Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"West Transmitted ",null,null,null,null,null,null,null,null,null,null,null,null,null,"North Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,"West Transmitted",null,null,null,null,null,null,null,null,null,null,null,null,null,"North Transmitted"]
[null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,{"$f":"DN4","v":0},{"$f":"DO4","v":"Jan"},"Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,0,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"DEGREES(C88)","v":99.788343906405132},99.573849854580544,101.3416666666667,103.19641763488619,103.1533200341792,101.78800300109879,100.91844645725399,102.33190223993917,105.09166666666661,106.76107447056985,105.645087512885,102.47306074123236,null,1,{"$f":"DEGREES(Q88)","v":85.572235564560927},76.249611819924681,65.813574371954743,54.201165094219782,45.941198931582079,42.670101691285133,45.45376757200404,53.902745238541485,66.205651119278414,77.065288585189407,86.148469460988252,89.367454807656344,null,null,null,1,{"$f":"IF(DO60<0,0,IF(0>C60,0,IF(50>C60,(( -0.000009*C60^2 + 0.0004*C60 + 0.7918)*Radiation!C4),IF(90>C60,((-0.0006*C60^2 + 0.0699*C60 - 1.2225)*Radiation!C4),0))))","v":0},{"$f":"IF(DP60<0,0,IF(0>D60,0,IF(50>D60,(( -0.000009*D60^2 + 0.0004*D60 + 0.7918)*Radiation!D4),IF(90>D60,((-0.0006*D60^2 + 0.0699*D60 - 1.2225)*Radiation!D4),0))))","v":0},{"$f":"IF(DQ60<0,0,IF(0>E60,0,IF(50>E60,(( -0.000009*E60^2 + 0.0004*E60 + 0.7918)*Radiation!E4),IF(90>E60,((-0.0006*E60^2 + 0.0699*E60 - 1.2225)*Radiation!E4),0))))","v":0},{"$f":"IF(DR60<0,0,IF(0>F60,0,IF(50>F60,(( -0.000009*F60^2 + 0.0004*F60 + 0.7918)*Radiation!F4),IF(90>F60,((-0.0006*F60^2 + 0.0699*F60 - 1.2225)*Radiation!F4),0))))","v":0},{"$f":"IF(DS60<0,0,IF(0>G60,0,IF(50>G60,(( -0.000009*G60^2 + 0.0004*G60 + 0.7918)*Radiation!G4),IF(90>G60,((-0.0006*G60^2 + 0.0699*G60 - 1.2225)*Radiation!G4),0))))","v":0},{"$f":"IF(DT60<0,0,IF(0>H60,0,IF(50>H60,(( -0.000009*H60^2 + 0.0004*H60 + 0.7918)*Radiation!H4),IF(90>H60,((-0.0006*H60^2 + 0.0699*H60 - 1.2225)*Radiation!H4),0))))","v":0},{"$f":"IF(DU60<0,0,IF(0>I60,0,IF(50>I60,(( -0.000009*I60^2 + 0.0004*I60 + 0.7918)*Radiation!I4),IF(90>I60,((-0.0006*I60^2 + 0.0699*I60 - 1.2225)*Radiation!I4),0))))","v":0},{"$f":"IF(DV60<0,0,IF(0>J60,0,IF(50>J60,(( -0.000009*J60^2 + 0.0004*J60 + 0.7918)*Radiation!J4),IF(90>J60,((-0.0006*J60^2 + 0.0699*J60 - 1.2225)*Radiation!J4),0))))","v":0},{"$f":"IF(DW60<0,0,IF(0>K60,0,IF(50>K60,(( -0.000009*K60^2 + 0.0004*K60 + 0.7918)*Radiation!K4),IF(90>K60,((-0.0006*K60^2 + 0.0699*K60 - 1.2225)*Radiation!K4),0))))","v":0},{"$f":"IF(DX60<0,0,IF(0>L60,0,IF(50>L60,(( -0.000009*L60^2 + 0.0004*L60 + 0.7918)*Radiation!L4),IF(90>L60,((-0.0006*L60^2 + 0.0699*L60 - 1.2225)*Radiation!L4),0))))","v":0},{"$f":"IF(DY60<0,0,IF(0>M60,0,IF(50>M60,(( -0.000009*M60^2 + 0.0004*M60 + 0.7918)*Radiation!M4),IF(90>M60,((-0.0006*M60^2 + 0.0699*M60 - 1.2225)*Radiation!M4),0))))","v":0},{"$f":"IF(DZ60<0,0,IF(0>N60,0,IF(50>N60,(( -0.000009*N60^2 + 0.0004*N60 + 0.7918)*Radiation!N4),IF(90>N60,((-0.0006*N60^2 + 0.0699*N60 - 1.2225)*Radiation!N4),0))))","v":0},null,1,{"$f":"IF(EC60<0,0,IF(0>Q60,0,IF(50>Q60,(( -0.000009*Q60^2 + 0.0004*Q60 + 0.7918)*Radiation!C4),IF(90>Q60,((-0.0006*Q60^2 + 0.0699*Q60 - 1.2225)*Radiation!C4),0))))","v":0},{"$f":"IF(ED60<0,0,IF(0>R60,0,IF(50>R60,(( -0.000009*R60^2 + 0.0004*R60 + 0.7918)*Radiation!D4),IF(90>R60,((-0.0006*R60^2 + 0.0699*R60 - 1.2225)*Radiation!D4),0))))","v":0},{"$f":"IF(EE60<0,0,IF(0>S60,0,IF(50>S60,(( -0.000009*S60^2 + 0.0004*S60 + 0.7918)*Radiation!E4),IF(90>S60,((-0.0006*S60^2 + 0.0699*S60 - 1.2225)*Radiation!E4),0))))","v":0},{"$f":"IF(EF60<0,0,IF(0>T60,0,IF(50>T60,(( -0.000009*T60^2 + 0.0004*T60 + 0.7918)*Radiation!F4),IF(90>T60,((-0.0006*T60^2 + 0.0699*T60 - 1.2225)*Radiation!F4),0))))","v":0},{"$f":"IF(EG60<0,0,IF(0>U60,0,IF(50>U60,(( -0.000009*U60^2 + 0.0004*U60 + 0.7918)*Radiation!G4),IF(90>U60,((-0.0006*U60^2 + 0.0699*U60 - 1.2225)*Radiation!G4),0))))","v":0},{"$f":"IF(EH60<0,0,IF(0>V60,0,IF(50>V60,(( -0.000009*V60^2 + 0.0004*V60 + 0.7918)*Radiation!H4),IF(90>V60,((-0.0006*V60^2 + 0.0699*V60 - 1.2225)*Radiation!H4),0))))","v":0},{"$f":"IF(EI60<0,0,IF(0>W60,0,IF(50>W60,(( -0.000009*W60^2 + 0.0004*W60 + 0.7918)*Radiation!I4),IF(90>W60,((-0.0006*W60^2 + 0.0699*W60 - 1.2225)*Radiation!I4),0))))","v":0},{"$f":"IF(EJ60<0,0,IF(0>X60,0,IF(50>X60,(( -0.000009*X60^2 + 0.0004*X60 + 0.7918)*Radiation!J4),IF(90>X60,((-0.0006*X60^2 + 0.0699*X60 - 1.2225)*Radiation!J4),0))))","v":0},{"$f":"IF(EK60<0,0,IF(0>Y60,0,IF(50>Y60,(( -0.000009*Y60^2 + 0.0004*Y60 + 0.7918)*Radiation!K4),IF(90>Y60,((-0.0006*Y60^2 + 0.0699*Y60 - 1.2225)*Radiation!K4),0))))","v":0},{"$f":"IF(EL60<0,0,IF(0>Z60,0,IF(50>Z60,(( -0.000009*Z60^2 + 0.0004*Z60 + 0.7918)*Radiation!L4),IF(90>Z60,((-0.0006*Z60^2 + 0.0699*Z60 - 1.2225)*Radiation!L4),0))))","v":0},{"$f":"IF(EM60<0,0,IF(0>AA60,0,IF(50>AA60,(( -0.000009*AA60^2 + 0.0004*AA60 + 0.7918)*Radiation!M4),IF(90>AA60,((-0.0006*AA60^2 + 0.0699*AA60 - 1.2225)*Radiation!M4),0))))","v":0},{"$f":"IF(EN60<0,0,IF(0>AB60,0,IF(50>AB60,(( -0.000009*AB60^2 + 0.0004*AB60 + 0.7918)*Radiation!N4),IF(90>AB60,((-0.0006*AB60^2 + 0.0699*AB60 - 1.2225)*Radiation!N4),0))))","v":0},null,null,1,{"$f":"AG60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU32","v":0},{"$f":"AH60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV32","v":0},{"$f":"AI60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW32","v":0},{"$f":"AJ60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX32","v":0},{"$f":"AK60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY32","v":0},{"$f":"AL60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ32","v":0},{"$f":"AM60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA32","v":0},{"$f":"AN60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB32","v":0},{"$f":"AO60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC32","v":0},{"$f":"AP60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD32","v":0},{"$f":"AQ60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE32","v":0},{"$f":"AR60*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF32","v":0},null,1,{"$f":"AU60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI32","v":0},{"$f":"AV60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ32","v":0},{"$f":"AW60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK32","v":0},{"$f":"AX60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL32","v":0},{"$f":"AY60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM32","v":0},{"$f":"AZ60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN32","v":0},{"$f":"BA60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO32","v":0},{"$f":"BB60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP32","v":0},{"$f":"BC60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ32","v":0},{"$f":"BD60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR32","v":0},{"$f":"BE60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS32","v":0},{"$f":"BF60*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT32","v":0},null,1,{"$f":"IF(BJ115=0,0,BJ60/BJ115)","v":0},{"$f":"IF(BK115=0,0,BK60/BK115)","v":0},{"$f":"IF(BL115=0,0,BL60/BL115)","v":0},{"$f":"IF(BM115=0,0,BM60/BM115)","v":0},{"$f":"IF(BN115=0,0,BN60/BN115)","v":0},{"$f":"IF(BO115=0,0,BO60/BO115)","v":0},{"$f":"IF(BP115=0,0,BP60/BP115)","v":0},{"$f":"IF(BQ115=0,0,BQ60/BQ115)","v":0},{"$f":"IF(BR115=0,0,BR60/BR115)","v":0},{"$f":"IF(BS115=0,0,BS60/BS115)","v":0},{"$f":"IF(BT115=0,0,BT60/BT115)","v":0},{"$f":"IF(BU115=0,0,BU60/BU115)","v":0},null,1,{"$f":"IF(BJ115=0,0,BX60/BJ115)","v":0},{"$f":"IF(BK115=0,0,BY60/BK115)","v":0},{"$f":"IF(BL115=0,0,BZ60/BL115)","v":0},{"$f":"IF(BM115=0,0,CA60/BM115)","v":0},{"$f":"IF(BN115=0,0,CB60/BN115)","v":0},{"$f":"IF(BO115=0,0,CC60/BO115)","v":0},{"$f":"IF(BP115=0,0,CD60/BP115)","v":0},{"$f":"IF(BQ115=0,0,CE60/BQ115)","v":0},{"$f":"IF(BR115=0,0,CF60/BR115)","v":0},{"$f":"IF(BS115=0,0,CG60/BS115)","v":0},{"$f":"IF(BT115=0,0,CH60/BT115)","v":0},{"$f":"IF(BU115=0,0,CI60/BU115)","v":0},null,null,1,{"$f":"DO5","v":-79.238745258454912},-73.135890206899091,-62.969753990761212,-51.103815741194268,-42.972420763986918,-40.259838967181594,-43.397326661656273,-51.194813940312706,-61.30334441705341,-68.588756925018274,-73.864057818332,-77.510392918823513,null,{"$f":"EB5","v":1},{"$f":"EC5","v":-79.238745258454912},-73.135890206899091,-62.969753990761212,-51.103815741194268,-42.972420763986918,-40.259838967181594,-43.397326661656273,-51.194813940312706,-61.30334441705341,-68.588756925018274,-73.864057818332,-77.510392918823513]
[null,2,{"$f":"DEGREES(C89)","v":113.80152664234691},114.29190709998224,116.34166666666667,117.82542048441523,117.08385192225033,115.39210484276569,114.85843623524882,116.95272273401245,120.09166666666664,121.44465353806184,119.57940178527426,116.06495948371041,null,2,{"$f":"DEGREES(Q89)","v":87.383667618220699},78.117161787287984,68.0079820369277,56.858870088191132,48.865386999593298,45.537732664498691,48.091876636369641,56.463149949608471,68.804658288796304,79.672361547642566,88.557180813590648,91.433362268728089,null,null,null,2,{"$f":"IF(DO61<0,0,IF(0>C61,0,IF(50>C61,(( -0.000009*C61^2 + 0.0004*C61 + 0.7918)*Radiation!C5),IF(90>C61,((-0.0006*C61^2 + 0.0699*C61 - 1.2225)*Radiation!C5),0))))","v":0},{"$f":"IF(DP61<0,0,IF(0>D61,0,IF(50>D61,(( -0.000009*D61^2 + 0.0004*D61 + 0.7918)*Radiation!D5),IF(90>D61,((-0.0006*D61^2 + 0.0699*D61 - 1.2225)*Radiation!D5),0))))","v":0},{"$f":"IF(DQ61<0,0,IF(0>E61,0,IF(50>E61,(( -0.000009*E61^2 + 0.0004*E61 + 0.7918)*Radiation!E5),IF(90>E61,((-0.0006*E61^2 + 0.0699*E61 - 1.2225)*Radiation!E5),0))))","v":0},{"$f":"IF(DR61<0,0,IF(0>F61,0,IF(50>F61,(( -0.000009*F61^2 + 0.0004*F61 + 0.7918)*Radiation!F5),IF(90>F61,((-0.0006*F61^2 + 0.0699*F61 - 1.2225)*Radiation!F5),0))))","v":0},{"$f":"IF(DS61<0,0,IF(0>G61,0,IF(50>G61,(( -0.000009*G61^2 + 0.0004*G61 + 0.7918)*Radiation!G5),IF(90>G61,((-0.0006*G61^2 + 0.0699*G61 - 1.2225)*Radiation!G5),0))))","v":0},{"$f":"IF(DT61<0,0,IF(0>H61,0,IF(50>H61,(( -0.000009*H61^2 + 0.0004*H61 + 0.7918)*Radiation!H5),IF(90>H61,((-0.0006*H61^2 + 0.0699*H61 - 1.2225)*Radiation!H5),0))))","v":0},{"$f":"IF(DU61<0,0,IF(0>I61,0,IF(50>I61,(( -0.000009*I61^2 + 0.0004*I61 + 0.7918)*Radiation!I5),IF(90>I61,((-0.0006*I61^2 + 0.0699*I61 - 1.2225)*Radiation!I5),0))))","v":0},{"$f":"IF(DV61<0,0,IF(0>J61,0,IF(50>J61,(( -0.000009*J61^2 + 0.0004*J61 + 0.7918)*Radiation!J5),IF(90>J61,((-0.0006*J61^2 + 0.0699*J61 - 1.2225)*Radiation!J5),0))))","v":0},{"$f":"IF(DW61<0,0,IF(0>K61,0,IF(50>K61,(( -0.000009*K61^2 + 0.0004*K61 + 0.7918)*Radiation!K5),IF(90>K61,((-0.0006*K61^2 + 0.0699*K61 - 1.2225)*Radiation!K5),0))))","v":0},{"$f":"IF(DX61<0,0,IF(0>L61,0,IF(50>L61,(( -0.000009*L61^2 + 0.0004*L61 + 0.7918)*Radiation!L5),IF(90>L61,((-0.0006*L61^2 + 0.0699*L61 - 1.2225)*Radiation!L5),0))))","v":0},{"$f":"IF(DY61<0,0,IF(0>M61,0,IF(50>M61,(( -0.000009*M61^2 + 0.0004*M61 + 0.7918)*Radiation!M5),IF(90>M61,((-0.0006*M61^2 + 0.0699*M61 - 1.2225)*Radiation!M5),0))))","v":0},{"$f":"IF(DZ61<0,0,IF(0>N61,0,IF(50>N61,(( -0.000009*N61^2 + 0.0004*N61 + 0.7918)*Radiation!N5),IF(90>N61,((-0.0006*N61^2 + 0.0699*N61 - 1.2225)*Radiation!N5),0))))","v":0},null,2,{"$f":"IF(EC61<0,0,IF(0>Q61,0,IF(50>Q61,(( -0.000009*Q61^2 + 0.0004*Q61 + 0.7918)*Radiation!C5),IF(90>Q61,((-0.0006*Q61^2 + 0.0699*Q61 - 1.2225)*Radiation!C5),0))))","v":0},{"$f":"IF(ED61<0,0,IF(0>R61,0,IF(50>R61,(( -0.000009*R61^2 + 0.0004*R61 + 0.7918)*Radiation!D5),IF(90>R61,((-0.0006*R61^2 + 0.0699*R61 - 1.2225)*Radiation!D5),0))))","v":0},{"$f":"IF(EE61<0,0,IF(0>S61,0,IF(50>S61,(( -0.000009*S61^2 + 0.0004*S61 + 0.7918)*Radiation!E5),IF(90>S61,((-0.0006*S61^2 + 0.0699*S61 - 1.2225)*Radiation!E5),0))))","v":0},{"$f":"IF(EF61<0,0,IF(0>T61,0,IF(50>T61,(( -0.000009*T61^2 + 0.0004*T61 + 0.7918)*Radiation!F5),IF(90>T61,((-0.0006*T61^2 + 0.0699*T61 - 1.2225)*Radiation!F5),0))))","v":0},{"$f":"IF(EG61<0,0,IF(0>U61,0,IF(50>U61,(( -0.000009*U61^2 + 0.0004*U61 + 0.7918)*Radiation!G5),IF(90>U61,((-0.0006*U61^2 + 0.0699*U61 - 1.2225)*Radiation!G5),0))))","v":0},{"$f":"IF(EH61<0,0,IF(0>V61,0,IF(50>V61,(( -0.000009*V61^2 + 0.0004*V61 + 0.7918)*Radiation!H5),IF(90>V61,((-0.0006*V61^2 + 0.0699*V61 - 1.2225)*Radiation!H5),0))))","v":0},{"$f":"IF(EI61<0,0,IF(0>W61,0,IF(50>W61,(( -0.000009*W61^2 + 0.0004*W61 + 0.7918)*Radiation!I5),IF(90>W61,((-0.0006*W61^2 + 0.0699*W61 - 1.2225)*Radiation!I5),0))))","v":0},{"$f":"IF(EJ61<0,0,IF(0>X61,0,IF(50>X61,(( -0.000009*X61^2 + 0.0004*X61 + 0.7918)*Radiation!J5),IF(90>X61,((-0.0006*X61^2 + 0.0699*X61 - 1.2225)*Radiation!J5),0))))","v":0},{"$f":"IF(EK61<0,0,IF(0>Y61,0,IF(50>Y61,(( -0.000009*Y61^2 + 0.0004*Y61 + 0.7918)*Radiation!K5),IF(90>Y61,((-0.0006*Y61^2 + 0.0699*Y61 - 1.2225)*Radiation!K5),0))))","v":0},{"$f":"IF(EL61<0,0,IF(0>Z61,0,IF(50>Z61,(( -0.000009*Z61^2 + 0.0004*Z61 + 0.7918)*Radiation!L5),IF(90>Z61,((-0.0006*Z61^2 + 0.0699*Z61 - 1.2225)*Radiation!L5),0))))","v":0},{"$f":"IF(EM61<0,0,IF(0>AA61,0,IF(50>AA61,(( -0.000009*AA61^2 + 0.0004*AA61 + 0.7918)*Radiation!M5),IF(90>AA61,((-0.0006*AA61^2 + 0.0699*AA61 - 1.2225)*Radiation!M5),0))))","v":0},{"$f":"IF(EN61<0,0,IF(0>AB61,0,IF(50>AB61,(( -0.000009*AB61^2 + 0.0004*AB61 + 0.7918)*Radiation!N5),IF(90>AB61,((-0.0006*AB61^2 + 0.0699*AB61 - 1.2225)*Radiation!N5),0))))","v":0},null,null,2,{"$f":"AG61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU33","v":0},{"$f":"AH61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV33","v":0},{"$f":"AI61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW33","v":0},{"$f":"AJ61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX33","v":0},{"$f":"AK61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY33","v":0},{"$f":"AL61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ33","v":0},{"$f":"AM61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA33","v":0},{"$f":"AN61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB33","v":0},{"$f":"AO61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC33","v":0},{"$f":"AP61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD33","v":0},{"$f":"AQ61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE33","v":0},{"$f":"AR61*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF33","v":0},null,2,{"$f":"AU61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI33","v":0},{"$f":"AV61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ33","v":0},{"$f":"AW61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK33","v":0},{"$f":"AX61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL33","v":0},{"$f":"AY61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM33","v":0},{"$f":"AZ61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN33","v":0},{"$f":"BA61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO33","v":0},{"$f":"BB61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP33","v":0},{"$f":"BC61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ33","v":0},{"$f":"BD61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR33","v":0},{"$f":"BE61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS33","v":0},{"$f":"BF61*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT33","v":0},null,2,0,0,0,0,0,0,0,0,0,0,0,0,null,2,0,0,0,0,0,0,0,0,0,0,0,0,null,null,2,-66.037221876299029,-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697,null,2,-66.037221876299029,-62.610262119735701,-54.505603493104644,-44.039138424385058,-36.867903866984811,-34.787290206430924,-37.887883453111968,-44.388788539159933,-51.819137025254065,-56.521775308526607,-60.378308807607461,-63.889653492857697]
[null,3,{"$f":"DEGREES(C90)","v":127.56258934981172},128.93344837599091,131.34166666666664,132.33451117149943,130.69277923171464,128.61670904570374,128.51326434673757,131.45620008264507,135.09166666666664,136.00634828680964,133.15236383168141,129.26111228713944,null,3,{"$f":"DEGREES(Q90)","v":90.578211812625696},81.447930428055443,71.715964657344173,61.054658050959716,53.350776148646887,50.020390173652956,52.370340220847865,60.585989059706606,72.842250661669055,83.627016248368037,92.269659054431997,94.818637197292418,null,null,null,3,{"$f":"IF(DO62<0,0,IF(0>C62,0,IF(50>C62,(( -0.000009*C62^2 + 0.0004*C62 + 0.7918)*Radiation!C6),IF(90>C62,((-0.0006*C62^2 + 0.0699*C62 - 1.2225)*Radiation!C6),0))))","v":0},{"$f":"IF(DP62<0,0,IF(0>D62,0,IF(50>D62,(( -0.000009*D62^2 + 0.0004*D62 + 0.7918)*Radiation!D6),IF(90>D62,((-0.0006*D62^2 + 0.0699*D62 - 1.2225)*Radiation!D6),0))))","v":0},{"$f":"IF(DQ62<0,0,IF(0>E62,0,IF(50>E62,(( -0.000009*E62^2 + 0.0004*E62 + 0.7918)*Radiation!E6),IF(90>E62,((-0.0006*E62^2 + 0.0699*E62 - 1.2225)*Radiation!E6),0))))","v":0},{"$f":"IF(DR62<0,0,IF(0>F62,0,IF(50>F62,(( -0.000009*F62^2 + 0.0004*F62 + 0.7918)*Radiation!F6),IF(90>F62,((-0.0006*F62^2 + 0.0699*F62 - 1.2225)*Radiation!F6),0))))","v":0},{"$f":"IF(DS62<0,0,IF(0>G62,0,IF(50>G62,(( -0.000009*G62^2 + 0.0004*G62 + 0.7918)*Radiation!G6),IF(90>G62,((-0.0006*G62^2 + 0.0699*G62 - 1.2225)*Radiation!G6),0))))","v":0},{"$f":"IF(DT62<0,0,IF(0>H62,0,IF(50>H62,(( -0.000009*H62^2 + 0.0004*H62 + 0.7918)*Radiation!H6),IF(90>H62,((-0.0006*H62^2 + 0.0699*H62 - 1.2225)*Radiation!H6),0))))","v":0},{"$f":"IF(DU62<0,0,IF(0>I62,0,IF(50>I62,(( -0.000009*I62^2 + 0.0004*I62 + 0.7918)*Radiation!I6),IF(90>I62,((-0.0006*I62^2 + 0.0699*I62 - 1.2225)*Radiation!I6),0))))","v":0},{"$f":"IF(DV62<0,0,IF(0>J62,0,IF(50>J62,(( -0.000009*J62^2 + 0.0004*J62 + 0.7918)*Radiation!J6),IF(90>J62,((-0.0006*J62^2 + 0.0699*J62 - 1.2225)*Radiation!J6),0))))","v":0},{"$f":"IF(DW62<0,0,IF(0>K62,0,IF(50>K62,(( -0.000009*K62^2 + 0.0004*K62 + 0.7918)*Radiation!K6),IF(90>K62,((-0.0006*K62^2 + 0.0699*K62 - 1.2225)*Radiation!K6),0))))","v":0},{"$f":"IF(DX62<0,0,IF(0>L62,0,IF(50>L62,(( -0.000009*L62^2 + 0.0004*L62 + 0.7918)*Radiation!L6),IF(90>L62,((-0.0006*L62^2 + 0.0699*L62 - 1.2225)*Radiation!L6),0))))","v":0},{"$f":"IF(DY62<0,0,IF(0>M62,0,IF(50>M62,(( -0.000009*M62^2 + 0.0004*M62 + 0.7918)*Radiation!M6),IF(90>M62,((-0.0006*M62^2 + 0.0699*M62 - 1.2225)*Radiation!M6),0))))","v":0},{"$f":"IF(DZ62<0,0,IF(0>N62,0,IF(50>N62,(( -0.000009*N62^2 + 0.0004*N62 + 0.7918)*Radiation!N6),IF(90>N62,((-0.0006*N62^2 + 0.0699*N62 - 1.2225)*Radiation!N6),0))))","v":0},null,3,{"$f":"IF(EC62<0,0,IF(0>Q62,0,IF(50>Q62,(( -0.000009*Q62^2 + 0.0004*Q62 + 0.7918)*Radiation!C6),IF(90>Q62,((-0.0006*Q62^2 + 0.0699*Q62 - 1.2225)*Radiation!C6),0))))","v":0},{"$f":"IF(ED62<0,0,IF(0>R62,0,IF(50>R62,(( -0.000009*R62^2 + 0.0004*R62 + 0.7918)*Radiation!D6),IF(90>R62,((-0.0006*R62^2 + 0.0699*R62 - 1.2225)*Radiation!D6),0))))","v":0},{"$f":"IF(EE62<0,0,IF(0>S62,0,IF(50>S62,(( -0.000009*S62^2 + 0.0004*S62 + 0.7918)*Radiation!E6),IF(90>S62,((-0.0006*S62^2 + 0.0699*S62 - 1.2225)*Radiation!E6),0))))","v":0},{"$f":"IF(EF62<0,0,IF(0>T62,0,IF(50>T62,(( -0.000009*T62^2 + 0.0004*T62 + 0.7918)*Radiation!F6),IF(90>T62,((-0.0006*T62^2 + 0.0699*T62 - 1.2225)*Radiation!F6),0))))","v":0},{"$f":"IF(EG62<0,0,IF(0>U62,0,IF(50>U62,(( -0.000009*U62^2 + 0.0004*U62 + 0.7918)*Radiation!G6),IF(90>U62,((-0.0006*U62^2 + 0.0699*U62 - 1.2225)*Radiation!G6),0))))","v":0},{"$f":"IF(EH62<0,0,IF(0>V62,0,IF(50>V62,(( -0.000009*V62^2 + 0.0004*V62 + 0.7918)*Radiation!H6),IF(90>V62,((-0.0006*V62^2 + 0.0699*V62 - 1.2225)*Radiation!H6),0))))","v":0},{"$f":"IF(EI62<0,0,IF(0>W62,0,IF(50>W62,(( -0.000009*W62^2 + 0.0004*W62 + 0.7918)*Radiation!I6),IF(90>W62,((-0.0006*W62^2 + 0.0699*W62 - 1.2225)*Radiation!I6),0))))","v":0},{"$f":"IF(EJ62<0,0,IF(0>X62,0,IF(50>X62,(( -0.000009*X62^2 + 0.0004*X62 + 0.7918)*Radiation!J6),IF(90>X62,((-0.0006*X62^2 + 0.0699*X62 - 1.2225)*Radiation!J6),0))))","v":0},{"$f":"IF(EK62<0,0,IF(0>Y62,0,IF(50>Y62,(( -0.000009*Y62^2 + 0.0004*Y62 + 0.7918)*Radiation!K6),IF(90>Y62,((-0.0006*Y62^2 + 0.0699*Y62 - 1.2225)*Radiation!K6),0))))","v":0},{"$f":"IF(EL62<0,0,IF(0>Z62,0,IF(50>Z62,(( -0.000009*Z62^2 + 0.0004*Z62 + 0.7918)*Radiation!L6),IF(90>Z62,((-0.0006*Z62^2 + 0.0699*Z62 - 1.2225)*Radiation!L6),0))))","v":0},{"$f":"IF(EM62<0,0,IF(0>AA62,0,IF(50>AA62,(( -0.000009*AA62^2 + 0.0004*AA62 + 0.7918)*Radiation!M6),IF(90>AA62,((-0.0006*AA62^2 + 0.0699*AA62 - 1.2225)*Radiation!M6),0))))","v":0},{"$f":"IF(EN62<0,0,IF(0>AB62,0,IF(50>AB62,(( -0.000009*AB62^2 + 0.0004*AB62 + 0.7918)*Radiation!N6),IF(90>AB62,((-0.0006*AB62^2 + 0.0699*AB62 - 1.2225)*Radiation!N6),0))))","v":0},null,null,3,{"$f":"AG62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU34","v":0},{"$f":"AH62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV34","v":0},{"$f":"AI62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW34","v":0},{"$f":"AJ62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX34","v":0},{"$f":"AK62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY34","v":0},{"$f":"AL62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ34","v":0},{"$f":"AM62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA34","v":0},{"$f":"AN62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB34","v":0},{"$f":"AO62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC34","v":0},{"$f":"AP62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD34","v":0},{"$f":"AQ62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE34","v":0},{"$f":"AR62*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF34","v":0},null,3,{"$f":"AU62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI34","v":0},{"$f":"AV62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ34","v":0},{"$f":"AW62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK34","v":0},{"$f":"AX62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL34","v":0},{"$f":"AY62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM34","v":0},{"$f":"AZ62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN34","v":0},{"$f":"BA62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO34","v":0},{"$f":"BB62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP34","v":0},{"$f":"BC62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ34","v":0},{"$f":"BD62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR34","v":0},{"$f":"BE62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS34","v":0},{"$f":"BF62*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT34","v":0},null,3,0,0,0,0,0,0,0,0,0,0,0,0,null,3,0,0,0,0,0,0,0,0,0,0,0,0,null,null,3,-52.431373562484438,-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552,null,3,-52.431373562484438,-49.776364898184575,-43.00744408924087,-33.970697614512481,-27.874166624770901,-26.397406240900974,-29.298461575777225,-34.480458721023354,-39.89507498863518,-43.286892300779471,-46.757596903257479,-50.32692672055552]
[null,4,{"$f":"DEGREES(C91)","v":140.72718463621587},143.38134756077289,146.34166666666667,146.53696034723595,143.54066211551256,140.97510241267139,141.49724263851596,145.66176552614004,150.09166666666667,150.24225996413057,145.85736453236672,141.55386757464609,null,4,{"$f":"DEGREES(Q91)","v":94.946017358585095},85.987048534297529,76.608808985374239,66.357315385285872,58.882181721612334,55.566974832079396,57.774926072012342,65.841029258367683,77.974072698698706,88.644018015546095,97.051404688636921,99.317393938466054,null,null,null,4,{"$f":"IF(DO63<0,0,IF(0>C63,0,IF(50>C63,(( -0.000009*C63^2 + 0.0004*C63 + 0.7918)*Radiation!C7),IF(90>C63,((-0.0006*C63^2 + 0.0699*C63 - 1.2225)*Radiation!C7),0))))","v":0},{"$f":"IF(DP63<0,0,IF(0>D63,0,IF(50>D63,(( -0.000009*D63^2 + 0.0004*D63 + 0.7918)*Radiation!D7),IF(90>D63,((-0.0006*D63^2 + 0.0699*D63 - 1.2225)*Radiation!D7),0))))","v":0},{"$f":"IF(DQ63<0,0,IF(0>E63,0,IF(50>E63,(( -0.000009*E63^2 + 0.0004*E63 + 0.7918)*Radiation!E7),IF(90>E63,((-0.0006*E63^2 + 0.0699*E63 - 1.2225)*Radiation!E7),0))))","v":0},{"$f":"IF(DR63<0,0,IF(0>F63,0,IF(50>F63,(( -0.000009*F63^2 + 0.0004*F63 + 0.7918)*Radiation!F7),IF(90>F63,((-0.0006*F63^2 + 0.0699*F63 - 1.2225)*Radiation!F7),0))))","v":0},{"$f":"IF(DS63<0,0,IF(0>G63,0,IF(50>G63,(( -0.000009*G63^2 + 0.0004*G63 + 0.7918)*Radiation!G7),IF(90>G63,((-0.0006*G63^2 + 0.0699*G63 - 1.2225)*Radiation!G7),0))))","v":0},{"$f":"IF(DT63<0,0,IF(0>H63,0,IF(50>H63,(( -0.000009*H63^2 + 0.0004*H63 + 0.7918)*Radiation!H7),IF(90>H63,((-0.0006*H63^2 + 0.0699*H63 - 1.2225)*Radiation!H7),0))))","v":0},{"$f":"IF(DU63<0,0,IF(0>I63,0,IF(50>I63,(( -0.000009*I63^2 + 0.0004*I63 + 0.7918)*Radiation!I7),IF(90>I63,((-0.0006*I63^2 + 0.0699*I63 - 1.2225)*Radiation!I7),0))))","v":0},{"$f":"IF(DV63<0,0,IF(0>J63,0,IF(50>J63,(( -0.000009*J63^2 + 0.0004*J63 + 0.7918)*Radiation!J7),IF(90>J63,((-0.0006*J63^2 + 0.0699*J63 - 1.2225)*Radiation!J7),0))))","v":0},{"$f":"IF(DW63<0,0,IF(0>K63,0,IF(50>K63,(( -0.000009*K63^2 + 0.0004*K63 + 0.7918)*Radiation!K7),IF(90>K63,((-0.0006*K63^2 + 0.0699*K63 - 1.2225)*Radiation!K7),0))))","v":0},{"$f":"IF(DX63<0,0,IF(0>L63,0,IF(50>L63,(( -0.000009*L63^2 + 0.0004*L63 + 0.7918)*Radiation!L7),IF(90>L63,((-0.0006*L63^2 + 0.0699*L63 - 1.2225)*Radiation!L7),0))))","v":0},{"$f":"IF(DY63<0,0,IF(0>M63,0,IF(50>M63,(( -0.000009*M63^2 + 0.0004*M63 + 0.7918)*Radiation!M7),IF(90>M63,((-0.0006*M63^2 + 0.0699*M63 - 1.2225)*Radiation!M7),0))))","v":0},{"$f":"IF(DZ63<0,0,IF(0>N63,0,IF(50>N63,(( -0.000009*N63^2 + 0.0004*N63 + 0.7918)*Radiation!N7),IF(90>N63,((-0.0006*N63^2 + 0.0699*N63 - 1.2225)*Radiation!N7),0))))","v":0},null,4,{"$f":"IF(EC63<0,0,IF(0>Q63,0,IF(50>Q63,(( -0.000009*Q63^2 + 0.0004*Q63 + 0.7918)*Radiation!C7),IF(90>Q63,((-0.0006*Q63^2 + 0.0699*Q63 - 1.2225)*Radiation!C7),0))))","v":0},{"$f":"IF(ED63<0,0,IF(0>R63,0,IF(50>R63,(( -0.000009*R63^2 + 0.0004*R63 + 0.7918)*Radiation!D7),IF(90>R63,((-0.0006*R63^2 + 0.0699*R63 - 1.2225)*Radiation!D7),0))))","v":0},{"$f":"IF(EE63<0,0,IF(0>S63,0,IF(50>S63,(( -0.000009*S63^2 + 0.0004*S63 + 0.7918)*Radiation!E7),IF(90>S63,((-0.0006*S63^2 + 0.0699*S63 - 1.2225)*Radiation!E7),0))))","v":0},{"$f":"IF(EF63<0,0,IF(0>T63,0,IF(50>T63,(( -0.000009*T63^2 + 0.0004*T63 + 0.7918)*Radiation!F7),IF(90>T63,((-0.0006*T63^2 + 0.0699*T63 - 1.2225)*Radiation!F7),0))))","v":0},{"$f":"IF(EG63<0,0,IF(0>U63,0,IF(50>U63,(( -0.000009*U63^2 + 0.0004*U63 + 0.7918)*Radiation!G7),IF(90>U63,((-0.0006*U63^2 + 0.0699*U63 - 1.2225)*Radiation!G7),0))))","v":0},{"$f":"IF(EH63<0,0,IF(0>V63,0,IF(50>V63,(( -0.000009*V63^2 + 0.0004*V63 + 0.7918)*Radiation!H7),IF(90>V63,((-0.0006*V63^2 + 0.0699*V63 - 1.2225)*Radiation!H7),0))))","v":0},{"$f":"IF(EI63<0,0,IF(0>W63,0,IF(50>W63,(( -0.000009*W63^2 + 0.0004*W63 + 0.7918)*Radiation!I7),IF(90>W63,((-0.0006*W63^2 + 0.0699*W63 - 1.2225)*Radiation!I7),0))))","v":0},{"$f":"IF(EJ63<0,0,IF(0>X63,0,IF(50>X63,(( -0.000009*X63^2 + 0.0004*X63 + 0.7918)*Radiation!J7),IF(90>X63,((-0.0006*X63^2 + 0.0699*X63 - 1.2225)*Radiation!J7),0))))","v":0},{"$f":"IF(EK63<0,0,IF(0>Y63,0,IF(50>Y63,(( -0.000009*Y63^2 + 0.0004*Y63 + 0.7918)*Radiation!K7),IF(90>Y63,((-0.0006*Y63^2 + 0.0699*Y63 - 1.2225)*Radiation!K7),0))))","v":0},{"$f":"IF(EL63<0,0,IF(0>Z63,0,IF(50>Z63,(( -0.000009*Z63^2 + 0.0004*Z63 + 0.7918)*Radiation!L7),IF(90>Z63,((-0.0006*Z63^2 + 0.0699*Z63 - 1.2225)*Radiation!L7),0))))","v":0},{"$f":"IF(EM63<0,0,IF(0>AA63,0,IF(50>AA63,(( -0.000009*AA63^2 + 0.0004*AA63 + 0.7918)*Radiation!M7),IF(90>AA63,((-0.0006*AA63^2 + 0.0699*AA63 - 1.2225)*Radiation!M7),0))))","v":0},{"$f":"IF(EN63<0,0,IF(0>AB63,0,IF(50>AB63,(( -0.000009*AB63^2 + 0.0004*AB63 + 0.7918)*Radiation!N7),IF(90>AB63,((-0.0006*AB63^2 + 0.0699*AB63 - 1.2225)*Radiation!N7),0))))","v":0},null,null,4,{"$f":"AG63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU35","v":0},{"$f":"AH63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV35","v":0},{"$f":"AI63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW35","v":0},{"$f":"AJ63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX35","v":0},{"$f":"AK63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY35","v":0},{"$f":"AL63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ35","v":0},{"$f":"AM63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA35","v":0},{"$f":"AN63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB35","v":0},{"$f":"AO63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC35","v":0},{"$f":"AP63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD35","v":0},{"$f":"AQ63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE35","v":0},{"$f":"AR63*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF35","v":0},null,4,{"$f":"AU63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI35","v":0},{"$f":"AV63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ35","v":0},{"$f":"AW63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK35","v":0},{"$f":"AX63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL35","v":0},{"$f":"AY63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM35","v":0},{"$f":"AZ63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN35","v":0},{"$f":"BA63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO35","v":0},{"$f":"BB63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP35","v":0},{"$f":"BC63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ35","v":0},{"$f":"BD63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR35","v":0},{"$f":"BE63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS35","v":0},{"$f":"BF63*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT35","v":0},null,4,0,0,0,0,0,0,0,0,0,0,0,0,null,4,0,0,0,0,0,0,0,0,0,0,0,0,null,null,4,-38.837571781392398,-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833,null,4,-38.837571781392398,-36.325136967893741,-30.23387910899125,-22.236891602714234,-17.058579195686843,-16.082853037589089,-18.740224973134019,-22.841111056638525,-26.935985833021629,-29.720493919992279,-33.206986937806654,-36.893522726896833]
[null,5,{"$f":"DEGREES(C92)","v":152.36212818793786},157.23977387018414,161.34166666666664,159.74701376251107,154.38832575868955,151.24619189772807,152.76402384128761,158.92734049062065,165.0916666666667,163.27261469342778,156.19756812451462,151.66134854942314,null,5,{"$f":"DEGREES(Q92)","v":100.22657304423616},91.426950809161212,82.317370695731256,72.330535489669984,64.979296811002683,61.674865747695719,63.814389844569796,71.789447838394508,83.828429315210968,94.40350172667992,102.62828937643877,104.67937322823005,null,null,null,5,{"$f":"IF(DO64<0,0,IF(0>C64,0,IF(50>C64,(( -0.000009*C64^2 + 0.0004*C64 + 0.7918)*Radiation!C8),IF(90>C64,((-0.0006*C64^2 + 0.0699*C64 - 1.2225)*Radiation!C8),0))))","v":0},{"$f":"IF(DP64<0,0,IF(0>D64,0,IF(50>D64,(( -0.000009*D64^2 + 0.0004*D64 + 0.7918)*Radiation!D8),IF(90>D64,((-0.0006*D64^2 + 0.0699*D64 - 1.2225)*Radiation!D8),0))))","v":0},{"$f":"IF(DQ64<0,0,IF(0>E64,0,IF(50>E64,(( -0.000009*E64^2 + 0.0004*E64 + 0.7918)*Radiation!E8),IF(90>E64,((-0.0006*E64^2 + 0.0699*E64 - 1.2225)*Radiation!E8),0))))","v":0},{"$f":"IF(DR64<0,0,IF(0>F64,0,IF(50>F64,(( -0.000009*F64^2 + 0.0004*F64 + 0.7918)*Radiation!F8),IF(90>F64,((-0.0006*F64^2 + 0.0699*F64 - 1.2225)*Radiation!F8),0))))","v":0},{"$f":"IF(DS64<0,0,IF(0>G64,0,IF(50>G64,(( -0.000009*G64^2 + 0.0004*G64 + 0.7918)*Radiation!G8),IF(90>G64,((-0.0006*G64^2 + 0.0699*G64 - 1.2225)*Radiation!G8),0))))","v":0},{"$f":"IF(DT64<0,0,IF(0>H64,0,IF(50>H64,(( -0.000009*H64^2 + 0.0004*H64 + 0.7918)*Radiation!H8),IF(90>H64,((-0.0006*H64^2 + 0.0699*H64 - 1.2225)*Radiation!H8),0))))","v":0},{"$f":"IF(DU64<0,0,IF(0>I64,0,IF(50>I64,(( -0.000009*I64^2 + 0.0004*I64 + 0.7918)*Radiation!I8),IF(90>I64,((-0.0006*I64^2 + 0.0699*I64 - 1.2225)*Radiation!I8),0))))","v":0},{"$f":"IF(DV64<0,0,IF(0>J64,0,IF(50>J64,(( -0.000009*J64^2 + 0.0004*J64 + 0.7918)*Radiation!J8),IF(90>J64,((-0.0006*J64^2 + 0.0699*J64 - 1.2225)*Radiation!J8),0))))","v":0},{"$f":"IF(DW64<0,0,IF(0>K64,0,IF(50>K64,(( -0.000009*K64^2 + 0.0004*K64 + 0.7918)*Radiation!K8),IF(90>K64,((-0.0006*K64^2 + 0.0699*K64 - 1.2225)*Radiation!K8),0))))","v":0},{"$f":"IF(DX64<0,0,IF(0>L64,0,IF(50>L64,(( -0.000009*L64^2 + 0.0004*L64 + 0.7918)*Radiation!L8),IF(90>L64,((-0.0006*L64^2 + 0.0699*L64 - 1.2225)*Radiation!L8),0))))","v":0},{"$f":"IF(DY64<0,0,IF(0>M64,0,IF(50>M64,(( -0.000009*M64^2 + 0.0004*M64 + 0.7918)*Radiation!M8),IF(90>M64,((-0.0006*M64^2 + 0.0699*M64 - 1.2225)*Radiation!M8),0))))","v":0},{"$f":"IF(DZ64<0,0,IF(0>N64,0,IF(50>N64,(( -0.000009*N64^2 + 0.0004*N64 + 0.7918)*Radiation!N8),IF(90>N64,((-0.0006*N64^2 + 0.0699*N64 - 1.2225)*Radiation!N8),0))))","v":0},null,5,{"$f":"IF(EC64<0,0,IF(0>Q64,0,IF(50>Q64,(( -0.000009*Q64^2 + 0.0004*Q64 + 0.7918)*Radiation!C8),IF(90>Q64,((-0.0006*Q64^2 + 0.0699*Q64 - 1.2225)*Radiation!C8),0))))","v":0},{"$f":"IF(ED64<0,0,IF(0>R64,0,IF(50>R64,(( -0.000009*R64^2 + 0.0004*R64 + 0.7918)*Radiation!D8),IF(90>R64,((-0.0006*R64^2 + 0.0699*R64 - 1.2225)*Radiation!D8),0))))","v":0},{"$f":"IF(EE64<0,0,IF(0>S64,0,IF(50>S64,(( -0.000009*S64^2 + 0.0004*S64 + 0.7918)*Radiation!E8),IF(90>S64,((-0.0006*S64^2 + 0.0699*S64 - 1.2225)*Radiation!E8),0))))","v":0},{"$f":"IF(EF64<0,0,IF(0>T64,0,IF(50>T64,(( -0.000009*T64^2 + 0.0004*T64 + 0.7918)*Radiation!F8),IF(90>T64,((-0.0006*T64^2 + 0.0699*T64 - 1.2225)*Radiation!F8),0))))","v":0},{"$f":"IF(EG64<0,0,IF(0>U64,0,IF(50>U64,(( -0.000009*U64^2 + 0.0004*U64 + 0.7918)*Radiation!G8),IF(90>U64,((-0.0006*U64^2 + 0.0699*U64 - 1.2225)*Radiation!G8),0))))","v":0},{"$f":"IF(EH64<0,0,IF(0>V64,0,IF(50>V64,(( -0.000009*V64^2 + 0.0004*V64 + 0.7918)*Radiation!H8),IF(90>V64,((-0.0006*V64^2 + 0.0699*V64 - 1.2225)*Radiation!H8),0))))","v":0},{"$f":"IF(EI64<0,0,IF(0>W64,0,IF(50>W64,(( -0.000009*W64^2 + 0.0004*W64 + 0.7918)*Radiation!I8),IF(90>W64,((-0.0006*W64^2 + 0.0699*W64 - 1.2225)*Radiation!I8),0))))","v":0},{"$f":"IF(EJ64<0,0,IF(0>X64,0,IF(50>X64,(( -0.000009*X64^2 + 0.0004*X64 + 0.7918)*Radiation!J8),IF(90>X64,((-0.0006*X64^2 + 0.0699*X64 - 1.2225)*Radiation!J8),0))))","v":0},{"$f":"IF(EK64<0,0,IF(0>Y64,0,IF(50>Y64,(( -0.000009*Y64^2 + 0.0004*Y64 + 0.7918)*Radiation!K8),IF(90>Y64,((-0.0006*Y64^2 + 0.0699*Y64 - 1.2225)*Radiation!K8),0))))","v":0},{"$f":"IF(EL64<0,0,IF(0>Z64,0,IF(50>Z64,(( -0.000009*Z64^2 + 0.0004*Z64 + 0.7918)*Radiation!L8),IF(90>Z64,((-0.0006*Z64^2 + 0.0699*Z64 - 1.2225)*Radiation!L8),0))))","v":0},{"$f":"IF(EM64<0,0,IF(0>AA64,0,IF(50>AA64,(( -0.000009*AA64^2 + 0.0004*AA64 + 0.7918)*Radiation!M8),IF(90>AA64,((-0.0006*AA64^2 + 0.0699*AA64 - 1.2225)*Radiation!M8),0))))","v":0},{"$f":"IF(EN64<0,0,IF(0>AB64,0,IF(50>AB64,(( -0.000009*AB64^2 + 0.0004*AB64 + 0.7918)*Radiation!N8),IF(90>AB64,((-0.0006*AB64^2 + 0.0699*AB64 - 1.2225)*Radiation!N8),0))))","v":0},null,null,5,{"$f":"AG64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU36","v":0},{"$f":"AH64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV36","v":0},{"$f":"AI64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW36","v":0},{"$f":"AJ64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX36","v":0},{"$f":"AK64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY36","v":0},{"$f":"AL64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ36","v":0},{"$f":"AM64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA36","v":0},{"$f":"AN64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB36","v":0},{"$f":"AO64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC36","v":0},{"$f":"AP64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD36","v":0},{"$f":"AQ64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE36","v":0},{"$f":"AR64*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF36","v":0},null,5,{"$f":"AU64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI36","v":0},{"$f":"AV64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ36","v":0},{"$f":"AW64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK36","v":0},{"$f":"AX64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL36","v":0},{"$f":"AY64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM36","v":0},{"$f":"AZ64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN36","v":0},{"$f":"BA64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO36","v":0},{"$f":"BB64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP36","v":0},{"$f":"BC64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ36","v":0},{"$f":"BD64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR36","v":0},{"$f":"BE64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS36","v":0},{"$f":"BF64*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT36","v":0},null,5,0,0,0,0,0,0,0,0,0,0,0,0,null,5,0,0,0,0,0,0,0,0,0,0,0,0,null,null,5,-25.376333918471747,-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006,null,5,-25.376333918471747,-22.7103856061896,-16.897092448538263,-9.5810693067706811,-5.1231262317655331,-4.54535827775074,-6.9688312964780383,-10.241982624949756,-13.517063375335365,-16.104385171900024,-19.830528453312528,-23.664530366970006]
[null,6,{"$f":"DEGREES(C93)","v":159.59987695565323},168.1807904979741,176.34166666666653,168.00615739830985,159.67834535239976,156.45861971246464,159.24228386747936,167.6709460623222,179.90833333333325,169.10452670079189,160.03314829433953,156.51153378947097,null,6,{"$f":"DEGREES(Q93)","v":106.13133949094842},97.439474064692533,88.472160386966152,78.574064824134922,71.231286059965129,67.925616006075415,70.066795543803167,78.028147895020638,90.038304468277531,100.5729270356283,108.70317264901392,110.62713250962913,null,null,null,6,{"$f":"IF(DO65<0,0,IF(0>C65,0,IF(50>C65,(( -0.000009*C65^2 + 0.0004*C65 + 0.7918)*Radiation!C9),IF(90>C65,((-0.0006*C65^2 + 0.0699*C65 - 1.2225)*Radiation!C9),0))))","v":0},{"$f":"IF(DP65<0,0,IF(0>D65,0,IF(50>D65,(( -0.000009*D65^2 + 0.0004*D65 + 0.7918)*Radiation!D9),IF(90>D65,((-0.0006*D65^2 + 0.0699*D65 - 1.2225)*Radiation!D9),0))))","v":0},{"$f":"IF(DQ65<0,0,IF(0>E65,0,IF(50>E65,(( -0.000009*E65^2 + 0.0004*E65 + 0.7918)*Radiation!E9),IF(90>E65,((-0.0006*E65^2 + 0.0699*E65 - 1.2225)*Radiation!E9),0))))","v":0},{"$f":"IF(DR65<0,0,IF(0>F65,0,IF(50>F65,(( -0.000009*F65^2 + 0.0004*F65 + 0.7918)*Radiation!F9),IF(90>F65,((-0.0006*F65^2 + 0.0699*F65 - 1.2225)*Radiation!F9),0))))","v":0},{"$f":"IF(DS65<0,0,IF(0>G65,0,IF(50>G65,(( -0.000009*G65^2 + 0.0004*G65 + 0.7918)*Radiation!G9),IF(90>G65,((-0.0006*G65^2 + 0.0699*G65 - 1.2225)*Radiation!G9),0))))","v":0},{"$f":"IF(DT65<0,0,IF(0>H65,0,IF(50>H65,(( -0.000009*H65^2 + 0.0004*H65 + 0.7918)*Radiation!H9),IF(90>H65,((-0.0006*H65^2 + 0.0699*H65 - 1.2225)*Radiation!H9),0))))","v":0},{"$f":"IF(DU65<0,0,IF(0>I65,0,IF(50>I65,(( -0.000009*I65^2 + 0.0004*I65 + 0.7918)*Radiation!I9),IF(90>I65,((-0.0006*I65^2 + 0.0699*I65 - 1.2225)*Radiation!I9),0))))","v":0},{"$f":"IF(DV65<0,0,IF(0>J65,0,IF(50>J65,(( -0.000009*J65^2 + 0.0004*J65 + 0.7918)*Radiation!J9),IF(90>J65,((-0.0006*J65^2 + 0.0699*J65 - 1.2225)*Radiation!J9),0))))","v":0},{"$f":"IF(DW65<0,0,IF(0>K65,0,IF(50>K65,(( -0.000009*K65^2 + 0.0004*K65 + 0.7918)*Radiation!K9),IF(90>K65,((-0.0006*K65^2 + 0.0699*K65 - 1.2225)*Radiation!K9),0))))","v":0},{"$f":"IF(DX65<0,0,IF(0>L65,0,IF(50>L65,(( -0.000009*L65^2 + 0.0004*L65 + 0.7918)*Radiation!L9),IF(90>L65,((-0.0006*L65^2 + 0.0699*L65 - 1.2225)*Radiation!L9),0))))","v":0},{"$f":"IF(DY65<0,0,IF(0>M65,0,IF(50>M65,(( -0.000009*M65^2 + 0.0004*M65 + 0.7918)*Radiation!M9),IF(90>M65,((-0.0006*M65^2 + 0.0699*M65 - 1.2225)*Radiation!M9),0))))","v":0},{"$f":"IF(DZ65<0,0,IF(0>N65,0,IF(50>N65,(( -0.000009*N65^2 + 0.0004*N65 + 0.7918)*Radiation!N9),IF(90>N65,((-0.0006*N65^2 + 0.0699*N65 - 1.2225)*Radiation!N9),0))))","v":0},null,6,{"$f":"IF(EC65<0,0,IF(0>Q65,0,IF(50>Q65,(( -0.000009*Q65^2 + 0.0004*Q65 + 0.7918)*Radiation!C9),IF(90>Q65,((-0.0006*Q65^2 + 0.0699*Q65 - 1.2225)*Radiation!C9),0))))","v":0},{"$f":"IF(ED65<0,0,IF(0>R65,0,IF(50>R65,(( -0.000009*R65^2 + 0.0004*R65 + 0.7918)*Radiation!D9),IF(90>R65,((-0.0006*R65^2 + 0.0699*R65 - 1.2225)*Radiation!D9),0))))","v":0},{"$f":"IF(EE65<0,0,IF(0>S65,0,IF(50>S65,(( -0.000009*S65^2 + 0.0004*S65 + 0.7918)*Radiation!E9),IF(90>S65,((-0.0006*S65^2 + 0.0699*S65 - 1.2225)*Radiation!E9),0))))","v":0},{"$f":"IF(EF65<0,0,IF(0>T65,0,IF(50>T65,(( -0.000009*T65^2 + 0.0004*T65 + 0.7918)*Radiation!F9),IF(90>T65,((-0.0006*T65^2 + 0.0699*T65 - 1.2225)*Radiation!F9),0))))","v":1.0755703445098641},{"$f":"IF(EG65<0,0,IF(0>U65,0,IF(50>U65,(( -0.000009*U65^2 + 0.0004*U65 + 0.7918)*Radiation!G9),IF(90>U65,((-0.0006*U65^2 + 0.0699*U65 - 1.2225)*Radiation!G9),0))))","v":3.6124104430505581},{"$f":"IF(EH65<0,0,IF(0>V65,0,IF(50>V65,(( -0.000009*V65^2 + 0.0004*V65 + 0.7918)*Radiation!H9),IF(90>V65,((-0.0006*V65^2 + 0.0699*V65 - 1.2225)*Radiation!H9),0))))","v":4.800417083437349},{"$f":"IF(EI65<0,0,IF(0>W65,0,IF(50>W65,(( -0.000009*W65^2 + 0.0004*W65 + 0.7918)*Radiation!I9),IF(90>W65,((-0.0006*W65^2 + 0.0699*W65 - 1.2225)*Radiation!I9),0))))","v":2.7752167001976069},{"$f":"IF(EJ65<0,0,IF(0>X65,0,IF(50>X65,(( -0.000009*X65^2 + 0.0004*X65 + 0.7918)*Radiation!J9),IF(90>X65,((-0.0006*X65^2 + 0.0699*X65 - 1.2225)*Radiation!J9),0))))","v":1.1005539270288507},{"$f":"IF(EK65<0,0,IF(0>Y65,0,IF(50>Y65,(( -0.000009*Y65^2 + 0.0004*Y65 + 0.7918)*Radiation!K9),IF(90>Y65,((-0.0006*Y65^2 + 0.0699*Y65 - 1.2225)*Radiation!K9),0))))","v":0},{"$f":"IF(EL65<0,0,IF(0>Z65,0,IF(50>Z65,(( -0.000009*Z65^2 + 0.0004*Z65 + 0.7918)*Radiation!L9),IF(90>Z65,((-0.0006*Z65^2 + 0.0699*Z65 - 1.2225)*Radiation!L9),0))))","v":0},{"$f":"IF(EM65<0,0,IF(0>AA65,0,IF(50>AA65,(( -0.000009*AA65^2 + 0.0004*AA65 + 0.7918)*Radiation!M9),IF(90>AA65,((-0.0006*AA65^2 + 0.0699*AA65 - 1.2225)*Radiation!M9),0))))","v":0},{"$f":"IF(EN65<0,0,IF(0>AB65,0,IF(50>AB65,(( -0.000009*AB65^2 + 0.0004*AB65 + 0.7918)*Radiation!N9),IF(90>AB65,((-0.0006*AB65^2 + 0.0699*AB65 - 1.2225)*Radiation!N9),0))))","v":0},null,null,6,{"$f":"AG65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU37","v":0},{"$f":"AH65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV37","v":0},{"$f":"AI65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW37","v":0},{"$f":"AJ65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX37","v":0},{"$f":"AK65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY37","v":0},{"$f":"AL65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ37","v":0},{"$f":"AM65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA37","v":0},{"$f":"AN65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB37","v":0},{"$f":"AO65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC37","v":0},{"$f":"AP65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD37","v":0},{"$f":"AQ65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE37","v":0},{"$f":"AR65*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF37","v":0},null,6,{"$f":"AU65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI37","v":0},{"$f":"AV65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ37","v":0},{"$f":"AW65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK37","v":0},{"$f":"AX65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL37","v":0},{"$f":"AY65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM37","v":0},{"$f":"AZ65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN37","v":0},{"$f":"BA65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO37","v":0},{"$f":"BB65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP37","v":0},{"$f":"BC65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ37","v":0},{"$f":"BD65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR37","v":0},{"$f":"BE65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS37","v":0},{"$f":"BF65*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT37","v":0},null,6,0,0,0,0,0,0,0,0,0,0,0,0,null,6,0,0,0,0,0,0,0,0,0,0,0,0,null,null,6,-12.151444093159176,-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719,null,6,-12.151444093159176,-9.1319080559186769,-3.3232309033445411,3.5985816694690373,7.5112987220277185,7.7738597839019823,5.5584053941199079,2.9033723023449274,8.3279910069695443E-2,-2.6015900354108483,-6.7413522567651629,-10.743396255327719]
[null,7,{"$f":"DEGREES(C94)","v":157.63688498626229},165.6412812783924,168.6583333333333,162.08351217694067,155.48661671610134,153.42793355434173,156.53753822231249,162.58709776891263,164.9083333333333,159.94140931706849,154.26159820121021,153.07774381747009,null,7,{"$f":"DEGREES(Q94)","v":112.3509519653864},103.68716030915026,94.713734410568321,84.724585507937306,77.284796979506481,73.968066456633792,76.171445709197073,84.192041856490007,96.246005842661603,106.80915200101074,114.95630857341712,116.85863471068787,null,null,null,7,{"$f":"IF(DO66<0,0,IF(0>C66,0,IF(50>C66,(( -0.000009*C66^2 + 0.0004*C66 + 0.7918)*Radiation!C10),IF(90>C66,((-0.0006*C66^2 + 0.0699*C66 - 1.2225)*Radiation!C10),0))))","v":0},{"$f":"IF(DP66<0,0,IF(0>D66,0,IF(50>D66,(( -0.000009*D66^2 + 0.0004*D66 + 0.7918)*Radiation!D10),IF(90>D66,((-0.0006*D66^2 + 0.0699*D66 - 1.2225)*Radiation!D10),0))))","v":0},{"$f":"IF(DQ66<0,0,IF(0>E66,0,IF(50>E66,(( -0.000009*E66^2 + 0.0004*E66 + 0.7918)*Radiation!E10),IF(90>E66,((-0.0006*E66^2 + 0.0699*E66 - 1.2225)*Radiation!E10),0))))","v":0},{"$f":"IF(DR66<0,0,IF(0>F66,0,IF(50>F66,(( -0.000009*F66^2 + 0.0004*F66 + 0.7918)*Radiation!F10),IF(90>F66,((-0.0006*F66^2 + 0.0699*F66 - 1.2225)*Radiation!F10),0))))","v":0},{"$f":"IF(DS66<0,0,IF(0>G66,0,IF(50>G66,(( -0.000009*G66^2 + 0.0004*G66 + 0.7918)*Radiation!G10),IF(90>G66,((-0.0006*G66^2 + 0.0699*G66 - 1.2225)*Radiation!G10),0))))","v":0},{"$f":"IF(DT66<0,0,IF(0>H66,0,IF(50>H66,(( -0.000009*H66^2 + 0.0004*H66 + 0.7918)*Radiation!H10),IF(90>H66,((-0.0006*H66^2 + 0.0699*H66 - 1.2225)*Radiation!H10),0))))","v":0},{"$f":"IF(DU66<0,0,IF(0>I66,0,IF(50>I66,(( -0.000009*I66^2 + 0.0004*I66 + 0.7918)*Radiation!I10),IF(90>I66,((-0.0006*I66^2 + 0.0699*I66 - 1.2225)*Radiation!I10),0))))","v":0},{"$f":"IF(DV66<0,0,IF(0>J66,0,IF(50>J66,(( -0.000009*J66^2 + 0.0004*J66 + 0.7918)*Radiation!J10),IF(90>J66,((-0.0006*J66^2 + 0.0699*J66 - 1.2225)*Radiation!J10),0))))","v":0},{"$f":"IF(DW66<0,0,IF(0>K66,0,IF(50>K66,(( -0.000009*K66^2 + 0.0004*K66 + 0.7918)*Radiation!K10),IF(90>K66,((-0.0006*K66^2 + 0.0699*K66 - 1.2225)*Radiation!K10),0))))","v":0},{"$f":"IF(DX66<0,0,IF(0>L66,0,IF(50>L66,(( -0.000009*L66^2 + 0.0004*L66 + 0.7918)*Radiation!L10),IF(90>L66,((-0.0006*L66^2 + 0.0699*L66 - 1.2225)*Radiation!L10),0))))","v":0},{"$f":"IF(DY66<0,0,IF(0>M66,0,IF(50>M66,(( -0.000009*M66^2 + 0.0004*M66 + 0.7918)*Radiation!M10),IF(90>M66,((-0.0006*M66^2 + 0.0699*M66 - 1.2225)*Radiation!M10),0))))","v":0},{"$f":"IF(DZ66<0,0,IF(0>N66,0,IF(50>N66,(( -0.000009*N66^2 + 0.0004*N66 + 0.7918)*Radiation!N10),IF(90>N66,((-0.0006*N66^2 + 0.0699*N66 - 1.2225)*Radiation!N10),0))))","v":0},null,7,{"$f":"IF(EC66<0,0,IF(0>Q66,0,IF(50>Q66,(( -0.000009*Q66^2 + 0.0004*Q66 + 0.7918)*Radiation!C10),IF(90>Q66,((-0.0006*Q66^2 + 0.0699*Q66 - 1.2225)*Radiation!C10),0))))","v":0},{"$f":"IF(ED66<0,0,IF(0>R66,0,IF(50>R66,(( -0.000009*R66^2 + 0.0004*R66 + 0.7918)*Radiation!D10),IF(90>R66,((-0.0006*R66^2 + 0.0699*R66 - 1.2225)*Radiation!D10),0))))","v":0},{"$f":"IF(EE66<0,0,IF(0>S66,0,IF(50>S66,(( -0.000009*S66^2 + 0.0004*S66 + 0.7918)*Radiation!E10),IF(90>S66,((-0.0006*S66^2 + 0.0699*S66 - 1.2225)*Radiation!E10),0))))","v":0},{"$f":"IF(EF66<0,0,IF(0>T66,0,IF(50>T66,(( -0.000009*T66^2 + 0.0004*T66 + 0.7918)*Radiation!F10),IF(90>T66,((-0.0006*T66^2 + 0.0699*T66 - 1.2225)*Radiation!F10),0))))","v":13.945741561128704},{"$f":"IF(EG66<0,0,IF(0>U66,0,IF(50>U66,(( -0.000009*U66^2 + 0.0004*U66 + 0.7918)*Radiation!G10),IF(90>U66,((-0.0006*U66^2 + 0.0699*U66 - 1.2225)*Radiation!G10),0))))","v":30.981766680503149},{"$f":"IF(EH66<0,0,IF(0>V66,0,IF(50>V66,(( -0.000009*V66^2 + 0.0004*V66 + 0.7918)*Radiation!H10),IF(90>V66,((-0.0006*V66^2 + 0.0699*V66 - 1.2225)*Radiation!H10),0))))","v":39.004786557110435},{"$f":"IF(EI66<0,0,IF(0>W66,0,IF(50>W66,(( -0.000009*W66^2 + 0.0004*W66 + 0.7918)*Radiation!I10),IF(90>W66,((-0.0006*W66^2 + 0.0699*W66 - 1.2225)*Radiation!I10),0))))","v":28.330417235934991},{"$f":"IF(EJ66<0,0,IF(0>X66,0,IF(50>X66,(( -0.000009*X66^2 + 0.0004*X66 + 0.7918)*Radiation!J10),IF(90>X66,((-0.0006*X66^2 + 0.0699*X66 - 1.2225)*Radiation!J10),0))))","v":14.80002670752841},{"$f":"IF(EK66<0,0,IF(0>Y66,0,IF(50>Y66,(( -0.000009*Y66^2 + 0.0004*Y66 + 0.7918)*Radiation!K10),IF(90>Y66,((-0.0006*Y66^2 + 0.0699*Y66 - 1.2225)*Radiation!K10),0))))","v":0},{"$f":"IF(EL66<0,0,IF(0>Z66,0,IF(50>Z66,(( -0.000009*Z66^2 + 0.0004*Z66 + 0.7918)*Radiation!L10),IF(90>Z66,((-0.0006*Z66^2 + 0.0699*Z66 - 1.2225)*Radiation!L10),0))))","v":0},{"$f":"IF(EM66<0,0,IF(0>AA66,0,IF(50>AA66,(( -0.000009*AA66^2 + 0.0004*AA66 + 0.7918)*Radiation!M10),IF(90>AA66,((-0.0006*AA66^2 + 0.0699*AA66 - 1.2225)*Radiation!M10),0))))","v":0},{"$f":"IF(EN66<0,0,IF(0>AB66,0,IF(50>AB66,(( -0.000009*AB66^2 + 0.0004*AB66 + 0.7918)*Radiation!N10),IF(90>AB66,((-0.0006*AB66^2 + 0.0699*AB66 - 1.2225)*Radiation!N10),0))))","v":0},null,null,7,{"$f":"AG66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU38","v":0},{"$f":"AH66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV38","v":0},{"$f":"AI66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW38","v":0},{"$f":"AJ66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX38","v":0},{"$f":"AK66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY38","v":0},{"$f":"AL66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ38","v":0},{"$f":"AM66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA38","v":0},{"$f":"AN66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB38","v":0},{"$f":"AO66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC38","v":0},{"$f":"AP66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD38","v":0},{"$f":"AQ66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE38","v":0},{"$f":"AR66*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF38","v":0},null,7,{"$f":"AU66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI38","v":0},{"$f":"AV66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ38","v":0},{"$f":"AW66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK38","v":0},{"$f":"AX66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL38","v":0},{"$f":"AY66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM38","v":0},{"$f":"AZ66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN38","v":0},{"$f":"BA66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO38","v":0},{"$f":"BB66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP38","v":0},{"$f":"BC66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ38","v":0},{"$f":"BD66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR38","v":0},{"$f":"BE66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS38","v":0},{"$f":"BF66*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT38","v":0},null,7,0,0,0,0,0,0,0,0,0,0,0,0,null,7,0,0,0,0,0,0,0,0,0,0,0,0,null,null,7,0.70023973357815916,4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048,null,7,0.70023973357815916,4.2572512510716702,10.292097151668541,17.071764306110264,20.59199880999245,20.602944398333847,18.567526961418682,16.357318748220177,13.682588857300253,10.626902061270702,5.8987575020687171,1.7151458456731048]
[null,8,{"$f":"DEGREES(C95)","v":148.13323739219499},153.21525979942476,153.65833333333333,149.31639654713646,145.08131660023739,144.19600228883124,146.82894645510487,150.04102520570484,149.9083333333333,146.37673625967994,143.1582726356977,143.64315809950043,null,8,{"$f":"DEGREES(Q95)","v":118.54677736025225},109.81753238579472,100.68545928652112,90.44195023199147,82.822622073747766,79.493111787368477,81.807216657832896,89.940424930203235,102.09376987845592,112.74747463067951,121.03148420528679,123.03465148536529,null,null,null,8,{"$f":"IF(DO67<0,0,IF(0>C67,0,IF(50>C67,(( -0.000009*C67^2 + 0.0004*C67 + 0.7918)*Radiation!C11),IF(90>C67,((-0.0006*C67^2 + 0.0699*C67 - 1.2225)*Radiation!C11),0))))","v":0},{"$f":"IF(DP67<0,0,IF(0>D67,0,IF(50>D67,(( -0.000009*D67^2 + 0.0004*D67 + 0.7918)*Radiation!D11),IF(90>D67,((-0.0006*D67^2 + 0.0699*D67 - 1.2225)*Radiation!D11),0))))","v":0},{"$f":"IF(DQ67<0,0,IF(0>E67,0,IF(50>E67,(( -0.000009*E67^2 + 0.0004*E67 + 0.7918)*Radiation!E11),IF(90>E67,((-0.0006*E67^2 + 0.0699*E67 - 1.2225)*Radiation!E11),0))))","v":0},{"$f":"IF(DR67<0,0,IF(0>F67,0,IF(50>F67,(( -0.000009*F67^2 + 0.0004*F67 + 0.7918)*Radiation!F11),IF(90>F67,((-0.0006*F67^2 + 0.0699*F67 - 1.2225)*Radiation!F11),0))))","v":0},{"$f":"IF(DS67<0,0,IF(0>G67,0,IF(50>G67,(( -0.000009*G67^2 + 0.0004*G67 + 0.7918)*Radiation!G11),IF(90>G67,((-0.0006*G67^2 + 0.0699*G67 - 1.2225)*Radiation!G11),0))))","v":0},{"$f":"IF(DT67<0,0,IF(0>H67,0,IF(50>H67,(( -0.000009*H67^2 + 0.0004*H67 + 0.7918)*Radiation!H11),IF(90>H67,((-0.0006*H67^2 + 0.0699*H67 - 1.2225)*Radiation!H11),0))))","v":0},{"$f":"IF(DU67<0,0,IF(0>I67,0,IF(50>I67,(( -0.000009*I67^2 + 0.0004*I67 + 0.7918)*Radiation!I11),IF(90>I67,((-0.0006*I67^2 + 0.0699*I67 - 1.2225)*Radiation!I11),0))))","v":0},{"$f":"IF(DV67<0,0,IF(0>J67,0,IF(50>J67,(( -0.000009*J67^2 + 0.0004*J67 + 0.7918)*Radiation!J11),IF(90>J67,((-0.0006*J67^2 + 0.0699*J67 - 1.2225)*Radiation!J11),0))))","v":0},{"$f":"IF(DW67<0,0,IF(0>K67,0,IF(50>K67,(( -0.000009*K67^2 + 0.0004*K67 + 0.7918)*Radiation!K11),IF(90>K67,((-0.0006*K67^2 + 0.0699*K67 - 1.2225)*Radiation!K11),0))))","v":0},{"$f":"IF(DX67<0,0,IF(0>L67,0,IF(50>L67,(( -0.000009*L67^2 + 0.0004*L67 + 0.7918)*Radiation!L11),IF(90>L67,((-0.0006*L67^2 + 0.0699*L67 - 1.2225)*Radiation!L11),0))))","v":0},{"$f":"IF(DY67<0,0,IF(0>M67,0,IF(50>M67,(( -0.000009*M67^2 + 0.0004*M67 + 0.7918)*Radiation!M11),IF(90>M67,((-0.0006*M67^2 + 0.0699*M67 - 1.2225)*Radiation!M11),0))))","v":0},{"$f":"IF(DZ67<0,0,IF(0>N67,0,IF(50>N67,(( -0.000009*N67^2 + 0.0004*N67 + 0.7918)*Radiation!N11),IF(90>N67,((-0.0006*N67^2 + 0.0699*N67 - 1.2225)*Radiation!N11),0))))","v":0},null,8,{"$f":"IF(EC67<0,0,IF(0>Q67,0,IF(50>Q67,(( -0.000009*Q67^2 + 0.0004*Q67 + 0.7918)*Radiation!C11),IF(90>Q67,((-0.0006*Q67^2 + 0.0699*Q67 - 1.2225)*Radiation!C11),0))))","v":0},{"$f":"IF(ED67<0,0,IF(0>R67,0,IF(50>R67,(( -0.000009*R67^2 + 0.0004*R67 + 0.7918)*Radiation!D11),IF(90>R67,((-0.0006*R67^2 + 0.0699*R67 - 1.2225)*Radiation!D11),0))))","v":0},{"$f":"IF(EE67<0,0,IF(0>S67,0,IF(50>S67,(( -0.000009*S67^2 + 0.0004*S67 + 0.7918)*Radiation!E11),IF(90>S67,((-0.0006*S67^2 + 0.0699*S67 - 1.2225)*Radiation!E11),0))))","v":0},{"$f":"IF(EF67<0,0,IF(0>T67,0,IF(50>T67,(( -0.000009*T67^2 + 0.0004*T67 + 0.7918)*Radiation!F11),IF(90>T67,((-0.0006*T67^2 + 0.0699*T67 - 1.2225)*Radiation!F11),0))))","v":0},{"$f":"IF(EG67<0,0,IF(0>U67,0,IF(50>U67,(( -0.000009*U67^2 + 0.0004*U67 + 0.7918)*Radiation!G11),IF(90>U67,((-0.0006*U67^2 + 0.0699*U67 - 1.2225)*Radiation!G11),0))))","v":54.619112562676328},{"$f":"IF(EH67<0,0,IF(0>V67,0,IF(50>V67,(( -0.000009*V67^2 + 0.0004*V67 + 0.7918)*Radiation!H11),IF(90>V67,((-0.0006*V67^2 + 0.0699*V67 - 1.2225)*Radiation!H11),0))))","v":72.582185659785196},{"$f":"IF(EI67<0,0,IF(0>W67,0,IF(50>W67,(( -0.000009*W67^2 + 0.0004*W67 + 0.7918)*Radiation!I11),IF(90>W67,((-0.0006*W67^2 + 0.0699*W67 - 1.2225)*Radiation!I11),0))))","v":57.103968537413216},{"$f":"IF(EJ67<0,0,IF(0>X67,0,IF(50>X67,(( -0.000009*X67^2 + 0.0004*X67 + 0.7918)*Radiation!J11),IF(90>X67,((-0.0006*X67^2 + 0.0699*X67 - 1.2225)*Radiation!J11),0))))","v":22.983690980474098},{"$f":"IF(EK67<0,0,IF(0>Y67,0,IF(50>Y67,(( -0.000009*Y67^2 + 0.0004*Y67 + 0.7918)*Radiation!K11),IF(90>Y67,((-0.0006*Y67^2 + 0.0699*Y67 - 1.2225)*Radiation!K11),0))))","v":0},{"$f":"IF(EL67<0,0,IF(0>Z67,0,IF(50>Z67,(( -0.000009*Z67^2 + 0.0004*Z67 + 0.7918)*Radiation!L11),IF(90>Z67,((-0.0006*Z67^2 + 0.0699*Z67 - 1.2225)*Radiation!L11),0))))","v":0},{"$f":"IF(EM67<0,0,IF(0>AA67,0,IF(50>AA67,(( -0.000009*AA67^2 + 0.0004*AA67 + 0.7918)*Radiation!M11),IF(90>AA67,((-0.0006*AA67^2 + 0.0699*AA67 - 1.2225)*Radiation!M11),0))))","v":0},{"$f":"IF(EN67<0,0,IF(0>AB67,0,IF(50>AB67,(( -0.000009*AB67^2 + 0.0004*AB67 + 0.7918)*Radiation!N11),IF(90>AB67,((-0.0006*AB67^2 + 0.0699*AB67 - 1.2225)*Radiation!N11),0))))","v":0},null,null,8,{"$f":"AG67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU39","v":0},{"$f":"AH67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV39","v":0},{"$f":"AI67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW39","v":0},{"$f":"AJ67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX39","v":0},{"$f":"AK67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY39","v":0},{"$f":"AL67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ39","v":0},{"$f":"AM67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA39","v":0},{"$f":"AN67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB39","v":0},{"$f":"AO67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC39","v":0},{"$f":"AP67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD39","v":0},{"$f":"AQ67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE39","v":0},{"$f":"AR67*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF39","v":0},null,8,{"$f":"AU67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI39","v":0},{"$f":"AV67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ39","v":0},{"$f":"AW67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK39","v":0},{"$f":"AX67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL39","v":0},{"$f":"AY67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM39","v":0},{"$f":"AZ67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN39","v":0},{"$f":"BA67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO39","v":0},{"$f":"BB67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP39","v":0},{"$f":"BC67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ39","v":0},{"$f":"BD67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR39","v":0},{"$f":"BE67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS39","v":0},{"$f":"BF67*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT39","v":0},null,8,0,0,0,0,0,0,0,0,0,0,0,0,null,8,0,0,0,0,0,0,0,0,0,0,0,0,null,null,8,12.968359542715392,17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182,null,8,12.968359542715392,17.270303982095768,23.773745192987032,30.67971943621767,33.959814353189685,33.770494749028082,31.887744015481577,29.958903207045175,27.097900221004789,23.350930400204959,17.832347455280527,13.467847656409182]
[null,9,{"$f":"DEGREES(C96)","v":135.71603163262765},139.09647815180844,138.65833333333333,135.22542089337185,132.39103758245219,132.25285571248872,134.40435211228032,136.01740948977312,134.90833333333333,132.01334596260335,130.18553699274204,131.61920109776082,null,9,{"$f":"DEGREES(Q96)","v":124.33155689806468},115.44955050597933,106.02287954007555,95.398237690219304,87.550239999561313,84.217891918710222,86.677148303333709,94.945469885644243,107.21445179579571,117.98888162526198,126.51505201270211,128.75481904371853,null,null,null,9,{"$f":"IF(DO68<0,0,IF(0>C68,0,IF(50>C68,(( -0.000009*C68^2 + 0.0004*C68 + 0.7918)*Radiation!C12),IF(90>C68,((-0.0006*C68^2 + 0.0699*C68 - 1.2225)*Radiation!C12),0))))","v":0},{"$f":"IF(DP68<0,0,IF(0>D68,0,IF(50>D68,(( -0.000009*D68^2 + 0.0004*D68 + 0.7918)*Radiation!D12),IF(90>D68,((-0.0006*D68^2 + 0.0699*D68 - 1.2225)*Radiation!D12),0))))","v":0},{"$f":"IF(DQ68<0,0,IF(0>E68,0,IF(50>E68,(( -0.000009*E68^2 + 0.0004*E68 + 0.7918)*Radiation!E12),IF(90>E68,((-0.0006*E68^2 + 0.0699*E68 - 1.2225)*Radiation!E12),0))))","v":0},{"$f":"IF(DR68<0,0,IF(0>F68,0,IF(50>F68,(( -0.000009*F68^2 + 0.0004*F68 + 0.7918)*Radiation!F12),IF(90>F68,((-0.0006*F68^2 + 0.0699*F68 - 1.2225)*Radiation!F12),0))))","v":0},{"$f":"IF(DS68<0,0,IF(0>G68,0,IF(50>G68,(( -0.000009*G68^2 + 0.0004*G68 + 0.7918)*Radiation!G12),IF(90>G68,((-0.0006*G68^2 + 0.0699*G68 - 1.2225)*Radiation!G12),0))))","v":0},{"$f":"IF(DT68<0,0,IF(0>H68,0,IF(50>H68,(( -0.000009*H68^2 + 0.0004*H68 + 0.7918)*Radiation!H12),IF(90>H68,((-0.0006*H68^2 + 0.0699*H68 - 1.2225)*Radiation!H12),0))))","v":0},{"$f":"IF(DU68<0,0,IF(0>I68,0,IF(50>I68,(( -0.000009*I68^2 + 0.0004*I68 + 0.7918)*Radiation!I12),IF(90>I68,((-0.0006*I68^2 + 0.0699*I68 - 1.2225)*Radiation!I12),0))))","v":0},{"$f":"IF(DV68<0,0,IF(0>J68,0,IF(50>J68,(( -0.000009*J68^2 + 0.0004*J68 + 0.7918)*Radiation!J12),IF(90>J68,((-0.0006*J68^2 + 0.0699*J68 - 1.2225)*Radiation!J12),0))))","v":0},{"$f":"IF(DW68<0,0,IF(0>K68,0,IF(50>K68,(( -0.000009*K68^2 + 0.0004*K68 + 0.7918)*Radiation!K12),IF(90>K68,((-0.0006*K68^2 + 0.0699*K68 - 1.2225)*Radiation!K12),0))))","v":0},{"$f":"IF(DX68<0,0,IF(0>L68,0,IF(50>L68,(( -0.000009*L68^2 + 0.0004*L68 + 0.7918)*Radiation!L12),IF(90>L68,((-0.0006*L68^2 + 0.0699*L68 - 1.2225)*Radiation!L12),0))))","v":0},{"$f":"IF(DY68<0,0,IF(0>M68,0,IF(50>M68,(( -0.000009*M68^2 + 0.0004*M68 + 0.7918)*Radiation!M12),IF(90>M68,((-0.0006*M68^2 + 0.0699*M68 - 1.2225)*Radiation!M12),0))))","v":0},{"$f":"IF(DZ68<0,0,IF(0>N68,0,IF(50>N68,(( -0.000009*N68^2 + 0.0004*N68 + 0.7918)*Radiation!N12),IF(90>N68,((-0.0006*N68^2 + 0.0699*N68 - 1.2225)*Radiation!N12),0))))","v":0},null,9,{"$f":"IF(EC68<0,0,IF(0>Q68,0,IF(50>Q68,(( -0.000009*Q68^2 + 0.0004*Q68 + 0.7918)*Radiation!C12),IF(90>Q68,((-0.0006*Q68^2 + 0.0699*Q68 - 1.2225)*Radiation!C12),0))))","v":0},{"$f":"IF(ED68<0,0,IF(0>R68,0,IF(50>R68,(( -0.000009*R68^2 + 0.0004*R68 + 0.7918)*Radiation!D12),IF(90>R68,((-0.0006*R68^2 + 0.0699*R68 - 1.2225)*Radiation!D12),0))))","v":0},{"$f":"IF(EE68<0,0,IF(0>S68,0,IF(50>S68,(( -0.000009*S68^2 + 0.0004*S68 + 0.7918)*Radiation!E12),IF(90>S68,((-0.0006*S68^2 + 0.0699*S68 - 1.2225)*Radiation!E12),0))))","v":0},{"$f":"IF(EF68<0,0,IF(0>T68,0,IF(50>T68,(( -0.000009*T68^2 + 0.0004*T68 + 0.7918)*Radiation!F12),IF(90>T68,((-0.0006*T68^2 + 0.0699*T68 - 1.2225)*Radiation!F12),0))))","v":0},{"$f":"IF(EG68<0,0,IF(0>U68,0,IF(50>U68,(( -0.000009*U68^2 + 0.0004*U68 + 0.7918)*Radiation!G12),IF(90>U68,((-0.0006*U68^2 + 0.0699*U68 - 1.2225)*Radiation!G12),0))))","v":55.58957327543601},{"$f":"IF(EH68<0,0,IF(0>V68,0,IF(50>V68,(( -0.000009*V68^2 + 0.0004*V68 + 0.7918)*Radiation!H12),IF(90>V68,((-0.0006*V68^2 + 0.0699*V68 - 1.2225)*Radiation!H12),0))))","v":84.349791499649044},{"$f":"IF(EI68<0,0,IF(0>W68,0,IF(50>W68,(( -0.000009*W68^2 + 0.0004*W68 + 0.7918)*Radiation!I12),IF(90>W68,((-0.0006*W68^2 + 0.0699*W68 - 1.2225)*Radiation!I12),0))))","v":63.412962692337821},{"$f":"IF(EJ68<0,0,IF(0>X68,0,IF(50>X68,(( -0.000009*X68^2 + 0.0004*X68 + 0.7918)*Radiation!J12),IF(90>X68,((-0.0006*X68^2 + 0.0699*X68 - 1.2225)*Radiation!J12),0))))","v":0},{"$f":"IF(EK68<0,0,IF(0>Y68,0,IF(50>Y68,(( -0.000009*Y68^2 + 0.0004*Y68 + 0.7918)*Radiation!K12),IF(90>Y68,((-0.0006*Y68^2 + 0.0699*Y68 - 1.2225)*Radiation!K12),0))))","v":0},{"$f":"IF(EL68<0,0,IF(0>Z68,0,IF(50>Z68,(( -0.000009*Z68^2 + 0.0004*Z68 + 0.7918)*Radiation!L12),IF(90>Z68,((-0.0006*Z68^2 + 0.0699*Z68 - 1.2225)*Radiation!L12),0))))","v":0},{"$f":"IF(EM68<0,0,IF(0>AA68,0,IF(50>AA68,(( -0.000009*AA68^2 + 0.0004*AA68 + 0.7918)*Radiation!M12),IF(90>AA68,((-0.0006*AA68^2 + 0.0699*AA68 - 1.2225)*Radiation!M12),0))))","v":0},{"$f":"IF(EN68<0,0,IF(0>AB68,0,IF(50>AB68,(( -0.000009*AB68^2 + 0.0004*AB68 + 0.7918)*Radiation!N12),IF(90>AB68,((-0.0006*AB68^2 + 0.0699*AB68 - 1.2225)*Radiation!N12),0))))","v":0},null,null,9,{"$f":"AG68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU40","v":0},{"$f":"AH68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV40","v":0},{"$f":"AI68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW40","v":0},{"$f":"AJ68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX40","v":0},{"$f":"AK68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY40","v":0},{"$f":"AL68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ40","v":0},{"$f":"AM68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA40","v":0},{"$f":"AN68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB40","v":0},{"$f":"AO68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC40","v":0},{"$f":"AP68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD40","v":0},{"$f":"AQ68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE40","v":0},{"$f":"AR68*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF40","v":0},null,9,{"$f":"AU68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI40","v":0},{"$f":"AV68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ40","v":0},{"$f":"AW68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK40","v":0},{"$f":"AX68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL40","v":0},{"$f":"AY68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM40","v":0},{"$f":"AZ68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN40","v":0},{"$f":"BA68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO40","v":0},{"$f":"BB68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP40","v":0},{"$f":"BC68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ40","v":0},{"$f":"BD68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR40","v":0},{"$f":"BE68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS40","v":0},{"$f":"BF68*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT40","v":0},null,9,0,0,0,0,0,0,0,0,0,0,0,0,null,9,0,0,0,0,0,0,0,0,0,0,0,0,null,null,9,24.306538235547787,29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159,null,9,24.306538235547787,29.607456719563572,36.877998514340362,44.267398869292073,47.503865138538167,47.16345799134892,45.403126432581416,43.556385601632783,40.048756889246128,35.170537312656599,28.628753160625717,24.120985503613159]
[null,10,{"$f":"DEGREES(C97)","v":122.25657509727938},124.5700332372281,123.65833333333332,120.75652012675037,118.84643748288642,119.20666482557658,120.97805808445807,121.57957777098981,119.9083333333333,117.40640051600555,116.50405138107803,118.53858289990018,null,10,{"$f":"DEGREES(Q97)","v":129.25149154982509},120.16627721247623,110.35371355363357,99.28026777201643,91.196867003161756,87.884721934733363,90.506924815696635,98.893707472179301,111.23643107049955,122.10302624963629,130.92589286413408,133.53599839475766,null,null,null,10,{"$f":"IF(DO69<0,0,IF(0>C69,0,IF(50>C69,(( -0.000009*C69^2 + 0.0004*C69 + 0.7918)*Radiation!C13),IF(90>C69,((-0.0006*C69^2 + 0.0699*C69 - 1.2225)*Radiation!C13),0))))","v":0},{"$f":"IF(DP69<0,0,IF(0>D69,0,IF(50>D69,(( -0.000009*D69^2 + 0.0004*D69 + 0.7918)*Radiation!D13),IF(90>D69,((-0.0006*D69^2 + 0.0699*D69 - 1.2225)*Radiation!D13),0))))","v":0},{"$f":"IF(DQ69<0,0,IF(0>E69,0,IF(50>E69,(( -0.000009*E69^2 + 0.0004*E69 + 0.7918)*Radiation!E13),IF(90>E69,((-0.0006*E69^2 + 0.0699*E69 - 1.2225)*Radiation!E13),0))))","v":0},{"$f":"IF(DR69<0,0,IF(0>F69,0,IF(50>F69,(( -0.000009*F69^2 + 0.0004*F69 + 0.7918)*Radiation!F13),IF(90>F69,((-0.0006*F69^2 + 0.0699*F69 - 1.2225)*Radiation!F13),0))))","v":0},{"$f":"IF(DS69<0,0,IF(0>G69,0,IF(50>G69,(( -0.000009*G69^2 + 0.0004*G69 + 0.7918)*Radiation!G13),IF(90>G69,((-0.0006*G69^2 + 0.0699*G69 - 1.2225)*Radiation!G13),0))))","v":0},{"$f":"IF(DT69<0,0,IF(0>H69,0,IF(50>H69,(( -0.000009*H69^2 + 0.0004*H69 + 0.7918)*Radiation!H13),IF(90>H69,((-0.0006*H69^2 + 0.0699*H69 - 1.2225)*Radiation!H13),0))))","v":0},{"$f":"IF(DU69<0,0,IF(0>I69,0,IF(50>I69,(( -0.000009*I69^2 + 0.0004*I69 + 0.7918)*Radiation!I13),IF(90>I69,((-0.0006*I69^2 + 0.0699*I69 - 1.2225)*Radiation!I13),0))))","v":0},{"$f":"IF(DV69<0,0,IF(0>J69,0,IF(50>J69,(( -0.000009*J69^2 + 0.0004*J69 + 0.7918)*Radiation!J13),IF(90>J69,((-0.0006*J69^2 + 0.0699*J69 - 1.2225)*Radiation!J13),0))))","v":0},{"$f":"IF(DW69<0,0,IF(0>K69,0,IF(50>K69,(( -0.000009*K69^2 + 0.0004*K69 + 0.7918)*Radiation!K13),IF(90>K69,((-0.0006*K69^2 + 0.0699*K69 - 1.2225)*Radiation!K13),0))))","v":0},{"$f":"IF(DX69<0,0,IF(0>L69,0,IF(50>L69,(( -0.000009*L69^2 + 0.0004*L69 + 0.7918)*Radiation!L13),IF(90>L69,((-0.0006*L69^2 + 0.0699*L69 - 1.2225)*Radiation!L13),0))))","v":0},{"$f":"IF(DY69<0,0,IF(0>M69,0,IF(50>M69,(( -0.000009*M69^2 + 0.0004*M69 + 0.7918)*Radiation!M13),IF(90>M69,((-0.0006*M69^2 + 0.0699*M69 - 1.2225)*Radiation!M13),0))))","v":0},{"$f":"IF(DZ69<0,0,IF(0>N69,0,IF(50>N69,(( -0.000009*N69^2 + 0.0004*N69 + 0.7918)*Radiation!N13),IF(90>N69,((-0.0006*N69^2 + 0.0699*N69 - 1.2225)*Radiation!N13),0))))","v":0},null,10,{"$f":"IF(EC69<0,0,IF(0>Q69,0,IF(50>Q69,(( -0.000009*Q69^2 + 0.0004*Q69 + 0.7918)*Radiation!C13),IF(90>Q69,((-0.0006*Q69^2 + 0.0699*Q69 - 1.2225)*Radiation!C13),0))))","v":0},{"$f":"IF(ED69<0,0,IF(0>R69,0,IF(50>R69,(( -0.000009*R69^2 + 0.0004*R69 + 0.7918)*Radiation!D13),IF(90>R69,((-0.0006*R69^2 + 0.0699*R69 - 1.2225)*Radiation!D13),0))))","v":0},{"$f":"IF(EE69<0,0,IF(0>S69,0,IF(50>S69,(( -0.000009*S69^2 + 0.0004*S69 + 0.7918)*Radiation!E13),IF(90>S69,((-0.0006*S69^2 + 0.0699*S69 - 1.2225)*Radiation!E13),0))))","v":0},{"$f":"IF(EF69<0,0,IF(0>T69,0,IF(50>T69,(( -0.000009*T69^2 + 0.0004*T69 + 0.7918)*Radiation!F13),IF(90>T69,((-0.0006*T69^2 + 0.0699*T69 - 1.2225)*Radiation!F13),0))))","v":0},{"$f":"IF(EG69<0,0,IF(0>U69,0,IF(50>U69,(( -0.000009*U69^2 + 0.0004*U69 + 0.7918)*Radiation!G13),IF(90>U69,((-0.0006*U69^2 + 0.0699*U69 - 1.2225)*Radiation!G13),0))))","v":0},{"$f":"IF(EH69<0,0,IF(0>V69,0,IF(50>V69,(( -0.000009*V69^2 + 0.0004*V69 + 0.7918)*Radiation!H13),IF(90>V69,((-0.0006*V69^2 + 0.0699*V69 - 1.2225)*Radiation!H13),0))))","v":76.355025508536954},{"$f":"IF(EI69<0,0,IF(0>W69,0,IF(50>W69,(( -0.000009*W69^2 + 0.0004*W69 + 0.7918)*Radiation!I13),IF(90>W69,((-0.0006*W69^2 + 0.0699*W69 - 1.2225)*Radiation!I13),0))))","v":0},{"$f":"IF(EJ69<0,0,IF(0>X69,0,IF(50>X69,(( -0.000009*X69^2 + 0.0004*X69 + 0.7918)*Radiation!J13),IF(90>X69,((-0.0006*X69^2 + 0.0699*X69 - 1.2225)*Radiation!J13),0))))","v":0},{"$f":"IF(EK69<0,0,IF(0>Y69,0,IF(50>Y69,(( -0.000009*Y69^2 + 0.0004*Y69 + 0.7918)*Radiation!K13),IF(90>Y69,((-0.0006*Y69^2 + 0.0699*Y69 - 1.2225)*Radiation!K13),0))))","v":0},{"$f":"IF(EL69<0,0,IF(0>Z69,0,IF(50>Z69,(( -0.000009*Z69^2 + 0.0004*Z69 + 0.7918)*Radiation!L13),IF(90>Z69,((-0.0006*Z69^2 + 0.0699*Z69 - 1.2225)*Radiation!L13),0))))","v":0},{"$f":"IF(EM69<0,0,IF(0>AA69,0,IF(50>AA69,(( -0.000009*AA69^2 + 0.0004*AA69 + 0.7918)*Radiation!M13),IF(90>AA69,((-0.0006*AA69^2 + 0.0699*AA69 - 1.2225)*Radiation!M13),0))))","v":0},{"$f":"IF(EN69<0,0,IF(0>AB69,0,IF(50>AB69,(( -0.000009*AB69^2 + 0.0004*AB69 + 0.7918)*Radiation!N13),IF(90>AB69,((-0.0006*AB69^2 + 0.0699*AB69 - 1.2225)*Radiation!N13),0))))","v":0},null,null,10,{"$f":"AG69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU41","v":0},{"$f":"AH69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV41","v":0},{"$f":"AI69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW41","v":0},{"$f":"AJ69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX41","v":0},{"$f":"AK69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY41","v":0},{"$f":"AL69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ41","v":0},{"$f":"AM69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA41","v":0},{"$f":"AN69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB41","v":0},{"$f":"AO69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC41","v":0},{"$f":"AP69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD41","v":0},{"$f":"AQ69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE41","v":0},{"$f":"AR69*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF41","v":0},null,10,{"$f":"AU69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI41","v":0},{"$f":"AV69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ41","v":0},{"$f":"AW69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK41","v":0},{"$f":"AX69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL41","v":0},{"$f":"AY69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM41","v":0},{"$f":"AZ69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN41","v":0},{"$f":"BA69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO41","v":0},{"$f":"BB69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP41","v":0},{"$f":"BC69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ41","v":0},{"$f":"BD69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR41","v":0},{"$f":"BE69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS41","v":0},{"$f":"BF69*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT41","v":0},null,10,0,0,0,0,0,0,0,0,0,0,0,0,null,10,0,0,0,0,0,0,0,0,0,0,0,0,null,null,10,34.130498638110296,40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,{"$f":"DY14","v":37.566870997040184},33.04159126014769,null,10,34.130498638110296,40.716949463115029,49.130640449349286,57.573642107854539,61.123995517612983,60.701791836412639,59.016860616830343,56.905164678924855,51.954064465377563,45.326184070335216,37.566870997040184,33.04159126014769]
[null,11,{"$f":"DEGREES(C98)","v":108.37068106959256},109.89788330261443,108.6583333333333,106.14373901256789,104.9432104815792,105.68003318692836,107.1350716066959,106.98525858570096,104.90833333333335,102.70466413740597,102.52381337636953,104.99686600055793,null,11,{"$f":"DEGREES(Q98)","v":132.79871557082069},123.535247886498,113.32244793982535,101.81155981633054,93.532542603230439,90.275152510860423,93.059417694439432,101.50667666353853,113.81602048287021,124.6710945086412,133.75387955892683,136.8301172934793,null,null,null,11,{"$f":"IF(DO70<0,0,IF(0>C70,0,IF(50>C70,(( -0.000009*C70^2 + 0.0004*C70 + 0.7918)*Radiation!C14),IF(90>C70,((-0.0006*C70^2 + 0.0699*C70 - 1.2225)*Radiation!C14),0))))","v":0},{"$f":"IF(DP70<0,0,IF(0>D70,0,IF(50>D70,(( -0.000009*D70^2 + 0.0004*D70 + 0.7918)*Radiation!D14),IF(90>D70,((-0.0006*D70^2 + 0.0699*D70 - 1.2225)*Radiation!D14),0))))","v":0},{"$f":"IF(DQ70<0,0,IF(0>E70,0,IF(50>E70,(( -0.000009*E70^2 + 0.0004*E70 + 0.7918)*Radiation!E14),IF(90>E70,((-0.0006*E70^2 + 0.0699*E70 - 1.2225)*Radiation!E14),0))))","v":0},{"$f":"IF(DR70<0,0,IF(0>F70,0,IF(50>F70,(( -0.000009*F70^2 + 0.0004*F70 + 0.7918)*Radiation!F14),IF(90>F70,((-0.0006*F70^2 + 0.0699*F70 - 1.2225)*Radiation!F14),0))))","v":0},{"$f":"IF(DS70<0,0,IF(0>G70,0,IF(50>G70,(( -0.000009*G70^2 + 0.0004*G70 + 0.7918)*Radiation!G14),IF(90>G70,((-0.0006*G70^2 + 0.0699*G70 - 1.2225)*Radiation!G14),0))))","v":0},{"$f":"IF(DT70<0,0,IF(0>H70,0,IF(50>H70,(( -0.000009*H70^2 + 0.0004*H70 + 0.7918)*Radiation!H14),IF(90>H70,((-0.0006*H70^2 + 0.0699*H70 - 1.2225)*Radiation!H14),0))))","v":0},{"$f":"IF(DU70<0,0,IF(0>I70,0,IF(50>I70,(( -0.000009*I70^2 + 0.0004*I70 + 0.7918)*Radiation!I14),IF(90>I70,((-0.0006*I70^2 + 0.0699*I70 - 1.2225)*Radiation!I14),0))))","v":0},{"$f":"IF(DV70<0,0,IF(0>J70,0,IF(50>J70,(( -0.000009*J70^2 + 0.0004*J70 + 0.7918)*Radiation!J14),IF(90>J70,((-0.0006*J70^2 + 0.0699*J70 - 1.2225)*Radiation!J14),0))))","v":0},{"$f":"IF(DW70<0,0,IF(0>K70,0,IF(50>K70,(( -0.000009*K70^2 + 0.0004*K70 + 0.7918)*Radiation!K14),IF(90>K70,((-0.0006*K70^2 + 0.0699*K70 - 1.2225)*Radiation!K14),0))))","v":0},{"$f":"IF(DX70<0,0,IF(0>L70,0,IF(50>L70,(( -0.000009*L70^2 + 0.0004*L70 + 0.7918)*Radiation!L14),IF(90>L70,((-0.0006*L70^2 + 0.0699*L70 - 1.2225)*Radiation!L14),0))))","v":0},{"$f":"IF(DY70<0,0,IF(0>M70,0,IF(50>M70,(( -0.000009*M70^2 + 0.0004*M70 + 0.7918)*Radiation!M14),IF(90>M70,((-0.0006*M70^2 + 0.0699*M70 - 1.2225)*Radiation!M14),0))))","v":0},{"$f":"IF(DZ70<0,0,IF(0>N70,0,IF(50>N70,(( -0.000009*N70^2 + 0.0004*N70 + 0.7918)*Radiation!N14),IF(90>N70,((-0.0006*N70^2 + 0.0699*N70 - 1.2225)*Radiation!N14),0))))","v":0},null,11,{"$f":"IF(EC70<0,0,IF(0>Q70,0,IF(50>Q70,(( -0.000009*Q70^2 + 0.0004*Q70 + 0.7918)*Radiation!C14),IF(90>Q70,((-0.0006*Q70^2 + 0.0699*Q70 - 1.2225)*Radiation!C14),0))))","v":0},{"$f":"IF(ED70<0,0,IF(0>R70,0,IF(50>R70,(( -0.000009*R70^2 + 0.0004*R70 + 0.7918)*Radiation!D14),IF(90>R70,((-0.0006*R70^2 + 0.0699*R70 - 1.2225)*Radiation!D14),0))))","v":0},{"$f":"IF(EE70<0,0,IF(0>S70,0,IF(50>S70,(( -0.000009*S70^2 + 0.0004*S70 + 0.7918)*Radiation!E14),IF(90>S70,((-0.0006*S70^2 + 0.0699*S70 - 1.2225)*Radiation!E14),0))))","v":0},{"$f":"IF(EF70<0,0,IF(0>T70,0,IF(50>T70,(( -0.000009*T70^2 + 0.0004*T70 + 0.7918)*Radiation!F14),IF(90>T70,((-0.0006*T70^2 + 0.0699*T70 - 1.2225)*Radiation!F14),0))))","v":0},{"$f":"IF(EG70<0,0,IF(0>U70,0,IF(50>U70,(( -0.000009*U70^2 + 0.0004*U70 + 0.7918)*Radiation!G14),IF(90>U70,((-0.0006*U70^2 + 0.0699*U70 - 1.2225)*Radiation!G14),0))))","v":0},{"$f":"IF(EH70<0,0,IF(0>V70,0,IF(50>V70,(( -0.000009*V70^2 + 0.0004*V70 + 0.7918)*Radiation!H14),IF(90>V70,((-0.0006*V70^2 + 0.0699*V70 - 1.2225)*Radiation!H14),0))))","v":0},{"$f":"IF(EI70<0,0,IF(0>W70,0,IF(50>W70,(( -0.000009*W70^2 + 0.0004*W70 + 0.7918)*Radiation!I14),IF(90>W70,((-0.0006*W70^2 + 0.0699*W70 - 1.2225)*Radiation!I14),0))))","v":0},{"$f":"IF(EJ70<0,0,IF(0>X70,0,IF(50>X70,(( -0.000009*X70^2 + 0.0004*X70 + 0.7918)*Radiation!J14),IF(90>X70,((-0.0006*X70^2 + 0.0699*X70 - 1.2225)*Radiation!J14),0))))","v":0},{"$f":"IF(EK70<0,0,IF(0>Y70,0,IF(50>Y70,(( -0.000009*Y70^2 + 0.0004*Y70 + 0.7918)*Radiation!K14),IF(90>Y70,((-0.0006*Y70^2 + 0.0699*Y70 - 1.2225)*Radiation!K14),0))))","v":0},{"$f":"IF(EL70<0,0,IF(0>Z70,0,IF(50>Z70,(( -0.000009*Z70^2 + 0.0004*Z70 + 0.7918)*Radiation!L14),IF(90>Z70,((-0.0006*Z70^2 + 0.0699*Z70 - 1.2225)*Radiation!L14),0))))","v":0},{"$f":"IF(EM70<0,0,IF(0>AA70,0,IF(50>AA70,(( -0.000009*AA70^2 + 0.0004*AA70 + 0.7918)*Radiation!M14),IF(90>AA70,((-0.0006*AA70^2 + 0.0699*AA70 - 1.2225)*Radiation!M14),0))))","v":0},{"$f":"IF(EN70<0,0,IF(0>AB70,0,IF(50>AB70,(( -0.000009*AB70^2 + 0.0004*AB70 + 0.7918)*Radiation!N14),IF(90>AB70,((-0.0006*AB70^2 + 0.0699*AB70 - 1.2225)*Radiation!N14),0))))","v":0},null,null,11,{"$f":"AG70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU42","v":0},{"$f":"AH70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV42","v":0},{"$f":"AI70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW42","v":0},{"$f":"AJ70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX42","v":0},{"$f":"AK70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY42","v":0},{"$f":"AL70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ42","v":0},{"$f":"AM70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA42","v":0},{"$f":"AN70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB42","v":0},{"$f":"AO70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC42","v":0},{"$f":"AP70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD42","v":0},{"$f":"AQ70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE42","v":0},{"$f":"AR70*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF42","v":0},null,11,{"$f":"AU70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI42","v":0},{"$f":"AV70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ42","v":0},{"$f":"AW70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK42","v":0},{"$f":"AX70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL42","v":0},{"$f":"AY70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM42","v":0},{"$f":"AZ70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN42","v":0},{"$f":"BA70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO42","v":0},{"$f":"BB70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP42","v":0},{"$f":"BC70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ42","v":0},{"$f":"BD70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR42","v":0},{"$f":"BE70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS42","v":0},{"$f":"BF70*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT42","v":0},null,11,0,0,0,0,0,0,0,0,0,0,0,0,null,11,0,0,0,0,0,0,0,0,0,0,0,0,null,null,11,41.499338482119107,49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983,null,11,41.499338482119107,49.543356395157261,59.402009530792824,69.801829865076741,74.625870049112294,74.317427946135254,72.577202871970812,69.283885987295108,61.393251168859464,52.417946997507137,43.550952586854685,39.297011346471983]
[null,12,{"$f":"DEGREES(C99)","v":94.309120207828713},95.168355397290782,93.658333333333175,91.475910468662789,90.898805184195908,91.957064778954177,93.122024366419723,92.330353831741036,90.091666666664693,92.030717925501506,91.56712126505532,91.269061121613845,null,12,{"$f":"DEGREES(Q99)","v":134.49898061492814},125.17874112603188,114.64631138922823,102.7916758170952,94.396849779564789,91.234772897284785,94.161957814102152,102.57925063945783,114.6999662728682,125.38122908371821,134.58662580985228,138.14040610236691,null,null,null,12,{"$f":"IF(DO71<0,0,IF(0>C71,0,IF(50>C71,(( -0.000009*C71^2 + 0.0004*C71 + 0.7918)*Radiation!C15),IF(90>C71,((-0.0006*C71^2 + 0.0699*C71 - 1.2225)*Radiation!C15),0))))","v":0},{"$f":"IF(DP71<0,0,IF(0>D71,0,IF(50>D71,(( -0.000009*D71^2 + 0.0004*D71 + 0.7918)*Radiation!D15),IF(90>D71,((-0.0006*D71^2 + 0.0699*D71 - 1.2225)*Radiation!D15),0))))","v":0},{"$f":"IF(DQ71<0,0,IF(0>E71,0,IF(50>E71,(( -0.000009*E71^2 + 0.0004*E71 + 0.7918)*Radiation!E15),IF(90>E71,((-0.0006*E71^2 + 0.0699*E71 - 1.2225)*Radiation!E15),0))))","v":0},{"$f":"IF(DR71<0,0,IF(0>F71,0,IF(50>F71,(( -0.000009*F71^2 + 0.0004*F71 + 0.7918)*Radiation!F15),IF(90>F71,((-0.0006*F71^2 + 0.0699*F71 - 1.2225)*Radiation!F15),0))))","v":0},{"$f":"IF(DS71<0,0,IF(0>G71,0,IF(50>G71,(( -0.000009*G71^2 + 0.0004*G71 + 0.7918)*Radiation!G15),IF(90>G71,((-0.0006*G71^2 + 0.0699*G71 - 1.2225)*Radiation!G15),0))))","v":0},{"$f":"IF(DT71<0,0,IF(0>H71,0,IF(50>H71,(( -0.000009*H71^2 + 0.0004*H71 + 0.7918)*Radiation!H15),IF(90>H71,((-0.0006*H71^2 + 0.0699*H71 - 1.2225)*Radiation!H15),0))))","v":0},{"$f":"IF(DU71<0,0,IF(0>I71,0,IF(50>I71,(( -0.000009*I71^2 + 0.0004*I71 + 0.7918)*Radiation!I15),IF(90>I71,((-0.0006*I71^2 + 0.0699*I71 - 1.2225)*Radiation!I15),0))))","v":0},{"$f":"IF(DV71<0,0,IF(0>J71,0,IF(50>J71,(( -0.000009*J71^2 + 0.0004*J71 + 0.7918)*Radiation!J15),IF(90>J71,((-0.0006*J71^2 + 0.0699*J71 - 1.2225)*Radiation!J15),0))))","v":0},{"$f":"IF(DW71<0,0,IF(0>K71,0,IF(50>K71,(( -0.000009*K71^2 + 0.0004*K71 + 0.7918)*Radiation!K15),IF(90>K71,((-0.0006*K71^2 + 0.0699*K71 - 1.2225)*Radiation!K15),0))))","v":0},{"$f":"IF(DX71<0,0,IF(0>L71,0,IF(50>L71,(( -0.000009*L71^2 + 0.0004*L71 + 0.7918)*Radiation!L15),IF(90>L71,((-0.0006*L71^2 + 0.0699*L71 - 1.2225)*Radiation!L15),0))))","v":0},{"$f":"IF(DY71<0,0,IF(0>M71,0,IF(50>M71,(( -0.000009*M71^2 + 0.0004*M71 + 0.7918)*Radiation!M15),IF(90>M71,((-0.0006*M71^2 + 0.0699*M71 - 1.2225)*Radiation!M15),0))))","v":0},{"$f":"IF(DZ71<0,0,IF(0>N71,0,IF(50>N71,(( -0.000009*N71^2 + 0.0004*N71 + 0.7918)*Radiation!N15),IF(90>N71,((-0.0006*N71^2 + 0.0699*N71 - 1.2225)*Radiation!N15),0))))","v":0},null,12,{"$f":"IF(EC71<0,0,IF(0>Q71,0,IF(50>Q71,(( -0.000009*Q71^2 + 0.0004*Q71 + 0.7918)*Radiation!C15),IF(90>Q71,((-0.0006*Q71^2 + 0.0699*Q71 - 1.2225)*Radiation!C15),0))))","v":0},{"$f":"IF(ED71<0,0,IF(0>R71,0,IF(50>R71,(( -0.000009*R71^2 + 0.0004*R71 + 0.7918)*Radiation!D15),IF(90>R71,((-0.0006*R71^2 + 0.0699*R71 - 1.2225)*Radiation!D15),0))))","v":0},{"$f":"IF(EE71<0,0,IF(0>S71,0,IF(50>S71,(( -0.000009*S71^2 + 0.0004*S71 + 0.7918)*Radiation!E15),IF(90>S71,((-0.0006*S71^2 + 0.0699*S71 - 1.2225)*Radiation!E15),0))))","v":0},{"$f":"IF(EF71<0,0,IF(0>T71,0,IF(50>T71,(( -0.000009*T71^2 + 0.0004*T71 + 0.7918)*Radiation!F15),IF(90>T71,((-0.0006*T71^2 + 0.0699*T71 - 1.2225)*Radiation!F15),0))))","v":0},{"$f":"IF(EG71<0,0,IF(0>U71,0,IF(50>U71,(( -0.000009*U71^2 + 0.0004*U71 + 0.7918)*Radiation!G15),IF(90>U71,((-0.0006*U71^2 + 0.0699*U71 - 1.2225)*Radiation!G15),0))))","v":0},{"$f":"IF(EH71<0,0,IF(0>V71,0,IF(50>V71,(( -0.000009*V71^2 + 0.0004*V71 + 0.7918)*Radiation!H15),IF(90>V71,((-0.0006*V71^2 + 0.0699*V71 - 1.2225)*Radiation!H15),0))))","v":0},{"$f":"IF(EI71<0,0,IF(0>W71,0,IF(50>W71,(( -0.000009*W71^2 + 0.0004*W71 + 0.7918)*Radiation!I15),IF(90>W71,((-0.0006*W71^2 + 0.0699*W71 - 1.2225)*Radiation!I15),0))))","v":0},{"$f":"IF(EJ71<0,0,IF(0>X71,0,IF(50>X71,(( -0.000009*X71^2 + 0.0004*X71 + 0.7918)*Radiation!J15),IF(90>X71,((-0.0006*X71^2 + 0.0699*X71 - 1.2225)*Radiation!J15),0))))","v":0},{"$f":"IF(EK71<0,0,IF(0>Y71,0,IF(50>Y71,(( -0.000009*Y71^2 + 0.0004*Y71 + 0.7918)*Radiation!K15),IF(90>Y71,((-0.0006*Y71^2 + 0.0699*Y71 - 1.2225)*Radiation!K15),0))))","v":0},{"$f":"IF(EL71<0,0,IF(0>Z71,0,IF(50>Z71,(( -0.000009*Z71^2 + 0.0004*Z71 + 0.7918)*Radiation!L15),IF(90>Z71,((-0.0006*Z71^2 + 0.0699*Z71 - 1.2225)*Radiation!L15),0))))","v":0},{"$f":"IF(EM71<0,0,IF(0>AA71,0,IF(50>AA71,(( -0.000009*AA71^2 + 0.0004*AA71 + 0.7918)*Radiation!M15),IF(90>AA71,((-0.0006*AA71^2 + 0.0699*AA71 - 1.2225)*Radiation!M15),0))))","v":0},{"$f":"IF(EN71<0,0,IF(0>AB71,0,IF(50>AB71,(( -0.000009*AB71^2 + 0.0004*AB71 + 0.7918)*Radiation!N15),IF(90>AB71,((-0.0006*AB71^2 + 0.0699*AB71 - 1.2225)*Radiation!N15),0))))","v":0},null,null,12,{"$f":"AG71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU43","v":0},{"$f":"AH71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV43","v":0},{"$f":"AI71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW43","v":0},{"$f":"AJ71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX43","v":0},{"$f":"AK71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY43","v":0},{"$f":"AL71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ43","v":0},{"$f":"AM71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA43","v":0},{"$f":"AN71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB43","v":0},{"$f":"AO71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC43","v":0},{"$f":"AP71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD43","v":0},{"$f":"AQ71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE43","v":0},{"$f":"AR71*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF43","v":0},null,12,{"$f":"AU71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI43","v":0},{"$f":"AV71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ43","v":0},{"$f":"AW71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK43","v":0},{"$f":"AX71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL43","v":0},{"$f":"AY71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM43","v":0},{"$f":"AZ71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN43","v":0},{"$f":"BA71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO43","v":0},{"$f":"BB71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP43","v":0},{"$f":"BC71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ43","v":0},{"$f":"BD71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR43","v":0},{"$f":"BE71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS43","v":0},{"$f":"BF71*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT43","v":0},null,12,0,0,0,0,0,0,0,0,0,0,0,0,null,12,0,0,0,0,0,0,0,0,0,0,0,0,null,null,12,45.177523796213436,54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598,null,12,45.177523796213436,54.329068465075267,65.047371814417531,77.120581963762746,85.511869047796154,87.685706703910299,84.793912346691229,77.199736149013034,65.299840573859427,54.542607240756659,45.370517861678998,41.831318434437598]
[null,13,{"$f":"DEGREES(C100)","v":80.211656093594939},80.42615014541957,78.658333333333346,76.80358236511384,76.846679965820869,78.211996998901242,79.081553542746079,77.668097760060789,74.908333333333303,73.238925529430134,74.354912487115001,77.526939258767612,null,13,{"$f":"DEGREES(Q100)","v":134.0812203568851},124.88527570127464,114.18642562804527,102.13787092633211,93.727340610309,90.698407209161374,93.735581990256804,102.02141588046763,113.79434888072156,124.13881879807526,133.28647063510959,137.23282032855676,null,null,null,13,{"$f":"IF(DO72<0,0,IF(0>C72,0,IF(50>C72,(( -0.000009*C72^2 + 0.0004*C72 + 0.7918)*Radiation!C16),IF(90>C72,((-0.0006*C72^2 + 0.0699*C72 - 1.2225)*Radiation!C16),0))))","v":108.78964141214273},{"$f":"IF(DP72<0,0,IF(0>D72,0,IF(50>D72,(( -0.000009*D72^2 + 0.0004*D72 + 0.7918)*Radiation!D16),IF(90>D72,((-0.0006*D72^2 + 0.0699*D72 - 1.2225)*Radiation!D16),0))))","v":123.3820782301095},{"$f":"IF(DQ72<0,0,IF(0>E72,0,IF(50>E72,(( -0.000009*E72^2 + 0.0004*E72 + 0.7918)*Radiation!E16),IF(90>E72,((-0.0006*E72^2 + 0.0699*E72 - 1.2225)*Radiation!E16),0))))","v":149.85284479231981},{"$f":"IF(DR72<0,0,IF(0>F72,0,IF(50>F72,(( -0.000009*F72^2 + 0.0004*F72 + 0.7918)*Radiation!F16),IF(90>F72,((-0.0006*F72^2 + 0.0699*F72 - 1.2225)*Radiation!F16),0))))","v":163.69286966731227},{"$f":"IF(DS72<0,0,IF(0>G72,0,IF(50>G72,(( -0.000009*G72^2 + 0.0004*G72 + 0.7918)*Radiation!G16),IF(90>G72,((-0.0006*G72^2 + 0.0699*G72 - 1.2225)*Radiation!G16),0))))","v":183.59886595030977},{"$f":"IF(DT72<0,0,IF(0>H72,0,IF(50>H72,(( -0.000009*H72^2 + 0.0004*H72 + 0.7918)*Radiation!H16),IF(90>H72,((-0.0006*H72^2 + 0.0699*H72 - 1.2225)*Radiation!H16),0))))","v":188.04321216475657},{"$f":"IF(DU72<0,0,IF(0>I72,0,IF(50>I72,(( -0.000009*I72^2 + 0.0004*I72 + 0.7918)*Radiation!I16),IF(90>I72,((-0.0006*I72^2 + 0.0699*I72 - 1.2225)*Radiation!I16),0))))","v":180.19732063725087},{"$f":"IF(DV72<0,0,IF(0>J72,0,IF(50>J72,(( -0.000009*J72^2 + 0.0004*J72 + 0.7918)*Radiation!J16),IF(90>J72,((-0.0006*J72^2 + 0.0699*J72 - 1.2225)*Radiation!J16),0))))","v":187.22652073317232},{"$f":"IF(DW72<0,0,IF(0>K72,0,IF(50>K72,(( -0.000009*K72^2 + 0.0004*K72 + 0.7918)*Radiation!K16),IF(90>K72,((-0.0006*K72^2 + 0.0699*K72 - 1.2225)*Radiation!K16),0))))","v":196.02450645125884},{"$f":"IF(DX72<0,0,IF(0>L72,0,IF(50>L72,(( -0.000009*L72^2 + 0.0004*L72 + 0.7918)*Radiation!L16),IF(90>L72,((-0.0006*L72^2 + 0.0699*L72 - 1.2225)*Radiation!L16),0))))","v":185.41205431263384},{"$f":"IF(DY72<0,0,IF(0>M72,0,IF(50>M72,(( -0.000009*M72^2 + 0.0004*M72 + 0.7918)*Radiation!M16),IF(90>M72,((-0.0006*M72^2 + 0.0699*M72 - 1.2225)*Radiation!M16),0))))","v":150.95053912600531},{"$f":"IF(DZ72<0,0,IF(0>N72,0,IF(50>N72,(( -0.000009*N72^2 + 0.0004*N72 + 0.7918)*Radiation!N16),IF(90>N72,((-0.0006*N72^2 + 0.0699*N72 - 1.2225)*Radiation!N16),0))))","v":106.86193892477711},null,13,{"$f":"IF(EC72<0,0,IF(0>Q72,0,IF(50>Q72,(( -0.000009*Q72^2 + 0.0004*Q72 + 0.7918)*Radiation!C16),IF(90>Q72,((-0.0006*Q72^2 + 0.0699*Q72 - 1.2225)*Radiation!C16),0))))","v":0},{"$f":"IF(ED72<0,0,IF(0>R72,0,IF(50>R72,(( -0.000009*R72^2 + 0.0004*R72 + 0.7918)*Radiation!D16),IF(90>R72,((-0.0006*R72^2 + 0.0699*R72 - 1.2225)*Radiation!D16),0))))","v":0},{"$f":"IF(EE72<0,0,IF(0>S72,0,IF(50>S72,(( -0.000009*S72^2 + 0.0004*S72 + 0.7918)*Radiation!E16),IF(90>S72,((-0.0006*S72^2 + 0.0699*S72 - 1.2225)*Radiation!E16),0))))","v":0},{"$f":"IF(EF72<0,0,IF(0>T72,0,IF(50>T72,(( -0.000009*T72^2 + 0.0004*T72 + 0.7918)*Radiation!F16),IF(90>T72,((-0.0006*T72^2 + 0.0699*T72 - 1.2225)*Radiation!F16),0))))","v":0},{"$f":"IF(EG72<0,0,IF(0>U72,0,IF(50>U72,(( -0.000009*U72^2 + 0.0004*U72 + 0.7918)*Radiation!G16),IF(90>U72,((-0.0006*U72^2 + 0.0699*U72 - 1.2225)*Radiation!G16),0))))","v":0},{"$f":"IF(EH72<0,0,IF(0>V72,0,IF(50>V72,(( -0.000009*V72^2 + 0.0004*V72 + 0.7918)*Radiation!H16),IF(90>V72,((-0.0006*V72^2 + 0.0699*V72 - 1.2225)*Radiation!H16),0))))","v":0},{"$f":"IF(EI72<0,0,IF(0>W72,0,IF(50>W72,(( -0.000009*W72^2 + 0.0004*W72 + 0.7918)*Radiation!I16),IF(90>W72,((-0.0006*W72^2 + 0.0699*W72 - 1.2225)*Radiation!I16),0))))","v":0},{"$f":"IF(EJ72<0,0,IF(0>X72,0,IF(50>X72,(( -0.000009*X72^2 + 0.0004*X72 + 0.7918)*Radiation!J16),IF(90>X72,((-0.0006*X72^2 + 0.0699*X72 - 1.2225)*Radiation!J16),0))))","v":0},{"$f":"IF(EK72<0,0,IF(0>Y72,0,IF(50>Y72,(( -0.000009*Y72^2 + 0.0004*Y72 + 0.7918)*Radiation!K16),IF(90>Y72,((-0.0006*Y72^2 + 0.0699*Y72 - 1.2225)*Radiation!K16),0))))","v":0},{"$f":"IF(EL72<0,0,IF(0>Z72,0,IF(50>Z72,(( -0.000009*Z72^2 + 0.0004*Z72 + 0.7918)*Radiation!L16),IF(90>Z72,((-0.0006*Z72^2 + 0.0699*Z72 - 1.2225)*Radiation!L16),0))))","v":0},{"$f":"IF(EM72<0,0,IF(0>AA72,0,IF(50>AA72,(( -0.000009*AA72^2 + 0.0004*AA72 + 0.7918)*Radiation!M16),IF(90>AA72,((-0.0006*AA72^2 + 0.0699*AA72 - 1.2225)*Radiation!M16),0))))","v":0},{"$f":"IF(EN72<0,0,IF(0>AB72,0,IF(50>AB72,(( -0.000009*AB72^2 + 0.0004*AB72 + 0.7918)*Radiation!N16),IF(90>AB72,((-0.0006*AB72^2 + 0.0699*AB72 - 1.2225)*Radiation!N16),0))))","v":0},null,null,13,{"$f":"AG72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU44","v":0},{"$f":"AH72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV44","v":0},{"$f":"AI72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW44","v":0},{"$f":"AJ72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX44","v":0},{"$f":"AK72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY44","v":0},{"$f":"AL72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ44","v":0},{"$f":"AM72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA44","v":0},{"$f":"AN72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB44","v":0},{"$f":"AO72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC44","v":0},{"$f":"AP72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD44","v":0},{"$f":"AQ72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE44","v":0},{"$f":"AR72*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF44","v":0},null,13,{"$f":"AU72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI44","v":0},{"$f":"AV72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ44","v":0},{"$f":"AW72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK44","v":0},{"$f":"AX72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL44","v":0},{"$f":"AY72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM44","v":0},{"$f":"AZ72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN44","v":0},{"$f":"BA72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO44","v":0},{"$f":"BB72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP44","v":0},{"$f":"BC72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ44","v":0},{"$f":"BD72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR44","v":0},{"$f":"BE72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS44","v":0},{"$f":"BF72*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT44","v":0},null,13,0,0,0,0,0,0,0,0,0,0,0,0,null,13,0,0,0,0,0,0,0,0,0,0,0,0,null,null,13,44.262516808487675,53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703,null,13,44.262516808487675,53.442649547558034,62.96975399076122,71.918657174425832,76.310429689037434,78.190731192893594,78.445286814888803,72.64341275146262,61.303344417053367,50.879096974273239,42.542599664242438,40.072467904514703]
[null,14,{"$f":"DEGREES(C101)","v":66.198473357653043},65.708092900017775,63.65833333333331,62.174579515584774,62.916148077749746,64.607895157234324,65.141563764751197,63.047277265987518,59.908333333333324,58.555346461938157,60.420598214725764,63.93504051628959,null,14,{"$f":"DEGREES(Q101)","v":131.6150761282353},122.69410222819029,111.9920179630723,99.905682520372707,91.572543070498924,88.702725497668141,91.811165520975209,99.880442573871704,111.19534171120367,121.1068756452287,130.06486882836012,134.27195529891088,null,null,null,14,{"$f":"IF(DO73<0,0,IF(0>C73,0,IF(50>C73,(( -0.000009*C73^2 + 0.0004*C73 + 0.7918)*Radiation!C17),IF(90>C73,((-0.0006*C73^2 + 0.0699*C73 - 1.2225)*Radiation!C17),0))))","v":146.0113693951335},{"$f":"IF(DP73<0,0,IF(0>D73,0,IF(50>D73,(( -0.000009*D73^2 + 0.0004*D73 + 0.7918)*Radiation!D17),IF(90>D73,((-0.0006*D73^2 + 0.0699*D73 - 1.2225)*Radiation!D17),0))))","v":175.05112788645263},{"$f":"IF(DQ73<0,0,IF(0>E73,0,IF(50>E73,(( -0.000009*E73^2 + 0.0004*E73 + 0.7918)*Radiation!E17),IF(90>E73,((-0.0006*E73^2 + 0.0699*E73 - 1.2225)*Radiation!E17),0))))","v":192.72930876288612},{"$f":"IF(DR73<0,0,IF(0>F73,0,IF(50>F73,(( -0.000009*F73^2 + 0.0004*F73 + 0.7918)*Radiation!F17),IF(90>F73,((-0.0006*F73^2 + 0.0699*F73 - 1.2225)*Radiation!F17),0))))","v":196.78073292943125},{"$f":"IF(DS73<0,0,IF(0>G73,0,IF(50>G73,(( -0.000009*G73^2 + 0.0004*G73 + 0.7918)*Radiation!G17),IF(90>G73,((-0.0006*G73^2 + 0.0699*G73 - 1.2225)*Radiation!G17),0))))","v":224.51178891417277},{"$f":"IF(DT73<0,0,IF(0>H73,0,IF(50>H73,(( -0.000009*H73^2 + 0.0004*H73 + 0.7918)*Radiation!H17),IF(90>H73,((-0.0006*H73^2 + 0.0699*H73 - 1.2225)*Radiation!H17),0))))","v":237.63152128531954},{"$f":"IF(DU73<0,0,IF(0>I73,0,IF(50>I73,(( -0.000009*I73^2 + 0.0004*I73 + 0.7918)*Radiation!I17),IF(90>I73,((-0.0006*I73^2 + 0.0699*I73 - 1.2225)*Radiation!I17),0))))","v":234.61234543908725},{"$f":"IF(DV73<0,0,IF(0>J73,0,IF(50>J73,(( -0.000009*J73^2 + 0.0004*J73 + 0.7918)*Radiation!J17),IF(90>J73,((-0.0006*J73^2 + 0.0699*J73 - 1.2225)*Radiation!J17),0))))","v":232.41329523049563},{"$f":"IF(DW73<0,0,IF(0>K73,0,IF(50>K73,(( -0.000009*K73^2 + 0.0004*K73 + 0.7918)*Radiation!K17),IF(90>K73,((-0.0006*K73^2 + 0.0699*K73 - 1.2225)*Radiation!K17),0))))","v":220.76663512726191},{"$f":"IF(DX73<0,0,IF(0>L73,0,IF(50>L73,(( -0.000009*L73^2 + 0.0004*L73 + 0.7918)*Radiation!L17),IF(90>L73,((-0.0006*L73^2 + 0.0699*L73 - 1.2225)*Radiation!L17),0))))","v":195.1614871193901},{"$f":"IF(DY73<0,0,IF(0>M73,0,IF(50>M73,(( -0.000009*M73^2 + 0.0004*M73 + 0.7918)*Radiation!M17),IF(90>M73,((-0.0006*M73^2 + 0.0699*M73 - 1.2225)*Radiation!M17),0))))","v":159.04010872897285},{"$f":"IF(DZ73<0,0,IF(0>N73,0,IF(50>N73,(( -0.000009*N73^2 + 0.0004*N73 + 0.7918)*Radiation!N17),IF(90>N73,((-0.0006*N73^2 + 0.0699*N73 - 1.2225)*Radiation!N17),0))))","v":128.60830358062771},null,14,{"$f":"IF(EC73<0,0,IF(0>Q73,0,IF(50>Q73,(( -0.000009*Q73^2 + 0.0004*Q73 + 0.7918)*Radiation!C17),IF(90>Q73,((-0.0006*Q73^2 + 0.0699*Q73 - 1.2225)*Radiation!C17),0))))","v":0},{"$f":"IF(ED73<0,0,IF(0>R73,0,IF(50>R73,(( -0.000009*R73^2 + 0.0004*R73 + 0.7918)*Radiation!D17),IF(90>R73,((-0.0006*R73^2 + 0.0699*R73 - 1.2225)*Radiation!D17),0))))","v":0},{"$f":"IF(EE73<0,0,IF(0>S73,0,IF(50>S73,(( -0.000009*S73^2 + 0.0004*S73 + 0.7918)*Radiation!E17),IF(90>S73,((-0.0006*S73^2 + 0.0699*S73 - 1.2225)*Radiation!E17),0))))","v":0},{"$f":"IF(EF73<0,0,IF(0>T73,0,IF(50>T73,(( -0.000009*T73^2 + 0.0004*T73 + 0.7918)*Radiation!F17),IF(90>T73,((-0.0006*T73^2 + 0.0699*T73 - 1.2225)*Radiation!F17),0))))","v":0},{"$f":"IF(EG73<0,0,IF(0>U73,0,IF(50>U73,(( -0.000009*U73^2 + 0.0004*U73 + 0.7918)*Radiation!G17),IF(90>U73,((-0.0006*U73^2 + 0.0699*U73 - 1.2225)*Radiation!G17),0))))","v":0},{"$f":"IF(EH73<0,0,IF(0>V73,0,IF(50>V73,(( -0.000009*V73^2 + 0.0004*V73 + 0.7918)*Radiation!H17),IF(90>V73,((-0.0006*V73^2 + 0.0699*V73 - 1.2225)*Radiation!H17),0))))","v":77.370028697902143},{"$f":"IF(EI73<0,0,IF(0>W73,0,IF(50>W73,(( -0.000009*W73^2 + 0.0004*W73 + 0.7918)*Radiation!I17),IF(90>W73,((-0.0006*W73^2 + 0.0699*W73 - 1.2225)*Radiation!I17),0))))","v":0},{"$f":"IF(EJ73<0,0,IF(0>X73,0,IF(50>X73,(( -0.000009*X73^2 + 0.0004*X73 + 0.7918)*Radiation!J17),IF(90>X73,((-0.0006*X73^2 + 0.0699*X73 - 1.2225)*Radiation!J17),0))))","v":0},{"$f":"IF(EK73<0,0,IF(0>Y73,0,IF(50>Y73,(( -0.000009*Y73^2 + 0.0004*Y73 + 0.7918)*Radiation!K17),IF(90>Y73,((-0.0006*Y73^2 + 0.0699*Y73 - 1.2225)*Radiation!K17),0))))","v":0},{"$f":"IF(EL73<0,0,IF(0>Z73,0,IF(50>Z73,(( -0.000009*Z73^2 + 0.0004*Z73 + 0.7918)*Radiation!L17),IF(90>Z73,((-0.0006*Z73^2 + 0.0699*Z73 - 1.2225)*Radiation!L17),0))))","v":0},{"$f":"IF(EM73<0,0,IF(0>AA73,0,IF(50>AA73,(( -0.000009*AA73^2 + 0.0004*AA73 + 0.7918)*Radiation!M17),IF(90>AA73,((-0.0006*AA73^2 + 0.0699*AA73 - 1.2225)*Radiation!M17),0))))","v":0},{"$f":"IF(EN73<0,0,IF(0>AB73,0,IF(50>AB73,(( -0.000009*AB73^2 + 0.0004*AB73 + 0.7918)*Radiation!N17),IF(90>AB73,((-0.0006*AB73^2 + 0.0699*AB73 - 1.2225)*Radiation!N17),0))))","v":0},null,null,14,{"$f":"AG73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU45","v":0},{"$f":"AH73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV45","v":0},{"$f":"AI73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW45","v":0},{"$f":"AJ73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX45","v":0},{"$f":"AK73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY45","v":0},{"$f":"AL73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ45","v":0},{"$f":"AM73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA45","v":0},{"$f":"AN73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB45","v":0},{"$f":"AO73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC45","v":0},{"$f":"AP73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD45","v":686.52449229956528},{"$f":"AQ73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE45","v":739.63225428742817},{"$f":"AR73*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF45","v":205.63474171395885},null,14,{"$f":"AU73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI45","v":0},{"$f":"AV73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ45","v":0},{"$f":"AW73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK45","v":0},{"$f":"AX73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL45","v":0},{"$f":"AY73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM45","v":0},{"$f":"AZ73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN45","v":0},{"$f":"BA73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO45","v":0},{"$f":"BB73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP45","v":0},{"$f":"BC73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ45","v":0},{"$f":"BD73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR45","v":0},{"$f":"BE73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS45","v":0},{"$f":"BF73*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT45","v":0},null,14,0,0,0,0,0,0,0,0,0,0.59894762087049969,0.26376602957948858,8.3417589987308416E-2,null,14,0,0,0,0,0,0,0,0,0,0,0,0,null,null,14,39.001643714284292,47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348,null,14,39.001643714284292,47.236569251778789,54.505603493104616,60.167275430762508,62.862961225627508,64.570010808670432,65.066621957768987,61.010544197086858,51.819137025254037,42.759898297268641,35.791762146841563,34.427909280399348]
[null,15,{"$f":"DEGREES(C102)","v":52.437410650188276},51.066551624009087,48.658333333333317,47.665488828500571,49.30722076828539,51.38329095429625,51.486735653262436,48.543799917354953,44.908333333333317,43.99365171319036,46.847636168318587,50.73888771286056,null,15,{"$f":"DEGREES(Q102)","v":127.47272411791445},118.87829918447085,108.28403534265583,96.274888421415028,88.081758090445774,85.379002203294903,88.522904745914786,96.328944658820305,107.15774933833093,116.63848701551217,125.37128251021061,129.72304247504246,null,null,null,15,{"$f":"IF(DO74<0,0,IF(0>C74,0,IF(50>C74,(( -0.000009*C74^2 + 0.0004*C74 + 0.7918)*Radiation!C18),IF(90>C74,((-0.0006*C74^2 + 0.0699*C74 - 1.2225)*Radiation!C18),0))))","v":117.9069404671294},{"$f":"IF(DP74<0,0,IF(0>D74,0,IF(50>D74,(( -0.000009*D74^2 + 0.0004*D74 + 0.7918)*Radiation!D18),IF(90>D74,((-0.0006*D74^2 + 0.0699*D74 - 1.2225)*Radiation!D18),0))))","v":146.32719105083788},{"$f":"IF(DQ74<0,0,IF(0>E74,0,IF(50>E74,(( -0.000009*E74^2 + 0.0004*E74 + 0.7918)*Radiation!E18),IF(90>E74,((-0.0006*E74^2 + 0.0699*E74 - 1.2225)*Radiation!E18),0))))","v":159.2636192734021},{"$f":"IF(DR74<0,0,IF(0>F74,0,IF(50>F74,(( -0.000009*F74^2 + 0.0004*F74 + 0.7918)*Radiation!F18),IF(90>F74,((-0.0006*F74^2 + 0.0699*F74 - 1.2225)*Radiation!F18),0))))","v":158.60539647031985},{"$f":"IF(DS74<0,0,IF(0>G74,0,IF(50>G74,(( -0.000009*G74^2 + 0.0004*G74 + 0.7918)*Radiation!G18),IF(90>G74,((-0.0006*G74^2 + 0.0699*G74 - 1.2225)*Radiation!G18),0))))","v":185.23340622628365},{"$f":"IF(DT74<0,0,IF(0>H74,0,IF(50>H74,(( -0.000009*H74^2 + 0.0004*H74 + 0.7918)*Radiation!H18),IF(90>H74,((-0.0006*H74^2 + 0.0699*H74 - 1.2225)*Radiation!H18),0))))","v":198.83803705223022},{"$f":"IF(DU74<0,0,IF(0>I74,0,IF(50>I74,(( -0.000009*I74^2 + 0.0004*I74 + 0.7918)*Radiation!I18),IF(90>I74,((-0.0006*I74^2 + 0.0699*I74 - 1.2225)*Radiation!I18),0))))","v":196.06278419507984},{"$f":"IF(DV74<0,0,IF(0>J74,0,IF(50>J74,(( -0.000009*J74^2 + 0.0004*J74 + 0.7918)*Radiation!J18),IF(90>J74,((-0.0006*J74^2 + 0.0699*J74 - 1.2225)*Radiation!J18),0))))","v":189.32639161491019},{"$f":"IF(DW74<0,0,IF(0>K74,0,IF(50>K74,(( -0.000009*K74^2 + 0.0004*K74 + 0.7918)*Radiation!K18),IF(90>K74,((-0.0006*K74^2 + 0.0699*K74 - 1.2225)*Radiation!K18),0))))","v":172.89768737490922},{"$f":"IF(DX74<0,0,IF(0>L74,0,IF(50>L74,(( -0.000009*L74^2 + 0.0004*L74 + 0.7918)*Radiation!L18),IF(90>L74,((-0.0006*L74^2 + 0.0699*L74 - 1.2225)*Radiation!L18),0))))","v":146.61673612942835},{"$f":"IF(DY74<0,0,IF(0>M74,0,IF(50>M74,(( -0.000009*M74^2 + 0.0004*M74 + 0.7918)*Radiation!M18),IF(90>M74,((-0.0006*M74^2 + 0.0699*M74 - 1.2225)*Radiation!M18),0))))","v":112.80522340493121},{"$f":"IF(DZ74<0,0,IF(0>N74,0,IF(50>N74,(( -0.000009*N74^2 + 0.0004*N74 + 0.7918)*Radiation!N18),IF(90>N74,((-0.0006*N74^2 + 0.0699*N74 - 1.2225)*Radiation!N18),0))))","v":95.87340424022166},null,15,{"$f":"IF(EC74<0,0,IF(0>Q74,0,IF(50>Q74,(( -0.000009*Q74^2 + 0.0004*Q74 + 0.7918)*Radiation!C18),IF(90>Q74,((-0.0006*Q74^2 + 0.0699*Q74 - 1.2225)*Radiation!C18),0))))","v":0},{"$f":"IF(ED74<0,0,IF(0>R74,0,IF(50>R74,(( -0.000009*R74^2 + 0.0004*R74 + 0.7918)*Radiation!D18),IF(90>R74,((-0.0006*R74^2 + 0.0699*R74 - 1.2225)*Radiation!D18),0))))","v":0},{"$f":"IF(EE74<0,0,IF(0>S74,0,IF(50>S74,(( -0.000009*S74^2 + 0.0004*S74 + 0.7918)*Radiation!E18),IF(90>S74,((-0.0006*S74^2 + 0.0699*S74 - 1.2225)*Radiation!E18),0))))","v":0},{"$f":"IF(EF74<0,0,IF(0>T74,0,IF(50>T74,(( -0.000009*T74^2 + 0.0004*T74 + 0.7918)*Radiation!F18),IF(90>T74,((-0.0006*T74^2 + 0.0699*T74 - 1.2225)*Radiation!F18),0))))","v":0},{"$f":"IF(EG74<0,0,IF(0>U74,0,IF(50>U74,(( -0.000009*U74^2 + 0.0004*U74 + 0.7918)*Radiation!G18),IF(90>U74,((-0.0006*U74^2 + 0.0699*U74 - 1.2225)*Radiation!G18),0))))","v":65.536015704422255},{"$f":"IF(EH74<0,0,IF(0>V74,0,IF(50>V74,(( -0.000009*V74^2 + 0.0004*V74 + 0.7918)*Radiation!H18),IF(90>V74,((-0.0006*V74^2 + 0.0699*V74 - 1.2225)*Radiation!H18),0))))","v":94.156986890000383},{"$f":"IF(EI74<0,0,IF(0>W74,0,IF(50>W74,(( -0.000009*W74^2 + 0.0004*W74 + 0.7918)*Radiation!I18),IF(90>W74,((-0.0006*W74^2 + 0.0699*W74 - 1.2225)*Radiation!I18),0))))","v":65.729499051842012},{"$f":"IF(EJ74<0,0,IF(0>X74,0,IF(50>X74,(( -0.000009*X74^2 + 0.0004*X74 + 0.7918)*Radiation!J18),IF(90>X74,((-0.0006*X74^2 + 0.0699*X74 - 1.2225)*Radiation!J18),0))))","v":0},{"$f":"IF(EK74<0,0,IF(0>Y74,0,IF(50>Y74,(( -0.000009*Y74^2 + 0.0004*Y74 + 0.7918)*Radiation!K18),IF(90>Y74,((-0.0006*Y74^2 + 0.0699*Y74 - 1.2225)*Radiation!K18),0))))","v":0},{"$f":"IF(EL74<0,0,IF(0>Z74,0,IF(50>Z74,(( -0.000009*Z74^2 + 0.0004*Z74 + 0.7918)*Radiation!L18),IF(90>Z74,((-0.0006*Z74^2 + 0.0699*Z74 - 1.2225)*Radiation!L18),0))))","v":0},{"$f":"IF(EM74<0,0,IF(0>AA74,0,IF(50>AA74,(( -0.000009*AA74^2 + 0.0004*AA74 + 0.7918)*Radiation!M18),IF(90>AA74,((-0.0006*AA74^2 + 0.0699*AA74 - 1.2225)*Radiation!M18),0))))","v":0},{"$f":"IF(EN74<0,0,IF(0>AB74,0,IF(50>AB74,(( -0.000009*AB74^2 + 0.0004*AB74 + 0.7918)*Radiation!N18),IF(90>AB74,((-0.0006*AB74^2 + 0.0699*AB74 - 1.2225)*Radiation!N18),0))))","v":0},null,null,15,{"$f":"AG74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU46","v":1926.5716949534467},{"$f":"AH74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV46","v":2262.7778473297494},{"$f":"AI74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW46","v":2635.5703218185467},{"$f":"AJ74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX46","v":2739.6260864388364},{"$f":"AK74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY46","v":2639.208561173924},{"$f":"AL74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ46","v":1868.8769897456732},{"$f":"AM74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA46","v":1817.2287126262747},{"$f":"AN74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB46","v":2938.0781685139464},{"$f":"AO74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC46","v":3923.7505691865708},{"$f":"AP74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD46","v":3823.612360059843},{"$f":"AQ74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE46","v":2779.6028668421336},{"$f":"AR74*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF46","v":1919.6025015893795},null,15,{"$f":"AU74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI46","v":0},{"$f":"AV74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ46","v":0},{"$f":"AW74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK46","v":0},{"$f":"AX74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL46","v":0},{"$f":"AY74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM46","v":0},{"$f":"AZ74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN46","v":0},{"$f":"BA74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO46","v":0},{"$f":"BB74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP46","v":0},{"$f":"BC74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ46","v":0},{"$f":"BD74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR46","v":0},{"$f":"BE74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS46","v":0},{"$f":"BF74*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT46","v":0},null,15,0.57014029461573867,0.86127599718114978,1,1,1,1,1,1,1,0.92771380590744001,0.68242887791708595,0.56294774267755432,null,15,0,0,0,0,0,0,0,0,0,0,0,0,null,null,15,30.541133571003865,37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655,null,15,30.541133571003865,37.574701882546435,43.007444089240849,46.978750874484376,49.242301300948341,51.002542825705397,51.447673176445399,47.843171633901541,39.895074988635152,32.038156511029932,26.359057025099464,25.920295493187655]
[null,16,{"$f":"DEGREES(C103)","v":39.272815363784105},36.618652439227091,33.658333333333317,33.463039652764046,36.459337884487468,39.024897587328624,38.502757361484086,34.338234473859956,29.90833333333336,29.757740035869446,34.142635467633305,38.446132425353902,null,16,{"$f":"DEGREES(Q103)","v":122.15815255245879},113.84254443629344,103.39119101462578,91.510217880198724,83.477800979092081,80.93025347326585,84.083095931601207,91.626811744991429,102.02592730130129,111.16306091796814,119.71693713061819,124.13714890659857,null,null,null,16,{"$f":"IF(DO75<0,0,IF(0>C75,0,IF(50>C75,(( -0.000009*C75^2 + 0.0004*C75 + 0.7918)*Radiation!C19),IF(90>C75,((-0.0006*C75^2 + 0.0699*C75 - 1.2225)*Radiation!C19),0))))","v":78.241046879594492},{"$f":"IF(DP75<0,0,IF(0>D75,0,IF(50>D75,(( -0.000009*D75^2 + 0.0004*D75 + 0.7918)*Radiation!D19),IF(90>D75,((-0.0006*D75^2 + 0.0699*D75 - 1.2225)*Radiation!D19),0))))","v":103.24499252705856},{"$f":"IF(DQ75<0,0,IF(0>E75,0,IF(50>E75,(( -0.000009*E75^2 + 0.0004*E75 + 0.7918)*Radiation!E19),IF(90>E75,((-0.0006*E75^2 + 0.0699*E75 - 1.2225)*Radiation!E19),0))))","v":114.4239945087761},{"$f":"IF(DR75<0,0,IF(0>F75,0,IF(50>F75,(( -0.000009*F75^2 + 0.0004*F75 + 0.7918)*Radiation!F19),IF(90>F75,((-0.0006*F75^2 + 0.0699*F75 - 1.2225)*Radiation!F19),0))))","v":115.18587435447513},{"$f":"IF(DS75<0,0,IF(0>G75,0,IF(50>G75,(( -0.000009*G75^2 + 0.0004*G75 + 0.7918)*Radiation!G19),IF(90>G75,((-0.0006*G75^2 + 0.0699*G75 - 1.2225)*Radiation!G19),0))))","v":138.75836831194195},{"$f":"IF(DT75<0,0,IF(0>H75,0,IF(50>H75,(( -0.000009*H75^2 + 0.0004*H75 + 0.7918)*Radiation!H19),IF(90>H75,((-0.0006*H75^2 + 0.0699*H75 - 1.2225)*Radiation!H19),0))))","v":151.46492984791001},{"$f":"IF(DU75<0,0,IF(0>I75,0,IF(50>I75,(( -0.000009*I75^2 + 0.0004*I75 + 0.7918)*Radiation!I19),IF(90>I75,((-0.0006*I75^2 + 0.0699*I75 - 1.2225)*Radiation!I19),0))))","v":149.48138079261057},{"$f":"IF(DV75<0,0,IF(0>J75,0,IF(50>J75,(( -0.000009*J75^2 + 0.0004*J75 + 0.7918)*Radiation!J19),IF(90>J75,((-0.0006*J75^2 + 0.0699*J75 - 1.2225)*Radiation!J19),0))))","v":139.85419746488196},{"$f":"IF(DW75<0,0,IF(0>K75,0,IF(50>K75,(( -0.000009*K75^2 + 0.0004*K75 + 0.7918)*Radiation!K19),IF(90>K75,((-0.0006*K75^2 + 0.0699*K75 - 1.2225)*Radiation!K19),0))))","v":118.8049519951546},{"$f":"IF(DX75<0,0,IF(0>L75,0,IF(50>L75,(( -0.000009*L75^2 + 0.0004*L75 + 0.7918)*Radiation!L19),IF(90>L75,((-0.0006*L75^2 + 0.0699*L75 - 1.2225)*Radiation!L19),0))))","v":90.304194368730094},{"$f":"IF(DY75<0,0,IF(0>M75,0,IF(50>M75,(( -0.000009*M75^2 + 0.0004*M75 + 0.7918)*Radiation!M19),IF(90>M75,((-0.0006*M75^2 + 0.0699*M75 - 1.2225)*Radiation!M19),0))))","v":60.732712951217557},{"$f":"IF(DZ75<0,0,IF(0>N75,0,IF(50>N75,(( -0.000009*N75^2 + 0.0004*N75 + 0.7918)*Radiation!N19),IF(90>N75,((-0.0006*N75^2 + 0.0699*N75 - 1.2225)*Radiation!N19),0))))","v":56.622916646270966},null,16,{"$f":"IF(EC75<0,0,IF(0>Q75,0,IF(50>Q75,(( -0.000009*Q75^2 + 0.0004*Q75 + 0.7918)*Radiation!C19),IF(90>Q75,((-0.0006*Q75^2 + 0.0699*Q75 - 1.2225)*Radiation!C19),0))))","v":0},{"$f":"IF(ED75<0,0,IF(0>R75,0,IF(50>R75,(( -0.000009*R75^2 + 0.0004*R75 + 0.7918)*Radiation!D19),IF(90>R75,((-0.0006*R75^2 + 0.0699*R75 - 1.2225)*Radiation!D19),0))))","v":0},{"$f":"IF(EE75<0,0,IF(0>S75,0,IF(50>S75,(( -0.000009*S75^2 + 0.0004*S75 + 0.7918)*Radiation!E19),IF(90>S75,((-0.0006*S75^2 + 0.0699*S75 - 1.2225)*Radiation!E19),0))))","v":0},{"$f":"IF(EF75<0,0,IF(0>T75,0,IF(50>T75,(( -0.000009*T75^2 + 0.0004*T75 + 0.7918)*Radiation!F19),IF(90>T75,((-0.0006*T75^2 + 0.0699*T75 - 1.2225)*Radiation!F19),0))))","v":0},{"$f":"IF(EG75<0,0,IF(0>U75,0,IF(50>U75,(( -0.000009*U75^2 + 0.0004*U75 + 0.7918)*Radiation!G19),IF(90>U75,((-0.0006*U75^2 + 0.0699*U75 - 1.2225)*Radiation!G19),0))))","v":75.363640347613952},{"$f":"IF(EH75<0,0,IF(0>V75,0,IF(50>V75,(( -0.000009*V75^2 + 0.0004*V75 + 0.7918)*Radiation!H19),IF(90>V75,((-0.0006*V75^2 + 0.0699*V75 - 1.2225)*Radiation!H19),0))))","v":96.313709571376592},{"$f":"IF(EI75<0,0,IF(0>W75,0,IF(50>W75,(( -0.000009*W75^2 + 0.0004*W75 + 0.7918)*Radiation!I19),IF(90>W75,((-0.0006*W75^2 + 0.0699*W75 - 1.2225)*Radiation!I19),0))))","v":77.753204194594218},{"$f":"IF(EJ75<0,0,IF(0>X75,0,IF(50>X75,(( -0.000009*X75^2 + 0.0004*X75 + 0.7918)*Radiation!J19),IF(90>X75,((-0.0006*X75^2 + 0.0699*X75 - 1.2225)*Radiation!J19),0))))","v":0},{"$f":"IF(EK75<0,0,IF(0>Y75,0,IF(50>Y75,(( -0.000009*Y75^2 + 0.0004*Y75 + 0.7918)*Radiation!K19),IF(90>Y75,((-0.0006*Y75^2 + 0.0699*Y75 - 1.2225)*Radiation!K19),0))))","v":0},{"$f":"IF(EL75<0,0,IF(0>Z75,0,IF(50>Z75,(( -0.000009*Z75^2 + 0.0004*Z75 + 0.7918)*Radiation!L19),IF(90>Z75,((-0.0006*Z75^2 + 0.0699*Z75 - 1.2225)*Radiation!L19),0))))","v":0},{"$f":"IF(EM75<0,0,IF(0>AA75,0,IF(50>AA75,(( -0.000009*AA75^2 + 0.0004*AA75 + 0.7918)*Radiation!M19),IF(90>AA75,((-0.0006*AA75^2 + 0.0699*AA75 - 1.2225)*Radiation!M19),0))))","v":0},{"$f":"IF(EN75<0,0,IF(0>AB75,0,IF(50>AB75,(( -0.000009*AB75^2 + 0.0004*AB75 + 0.7918)*Radiation!N19),IF(90>AB75,((-0.0006*AB75^2 + 0.0699*AB75 - 1.2225)*Radiation!N19),0))))","v":0},null,null,16,{"$f":"AG75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU47","v":2774.6294384683138},{"$f":"AH75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV47","v":3734.587299212772},{"$f":"AI75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW47","v":4446.8095707895973},{"$f":"AJ75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX47","v":4774.3448944164402},{"$f":"AK75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY47","v":4971.3533893484409},{"$f":"AL75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ47","v":4803.02801605271},{"$f":"AM75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA47","v":4929.1205423900001},{"$f":"AN75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB47","v":5622.3905501017762},{"$f":"AO75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC47","v":5190.4573655804825},{"$f":"AP75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD47","v":4062.4502685123566},{"$f":"AQ75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE47","v":2589.6992330867606},{"$f":"AR75*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF47","v":2164.3138343325777},null,16,{"$f":"AU75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI47","v":0},{"$f":"AV75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ47","v":0},{"$f":"AW75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK47","v":0},{"$f":"AX75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL47","v":0},{"$f":"AY75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM47","v":0},{"$f":"AZ75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN47","v":0},{"$f":"BA75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO47","v":0},{"$f":"BB75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP47","v":0},{"$f":"BC75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ47","v":0},{"$f":"BD75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR47","v":0},{"$f":"BE75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS47","v":0},{"$f":"BF75*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT47","v":0},null,16,0.79541267501641133,0.99722917431931501,1,1,1,1,1,1,1,1,0.87146580361454828,0.75810235728560871,null,16,0,0,0,0,0,0,0,0,0,0,0,0,null,null,16,20.038281727598083,26.016647471873153,30.233879108991232,33.419767540103443,35.682648220686666,37.56104623172925,37.876258416390314,34.288646107643089,26.935985833021654,19.913519068774189,15.259931573481456,15.530455637101428,null,16,20.038281727598083,26.016647471873153,30.233879108991232,33.419767540103443,35.682648220686666,37.56104623172925,37.876258416390314,34.288646107643089,26.935985833021654,19.913519068774189,15.259931573481456,15.530455637101428]
[null,17,{"$f":"DEGREES(C104)","v":27.637871812062137},22.760226129815841,18.65833333333336,20.252986237488901,25.611674241310453,28.753808102271957,27.235976158712404,21.072659509379324,14.908333333333339,16.727385306572259,23.80243187548535,28.338651450576869,null,17,{"$f":"DEGREES(Q104)","v":116.16349119299026},108.01947222023406,97.682629304268758,85.919896139154616,78.027509078728187,75.605035317805985,78.752235944073007,86.079601230215246,96.171570684789046,105.10443925001162,113.56881053129125,118.01284291527482,null,null,null,17,{"$f":"IF(DO76<0,0,IF(0>C76,0,IF(50>C76,(( -0.000009*C76^2 + 0.0004*C76 + 0.7918)*Radiation!C20),IF(90>C76,((-0.0006*C76^2 + 0.0699*C76 - 1.2225)*Radiation!C20),0))))","v":30.531286411629324},{"$f":"IF(DP76<0,0,IF(0>D76,0,IF(50>D76,(( -0.000009*D76^2 + 0.0004*D76 + 0.7918)*Radiation!D20),IF(90>D76,((-0.0006*D76^2 + 0.0699*D76 - 1.2225)*Radiation!D20),0))))","v":49.471876134950492},{"$f":"IF(DQ76<0,0,IF(0>E76,0,IF(50>E76,(( -0.000009*E76^2 + 0.0004*E76 + 0.7918)*Radiation!E20),IF(90>E76,((-0.0006*E76^2 + 0.0699*E76 - 1.2225)*Radiation!E20),0))))","v":61.07405314525311},{"$f":"IF(DR76<0,0,IF(0>F76,0,IF(50>F76,(( -0.000009*F76^2 + 0.0004*F76 + 0.7918)*Radiation!F20),IF(90>F76,((-0.0006*F76^2 + 0.0699*F76 - 1.2225)*Radiation!F20),0))))","v":63.604117967340969},{"$f":"IF(DS76<0,0,IF(0>G76,0,IF(50>G76,(( -0.000009*G76^2 + 0.0004*G76 + 0.7918)*Radiation!G20),IF(90>G76,((-0.0006*G76^2 + 0.0699*G76 - 1.2225)*Radiation!G20),0))))","v":78.741181233744186},{"$f":"IF(DT76<0,0,IF(0>H76,0,IF(50>H76,(( -0.000009*H76^2 + 0.0004*H76 + 0.7918)*Radiation!H20),IF(90>H76,((-0.0006*H76^2 + 0.0699*H76 - 1.2225)*Radiation!H20),0))))","v":92.841485011688377},{"$f":"IF(DU76<0,0,IF(0>I76,0,IF(50>I76,(( -0.000009*I76^2 + 0.0004*I76 + 0.7918)*Radiation!I20),IF(90>I76,((-0.0006*I76^2 + 0.0699*I76 - 1.2225)*Radiation!I20),0))))","v":91.345863489899813},{"$f":"IF(DV76<0,0,IF(0>J76,0,IF(50>J76,(( -0.000009*J76^2 + 0.0004*J76 + 0.7918)*Radiation!J20),IF(90>J76,((-0.0006*J76^2 + 0.0699*J76 - 1.2225)*Radiation!J20),0))))","v":79.759849456003579},{"$f":"IF(DW76<0,0,IF(0>K76,0,IF(50>K76,(( -0.000009*K76^2 + 0.0004*K76 + 0.7918)*Radiation!K20),IF(90>K76,((-0.0006*K76^2 + 0.0699*K76 - 1.2225)*Radiation!K20),0))))","v":56.505286282316092},{"$f":"IF(DX76<0,0,IF(0>L76,0,IF(50>L76,(( -0.000009*L76^2 + 0.0004*L76 + 0.7918)*Radiation!L20),IF(90>L76,((-0.0006*L76^2 + 0.0699*L76 - 1.2225)*Radiation!L20),0))))","v":30.530988158514464},{"$f":"IF(DY76<0,0,IF(0>M76,0,IF(50>M76,(( -0.000009*M76^2 + 0.0004*M76 + 0.7918)*Radiation!M20),IF(90>M76,((-0.0006*M76^2 + 0.0699*M76 - 1.2225)*Radiation!M20),0))))","v":11.862857951248481},{"$f":"IF(DZ76<0,0,IF(0>N76,0,IF(50>N76,(( -0.000009*N76^2 + 0.0004*N76 + 0.7918)*Radiation!N20),IF(90>N76,((-0.0006*N76^2 + 0.0699*N76 - 1.2225)*Radiation!N20),0))))","v":14.128890990240253},null,17,{"$f":"IF(EC76<0,0,IF(0>Q76,0,IF(50>Q76,(( -0.000009*Q76^2 + 0.0004*Q76 + 0.7918)*Radiation!C20),IF(90>Q76,((-0.0006*Q76^2 + 0.0699*Q76 - 1.2225)*Radiation!C20),0))))","v":0},{"$f":"IF(ED76<0,0,IF(0>R76,0,IF(50>R76,(( -0.000009*R76^2 + 0.0004*R76 + 0.7918)*Radiation!D20),IF(90>R76,((-0.0006*R76^2 + 0.0699*R76 - 1.2225)*Radiation!D20),0))))","v":0},{"$f":"IF(EE76<0,0,IF(0>S76,0,IF(50>S76,(( -0.000009*S76^2 + 0.0004*S76 + 0.7918)*Radiation!E20),IF(90>S76,((-0.0006*S76^2 + 0.0699*S76 - 1.2225)*Radiation!E20),0))))","v":0},{"$f":"IF(EF76<0,0,IF(0>T76,0,IF(50>T76,(( -0.000009*T76^2 + 0.0004*T76 + 0.7918)*Radiation!F20),IF(90>T76,((-0.0006*T76^2 + 0.0699*T76 - 1.2225)*Radiation!F20),0))))","v":28.275902119715202},{"$f":"IF(EG76<0,0,IF(0>U76,0,IF(50>U76,(( -0.000009*U76^2 + 0.0004*U76 + 0.7918)*Radiation!G20),IF(90>U76,((-0.0006*U76^2 + 0.0699*U76 - 1.2225)*Radiation!G20),0))))","v":57.230303709902905},{"$f":"IF(EH76<0,0,IF(0>V76,0,IF(50>V76,(( -0.000009*V76^2 + 0.0004*V76 + 0.7918)*Radiation!H20),IF(90>V76,((-0.0006*V76^2 + 0.0699*V76 - 1.2225)*Radiation!H20),0))))","v":73.798488589092756},{"$f":"IF(EI76<0,0,IF(0>W76,0,IF(50>W76,(( -0.000009*W76^2 + 0.0004*W76 + 0.7918)*Radiation!I20),IF(90>W76,((-0.0006*W76^2 + 0.0699*W76 - 1.2225)*Radiation!I20),0))))","v":64.391909343470772},{"$f":"IF(EJ76<0,0,IF(0>X76,0,IF(50>X76,(( -0.000009*X76^2 + 0.0004*X76 + 0.7918)*Radiation!J20),IF(90>X76,((-0.0006*X76^2 + 0.0699*X76 - 1.2225)*Radiation!J20),0))))","v":34.924358143704048},{"$f":"IF(EK76<0,0,IF(0>Y76,0,IF(50>Y76,(( -0.000009*Y76^2 + 0.0004*Y76 + 0.7918)*Radiation!K20),IF(90>Y76,((-0.0006*Y76^2 + 0.0699*Y76 - 1.2225)*Radiation!K20),0))))","v":0},{"$f":"IF(EL76<0,0,IF(0>Z76,0,IF(50>Z76,(( -0.000009*Z76^2 + 0.0004*Z76 + 0.7918)*Radiation!L20),IF(90>Z76,((-0.0006*Z76^2 + 0.0699*Z76 - 1.2225)*Radiation!L20),0))))","v":0},{"$f":"IF(EM76<0,0,IF(0>AA76,0,IF(50>AA76,(( -0.000009*AA76^2 + 0.0004*AA76 + 0.7918)*Radiation!M20),IF(90>AA76,((-0.0006*AA76^2 + 0.0699*AA76 - 1.2225)*Radiation!M20),0))))","v":0},{"$f":"IF(EN76<0,0,IF(0>AB76,0,IF(50>AB76,(( -0.000009*AB76^2 + 0.0004*AB76 + 0.7918)*Radiation!N20),IF(90>AB76,((-0.0006*AB76^2 + 0.0699*AB76 - 1.2225)*Radiation!N20),0))))","v":0},null,null,17,{"$f":"AG76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU48","v":1591.2164963126143},{"$f":"AH76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV48","v":2655.3121550436108},{"$f":"AI76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW48","v":3490.2420072817777},{"$f":"AJ76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX48","v":3580.241138149192},{"$f":"AK76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY48","v":3849.9681326621317},{"$f":"AL76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ48","v":4187.313761054791},{"$f":"AM76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA48","v":4292.2891157890799},{"$f":"AN76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB48","v":4423.2439261434729},{"$f":"AO76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC48","v":3470.8202131864714},{"$f":"AP76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD48","v":1880.8404833431982},{"$f":"AQ76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE48","v":695.47656043259258},{"$f":"AR76*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF48","v":766.73880398976189},null,17,{"$f":"AU76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI48","v":0},{"$f":"AV76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ48","v":0},{"$f":"AW76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK48","v":0},{"$f":"AX76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL48","v":0},{"$f":"AY76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM48","v":0},{"$f":"AZ76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN48","v":0},{"$f":"BA76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO48","v":0},{"$f":"BB76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP48","v":0},{"$f":"BC76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ48","v":0},{"$f":"BD76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR48","v":0},{"$f":"BE76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS48","v":0},{"$f":"BF76*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT48","v":0},null,17,1,1,1,1,1,1,1,1,1,1,1,0.94109284264869175,null,17,0,0,0,0,0,0,0,0,0,0,0,0,null,null,17,8.2848854255444504,13.434807821200849,16.897092448538277,19.80224832363653,22.286756355186323,24.319689951925163,24.456964963286701,20.670382142796534,13.51706337533537,7.0202572324504446,3.1397975005302774,3.9451572875932328,null,17,8.2848854255444504,13.434807821200849,16.897092448538277,19.80224832363653,22.286756355186323,24.319689951925163,24.456964963286701,20.670382142796534,13.51706337533537,7.0202572324504446,3.1397975005302774,3.9451572875932328]
[null,18,{"$f":"DEGREES(C105)","v":20.400123044346774},11.819209502025943,3.6583333333332755,11.993842601690101,20.321654647600202,23.541380287535372,20.75771613252067,12.329053937677777,9.1666666666745777E-2,10.895473299208135,19.966851705660439,23.488466210529062,null,18,{"$f":"DEGREES(Q105)","v":109.91557089227641},101.81567437582528,91.527839613033834,79.829654177638858,72.022769427832742,69.679623246047981,72.817988123224652,80.011574541330674,89.961695531722455,98.85140476799117,107.32610019466784,111.76461154705702,null,null,null,18,{"$f":"IF(DO77<0,0,IF(0>C77,0,IF(50>C77,(( -0.000009*C77^2 + 0.0004*C77 + 0.7918)*Radiation!C21),IF(90>C77,((-0.0006*C77^2 + 0.0699*C77 - 1.2225)*Radiation!C21),0))))","v":0},{"$f":"IF(DP77<0,0,IF(0>D77,0,IF(50>D77,(( -0.000009*D77^2 + 0.0004*D77 + 0.7918)*Radiation!D21),IF(90>D77,((-0.0006*D77^2 + 0.0699*D77 - 1.2225)*Radiation!D21),0))))","v":6.0503903805436146},{"$f":"IF(DQ77<0,0,IF(0>E77,0,IF(50>E77,(( -0.000009*E77^2 + 0.0004*E77 + 0.7918)*Radiation!E21),IF(90>E77,((-0.0006*E77^2 + 0.0699*E77 - 1.2225)*Radiation!E21),0))))","v":11.062707322966673},{"$f":"IF(DR77<0,0,IF(0>F77,0,IF(50>F77,(( -0.000009*F77^2 + 0.0004*F77 + 0.7918)*Radiation!F21),IF(90>F77,((-0.0006*F77^2 + 0.0699*F77 - 1.2225)*Radiation!F21),0))))","v":15.630812453693762},{"$f":"IF(DS77<0,0,IF(0>G77,0,IF(50>G77,(( -0.000009*G77^2 + 0.0004*G77 + 0.7918)*Radiation!G21),IF(90>G77,((-0.0006*G77^2 + 0.0699*G77 - 1.2225)*Radiation!G21),0))))","v":24.482611010513615},{"$f":"IF(DT77<0,0,IF(0>H77,0,IF(50>H77,(( -0.000009*H77^2 + 0.0004*H77 + 0.7918)*Radiation!H21),IF(90>H77,((-0.0006*H77^2 + 0.0699*H77 - 1.2225)*Radiation!H21),0))))","v":34.831668149435906},{"$f":"IF(DU77<0,0,IF(0>I77,0,IF(50>I77,(( -0.000009*I77^2 + 0.0004*I77 + 0.7918)*Radiation!I21),IF(90>I77,((-0.0006*I77^2 + 0.0699*I77 - 1.2225)*Radiation!I21),0))))","v":33.82189990115873},{"$f":"IF(DV77<0,0,IF(0>J77,0,IF(50>J77,(( -0.000009*J77^2 + 0.0004*J77 + 0.7918)*Radiation!J21),IF(90>J77,((-0.0006*J77^2 + 0.0699*J77 - 1.2225)*Radiation!J21),0))))","v":23.700137430515831},{"$f":"IF(DW77<0,0,IF(0>K77,0,IF(50>K77,(( -0.000009*K77^2 + 0.0004*K77 + 0.7918)*Radiation!K21),IF(90>K77,((-0.0006*K77^2 + 0.0699*K77 - 1.2225)*Radiation!K21),0))))","v":0},{"$f":"IF(DX77<0,0,IF(0>L77,0,IF(50>L77,(( -0.000009*L77^2 + 0.0004*L77 + 0.7918)*Radiation!L21),IF(90>L77,((-0.0006*L77^2 + 0.0699*L77 - 1.2225)*Radiation!L21),0))))","v":0},{"$f":"IF(DY77<0,0,IF(0>M77,0,IF(50>M77,(( -0.000009*M77^2 + 0.0004*M77 + 0.7918)*Radiation!M21),IF(90>M77,((-0.0006*M77^2 + 0.0699*M77 - 1.2225)*Radiation!M21),0))))","v":0},{"$f":"IF(DZ77<0,0,IF(0>N77,0,IF(50>N77,(( -0.000009*N77^2 + 0.0004*N77 + 0.7918)*Radiation!N21),IF(90>N77,((-0.0006*N77^2 + 0.0699*N77 - 1.2225)*Radiation!N21),0))))","v":0},null,18,{"$f":"IF(EC77<0,0,IF(0>Q77,0,IF(50>Q77,(( -0.000009*Q77^2 + 0.0004*Q77 + 0.7918)*Radiation!C21),IF(90>Q77,((-0.0006*Q77^2 + 0.0699*Q77 - 1.2225)*Radiation!C21),0))))","v":0},{"$f":"IF(ED77<0,0,IF(0>R77,0,IF(50>R77,(( -0.000009*R77^2 + 0.0004*R77 + 0.7918)*Radiation!D21),IF(90>R77,((-0.0006*R77^2 + 0.0699*R77 - 1.2225)*Radiation!D21),0))))","v":0},{"$f":"IF(EE77<0,0,IF(0>S77,0,IF(50>S77,(( -0.000009*S77^2 + 0.0004*S77 + 0.7918)*Radiation!E21),IF(90>S77,((-0.0006*S77^2 + 0.0699*S77 - 1.2225)*Radiation!E21),0))))","v":0},{"$f":"IF(EF77<0,0,IF(0>T77,0,IF(50>T77,(( -0.000009*T77^2 + 0.0004*T77 + 0.7918)*Radiation!F21),IF(90>T77,((-0.0006*T77^2 + 0.0699*T77 - 1.2225)*Radiation!F21),0))))","v":10.493785951960682},{"$f":"IF(EG77<0,0,IF(0>U77,0,IF(50>U77,(( -0.000009*U77^2 + 0.0004*U77 + 0.7918)*Radiation!G21),IF(90>U77,((-0.0006*U77^2 + 0.0699*U77 - 1.2225)*Radiation!G21),0))))","v":21.509566823571788},{"$f":"IF(EH77<0,0,IF(0>V77,0,IF(50>V77,(( -0.000009*V77^2 + 0.0004*V77 + 0.7918)*Radiation!H21),IF(90>V77,((-0.0006*V77^2 + 0.0699*V77 - 1.2225)*Radiation!H21),0))))","v":32.151229088259853},{"$f":"IF(EI77<0,0,IF(0>W77,0,IF(50>W77,(( -0.000009*W77^2 + 0.0004*W77 + 0.7918)*Radiation!I21),IF(90>W77,((-0.0006*W77^2 + 0.0699*W77 - 1.2225)*Radiation!I21),0))))","v":29.139850961181473},{"$f":"IF(EJ77<0,0,IF(0>X77,0,IF(50>X77,(( -0.000009*X77^2 + 0.0004*X77 + 0.7918)*Radiation!J21),IF(90>X77,((-0.0006*X77^2 + 0.0699*X77 - 1.2225)*Radiation!J21),0))))","v":15.768966054354156},{"$f":"IF(EK77<0,0,IF(0>Y77,0,IF(50>Y77,(( -0.000009*Y77^2 + 0.0004*Y77 + 0.7918)*Radiation!K21),IF(90>Y77,((-0.0006*Y77^2 + 0.0699*Y77 - 1.2225)*Radiation!K21),0))))","v":0},{"$f":"IF(EL77<0,0,IF(0>Z77,0,IF(50>Z77,(( -0.000009*Z77^2 + 0.0004*Z77 + 0.7918)*Radiation!L21),IF(90>Z77,((-0.0006*Z77^2 + 0.0699*Z77 - 1.2225)*Radiation!L21),0))))","v":0},{"$f":"IF(EM77<0,0,IF(0>AA77,0,IF(50>AA77,(( -0.000009*AA77^2 + 0.0004*AA77 + 0.7918)*Radiation!M21),IF(90>AA77,((-0.0006*AA77^2 + 0.0699*AA77 - 1.2225)*Radiation!M21),0))))","v":0},{"$f":"IF(EN77<0,0,IF(0>AB77,0,IF(50>AB77,(( -0.000009*AB77^2 + 0.0004*AB77 + 0.7918)*Radiation!N21),IF(90>AB77,((-0.0006*AB77^2 + 0.0699*AB77 - 1.2225)*Radiation!N21),0))))","v":0},null,null,18,{"$f":"AG77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU49","v":0},{"$f":"AH77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV49","v":422.68319711735165},{"$f":"AI77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW49","v":819.88818854556575},{"$f":"AJ77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX49","v":1026.1250812956971},{"$f":"AK77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY49","v":1411.1756989981864},{"$f":"AL77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ49","v":1877.6960626038615},{"$f":"AM77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA49","v":1903.0570696083062},{"$f":"AN77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB49","v":1540.0957842881564},{"$f":"AO77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC49","v":0},{"$f":"AP77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD49","v":0},{"$f":"AQ77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE49","v":0},{"$f":"AR77*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF49","v":0},null,18,{"$f":"AU77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI49","v":0},{"$f":"AV77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ49","v":0},{"$f":"AW77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK49","v":0},{"$f":"AX77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL49","v":0},{"$f":"AY77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM49","v":0},{"$f":"AZ77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN49","v":0},{"$f":"BA77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO49","v":0},{"$f":"BB77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP49","v":0},{"$f":"BC77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ49","v":0},{"$f":"BD77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR49","v":0},{"$f":"BE77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS49","v":0},{"$f":"BF77*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT49","v":0},null,18,0,1,1,1,1,1,1,1,0,0,0,0,null,18,0,0,0,0,0,0,0,0,0,0,0,0,null,null,18,-4.242067037456934,0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772,null,18,-4.242067037456934,0.28496224246637836,3.3232309033445016,6.2903017477886056,9.1618728727979484,11.380032986011807,11.292623329902437,7.1538265372891177,-8.3279910069723753E-2,-6.3024734223343577,-9.6180467382750852,-8.4049479592926772]
[null,19,{"$f":"DEGREES(C106)","v":22.363115013737705},14.358718721607621,11.341666666666733,17.916487823059356,24.513383283898683,26.572066445658255,23.462461777687516,17.412902231087408,15.091666666666717,20.058590682931573,25.738401798789784,26.922256182529942,null,19,{"$f":"DEGREES(Q106)","v":103.78011662804725},95.602262060389066,85.286265589431665,73.576609673297611,65.77740485075087,63.454644632248254,66.589558720250906,73.758542283621054,83.753994157338354,92.761268205895448,101.3351784075563,105.74094989412582,null,null,null,19,{"$f":"IF(DO78<0,0,IF(0>C78,0,IF(50>C78,(( -0.000009*C78^2 + 0.0004*C78 + 0.7918)*Radiation!C22),IF(90>C78,((-0.0006*C78^2 + 0.0699*C78 - 1.2225)*Radiation!C22),0))))","v":0},{"$f":"IF(DP78<0,0,IF(0>D78,0,IF(50>D78,(( -0.000009*D78^2 + 0.0004*D78 + 0.7918)*Radiation!D22),IF(90>D78,((-0.0006*D78^2 + 0.0699*D78 - 1.2225)*Radiation!D22),0))))","v":0},{"$f":"IF(DQ78<0,0,IF(0>E78,0,IF(50>E78,(( -0.000009*E78^2 + 0.0004*E78 + 0.7918)*Radiation!E22),IF(90>E78,((-0.0006*E78^2 + 0.0699*E78 - 1.2225)*Radiation!E22),0))))","v":0},{"$f":"IF(DR78<0,0,IF(0>F78,0,IF(50>F78,(( -0.000009*F78^2 + 0.0004*F78 + 0.7918)*Radiation!F22),IF(90>F78,((-0.0006*F78^2 + 0.0699*F78 - 1.2225)*Radiation!F22),0))))","v":0},{"$f":"IF(DS78<0,0,IF(0>G78,0,IF(50>G78,(( -0.000009*G78^2 + 0.0004*G78 + 0.7918)*Radiation!G22),IF(90>G78,((-0.0006*G78^2 + 0.0699*G78 - 1.2225)*Radiation!G22),0))))","v":0},{"$f":"IF(DT78<0,0,IF(0>H78,0,IF(50>H78,(( -0.000009*H78^2 + 0.0004*H78 + 0.7918)*Radiation!H22),IF(90>H78,((-0.0006*H78^2 + 0.0699*H78 - 1.2225)*Radiation!H22),0))))","v":0},{"$f":"IF(DU78<0,0,IF(0>I78,0,IF(50>I78,(( -0.000009*I78^2 + 0.0004*I78 + 0.7918)*Radiation!I22),IF(90>I78,((-0.0006*I78^2 + 0.0699*I78 - 1.2225)*Radiation!I22),0))))","v":0},{"$f":"IF(DV78<0,0,IF(0>J78,0,IF(50>J78,(( -0.000009*J78^2 + 0.0004*J78 + 0.7918)*Radiation!J22),IF(90>J78,((-0.0006*J78^2 + 0.0699*J78 - 1.2225)*Radiation!J22),0))))","v":0},{"$f":"IF(DW78<0,0,IF(0>K78,0,IF(50>K78,(( -0.000009*K78^2 + 0.0004*K78 + 0.7918)*Radiation!K22),IF(90>K78,((-0.0006*K78^2 + 0.0699*K78 - 1.2225)*Radiation!K22),0))))","v":0},{"$f":"IF(DX78<0,0,IF(0>L78,0,IF(50>L78,(( -0.000009*L78^2 + 0.0004*L78 + 0.7918)*Radiation!L22),IF(90>L78,((-0.0006*L78^2 + 0.0699*L78 - 1.2225)*Radiation!L22),0))))","v":0},{"$f":"IF(DY78<0,0,IF(0>M78,0,IF(50>M78,(( -0.000009*M78^2 + 0.0004*M78 + 0.7918)*Radiation!M22),IF(90>M78,((-0.0006*M78^2 + 0.0699*M78 - 1.2225)*Radiation!M22),0))))","v":0},{"$f":"IF(DZ78<0,0,IF(0>N78,0,IF(50>N78,(( -0.000009*N78^2 + 0.0004*N78 + 0.7918)*Radiation!N22),IF(90>N78,((-0.0006*N78^2 + 0.0699*N78 - 1.2225)*Radiation!N22),0))))","v":0},null,19,{"$f":"IF(EC78<0,0,IF(0>Q78,0,IF(50>Q78,(( -0.000009*Q78^2 + 0.0004*Q78 + 0.7918)*Radiation!C22),IF(90>Q78,((-0.0006*Q78^2 + 0.0699*Q78 - 1.2225)*Radiation!C22),0))))","v":0},{"$f":"IF(ED78<0,0,IF(0>R78,0,IF(50>R78,(( -0.000009*R78^2 + 0.0004*R78 + 0.7918)*Radiation!D22),IF(90>R78,((-0.0006*R78^2 + 0.0699*R78 - 1.2225)*Radiation!D22),0))))","v":0},{"$f":"IF(EE78<0,0,IF(0>S78,0,IF(50>S78,(( -0.000009*S78^2 + 0.0004*S78 + 0.7918)*Radiation!E22),IF(90>S78,((-0.0006*S78^2 + 0.0699*S78 - 1.2225)*Radiation!E22),0))))","v":0},{"$f":"IF(EF78<0,0,IF(0>T78,0,IF(50>T78,(( -0.000009*T78^2 + 0.0004*T78 + 0.7918)*Radiation!F22),IF(90>T78,((-0.0006*T78^2 + 0.0699*T78 - 1.2225)*Radiation!F22),0))))","v":0},{"$f":"IF(EG78<0,0,IF(0>U78,0,IF(50>U78,(( -0.000009*U78^2 + 0.0004*U78 + 0.7918)*Radiation!G22),IF(90>U78,((-0.0006*U78^2 + 0.0699*U78 - 1.2225)*Radiation!G22),0))))","v":0},{"$f":"IF(EH78<0,0,IF(0>V78,0,IF(50>V78,(( -0.000009*V78^2 + 0.0004*V78 + 0.7918)*Radiation!H22),IF(90>V78,((-0.0006*V78^2 + 0.0699*V78 - 1.2225)*Radiation!H22),0))))","v":0},{"$f":"IF(EI78<0,0,IF(0>W78,0,IF(50>W78,(( -0.000009*W78^2 + 0.0004*W78 + 0.7918)*Radiation!I22),IF(90>W78,((-0.0006*W78^2 + 0.0699*W78 - 1.2225)*Radiation!I22),0))))","v":0},{"$f":"IF(EJ78<0,0,IF(0>X78,0,IF(50>X78,(( -0.000009*X78^2 + 0.0004*X78 + 0.7918)*Radiation!J22),IF(90>X78,((-0.0006*X78^2 + 0.0699*X78 - 1.2225)*Radiation!J22),0))))","v":0},{"$f":"IF(EK78<0,0,IF(0>Y78,0,IF(50>Y78,(( -0.000009*Y78^2 + 0.0004*Y78 + 0.7918)*Radiation!K22),IF(90>Y78,((-0.0006*Y78^2 + 0.0699*Y78 - 1.2225)*Radiation!K22),0))))","v":0},{"$f":"IF(EL78<0,0,IF(0>Z78,0,IF(50>Z78,(( -0.000009*Z78^2 + 0.0004*Z78 + 0.7918)*Radiation!L22),IF(90>Z78,((-0.0006*Z78^2 + 0.0699*Z78 - 1.2225)*Radiation!L22),0))))","v":0},{"$f":"IF(EM78<0,0,IF(0>AA78,0,IF(50>AA78,(( -0.000009*AA78^2 + 0.0004*AA78 + 0.7918)*Radiation!M22),IF(90>AA78,((-0.0006*AA78^2 + 0.0699*AA78 - 1.2225)*Radiation!M22),0))))","v":0},{"$f":"IF(EN78<0,0,IF(0>AB78,0,IF(50>AB78,(( -0.000009*AB78^2 + 0.0004*AB78 + 0.7918)*Radiation!N22),IF(90>AB78,((-0.0006*AB78^2 + 0.0699*AB78 - 1.2225)*Radiation!N22),0))))","v":0},null,null,19,{"$f":"AG78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU50","v":0},{"$f":"AH78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV50","v":0},{"$f":"AI78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW50","v":0},{"$f":"AJ78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX50","v":0},{"$f":"AK78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY50","v":0},{"$f":"AL78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ50","v":0},{"$f":"AM78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA50","v":0},{"$f":"AN78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB50","v":0},{"$f":"AO78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC50","v":0},{"$f":"AP78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD50","v":0},{"$f":"AQ78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE50","v":0},{"$f":"AR78*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF50","v":0},null,19,{"$f":"AU78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI50","v":0},{"$f":"AV78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ50","v":0},{"$f":"AW78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK50","v":0},{"$f":"AX78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL50","v":0},{"$f":"AY78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM50","v":0},{"$f":"AZ78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN50","v":0},{"$f":"BA78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO50","v":0},{"$f":"BB78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP50","v":0},{"$f":"BC78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ50","v":0},{"$f":"BD78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR50","v":0},{"$f":"BE78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS50","v":0},{"$f":"BF78*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT50","v":0},null,19,0,0,0,0,0,0,0,0,0,0,0,0,null,19,0,0,0,0,0,0,0,0,0,0,0,0,null,null,19,-17.258784755357599,-13.177535073458104,-10.292097151668569,-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176,null,19,-17.258784755357599,-13.177535073458104,-10.292097151668569,-6.9635212465343193,-3.5411252469823715,-1.1064784283971907,-1.4750612815819091,-6.1102162570653853,-13.682588857300294,-19.851334869589788,-22.782734775346487,-21.2544074674176]
[null,20,{"$f":"DEGREES(C107)","v":31.866762607805054},26.784740200575246,26.341666666666704,30.68360345286353,34.918683399762628,35.803997711168726,33.171053544895145,29.958974794295209,30.091666666666701,33.623263740320077,36.841727364302308,36.356841900499532,null,20,{"$f":"DEGREES(Q107)","v":98.082516534125716},89.725941823403787,79.314540713478863,67.518209627724133,59.63902038096218,57.266963746729203,60.407484989281265,67.676192068474379,77.906230121544084,87.173539413040174,95.910003046029956,100.24938732278783,null,null,null,20,{"$f":"IF(DO79<0,0,IF(0>C79,0,IF(50>C79,(( -0.000009*C79^2 + 0.0004*C79 + 0.7918)*Radiation!C23),IF(90>C79,((-0.0006*C79^2 + 0.0699*C79 - 1.2225)*Radiation!C23),0))))","v":0},{"$f":"IF(DP79<0,0,IF(0>D79,0,IF(50>D79,(( -0.000009*D79^2 + 0.0004*D79 + 0.7918)*Radiation!D23),IF(90>D79,((-0.0006*D79^2 + 0.0699*D79 - 1.2225)*Radiation!D23),0))))","v":0},{"$f":"IF(DQ79<0,0,IF(0>E79,0,IF(50>E79,(( -0.000009*E79^2 + 0.0004*E79 + 0.7918)*Radiation!E23),IF(90>E79,((-0.0006*E79^2 + 0.0699*E79 - 1.2225)*Radiation!E23),0))))","v":0},{"$f":"IF(DR79<0,0,IF(0>F79,0,IF(50>F79,(( -0.000009*F79^2 + 0.0004*F79 + 0.7918)*Radiation!F23),IF(90>F79,((-0.0006*F79^2 + 0.0699*F79 - 1.2225)*Radiation!F23),0))))","v":0},{"$f":"IF(DS79<0,0,IF(0>G79,0,IF(50>G79,(( -0.000009*G79^2 + 0.0004*G79 + 0.7918)*Radiation!G23),IF(90>G79,((-0.0006*G79^2 + 0.0699*G79 - 1.2225)*Radiation!G23),0))))","v":0},{"$f":"IF(DT79<0,0,IF(0>H79,0,IF(50>H79,(( -0.000009*H79^2 + 0.0004*H79 + 0.7918)*Radiation!H23),IF(90>H79,((-0.0006*H79^2 + 0.0699*H79 - 1.2225)*Radiation!H23),0))))","v":0},{"$f":"IF(DU79<0,0,IF(0>I79,0,IF(50>I79,(( -0.000009*I79^2 + 0.0004*I79 + 0.7918)*Radiation!I23),IF(90>I79,((-0.0006*I79^2 + 0.0699*I79 - 1.2225)*Radiation!I23),0))))","v":0},{"$f":"IF(DV79<0,0,IF(0>J79,0,IF(50>J79,(( -0.000009*J79^2 + 0.0004*J79 + 0.7918)*Radiation!J23),IF(90>J79,((-0.0006*J79^2 + 0.0699*J79 - 1.2225)*Radiation!J23),0))))","v":0},{"$f":"IF(DW79<0,0,IF(0>K79,0,IF(50>K79,(( -0.000009*K79^2 + 0.0004*K79 + 0.7918)*Radiation!K23),IF(90>K79,((-0.0006*K79^2 + 0.0699*K79 - 1.2225)*Radiation!K23),0))))","v":0},{"$f":"IF(DX79<0,0,IF(0>L79,0,IF(50>L79,(( -0.000009*L79^2 + 0.0004*L79 + 0.7918)*Radiation!L23),IF(90>L79,((-0.0006*L79^2 + 0.0699*L79 - 1.2225)*Radiation!L23),0))))","v":0},{"$f":"IF(DY79<0,0,IF(0>M79,0,IF(50>M79,(( -0.000009*M79^2 + 0.0004*M79 + 0.7918)*Radiation!M23),IF(90>M79,((-0.0006*M79^2 + 0.0699*M79 - 1.2225)*Radiation!M23),0))))","v":0},{"$f":"IF(DZ79<0,0,IF(0>N79,0,IF(50>N79,(( -0.000009*N79^2 + 0.0004*N79 + 0.7918)*Radiation!N23),IF(90>N79,((-0.0006*N79^2 + 0.0699*N79 - 1.2225)*Radiation!N23),0))))","v":0},null,20,{"$f":"IF(EC79<0,0,IF(0>Q79,0,IF(50>Q79,(( -0.000009*Q79^2 + 0.0004*Q79 + 0.7918)*Radiation!C23),IF(90>Q79,((-0.0006*Q79^2 + 0.0699*Q79 - 1.2225)*Radiation!C23),0))))","v":0},{"$f":"IF(ED79<0,0,IF(0>R79,0,IF(50>R79,(( -0.000009*R79^2 + 0.0004*R79 + 0.7918)*Radiation!D23),IF(90>R79,((-0.0006*R79^2 + 0.0699*R79 - 1.2225)*Radiation!D23),0))))","v":0},{"$f":"IF(EE79<0,0,IF(0>S79,0,IF(50>S79,(( -0.000009*S79^2 + 0.0004*S79 + 0.7918)*Radiation!E23),IF(90>S79,((-0.0006*S79^2 + 0.0699*S79 - 1.2225)*Radiation!E23),0))))","v":0},{"$f":"IF(EF79<0,0,IF(0>T79,0,IF(50>T79,(( -0.000009*T79^2 + 0.0004*T79 + 0.7918)*Radiation!F23),IF(90>T79,((-0.0006*T79^2 + 0.0699*T79 - 1.2225)*Radiation!F23),0))))","v":0},{"$f":"IF(EG79<0,0,IF(0>U79,0,IF(50>U79,(( -0.000009*U79^2 + 0.0004*U79 + 0.7918)*Radiation!G23),IF(90>U79,((-0.0006*U79^2 + 0.0699*U79 - 1.2225)*Radiation!G23),0))))","v":0},{"$f":"IF(EH79<0,0,IF(0>V79,0,IF(50>V79,(( -0.000009*V79^2 + 0.0004*V79 + 0.7918)*Radiation!H23),IF(90>V79,((-0.0006*V79^2 + 0.0699*V79 - 1.2225)*Radiation!H23),0))))","v":0},{"$f":"IF(EI79<0,0,IF(0>W79,0,IF(50>W79,(( -0.000009*W79^2 + 0.0004*W79 + 0.7918)*Radiation!I23),IF(90>W79,((-0.0006*W79^2 + 0.0699*W79 - 1.2225)*Radiation!I23),0))))","v":0},{"$f":"IF(EJ79<0,0,IF(0>X79,0,IF(50>X79,(( -0.000009*X79^2 + 0.0004*X79 + 0.7918)*Radiation!J23),IF(90>X79,((-0.0006*X79^2 + 0.0699*X79 - 1.2225)*Radiation!J23),0))))","v":0},{"$f":"IF(EK79<0,0,IF(0>Y79,0,IF(50>Y79,(( -0.000009*Y79^2 + 0.0004*Y79 + 0.7918)*Radiation!K23),IF(90>Y79,((-0.0006*Y79^2 + 0.0699*Y79 - 1.2225)*Radiation!K23),0))))","v":0},{"$f":"IF(EL79<0,0,IF(0>Z79,0,IF(50>Z79,(( -0.000009*Z79^2 + 0.0004*Z79 + 0.7918)*Radiation!L23),IF(90>Z79,((-0.0006*Z79^2 + 0.0699*Z79 - 1.2225)*Radiation!L23),0))))","v":0},{"$f":"IF(EM79<0,0,IF(0>AA79,0,IF(50>AA79,(( -0.000009*AA79^2 + 0.0004*AA79 + 0.7918)*Radiation!M23),IF(90>AA79,((-0.0006*AA79^2 + 0.0699*AA79 - 1.2225)*Radiation!M23),0))))","v":0},{"$f":"IF(EN79<0,0,IF(0>AB79,0,IF(50>AB79,(( -0.000009*AB79^2 + 0.0004*AB79 + 0.7918)*Radiation!N23),IF(90>AB79,((-0.0006*AB79^2 + 0.0699*AB79 - 1.2225)*Radiation!N23),0))))","v":0},null,null,20,{"$f":"AG79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU51","v":0},{"$f":"AH79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV51","v":0},{"$f":"AI79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW51","v":0},{"$f":"AJ79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX51","v":0},{"$f":"AK79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY51","v":0},{"$f":"AL79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ51","v":0},{"$f":"AM79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA51","v":0},{"$f":"AN79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB51","v":0},{"$f":"AO79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC51","v":0},{"$f":"AP79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD51","v":0},{"$f":"AQ79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE51","v":0},{"$f":"AR79*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF51","v":0},null,20,{"$f":"AU79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI51","v":0},{"$f":"AV79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ51","v":0},{"$f":"AW79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK51","v":0},{"$f":"AX79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL51","v":0},{"$f":"AY79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM51","v":0},{"$f":"AZ79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN51","v":0},{"$f":"BA79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO51","v":0},{"$f":"BB79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP51","v":0},{"$f":"BC79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ51","v":0},{"$f":"BD79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR51","v":0},{"$f":"BE79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS51","v":0},{"$f":"BF79*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT51","v":0},null,20,0,0,0,0,0,0,0,0,0,0,0,0,null,20,0,0,0,0,0,0,0,0,0,0,0,0,null,null,20,-30.589239677830651,-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,{"$f":"DT24","v":-12.902247652391463},-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299,null,20,-30.589239677830651,-26.783110901661868,-23.773745192987072,-19.749387170381588,-15.584861719885295,-12.902247652391463,-13.625605199002544,-18.916708643772196,-27.097900221004799,-33.472019280706604,-36.206670576844481,-34.435555539572299]
[null,21,{"$f":"DEGREES(C108)","v":44.283968367372367},40.903521848191545,41.341666666666683,44.774579106628124,47.608962417547851,47.747144287511205,45.595647887719707,43.982590510226885,45.091666666666676,47.986654037396697,49.814463007257956,48.380798902239192,null,21,{"$f":"DEGREES(Q108)","v":93.123838203124365},84.521422024626432,73.977120459924436,62.046549186276351,54.009974652573355,51.513256111399926,54.663997444819444,62.154565368010999,72.785548204204289,82.418233802575358,91.343208553675936,95.571630337473579,null,null,null,21,{"$f":"IF(DO80<0,0,IF(0>C80,0,IF(50>C80,(( -0.000009*C80^2 + 0.0004*C80 + 0.7918)*Radiation!C24),IF(90>C80,((-0.0006*C80^2 + 0.0699*C80 - 1.2225)*Radiation!C24),0))))","v":0},{"$f":"IF(DP80<0,0,IF(0>D80,0,IF(50>D80,(( -0.000009*D80^2 + 0.0004*D80 + 0.7918)*Radiation!D24),IF(90>D80,((-0.0006*D80^2 + 0.0699*D80 - 1.2225)*Radiation!D24),0))))","v":0},{"$f":"IF(DQ80<0,0,IF(0>E80,0,IF(50>E80,(( -0.000009*E80^2 + 0.0004*E80 + 0.7918)*Radiation!E24),IF(90>E80,((-0.0006*E80^2 + 0.0699*E80 - 1.2225)*Radiation!E24),0))))","v":0},{"$f":"IF(DR80<0,0,IF(0>F80,0,IF(50>F80,(( -0.000009*F80^2 + 0.0004*F80 + 0.7918)*Radiation!F24),IF(90>F80,((-0.0006*F80^2 + 0.0699*F80 - 1.2225)*Radiation!F24),0))))","v":0},{"$f":"IF(DS80<0,0,IF(0>G80,0,IF(50>G80,(( -0.000009*G80^2 + 0.0004*G80 + 0.7918)*Radiation!G24),IF(90>G80,((-0.0006*G80^2 + 0.0699*G80 - 1.2225)*Radiation!G24),0))))","v":0},{"$f":"IF(DT80<0,0,IF(0>H80,0,IF(50>H80,(( -0.000009*H80^2 + 0.0004*H80 + 0.7918)*Radiation!H24),IF(90>H80,((-0.0006*H80^2 + 0.0699*H80 - 1.2225)*Radiation!H24),0))))","v":0},{"$f":"IF(DU80<0,0,IF(0>I80,0,IF(50>I80,(( -0.000009*I80^2 + 0.0004*I80 + 0.7918)*Radiation!I24),IF(90>I80,((-0.0006*I80^2 + 0.0699*I80 - 1.2225)*Radiation!I24),0))))","v":0},{"$f":"IF(DV80<0,0,IF(0>J80,0,IF(50>J80,(( -0.000009*J80^2 + 0.0004*J80 + 0.7918)*Radiation!J24),IF(90>J80,((-0.0006*J80^2 + 0.0699*J80 - 1.2225)*Radiation!J24),0))))","v":0},{"$f":"IF(DW80<0,0,IF(0>K80,0,IF(50>K80,(( -0.000009*K80^2 + 0.0004*K80 + 0.7918)*Radiation!K24),IF(90>K80,((-0.0006*K80^2 + 0.0699*K80 - 1.2225)*Radiation!K24),0))))","v":0},{"$f":"IF(DX80<0,0,IF(0>L80,0,IF(50>L80,(( -0.000009*L80^2 + 0.0004*L80 + 0.7918)*Radiation!L24),IF(90>L80,((-0.0006*L80^2 + 0.0699*L80 - 1.2225)*Radiation!L24),0))))","v":0},{"$f":"IF(DY80<0,0,IF(0>M80,0,IF(50>M80,(( -0.000009*M80^2 + 0.0004*M80 + 0.7918)*Radiation!M24),IF(90>M80,((-0.0006*M80^2 + 0.0699*M80 - 1.2225)*Radiation!M24),0))))","v":0},{"$f":"IF(DZ80<0,0,IF(0>N80,0,IF(50>N80,(( -0.000009*N80^2 + 0.0004*N80 + 0.7918)*Radiation!N24),IF(90>N80,((-0.0006*N80^2 + 0.0699*N80 - 1.2225)*Radiation!N24),0))))","v":0},null,21,{"$f":"IF(EC80<0,0,IF(0>Q80,0,IF(50>Q80,(( -0.000009*Q80^2 + 0.0004*Q80 + 0.7918)*Radiation!C24),IF(90>Q80,((-0.0006*Q80^2 + 0.0699*Q80 - 1.2225)*Radiation!C24),0))))","v":0},{"$f":"IF(ED80<0,0,IF(0>R80,0,IF(50>R80,(( -0.000009*R80^2 + 0.0004*R80 + 0.7918)*Radiation!D24),IF(90>R80,((-0.0006*R80^2 + 0.0699*R80 - 1.2225)*Radiation!D24),0))))","v":0},{"$f":"IF(EE80<0,0,IF(0>S80,0,IF(50>S80,(( -0.000009*S80^2 + 0.0004*S80 + 0.7918)*Radiation!E24),IF(90>S80,((-0.0006*S80^2 + 0.0699*S80 - 1.2225)*Radiation!E24),0))))","v":0},{"$f":"IF(EF80<0,0,IF(0>T80,0,IF(50>T80,(( -0.000009*T80^2 + 0.0004*T80 + 0.7918)*Radiation!F24),IF(90>T80,((-0.0006*T80^2 + 0.0699*T80 - 1.2225)*Radiation!F24),0))))","v":0},{"$f":"IF(EG80<0,0,IF(0>U80,0,IF(50>U80,(( -0.000009*U80^2 + 0.0004*U80 + 0.7918)*Radiation!G24),IF(90>U80,((-0.0006*U80^2 + 0.0699*U80 - 1.2225)*Radiation!G24),0))))","v":0},{"$f":"IF(EH80<0,0,IF(0>V80,0,IF(50>V80,(( -0.000009*V80^2 + 0.0004*V80 + 0.7918)*Radiation!H24),IF(90>V80,((-0.0006*V80^2 + 0.0699*V80 - 1.2225)*Radiation!H24),0))))","v":0},{"$f":"IF(EI80<0,0,IF(0>W80,0,IF(50>W80,(( -0.000009*W80^2 + 0.0004*W80 + 0.7918)*Radiation!I24),IF(90>W80,((-0.0006*W80^2 + 0.0699*W80 - 1.2225)*Radiation!I24),0))))","v":0},{"$f":"IF(EJ80<0,0,IF(0>X80,0,IF(50>X80,(( -0.000009*X80^2 + 0.0004*X80 + 0.7918)*Radiation!J24),IF(90>X80,((-0.0006*X80^2 + 0.0699*X80 - 1.2225)*Radiation!J24),0))))","v":0},{"$f":"IF(EK80<0,0,IF(0>Y80,0,IF(50>Y80,(( -0.000009*Y80^2 + 0.0004*Y80 + 0.7918)*Radiation!K24),IF(90>Y80,((-0.0006*Y80^2 + 0.0699*Y80 - 1.2225)*Radiation!K24),0))))","v":0},{"$f":"IF(EL80<0,0,IF(0>Z80,0,IF(50>Z80,(( -0.000009*Z80^2 + 0.0004*Z80 + 0.7918)*Radiation!L24),IF(90>Z80,((-0.0006*Z80^2 + 0.0699*Z80 - 1.2225)*Radiation!L24),0))))","v":0},{"$f":"IF(EM80<0,0,IF(0>AA80,0,IF(50>AA80,(( -0.000009*AA80^2 + 0.0004*AA80 + 0.7918)*Radiation!M24),IF(90>AA80,((-0.0006*AA80^2 + 0.0699*AA80 - 1.2225)*Radiation!M24),0))))","v":0},{"$f":"IF(EN80<0,0,IF(0>AB80,0,IF(50>AB80,(( -0.000009*AB80^2 + 0.0004*AB80 + 0.7918)*Radiation!N24),IF(90>AB80,((-0.0006*AB80^2 + 0.0699*AB80 - 1.2225)*Radiation!N24),0))))","v":0},null,null,21,{"$f":"AG80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU52","v":0},{"$f":"AH80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV52","v":0},{"$f":"AI80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW52","v":0},{"$f":"AJ80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX52","v":0},{"$f":"AK80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY52","v":0},{"$f":"AL80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ52","v":0},{"$f":"AM80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA52","v":0},{"$f":"AN80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB52","v":0},{"$f":"AO80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC52","v":0},{"$f":"AP80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD52","v":0},{"$f":"AQ80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE52","v":0},{"$f":"AR80*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF52","v":0},null,21,{"$f":"AU80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI52","v":0},{"$f":"AV80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ52","v":0},{"$f":"AW80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK52","v":0},{"$f":"AX80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL52","v":0},{"$f":"AY80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM52","v":0},{"$f":"AZ80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN52","v":0},{"$f":"BA80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO52","v":0},{"$f":"BB80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP52","v":0},{"$f":"BC80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ52","v":0},{"$f":"BD80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR52","v":0},{"$f":"BE80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS52","v":0},{"$f":"BF80*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT52","v":0},null,21,0,0,0,0,0,0,0,0,0,0,0,0,null,21,0,0,0,0,0,0,0,0,0,0,0,0,null,null,21,-44.11375465474292,-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762,null,21,-44.11375465474292,-40.375142281624065,-36.877998514340369,-31.713766855869693,-26.575515215416551,-23.623016903493113,-24.79570873532365,-30.92280247893752,-40.048756889246128,-46.985407153208357,-49.782532508401836,-47.837496220337762]
[null,22,{"$f":"DEGREES(C109)","v":57.743424902720662},55.429966762771876,56.341666666666704,59.243479873249605,61.153562517113642,60.793335174423376,59.021941915541987,58.420422229010185,60.091666666666704,62.593599483994502,63.495948618921908,61.461417100099801,null,22,{"$f":"DEGREES(Q109)","v":89.18349157577498},80.312835430181281,69.646286446366432,57.592295680443918,49.36216143655561,46.672388870306328,49.820832576886225,57.623378382800993,68.763568929500451,78.808778956009832,87.90209782845865,91.963852768882518,null,null,null,22,{"$f":"IF(DO81<0,0,IF(0>C81,0,IF(50>C81,(( -0.000009*C81^2 + 0.0004*C81 + 0.7918)*Radiation!C25),IF(90>C81,((-0.0006*C81^2 + 0.0699*C81 - 1.2225)*Radiation!C25),0))))","v":0},{"$f":"IF(DP81<0,0,IF(0>D81,0,IF(50>D81,(( -0.000009*D81^2 + 0.0004*D81 + 0.7918)*Radiation!D25),IF(90>D81,((-0.0006*D81^2 + 0.0699*D81 - 1.2225)*Radiation!D25),0))))","v":0},{"$f":"IF(DQ81<0,0,IF(0>E81,0,IF(50>E81,(( -0.000009*E81^2 + 0.0004*E81 + 0.7918)*Radiation!E25),IF(90>E81,((-0.0006*E81^2 + 0.0699*E81 - 1.2225)*Radiation!E25),0))))","v":0},{"$f":"IF(DR81<0,0,IF(0>F81,0,IF(50>F81,(( -0.000009*F81^2 + 0.0004*F81 + 0.7918)*Radiation!F25),IF(90>F81,((-0.0006*F81^2 + 0.0699*F81 - 1.2225)*Radiation!F25),0))))","v":0},{"$f":"IF(DS81<0,0,IF(0>G81,0,IF(50>G81,(( -0.000009*G81^2 + 0.0004*G81 + 0.7918)*Radiation!G25),IF(90>G81,((-0.0006*G81^2 + 0.0699*G81 - 1.2225)*Radiation!G25),0))))","v":0},{"$f":"IF(DT81<0,0,IF(0>H81,0,IF(50>H81,(( -0.000009*H81^2 + 0.0004*H81 + 0.7918)*Radiation!H25),IF(90>H81,((-0.0006*H81^2 + 0.0699*H81 - 1.2225)*Radiation!H25),0))))","v":0},{"$f":"IF(DU81<0,0,IF(0>I81,0,IF(50>I81,(( -0.000009*I81^2 + 0.0004*I81 + 0.7918)*Radiation!I25),IF(90>I81,((-0.0006*I81^2 + 0.0699*I81 - 1.2225)*Radiation!I25),0))))","v":0},{"$f":"IF(DV81<0,0,IF(0>J81,0,IF(50>J81,(( -0.000009*J81^2 + 0.0004*J81 + 0.7918)*Radiation!J25),IF(90>J81,((-0.0006*J81^2 + 0.0699*J81 - 1.2225)*Radiation!J25),0))))","v":0},{"$f":"IF(DW81<0,0,IF(0>K81,0,IF(50>K81,(( -0.000009*K81^2 + 0.0004*K81 + 0.7918)*Radiation!K25),IF(90>K81,((-0.0006*K81^2 + 0.0699*K81 - 1.2225)*Radiation!K25),0))))","v":0},{"$f":"IF(DX81<0,0,IF(0>L81,0,IF(50>L81,(( -0.000009*L81^2 + 0.0004*L81 + 0.7918)*Radiation!L25),IF(90>L81,((-0.0006*L81^2 + 0.0699*L81 - 1.2225)*Radiation!L25),0))))","v":0},{"$f":"IF(DY81<0,0,IF(0>M81,0,IF(50>M81,(( -0.000009*M81^2 + 0.0004*M81 + 0.7918)*Radiation!M25),IF(90>M81,((-0.0006*M81^2 + 0.0699*M81 - 1.2225)*Radiation!M25),0))))","v":0},{"$f":"IF(DZ81<0,0,IF(0>N81,0,IF(50>N81,(( -0.000009*N81^2 + 0.0004*N81 + 0.7918)*Radiation!N25),IF(90>N81,((-0.0006*N81^2 + 0.0699*N81 - 1.2225)*Radiation!N25),0))))","v":0},null,22,{"$f":"IF(EC81<0,0,IF(0>Q81,0,IF(50>Q81,(( -0.000009*Q81^2 + 0.0004*Q81 + 0.7918)*Radiation!C25),IF(90>Q81,((-0.0006*Q81^2 + 0.0699*Q81 - 1.2225)*Radiation!C25),0))))","v":0},{"$f":"IF(ED81<0,0,IF(0>R81,0,IF(50>R81,(( -0.000009*R81^2 + 0.0004*R81 + 0.7918)*Radiation!D25),IF(90>R81,((-0.0006*R81^2 + 0.0699*R81 - 1.2225)*Radiation!D25),0))))","v":0},{"$f":"IF(EE81<0,0,IF(0>S81,0,IF(50>S81,(( -0.000009*S81^2 + 0.0004*S81 + 0.7918)*Radiation!E25),IF(90>S81,((-0.0006*S81^2 + 0.0699*S81 - 1.2225)*Radiation!E25),0))))","v":0},{"$f":"IF(EF81<0,0,IF(0>T81,0,IF(50>T81,(( -0.000009*T81^2 + 0.0004*T81 + 0.7918)*Radiation!F25),IF(90>T81,((-0.0006*T81^2 + 0.0699*T81 - 1.2225)*Radiation!F25),0))))","v":0},{"$f":"IF(EG81<0,0,IF(0>U81,0,IF(50>U81,(( -0.000009*U81^2 + 0.0004*U81 + 0.7918)*Radiation!G25),IF(90>U81,((-0.0006*U81^2 + 0.0699*U81 - 1.2225)*Radiation!G25),0))))","v":0},{"$f":"IF(EH81<0,0,IF(0>V81,0,IF(50>V81,(( -0.000009*V81^2 + 0.0004*V81 + 0.7918)*Radiation!H25),IF(90>V81,((-0.0006*V81^2 + 0.0699*V81 - 1.2225)*Radiation!H25),0))))","v":0},{"$f":"IF(EI81<0,0,IF(0>W81,0,IF(50>W81,(( -0.000009*W81^2 + 0.0004*W81 + 0.7918)*Radiation!I25),IF(90>W81,((-0.0006*W81^2 + 0.0699*W81 - 1.2225)*Radiation!I25),0))))","v":0},{"$f":"IF(EJ81<0,0,IF(0>X81,0,IF(50>X81,(( -0.000009*X81^2 + 0.0004*X81 + 0.7918)*Radiation!J25),IF(90>X81,((-0.0006*X81^2 + 0.0699*X81 - 1.2225)*Radiation!J25),0))))","v":0},{"$f":"IF(EK81<0,0,IF(0>Y81,0,IF(50>Y81,(( -0.000009*Y81^2 + 0.0004*Y81 + 0.7918)*Radiation!K25),IF(90>Y81,((-0.0006*Y81^2 + 0.0699*Y81 - 1.2225)*Radiation!K25),0))))","v":0},{"$f":"IF(EL81<0,0,IF(0>Z81,0,IF(50>Z81,(( -0.000009*Z81^2 + 0.0004*Z81 + 0.7918)*Radiation!L25),IF(90>Z81,((-0.0006*Z81^2 + 0.0699*Z81 - 1.2225)*Radiation!L25),0))))","v":0},{"$f":"IF(EM81<0,0,IF(0>AA81,0,IF(50>AA81,(( -0.000009*AA81^2 + 0.0004*AA81 + 0.7918)*Radiation!M25),IF(90>AA81,((-0.0006*AA81^2 + 0.0699*AA81 - 1.2225)*Radiation!M25),0))))","v":0},{"$f":"IF(EN81<0,0,IF(0>AB81,0,IF(50>AB81,(( -0.000009*AB81^2 + 0.0004*AB81 + 0.7918)*Radiation!N25),IF(90>AB81,((-0.0006*AB81^2 + 0.0699*AB81 - 1.2225)*Radiation!N25),0))))","v":0},null,null,22,{"$f":"AG81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU53","v":0},{"$f":"AH81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV53","v":0},{"$f":"AI81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW53","v":0},{"$f":"AJ81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX53","v":0},{"$f":"AK81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY53","v":0},{"$f":"AL81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ53","v":0},{"$f":"AM81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA53","v":0},{"$f":"AN81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB53","v":0},{"$f":"AO81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC53","v":0},{"$f":"AP81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD53","v":0},{"$f":"AQ81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE53","v":0},{"$f":"AR81*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF53","v":0},null,22,{"$f":"AU81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI53","v":0},{"$f":"AV81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ53","v":0},{"$f":"AW81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK53","v":0},{"$f":"AX81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL53","v":0},{"$f":"AY81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM53","v":0},{"$f":"AZ81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN53","v":0},{"$f":"BA81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO53","v":0},{"$f":"BB81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP53","v":0},{"$f":"BC81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ53","v":0},{"$f":"BD81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR53","v":0},{"$f":"BE81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS53","v":0},{"$f":"BF81*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT53","v":0},null,22,0,0,0,0,0,0,0,0,0,0,0,0,null,22,0,0,0,0,0,0,0,0,0,0,0,0,null,null,22,-57.730536859646747,-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132,null,22,-57.730536859646747,-53.7124665497957,-49.130640449349315,-42.202232941267965,-35.853933091501311,-32.649969945256942,-34.377195915482893,-41.497131280000914,-51.954064465377563,-60.030194510304511,-63.399939655490947,-61.381330079855132]
[null,23,{"$f":"DEGREES(C110)","v":71.629318930407436},70.102116697385569,71.341666666666697,73.856260987432151,75.056789518420828,74.31996681307163,72.864928393304098,73.014741414299053,75.091666666666711,77.295335862594058,77.47618662363044,75.003133999442127,null,23,{"$f":"DEGREES(Q110)","v":86.505676751842842},77.396240998403499,66.677552060174648,54.593761761500758,46.211110655663596,43.29091697837746,46.393311160377472,54.523958369109877,66.183979517129771,76.614282505937013,85.808700220759377,89.641945769867107,null,null,null,23,{"$f":"IF(DO82<0,0,IF(0>C82,0,IF(50>C82,(( -0.000009*C82^2 + 0.0004*C82 + 0.7918)*Radiation!C26),IF(90>C82,((-0.0006*C82^2 + 0.0699*C82 - 1.2225)*Radiation!C26),0))))","v":0},{"$f":"IF(DP82<0,0,IF(0>D82,0,IF(50>D82,(( -0.000009*D82^2 + 0.0004*D82 + 0.7918)*Radiation!D26),IF(90>D82,((-0.0006*D82^2 + 0.0699*D82 - 1.2225)*Radiation!D26),0))))","v":0},{"$f":"IF(DQ82<0,0,IF(0>E82,0,IF(50>E82,(( -0.000009*E82^2 + 0.0004*E82 + 0.7918)*Radiation!E26),IF(90>E82,((-0.0006*E82^2 + 0.0699*E82 - 1.2225)*Radiation!E26),0))))","v":0},{"$f":"IF(DR82<0,0,IF(0>F82,0,IF(50>F82,(( -0.000009*F82^2 + 0.0004*F82 + 0.7918)*Radiation!F26),IF(90>F82,((-0.0006*F82^2 + 0.0699*F82 - 1.2225)*Radiation!F26),0))))","v":0},{"$f":"IF(DS82<0,0,IF(0>G82,0,IF(50>G82,(( -0.000009*G82^2 + 0.0004*G82 + 0.7918)*Radiation!G26),IF(90>G82,((-0.0006*G82^2 + 0.0699*G82 - 1.2225)*Radiation!G26),0))))","v":0},{"$f":"IF(DT82<0,0,IF(0>H82,0,IF(50>H82,(( -0.000009*H82^2 + 0.0004*H82 + 0.7918)*Radiation!H26),IF(90>H82,((-0.0006*H82^2 + 0.0699*H82 - 1.2225)*Radiation!H26),0))))","v":0},{"$f":"IF(DU82<0,0,IF(0>I82,0,IF(50>I82,(( -0.000009*I82^2 + 0.0004*I82 + 0.7918)*Radiation!I26),IF(90>I82,((-0.0006*I82^2 + 0.0699*I82 - 1.2225)*Radiation!I26),0))))","v":0},{"$f":"IF(DV82<0,0,IF(0>J82,0,IF(50>J82,(( -0.000009*J82^2 + 0.0004*J82 + 0.7918)*Radiation!J26),IF(90>J82,((-0.0006*J82^2 + 0.0699*J82 - 1.2225)*Radiation!J26),0))))","v":0},{"$f":"IF(DW82<0,0,IF(0>K82,0,IF(50>K82,(( -0.000009*K82^2 + 0.0004*K82 + 0.7918)*Radiation!K26),IF(90>K82,((-0.0006*K82^2 + 0.0699*K82 - 1.2225)*Radiation!K26),0))))","v":0},{"$f":"IF(DX82<0,0,IF(0>L82,0,IF(50>L82,(( -0.000009*L82^2 + 0.0004*L82 + 0.7918)*Radiation!L26),IF(90>L82,((-0.0006*L82^2 + 0.0699*L82 - 1.2225)*Radiation!L26),0))))","v":0},{"$f":"IF(DY82<0,0,IF(0>M82,0,IF(50>M82,(( -0.000009*M82^2 + 0.0004*M82 + 0.7918)*Radiation!M26),IF(90>M82,((-0.0006*M82^2 + 0.0699*M82 - 1.2225)*Radiation!M26),0))))","v":0},{"$f":"IF(DZ82<0,0,IF(0>N82,0,IF(50>N82,(( -0.000009*N82^2 + 0.0004*N82 + 0.7918)*Radiation!N26),IF(90>N82,((-0.0006*N82^2 + 0.0699*N82 - 1.2225)*Radiation!N26),0))))","v":0},null,23,{"$f":"IF(EC82<0,0,IF(0>Q82,0,IF(50>Q82,(( -0.000009*Q82^2 + 0.0004*Q82 + 0.7918)*Radiation!C26),IF(90>Q82,((-0.0006*Q82^2 + 0.0699*Q82 - 1.2225)*Radiation!C26),0))))","v":0},{"$f":"IF(ED82<0,0,IF(0>R82,0,IF(50>R82,(( -0.000009*R82^2 + 0.0004*R82 + 0.7918)*Radiation!D26),IF(90>R82,((-0.0006*R82^2 + 0.0699*R82 - 1.2225)*Radiation!D26),0))))","v":0},{"$f":"IF(EE82<0,0,IF(0>S82,0,IF(50>S82,(( -0.000009*S82^2 + 0.0004*S82 + 0.7918)*Radiation!E26),IF(90>S82,((-0.0006*S82^2 + 0.0699*S82 - 1.2225)*Radiation!E26),0))))","v":0},{"$f":"IF(EF82<0,0,IF(0>T82,0,IF(50>T82,(( -0.000009*T82^2 + 0.0004*T82 + 0.7918)*Radiation!F26),IF(90>T82,((-0.0006*T82^2 + 0.0699*T82 - 1.2225)*Radiation!F26),0))))","v":0},{"$f":"IF(EG82<0,0,IF(0>U82,0,IF(50>U82,(( -0.000009*U82^2 + 0.0004*U82 + 0.7918)*Radiation!G26),IF(90>U82,((-0.0006*U82^2 + 0.0699*U82 - 1.2225)*Radiation!G26),0))))","v":0},{"$f":"IF(EH82<0,0,IF(0>V82,0,IF(50>V82,(( -0.000009*V82^2 + 0.0004*V82 + 0.7918)*Radiation!H26),IF(90>V82,((-0.0006*V82^2 + 0.0699*V82 - 1.2225)*Radiation!H26),0))))","v":0},{"$f":"IF(EI82<0,0,IF(0>W82,0,IF(50>W82,(( -0.000009*W82^2 + 0.0004*W82 + 0.7918)*Radiation!I26),IF(90>W82,((-0.0006*W82^2 + 0.0699*W82 - 1.2225)*Radiation!I26),0))))","v":0},{"$f":"IF(EJ82<0,0,IF(0>X82,0,IF(50>X82,(( -0.000009*X82^2 + 0.0004*X82 + 0.7918)*Radiation!J26),IF(90>X82,((-0.0006*X82^2 + 0.0699*X82 - 1.2225)*Radiation!J26),0))))","v":0},{"$f":"IF(EK82<0,0,IF(0>Y82,0,IF(50>Y82,(( -0.000009*Y82^2 + 0.0004*Y82 + 0.7918)*Radiation!K26),IF(90>Y82,((-0.0006*Y82^2 + 0.0699*Y82 - 1.2225)*Radiation!K26),0))))","v":0},{"$f":"IF(EL82<0,0,IF(0>Z82,0,IF(50>Z82,(( -0.000009*Z82^2 + 0.0004*Z82 + 0.7918)*Radiation!L26),IF(90>Z82,((-0.0006*Z82^2 + 0.0699*Z82 - 1.2225)*Radiation!L26),0))))","v":0},{"$f":"IF(EM82<0,0,IF(0>AA82,0,IF(50>AA82,(( -0.000009*AA82^2 + 0.0004*AA82 + 0.7918)*Radiation!M26),IF(90>AA82,((-0.0006*AA82^2 + 0.0699*AA82 - 1.2225)*Radiation!M26),0))))","v":0},{"$f":"IF(EN82<0,0,IF(0>AB82,0,IF(50>AB82,(( -0.000009*AB82^2 + 0.0004*AB82 + 0.7918)*Radiation!N26),IF(90>AB82,((-0.0006*AB82^2 + 0.0699*AB82 - 1.2225)*Radiation!N26),0))))","v":0},null,null,23,{"$f":"AG82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU54","v":0},{"$f":"AH82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV54","v":0},{"$f":"AI82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW54","v":0},{"$f":"AJ82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX54","v":0},{"$f":"AK82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY54","v":0},{"$f":"AL82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ54","v":0},{"$f":"AM82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA54","v":0},{"$f":"AN82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB54","v":0},{"$f":"AO82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC54","v":0},{"$f":"AP82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD54","v":0},{"$f":"AQ82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE54","v":0},{"$f":"AR82*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF54","v":0},null,23,{"$f":"AU82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI54","v":0},{"$f":"AV82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ54","v":0},{"$f":"AW82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK54","v":0},{"$f":"AX82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL54","v":0},{"$f":"AY82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM54","v":0},{"$f":"AZ82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN54","v":0},{"$f":"BA82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO54","v":0},{"$f":"BB82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP54","v":0},{"$f":"BC82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ54","v":0},{"$f":"BD82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR54","v":0},{"$f":"BE82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS54","v":0},{"$f":"BF82*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT54","v":0},null,23,0,0,0,0,0,0,0,0,0,0,0,0,null,23,0,0,0,0,0,0,0,0,0,0,0,0,null,null,23,-71.276413671366612,-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272,null,23,-71.276413671366612,-66.153465993410151,-59.402009530792824,-50.011386554405469,-42.39742803240717,-39.064492418979341,-41.409864595350896,-49.478233796277678,-61.393251168859493,-71.378499679687209,-76.771747562226409,-74.998658692112272]
[null,24,{"$f":"DEGREES(C111)","v":85.69087979217116},84.831644602709105,86.341666666666839,88.524089531336969,89.10119481580432,88.042935221045781,86.877975633580505,87.669646168259078,89.908333333336003,87.969282074498523,88.432878734944595,88.730938878386283,null,24,{"$f":"DEGREES(Q111)","v":85.272240491883181},76.002091710358854,65.353688610771755,53.410110546849175,45.004441791451981,41.872812550461703,44.853819434419648,53.225285791219626,65.300033727131805,76.015770399929167,85.209557319861261,88.75640299740472,null,null,null,24,{"$f":"IF(DO83<0,0,IF(0>C83,0,IF(50>C83,(( -0.000009*C83^2 + 0.0004*C83 + 0.7918)*Radiation!C27),IF(90>C83,((-0.0006*C83^2 + 0.0699*C83 - 1.2225)*Radiation!C27),0))))","v":0},{"$f":"IF(DP83<0,0,IF(0>D83,0,IF(50>D83,(( -0.000009*D83^2 + 0.0004*D83 + 0.7918)*Radiation!D27),IF(90>D83,((-0.0006*D83^2 + 0.0699*D83 - 1.2225)*Radiation!D27),0))))","v":0},{"$f":"IF(DQ83<0,0,IF(0>E83,0,IF(50>E83,(( -0.000009*E83^2 + 0.0004*E83 + 0.7918)*Radiation!E27),IF(90>E83,((-0.0006*E83^2 + 0.0699*E83 - 1.2225)*Radiation!E27),0))))","v":0},{"$f":"IF(DR83<0,0,IF(0>F83,0,IF(50>F83,(( -0.000009*F83^2 + 0.0004*F83 + 0.7918)*Radiation!F27),IF(90>F83,((-0.0006*F83^2 + 0.0699*F83 - 1.2225)*Radiation!F27),0))))","v":0},{"$f":"IF(DS83<0,0,IF(0>G83,0,IF(50>G83,(( -0.000009*G83^2 + 0.0004*G83 + 0.7918)*Radiation!G27),IF(90>G83,((-0.0006*G83^2 + 0.0699*G83 - 1.2225)*Radiation!G27),0))))","v":0},{"$f":"IF(DT83<0,0,IF(0>H83,0,IF(50>H83,(( -0.000009*H83^2 + 0.0004*H83 + 0.7918)*Radiation!H27),IF(90>H83,((-0.0006*H83^2 + 0.0699*H83 - 1.2225)*Radiation!H27),0))))","v":0},{"$f":"IF(DU83<0,0,IF(0>I83,0,IF(50>I83,(( -0.000009*I83^2 + 0.0004*I83 + 0.7918)*Radiation!I27),IF(90>I83,((-0.0006*I83^2 + 0.0699*I83 - 1.2225)*Radiation!I27),0))))","v":0},{"$f":"IF(DV83<0,0,IF(0>J83,0,IF(50>J83,(( -0.000009*J83^2 + 0.0004*J83 + 0.7918)*Radiation!J27),IF(90>J83,((-0.0006*J83^2 + 0.0699*J83 - 1.2225)*Radiation!J27),0))))","v":0},{"$f":"IF(DW83<0,0,IF(0>K83,0,IF(50>K83,(( -0.000009*K83^2 + 0.0004*K83 + 0.7918)*Radiation!K27),IF(90>K83,((-0.0006*K83^2 + 0.0699*K83 - 1.2225)*Radiation!K27),0))))","v":0},{"$f":"IF(DX83<0,0,IF(0>L83,0,IF(50>L83,(( -0.000009*L83^2 + 0.0004*L83 + 0.7918)*Radiation!L27),IF(90>L83,((-0.0006*L83^2 + 0.0699*L83 - 1.2225)*Radiation!L27),0))))","v":0},{"$f":"IF(DY83<0,0,IF(0>M83,0,IF(50>M83,(( -0.000009*M83^2 + 0.0004*M83 + 0.7918)*Radiation!M27),IF(90>M83,((-0.0006*M83^2 + 0.0699*M83 - 1.2225)*Radiation!M27),0))))","v":0},{"$f":"IF(DZ83<0,0,IF(0>N83,0,IF(50>N83,(( -0.000009*N83^2 + 0.0004*N83 + 0.7918)*Radiation!N27),IF(90>N83,((-0.0006*N83^2 + 0.0699*N83 - 1.2225)*Radiation!N27),0))))","v":0},null,24,{"$f":"IF(EC83<0,0,IF(0>Q83,0,IF(50>Q83,(( -0.000009*Q83^2 + 0.0004*Q83 + 0.7918)*Radiation!C27),IF(90>Q83,((-0.0006*Q83^2 + 0.0699*Q83 - 1.2225)*Radiation!C27),0))))","v":0},{"$f":"IF(ED83<0,0,IF(0>R83,0,IF(50>R83,(( -0.000009*R83^2 + 0.0004*R83 + 0.7918)*Radiation!D27),IF(90>R83,((-0.0006*R83^2 + 0.0699*R83 - 1.2225)*Radiation!D27),0))))","v":0},{"$f":"IF(EE83<0,0,IF(0>S83,0,IF(50>S83,(( -0.000009*S83^2 + 0.0004*S83 + 0.7918)*Radiation!E27),IF(90>S83,((-0.0006*S83^2 + 0.0699*S83 - 1.2225)*Radiation!E27),0))))","v":0},{"$f":"IF(EF83<0,0,IF(0>T83,0,IF(50>T83,(( -0.000009*T83^2 + 0.0004*T83 + 0.7918)*Radiation!F27),IF(90>T83,((-0.0006*T83^2 + 0.0699*T83 - 1.2225)*Radiation!F27),0))))","v":0},{"$f":"IF(EG83<0,0,IF(0>U83,0,IF(50>U83,(( -0.000009*U83^2 + 0.0004*U83 + 0.7918)*Radiation!G27),IF(90>U83,((-0.0006*U83^2 + 0.0699*U83 - 1.2225)*Radiation!G27),0))))","v":0},{"$f":"IF(EH83<0,0,IF(0>V83,0,IF(50>V83,(( -0.000009*V83^2 + 0.0004*V83 + 0.7918)*Radiation!H27),IF(90>V83,((-0.0006*V83^2 + 0.0699*V83 - 1.2225)*Radiation!H27),0))))","v":0},{"$f":"IF(EI83<0,0,IF(0>W83,0,IF(50>W83,(( -0.000009*W83^2 + 0.0004*W83 + 0.7918)*Radiation!I27),IF(90>W83,((-0.0006*W83^2 + 0.0699*W83 - 1.2225)*Radiation!I27),0))))","v":0},{"$f":"IF(EJ83<0,0,IF(0>X83,0,IF(50>X83,(( -0.000009*X83^2 + 0.0004*X83 + 0.7918)*Radiation!J27),IF(90>X83,((-0.0006*X83^2 + 0.0699*X83 - 1.2225)*Radiation!J27),0))))","v":0},{"$f":"IF(EK83<0,0,IF(0>Y83,0,IF(50>Y83,(( -0.000009*Y83^2 + 0.0004*Y83 + 0.7918)*Radiation!K27),IF(90>Y83,((-0.0006*Y83^2 + 0.0699*Y83 - 1.2225)*Radiation!K27),0))))","v":0},{"$f":"IF(EL83<0,0,IF(0>Z83,0,IF(50>Z83,(( -0.000009*Z83^2 + 0.0004*Z83 + 0.7918)*Radiation!L27),IF(90>Z83,((-0.0006*Z83^2 + 0.0699*Z83 - 1.2225)*Radiation!L27),0))))","v":0},{"$f":"IF(EM83<0,0,IF(0>AA83,0,IF(50>AA83,(( -0.000009*AA83^2 + 0.0004*AA83 + 0.7918)*Radiation!M27),IF(90>AA83,((-0.0006*AA83^2 + 0.0699*AA83 - 1.2225)*Radiation!M27),0))))","v":0},{"$f":"IF(EN83<0,0,IF(0>AB83,0,IF(50>AB83,(( -0.000009*AB83^2 + 0.0004*AB83 + 0.7918)*Radiation!N27),IF(90>AB83,((-0.0006*AB83^2 + 0.0699*AB83 - 1.2225)*Radiation!N27),0))))","v":0},null,null,24,{"$f":"AG83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CU55","v":0},{"$f":"AH83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CV55","v":0},{"$f":"AI83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CW55","v":0},{"$f":"AJ83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CX55","v":0},{"$f":"AK83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CY55","v":0},{"$f":"AL83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!CZ55","v":0},{"$f":"AM83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DA55","v":0},{"$f":"AN83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DB55","v":0},{"$f":"AO83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DC55","v":0},{"$f":"AP83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DD55","v":0},{"$f":"AQ83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DE55","v":0},{"$f":"AR83*'Input Data'!$F$38*'Input Data'!$F$39*'Operative BP'!DF55","v":0},null,24,{"$f":"AU83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DI55","v":0},{"$f":"AV83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DJ55","v":0},{"$f":"AW83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DK55","v":0},{"$f":"AX83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DL55","v":0},{"$f":"AY83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DM55","v":0},{"$f":"AZ83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DN55","v":0},{"$f":"BA83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DO55","v":0},{"$f":"BB83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DP55","v":0},{"$f":"BC83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DQ55","v":0},{"$f":"BD83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DR55","v":0},{"$f":"BE83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DS55","v":0},{"$f":"BF83*'Input Data'!$F$29*'Input Data'!$F$30*'Operative BP'!DT55","v":0},null,24,0,0,0,0,0,0,0,0,0,0,0,0,null,24,0,0,0,0,0,0,0,0,0,0,0,0,null,null,24,-83.596484892158756,-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205,null,24,-83.596484892158756,-75.041691580826409,-65.047371814417531,-53.370409687127484,-44.990343292174892,-41.805581832384377,-44.683864079458822,-53.126563822663151,-65.299840573859427,-75.863131931954825,-84.958601709687045,-88.223048770244205]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T",{"$f":"SUM(BJ60:BJ83)","v":6292.4176297343747},9075.3604987034851,11392.510088435487,12120.337200300164,12871.705782182682,12736.914829457035,12941.695440413661,14523.808429047351,12585.028147953524,10453.427604214963,6804.4109146489154,5056.2898816256784,null,"T",{"$f":"SUM(BX60:BX83)","v":0},0,0,0,0,0,0,0,0,0,0,0,null,"T",0.25554218854995925,0.552945977389245,0.6220282264759458,0.58997297021880635,0.59796483775241493,0.57971275154795043,0.58928512251789056,0.60380661672683134,0.60215431652788975,0.54737569761589777,0.25414646870395091,0.21104511739393619,null,"T",0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Max Tons",{"$f":"(MAX(BJ60:BJ83))*0.000083333","v":0.23121819499587998},{"$f":"(MAX(BK60:BK83))*0.000083333","v":0.3112143634052979},0.37056598196260948,0.3978604830864052,0.4142777919945736,0.40025073366172048,0.41075840215898585,0.46853067171163132,0.43253638364591834,0.33853616822594018,0.23163264570255551,0.1803587647564367,null,"Max Tons",{"$f":"(MAX(BX60:BX83))*0.000083333","v":0},{"$f":"(MAX(BY60:BY83))*0.000083333","v":0},0,0,0,0,0,0,0,0,0,0]
[]
[null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"ACOS((COS('Solar Altitude'!C31)*COS('Surface Solar Azimuth Angles'!C85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C31)*COS('Input Data'!$G$14)))","v":1.7416351562791899},{"$f":"ACOS((COS('Solar Altitude'!D31)*COS('Surface Solar Azimuth Angles'!D85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D31)*COS('Input Data'!$G$14)))","v":1.7378915288489074},{"$f":"ACOS((COS('Solar Altitude'!E31)*COS('Surface Solar Azimuth Angles'!E85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E31)*COS('Input Data'!$G$14)))","v":1.7687457527919206},{"$f":"ACOS((COS('Solar Altitude'!F31)*COS('Surface Solar Azimuth Angles'!F85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F31)*COS('Input Data'!$G$14)))","v":1.8011172639919035},{"$f":"ACOS((COS('Solar Altitude'!G31)*COS('Surface Solar Azimuth Angles'!G85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G31)*COS('Input Data'!$G$14)))","v":1.8003650689598567},{"$f":"ACOS((COS('Solar Altitude'!H31)*COS('Surface Solar Azimuth Angles'!H85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H31)*COS('Input Data'!$G$14)))","v":1.7765357913990432},{"$f":"ACOS((COS('Solar Altitude'!I31)*COS('Surface Solar Azimuth Angles'!I85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I31)*COS('Input Data'!$G$14)))","v":1.761359166676689},{"$f":"ACOS((COS('Solar Altitude'!J31)*COS('Surface Solar Azimuth Angles'!J85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J31)*COS('Input Data'!$G$14)))","v":1.7860286239158989},{"$f":"ACOS((COS('Solar Altitude'!K31)*COS('Surface Solar Azimuth Angles'!K85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K31)*COS('Input Data'!$G$14)))","v":1.8341955997417065},{"$f":"ACOS((COS('Solar Altitude'!L31)*COS('Surface Solar Azimuth Angles'!L85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L31)*COS('Input Data'!$G$14)))","v":1.863332262478306},{"$f":"ACOS((COS('Solar Altitude'!M31)*COS('Surface Solar Azimuth Angles'!M85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M31)*COS('Input Data'!$G$14)))","v":1.8438546156573905},{"$f":"ACOS((COS('Solar Altitude'!N31)*COS('Surface Solar Azimuth Angles'!N85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N31)*COS('Input Data'!$G$14)))","v":1.7884923045306456},null,1,{"$f":"ACOS((COS('Solar Altitude'!C31)*COS('Surface Solar Azimuth Angles'!Q85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C31)*COS('Input Data'!$G$14)))","v":1.4935172588937768},{"$f":"ACOS((COS('Solar Altitude'!D31)*COS('Surface Solar Azimuth Angles'!R85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D31)*COS('Input Data'!$G$14)))","v":1.3308067796252714},{"$f":"ACOS((COS('Solar Altitude'!E31)*COS('Surface Solar Azimuth Angles'!S85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E31)*COS('Input Data'!$G$14)))","v":1.1486635652967694},{"$f":"ACOS((COS('Solar Altitude'!F31)*COS('Surface Solar Azimuth Angles'!T85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F31)*COS('Input Data'!$G$14)))","v":0.94598878931115771},{"$f":"ACOS((COS('Solar Altitude'!G31)*COS('Surface Solar Azimuth Angles'!U85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G31)*COS('Input Data'!$G$14)))","v":0.80182518366980837},{"$f":"ACOS((COS('Solar Altitude'!H31)*COS('Surface Solar Azimuth Angles'!V85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H31)*COS('Input Data'!$G$14)))","v":0.74473376667372659},{"$f":"ACOS((COS('Solar Altitude'!I31)*COS('Surface Solar Azimuth Angles'!W85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I31)*COS('Input Data'!$G$14)))","v":0.79331790156769921},{"$f":"ACOS((COS('Solar Altitude'!J31)*COS('Surface Solar Azimuth Angles'!X85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J31)*COS('Input Data'!$G$14)))","v":0.94078038027624522},{"$f":"ACOS((COS('Solar Altitude'!K31)*COS('Surface Solar Azimuth Angles'!Y85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K31)*COS('Input Data'!$G$14)))","v":1.1555065954580774},{"$f":"ACOS((COS('Solar Altitude'!L31)*COS('Surface Solar Azimuth Angles'!Z85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L31)*COS('Input Data'!$G$14)))","v":1.3450430248111578},{"$f":"ACOS((COS('Solar Altitude'!M31)*COS('Surface Solar Azimuth Angles'!AA85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M31)*COS('Input Data'!$G$14)))","v":1.5035744376480296},{"$f":"ACOS((COS('Solar Altitude'!N31)*COS('Surface Solar Azimuth Angles'!AB85)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N31)*COS('Input Data'!$G$14)))","v":1.5597563305208391}]
[null,2,{"$f":"ACOS((COS('Solar Altitude'!C32)*COS('Surface Solar Azimuth Angles'!C86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C32)*COS('Input Data'!$G$14)))","v":1.9862113337050011},{"$f":"ACOS((COS('Solar Altitude'!D32)*COS('Surface Solar Azimuth Angles'!D86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D32)*COS('Input Data'!$G$14)))","v":1.994770087278174},{"$f":"ACOS((COS('Solar Altitude'!E32)*COS('Surface Solar Azimuth Angles'!E86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E32)*COS('Input Data'!$G$14)))","v":2.0305451405910695},{"$f":"ACOS((COS('Solar Altitude'!F32)*COS('Surface Solar Azimuth Angles'!F86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F32)*COS('Input Data'!$G$14)))","v":2.0564415299998178},{"$f":"ACOS((COS('Solar Altitude'!G32)*COS('Surface Solar Azimuth Angles'!G86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G32)*COS('Input Data'!$G$14)))","v":2.0434987169607601},{"$f":"ACOS((COS('Solar Altitude'!H32)*COS('Surface Solar Azimuth Angles'!H86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H32)*COS('Input Data'!$G$14)))","v":2.0139721603127549},{"$f":"ACOS((COS('Solar Altitude'!I32)*COS('Surface Solar Azimuth Angles'!I86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I32)*COS('Input Data'!$G$14)))","v":2.0046578859970521},{"$f":"ACOS((COS('Solar Altitude'!J32)*COS('Surface Solar Azimuth Angles'!J86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J32)*COS('Input Data'!$G$14)))","v":2.0412100808805418},{"$f":"ACOS((COS('Solar Altitude'!K32)*COS('Surface Solar Azimuth Angles'!K86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K32)*COS('Input Data'!$G$14)))","v":2.0959949875408563},{"$f":"ACOS((COS('Solar Altitude'!L32)*COS('Surface Solar Azimuth Angles'!L86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L32)*COS('Input Data'!$G$14)))","v":2.1196090631829598},{"$f":"ACOS((COS('Solar Altitude'!M32)*COS('Surface Solar Azimuth Angles'!M86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M32)*COS('Input Data'!$G$14)))","v":2.0870542787182211},{"$f":"ACOS((COS('Solar Altitude'!N32)*COS('Surface Solar Azimuth Angles'!N86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N32)*COS('Input Data'!$G$14)))","v":2.0257156891845645},null,2,{"$f":"ACOS((COS('Solar Altitude'!C32)*COS('Surface Solar Azimuth Angles'!Q86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C32)*COS('Input Data'!$G$14)))","v":1.5251327124063025},{"$f":"ACOS((COS('Solar Altitude'!D32)*COS('Surface Solar Azimuth Angles'!R86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D32)*COS('Input Data'!$G$14)))","v":1.3634016755012737},{"$f":"ACOS((COS('Solar Altitude'!E32)*COS('Surface Solar Azimuth Angles'!S86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E32)*COS('Input Data'!$G$14)))","v":1.1869632041815481},{"$f":"ACOS((COS('Solar Altitude'!F32)*COS('Surface Solar Azimuth Angles'!T86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F32)*COS('Input Data'!$G$14)))","v":0.99237449200265382},{"$f":"ACOS((COS('Solar Altitude'!G32)*COS('Surface Solar Azimuth Angles'!U86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G32)*COS('Input Data'!$G$14)))","v":0.8528618934041361},{"$f":"ACOS((COS('Solar Altitude'!H32)*COS('Surface Solar Azimuth Angles'!V86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H32)*COS('Input Data'!$G$14)))","v":0.79478336888847245},{"$f":"ACOS((COS('Solar Altitude'!I32)*COS('Surface Solar Azimuth Angles'!W86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I32)*COS('Input Data'!$G$14)))","v":0.83936159076758599},{"$f":"ACOS((COS('Solar Altitude'!J32)*COS('Surface Solar Azimuth Angles'!X86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J32)*COS('Input Data'!$G$14)))","v":0.98546787266793823},{"$f":"ACOS((COS('Solar Altitude'!K32)*COS('Surface Solar Azimuth Angles'!Y86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K32)*COS('Input Data'!$G$14)))","v":1.200867827849103},{"$f":"ACOS((COS('Solar Altitude'!L32)*COS('Surface Solar Azimuth Angles'!Z86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L32)*COS('Input Data'!$G$14)))","v":1.3905450318456878},{"$f":"ACOS((COS('Solar Altitude'!M32)*COS('Surface Solar Azimuth Angles'!AA86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M32)*COS('Input Data'!$G$14)))","v":1.5456143814811076},{"$f":"ACOS((COS('Solar Altitude'!N32)*COS('Surface Solar Azimuth Angles'!AB86)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N32)*COS('Input Data'!$G$14)))","v":1.5958132177580575}]
[null,3,{"$f":"ACOS((COS('Solar Altitude'!C33)*COS('Surface Solar Azimuth Angles'!C87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C33)*COS('Input Data'!$G$14)))","v":2.2263871865236671},{"$f":"ACOS((COS('Solar Altitude'!D33)*COS('Surface Solar Azimuth Angles'!D87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D33)*COS('Input Data'!$G$14)))","v":2.2503131901111773},{"$f":"ACOS((COS('Solar Altitude'!E33)*COS('Surface Solar Azimuth Angles'!E87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E33)*COS('Input Data'!$G$14)))","v":2.2923445283902186},{"$f":"ACOS((COS('Solar Altitude'!F33)*COS('Surface Solar Azimuth Angles'!F87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F33)*COS('Input Data'!$G$14)))","v":2.3096729339598836},{"$f":"ACOS((COS('Solar Altitude'!G33)*COS('Surface Solar Azimuth Angles'!G87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G33)*COS('Input Data'!$G$14)))","v":2.2810193061754855},{"$f":"ACOS((COS('Solar Altitude'!H33)*COS('Surface Solar Azimuth Angles'!H87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H33)*COS('Input Data'!$G$14)))","v":2.2447850459271042},{"$f":"ACOS((COS('Solar Altitude'!I33)*COS('Surface Solar Azimuth Angles'!I87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I33)*COS('Input Data'!$G$14)))","v":2.2429795953364104},{"$f":"ACOS((COS('Solar Altitude'!J33)*COS('Surface Solar Azimuth Angles'!J87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J33)*COS('Input Data'!$G$14)))","v":2.2943435136025983},{"$f":"ACOS((COS('Solar Altitude'!K33)*COS('Surface Solar Azimuth Angles'!K87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K33)*COS('Input Data'!$G$14)))","v":2.3577943753400059},{"$f":"ACOS((COS('Solar Altitude'!L33)*COS('Surface Solar Azimuth Angles'!L87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L33)*COS('Input Data'!$G$14)))","v":2.3737585812189774},{"$f":"ACOS((COS('Solar Altitude'!M33)*COS('Surface Solar Azimuth Angles'!M87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M33)*COS('Input Data'!$G$14)))","v":2.3239471556762532},{"$f":"ACOS((COS('Solar Altitude'!N33)*COS('Surface Solar Azimuth Angles'!N87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N33)*COS('Input Data'!$G$14)))","v":2.2560320042006814},null,3,{"$f":"ACOS((COS('Solar Altitude'!C33)*COS('Surface Solar Azimuth Angles'!Q87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C33)*COS('Input Data'!$G$14)))","v":1.5808880266991394},{"$f":"ACOS((COS('Solar Altitude'!D33)*COS('Surface Solar Azimuth Angles'!R87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D33)*COS('Input Data'!$G$14)))","v":1.4215345549048419},{"$f":"ACOS((COS('Solar Altitude'!E33)*COS('Surface Solar Azimuth Angles'!S87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E33)*COS('Input Data'!$G$14)))","v":1.2516797095145427},{"$f":"ACOS((COS('Solar Altitude'!F33)*COS('Surface Solar Azimuth Angles'!T87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F33)*COS('Input Data'!$G$14)))","v":1.0656048066685109},{"$f":"ACOS((COS('Solar Altitude'!G33)*COS('Surface Solar Azimuth Angles'!U87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G33)*COS('Input Data'!$G$14)))","v":0.93114670228834784},{"$f":"ACOS((COS('Solar Altitude'!H33)*COS('Surface Solar Azimuth Angles'!V87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H33)*COS('Input Data'!$G$14)))","v":0.87302050166246226},{"$f":"ACOS((COS('Solar Altitude'!I33)*COS('Surface Solar Azimuth Angles'!W87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I33)*COS('Input Data'!$G$14)))","v":0.91403486724340954},{"$f":"ACOS((COS('Solar Altitude'!J33)*COS('Surface Solar Azimuth Angles'!X87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J33)*COS('Input Data'!$G$14)))","v":1.0574249896691437},{"$f":"ACOS((COS('Solar Altitude'!K33)*COS('Surface Solar Azimuth Angles'!Y87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K33)*COS('Input Data'!$G$14)))","v":1.271337108609143},{"$f":"ACOS((COS('Solar Altitude'!L33)*COS('Surface Solar Azimuth Angles'!Z87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L33)*COS('Input Data'!$G$14)))","v":1.4595667771528182},{"$f":"ACOS((COS('Solar Altitude'!M33)*COS('Surface Solar Azimuth Angles'!AA87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M33)*COS('Input Data'!$G$14)))","v":1.6104093501924361},{"$f":"ACOS((COS('Solar Altitude'!N33)*COS('Surface Solar Azimuth Angles'!AB87)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N33)*COS('Input Data'!$G$14)))","v":1.6548974113467207}]
[null,4,{"$f":"ACOS((COS('Solar Altitude'!C34)*COS('Surface Solar Azimuth Angles'!C88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C34)*COS('Input Data'!$G$14)))","v":2.4561527189639456},{"$f":"ACOS((COS('Solar Altitude'!D34)*COS('Surface Solar Azimuth Angles'!D88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D34)*COS('Input Data'!$G$14)))","v":2.5024766008818276},{"$f":"ACOS((COS('Solar Altitude'!E34)*COS('Surface Solar Azimuth Angles'!E88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E34)*COS('Input Data'!$G$14)))","v":2.5541439161893686},{"$f":"ACOS((COS('Solar Altitude'!F34)*COS('Surface Solar Azimuth Angles'!F88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F34)*COS('Input Data'!$G$14)))","v":2.5575524339236404},{"$f":"ACOS((COS('Solar Altitude'!G34)*COS('Surface Solar Azimuth Angles'!G88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G34)*COS('Input Data'!$G$14)))","v":2.5052571644083832},{"$f":"ACOS((COS('Solar Altitude'!H34)*COS('Surface Solar Azimuth Angles'!H88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H34)*COS('Input Data'!$G$14)))","v":2.4604797004373173},{"$f":"ACOS((COS('Solar Altitude'!I34)*COS('Surface Solar Azimuth Angles'!I88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I34)*COS('Input Data'!$G$14)))","v":2.469592766535412},{"$f":"ACOS((COS('Solar Altitude'!J34)*COS('Surface Solar Azimuth Angles'!J88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J34)*COS('Input Data'!$G$14)))","v":2.542277402699114},{"$f":"ACOS((COS('Solar Altitude'!K34)*COS('Surface Solar Azimuth Angles'!K88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K34)*COS('Input Data'!$G$14)))","v":2.6195937631391559},{"$f":"ACOS((COS('Solar Altitude'!L34)*COS('Surface Solar Azimuth Angles'!L88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L34)*COS('Input Data'!$G$14)))","v":2.622222112011336},{"$f":"ACOS((COS('Solar Altitude'!M34)*COS('Surface Solar Azimuth Angles'!M88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M34)*COS('Input Data'!$G$14)))","v":2.5456912493713983},{"$f":"ACOS((COS('Solar Altitude'!N34)*COS('Surface Solar Azimuth Angles'!N88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N34)*COS('Input Data'!$G$14)))","v":2.4705810581096146},null,4,{"$f":"ACOS((COS('Solar Altitude'!C34)*COS('Surface Solar Azimuth Angles'!Q88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C34)*COS('Input Data'!$G$14)))","v":1.6571206145629995},{"$f":"ACOS((COS('Solar Altitude'!D34)*COS('Surface Solar Azimuth Angles'!R88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D34)*COS('Input Data'!$G$14)))","v":1.5007571109956561},{"$f":"ACOS((COS('Solar Altitude'!E34)*COS('Surface Solar Azimuth Angles'!S88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E34)*COS('Input Data'!$G$14)))","v":1.3370759528261968},{"$f":"ACOS((COS('Solar Altitude'!F34)*COS('Surface Solar Azimuth Angles'!T88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F34)*COS('Input Data'!$G$14)))","v":1.158153636257528},{"$f":"ACOS((COS('Solar Altitude'!G34)*COS('Surface Solar Azimuth Angles'!U88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G34)*COS('Input Data'!$G$14)))","v":1.0276879417997584},{"$f":"ACOS((COS('Solar Altitude'!H34)*COS('Surface Solar Azimuth Angles'!V88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H34)*COS('Input Data'!$G$14)))","v":0.96982666619260871},{"$f":"ACOS((COS('Solar Altitude'!I34)*COS('Surface Solar Azimuth Angles'!W88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I34)*COS('Input Data'!$G$14)))","v":1.0083626850529299},{"$f":"ACOS((COS('Solar Altitude'!J34)*COS('Surface Solar Azimuth Angles'!X88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J34)*COS('Input Data'!$G$14)))","v":1.1491427434604364},{"$f":"ACOS((COS('Solar Altitude'!K34)*COS('Surface Solar Azimuth Angles'!Y88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K34)*COS('Input Data'!$G$14)))","v":1.3609042997817129},{"$f":"ACOS((COS('Solar Altitude'!L34)*COS('Surface Solar Azimuth Angles'!Z88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L34)*COS('Input Data'!$G$14)))","v":1.5471299765684494},{"$f":"ACOS((COS('Solar Altitude'!M34)*COS('Surface Solar Azimuth Angles'!AA88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M34)*COS('Input Data'!$G$14)))","v":1.6938665555021764},{"$f":"ACOS((COS('Solar Altitude'!N34)*COS('Surface Solar Azimuth Angles'!AB88)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N34)*COS('Input Data'!$G$14)))","v":1.7334155287264912}]
[null,5,{"$f":"ACOS((COS('Solar Altitude'!C35)*COS('Surface Solar Azimuth Angles'!C89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C35)*COS('Input Data'!$G$14)))","v":2.6592207922251774},{"$f":"ACOS((COS('Solar Altitude'!D35)*COS('Surface Solar Azimuth Angles'!D89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D35)*COS('Input Data'!$G$14)))","v":2.7443517691260602},{"$f":"ACOS((COS('Solar Altitude'!E35)*COS('Surface Solar Azimuth Angles'!E89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E35)*COS('Input Data'!$G$14)))","v":2.8159433039885173},{"$f":"ACOS((COS('Solar Altitude'!F35)*COS('Surface Solar Azimuth Angles'!F89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F35)*COS('Input Data'!$G$14)))","v":2.7881113603845131},{"$f":"ACOS((COS('Solar Altitude'!G35)*COS('Surface Solar Azimuth Angles'!G89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G35)*COS('Input Data'!$G$14)))","v":2.694584611130705},{"$f":"ACOS((COS('Solar Altitude'!H35)*COS('Surface Solar Azimuth Angles'!H89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H35)*COS('Input Data'!$G$14)))","v":2.6397440297185257},{"$f":"ACOS((COS('Solar Altitude'!I35)*COS('Surface Solar Azimuth Angles'!I89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I35)*COS('Input Data'!$G$14)))","v":2.6662351946255844},{"$f":"ACOS((COS('Solar Altitude'!J35)*COS('Surface Solar Azimuth Angles'!J89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J35)*COS('Input Data'!$G$14)))","v":2.7738053629994308},{"$f":"ACOS((COS('Solar Altitude'!K35)*COS('Surface Solar Azimuth Angles'!K89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K35)*COS('Input Data'!$G$14)))","v":2.8813931509383055},{"$f":"ACOS((COS('Solar Altitude'!L35)*COS('Surface Solar Azimuth Angles'!L89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L35)*COS('Input Data'!$G$14)))","v":2.849644704740387},{"$f":"ACOS((COS('Solar Altitude'!M35)*COS('Surface Solar Azimuth Angles'!M89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M35)*COS('Input Data'!$G$14)))","v":2.7261618473809244},{"$f":"ACOS((COS('Solar Altitude'!N35)*COS('Surface Solar Azimuth Angles'!N89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N35)*COS('Input Data'!$G$14)))","v":2.6469898802021596},null,5,{"$f":"ACOS((COS('Solar Altitude'!C35)*COS('Surface Solar Azimuth Angles'!Q89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C35)*COS('Input Data'!$G$14)))","v":1.7492836976125172},{"$f":"ACOS((COS('Solar Altitude'!D35)*COS('Surface Solar Azimuth Angles'!R89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D35)*COS('Input Data'!$G$14)))","v":1.595701316678757},{"$f":"ACOS((COS('Solar Altitude'!E35)*COS('Surface Solar Azimuth Angles'!S89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E35)*COS('Input Data'!$G$14)))","v":1.4367091502252056},{"$f":"ACOS((COS('Solar Altitude'!F35)*COS('Surface Solar Azimuth Angles'!T89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F35)*COS('Input Data'!$G$14)))","v":1.2624059940253503},{"$f":"ACOS((COS('Solar Altitude'!G35)*COS('Surface Solar Azimuth Angles'!U89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G35)*COS('Input Data'!$G$14)))","v":1.1341026749826484},{"$f":"ACOS((COS('Solar Altitude'!H35)*COS('Surface Solar Azimuth Angles'!V89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H35)*COS('Input Data'!$G$14)))","v":1.0764294730227646},{"$f":"ACOS((COS('Solar Altitude'!I35)*COS('Surface Solar Azimuth Angles'!W89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I35)*COS('Input Data'!$G$14)))","v":1.1137712129389754},{"$f":"ACOS((COS('Solar Altitude'!J35)*COS('Surface Solar Azimuth Angles'!X89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J35)*COS('Input Data'!$G$14)))","v":1.2529622329687102},{"$f":"ACOS((COS('Solar Altitude'!K35)*COS('Surface Solar Azimuth Angles'!Y89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K35)*COS('Input Data'!$G$14)))","v":1.4630820983257669},{"$f":"ACOS((COS('Solar Altitude'!L35)*COS('Surface Solar Azimuth Angles'!Z89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L35)*COS('Input Data'!$G$14)))","v":1.6476519305427166},{"$f":"ACOS((COS('Solar Altitude'!M35)*COS('Surface Solar Azimuth Angles'!AA89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M35)*COS('Input Data'!$G$14)))","v":1.7912015553083749},{"$f":"ACOS((COS('Solar Altitude'!N35)*COS('Surface Solar Azimuth Angles'!AB89)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N35)*COS('Input Data'!$G$14)))","v":1.8269997217566198}]
[null,6,{"$f":"ACOS((COS('Solar Altitude'!C36)*COS('Surface Solar Azimuth Angles'!C90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C36)*COS('Input Data'!$G$14)))","v":2.785543338653973},{"$f":"ACOS((COS('Solar Altitude'!D36)*COS('Surface Solar Azimuth Angles'!D90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D36)*COS('Input Data'!$G$14)))","v":2.9353085327964417},{"$f":"ACOS((COS('Solar Altitude'!E36)*COS('Surface Solar Azimuth Angles'!E90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E36)*COS('Input Data'!$G$14)))","v":3.0777426917876647},{"$f":"ACOS((COS('Solar Altitude'!F36)*COS('Surface Solar Azimuth Angles'!F90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F36)*COS('Input Data'!$G$14)))","v":2.9322606102243371},{"$f":"ACOS((COS('Solar Altitude'!G36)*COS('Surface Solar Azimuth Angles'!G90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G36)*COS('Input Data'!$G$14)))","v":2.7869128705359612},{"$f":"ACOS((COS('Solar Altitude'!H36)*COS('Surface Solar Azimuth Angles'!H90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H36)*COS('Input Data'!$G$14)))","v":2.7307180571082119},{"$f":"ACOS((COS('Solar Altitude'!I36)*COS('Surface Solar Azimuth Angles'!I90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I36)*COS('Input Data'!$G$14)))","v":2.7793021618829643},{"$f":"ACOS((COS('Solar Altitude'!J36)*COS('Surface Solar Azimuth Angles'!J90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J36)*COS('Input Data'!$G$14)))","v":2.9264100687213439},{"$f":"ACOS((COS('Solar Altitude'!K36)*COS('Surface Solar Azimuth Angles'!K90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K36)*COS('Input Data'!$G$14)))","v":3.1399927684421303},{"$f":"ACOS((COS('Solar Altitude'!L36)*COS('Surface Solar Azimuth Angles'!L90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L36)*COS('Input Data'!$G$14)))","v":2.9514307709554823},{"$f":"ACOS((COS('Solar Altitude'!M36)*COS('Surface Solar Azimuth Angles'!M90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M36)*COS('Input Data'!$G$14)))","v":2.7931053500685721},{"$f":"ACOS((COS('Solar Altitude'!N36)*COS('Surface Solar Azimuth Angles'!N90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N36)*COS('Input Data'!$G$14)))","v":2.7316415819726259},null,6,{"$f":"ACOS((COS('Solar Altitude'!C36)*COS('Surface Solar Azimuth Angles'!Q90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C36)*COS('Input Data'!$G$14)))","v":1.8523413136689326},{"$f":"ACOS((COS('Solar Altitude'!D36)*COS('Surface Solar Azimuth Angles'!R90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D36)*COS('Input Data'!$G$14)))","v":1.7006396438405069},{"$f":"ACOS((COS('Solar Altitude'!E36)*COS('Surface Solar Azimuth Angles'!S90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E36)*COS('Input Data'!$G$14)))","v":1.5441304951050598},{"$f":"ACOS((COS('Solar Altitude'!F36)*COS('Surface Solar Azimuth Angles'!T90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F36)*COS('Input Data'!$G$14)))","v":1.3713761378566136},{"$f":"ACOS((COS('Solar Altitude'!G36)*COS('Surface Solar Azimuth Angles'!U90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G36)*COS('Input Data'!$G$14)))","v":1.2432204721763305},{"$f":"ACOS((COS('Solar Altitude'!H36)*COS('Surface Solar Azimuth Angles'!V90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H36)*COS('Input Data'!$G$14)))","v":1.1855256457513765},{"$f":"ACOS((COS('Solar Altitude'!I36)*COS('Surface Solar Azimuth Angles'!W90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I36)*COS('Input Data'!$G$14)))","v":1.222896278561056},{"$f":"ACOS((COS('Solar Altitude'!J36)*COS('Surface Solar Azimuth Angles'!X90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J36)*COS('Input Data'!$G$14)))","v":1.3618480900011929},{"$f":"ACOS((COS('Solar Altitude'!K36)*COS('Surface Solar Azimuth Angles'!Y90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K36)*COS('Input Data'!$G$14)))","v":1.5714648658845651},{"$f":"ACOS((COS('Solar Altitude'!L36)*COS('Surface Solar Azimuth Angles'!Z90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L36)*COS('Input Data'!$G$14)))","v":1.7553287151397341},{"$f":"ACOS((COS('Solar Altitude'!M36)*COS('Surface Solar Azimuth Angles'!AA90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M36)*COS('Input Data'!$G$14)))","v":1.8972282700891392},{"$f":"ACOS((COS('Solar Altitude'!N36)*COS('Surface Solar Azimuth Angles'!AB90)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N36)*COS('Input Data'!$G$14)))","v":1.930807704333086}]
[null,7,{"$f":"ACOS((COS('Solar Altitude'!C37)*COS('Surface Solar Azimuth Angles'!C91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C37)*COS('Input Data'!$G$14)))","v":2.751282665597893},{"$f":"ACOS((COS('Solar Altitude'!D37)*COS('Surface Solar Azimuth Angles'!D91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D37)*COS('Input Data'!$G$14)))","v":2.8909857355299895},{"$f":"ACOS((COS('Solar Altitude'!E37)*COS('Surface Solar Azimuth Angles'!E91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E37)*COS('Input Data'!$G$14)))","v":2.9436432275927693},{"$f":"ACOS((COS('Solar Altitude'!F37)*COS('Surface Solar Azimuth Angles'!F91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F37)*COS('Input Data'!$G$14)))","v":2.8288909506839368},{"$f":"ACOS((COS('Solar Altitude'!G37)*COS('Surface Solar Azimuth Angles'!G91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G37)*COS('Input Data'!$G$14)))","v":2.7137534044824214},{"$f":"ACOS((COS('Solar Altitude'!H37)*COS('Surface Solar Azimuth Angles'!H91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H37)*COS('Input Data'!$G$14)))","v":2.6778226050543497},{"$f":"ACOS((COS('Solar Altitude'!I37)*COS('Surface Solar Azimuth Angles'!I91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I37)*COS('Input Data'!$G$14)))","v":2.7320954449458243},{"$f":"ACOS((COS('Solar Altitude'!J37)*COS('Surface Solar Azimuth Angles'!J91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J37)*COS('Input Data'!$G$14)))","v":2.8376801773294518},{"$f":"ACOS((COS('Solar Altitude'!K37)*COS('Surface Solar Azimuth Angles'!K91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K37)*COS('Input Data'!$G$14)))","v":2.8781933806429816},{"$f":"ACOS((COS('Solar Altitude'!L37)*COS('Surface Solar Azimuth Angles'!L91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L37)*COS('Input Data'!$G$14)))","v":2.7915042028627801},{"$f":"ACOS((COS('Solar Altitude'!M37)*COS('Surface Solar Azimuth Angles'!M91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M37)*COS('Input Data'!$G$14)))","v":2.6923727979996803},{"$f":"ACOS((COS('Solar Altitude'!N37)*COS('Surface Solar Azimuth Angles'!N91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N37)*COS('Input Data'!$G$14)))","v":2.6717106411392466},null,7,{"$f":"ACOS((COS('Solar Altitude'!C37)*COS('Surface Solar Azimuth Angles'!Q91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C37)*COS('Input Data'!$G$14)))","v":1.9608940295459869},{"$f":"ACOS((COS('Solar Altitude'!D37)*COS('Surface Solar Azimuth Angles'!R91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D37)*COS('Input Data'!$G$14)))","v":1.8096823394378536},{"$f":"ACOS((COS('Solar Altitude'!E37)*COS('Surface Solar Azimuth Angles'!S91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E37)*COS('Input Data'!$G$14)))","v":1.6530665123238679},{"$f":"ACOS((COS('Solar Altitude'!F37)*COS('Surface Solar Azimuth Angles'!T91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F37)*COS('Input Data'!$G$14)))","v":1.4787229745009782},{"$f":"ACOS((COS('Solar Altitude'!G37)*COS('Surface Solar Azimuth Angles'!U91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G37)*COS('Input Data'!$G$14)))","v":1.3488741690277566},{"$f":"ACOS((COS('Solar Altitude'!H37)*COS('Surface Solar Azimuth Angles'!V91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H37)*COS('Input Data'!$G$14)))","v":1.2909863010022351},{"$f":"ACOS((COS('Solar Altitude'!I37)*COS('Surface Solar Azimuth Angles'!W91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I37)*COS('Input Data'!$G$14)))","v":1.3294425236295961},{"$f":"ACOS((COS('Solar Altitude'!J37)*COS('Surface Solar Azimuth Angles'!X91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J37)*COS('Input Data'!$G$14)))","v":1.4694283343726298},{"$f":"ACOS((COS('Solar Altitude'!K37)*COS('Surface Solar Azimuth Angles'!Y91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K37)*COS('Input Data'!$G$14)))","v":1.6798096938481444},{"$f":"ACOS((COS('Solar Altitude'!L37)*COS('Surface Solar Azimuth Angles'!Z91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L37)*COS('Input Data'!$G$14)))","v":1.8641713736807273},{"$f":"ACOS((COS('Solar Altitude'!M37)*COS('Surface Solar Azimuth Angles'!AA91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M37)*COS('Input Data'!$G$14)))","v":2.0063660805447143},{"$f":"ACOS((COS('Solar Altitude'!N37)*COS('Surface Solar Azimuth Angles'!AB91)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N37)*COS('Input Data'!$G$14)))","v":2.0395679350868345}]
[null,8,{"$f":"ACOS((COS('Solar Altitude'!C38)*COS('Surface Solar Azimuth Angles'!C92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C38)*COS('Input Data'!$G$14)))","v":2.5854127241321812},{"$f":"ACOS((COS('Solar Altitude'!D38)*COS('Surface Solar Azimuth Angles'!D92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D38)*COS('Input Data'!$G$14)))","v":2.6741107477984687},{"$f":"ACOS((COS('Solar Altitude'!E38)*COS('Surface Solar Azimuth Angles'!E92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E38)*COS('Input Data'!$G$14)))","v":2.6818438397936202},{"$f":"ACOS((COS('Solar Altitude'!F38)*COS('Surface Solar Azimuth Angles'!F92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F38)*COS('Input Data'!$G$14)))","v":2.6060627469610238},{"$f":"ACOS((COS('Solar Altitude'!G38)*COS('Surface Solar Azimuth Angles'!G92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G38)*COS('Input Data'!$G$14)))","v":2.5321466578024481},{"$f":"ACOS((COS('Solar Altitude'!H38)*COS('Surface Solar Azimuth Angles'!H92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H38)*COS('Input Data'!$G$14)))","v":2.5166950081533845},{"$f":"ACOS((COS('Solar Altitude'!I38)*COS('Surface Solar Azimuth Angles'!I92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I38)*COS('Input Data'!$G$14)))","v":2.5626485528760363},{"$f":"ACOS((COS('Solar Altitude'!J38)*COS('Surface Solar Azimuth Angles'!J92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J38)*COS('Input Data'!$G$14)))","v":2.6187099029073515},{"$f":"ACOS((COS('Solar Altitude'!K38)*COS('Surface Solar Azimuth Angles'!K92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K38)*COS('Input Data'!$G$14)))","v":2.6163939928438325},{"$f":"ACOS((COS('Solar Altitude'!L38)*COS('Surface Solar Azimuth Angles'!L92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L38)*COS('Input Data'!$G$14)))","v":2.5547559960547845},{"$f":"ACOS((COS('Solar Altitude'!M38)*COS('Surface Solar Azimuth Angles'!M92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M38)*COS('Input Data'!$G$14)))","v":2.4985832089606257},{"$f":"ACOS((COS('Solar Altitude'!N38)*COS('Surface Solar Azimuth Angles'!N92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N38)*COS('Input Data'!$G$14)))","v":2.5070460567990431},null,8,{"$f":"ACOS((COS('Solar Altitude'!C38)*COS('Surface Solar Azimuth Angles'!Q92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C38)*COS('Input Data'!$G$14)))","v":2.0690315825650738},{"$f":"ACOS((COS('Solar Altitude'!D38)*COS('Surface Solar Azimuth Angles'!R92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D38)*COS('Input Data'!$G$14)))","v":1.9166775165476215},{"$f":"ACOS((COS('Solar Altitude'!E38)*COS('Surface Solar Azimuth Angles'!S92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E38)*COS('Input Data'!$G$14)))","v":1.7572927734324943},{"$f":"ACOS((COS('Solar Altitude'!F38)*COS('Surface Solar Azimuth Angles'!T92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F38)*COS('Input Data'!$G$14)))","v":1.5785098134731006},{"$f":"ACOS((COS('Solar Altitude'!G38)*COS('Surface Solar Azimuth Angles'!U92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G38)*COS('Input Data'!$G$14)))","v":1.4455274503218323},{"$f":"ACOS((COS('Solar Altitude'!H38)*COS('Surface Solar Azimuth Angles'!V92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H38)*COS('Input Data'!$G$14)))","v":1.3874165333454944},{"$f":"ACOS((COS('Solar Altitude'!I38)*COS('Surface Solar Azimuth Angles'!W92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I38)*COS('Input Data'!$G$14)))","v":1.4278052825715355},{"$f":"ACOS((COS('Solar Altitude'!J38)*COS('Surface Solar Azimuth Angles'!X92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J38)*COS('Input Data'!$G$14)))","v":1.5697565456748377},{"$f":"ACOS((COS('Solar Altitude'!K38)*COS('Surface Solar Azimuth Angles'!Y92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K38)*COS('Input Data'!$G$14)))","v":1.7818724301524667},{"$f":"ACOS((COS('Solar Altitude'!L38)*COS('Surface Solar Azimuth Angles'!Z92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L38)*COS('Input Data'!$G$14)))","v":1.9678146556141352},{"$f":"ACOS((COS('Solar Altitude'!M38)*COS('Surface Solar Azimuth Angles'!AA92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M38)*COS('Input Data'!$G$14)))","v":2.1123978979577669},{"$f":"ACOS((COS('Solar Altitude'!N38)*COS('Surface Solar Azimuth Angles'!AB92)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N38)*COS('Input Data'!$G$14)))","v":2.1473597624633562}]
[null,9,{"$f":"ACOS((COS('Solar Altitude'!C39)*COS('Surface Solar Azimuth Angles'!C93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C39)*COS('Input Data'!$G$14)))","v":2.3686915997301279},{"$f":"ACOS((COS('Solar Altitude'!D39)*COS('Surface Solar Azimuth Angles'!D93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D39)*COS('Input Data'!$G$14)))","v":2.4276915216774144},{"$f":"ACOS((COS('Solar Altitude'!E39)*COS('Surface Solar Azimuth Angles'!E93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E39)*COS('Input Data'!$G$14)))","v":2.4200444519944706},{"$f":"ACOS((COS('Solar Altitude'!F39)*COS('Surface Solar Azimuth Angles'!F93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F39)*COS('Input Data'!$G$14)))","v":2.3601288269844707},{"$f":"ACOS((COS('Solar Altitude'!G39)*COS('Surface Solar Azimuth Angles'!G93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G39)*COS('Input Data'!$G$14)))","v":2.3106595059453445},{"$f":"ACOS((COS('Solar Altitude'!H39)*COS('Surface Solar Azimuth Angles'!H93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H39)*COS('Input Data'!$G$14)))","v":2.3082477773479195},{"$f":"ACOS((COS('Solar Altitude'!I39)*COS('Surface Solar Azimuth Angles'!I93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I39)*COS('Input Data'!$G$14)))","v":2.3457984733690869},{"$f":"ACOS((COS('Solar Altitude'!J39)*COS('Surface Solar Azimuth Angles'!J93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J39)*COS('Input Data'!$G$14)))","v":2.3739516356299215},{"$f":"ACOS((COS('Solar Altitude'!K39)*COS('Surface Solar Azimuth Angles'!K93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K39)*COS('Input Data'!$G$14)))","v":2.3545946050446833},{"$f":"ACOS((COS('Solar Altitude'!L39)*COS('Surface Solar Azimuth Angles'!L93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L39)*COS('Input Data'!$G$14)))","v":2.3040675436217914},{"$f":"ACOS((COS('Solar Altitude'!M39)*COS('Surface Solar Azimuth Angles'!M93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M39)*COS('Input Data'!$G$14)))","v":2.2721662590002256},{"$f":"ACOS((COS('Solar Altitude'!N39)*COS('Surface Solar Azimuth Angles'!N93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N39)*COS('Input Data'!$G$14)))","v":2.2971884180004611},null,9,{"$f":"ACOS((COS('Solar Altitude'!C39)*COS('Surface Solar Azimuth Angles'!Q93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C39)*COS('Input Data'!$G$14)))","v":2.1699950320018964},{"$f":"ACOS((COS('Solar Altitude'!D39)*COS('Surface Solar Azimuth Angles'!R93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D39)*COS('Input Data'!$G$14)))","v":2.0149747762768246},{"$f":"ACOS((COS('Solar Altitude'!E39)*COS('Surface Solar Azimuth Angles'!S93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E39)*COS('Input Data'!$G$14)))","v":1.8504483304196497},{"$f":"ACOS((COS('Solar Altitude'!F39)*COS('Surface Solar Azimuth Angles'!T93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F39)*COS('Input Data'!$G$14)))","v":1.6650133482944771},{"$f":"ACOS((COS('Solar Altitude'!G39)*COS('Surface Solar Azimuth Angles'!U93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G39)*COS('Input Data'!$G$14)))","v":1.5280399489035836},{"$f":"ACOS((COS('Solar Altitude'!H39)*COS('Surface Solar Azimuth Angles'!V93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H39)*COS('Input Data'!$G$14)))","v":1.4698795030702181},{"$f":"ACOS((COS('Solar Altitude'!I39)*COS('Surface Solar Azimuth Angles'!W93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I39)*COS('Input Data'!$G$14)))","v":1.5128016241325899},{"$f":"ACOS((COS('Solar Altitude'!J39)*COS('Surface Solar Azimuth Angles'!X93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J39)*COS('Input Data'!$G$14)))","v":1.6571110593576162},{"$f":"ACOS((COS('Solar Altitude'!K39)*COS('Surface Solar Azimuth Angles'!Y93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K39)*COS('Input Data'!$G$14)))","v":1.8712451895573823},{"$f":"ACOS((COS('Solar Altitude'!L39)*COS('Surface Solar Azimuth Angles'!Z93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L39)*COS('Input Data'!$G$14)))","v":2.0592944651066598},{"$f":"ACOS((COS('Solar Altitude'!M39)*COS('Surface Solar Azimuth Angles'!AA93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M39)*COS('Input Data'!$G$14)))","v":2.2081042109535307},{"$f":"ACOS((COS('Solar Altitude'!N39)*COS('Surface Solar Azimuth Angles'!AB93)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N39)*COS('Input Data'!$G$14)))","v":2.2471955201223852}]
[null,10,{"$f":"ACOS((COS('Solar Altitude'!C40)*COS('Surface Solar Azimuth Angles'!C94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C40)*COS('Input Data'!$G$14)))","v":2.1337797676592318},{"$f":"ACOS((COS('Solar Altitude'!D40)*COS('Surface Solar Azimuth Angles'!D94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D40)*COS('Input Data'!$G$14)))","v":2.1741572293084008},{"$f":"ACOS((COS('Solar Altitude'!E40)*COS('Surface Solar Azimuth Angles'!E94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E40)*COS('Input Data'!$G$14)))","v":2.158245064195321},{"$f":"ACOS((COS('Solar Altitude'!F40)*COS('Surface Solar Azimuth Angles'!F94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F40)*COS('Input Data'!$G$14)))","v":2.1075988694625942},{"$f":"ACOS((COS('Solar Altitude'!G40)*COS('Surface Solar Azimuth Angles'!G94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G40)*COS('Input Data'!$G$14)))","v":2.0742616383419699},{"$f":"ACOS((COS('Solar Altitude'!H40)*COS('Surface Solar Azimuth Angles'!H94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H40)*COS('Input Data'!$G$14)))","v":2.0805487915276233},{"$f":"ACOS((COS('Solar Altitude'!I40)*COS('Surface Solar Azimuth Angles'!I94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I40)*COS('Input Data'!$G$14)))","v":2.1114654362427374},{"$f":"ACOS((COS('Solar Altitude'!J40)*COS('Surface Solar Azimuth Angles'!J94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J40)*COS('Input Data'!$G$14)))","v":2.1219639352882806},{"$f":"ACOS((COS('Solar Altitude'!K40)*COS('Surface Solar Azimuth Angles'!K94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K40)*COS('Input Data'!$G$14)))","v":2.0927952172455333},{"$f":"ACOS((COS('Solar Altitude'!L40)*COS('Surface Solar Azimuth Angles'!L94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L40)*COS('Input Data'!$G$14)))","v":2.0491282519194662},{"$f":"ACOS((COS('Solar Altitude'!M40)*COS('Surface Solar Azimuth Angles'!M94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M40)*COS('Input Data'!$G$14)))","v":2.0333792885124584},{"$f":"ACOS((COS('Solar Altitude'!N40)*COS('Surface Solar Azimuth Angles'!N94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N40)*COS('Input Data'!$G$14)))","v":2.0688885622515061},null,10,{"$f":"ACOS((COS('Solar Altitude'!C40)*COS('Surface Solar Azimuth Angles'!Q94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C40)*COS('Input Data'!$G$14)))","v":2.2558640906580765},{"$f":"ACOS((COS('Solar Altitude'!D40)*COS('Surface Solar Azimuth Angles'!R94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D40)*COS('Input Data'!$G$14)))","v":2.0972971872219439},{"$f":"ACOS((COS('Solar Altitude'!E40)*COS('Surface Solar Azimuth Angles'!S94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E40)*COS('Input Data'!$G$14)))","v":1.9260356433135977},{"$f":"ACOS((COS('Solar Altitude'!F40)*COS('Surface Solar Azimuth Angles'!T94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F40)*COS('Input Data'!$G$14)))","v":1.7327675548833017},{"$f":"ACOS((COS('Solar Altitude'!G40)*COS('Surface Solar Azimuth Angles'!U94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G40)*COS('Input Data'!$G$14)))","v":1.5916855967085466},{"$f":"ACOS((COS('Solar Altitude'!H40)*COS('Surface Solar Azimuth Angles'!V94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H40)*COS('Input Data'!$G$14)))","v":1.5338777599607782},{"$f":"ACOS((COS('Solar Altitude'!I40)*COS('Surface Solar Azimuth Angles'!W94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I40)*COS('Input Data'!$G$14)))","v":1.5796438338888683},{"$f":"ACOS((COS('Solar Altitude'!J40)*COS('Surface Solar Azimuth Angles'!X94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J40)*COS('Input Data'!$G$14)))","v":1.7260208048936474},{"$f":"ACOS((COS('Solar Altitude'!K40)*COS('Surface Solar Azimuth Angles'!Y94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K40)*COS('Input Data'!$G$14)))","v":1.9414419703479378},{"$f":"ACOS((COS('Solar Altitude'!L40)*COS('Surface Solar Azimuth Angles'!Z94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L40)*COS('Input Data'!$G$14)))","v":2.1310998347052168},{"$f":"ACOS((COS('Solar Altitude'!M40)*COS('Surface Solar Azimuth Angles'!AA94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M40)*COS('Input Data'!$G$14)))","v":2.2850879065924885},{"$f":"ACOS((COS('Solar Altitude'!N40)*COS('Surface Solar Azimuth Angles'!AB94)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N40)*COS('Input Data'!$G$14)))","v":2.3306428419263838}]
[null,11,{"$f":"ACOS((COS('Solar Altitude'!C41)*COS('Surface Solar Azimuth Angles'!C95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C41)*COS('Input Data'!$G$14)))","v":1.8914251972930805},{"$f":"ACOS((COS('Solar Altitude'!D41)*COS('Surface Solar Azimuth Angles'!D95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D41)*COS('Input Data'!$G$14)))","v":1.9180799046031216},{"$f":"ACOS((COS('Solar Altitude'!E41)*COS('Surface Solar Azimuth Angles'!E95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E41)*COS('Input Data'!$G$14)))","v":1.8964456763961715},{"$f":"ACOS((COS('Solar Altitude'!F41)*COS('Surface Solar Azimuth Angles'!F95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F41)*COS('Input Data'!$G$14)))","v":1.8525577261468644},{"$f":"ACOS((COS('Solar Altitude'!G41)*COS('Surface Solar Azimuth Angles'!G95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G41)*COS('Input Data'!$G$14)))","v":1.8316045505169811},{"$f":"ACOS((COS('Solar Altitude'!H41)*COS('Surface Solar Azimuth Angles'!H95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H41)*COS('Input Data'!$G$14)))","v":1.8444645327287759},{"$f":"ACOS((COS('Solar Altitude'!I41)*COS('Surface Solar Azimuth Angles'!I95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I41)*COS('Input Data'!$G$14)))","v":1.8698597438967348},{"$f":"ACOS((COS('Solar Altitude'!J41)*COS('Surface Solar Azimuth Angles'!J95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J41)*COS('Input Data'!$G$14)))","v":1.8672450134180139},{"$f":"ACOS((COS('Solar Altitude'!K41)*COS('Surface Solar Azimuth Angles'!K95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K41)*COS('Input Data'!$G$14)))","v":1.8309958294463846},{"$f":"ACOS((COS('Solar Altitude'!L41)*COS('Surface Solar Azimuth Angles'!L95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L41)*COS('Input Data'!$G$14)))","v":1.7925345463526761},{"$f":"ACOS((COS('Solar Altitude'!M41)*COS('Surface Solar Azimuth Angles'!M95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M41)*COS('Input Data'!$G$14)))","v":1.7893781051178528},{"$f":"ACOS((COS('Solar Altitude'!N41)*COS('Surface Solar Azimuth Angles'!N95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N41)*COS('Input Data'!$G$14)))","v":1.8325410159850262},null,11,{"$f":"ACOS((COS('Solar Altitude'!C41)*COS('Surface Solar Azimuth Angles'!Q95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C41)*COS('Input Data'!$G$14)))","v":2.3177748291302818},{"$f":"ACOS((COS('Solar Altitude'!D41)*COS('Surface Solar Azimuth Angles'!R95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D41)*COS('Input Data'!$G$14)))","v":2.1560968178867563},{"$f":"ACOS((COS('Solar Altitude'!E41)*COS('Surface Solar Azimuth Angles'!S95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E41)*COS('Input Data'!$G$14)))","v":1.9778498329698173},{"$f":"ACOS((COS('Solar Altitude'!F41)*COS('Surface Solar Azimuth Angles'!T95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F41)*COS('Input Data'!$G$14)))","v":1.7769469353861214},{"$f":"ACOS((COS('Solar Altitude'!G41)*COS('Surface Solar Azimuth Angles'!U95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G41)*COS('Input Data'!$G$14)))","v":1.6324508261882393},{"$f":"ACOS((COS('Solar Altitude'!H41)*COS('Surface Solar Azimuth Angles'!V95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H41)*COS('Input Data'!$G$14)))","v":1.5755986440545404},{"$f":"ACOS((COS('Solar Altitude'!I41)*COS('Surface Solar Azimuth Angles'!W95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I41)*COS('Input Data'!$G$14)))","v":1.6241932387566385},{"$f":"ACOS((COS('Solar Altitude'!J41)*COS('Surface Solar Azimuth Angles'!X95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J41)*COS('Input Data'!$G$14)))","v":1.7716257205360397},{"$f":"ACOS((COS('Solar Altitude'!K41)*COS('Surface Solar Azimuth Angles'!Y95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K41)*COS('Input Data'!$G$14)))","v":1.9864642989433916},{"$f":"ACOS((COS('Solar Altitude'!L41)*COS('Surface Solar Azimuth Angles'!Z95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L41)*COS('Input Data'!$G$14)))","v":2.1759210812408112},{"$f":"ACOS((COS('Solar Altitude'!M41)*COS('Surface Solar Azimuth Angles'!AA95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M41)*COS('Input Data'!$G$14)))","v":2.3344455856192141},{"$f":"ACOS((COS('Solar Altitude'!N41)*COS('Surface Solar Azimuth Angles'!AB95)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N41)*COS('Input Data'!$G$14)))","v":2.3881360626612462}]
[null,12,{"$f":"ACOS((COS('Solar Altitude'!C42)*COS('Surface Solar Azimuth Angles'!C96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C42)*COS('Input Data'!$G$14)))","v":1.6460046622857298},{"$f":"ACOS((COS('Solar Altitude'!D42)*COS('Surface Solar Azimuth Angles'!D96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D42)*COS('Input Data'!$G$14)))","v":1.6610011453908404},{"$f":"ACOS((COS('Solar Altitude'!E42)*COS('Surface Solar Azimuth Angles'!E96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E42)*COS('Input Data'!$G$14)))","v":1.6346462885970197},{"$f":"ACOS((COS('Solar Altitude'!F42)*COS('Surface Solar Azimuth Angles'!F96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F42)*COS('Input Data'!$G$14)))","v":1.5965558239377149},{"$f":"ACOS((COS('Solar Altitude'!G42)*COS('Surface Solar Azimuth Angles'!G96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G42)*COS('Input Data'!$G$14)))","v":1.5864834365931093},{"$f":"ACOS((COS('Solar Altitude'!H42)*COS('Surface Solar Azimuth Angles'!H96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H42)*COS('Input Data'!$G$14)))","v":1.6049535508624619},{"$f":"ACOS((COS('Solar Altitude'!I42)*COS('Surface Solar Azimuth Angles'!I96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I42)*COS('Input Data'!$G$14)))","v":1.6252859313164105},{"$f":"ACOS((COS('Solar Altitude'!J42)*COS('Surface Solar Azimuth Angles'!J96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J42)*COS('Input Data'!$G$14)))","v":1.6114686738952435},{"$f":"ACOS((COS('Solar Altitude'!K42)*COS('Surface Solar Azimuth Angles'!K96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K42)*COS('Input Data'!$G$14)))","v":1.5723962119425237},{"$f":"ACOS((COS('Solar Altitude'!L42)*COS('Surface Solar Azimuth Angles'!L96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L42)*COS('Input Data'!$G$14)))","v":1.6062390407741667},{"$f":"ACOS((COS('Solar Altitude'!M42)*COS('Surface Solar Azimuth Angles'!M96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M42)*COS('Input Data'!$G$14)))","v":1.5981477526481307},{"$f":"ACOS((COS('Solar Altitude'!N42)*COS('Surface Solar Azimuth Angles'!N96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N42)*COS('Input Data'!$G$14)))","v":1.5929456217761104},null,12,{"$f":"ACOS((COS('Solar Altitude'!C42)*COS('Surface Solar Azimuth Angles'!Q96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C42)*COS('Input Data'!$G$14)))","v":2.3474500523065238},{"$f":"ACOS((COS('Solar Altitude'!D42)*COS('Surface Solar Azimuth Angles'!R96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D42)*COS('Input Data'!$G$14)))","v":2.1847811861508903},{"$f":"ACOS((COS('Solar Altitude'!E42)*COS('Surface Solar Azimuth Angles'!S96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E42)*COS('Input Data'!$G$14)))","v":2.0009556090087068},{"$f":"ACOS((COS('Solar Altitude'!F42)*COS('Surface Solar Azimuth Angles'!T96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F42)*COS('Input Data'!$G$14)))","v":1.7940531866509437},{"$f":"ACOS((COS('Solar Altitude'!G42)*COS('Surface Solar Azimuth Angles'!U96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G42)*COS('Input Data'!$G$14)))","v":1.6475358321638891},{"$f":"ACOS((COS('Solar Altitude'!H42)*COS('Surface Solar Azimuth Angles'!V96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H42)*COS('Input Data'!$G$14)))","v":1.5923471793669057},{"$f":"ACOS((COS('Solar Altitude'!I42)*COS('Surface Solar Azimuth Angles'!W96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I42)*COS('Input Data'!$G$14)))","v":1.6434361939800852},{"$f":"ACOS((COS('Solar Altitude'!J42)*COS('Surface Solar Azimuth Angles'!X96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J42)*COS('Input Data'!$G$14)))","v":1.7903456678870378},{"$f":"ACOS((COS('Solar Altitude'!K42)*COS('Surface Solar Azimuth Angles'!Y96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K42)*COS('Input Data'!$G$14)))","v":2.0018920633879986},{"$f":"ACOS((COS('Solar Altitude'!L42)*COS('Surface Solar Azimuth Angles'!Z96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L42)*COS('Input Data'!$G$14)))","v":2.1883152677081559},{"$f":"ACOS((COS('Solar Altitude'!M42)*COS('Surface Solar Azimuth Angles'!AA96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M42)*COS('Input Data'!$G$14)))","v":2.3489797495315021},{"$f":"ACOS((COS('Solar Altitude'!N42)*COS('Surface Solar Azimuth Angles'!AB96)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N42)*COS('Input Data'!$G$14)))","v":2.4110049165283693}]
[null,13,{"$f":"ACOS((COS('Solar Altitude'!C43)*COS('Surface Solar Azimuth Angles'!C97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C43)*COS('Input Data'!$G$14)))","v":1.3999574973106046},{"$f":"ACOS((COS('Solar Altitude'!D43)*COS('Surface Solar Azimuth Angles'!D97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D43)*COS('Input Data'!$G$14)))","v":1.4037011247408877},{"$f":"ACOS((COS('Solar Altitude'!E43)*COS('Surface Solar Azimuth Angles'!E97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E43)*COS('Input Data'!$G$14)))","v":1.3728469007978732},{"$f":"ACOS((COS('Solar Altitude'!F43)*COS('Surface Solar Azimuth Angles'!F97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F43)*COS('Input Data'!$G$14)))","v":1.3404753895978903},{"$f":"ACOS((COS('Solar Altitude'!G43)*COS('Surface Solar Azimuth Angles'!G97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G43)*COS('Input Data'!$G$14)))","v":1.3412275846299375},{"$f":"ACOS((COS('Solar Altitude'!H43)*COS('Surface Solar Azimuth Angles'!H97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H43)*COS('Input Data'!$G$14)))","v":1.3650568621907504},{"$f":"ACOS((COS('Solar Altitude'!I43)*COS('Surface Solar Azimuth Angles'!I97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I43)*COS('Input Data'!$G$14)))","v":1.3802334869131052},{"$f":"ACOS((COS('Solar Altitude'!J43)*COS('Surface Solar Azimuth Angles'!J97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J43)*COS('Input Data'!$G$14)))","v":1.3555640296738936},{"$f":"ACOS((COS('Solar Altitude'!K43)*COS('Surface Solar Azimuth Angles'!K97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K43)*COS('Input Data'!$G$14)))","v":1.3073970538480852},{"$f":"ACOS((COS('Solar Altitude'!L43)*COS('Surface Solar Azimuth Angles'!L97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L43)*COS('Input Data'!$G$14)))","v":1.2782603911114869},{"$f":"ACOS((COS('Solar Altitude'!M43)*COS('Surface Solar Azimuth Angles'!M97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M43)*COS('Input Data'!$G$14)))","v":1.2977380379324026},{"$f":"ACOS((COS('Solar Altitude'!N43)*COS('Surface Solar Azimuth Angles'!N97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N43)*COS('Input Data'!$G$14)))","v":1.3531003490591469},null,13,{"$f":"ACOS((COS('Solar Altitude'!C43)*COS('Surface Solar Azimuth Angles'!Q97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C43)*COS('Input Data'!$G$14)))","v":2.3401587603196914},{"$f":"ACOS((COS('Solar Altitude'!D43)*COS('Surface Solar Azimuth Angles'!R97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D43)*COS('Input Data'!$G$14)))","v":2.1796592482481127},{"$f":"ACOS((COS('Solar Altitude'!E43)*COS('Surface Solar Azimuth Angles'!S97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E43)*COS('Input Data'!$G$14)))","v":1.992929088293024},{"$f":"ACOS((COS('Solar Altitude'!F43)*COS('Surface Solar Azimuth Angles'!T97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F43)*COS('Input Data'!$G$14)))","v":1.7826421386414861},{"$f":"ACOS((COS('Solar Altitude'!G43)*COS('Surface Solar Azimuth Angles'!U97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G43)*COS('Input Data'!$G$14)))","v":1.6358506927880836},{"$f":"ACOS((COS('Solar Altitude'!H43)*COS('Surface Solar Azimuth Angles'!V97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H43)*COS('Input Data'!$G$14)))","v":1.5829858321144272},{"$f":"ACOS((COS('Solar Altitude'!I43)*COS('Surface Solar Azimuth Angles'!W97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I43)*COS('Input Data'!$G$14)))","v":1.6359945320030804},{"$f":"ACOS((COS('Solar Altitude'!J43)*COS('Surface Solar Azimuth Angles'!X97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J43)*COS('Input Data'!$G$14)))","v":1.7806096146605899},{"$f":"ACOS((COS('Solar Altitude'!K43)*COS('Surface Solar Azimuth Angles'!Y97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K43)*COS('Input Data'!$G$14)))","v":1.9860860581317152},{"$f":"ACOS((COS('Solar Altitude'!L43)*COS('Surface Solar Azimuth Angles'!Z97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L43)*COS('Input Data'!$G$14)))","v":2.1666311175630431},{"$f":"ACOS((COS('Solar Altitude'!M43)*COS('Surface Solar Azimuth Angles'!AA97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M43)*COS('Input Data'!$G$14)))","v":2.3262877609453998},{"$f":"ACOS((COS('Solar Altitude'!N43)*COS('Surface Solar Azimuth Angles'!AB97)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N43)*COS('Input Data'!$G$14)))","v":2.3951645565311219}]
[null,14,{"$f":"ACOS((COS('Solar Altitude'!C44)*COS('Surface Solar Azimuth Angles'!C98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C44)*COS('Input Data'!$G$14)))","v":1.1553813198847913},{"$f":"ACOS((COS('Solar Altitude'!D44)*COS('Surface Solar Azimuth Angles'!D98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D44)*COS('Input Data'!$G$14)))","v":1.1468225663116194},{"$f":"ACOS((COS('Solar Altitude'!E44)*COS('Surface Solar Azimuth Angles'!E98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E44)*COS('Input Data'!$G$14)))","v":1.1110475129987232},{"$f":"ACOS((COS('Solar Altitude'!F44)*COS('Surface Solar Azimuth Angles'!F98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F44)*COS('Input Data'!$G$14)))","v":1.0851511235899753},{"$f":"ACOS((COS('Solar Altitude'!G44)*COS('Surface Solar Azimuth Angles'!G98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G44)*COS('Input Data'!$G$14)))","v":1.0980939366290343},{"$f":"ACOS((COS('Solar Altitude'!H44)*COS('Surface Solar Azimuth Angles'!H98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H44)*COS('Input Data'!$G$14)))","v":1.1276204932770384},{"$f":"ACOS((COS('Solar Altitude'!I44)*COS('Surface Solar Azimuth Angles'!I98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I44)*COS('Input Data'!$G$14)))","v":1.1369347675927413},{"$f":"ACOS((COS('Solar Altitude'!J44)*COS('Surface Solar Azimuth Angles'!J98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J44)*COS('Input Data'!$G$14)))","v":1.1003825727092509},{"$f":"ACOS((COS('Solar Altitude'!K44)*COS('Surface Solar Azimuth Angles'!K98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K44)*COS('Input Data'!$G$14)))","v":1.0455976660489361},{"$f":"ACOS((COS('Solar Altitude'!L44)*COS('Surface Solar Azimuth Angles'!L98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L44)*COS('Input Data'!$G$14)))","v":1.0219835904068333},{"$f":"ACOS((COS('Solar Altitude'!M44)*COS('Surface Solar Azimuth Angles'!M98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M44)*COS('Input Data'!$G$14)))","v":1.0545383748715724},{"$f":"ACOS((COS('Solar Altitude'!N44)*COS('Surface Solar Azimuth Angles'!N98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N44)*COS('Input Data'!$G$14)))","v":1.1158769644052287},null,14,{"$f":"ACOS((COS('Solar Altitude'!C44)*COS('Surface Solar Azimuth Angles'!Q98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C44)*COS('Input Data'!$G$14)))","v":2.2971164237006967},{"$f":"ACOS((COS('Solar Altitude'!D44)*COS('Surface Solar Azimuth Angles'!R98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D44)*COS('Input Data'!$G$14)))","v":2.1414160566604314},{"$f":"ACOS((COS('Solar Altitude'!E44)*COS('Surface Solar Azimuth Angles'!S98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E44)*COS('Input Data'!$G$14)))","v":1.954629449408245},{"$f":"ACOS((COS('Solar Altitude'!F44)*COS('Surface Solar Azimuth Angles'!T98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F44)*COS('Input Data'!$G$14)))","v":1.7436831014326506},{"$f":"ACOS((COS('Solar Altitude'!G44)*COS('Surface Solar Azimuth Angles'!U98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G44)*COS('Input Data'!$G$14)))","v":1.5982423810045241},{"$f":"ACOS((COS('Solar Altitude'!H44)*COS('Surface Solar Azimuth Angles'!V98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H44)*COS('Input Data'!$G$14)))","v":1.5481546154270347},{"$f":"ACOS((COS('Solar Altitude'!I44)*COS('Surface Solar Azimuth Angles'!W98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I44)*COS('Input Data'!$G$14)))","v":1.6024071284345123},{"$f":"ACOS((COS('Solar Altitude'!J44)*COS('Surface Solar Azimuth Angles'!X98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J44)*COS('Input Data'!$G$14)))","v":1.7432425812631809},{"$f":"ACOS((COS('Solar Altitude'!K44)*COS('Surface Solar Azimuth Angles'!Y98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K44)*COS('Input Data'!$G$14)))","v":1.9407248257406897},{"$f":"ACOS((COS('Solar Altitude'!L44)*COS('Surface Solar Azimuth Angles'!Z98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L44)*COS('Input Data'!$G$14)))","v":2.113713726812573},{"$f":"ACOS((COS('Solar Altitude'!M44)*COS('Surface Solar Azimuth Angles'!AA98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M44)*COS('Input Data'!$G$14)))","v":2.2700602022294234},{"$f":"ACOS((COS('Solar Altitude'!N44)*COS('Surface Solar Azimuth Angles'!AB98)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N44)*COS('Input Data'!$G$14)))","v":2.3434877130566418}]
[null,15,{"$f":"ACOS((COS('Solar Altitude'!C45)*COS('Surface Solar Azimuth Angles'!C99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C45)*COS('Input Data'!$G$14)))","v":0.91520546706612593},{"$f":"ACOS((COS('Solar Altitude'!D45)*COS('Surface Solar Azimuth Angles'!D99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D45)*COS('Input Data'!$G$14)))","v":0.89127946347861597},{"$f":"ACOS((COS('Solar Altitude'!E45)*COS('Surface Solar Azimuth Angles'!E99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E45)*COS('Input Data'!$G$14)))","v":0.84924812519957393},{"$f":"ACOS((COS('Solar Altitude'!F45)*COS('Surface Solar Azimuth Angles'!F99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F45)*COS('Input Data'!$G$14)))","v":0.83191971962990974},{"$f":"ACOS((COS('Solar Altitude'!G45)*COS('Surface Solar Azimuth Angles'!G99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G45)*COS('Input Data'!$G$14)))","v":0.86057334741430813},{"$f":"ACOS((COS('Solar Altitude'!H45)*COS('Surface Solar Azimuth Angles'!H99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H45)*COS('Input Data'!$G$14)))","v":0.89680760766268874},{"$f":"ACOS((COS('Solar Altitude'!I45)*COS('Surface Solar Azimuth Angles'!I99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I45)*COS('Input Data'!$G$14)))","v":0.898613058253383},{"$f":"ACOS((COS('Solar Altitude'!J45)*COS('Surface Solar Azimuth Angles'!J99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J45)*COS('Input Data'!$G$14)))","v":0.84724913998719509},{"$f":"ACOS((COS('Solar Altitude'!K45)*COS('Surface Solar Azimuth Angles'!K99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K45)*COS('Input Data'!$G$14)))","v":0.78379827824978654},{"$f":"ACOS((COS('Solar Altitude'!L45)*COS('Surface Solar Azimuth Angles'!L99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L45)*COS('Input Data'!$G$14)))","v":0.7678340723708158},{"$f":"ACOS((COS('Solar Altitude'!M45)*COS('Surface Solar Azimuth Angles'!M99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M45)*COS('Input Data'!$G$14)))","v":0.8176454979135398},{"$f":"ACOS((COS('Solar Altitude'!N45)*COS('Surface Solar Azimuth Angles'!N99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N45)*COS('Input Data'!$G$14)))","v":0.88556064938911194},null,15,{"$f":"ACOS((COS('Solar Altitude'!C45)*COS('Surface Solar Azimuth Angles'!Q99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C45)*COS('Input Data'!$G$14)))","v":2.2248187423439916},{"$f":"ACOS((COS('Solar Altitude'!D45)*COS('Surface Solar Azimuth Angles'!R99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D45)*COS('Input Data'!$G$14)))","v":2.0748177299399062},{"$f":"ACOS((COS('Solar Altitude'!E45)*COS('Surface Solar Azimuth Angles'!S99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E45)*COS('Input Data'!$G$14)))","v":1.8899129440752502},{"$f":"ACOS((COS('Solar Altitude'!F45)*COS('Surface Solar Azimuth Angles'!T99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F45)*COS('Input Data'!$G$14)))","v":1.6803137899438583},{"$f":"ACOS((COS('Solar Altitude'!G45)*COS('Surface Solar Azimuth Angles'!U99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G45)*COS('Input Data'!$G$14)))","v":1.537316689623432},{"$f":"ACOS((COS('Solar Altitude'!H45)*COS('Surface Solar Azimuth Angles'!V99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H45)*COS('Input Data'!$G$14)))","v":1.490144700514989},{"$f":"ACOS((COS('Solar Altitude'!I45)*COS('Surface Solar Azimuth Angles'!W99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I45)*COS('Input Data'!$G$14)))","v":1.5450161512455274},{"$f":"ACOS((COS('Solar Altitude'!J45)*COS('Surface Solar Azimuth Angles'!X99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J45)*COS('Input Data'!$G$14)))","v":1.6812572492678202},{"$f":"ACOS((COS('Solar Altitude'!K45)*COS('Surface Solar Azimuth Angles'!Y99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K45)*COS('Input Data'!$G$14)))","v":1.8702555449806497},{"$f":"ACOS((COS('Solar Altitude'!L45)*COS('Surface Solar Azimuth Angles'!Z99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L45)*COS('Input Data'!$G$14)))","v":2.0357256329653417},{"$f":"ACOS((COS('Solar Altitude'!M45)*COS('Surface Solar Azimuth Angles'!AA99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M45)*COS('Input Data'!$G$14)))","v":2.1881416672511564},{"$f":"ACOS((COS('Solar Altitude'!N45)*COS('Surface Solar Azimuth Angles'!AB99)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N45)*COS('Input Data'!$G$14)))","v":2.2640942068939451}]
[null,16,{"$f":"ACOS((COS('Solar Altitude'!C46)*COS('Surface Solar Azimuth Angles'!C100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C46)*COS('Input Data'!$G$14)))","v":0.68543993462584729},{"$f":"ACOS((COS('Solar Altitude'!D46)*COS('Surface Solar Azimuth Angles'!D100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D46)*COS('Input Data'!$G$14)))","v":0.63911605270796545},{"$f":"ACOS((COS('Solar Altitude'!E46)*COS('Surface Solar Azimuth Angles'!E100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E46)*COS('Input Data'!$G$14)))","v":0.58744873740042447},{"$f":"ACOS((COS('Solar Altitude'!F46)*COS('Surface Solar Azimuth Angles'!F100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F46)*COS('Input Data'!$G$14)))","v":0.5840402196661526},{"$f":"ACOS((COS('Solar Altitude'!G46)*COS('Surface Solar Azimuth Angles'!G100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G46)*COS('Input Data'!$G$14)))","v":0.63633548918141036},{"$f":"ACOS((COS('Solar Altitude'!H46)*COS('Surface Solar Azimuth Angles'!H100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H46)*COS('Input Data'!$G$14)))","v":0.68111295315247578},{"$f":"ACOS((COS('Solar Altitude'!I46)*COS('Surface Solar Azimuth Angles'!I100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I46)*COS('Input Data'!$G$14)))","v":0.67199988705438185},{"$f":"ACOS((COS('Solar Altitude'!J46)*COS('Surface Solar Azimuth Angles'!J100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J46)*COS('Input Data'!$G$14)))","v":0.59931525089067894},{"$f":"ACOS((COS('Solar Altitude'!K46)*COS('Surface Solar Azimuth Angles'!K100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K46)*COS('Input Data'!$G$14)))","v":0.52199889045063785},{"$f":"ACOS((COS('Solar Altitude'!L46)*COS('Surface Solar Azimuth Angles'!L100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L46)*COS('Input Data'!$G$14)))","v":0.5193705415784573},{"$f":"ACOS((COS('Solar Altitude'!M46)*COS('Surface Solar Azimuth Angles'!M100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M46)*COS('Input Data'!$G$14)))","v":0.59590140421839499},{"$f":"ACOS((COS('Solar Altitude'!N46)*COS('Surface Solar Azimuth Angles'!N100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N46)*COS('Input Data'!$G$14)))","v":0.67101159548017864},null,16,{"$f":"ACOS((COS('Solar Altitude'!C46)*COS('Surface Solar Azimuth Angles'!Q100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C46)*COS('Input Data'!$G$14)))","v":2.132061970193921},{"$f":"ACOS((COS('Solar Altitude'!D46)*COS('Surface Solar Azimuth Angles'!R100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D46)*COS('Input Data'!$G$14)))","v":1.9869272292612725},{"$f":"ACOS((COS('Solar Altitude'!E46)*COS('Surface Solar Azimuth Angles'!S100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E46)*COS('Input Data'!$G$14)))","v":1.8045167007635965},{"$f":"ACOS((COS('Solar Altitude'!F46)*COS('Surface Solar Azimuth Angles'!T100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F46)*COS('Input Data'!$G$14)))","v":1.5971546012268536},{"$f":"ACOS((COS('Solar Altitude'!G46)*COS('Surface Solar Azimuth Angles'!U100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G46)*COS('Input Data'!$G$14)))","v":1.4569624794097029},{"$f":"ACOS((COS('Solar Altitude'!H46)*COS('Surface Solar Azimuth Angles'!V100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H46)*COS('Input Data'!$G$14)))","v":1.4124993875820657},{"$f":"ACOS((COS('Solar Altitude'!I46)*COS('Surface Solar Azimuth Angles'!W100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I46)*COS('Input Data'!$G$14)))","v":1.4675268692766898},{"$f":"ACOS((COS('Solar Altitude'!J46)*COS('Surface Solar Azimuth Angles'!X100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J46)*COS('Input Data'!$G$14)))","v":1.5991895480551113},{"$f":"ACOS((COS('Solar Altitude'!K46)*COS('Surface Solar Azimuth Angles'!Y100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K46)*COS('Input Data'!$G$14)))","v":1.7806883538080802},{"$f":"ACOS((COS('Solar Altitude'!L46)*COS('Surface Solar Azimuth Angles'!Z100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L46)*COS('Input Data'!$G$14)))","v":1.9401614196135741},{"$f":"ACOS((COS('Solar Altitude'!M46)*COS('Surface Solar Azimuth Angles'!AA100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M46)*COS('Input Data'!$G$14)))","v":2.0894547233323402},{"$f":"ACOS((COS('Solar Altitude'!N46)*COS('Surface Solar Azimuth Angles'!AB100)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N46)*COS('Input Data'!$G$14)))","v":2.1666019724586238}]
[null,17,{"$f":"ACOS((COS('Solar Altitude'!C47)*COS('Surface Solar Azimuth Angles'!C101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C47)*COS('Input Data'!$G$14)))","v":0.48237186136461574},{"$f":"ACOS((COS('Solar Altitude'!D47)*COS('Surface Solar Azimuth Angles'!D101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D47)*COS('Input Data'!$G$14)))","v":0.39724088446373274},{"$f":"ACOS((COS('Solar Altitude'!E47)*COS('Surface Solar Azimuth Angles'!E101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E47)*COS('Input Data'!$G$14)))","v":0.32564934960127578},{"$f":"ACOS((COS('Solar Altitude'!F47)*COS('Surface Solar Azimuth Angles'!F101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F47)*COS('Input Data'!$G$14)))","v":0.35348129320527955},{"$f":"ACOS((COS('Solar Altitude'!G47)*COS('Surface Solar Azimuth Angles'!G101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G47)*COS('Input Data'!$G$14)))","v":0.4470080424590881},{"$f":"ACOS((COS('Solar Altitude'!H47)*COS('Surface Solar Azimuth Angles'!H101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H47)*COS('Input Data'!$G$14)))","v":0.50184862387126805},{"$f":"ACOS((COS('Solar Altitude'!I47)*COS('Surface Solar Azimuth Angles'!I101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I47)*COS('Input Data'!$G$14)))","v":0.47535745896420911},{"$f":"ACOS((COS('Solar Altitude'!J47)*COS('Surface Solar Azimuth Angles'!J101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J47)*COS('Input Data'!$G$14)))","v":0.36778729059036208},{"$f":"ACOS((COS('Solar Altitude'!K47)*COS('Surface Solar Azimuth Angles'!K101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K47)*COS('Input Data'!$G$14)))","v":0.26019950265148806},{"$f":"ACOS((COS('Solar Altitude'!L47)*COS('Surface Solar Azimuth Angles'!L101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L47)*COS('Input Data'!$G$14)))","v":0.291947948849407},{"$f":"ACOS((COS('Solar Altitude'!M47)*COS('Surface Solar Azimuth Angles'!M101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M47)*COS('Input Data'!$G$14)))","v":0.4154308062088683},{"$f":"ACOS((COS('Solar Altitude'!N47)*COS('Surface Solar Azimuth Angles'!N101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N47)*COS('Input Data'!$G$14)))","v":0.49460277338763348},null,17,{"$f":"ACOS((COS('Solar Altitude'!C47)*COS('Surface Solar Azimuth Angles'!Q101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C47)*COS('Input Data'!$G$14)))","v":2.0274353919291159},{"$f":"ACOS((COS('Solar Altitude'!D47)*COS('Surface Solar Azimuth Angles'!R101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D47)*COS('Input Data'!$G$14)))","v":1.8852954465096339},{"$f":"ACOS((COS('Solar Altitude'!E47)*COS('Surface Solar Azimuth Angles'!S101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E47)*COS('Input Data'!$G$14)))","v":1.7048835033645877},{"$f":"ACOS((COS('Solar Altitude'!F47)*COS('Surface Solar Azimuth Angles'!T101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F47)*COS('Input Data'!$G$14)))","v":1.4995850805998121},{"$f":"ACOS((COS('Solar Altitude'!G47)*COS('Surface Solar Azimuth Angles'!U101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G47)*COS('Input Data'!$G$14)))","v":1.3618369405535742},{"$f":"ACOS((COS('Solar Altitude'!H47)*COS('Surface Solar Azimuth Angles'!V101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H47)*COS('Input Data'!$G$14)))","v":1.3195567973823119},{"$f":"ACOS((COS('Solar Altitude'!I47)*COS('Surface Solar Azimuth Angles'!W101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I47)*COS('Input Data'!$G$14)))","v":1.374485810531499},{"$f":"ACOS((COS('Solar Altitude'!J47)*COS('Surface Solar Azimuth Angles'!X101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J47)*COS('Input Data'!$G$14)))","v":1.5023724602710173},{"$f":"ACOS((COS('Solar Altitude'!K47)*COS('Surface Solar Azimuth Angles'!Y101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K47)*COS('Input Data'!$G$14)))","v":1.6785105552640265},{"$f":"ACOS((COS('Solar Altitude'!L47)*COS('Surface Solar Azimuth Angles'!Z101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L47)*COS('Input Data'!$G$14)))","v":1.8344185233750623},{"$f":"ACOS((COS('Solar Altitude'!M47)*COS('Surface Solar Azimuth Angles'!AA101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M47)*COS('Input Data'!$G$14)))","v":1.9821496713446429},{"$f":"ACOS((COS('Solar Altitude'!N47)*COS('Surface Solar Azimuth Angles'!AB101)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N47)*COS('Input Data'!$G$14)))","v":2.059712668510409}]
[null,18,{"$f":"ACOS((COS('Solar Altitude'!C48)*COS('Surface Solar Azimuth Angles'!C102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C48)*COS('Input Data'!$G$14)))","v":0.35604931493582037},{"$f":"ACOS((COS('Solar Altitude'!D48)*COS('Surface Solar Azimuth Angles'!D102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D48)*COS('Input Data'!$G$14)))","v":0.20628412079335212},{"$f":"ACOS((COS('Solar Altitude'!E48)*COS('Surface Solar Azimuth Angles'!E102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E48)*COS('Input Data'!$G$14)))","v":6.3849961802124877E-2},{"$f":"ACOS((COS('Solar Altitude'!F48)*COS('Surface Solar Azimuth Angles'!F102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F48)*COS('Input Data'!$G$14)))","v":0.20933204336545508},{"$f":"ACOS((COS('Solar Altitude'!G48)*COS('Surface Solar Azimuth Angles'!G102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G48)*COS('Input Data'!$G$14)))","v":0.35467978305383152},{"$f":"ACOS((COS('Solar Altitude'!H48)*COS('Surface Solar Azimuth Angles'!H102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H48)*COS('Input Data'!$G$14)))","v":0.41087459648158164},{"$f":"ACOS((COS('Solar Altitude'!I48)*COS('Surface Solar Azimuth Angles'!I102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I48)*COS('Input Data'!$G$14)))","v":0.36229049170682925},{"$f":"ACOS((COS('Solar Altitude'!J48)*COS('Surface Solar Azimuth Angles'!J102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J48)*COS('Input Data'!$G$14)))","v":0.21518258486844899},{"$f":"ACOS((COS('Solar Altitude'!K48)*COS('Surface Solar Azimuth Angles'!K102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K48)*COS('Input Data'!$G$14)))","v":1.5998851476628495E-3},{"$f":"ACOS((COS('Solar Altitude'!L48)*COS('Surface Solar Azimuth Angles'!L102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L48)*COS('Input Data'!$G$14)))","v":0.19016188263431122},{"$f":"ACOS((COS('Solar Altitude'!M48)*COS('Surface Solar Azimuth Angles'!M102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M48)*COS('Input Data'!$G$14)))","v":0.34848730352122037},{"$f":"ACOS((COS('Solar Altitude'!N48)*COS('Surface Solar Azimuth Angles'!N102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N48)*COS('Input Data'!$G$14)))","v":0.40995107161716771},null,18,{"$f":"ACOS((COS('Solar Altitude'!C48)*COS('Surface Solar Azimuth Angles'!Q102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C48)*COS('Input Data'!$G$14)))","v":1.9183886112794648},{"$f":"ACOS((COS('Solar Altitude'!D48)*COS('Surface Solar Azimuth Angles'!R102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D48)*COS('Input Data'!$G$14)))","v":1.7770187479965736},{"$f":"ACOS((COS('Solar Altitude'!E48)*COS('Surface Solar Azimuth Angles'!S102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E48)*COS('Input Data'!$G$14)))","v":1.5974621584847331},{"$f":"ACOS((COS('Solar Altitude'!F48)*COS('Surface Solar Azimuth Angles'!T102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F48)*COS('Input Data'!$G$14)))","v":1.3932903061282442},{"$f":"ACOS((COS('Solar Altitude'!G48)*COS('Surface Solar Azimuth Angles'!U102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G48)*COS('Input Data'!$G$14)))","v":1.2570344629203938},{"$f":"ACOS((COS('Solar Altitude'!H48)*COS('Surface Solar Azimuth Angles'!V102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H48)*COS('Input Data'!$G$14)))","v":1.2161388471927161},{"$f":"ACOS((COS('Solar Altitude'!I48)*COS('Surface Solar Azimuth Angles'!W102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I48)*COS('Input Data'!$G$14)))","v":1.2709136474283964},{"$f":"ACOS((COS('Solar Altitude'!J48)*COS('Surface Solar Azimuth Angles'!X102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J48)*COS('Input Data'!$G$14)))","v":1.396465415451092},{"$f":"ACOS((COS('Solar Altitude'!K48)*COS('Surface Solar Azimuth Angles'!Y102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K48)*COS('Input Data'!$G$14)))","v":1.5701277877052278},{"$f":"ACOS((COS('Solar Altitude'!L48)*COS('Surface Solar Azimuth Angles'!Z102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L48)*COS('Input Data'!$G$14)))","v":1.7252824834230673},{"$f":"ACOS((COS('Solar Altitude'!M48)*COS('Surface Solar Azimuth Angles'!AA102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M48)*COS('Input Data'!$G$14)))","v":1.873193821722281},{"$f":"ACOS((COS('Solar Altitude'!N48)*COS('Surface Solar Azimuth Angles'!AB102)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N48)*COS('Input Data'!$G$14)))","v":1.9506604587086183}]
[null,19,{"$f":"ACOS((COS('Solar Altitude'!C49)*COS('Surface Solar Azimuth Angles'!C103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C49)*COS('Input Data'!$G$14)))","v":0.39030998799189986},{"$f":"ACOS((COS('Solar Altitude'!D49)*COS('Surface Solar Azimuth Angles'!D103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D49)*COS('Input Data'!$G$14)))","v":0.25060691805980406},{"$f":"ACOS((COS('Solar Altitude'!E49)*COS('Surface Solar Azimuth Angles'!E103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E49)*COS('Input Data'!$G$14)))","v":0.1979494259970247},{"$f":"ACOS((COS('Solar Altitude'!F49)*COS('Surface Solar Azimuth Angles'!F103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F49)*COS('Input Data'!$G$14)))","v":0.31270170290585697},{"$f":"ACOS((COS('Solar Altitude'!G49)*COS('Surface Solar Azimuth Angles'!G103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G49)*COS('Input Data'!$G$14)))","v":0.42783924910737192},{"$f":"ACOS((COS('Solar Altitude'!H49)*COS('Surface Solar Azimuth Angles'!H103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H49)*COS('Input Data'!$G$14)))","v":0.46377004853544346},{"$f":"ACOS((COS('Solar Altitude'!I49)*COS('Surface Solar Azimuth Angles'!I103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I49)*COS('Input Data'!$G$14)))","v":0.40949720864396899},{"$f":"ACOS((COS('Solar Altitude'!J49)*COS('Surface Solar Azimuth Angles'!J103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J49)*COS('Input Data'!$G$14)))","v":0.30391247626034179},{"$f":"ACOS((COS('Solar Altitude'!K49)*COS('Surface Solar Azimuth Angles'!K103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K49)*COS('Input Data'!$G$14)))","v":0.26339927294681176},{"$f":"ACOS((COS('Solar Altitude'!L49)*COS('Surface Solar Azimuth Angles'!L103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L49)*COS('Input Data'!$G$14)))","v":0.35008845072701389},{"$f":"ACOS((COS('Solar Altitude'!M49)*COS('Surface Solar Azimuth Angles'!M103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M49)*COS('Input Data'!$G$14)))","v":0.44921985559011279},{"$f":"ACOS((COS('Solar Altitude'!N49)*COS('Surface Solar Azimuth Angles'!N103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N49)*COS('Input Data'!$G$14)))","v":0.46988201245054695},null,19,{"$f":"ACOS((COS('Solar Altitude'!C49)*COS('Surface Solar Azimuth Angles'!Q103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C49)*COS('Input Data'!$G$14)))","v":1.8113047332631398},{"$f":"ACOS((COS('Solar Altitude'!D49)*COS('Surface Solar Azimuth Angles'!R103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D49)*COS('Input Data'!$G$14)))","v":1.6685742453082473},{"$f":"ACOS((COS('Solar Altitude'!E49)*COS('Surface Solar Azimuth Angles'!S103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E49)*COS('Input Data'!$G$14)))","v":1.488526141265925},{"$f":"ACOS((COS('Solar Altitude'!F49)*COS('Surface Solar Azimuth Angles'!T103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F49)*COS('Input Data'!$G$14)))","v":1.2841540912537528},{"$f":"ACOS((COS('Solar Altitude'!G49)*COS('Surface Solar Azimuth Angles'!U103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G49)*COS('Input Data'!$G$14)))","v":1.1480322880628919},{"$f":"ACOS((COS('Solar Altitude'!H49)*COS('Surface Solar Azimuth Angles'!V103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H49)*COS('Input Data'!$G$14)))","v":1.1074924745156784},{"$f":"ACOS((COS('Solar Altitude'!I49)*COS('Surface Solar Azimuth Angles'!W103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I49)*COS('Input Data'!$G$14)))","v":1.16220704711848},{"$f":"ACOS((COS('Solar Altitude'!J49)*COS('Surface Solar Azimuth Angles'!X103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J49)*COS('Input Data'!$G$14)))","v":1.2873294143206446},{"$f":"ACOS((COS('Solar Altitude'!K49)*COS('Surface Solar Azimuth Angles'!Y103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K49)*COS('Input Data'!$G$14)))","v":1.4617829597416481},{"$f":"ACOS((COS('Solar Altitude'!L49)*COS('Surface Solar Azimuth Angles'!Z103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L49)*COS('Input Data'!$G$14)))","v":1.6189895485184089},{"$f":"ACOS((COS('Solar Altitude'!M49)*COS('Surface Solar Azimuth Angles'!AA103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M49)*COS('Input Data'!$G$14)))","v":1.7686325113077217},{"$f":"ACOS((COS('Solar Altitude'!N49)*COS('Surface Solar Azimuth Angles'!AB103)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N49)*COS('Input Data'!$G$14)))","v":1.8455277298388448}]
[null,20,{"$f":"ACOS((COS('Solar Altitude'!C50)*COS('Surface Solar Azimuth Angles'!C104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C50)*COS('Input Data'!$G$14)))","v":0.55617992945761263},{"$f":"ACOS((COS('Solar Altitude'!D50)*COS('Surface Solar Azimuth Angles'!D104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D50)*COS('Input Data'!$G$14)))","v":0.46748190579132443},{"$f":"ACOS((COS('Solar Altitude'!E50)*COS('Surface Solar Azimuth Angles'!E104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E50)*COS('Input Data'!$G$14)))","v":0.45974881379617361},{"$f":"ACOS((COS('Solar Altitude'!F50)*COS('Surface Solar Azimuth Angles'!F104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F50)*COS('Input Data'!$G$14)))","v":0.53552990662876931},{"$f":"ACOS((COS('Solar Altitude'!G50)*COS('Surface Solar Azimuth Angles'!G104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G50)*COS('Input Data'!$G$14)))","v":0.60944599578734515},{"$f":"ACOS((COS('Solar Altitude'!H50)*COS('Surface Solar Azimuth Angles'!H104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H50)*COS('Input Data'!$G$14)))","v":0.62489764543640802},{"$f":"ACOS((COS('Solar Altitude'!I50)*COS('Surface Solar Azimuth Angles'!I104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I50)*COS('Input Data'!$G$14)))","v":0.57894410071375701},{"$f":"ACOS((COS('Solar Altitude'!J50)*COS('Surface Solar Azimuth Angles'!J104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J50)*COS('Input Data'!$G$14)))","v":0.52288275068244228},{"$f":"ACOS((COS('Solar Altitude'!K50)*COS('Surface Solar Azimuth Angles'!K104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K50)*COS('Input Data'!$G$14)))","v":0.52519866074596089},{"$f":"ACOS((COS('Solar Altitude'!L50)*COS('Surface Solar Azimuth Angles'!L104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L50)*COS('Input Data'!$G$14)))","v":0.58683665753500902},{"$f":"ACOS((COS('Solar Altitude'!M50)*COS('Surface Solar Azimuth Angles'!M104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M50)*COS('Input Data'!$G$14)))","v":0.64300944462916765},{"$f":"ACOS((COS('Solar Altitude'!N50)*COS('Surface Solar Azimuth Angles'!N104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N50)*COS('Input Data'!$G$14)))","v":0.63454659679074943},null,20,{"$f":"ACOS((COS('Solar Altitude'!C50)*COS('Surface Solar Azimuth Angles'!Q104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C50)*COS('Input Data'!$G$14)))","v":1.711862852162271},{"$f":"ACOS((COS('Solar Altitude'!D50)*COS('Surface Solar Azimuth Angles'!R104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D50)*COS('Input Data'!$G$14)))","v":1.5660131092712806},{"$f":"ACOS((COS('Solar Altitude'!E50)*COS('Surface Solar Azimuth Angles'!S104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E50)*COS('Input Data'!$G$14)))","v":1.3842998801572985},{"$f":"ACOS((COS('Solar Altitude'!F50)*COS('Surface Solar Azimuth Angles'!T104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F50)*COS('Input Data'!$G$14)))","v":1.178415063055521},{"$f":"ACOS((COS('Solar Altitude'!G50)*COS('Surface Solar Azimuth Angles'!U104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G50)*COS('Input Data'!$G$14)))","v":1.040897268311793},{"$f":"ACOS((COS('Solar Altitude'!H50)*COS('Surface Solar Azimuth Angles'!V104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H50)*COS('Input Data'!$G$14)))","v":0.99949707000065269},{"$f":"ACOS((COS('Solar Altitude'!I50)*COS('Surface Solar Azimuth Angles'!W104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I50)*COS('Input Data'!$G$14)))","v":1.0543095059120096},{"$f":"ACOS((COS('Solar Altitude'!J50)*COS('Surface Solar Azimuth Angles'!X104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J50)*COS('Input Data'!$G$14)))","v":1.1811723768069495},{"$f":"ACOS((COS('Solar Altitude'!K50)*COS('Surface Solar Azimuth Angles'!Y104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K50)*COS('Input Data'!$G$14)))","v":1.3597202234373265},{"$f":"ACOS((COS('Solar Altitude'!L50)*COS('Surface Solar Azimuth Angles'!Z104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L50)*COS('Input Data'!$G$14)))","v":1.5214652833745961},{"$f":"ACOS((COS('Solar Altitude'!M50)*COS('Surface Solar Azimuth Angles'!AA104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M50)*COS('Input Data'!$G$14)))","v":1.6739453387510133},{"$f":"ACOS((COS('Solar Altitude'!N50)*COS('Surface Solar Azimuth Angles'!AB104)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N50)*COS('Input Data'!$G$14)))","v":1.7496818818897109}]
[null,21,{"$f":"ACOS((COS('Solar Altitude'!C51)*COS('Surface Solar Azimuth Angles'!C105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C51)*COS('Input Data'!$G$14)))","v":0.77290105385966568},{"$f":"ACOS((COS('Solar Altitude'!D51)*COS('Surface Solar Azimuth Angles'!D105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D51)*COS('Input Data'!$G$14)))","v":0.71390113191237869},{"$f":"ACOS((COS('Solar Altitude'!E51)*COS('Surface Solar Azimuth Angles'!E105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E51)*COS('Input Data'!$G$14)))","v":0.72154820159532274},{"$f":"ACOS((COS('Solar Altitude'!F51)*COS('Surface Solar Azimuth Angles'!F105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F51)*COS('Input Data'!$G$14)))","v":0.78146382660532199},{"$f":"ACOS((COS('Solar Altitude'!G51)*COS('Surface Solar Azimuth Angles'!G105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G51)*COS('Input Data'!$G$14)))","v":0.83093314764444937},{"$f":"ACOS((COS('Solar Altitude'!H51)*COS('Surface Solar Azimuth Angles'!H105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H51)*COS('Input Data'!$G$14)))","v":0.83334487624187259},{"$f":"ACOS((COS('Solar Altitude'!I51)*COS('Surface Solar Azimuth Angles'!I105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I51)*COS('Input Data'!$G$14)))","v":0.79579418022070669},{"$f":"ACOS((COS('Solar Altitude'!J51)*COS('Surface Solar Azimuth Angles'!J105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J51)*COS('Input Data'!$G$14)))","v":0.76764101795987183},{"$f":"ACOS((COS('Solar Altitude'!K51)*COS('Surface Solar Azimuth Angles'!K105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K51)*COS('Input Data'!$G$14)))","v":0.78699804854510991},{"$f":"ACOS((COS('Solar Altitude'!L51)*COS('Surface Solar Azimuth Angles'!L105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L51)*COS('Input Data'!$G$14)))","v":0.83752510996800245},{"$f":"ACOS((COS('Solar Altitude'!M51)*COS('Surface Solar Azimuth Angles'!M105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M51)*COS('Input Data'!$G$14)))","v":0.86942639458956728},{"$f":"ACOS((COS('Solar Altitude'!N51)*COS('Surface Solar Azimuth Angles'!N105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N51)*COS('Input Data'!$G$14)))","v":0.84440423558933209},null,21,{"$f":"ACOS((COS('Solar Altitude'!C51)*COS('Surface Solar Azimuth Angles'!Q105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C51)*COS('Input Data'!$G$14)))","v":1.6253175887390001},{"$f":"ACOS((COS('Solar Altitude'!D51)*COS('Surface Solar Azimuth Angles'!R105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D51)*COS('Input Data'!$G$14)))","v":1.475177102797383},{"$f":"ACOS((COS('Solar Altitude'!E51)*COS('Surface Solar Azimuth Angles'!S105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E51)*COS('Input Data'!$G$14)))","v":1.2911443231701432},{"$f":"ACOS((COS('Solar Altitude'!F51)*COS('Surface Solar Azimuth Angles'!T105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F51)*COS('Input Data'!$G$14)))","v":1.0829165728011307},{"$f":"ACOS((COS('Solar Altitude'!G51)*COS('Surface Solar Azimuth Angles'!U105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G51)*COS('Input Data'!$G$14)))","v":0.94265188660608557},{"$f":"ACOS((COS('Solar Altitude'!H51)*COS('Surface Solar Azimuth Angles'!V105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H51)*COS('Input Data'!$G$14)))","v":0.89907592756701959},{"$f":"ACOS((COS('Solar Altitude'!I51)*COS('Surface Solar Azimuth Angles'!W105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I51)*COS('Input Data'!$G$14)))","v":0.95406673771386663},{"$f":"ACOS((COS('Solar Altitude'!J51)*COS('Surface Solar Azimuth Angles'!X105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J51)*COS('Input Data'!$G$14)))","v":1.084801810817833},{"$f":"ACOS((COS('Solar Altitude'!K51)*COS('Surface Solar Azimuth Angles'!Y105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K51)*COS('Input Data'!$G$14)))","v":1.2703474640324108},{"$f":"ACOS((COS('Solar Altitude'!L51)*COS('Surface Solar Azimuth Angles'!Z105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L51)*COS('Input Data'!$G$14)))","v":1.438469543533426},{"$f":"ACOS((COS('Solar Altitude'!M51)*COS('Surface Solar Azimuth Angles'!AA105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M51)*COS('Input Data'!$G$14)))","v":1.5942397385974927},{"$f":"ACOS((COS('Solar Altitude'!N51)*COS('Surface Solar Azimuth Angles'!AB105)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N51)*COS('Input Data'!$G$14)))","v":1.6680396208878134}]
[null,22,{"$f":"ACOS((COS('Solar Altitude'!C52)*COS('Surface Solar Azimuth Angles'!C106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C52)*COS('Input Data'!$G$14)))","v":1.007812885930562},{"$f":"ACOS((COS('Solar Altitude'!D52)*COS('Surface Solar Azimuth Angles'!D106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D52)*COS('Input Data'!$G$14)))","v":0.96743542428139184},{"$f":"ACOS((COS('Solar Altitude'!E52)*COS('Surface Solar Azimuth Angles'!E106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E52)*COS('Input Data'!$G$14)))","v":0.98334758939447242},{"$f":"ACOS((COS('Solar Altitude'!F52)*COS('Surface Solar Azimuth Angles'!F106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F52)*COS('Input Data'!$G$14)))","v":1.0339937841271984},{"$f":"ACOS((COS('Solar Altitude'!G52)*COS('Surface Solar Azimuth Angles'!G106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G52)*COS('Input Data'!$G$14)))","v":1.0673310152478241},{"$f":"ACOS((COS('Solar Altitude'!H52)*COS('Surface Solar Azimuth Angles'!H106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H52)*COS('Input Data'!$G$14)))","v":1.0610438620621692},{"$f":"ACOS((COS('Solar Altitude'!I52)*COS('Surface Solar Azimuth Angles'!I106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I52)*COS('Input Data'!$G$14)))","v":1.0301272173470566},{"$f":"ACOS((COS('Solar Altitude'!J52)*COS('Surface Solar Azimuth Angles'!J106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J52)*COS('Input Data'!$G$14)))","v":1.0196287183015125},{"$f":"ACOS((COS('Solar Altitude'!K52)*COS('Surface Solar Azimuth Angles'!K106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K52)*COS('Input Data'!$G$14)))","v":1.0487974363442598},{"$f":"ACOS((COS('Solar Altitude'!L52)*COS('Surface Solar Azimuth Angles'!L106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L52)*COS('Input Data'!$G$14)))","v":1.0924644016703278},{"$f":"ACOS((COS('Solar Altitude'!M52)*COS('Surface Solar Azimuth Angles'!M106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M52)*COS('Input Data'!$G$14)))","v":1.1082133650773336},{"$f":"ACOS((COS('Solar Altitude'!N52)*COS('Surface Solar Azimuth Angles'!N106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N52)*COS('Input Data'!$G$14)))","v":1.0727040913382868},null,22,{"$f":"ACOS((COS('Solar Altitude'!C52)*COS('Surface Solar Azimuth Angles'!Q106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C52)*COS('Input Data'!$G$14)))","v":1.5565455664218992},{"$f":"ACOS((COS('Solar Altitude'!D52)*COS('Surface Solar Azimuth Angles'!R106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D52)*COS('Input Data'!$G$14)))","v":1.4017234098690199},{"$f":"ACOS((COS('Solar Altitude'!E52)*COS('Surface Solar Azimuth Angles'!S106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E52)*COS('Input Data'!$G$14)))","v":1.2155570102761952},{"$f":"ACOS((COS('Solar Altitude'!F52)*COS('Surface Solar Azimuth Angles'!T106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F52)*COS('Input Data'!$G$14)))","v":1.0051751834058544},{"$f":"ACOS((COS('Solar Altitude'!G52)*COS('Surface Solar Azimuth Angles'!U106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G52)*COS('Input Data'!$G$14)))","v":0.86153224296886943},{"$f":"ACOS((COS('Solar Altitude'!H52)*COS('Surface Solar Azimuth Angles'!V106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H52)*COS('Input Data'!$G$14)))","v":0.81458685555800214},{"$f":"ACOS((COS('Solar Altitude'!I52)*COS('Surface Solar Azimuth Angles'!W106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I52)*COS('Input Data'!$G$14)))","v":0.86953756455151565},{"$f":"ACOS((COS('Solar Altitude'!J52)*COS('Surface Solar Azimuth Angles'!X106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J52)*COS('Input Data'!$G$14)))","v":1.0057176789024027},{"$f":"ACOS((COS('Solar Altitude'!K52)*COS('Surface Solar Azimuth Angles'!Y106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K52)*COS('Input Data'!$G$14)))","v":1.2001506832418554},{"$f":"ACOS((COS('Solar Altitude'!L52)*COS('Surface Solar Azimuth Angles'!Z106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L52)*COS('Input Data'!$G$14)))","v":1.3754726722587909},{"$f":"ACOS((COS('Solar Altitude'!M52)*COS('Surface Solar Azimuth Angles'!AA106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M52)*COS('Input Data'!$G$14)))","v":1.5341810265167612},{"$f":"ACOS((COS('Solar Altitude'!N52)*COS('Surface Solar Azimuth Angles'!AB106)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N52)*COS('Input Data'!$G$14)))","v":1.6050720236363036}]
[null,23,{"$f":"ACOS((COS('Solar Altitude'!C53)*COS('Surface Solar Azimuth Angles'!C107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C53)*COS('Input Data'!$G$14)))","v":1.2501674562967127},{"$f":"ACOS((COS('Solar Altitude'!D53)*COS('Surface Solar Azimuth Angles'!D107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D53)*COS('Input Data'!$G$14)))","v":1.2235127489866715},{"$f":"ACOS((COS('Solar Altitude'!E53)*COS('Surface Solar Azimuth Angles'!E107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E53)*COS('Input Data'!$G$14)))","v":1.2451469771936217},{"$f":"ACOS((COS('Solar Altitude'!F53)*COS('Surface Solar Azimuth Angles'!F107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F53)*COS('Input Data'!$G$14)))","v":1.2890349274429294},{"$f":"ACOS((COS('Solar Altitude'!G53)*COS('Surface Solar Azimuth Angles'!G107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G53)*COS('Input Data'!$G$14)))","v":1.3099881030728127},{"$f":"ACOS((COS('Solar Altitude'!H53)*COS('Surface Solar Azimuth Angles'!H107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H53)*COS('Input Data'!$G$14)))","v":1.297128120861017},{"$f":"ACOS((COS('Solar Altitude'!I53)*COS('Surface Solar Azimuth Angles'!I107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I53)*COS('Input Data'!$G$14)))","v":1.2717329096930583},{"$f":"ACOS((COS('Solar Altitude'!J53)*COS('Surface Solar Azimuth Angles'!J107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J53)*COS('Input Data'!$G$14)))","v":1.2743476401717797},{"$f":"ACOS((COS('Solar Altitude'!K53)*COS('Surface Solar Azimuth Angles'!K107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K53)*COS('Input Data'!$G$14)))","v":1.3105968241434094},{"$f":"ACOS((COS('Solar Altitude'!L53)*COS('Surface Solar Azimuth Angles'!L107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L53)*COS('Input Data'!$G$14)))","v":1.3490581072371175},{"$f":"ACOS((COS('Solar Altitude'!M53)*COS('Surface Solar Azimuth Angles'!M107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M53)*COS('Input Data'!$G$14)))","v":1.3522145484719399},{"$f":"ACOS((COS('Solar Altitude'!N53)*COS('Surface Solar Azimuth Angles'!N107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N53)*COS('Input Data'!$G$14)))","v":1.3090516376047678},null,23,{"$f":"ACOS((COS('Solar Altitude'!C53)*COS('Surface Solar Azimuth Angles'!Q107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C53)*COS('Input Data'!$G$14)))","v":1.5098088809855712},{"$f":"ACOS((COS('Solar Altitude'!D53)*COS('Surface Solar Azimuth Angles'!R107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D53)*COS('Input Data'!$G$14)))","v":1.3508192340891645},{"$f":"ACOS((COS('Solar Altitude'!E53)*COS('Surface Solar Azimuth Angles'!S107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E53)*COS('Input Data'!$G$14)))","v":1.1637428206199758},{"$f":"ACOS((COS('Solar Altitude'!F53)*COS('Surface Solar Azimuth Angles'!T107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F53)*COS('Input Data'!$G$14)))","v":0.95284089378756753},{"$f":"ACOS((COS('Solar Altitude'!G53)*COS('Surface Solar Azimuth Angles'!U107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G53)*COS('Input Data'!$G$14)))","v":0.80653603194476531},{"$f":"ACOS((COS('Solar Altitude'!H53)*COS('Surface Solar Azimuth Angles'!V107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H53)*COS('Input Data'!$G$14)))","v":0.75556903748020154},{"$f":"ACOS((COS('Solar Altitude'!I53)*COS('Surface Solar Azimuth Angles'!W107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I53)*COS('Input Data'!$G$14)))","v":0.80971603065081799},{"$f":"ACOS((COS('Solar Altitude'!J53)*COS('Surface Solar Azimuth Angles'!X107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J53)*COS('Input Data'!$G$14)))","v":0.95162259476128508},{"$f":"ACOS((COS('Solar Altitude'!K53)*COS('Surface Solar Azimuth Angles'!Y107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K53)*COS('Input Data'!$G$14)))","v":1.1551283546464013},{"$f":"ACOS((COS('Solar Altitude'!L53)*COS('Surface Solar Azimuth Angles'!Z107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L53)*COS('Input Data'!$G$14)))","v":1.337171483781693},{"$f":"ACOS((COS('Solar Altitude'!M53)*COS('Surface Solar Azimuth Angles'!AA107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M53)*COS('Input Data'!$G$14)))","v":1.4976443457090363},{"$f":"ACOS((COS('Solar Altitude'!N53)*COS('Surface Solar Azimuth Angles'!AB107)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N53)*COS('Input Data'!$G$14)))","v":1.5645471015783841}]
[null,24,{"$f":"ACOS((COS('Solar Altitude'!C54)*COS('Surface Solar Azimuth Angles'!C108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C54)*COS('Input Data'!$G$14)))","v":1.4955879913040611},{"$f":"ACOS((COS('Solar Altitude'!D54)*COS('Surface Solar Azimuth Angles'!D108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D54)*COS('Input Data'!$G$14)))","v":1.4805915081989509},{"$f":"ACOS((COS('Solar Altitude'!E54)*COS('Surface Solar Azimuth Angles'!E108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E54)*COS('Input Data'!$G$14)))","v":1.5069463649927737},{"$f":"ACOS((COS('Solar Altitude'!F54)*COS('Surface Solar Azimuth Angles'!F108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F54)*COS('Input Data'!$G$14)))","v":1.545036829652074},{"$f":"ACOS((COS('Solar Altitude'!G54)*COS('Surface Solar Azimuth Angles'!G108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G54)*COS('Input Data'!$G$14)))","v":1.5551092169966878},{"$f":"ACOS((COS('Solar Altitude'!H54)*COS('Surface Solar Azimuth Angles'!H108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H54)*COS('Input Data'!$G$14)))","v":1.5366391027273305},{"$f":"ACOS((COS('Solar Altitude'!I54)*COS('Surface Solar Azimuth Angles'!I108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I54)*COS('Input Data'!$G$14)))","v":1.5163067222733864},{"$f":"ACOS((COS('Solar Altitude'!J54)*COS('Surface Solar Azimuth Angles'!J108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J54)*COS('Input Data'!$G$14)))","v":1.5301239796945516},{"$f":"ACOS((COS('Solar Altitude'!K54)*COS('Surface Solar Azimuth Angles'!K108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K54)*COS('Input Data'!$G$14)))","v":1.5691964416472817},{"$f":"ACOS((COS('Solar Altitude'!L54)*COS('Surface Solar Azimuth Angles'!L108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L54)*COS('Input Data'!$G$14)))","v":1.5353536128156269},{"$f":"ACOS((COS('Solar Altitude'!M54)*COS('Surface Solar Azimuth Angles'!M108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M54)*COS('Input Data'!$G$14)))","v":1.5434449009416611},{"$f":"ACOS((COS('Solar Altitude'!N54)*COS('Surface Solar Azimuth Angles'!N108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N54)*COS('Input Data'!$G$14)))","v":1.5486470318136849},null,24,{"$f":"ACOS((COS('Solar Altitude'!C54)*COS('Surface Solar Azimuth Angles'!Q108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!C54)*COS('Input Data'!$G$14)))","v":1.4882813571357905},{"$f":"ACOS((COS('Solar Altitude'!D54)*COS('Surface Solar Azimuth Angles'!R108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!D54)*COS('Input Data'!$G$14)))","v":1.3264867387484505},{"$f":"ACOS((COS('Solar Altitude'!E54)*COS('Surface Solar Azimuth Angles'!S108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!E54)*COS('Input Data'!$G$14)))","v":1.1406370445810861},{"$f":"ACOS((COS('Solar Altitude'!F54)*COS('Surface Solar Azimuth Angles'!T108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!F54)*COS('Input Data'!$G$14)))","v":0.93218228289666727},{"$f":"ACOS((COS('Solar Altitude'!G54)*COS('Surface Solar Azimuth Angles'!U108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!G54)*COS('Input Data'!$G$14)))","v":0.78547568728297235},{"$f":"ACOS((COS('Solar Altitude'!H54)*COS('Surface Solar Azimuth Angles'!V108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!H54)*COS('Input Data'!$G$14)))","v":0.73081844607596091},{"$f":"ACOS((COS('Solar Altitude'!I54)*COS('Surface Solar Azimuth Angles'!W108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!I54)*COS('Input Data'!$G$14)))","v":0.78284683122564369},{"$f":"ACOS((COS('Solar Altitude'!J54)*COS('Surface Solar Azimuth Angles'!X108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!J54)*COS('Input Data'!$G$14)))","v":0.92895648237173767},{"$f":"ACOS((COS('Solar Altitude'!K54)*COS('Surface Solar Azimuth Angles'!Y108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!K54)*COS('Input Data'!$G$14)))","v":1.1397005902017945},{"$f":"ACOS((COS('Solar Altitude'!L54)*COS('Surface Solar Azimuth Angles'!Z108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!L54)*COS('Input Data'!$G$14)))","v":1.3267254769188106},{"$f":"ACOS((COS('Solar Altitude'!M54)*COS('Surface Solar Azimuth Angles'!AA108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!M54)*COS('Input Data'!$G$14)))","v":1.4871873293984139},{"$f":"ACOS((COS('Solar Altitude'!N54)*COS('Surface Solar Azimuth Angles'!AB108)*SIN('Input Data'!$G$14))+(SIN('Solar Altitude'!N54)*COS('Input Data'!$G$14)))","v":1.5490914645316765}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total Transmitted BTU",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total Transmitted Tons"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"'Operative BP'!C58","v":0},{"$f":"'Operative BP'!D58","v":0},{"$f":"'Operative BP'!E58","v":0},{"$f":"'Operative BP'!F58","v":0},{"$f":"'Operative BP'!G58","v":0},{"$f":"'Operative BP'!H58","v":0},{"$f":"'Operative BP'!I58","v":0},{"$f":"'Operative BP'!J58","v":0},{"$f":"'Operative BP'!K58","v":0},{"$f":"'Operative BP'!L58","v":0},{"$f":"'Operative BP'!M58","v":0},{"$f":"'Operative BP'!N58","v":0},null,null,null,1,{"$f":"BJ115*0.000083333","v":0},{"$f":"BK115*0.000083333","v":0},0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,{"$f":"'Operative BP'!C59","v":0},{"$f":"'Operative BP'!D59","v":0},{"$f":"'Operative BP'!E59","v":0},{"$f":"'Operative BP'!F59","v":0},{"$f":"'Operative BP'!G59","v":0},{"$f":"'Operative BP'!H59","v":0},{"$f":"'Operative BP'!I59","v":0},{"$f":"'Operative BP'!J59","v":0},{"$f":"'Operative BP'!K59","v":0},{"$f":"'Operative BP'!L59","v":0},{"$f":"'Operative BP'!M59","v":0},{"$f":"'Operative BP'!N59","v":0},null,null,null,2,{"$f":"BJ116*0.000083333","v":0},{"$f":"BK116*0.000083333","v":0},{"$f":"BL116*0.000083333","v":0},{"$f":"BM116*0.000083333","v":0},{"$f":"BN116*0.000083333","v":0},{"$f":"BO116*0.000083333","v":0},{"$f":"BP116*0.000083333","v":0},{"$f":"BQ116*0.000083333","v":0},{"$f":"BR116*0.000083333","v":0},{"$f":"BS116*0.000083333","v":0},{"$f":"BT116*0.000083333","v":0},{"$f":"BU116*0.000083333","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3,{"$f":"'Operative BP'!C60","v":0},{"$f":"'Operative BP'!D60","v":0},{"$f":"'Operative BP'!E60","v":0},{"$f":"'Operative BP'!F60","v":0},{"$f":"'Operative BP'!G60","v":0},{"$f":"'Operative BP'!H60","v":0},{"$f":"'Operative BP'!I60","v":0},{"$f":"'Operative BP'!J60","v":0},{"$f":"'Operative BP'!K60","v":0},{"$f":"'Operative BP'!L60","v":0},{"$f":"'Operative BP'!M60","v":0},{"$f":"'Operative BP'!N60","v":0},null,null,null,3,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4,{"$f":"'Operative BP'!C61","v":0},{"$f":"'Operative BP'!D61","v":0},{"$f":"'Operative BP'!E61","v":0},{"$f":"'Operative BP'!F61","v":0},{"$f":"'Operative BP'!G61","v":0},{"$f":"'Operative BP'!H61","v":0},{"$f":"'Operative BP'!I61","v":0},{"$f":"'Operative BP'!J61","v":0},{"$f":"'Operative BP'!K61","v":0},{"$f":"'Operative BP'!L61","v":0},{"$f":"'Operative BP'!M61","v":0},{"$f":"'Operative BP'!N61","v":0},null,null,null,4,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,{"$f":"'Operative BP'!C62","v":0},{"$f":"'Operative BP'!D62","v":0},{"$f":"'Operative BP'!E62","v":0},{"$f":"'Operative BP'!F62","v":0},{"$f":"'Operative BP'!G62","v":0},{"$f":"'Operative BP'!H62","v":0},{"$f":"'Operative BP'!I62","v":0},{"$f":"'Operative BP'!J62","v":0},{"$f":"'Operative BP'!K62","v":0},{"$f":"'Operative BP'!L62","v":0},{"$f":"'Operative BP'!M62","v":0},{"$f":"'Operative BP'!N62","v":0},null,null,null,5,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,{"$f":"'Operative BP'!C63","v":0},{"$f":"'Operative BP'!D63","v":0},{"$f":"'Operative BP'!E63","v":0},{"$f":"'Operative BP'!F63","v":85.291254678098866},{"$f":"'Operative BP'!G63","v":200.04067612922577},{"$f":"'Operative BP'!H63","v":238.69148403224921},{"$f":"'Operative BP'!I63","v":151.55996159633474},{"$f":"'Operative BP'!J63","v":85.484580900045813},{"$f":"'Operative BP'!K63","v":49.076156240520959},{"$f":"'Operative BP'!L63","v":0},{"$f":"'Operative BP'!M63","v":0},{"$f":"'Operative BP'!N63","v":0},null,null,null,6,0,0,0,7.1075761260900126E-3,1.6669989663876769E-2,1.9890877438859422E-2,1.2629946279707363E-2,7.1236865801435172E-3,4.0896633279913332E-3,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7,{"$f":"'Operative BP'!C64","v":64.898513253972396},{"$f":"'Operative BP'!D64","v":165.40677030899579},{"$f":"'Operative BP'!E64","v":477.20353172430015},{"$f":"'Operative BP'!F64","v":1430.2072767776865},{"$f":"'Operative BP'!G64","v":1823.5313692542443},{"$f":"'Operative BP'!H64","v":1967.8167757820027},{"$f":"'Operative BP'!I64","v":1633.0294584747032},{"$f":"'Operative BP'!J64","v":1462.7309965171892},{"$f":"'Operative BP'!K64","v":1232.2064066489952},{"$f":"'Operative BP'!L64","v":786.71694263200231},{"$f":"'Operative BP'!M64","v":234.94895166423882},{"$f":"'Operative BP'!N64","v":97.889730060419623},null,null,null,7,5.4081878049932813E-3,1.3783842390159546E-2,3.9766801909181103E-2,0.11918346299571494,0.15196033959406394,0.16398407537624163,0.13608524386307244,0.12189376213276693,0.10268345648528071,6.5559482980352649E-2,1.9579000989036012E-2,8.157444875124948E-3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,{"$f":"'Operative BP'!C65","v":1241.5929894223018},{"$f":"'Operative BP'!D65","v":1580.2679856218936},{"$f":"'Operative BP'!E65","v":2274.2562020804671},{"$f":"'Operative BP'!F65","v":3450.0632210657404},{"$f":"'Operative BP'!G65","v":3430.0891695915338},{"$f":"'Operative BP'!H65","v":3624.4253921251366},{"$f":"'Operative BP'!I65","v":3506.0504040840974},{"$f":"'Operative BP'!J65","v":3701.4693967750522},{"$f":"'Operative BP'!K65","v":3245.9243592338794},{"$f":"'Operative BP'!L65","v":2588.9845220993402},{"$f":"'Operative BP'!M65","v":1925.9803833288147},{"$f":"'Operative BP'!N65","v":1308.3238737193474},null,null,null,8,0.10346566858752868,0.13168847204582926,0.18952059208797156,0.28750411840107132,0.28583962076957126,0.30203424120196398,0.29216969832354006,0.30845454924145543,0.27049261462803686,0.21574784718010431,0.1604977232839401,0.10902655336865437]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,{"$f":"'Operative BP'!C66","v":2749.2275008212341},{"$f":"'Operative BP'!D66","v":2537.8051388230988},{"$f":"'Operative BP'!E66","v":2912.014825963},{"$f":"'Operative BP'!F66","v":3360.4158657250155},{"$f":"'Operative BP'!G66","v":3200.4903267677082},{"$f":"'Operative BP'!H66","v":3403.2308082119139},{"$f":"'Operative BP'!I66","v":3720.9239883772384},{"$f":"'Operative BP'!J66","v":3826.0863600764724},{"$f":"'Operative BP'!K66","v":3354.2128592006602},{"$f":"'Operative BP'!L66","v":2988.0593283731764},{"$f":"'Operative BP'!M66","v":3099.6411159120394},{"$f":"'Operative BP'!N66","v":2349.5832515431184},null,null,null,9,0.22910137532593589,0.21148291563354529,0.24266693149197466,0.2800335353384627,0.26670646040053342,0.28360143294072343,0.3100757587234404,0.31883925464425267,0.27951662019576862,0.24900394801132189,0.25830239311229797,0.19579782110084268]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"'Operative BP'!C67","v":2690.2536552472798},{"$f":"'Operative BP'!D67","v":1812.2695779055475},{"$f":"'Operative BP'!E67","v":1259.1168271411946},{"$f":"'Operative BP'!F67","v":97.570769643937751},{"$f":"'Operative BP'!G67","v":0},{"$f":"'Operative BP'!H67","v":0},{"$f":"'Operative BP'!I67","v":8.4277910379317671},{"$f":"'Operative BP'!J67","v":454.16199224679519},{"$f":"'Operative BP'!K67","v":433.5569407707585},{"$f":"'Operative BP'!L67","v":753.06035235792501},{"$f":"'Operative BP'!M67","v":2427.8881685207261},{"$f":"'Operative BP'!N67","v":2340.1429247453757},null,null,null,10,0.22418690785272155,0.15102186073560298,0.10492598255615716,8.130864946738264E-3,0,0,7.023131105639679E-4,3.784668129990218E-2,3.6129600545249614E-2,6.2754778343042966E-2,0.20232320474733767,0.19501113034780637]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11,{"$f":"'Operative BP'!C68","v":2137.1317305137704},{"$f":"'Operative BP'!D68","v":246.19203113518182},{"$f":"'Operative BP'!E68","v":0},{"$f":"'Operative BP'!F68","v":0},{"$f":"'Operative BP'!G68","v":0},{"$f":"'Operative BP'!H68","v":0},{"$f":"'Operative BP'!I68","v":0},{"$f":"'Operative BP'!J68","v":0},{"$f":"'Operative BP'!K68","v":0},{"$f":"'Operative BP'!L68","v":254.59312019607125},{"$f":"'Operative BP'!M68","v":2668.0021945218805},{"$f":"'Operative BP'!N68","v":2449.42891745922},null,null,null,11,0.17809359849890402,2.0515920530588105E-2,0,0,0,0,0,0,0,2.1216008485299205E-2,0.22233262687609184,0.20411825997862917]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,{"$f":"'Operative BP'!C69","v":2660.7704140368955},{"$f":"'Operative BP'!D69","v":129.99219692738231},{"$f":"'Operative BP'!E69","v":0},{"$f":"'Operative BP'!F69","v":0},{"$f":"'Operative BP'!G69","v":0},{"$f":"'Operative BP'!H69","v":0},{"$f":"'Operative BP'!I69","v":0},{"$f":"'Operative BP'!J69","v":0},{"$f":"'Operative BP'!K69","v":0},{"$f":"'Operative BP'!L69","v":199.34268060830314},{"$f":"'Operative BP'!M69","v":3190.3469256777284},{"$f":"'Operative BP'!N69","v":3062.0963422731697},null,null,null,12,0.22172998091293661,1.0832639746549549E-2,0,0,0,0,0,0,0,1.6611823603131726E-2,0.26586118035750211,0.25517367449065004]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,{"$f":"'Operative BP'!C70","v":2550.173141104859},{"$f":"'Operative BP'!D70","v":164.68058328163184},{"$f":"'Operative BP'!E70","v":0},{"$f":"'Operative BP'!F70","v":0},{"$f":"'Operative BP'!G70","v":0},{"$f":"'Operative BP'!H70","v":0},{"$f":"'Operative BP'!I70","v":0},{"$f":"'Operative BP'!J70","v":0},{"$f":"'Operative BP'!K70","v":0},{"$f":"'Operative BP'!L70","v":315.54561787258626},{"$f":"'Operative BP'!M70","v":2682.4119372208993},{"$f":"'Operative BP'!N70","v":2806.1921484791264},null,null,null,13,0.21251357836769122,1.3723327046608226E-2,0,0,0,0,0,0,0,2.6295362974176228E-2,0.22353343396442918,0.23384841030921102]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,{"$f":"'Operative BP'!C71","v":2071.1194620481665},{"$f":"'Operative BP'!D71","v":325.93097583385139},{"$f":"'Operative BP'!E71","v":0},{"$f":"'Operative BP'!F71","v":0},{"$f":"'Operative BP'!G71","v":0},{"$f":"'Operative BP'!H71","v":0},{"$f":"'Operative BP'!I71","v":0},{"$f":"'Operative BP'!J71","v":0},{"$f":"'Operative BP'!K71","v":0},{"$f":"'Operative BP'!L71","v":1146.217913516015},{"$f":"'Operative BP'!M71","v":2804.1224848650663},{"$f":"'Operative BP'!N71","v":2465.1244629009921},null,null,null,14,0.17259259813085986,2.7160806009162337E-2,0,0,0,0,0,0,0,9.5517777387030073E-2,0.23367593903126055,0.20542621686692836]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,{"$f":"'Operative BP'!C72","v":3379.1186364961477},{"$f":"'Operative BP'!D72","v":2627.2389509698896},{"$f":"'Operative BP'!E72","v":2635.5703218185467},{"$f":"'Operative BP'!F72","v":2739.6260864388364},{"$f":"'Operative BP'!G72","v":2639.208561173924},{"$f":"'Operative BP'!H72","v":1868.8769897456732},{"$f":"'Operative BP'!I72","v":1817.2287126262747},{"$f":"'Operative BP'!J72","v":2938.0781685139464},{"$f":"'Operative BP'!K72","v":3923.7505691865708},{"$f":"'Operative BP'!L72","v":4121.5430186681224},{"$f":"'Operative BP'!M72","v":4073.1026437891323},{"$f":"'Operative BP'!N72","v":3409.9124235922036},null,null,null,15,0.28159209333513346,0.21893570350117381,0.21962998162810496,0.22830126066120754,0.21993316702830659,0.15573912618647617,0.15143512030928535,0.24483886801677268,0.32697790618202449,0.34346054437467061,0.33942386261487978,0.28415823199520907]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,{"$f":"'Operative BP'!C73","v":3488.2891932933635},{"$f":"'Operative BP'!D73","v":3744.9639414750504},{"$f":"'Operative BP'!E73","v":4446.8095707895973},{"$f":"'Operative BP'!F73","v":4774.3448944164402},{"$f":"'Operative BP'!G73","v":4971.3533893484409},{"$f":"'Operative BP'!H73","v":4803.02801605271},{"$f":"'Operative BP'!I73","v":4929.1205423900001},{"$f":"'Operative BP'!J73","v":5622.3905501017762},{"$f":"'Operative BP'!K73","v":5190.4573655804825},{"$f":"'Operative BP'!L73","v":4062.4502685123566},{"$f":"'Operative BP'!M73","v":2971.6590396841225},{"$f":"'Operative BP'!N73","v":2854.9097803651739},null,null,null,16,0.29068960334471583,0.31207908013494035,0.37056598196260948,0.3978604830864052,0.4142777919945736,0.40025073366172048,0.41075840215898585,0.46853067171163132,0.43253638364591834,0.33853616822594018,0.24763726275399697,0.23790819672717103]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17,{"$f":"'Operative BP'!C74","v":1591.2164963126143},{"$f":"'Operative BP'!D74","v":2655.3121550436108},{"$f":"'Operative BP'!E74","v":3490.2420072817777},{"$f":"'Operative BP'!F74","v":3580.241138149192},{"$f":"'Operative BP'!G74","v":3849.9681326621317},{"$f":"'Operative BP'!H74","v":4187.313761054791},{"$f":"'Operative BP'!I74","v":4292.2891157890799},{"$f":"'Operative BP'!J74","v":4423.2439261434729},{"$f":"'Operative BP'!K74","v":3470.8202131864714},{"$f":"'Operative BP'!L74","v":1880.8404833431982},{"$f":"'Operative BP'!M74","v":695.47656043259258},{"$f":"'Operative BP'!N74","v":814.73237202802113},null,null,null,17,0.13260084428721908,0.22127512781624922,0.29085233719281234,0.29835223476538658,0.32082939439913338,0.34894141764997888,0.35768932888605137,0.36860218609731399,0.2892338608254682,0.15673607999843872,5.7956148210529232E-2,6.789409275821108E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,18,{"$f":"'Operative BP'!C75","v":0},{"$f":"'Operative BP'!D75","v":422.68319711735165},{"$f":"'Operative BP'!E75","v":819.88818854556575},{"$f":"'Operative BP'!F75","v":1026.1250812956971},{"$f":"'Operative BP'!G75","v":1411.1756989981864},{"$f":"'Operative BP'!H75","v":1877.6960626038615},{"$f":"'Operative BP'!I75","v":1903.0570696083062},{"$f":"'Operative BP'!J75","v":1540.0957842881564},{"$f":"'Operative BP'!K75","v":0},{"$f":"'Operative BP'!L75","v":0},{"$f":"'Operative BP'!M75","v":0},{"$f":"'Operative BP'!N75","v":0},null,null,null,18,0,3.5223458865380267E-2,6.8323742416067632E-2,8.5510081399614329E-2,0.11759750452461586,0.15647404598496759,0.15858745478166897,0.12834080199208495,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,19,{"$f":"'Operative BP'!C76","v":0},{"$f":"'Operative BP'!D76","v":0},{"$f":"'Operative BP'!E76","v":0},{"$f":"'Operative BP'!F76","v":0},{"$f":"'Operative BP'!G76","v":0},{"$f":"'Operative BP'!H76","v":0},{"$f":"'Operative BP'!I76","v":0},{"$f":"'Operative BP'!J76","v":0},{"$f":"'Operative BP'!K76","v":0},{"$f":"'Operative BP'!L76","v":0},{"$f":"'Operative BP'!M76","v":0},{"$f":"'Operative BP'!N76","v":0},null,null,null,19,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,{"$f":"'Operative BP'!C77","v":0},{"$f":"'Operative BP'!D77","v":0},{"$f":"'Operative BP'!E77","v":0},{"$f":"'Operative BP'!F77","v":0},{"$f":"'Operative BP'!G77","v":0},{"$f":"'Operative BP'!H77","v":0},{"$f":"'Operative BP'!I77","v":0},{"$f":"'Operative BP'!J77","v":0},{"$f":"'Operative BP'!K77","v":0},{"$f":"'Operative BP'!L77","v":0},{"$f":"'Operative BP'!M77","v":0},{"$f":"'Operative BP'!N77","v":0},null,null,null,20,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,21,{"$f":"'Operative BP'!C78","v":0},{"$f":"'Operative BP'!D78","v":0},{"$f":"'Operative BP'!E78","v":0},{"$f":"'Operative BP'!F78","v":0},{"$f":"'Operative BP'!G78","v":0},{"$f":"'Operative BP'!H78","v":0},{"$f":"'Operative BP'!I78","v":0},{"$f":"'Operative BP'!J78","v":0},{"$f":"'Operative BP'!K78","v":0},{"$f":"'Operative BP'!L78","v":0},{"$f":"'Operative BP'!M78","v":0},{"$f":"'Operative BP'!N78","v":0},null,null,null,21,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,{"$f":"'Operative BP'!C79","v":0},{"$f":"'Operative BP'!D79","v":0},{"$f":"'Operative BP'!E79","v":0},{"$f":"'Operative BP'!F79","v":0},{"$f":"'Operative BP'!G79","v":0},{"$f":"'Operative BP'!H79","v":0},{"$f":"'Operative BP'!I79","v":0},{"$f":"'Operative BP'!J79","v":0},{"$f":"'Operative BP'!K79","v":0},{"$f":"'Operative BP'!L79","v":0},{"$f":"'Operative BP'!M79","v":0},{"$f":"'Operative BP'!N79","v":0},null,null,null,22,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,{"$f":"'Operative BP'!C80","v":0},{"$f":"'Operative BP'!D80","v":0},{"$f":"'Operative BP'!E80","v":0},{"$f":"'Operative BP'!F80","v":0},{"$f":"'Operative BP'!G80","v":0},{"$f":"'Operative BP'!H80","v":0},{"$f":"'Operative BP'!I80","v":0},{"$f":"'Operative BP'!J80","v":0},{"$f":"'Operative BP'!K80","v":0},{"$f":"'Operative BP'!L80","v":0},{"$f":"'Operative BP'!M80","v":0},{"$f":"'Operative BP'!N80","v":0},null,null,null,23,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,{"$f":"'Operative BP'!C81","v":0},{"$f":"'Operative BP'!D81","v":0},{"$f":"'Operative BP'!E81","v":0},{"$f":"'Operative BP'!F81","v":0},{"$f":"'Operative BP'!G81","v":0},{"$f":"'Operative BP'!H81","v":0},{"$f":"'Operative BP'!I81","v":0},{"$f":"'Operative BP'!J81","v":0},{"$f":"'Operative BP'!K81","v":0},{"$f":"'Operative BP'!L81","v":0},{"$f":"'Operative BP'!M81","v":0},{"$f":"'Operative BP'!N81","v":0},null,null,null,24,0,0,0,0,0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"T",{"$f":"SUM(BJ115:BJ138)","v":24623.791732550606},{"$f":"SUM(BK115:BK138)","v":16412.743504443486},{"$f":"SUM(BL115:BL138)","v":18315.101475344451},20543.885588190646,21525.857323925396,21971.079289608333,21961.687043983966,24053.741755562907,20900.004870048338,19097.354248179097,26773.580405617242,23958.336227166168,null,null,null,"Combined",{"$f":"MAX(BZ115:BZ138)","v":0.29068960334471583},{"$f":"MAX(CA115:CA138)","v":0.31207908013494035},0.37056598196260948,0.3978604830864052,0.4142777919945736,0.40025073366172048,0.41075840215898585,0.46853067171163132,0.43253638364591834,0.34346054437467061,0.33942386261487978,0.28415823199520907]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"June 21st - eQUEST",null,null,null,null,null,null,null,null,"December 21st - eQUEST"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Window\nSolar Load","Window \nSolar Gain","Window\nSolar Load","Window \nSolar Gain","Window\nSolar Load","Window \nSolar Gain","eQUEST - \nSolar Load","eQUEST - \nSolar Gain",null,"Window\nSolar Load","Window \nSolar Gain","Window\nSolar Load","Window \nSolar Gain","Window\nSolar Load","Window \nSolar Gain","eQUEST - \nSolar Load","eQUEST - \nSolar Gain"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8810.2999999999993,0,9341.1,0,9362.44,0,{"$f":"BI144+BK144+BM144","v":27513.840000000004},{"$f":"BJ144+BL144+BN144","v":0},null,3620.04,0,2892.85,0,2522.58,0,{"$f":"BR144+BT144+BV144","v":9035.4699999999993},{"$f":"BS144+BU144+BW144","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8410.82,0,8620.52,0,8145.32,0,{"$f":"BI145+BK145+BM145","v":25176.66},0,null,3503.82,0,2670.09,0,2194.65,0,{"$f":"BR145+BT145+BV145","v":8368.56},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8078.16,0,7956.31,0,7086.43,0,23120.9,0,null,3401.06,0,2464.5300000000002,0,1909.34,0,7774.93,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7795.07,0,7343.6,0,6165.19,0,21303.86,0,null,3308.49,0,2274.8000000000002,0,1661.13,0,7244.42,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7548.95,0,6778.21,0,5363.72,0,19690.88,0,null,3223.72,0,2099.69,0,1445.18,0,6768.59,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7484.82,842.3,6411.17,842.3,4832.37,842.3,18728.36,2526.8999999999996,null,3144.98,0,1938.06,0,1257.31,0,6340.35,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7947.34,4207.1099999999997,6595.97,4207.1099999999997,4976.53,4207.1099999999997,19519.84,12621.329999999998,null,3070.99,0,1788.88,0,1093.8599999999999,0,5953.73,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9591.6,13037.17,8007.92,13037.17,6616.03,13037.17,24215.55,39111.51,null,3119.57,648.62,1770.35,648.62,1079.43,648.62,5969.35,1945.8600000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10830.39,17332.66,9095.35,17332.66,8296.99,17332.66,28222.729999999996,51997.979999999996,null,5103.51,11667.12,3704.88,11667.12,3194.07,11667.12,12002.46,35001.360000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12309.91,22424.02,10516.86,22424.02,10474.620000000001,22424.02,33301.39,67272.06,null,7748.39,23194.68,6367.79,23194.68,6566.5,23194.68,20682.68,69584.040000000008]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14119.48,28658.5,12373.38,28658.5,13256.24,28658.5,39749.1,85975.5,null,9967.35,29848.85,8714.5400000000009,29848.85,10039.030000000001,29848.85,28720.92,89546.549999999988]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14664.35,27115.26,13073.67,27115.26,14954.51,27115.26,42692.53,81345.78,null,11581.65,32582.14,10580.47,32582.14,13152.77,32582.14,35314.89,97746.42]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15929.23,31001.53,14574.74,31001.53,17301,31001.53,47804.97,93004.59,null,12132,30086.18,11492.18,30086.18,15186.88,30086.18,38811.06,90258.540000000008]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16222.14,29151.18,15175.12,29151.18,18717.55,29151.18,50114.81,87453.540000000008,null,13652.38,34768.97,13447.16,34768.97,18046.3,34768.97,45145.84,104306.91]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16387.34,27873.85,15686.11,27873.85,19822.29,27873.85,51895.740000000005,83621.549999999988,null,16031.24,43511.39,16328.68,43511.39,21942.5,43511.39,54302.42,130534.17]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16512.189999999999,27167,16170.95,27167,20729.740000000002,27167,53412.880000000005,81501,null,18090.61,48843.4,18968.39,48843.4,25796.87,48843.4,62855.869999999995,146530.20000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15266.88,19410.400000000001,15276.8,19410.400000000001,20038.54,19410.400000000001,50582.22,58231.200000000004,null,17916.740000000002,41627.370000000003,19443.28,41627.370000000003,27371.360000000001,41627.370000000003,64731.380000000005,124882.11000000002]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14295.23,15478.63,14605.04,15478.63,19182.32,15478.63,48082.59,46435.89,null,12860.33,10991.49,15030.85,10991.49,23189.37,10991.49,51080.55,32974.47]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,10,20,30,40,50,60,70,80,90,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13453.74,12971.72,13994.11,12971.72,18206.98,12971.72,45654.83,38915.159999999996,null,9730.7000000000007,0,12393.1,0,19438.32,0,41562.120000000003,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.79,0.79,0.78,0.77,0.76,0.75,0.72,0.6,0.37,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11304.69,3489.31,11994.35,3489.31,15658.36,3489.31,38957.4,10467.93,null,8344.56,0,11301.53,0,16911.34,0,36557.43,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9862.25,0,10591.87,0,13388.99,0,33843.11,0,null,7308.21,0,10375.120000000001,0,14712.87,0,32396.200000000004,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9063.5400000000009,0,9729.1200000000008,0,11648.42,0,30441.08,0,null,6527.32,0,9553.32,0,12800.19,0,28880.83,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8442.2999999999993,0,8960.75,0,10134.129999999999,0,27537.18,0,null,5933.14,0,8808.43,0,11136.17,0,25877.739999999998,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7951.21,0,8263,0,8816.69,0,25030.9,0,null,5475.57,0,8126.49,0,9688.4699999999993,0,23290.53,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"y = -2E-05x2 + 0.0004x + 0.8146 "]

{"sheet":"Input Data","index":12,"n_rows":58,"n_cols":32,"rows_kept":58,"cut":false,"hidden":true,"merged":[[35,28,57,28],[1,2,12,2],[13,2,27,2],[37,12,39,12],[26,13,26,25],[28,12,30,12],[31,12,33,12],[34,12,36,12],[34,3,36,3],[6,16,6,18],[6,20,6,22],[26,9,27,11],[2,16,2,18],[4,16,4,18],[4,20,4,22],[2,20,2,22],[28,2,39,2],[35,1,47,1],[8,1,34,1],[28,3,30,3],[31,3,33,3],[37,3,39,3],[40,2,58,2]]}
[]
[null,null,"Climate"]
[null,null,null,null,"Latitude",{"$f":"STAT!B4+(STAT!D4/60)","v":24.7},{"$f":"RADIANS(F3)","v":0.43109632524259939},null,null,null,null,null,null,null,null,null,"Dry Bulb T",null,null,null,"Cooling Season"]
[]
[null,null,null,null,"Longitude",{"$f":"STAT!G4+(STAT!I4/60)","v":46.783333333333331},{"$f":"RADIANS(F5)","v":0.81652320172468051},null,null,null,null,null,null,null,null,null,"Radiation",null,null,null,"Balance Point"]
[]
[null,null,null,null,"Local Time Meridian",{"$f":"'Operative BP'!P20","v":45},null,null,null,null,null,null,null,null,null,null,"Profile Angles",null,null,null,"SS Azimuth"]
[]
[null,{"$f":"#REF!","v":{"$error":"#REF!"}},null,null,"South Surface Azimuth",{"$f":"'Operative BP'!P17","v":0},{"$f":"RADIANS(F9)","v":0}]
[null,null,null,null,"East = +",{"$f":"F9+90","v":90},{"$f":"RADIANS(F10)","v":1.5707963267948966}]
[null,null,null,null,"West = -",{"$f":"F9-90","v":-90},{"$f":"RADIANS(F11)","v":-1.5707963267948966}]
[null,null,null,null,"North",{"$f":"F9-180","v":-180},{"$f":"RADIANS(F12)","v":-3.1415926535897931}]
[]
[null,null,"Building",null,"Surface Tilt",90,{"$f":"RADIANS(F14)","v":1.5707963267948966}]
[null,null,null,null,"(Walls = 90)"]
[]
[null,null,null,null,"Thermostat Setpoint",{"$f":"'Operative BP'!P15","v":75}]
[]
[null,null,null,null,"Building Height",{"$f":"'Operative BP'!P9","v":15}]
[]
[null,null,null,null,"Building Length (N-S)",{"$f":"'Operative BP'!P3","v":30}]
[]
[null,null,null,null,"Building Width (E-W)",{"$f":"'Operative BP'!P6","v":30}]
[]
[null,null,null,null,"Walls U value",{"$f":"'Operative BP'!P11","v":0.05}]
[]
[null,null,null,null,"Roof U-value",{"$f":"'Operative BP'!P13","v":0.04},null,"WWR",null,"Suggested Shading Angle",null,null,null,"Solar Transmitted"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,null,"Windows","North","Window Area",{"$f":"'Operative BP'!Q50","v":247.5},null,null,null,null,null,null,"North",{"$f":"'Incident angle'!BX85","v":0},{"$f":"'Incident angle'!BY85","v":0},{"$f":"'Incident angle'!BZ85","v":0},{"$f":"'Incident angle'!CA85","v":0},{"$f":"'Incident angle'!CB85","v":0},{"$f":"'Incident angle'!CC85","v":0},{"$f":"'Incident angle'!CD85","v":0},{"$f":"'Incident angle'!CE85","v":0},{"$f":"'Incident angle'!CF85","v":0},{"$f":"'Incident angle'!CG85","v":0},{"$f":"'Incident angle'!CH85","v":0},{"$f":"'Incident angle'!CI85","v":0},"Tons"]
[null,null,null,null,"Shading Coefficient",{"$f":"'Operative BP'!Q51","v":0.28999999999999998},null,{"$f":"F29/(F21*F19)","v":0.55000000000000004},null,{"$f":"'Profile angles'!Z58","v":"-"},"-",{"$f":"'Profile angles'!AB58","v":"-"},null,{"$f":"'Incident angle'!BX84/1000","v":0},{"$f":"'Incident angle'!BY84/1000","v":0},{"$f":"'Incident angle'!BZ84/1000","v":0},{"$f":"'Incident angle'!CA84/1000","v":0},{"$f":"'Incident angle'!CB84/1000","v":0},{"$f":"'Incident angle'!CC84/1000","v":0},{"$f":"'Incident angle'!CD84/1000","v":0},{"$f":"'Incident angle'!CE84/1000","v":0},{"$f":"'Incident angle'!CF84/1000","v":0},{"$f":"'Incident angle'!CG84/1000","v":0},{"$f":"'Incident angle'!CH84/1000","v":0},{"$f":"'Incident angle'!CI84/1000","v":0},"KBTU",null,null,null,null,null,1092035]
[null,null,null,null,"U-Value",{"$f":"'Operative BP'!Q52","v":0.5},null,null,null,null,null,null,null,{"$f":"'Incident angle'!CZ84","v":0},{"$f":"'Incident angle'!DA84","v":0},{"$f":"'Incident angle'!DB84","v":0},{"$f":"'Incident angle'!DC84","v":0},{"$f":"'Incident angle'!DD84","v":0},{"$f":"'Incident angle'!DE84","v":0},{"$f":"'Incident angle'!DF84","v":0},{"$f":"'Incident angle'!DG84","v":0},{"$f":"'Incident angle'!DH84","v":0},{"$f":"'Incident angle'!DI84","v":0},{"$f":"'Incident angle'!DJ84","v":0},{"$f":"'Incident angle'!DK84","v":0},"%",null,null,null,null,null,{"$f":"AF30/1000","v":1092.0350000000001}]
[null,null,null,"South","Window Area",{"$f":"'Operative BP'!Q29","v":270},null,null,null,null,null,null,"South",{"$f":"'Incident angle'!BJ30","v":0.22172998091293661},{"$f":"'Incident angle'!BK30","v":3.0371637149643783E-2},{"$f":"'Incident angle'!BL30","v":0},{"$f":"'Incident angle'!BM30","v":0},{"$f":"'Incident angle'!BN30","v":0},{"$f":"'Incident angle'!BO30","v":0},{"$f":"'Incident angle'!BP30","v":0},{"$f":"'Incident angle'!BQ30","v":0},{"$f":"'Incident angle'!BR30","v":0},{"$f":"'Incident angle'!BS30","v":3.830763187023041E-2},{"$f":"'Incident angle'!BT30","v":0.26586118035750211},{"$f":"'Incident angle'!BU30","v":0.25517367449065004},"Tons"]
[null,null,null,null,"Shading Coefficient",{"$f":"'Operative BP'!Q30","v":0.22},null,{"$f":"F32/(F21*F19)","v":0.6},null,{"$f":"'Profile angles'!L29","v":1000},"-",{"$f":"'Profile angles'!N29","v":1010},null,{"$f":"'Incident angle'!BJ29/1000","v":14.030784632581037},{"$f":"'Incident angle'!BK29/1000","v":1.6750695302373959},{"$f":"'Incident angle'!BL29/1000","v":0},{"$f":"'Incident angle'!BM29/1000","v":0},{"$f":"'Incident angle'!BN29/1000","v":0},{"$f":"'Incident angle'!BO29/1000","v":0},{"$f":"'Incident angle'!BP29/1000","v":0},{"$f":"'Incident angle'!BQ29/1000","v":0},{"$f":"'Incident angle'!BR29/1000","v":0},{"$f":"'Incident angle'!BS29/1000","v":2.2353795226721065},{"$f":"'Incident angle'!BT29/1000","v":15.798901292159933},{"$f":"'Incident angle'!BU29/1000","v":15.826439540382029},"KBTU"]
[null,null,null,null,"U-Value",{"$f":"'Operative BP'!Q31","v":0.4},null,null,null,null,null,null,null,{"$f":"'Incident angle'!CL29","v":0.56980601464531988},{"$f":"'Incident angle'!CM29","v":0.10205908169977175},{"$f":"'Incident angle'!CN29","v":0},{"$f":"'Incident angle'!CO29","v":0},{"$f":"'Incident angle'!CP29","v":0},{"$f":"'Incident angle'!CQ29","v":0},{"$f":"'Incident angle'!CR29","v":0},{"$f":"'Incident angle'!CS29","v":0},{"$f":"'Incident angle'!CT29","v":0},{"$f":"'Incident angle'!CU29","v":0.11705179123884379},{"$f":"'Incident angle'!CV29","v":0.59009295928329553},{"$f":"'Incident angle'!CW29","v":0.66058174450513618},"%"]
[null,null,null,"East","Window Area",{"$f":"'Operative BP'!Q36","v":225},null,null,null,null,null,null,"East",{"$f":"'Incident angle'!BX30","v":0.1614785148002717},{"$f":"'Incident angle'!BY30","v":0.20159927985163262},{"$f":"'Incident angle'!BZ30","v":0.24266693149197466},{"$f":"'Incident angle'!CA30","v":0.28750411840107132},{"$f":"'Incident angle'!CB30","v":0.28583962076957126},{"$f":"'Incident angle'!CC30","v":0.30203424120196398},{"$f":"'Incident angle'!CD30","v":0.3100757587234404},{"$f":"'Incident angle'!CE30","v":0.31883925464425267},{"$f":"'Incident angle'!CF30","v":0.27951662019576862},{"$f":"'Incident angle'!CG30","v":0.22246852130519268},{"$f":"'Incident angle'!CH30","v":0.15979069429134463},{"$f":"'Incident angle'!CI30","v":0.11583124004575107},"Tons",null,null,null,null,null,{"$f":"P30+P33+P36+P39","v":18.315101475344449}]
[null,"BUILDING DATA",null,null,"Shading Coefficient",{"$f":"'Operative BP'!Q37","v":0.28999999999999998},null,{"$f":"F35/(F23*F19)","v":0.5},null,{"$f":"'Profile angles'!L58","v":"-"},"-",{"$f":"'Profile angles'!N58","v":"-"},null,{"$f":"'Incident angle'!BX29/1000","v":4.3005894702351926},{"$f":"'Incident angle'!BY29/1000","v":5.6623134755026054},{"$f":"'Incident angle'!BZ29/1000","v":6.9225913869089615},{"$f":"'Incident angle'!CA29/1000","v":8.4235483878904791},{"$f":"'Incident angle'!CB29/1000","v":8.65415154174271},{"$f":"'Incident angle'!CC29/1000","v":9.2341644601513018},{"$f":"'Incident angle'!CD29/1000","v":9.0199916035703041},{"$f":"'Incident angle'!CE29/1000","v":9.5299333265155539},{"$f":"'Incident angle'!CF29/1000","v":8.3149767220948139},{"$f":"'Incident angle'!CG29/1000","v":6.4085471212920275},{"$f":"'Incident angle'!CH29/1000","v":4.1702681988083912},{"$f":"'Incident angle'!CI29/1000","v":3.0756068051584582},"KBTU",null,null,"Chhaya© 2004 Vikram Sami & Victor Olgyay"]
[null,null,null,null,"U-Value",{"$f":"'Operative BP'!Q38","v":0.45},null,null,null,null,null,null,null,{"$f":"'Incident angle'!CZ29","v":0.17465179680472082},{"$f":"'Incident angle'!DA29","v":0.34499494091098332},{"$f":"'Incident angle'!DB29","v":0.37797177352405409},{"$f":"'Incident angle'!DC29","v":0.4100270297811936},{"$f":"'Incident angle'!DD29","v":0.4020351622475849},{"$f":"'Incident angle'!DE29","v":0.42028724845204973},{"$f":"'Incident angle'!DF29","v":0.41071487748210944},{"$f":"'Incident angle'!DG29","v":0.39619338327316861},{"$f":"'Incident angle'!DH29","v":0.39784568347211025},{"$f":"'Incident angle'!DI29","v":0.33557251114525838},{"$f":"'Incident angle'!DJ29","v":0.15576057201275353},{"$f":"'Incident angle'!DK29","v":0.12837313810092754},"%"]
[null,null,null,"West","Window Area",{"$f":"'Operative BP'!Q43","v":270},null,null,null,null,null,null,"West",{"$f":"'Incident angle'!BJ85","v":0.23121819499587998},{"$f":"'Incident angle'!BK85","v":0.3112143634052979},{"$f":"'Incident angle'!BL85","v":0.37056598196260948},{"$f":"'Incident angle'!BM85","v":0.3978604830864052},{"$f":"'Incident angle'!BN85","v":0.4142777919945736},{"$f":"'Incident angle'!BO85","v":0.40025073366172048},{"$f":"'Incident angle'!BP85","v":0.41075840215898585},{"$f":"'Incident angle'!BQ85","v":0.46853067171163132},{"$f":"'Incident angle'!BR85","v":0.43253638364591834},{"$f":"'Incident angle'!BS85","v":0.33853616822594018},{"$f":"'Incident angle'!BT85","v":0.23163264570255551},{"$f":"'Incident angle'!BU85","v":0.1803587647564367},"Tons"]
[null,null,null,null,"Shading Coefficient",{"$f":"'Operative BP'!Q44","v":0.28999999999999998},null,{"$f":"F38/(F23*F19)","v":0.6},null,{"$f":"'Profile angles'!Z29","v":"-"},"-",{"$f":"'Profile angles'!AB29","v":"-"},null,{"$f":"'Incident angle'!BJ84/1000","v":6.2924176297343744},{"$f":"'Incident angle'!BK84/1000","v":9.0753604987034855},{"$f":"'Incident angle'!BL84/1000","v":11.392510088435486},{"$f":"'Incident angle'!BM84/1000","v":12.120337200300163},{"$f":"'Incident angle'!BN84/1000","v":12.871705782182682},{"$f":"'Incident angle'!BO84/1000","v":12.736914829457035},{"$f":"'Incident angle'!BP84/1000","v":12.941695440413662},{"$f":"'Incident angle'!BQ84/1000","v":14.523808429047351},{"$f":"'Incident angle'!BR84/1000","v":12.585028147953524},{"$f":"'Incident angle'!BS84/1000","v":10.453427604214964},{"$f":"'Incident angle'!BT84/1000","v":6.8044109146489156},{"$f":"'Incident angle'!BU84/1000","v":5.0562898816256787},"KBTU"]
[null,null,null,null,"U-Value",{"$f":"'Operative BP'!Q45","v":0.45},null,null,null,null,null,null,null,{"$f":"'Incident angle'!CL84","v":0.25554218854995925},{"$f":"'Incident angle'!CM84","v":0.552945977389245},{"$f":"'Incident angle'!CN84","v":0.6220282264759458},{"$f":"'Incident angle'!CO84","v":0.58997297021880635},{"$f":"'Incident angle'!CP84","v":0.59796483775241493},{"$f":"'Incident angle'!CQ84","v":0.57971275154795043},{"$f":"'Incident angle'!CR84","v":0.58928512251789056},{"$f":"'Incident angle'!CS84","v":0.60380661672683134},{"$f":"'Incident angle'!CT84","v":0.60215431652788975},{"$f":"'Incident angle'!CU84","v":0.54737569761589777},{"$f":"'Incident angle'!CV84","v":0.25414646870395091},{"$f":"'Incident angle'!CW84","v":0.21104511739393619},"%"]
[null,null,"Internal Gains",null,{"$f":"('Operative BP'!R32*(('Operative BP'!P3*'Operative BP'!P9)-'Operative BP'!Q29))+('Operative BP'!R53*(('Operative BP'!P3*'Operative BP'!P9)-'Operative BP'!Q50))+('Operative BP'!R39*(('Operative BP'!P6*'Operative BP'!P9)-'Operative BP'!Q36))+('Operative BP'!R46*(('Operative BP'!P6*'Operative BP'!P9)-'Operative BP'!Q43))","v":787.5},{"$f":"('Operative BP'!R32*(('Operative BP'!P3*'Operative BP'!P9)-'Operative BP'!Q29))+('Operative BP'!R53*(('Operative BP'!P3*'Operative BP'!P9)-'Operative BP'!Q50))+('Operative BP'!R39*(('Operative BP'!P6*'Operative BP'!P9)-'Operative BP'!Q36))+('Operative BP'!R46*(('Operative BP'!P6*'Operative BP'!P9)-'Operative BP'!Q43))","v":787.5},"Wall Area"]
[null,null,null,null,null,{"$f":"F21*F23","v":900},"Roof Area"]
[null,null,null,null,null,{"$f":"F29+F32+F35+F38","v":1012.5},"Window Area"]
[null,null,null,null,null,{"$f":"((F41*F25)+(F42*F27)+(F29*F31)+(F32*F34)+(F35*F37)+(F38*F40))","v":529.875},"UA"]
[null,null,null,null,null,{"$f":"F46*'Operative BP'!T9","v":0.5},null,"8-6 (y/n)","24 hrs (y/n)"]
[null,null,null,null,"Light & Epuipment (W/ft2)",{"$f":"'Operative BP'!T33","v":0.5},null,"n",{"$f":"IF(H46=\"y\",\"n\",IF(H46=\"n\",\"y\",\"ERROR!\"))","v":"y"}]
[null,null,null,null,null,{"$f":"F45*F42*3.412","v":1535.3999999999999}]
[null,null,null,null,"No of Occupants",{"$f":"'Operative BP'!T29","v":4.5},null,"n",{"$f":"IF(H48=\"y\",\"n\",IF(H48=\"n\",\"y\",\"ERROR!\"))","v":"y"}]
[null,null,null,null,null,{"$f":"F48*250","v":1125}]
[null,null,null,null,"Air Changes per Hour",{"$f":"'Operative BP'!P25","v":0.5}]
[]
[]
[null,null,null,null,{"$f":"AVERAGE(F53:F56)","v":123.46875},{"$f":"((F21*F19-F29)*F25)+F29*F31","v":133.875},"UA North"]
[null,null,null,null,null,{"$f":"((F21*F19-F32)*F25)+F32*F34","v":117},"UA South"]
[null,null,null,null,null,{"$f":"((F23*F19-F35)*F25)+F35*F37","v":112.5},"UA East"]
[null,null,null,null,null,{"$f":"((F23*F19-F38)*F25)+F38*F40","v":130.5},"UA West"]
[null,null,null,null,null,{"$f":"SUM(F53:F56)","v":493.875}]
[null,null,null,null,null,{"$f":"F44-(F42*F27)","v":493.875}]

{"sheet":"Heat gain from airflow","index":13,"n_rows":27,"n_cols":28,"rows_kept":27,"cut":false,"hidden":true,"merged":[[1,24,1,27],[28,16,28,17],[1,10,1,13],[1,1,1,2],[1,3,1,9],[28,2,28,3],[1,15,1,16],[1,17,1,23]]}
[]
[null,"Table1",null,{"$f":"STAT!$A$2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,null,"Heat gain from OA",null,null,null,null,"Table1",null,{"$f":"STAT!$A$2","v":" Statistics for SAU_Riyadh.404380_IWEC"},null,null,null,null,null,null,"Heat gain from OA"]
[null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D5-'Input Data'!$F$17)","v":-2692.5072300000006},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E5-'Input Data'!$F$17)","v":-2144.7548550000006},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F5-'Input Data'!$F$17)","v":-1312.1712450000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G5-'Input Data'!$F$17)","v":-238.57658999999924},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H5-'Input Data'!$F$17)","v":1163.6694900000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I5-'Input Data'!$F$17)","v":1777.1521499999994},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J5-'Input Data'!$F$17)","v":1930.522815},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K5-'Input Data'!$F$17)","v":1996.2531000000008},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L5-'Input Data'!$F$17)","v":1317.0401549999992},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M5-'Input Data'!$F$17)","v":133.89502499999932},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N5-'Input Data'!$F$17)","v":-1202.6207699999995},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O5-'Input Data'!$F$17)","v":-2451.496185},null,1,{"$f":"IF('Dry Bulb'!D5>'Operative BP'!$P$22,IF('Dry Bulb'!D5<'Operative BP'!$P$23,C4,0),0)","v":0},{"$f":"IF('Dry Bulb'!E5>'Operative BP'!$P$22,IF('Dry Bulb'!E5<'Operative BP'!$P$23,D4,0),0)","v":0},{"$f":"IF('Dry Bulb'!F5>'Operative BP'!$P$22,IF('Dry Bulb'!F5<'Operative BP'!$P$23,E4,0),0)","v":0},{"$f":"IF('Dry Bulb'!G5>'Operative BP'!$P$22,IF('Dry Bulb'!G5<'Operative BP'!$P$23,F4,0),0)","v":-238.57658999999924},{"$f":"IF('Dry Bulb'!H5>'Operative BP'!$P$22,IF('Dry Bulb'!H5<'Operative BP'!$P$23,G4,0),0)","v":0},{"$f":"IF('Dry Bulb'!I5>'Operative BP'!$P$22,IF('Dry Bulb'!I5<'Operative BP'!$P$23,H4,0),0)","v":0},{"$f":"IF('Dry Bulb'!J5>'Operative BP'!$P$22,IF('Dry Bulb'!J5<'Operative BP'!$P$23,I4,0),0)","v":0},{"$f":"IF('Dry Bulb'!K5>'Operative BP'!$P$22,IF('Dry Bulb'!K5<'Operative BP'!$P$23,J4,0),0)","v":0},{"$f":"IF('Dry Bulb'!L5>'Operative BP'!$P$22,IF('Dry Bulb'!L5<'Operative BP'!$P$23,K4,0),0)","v":0},{"$f":"IF('Dry Bulb'!M5>'Operative BP'!$P$22,IF('Dry Bulb'!M5<'Operative BP'!$P$23,L4,0),0)","v":133.89502499999932},{"$f":"IF('Dry Bulb'!N5>'Operative BP'!$P$22,IF('Dry Bulb'!N5<'Operative BP'!$P$23,M4,0),0)","v":-1202.6207699999995},{"$f":"IF('Dry Bulb'!O5>'Operative BP'!$P$22,IF('Dry Bulb'!O5<'Operative BP'!$P$23,N4,0),0)","v":0}]
[null,2,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D6-'Input Data'!$F$17)","v":-2802.0577050000006},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E6-'Input Data'!$F$17)","v":-2276.2154250000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F6-'Input Data'!$F$17)","v":-1465.5419100000008},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G6-'Input Data'!$F$17)","v":-370.03716000000077},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H6-'Input Data'!$F$17)","v":988.38873000000058},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I6-'Input Data'!$F$17)","v":1558.0511999999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J6-'Input Data'!$F$17)","v":1733.3319599999995},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K6-'Input Data'!$F$17)","v":1799.0622450000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L6-'Input Data'!$F$17)","v":1097.9392049999994},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M6-'Input Data'!$F$17)","v":-19.475639999999586},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N6-'Input Data'!$F$17)","v":-1399.811625},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O6-'Input Data'!$F$17)","v":-2539.1365650000002},null,2,{"$f":"IF('Dry Bulb'!D6>'Operative BP'!$P$22,IF('Dry Bulb'!D6<'Operative BP'!$P$23,C5,0),0)","v":0},{"$f":"IF('Dry Bulb'!E6>'Operative BP'!$P$22,IF('Dry Bulb'!E6<'Operative BP'!$P$23,D5,0),0)","v":0},{"$f":"IF('Dry Bulb'!F6>'Operative BP'!$P$22,IF('Dry Bulb'!F6<'Operative BP'!$P$23,E5,0),0)","v":0},{"$f":"IF('Dry Bulb'!G6>'Operative BP'!$P$22,IF('Dry Bulb'!G6<'Operative BP'!$P$23,F5,0),0)","v":-370.03716000000077},{"$f":"IF('Dry Bulb'!H6>'Operative BP'!$P$22,IF('Dry Bulb'!H6<'Operative BP'!$P$23,G5,0),0)","v":0},{"$f":"IF('Dry Bulb'!I6>'Operative BP'!$P$22,IF('Dry Bulb'!I6<'Operative BP'!$P$23,H5,0),0)","v":0},{"$f":"IF('Dry Bulb'!J6>'Operative BP'!$P$22,IF('Dry Bulb'!J6<'Operative BP'!$P$23,I5,0),0)","v":0},{"$f":"IF('Dry Bulb'!K6>'Operative BP'!$P$22,IF('Dry Bulb'!K6<'Operative BP'!$P$23,J5,0),0)","v":0},{"$f":"IF('Dry Bulb'!L6>'Operative BP'!$P$22,IF('Dry Bulb'!L6<'Operative BP'!$P$23,K5,0),0)","v":0},{"$f":"IF('Dry Bulb'!M6>'Operative BP'!$P$22,IF('Dry Bulb'!M6<'Operative BP'!$P$23,L5,0),0)","v":-19.475639999999586},{"$f":"IF('Dry Bulb'!N6>'Operative BP'!$P$22,IF('Dry Bulb'!N6<'Operative BP'!$P$23,M5,0),0)","v":0},{"$f":"IF('Dry Bulb'!O6>'Operative BP'!$P$22,IF('Dry Bulb'!O6<'Operative BP'!$P$23,N5,0),0)","v":0}]
[null,3,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D7-'Input Data'!$F$17)","v":-2867.7879900000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E7-'Input Data'!$F$17)","v":-2407.6759950000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F7-'Input Data'!$F$17)","v":-1618.9125749999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G7-'Input Data'!$F$17)","v":-501.49773000000056},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H7-'Input Data'!$F$17)","v":856.92816000000084},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I7-'Input Data'!$F$17)","v":1448.5007250000008},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J7-'Input Data'!$F$17)","v":1601.8713899999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K7-'Input Data'!$F$17)","v":1601.8713899999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L7-'Input Data'!$F$17)","v":900.74835000000076},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M7-'Input Data'!$F$17)","v":-216.66649500000014},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N7-'Input Data'!$F$17)","v":-1553.1822899999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O7-'Input Data'!$F$17)","v":-2626.7769450000001},null,3,{"$f":"IF('Dry Bulb'!D7>'Operative BP'!$P$22,IF('Dry Bulb'!D7<'Operative BP'!$P$23,C6,0),0)","v":0},{"$f":"IF('Dry Bulb'!E7>'Operative BP'!$P$22,IF('Dry Bulb'!E7<'Operative BP'!$P$23,D6,0),0)","v":0},{"$f":"IF('Dry Bulb'!F7>'Operative BP'!$P$22,IF('Dry Bulb'!F7<'Operative BP'!$P$23,E6,0),0)","v":0},{"$f":"IF('Dry Bulb'!G7>'Operative BP'!$P$22,IF('Dry Bulb'!G7<'Operative BP'!$P$23,F6,0),0)","v":-501.49773000000056},{"$f":"IF('Dry Bulb'!H7>'Operative BP'!$P$22,IF('Dry Bulb'!H7<'Operative BP'!$P$23,G6,0),0)","v":0},{"$f":"IF('Dry Bulb'!I7>'Operative BP'!$P$22,IF('Dry Bulb'!I7<'Operative BP'!$P$23,H6,0),0)","v":0},{"$f":"IF('Dry Bulb'!J7>'Operative BP'!$P$22,IF('Dry Bulb'!J7<'Operative BP'!$P$23,I6,0),0)","v":0},{"$f":"IF('Dry Bulb'!K7>'Operative BP'!$P$22,IF('Dry Bulb'!K7<'Operative BP'!$P$23,J6,0),0)","v":0},{"$f":"IF('Dry Bulb'!L7>'Operative BP'!$P$22,IF('Dry Bulb'!L7<'Operative BP'!$P$23,K6,0),0)","v":0},{"$f":"IF('Dry Bulb'!M7>'Operative BP'!$P$22,IF('Dry Bulb'!M7<'Operative BP'!$P$23,L6,0),0)","v":-216.66649500000014},{"$f":"IF('Dry Bulb'!N7>'Operative BP'!$P$22,IF('Dry Bulb'!N7<'Operative BP'!$P$23,M6,0),0)","v":0},{"$f":"IF('Dry Bulb'!O7>'Operative BP'!$P$22,IF('Dry Bulb'!O7<'Operative BP'!$P$23,N6,0),0)","v":0}]
[null,4,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D8-'Input Data'!$F$17)","v":-2977.3384650000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E8-'Input Data'!$F$17)","v":-2539.1365650000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F8-'Input Data'!$F$17)","v":-1728.4630500000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G8-'Input Data'!$F$17)","v":-676.77849000000026},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H8-'Input Data'!$F$17)","v":791.19787500000007},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I8-'Input Data'!$F$17)","v":1317.0401549999992},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J8-'Input Data'!$F$17)","v":1426.5906299999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K8-'Input Data'!$F$17)","v":1448.5007250000008},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L8-'Input Data'!$F$17)","v":725.46758999999929},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M8-'Input Data'!$F$17)","v":-304.30687499999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N8-'Input Data'!$F$17)","v":-1706.5529549999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O8-'Input Data'!$F$17)","v":-2736.3274199999996},null,4,{"$f":"IF('Dry Bulb'!D8>'Operative BP'!$P$22,IF('Dry Bulb'!D8<'Operative BP'!$P$23,C7,0),0)","v":0},{"$f":"IF('Dry Bulb'!E8>'Operative BP'!$P$22,IF('Dry Bulb'!E8<'Operative BP'!$P$23,D7,0),0)","v":0},{"$f":"IF('Dry Bulb'!F8>'Operative BP'!$P$22,IF('Dry Bulb'!F8<'Operative BP'!$P$23,E7,0),0)","v":0},{"$f":"IF('Dry Bulb'!G8>'Operative BP'!$P$22,IF('Dry Bulb'!G8<'Operative BP'!$P$23,F7,0),0)","v":-676.77849000000026},{"$f":"IF('Dry Bulb'!H8>'Operative BP'!$P$22,IF('Dry Bulb'!H8<'Operative BP'!$P$23,G7,0),0)","v":0},{"$f":"IF('Dry Bulb'!I8>'Operative BP'!$P$22,IF('Dry Bulb'!I8<'Operative BP'!$P$23,H7,0),0)","v":0},{"$f":"IF('Dry Bulb'!J8>'Operative BP'!$P$22,IF('Dry Bulb'!J8<'Operative BP'!$P$23,I7,0),0)","v":0},{"$f":"IF('Dry Bulb'!K8>'Operative BP'!$P$22,IF('Dry Bulb'!K8<'Operative BP'!$P$23,J7,0),0)","v":0},{"$f":"IF('Dry Bulb'!L8>'Operative BP'!$P$22,IF('Dry Bulb'!L8<'Operative BP'!$P$23,K7,0),0)","v":0},{"$f":"IF('Dry Bulb'!M8>'Operative BP'!$P$22,IF('Dry Bulb'!M8<'Operative BP'!$P$23,L7,0),0)","v":-304.30687499999999},{"$f":"IF('Dry Bulb'!N8>'Operative BP'!$P$22,IF('Dry Bulb'!N8<'Operative BP'!$P$23,M7,0),0)","v":0},{"$f":"IF('Dry Bulb'!O8>'Operative BP'!$P$22,IF('Dry Bulb'!O8<'Operative BP'!$P$23,N7,0),0)","v":0}]
[null,5,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D9-'Input Data'!$F$17)","v":-3108.799035},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E9-'Input Data'!$F$17)","v":-2626.7769450000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F9-'Input Data'!$F$17)","v":-1838.0135250000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G9-'Input Data'!$F$17)","v":-808.23906000000011},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H9-'Input Data'!$F$17)","v":615.91711500000031},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I9-'Input Data'!$F$17)","v":1163.6694900000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J9-'Input Data'!$F$17)","v":1338.9502500000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K9-'Input Data'!$F$17)","v":1317.0401549999992},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L9-'Input Data'!$F$17)","v":637.82721000000117},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M9-'Input Data'!$F$17)","v":-479.58763499999975},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N9-'Input Data'!$F$17)","v":-1881.8337149999993},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O9-'Input Data'!$F$17)","v":-2845.8778949999996},null,5,{"$f":"IF('Dry Bulb'!D9>'Operative BP'!$P$22,IF('Dry Bulb'!D9<'Operative BP'!$P$23,C8,0),0)","v":0},{"$f":"IF('Dry Bulb'!E9>'Operative BP'!$P$22,IF('Dry Bulb'!E9<'Operative BP'!$P$23,D8,0),0)","v":0},{"$f":"IF('Dry Bulb'!F9>'Operative BP'!$P$22,IF('Dry Bulb'!F9<'Operative BP'!$P$23,E8,0),0)","v":0},{"$f":"IF('Dry Bulb'!G9>'Operative BP'!$P$22,IF('Dry Bulb'!G9<'Operative BP'!$P$23,F8,0),0)","v":-808.23906000000011},{"$f":"IF('Dry Bulb'!H9>'Operative BP'!$P$22,IF('Dry Bulb'!H9<'Operative BP'!$P$23,G8,0),0)","v":0},{"$f":"IF('Dry Bulb'!I9>'Operative BP'!$P$22,IF('Dry Bulb'!I9<'Operative BP'!$P$23,H8,0),0)","v":0},{"$f":"IF('Dry Bulb'!J9>'Operative BP'!$P$22,IF('Dry Bulb'!J9<'Operative BP'!$P$23,I8,0),0)","v":0},{"$f":"IF('Dry Bulb'!K9>'Operative BP'!$P$22,IF('Dry Bulb'!K9<'Operative BP'!$P$23,J8,0),0)","v":0},{"$f":"IF('Dry Bulb'!L9>'Operative BP'!$P$22,IF('Dry Bulb'!L9<'Operative BP'!$P$23,K8,0),0)","v":0},{"$f":"IF('Dry Bulb'!M9>'Operative BP'!$P$22,IF('Dry Bulb'!M9<'Operative BP'!$P$23,L8,0),0)","v":-479.58763499999975},{"$f":"IF('Dry Bulb'!N9>'Operative BP'!$P$22,IF('Dry Bulb'!N9<'Operative BP'!$P$23,M8,0),0)","v":0},{"$f":"IF('Dry Bulb'!O9>'Operative BP'!$P$22,IF('Dry Bulb'!O9<'Operative BP'!$P$23,N8,0),0)","v":0}]
[null,6,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D10-'Input Data'!$F$17)","v":-3174.5293200000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E10-'Input Data'!$F$17)","v":-2714.4173249999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F10-'Input Data'!$F$17)","v":-1903.7438100000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G10-'Input Data'!$F$17)","v":-895.87943999999993},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H10-'Input Data'!$F$17)","v":462.54644999999965},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I10-'Input Data'!$F$17)","v":1032.2089200000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J10-'Input Data'!$F$17)","v":1251.3098700000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K10-'Input Data'!$F$17)","v":1207.4896799999985},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L10-'Input Data'!$F$17)","v":572.0969250000004},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M10-'Input Data'!$F$17)","v":-589.13811000000044},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N10-'Input Data'!$F$17)","v":-1925.6539050000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O10-'Input Data'!$F$17)","v":-2845.8778949999996},null,6,{"$f":"IF('Dry Bulb'!D10>'Operative BP'!$P$22,IF('Dry Bulb'!D10<'Operative BP'!$P$23,C9,0),0)","v":0},{"$f":"IF('Dry Bulb'!E10>'Operative BP'!$P$22,IF('Dry Bulb'!E10<'Operative BP'!$P$23,D9,0),0)","v":0},{"$f":"IF('Dry Bulb'!F10>'Operative BP'!$P$22,IF('Dry Bulb'!F10<'Operative BP'!$P$23,E9,0),0)","v":0},{"$f":"IF('Dry Bulb'!G10>'Operative BP'!$P$22,IF('Dry Bulb'!G10<'Operative BP'!$P$23,F9,0),0)","v":-895.87943999999993},{"$f":"IF('Dry Bulb'!H10>'Operative BP'!$P$22,IF('Dry Bulb'!H10<'Operative BP'!$P$23,G9,0),0)","v":462.54644999999965},{"$f":"IF('Dry Bulb'!I10>'Operative BP'!$P$22,IF('Dry Bulb'!I10<'Operative BP'!$P$23,H9,0),0)","v":0},{"$f":"IF('Dry Bulb'!J10>'Operative BP'!$P$22,IF('Dry Bulb'!J10<'Operative BP'!$P$23,I9,0),0)","v":0},{"$f":"IF('Dry Bulb'!K10>'Operative BP'!$P$22,IF('Dry Bulb'!K10<'Operative BP'!$P$23,J9,0),0)","v":0},{"$f":"IF('Dry Bulb'!L10>'Operative BP'!$P$22,IF('Dry Bulb'!L10<'Operative BP'!$P$23,K9,0),0)","v":572.0969250000004},{"$f":"IF('Dry Bulb'!M10>'Operative BP'!$P$22,IF('Dry Bulb'!M10<'Operative BP'!$P$23,L9,0),0)","v":-589.13811000000044},{"$f":"IF('Dry Bulb'!N10>'Operative BP'!$P$22,IF('Dry Bulb'!N10<'Operative BP'!$P$23,M9,0),0)","v":0},{"$f":"IF('Dry Bulb'!O10>'Operative BP'!$P$22,IF('Dry Bulb'!O10<'Operative BP'!$P$23,N9,0),0)","v":0}]
[null,7,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D11-'Input Data'!$F$17)","v":-3174.5293200000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E11-'Input Data'!$F$17)","v":-2714.4173249999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F11-'Input Data'!$F$17)","v":-1903.7438100000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G11-'Input Data'!$F$17)","v":-676.77849000000026},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H11-'Input Data'!$F$17)","v":703.55749500000013},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I11-'Input Data'!$F$17)","v":1382.77044},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J11-'Input Data'!$F$17)","v":1579.9612950000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K11-'Input Data'!$F$17)","v":1514.2310099999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L11-'Input Data'!$F$17)","v":813.10797000000082},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M11-'Input Data'!$F$17)","v":-479.58763499999975},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N11-'Input Data'!$F$17)","v":-1969.474095},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O11-'Input Data'!$F$17)","v":-2889.6980850000004},null,7,{"$f":"IF('Dry Bulb'!D11>'Operative BP'!$P$22,IF('Dry Bulb'!D11<'Operative BP'!$P$23,C10,0),0)","v":0},{"$f":"IF('Dry Bulb'!E11>'Operative BP'!$P$22,IF('Dry Bulb'!E11<'Operative BP'!$P$23,D10,0),0)","v":0},{"$f":"IF('Dry Bulb'!F11>'Operative BP'!$P$22,IF('Dry Bulb'!F11<'Operative BP'!$P$23,E10,0),0)","v":0},{"$f":"IF('Dry Bulb'!G11>'Operative BP'!$P$22,IF('Dry Bulb'!G11<'Operative BP'!$P$23,F10,0),0)","v":-676.77849000000026},{"$f":"IF('Dry Bulb'!H11>'Operative BP'!$P$22,IF('Dry Bulb'!H11<'Operative BP'!$P$23,G10,0),0)","v":0},{"$f":"IF('Dry Bulb'!I11>'Operative BP'!$P$22,IF('Dry Bulb'!I11<'Operative BP'!$P$23,H10,0),0)","v":0},{"$f":"IF('Dry Bulb'!J11>'Operative BP'!$P$22,IF('Dry Bulb'!J11<'Operative BP'!$P$23,I10,0),0)","v":0},{"$f":"IF('Dry Bulb'!K11>'Operative BP'!$P$22,IF('Dry Bulb'!K11<'Operative BP'!$P$23,J10,0),0)","v":0},{"$f":"IF('Dry Bulb'!L11>'Operative BP'!$P$22,IF('Dry Bulb'!L11<'Operative BP'!$P$23,K10,0),0)","v":0},{"$f":"IF('Dry Bulb'!M11>'Operative BP'!$P$22,IF('Dry Bulb'!M11<'Operative BP'!$P$23,L10,0),0)","v":-479.58763499999975},{"$f":"IF('Dry Bulb'!N11>'Operative BP'!$P$22,IF('Dry Bulb'!N11<'Operative BP'!$P$23,M10,0),0)","v":0},{"$f":"IF('Dry Bulb'!O11>'Operative BP'!$P$22,IF('Dry Bulb'!O11<'Operative BP'!$P$23,N10,0),0)","v":0}]
[null,8,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D12-'Input Data'!$F$17)","v":-2889.6980850000004},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E12-'Input Data'!$F$17)","v":-2429.5860900000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F12-'Input Data'!$F$17)","v":-1531.2721949999998},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G12-'Input Data'!$F$17)","v":-282.39677999999918},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H12-'Input Data'!$F$17)","v":1141.7593950000012},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I12-'Input Data'!$F$17)","v":1820.9723400000009},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J12-'Input Data'!$F$17)","v":2018.1631950000017},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K12-'Input Data'!$F$17)","v":1996.2531000000008},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L12-'Input Data'!$F$17)","v":1360.860345000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M12-'Input Data'!$F$17)","v":2.4344549999995158},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N12-'Input Data'!$F$17)","v":-1377.9015300000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O12-'Input Data'!$F$17)","v":-2692.5072300000006},null,8,{"$f":"IF('Dry Bulb'!D12>'Operative BP'!$P$22,IF('Dry Bulb'!D12<'Operative BP'!$P$23,C11,0),0)","v":0},{"$f":"IF('Dry Bulb'!E12>'Operative BP'!$P$22,IF('Dry Bulb'!E12<'Operative BP'!$P$23,D11,0),0)","v":0},{"$f":"IF('Dry Bulb'!F12>'Operative BP'!$P$22,IF('Dry Bulb'!F12<'Operative BP'!$P$23,E11,0),0)","v":0},{"$f":"IF('Dry Bulb'!G12>'Operative BP'!$P$22,IF('Dry Bulb'!G12<'Operative BP'!$P$23,F11,0),0)","v":-282.39677999999918},{"$f":"IF('Dry Bulb'!H12>'Operative BP'!$P$22,IF('Dry Bulb'!H12<'Operative BP'!$P$23,G11,0),0)","v":0},{"$f":"IF('Dry Bulb'!I12>'Operative BP'!$P$22,IF('Dry Bulb'!I12<'Operative BP'!$P$23,H11,0),0)","v":0},{"$f":"IF('Dry Bulb'!J12>'Operative BP'!$P$22,IF('Dry Bulb'!J12<'Operative BP'!$P$23,I11,0),0)","v":0},{"$f":"IF('Dry Bulb'!K12>'Operative BP'!$P$22,IF('Dry Bulb'!K12<'Operative BP'!$P$23,J11,0),0)","v":0},{"$f":"IF('Dry Bulb'!L12>'Operative BP'!$P$22,IF('Dry Bulb'!L12<'Operative BP'!$P$23,K11,0),0)","v":0},{"$f":"IF('Dry Bulb'!M12>'Operative BP'!$P$22,IF('Dry Bulb'!M12<'Operative BP'!$P$23,L11,0),0)","v":2.4344549999995158},{"$f":"IF('Dry Bulb'!N12>'Operative BP'!$P$22,IF('Dry Bulb'!N12<'Operative BP'!$P$23,M11,0),0)","v":0},{"$f":"IF('Dry Bulb'!O12>'Operative BP'!$P$22,IF('Dry Bulb'!O12<'Operative BP'!$P$23,N11,0),0)","v":0}]
[null,9,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D13-'Input Data'!$F$17)","v":-2561.04666},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E13-'Input Data'!$F$17)","v":-2079.02457},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F13-'Input Data'!$F$17)","v":-1268.3510550000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G13-'Input Data'!$F$17)","v":243.44550000000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H13-'Input Data'!$F$17)","v":1492.3209150000007},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I13-'Input Data'!$F$17)","v":2237.2641450000015},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J13-'Input Data'!$F$17)","v":2544.0054750000008},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K13-'Input Data'!$F$17)","v":2565.9155700000015},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L13-'Input Data'!$F$17)","v":1864.7925299999993},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M13-'Input Data'!$F$17)","v":506.36663999999962},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N13-'Input Data'!$F$17)","v":-786.32896499999924},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O13-'Input Data'!$F$17)","v":-2341.9457100000004},null,9,{"$f":"IF('Dry Bulb'!D13>'Operative BP'!$P$22,IF('Dry Bulb'!D13<'Operative BP'!$P$23,C12,0),0)","v":0},{"$f":"IF('Dry Bulb'!E13>'Operative BP'!$P$22,IF('Dry Bulb'!E13<'Operative BP'!$P$23,D12,0),0)","v":0},{"$f":"IF('Dry Bulb'!F13>'Operative BP'!$P$22,IF('Dry Bulb'!F13<'Operative BP'!$P$23,E12,0),0)","v":0},{"$f":"IF('Dry Bulb'!G13>'Operative BP'!$P$22,IF('Dry Bulb'!G13<'Operative BP'!$P$23,F12,0),0)","v":243.44550000000001},{"$f":"IF('Dry Bulb'!H13>'Operative BP'!$P$22,IF('Dry Bulb'!H13<'Operative BP'!$P$23,G12,0),0)","v":0},{"$f":"IF('Dry Bulb'!I13>'Operative BP'!$P$22,IF('Dry Bulb'!I13<'Operative BP'!$P$23,H12,0),0)","v":0},{"$f":"IF('Dry Bulb'!J13>'Operative BP'!$P$22,IF('Dry Bulb'!J13<'Operative BP'!$P$23,I12,0),0)","v":0},{"$f":"IF('Dry Bulb'!K13>'Operative BP'!$P$22,IF('Dry Bulb'!K13<'Operative BP'!$P$23,J12,0),0)","v":0},{"$f":"IF('Dry Bulb'!L13>'Operative BP'!$P$22,IF('Dry Bulb'!L13<'Operative BP'!$P$23,K12,0),0)","v":0},{"$f":"IF('Dry Bulb'!M13>'Operative BP'!$P$22,IF('Dry Bulb'!M13<'Operative BP'!$P$23,L12,0),0)","v":506.36663999999962},{"$f":"IF('Dry Bulb'!N13>'Operative BP'!$P$22,IF('Dry Bulb'!N13<'Operative BP'!$P$23,M12,0),0)","v":-786.32896499999924},{"$f":"IF('Dry Bulb'!O13>'Operative BP'!$P$22,IF('Dry Bulb'!O13<'Operative BP'!$P$23,N12,0),0)","v":0}]
[null,10,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D14-'Input Data'!$F$17)","v":-2210.4851399999998},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E14-'Input Data'!$F$17)","v":-1706.5529549999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F14-'Input Data'!$F$17)","v":-917.7895350000008},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G14-'Input Data'!$F$17)","v":659.73730500000022},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H14-'Input Data'!$F$17)","v":1864.7925299999993},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I14-'Input Data'!$F$17)","v":2609.73576},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J14-'Input Data'!$F$17)","v":3004.117470000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K14-'Input Data'!$F$17)","v":3069.8477549999998},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L14-'Input Data'!$F$17)","v":2302.9944299999984},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M14-'Input Data'!$F$17)","v":966.47863499999971},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N14-'Input Data'!$F$17)","v":-304.30687499999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O14-'Input Data'!$F$17)","v":-1969.474095},null,10,{"$f":"IF('Dry Bulb'!D14>'Operative BP'!$P$22,IF('Dry Bulb'!D14<'Operative BP'!$P$23,C13,0),0)","v":0},{"$f":"IF('Dry Bulb'!E14>'Operative BP'!$P$22,IF('Dry Bulb'!E14<'Operative BP'!$P$23,D13,0),0)","v":0},{"$f":"IF('Dry Bulb'!F14>'Operative BP'!$P$22,IF('Dry Bulb'!F14<'Operative BP'!$P$23,E13,0),0)","v":-917.7895350000008},{"$f":"IF('Dry Bulb'!G14>'Operative BP'!$P$22,IF('Dry Bulb'!G14<'Operative BP'!$P$23,F13,0),0)","v":0},{"$f":"IF('Dry Bulb'!H14>'Operative BP'!$P$22,IF('Dry Bulb'!H14<'Operative BP'!$P$23,G13,0),0)","v":0},{"$f":"IF('Dry Bulb'!I14>'Operative BP'!$P$22,IF('Dry Bulb'!I14<'Operative BP'!$P$23,H13,0),0)","v":0},{"$f":"IF('Dry Bulb'!J14>'Operative BP'!$P$22,IF('Dry Bulb'!J14<'Operative BP'!$P$23,I13,0),0)","v":0},{"$f":"IF('Dry Bulb'!K14>'Operative BP'!$P$22,IF('Dry Bulb'!K14<'Operative BP'!$P$23,J13,0),0)","v":0},{"$f":"IF('Dry Bulb'!L14>'Operative BP'!$P$22,IF('Dry Bulb'!L14<'Operative BP'!$P$23,K13,0),0)","v":0},{"$f":"IF('Dry Bulb'!M14>'Operative BP'!$P$22,IF('Dry Bulb'!M14<'Operative BP'!$P$23,L13,0),0)","v":0},{"$f":"IF('Dry Bulb'!N14>'Operative BP'!$P$22,IF('Dry Bulb'!N14<'Operative BP'!$P$23,M13,0),0)","v":-304.30687499999999},{"$f":"IF('Dry Bulb'!O14>'Operative BP'!$P$22,IF('Dry Bulb'!O14<'Operative BP'!$P$23,N13,0),0)","v":0}]
[null,11,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D15-'Input Data'!$F$17)","v":-1903.7438100000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E15-'Input Data'!$F$17)","v":-1290.2611499999994},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F15-'Input Data'!$F$17)","v":-611.04820499999948},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G15-'Input Data'!$F$17)","v":1010.2988249999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H15-'Input Data'!$F$17)","v":2171.5338600000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I15-'Input Data'!$F$17)","v":2938.387185},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J15-'Input Data'!$F$17)","v":3354.6789900000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K15-'Input Data'!$F$17)","v":3486.1395600000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L15-'Input Data'!$F$17)","v":2609.73576},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M15-'Input Data'!$F$17)","v":1338.9502500000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N15-'Input Data'!$F$17)","v":133.89502499999932},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O15-'Input Data'!$F$17)","v":-1597.0024799999997},null,11,{"$f":"IF('Dry Bulb'!D15>'Operative BP'!$P$22,IF('Dry Bulb'!D15<'Operative BP'!$P$23,C14,0),0)","v":0},{"$f":"IF('Dry Bulb'!E15>'Operative BP'!$P$22,IF('Dry Bulb'!E15<'Operative BP'!$P$23,D14,0),0)","v":0},{"$f":"IF('Dry Bulb'!F15>'Operative BP'!$P$22,IF('Dry Bulb'!F15<'Operative BP'!$P$23,E14,0),0)","v":-611.04820499999948},{"$f":"IF('Dry Bulb'!G15>'Operative BP'!$P$22,IF('Dry Bulb'!G15<'Operative BP'!$P$23,F14,0),0)","v":0},{"$f":"IF('Dry Bulb'!H15>'Operative BP'!$P$22,IF('Dry Bulb'!H15<'Operative BP'!$P$23,G14,0),0)","v":0},{"$f":"IF('Dry Bulb'!I15>'Operative BP'!$P$22,IF('Dry Bulb'!I15<'Operative BP'!$P$23,H14,0),0)","v":0},{"$f":"IF('Dry Bulb'!J15>'Operative BP'!$P$22,IF('Dry Bulb'!J15<'Operative BP'!$P$23,I14,0),0)","v":0},{"$f":"IF('Dry Bulb'!K15>'Operative BP'!$P$22,IF('Dry Bulb'!K15<'Operative BP'!$P$23,J14,0),0)","v":0},{"$f":"IF('Dry Bulb'!L15>'Operative BP'!$P$22,IF('Dry Bulb'!L15<'Operative BP'!$P$23,K14,0),0)","v":0},{"$f":"IF('Dry Bulb'!M15>'Operative BP'!$P$22,IF('Dry Bulb'!M15<'Operative BP'!$P$23,L14,0),0)","v":0},{"$f":"IF('Dry Bulb'!N15>'Operative BP'!$P$22,IF('Dry Bulb'!N15<'Operative BP'!$P$23,M14,0),0)","v":133.89502499999932},{"$f":"IF('Dry Bulb'!O15>'Operative BP'!$P$22,IF('Dry Bulb'!O15<'Operative BP'!$P$23,N14,0),0)","v":0}]
[null,12,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D16-'Input Data'!$F$17)","v":-1597.0024799999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E16-'Input Data'!$F$17)","v":-983.51981999999987},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F16-'Input Data'!$F$17)","v":-413.85735000000074},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G16-'Input Data'!$F$17)","v":1273.2199650000009},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H16-'Input Data'!$F$17)","v":2412.5449049999993},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I16-'Input Data'!$F$17)","v":3223.2184200000006},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J16-'Input Data'!$F$17)","v":3573.7799399999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K16-'Input Data'!$F$17)","v":3727.1506049999989},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L16-'Input Data'!$F$17)","v":2828.8367099999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M16-'Input Data'!$F$17)","v":1645.6915799999995},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N16-'Input Data'!$F$17)","v":440.63635500000055},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O16-'Input Data'!$F$17)","v":-1334.0813399999993},null,12,{"$f":"IF('Dry Bulb'!D16>'Operative BP'!$P$22,IF('Dry Bulb'!D16<'Operative BP'!$P$23,C15,0),0)","v":0},{"$f":"IF('Dry Bulb'!E16>'Operative BP'!$P$22,IF('Dry Bulb'!E16<'Operative BP'!$P$23,D15,0),0)","v":-983.51981999999987},{"$f":"IF('Dry Bulb'!F16>'Operative BP'!$P$22,IF('Dry Bulb'!F16<'Operative BP'!$P$23,E15,0),0)","v":-413.85735000000074},{"$f":"IF('Dry Bulb'!G16>'Operative BP'!$P$22,IF('Dry Bulb'!G16<'Operative BP'!$P$23,F15,0),0)","v":0},{"$f":"IF('Dry Bulb'!H16>'Operative BP'!$P$22,IF('Dry Bulb'!H16<'Operative BP'!$P$23,G15,0),0)","v":0},{"$f":"IF('Dry Bulb'!I16>'Operative BP'!$P$22,IF('Dry Bulb'!I16<'Operative BP'!$P$23,H15,0),0)","v":0},{"$f":"IF('Dry Bulb'!J16>'Operative BP'!$P$22,IF('Dry Bulb'!J16<'Operative BP'!$P$23,I15,0),0)","v":0},{"$f":"IF('Dry Bulb'!K16>'Operative BP'!$P$22,IF('Dry Bulb'!K16<'Operative BP'!$P$23,J15,0),0)","v":0},{"$f":"IF('Dry Bulb'!L16>'Operative BP'!$P$22,IF('Dry Bulb'!L16<'Operative BP'!$P$23,K15,0),0)","v":0},{"$f":"IF('Dry Bulb'!M16>'Operative BP'!$P$22,IF('Dry Bulb'!M16<'Operative BP'!$P$23,L15,0),0)","v":0},{"$f":"IF('Dry Bulb'!N16>'Operative BP'!$P$22,IF('Dry Bulb'!N16<'Operative BP'!$P$23,M15,0),0)","v":440.63635500000055},{"$f":"IF('Dry Bulb'!O16>'Operative BP'!$P$22,IF('Dry Bulb'!O16<'Operative BP'!$P$23,N15,0),0)","v":0}]
[null,13,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D17-'Input Data'!$F$17)","v":-1355.9914350000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E17-'Input Data'!$F$17)","v":-654.86839499999951},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F17-'Input Data'!$F$17)","v":24.344550000000346},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G17-'Input Data'!$F$17)","v":1426.5906299999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H17-'Input Data'!$F$17)","v":2653.5559499999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I17-'Input Data'!$F$17)","v":3376.5890849999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J17-'Input Data'!$F$17)","v":3749.0607},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K17-'Input Data'!$F$17)","v":3968.1616499999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L17-'Input Data'!$F$17)","v":3047.9376599999991},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M17-'Input Data'!$F$17)","v":1864.7925299999993},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N17-'Input Data'!$F$17)","v":703.55749500000013},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O17-'Input Data'!$F$17)","v":-1071.1601999999998},null,13,{"$f":"IF('Dry Bulb'!D17>'Operative BP'!$P$22,IF('Dry Bulb'!D17<'Operative BP'!$P$23,C16,0),0)","v":0},{"$f":"IF('Dry Bulb'!E17>'Operative BP'!$P$22,IF('Dry Bulb'!E17<'Operative BP'!$P$23,D16,0),0)","v":-654.86839499999951},{"$f":"IF('Dry Bulb'!F17>'Operative BP'!$P$22,IF('Dry Bulb'!F17<'Operative BP'!$P$23,E16,0),0)","v":24.344550000000346},{"$f":"IF('Dry Bulb'!G17>'Operative BP'!$P$22,IF('Dry Bulb'!G17<'Operative BP'!$P$23,F16,0),0)","v":0},{"$f":"IF('Dry Bulb'!H17>'Operative BP'!$P$22,IF('Dry Bulb'!H17<'Operative BP'!$P$23,G16,0),0)","v":0},{"$f":"IF('Dry Bulb'!I17>'Operative BP'!$P$22,IF('Dry Bulb'!I17<'Operative BP'!$P$23,H16,0),0)","v":0},{"$f":"IF('Dry Bulb'!J17>'Operative BP'!$P$22,IF('Dry Bulb'!J17<'Operative BP'!$P$23,I16,0),0)","v":0},{"$f":"IF('Dry Bulb'!K17>'Operative BP'!$P$22,IF('Dry Bulb'!K17<'Operative BP'!$P$23,J16,0),0)","v":0},{"$f":"IF('Dry Bulb'!L17>'Operative BP'!$P$22,IF('Dry Bulb'!L17<'Operative BP'!$P$23,K16,0),0)","v":0},{"$f":"IF('Dry Bulb'!M17>'Operative BP'!$P$22,IF('Dry Bulb'!M17<'Operative BP'!$P$23,L16,0),0)","v":0},{"$f":"IF('Dry Bulb'!N17>'Operative BP'!$P$22,IF('Dry Bulb'!N17<'Operative BP'!$P$23,M16,0),0)","v":0},{"$f":"IF('Dry Bulb'!O17>'Operative BP'!$P$22,IF('Dry Bulb'!O17<'Operative BP'!$P$23,N16,0),0)","v":-1071.1601999999998}]
[null,14,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D18-'Input Data'!$F$17)","v":-1158.8005799999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E18-'Input Data'!$F$17)","v":-413.85735000000074},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F18-'Input Data'!$F$17)","v":221.53540499999917},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G18-'Input Data'!$F$17)","v":1601.8713899999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H18-'Input Data'!$F$17)","v":2828.8367099999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I18-'Input Data'!$F$17)","v":3639.5102250000009},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J18-'Input Data'!$F$17)","v":3946.2515549999985},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K18-'Input Data'!$F$17)","v":4077.712125},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L18-'Input Data'!$F$17)","v":3179.3982299999989},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M18-'Input Data'!$F$17)","v":2040.0732900000007},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N18-'Input Data'!$F$17)","v":813.10797000000082},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O18-'Input Data'!$F$17)","v":-895.87943999999993},null,14,{"$f":"IF('Dry Bulb'!D18>'Operative BP'!$P$22,IF('Dry Bulb'!D18<'Operative BP'!$P$23,C17,0),0)","v":-1158.8005799999996},{"$f":"IF('Dry Bulb'!E18>'Operative BP'!$P$22,IF('Dry Bulb'!E18<'Operative BP'!$P$23,D17,0),0)","v":-413.85735000000074},{"$f":"IF('Dry Bulb'!F18>'Operative BP'!$P$22,IF('Dry Bulb'!F18<'Operative BP'!$P$23,E17,0),0)","v":221.53540499999917},{"$f":"IF('Dry Bulb'!G18>'Operative BP'!$P$22,IF('Dry Bulb'!G18<'Operative BP'!$P$23,F17,0),0)","v":0},{"$f":"IF('Dry Bulb'!H18>'Operative BP'!$P$22,IF('Dry Bulb'!H18<'Operative BP'!$P$23,G17,0),0)","v":0},{"$f":"IF('Dry Bulb'!I18>'Operative BP'!$P$22,IF('Dry Bulb'!I18<'Operative BP'!$P$23,H17,0),0)","v":0},{"$f":"IF('Dry Bulb'!J18>'Operative BP'!$P$22,IF('Dry Bulb'!J18<'Operative BP'!$P$23,I17,0),0)","v":0},{"$f":"IF('Dry Bulb'!K18>'Operative BP'!$P$22,IF('Dry Bulb'!K18<'Operative BP'!$P$23,J17,0),0)","v":0},{"$f":"IF('Dry Bulb'!L18>'Operative BP'!$P$22,IF('Dry Bulb'!L18<'Operative BP'!$P$23,K17,0),0)","v":0},{"$f":"IF('Dry Bulb'!M18>'Operative BP'!$P$22,IF('Dry Bulb'!M18<'Operative BP'!$P$23,L17,0),0)","v":0},{"$f":"IF('Dry Bulb'!N18>'Operative BP'!$P$22,IF('Dry Bulb'!N18<'Operative BP'!$P$23,M17,0),0)","v":0},{"$f":"IF('Dry Bulb'!O18>'Operative BP'!$P$22,IF('Dry Bulb'!O18<'Operative BP'!$P$23,N17,0),0)","v":-895.87943999999993}]
[null,15,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D19-'Input Data'!$F$17)","v":-1093.0702950000004},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E19-'Input Data'!$F$17)","v":-282.39677999999918},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F19-'Input Data'!$F$17)","v":352.99597500000073},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G19-'Input Data'!$F$17)","v":1711.4218650000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H19-'Input Data'!$F$17)","v":2872.6568999999995},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I19-'Input Data'!$F$17)","v":3727.1506049999989},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J19-'Input Data'!$F$17)","v":4055.8020299999994},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K19-'Input Data'!$F$17)","v":4121.5323150000004},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L19-'Input Data'!$F$17)","v":3267.0386100000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M19-'Input Data'!$F$17)","v":2149.6237649999998},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N19-'Input Data'!$F$17)","v":966.47863499999971},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O19-'Input Data'!$F$17)","v":-808.23906000000011},null,15,{"$f":"IF('Dry Bulb'!D19>'Operative BP'!$P$22,IF('Dry Bulb'!D19<'Operative BP'!$P$23,C18,0),0)","v":-1093.0702950000004},{"$f":"IF('Dry Bulb'!E19>'Operative BP'!$P$22,IF('Dry Bulb'!E19<'Operative BP'!$P$23,D18,0),0)","v":-282.39677999999918},{"$f":"IF('Dry Bulb'!F19>'Operative BP'!$P$22,IF('Dry Bulb'!F19<'Operative BP'!$P$23,E18,0),0)","v":352.99597500000073},{"$f":"IF('Dry Bulb'!G19>'Operative BP'!$P$22,IF('Dry Bulb'!G19<'Operative BP'!$P$23,F18,0),0)","v":0},{"$f":"IF('Dry Bulb'!H19>'Operative BP'!$P$22,IF('Dry Bulb'!H19<'Operative BP'!$P$23,G18,0),0)","v":0},{"$f":"IF('Dry Bulb'!I19>'Operative BP'!$P$22,IF('Dry Bulb'!I19<'Operative BP'!$P$23,H18,0),0)","v":0},{"$f":"IF('Dry Bulb'!J19>'Operative BP'!$P$22,IF('Dry Bulb'!J19<'Operative BP'!$P$23,I18,0),0)","v":0},{"$f":"IF('Dry Bulb'!K19>'Operative BP'!$P$22,IF('Dry Bulb'!K19<'Operative BP'!$P$23,J18,0),0)","v":0},{"$f":"IF('Dry Bulb'!L19>'Operative BP'!$P$22,IF('Dry Bulb'!L19<'Operative BP'!$P$23,K18,0),0)","v":0},{"$f":"IF('Dry Bulb'!M19>'Operative BP'!$P$22,IF('Dry Bulb'!M19<'Operative BP'!$P$23,L18,0),0)","v":0},{"$f":"IF('Dry Bulb'!N19>'Operative BP'!$P$22,IF('Dry Bulb'!N19<'Operative BP'!$P$23,M18,0),0)","v":0},{"$f":"IF('Dry Bulb'!O19>'Operative BP'!$P$22,IF('Dry Bulb'!O19<'Operative BP'!$P$23,N18,0),0)","v":-808.23906000000011}]
[null,16,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D20-'Input Data'!$F$17)","v":-1071.1601999999998},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E20-'Input Data'!$F$17)","v":-326.21697000000086},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F20-'Input Data'!$F$17)","v":396.81616499999893},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G20-'Input Data'!$F$17)","v":1623.7814850000004},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H20-'Input Data'!$F$17)","v":2894.5669950000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I20-'Input Data'!$F$17)","v":3749.0607},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J20-'Input Data'!$F$17)","v":4033.8919350000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K20-'Input Data'!$F$17)","v":4055.8020299999994},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L20-'Input Data'!$F$17)","v":3245.1285149999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M20-'Input Data'!$F$17)","v":2083.8934799999988},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N20-'Input Data'!$F$17)","v":856.92816000000084},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O20-'Input Data'!$F$17)","v":-895.87943999999993},null,16,{"$f":"IF('Dry Bulb'!D20>'Operative BP'!$P$22,IF('Dry Bulb'!D20<'Operative BP'!$P$23,C19,0),0)","v":-1071.1601999999998},{"$f":"IF('Dry Bulb'!E20>'Operative BP'!$P$22,IF('Dry Bulb'!E20<'Operative BP'!$P$23,D19,0),0)","v":-326.21697000000086},{"$f":"IF('Dry Bulb'!F20>'Operative BP'!$P$22,IF('Dry Bulb'!F20<'Operative BP'!$P$23,E19,0),0)","v":396.81616499999893},{"$f":"IF('Dry Bulb'!G20>'Operative BP'!$P$22,IF('Dry Bulb'!G20<'Operative BP'!$P$23,F19,0),0)","v":0},{"$f":"IF('Dry Bulb'!H20>'Operative BP'!$P$22,IF('Dry Bulb'!H20<'Operative BP'!$P$23,G19,0),0)","v":0},{"$f":"IF('Dry Bulb'!I20>'Operative BP'!$P$22,IF('Dry Bulb'!I20<'Operative BP'!$P$23,H19,0),0)","v":0},{"$f":"IF('Dry Bulb'!J20>'Operative BP'!$P$22,IF('Dry Bulb'!J20<'Operative BP'!$P$23,I19,0),0)","v":0},{"$f":"IF('Dry Bulb'!K20>'Operative BP'!$P$22,IF('Dry Bulb'!K20<'Operative BP'!$P$23,J19,0),0)","v":0},{"$f":"IF('Dry Bulb'!L20>'Operative BP'!$P$22,IF('Dry Bulb'!L20<'Operative BP'!$P$23,K19,0),0)","v":0},{"$f":"IF('Dry Bulb'!M20>'Operative BP'!$P$22,IF('Dry Bulb'!M20<'Operative BP'!$P$23,L19,0),0)","v":0},{"$f":"IF('Dry Bulb'!N20>'Operative BP'!$P$22,IF('Dry Bulb'!N20<'Operative BP'!$P$23,M19,0),0)","v":0},{"$f":"IF('Dry Bulb'!O20>'Operative BP'!$P$22,IF('Dry Bulb'!O20<'Operative BP'!$P$23,N19,0),0)","v":-895.87943999999993}]
[null,17,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D21-'Input Data'!$F$17)","v":-1202.6207699999995},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E21-'Input Data'!$F$17)","v":-501.49773000000056},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F21-'Input Data'!$F$17)","v":265.35559500000085},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G21-'Input Data'!$F$17)","v":1426.5906299999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H21-'Input Data'!$F$17)","v":2872.6568999999995},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I21-'Input Data'!$F$17)","v":3661.4203200000015},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J21-'Input Data'!$F$17)","v":3968.1616499999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K21-'Input Data'!$F$17)","v":3902.4313650000004},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L21-'Input Data'!$F$17)","v":3069.8477549999998},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M21-'Input Data'!$F$17)","v":1952.4329099999991},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N21-'Input Data'!$F$17)","v":659.73730500000022},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O21-'Input Data'!$F$17)","v":-1136.8904850000004},null,17,{"$f":"IF('Dry Bulb'!D21>'Operative BP'!$P$22,IF('Dry Bulb'!D21<'Operative BP'!$P$23,C20,0),0)","v":-1202.6207699999995},{"$f":"IF('Dry Bulb'!E21>'Operative BP'!$P$22,IF('Dry Bulb'!E21<'Operative BP'!$P$23,D20,0),0)","v":-501.49773000000056},{"$f":"IF('Dry Bulb'!F21>'Operative BP'!$P$22,IF('Dry Bulb'!F21<'Operative BP'!$P$23,E20,0),0)","v":265.35559500000085},{"$f":"IF('Dry Bulb'!G21>'Operative BP'!$P$22,IF('Dry Bulb'!G21<'Operative BP'!$P$23,F20,0),0)","v":0},{"$f":"IF('Dry Bulb'!H21>'Operative BP'!$P$22,IF('Dry Bulb'!H21<'Operative BP'!$P$23,G20,0),0)","v":0},{"$f":"IF('Dry Bulb'!I21>'Operative BP'!$P$22,IF('Dry Bulb'!I21<'Operative BP'!$P$23,H20,0),0)","v":0},{"$f":"IF('Dry Bulb'!J21>'Operative BP'!$P$22,IF('Dry Bulb'!J21<'Operative BP'!$P$23,I20,0),0)","v":0},{"$f":"IF('Dry Bulb'!K21>'Operative BP'!$P$22,IF('Dry Bulb'!K21<'Operative BP'!$P$23,J20,0),0)","v":0},{"$f":"IF('Dry Bulb'!L21>'Operative BP'!$P$22,IF('Dry Bulb'!L21<'Operative BP'!$P$23,K20,0),0)","v":0},{"$f":"IF('Dry Bulb'!M21>'Operative BP'!$P$22,IF('Dry Bulb'!M21<'Operative BP'!$P$23,L20,0),0)","v":0},{"$f":"IF('Dry Bulb'!N21>'Operative BP'!$P$22,IF('Dry Bulb'!N21<'Operative BP'!$P$23,M20,0),0)","v":0},{"$f":"IF('Dry Bulb'!O21>'Operative BP'!$P$22,IF('Dry Bulb'!O21<'Operative BP'!$P$23,N20,0),0)","v":-1136.8904850000004}]
[null,18,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D22-'Input Data'!$F$17)","v":-1421.72172},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E22-'Input Data'!$F$17)","v":-720.59868000000029},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F22-'Input Data'!$F$17)","v":111.98493000000022},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G22-'Input Data'!$F$17)","v":1251.3098700000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H22-'Input Data'!$F$17)","v":2719.2862350000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I22-'Input Data'!$F$17)","v":3551.8698450000011},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J22-'Input Data'!$F$17)","v":3792.8808899999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K22-'Input Data'!$F$17)","v":3705.2405100000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L22-'Input Data'!$F$17)","v":2938.387185},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M22-'Input Data'!$F$17)","v":1777.1521499999994},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N22-'Input Data'!$F$17)","v":352.99597500000073},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O22-'Input Data'!$F$17)","v":-1290.2611499999994},null,18,{"$f":"IF('Dry Bulb'!D22>'Operative BP'!$P$22,IF('Dry Bulb'!D22<'Operative BP'!$P$23,C21,0),0)","v":0},{"$f":"IF('Dry Bulb'!E22>'Operative BP'!$P$22,IF('Dry Bulb'!E22<'Operative BP'!$P$23,D21,0),0)","v":-720.59868000000029},{"$f":"IF('Dry Bulb'!F22>'Operative BP'!$P$22,IF('Dry Bulb'!F22<'Operative BP'!$P$23,E21,0),0)","v":111.98493000000022},{"$f":"IF('Dry Bulb'!G22>'Operative BP'!$P$22,IF('Dry Bulb'!G22<'Operative BP'!$P$23,F21,0),0)","v":0},{"$f":"IF('Dry Bulb'!H22>'Operative BP'!$P$22,IF('Dry Bulb'!H22<'Operative BP'!$P$23,G21,0),0)","v":0},{"$f":"IF('Dry Bulb'!I22>'Operative BP'!$P$22,IF('Dry Bulb'!I22<'Operative BP'!$P$23,H21,0),0)","v":0},{"$f":"IF('Dry Bulb'!J22>'Operative BP'!$P$22,IF('Dry Bulb'!J22<'Operative BP'!$P$23,I21,0),0)","v":0},{"$f":"IF('Dry Bulb'!K22>'Operative BP'!$P$22,IF('Dry Bulb'!K22<'Operative BP'!$P$23,J21,0),0)","v":0},{"$f":"IF('Dry Bulb'!L22>'Operative BP'!$P$22,IF('Dry Bulb'!L22<'Operative BP'!$P$23,K21,0),0)","v":0},{"$f":"IF('Dry Bulb'!M22>'Operative BP'!$P$22,IF('Dry Bulb'!M22<'Operative BP'!$P$23,L21,0),0)","v":0},{"$f":"IF('Dry Bulb'!N22>'Operative BP'!$P$22,IF('Dry Bulb'!N22<'Operative BP'!$P$23,M21,0),0)","v":352.99597500000073},{"$f":"IF('Dry Bulb'!O22>'Operative BP'!$P$22,IF('Dry Bulb'!O22<'Operative BP'!$P$23,N21,0),0)","v":0}]
[null,19,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D23-'Input Data'!$F$17)","v":-1640.8226700000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E23-'Input Data'!$F$17)","v":-939.69962999999984},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F23-'Input Data'!$F$17)","v":-85.205925000000349},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G23-'Input Data'!$F$17)","v":944.56853999999896},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H23-'Input Data'!$F$17)","v":2522.0953799999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I23-'Input Data'!$F$17)","v":3310.8588000000004},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J23-'Input Data'!$F$17)","v":3486.1395600000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K23-'Input Data'!$F$17)","v":3420.4092749999995},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L23-'Input Data'!$F$17)","v":2719.2862350000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M23-'Input Data'!$F$17)","v":1536.1411049999988},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N23-'Input Data'!$F$17)","v":111.98493000000022},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O23-'Input Data'!$F$17)","v":-1597.0024799999997},null,19,{"$f":"IF('Dry Bulb'!D23>'Operative BP'!$P$22,IF('Dry Bulb'!D23<'Operative BP'!$P$23,C22,0),0)","v":0},{"$f":"IF('Dry Bulb'!E23>'Operative BP'!$P$22,IF('Dry Bulb'!E23<'Operative BP'!$P$23,D22,0),0)","v":-939.69962999999984},{"$f":"IF('Dry Bulb'!F23>'Operative BP'!$P$22,IF('Dry Bulb'!F23<'Operative BP'!$P$23,E22,0),0)","v":-85.205925000000349},{"$f":"IF('Dry Bulb'!G23>'Operative BP'!$P$22,IF('Dry Bulb'!G23<'Operative BP'!$P$23,F22,0),0)","v":0},{"$f":"IF('Dry Bulb'!H23>'Operative BP'!$P$22,IF('Dry Bulb'!H23<'Operative BP'!$P$23,G22,0),0)","v":0},{"$f":"IF('Dry Bulb'!I23>'Operative BP'!$P$22,IF('Dry Bulb'!I23<'Operative BP'!$P$23,H22,0),0)","v":0},{"$f":"IF('Dry Bulb'!J23>'Operative BP'!$P$22,IF('Dry Bulb'!J23<'Operative BP'!$P$23,I22,0),0)","v":0},{"$f":"IF('Dry Bulb'!K23>'Operative BP'!$P$22,IF('Dry Bulb'!K23<'Operative BP'!$P$23,J22,0),0)","v":0},{"$f":"IF('Dry Bulb'!L23>'Operative BP'!$P$22,IF('Dry Bulb'!L23<'Operative BP'!$P$23,K22,0),0)","v":0},{"$f":"IF('Dry Bulb'!M23>'Operative BP'!$P$22,IF('Dry Bulb'!M23<'Operative BP'!$P$23,L22,0),0)","v":0},{"$f":"IF('Dry Bulb'!N23>'Operative BP'!$P$22,IF('Dry Bulb'!N23<'Operative BP'!$P$23,M22,0),0)","v":111.98493000000022},{"$f":"IF('Dry Bulb'!O23>'Operative BP'!$P$22,IF('Dry Bulb'!O23<'Operative BP'!$P$23,N22,0),0)","v":0}]
[null,20,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D24-'Input Data'!$F$17)","v":-1881.8337149999993},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E24-'Input Data'!$F$17)","v":-1224.5308650000004},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F24-'Input Data'!$F$17)","v":-391.94725499999987},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G24-'Input Data'!$F$17)","v":747.37768500000016},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H24-'Input Data'!$F$17)","v":2237.2641450000015},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I24-'Input Data'!$F$17)","v":3004.117470000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J24-'Input Data'!$F$17)","v":3047.9376599999991},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K24-'Input Data'!$F$17)","v":3069.8477549999998},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L24-'Input Data'!$F$17)","v":2434.4549999999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M24-'Input Data'!$F$17)","v":1163.6694900000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N24-'Input Data'!$F$17)","v":-194.7563999999993},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O24-'Input Data'!$F$17)","v":-1816.1034300000003},null,20,{"$f":"IF('Dry Bulb'!D24>'Operative BP'!$P$22,IF('Dry Bulb'!D24<'Operative BP'!$P$23,C23,0),0)","v":0},{"$f":"IF('Dry Bulb'!E24>'Operative BP'!$P$22,IF('Dry Bulb'!E24<'Operative BP'!$P$23,D23,0),0)","v":0},{"$f":"IF('Dry Bulb'!F24>'Operative BP'!$P$22,IF('Dry Bulb'!F24<'Operative BP'!$P$23,E23,0),0)","v":-391.94725499999987},{"$f":"IF('Dry Bulb'!G24>'Operative BP'!$P$22,IF('Dry Bulb'!G24<'Operative BP'!$P$23,F23,0),0)","v":0},{"$f":"IF('Dry Bulb'!H24>'Operative BP'!$P$22,IF('Dry Bulb'!H24<'Operative BP'!$P$23,G23,0),0)","v":0},{"$f":"IF('Dry Bulb'!I24>'Operative BP'!$P$22,IF('Dry Bulb'!I24<'Operative BP'!$P$23,H23,0),0)","v":0},{"$f":"IF('Dry Bulb'!J24>'Operative BP'!$P$22,IF('Dry Bulb'!J24<'Operative BP'!$P$23,I23,0),0)","v":0},{"$f":"IF('Dry Bulb'!K24>'Operative BP'!$P$22,IF('Dry Bulb'!K24<'Operative BP'!$P$23,J23,0),0)","v":0},{"$f":"IF('Dry Bulb'!L24>'Operative BP'!$P$22,IF('Dry Bulb'!L24<'Operative BP'!$P$23,K23,0),0)","v":0},{"$f":"IF('Dry Bulb'!M24>'Operative BP'!$P$22,IF('Dry Bulb'!M24<'Operative BP'!$P$23,L23,0),0)","v":0},{"$f":"IF('Dry Bulb'!N24>'Operative BP'!$P$22,IF('Dry Bulb'!N24<'Operative BP'!$P$23,M23,0),0)","v":-194.7563999999993},{"$f":"IF('Dry Bulb'!O24>'Operative BP'!$P$22,IF('Dry Bulb'!O24<'Operative BP'!$P$23,N23,0),0)","v":0}]
[null,21,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D25-'Input Data'!$F$17)","v":-2035.2043799999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E25-'Input Data'!$F$17)","v":-1443.631815},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F25-'Input Data'!$F$17)","v":-567.22801499999957},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G25-'Input Data'!$F$17)","v":550.18682999999953},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H25-'Input Data'!$F$17)","v":1996.2531000000008},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I25-'Input Data'!$F$17)","v":2675.4660450000006},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J25-'Input Data'!$F$17)","v":2697.3761399999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K25-'Input Data'!$F$17)","v":2828.8367099999996},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L25-'Input Data'!$F$17)","v":2127.7136700000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M25-'Input Data'!$F$17)","v":922.6584449999998},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N25-'Input Data'!$F$17)","v":-391.94725499999987},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O25-'Input Data'!$F$17)","v":-1969.474095},null,21,{"$f":"IF('Dry Bulb'!D25>'Operative BP'!$P$22,IF('Dry Bulb'!D25<'Operative BP'!$P$23,C24,0),0)","v":0},{"$f":"IF('Dry Bulb'!E25>'Operative BP'!$P$22,IF('Dry Bulb'!E25<'Operative BP'!$P$23,D24,0),0)","v":0},{"$f":"IF('Dry Bulb'!F25>'Operative BP'!$P$22,IF('Dry Bulb'!F25<'Operative BP'!$P$23,E24,0),0)","v":-567.22801499999957},{"$f":"IF('Dry Bulb'!G25>'Operative BP'!$P$22,IF('Dry Bulb'!G25<'Operative BP'!$P$23,F24,0),0)","v":550.18682999999953},{"$f":"IF('Dry Bulb'!H25>'Operative BP'!$P$22,IF('Dry Bulb'!H25<'Operative BP'!$P$23,G24,0),0)","v":0},{"$f":"IF('Dry Bulb'!I25>'Operative BP'!$P$22,IF('Dry Bulb'!I25<'Operative BP'!$P$23,H24,0),0)","v":0},{"$f":"IF('Dry Bulb'!J25>'Operative BP'!$P$22,IF('Dry Bulb'!J25<'Operative BP'!$P$23,I24,0),0)","v":0},{"$f":"IF('Dry Bulb'!K25>'Operative BP'!$P$22,IF('Dry Bulb'!K25<'Operative BP'!$P$23,J24,0),0)","v":0},{"$f":"IF('Dry Bulb'!L25>'Operative BP'!$P$22,IF('Dry Bulb'!L25<'Operative BP'!$P$23,K24,0),0)","v":0},{"$f":"IF('Dry Bulb'!M25>'Operative BP'!$P$22,IF('Dry Bulb'!M25<'Operative BP'!$P$23,L24,0),0)","v":0},{"$f":"IF('Dry Bulb'!N25>'Operative BP'!$P$22,IF('Dry Bulb'!N25<'Operative BP'!$P$23,M24,0),0)","v":-391.94725499999987},{"$f":"IF('Dry Bulb'!O25>'Operative BP'!$P$22,IF('Dry Bulb'!O25<'Operative BP'!$P$23,N24,0),0)","v":0}]
[null,22,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D26-'Input Data'!$F$17)","v":-2210.4851399999998},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E26-'Input Data'!$F$17)","v":-1662.7327649999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F26-'Input Data'!$F$17)","v":-764.4188700000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G26-'Input Data'!$F$17)","v":352.99597500000073},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H26-'Input Data'!$F$17)","v":1777.1521499999994},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I26-'Input Data'!$F$17)","v":2390.63481},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J26-'Input Data'!$F$17)","v":2368.7247150000012},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K26-'Input Data'!$F$17)","v":2587.8256650000008},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L26-'Input Data'!$F$17)","v":1908.612720000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M26-'Input Data'!$F$17)","v":681.64739999999938},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N26-'Input Data'!$F$17)","v":-632.95830000000035},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O26-'Input Data'!$F$17)","v":-2122.84476},null,22,{"$f":"IF('Dry Bulb'!D26>'Operative BP'!$P$22,IF('Dry Bulb'!D26<'Operative BP'!$P$23,C25,0),0)","v":0},{"$f":"IF('Dry Bulb'!E26>'Operative BP'!$P$22,IF('Dry Bulb'!E26<'Operative BP'!$P$23,D25,0),0)","v":0},{"$f":"IF('Dry Bulb'!F26>'Operative BP'!$P$22,IF('Dry Bulb'!F26<'Operative BP'!$P$23,E25,0),0)","v":-764.4188700000002},{"$f":"IF('Dry Bulb'!G26>'Operative BP'!$P$22,IF('Dry Bulb'!G26<'Operative BP'!$P$23,F25,0),0)","v":352.99597500000073},{"$f":"IF('Dry Bulb'!H26>'Operative BP'!$P$22,IF('Dry Bulb'!H26<'Operative BP'!$P$23,G25,0),0)","v":0},{"$f":"IF('Dry Bulb'!I26>'Operative BP'!$P$22,IF('Dry Bulb'!I26<'Operative BP'!$P$23,H25,0),0)","v":0},{"$f":"IF('Dry Bulb'!J26>'Operative BP'!$P$22,IF('Dry Bulb'!J26<'Operative BP'!$P$23,I25,0),0)","v":0},{"$f":"IF('Dry Bulb'!K26>'Operative BP'!$P$22,IF('Dry Bulb'!K26<'Operative BP'!$P$23,J25,0),0)","v":0},{"$f":"IF('Dry Bulb'!L26>'Operative BP'!$P$22,IF('Dry Bulb'!L26<'Operative BP'!$P$23,K25,0),0)","v":0},{"$f":"IF('Dry Bulb'!M26>'Operative BP'!$P$22,IF('Dry Bulb'!M26<'Operative BP'!$P$23,L25,0),0)","v":0},{"$f":"IF('Dry Bulb'!N26>'Operative BP'!$P$22,IF('Dry Bulb'!N26<'Operative BP'!$P$23,M25,0),0)","v":-632.95830000000035},{"$f":"IF('Dry Bulb'!O26>'Operative BP'!$P$22,IF('Dry Bulb'!O26<'Operative BP'!$P$23,N25,0),0)","v":0}]
[null,23,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D27-'Input Data'!$F$17)","v":-2363.8558050000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E27-'Input Data'!$F$17)","v":-1838.0135250000003},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F27-'Input Data'!$F$17)","v":-939.69962999999984},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G27-'Input Data'!$F$17)","v":90.074835000001116},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H27-'Input Data'!$F$17)","v":1558.0511999999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I27-'Input Data'!$F$17)","v":2171.5338600000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J27-'Input Data'!$F$17)","v":2193.4439549999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K27-'Input Data'!$F$17)","v":2390.63481},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L27-'Input Data'!$F$17)","v":1689.5117700000012},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M27-'Input Data'!$F$17)","v":484.45654500000052},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N27-'Input Data'!$F$17)","v":-873.96934500000089},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O27-'Input Data'!$F$17)","v":-2232.3952350000004},null,23,{"$f":"IF('Dry Bulb'!D27>'Operative BP'!$P$22,IF('Dry Bulb'!D27<'Operative BP'!$P$23,C26,0),0)","v":0},{"$f":"IF('Dry Bulb'!E27>'Operative BP'!$P$22,IF('Dry Bulb'!E27<'Operative BP'!$P$23,D26,0),0)","v":0},{"$f":"IF('Dry Bulb'!F27>'Operative BP'!$P$22,IF('Dry Bulb'!F27<'Operative BP'!$P$23,E26,0),0)","v":-939.69962999999984},{"$f":"IF('Dry Bulb'!G27>'Operative BP'!$P$22,IF('Dry Bulb'!G27<'Operative BP'!$P$23,F26,0),0)","v":90.074835000001116},{"$f":"IF('Dry Bulb'!H27>'Operative BP'!$P$22,IF('Dry Bulb'!H27<'Operative BP'!$P$23,G26,0),0)","v":0},{"$f":"IF('Dry Bulb'!I27>'Operative BP'!$P$22,IF('Dry Bulb'!I27<'Operative BP'!$P$23,H26,0),0)","v":0},{"$f":"IF('Dry Bulb'!J27>'Operative BP'!$P$22,IF('Dry Bulb'!J27<'Operative BP'!$P$23,I26,0),0)","v":0},{"$f":"IF('Dry Bulb'!K27>'Operative BP'!$P$22,IF('Dry Bulb'!K27<'Operative BP'!$P$23,J26,0),0)","v":0},{"$f":"IF('Dry Bulb'!L27>'Operative BP'!$P$22,IF('Dry Bulb'!L27<'Operative BP'!$P$23,K26,0),0)","v":0},{"$f":"IF('Dry Bulb'!M27>'Operative BP'!$P$22,IF('Dry Bulb'!M27<'Operative BP'!$P$23,L26,0),0)","v":484.45654500000052},{"$f":"IF('Dry Bulb'!N27>'Operative BP'!$P$22,IF('Dry Bulb'!N27<'Operative BP'!$P$23,M26,0),0)","v":-873.96934500000089},{"$f":"IF('Dry Bulb'!O27>'Operative BP'!$P$22,IF('Dry Bulb'!O27<'Operative BP'!$P$23,N26,0),0)","v":0}]
[null,24,{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!D28-'Input Data'!$F$17)","v":-2473.4062800000002},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!E28-'Input Data'!$F$17)","v":-2035.2043799999999},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!F28-'Input Data'!$F$17)","v":-1114.9803899999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!G28-'Input Data'!$F$17)","v":-85.205925000000349},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!H28-'Input Data'!$F$17)","v":1360.860345000001},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!I28-'Input Data'!$F$17)","v":1952.4329099999991},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!J28-'Input Data'!$F$17)","v":2040.0732900000007},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!K28-'Input Data'!$F$17)","v":2171.5338600000005},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!L28-'Input Data'!$F$17)","v":1492.3209150000007},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!M28-'Input Data'!$F$17)","v":309.17578500000076},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!N28-'Input Data'!$F$17)","v":-1027.3400099999997},{"$f":"0.018033*('Input Data'!$F$50*'Input Data'!$F$19*'Input Data'!$F$21*'Input Data'!$F$23)*('Dry Bulb'!O28-'Input Data'!$F$17)","v":-2429.5860900000002},null,24,{"$f":"IF('Dry Bulb'!D28>'Operative BP'!$P$22,IF('Dry Bulb'!D28<'Operative BP'!$P$23,C27,0),0)","v":0},{"$f":"IF('Dry Bulb'!E28>'Operative BP'!$P$22,IF('Dry Bulb'!E28<'Operative BP'!$P$23,D27,0),0)","v":0},{"$f":"IF('Dry Bulb'!F28>'Operative BP'!$P$22,IF('Dry Bulb'!F28<'Operative BP'!$P$23,E27,0),0)","v":-1114.9803899999997},{"$f":"IF('Dry Bulb'!G28>'Operative BP'!$P$22,IF('Dry Bulb'!G28<'Operative BP'!$P$23,F27,0),0)","v":-85.205925000000349},{"$f":"IF('Dry Bulb'!H28>'Operative BP'!$P$22,IF('Dry Bulb'!H28<'Operative BP'!$P$23,G27,0),0)","v":0},{"$f":"IF('Dry Bulb'!I28>'Operative BP'!$P$22,IF('Dry Bulb'!I28<'Operative BP'!$P$23,H27,0),0)","v":0},{"$f":"IF('Dry Bulb'!J28>'Operative BP'!$P$22,IF('Dry Bulb'!J28<'Operative BP'!$P$23,I27,0),0)","v":0},{"$f":"IF('Dry Bulb'!K28>'Operative BP'!$P$22,IF('Dry Bulb'!K28<'Operative BP'!$P$23,J27,0),0)","v":0},{"$f":"IF('Dry Bulb'!L28>'Operative BP'!$P$22,IF('Dry Bulb'!L28<'Operative BP'!$P$23,K27,0),0)","v":0},{"$f":"IF('Dry Bulb'!M28>'Operative BP'!$P$22,IF('Dry Bulb'!M28<'Operative BP'!$P$23,L27,0),0)","v":309.17578500000076},{"$f":"IF('Dry Bulb'!N28>'Operative BP'!$P$22,IF('Dry Bulb'!N28<'Operative BP'!$P$23,M27,0),0)","v":-1027.3400099999997},{"$f":"IF('Dry Bulb'!O28>'Operative BP'!$P$22,IF('Dry Bulb'!O28<'Operative BP'!$P$23,N27,0),0)","v":0}]

{"sheet":"eq of time","index":14,"n_rows":33,"n_cols":14,"rows_kept":33,"cut":false,"hidden":true,"merged":[[13,1,13,3]]}
[]
[null,null,"2004-01-21","2004-02-21","2004-03-21","2004-04-21","2004-05-21","2004-06-21","2004-07-21","2004-08-21","2004-09-21","2004-10-21","2004-11-21","2004-12-21"]
[null,"Eq of time",-11.2,-13.9,-7.5,1.1000000000000001,3.3,-1.4,-6.2,-2.4,7.5,15.4,13.8,1.6]
[null,"Declination",-19.899999999999999,-10.6,0,11.9,20.3,23.45,20.5,12.1,0,-10.7,-19.899999999999999,-23.45]
[null,"Radians",{"$f":"RADIANS(C4)","v":-0.34732052114687156},-0.18500490071139894,0,0.20769418098732523,0.35430183815484889,0.40927970959267029,0.35779249665883756,0.21118483949131386,0,-0.18675022996339324,-0.34732052114687156,-0.40927970959267029]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Equation ofTime calc"]
[null,null,"Day ","equ Time"]
[null,null,21,{"$f":"(9.87*SIN(D19))-(7.53*COS(D18))-(1.5*SIN(D18))","v":-11.25573124913212}]
[]
[null,"B",{"$f":"(360*(C16-81))/365","v":-59.178082191780824},{"$f":"RADIANS(C18)","v":-1.0328523792623978}]
[null,"2B",{"$f":"C18*2","v":-118.35616438356165},{"$f":"RADIANS(C19)","v":-2.0657047585247956}]
[]
[null,null,null,null,"Day of the month","Day of the Year"]
[null,"Jan",31,0,21,{"$f":"SUM(D22:E22)","v":21}]
[null,"Feb",28,{"$f":"SUM(C22)","v":31},21,52]
[null,"Mar",31,{"$f":"SUM(C23:D23)","v":59},21,80]
[null,"Apr",30,90,21,111]
[null,"May",31,120,21,141]
[null,"Jun",30,151,21,172]
[null,"Jul",31,181,21,202]
[null,"Aug",31,212,21,233]
[null,"Sep",30,243,21,264]
[null,"Oct",31,273,21,294]
[null,"Nov",30,304,21,325]
[null,"Dec",31,334,21,355]

{"sheet":"Occupancy","index":15,"n_rows":27,"n_cols":27,"rows_kept":27,"cut":false,"hidden":true,"merged":[[1,0,1,12],[1,14,1,26]]}
[]
["Occupancy",null,null,null,null,null,null,null,null,null,null,null,null,null,"Equipment"]
["HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"HR","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[1,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,1,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[2,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,2,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[3,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,3,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[4,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,4,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[5,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,5,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[6,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,6,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[7,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,7,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[8,1,1,1,1,1,1,1,1,1,1,1,1,null,8,1,1,1,1,1,1,1,1,1,1,1,1]
[9,1,1,1,1,1,1,1,1,1,1,1,1,null,9,1,1,1,1,1,1,1,1,1,1,1,1]
[10,1,1,1,1,1,1,1,1,1,1,1,1,null,10,1,1,1,1,1,1,1,1,1,1,1,1]
[11,1,1,1,1,1,1,1,1,1,1,1,1,null,11,1,1,1,1,1,1,1,1,1,1,1,1]
[12,1,1,1,1,1,1,1,1,1,1,1,1,null,12,1,1,1,1,1,1,1,1,1,1,1,1]
[13,1,1,1,1,1,1,1,1,1,1,1,1,null,13,1,1,1,1,1,1,1,1,1,1,1,1]
[14,1,1,1,1,1,1,1,1,1,1,1,1,null,14,1,1,1,1,1,1,1,1,1,1,1,1]
[15,1,1,1,1,1,1,1,1,1,1,1,1,null,15,1,1,1,1,1,1,1,1,1,1,1,1]
[16,1,1,1,1,1,1,1,1,1,1,1,1,null,16,1,1,1,1,1,1,1,1,1,1,1,1]
[17,1,1,1,1,1,1,1,1,1,1,1,1,null,17,1,1,1,1,1,1,1,1,1,1,1,1]
[18,1,1,1,1,1,1,1,1,1,1,1,1,null,18,1,1,1,1,1,1,1,1,1,1,1,1]
[19,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,19,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[20,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,20,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[21,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,21,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[22,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,22,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[23,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,23,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]
[24,{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$48=\"y\",0,1)","v":1},null,24,{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1},{"$f":"IF('Input Data'!$H$46=\"y\",0,1)","v":1}]

{"sheet":"Profile calcs","index":16,"n_rows":54,"n_cols":70,"rows_kept":54,"cut":false,"hidden":true,"merged":[[1,43,1,55],[1,1,1,13],[1,15,1,27],[1,29,1,41]]}
[]
[null,"South Profile",null,null,null,null,null,null,null,null,null,null,null,null,null,"East Profile",null,null,null,null,null,null,null,null,null,null,null,null,null,"West Profile",null,null,null,null,null,null,null,null,null,null,null,null,null,"North Profile"]
[null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$f":"'Solar Altitude'!B3","v":0},{"$f":"'Solar Altitude'!C3","v":"Jan"},{"$f":"'Solar Altitude'!D3","v":"Feb"},{"$f":"'Solar Altitude'!E3","v":"Mar"},{"$f":"'Solar Altitude'!F3","v":"Apr"},{"$f":"'Solar Altitude'!G3","v":"May"},{"$f":"'Solar Altitude'!H3","v":"Jun"},{"$f":"'Solar Altitude'!I3","v":"Jul"},{"$f":"'Solar Altitude'!J3","v":"Aug"},{"$f":"'Solar Altitude'!K3","v":"Sep"},{"$f":"'Solar Altitude'!L3","v":"Oct"},{"$f":"'Solar Altitude'!M3","v":"Nov"},{"$f":"'Solar Altitude'!N3","v":"Dec"}]
[null,1,{"$f":"DEGREES(C31)","v":85.506692771390249},76.051491134901724,65.3,53.072313870844596,44.427911140068865,41.313454586896434,44.404551466519109,52.909735984441284,65.3,76.480736118519602,86.000045802283125,89.352163729921244,null,1,{"$f":"DEGREES(Q31)","v":-80.182065177734387},-80.140892672943934,-77.550222553105996,-73.652297950713162,-71.539168870383421,-72.457459123618534,-74.587173801009939,-74.673520776603795,-73.467983805952244,-72.789127866510924,-74.318586949653394,-77.526166860808985,null,1,{"$f":"DEGREES(AE31)","v":80.182065177734387},80.140892672943934,77.550222553106011,73.652297950713148,71.539168870383392,72.45745912361852,74.587173801009925,74.673520776603795,73.467983805952244,72.789127866510924,74.318586949653394,77.526166860808985,null,1,{"$f":"DEGREES(AS31)","v":-85.506692771390249},-76.051491134901724,-65.300000000000011,-53.072313870844596,-44.427911140068865,-41.313454586896434,-44.404551466519116,-52.909735984441276,-65.3,-76.480736118519602,-86.000045802283125,-89.352163729921244,null,{"$f":"'Solar Altitude'!B4","v":1},{"$f":"'Solar Altitude'!C4","v":-79.238745258454912},{"$f":"'Solar Altitude'!D4","v":-73.135890206899091},{"$f":"'Solar Altitude'!E4","v":-62.969753990761212},{"$f":"'Solar Altitude'!F4","v":-51.103815741194268},{"$f":"'Solar Altitude'!G4","v":-42.972420763986918},{"$f":"'Solar Altitude'!H4","v":-40.259838967181594},{"$f":"'Solar Altitude'!I4","v":-43.397326661656273},{"$f":"'Solar Altitude'!J4","v":-51.194813940312706},{"$f":"'Solar Altitude'!K4","v":-61.30334441705341},{"$f":"'Solar Altitude'!L4","v":-68.588756925018274},{"$f":"'Solar Altitude'!M4","v":-73.864057818332},{"$f":"'Solar Altitude'!N4","v":-77.510392918823513}]
[null,2,{"$f":"DEGREES(C32)","v":87.14026715835297},76.943421516331355,65.3,51.816577532022961,42.36628329809723,39.16397217391814,42.596177753639978,51.698849875501857,65.300000000000011,77.869647984236934,88.340906011691416,-88.404315155295123,null,2,{"$f":"DEGREES(Q32)","v":-66.172099329250003},-65.140511421698733,-61.409664244736128,-56.119428429528291,-52.806644981683412,-53.071524478923401,-55.607487949913953,-57.058845303129402,-57.468525117430296,-57.976591294307511,-60.410283592762973,-63.926268100735683,null,2,{"$f":"DEGREES(AE32)","v":66.172099329250003},65.140511421698719,61.409664244736142,56.119428429528277,52.806644981683391,53.071524478923379,55.607487949913931,57.058845303129395,57.468525117430296,57.976591294307511,60.410283592762973,63.926268100735683,null,2,{"$f":"DEGREES(AS32)","v":-87.14026715835297},-76.94342151633137,-65.300000000000011,-51.816577532022968,-42.36628329809723,-39.16397217391814,-42.596177753639978,-51.698849875501864,-65.3,-77.869647984236934,-88.340906011691416,88.404315155295109,null,{"$f":"'Solar Altitude'!B5","v":2},{"$f":"'Solar Altitude'!C5","v":-66.037221876299029},{"$f":"'Solar Altitude'!D5","v":-62.610262119735701},{"$f":"'Solar Altitude'!E5","v":-54.505603493104644},{"$f":"'Solar Altitude'!F5","v":-44.039138424385058},{"$f":"'Solar Altitude'!G5","v":-36.867903866984811},{"$f":"'Solar Altitude'!H5","v":-34.787290206430924},{"$f":"'Solar Altitude'!I5","v":-37.887883453111968},{"$f":"'Solar Altitude'!J5","v":-44.388788539159933},{"$f":"'Solar Altitude'!K5","v":-51.819137025254065},{"$f":"'Solar Altitude'!L5","v":-56.521775308526607},{"$f":"'Solar Altitude'!M5","v":-60.378308807607461},{"$f":"'Solar Altitude'!N5","v":-63.889653492857697}]
[null,3,{"$f":"DEGREES(C33)","v":-89.27056077739023},78.978814169951136,65.300000000000011,49.102677830512903,38.0697107147043,34.68168355761518,38.712119041692716,49.05817483751602,65.300000000000011,80.804155317269903,-86.888190980331871,-83.771615174618546,null,3,{"$f":"DEGREES(Q33)","v":-52.435166723015541},-50.544173289630855,-45.91935428010499,-39.682535750671363,-35.643149417229338,-35.46488164814032,-38.162804391158723,-40.534175714629342,-42.164171017516495,-43.623401532687339,-46.805449667898792,-50.572582527440368,null,3,{"$f":"DEGREES(AE33)","v":52.435166723015541},50.544173289630855,45.91935428010499,39.682535750671363,35.643149417229338,35.46488164814032,38.162804391158723,40.534175714629335,42.164171017516502,43.623401532687332,46.805449667898792,50.572582527440368,null,3,{"$f":"DEGREES(AS33)","v":89.27056077739023},-78.978814169951136,-65.300000000000011,-49.102677830512903,-38.069710714704293,-34.68168355761518,-38.712119041692716,-49.058174837516013,-65.300000000000011,-80.804155317269903,86.888190980331885,83.771615174618546,null,{"$f":"'Solar Altitude'!B6","v":3},{"$f":"'Solar Altitude'!C6","v":-52.431373562484438},{"$f":"'Solar Altitude'!D6","v":-49.776364898184575},{"$f":"'Solar Altitude'!E6","v":-43.00744408924087},{"$f":"'Solar Altitude'!F6","v":-33.970697614512481},{"$f":"'Solar Altitude'!G6","v":-27.874166624770901},{"$f":"'Solar Altitude'!H6","v":-26.397406240900974},{"$f":"'Solar Altitude'!I6","v":-29.298461575777225},{"$f":"'Solar Altitude'!J6","v":-34.480458721023354},{"$f":"'Solar Altitude'!K6","v":-39.89507498863518},{"$f":"'Solar Altitude'!L6","v":-43.286892300779471},{"$f":"'Solar Altitude'!M6","v":-46.757596903257479},{"$f":"'Solar Altitude'!N6","v":-50.32692672055552}]
[null,4,{"$f":"DEGREES(C34)","v":-82.17192424427256},83.262329332993176,65.300000000000011,43.339610901243866,29.580403720895195,26.101608463035426,31.06871667763788,43.484854535342002,65.300000000000011,87.267222857858812,-77.36591787164663,-74.90694041138012,null,4,{"$f":"DEGREES(Q34)","v":-39.010190181198872},-36.428743475161504,-31.171654482760939,-24.400458127908184,-20.038723532033892,-19.625868131864095,-22.32000203357995,-25.178501666912496,-27.591172995772343,-29.729656317315495,-33.493277499644961,-37.470732683841966,null,4,{"$f":"DEGREES(AE34)","v":39.010190181198872},36.428743475161504,31.171654482760939,24.400458127908184,20.038723532033892,19.625868131864095,22.320002033579943,25.178501666912496,27.591172995772343,29.729656317315495,33.493277499644961,37.470732683841966,null,4,{"$f":"DEGREES(AS34)","v":82.17192424427256},-83.262329332993176,-65.300000000000026,-43.339610901243866,-29.580403720895195,-26.101608463035426,-31.06871667763788,-43.484854535341988,-65.3,-87.267222857858798,77.365917871646644,74.906940411380106,null,{"$f":"'Solar Altitude'!B7","v":4},{"$f":"'Solar Altitude'!C7","v":-38.837571781392398},{"$f":"'Solar Altitude'!D7","v":-36.325136967893741},{"$f":"'Solar Altitude'!E7","v":-30.23387910899125},{"$f":"'Solar Altitude'!F7","v":-22.236891602714234},{"$f":"'Solar Altitude'!G7","v":-17.058579195686843},{"$f":"'Solar Altitude'!H7","v":-16.082853037589089},{"$f":"'Solar Altitude'!I7","v":-18.740224973134019},{"$f":"'Solar Altitude'!J7","v":-22.841111056638525},{"$f":"'Solar Altitude'!K7","v":-26.935985833021629},{"$f":"'Solar Altitude'!L7","v":-29.720493919992279},{"$f":"'Solar Altitude'!M7","v":-33.206986937806654},{"$f":"'Solar Altitude'!N7","v":-36.893522726896833}]
[null,5,{"$f":"DEGREES(C35)","v":-67.497147561415503},-86.309432298850382,65.300000000000011,28.738866865290532,11.921747515833621,9.482202464658485,15.373504841898113,29.638177006237576,65.300000000000011,-74.528119824042165,-57.19996124585586,-57.733947337338257,null,5,{"$f":"DEGREES(Q35)","v":-25.815859178831762},-22.717824490126432,-17.054801329090406,-10.060267103118708,-5.6553451463568249,-5.1651785422524581,-7.7705114298265903,-10.788309881886676,-13.597367832295642,-16.153367731431349,-20.343596801848918,-24.514554175011249,null,5,{"$f":"DEGREES(AE35)","v":25.815859178831762},22.717824490126432,17.054801329090406,10.060267103118706,5.6553451463568241,5.1651785422524581,7.7705114298265903,10.788309881886676,13.597367832295642,16.153367731431349,20.343596801848918,24.514554175011252,null,5,{"$f":"DEGREES(AS35)","v":67.497147561415517},86.309432298850368,-65.300000000000026,-28.738866865290543,-11.921747515833617,-9.4822024646584833,-15.373504841898106,-29.638177006237569,-65.30000000000004,74.528119824042179,57.199961245855874,57.733947337338272,null,{"$f":"'Solar Altitude'!B8","v":5},{"$f":"'Solar Altitude'!C8","v":-25.376333918471747},{"$f":"'Solar Altitude'!D8","v":-22.7103856061896},{"$f":"'Solar Altitude'!E8","v":-16.897092448538263},{"$f":"'Solar Altitude'!F8","v":-9.5810693067706811},{"$f":"'Solar Altitude'!G8","v":-5.1231262317655331},{"$f":"'Solar Altitude'!H8","v":-4.54535827775074},{"$f":"'Solar Altitude'!I8","v":-6.9688312964780383},{"$f":"'Solar Altitude'!J8","v":-10.241982624949756},{"$f":"'Solar Altitude'!K8","v":-13.517063375335365},{"$f":"'Solar Altitude'!L8","v":-16.104385171900024},{"$f":"'Solar Altitude'!M8","v":-19.830528453312528},{"$f":"'Solar Altitude'!N8","v":-23.664530366970006}]
[null,6,{"$f":"DEGREES(C36)","v":-37.148186571308401},-50.791383654081223,65.300000000000054,-17.580147546281751,-22.111172344820318,-19.795090464953187,-15.860431327653474,-13.722280285934321,65.300000000001162,-13.894791408071965,-20.106401019882362,-27.88546048481528,null,6,{"$f":"DEGREES(Q36)","v":-12.657580240548544},-9.2101030414712177,-3.3244141005449075,3.6714405326866673,7.9357874829851527,8.3930552361023523,5.9138516774857015,2.9679829754440079,8.3279928680461496E-2,-2.6465539816926205,-7.1190871836640657,-11.488991114943707,null,6,{"$f":"DEGREES(AE36)","v":12.657580240548544},9.2101030414712177,3.3244141005449075,-3.6714405326866673,-7.9357874829851545,-8.3930552361023505,-5.9138516774857015,-2.9679829754440075,-8.3279928680461496E-2,2.64655398169262,7.1190871836640657,11.488991114943707,null,6,{"$f":"DEGREES(AS36)","v":37.148186571308415},50.791383654081251,-65.299999999999955,17.58014754628174,22.111172344820307,19.79509046495318,15.860431327653469,13.722280285934318,-65.300000000005156,13.894791408071976,20.106401019882369,27.885460484815273,null,{"$f":"'Solar Altitude'!B9","v":6},{"$f":"'Solar Altitude'!C9","v":-12.151444093159176},{"$f":"'Solar Altitude'!D9","v":-9.1319080559186769},{"$f":"'Solar Altitude'!E9","v":-3.3232309033445411},{"$f":"'Solar Altitude'!F9","v":3.5985816694690373},{"$f":"'Solar Altitude'!G9","v":7.5112987220277185},{"$f":"'Solar Altitude'!H9","v":7.7738597839019823},{"$f":"'Solar Altitude'!I9","v":5.5584053941199079},{"$f":"'Solar Altitude'!J9","v":2.9033723023449274},{"$f":"'Solar Altitude'!K9","v":8.3279910069695443E-2},{"$f":"'Solar Altitude'!L9","v":-2.6015900354108483},{"$f":"'Solar Altitude'!M9","v":-6.7413522567651629},{"$f":"'Solar Altitude'!N9","v":-10.743396255327719}]
[null,7,{"$f":"DEGREES(C37)","v":1.8407058775768048},17.418156461309621,65.299999999999969,-72.609902347589838,-57.961158312930344,-51.874170400534652,-53.106981432720829,-70.235558391915404,65.3,32.525623758734746,13.689263813478037,3.7902225360911945,null,7,{"$f":"DEGREES(Q37)","v":0.75712395765969032},4.3819211908166711,10.327408658619172,17.146626992599682,21.134165658355119,21.477097073214686,19.142999224755304,16.444109273248728,13.765898970431955,11.107118463724456,6.5087495886135249,1.9226157929385757,null,7,{"$f":"DEGREES(AE37)","v":-0.75712395765969032},-4.3819211908166711,-10.327408658619172,-17.146626992599682,-21.134165658355119,-21.477097073214686,-19.142999224755304,-16.444109273248728,-13.765898970431955,-11.107118463724456,-6.5087495886135249,-1.9226157929385757,null,7,{"$f":"DEGREES(AS37)","v":-1.8407058775768053},-17.418156461309618,-65.300000000000011,72.609902347589809,57.96115831293033,51.874170400534645,53.106981432720829,70.235558391915376,-65.300000000000026,-32.525623758734753,-13.689263813478044,-3.7902225360911941,null,{"$f":"'Solar Altitude'!B10","v":7},{"$f":"'Solar Altitude'!C10","v":0.70023973357815916},{"$f":"'Solar Altitude'!D10","v":4.2572512510716702},{"$f":"'Solar Altitude'!E10","v":10.292097151668541},{"$f":"'Solar Altitude'!F10","v":17.071764306110264},{"$f":"'Solar Altitude'!G10","v":20.59199880999245},{"$f":"'Solar Altitude'!H10","v":20.602944398333847},{"$f":"'Solar Altitude'!I10","v":18.567526961418682},{"$f":"'Solar Altitude'!J10","v":16.357318748220177},{"$f":"'Solar Altitude'!K10","v":13.682588857300253},{"$f":"'Solar Altitude'!L10","v":10.626902061270702},{"$f":"'Solar Altitude'!M10","v":5.8987575020687171},{"$f":"'Solar Altitude'!N10","v":1.7151458456731048}]
[null,8,{"$f":"DEGREES(C38)","v":25.154979301423634},41.208162613283584,65.300000000000011,89.133910589679402,-77.392469719775818,-71.837796305169576,-74.903067121246494,-89.880701812612713,65.3,45.709102960920774,30.711991515210524,23.133349654536577,null,8,{"$f":"DEGREES(Q38)","v":14.801512993977905},18.395161326018542,24.21988645529855,30.680730702005945,34.26512345162336,34.426376431243654,32.256035415094608,29.958921059436694,27.765335603992927,25.454349023394592,20.939346821539349,16.129552534651118,null,8,{"$f":"DEGREES(AE38)","v":-14.801512993977905},-18.395161326018538,-24.21988645529855,-30.680730702005945,-34.26512345162336,-34.426376431243654,-32.256035415094608,-29.958921059436694,-27.765335603992927,-25.454349023394595,-20.939346821539349,-16.129552534651118,null,8,{"$f":"DEGREES(AS38)","v":-25.15497930142363},-41.208162613283591,-65.3,-89.133910589679402,77.392469719775818,71.837796305169562,74.90306712124648,89.880701812612699,-65.300000000000011,-45.709102960920774,-30.711991515210528,-23.133349654536577,null,{"$f":"'Solar Altitude'!B11","v":8},{"$f":"'Solar Altitude'!C11","v":12.968359542715392},{"$f":"'Solar Altitude'!D11","v":17.270303982095768},{"$f":"'Solar Altitude'!E11","v":23.773745192987032},{"$f":"'Solar Altitude'!F11","v":30.67971943621767},{"$f":"'Solar Altitude'!G11","v":33.959814353189685},{"$f":"'Solar Altitude'!H11","v":33.770494749028082},{"$f":"'Solar Altitude'!I11","v":31.887744015481577},{"$f":"'Solar Altitude'!J11","v":29.958903207045175},{"$f":"'Solar Altitude'!K11","v":27.097900221004789},{"$f":"'Solar Altitude'!L11","v":23.350930400204959},{"$f":"'Solar Altitude'!M11","v":17.832347455280527},{"$f":"'Solar Altitude'!N11","v":13.467847656409182}]
[null,9,{"$f":"DEGREES(C39)","v":36.123628972409719},48.984103271498903,65.3,82.323917470741151,-86.682219236973438,-82.177260396790928,-85.346370921243249,82.868918499232819,65.300000000000011,50.828908694033096,38.841664176975662,33.137728896941795,null,9,{"$f":"DEGREES(Q39)","v":29.897860503845664},33.171578582642681,38.635878844024361,44.516730121969097,47.561101053580373,47.480410935356453,45.501067907501131,43.760303315048105,42.346663637257642,40.715743852069998,36.595216615504739,31.603785496296783,null,9,{"$f":"DEGREES(AE39)","v":-29.897860503845664},-33.171578582642681,-38.635878844024361,-44.516730121969097,-47.561101053580373,-47.480410935356453,-45.501067907501131,-43.760303315048105,-42.346663637257642,-40.715743852069998,-36.595216615504739,-31.603785496296783,null,9,{"$f":"DEGREES(AS39)","v":-36.123628972409719},-48.984103271498903,-65.300000000000011,-82.323917470741165,86.682219236973438,82.177260396790942,85.346370921243249,-82.868918499232805,-65.3,-50.828908694033096,-38.841664176975669,-33.137728896941802,null,{"$f":"'Solar Altitude'!B12","v":9},{"$f":"'Solar Altitude'!C12","v":24.306538235547787},{"$f":"'Solar Altitude'!D12","v":29.607456719563572},{"$f":"'Solar Altitude'!E12","v":36.877998514340362},{"$f":"'Solar Altitude'!F12","v":44.267398869292073},{"$f":"'Solar Altitude'!G12","v":47.503865138538167},{"$f":"'Solar Altitude'!H12","v":47.16345799134892},{"$f":"'Solar Altitude'!I12","v":45.403126432581416},{"$f":"'Solar Altitude'!J12","v":43.556385601632783},{"$f":"'Solar Altitude'!K12","v":40.048756889246128},{"$f":"'Solar Altitude'!L12","v":35.170537312656599},{"$f":"'Solar Altitude'!M12","v":28.628753160625717},{"$f":"'Solar Altitude'!N12","v":24.120985503613159}]
[null,10,{"$f":"DEGREES(C40)","v":41.565533524141749},52.391449411165148,65.3,79.183835184665355,88.633552185609801,-87.576455047188773,89.408737808154712,79.54425546635963,65.3,53.228063715971984,42.944409695388977,38.364397938009645,null,10,{"$f":"DEGREES(Q40)","v":46.432009669114628},48.982108380980456,53.761437623792659,58.790214649196741,61.14667544282198,60.771492120895445,59.020595594487986,57.990814089298965,57.660184602658042,57.085561042213271,53.797693072162787,48.774894172678039,null,10,{"$f":"DEGREES(AE40)","v":-46.432009669114628},-48.98210838098047,-53.761437623792659,-58.790214649196756,-61.14667544282198,-60.771492120895445,-59.020595594487986,-57.990814089298965,-57.660184602658042,-57.085561042213271,-53.797693072162787,-48.774894172678053,null,10,{"$f":"DEGREES(AS40)","v":-41.565533524141735},-52.391449411165141,-65.300000000000011,-79.183835184665355,-88.633552185609801,87.576455047188773,-89.408737808154712,-79.54425546635963,-65.3,-53.228063715971977,-42.944409695388977,-38.364397938009652,null,{"$f":"'Solar Altitude'!B13","v":10},{"$f":"'Solar Altitude'!C13","v":34.130498638110296},{"$f":"'Solar Altitude'!D13","v":40.716949463115029},{"$f":"'Solar Altitude'!E13","v":49.130640449349286},{"$f":"'Solar Altitude'!F13","v":57.573642107854539},{"$f":"'Solar Altitude'!G13","v":61.123995517612983},{"$f":"'Solar Altitude'!H13","v":60.701791836412639},{"$f":"'Solar Altitude'!I13","v":59.016860616830343},{"$f":"'Solar Altitude'!J13","v":56.905164678924855},{"$f":"'Solar Altitude'!K13","v":51.954064465377563},{"$f":"'Solar Altitude'!L13","v":45.326184070335216},{"$f":"'Solar Altitude'!M13","v":37.566870997040184},{"$f":"'Solar Altitude'!N13","v":33.04159126014769}]
[null,11,{"$f":"DEGREES(C41)","v":44.282217904128672},54.018451059115115,65.300000000000011,77.69612062717222,86.343646743656691,89.714212091310287,86.798330968762983,77.960826272965903,65.300000000000011,54.328164209664372,44.893647845797645,40.97067975660989,null,11,{"$f":"DEGREES(Q41)","v":64.562443951008888},65.901314539685401,69.61109114186894,73.497168133288227,75.027677809677201,74.319781349482838,72.839713407261911,72.655436766674285,73.666960034724283,74.489845422408862,72.52990498677552,67.776371428052769,null,11,{"$f":"DEGREES(AE41)","v":-64.562443951008902},-65.901314539685401,-69.61109114186894,-73.497168133288227,-75.027677809677201,-74.319781349482838,-72.839713407261911,-72.655436766674285,-73.666960034724269,-74.489845422408848,-72.529904986775534,-67.776371428052769,null,11,{"$f":"DEGREES(AS41)","v":-44.282217904128672},-54.018451059115115,-65.300000000000011,-77.69612062717222,-86.343646743656691,-89.714212091310301,-86.798330968762997,-77.960826272965903,-65.300000000000011,-54.328164209664372,-44.893647845797645,-40.97067975660989,null,{"$f":"'Solar Altitude'!B14","v":11},{"$f":"'Solar Altitude'!C14","v":41.499338482119107},{"$f":"'Solar Altitude'!D14","v":49.543356395157261},{"$f":"'Solar Altitude'!E14","v":59.402009530792824},{"$f":"'Solar Altitude'!F14","v":69.801829865076741},{"$f":"'Solar Altitude'!G14","v":74.625870049112294},{"$f":"'Solar Altitude'!H14","v":74.317427946135254},{"$f":"'Solar Altitude'!I14","v":72.577202871970812},{"$f":"'Solar Altitude'!J14","v":69.283885987295108},{"$f":"'Solar Altitude'!K14","v":61.393251168859464},{"$f":"'Solar Altitude'!L14","v":52.417946997507137},{"$f":"'Solar Altitude'!M14","v":43.550952586854685},{"$f":"'Solar Altitude'!N14","v":39.297011346471983}]
[null,12,{"$f":"DEGREES(C42)","v":45.341192522261665},54.65622400407787,65.300000000000011,77.204007036944958,85.602608099870324,88.764506326073786,85.831844934745362,77.410166839433359,65.3,54.593196533889113,45.392239295822165,41.843902161818413,null,12,{"$f":"DEGREES(Q42)","v":83.953055253243946},83.672477687445479,85.9744082667399,88.486518830478445,89.098541577633242,88.042480487312574,86.869712514125027,87.612299057311645,89.899102008780474,87.509028766495277,87.799307231125709,88.09804255680524,null,12,{"$f":"DEGREES(AE42)","v":-83.95305525324396},-83.672477687445479,-85.9744082667399,-88.486518830478445,-89.098541577633242,-88.042480487312574,-86.869712514125027,-87.612299057311645,-89.899102008780474,-87.509028766495277,-87.799307231125709,-88.098042556805254,null,12,{"$f":"DEGREES(AS42)","v":-45.341192522261665},-54.65622400407787,-65.300000000000011,-77.204007036944958,-85.602608099870324,-88.764506326073786,-85.831844934745362,-77.410166839433359,-65.3,-54.593196533889113,-45.392239295822165,-41.843902161818413,null,{"$f":"'Solar Altitude'!B15","v":12},{"$f":"'Solar Altitude'!C15","v":45.177523796213436},{"$f":"'Solar Altitude'!D15","v":54.329068465075267},{"$f":"'Solar Altitude'!E15","v":65.047371814417531},{"$f":"'Solar Altitude'!F15","v":77.120581963762746},{"$f":"'Solar Altitude'!G15","v":85.511869047796154},{"$f":"'Solar Altitude'!H15","v":87.685706703910299},{"$f":"'Solar Altitude'!I15","v":84.793912346691229},{"$f":"'Solar Altitude'!J15","v":77.199736149013034},{"$f":"'Solar Altitude'!K15","v":65.299840573859427},{"$f":"'Solar Altitude'!L15","v":54.542607240756659},{"$f":"'Solar Altitude'!M15","v":45.370517861678998},{"$f":"'Solar Altitude'!N15","v":41.831318434437598}]
[null,13,{"$f":"DEGREES(C43)","v":45.093307228609767},54.548508865098285,65.300000000000011,77.527686129155398,86.172088859931137,89.286545413103582,86.195448533480899,77.690264015558725,65.300000000000011,54.1192638814804,44.599954197716883,41.247836270078757,null,13,{"$f":"DEGREES(Q43)","v":-76.310236007231211},-78.301959925225134,-77.550222553106039,-76.496177068295182,-76.818295906325048,-78.211108618523411,-79.058019787475942,-77.387091031608094,-73.467983805952144,-69.609222192948593,-68.255417985347776,-71.453363412613228,null,13,{"$f":"DEGREES(AE43)","v":76.310236007231225},78.301959925225134,77.550222553106053,76.496177068295182,76.818295906325034,78.211108618523411,79.058019787475942,77.387091031608094,73.467983805952144,69.609222192948593,68.255417985347762,71.453363412613214,null,13,{"$f":"DEGREES(AS43)","v":-45.093307228609767},-54.548508865098285,-65.300000000000011,-77.527686129155384,-86.172088859931137,-89.286545413103582,-86.195448533480899,-77.690264015558725,-65.300000000000011,-54.1192638814804,-44.599954197716883,-41.247836270078757,null,{"$f":"'Solar Altitude'!B16","v":13},{"$f":"'Solar Altitude'!C16","v":44.262516808487675},{"$f":"'Solar Altitude'!D16","v":53.442649547558034},{"$f":"'Solar Altitude'!E16","v":62.96975399076122},{"$f":"'Solar Altitude'!F16","v":71.918657174425832},{"$f":"'Solar Altitude'!G16","v":76.310429689037434},{"$f":"'Solar Altitude'!H16","v":78.190731192893594},{"$f":"'Solar Altitude'!I16","v":78.445286814888803},{"$f":"'Solar Altitude'!J16","v":72.64341275146262},{"$f":"'Solar Altitude'!K16","v":61.303344417053367},{"$f":"'Solar Altitude'!L16","v":50.879096974273239},{"$f":"'Solar Altitude'!M16","v":42.542599664242438},{"$f":"'Solar Altitude'!N16","v":40.072467904514703}]
[null,14,{"$f":"DEGREES(C44)","v":43.459732841647039},53.656578483668653,65.3,78.783422467977019,88.233716701902779,-88.563972173918131,88.003822246360016,78.90115012449813,65.3,52.730352015763074,42.259093988308607,39.004315155295124,null,14,{"$f":"DEGREES(Q44)","v":-57.32973993752023},-60.7360775958551,-61.409664244736106,-61.715956668379413,-62.905108672619058,-64.600922398571711,-65.128294922488053,-62.607791450328726,-57.468525117430246,-52.462028938168871,-49.834295771439308,-52.146583450749397,null,14,{"$f":"DEGREES(AE44)","v":57.329739937520216},60.7360775958551,61.409664244736106,61.715956668379413,62.905108672619058,64.600922398571711,65.128294922488053,62.607791450328726,57.468525117430246,52.462028938168871,49.834295771439308,52.146583450749397,null,14,{"$f":"DEGREES(AS44)","v":-43.459732841647046},-53.656578483668653,-65.3,-78.783422467977033,-88.233716701902779,88.563972173918145,-88.003822246360016,-78.901150124498145,-65.300000000000011,-52.730352015763074,-42.259093988308607,-39.004315155295124,null,{"$f":"'Solar Altitude'!B17","v":14},{"$f":"'Solar Altitude'!C17","v":39.001643714284292},{"$f":"'Solar Altitude'!D17","v":47.236569251778789},{"$f":"'Solar Altitude'!E17","v":54.505603493104616},{"$f":"'Solar Altitude'!F17","v":60.167275430762508},{"$f":"'Solar Altitude'!G17","v":62.862961225627508},{"$f":"'Solar Altitude'!H17","v":64.570010808670432},{"$f":"'Solar Altitude'!I17","v":65.066621957768987},{"$f":"'Solar Altitude'!J17","v":61.010544197086858},{"$f":"'Solar Altitude'!K17","v":51.819137025254037},{"$f":"'Solar Altitude'!L17","v":42.759898297268641},{"$f":"'Solar Altitude'!M17","v":35.791762146841563},{"$f":"'Solar Altitude'!N17","v":34.427909280399348}]
[null,15,{"$f":"DEGREES(C45)","v":39.870560777390224},51.621185830048873,65.300000000000011,81.497322169487106,-87.46971071470432,-84.081683557615165,-88.112119041692736,81.541825162483974,65.3,49.795844682730099,37.488190980331879,34.371615174618547,null,15,{"$f":"DEGREES(Q45)","v":-39.812986834028628},-44.138369778725995,-45.919354280104955,-47.350089337983867,-49.279589339957219,-51.233884049672319,-51.471577651808317,-48.232694478544275,-42.164171017516459,-36.404340467875535,-32.990491768082641,-34.633273198345073,null,15,{"$f":"DEGREES(AE45)","v":39.812986834028628},44.138369778725988,45.919354280104962,47.350089337983867,49.279589339957219,51.233884049672319,51.471577651808317,48.232694478544275,42.164171017516459,36.404340467875528,32.990491768082641,34.633273198345066,null,15,{"$f":"DEGREES(AS45)","v":-39.870560777390232},-51.621185830048873,-65.300000000000011,-81.497322169487106,87.46971071470432,84.081683557615165,88.112119041692722,-81.541825162483974,-65.300000000000011,-49.795844682730106,-37.488190980331893,-34.371615174618547,null,{"$f":"'Solar Altitude'!B18","v":15},{"$f":"'Solar Altitude'!C18","v":30.541133571003865},{"$f":"'Solar Altitude'!D18","v":37.574701882546435},{"$f":"'Solar Altitude'!E18","v":43.007444089240849},{"$f":"'Solar Altitude'!F18","v":46.978750874484376},{"$f":"'Solar Altitude'!G18","v":49.242301300948341},{"$f":"'Solar Altitude'!H18","v":51.002542825705397},{"$f":"'Solar Altitude'!I18","v":51.447673176445399},{"$f":"'Solar Altitude'!J18","v":47.843171633901541},{"$f":"'Solar Altitude'!K18","v":39.895074988635152},{"$f":"'Solar Altitude'!L18","v":32.038156511029932},{"$f":"'Solar Altitude'!M18","v":26.359057025099464},{"$f":"'Solar Altitude'!N18","v":25.920295493187655}]
[null,16,{"$f":"DEGREES(C46)","v":32.771924244272569},47.337670667006847,65.3,87.260389098756136,-78.980403720895211,-75.501608463035367,-80.468716677637914,87.115145464657985,65.300000000000011,43.332777142141182,27.965917871646649,25.506940411380103,null,16,{"$f":"DEGREES(Q46)","v":-23.875002480593199},-28.656528802721059,-31.171654482760921,-33.432906045521179,-35.951128585501792,-38.121029600348642,-38.115343474138719,-34.304400656996243,-27.591172995772371,-21.421982311981434,-17.641166819660786,-18.874041457280981,null,16,{"$f":"DEGREES(AE46)","v":23.875002480593196},28.656528802721059,31.171654482760921,33.432906045521179,35.951128585501792,38.121029600348642,38.115343474138719,34.304400656996243,27.591172995772371,21.421982311981434,17.641166819660786,18.874041457280981,null,16,{"$f":"DEGREES(AS46)","v":-32.771924244272576},-47.337670667006861,-65.3,-87.26038909875615,78.980403720895197,75.501608463035367,80.468716677637929,-87.115145464657999,-65.300000000000011,-43.332777142141182,-27.965917871646653,-25.506940411380103,null,{"$f":"'Solar Altitude'!B19","v":16},{"$f":"'Solar Altitude'!C19","v":20.038281727598083},{"$f":"'Solar Altitude'!D19","v":26.016647471873153},{"$f":"'Solar Altitude'!E19","v":30.233879108991232},{"$f":"'Solar Altitude'!F19","v":33.419767540103443},{"$f":"'Solar Altitude'!G19","v":35.682648220686666},{"$f":"'Solar Altitude'!H19","v":37.56104623172925},{"$f":"'Solar Altitude'!I19","v":37.876258416390314},{"$f":"'Solar Altitude'!J19","v":34.288646107643089},{"$f":"'Solar Altitude'!K19","v":26.935985833021654},{"$f":"'Solar Altitude'!L19","v":19.913519068774189},{"$f":"'Solar Altitude'!M19","v":15.259931573481456},{"$f":"'Solar Altitude'!N19","v":15.530455637101428}]
[null,17,{"$f":"DEGREES(C47)","v":18.097147561415554},36.90943229885039,65.299999999999983,-78.138866865290538,-61.321747515833643,-58.88220246465854,-64.773504841898102,-79.038177006237561,65.3,25.128119824042169,7.7999612458558687,8.333947337338298,null,17,{"$f":"DEGREES(Q47)","v":-9.2385105897919768},-14.141799097654047,-17.05480132909042,-19.854676249106344,-22.809925103490791,-25.161800037123335,-24.96833403497148,-20.721091695019808,-13.597367832295648,-7.2728027816997747,-3.4258822939894862,-4.469701583642955,null,17,{"$f":"DEGREES(AE47)","v":9.2385105897919768},14.141799097654047,17.054801329090424,19.854676249106344,22.809925103490791,25.161800037123339,24.96833403497148,20.721091695019812,13.597367832295648,7.2728027816997747,3.4258822939894862,4.469701583642955,null,17,{"$f":"DEGREES(AS47)","v":-18.097147561415564},-36.909432298850398,-65.300000000000011,78.138866865290566,61.321747515833657,58.882202464658548,64.773504841898102,79.038177006237575,-65.299999999999983,-25.128119824042177,-7.7999612458558714,-8.3339473373382997,null,{"$f":"'Solar Altitude'!B20","v":17},{"$f":"'Solar Altitude'!C20","v":8.2848854255444504},{"$f":"'Solar Altitude'!D20","v":13.434807821200849},{"$f":"'Solar Altitude'!E20","v":16.897092448538277},{"$f":"'Solar Altitude'!F20","v":19.80224832363653},{"$f":"'Solar Altitude'!G20","v":22.286756355186323},{"$f":"'Solar Altitude'!H20","v":24.319689951925163},{"$f":"'Solar Altitude'!I20","v":24.456964963286701},{"$f":"'Solar Altitude'!J20","v":20.670382142796534},{"$f":"'Solar Altitude'!K20","v":13.51706337533537},{"$f":"'Solar Altitude'!L20","v":7.0202572324504446},{"$f":"'Solar Altitude'!M20","v":3.1397975005302774},{"$f":"'Solar Altitude'!N20","v":3.9451572875932328}]
[null,18,{"$f":"DEGREES(C48)","v":-12.251813428691667},1.391383654081259,65.299999999999883,-31.81985245371823,-27.288827655179645,-29.604909535046897,-33.539568672346476,-35.677719714065731,65.300000000005312,-35.505208591928351,-29.293598980117586,-21.514539515184669,null,18,{"$f":"DEGREES(Q48)","v":4.5124409084911488},-0.2911309486956099,-3.324414100544868,-6.3911335111384062,-9.6364921571497923,-12.146410157593207,-11.827587615885065,-7.2645164628018666,8.3279928680489793E-2,6.378749450365131,10.079870372411358,9.055310015770992,null,18,{"$f":"DEGREES(AE48)","v":-4.5124409084911488},0.2911309486956099,3.324414100544868,6.3911335111384062,9.6364921571497923,12.146410157593207,11.827587615885063,7.2645164628018666,-8.3279928680489793E-2,-6.3787494503651301,-10.079870372411357,-9.055310015770992,null,18,{"$f":"DEGREES(AS48)","v":12.251813428691671},-1.3913836540812599,-65.299999999999983,31.819852453718237,27.288827655179634,29.60490953504689,33.539568672346483,35.677719714065745,-65.300000000001333,35.505208591928337,29.293598980117594,21.514539515184662,null,{"$f":"'Solar Altitude'!B21","v":18},{"$f":"'Solar Altitude'!C21","v":-4.242067037456934},{"$f":"'Solar Altitude'!D21","v":0.28496224246637836},{"$f":"'Solar Altitude'!E21","v":3.3232309033445016},{"$f":"'Solar Altitude'!F21","v":6.2903017477886056},{"$f":"'Solar Altitude'!G21","v":9.1618728727979484},{"$f":"'Solar Altitude'!H21","v":11.380032986011807},{"$f":"'Solar Altitude'!I21","v":11.292623329902437},{"$f":"'Solar Altitude'!J21","v":7.1538265372891177},{"$f":"'Solar Altitude'!K21","v":-8.3279910069723753E-2},{"$f":"'Solar Altitude'!L21","v":-6.3024734223343577},{"$f":"'Solar Altitude'!M21","v":-9.6180467382750852},{"$f":"'Solar Altitude'!N21","v":-8.4049479592926772}]
[null,19,{"$f":"DEGREES(C49)","v":-51.240705877576872},-66.818156461309627,65.300000000000011,23.209902347589786,8.5611583129303881,2.4741704005345873,3.7069814327208346,20.835558391915374,65.300000000000011,-81.925623758734844,-63.089263813477999,-53.190222536091191,null,19,{"$f":"DEGREES(Q49)","v":17.787083138469381},13.241926751478145,10.3274086586192,7.2612910314068415,3.8834912247576012,1.2368871636337018,1.6074102522073654,6.3652304276825138,13.765898970431998,19.875382193162707,23.262321940359538,22.125354369783608,null,19,{"$f":"DEGREES(AE49)","v":-17.787083138469381},-13.241926751478145,-10.3274086586192,-7.2612910314068433,-3.8834912247576012,-1.2368871636337018,-1.6074102522073654,-6.3652304276825138,-13.765898970431998,-19.875382193162707,-23.262321940359538,-22.125354369783608,null,19,{"$f":"DEGREES(AS49)","v":51.240705877576879},66.818156461309655,-65.299999999999969,-23.209902347589793,-8.5611583129303863,-2.4741704005345868,-3.7069814327208337,-20.835558391915377,-65.299999999999983,81.925623758734872,63.089263813477984,53.190222536091184,null,{"$f":"'Solar Altitude'!B22","v":19},{"$f":"'Solar Altitude'!C22","v":-17.258784755357599},{"$f":"'Solar Altitude'!D22","v":-13.177535073458104},{"$f":"'Solar Altitude'!E22","v":-10.292097151668569},{"$f":"'Solar Altitude'!F22","v":-6.9635212465343193},{"$f":"'Solar Altitude'!G22","v":-3.5411252469823715},{"$f":"'Solar Altitude'!H22","v":-1.1064784283971907},{"$f":"'Solar Altitude'!I22","v":-1.4750612815819091},{"$f":"'Solar Altitude'!J22","v":-6.1102162570653853},{"$f":"'Solar Altitude'!K22","v":-13.682588857300294},{"$f":"'Solar Altitude'!L22","v":-19.851334869589788},{"$f":"'Solar Altitude'!M22","v":-22.782734775346487},{"$f":"'Solar Altitude'!N22","v":-21.2544074674176}]
[null,20,{"$f":"DEGREES(C50)","v":-74.554979301423643},89.391837386716404,65.300000000000011,41.466089410320606,27.99246971977583,22.437796305169524,25.503067121246531,40.480701812612722,65.300000000000011,84.890897039079221,-80.111991515210519,-72.533349654536536,null,20,{"$f":"DEGREES(Q50)","v":30.929660168946619},26.783441749367146,24.219886455298596,21.450631303008365,18.141617234558208,15.393131364902054,15.718705218374629,20.515426310682393,27.765335603992941,33.518173513343072,36.431124914543311,35.075043189143301,null,20,{"$f":"DEGREES(AE50)","v":-30.929660168946619},-26.783441749367146,-24.219886455298596,-21.450631303008365,-18.141617234558211,-15.393131364902047,-15.718705218374629,-20.515426310682397,-27.765335603992941,-33.518173513343072,-36.431124914543311,-35.075043189143301,null,20,{"$f":"DEGREES(AS50)","v":74.554979301423629},-89.391837386716418,-65.3,-41.466089410320599,-27.992469719775826,-22.437796305169524,-25.503067121246527,-40.480701812612715,-65.3,-84.890897039079206,80.111991515210534,72.533349654536536,null,{"$f":"'Solar Altitude'!B23","v":20},{"$f":"'Solar Altitude'!C23","v":-30.589239677830651},{"$f":"'Solar Altitude'!D23","v":-26.783110901661868},{"$f":"'Solar Altitude'!E23","v":-23.773745192987072},{"$f":"'Solar Altitude'!F23","v":-19.749387170381588},{"$f":"'Solar Altitude'!G23","v":-15.584861719885295},{"$f":"'Solar Altitude'!H23","v":-12.902247652391463},{"$f":"'Solar Altitude'!I23","v":-13.625605199002544},{"$f":"'Solar Altitude'!J23","v":-18.916708643772196},{"$f":"'Solar Altitude'!K23","v":-27.097900221004799},{"$f":"'Solar Altitude'!L23","v":-33.472019280706604},{"$f":"'Solar Altitude'!M23","v":-36.206670576844481},{"$f":"'Solar Altitude'!N23","v":-34.435555539572299}]
[null,21,{"$f":"DEGREES(C51)","v":-85.523628972409725},81.615896728501113,65.300000000000011,48.276082529258858,37.282219236973447,32.777260396790922,35.946370921243286,47.731081500767182,65.3,79.771091305966891,-88.241664176975647,-82.5377288969418,null,21,{"$f":"DEGREES(Q51)","v":44.196478266846057},40.599089566496509,38.635878844024383,36.520338007765019,33.567457399080453,30.792711025689055,30.936867265726114,35.533344323926315,42.346663637257642,47.52980172868061,49.801160168555157,48.138711526458181,null,21,{"$f":"DEGREES(AE51)","v":-44.196478266846057},-40.599089566496509,-38.635878844024383,-36.520338007765027,-33.567457399080453,-30.792711025689055,-30.936867265726114,-35.533344323926308,-42.346663637257642,-47.52980172868061,-49.801160168555157,-48.138711526458181,null,21,{"$f":"DEGREES(AS51)","v":85.523628972409725},-81.615896728501099,-65.3,-48.276082529258844,-37.282219236973447,-32.777260396790929,-35.946370921243279,-47.731081500767182,-65.300000000000011,-79.771091305966891,88.241664176975661,82.537728896941786,null,{"$f":"'Solar Altitude'!B24","v":21},{"$f":"'Solar Altitude'!C24","v":-44.11375465474292},{"$f":"'Solar Altitude'!D24","v":-40.375142281624065},{"$f":"'Solar Altitude'!E24","v":-36.877998514340369},{"$f":"'Solar Altitude'!F24","v":-31.713766855869693},{"$f":"'Solar Altitude'!G24","v":-26.575515215416551},{"$f":"'Solar Altitude'!H24","v":-23.623016903493113},{"$f":"'Solar Altitude'!I24","v":-24.79570873532365},{"$f":"'Solar Altitude'!J24","v":-30.92280247893752},{"$f":"'Solar Altitude'!K24","v":-40.048756889246128},{"$f":"'Solar Altitude'!L24","v":-46.985407153208357},{"$f":"'Solar Altitude'!M24","v":-49.782532508401836},{"$f":"'Solar Altitude'!N24","v":-47.837496220337762}]
[null,22,{"$f":"DEGREES(C52)","v":89.034466475858267},78.208550588834868,65.300000000000011,51.41616481533466,41.966447814390222,38.176455047188753,41.191262191845297,51.055744533640386,65.3,77.37193628402801,87.655590304611039,-87.764397938009651,null,22,{"$f":"DEGREES(Q52)","v":57.739752741902734},54.856879804295147,53.761437623792695,52.718628788708926,50.521398141456501,47.871905572894399,47.648515276704565,51.678377748209421,57.660184602658042,62.016242169118094,63.476783571899695,61.443103356413083,null,22,{"$f":"DEGREES(AE52)","v":-57.739752741902734},-54.856879804295147,-53.761437623792688,-52.718628788708926,-50.521398141456487,-47.871905572894391,-47.648515276704565,-51.678377748209428,-57.660184602658042,-62.016242169118094,-63.476783571899695,-61.443103356413083,null,22,{"$f":"DEGREES(AS52)","v":-89.034466475858252},-78.208550588834868,-65.300000000000011,-51.41616481533466,-41.966447814390222,-38.17645504718876,-41.191262191845297,-51.055744533640386,-65.3,-77.37193628402801,-87.655590304611039,87.764397938009637,null,{"$f":"'Solar Altitude'!B25","v":22},{"$f":"'Solar Altitude'!C25","v":-57.730536859646747},{"$f":"'Solar Altitude'!D25","v":-53.7124665497957},{"$f":"'Solar Altitude'!E25","v":-49.130640449349315},{"$f":"'Solar Altitude'!F25","v":-42.202232941267965},{"$f":"'Solar Altitude'!G25","v":-35.853933091501311},{"$f":"'Solar Altitude'!H25","v":-32.649969945256942},{"$f":"'Solar Altitude'!I25","v":-34.377195915482893},{"$f":"'Solar Altitude'!J25","v":-41.497131280000914},{"$f":"'Solar Altitude'!K25","v":-51.954064465377563},{"$f":"'Solar Altitude'!L25","v":-60.030194510304511},{"$f":"'Solar Altitude'!M25","v":-63.399939655490947},{"$f":"'Solar Altitude'!N25","v":-61.381330079855132}]
[null,23,{"$f":"DEGREES(C53)","v":86.317782095871337},76.581548940884886,65.300000000000011,52.903879372827781,44.256353256343338,40.885787908689707,43.801669031237033,52.639173727034112,65.300000000000011,76.271835790335643,85.706352154202364,89.629320243390126,null,23,{"$f":"DEGREES(Q53)","v":71.593874807745053},69.589194473644923,69.61109114186894,70.053891850109665,69.071591312252522,66.787471568061861,65.990399025379261,68.97846377500592,73.666960034724326,76.934368103437876,77.442055417846433,75.002834283541929,null,23,{"$f":"DEGREES(AE53)","v":-71.593874807745053},-69.589194473644923,-69.61109114186894,-70.053891850109679,-69.071591312252522,-66.787471568061889,-65.990399025379276,-68.978463775005906,-73.666960034724326,-76.93436810343789,-77.442055417846433,-75.002834283541929,null,23,{"$f":"DEGREES(AS53)","v":-86.317782095871323},-76.581548940884886,-65.300000000000011,-52.903879372827781,-44.256353256343338,-40.885787908689707,-43.801669031237026,-52.639173727034112,-65.300000000000011,-76.271835790335643,-85.706352154202364,-89.629320243390126,null,{"$f":"'Solar Altitude'!B26","v":23},{"$f":"'Solar Altitude'!C26","v":-71.276413671366612},{"$f":"'Solar Altitude'!D26","v":-66.153465993410151},{"$f":"'Solar Altitude'!E26","v":-59.402009530792824},{"$f":"'Solar Altitude'!F26","v":-50.011386554405469},{"$f":"'Solar Altitude'!G26","v":-42.39742803240717},{"$f":"'Solar Altitude'!H26","v":-39.064492418979341},{"$f":"'Solar Altitude'!I26","v":-41.409864595350896},{"$f":"'Solar Altitude'!J26","v":-49.478233796277678},{"$f":"'Solar Altitude'!K26","v":-61.393251168859493},{"$f":"'Solar Altitude'!L26","v":-71.378499679687209},{"$f":"'Solar Altitude'!M26","v":-76.771747562226409},{"$f":"'Solar Altitude'!N26","v":-74.998658692112272}]
[null,24,{"$f":"DEGREES(C54)","v":85.258807477738344},75.943775995922138,65.3,53.395992963055065,44.997391900129685,41.835493673926223,44.768155065254646,53.189833160566664,65.3,76.006803466110895,85.207760704177844,88.756097838181603,null,24,{"$f":"DEGREES(Q54)","v":85.676140318453747},84.673020487038187,85.974408266739928,88.161715299139843,88.728943923930075,87.067266457680972,85.571264313099348,87.09022999649082,89.899102008781256,87.907230778803338,88.427383905065867,88.730639842766692,null,24,{"$f":"DEGREES(AE54)","v":-85.676140318453747},-84.673020487038187,-85.974408266739914,-88.161715299139871,-88.728943923930075,-87.067266457680958,-85.571264313099363,-87.09022999649082,-89.899102008781256,-87.907230778803338,-88.427383905065867,-88.730639842766692,null,24,{"$f":"DEGREES(AS54)","v":-85.258807477738344},-75.943775995922138,-65.3,-53.395992963055065,-44.997391900129685,-41.835493673926223,-44.768155065254646,-53.189833160566664,-65.3,-76.006803466110895,-85.207760704177844,-88.756097838181603,null,{"$f":"'Solar Altitude'!B27","v":24},{"$f":"'Solar Altitude'!C27","v":-83.596484892158756},{"$f":"'Solar Altitude'!D27","v":-75.041691580826409},{"$f":"'Solar Altitude'!E27","v":-65.047371814417531},{"$f":"'Solar Altitude'!F27","v":-53.370409687127484},{"$f":"'Solar Altitude'!G27","v":-44.990343292174892},{"$f":"'Solar Altitude'!H27","v":-41.805581832384377},{"$f":"'Solar Altitude'!I27","v":-44.683864079458822},{"$f":"'Solar Altitude'!J27","v":-53.126563822663151},{"$f":"'Solar Altitude'!K27","v":-65.299840573859427},{"$f":"'Solar Altitude'!L27","v":-75.863131931954825},{"$f":"'Solar Altitude'!M27","v":-84.958601709687045},{"$f":"'Solar Altitude'!N27","v":-88.223048770244205}]
[]
[]
[null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"ATAN(TAN('Solar Altitude'!C31)/COS('Surface Solar Azimuth Angles'!C30))","v":1.492373321351995},{"$f":"ATAN(TAN('Solar Altitude'!D31)/COS('Surface Solar Azimuth Angles'!D30))","v":1.327348921355314},{"$f":"ATAN(TAN('Solar Altitude'!E31)/COS('Surface Solar Azimuth Angles'!E30))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F31)/COS('Surface Solar Azimuth Angles'!F30))","v":0.92628661869809481},{"$f":"ATAN(TAN('Solar Altitude'!G31)/COS('Surface Solar Azimuth Angles'!G30))","v":0.77541332917766925},{"$f":"ATAN(TAN('Solar Altitude'!H31)/COS('Surface Solar Azimuth Angles'!H30))","v":0.72105580791449653},{"$f":"ATAN(TAN('Solar Altitude'!I31)/COS('Surface Solar Azimuth Angles'!I30))","v":0.77500562596203504},{"$f":"ATAN(TAN('Solar Altitude'!J31)/COS('Surface Solar Azimuth Angles'!J30))","v":0.92344909928942365},{"$f":"ATAN(TAN('Solar Altitude'!K31)/COS('Surface Solar Azimuth Angles'!K30))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L31)/COS('Surface Solar Azimuth Angles'!L30))","v":1.3348406596171152},{"$f":"ATAN(TAN('Solar Altitude'!M31)/COS('Surface Solar Azimuth Angles'!M30))","v":1.500983956115769},{"$f":"ATAN(TAN('Solar Altitude'!N31)/COS('Surface Solar Azimuth Angles'!N30))","v":1.5594894508681831},null,1,{"$f":"ATAN(TAN('Solar Altitude'!C31)/COS('Surface Solar Azimuth Angles'!Q30))","v":-1.3994410384001572},{"$f":"ATAN(TAN('Solar Altitude'!D31)/COS('Surface Solar Azimuth Angles'!R30))","v":-1.3987224426302709},{"$f":"ATAN(TAN('Solar Altitude'!E31)/COS('Surface Solar Azimuth Angles'!S30))","v":-1.3535067192060628},{"$f":"ATAN(TAN('Solar Altitude'!F31)/COS('Surface Solar Azimuth Angles'!T30))","v":-1.2854751008998169},{"$f":"ATAN(TAN('Solar Altitude'!G31)/COS('Surface Solar Azimuth Angles'!U30))","v":-1.2485940409284231},{"$f":"ATAN(TAN('Solar Altitude'!H31)/COS('Surface Solar Azimuth Angles'!V30))","v":-1.2646212293363484},{"$f":"ATAN(TAN('Solar Altitude'!I31)/COS('Surface Solar Azimuth Angles'!W30))","v":-1.3017917625848772},{"$f":"ATAN(TAN('Solar Altitude'!J31)/COS('Surface Solar Azimuth Angles'!X30))","v":-1.3032988016081293},{"$f":"ATAN(TAN('Solar Altitude'!K31)/COS('Surface Solar Azimuth Angles'!Y30))","v":-1.2822582122157415},{"$f":"ATAN(TAN('Solar Altitude'!L31)/COS('Surface Solar Azimuth Angles'!Z30))","v":-1.2704099409257712},{"$f":"ATAN(TAN('Solar Altitude'!M31)/COS('Surface Solar Azimuth Angles'!AA30))","v":-1.2971040377011409},{"$f":"ATAN(TAN('Solar Altitude'!N31)/COS('Surface Solar Azimuth Angles'!AB30))","v":-1.3530868681716333},null,1,{"$f":"ATAN(TAN('Solar Altitude'!C31)/COS('Surface Solar Azimuth Angles'!C85))","v":1.3994410384001572},{"$f":"ATAN(TAN('Solar Altitude'!D31)/COS('Surface Solar Azimuth Angles'!D85))","v":1.3987224426302707},{"$f":"ATAN(TAN('Solar Altitude'!E31)/COS('Surface Solar Azimuth Angles'!E85))","v":1.353506719206063},{"$f":"ATAN(TAN('Solar Altitude'!F31)/COS('Surface Solar Azimuth Angles'!F85))","v":1.2854751008998166},{"$f":"ATAN(TAN('Solar Altitude'!G31)/COS('Surface Solar Azimuth Angles'!G85))","v":1.2485940409284226},{"$f":"ATAN(TAN('Solar Altitude'!H31)/COS('Surface Solar Azimuth Angles'!H85))","v":1.2646212293363481},{"$f":"ATAN(TAN('Solar Altitude'!I31)/COS('Surface Solar Azimuth Angles'!I85))","v":1.3017917625848769},{"$f":"ATAN(TAN('Solar Altitude'!J31)/COS('Surface Solar Azimuth Angles'!J85))","v":1.3032988016081293},{"$f":"ATAN(TAN('Solar Altitude'!K31)/COS('Surface Solar Azimuth Angles'!K85))","v":1.2822582122157413},{"$f":"ATAN(TAN('Solar Altitude'!L31)/COS('Surface Solar Azimuth Angles'!L85))","v":1.2704099409257712},{"$f":"ATAN(TAN('Solar Altitude'!M31)/COS('Surface Solar Azimuth Angles'!M85))","v":1.2971040377011409},{"$f":"ATAN(TAN('Solar Altitude'!N31)/COS('Surface Solar Azimuth Angles'!N85))","v":1.3530868681716333},null,1,{"$f":"ATAN(TAN('Solar Altitude'!C31)/COS('Surface Solar Azimuth Angles'!Q85))","v":-1.4923733213519947},{"$f":"ATAN(TAN('Solar Altitude'!D31)/COS('Surface Solar Azimuth Angles'!R85))","v":-1.327348921355314},{"$f":"ATAN(TAN('Solar Altitude'!E31)/COS('Surface Solar Azimuth Angles'!S85))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F31)/COS('Surface Solar Azimuth Angles'!T85))","v":-0.92628661869809481},{"$f":"ATAN(TAN('Solar Altitude'!G31)/COS('Surface Solar Azimuth Angles'!U85))","v":-0.77541332917766936},{"$f":"ATAN(TAN('Solar Altitude'!H31)/COS('Surface Solar Azimuth Angles'!V85))","v":-0.72105580791449653},{"$f":"ATAN(TAN('Solar Altitude'!I31)/COS('Surface Solar Azimuth Angles'!W85))","v":-0.77500562596203515},{"$f":"ATAN(TAN('Solar Altitude'!J31)/COS('Surface Solar Azimuth Angles'!X85))","v":-0.92344909928942354},{"$f":"ATAN(TAN('Solar Altitude'!K31)/COS('Surface Solar Azimuth Angles'!Y85))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L31)/COS('Surface Solar Azimuth Angles'!Z85))","v":-1.3348406596171152},{"$f":"ATAN(TAN('Solar Altitude'!M31)/COS('Surface Solar Azimuth Angles'!AA85))","v":-1.5009839561157687},{"$f":"ATAN(TAN('Solar Altitude'!N31)/COS('Surface Solar Azimuth Angles'!AB85))","v":-1.5594894508681831}]
[null,2,{"$f":"ATAN(TAN('Solar Altitude'!C32)/COS('Surface Solar Azimuth Angles'!C31))","v":1.5208845729807423},{"$f":"ATAN(TAN('Solar Altitude'!D32)/COS('Surface Solar Azimuth Angles'!D31))","v":1.3429160432098302},{"$f":"ATAN(TAN('Solar Altitude'!E32)/COS('Surface Solar Azimuth Angles'!E31))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F32)/COS('Surface Solar Azimuth Angles'!F31))","v":0.90436988504871818},{"$f":"ATAN(TAN('Solar Altitude'!G32)/COS('Surface Solar Azimuth Angles'!G31))","v":0.73943113538447891},{"$f":"ATAN(TAN('Solar Altitude'!H32)/COS('Surface Solar Azimuth Angles'!H31))","v":0.68354026259431278},{"$f":"ATAN(TAN('Solar Altitude'!I32)/COS('Surface Solar Azimuth Angles'!I31))","v":0.7434435505657796},{"$f":"ATAN(TAN('Solar Altitude'!J32)/COS('Surface Solar Azimuth Angles'!J31))","v":0.90231514982176786},{"$f":"ATAN(TAN('Solar Altitude'!K32)/COS('Surface Solar Azimuth Angles'!K31))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L32)/COS('Surface Solar Azimuth Angles'!L31))","v":1.3590817446939001},{"$f":"ATAN(TAN('Solar Altitude'!M32)/COS('Surface Solar Azimuth Angles'!M31))","v":1.5418396740988674},{"$f":"ATAN(TAN('Solar Altitude'!N32)/COS('Surface Solar Azimuth Angles'!N31))","v":-1.542946372430622},null,2,{"$f":"ATAN(TAN('Solar Altitude'!C32)/COS('Surface Solar Azimuth Angles'!Q31))","v":-1.1549210062521438},{"$f":"ATAN(TAN('Solar Altitude'!D32)/COS('Surface Solar Azimuth Angles'!R31))","v":-1.1369164007416153},{"$f":"ATAN(TAN('Solar Altitude'!E32)/COS('Surface Solar Azimuth Angles'!S31))","v":-1.0718008336148823},{"$f":"ATAN(TAN('Solar Altitude'!F32)/COS('Surface Solar Azimuth Angles'!T31))","v":-0.97946880043257922},{"$f":"ATAN(TAN('Solar Altitude'!G32)/COS('Surface Solar Azimuth Angles'!U31))","v":-0.92164982186211619},{"$f":"ATAN(TAN('Solar Altitude'!H32)/COS('Surface Solar Azimuth Angles'!V31))","v":-0.92627284120998121},{"$f":"ATAN(TAN('Solar Altitude'!I32)/COS('Surface Solar Azimuth Angles'!W31))","v":-0.97053375348907012},{"$f":"ATAN(TAN('Solar Altitude'!J32)/COS('Surface Solar Azimuth Angles'!X31))","v":-0.99586471792571007},{"$f":"ATAN(TAN('Solar Altitude'!K32)/COS('Surface Solar Azimuth Angles'!Y31))","v":-1.0030149795642196},{"$f":"ATAN(TAN('Solar Altitude'!L32)/COS('Surface Solar Azimuth Angles'!Z31))","v":-1.0118824071687469},{"$f":"ATAN(TAN('Solar Altitude'!M32)/COS('Surface Solar Azimuth Angles'!AA31))","v":-1.0543583507572232},{"$f":"ATAN(TAN('Solar Altitude'!N32)/COS('Surface Solar Azimuth Angles'!AB31))","v":-1.1157238568704597},null,2,{"$f":"ATAN(TAN('Solar Altitude'!C32)/COS('Surface Solar Azimuth Angles'!C86))","v":1.1549210062521438},{"$f":"ATAN(TAN('Solar Altitude'!D32)/COS('Surface Solar Azimuth Angles'!D86))","v":1.136916400741615},{"$f":"ATAN(TAN('Solar Altitude'!E32)/COS('Surface Solar Azimuth Angles'!E86))","v":1.0718008336148825},{"$f":"ATAN(TAN('Solar Altitude'!F32)/COS('Surface Solar Azimuth Angles'!F86))","v":0.979468800432579},{"$f":"ATAN(TAN('Solar Altitude'!G32)/COS('Surface Solar Azimuth Angles'!G86))","v":0.92164982186211586},{"$f":"ATAN(TAN('Solar Altitude'!H32)/COS('Surface Solar Azimuth Angles'!H86))","v":0.92627284120998088},{"$f":"ATAN(TAN('Solar Altitude'!I32)/COS('Surface Solar Azimuth Angles'!I86))","v":0.97053375348906978},{"$f":"ATAN(TAN('Solar Altitude'!J32)/COS('Surface Solar Azimuth Angles'!J86))","v":0.99586471792570985},{"$f":"ATAN(TAN('Solar Altitude'!K32)/COS('Surface Solar Azimuth Angles'!K86))","v":1.0030149795642196},{"$f":"ATAN(TAN('Solar Altitude'!L32)/COS('Surface Solar Azimuth Angles'!L86))","v":1.0118824071687469},{"$f":"ATAN(TAN('Solar Altitude'!M32)/COS('Surface Solar Azimuth Angles'!M86))","v":1.0543583507572232},{"$f":"ATAN(TAN('Solar Altitude'!N32)/COS('Surface Solar Azimuth Angles'!N86))","v":1.1157238568704597},null,2,{"$f":"ATAN(TAN('Solar Altitude'!C32)/COS('Surface Solar Azimuth Angles'!Q86))","v":-1.5208845729807423},{"$f":"ATAN(TAN('Solar Altitude'!D32)/COS('Surface Solar Azimuth Angles'!R86))","v":-1.3429160432098304},{"$f":"ATAN(TAN('Solar Altitude'!E32)/COS('Surface Solar Azimuth Angles'!S86))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F32)/COS('Surface Solar Azimuth Angles'!T86))","v":-0.90436988504871829},{"$f":"ATAN(TAN('Solar Altitude'!G32)/COS('Surface Solar Azimuth Angles'!U86))","v":-0.73943113538447891},{"$f":"ATAN(TAN('Solar Altitude'!H32)/COS('Surface Solar Azimuth Angles'!V86))","v":-0.68354026259431278},{"$f":"ATAN(TAN('Solar Altitude'!I32)/COS('Surface Solar Azimuth Angles'!W86))","v":-0.7434435505657796},{"$f":"ATAN(TAN('Solar Altitude'!J32)/COS('Surface Solar Azimuth Angles'!X86))","v":-0.90231514982176808},{"$f":"ATAN(TAN('Solar Altitude'!K32)/COS('Surface Solar Azimuth Angles'!Y86))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L32)/COS('Surface Solar Azimuth Angles'!Z86))","v":-1.3590817446938999},{"$f":"ATAN(TAN('Solar Altitude'!M32)/COS('Surface Solar Azimuth Angles'!AA86))","v":-1.5418396740988674},{"$f":"ATAN(TAN('Solar Altitude'!N32)/COS('Surface Solar Azimuth Angles'!AB86))","v":1.5429463724306218}]
[null,3,{"$f":"ATAN(TAN('Solar Altitude'!C33)/COS('Surface Solar Azimuth Angles'!C32))","v":-1.5580652106671682},{"$f":"ATAN(TAN('Solar Altitude'!D33)/COS('Surface Solar Azimuth Angles'!D32))","v":1.3784403465863997},{"$f":"ATAN(TAN('Solar Altitude'!E33)/COS('Surface Solar Azimuth Angles'!E32))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F33)/COS('Surface Solar Azimuth Angles'!F32))","v":0.85700339968847628},{"$f":"ATAN(TAN('Solar Altitude'!G33)/COS('Surface Solar Azimuth Angles'!G32))","v":0.66444179725335362},{"$f":"ATAN(TAN('Solar Altitude'!H33)/COS('Surface Solar Azimuth Angles'!H32))","v":0.60530956821516535},{"$f":"ATAN(TAN('Solar Altitude'!I33)/COS('Surface Solar Azimuth Angles'!I32))","v":0.67565393770152993},{"$f":"ATAN(TAN('Solar Altitude'!J33)/COS('Surface Solar Azimuth Angles'!J32))","v":0.85622667593368873},{"$f":"ATAN(TAN('Solar Altitude'!K33)/COS('Surface Solar Azimuth Angles'!K32))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L33)/COS('Surface Solar Azimuth Angles'!L32))","v":1.410298559579243},{"$f":"ATAN(TAN('Solar Altitude'!M33)/COS('Surface Solar Azimuth Angles'!M32))","v":-1.5164850137084307},{"$f":"ATAN(TAN('Solar Altitude'!N33)/COS('Surface Solar Azimuth Angles'!N32))","v":-1.4620905045107382},null,3,{"$f":"ATAN(TAN('Solar Altitude'!C33)/COS('Surface Solar Azimuth Angles'!Q32))","v":-0.91516630314878677},{"$f":"ATAN(TAN('Solar Altitude'!D33)/COS('Surface Solar Azimuth Angles'!R32))","v":-0.8821622416026319},{"$f":"ATAN(TAN('Solar Altitude'!E33)/COS('Surface Solar Azimuth Angles'!S32))","v":-0.80144392257758257},{"$f":"ATAN(TAN('Solar Altitude'!F33)/COS('Surface Solar Azimuth Angles'!T32))","v":-0.69259090438957494},{"$f":"ATAN(TAN('Solar Altitude'!G33)/COS('Surface Solar Azimuth Angles'!U32))","v":-0.62209031311095009},{"$f":"ATAN(TAN('Solar Altitude'!H33)/COS('Surface Solar Azimuth Angles'!V32))","v":-0.61897895359016175},{"$f":"ATAN(TAN('Solar Altitude'!I33)/COS('Surface Solar Azimuth Angles'!W32))","v":-0.66606658842026967},{"$f":"ATAN(TAN('Solar Altitude'!J33)/COS('Surface Solar Azimuth Angles'!X32))","v":-0.70745482580220742},{"$f":"ATAN(TAN('Solar Altitude'!K33)/COS('Surface Solar Azimuth Angles'!Y32))","v":-0.7359036106296305},{"$f":"ATAN(TAN('Solar Altitude'!L33)/COS('Surface Solar Azimuth Angles'!Z32))","v":-0.76137198766493486},{"$f":"ATAN(TAN('Solar Altitude'!M33)/COS('Surface Solar Azimuth Angles'!AA32))","v":-0.81690920458132033},{"$f":"ATAN(TAN('Solar Altitude'!N33)/COS('Surface Solar Azimuth Angles'!AB32))","v":-0.88265807634038995},null,3,{"$f":"ATAN(TAN('Solar Altitude'!C33)/COS('Surface Solar Azimuth Angles'!C87))","v":0.91516630314878677},{"$f":"ATAN(TAN('Solar Altitude'!D33)/COS('Surface Solar Azimuth Angles'!D87))","v":0.8821622416026319},{"$f":"ATAN(TAN('Solar Altitude'!E33)/COS('Surface Solar Azimuth Angles'!E87))","v":0.80144392257758257},{"$f":"ATAN(TAN('Solar Altitude'!F33)/COS('Surface Solar Azimuth Angles'!F87))","v":0.69259090438957494},{"$f":"ATAN(TAN('Solar Altitude'!G33)/COS('Surface Solar Azimuth Angles'!G87))","v":0.62209031311094998},{"$f":"ATAN(TAN('Solar Altitude'!H33)/COS('Surface Solar Azimuth Angles'!H87))","v":0.61897895359016175},{"$f":"ATAN(TAN('Solar Altitude'!I33)/COS('Surface Solar Azimuth Angles'!I87))","v":0.66606658842026967},{"$f":"ATAN(TAN('Solar Altitude'!J33)/COS('Surface Solar Azimuth Angles'!J87))","v":0.70745482580220731},{"$f":"ATAN(TAN('Solar Altitude'!K33)/COS('Surface Solar Azimuth Angles'!K87))","v":0.73590361062963061},{"$f":"ATAN(TAN('Solar Altitude'!L33)/COS('Surface Solar Azimuth Angles'!L87))","v":0.76137198766493475},{"$f":"ATAN(TAN('Solar Altitude'!M33)/COS('Surface Solar Azimuth Angles'!M87))","v":0.81690920458132033},{"$f":"ATAN(TAN('Solar Altitude'!N33)/COS('Surface Solar Azimuth Angles'!N87))","v":0.88265807634038995},null,3,{"$f":"ATAN(TAN('Solar Altitude'!C33)/COS('Surface Solar Azimuth Angles'!Q87))","v":1.5580652106671682},{"$f":"ATAN(TAN('Solar Altitude'!D33)/COS('Surface Solar Azimuth Angles'!R87))","v":-1.3784403465863997},{"$f":"ATAN(TAN('Solar Altitude'!E33)/COS('Surface Solar Azimuth Angles'!S87))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F33)/COS('Surface Solar Azimuth Angles'!T87))","v":-0.85700339968847628},{"$f":"ATAN(TAN('Solar Altitude'!G33)/COS('Surface Solar Azimuth Angles'!U87))","v":-0.66444179725335351},{"$f":"ATAN(TAN('Solar Altitude'!H33)/COS('Surface Solar Azimuth Angles'!V87))","v":-0.60530956821516535},{"$f":"ATAN(TAN('Solar Altitude'!I33)/COS('Surface Solar Azimuth Angles'!W87))","v":-0.67565393770152993},{"$f":"ATAN(TAN('Solar Altitude'!J33)/COS('Surface Solar Azimuth Angles'!X87))","v":-0.85622667593368862},{"$f":"ATAN(TAN('Solar Altitude'!K33)/COS('Surface Solar Azimuth Angles'!Y87))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L33)/COS('Surface Solar Azimuth Angles'!Z87))","v":-1.410298559579243},{"$f":"ATAN(TAN('Solar Altitude'!M33)/COS('Surface Solar Azimuth Angles'!AA87))","v":1.5164850137084309},{"$f":"ATAN(TAN('Solar Altitude'!N33)/COS('Surface Solar Azimuth Angles'!AB87))","v":1.4620905045107382}]
[null,4,{"$f":"ATAN(TAN('Solar Altitude'!C34)/COS('Surface Solar Azimuth Angles'!C33))","v":-1.4341706307619093},{"$f":"ATAN(TAN('Solar Altitude'!D34)/COS('Surface Solar Azimuth Angles'!D33))","v":1.4532017897405849},{"$f":"ATAN(TAN('Solar Altitude'!E34)/COS('Surface Solar Azimuth Angles'!E33))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F34)/COS('Surface Solar Azimuth Angles'!F33))","v":0.75641890675993251},{"$f":"ATAN(TAN('Solar Altitude'!G34)/COS('Surface Solar Azimuth Angles'!G33))","v":0.5162754389988029},{"$f":"ATAN(TAN('Solar Altitude'!H34)/COS('Surface Solar Azimuth Angles'!H33))","v":0.4555590077463848},{"$f":"ATAN(TAN('Solar Altitude'!I34)/COS('Surface Solar Azimuth Angles'!I33))","v":0.54225140039405473},{"$f":"ATAN(TAN('Solar Altitude'!J34)/COS('Surface Solar Azimuth Angles'!J33))","v":0.75895388639250683},{"$f":"ATAN(TAN('Solar Altitude'!K34)/COS('Surface Solar Azimuth Angles'!K33))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L34)/COS('Surface Solar Azimuth Angles'!L33))","v":1.5231003679412918},{"$f":"ATAN(TAN('Solar Altitude'!M34)/COS('Surface Solar Azimuth Angles'!M33))","v":-1.3502899956877574},{"$f":"ATAN(TAN('Solar Altitude'!N34)/COS('Surface Solar Azimuth Angles'!N33))","v":-1.3073727427737787},null,4,{"$f":"ATAN(TAN('Solar Altitude'!C34)/COS('Surface Solar Azimuth Angles'!Q33))","v":-0.68085626049108372},{"$f":"ATAN(TAN('Solar Altitude'!D34)/COS('Surface Solar Azimuth Angles'!R33))","v":-0.63580151600596935},{"$f":"ATAN(TAN('Solar Altitude'!E34)/COS('Surface Solar Azimuth Angles'!S33))","v":-0.54404800401822839},{"$f":"ATAN(TAN('Solar Altitude'!F34)/COS('Surface Solar Azimuth Angles'!T33))","v":-0.42586833332700952},{"$f":"ATAN(TAN('Solar Altitude'!G34)/COS('Surface Solar Azimuth Angles'!U33))","v":-0.34974170353085882},{"$f":"ATAN(TAN('Solar Altitude'!H34)/COS('Surface Solar Azimuth Angles'!V33))","v":-0.34253601746325713},{"$f":"ATAN(TAN('Solar Altitude'!I34)/COS('Surface Solar Azimuth Angles'!W33))","v":-0.38955752453780007},{"$f":"ATAN(TAN('Solar Altitude'!J34)/COS('Surface Solar Azimuth Angles'!X33))","v":-0.43944775480650367},{"$f":"ATAN(TAN('Solar Altitude'!K34)/COS('Surface Solar Azimuth Angles'!Y33))","v":-0.48155681326357486},{"$f":"ATAN(TAN('Solar Altitude'!L34)/COS('Surface Solar Azimuth Angles'!Z33))","v":-0.51888038822348748},{"$f":"ATAN(TAN('Solar Altitude'!M34)/COS('Surface Solar Azimuth Angles'!AA33))","v":-0.58456796965293845},{"$f":"ATAN(TAN('Solar Altitude'!N34)/COS('Surface Solar Azimuth Angles'!AB33))","v":-0.6539876584676938},null,4,{"$f":"ATAN(TAN('Solar Altitude'!C34)/COS('Surface Solar Azimuth Angles'!C88))","v":0.68085626049108372},{"$f":"ATAN(TAN('Solar Altitude'!D34)/COS('Surface Solar Azimuth Angles'!D88))","v":0.63580151600596935},{"$f":"ATAN(TAN('Solar Altitude'!E34)/COS('Surface Solar Azimuth Angles'!E88))","v":0.54404800401822839},{"$f":"ATAN(TAN('Solar Altitude'!F34)/COS('Surface Solar Azimuth Angles'!F88))","v":0.42586833332700952},{"$f":"ATAN(TAN('Solar Altitude'!G34)/COS('Surface Solar Azimuth Angles'!G88))","v":0.34974170353085882},{"$f":"ATAN(TAN('Solar Altitude'!H34)/COS('Surface Solar Azimuth Angles'!H88))","v":0.34253601746325713},{"$f":"ATAN(TAN('Solar Altitude'!I34)/COS('Surface Solar Azimuth Angles'!I88))","v":0.38955752453779996},{"$f":"ATAN(TAN('Solar Altitude'!J34)/COS('Surface Solar Azimuth Angles'!J88))","v":0.43944775480650367},{"$f":"ATAN(TAN('Solar Altitude'!K34)/COS('Surface Solar Azimuth Angles'!K88))","v":0.48155681326357486},{"$f":"ATAN(TAN('Solar Altitude'!L34)/COS('Surface Solar Azimuth Angles'!L88))","v":0.51888038822348748},{"$f":"ATAN(TAN('Solar Altitude'!M34)/COS('Surface Solar Azimuth Angles'!M88))","v":0.58456796965293845},{"$f":"ATAN(TAN('Solar Altitude'!N34)/COS('Surface Solar Azimuth Angles'!N88))","v":0.6539876584676938},null,4,{"$f":"ATAN(TAN('Solar Altitude'!C34)/COS('Surface Solar Azimuth Angles'!Q88))","v":1.4341706307619093},{"$f":"ATAN(TAN('Solar Altitude'!D34)/COS('Surface Solar Azimuth Angles'!R88))","v":-1.4532017897405849},{"$f":"ATAN(TAN('Solar Altitude'!E34)/COS('Surface Solar Azimuth Angles'!S88))","v":-1.1397000015522976},{"$f":"ATAN(TAN('Solar Altitude'!F34)/COS('Surface Solar Azimuth Angles'!T88))","v":-0.7564189067599324},{"$f":"ATAN(TAN('Solar Altitude'!G34)/COS('Surface Solar Azimuth Angles'!U88))","v":-0.5162754389988029},{"$f":"ATAN(TAN('Solar Altitude'!H34)/COS('Surface Solar Azimuth Angles'!V88))","v":-0.4555590077463848},{"$f":"ATAN(TAN('Solar Altitude'!I34)/COS('Surface Solar Azimuth Angles'!W88))","v":-0.54225140039405473},{"$f":"ATAN(TAN('Solar Altitude'!J34)/COS('Surface Solar Azimuth Angles'!X88))","v":-0.7589538863925066},{"$f":"ATAN(TAN('Solar Altitude'!K34)/COS('Surface Solar Azimuth Angles'!Y88))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L34)/COS('Surface Solar Azimuth Angles'!Z88))","v":-1.5231003679412916},{"$f":"ATAN(TAN('Solar Altitude'!M34)/COS('Surface Solar Azimuth Angles'!AA88))","v":1.3502899956877576},{"$f":"ATAN(TAN('Solar Altitude'!N34)/COS('Surface Solar Azimuth Angles'!AB88))","v":1.3073727427737785}]
[null,5,{"$f":"ATAN(TAN('Solar Altitude'!C35)/COS('Surface Solar Azimuth Angles'!C34))","v":-1.1780474606511619},{"$f":"ATAN(TAN('Solar Altitude'!D35)/COS('Surface Solar Azimuth Angles'!D34))","v":-1.5063837691420776},{"$f":"ATAN(TAN('Solar Altitude'!E35)/COS('Surface Solar Azimuth Angles'!E34))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F35)/COS('Surface Solar Azimuth Angles'!F34))","v":0.50158785009162143},{"$f":"ATAN(TAN('Solar Altitude'!G35)/COS('Surface Solar Azimuth Angles'!G34))","v":0.2080737467427515},{"$f":"ATAN(TAN('Solar Altitude'!H35)/COS('Surface Solar Azimuth Angles'!H34))","v":0.16549565334901181},{"$f":"ATAN(TAN('Solar Altitude'!I35)/COS('Surface Solar Azimuth Angles'!I34))","v":0.26831827706241235},{"$f":"ATAN(TAN('Solar Altitude'!J35)/COS('Surface Solar Azimuth Angles'!J34))","v":0.51728377304772166},{"$f":"ATAN(TAN('Solar Altitude'!K35)/COS('Surface Solar Azimuth Angles'!K34))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L35)/COS('Surface Solar Azimuth Angles'!L34))","v":-1.3007610762503927},{"$f":"ATAN(TAN('Solar Altitude'!M35)/COS('Surface Solar Azimuth Angles'!M34))","v":-0.99832765575334248},{"$f":"ATAN(TAN('Solar Altitude'!N35)/COS('Surface Solar Azimuth Angles'!N34))","v":-1.007647471209566},null,5,{"$f":"ATAN(TAN('Solar Altitude'!C35)/COS('Surface Solar Azimuth Angles'!Q34))","v":-0.45057174190181382},{"$f":"ATAN(TAN('Solar Altitude'!D35)/COS('Surface Solar Azimuth Angles'!R34))","v":-0.39650083624290827},{"$f":"ATAN(TAN('Solar Altitude'!E35)/COS('Surface Solar Azimuth Angles'!S34))","v":-0.29766243646613255},{"$f":"ATAN(TAN('Solar Altitude'!F35)/COS('Surface Solar Azimuth Angles'!T34))","v":-0.17558478457949334},{"$f":"ATAN(TAN('Solar Altitude'!G35)/COS('Surface Solar Azimuth Angles'!U34))","v":-9.8704393140607194E-2},{"$f":"ATAN(TAN('Solar Altitude'!H35)/COS('Surface Solar Azimuth Angles'!V34))","v":-9.0149372015666446E-2},{"$f":"ATAN(TAN('Solar Altitude'!I35)/COS('Surface Solar Azimuth Angles'!W34))","v":-0.1356210090143263},{"$f":"ATAN(TAN('Solar Altitude'!J35)/COS('Surface Solar Azimuth Angles'!X34))","v":-0.18829152816436306},{"$f":"ATAN(TAN('Solar Altitude'!K35)/COS('Surface Solar Azimuth Angles'!Y34))","v":-0.23731883827832312},{"$f":"ATAN(TAN('Solar Altitude'!L35)/COS('Surface Solar Azimuth Angles'!Z34))","v":-0.28192945219888416},{"$f":"ATAN(TAN('Solar Altitude'!M35)/COS('Surface Solar Azimuth Angles'!AA34))","v":-0.35506274589045206},{"$f":"ATAN(TAN('Solar Altitude'!N35)/COS('Surface Solar Azimuth Angles'!AB34))","v":-0.42785968501246852},null,5,{"$f":"ATAN(TAN('Solar Altitude'!C35)/COS('Surface Solar Azimuth Angles'!C89))","v":0.45057174190181382},{"$f":"ATAN(TAN('Solar Altitude'!D35)/COS('Surface Solar Azimuth Angles'!D89))","v":0.39650083624290827},{"$f":"ATAN(TAN('Solar Altitude'!E35)/COS('Surface Solar Azimuth Angles'!E89))","v":0.29766243646613255},{"$f":"ATAN(TAN('Solar Altitude'!F35)/COS('Surface Solar Azimuth Angles'!F89))","v":0.17558478457949331},{"$f":"ATAN(TAN('Solar Altitude'!G35)/COS('Surface Solar Azimuth Angles'!G89))","v":9.870439314060718E-2},{"$f":"ATAN(TAN('Solar Altitude'!H35)/COS('Surface Solar Azimuth Angles'!H89))","v":9.0149372015666446E-2},{"$f":"ATAN(TAN('Solar Altitude'!I35)/COS('Surface Solar Azimuth Angles'!I89))","v":0.1356210090143263},{"$f":"ATAN(TAN('Solar Altitude'!J35)/COS('Surface Solar Azimuth Angles'!J89))","v":0.18829152816436306},{"$f":"ATAN(TAN('Solar Altitude'!K35)/COS('Surface Solar Azimuth Angles'!K89))","v":0.23731883827832312},{"$f":"ATAN(TAN('Solar Altitude'!L35)/COS('Surface Solar Azimuth Angles'!L89))","v":0.28192945219888416},{"$f":"ATAN(TAN('Solar Altitude'!M35)/COS('Surface Solar Azimuth Angles'!M89))","v":0.35506274589045206},{"$f":"ATAN(TAN('Solar Altitude'!N35)/COS('Surface Solar Azimuth Angles'!N89))","v":0.42785968501246857},null,5,{"$f":"ATAN(TAN('Solar Altitude'!C35)/COS('Surface Solar Azimuth Angles'!Q89))","v":1.1780474606511622},{"$f":"ATAN(TAN('Solar Altitude'!D35)/COS('Surface Solar Azimuth Angles'!R89))","v":1.5063837691420774},{"$f":"ATAN(TAN('Solar Altitude'!E35)/COS('Surface Solar Azimuth Angles'!S89))","v":-1.1397000015522976},{"$f":"ATAN(TAN('Solar Altitude'!F35)/COS('Surface Solar Azimuth Angles'!T89))","v":-0.50158785009162166},{"$f":"ATAN(TAN('Solar Altitude'!G35)/COS('Surface Solar Azimuth Angles'!U89))","v":-0.20807374674275145},{"$f":"ATAN(TAN('Solar Altitude'!H35)/COS('Surface Solar Azimuth Angles'!V89))","v":-0.16549565334901178},{"$f":"ATAN(TAN('Solar Altitude'!I35)/COS('Surface Solar Azimuth Angles'!W89))","v":-0.26831827706241224},{"$f":"ATAN(TAN('Solar Altitude'!J35)/COS('Surface Solar Azimuth Angles'!X89))","v":-0.51728377304772155},{"$f":"ATAN(TAN('Solar Altitude'!K35)/COS('Surface Solar Azimuth Angles'!Y89))","v":-1.1397000015522978},{"$f":"ATAN(TAN('Solar Altitude'!L35)/COS('Surface Solar Azimuth Angles'!Z89))","v":1.3007610762503929},{"$f":"ATAN(TAN('Solar Altitude'!M35)/COS('Surface Solar Azimuth Angles'!AA89))","v":0.9983276557533427},{"$f":"ATAN(TAN('Solar Altitude'!N35)/COS('Surface Solar Azimuth Angles'!AB89))","v":1.0076474712095662}]
[null,6,{"$f":"ATAN(TAN('Solar Altitude'!C36)/COS('Surface Solar Azimuth Angles'!C35))","v":-0.64835816681447489},{"$f":"ATAN(TAN('Solar Altitude'!D36)/COS('Surface Solar Azimuth Angles'!D35))","v":-0.88647687640734596},{"$f":"ATAN(TAN('Solar Altitude'!E36)/COS('Surface Solar Azimuth Angles'!E35))","v":1.1397000015522982},{"$f":"ATAN(TAN('Solar Altitude'!F36)/COS('Surface Solar Azimuth Angles'!F35))","v":-0.30683145766901876},{"$f":"ATAN(TAN('Solar Altitude'!G36)/COS('Surface Solar Azimuth Angles'!G35))","v":-0.38591275889302951},{"$f":"ATAN(TAN('Solar Altitude'!H36)/COS('Surface Solar Azimuth Angles'!H35))","v":-0.34548950434356829},{"$f":"ATAN(TAN('Solar Altitude'!I36)/COS('Surface Solar Azimuth Angles'!I35))","v":-0.27681674745400869},{"$f":"ATAN(TAN('Solar Altitude'!J36)/COS('Surface Solar Azimuth Angles'!J35))","v":-0.23949897187106284},{"$f":"ATAN(TAN('Solar Altitude'!K36)/COS('Surface Solar Azimuth Angles'!K35))","v":1.1397000015523175},{"$f":"ATAN(TAN('Solar Altitude'!L36)/COS('Surface Solar Azimuth Angles'!L35))","v":-0.2425098589486748},{"$f":"ATAN(TAN('Solar Altitude'!M36)/COS('Surface Solar Azimuth Angles'!M35))","v":-0.35092289852329306},{"$f":"ATAN(TAN('Solar Altitude'!N36)/COS('Surface Solar Azimuth Angles'!N35))","v":-0.48669309889480084},null,6,{"$f":"ATAN(TAN('Solar Altitude'!C36)/COS('Surface Solar Azimuth Angles'!Q35))","v":-0.22091645053294795},{"$f":"ATAN(TAN('Solar Altitude'!D36)/COS('Surface Solar Azimuth Angles'!R35))","v":-0.16074662252161659},{"$f":"ATAN(TAN('Solar Altitude'!E36)/COS('Surface Solar Azimuth Angles'!S35))","v":-5.8021971754234451E-2},{"$f":"ATAN(TAN('Solar Altitude'!F36)/COS('Surface Solar Azimuth Angles'!T35))","v":6.4078725586556834E-2},{"$f":"ATAN(TAN('Solar Altitude'!G36)/COS('Surface Solar Azimuth Angles'!U35))","v":0.1385056203166444},{"$f":"ATAN(TAN('Solar Altitude'!H36)/COS('Surface Solar Azimuth Angles'!V35))","v":0.14648644817173609},{"$f":"ATAN(TAN('Solar Altitude'!I36)/COS('Surface Solar Azimuth Angles'!W35))","v":0.1032161832467153},{"$f":"ATAN(TAN('Solar Altitude'!J36)/COS('Surface Solar Azimuth Angles'!X35))","v":5.1801075064635944E-2},{"$f":"ATAN(TAN('Solar Altitude'!K36)/COS('Surface Solar Azimuth Angles'!Y35))","v":1.4535089563001097E-3},{"$f":"ATAN(TAN('Solar Altitude'!L36)/COS('Surface Solar Azimuth Angles'!Z35))","v":-4.6191080812301957E-2},{"$f":"ATAN(TAN('Solar Altitude'!M36)/COS('Surface Solar Azimuth Angles'!AA35))","v":-0.12425151109146822},{"$f":"ATAN(TAN('Solar Altitude'!N36)/COS('Surface Solar Azimuth Angles'!AB35))","v":-0.20052072268814197},null,6,{"$f":"ATAN(TAN('Solar Altitude'!C36)/COS('Surface Solar Azimuth Angles'!C90))","v":0.22091645053294795},{"$f":"ATAN(TAN('Solar Altitude'!D36)/COS('Surface Solar Azimuth Angles'!D90))","v":0.16074662252161659},{"$f":"ATAN(TAN('Solar Altitude'!E36)/COS('Surface Solar Azimuth Angles'!E90))","v":5.8021971754234451E-2},{"$f":"ATAN(TAN('Solar Altitude'!F36)/COS('Surface Solar Azimuth Angles'!F90))","v":-6.4078725586556834E-2},{"$f":"ATAN(TAN('Solar Altitude'!G36)/COS('Surface Solar Azimuth Angles'!G90))","v":-0.13850562031664443},{"$f":"ATAN(TAN('Solar Altitude'!H36)/COS('Surface Solar Azimuth Angles'!H90))","v":-0.14648644817173606},{"$f":"ATAN(TAN('Solar Altitude'!I36)/COS('Surface Solar Azimuth Angles'!I90))","v":-0.1032161832467153},{"$f":"ATAN(TAN('Solar Altitude'!J36)/COS('Surface Solar Azimuth Angles'!J90))","v":-5.1801075064635937E-2},{"$f":"ATAN(TAN('Solar Altitude'!K36)/COS('Surface Solar Azimuth Angles'!K90))","v":-1.4535089563001097E-3},{"$f":"ATAN(TAN('Solar Altitude'!L36)/COS('Surface Solar Azimuth Angles'!L90))","v":4.619108081230195E-2},{"$f":"ATAN(TAN('Solar Altitude'!M36)/COS('Surface Solar Azimuth Angles'!M90))","v":0.12425151109146822},{"$f":"ATAN(TAN('Solar Altitude'!N36)/COS('Surface Solar Azimuth Angles'!N90))","v":0.20052072268814197},null,6,{"$f":"ATAN(TAN('Solar Altitude'!C36)/COS('Surface Solar Azimuth Angles'!Q90))","v":0.64835816681447511},{"$f":"ATAN(TAN('Solar Altitude'!D36)/COS('Surface Solar Azimuth Angles'!R90))","v":0.8864768764073464},{"$f":"ATAN(TAN('Solar Altitude'!E36)/COS('Surface Solar Azimuth Angles'!S90))","v":-1.1397000015522964},{"$f":"ATAN(TAN('Solar Altitude'!F36)/COS('Surface Solar Azimuth Angles'!T90))","v":0.30683145766901854},{"$f":"ATAN(TAN('Solar Altitude'!G36)/COS('Surface Solar Azimuth Angles'!U90))","v":0.38591275889302934},{"$f":"ATAN(TAN('Solar Altitude'!H36)/COS('Surface Solar Azimuth Angles'!V90))","v":0.34548950434356818},{"$f":"ATAN(TAN('Solar Altitude'!I36)/COS('Surface Solar Azimuth Angles'!W90))","v":0.27681674745400858},{"$f":"ATAN(TAN('Solar Altitude'!J36)/COS('Surface Solar Azimuth Angles'!X90))","v":0.23949897187106275},{"$f":"ATAN(TAN('Solar Altitude'!K36)/COS('Surface Solar Azimuth Angles'!Y90))","v":-1.139700001552387},{"$f":"ATAN(TAN('Solar Altitude'!L36)/COS('Surface Solar Azimuth Angles'!Z90))","v":0.24250985894867499},{"$f":"ATAN(TAN('Solar Altitude'!M36)/COS('Surface Solar Azimuth Angles'!AA90))","v":0.35092289852329317},{"$f":"ATAN(TAN('Solar Altitude'!N36)/COS('Surface Solar Azimuth Angles'!AB90))","v":0.48669309889480072}]
[null,7,{"$f":"ATAN(TAN('Solar Altitude'!C37)/COS('Surface Solar Azimuth Angles'!C36))","v":3.2126378124526907E-2},{"$f":"ATAN(TAN('Solar Altitude'!D37)/COS('Surface Solar Azimuth Angles'!D36))","v":0.30400417987737721},{"$f":"ATAN(TAN('Solar Altitude'!E37)/COS('Surface Solar Azimuth Angles'!E36))","v":1.1397000015522967},{"$f":"ATAN(TAN('Solar Altitude'!F37)/COS('Surface Solar Azimuth Angles'!F36))","v":-1.2672818655170028},{"$f":"ATAN(TAN('Solar Altitude'!G37)/COS('Surface Solar Azimuth Angles'!G36))","v":-1.0116130508303163},{"$f":"ATAN(TAN('Solar Altitude'!H37)/COS('Surface Solar Azimuth Angles'!H36))","v":-0.90537507022991537},{"$f":"ATAN(TAN('Solar Altitude'!I37)/COS('Surface Solar Azimuth Angles'!I36))","v":-0.92689168179647385},{"$f":"ATAN(TAN('Solar Altitude'!J37)/COS('Surface Solar Azimuth Angles'!J36))","v":-1.2258417459156576},{"$f":"ATAN(TAN('Solar Altitude'!K37)/COS('Surface Solar Azimuth Angles'!K36))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L37)/COS('Surface Solar Azimuth Angles'!L36))","v":0.56767922585481501},{"$f":"ATAN(TAN('Solar Altitude'!M37)/COS('Surface Solar Azimuth Angles'!M36))","v":0.23892272571930664},{"$f":"ATAN(TAN('Solar Altitude'!N37)/COS('Surface Solar Azimuth Angles'!N36))","v":6.6151862638080955E-2},null,7,{"$f":"ATAN(TAN('Solar Altitude'!C37)/COS('Surface Solar Azimuth Angles'!Q36))","v":1.3214305906891736E-2},{"$f":"ATAN(TAN('Solar Altitude'!D37)/COS('Surface Solar Azimuth Angles'!R36))","v":7.6478952342661624E-2},{"$f":"ATAN(TAN('Solar Altitude'!E37)/COS('Surface Solar Azimuth Angles'!S36))","v":0.18024728429187561},{"$f":"ATAN(TAN('Solar Altitude'!F37)/COS('Surface Solar Azimuth Angles'!T36))","v":0.2992650966321978},{"$f":"ATAN(TAN('Solar Altitude'!G37)/COS('Surface Solar Azimuth Angles'!U36))","v":0.36886077540021189},{"$f":"ATAN(TAN('Solar Altitude'!H37)/COS('Surface Solar Azimuth Angles'!V36))","v":0.37484605769803392},{"$f":"ATAN(TAN('Solar Altitude'!I37)/COS('Surface Solar Azimuth Angles'!W36))","v":0.33410836517870202},{"$f":"ATAN(TAN('Solar Altitude'!J37)/COS('Surface Solar Azimuth Angles'!X36))","v":0.28700384937592222},{"$f":"ATAN(TAN('Solar Altitude'!K37)/COS('Surface Solar Azimuth Angles'!Y36))","v":0.24026026153093516},{"$f":"ATAN(TAN('Solar Altitude'!L37)/COS('Surface Solar Azimuth Angles'!Z36))","v":0.1938557876010461},{"$f":"ATAN(TAN('Solar Altitude'!M37)/COS('Surface Solar Azimuth Angles'!AA36))","v":0.11359911050913243},{"$f":"ATAN(TAN('Solar Altitude'!N37)/COS('Surface Solar Azimuth Angles'!AB36))","v":3.3555975837619691E-2},null,7,{"$f":"ATAN(TAN('Solar Altitude'!C37)/COS('Surface Solar Azimuth Angles'!C91))","v":-1.3214305906891738E-2},{"$f":"ATAN(TAN('Solar Altitude'!D37)/COS('Surface Solar Azimuth Angles'!D91))","v":-7.6478952342661624E-2},{"$f":"ATAN(TAN('Solar Altitude'!E37)/COS('Surface Solar Azimuth Angles'!E91))","v":-0.18024728429187561},{"$f":"ATAN(TAN('Solar Altitude'!F37)/COS('Surface Solar Azimuth Angles'!F91))","v":-0.2992650966321978},{"$f":"ATAN(TAN('Solar Altitude'!G37)/COS('Surface Solar Azimuth Angles'!G91))","v":-0.36886077540021189},{"$f":"ATAN(TAN('Solar Altitude'!H37)/COS('Surface Solar Azimuth Angles'!H91))","v":-0.37484605769803392},{"$f":"ATAN(TAN('Solar Altitude'!I37)/COS('Surface Solar Azimuth Angles'!I91))","v":-0.33410836517870202},{"$f":"ATAN(TAN('Solar Altitude'!J37)/COS('Surface Solar Azimuth Angles'!J91))","v":-0.28700384937592222},{"$f":"ATAN(TAN('Solar Altitude'!K37)/COS('Surface Solar Azimuth Angles'!K91))","v":-0.24026026153093516},{"$f":"ATAN(TAN('Solar Altitude'!L37)/COS('Surface Solar Azimuth Angles'!L91))","v":-0.1938557876010461},{"$f":"ATAN(TAN('Solar Altitude'!M37)/COS('Surface Solar Azimuth Angles'!M91))","v":-0.11359911050913243},{"$f":"ATAN(TAN('Solar Altitude'!N37)/COS('Surface Solar Azimuth Angles'!N91))","v":-3.3555975837619691E-2},null,7,{"$f":"ATAN(TAN('Solar Altitude'!C37)/COS('Surface Solar Azimuth Angles'!Q91))","v":-3.2126378124526914E-2},{"$f":"ATAN(TAN('Solar Altitude'!D37)/COS('Surface Solar Azimuth Angles'!R91))","v":-0.30400417987737716},{"$f":"ATAN(TAN('Solar Altitude'!E37)/COS('Surface Solar Azimuth Angles'!S91))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F37)/COS('Surface Solar Azimuth Angles'!T91))","v":1.2672818655170024},{"$f":"ATAN(TAN('Solar Altitude'!G37)/COS('Surface Solar Azimuth Angles'!U91))","v":1.0116130508303161},{"$f":"ATAN(TAN('Solar Altitude'!H37)/COS('Surface Solar Azimuth Angles'!V91))","v":0.90537507022991526},{"$f":"ATAN(TAN('Solar Altitude'!I37)/COS('Surface Solar Azimuth Angles'!W91))","v":0.92689168179647385},{"$f":"ATAN(TAN('Solar Altitude'!J37)/COS('Surface Solar Azimuth Angles'!X91))","v":1.2258417459156572},{"$f":"ATAN(TAN('Solar Altitude'!K37)/COS('Surface Solar Azimuth Angles'!Y91))","v":-1.1397000015522976},{"$f":"ATAN(TAN('Solar Altitude'!L37)/COS('Surface Solar Azimuth Angles'!Z91))","v":-0.56767922585481523},{"$f":"ATAN(TAN('Solar Altitude'!M37)/COS('Surface Solar Azimuth Angles'!AA91))","v":-0.23892272571930678},{"$f":"ATAN(TAN('Solar Altitude'!N37)/COS('Surface Solar Azimuth Angles'!AB91))","v":-6.6151862638080941E-2}]
[null,8,{"$f":"ATAN(TAN('Solar Altitude'!C38)/COS('Surface Solar Azimuth Angles'!C37))","v":0.43903721208086555},{"$f":"ATAN(TAN('Solar Altitude'!D38)/COS('Surface Solar Azimuth Angles'!D37))","v":0.71921811629902932},{"$f":"ATAN(TAN('Solar Altitude'!E38)/COS('Surface Solar Azimuth Angles'!E37))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F38)/COS('Surface Solar Azimuth Angles'!F37))","v":1.5556802149681459},{"$f":"ATAN(TAN('Solar Altitude'!G38)/COS('Surface Solar Azimuth Angles'!G37))","v":-1.3507534128601013},{"$f":"ATAN(TAN('Solar Altitude'!H38)/COS('Surface Solar Azimuth Angles'!H37))","v":-1.2538060729022262},{"$f":"ATAN(TAN('Solar Altitude'!I38)/COS('Surface Solar Azimuth Angles'!I37))","v":-1.3073051411080621},{"$f":"ATAN(TAN('Solar Altitude'!J38)/COS('Surface Solar Azimuth Angles'!J37))","v":-1.5687141806333271},{"$f":"ATAN(TAN('Solar Altitude'!K38)/COS('Surface Solar Azimuth Angles'!K37))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L38)/COS('Surface Solar Azimuth Angles'!L37))","v":0.7977743448011565},{"$f":"ATAN(TAN('Solar Altitude'!M38)/COS('Surface Solar Azimuth Angles'!M37))","v":0.53602537178498577},{"$f":"ATAN(TAN('Solar Altitude'!N38)/COS('Surface Solar Azimuth Angles'!N37))","v":0.40375311848675605},null,8,{"$f":"ATAN(TAN('Solar Altitude'!C38)/COS('Surface Solar Azimuth Angles'!Q37))","v":0.25833513602163805},{"$f":"ATAN(TAN('Solar Altitude'!D38)/COS('Surface Solar Azimuth Angles'!R37))","v":0.3210561315745496},{"$f":"ATAN(TAN('Solar Altitude'!E38)/COS('Surface Solar Azimuth Angles'!S37))","v":0.42271676310413814},{"$f":"ATAN(TAN('Solar Altitude'!F38)/COS('Surface Solar Azimuth Angles'!T37))","v":0.53547976766771499},{"$f":"ATAN(TAN('Solar Altitude'!G38)/COS('Surface Solar Azimuth Angles'!U37))","v":0.59803922283315158},{"$f":"ATAN(TAN('Solar Altitude'!H38)/COS('Surface Solar Azimuth Angles'!V37))","v":0.600853618256177},{"$f":"ATAN(TAN('Solar Altitude'!I38)/COS('Surface Solar Azimuth Angles'!W37))","v":0.5629740216332968},{"$f":"ATAN(TAN('Solar Altitude'!J38)/COS('Surface Solar Azimuth Angles'!X37))","v":0.52288181283223811},{"$f":"ATAN(TAN('Solar Altitude'!K38)/COS('Surface Solar Azimuth Angles'!Y37))","v":0.484596524210885},{"$f":"ATAN(TAN('Solar Altitude'!L38)/COS('Surface Solar Azimuth Angles'!Z37))","v":0.44426219941003875},{"$f":"ATAN(TAN('Solar Altitude'!M38)/COS('Surface Solar Azimuth Angles'!AA37))","v":0.36546054525287114},{"$f":"ATAN(TAN('Solar Altitude'!N38)/COS('Surface Solar Azimuth Angles'!AB37))","v":0.28151379860305881},null,8,{"$f":"ATAN(TAN('Solar Altitude'!C38)/COS('Surface Solar Azimuth Angles'!C92))","v":-0.25833513602163805},{"$f":"ATAN(TAN('Solar Altitude'!D38)/COS('Surface Solar Azimuth Angles'!D92))","v":-0.32105613157454954},{"$f":"ATAN(TAN('Solar Altitude'!E38)/COS('Surface Solar Azimuth Angles'!E92))","v":-0.42271676310413814},{"$f":"ATAN(TAN('Solar Altitude'!F38)/COS('Surface Solar Azimuth Angles'!F92))","v":-0.53547976766771499},{"$f":"ATAN(TAN('Solar Altitude'!G38)/COS('Surface Solar Azimuth Angles'!G92))","v":-0.59803922283315158},{"$f":"ATAN(TAN('Solar Altitude'!H38)/COS('Surface Solar Azimuth Angles'!H92))","v":-0.600853618256177},{"$f":"ATAN(TAN('Solar Altitude'!I38)/COS('Surface Solar Azimuth Angles'!I92))","v":-0.5629740216332968},{"$f":"ATAN(TAN('Solar Altitude'!J38)/COS('Surface Solar Azimuth Angles'!J92))","v":-0.52288181283223811},{"$f":"ATAN(TAN('Solar Altitude'!K38)/COS('Surface Solar Azimuth Angles'!K92))","v":-0.484596524210885},{"$f":"ATAN(TAN('Solar Altitude'!L38)/COS('Surface Solar Azimuth Angles'!L92))","v":-0.4442621994100388},{"$f":"ATAN(TAN('Solar Altitude'!M38)/COS('Surface Solar Azimuth Angles'!M92))","v":-0.36546054525287114},{"$f":"ATAN(TAN('Solar Altitude'!N38)/COS('Surface Solar Azimuth Angles'!N92))","v":-0.28151379860305881},null,8,{"$f":"ATAN(TAN('Solar Altitude'!C38)/COS('Surface Solar Azimuth Angles'!Q92))","v":-0.43903721208086544},{"$f":"ATAN(TAN('Solar Altitude'!D38)/COS('Surface Solar Azimuth Angles'!R92))","v":-0.71921811629902943},{"$f":"ATAN(TAN('Solar Altitude'!E38)/COS('Surface Solar Azimuth Angles'!S92))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F38)/COS('Surface Solar Azimuth Angles'!T92))","v":-1.5556802149681459},{"$f":"ATAN(TAN('Solar Altitude'!G38)/COS('Surface Solar Azimuth Angles'!U92))","v":1.3507534128601013},{"$f":"ATAN(TAN('Solar Altitude'!H38)/COS('Surface Solar Azimuth Angles'!V92))","v":1.253806072902226},{"$f":"ATAN(TAN('Solar Altitude'!I38)/COS('Surface Solar Azimuth Angles'!W92))","v":1.3073051411080618},{"$f":"ATAN(TAN('Solar Altitude'!J38)/COS('Surface Solar Azimuth Angles'!X92))","v":1.5687141806333269},{"$f":"ATAN(TAN('Solar Altitude'!K38)/COS('Surface Solar Azimuth Angles'!Y92))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L38)/COS('Surface Solar Azimuth Angles'!Z92))","v":-0.7977743448011565},{"$f":"ATAN(TAN('Solar Altitude'!M38)/COS('Surface Solar Azimuth Angles'!AA92))","v":-0.53602537178498588},{"$f":"ATAN(TAN('Solar Altitude'!N38)/COS('Surface Solar Azimuth Angles'!AB92))","v":-0.40375311848675605}]
[null,9,{"$f":"ATAN(TAN('Solar Altitude'!C39)/COS('Surface Solar Azimuth Angles'!C38))","v":0.63047626333736551},{"$f":"ATAN(TAN('Solar Altitude'!D39)/COS('Surface Solar Azimuth Angles'!D38))","v":0.85493388322458164},{"$f":"ATAN(TAN('Solar Altitude'!E39)/COS('Surface Solar Azimuth Angles'!E38))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F39)/COS('Surface Solar Azimuth Angles'!F38))","v":1.4368234130045157},{"$f":"ATAN(TAN('Solar Altitude'!G39)/COS('Surface Solar Azimuth Angles'!G38))","v":-1.5128901286207532},{"$f":"ATAN(TAN('Solar Altitude'!H39)/COS('Surface Solar Azimuth Angles'!H38))","v":-1.4342637641927436},{"$f":"ATAN(TAN('Solar Altitude'!I39)/COS('Surface Solar Azimuth Angles'!I38))","v":-1.4895751772040409},{"$f":"ATAN(TAN('Solar Altitude'!J39)/COS('Surface Solar Azimuth Angles'!J38))","v":1.4463354753784508},{"$f":"ATAN(TAN('Solar Altitude'!K39)/COS('Surface Solar Azimuth Angles'!K38))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L39)/COS('Surface Solar Azimuth Angles'!L38))","v":0.88713181190644852},{"$f":"ATAN(TAN('Solar Altitude'!M39)/COS('Surface Solar Azimuth Angles'!M38))","v":0.67791492684215882},{"$f":"ATAN(TAN('Solar Altitude'!N39)/COS('Surface Solar Azimuth Angles'!N38))","v":0.57836247588490297},null,9,{"$f":"ATAN(TAN('Solar Altitude'!C39)/COS('Surface Solar Azimuth Angles'!Q38))","v":0.52181610509407761},{"$f":"ATAN(TAN('Solar Altitude'!D39)/COS('Surface Solar Azimuth Angles'!R38))","v":0.57895326435114869},{"$f":"ATAN(TAN('Solar Altitude'!E39)/COS('Surface Solar Azimuth Angles'!S38))","v":0.6743232952298458},{"$f":"ATAN(TAN('Solar Altitude'!F39)/COS('Surface Solar Azimuth Angles'!T38))","v":0.77696351285009757},{"$f":"ATAN(TAN('Solar Altitude'!G39)/COS('Surface Solar Azimuth Angles'!U38))","v":0.83009780925872145},{"$f":"ATAN(TAN('Solar Altitude'!H39)/COS('Surface Solar Azimuth Angles'!V38))","v":0.82868950102189065},{"$f":"ATAN(TAN('Solar Altitude'!I39)/COS('Surface Solar Azimuth Angles'!W38))","v":0.79414344815942139},{"$f":"ATAN(TAN('Solar Altitude'!J39)/COS('Surface Solar Azimuth Angles'!X38))","v":0.76376137451897885},{"$f":"ATAN(TAN('Solar Altitude'!K39)/COS('Surface Solar Azimuth Angles'!Y38))","v":0.73908870770470347},{"$f":"ATAN(TAN('Solar Altitude'!L39)/COS('Surface Solar Azimuth Angles'!Z38))","v":0.71062378761726053},{"$f":"ATAN(TAN('Solar Altitude'!M39)/COS('Surface Solar Azimuth Angles'!AA38))","v":0.6387070204210934},{"$f":"ATAN(TAN('Solar Altitude'!N39)/COS('Surface Solar Azimuth Angles'!AB38))","v":0.55159011300440908},null,9,{"$f":"ATAN(TAN('Solar Altitude'!C39)/COS('Surface Solar Azimuth Angles'!C93))","v":-0.52181610509407761},{"$f":"ATAN(TAN('Solar Altitude'!D39)/COS('Surface Solar Azimuth Angles'!D93))","v":-0.57895326435114869},{"$f":"ATAN(TAN('Solar Altitude'!E39)/COS('Surface Solar Azimuth Angles'!E93))","v":-0.6743232952298458},{"$f":"ATAN(TAN('Solar Altitude'!F39)/COS('Surface Solar Azimuth Angles'!F93))","v":-0.77696351285009757},{"$f":"ATAN(TAN('Solar Altitude'!G39)/COS('Surface Solar Azimuth Angles'!G93))","v":-0.83009780925872145},{"$f":"ATAN(TAN('Solar Altitude'!H39)/COS('Surface Solar Azimuth Angles'!H93))","v":-0.82868950102189065},{"$f":"ATAN(TAN('Solar Altitude'!I39)/COS('Surface Solar Azimuth Angles'!I93))","v":-0.79414344815942139},{"$f":"ATAN(TAN('Solar Altitude'!J39)/COS('Surface Solar Azimuth Angles'!J93))","v":-0.76376137451897885},{"$f":"ATAN(TAN('Solar Altitude'!K39)/COS('Surface Solar Azimuth Angles'!K93))","v":-0.73908870770470347},{"$f":"ATAN(TAN('Solar Altitude'!L39)/COS('Surface Solar Azimuth Angles'!L93))","v":-0.71062378761726053},{"$f":"ATAN(TAN('Solar Altitude'!M39)/COS('Surface Solar Azimuth Angles'!M93))","v":-0.6387070204210934},{"$f":"ATAN(TAN('Solar Altitude'!N39)/COS('Surface Solar Azimuth Angles'!N93))","v":-0.55159011300440908},null,9,{"$f":"ATAN(TAN('Solar Altitude'!C39)/COS('Surface Solar Azimuth Angles'!Q93))","v":-0.63047626333736551},{"$f":"ATAN(TAN('Solar Altitude'!D39)/COS('Surface Solar Azimuth Angles'!R93))","v":-0.85493388322458175},{"$f":"ATAN(TAN('Solar Altitude'!E39)/COS('Surface Solar Azimuth Angles'!S93))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F39)/COS('Surface Solar Azimuth Angles'!T93))","v":-1.4368234130045159},{"$f":"ATAN(TAN('Solar Altitude'!G39)/COS('Surface Solar Azimuth Angles'!U93))","v":1.5128901286207532},{"$f":"ATAN(TAN('Solar Altitude'!H39)/COS('Surface Solar Azimuth Angles'!V93))","v":1.4342637641927438},{"$f":"ATAN(TAN('Solar Altitude'!I39)/COS('Surface Solar Azimuth Angles'!W93))","v":1.4895751772040409},{"$f":"ATAN(TAN('Solar Altitude'!J39)/COS('Surface Solar Azimuth Angles'!X93))","v":-1.4463354753784505},{"$f":"ATAN(TAN('Solar Altitude'!K39)/COS('Surface Solar Azimuth Angles'!Y93))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L39)/COS('Surface Solar Azimuth Angles'!Z93))","v":-0.88713181190644852},{"$f":"ATAN(TAN('Solar Altitude'!M39)/COS('Surface Solar Azimuth Angles'!AA93))","v":-0.67791492684215893},{"$f":"ATAN(TAN('Solar Altitude'!N39)/COS('Surface Solar Azimuth Angles'!AB93))","v":-0.57836247588490308}]
[null,10,{"$f":"ATAN(TAN('Solar Altitude'!C40)/COS('Surface Solar Azimuth Angles'!C39))","v":0.72545541534435543},{"$f":"ATAN(TAN('Solar Altitude'!D40)/COS('Surface Solar Azimuth Angles'!D39))","v":0.91440329211687621},{"$f":"ATAN(TAN('Solar Altitude'!E40)/COS('Surface Solar Azimuth Angles'!E39))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F40)/COS('Surface Solar Azimuth Angles'!F39))","v":1.3820186383289426},{"$f":"ATAN(TAN('Solar Altitude'!G40)/COS('Surface Solar Azimuth Angles'!G39))","v":1.5469473133771072},{"$f":"ATAN(TAN('Solar Altitude'!H40)/COS('Surface Solar Azimuth Angles'!H39))","v":-1.52849748779825},{"$f":"ATAN(TAN('Solar Altitude'!I40)/COS('Surface Solar Azimuth Angles'!I39))","v":1.5604768548046379},{"$f":"ATAN(TAN('Solar Altitude'!J40)/COS('Surface Solar Azimuth Angles'!J39))","v":1.388309158935473},{"$f":"ATAN(TAN('Solar Altitude'!K40)/COS('Surface Solar Azimuth Angles'!K39))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L40)/COS('Surface Solar Azimuth Angles'!L39))","v":0.92900496630503893},{"$f":"ATAN(TAN('Solar Altitude'!M40)/COS('Surface Solar Azimuth Angles'!M39))","v":0.7495213445099127},{"$f":"ATAN(TAN('Solar Altitude'!N40)/COS('Surface Solar Azimuth Angles'!N39))","v":0.66958505956359171},null,10,{"$f":"ATAN(TAN('Solar Altitude'!C40)/COS('Surface Solar Azimuth Angles'!Q39))","v":0.8103914470438931},{"$f":"ATAN(TAN('Solar Altitude'!D40)/COS('Surface Solar Azimuth Angles'!R39))","v":0.85489906581681796},{"$f":"ATAN(TAN('Solar Altitude'!E40)/COS('Surface Solar Azimuth Angles'!S39))","v":0.93831409714073843},{"$f":"ATAN(TAN('Solar Altitude'!F40)/COS('Surface Solar Azimuth Angles'!T39))","v":1.0260828135826863},{"$f":"ATAN(TAN('Solar Altitude'!G40)/COS('Surface Solar Azimuth Angles'!U39))","v":1.0672108131256053},{"$f":"ATAN(TAN('Solar Altitude'!H40)/COS('Surface Solar Azimuth Angles'!V39))","v":1.0606626288594174},{"$f":"ATAN(TAN('Solar Altitude'!I40)/COS('Surface Solar Azimuth Angles'!W39))","v":1.0301037196118754},{"$f":"ATAN(TAN('Solar Altitude'!J40)/COS('Surface Solar Azimuth Angles'!X39))","v":1.0121306417701839},{"$f":"ATAN(TAN('Solar Altitude'!K40)/COS('Surface Solar Azimuth Angles'!Y39))","v":1.0063600686241212},{"$f":"ATAN(TAN('Solar Altitude'!L40)/COS('Surface Solar Azimuth Angles'!Z39))","v":0.99633099553482729},{"$f":"ATAN(TAN('Solar Altitude'!M40)/COS('Surface Solar Azimuth Angles'!AA39))","v":0.93894687408658395},{"$f":"ATAN(TAN('Solar Altitude'!N40)/COS('Surface Solar Azimuth Angles'!AB39))","v":0.85128249562502745},null,10,{"$f":"ATAN(TAN('Solar Altitude'!C40)/COS('Surface Solar Azimuth Angles'!C94))","v":-0.8103914470438931},{"$f":"ATAN(TAN('Solar Altitude'!D40)/COS('Surface Solar Azimuth Angles'!D94))","v":-0.85489906581681818},{"$f":"ATAN(TAN('Solar Altitude'!E40)/COS('Surface Solar Azimuth Angles'!E94))","v":-0.93831409714073843},{"$f":"ATAN(TAN('Solar Altitude'!F40)/COS('Surface Solar Azimuth Angles'!F94))","v":-1.0260828135826865},{"$f":"ATAN(TAN('Solar Altitude'!G40)/COS('Surface Solar Azimuth Angles'!G94))","v":-1.0672108131256053},{"$f":"ATAN(TAN('Solar Altitude'!H40)/COS('Surface Solar Azimuth Angles'!H94))","v":-1.0606626288594174},{"$f":"ATAN(TAN('Solar Altitude'!I40)/COS('Surface Solar Azimuth Angles'!I94))","v":-1.0301037196118754},{"$f":"ATAN(TAN('Solar Altitude'!J40)/COS('Surface Solar Azimuth Angles'!J94))","v":-1.0121306417701839},{"$f":"ATAN(TAN('Solar Altitude'!K40)/COS('Surface Solar Azimuth Angles'!K94))","v":-1.0063600686241212},{"$f":"ATAN(TAN('Solar Altitude'!L40)/COS('Surface Solar Azimuth Angles'!L94))","v":-0.99633099553482729},{"$f":"ATAN(TAN('Solar Altitude'!M40)/COS('Surface Solar Azimuth Angles'!M94))","v":-0.93894687408658395},{"$f":"ATAN(TAN('Solar Altitude'!N40)/COS('Surface Solar Azimuth Angles'!N94))","v":-0.85128249562502767},null,10,{"$f":"ATAN(TAN('Solar Altitude'!C40)/COS('Surface Solar Azimuth Angles'!Q94))","v":-0.7254554153443552},{"$f":"ATAN(TAN('Solar Altitude'!D40)/COS('Surface Solar Azimuth Angles'!R94))","v":-0.9144032921168761},{"$f":"ATAN(TAN('Solar Altitude'!E40)/COS('Surface Solar Azimuth Angles'!S94))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F40)/COS('Surface Solar Azimuth Angles'!T94))","v":-1.3820186383289426},{"$f":"ATAN(TAN('Solar Altitude'!G40)/COS('Surface Solar Azimuth Angles'!U94))","v":-1.5469473133771072},{"$f":"ATAN(TAN('Solar Altitude'!H40)/COS('Surface Solar Azimuth Angles'!V94))","v":1.52849748779825},{"$f":"ATAN(TAN('Solar Altitude'!I40)/COS('Surface Solar Azimuth Angles'!W94))","v":-1.5604768548046379},{"$f":"ATAN(TAN('Solar Altitude'!J40)/COS('Surface Solar Azimuth Angles'!X94))","v":-1.388309158935473},{"$f":"ATAN(TAN('Solar Altitude'!K40)/COS('Surface Solar Azimuth Angles'!Y94))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L40)/COS('Surface Solar Azimuth Angles'!Z94))","v":-0.92900496630503882},{"$f":"ATAN(TAN('Solar Altitude'!M40)/COS('Surface Solar Azimuth Angles'!AA94))","v":-0.7495213445099127},{"$f":"ATAN(TAN('Solar Altitude'!N40)/COS('Surface Solar Azimuth Angles'!AB94))","v":-0.66958505956359182}]
[null,11,{"$f":"ATAN(TAN('Solar Altitude'!C41)/COS('Surface Solar Azimuth Angles'!C40))","v":0.77287050251262801},{"$f":"ATAN(TAN('Solar Altitude'!D41)/COS('Surface Solar Azimuth Angles'!D40))","v":0.94279982780897675},{"$f":"ATAN(TAN('Solar Altitude'!E41)/COS('Surface Solar Azimuth Angles'!E40))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F41)/COS('Surface Solar Azimuth Angles'!F40))","v":1.3560531209708369},{"$f":"ATAN(TAN('Solar Altitude'!G41)/COS('Surface Solar Azimuth Angles'!G40))","v":1.5069809238556895},{"$f":"ATAN(TAN('Solar Altitude'!H41)/COS('Surface Solar Azimuth Angles'!H40))","v":1.5658083868258721},{"$f":"ATAN(TAN('Solar Altitude'!I41)/COS('Surface Solar Azimuth Angles'!I40))","v":1.5149166606406734},{"$f":"ATAN(TAN('Solar Altitude'!J41)/COS('Surface Solar Azimuth Angles'!J40))","v":1.3606731060385544},{"$f":"ATAN(TAN('Solar Altitude'!K41)/COS('Surface Solar Azimuth Angles'!K40))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L41)/COS('Surface Solar Azimuth Angles'!L40))","v":0.94820534202278628},{"$f":"ATAN(TAN('Solar Altitude'!M41)/COS('Surface Solar Azimuth Angles'!M40))","v":0.78354196814002852},{"$f":"ATAN(TAN('Solar Altitude'!N41)/COS('Surface Solar Azimuth Angles'!N40))","v":0.71507325853303161},null,11,{"$f":"ATAN(TAN('Solar Altitude'!C41)/COS('Surface Solar Azimuth Angles'!Q40))","v":1.1268272200794016},{"$f":"ATAN(TAN('Solar Altitude'!D41)/COS('Surface Solar Azimuth Angles'!R40))","v":1.1501949201099215},{"$f":"ATAN(TAN('Solar Altitude'!E41)/COS('Surface Solar Azimuth Angles'!S40))","v":1.2149427363314722},{"$f":"ATAN(TAN('Solar Altitude'!F41)/COS('Surface Solar Azimuth Angles'!T40))","v":1.2827675748177341},{"$f":"ATAN(TAN('Solar Altitude'!G41)/COS('Surface Solar Azimuth Angles'!U40))","v":1.3094800079043547},{"$f":"ATAN(TAN('Solar Altitude'!H41)/COS('Surface Solar Azimuth Angles'!V40))","v":1.2971248839107501},{"$f":"ATAN(TAN('Solar Altitude'!I41)/COS('Surface Solar Azimuth Angles'!W40))","v":1.2712928251657776},{"$f":"ATAN(TAN('Solar Altitude'!J41)/COS('Surface Solar Azimuth Angles'!X40))","v":1.2680765910530094},{"$f":"ATAN(TAN('Solar Altitude'!K41)/COS('Surface Solar Azimuth Angles'!Y40))","v":1.2857310025410149},{"$f":"ATAN(TAN('Solar Altitude'!L41)/COS('Surface Solar Azimuth Angles'!Z40))","v":1.3000930619226609},{"$f":"ATAN(TAN('Solar Altitude'!M41)/COS('Surface Solar Azimuth Angles'!AA40))","v":1.2658856481778871},{"$f":"ATAN(TAN('Solar Altitude'!N41)/COS('Surface Solar Azimuth Angles'!AB40))","v":1.1829208364741319},null,11,{"$f":"ATAN(TAN('Solar Altitude'!C41)/COS('Surface Solar Azimuth Angles'!C95))","v":-1.1268272200794018},{"$f":"ATAN(TAN('Solar Altitude'!D41)/COS('Surface Solar Azimuth Angles'!D95))","v":-1.1501949201099215},{"$f":"ATAN(TAN('Solar Altitude'!E41)/COS('Surface Solar Azimuth Angles'!E95))","v":-1.2149427363314722},{"$f":"ATAN(TAN('Solar Altitude'!F41)/COS('Surface Solar Azimuth Angles'!F95))","v":-1.2827675748177341},{"$f":"ATAN(TAN('Solar Altitude'!G41)/COS('Surface Solar Azimuth Angles'!G95))","v":-1.3094800079043547},{"$f":"ATAN(TAN('Solar Altitude'!H41)/COS('Surface Solar Azimuth Angles'!H95))","v":-1.2971248839107501},{"$f":"ATAN(TAN('Solar Altitude'!I41)/COS('Surface Solar Azimuth Angles'!I95))","v":-1.2712928251657776},{"$f":"ATAN(TAN('Solar Altitude'!J41)/COS('Surface Solar Azimuth Angles'!J95))","v":-1.2680765910530094},{"$f":"ATAN(TAN('Solar Altitude'!K41)/COS('Surface Solar Azimuth Angles'!K95))","v":-1.2857310025410147},{"$f":"ATAN(TAN('Solar Altitude'!L41)/COS('Surface Solar Azimuth Angles'!L95))","v":-1.3000930619226607},{"$f":"ATAN(TAN('Solar Altitude'!M41)/COS('Surface Solar Azimuth Angles'!M95))","v":-1.2658856481778873},{"$f":"ATAN(TAN('Solar Altitude'!N41)/COS('Surface Solar Azimuth Angles'!N95))","v":-1.1829208364741319},null,11,{"$f":"ATAN(TAN('Solar Altitude'!C41)/COS('Surface Solar Azimuth Angles'!Q95))","v":-0.77287050251262801},{"$f":"ATAN(TAN('Solar Altitude'!D41)/COS('Surface Solar Azimuth Angles'!R95))","v":-0.94279982780897686},{"$f":"ATAN(TAN('Solar Altitude'!E41)/COS('Surface Solar Azimuth Angles'!S95))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F41)/COS('Surface Solar Azimuth Angles'!T95))","v":-1.3560531209708369},{"$f":"ATAN(TAN('Solar Altitude'!G41)/COS('Surface Solar Azimuth Angles'!U95))","v":-1.5069809238556895},{"$f":"ATAN(TAN('Solar Altitude'!H41)/COS('Surface Solar Azimuth Angles'!V95))","v":-1.5658083868258723},{"$f":"ATAN(TAN('Solar Altitude'!I41)/COS('Surface Solar Azimuth Angles'!W95))","v":-1.5149166606406737},{"$f":"ATAN(TAN('Solar Altitude'!J41)/COS('Surface Solar Azimuth Angles'!X95))","v":-1.3606731060385544},{"$f":"ATAN(TAN('Solar Altitude'!K41)/COS('Surface Solar Azimuth Angles'!Y95))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L41)/COS('Surface Solar Azimuth Angles'!Z95))","v":-0.94820534202278628},{"$f":"ATAN(TAN('Solar Altitude'!M41)/COS('Surface Solar Azimuth Angles'!AA95))","v":-0.78354196814002852},{"$f":"ATAN(TAN('Solar Altitude'!N41)/COS('Surface Solar Azimuth Angles'!AB95))","v":-0.71507325853303161}]
[null,12,{"$f":"ATAN(TAN('Solar Altitude'!C42)/COS('Surface Solar Azimuth Angles'!C41))","v":0.79135309629409833},{"$f":"ATAN(TAN('Solar Altitude'!D42)/COS('Surface Solar Azimuth Angles'!D41))","v":0.95393106557871743},{"$f":"ATAN(TAN('Solar Altitude'!E42)/COS('Surface Solar Azimuth Angles'!E41))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F42)/COS('Surface Solar Azimuth Angles'!F41))","v":1.3474641185275609},{"$f":"ATAN(TAN('Solar Altitude'!G42)/COS('Surface Solar Azimuth Angles'!G41))","v":1.494047359637104},{"$f":"ATAN(TAN('Solar Altitude'!H42)/COS('Surface Solar Azimuth Angles'!H41))","v":1.5492328942973228},{"$f":"ATAN(TAN('Solar Altitude'!I42)/COS('Surface Solar Azimuth Angles'!I41))","v":1.498048297172524},{"$f":"ATAN(TAN('Solar Altitude'!J42)/COS('Surface Solar Azimuth Angles'!J41))","v":1.3510622858662447},{"$f":"ATAN(TAN('Solar Altitude'!K42)/COS('Surface Solar Azimuth Angles'!K41))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L42)/COS('Surface Solar Azimuth Angles'!L41))","v":0.95283102870472114},{"$f":"ATAN(TAN('Solar Altitude'!M42)/COS('Surface Solar Azimuth Angles'!M41))","v":0.79224403056524906},{"$f":"ATAN(TAN('Solar Altitude'!N42)/COS('Surface Solar Azimuth Angles'!N41))","v":0.73031386460610437},null,12,{"$f":"ATAN(TAN('Solar Altitude'!C42)/COS('Surface Solar Azimuth Angles'!Q41))","v":1.4652572312778287},{"$f":"ATAN(TAN('Solar Altitude'!D42)/COS('Surface Solar Azimuth Angles'!R41))","v":1.4603602289474145},{"$f":"ATAN(TAN('Solar Altitude'!E42)/COS('Surface Solar Azimuth Angles'!S41))","v":1.5005364967084425},{"$f":"ATAN(TAN('Solar Altitude'!F42)/COS('Surface Solar Azimuth Angles'!T41))","v":1.5443810972198109},{"$f":"ATAN(TAN('Solar Altitude'!G42)/COS('Surface Solar Azimuth Angles'!U41))","v":1.555062909254763},{"$f":"ATAN(TAN('Solar Altitude'!H42)/COS('Surface Solar Azimuth Angles'!V41))","v":1.536631166126466},{"$f":"ATAN(TAN('Solar Altitude'!I42)/COS('Surface Solar Azimuth Angles'!W41))","v":1.5161625036324029},{"$f":"ATAN(TAN('Solar Altitude'!J42)/COS('Surface Solar Azimuth Angles'!X41))","v":1.5291230837920122},{"$f":"ATAN(TAN('Solar Altitude'!K42)/COS('Surface Solar Azimuth Angles'!Y41))","v":1.5690353246394675},{"$f":"ATAN(TAN('Solar Altitude'!L42)/COS('Surface Solar Azimuth Angles'!Z41))","v":1.5273206771977748},{"$f":"ATAN(TAN('Solar Altitude'!M42)/COS('Surface Solar Azimuth Angles'!AA41))","v":1.5323869921532096},{"$f":"ATAN(TAN('Solar Altitude'!N42)/COS('Surface Solar Azimuth Angles'!AB41))","v":1.537600907178335},null,12,{"$f":"ATAN(TAN('Solar Altitude'!C42)/COS('Surface Solar Azimuth Angles'!C96))","v":-1.4652572312778289},{"$f":"ATAN(TAN('Solar Altitude'!D42)/COS('Surface Solar Azimuth Angles'!D96))","v":-1.4603602289474145},{"$f":"ATAN(TAN('Solar Altitude'!E42)/COS('Surface Solar Azimuth Angles'!E96))","v":-1.5005364967084425},{"$f":"ATAN(TAN('Solar Altitude'!F42)/COS('Surface Solar Azimuth Angles'!F96))","v":-1.5443810972198109},{"$f":"ATAN(TAN('Solar Altitude'!G42)/COS('Surface Solar Azimuth Angles'!G96))","v":-1.555062909254763},{"$f":"ATAN(TAN('Solar Altitude'!H42)/COS('Surface Solar Azimuth Angles'!H96))","v":-1.536631166126466},{"$f":"ATAN(TAN('Solar Altitude'!I42)/COS('Surface Solar Azimuth Angles'!I96))","v":-1.5161625036324029},{"$f":"ATAN(TAN('Solar Altitude'!J42)/COS('Surface Solar Azimuth Angles'!J96))","v":-1.5291230837920122},{"$f":"ATAN(TAN('Solar Altitude'!K42)/COS('Surface Solar Azimuth Angles'!K96))","v":-1.5690353246394675},{"$f":"ATAN(TAN('Solar Altitude'!L42)/COS('Surface Solar Azimuth Angles'!L96))","v":-1.5273206771977748},{"$f":"ATAN(TAN('Solar Altitude'!M42)/COS('Surface Solar Azimuth Angles'!M96))","v":-1.5323869921532096},{"$f":"ATAN(TAN('Solar Altitude'!N42)/COS('Surface Solar Azimuth Angles'!N96))","v":-1.5376009071783352},null,12,{"$f":"ATAN(TAN('Solar Altitude'!C42)/COS('Surface Solar Azimuth Angles'!Q96))","v":-0.79135309629409833},{"$f":"ATAN(TAN('Solar Altitude'!D42)/COS('Surface Solar Azimuth Angles'!R96))","v":-0.95393106557871743},{"$f":"ATAN(TAN('Solar Altitude'!E42)/COS('Surface Solar Azimuth Angles'!S96))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F42)/COS('Surface Solar Azimuth Angles'!T96))","v":-1.3474641185275609},{"$f":"ATAN(TAN('Solar Altitude'!G42)/COS('Surface Solar Azimuth Angles'!U96))","v":-1.494047359637104},{"$f":"ATAN(TAN('Solar Altitude'!H42)/COS('Surface Solar Azimuth Angles'!V96))","v":-1.5492328942973228},{"$f":"ATAN(TAN('Solar Altitude'!I42)/COS('Surface Solar Azimuth Angles'!W96))","v":-1.498048297172524},{"$f":"ATAN(TAN('Solar Altitude'!J42)/COS('Surface Solar Azimuth Angles'!X96))","v":-1.3510622858662447},{"$f":"ATAN(TAN('Solar Altitude'!K42)/COS('Surface Solar Azimuth Angles'!Y96))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L42)/COS('Surface Solar Azimuth Angles'!Z96))","v":-0.95283102870472114},{"$f":"ATAN(TAN('Solar Altitude'!M42)/COS('Surface Solar Azimuth Angles'!AA96))","v":-0.79224403056524906},{"$f":"ATAN(TAN('Solar Altitude'!N42)/COS('Surface Solar Azimuth Angles'!AB96))","v":-0.73031386460610437}]
[null,13,{"$f":"ATAN(TAN('Solar Altitude'!C43)/COS('Surface Solar Azimuth Angles'!C42))","v":0.78702668175259982},{"$f":"ATAN(TAN('Solar Altitude'!D43)/COS('Surface Solar Azimuth Angles'!D42))","v":0.95205108174928044},{"$f":"ATAN(TAN('Solar Altitude'!E43)/COS('Surface Solar Azimuth Angles'!E42))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F43)/COS('Surface Solar Azimuth Angles'!F42))","v":1.3531133844064995},{"$f":"ATAN(TAN('Solar Altitude'!G43)/COS('Surface Solar Azimuth Angles'!G42))","v":1.503986673926925},{"$f":"ATAN(TAN('Solar Altitude'!H43)/COS('Surface Solar Azimuth Angles'!H42))","v":1.558344195190098},{"$f":"ATAN(TAN('Solar Altitude'!I43)/COS('Surface Solar Azimuth Angles'!I42))","v":1.5043943771425594},{"$f":"ATAN(TAN('Solar Altitude'!J43)/COS('Surface Solar Azimuth Angles'!J42))","v":1.3559509038151709},{"$f":"ATAN(TAN('Solar Altitude'!K43)/COS('Surface Solar Azimuth Angles'!K42))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L43)/COS('Surface Solar Azimuth Angles'!L42))","v":0.94455934348747916},{"$f":"ATAN(TAN('Solar Altitude'!M43)/COS('Surface Solar Azimuth Angles'!M42))","v":0.77841604698882561},{"$f":"ATAN(TAN('Solar Altitude'!N43)/COS('Surface Solar Azimuth Angles'!N42))","v":0.71991055223641132},null,13,{"$f":"ATAN(TAN('Solar Altitude'!C43)/COS('Surface Solar Azimuth Angles'!Q42))","v":-1.331864871300116},{"$f":"ATAN(TAN('Solar Altitude'!D43)/COS('Surface Solar Azimuth Angles'!R42))","v":-1.3666270114598316},{"$f":"ATAN(TAN('Solar Altitude'!E43)/COS('Surface Solar Azimuth Angles'!S42))","v":-1.3535067192060635},{"$f":"ATAN(TAN('Solar Altitude'!F43)/COS('Surface Solar Azimuth Angles'!T42))","v":-1.3351101550303341},{"$f":"ATAN(TAN('Solar Altitude'!G43)/COS('Surface Solar Azimuth Angles'!U42))","v":-1.3407321893366535},{"$f":"ATAN(TAN('Solar Altitude'!H43)/COS('Surface Solar Azimuth Angles'!V42))","v":-1.3650413570281472},{"$f":"ATAN(TAN('Solar Altitude'!I43)/COS('Surface Solar Azimuth Angles'!W42))","v":-1.3798227453982828},{"$f":"ATAN(TAN('Solar Altitude'!J43)/COS('Surface Solar Azimuth Angles'!X42))","v":-1.3506595370421364},{"$f":"ATAN(TAN('Solar Altitude'!K43)/COS('Surface Solar Azimuth Angles'!Y42))","v":-1.2822582122157398},{"$f":"ATAN(TAN('Solar Altitude'!L43)/COS('Surface Solar Azimuth Angles'!Z42))","v":-1.2149101170192604},{"$f":"ATAN(TAN('Solar Altitude'!M43)/COS('Surface Solar Azimuth Angles'!AA42))","v":-1.1912817761692733},{"$f":"ATAN(TAN('Solar Altitude'!N43)/COS('Surface Solar Azimuth Angles'!AB42))","v":-1.2470964531741524},null,13,{"$f":"ATAN(TAN('Solar Altitude'!C43)/COS('Surface Solar Azimuth Angles'!C97))","v":1.3318648713001162},{"$f":"ATAN(TAN('Solar Altitude'!D43)/COS('Surface Solar Azimuth Angles'!D97))","v":1.3666270114598316},{"$f":"ATAN(TAN('Solar Altitude'!E43)/COS('Surface Solar Azimuth Angles'!E97))","v":1.3535067192060637},{"$f":"ATAN(TAN('Solar Altitude'!F43)/COS('Surface Solar Azimuth Angles'!F97))","v":1.3351101550303341},{"$f":"ATAN(TAN('Solar Altitude'!G43)/COS('Surface Solar Azimuth Angles'!G97))","v":1.3407321893366533},{"$f":"ATAN(TAN('Solar Altitude'!H43)/COS('Surface Solar Azimuth Angles'!H97))","v":1.3650413570281472},{"$f":"ATAN(TAN('Solar Altitude'!I43)/COS('Surface Solar Azimuth Angles'!I97))","v":1.3798227453982828},{"$f":"ATAN(TAN('Solar Altitude'!J43)/COS('Surface Solar Azimuth Angles'!J97))","v":1.3506595370421364},{"$f":"ATAN(TAN('Solar Altitude'!K43)/COS('Surface Solar Azimuth Angles'!K97))","v":1.2822582122157398},{"$f":"ATAN(TAN('Solar Altitude'!L43)/COS('Surface Solar Azimuth Angles'!L97))","v":1.2149101170192604},{"$f":"ATAN(TAN('Solar Altitude'!M43)/COS('Surface Solar Azimuth Angles'!M97))","v":1.1912817761692731},{"$f":"ATAN(TAN('Solar Altitude'!N43)/COS('Surface Solar Azimuth Angles'!N97))","v":1.2470964531741522},null,13,{"$f":"ATAN(TAN('Solar Altitude'!C43)/COS('Surface Solar Azimuth Angles'!Q97))","v":-0.78702668175259982},{"$f":"ATAN(TAN('Solar Altitude'!D43)/COS('Surface Solar Azimuth Angles'!R97))","v":-0.95205108174928044},{"$f":"ATAN(TAN('Solar Altitude'!E43)/COS('Surface Solar Azimuth Angles'!S97))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F43)/COS('Surface Solar Azimuth Angles'!T97))","v":-1.3531133844064993},{"$f":"ATAN(TAN('Solar Altitude'!G43)/COS('Surface Solar Azimuth Angles'!U97))","v":-1.503986673926925},{"$f":"ATAN(TAN('Solar Altitude'!H43)/COS('Surface Solar Azimuth Angles'!V97))","v":-1.558344195190098},{"$f":"ATAN(TAN('Solar Altitude'!I43)/COS('Surface Solar Azimuth Angles'!W97))","v":-1.5043943771425594},{"$f":"ATAN(TAN('Solar Altitude'!J43)/COS('Surface Solar Azimuth Angles'!X97))","v":-1.3559509038151709},{"$f":"ATAN(TAN('Solar Altitude'!K43)/COS('Surface Solar Azimuth Angles'!Y97))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L43)/COS('Surface Solar Azimuth Angles'!Z97))","v":-0.94455934348747916},{"$f":"ATAN(TAN('Solar Altitude'!M43)/COS('Surface Solar Azimuth Angles'!AA97))","v":-0.77841604698882561},{"$f":"ATAN(TAN('Solar Altitude'!N43)/COS('Surface Solar Azimuth Angles'!AB97))","v":-0.71991055223641132}]
[null,14,{"$f":"ATAN(TAN('Solar Altitude'!C44)/COS('Surface Solar Azimuth Angles'!C43))","v":0.75851543012385225},{"$f":"ATAN(TAN('Solar Altitude'!D44)/COS('Surface Solar Azimuth Angles'!D43))","v":0.93648395989476441},{"$f":"ATAN(TAN('Solar Altitude'!E44)/COS('Surface Solar Azimuth Angles'!E43))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F44)/COS('Surface Solar Azimuth Angles'!F43))","v":1.3750301180558759},{"$f":"ATAN(TAN('Solar Altitude'!G44)/COS('Surface Solar Azimuth Angles'!G43))","v":1.5399688677201155},{"$f":"ATAN(TAN('Solar Altitude'!H44)/COS('Surface Solar Azimuth Angles'!H43))","v":-1.5457329130795114},{"$f":"ATAN(TAN('Solar Altitude'!I44)/COS('Surface Solar Azimuth Angles'!I43))","v":1.5359564525388147},{"$f":"ATAN(TAN('Solar Altitude'!J44)/COS('Surface Solar Azimuth Angles'!J43))","v":1.3770848532828261},{"$f":"ATAN(TAN('Solar Altitude'!K44)/COS('Surface Solar Azimuth Angles'!K43))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L44)/COS('Surface Solar Azimuth Angles'!L43))","v":0.92031825841069448},{"$f":"ATAN(TAN('Solar Altitude'!M44)/COS('Surface Solar Azimuth Angles'!M43))","v":0.73756032900572732},{"$f":"ATAN(TAN('Solar Altitude'!N44)/COS('Surface Solar Azimuth Angles'!N43))","v":0.68075372194542327},null,14,{"$f":"ATAN(TAN('Solar Altitude'!C44)/COS('Surface Solar Azimuth Angles'!Q43))","v":-1.0005927212218162},{"$f":"ATAN(TAN('Solar Altitude'!D44)/COS('Surface Solar Azimuth Angles'!R43))","v":-1.0600445287944333},{"$f":"ATAN(TAN('Solar Altitude'!E44)/COS('Surface Solar Azimuth Angles'!S43))","v":-1.0718008336148819},{"$f":"ATAN(TAN('Solar Altitude'!F44)/COS('Surface Solar Azimuth Angles'!T43))","v":-1.0771466448813709},{"$f":"ATAN(TAN('Solar Altitude'!G44)/COS('Surface Solar Azimuth Angles'!U43))","v":-1.0979012626620424},{"$f":"ATAN(TAN('Solar Altitude'!H44)/COS('Surface Solar Azimuth Angles'!V43))","v":-1.127498795680429},{"$f":"ATAN(TAN('Solar Altitude'!I44)/COS('Surface Solar Azimuth Angles'!W43))","v":-1.1367031826073217},{"$f":"ATAN(TAN('Solar Altitude'!J44)/COS('Surface Solar Azimuth Angles'!X43))","v":-1.0927120982101921},{"$f":"ATAN(TAN('Solar Altitude'!K44)/COS('Surface Solar Azimuth Angles'!Y43))","v":-1.0030149795642187},{"$f":"ATAN(TAN('Solar Altitude'!L44)/COS('Surface Solar Azimuth Angles'!Z43))","v":-0.91563513724759149},{"$f":"ATAN(TAN('Solar Altitude'!M44)/COS('Surface Solar Azimuth Angles'!AA43))","v":-0.8697725416243034},{"$f":"ATAN(TAN('Solar Altitude'!N44)/COS('Surface Solar Azimuth Angles'!AB43))","v":-0.91012957488156332},null,14,{"$f":"ATAN(TAN('Solar Altitude'!C44)/COS('Surface Solar Azimuth Angles'!C98))","v":1.000592721221816},{"$f":"ATAN(TAN('Solar Altitude'!D44)/COS('Surface Solar Azimuth Angles'!D98))","v":1.0600445287944333},{"$f":"ATAN(TAN('Solar Altitude'!E44)/COS('Surface Solar Azimuth Angles'!E98))","v":1.0718008336148819},{"$f":"ATAN(TAN('Solar Altitude'!F44)/COS('Surface Solar Azimuth Angles'!F98))","v":1.0771466448813709},{"$f":"ATAN(TAN('Solar Altitude'!G44)/COS('Surface Solar Azimuth Angles'!G98))","v":1.0979012626620424},{"$f":"ATAN(TAN('Solar Altitude'!H44)/COS('Surface Solar Azimuth Angles'!H98))","v":1.127498795680429},{"$f":"ATAN(TAN('Solar Altitude'!I44)/COS('Surface Solar Azimuth Angles'!I98))","v":1.1367031826073217},{"$f":"ATAN(TAN('Solar Altitude'!J44)/COS('Surface Solar Azimuth Angles'!J98))","v":1.0927120982101921},{"$f":"ATAN(TAN('Solar Altitude'!K44)/COS('Surface Solar Azimuth Angles'!K98))","v":1.0030149795642187},{"$f":"ATAN(TAN('Solar Altitude'!L44)/COS('Surface Solar Azimuth Angles'!L98))","v":0.91563513724759149},{"$f":"ATAN(TAN('Solar Altitude'!M44)/COS('Surface Solar Azimuth Angles'!M98))","v":0.8697725416243034},{"$f":"ATAN(TAN('Solar Altitude'!N44)/COS('Surface Solar Azimuth Angles'!N98))","v":0.91012957488156332},null,14,{"$f":"ATAN(TAN('Solar Altitude'!C44)/COS('Surface Solar Azimuth Angles'!Q98))","v":-0.75851543012385236},{"$f":"ATAN(TAN('Solar Altitude'!D44)/COS('Surface Solar Azimuth Angles'!R98))","v":-0.93648395989476441},{"$f":"ATAN(TAN('Solar Altitude'!E44)/COS('Surface Solar Azimuth Angles'!S98))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F44)/COS('Surface Solar Azimuth Angles'!T98))","v":-1.3750301180558762},{"$f":"ATAN(TAN('Solar Altitude'!G44)/COS('Surface Solar Azimuth Angles'!U98))","v":-1.5399688677201155},{"$f":"ATAN(TAN('Solar Altitude'!H44)/COS('Surface Solar Azimuth Angles'!V98))","v":1.5457329130795117},{"$f":"ATAN(TAN('Solar Altitude'!I44)/COS('Surface Solar Azimuth Angles'!W98))","v":-1.5359564525388147},{"$f":"ATAN(TAN('Solar Altitude'!J44)/COS('Surface Solar Azimuth Angles'!X98))","v":-1.3770848532828264},{"$f":"ATAN(TAN('Solar Altitude'!K44)/COS('Surface Solar Azimuth Angles'!Y98))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L44)/COS('Surface Solar Azimuth Angles'!Z98))","v":-0.92031825841069448},{"$f":"ATAN(TAN('Solar Altitude'!M44)/COS('Surface Solar Azimuth Angles'!AA98))","v":-0.73756032900572732},{"$f":"ATAN(TAN('Solar Altitude'!N44)/COS('Surface Solar Azimuth Angles'!AB98))","v":-0.68075372194542327}]
[null,15,{"$f":"ATAN(TAN('Solar Altitude'!C45)/COS('Surface Solar Azimuth Angles'!C44))","v":0.6958725601819693},{"$f":"ATAN(TAN('Solar Altitude'!D45)/COS('Surface Solar Azimuth Angles'!D44))","v":0.90095965651819476},{"$f":"ATAN(TAN('Solar Altitude'!E45)/COS('Surface Solar Azimuth Angles'!E44))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F45)/COS('Surface Solar Azimuth Angles'!F44))","v":1.4223966034161182},{"$f":"ATAN(TAN('Solar Altitude'!G45)/COS('Surface Solar Azimuth Angles'!G44))","v":-1.5266344477385527},{"$f":"ATAN(TAN('Solar Altitude'!H45)/COS('Surface Solar Azimuth Angles'!H44))","v":-1.4675022187003639},{"$f":"ATAN(TAN('Solar Altitude'!I45)/COS('Surface Solar Azimuth Angles'!I44))","v":-1.5378465881867289},{"$f":"ATAN(TAN('Solar Altitude'!J45)/COS('Surface Solar Azimuth Angles'!J44))","v":1.4231733271709055},{"$f":"ATAN(TAN('Solar Altitude'!K45)/COS('Surface Solar Azimuth Angles'!K44))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L45)/COS('Surface Solar Azimuth Angles'!L44))","v":0.86910144352535135},{"$f":"ATAN(TAN('Solar Altitude'!M45)/COS('Surface Solar Azimuth Angles'!M44))","v":0.65429236322323214},{"$f":"ATAN(TAN('Solar Altitude'!N45)/COS('Surface Solar Azimuth Angles'!N44))","v":0.5998978540255393},null,15,{"$f":"ATAN(TAN('Solar Altitude'!C45)/COS('Surface Solar Azimuth Angles'!Q44))","v":-0.69486770530695274},{"$f":"ATAN(TAN('Solar Altitude'!D45)/COS('Surface Solar Azimuth Angles'!R44))","v":-0.77035987910152959},{"$f":"ATAN(TAN('Solar Altitude'!E45)/COS('Surface Solar Azimuth Angles'!S44))","v":-0.8014439225775819},{"$f":"ATAN(TAN('Solar Altitude'!F45)/COS('Surface Solar Azimuth Angles'!T44))","v":-0.82641496006128057},{"$f":"ATAN(TAN('Solar Altitude'!G45)/COS('Surface Solar Azimuth Angles'!U44))","v":-0.86009108801295264},{"$f":"ATAN(TAN('Solar Altitude'!H45)/COS('Surface Solar Azimuth Angles'!V44))","v":-0.89419996525178802},{"$f":"ATAN(TAN('Solar Altitude'!I45)/COS('Surface Solar Azimuth Angles'!W44))","v":-0.89834850121998655},{"$f":"ATAN(TAN('Solar Altitude'!J45)/COS('Surface Solar Azimuth Angles'!X44))","v":-0.84181932575908702},{"$f":"ATAN(TAN('Solar Altitude'!K45)/COS('Surface Solar Azimuth Angles'!Y44))","v":-0.73590361062962983},{"$f":"ATAN(TAN('Solar Altitude'!L45)/COS('Surface Solar Azimuth Angles'!Z44))","v":-0.63537560318144104},{"$f":"ATAN(TAN('Solar Altitude'!M45)/COS('Surface Solar Azimuth Angles'!AA44))","v":-0.57579270320512765},{"$f":"ATAN(TAN('Solar Altitude'!N45)/COS('Surface Solar Azimuth Angles'!AB44))","v":-0.6044646480538286},null,15,{"$f":"ATAN(TAN('Solar Altitude'!C45)/COS('Surface Solar Azimuth Angles'!C99))","v":0.69486770530695274},{"$f":"ATAN(TAN('Solar Altitude'!D45)/COS('Surface Solar Azimuth Angles'!D99))","v":0.77035987910152948},{"$f":"ATAN(TAN('Solar Altitude'!E45)/COS('Surface Solar Azimuth Angles'!E99))","v":0.80144392257758201},{"$f":"ATAN(TAN('Solar Altitude'!F45)/COS('Surface Solar Azimuth Angles'!F99))","v":0.82641496006128057},{"$f":"ATAN(TAN('Solar Altitude'!G45)/COS('Surface Solar Azimuth Angles'!G99))","v":0.86009108801295264},{"$f":"ATAN(TAN('Solar Altitude'!H45)/COS('Surface Solar Azimuth Angles'!H99))","v":0.89419996525178802},{"$f":"ATAN(TAN('Solar Altitude'!I45)/COS('Surface Solar Azimuth Angles'!I99))","v":0.89834850121998655},{"$f":"ATAN(TAN('Solar Altitude'!J45)/COS('Surface Solar Azimuth Angles'!J99))","v":0.84181932575908702},{"$f":"ATAN(TAN('Solar Altitude'!K45)/COS('Surface Solar Azimuth Angles'!K99))","v":0.73590361062962983},{"$f":"ATAN(TAN('Solar Altitude'!L45)/COS('Surface Solar Azimuth Angles'!L99))","v":0.63537560318144093},{"$f":"ATAN(TAN('Solar Altitude'!M45)/COS('Surface Solar Azimuth Angles'!M99))","v":0.57579270320512765},{"$f":"ATAN(TAN('Solar Altitude'!N45)/COS('Surface Solar Azimuth Angles'!N99))","v":0.60446464805382849},null,15,{"$f":"ATAN(TAN('Solar Altitude'!C45)/COS('Surface Solar Azimuth Angles'!Q99))","v":-0.69587256018196941},{"$f":"ATAN(TAN('Solar Altitude'!D45)/COS('Surface Solar Azimuth Angles'!R99))","v":-0.90095965651819487},{"$f":"ATAN(TAN('Solar Altitude'!E45)/COS('Surface Solar Azimuth Angles'!S99))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F45)/COS('Surface Solar Azimuth Angles'!T99))","v":-1.4223966034161182},{"$f":"ATAN(TAN('Solar Altitude'!G45)/COS('Surface Solar Azimuth Angles'!U99))","v":1.5266344477385527},{"$f":"ATAN(TAN('Solar Altitude'!H45)/COS('Surface Solar Azimuth Angles'!V99))","v":1.4675022187003639},{"$f":"ATAN(TAN('Solar Altitude'!I45)/COS('Surface Solar Azimuth Angles'!W99))","v":1.5378465881867287},{"$f":"ATAN(TAN('Solar Altitude'!J45)/COS('Surface Solar Azimuth Angles'!X99))","v":-1.4231733271709055},{"$f":"ATAN(TAN('Solar Altitude'!K45)/COS('Surface Solar Azimuth Angles'!Y99))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L45)/COS('Surface Solar Azimuth Angles'!Z99))","v":-0.86910144352535146},{"$f":"ATAN(TAN('Solar Altitude'!M45)/COS('Surface Solar Azimuth Angles'!AA99))","v":-0.65429236322323236},{"$f":"ATAN(TAN('Solar Altitude'!N45)/COS('Surface Solar Azimuth Angles'!AB99))","v":-0.59989785402553941}]
[null,16,{"$f":"ATAN(TAN('Solar Altitude'!C46)/COS('Surface Solar Azimuth Angles'!C45))","v":0.57197798027671076},{"$f":"ATAN(TAN('Solar Altitude'!D46)/COS('Surface Solar Azimuth Angles'!D45))","v":0.82619821336400978},{"$f":"ATAN(TAN('Solar Altitude'!E46)/COS('Surface Solar Azimuth Angles'!E45))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F46)/COS('Surface Solar Azimuth Angles'!F45))","v":1.5229810963446619},{"$f":"ATAN(TAN('Solar Altitude'!G46)/COS('Surface Solar Azimuth Angles'!G45))","v":-1.378468089484002},{"$f":"ATAN(TAN('Solar Altitude'!H46)/COS('Surface Solar Azimuth Angles'!H45))","v":-1.3177516582315827},{"$f":"ATAN(TAN('Solar Altitude'!I46)/COS('Surface Solar Azimuth Angles'!I45))","v":-1.4044440508792542},{"$f":"ATAN(TAN('Solar Altitude'!J46)/COS('Surface Solar Azimuth Angles'!J45))","v":1.5204461167120873},{"$f":"ATAN(TAN('Solar Altitude'!K46)/COS('Surface Solar Azimuth Angles'!K45))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L46)/COS('Surface Solar Azimuth Angles'!L45))","v":0.75629963516330245},{"$f":"ATAN(TAN('Solar Altitude'!M46)/COS('Surface Solar Azimuth Angles'!M45))","v":0.48809734520255899},{"$f":"ATAN(TAN('Solar Altitude'!N46)/COS('Surface Solar Azimuth Angles'!N45))","v":0.44518009228857969},null,16,{"$f":"ATAN(TAN('Solar Altitude'!C46)/COS('Surface Solar Azimuth Angles'!Q45))","v":-0.41669740220816492},{"$f":"ATAN(TAN('Solar Altitude'!D46)/COS('Surface Solar Azimuth Angles'!R45))","v":-0.50015077980007105},{"$f":"ATAN(TAN('Solar Altitude'!E46)/COS('Surface Solar Azimuth Angles'!S45))","v":-0.54404800401822806},{"$f":"ATAN(TAN('Solar Altitude'!F46)/COS('Surface Solar Azimuth Angles'!T45))","v":-0.58351428900426172},{"$f":"ATAN(TAN('Solar Altitude'!G46)/COS('Surface Solar Azimuth Angles'!U45))","v":-0.62746556362485806},{"$f":"ATAN(TAN('Solar Altitude'!H46)/COS('Surface Solar Azimuth Angles'!V45))","v":-0.66533748077630195},{"$f":"ATAN(TAN('Solar Altitude'!I46)/COS('Surface Solar Azimuth Angles'!W45))","v":-0.66523823915225477},{"$f":"ATAN(TAN('Solar Altitude'!J46)/COS('Surface Solar Azimuth Angles'!X45))","v":-0.59872473938789039},{"$f":"ATAN(TAN('Solar Altitude'!K46)/COS('Surface Solar Azimuth Angles'!Y45))","v":-0.48155681326357536},{"$f":"ATAN(TAN('Solar Altitude'!L46)/COS('Surface Solar Azimuth Angles'!Z45))","v":-0.37388412364806317},{"$f":"ATAN(TAN('Solar Altitude'!M46)/COS('Surface Solar Azimuth Angles'!AA45))","v":-0.30789644489665746},{"$f":"ATAN(TAN('Solar Altitude'!N46)/COS('Surface Solar Azimuth Angles'!AB45))","v":-0.32941416658746181},null,16,{"$f":"ATAN(TAN('Solar Altitude'!C46)/COS('Surface Solar Azimuth Angles'!C100))","v":0.41669740220816487},{"$f":"ATAN(TAN('Solar Altitude'!D46)/COS('Surface Solar Azimuth Angles'!D100))","v":0.50015077980007105},{"$f":"ATAN(TAN('Solar Altitude'!E46)/COS('Surface Solar Azimuth Angles'!E100))","v":0.54404800401822806},{"$f":"ATAN(TAN('Solar Altitude'!F46)/COS('Surface Solar Azimuth Angles'!F100))","v":0.58351428900426172},{"$f":"ATAN(TAN('Solar Altitude'!G46)/COS('Surface Solar Azimuth Angles'!G100))","v":0.62746556362485806},{"$f":"ATAN(TAN('Solar Altitude'!H46)/COS('Surface Solar Azimuth Angles'!H100))","v":0.66533748077630195},{"$f":"ATAN(TAN('Solar Altitude'!I46)/COS('Surface Solar Azimuth Angles'!I100))","v":0.66523823915225477},{"$f":"ATAN(TAN('Solar Altitude'!J46)/COS('Surface Solar Azimuth Angles'!J100))","v":0.59872473938789039},{"$f":"ATAN(TAN('Solar Altitude'!K46)/COS('Surface Solar Azimuth Angles'!K100))","v":0.48155681326357536},{"$f":"ATAN(TAN('Solar Altitude'!L46)/COS('Surface Solar Azimuth Angles'!L100))","v":0.37388412364806317},{"$f":"ATAN(TAN('Solar Altitude'!M46)/COS('Surface Solar Azimuth Angles'!M100))","v":0.30789644489665746},{"$f":"ATAN(TAN('Solar Altitude'!N46)/COS('Surface Solar Azimuth Angles'!N100))","v":0.32941416658746181},null,16,{"$f":"ATAN(TAN('Solar Altitude'!C46)/COS('Surface Solar Azimuth Angles'!Q100))","v":-0.57197798027671087},{"$f":"ATAN(TAN('Solar Altitude'!D46)/COS('Surface Solar Azimuth Angles'!R100))","v":-0.82619821336401},{"$f":"ATAN(TAN('Solar Altitude'!E46)/COS('Surface Solar Azimuth Angles'!S100))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F46)/COS('Surface Solar Azimuth Angles'!T100))","v":-1.5229810963446622},{"$f":"ATAN(TAN('Solar Altitude'!G46)/COS('Surface Solar Azimuth Angles'!U100))","v":1.3784680894840018},{"$f":"ATAN(TAN('Solar Altitude'!H46)/COS('Surface Solar Azimuth Angles'!V100))","v":1.3177516582315827},{"$f":"ATAN(TAN('Solar Altitude'!I46)/COS('Surface Solar Azimuth Angles'!W100))","v":1.4044440508792544},{"$f":"ATAN(TAN('Solar Altitude'!J46)/COS('Surface Solar Azimuth Angles'!X100))","v":-1.5204461167120875},{"$f":"ATAN(TAN('Solar Altitude'!K46)/COS('Surface Solar Azimuth Angles'!Y100))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L46)/COS('Surface Solar Azimuth Angles'!Z100))","v":-0.75629963516330245},{"$f":"ATAN(TAN('Solar Altitude'!M46)/COS('Surface Solar Azimuth Angles'!AA100))","v":-0.48809734520255904},{"$f":"ATAN(TAN('Solar Altitude'!N46)/COS('Surface Solar Azimuth Angles'!AB100))","v":-0.44518009228857969}]
[null,17,{"$f":"ATAN(TAN('Solar Altitude'!C47)/COS('Surface Solar Azimuth Angles'!C46))","v":0.31585481016596412},{"$f":"ATAN(TAN('Solar Altitude'!D47)/COS('Surface Solar Azimuth Angles'!D46))","v":0.64419111865687895},{"$f":"ATAN(TAN('Solar Altitude'!E47)/COS('Surface Solar Azimuth Angles'!E46))","v":1.1397000015522969},{"$f":"ATAN(TAN('Solar Altitude'!F47)/COS('Surface Solar Azimuth Angles'!F46))","v":-1.3637805005768204},{"$f":"ATAN(TAN('Solar Altitude'!G47)/COS('Surface Solar Azimuth Angles'!G46))","v":-1.0702663972279507},{"$f":"ATAN(TAN('Solar Altitude'!H47)/COS('Surface Solar Azimuth Angles'!H46))","v":-1.0276883038342115},{"$f":"ATAN(TAN('Solar Altitude'!I47)/COS('Surface Solar Azimuth Angles'!I46))","v":-1.1305109275476111},{"$f":"ATAN(TAN('Solar Altitude'!J47)/COS('Surface Solar Azimuth Angles'!J46))","v":-1.3794764235329202},{"$f":"ATAN(TAN('Solar Altitude'!K47)/COS('Surface Solar Azimuth Angles'!K46))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L47)/COS('Surface Solar Azimuth Angles'!L46))","v":0.438568425765194},{"$f":"ATAN(TAN('Solar Altitude'!M47)/COS('Surface Solar Azimuth Angles'!M46))","v":0.13613500526814382},{"$f":"ATAN(TAN('Solar Altitude'!N47)/COS('Surface Solar Azimuth Angles'!N46))","v":0.14545482072436786},null,17,{"$f":"ATAN(TAN('Solar Altitude'!C47)/COS('Surface Solar Azimuth Angles'!Q46))","v":-0.16124242777223322},{"$f":"ATAN(TAN('Solar Altitude'!D47)/COS('Surface Solar Azimuth Angles'!R46))","v":-0.24682095640962623},{"$f":"ATAN(TAN('Solar Altitude'!E47)/COS('Surface Solar Azimuth Angles'!S46))","v":-0.29766243646613283},{"$f":"ATAN(TAN('Solar Altitude'!F47)/COS('Surface Solar Azimuth Angles'!T46))","v":-0.34652947246442356},{"$f":"ATAN(TAN('Solar Altitude'!G47)/COS('Surface Solar Azimuth Angles'!U46))","v":-0.39810829518922258},{"$f":"ATAN(TAN('Solar Altitude'!H47)/COS('Surface Solar Azimuth Angles'!V46))","v":-0.43915625637623362},{"$f":"ATAN(TAN('Solar Altitude'!I47)/COS('Surface Solar Azimuth Angles'!W46))","v":-0.43577963764801331},{"$f":"ATAN(TAN('Solar Altitude'!J47)/COS('Surface Solar Azimuth Angles'!X46))","v":-0.36165127468574837},{"$f":"ATAN(TAN('Solar Altitude'!K47)/COS('Surface Solar Azimuth Angles'!Y46))","v":-0.2373188382783232},{"$f":"ATAN(TAN('Solar Altitude'!L47)/COS('Surface Solar Azimuth Angles'!Z46))","v":-0.12693435438886347},{"$f":"ATAN(TAN('Solar Altitude'!M47)/COS('Surface Solar Azimuth Angles'!AA46))","v":-5.9792925815892878E-2},{"$f":"ATAN(TAN('Solar Altitude'!N47)/COS('Surface Solar Azimuth Angles'!AB46))","v":-7.8011009216174293E-2},null,17,{"$f":"ATAN(TAN('Solar Altitude'!C47)/COS('Surface Solar Azimuth Angles'!C101))","v":0.16124242777223324},{"$f":"ATAN(TAN('Solar Altitude'!D47)/COS('Surface Solar Azimuth Angles'!D101))","v":0.24682095640962623},{"$f":"ATAN(TAN('Solar Altitude'!E47)/COS('Surface Solar Azimuth Angles'!E101))","v":0.29766243646613288},{"$f":"ATAN(TAN('Solar Altitude'!F47)/COS('Surface Solar Azimuth Angles'!F101))","v":0.34652947246442356},{"$f":"ATAN(TAN('Solar Altitude'!G47)/COS('Surface Solar Azimuth Angles'!G101))","v":0.39810829518922258},{"$f":"ATAN(TAN('Solar Altitude'!H47)/COS('Surface Solar Azimuth Angles'!H101))","v":0.43915625637623368},{"$f":"ATAN(TAN('Solar Altitude'!I47)/COS('Surface Solar Azimuth Angles'!I101))","v":0.43577963764801336},{"$f":"ATAN(TAN('Solar Altitude'!J47)/COS('Surface Solar Azimuth Angles'!J101))","v":0.36165127468574843},{"$f":"ATAN(TAN('Solar Altitude'!K47)/COS('Surface Solar Azimuth Angles'!K101))","v":0.2373188382783232},{"$f":"ATAN(TAN('Solar Altitude'!L47)/COS('Surface Solar Azimuth Angles'!L101))","v":0.12693435438886347},{"$f":"ATAN(TAN('Solar Altitude'!M47)/COS('Surface Solar Azimuth Angles'!M101))","v":5.9792925815892878E-2},{"$f":"ATAN(TAN('Solar Altitude'!N47)/COS('Surface Solar Azimuth Angles'!N101))","v":7.8011009216174293E-2},null,17,{"$f":"ATAN(TAN('Solar Altitude'!C47)/COS('Surface Solar Azimuth Angles'!Q101))","v":-0.31585481016596428},{"$f":"ATAN(TAN('Solar Altitude'!D47)/COS('Surface Solar Azimuth Angles'!R101))","v":-0.64419111865687906},{"$f":"ATAN(TAN('Solar Altitude'!E47)/COS('Surface Solar Azimuth Angles'!S101))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F47)/COS('Surface Solar Azimuth Angles'!T101))","v":1.3637805005768209},{"$f":"ATAN(TAN('Solar Altitude'!G47)/COS('Surface Solar Azimuth Angles'!U101))","v":1.0702663972279509},{"$f":"ATAN(TAN('Solar Altitude'!H47)/COS('Surface Solar Azimuth Angles'!V101))","v":1.0276883038342117},{"$f":"ATAN(TAN('Solar Altitude'!I47)/COS('Surface Solar Azimuth Angles'!W101))","v":1.1305109275476108},{"$f":"ATAN(TAN('Solar Altitude'!J47)/COS('Surface Solar Azimuth Angles'!X101))","v":1.3794764235329204},{"$f":"ATAN(TAN('Solar Altitude'!K47)/COS('Surface Solar Azimuth Angles'!Y101))","v":-1.1397000015522969},{"$f":"ATAN(TAN('Solar Altitude'!L47)/COS('Surface Solar Azimuth Angles'!Z101))","v":-0.43856842576519417},{"$f":"ATAN(TAN('Solar Altitude'!M47)/COS('Surface Solar Azimuth Angles'!AA101))","v":-0.13613500526814387},{"$f":"ATAN(TAN('Solar Altitude'!N47)/COS('Surface Solar Azimuth Angles'!AB101))","v":-0.14545482072436788}]
[null,18,{"$f":"ATAN(TAN('Solar Altitude'!C48)/COS('Surface Solar Azimuth Angles'!C47))","v":-0.21383448367072508},{"$f":"ATAN(TAN('Solar Altitude'!D48)/COS('Surface Solar Azimuth Angles'!D47))","v":2.4284225922147806E-2},{"$f":"ATAN(TAN('Solar Altitude'!E48)/COS('Surface Solar Azimuth Angles'!E47))","v":1.1397000015522951},{"$f":"ATAN(TAN('Solar Altitude'!F48)/COS('Surface Solar Azimuth Angles'!F47))","v":-0.55536119281617968},{"$f":"ATAN(TAN('Solar Altitude'!G48)/COS('Surface Solar Azimuth Angles'!G47))","v":-0.4762798915921686},{"$f":"ATAN(TAN('Solar Altitude'!H48)/COS('Surface Solar Azimuth Angles'!H47))","v":-0.51670314614163193},{"$f":"ATAN(TAN('Solar Altitude'!I48)/COS('Surface Solar Azimuth Angles'!I47))","v":-0.58537590303118925},{"$f":"ATAN(TAN('Solar Altitude'!J48)/COS('Surface Solar Azimuth Angles'!J47))","v":-0.62269367861413683},{"$f":"ATAN(TAN('Solar Altitude'!K48)/COS('Surface Solar Azimuth Angles'!K47))","v":1.1397000015523899},{"$f":"ATAN(TAN('Solar Altitude'!L48)/COS('Surface Solar Azimuth Angles'!L47))","v":-0.6196827915365295},{"$f":"ATAN(TAN('Solar Altitude'!M48)/COS('Surface Solar Azimuth Angles'!M47))","v":-0.51126975196190483},{"$f":"ATAN(TAN('Solar Altitude'!N48)/COS('Surface Solar Azimuth Angles'!N47))","v":-0.37549955159039705},null,18,{"$f":"ATAN(TAN('Solar Altitude'!C48)/COS('Surface Solar Azimuth Angles'!Q47))","v":7.875695115485469E-2},{"$f":"ATAN(TAN('Solar Altitude'!D48)/COS('Surface Solar Azimuth Angles'!R47))","v":-5.0811936091930835E-3},{"$f":"ATAN(TAN('Solar Altitude'!E48)/COS('Surface Solar Azimuth Angles'!S47))","v":-5.8021971754233764E-2},{"$f":"ATAN(TAN('Solar Altitude'!F48)/COS('Surface Solar Azimuth Angles'!T47))","v":-0.11154632270391088},{"$f":"ATAN(TAN('Solar Altitude'!G48)/COS('Surface Solar Azimuth Angles'!U47))","v":-0.16818851648487471},{"$f":"ATAN(TAN('Solar Altitude'!H48)/COS('Surface Solar Azimuth Angles'!V47))","v":-0.2119948495476848},{"$f":"ATAN(TAN('Solar Altitude'!I48)/COS('Surface Solar Azimuth Angles'!W47))","v":-0.20643034646530076},{"$f":"ATAN(TAN('Solar Altitude'!J48)/COS('Surface Solar Azimuth Angles'!X47))","v":-0.12678973084122475},{"$f":"ATAN(TAN('Solar Altitude'!K48)/COS('Surface Solar Azimuth Angles'!Y47))","v":1.4535089563006036E-3},{"$f":"ATAN(TAN('Solar Altitude'!L48)/COS('Surface Solar Azimuth Angles'!Z47))","v":0.11133018006865014},{"$f":"ATAN(TAN('Solar Altitude'!M48)/COS('Surface Solar Azimuth Angles'!AA47))","v":0.1759269261728052},{"$f":"ATAN(TAN('Solar Altitude'!N48)/COS('Surface Solar Azimuth Angles'!AB47))","v":0.15804497456402347},null,18,{"$f":"ATAN(TAN('Solar Altitude'!C48)/COS('Surface Solar Azimuth Angles'!C102))","v":-7.875695115485469E-2},{"$f":"ATAN(TAN('Solar Altitude'!D48)/COS('Surface Solar Azimuth Angles'!D102))","v":5.0811936091930835E-3},{"$f":"ATAN(TAN('Solar Altitude'!E48)/COS('Surface Solar Azimuth Angles'!E102))","v":5.8021971754233764E-2},{"$f":"ATAN(TAN('Solar Altitude'!F48)/COS('Surface Solar Azimuth Angles'!F102))","v":0.11154632270391088},{"$f":"ATAN(TAN('Solar Altitude'!G48)/COS('Surface Solar Azimuth Angles'!G102))","v":0.16818851648487471},{"$f":"ATAN(TAN('Solar Altitude'!H48)/COS('Surface Solar Azimuth Angles'!H102))","v":0.2119948495476848},{"$f":"ATAN(TAN('Solar Altitude'!I48)/COS('Surface Solar Azimuth Angles'!I102))","v":0.20643034646530073},{"$f":"ATAN(TAN('Solar Altitude'!J48)/COS('Surface Solar Azimuth Angles'!J102))","v":0.12678973084122475},{"$f":"ATAN(TAN('Solar Altitude'!K48)/COS('Surface Solar Azimuth Angles'!K102))","v":-1.4535089563006036E-3},{"$f":"ATAN(TAN('Solar Altitude'!L48)/COS('Surface Solar Azimuth Angles'!L102))","v":-0.11133018006865013},{"$f":"ATAN(TAN('Solar Altitude'!M48)/COS('Surface Solar Azimuth Angles'!M102))","v":-0.17592692617280517},{"$f":"ATAN(TAN('Solar Altitude'!N48)/COS('Surface Solar Azimuth Angles'!N102))","v":-0.15804497456402347},null,18,{"$f":"ATAN(TAN('Solar Altitude'!C48)/COS('Surface Solar Azimuth Angles'!Q102))","v":0.21383448367072516},{"$f":"ATAN(TAN('Solar Altitude'!D48)/COS('Surface Solar Azimuth Angles'!R102))","v":-2.4284225922147823E-2},{"$f":"ATAN(TAN('Solar Altitude'!E48)/COS('Surface Solar Azimuth Angles'!S102))","v":-1.1397000015522969},{"$f":"ATAN(TAN('Solar Altitude'!F48)/COS('Surface Solar Azimuth Angles'!T102))","v":0.55536119281617979},{"$f":"ATAN(TAN('Solar Altitude'!G48)/COS('Surface Solar Azimuth Angles'!U102))","v":0.47627989159216844},{"$f":"ATAN(TAN('Solar Altitude'!H48)/COS('Surface Solar Azimuth Angles'!V102))","v":0.51670314614163182},{"$f":"ATAN(TAN('Solar Altitude'!I48)/COS('Surface Solar Azimuth Angles'!W102))","v":0.58537590303118936},{"$f":"ATAN(TAN('Solar Altitude'!J48)/COS('Surface Solar Azimuth Angles'!X102))","v":0.62269367861413716},{"$f":"ATAN(TAN('Solar Altitude'!K48)/COS('Surface Solar Azimuth Angles'!Y102))","v":-1.1397000015523204},{"$f":"ATAN(TAN('Solar Altitude'!L48)/COS('Surface Solar Azimuth Angles'!Z102))","v":0.61968279153652928},{"$f":"ATAN(TAN('Solar Altitude'!M48)/COS('Surface Solar Azimuth Angles'!AA102))","v":0.51126975196190494},{"$f":"ATAN(TAN('Solar Altitude'!N48)/COS('Surface Solar Azimuth Angles'!AB102))","v":0.37549955159039694}]
[null,19,{"$f":"ATAN(TAN('Solar Altitude'!C49)/COS('Surface Solar Azimuth Angles'!C48))","v":-0.8943190286097269},{"$f":"ATAN(TAN('Solar Altitude'!D49)/COS('Surface Solar Azimuth Angles'!D48))","v":-1.166196830362576},{"$f":"ATAN(TAN('Solar Altitude'!E49)/COS('Surface Solar Azimuth Angles'!E48))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F49)/COS('Surface Solar Azimuth Angles'!F48))","v":0.40508921503180312},{"$f":"ATAN(TAN('Solar Altitude'!G49)/COS('Surface Solar Azimuth Angles'!G48))","v":0.1494204003451183},{"$f":"ATAN(TAN('Solar Altitude'!H49)/COS('Surface Solar Azimuth Angles'!H48))","v":4.3182419744715421E-2},{"$f":"ATAN(TAN('Solar Altitude'!I49)/COS('Surface Solar Azimuth Angles'!I48))","v":6.4699031311275218E-2},{"$f":"ATAN(TAN('Solar Altitude'!J49)/COS('Surface Solar Azimuth Angles'!J48))","v":0.36364909543045837},{"$f":"ATAN(TAN('Solar Altitude'!K49)/COS('Surface Solar Azimuth Angles'!K48))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L49)/COS('Surface Solar Azimuth Angles'!L48))","v":-1.4298718763400156},{"$f":"ATAN(TAN('Solar Altitude'!M49)/COS('Surface Solar Azimuth Angles'!M48))","v":-1.1011153762045047},{"$f":"ATAN(TAN('Solar Altitude'!N49)/COS('Surface Solar Azimuth Angles'!N48))","v":-0.9283445131232797},null,19,{"$f":"ATAN(TAN('Solar Altitude'!C49)/COS('Surface Solar Azimuth Angles'!Q48))","v":0.31044316509225717},{"$f":"ATAN(TAN('Solar Altitude'!D49)/COS('Surface Solar Azimuth Angles'!R48))","v":0.23111522112121052},{"$f":"ATAN(TAN('Solar Altitude'!E49)/COS('Surface Solar Azimuth Angles'!S48))","v":0.18024728429187611},{"$f":"ATAN(TAN('Solar Altitude'!F49)/COS('Surface Solar Azimuth Angles'!T48))","v":0.12673343644358437},{"$f":"ATAN(TAN('Solar Altitude'!G49)/COS('Surface Solar Azimuth Angles'!U48))","v":6.7779708344327269E-2},{"$f":"ATAN(TAN('Solar Altitude'!H49)/COS('Surface Solar Azimuth Angles'!V48))","v":2.1587753481061966E-2},{"$f":"ATAN(TAN('Solar Altitude'!I49)/COS('Surface Solar Azimuth Angles'!W48))","v":2.8054601331330975E-2},{"$f":"ATAN(TAN('Solar Altitude'!J49)/COS('Surface Solar Azimuth Angles'!X48))","v":0.11109422861118667},{"$f":"ATAN(TAN('Solar Altitude'!K49)/COS('Surface Solar Azimuth Angles'!Y48))","v":0.24026026153093591},{"$f":"ATAN(TAN('Solar Altitude'!L49)/COS('Surface Solar Azimuth Angles'!Z48))","v":0.34689085936294084},{"$f":"ATAN(TAN('Solar Altitude'!M49)/COS('Surface Solar Azimuth Angles'!AA48))","v":0.40600410951818994},{"$f":"ATAN(TAN('Solar Altitude'!N49)/COS('Surface Solar Azimuth Angles'!AB48))","v":0.38616028192323892},null,19,{"$f":"ATAN(TAN('Solar Altitude'!C49)/COS('Surface Solar Azimuth Angles'!C103))","v":-0.31044316509225717},{"$f":"ATAN(TAN('Solar Altitude'!D49)/COS('Surface Solar Azimuth Angles'!D103))","v":-0.23111522112121052},{"$f":"ATAN(TAN('Solar Altitude'!E49)/COS('Surface Solar Azimuth Angles'!E103))","v":-0.18024728429187611},{"$f":"ATAN(TAN('Solar Altitude'!F49)/COS('Surface Solar Azimuth Angles'!F103))","v":-0.1267334364435844},{"$f":"ATAN(TAN('Solar Altitude'!G49)/COS('Surface Solar Azimuth Angles'!G103))","v":-6.7779708344327269E-2},{"$f":"ATAN(TAN('Solar Altitude'!H49)/COS('Surface Solar Azimuth Angles'!H103))","v":-2.1587753481061966E-2},{"$f":"ATAN(TAN('Solar Altitude'!I49)/COS('Surface Solar Azimuth Angles'!I103))","v":-2.8054601331330975E-2},{"$f":"ATAN(TAN('Solar Altitude'!J49)/COS('Surface Solar Azimuth Angles'!J103))","v":-0.11109422861118667},{"$f":"ATAN(TAN('Solar Altitude'!K49)/COS('Surface Solar Azimuth Angles'!K103))","v":-0.24026026153093591},{"$f":"ATAN(TAN('Solar Altitude'!L49)/COS('Surface Solar Azimuth Angles'!L103))","v":-0.34689085936294084},{"$f":"ATAN(TAN('Solar Altitude'!M49)/COS('Surface Solar Azimuth Angles'!M103))","v":-0.40600410951818994},{"$f":"ATAN(TAN('Solar Altitude'!N49)/COS('Surface Solar Azimuth Angles'!N103))","v":-0.38616028192323892},null,19,{"$f":"ATAN(TAN('Solar Altitude'!C49)/COS('Surface Solar Azimuth Angles'!Q103))","v":0.89431902860972701},{"$f":"ATAN(TAN('Solar Altitude'!D49)/COS('Surface Solar Azimuth Angles'!R103))","v":1.1661968303625765},{"$f":"ATAN(TAN('Solar Altitude'!E49)/COS('Surface Solar Azimuth Angles'!S103))","v":-1.1397000015522967},{"$f":"ATAN(TAN('Solar Altitude'!F49)/COS('Surface Solar Azimuth Angles'!T103))","v":-0.40508921503180328},{"$f":"ATAN(TAN('Solar Altitude'!G49)/COS('Surface Solar Azimuth Angles'!U103))","v":-0.14942040034511828},{"$f":"ATAN(TAN('Solar Altitude'!H49)/COS('Surface Solar Azimuth Angles'!V103))","v":-4.3182419744715414E-2},{"$f":"ATAN(TAN('Solar Altitude'!I49)/COS('Surface Solar Azimuth Angles'!W103))","v":-6.4699031311275204E-2},{"$f":"ATAN(TAN('Solar Altitude'!J49)/COS('Surface Solar Azimuth Angles'!X103))","v":-0.36364909543045842},{"$f":"ATAN(TAN('Solar Altitude'!K49)/COS('Surface Solar Azimuth Angles'!Y103))","v":-1.1397000015522969},{"$f":"ATAN(TAN('Solar Altitude'!L49)/COS('Surface Solar Azimuth Angles'!Z103))","v":1.429871876340016},{"$f":"ATAN(TAN('Solar Altitude'!M49)/COS('Surface Solar Azimuth Angles'!AA103))","v":1.1011153762045045},{"$f":"ATAN(TAN('Solar Altitude'!N49)/COS('Surface Solar Azimuth Angles'!AB103))","v":0.92834451312327959}]
[null,20,{"$f":"ATAN(TAN('Solar Altitude'!C50)/COS('Surface Solar Azimuth Angles'!C49))","v":-1.3012298625660645},{"$f":"ATAN(TAN('Solar Altitude'!D50)/COS('Surface Solar Azimuth Angles'!D49))","v":1.5601818868055648},{"$f":"ATAN(TAN('Solar Altitude'!E50)/COS('Surface Solar Azimuth Angles'!E49))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F50)/COS('Surface Solar Azimuth Angles'!F49))","v":0.72371978813644855},{"$f":"ATAN(TAN('Solar Altitude'!G50)/COS('Surface Solar Azimuth Angles'!G49))","v":0.4885607623749027},{"$f":"ATAN(TAN('Solar Altitude'!H50)/COS('Surface Solar Azimuth Angles'!H49))","v":0.39161342241702657},{"$f":"ATAN(TAN('Solar Altitude'!I50)/COS('Surface Solar Azimuth Angles'!I49))","v":0.44511249062286384},{"$f":"ATAN(TAN('Solar Altitude'!J50)/COS('Surface Solar Azimuth Angles'!J49))","v":0.70652153014812857},{"$f":"ATAN(TAN('Solar Altitude'!K50)/COS('Surface Solar Azimuth Angles'!K49))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L50)/COS('Surface Solar Azimuth Angles'!L49))","v":1.4816256583034377},{"$f":"ATAN(TAN('Solar Altitude'!M50)/COS('Surface Solar Azimuth Angles'!M49))","v":-1.3982180222701845},{"$f":"ATAN(TAN('Solar Altitude'!N50)/COS('Surface Solar Azimuth Angles'!N49))","v":-1.2659457689719542},null,20,{"$f":"ATAN(TAN('Solar Altitude'!C50)/COS('Surface Solar Azimuth Angles'!Q49))","v":0.53982440647106411},{"$f":"ATAN(TAN('Solar Altitude'!D50)/COS('Surface Solar Azimuth Angles'!R49))","v":0.46745924354256657},{"$f":"ATAN(TAN('Solar Altitude'!E50)/COS('Surface Solar Azimuth Angles'!S49))","v":0.42271676310413892},{"$f":"ATAN(TAN('Solar Altitude'!F50)/COS('Surface Solar Azimuth Angles'!T49))","v":0.37438414286885741},{"$f":"ATAN(TAN('Solar Altitude'!G50)/COS('Surface Solar Azimuth Angles'!U49))","v":0.3166309523795891},{"$f":"ATAN(TAN('Solar Altitude'!H50)/COS('Surface Solar Azimuth Angles'!V49))","v":0.26866082450954953},{"$f":"ATAN(TAN('Solar Altitude'!I50)/COS('Surface Solar Azimuth Angles'!W49))","v":0.27434316021105154},{"$f":"ATAN(TAN('Solar Altitude'!J50)/COS('Surface Solar Azimuth Angles'!X49))","v":0.35806173657168089},{"$f":"ATAN(TAN('Solar Altitude'!K50)/COS('Surface Solar Azimuth Angles'!Y49))","v":0.48459652421088523},{"$f":"ATAN(TAN('Solar Altitude'!L50)/COS('Surface Solar Azimuth Angles'!Z49))","v":0.58500248706259217},{"$f":"ATAN(TAN('Solar Altitude'!M50)/COS('Surface Solar Azimuth Angles'!AA49))","v":0.6358430799641186},{"$f":"ATAN(TAN('Solar Altitude'!N50)/COS('Surface Solar Azimuth Angles'!AB49))","v":0.61217498892976274},null,20,{"$f":"ATAN(TAN('Solar Altitude'!C50)/COS('Surface Solar Azimuth Angles'!C104))","v":-0.53982440647106411},{"$f":"ATAN(TAN('Solar Altitude'!D50)/COS('Surface Solar Azimuth Angles'!D104))","v":-0.46745924354256657},{"$f":"ATAN(TAN('Solar Altitude'!E50)/COS('Surface Solar Azimuth Angles'!E104))","v":-0.42271676310413892},{"$f":"ATAN(TAN('Solar Altitude'!F50)/COS('Surface Solar Azimuth Angles'!F104))","v":-0.37438414286885741},{"$f":"ATAN(TAN('Solar Altitude'!G50)/COS('Surface Solar Azimuth Angles'!G104))","v":-0.31663095237958921},{"$f":"ATAN(TAN('Solar Altitude'!H50)/COS('Surface Solar Azimuth Angles'!H104))","v":-0.26866082450954942},{"$f":"ATAN(TAN('Solar Altitude'!I50)/COS('Surface Solar Azimuth Angles'!I104))","v":-0.27434316021105154},{"$f":"ATAN(TAN('Solar Altitude'!J50)/COS('Surface Solar Azimuth Angles'!J104))","v":-0.35806173657168094},{"$f":"ATAN(TAN('Solar Altitude'!K50)/COS('Surface Solar Azimuth Angles'!K104))","v":-0.48459652421088523},{"$f":"ATAN(TAN('Solar Altitude'!L50)/COS('Surface Solar Azimuth Angles'!L104))","v":-0.58500248706259217},{"$f":"ATAN(TAN('Solar Altitude'!M50)/COS('Surface Solar Azimuth Angles'!M104))","v":-0.6358430799641186},{"$f":"ATAN(TAN('Solar Altitude'!N50)/COS('Surface Solar Azimuth Angles'!N104))","v":-0.61217498892976274},null,20,{"$f":"ATAN(TAN('Solar Altitude'!C50)/COS('Surface Solar Azimuth Angles'!Q104))","v":1.3012298625660643},{"$f":"ATAN(TAN('Solar Altitude'!D50)/COS('Surface Solar Azimuth Angles'!R104))","v":-1.560181886805565},{"$f":"ATAN(TAN('Solar Altitude'!E50)/COS('Surface Solar Azimuth Angles'!S104))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F50)/COS('Surface Solar Azimuth Angles'!T104))","v":-0.72371978813644844},{"$f":"ATAN(TAN('Solar Altitude'!G50)/COS('Surface Solar Azimuth Angles'!U104))","v":-0.48856076237490259},{"$f":"ATAN(TAN('Solar Altitude'!H50)/COS('Surface Solar Azimuth Angles'!V104))","v":-0.39161342241702657},{"$f":"ATAN(TAN('Solar Altitude'!I50)/COS('Surface Solar Azimuth Angles'!W104))","v":-0.44511249062286379},{"$f":"ATAN(TAN('Solar Altitude'!J50)/COS('Surface Solar Azimuth Angles'!X104))","v":-0.70652153014812846},{"$f":"ATAN(TAN('Solar Altitude'!K50)/COS('Surface Solar Azimuth Angles'!Y104))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L50)/COS('Surface Solar Azimuth Angles'!Z104))","v":-1.4816256583034375},{"$f":"ATAN(TAN('Solar Altitude'!M50)/COS('Surface Solar Azimuth Angles'!AA104))","v":1.3982180222701848},{"$f":"ATAN(TAN('Solar Altitude'!N50)/COS('Surface Solar Azimuth Angles'!AB104))","v":1.2659457689719542}]
[null,21,{"$f":"ATAN(TAN('Solar Altitude'!C51)/COS('Surface Solar Azimuth Angles'!C50))","v":-1.4926689138225644},{"$f":"ATAN(TAN('Solar Altitude'!D51)/COS('Surface Solar Azimuth Angles'!D50))","v":1.4244661198800128},{"$f":"ATAN(TAN('Solar Altitude'!E51)/COS('Surface Solar Azimuth Angles'!E50))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F51)/COS('Surface Solar Azimuth Angles'!F50))","v":0.84257659010007879},{"$f":"ATAN(TAN('Solar Altitude'!G51)/COS('Surface Solar Azimuth Angles'!G50))","v":0.65069747813555467},{"$f":"ATAN(TAN('Solar Altitude'!H51)/COS('Surface Solar Azimuth Angles'!H50))","v":0.5720711137075446},{"$f":"ATAN(TAN('Solar Altitude'!I51)/COS('Surface Solar Azimuth Angles'!I50))","v":0.62738252671884265},{"$f":"ATAN(TAN('Solar Altitude'!J51)/COS('Surface Solar Azimuth Angles'!J50))","v":0.8330645277261437},{"$f":"ATAN(TAN('Solar Altitude'!K51)/COS('Surface Solar Azimuth Angles'!K50))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L51)/COS('Surface Solar Azimuth Angles'!L50))","v":1.3922681911981456},{"$f":"ATAN(TAN('Solar Altitude'!M51)/COS('Surface Solar Azimuth Angles'!M50))","v":-1.5401075773273574},{"$f":"ATAN(TAN('Solar Altitude'!N51)/COS('Surface Solar Azimuth Angles'!N50))","v":-1.440555126370102},null,21,{"$f":"ATAN(TAN('Solar Altitude'!C51)/COS('Surface Solar Azimuth Angles'!Q50))","v":0.77137406354258065},{"$f":"ATAN(TAN('Solar Altitude'!D51)/COS('Surface Solar Azimuth Angles'!R50))","v":0.70858778624744145},{"$f":"ATAN(TAN('Solar Altitude'!E51)/COS('Surface Solar Azimuth Angles'!S50))","v":0.67432329522984613},{"$f":"ATAN(TAN('Solar Altitude'!F51)/COS('Surface Solar Azimuth Angles'!T50))","v":0.63740014217672603},{"$f":"ATAN(TAN('Solar Altitude'!G51)/COS('Surface Solar Azimuth Angles'!U50))","v":0.58586265313688612},{"$f":"ATAN(TAN('Solar Altitude'!H51)/COS('Surface Solar Azimuth Angles'!V50))","v":0.5374341930134342},{"$f":"ATAN(TAN('Solar Altitude'!I51)/COS('Surface Solar Azimuth Angles'!W50))","v":0.53995019403937616},{"$f":"ATAN(TAN('Solar Altitude'!J51)/COS('Surface Solar Azimuth Angles'!X50))","v":0.6201738526973527},{"$f":"ATAN(TAN('Solar Altitude'!K51)/COS('Surface Solar Azimuth Angles'!Y50))","v":0.73908870770470347},{"$f":"ATAN(TAN('Solar Altitude'!L51)/COS('Surface Solar Azimuth Angles'!Z50))","v":0.82955153298556916},{"$f":"ATAN(TAN('Solar Altitude'!M51)/COS('Surface Solar Azimuth Angles'!AA50))","v":0.86919421625434168},{"$f":"ATAN(TAN('Solar Altitude'!N51)/COS('Surface Solar Azimuth Angles'!AB50))","v":0.84017901380444071},null,21,{"$f":"ATAN(TAN('Solar Altitude'!C51)/COS('Surface Solar Azimuth Angles'!C105))","v":-0.77137406354258065},{"$f":"ATAN(TAN('Solar Altitude'!D51)/COS('Surface Solar Azimuth Angles'!D105))","v":-0.70858778624744145},{"$f":"ATAN(TAN('Solar Altitude'!E51)/COS('Surface Solar Azimuth Angles'!E105))","v":-0.67432329522984613},{"$f":"ATAN(TAN('Solar Altitude'!F51)/COS('Surface Solar Azimuth Angles'!F105))","v":-0.63740014217672614},{"$f":"ATAN(TAN('Solar Altitude'!G51)/COS('Surface Solar Azimuth Angles'!G105))","v":-0.58586265313688612},{"$f":"ATAN(TAN('Solar Altitude'!H51)/COS('Surface Solar Azimuth Angles'!H105))","v":-0.5374341930134342},{"$f":"ATAN(TAN('Solar Altitude'!I51)/COS('Surface Solar Azimuth Angles'!I105))","v":-0.53995019403937616},{"$f":"ATAN(TAN('Solar Altitude'!J51)/COS('Surface Solar Azimuth Angles'!J105))","v":-0.62017385269735259},{"$f":"ATAN(TAN('Solar Altitude'!K51)/COS('Surface Solar Azimuth Angles'!K105))","v":-0.73908870770470347},{"$f":"ATAN(TAN('Solar Altitude'!L51)/COS('Surface Solar Azimuth Angles'!L105))","v":-0.82955153298556916},{"$f":"ATAN(TAN('Solar Altitude'!M51)/COS('Surface Solar Azimuth Angles'!M105))","v":-0.86919421625434168},{"$f":"ATAN(TAN('Solar Altitude'!N51)/COS('Surface Solar Azimuth Angles'!N105))","v":-0.84017901380444071},null,21,{"$f":"ATAN(TAN('Solar Altitude'!C51)/COS('Surface Solar Azimuth Angles'!Q105))","v":1.4926689138225644},{"$f":"ATAN(TAN('Solar Altitude'!D51)/COS('Surface Solar Azimuth Angles'!R105))","v":-1.4244661198800126},{"$f":"ATAN(TAN('Solar Altitude'!E51)/COS('Surface Solar Azimuth Angles'!S105))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F51)/COS('Surface Solar Azimuth Angles'!T105))","v":-0.84257659010007857},{"$f":"ATAN(TAN('Solar Altitude'!G51)/COS('Surface Solar Azimuth Angles'!U105))","v":-0.65069747813555467},{"$f":"ATAN(TAN('Solar Altitude'!H51)/COS('Surface Solar Azimuth Angles'!V105))","v":-0.57207111370754471},{"$f":"ATAN(TAN('Solar Altitude'!I51)/COS('Surface Solar Azimuth Angles'!W105))","v":-0.62738252671884254},{"$f":"ATAN(TAN('Solar Altitude'!J51)/COS('Surface Solar Azimuth Angles'!X105))","v":-0.8330645277261437},{"$f":"ATAN(TAN('Solar Altitude'!K51)/COS('Surface Solar Azimuth Angles'!Y105))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L51)/COS('Surface Solar Azimuth Angles'!Z105))","v":-1.3922681911981456},{"$f":"ATAN(TAN('Solar Altitude'!M51)/COS('Surface Solar Azimuth Angles'!AA105))","v":1.5401075773273576},{"$f":"ATAN(TAN('Solar Altitude'!N51)/COS('Surface Solar Azimuth Angles'!AB105))","v":1.4405551263701017}]
[null,22,{"$f":"ATAN(TAN('Solar Altitude'!C52)/COS('Surface Solar Azimuth Angles'!C51))","v":1.5539445877602391},{"$f":"ATAN(TAN('Solar Altitude'!D52)/COS('Surface Solar Azimuth Angles'!D51))","v":1.3649967109877184},{"$f":"ATAN(TAN('Solar Altitude'!E52)/COS('Surface Solar Azimuth Angles'!E51))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F52)/COS('Surface Solar Azimuth Angles'!F51))","v":0.89738136477565211},{"$f":"ATAN(TAN('Solar Altitude'!G52)/COS('Surface Solar Azimuth Angles'!G51))","v":0.73245268972748745},{"$f":"ATAN(TAN('Solar Altitude'!H52)/COS('Surface Solar Azimuth Angles'!H51))","v":0.6663048373130509},{"$f":"ATAN(TAN('Solar Altitude'!I52)/COS('Surface Solar Azimuth Angles'!I51))","v":0.71892314829995663},{"$f":"ATAN(TAN('Solar Altitude'!J52)/COS('Surface Solar Azimuth Angles'!J51))","v":0.89109084416912154},{"$f":"ATAN(TAN('Solar Altitude'!K52)/COS('Surface Solar Azimuth Angles'!K51))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L52)/COS('Surface Solar Azimuth Angles'!L51))","v":1.3503950367995552},{"$f":"ATAN(TAN('Solar Altitude'!M52)/COS('Surface Solar Azimuth Angles'!M51))","v":1.529878658594682},{"$f":"ATAN(TAN('Solar Altitude'!N52)/COS('Surface Solar Azimuth Angles'!N51))","v":-1.5317777100487906},null,22,{"$f":"ATAN(TAN('Solar Altitude'!C52)/COS('Surface Solar Azimuth Angles'!Q51))","v":1.0077487946336263},{"$f":"ATAN(TAN('Solar Altitude'!D52)/COS('Surface Solar Azimuth Angles'!R51))","v":0.95743316995573291},{"$f":"ATAN(TAN('Solar Altitude'!E52)/COS('Surface Solar Azimuth Angles'!S51))","v":0.9383140971407391},{"$f":"ATAN(TAN('Solar Altitude'!F52)/COS('Surface Solar Azimuth Angles'!T51))","v":0.92011364949964081},{"$f":"ATAN(TAN('Solar Altitude'!G52)/COS('Surface Solar Azimuth Angles'!U51))","v":0.8817647402793598},{"$f":"ATAN(TAN('Solar Altitude'!H52)/COS('Surface Solar Azimuth Angles'!V51))","v":0.83552237145082953},{"$f":"ATAN(TAN('Solar Altitude'!I52)/COS('Surface Solar Azimuth Angles'!W51))","v":0.83162347526531155},{"$f":"ATAN(TAN('Solar Altitude'!J52)/COS('Surface Solar Azimuth Angles'!X51))","v":0.90195784379562749},{"$f":"ATAN(TAN('Solar Altitude'!K52)/COS('Surface Solar Azimuth Angles'!Y51))","v":1.0063600686241212},{"$f":"ATAN(TAN('Solar Altitude'!L52)/COS('Surface Solar Azimuth Angles'!Z51))","v":1.0823876155652608},{"$f":"ATAN(TAN('Solar Altitude'!M52)/COS('Surface Solar Azimuth Angles'!AA51))","v":1.1078788719054964},{"$f":"ATAN(TAN('Solar Altitude'!N52)/COS('Surface Solar Azimuth Angles'!AB51))","v":1.0723844562125873},null,22,{"$f":"ATAN(TAN('Solar Altitude'!C52)/COS('Surface Solar Azimuth Angles'!C106))","v":-1.0077487946336263},{"$f":"ATAN(TAN('Solar Altitude'!D52)/COS('Surface Solar Azimuth Angles'!D106))","v":-0.95743316995573291},{"$f":"ATAN(TAN('Solar Altitude'!E52)/COS('Surface Solar Azimuth Angles'!E106))","v":-0.93831409714073899},{"$f":"ATAN(TAN('Solar Altitude'!F52)/COS('Surface Solar Azimuth Angles'!F106))","v":-0.92011364949964081},{"$f":"ATAN(TAN('Solar Altitude'!G52)/COS('Surface Solar Azimuth Angles'!G106))","v":-0.88176474027935958},{"$f":"ATAN(TAN('Solar Altitude'!H52)/COS('Surface Solar Azimuth Angles'!H106))","v":-0.83552237145082942},{"$f":"ATAN(TAN('Solar Altitude'!I52)/COS('Surface Solar Azimuth Angles'!I106))","v":-0.83162347526531155},{"$f":"ATAN(TAN('Solar Altitude'!J52)/COS('Surface Solar Azimuth Angles'!J106))","v":-0.9019578437956276},{"$f":"ATAN(TAN('Solar Altitude'!K52)/COS('Surface Solar Azimuth Angles'!K106))","v":-1.0063600686241212},{"$f":"ATAN(TAN('Solar Altitude'!L52)/COS('Surface Solar Azimuth Angles'!L106))","v":-1.0823876155652608},{"$f":"ATAN(TAN('Solar Altitude'!M52)/COS('Surface Solar Azimuth Angles'!M106))","v":-1.1078788719054964},{"$f":"ATAN(TAN('Solar Altitude'!N52)/COS('Surface Solar Azimuth Angles'!N106))","v":-1.0723844562125873},null,22,{"$f":"ATAN(TAN('Solar Altitude'!C52)/COS('Surface Solar Azimuth Angles'!Q106))","v":-1.5539445877602389},{"$f":"ATAN(TAN('Solar Altitude'!D52)/COS('Surface Solar Azimuth Angles'!R106))","v":-1.3649967109877184},{"$f":"ATAN(TAN('Solar Altitude'!E52)/COS('Surface Solar Azimuth Angles'!S106))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F52)/COS('Surface Solar Azimuth Angles'!T106))","v":-0.89738136477565211},{"$f":"ATAN(TAN('Solar Altitude'!G52)/COS('Surface Solar Azimuth Angles'!U106))","v":-0.73245268972748745},{"$f":"ATAN(TAN('Solar Altitude'!H52)/COS('Surface Solar Azimuth Angles'!V106))","v":-0.66630483731305101},{"$f":"ATAN(TAN('Solar Altitude'!I52)/COS('Surface Solar Azimuth Angles'!W106))","v":-0.71892314829995663},{"$f":"ATAN(TAN('Solar Altitude'!J52)/COS('Surface Solar Azimuth Angles'!X106))","v":-0.89109084416912154},{"$f":"ATAN(TAN('Solar Altitude'!K52)/COS('Surface Solar Azimuth Angles'!Y106))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L52)/COS('Surface Solar Azimuth Angles'!Z106))","v":-1.3503950367995554},{"$f":"ATAN(TAN('Solar Altitude'!M52)/COS('Surface Solar Azimuth Angles'!AA106))","v":-1.529878658594682},{"$f":"ATAN(TAN('Solar Altitude'!N52)/COS('Surface Solar Azimuth Angles'!AB106))","v":1.5317777100487904}]
[null,23,{"$f":"ATAN(TAN('Solar Altitude'!C53)/COS('Surface Solar Azimuth Angles'!C52))","v":1.5065295005919666},{"$f":"ATAN(TAN('Solar Altitude'!D53)/COS('Surface Solar Azimuth Angles'!D52))","v":1.3366001752956176},{"$f":"ATAN(TAN('Solar Altitude'!E53)/COS('Surface Solar Azimuth Angles'!E52))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F53)/COS('Surface Solar Azimuth Angles'!F52))","v":0.92334688213375749},{"$f":"ATAN(TAN('Solar Altitude'!G53)/COS('Surface Solar Azimuth Angles'!G52))","v":0.77241907924890529},{"$f":"ATAN(TAN('Solar Altitude'!H53)/COS('Surface Solar Azimuth Angles'!H52))","v":0.71359161627872214},{"$f":"ATAN(TAN('Solar Altitude'!I53)/COS('Surface Solar Azimuth Angles'!I52))","v":0.76448334246392113},{"$f":"ATAN(TAN('Solar Altitude'!J53)/COS('Surface Solar Azimuth Angles'!J52))","v":0.91872689706604005},{"$f":"ATAN(TAN('Solar Altitude'!K53)/COS('Surface Solar Azimuth Angles'!K52))","v":1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L53)/COS('Surface Solar Azimuth Angles'!L52))","v":1.3311946610818084},{"$f":"ATAN(TAN('Solar Altitude'!M53)/COS('Surface Solar Azimuth Angles'!M52))","v":1.495858034964566},{"$f":"ATAN(TAN('Solar Altitude'!N53)/COS('Surface Solar Azimuth Angles'!N52))","v":1.564326744571563},null,23,{"$f":"ATAN(TAN('Solar Altitude'!C53)/COS('Surface Solar Azimuth Angles'!Q52))","v":1.2495488396557735},{"$f":"ATAN(TAN('Solar Altitude'!D53)/COS('Surface Solar Azimuth Angles'!R52))","v":1.2145605673757462},{"$f":"ATAN(TAN('Solar Altitude'!E53)/COS('Surface Solar Azimuth Angles'!S52))","v":1.2149427363314722},{"$f":"ATAN(TAN('Solar Altitude'!F53)/COS('Surface Solar Azimuth Angles'!T52))","v":1.2226710666204357},{"$f":"ATAN(TAN('Solar Altitude'!G53)/COS('Surface Solar Azimuth Angles'!U52))","v":1.2055266879907172},{"$f":"ATAN(TAN('Solar Altitude'!H53)/COS('Surface Solar Azimuth Angles'!V52))","v":1.1656612779447797},{"$f":"ATAN(TAN('Solar Altitude'!I53)/COS('Surface Solar Azimuth Angles'!W52))","v":1.1517497376977253},{"$f":"ATAN(TAN('Solar Altitude'!J53)/COS('Surface Solar Azimuth Angles'!X52))","v":1.2039013058414905},{"$f":"ATAN(TAN('Solar Altitude'!K53)/COS('Surface Solar Azimuth Angles'!Y52))","v":1.2857310025410158},{"$f":"ATAN(TAN('Solar Altitude'!L53)/COS('Surface Solar Azimuth Angles'!Z52))","v":1.3427580313462963},{"$f":"ATAN(TAN('Solar Altitude'!M53)/COS('Surface Solar Azimuth Angles'!AA52))","v":1.3516188465533332},{"$f":"ATAN(TAN('Solar Altitude'!N53)/COS('Surface Solar Azimuth Angles'!AB52))","v":1.309046406575489},null,23,{"$f":"ATAN(TAN('Solar Altitude'!C53)/COS('Surface Solar Azimuth Angles'!C107))","v":-1.2495488396557735},{"$f":"ATAN(TAN('Solar Altitude'!D53)/COS('Surface Solar Azimuth Angles'!D107))","v":-1.2145605673757462},{"$f":"ATAN(TAN('Solar Altitude'!E53)/COS('Surface Solar Azimuth Angles'!E107))","v":-1.2149427363314722},{"$f":"ATAN(TAN('Solar Altitude'!F53)/COS('Surface Solar Azimuth Angles'!F107))","v":-1.2226710666204359},{"$f":"ATAN(TAN('Solar Altitude'!G53)/COS('Surface Solar Azimuth Angles'!G107))","v":-1.2055266879907172},{"$f":"ATAN(TAN('Solar Altitude'!H53)/COS('Surface Solar Azimuth Angles'!H107))","v":-1.1656612779447801},{"$f":"ATAN(TAN('Solar Altitude'!I53)/COS('Surface Solar Azimuth Angles'!I107))","v":-1.1517497376977255},{"$f":"ATAN(TAN('Solar Altitude'!J53)/COS('Surface Solar Azimuth Angles'!J107))","v":-1.2039013058414902},{"$f":"ATAN(TAN('Solar Altitude'!K53)/COS('Surface Solar Azimuth Angles'!K107))","v":-1.2857310025410158},{"$f":"ATAN(TAN('Solar Altitude'!L53)/COS('Surface Solar Azimuth Angles'!L107))","v":-1.3427580313462966},{"$f":"ATAN(TAN('Solar Altitude'!M53)/COS('Surface Solar Azimuth Angles'!M107))","v":-1.3516188465533332},{"$f":"ATAN(TAN('Solar Altitude'!N53)/COS('Surface Solar Azimuth Angles'!N107))","v":-1.309046406575489},null,23,{"$f":"ATAN(TAN('Solar Altitude'!C53)/COS('Surface Solar Azimuth Angles'!Q107))","v":-1.5065295005919663},{"$f":"ATAN(TAN('Solar Altitude'!D53)/COS('Surface Solar Azimuth Angles'!R107))","v":-1.3366001752956176},{"$f":"ATAN(TAN('Solar Altitude'!E53)/COS('Surface Solar Azimuth Angles'!S107))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!F53)/COS('Surface Solar Azimuth Angles'!T107))","v":-0.92334688213375749},{"$f":"ATAN(TAN('Solar Altitude'!G53)/COS('Surface Solar Azimuth Angles'!U107))","v":-0.77241907924890529},{"$f":"ATAN(TAN('Solar Altitude'!H53)/COS('Surface Solar Azimuth Angles'!V107))","v":-0.71359161627872203},{"$f":"ATAN(TAN('Solar Altitude'!I53)/COS('Surface Solar Azimuth Angles'!W107))","v":-0.76448334246392102},{"$f":"ATAN(TAN('Solar Altitude'!J53)/COS('Surface Solar Azimuth Angles'!X107))","v":-0.91872689706604016},{"$f":"ATAN(TAN('Solar Altitude'!K53)/COS('Surface Solar Azimuth Angles'!Y107))","v":-1.1397000015522973},{"$f":"ATAN(TAN('Solar Altitude'!L53)/COS('Surface Solar Azimuth Angles'!Z107))","v":-1.3311946610818084},{"$f":"ATAN(TAN('Solar Altitude'!M53)/COS('Surface Solar Azimuth Angles'!AA107))","v":-1.495858034964566},{"$f":"ATAN(TAN('Solar Altitude'!N53)/COS('Surface Solar Azimuth Angles'!AB107))","v":-1.564326744571563}]
[null,24,{"$f":"ATAN(TAN('Solar Altitude'!C54)/COS('Surface Solar Azimuth Angles'!C53))","v":1.488046906810496},{"$f":"ATAN(TAN('Solar Altitude'!D54)/COS('Surface Solar Azimuth Angles'!D53))","v":1.325468937525877},{"$f":"ATAN(TAN('Solar Altitude'!E54)/COS('Surface Solar Azimuth Angles'!E53))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F54)/COS('Surface Solar Azimuth Angles'!F53))","v":0.9319358845770338},{"$f":"ATAN(TAN('Solar Altitude'!G54)/COS('Surface Solar Azimuth Angles'!G53))","v":0.78535264346749045},{"$f":"ATAN(TAN('Solar Altitude'!H54)/COS('Surface Solar Azimuth Angles'!H53))","v":0.73016710880727165},{"$f":"ATAN(TAN('Solar Altitude'!I54)/COS('Surface Solar Azimuth Angles'!I53))","v":0.78135170593207048},{"$f":"ATAN(TAN('Solar Altitude'!J54)/COS('Surface Solar Azimuth Angles'!J53))","v":0.92833771723835001},{"$f":"ATAN(TAN('Solar Altitude'!K54)/COS('Surface Solar Azimuth Angles'!K53))","v":1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L54)/COS('Surface Solar Azimuth Angles'!L53))","v":1.3265689743998734},{"$f":"ATAN(TAN('Solar Altitude'!M54)/COS('Surface Solar Azimuth Angles'!M53))","v":1.4871559725393455},{"$f":"ATAN(TAN('Solar Altitude'!N54)/COS('Surface Solar Azimuth Angles'!N53))","v":1.5490861384984902},null,24,{"$f":"ATAN(TAN('Solar Altitude'!C54)/COS('Surface Solar Azimuth Angles'!Q53))","v":1.4953307389576809},{"$f":"ATAN(TAN('Solar Altitude'!D54)/COS('Surface Solar Azimuth Angles'!R53))","v":1.4778229951074291},{"$f":"ATAN(TAN('Solar Altitude'!E54)/COS('Surface Solar Azimuth Angles'!S53))","v":1.5005364967084429},{"$f":"ATAN(TAN('Solar Altitude'!F54)/COS('Surface Solar Azimuth Angles'!T53))","v":1.5387122061758478},{"$f":"ATAN(TAN('Solar Altitude'!G54)/COS('Surface Solar Azimuth Angles'!U53))","v":1.5486122132899969},{"$f":"ATAN(TAN('Solar Altitude'!H54)/COS('Surface Solar Azimuth Angles'!V53))","v":1.5196104703977531},{"$f":"ATAN(TAN('Solar Altitude'!I54)/COS('Surface Solar Azimuth Angles'!W53))","v":1.4935003073579074},{"$f":"ATAN(TAN('Solar Altitude'!J54)/COS('Surface Solar Azimuth Angles'!X53))","v":1.5200112597578943},{"$f":"ATAN(TAN('Solar Altitude'!K54)/COS('Surface Solar Azimuth Angles'!Y53))","v":1.5690353246394813},{"$f":"ATAN(TAN('Solar Altitude'!L54)/COS('Surface Solar Azimuth Angles'!Z53))","v":1.5342706134006172},{"$f":"ATAN(TAN('Solar Altitude'!M54)/COS('Surface Solar Azimuth Angles'!AA53))","v":1.5433489980684403},{"$f":"ATAN(TAN('Solar Altitude'!N54)/COS('Surface Solar Azimuth Angles'!AB53))","v":1.5486418126575423},null,24,{"$f":"ATAN(TAN('Solar Altitude'!C54)/COS('Surface Solar Azimuth Angles'!C108))","v":-1.4953307389576809},{"$f":"ATAN(TAN('Solar Altitude'!D54)/COS('Surface Solar Azimuth Angles'!D108))","v":-1.4778229951074291},{"$f":"ATAN(TAN('Solar Altitude'!E54)/COS('Surface Solar Azimuth Angles'!E108))","v":-1.5005364967084427},{"$f":"ATAN(TAN('Solar Altitude'!F54)/COS('Surface Solar Azimuth Angles'!F108))","v":-1.5387122061758483},{"$f":"ATAN(TAN('Solar Altitude'!G54)/COS('Surface Solar Azimuth Angles'!G108))","v":-1.5486122132899969},{"$f":"ATAN(TAN('Solar Altitude'!H54)/COS('Surface Solar Azimuth Angles'!H108))","v":-1.5196104703977529},{"$f":"ATAN(TAN('Solar Altitude'!I54)/COS('Surface Solar Azimuth Angles'!I108))","v":-1.4935003073579076},{"$f":"ATAN(TAN('Solar Altitude'!J54)/COS('Surface Solar Azimuth Angles'!J108))","v":-1.5200112597578943},{"$f":"ATAN(TAN('Solar Altitude'!K54)/COS('Surface Solar Azimuth Angles'!K108))","v":-1.569035324639481},{"$f":"ATAN(TAN('Solar Altitude'!L54)/COS('Surface Solar Azimuth Angles'!L108))","v":-1.5342706134006172},{"$f":"ATAN(TAN('Solar Altitude'!M54)/COS('Surface Solar Azimuth Angles'!M108))","v":-1.5433489980684403},{"$f":"ATAN(TAN('Solar Altitude'!N54)/COS('Surface Solar Azimuth Angles'!N108))","v":-1.5486418126575423},null,24,{"$f":"ATAN(TAN('Solar Altitude'!C54)/COS('Surface Solar Azimuth Angles'!Q108))","v":-1.488046906810496},{"$f":"ATAN(TAN('Solar Altitude'!D54)/COS('Surface Solar Azimuth Angles'!R108))","v":-1.325468937525877},{"$f":"ATAN(TAN('Solar Altitude'!E54)/COS('Surface Solar Azimuth Angles'!S108))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!F54)/COS('Surface Solar Azimuth Angles'!T108))","v":-0.9319358845770338},{"$f":"ATAN(TAN('Solar Altitude'!G54)/COS('Surface Solar Azimuth Angles'!U108))","v":-0.78535264346749045},{"$f":"ATAN(TAN('Solar Altitude'!H54)/COS('Surface Solar Azimuth Angles'!V108))","v":-0.73016710880727165},{"$f":"ATAN(TAN('Solar Altitude'!I54)/COS('Surface Solar Azimuth Angles'!W108))","v":-0.78135170593207048},{"$f":"ATAN(TAN('Solar Altitude'!J54)/COS('Surface Solar Azimuth Angles'!X108))","v":-0.92833771723835001},{"$f":"ATAN(TAN('Solar Altitude'!K54)/COS('Surface Solar Azimuth Angles'!Y108))","v":-1.1397000015522971},{"$f":"ATAN(TAN('Solar Altitude'!L54)/COS('Surface Solar Azimuth Angles'!Z108))","v":-1.3265689743998734},{"$f":"ATAN(TAN('Solar Altitude'!M54)/COS('Surface Solar Azimuth Angles'!AA108))","v":-1.4871559725393455},{"$f":"ATAN(TAN('Solar Altitude'!N54)/COS('Surface Solar Azimuth Angles'!AB108))","v":-1.5490861384984902}]

{"sheet":"Solar Azimuth","index":17,"n_rows":53,"n_cols":29,"rows_kept":53,"cut":false,"hidden":true,"merged":[[2,28,2,29]]}
[]
[null,null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec",null,{"$error":"#REF!"},"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"DEGREES(C30)","v":114.42309856189749},145.01866125000959,154.35900651846384,158.68036485144134,161.88012117394979,164.47228133381614,164.88960695959625,160.07401314187376,147.16438917420371,127.81849177627836,103.98661304621145,92.926107523614064,null,1,-67.34291307045126,-58.873944547125859,-48.247906843226311,-36.196403399043412,-27.919347230648427,-25.095644420933699,-28.212562730491825,-36.210475033762386,-47.143442994419665,-56.273650868447859,-64.431619800093173,-68.961381110697076,"Home"]
[null,2,{"$f":"DEGREES(C31)","v":96.453295295662869},116.58936603917034,130.1624952301172,139.50906482919788,145.31232618983634,148.52493328219171,147.81507211585009,140.63416607539401,125.79538213031562,108.96560729234663,92.920040610035116,86.74169228845723,null,2,-59.253830266299929,-52.368647392734104,-42.500052549852711,-30.984400236091219,-23.201487232507503,-20.790977563535858,-23.939353009945375,-31.186206449489852,-40.581317954717477,-48.114573505537905,-55.063627845477271,-59.536188478064517]
[null,3,{"$f":"DEGREES(C32)","v":89.051635649875607},103.31352191067661,115.40543082307254,125.70260632132135,132.47437783928015,135.83260490366516,134.43597736215381,126.56858704244209,112.61329653323939,98.771121643370421,86.68606599673916,82.439051076130838,null,3,-48.798281851244163,-42.997519930765392,-33.994154337292343,-23.262138426459856,-16.120459836107415,-14.13260505974079,-17.205608899453892,-23.604311052306677,-31.578219022957924,-37.927353025891577,-44.150799722550104,-48.525634871649785]
[null,4,{"$f":"DEGREES(C33)","v":83.645077965680898},94.983105135991053,105.54889999051608,115.67424185262344,122.72328942010087,126.04880339758887,124.27040515449995,116.36534992403649,103.51551123372408,91.561421644549611,81.563139551542861,78.320210105456809,null,4,-37.516186466663655,-32.246362637149872,-23.861267050468381,-13.834912200772216,-7.3095696423615601,-5.698998741316637,-8.6463118192006174,-14.273141613573273,-21.168432848804272,-26.813459668745324,-32.73481634221605,-37.079780076826268]
[null,5,{"$f":"DEGREES(C34)","v":78.667572941814512},88.453088384837585,98.0315040139551,107.92784498628035,115.12801284478837,118.42261537221856,116.3954983583661,108.51604214772064,96.348104005150986,85.416260532668915,76.561191142844791,73.938144334618258,null,5,-26.039128387868409,-20.906969341202434,-12.848329386468352,-3.324049871165903,2.6976333808670212,4.0002926212727177,1.1871627358841379,-3.8237538015881283,-10.017590037183291,-15.361298690679538,-21.285343418032358,-25.654571832144214]
[null,6,{"$f":"DEGREES(C35)","v":73.488492077926935},82.464473557261059,91.530413775338687,101.44881339595754,108.93731604152855,112.29007277032856,110.03139679027041,101.98746755551197,89.961695491259746,79.416038586607996,71.161731793949599,68.987603220711861,null,6,-14.713057127587101,-9.4322683077017686,-1.4362273821002971,7.8247315987352639,13.494423779465302,14.566497497423766,11.870491752344792,7.2902942503321162,1.4362273821003024,-3.9452246222390919,-10.104600138376378,-14.530195511023541]
[null,7,{"$f":"DEGREES(C36)","v":67.647288527019725},76.274229184511228,85.209001105128564,95.51931316773377,103.59914856777166,107.16015360598314,104.6042787468042,96.053854503327031,83.570803318642589,72.888563250533565,64.901671637150741,63.128359138793968,null,7,-3.8172313160401323,1.8451738042345256,10.017590037183295,19.270251900735218,24.76713343071405,25.692296291946072,23.079294024613102,18.724334672709144,12.848329386468352,7.1146387627072185,0.52526019866404239,-3.9663293986980483]
[null,8,{"$f":"DEGREES(C37)","v":60.634193010300976},69.204562240532979,78.310385534053466,89.486122264914655,98.663754358878165,102.67188093597633,99.661837469673486,90.068762910981377,76.387961658043494,65.091765063126061,57.212438245033646,55.905386143263541,null,8,6.3416614129377571,12.593168449752618,21.168432848804265,30.693647378695427,36.239358184359844,37.118076936105247,34.536802784154659,30.161534504288316,23.861267050468388,17.453948508754195,10.267582525633415,5.7294655452000383]
[null,9,{"$f":"DEGREES(C38)","v":51.768748339976497},60.379685639709628,69.814353609182064,82.45083421497344,93.627688952569216,98.521187051411133,94.735373704691739,83.168099105996617,67.256262036750698,54.962752878328075,47.319157053161554,46.69540702919015,null,9,15.369939199198676,22.391847480615322,31.578219022957924,41.691335060208353,47.586746292272693,48.563410565501172,45.936655755399158,41.208862760397267,33.994154337292336,26.580184965290567,18.679024282565258,14.15806059503065]
[null,10,{"$f":"DEGREES(C39)","v":40.148034381332685},48.471328297789526,57.889532705571163,72.497654057460437,87.520988749472963,94.32570869615293,89.01523478336928,73.552305529127068,54.003522769149818,40.89681624413825,34.26382672583707,34.744710793512169,null,10,22.747483925566623,30.652669196304778,40.581317954717484,51.581548868691684,58.246756428510785,59.571252831647172,56.780573723037691,51.210965171546022,42.500052549852711,33.802676213029343,25.185543515834862,20.80955841975068]
[null,11,{"$f":"DEGREES(C40)","v":24.885076293015025},31.635752238757334,38.941064079848665,53.640222898119461,76.561283289908715,88.98202668740042,79.732186026550423,55.672233384753454,32.502388308448495,21.136723538029337,17.409277392405681,19.534720568739846,null,11,27.841641845394268,36.578518995643407,47.143442994419665,59.037957699912447,66.866937328669266,68.987347949028148,65.911372667518705,58.889615974212646,48.247906843226311,38.255741942845674,29.138661402864003,25.105441885715948]
[null,12,{"$f":"DEGREES(C41)","v":6.1188489470903447},8.886713641915156,8.6992261524728125,6.6354940803276321,11.563825851086857,57.747874143760271,36.885376570622384,10.575312516834758,0.21936712106550094,3.5020973891401352,2.231001794012502,1.7032943301877761,null,12,30.043065592921938,39.297422050811605,49.96345460797054,61.898949753135703,70.287344871146473,73.447362784585749,70.454985838193679,62.094971647097431,49.96345460797054,39.174338794154615,30.013585327070484,26.548903072705901]
[null,13,{"$f":"DEGREES(C42)","v":-13.732736529787083},-16.214430009759653,-25.640993481536086,-47.353608937771028,-74.056458822561879,-86.585446106298974,-71.01828631253062,-45.719410912822127,-32.835610825796458,-27.197074749164472,-21.470648812116224,-16.394081517196998,null,13,29.028417232729712,38.283193148823699,48.247906843226311,58.831175781038695,66.098038897969786,69.345344212800683,67.36300929531231,59.342823779550301,47.143442994419665,36.370932809694331,27.677047917356862,24.944854138597314]
[null,14,{"$f":"DEGREES(C43)","v":-31.28592570493214},-37.293205030475256,-49.837504769882834,-69.769134988610915,-86.550699785984065,-93.022220626043548,-85.700382385824142,-69.264391581123419,-54.204617869684419,-45.278037008383571,-37.485193501585897,-32.187947719108017,null,14,24.951888025418906,33.743255349927217,42.500052549852711,51.251023866588341,57.137758950733314,60.060473121473578,58.868986713807793,51.93404290064872,40.581317954717484,30.384006920425502,22.470331831080628,20.50913126771437]
[null,15,{"$f":"DEGREES(C44)","v":-45.058519967661788},-52.457029272774619,-64.594569176927493,-80.781572637663501,-92.938946076383814,-97.35546955215915,-92.370481478237664,-80.54650204480518,-67.386703466760636,-58.067744603194065,-49.756153233223152,-44.719738705082868,null,15,18.349443127303218,26.454270998210269,33.994154337292336,41.302121857975443,46.358286307558956,49.091803085097418,48.246740749638235,42.059224555704382,31.578219022957924,22.08449010973154,15.008700184081292,13.748426210035035]
[null,16,{"$f":"DEGREES(C45)","v":-55.489647334482406},-63.268838319612385,-74.451100009483923,-88.190523243217299,-98.038708423169382,-101.47026561710798,-97.504147180777991,-88.03087166189701,-76.484488766275902,-67.419407516747285,-59.080566092086663,-54.377535612582086,null,16,9.8693453359863668,17.282156871461542,23.861267050468388,30.279332346250538,34.976621684622607,37.654264268640453,36.909472861263531,31.066003604870311,21.168432848804265,12.262965835366582,5.9216307857404376,5.2403316347409667]
[null,17,{"$f":"DEGREES(C46)","v":-63.539276864661694},-71.455355595557094,-81.968495986044886,-94.337010348548603,-102.95522704697413,-105.83177114686136,-102.37321631179329,-94.190598078587101,-83.651895994848999,-74.778716570691742,-66.393607183024301,-61.914731817905739,null,17,8.0290509663246551E-2,6.9133606198289508,12.848329386468352,18.848933627939225,23.512347180587447,26.220785722188356,25.435802303802891,19.6435787872284,10.017590037183295,1.5022637240415271,-4.2765520266745858,-4.5108792992946594]
[null,18,{"$f":"DEGREES(C47)","v":-70.027393642454314},-78.184177378909311,-88.469586224661327,-100.23260842709193,-108.21764026515396,-110.74646928371035,-107.53210586168318,-100.0676048936829,-90.038304508740268,-81.094337680102015,-72.41888926958508,-67.986814060671676,null,18,-10.579820253990412,-4.163436110610812,1.4362273821003024,7.4087926120293481,12.278348067636838,15.075368752325566,14.153334325863906,8.1973900724136648,-1.4362273821002971,-9.7811699755294921,-15.196946322592352,-15.111762260291776]
[null,19,{"$f":"DEGREES(C48)","v":-75.556391539792401},-84.245727157077454,-94.79099889487145,-106.54893394025623,-114.27191412220648,-116.55069372400413,-113.41866453412055,-106.33684414244284,-96.429196681357439,-87.064134050269075,-77.691193599583684,-73.076880837173803,null,19,-21.777891428440284,-15.585858558235014,-10.017590037183291,-3.7230253587200623,1.5517932904361937,4.4767742274235207,3.3372603357716155,-2.9540368719808745,-12.848329386468352,-21.256477811065686,-26.535415779836313,-26.258559384200282]
[null,20,{"$f":"DEGREES(C49)","v":-80.599865452912837},-90.306993062276334,-101.68961446594655,-113.97185161701486,-121.65067573224731,-123.69219192139745,-120.53929365745837,-113.67365388535441,-103.61203834195651,-93.389012330405194,-82.668583232769393,-77.541146776659929,null,20,-33.232689038050758,-27.033422535648885,-21.168432848804272,-14.202907972745095,-8.3458483020022562,-5.2710059849994169,-6.7027006227320731,-13.471353470780777,-23.861267050468381,-32.590259160291865,-38.012183628954979,-37.692565133941223]
[null,21,{"$f":"DEGREES(C50)","v":-85.646972023274472},-97.199415582430262,-110.18564639081795,-123.43780160531772,-131.07652361833965,-132.785358202845,-129.57634581131595,-122.98914291063117,-112.7437379632493,-101.151822128156,-87.919466525852556,-81.683344132077423,null,21,-44.638695834079385,-38.128127309747875,-31.578219022957924,-23.57983142969492,-16.994952910323736,-13.774174242063397,-15.566310373178142,-22.912530896636454,-33.994154337292343,-43.325188261570887,-49.274998449936852,-49.129511134693338]
[null,22,{"$f":"DEGREES(C51)","v":-91.529453169268862},-106.51792647513759,-122.11046729442886,-136.34276711408791,-143.46901721591678,-144.58190194480306,-141.41793606781556,-135.63829506381219,-125.99647723085019,-112.86261366161574,-94.689514278894165,-85.897207065730697,null,22,-55.512928960509555,-48.272235528931432,-40.581317954717477,-31.225148249783931,-23.847930357512382,-20.528103037474033,-22.728239055250722,-30.662326982023345,-42.500052549852711,-52.657411948411088,-59.670366582469114,-60.09529480048743]
[null,23,{"$f":"DEGREES(C52)","v":-100.94534800876922},-122.66538882339935,-141.05893592015133,-154.36297602700361,-159.5630698100631,-159.62986186666328,-156.86896866670523,-153.28158651377788,-147.49761169155158,-136.46938858849168,-108.62615799444323,-91.383419869830902,null,23,-64.771202166269092,-56.346809716872606,-47.143442994419665,-36.328737409072268,-28.267133802853241,-24.955129611825427,-27.561295345606922,-35.922684824324769,-48.247906843226311,-59.077263046421628,-67.594339095971577,-69.370511622090149]
[null,24,{"$f":"DEGREES(C53)","v":-137.64688656852812},-159.57383416203882,-171.30077384752721,-177.5257986958168,-178.72905959747521,-177.37410739696531,-175.60682113053886,-176.11448991066359,-179.78063287893619,-171.65782889745896,-161.86764260752923,-134.41945830007725,null,24,-69.757115045995235,-60.438815152921329,-49.96345460797054,-38.099371377431837,-29.695087450456722,-26.549160163299536,-29.482718077635045,-37.897017981208357,-49.96345460797054,-60.501729867895293,-69.683476500791514,-73.446555558668365]
[]
[]
[null,"Rad","Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[null,1,{"$f":"ACOS(((SIN('Solar Altitude'!C31)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C31)*COS('Input Data'!$G$3)))","v":1.9970598102391},{"$f":"ACOS(((SIN('Solar Altitude'!D31)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D31)*COS('Input Data'!$G$3)))","v":2.5310531156469827},{"$f":"ACOS(((SIN('Solar Altitude'!E31)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E31)*COS('Input Data'!$G$3)))","v":2.6940728938545835},{"$f":"ACOS(((SIN('Solar Altitude'!F31)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F31)*COS('Input Data'!$G$3)))","v":2.7694948249235343},{"$f":"ACOS(((SIN('Solar Altitude'!G31)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G31)*COS('Input Data'!$G$3)))","v":2.8253411080128119},{"$f":"ACOS(((SIN('Solar Altitude'!H31)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H31)*COS('Input Data'!$G$3)))","v":2.8705828375415026},{"$f":"ACOS(((SIN('Solar Altitude'!I31)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I31)*COS('Input Data'!$G$3)))","v":2.8778665437643109},{"$f":"ACOS(((SIN('Solar Altitude'!J31)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J31)*COS('Input Data'!$G$3)))","v":2.7938185762063701},{"$f":"ACOS(((SIN('Solar Altitude'!K31)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K31)*COS('Input Data'!$G$3)))","v":2.5685031327761534},{"$f":"ACOS(((SIN('Solar Altitude'!L31)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L31)*COS('Input Data'!$G$3)))","v":2.2308535264293528},{"$f":"ACOS(((SIN('Solar Altitude'!M31)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M31)*COS('Input Data'!$G$3)))","v":1.8149087756536801},{"$f":"ACOS(((SIN('Solar Altitude'!N31)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N31)*COS('Input Data'!$G$3)))","v":1.6218665373493397}]
[null,2,{"$f":"ACOS(((SIN('Solar Altitude'!C32)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C32)*COS('Input Data'!$G$3)))","v":1.6834275773076746},{"$f":"ACOS(((SIN('Solar Altitude'!D32)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D32)*COS('Input Data'!$G$3)))","v":2.0348683101963827},{"$f":"ACOS(((SIN('Solar Altitude'!E32)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E32)*COS('Input Data'!$G$3)))","v":2.2717641043769596},{"$f":"ACOS(((SIN('Solar Altitude'!F32)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F32)*COS('Input Data'!$G$3)))","v":2.4348925176477234},{"$f":"ACOS(((SIN('Solar Altitude'!G32)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G32)*COS('Input Data'!$G$3)))","v":2.5361785357446309},{"$f":"ACOS(((SIN('Solar Altitude'!H32)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H32)*COS('Input Data'!$G$3)))","v":2.5922491070791533},{"$f":"ACOS(((SIN('Solar Altitude'!I32)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I32)*COS('Input Data'!$G$3)))","v":2.5798596924944448},{"$f":"ACOS(((SIN('Solar Altitude'!J32)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J32)*COS('Input Data'!$G$3)))","v":2.4545292388121371},{"$f":"ACOS(((SIN('Solar Altitude'!K32)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K32)*COS('Input Data'!$G$3)))","v":2.195543601978446},{"$f":"ACOS(((SIN('Solar Altitude'!L32)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L32)*COS('Input Data'!$G$3)))","v":1.9018086186865921},{"$f":"ACOS(((SIN('Solar Altitude'!M32)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M32)*COS('Input Data'!$G$3)))","v":1.6217606497319532},{"$f":"ACOS(((SIN('Solar Altitude'!N32)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N32)*COS('Input Data'!$G$3)))","v":1.5139281291853535}]
[null,3,{"$f":"ACOS(((SIN('Solar Altitude'!C33)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C33)*COS('Input Data'!$G$3)))","v":1.5542442463766897},{"$f":"ACOS(((SIN('Solar Altitude'!D33)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D33)*COS('Input Data'!$G$3)))","v":1.8031611191726098},{"$f":"ACOS(((SIN('Solar Altitude'!E33)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E33)*COS('Input Data'!$G$3)))","v":2.0142047425451652},{"$f":"ACOS(((SIN('Solar Altitude'!F33)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F33)*COS('Input Data'!$G$3)))","v":2.1939243586452948},{"$f":"ACOS(((SIN('Solar Altitude'!G33)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G33)*COS('Input Data'!$G$3)))","v":2.31211406782645},{"$f":"ACOS(((SIN('Solar Altitude'!H33)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H33)*COS('Input Data'!$G$3)))","v":2.3707261871295522},{"$f":"ACOS(((SIN('Solar Altitude'!I33)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I33)*COS('Input Data'!$G$3)))","v":2.3463504381061453},{"$f":"ACOS(((SIN('Solar Altitude'!J33)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J33)*COS('Input Data'!$G$3)))","v":2.2090385734876463},{"$f":"ACOS(((SIN('Solar Altitude'!K33)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K33)*COS('Input Data'!$G$3)))","v":1.9654728060297433},{"$f":"ACOS(((SIN('Solar Altitude'!L33)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L33)*COS('Input Data'!$G$3)))","v":1.7238812785646462},{"$f":"ACOS(((SIN('Solar Altitude'!M33)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M33)*COS('Input Data'!$G$3)))","v":1.5129572672441984},{"$f":"ACOS(((SIN('Solar Altitude'!N33)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N33)*COS('Input Data'!$G$3)))","v":1.4388328734982576}]
[null,4,{"$f":"ACOS(((SIN('Solar Altitude'!C34)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C34)*COS('Input Data'!$G$3)))","v":1.4598820135884922},{"$f":"ACOS(((SIN('Solar Altitude'!D34)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D34)*COS('Input Data'!$G$3)))","v":1.6577679183909801},{"$f":"ACOS(((SIN('Solar Altitude'!E34)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E34)*COS('Input Data'!$G$3)))","v":1.8421758266927173},{"$f":"ACOS(((SIN('Solar Altitude'!F34)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F34)*COS('Input Data'!$G$3)))","v":2.0188963800765043},{"$f":"ACOS(((SIN('Solar Altitude'!G34)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G34)*COS('Input Data'!$G$3)))","v":2.1419254692586827},{"$f":"ACOS(((SIN('Solar Altitude'!H34)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H34)*COS('Input Data'!$G$3)))","v":2.1999666374869409},{"$f":"ACOS(((SIN('Solar Altitude'!I34)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I34)*COS('Input Data'!$G$3)))","v":2.1689277327333567},{"$f":"ACOS(((SIN('Solar Altitude'!J34)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J34)*COS('Input Data'!$G$3)))","v":2.0309584914097703},{"$f":"ACOS(((SIN('Solar Altitude'!K34)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K34)*COS('Input Data'!$G$3)))","v":1.8066864979136628},{"$f":"ACOS(((SIN('Solar Altitude'!L34)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L34)*COS('Input Data'!$G$3)))","v":1.5980482755041918},{"$f":"ACOS(((SIN('Solar Altitude'!M34)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M34)*COS('Input Data'!$G$3)))","v":1.4235453334380341},{"$f":"ACOS(((SIN('Solar Altitude'!N34)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N34)*COS('Input Data'!$G$3)))","v":1.3669455371939565}]
[null,5,{"$f":"ACOS(((SIN('Solar Altitude'!C35)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C35)*COS('Input Data'!$G$3)))","v":1.3730081623874648},{"$f":"ACOS(((SIN('Solar Altitude'!D35)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D35)*COS('Input Data'!$G$3)))","v":1.5437976258729691},{"$f":"ACOS(((SIN('Solar Altitude'!E35)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E35)*COS('Input Data'!$G$3)))","v":1.7109725157255538},{"$f":"ACOS(((SIN('Solar Altitude'!F35)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F35)*COS('Input Data'!$G$3)))","v":1.8836962495926464},{"$f":"ACOS(((SIN('Solar Altitude'!G35)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G35)*COS('Input Data'!$G$3)))","v":2.0093628854198804},{"$f":"ACOS(((SIN('Solar Altitude'!H35)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H35)*COS('Input Data'!$G$3)))","v":2.066864547068064},{"$f":"ACOS(((SIN('Solar Altitude'!I35)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I35)*COS('Input Data'!$G$3)))","v":2.031484680853143},{"$f":"ACOS(((SIN('Solar Altitude'!J35)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J35)*COS('Input Data'!$G$3)))","v":1.8939622267106639},{"$f":"ACOS(((SIN('Solar Altitude'!K35)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K35)*COS('Input Data'!$G$3)))","v":1.6815916429438205},{"$f":"ACOS(((SIN('Solar Altitude'!L35)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L35)*COS('Input Data'!$G$3)))","v":1.4907949810363581},{"$f":"ACOS(((SIN('Solar Altitude'!M35)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M35)*COS('Input Data'!$G$3)))","v":1.3362448646913618},{"$f":"ACOS(((SIN('Solar Altitude'!N35)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N35)*COS('Input Data'!$G$3)))","v":1.2904640614538805}]
[null,6,{"$f":"ACOS(((SIN('Solar Altitude'!C36)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C36)*COS('Input Data'!$G$3)))","v":1.2826161490855943},{"$f":"ACOS(((SIN('Solar Altitude'!D36)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D36)*COS('Input Data'!$G$3)))","v":1.439276579498006},{"$f":"ACOS(((SIN('Solar Altitude'!E36)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E36)*COS('Input Data'!$G$3)))","v":1.5975070860924334},{"$f":"ACOS(((SIN('Solar Altitude'!F36)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F36)*COS('Input Data'!$G$3)))","v":1.770615816000789},{"$f":"ACOS(((SIN('Solar Altitude'!G36)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G36)*COS('Input Data'!$G$3)))","v":1.9013148432103089},{"$f":"ACOS(((SIN('Solar Altitude'!H36)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H36)*COS('Input Data'!$G$3)))","v":1.9598314871462639},{"$f":"ACOS(((SIN('Solar Altitude'!I36)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I36)*COS('Input Data'!$G$3)))","v":1.9204101545585393},{"$f":"ACOS(((SIN('Solar Altitude'!J36)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J36)*COS('Input Data'!$G$3)))","v":1.7800171046145765},{"$f":"ACOS(((SIN('Solar Altitude'!K36)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K36)*COS('Input Data'!$G$3)))","v":1.5701277869990202},{"$f":"ACOS(((SIN('Solar Altitude'!L36)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L36)*COS('Input Data'!$G$3)))","v":1.3860713522271735},{"$f":"ACOS(((SIN('Solar Altitude'!M36)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M36)*COS('Input Data'!$G$3)))","v":1.2420065212255516},{"$f":"ACOS(((SIN('Solar Altitude'!N36)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N36)*COS('Input Data'!$G$3)))","v":1.2040608192608664}]
[null,7,{"$f":"ACOS(((SIN('Solar Altitude'!C37)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C37)*COS('Input Data'!$G$3)))","v":1.1806679148430792},{"$f":"ACOS(((SIN('Solar Altitude'!D37)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D37)*COS('Input Data'!$G$3)))","v":1.3312364336904705},{"$f":"ACOS(((SIN('Solar Altitude'!E37)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E37)*COS('Input Data'!$G$3)))","v":1.4871776216199803},{"$f":"ACOS(((SIN('Solar Altitude'!F37)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F37)*COS('Input Data'!$G$3)))","v":1.6671265140205289},{"$f":"ACOS(((SIN('Solar Altitude'!G37)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G37)*COS('Input Data'!$G$3)))","v":1.8081462447703833},{"$f":"ACOS(((SIN('Solar Altitude'!H37)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H37)*COS('Input Data'!$G$3)))","v":1.8702975073672801},{"$f":"ACOS(((SIN('Solar Altitude'!I37)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I37)*COS('Input Data'!$G$3)))","v":1.8256890758056612},{"$f":"ACOS(((SIN('Solar Altitude'!J37)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J37)*COS('Input Data'!$G$3)))","v":1.6764560203146393},{"$f":"ACOS(((SIN('Solar Altitude'!K37)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K37)*COS('Input Data'!$G$3)))","v":1.4585856764469169},{"$f":"ACOS(((SIN('Solar Altitude'!L37)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L37)*COS('Input Data'!$G$3)))","v":1.2721454157699512},{"$f":"ACOS(((SIN('Solar Altitude'!M37)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M37)*COS('Input Data'!$G$3)))","v":1.1327478601164989},{"$f":"ACOS(((SIN('Solar Altitude'!N37)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N37)*COS('Input Data'!$G$3)))","v":1.1017977183534067}]
[null,8,{"$f":"ACOS(((SIN('Solar Altitude'!C38)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C38)*COS('Input Data'!$G$3)))","v":1.058266307319484},{"$f":"ACOS(((SIN('Solar Altitude'!D38)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D38)*COS('Input Data'!$G$3)))","v":1.2078474684986444},{"$f":"ACOS(((SIN('Solar Altitude'!E38)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E38)*COS('Input Data'!$G$3)))","v":1.3667740660753709},{"$f":"ACOS(((SIN('Solar Altitude'!F38)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F38)*COS('Input Data'!$G$3)))","v":1.5618274683649662},{"$f":"ACOS(((SIN('Solar Altitude'!G38)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G38)*COS('Input Data'!$G$3)))","v":1.7220073659413311},{"$f":"ACOS(((SIN('Solar Altitude'!H38)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H38)*COS('Input Data'!$G$3)))","v":1.7919623715483843},{"$f":"ACOS(((SIN('Solar Altitude'!I38)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I38)*COS('Input Data'!$G$3)))","v":1.7394272024332567},{"$f":"ACOS(((SIN('Solar Altitude'!J38)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J38)*COS('Input Data'!$G$3)))","v":1.5719964659947774},{"$f":"ACOS(((SIN('Solar Altitude'!K38)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K38)*COS('Input Data'!$G$3)))","v":1.3332214398200457},{"$f":"ACOS(((SIN('Solar Altitude'!L38)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L38)*COS('Input Data'!$G$3)))","v":1.1360656162861644},{"$f":"ACOS(((SIN('Solar Altitude'!M38)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M38)*COS('Input Data'!$G$3)))","v":0.99854542046976347},{"$f":"ACOS(((SIN('Solar Altitude'!N38)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N38)*COS('Input Data'!$G$3)))","v":0.97573305779876307}]
[null,9,{"$f":"ACOS(((SIN('Solar Altitude'!C39)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C39)*COS('Input Data'!$G$3)))","v":0.90353510816893867},{"$f":"ACOS(((SIN('Solar Altitude'!D39)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D39)*COS('Input Data'!$G$3)))","v":1.0538243157320717},{"$f":"ACOS(((SIN('Solar Altitude'!E39)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E39)*COS('Input Data'!$G$3)))","v":1.2184903356318135},{"$f":"ACOS(((SIN('Solar Altitude'!F39)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F39)*COS('Input Data'!$G$3)))","v":1.4390385280672806},{"$f":"ACOS(((SIN('Solar Altitude'!G39)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G39)*COS('Input Data'!$G$3)))","v":1.6341114432554538},{"$f":"ACOS(((SIN('Solar Altitude'!H39)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H39)*COS('Input Data'!$G$3)))","v":1.7195190970203282},{"$f":"ACOS(((SIN('Solar Altitude'!I39)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I39)*COS('Input Data'!$G$3)))","v":1.6534441892541289},{"$f":"ACOS(((SIN('Solar Altitude'!J39)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J39)*COS('Input Data'!$G$3)))","v":1.4515571620245935},{"$f":"ACOS(((SIN('Solar Altitude'!K39)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K39)*COS('Input Data'!$G$3)))","v":1.173843215125367},{"$f":"ACOS(((SIN('Solar Altitude'!L39)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L39)*COS('Input Data'!$G$3)))","v":0.95928100368681524},{"$f":"ACOS(((SIN('Solar Altitude'!M39)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M39)*COS('Input Data'!$G$3)))","v":0.82587508984596658},{"$f":"ACOS(((SIN('Solar Altitude'!N39)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N39)*COS('Input Data'!$G$3)))","v":0.81498859821827208}]
[null,10,{"$f":"ACOS(((SIN('Solar Altitude'!C40)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C40)*COS('Input Data'!$G$3)))","v":0.70071538815813994},{"$f":"ACOS(((SIN('Solar Altitude'!D40)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D40)*COS('Input Data'!$G$3)))","v":0.84598427161152567},{"$f":"ACOS(((SIN('Solar Altitude'!E40)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E40)*COS('Input Data'!$G$3)))","v":1.010362948153158},{"$f":"ACOS(((SIN('Solar Altitude'!F40)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F40)*COS('Input Data'!$G$3)))","v":1.265322763274511},{"$f":"ACOS(((SIN('Solar Altitude'!G40)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G40)*COS('Input Data'!$G$3)))","v":1.5275294182792178},{"$f":"ACOS(((SIN('Solar Altitude'!H40)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H40)*COS('Input Data'!$G$3)))","v":1.6462941860249161},{"$f":"ACOS(((SIN('Solar Altitude'!I40)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I40)*COS('Input Data'!$G$3)))","v":1.5536089314055752},{"$f":"ACOS(((SIN('Solar Altitude'!J40)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J40)*COS('Input Data'!$G$3)))","v":1.2837299039160972},{"$f":"ACOS(((SIN('Solar Altitude'!K40)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K40)*COS('Input Data'!$G$3)))","v":0.94253927999738996},{"$f":"ACOS(((SIN('Solar Altitude'!L40)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L40)*COS('Input Data'!$G$3)))","v":0.71378409704331358},{"$f":"ACOS(((SIN('Solar Altitude'!M40)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M40)*COS('Input Data'!$G$3)))","v":0.59801659069868529},{"$f":"ACOS(((SIN('Solar Altitude'!N40)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N40)*COS('Input Data'!$G$3)))","v":0.60640960099999908}]
[null,11,{"$f":"ACOS(((SIN('Solar Altitude'!C41)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C41)*COS('Input Data'!$G$3)))","v":0.43432651592309734},{"$f":"ACOS(((SIN('Solar Altitude'!D41)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D41)*COS('Input Data'!$G$3)))","v":0.5521480379114827},{"$f":"ACOS(((SIN('Solar Altitude'!E41)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E41)*COS('Input Data'!$G$3)))","v":0.6796497824234552},{"$f":"ACOS(((SIN('Solar Altitude'!F41)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F41)*COS('Input Data'!$G$3)))","v":0.93619850107583946},{"$f":"ACOS(((SIN('Solar Altitude'!G41)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G41)*COS('Input Data'!$G$3)))","v":1.3362464729610233},{"$f":"ACOS(((SIN('Solar Altitude'!H41)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H41)*COS('Input Data'!$G$3)))","v":1.5530293407926004},{"$f":"ACOS(((SIN('Solar Altitude'!I41)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I41)*COS('Input Data'!$G$3)))","v":1.3915891659759199},{"$f":"ACOS(((SIN('Solar Altitude'!J41)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J41)*COS('Input Data'!$G$3)))","v":0.97166377450265484},{"$f":"ACOS(((SIN('Solar Altitude'!K41)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K41)*COS('Input Data'!$G$3)))","v":0.56727369074413647},{"$f":"ACOS(((SIN('Solar Altitude'!L41)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L41)*COS('Input Data'!$G$3)))","v":0.3689054188223968},{"$f":"ACOS(((SIN('Solar Altitude'!M41)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M41)*COS('Input Data'!$G$3)))","v":0.30384921089049199},{"$f":"ACOS(((SIN('Solar Altitude'!N41)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N41)*COS('Input Data'!$G$3)))","v":0.34094519238156962}]
[null,12,{"$f":"ACOS(((SIN('Solar Altitude'!C42)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C42)*COS('Input Data'!$G$3)))","v":0.10679406055891483},{"$f":"ACOS(((SIN('Solar Altitude'!D42)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D42)*COS('Input Data'!$G$3)))","v":0.15510241273331582},{"$f":"ACOS(((SIN('Solar Altitude'!E42)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E42)*COS('Input Data'!$G$3)))","v":0.15183013873624884},{"$f":"ACOS(((SIN('Solar Altitude'!F42)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F42)*COS('Input Data'!$G$3)))","v":0.11581121919831028},{"$f":"ACOS(((SIN('Solar Altitude'!G42)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G42)*COS('Input Data'!$G$3)))","v":0.20182683522870115},{"$f":"ACOS(((SIN('Solar Altitude'!H42)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H42)*COS('Input Data'!$G$3)))","v":1.0078905398359179},{"$f":"ACOS(((SIN('Solar Altitude'!I42)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I42)*COS('Input Data'!$G$3)))","v":0.64377126699533527},{"$f":"ACOS(((SIN('Solar Altitude'!J42)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J42)*COS('Input Data'!$G$3)))","v":0.18457402284613478},{"$f":"ACOS(((SIN('Solar Altitude'!K42)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K42)*COS('Input Data'!$G$3)))","v":3.8286785332140028E-3},{"$f":"ACOS(((SIN('Solar Altitude'!L42)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L42)*COS('Input Data'!$G$3)))","v":6.1123130165992468E-2},{"$f":"ACOS(((SIN('Solar Altitude'!M42)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M42)*COS('Input Data'!$G$3)))","v":3.8938326923418476E-2},{"$f":"ACOS(((SIN('Solar Altitude'!N42)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N42)*COS('Input Data'!$G$3)))","v":2.9728094192328136E-2}]
[null,13,{"$f":"-ACOS(((SIN('Solar Altitude'!C43)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C43)*COS('Input Data'!$G$3)))","v":-0.23968146775368493},{"$f":"-ACOS(((SIN('Solar Altitude'!D43)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D43)*COS('Input Data'!$G$3)))","v":-0.28299519000448226},{"$f":"-ACOS(((SIN('Solar Altitude'!E43)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E43)*COS('Input Data'!$G$3)))","v":-0.44751975973520852},{"$f":"-ACOS(((SIN('Solar Altitude'!F43)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F43)*COS('Input Data'!$G$3)))","v":-0.8264763886659191},{"$f":"-ACOS(((SIN('Solar Altitude'!G43)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G43)*COS('Input Data'!$G$3)))","v":-1.292529038821308},{"$f":"-ACOS(((SIN('Solar Altitude'!H43)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H43)*COS('Input Data'!$G$3)))","v":-1.5112011188630212},{"$f":"-ACOS(((SIN('Solar Altitude'!I43)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I43)*COS('Input Data'!$G$3)))","v":-1.2395029252776819},{"$f":"-ACOS(((SIN('Solar Altitude'!J43)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J43)*COS('Input Data'!$G$3)))","v":-0.79795425250097229},{"$f":"-ACOS(((SIN('Solar Altitude'!K43)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K43)*COS('Input Data'!$G$3)))","v":-0.57308952081364239},{"$f":"-ACOS(((SIN('Solar Altitude'!L43)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L43)*COS('Input Data'!$G$3)))","v":-0.47467850128393096},{"$f":"-ACOS(((SIN('Solar Altitude'!M43)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M43)*COS('Input Data'!$G$3)))","v":-0.37473351431083746},{"$f":"-ACOS(((SIN('Solar Altitude'!N43)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N43)*COS('Input Data'!$G$3)))","v":-0.28613070031543497}]
[null,14,{"$f":"-ACOS(((SIN('Solar Altitude'!C44)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C44)*COS('Input Data'!$G$3)))","v":-0.54604241308539381},{"$f":"-ACOS(((SIN('Solar Altitude'!D44)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D44)*COS('Input Data'!$G$3)))","v":-0.65088921640310549},{"$f":"-ACOS(((SIN('Solar Altitude'!E44)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E44)*COS('Input Data'!$G$3)))","v":-0.86982854921283437},{"$f":"-ACOS(((SIN('Solar Altitude'!F44)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F44)*COS('Input Data'!$G$3)))","v":-1.217701121819637},{"$f":"-ACOS(((SIN('Solar Altitude'!G44)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G44)*COS('Input Data'!$G$3)))","v":-1.5105946811705735},{"$f":"-ACOS(((SIN('Solar Altitude'!H44)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H44)*COS('Input Data'!$G$3)))","v":-1.6235440274410409},{"$f":"-ACOS(((SIN('Solar Altitude'!I44)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I44)*COS('Input Data'!$G$3)))","v":-1.4957538428507846},{"$f":"-ACOS(((SIN('Solar Altitude'!J44)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J44)*COS('Input Data'!$G$3)))","v":-1.2088916874812448},{"$f":"-ACOS(((SIN('Solar Altitude'!K44)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K44)*COS('Input Data'!$G$3)))","v":-0.94604905161134778},{"$f":"-ACOS(((SIN('Solar Altitude'!L44)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L44)*COS('Input Data'!$G$3)))","v":-0.79025082463613672},{"$f":"-ACOS(((SIN('Solar Altitude'!M44)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M44)*COS('Input Data'!$G$3)))","v":-0.65424004734985619},{"$f":"-ACOS(((SIN('Solar Altitude'!N44)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N44)*COS('Input Data'!$G$3)))","v":-0.56178566715823375}]
[null,15,{"$f":"-ACOS(((SIN('Solar Altitude'!C45)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C45)*COS('Input Data'!$G$3)))","v":-0.78641952951130711},{"$f":"-ACOS(((SIN('Solar Altitude'!D45)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D45)*COS('Input Data'!$G$3)))","v":-0.91554787662496373},{"$f":"-ACOS(((SIN('Solar Altitude'!E45)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E45)*COS('Input Data'!$G$3)))","v":-1.1273879110446283},{"$f":"-ACOS(((SIN('Solar Altitude'!F45)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F45)*COS('Input Data'!$G$3)))","v":-1.4099044174661883},{"$f":"-ACOS(((SIN('Solar Altitude'!G45)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G45)*COS('Input Data'!$G$3)))","v":-1.622090612366363},{"$f":"-ACOS(((SIN('Solar Altitude'!H45)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H45)*COS('Input Data'!$G$3)))","v":-1.6991734885102665},{"$f":"-ACOS(((SIN('Solar Altitude'!I45)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I45)*COS('Input Data'!$G$3)))","v":-1.6121690334476861},{"$f":"-ACOS(((SIN('Solar Altitude'!J45)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J45)*COS('Input Data'!$G$3)))","v":-1.4058016616461957},{"$f":"-ACOS(((SIN('Solar Altitude'!K45)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K45)*COS('Input Data'!$G$3)))","v":-1.1761198475600503},{"$f":"-ACOS(((SIN('Solar Altitude'!L45)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L45)*COS('Input Data'!$G$3)))","v":-1.0134733325329046},{"$f":"-ACOS(((SIN('Solar Altitude'!M45)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M45)*COS('Input Data'!$G$3)))","v":-0.86840869704656609},{"$f":"-ACOS(((SIN('Solar Altitude'!N45)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N45)*COS('Input Data'!$G$3)))","v":-0.78050668103524146}]
[null,16,{"$f":"-ACOS(((SIN('Solar Altitude'!C46)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C46)*COS('Input Data'!$G$3)))","v":-0.96847704675721313},{"$f":"-ACOS(((SIN('Solar Altitude'!D46)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D46)*COS('Input Data'!$G$3)))","v":-1.1042495425891925},{"$f":"-ACOS(((SIN('Solar Altitude'!E46)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E46)*COS('Input Data'!$G$3)))","v":-1.299416826897076},{"$f":"-ACOS(((SIN('Solar Altitude'!F46)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F46)*COS('Input Data'!$G$3)))","v":-1.5392149996507298},{"$f":"-ACOS(((SIN('Solar Altitude'!G46)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G46)*COS('Input Data'!$G$3)))","v":-1.7110982563870039},{"$f":"-ACOS(((SIN('Solar Altitude'!H46)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H46)*COS('Input Data'!$G$3)))","v":-1.77099022789173},{"$f":"-ACOS(((SIN('Solar Altitude'!I46)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I46)*COS('Input Data'!$G$3)))","v":-1.7017684026537228},{"$f":"-ACOS(((SIN('Solar Altitude'!J46)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J46)*COS('Input Data'!$G$3)))","v":-1.5364285539006752},{"$f":"-ACOS(((SIN('Solar Altitude'!K46)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K46)*COS('Input Data'!$G$3)))","v":-1.3349061556761301},{"$f":"-ACOS(((SIN('Solar Altitude'!L46)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L46)*COS('Input Data'!$G$3)))","v":-1.1766906409110542},{"$f":"-ACOS(((SIN('Solar Altitude'!M46)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M46)*COS('Input Data'!$G$3)))","v":-1.0311504022490317},{"$f":"-ACOS(((SIN('Solar Altitude'!N46)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N46)*COS('Input Data'!$G$3)))","v":-0.94906703556002914}]
[null,17,{"$f":"-ACOS(((SIN('Solar Altitude'!C47)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C47)*COS('Input Data'!$G$3)))","v":-1.108969585624606},{"$f":"-ACOS(((SIN('Solar Altitude'!D47)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D47)*COS('Input Data'!$G$3)))","v":-1.2471312233258249},{"$f":"-ACOS(((SIN('Solar Altitude'!E47)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E47)*COS('Input Data'!$G$3)))","v":-1.4306201378642391},{"$f":"-ACOS(((SIN('Solar Altitude'!F47)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F47)*COS('Input Data'!$G$3)))","v":-1.6464914370701367},{"$f":"-ACOS(((SIN('Solar Altitude'!G47)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G47)*COS('Input Data'!$G$3)))","v":-1.7969076941080173},{"$f":"-ACOS(((SIN('Solar Altitude'!H47)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H47)*COS('Input Data'!$G$3)))","v":-1.8471128597298661},{"$f":"-ACOS(((SIN('Solar Altitude'!I47)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I47)*COS('Input Data'!$G$3)))","v":-1.7867496904971587},{"$f":"-ACOS(((SIN('Solar Altitude'!J47)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J47)*COS('Input Data'!$G$3)))","v":-1.6439360608939895},{"$f":"-ACOS(((SIN('Solar Altitude'!K47)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K47)*COS('Input Data'!$G$3)))","v":-1.4600010106459727},{"$f":"-ACOS(((SIN('Solar Altitude'!L47)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L47)*COS('Input Data'!$G$3)))","v":-1.3051348145742139},{"$f":"-ACOS(((SIN('Solar Altitude'!M47)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M47)*COS('Input Data'!$G$3)))","v":-1.1587870476195314},{"$f":"-ACOS(((SIN('Solar Altitude'!N47)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N47)*COS('Input Data'!$G$3)))","v":-1.0806159257117494}]
[null,18,{"$f":"-ACOS(((SIN('Solar Altitude'!C48)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C48)*COS('Input Data'!$G$3)))","v":-1.2222085856509726},{"$f":"-ACOS(((SIN('Solar Altitude'!D48)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D48)*COS('Input Data'!$G$3)))","v":-1.3645713182252377},{"$f":"-ACOS(((SIN('Solar Altitude'!E48)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E48)*COS('Input Data'!$G$3)))","v":-1.5440855674973599},{"$f":"-ACOS(((SIN('Solar Altitude'!F48)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F48)*COS('Input Data'!$G$3)))","v":-1.749389034914969},{"$f":"-ACOS(((SIN('Solar Altitude'!G48)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G48)*COS('Input Data'!$G$3)))","v":-1.8887541313657259},{"$f":"-ACOS(((SIN('Solar Altitude'!H48)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H48)*COS('Input Data'!$G$3)))","v":-1.9328905239595118},{"$f":"-ACOS(((SIN('Solar Altitude'!I48)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I48)*COS('Input Data'!$G$3)))","v":-1.8767892988894657},{"$f":"-ACOS(((SIN('Solar Altitude'!J48)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J48)*COS('Input Data'!$G$3)))","v":-1.7465091799795569},{"$f":"-ACOS(((SIN('Solar Altitude'!K48)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K48)*COS('Input Data'!$G$3)))","v":-1.5714648665907731},{"$f":"-ACOS(((SIN('Solar Altitude'!L48)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L48)*COS('Input Data'!$G$3)))","v":-1.4153631972418801},{"$f":"-ACOS(((SIN('Solar Altitude'!M48)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M48)*COS('Input Data'!$G$3)))","v":-1.2639480583914511},{"$f":"-ACOS(((SIN('Solar Altitude'!N48)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N48)*COS('Input Data'!$G$3)))","v":-1.1865937532998967}]
[null,19,{"$f":"-ACOS(((SIN('Solar Altitude'!C49)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C49)*COS('Input Data'!$G$3)))","v":-1.3187078032953656},{"$f":"-ACOS(((SIN('Solar Altitude'!D49)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D49)*COS('Input Data'!$G$3)))","v":-1.4703653196278037},{"$f":"-ACOS(((SIN('Solar Altitude'!E49)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E49)*COS('Input Data'!$G$3)))","v":-1.654415031969813},{"$f":"-ACOS(((SIN('Solar Altitude'!F49)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F49)*COS('Input Data'!$G$3)))","v":-1.8596297117474063},{"$f":"-ACOS(((SIN('Solar Altitude'!G49)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G49)*COS('Input Data'!$G$3)))","v":-1.994421143988709},{"$f":"-ACOS(((SIN('Solar Altitude'!H49)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H49)*COS('Input Data'!$G$3)))","v":-2.0341933509673633},{"$f":"-ACOS(((SIN('Solar Altitude'!I49)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I49)*COS('Input Data'!$G$3)))","v":-1.9795291293353241},{"$f":"-ACOS(((SIN('Solar Altitude'!J49)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J49)*COS('Input Data'!$G$3)))","v":-1.8559280464656736},{"$f":"-ACOS(((SIN('Solar Altitude'!K49)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K49)*COS('Input Data'!$G$3)))","v":-1.6830069771428766},{"$f":"-ACOS(((SIN('Solar Altitude'!L49)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L49)*COS('Input Data'!$G$3)))","v":-1.5195557995749016},{"$f":"-ACOS(((SIN('Solar Altitude'!M49)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M49)*COS('Input Data'!$G$3)))","v":-1.3559671281170804},{"$f":"-ACOS(((SIN('Solar Altitude'!N49)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N49)*COS('Input Data'!$G$3)))","v":-1.2754321776962332}]
[null,20,{"$f":"-ACOS(((SIN('Solar Altitude'!C50)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C50)*COS('Input Data'!$G$3)))","v":-1.4067330288177597},{"$f":"-ACOS(((SIN('Solar Altitude'!D50)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D50)*COS('Input Data'!$G$3)))","v":-1.5761543665123987},{"$f":"-ACOS(((SIN('Solar Altitude'!E50)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E50)*COS('Input Data'!$G$3)))","v":-1.7748185875144225},{"$f":"-ACOS(((SIN('Solar Altitude'!F50)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F50)*COS('Input Data'!$G$3)))","v":-1.9891840653113326},{"$f":"-ACOS(((SIN('Solar Altitude'!G50)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G50)*COS('Input Data'!$G$3)))","v":-2.1232048288036793},{"$f":"-ACOS(((SIN('Solar Altitude'!H50)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H50)*COS('Input Data'!$G$3)))","v":-2.1588360080371167},{"$f":"-ACOS(((SIN('Solar Altitude'!I50)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I50)*COS('Input Data'!$G$3)))","v":-2.1038075523509665},{"$f":"-ACOS(((SIN('Solar Altitude'!J50)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J50)*COS('Input Data'!$G$3)))","v":-1.9839795330718792},{"$f":"-ACOS(((SIN('Solar Altitude'!K50)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K50)*COS('Input Data'!$G$3)))","v":-1.8083712137697474},{"$f":"-ACOS(((SIN('Solar Altitude'!L50)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L50)*COS('Input Data'!$G$3)))","v":-1.6299457503511532},{"$f":"-ACOS(((SIN('Solar Altitude'!M50)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M50)*COS('Input Data'!$G$3)))","v":-1.4428389653708038},{"$f":"-ACOS(((SIN('Solar Altitude'!N50)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N50)*COS('Input Data'!$G$3)))","v":-1.3533483170249039}]
[null,21,{"$f":"-ACOS(((SIN('Solar Altitude'!C51)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C51)*COS('Input Data'!$G$3)))","v":-1.494821656169609},{"$f":"-ACOS(((SIN('Solar Altitude'!D51)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D51)*COS('Input Data'!$G$3)))","v":-1.6964498329276898},{"$f":"-ACOS(((SIN('Solar Altitude'!E51)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E51)*COS('Input Data'!$G$3)))","v":-1.9231023179579798},{"$f":"-ACOS(((SIN('Solar Altitude'!F51)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F51)*COS('Input Data'!$G$3)))","v":-2.1543960594363361},{"$f":"-ACOS(((SIN('Solar Altitude'!G51)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G51)*COS('Input Data'!$G$3)))","v":-2.2877169092081382},{"$f":"-ACOS(((SIN('Solar Altitude'!H51)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H51)*COS('Input Data'!$G$3)))","v":-2.317541699079706},{"$f":"-ACOS(((SIN('Solar Altitude'!I51)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I51)*COS('Input Data'!$G$3)))","v":-2.2615338671102263},{"$f":"-ACOS(((SIN('Solar Altitude'!J51)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J51)*COS('Input Data'!$G$3)))","v":-2.146565487996356},{"$f":"-ACOS(((SIN('Solar Altitude'!K51)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K51)*COS('Input Data'!$G$3)))","v":-1.9677494384644261},{"$f":"-ACOS(((SIN('Solar Altitude'!L51)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L51)*COS('Input Data'!$G$3)))","v":-1.7654323405279797},{"$f":"-ACOS(((SIN('Solar Altitude'!M51)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M51)*COS('Input Data'!$G$3)))","v":-1.5344841674730674},{"$f":"-ACOS(((SIN('Solar Altitude'!N51)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N51)*COS('Input Data'!$G$3)))","v":-1.4256432991443408}]
[null,22,{"$f":"-ACOS(((SIN('Solar Altitude'!C52)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C52)*COS('Input Data'!$G$3)))","v":-1.5974903203537003},{"$f":"-ACOS(((SIN('Solar Altitude'!D52)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D52)*COS('Input Data'!$G$3)))","v":-1.8590885293883888},{"$f":"-ACOS(((SIN('Solar Altitude'!E52)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E52)*COS('Input Data'!$G$3)))","v":-2.1312297054366356},{"$f":"-ACOS(((SIN('Solar Altitude'!F52)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F52)*COS('Input Data'!$G$3)))","v":-2.3796301974206813},{"$f":"-ACOS(((SIN('Solar Altitude'!G52)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G52)*COS('Input Data'!$G$3)))","v":-2.5040067250181761},{"$f":"-ACOS(((SIN('Solar Altitude'!H52)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H52)*COS('Input Data'!$G$3)))","v":-2.5234302277324061},{"$f":"-ACOS(((SIN('Solar Altitude'!I52)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I52)*COS('Input Data'!$G$3)))","v":-2.4682086057582242},{"$f":"-ACOS(((SIN('Solar Altitude'!J52)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J52)*COS('Input Data'!$G$3)))","v":-2.3673348406550949},{"$f":"-ACOS(((SIN('Solar Altitude'!K52)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K52)*COS('Input Data'!$G$3)))","v":-2.1990533735924034},{"$f":"-ACOS(((SIN('Solar Altitude'!L52)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L52)*COS('Input Data'!$G$3)))","v":-1.969824210801528},{"$f":"-ACOS(((SIN('Solar Altitude'!M52)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M52)*COS('Input Data'!$G$3)))","v":-1.6526437912808873},{"$f":"-ACOS(((SIN('Solar Altitude'!N52)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N52)*COS('Input Data'!$G$3)))","v":-1.4991890815643381}]
[null,23,{"$f":"-ACOS(((SIN('Solar Altitude'!C53)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C53)*COS('Input Data'!$G$3)))","v":-1.7618286873245246},{"$f":"-ACOS(((SIN('Solar Altitude'!D53)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D53)*COS('Input Data'!$G$3)))","v":-2.1409149132073719},{"$f":"-ACOS(((SIN('Solar Altitude'!E53)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E53)*COS('Input Data'!$G$3)))","v":-2.4619428711663378},{"$f":"-ACOS(((SIN('Solar Altitude'!F53)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F53)*COS('Input Data'!$G$3)))","v":-2.6941421748482881},{"$f":"-ACOS(((SIN('Solar Altitude'!G53)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G53)*COS('Input Data'!$G$3)))","v":-2.7849009327751642},{"$f":"-ACOS(((SIN('Solar Altitude'!H53)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H53)*COS('Input Data'!$G$3)))","v":-2.7860666740770155},{"$f":"-ACOS(((SIN('Solar Altitude'!I53)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I53)*COS('Input Data'!$G$3)))","v":-2.7378799974418255},{"$f":"-ACOS(((SIN('Solar Altitude'!J53)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J53)*COS('Input Data'!$G$3)))","v":-2.6752683673459607},{"$f":"-ACOS(((SIN('Solar Altitude'!K53)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K53)*COS('Input Data'!$G$3)))","v":-2.5743189628456582},{"$f":"-ACOS(((SIN('Solar Altitude'!L53)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L53)*COS('Input Data'!$G$3)))","v":-2.3818401590527567},{"$f":"-ACOS(((SIN('Solar Altitude'!M53)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M53)*COS('Input Data'!$G$3)))","v":-1.8958841107945947},{"$f":"-ACOS(((SIN('Solar Altitude'!N53)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N53)*COS('Input Data'!$G$3)))","v":-1.5949415584609572}]
[null,24,{"$f":"-ACOS(((SIN('Solar Altitude'!C54)*SIN('Input Data'!$G$3))-SIN('eq of time'!C$5))/(COS('Solar Altitude'!C54)*COS('Input Data'!$G$3)))","v":-2.4023913757399749},{"$f":"-ACOS(((SIN('Solar Altitude'!D54)*SIN('Input Data'!$G$3))-SIN('eq of time'!D$5))/(COS('Solar Altitude'!D54)*COS('Input Data'!$G$3)))","v":-2.785088806158984},{"$f":"-ACOS(((SIN('Solar Altitude'!E54)*SIN('Input Data'!$G$3))-SIN('eq of time'!E$5))/(COS('Solar Altitude'!E54)*COS('Input Data'!$G$3)))","v":-2.9897625148535445},{"$f":"-ACOS(((SIN('Solar Altitude'!F54)*SIN('Input Data'!$G$3))-SIN('eq of time'!F$5))/(COS('Solar Altitude'!F54)*COS('Input Data'!$G$3)))","v":-3.0984096944746584},{"$f":"-ACOS(((SIN('Solar Altitude'!G54)*SIN('Input Data'!$G$3))-SIN('eq of time'!G$5))/(COS('Solar Altitude'!G54)*COS('Input Data'!$G$3)))","v":-3.1194105589691135},{"$f":"-ACOS(((SIN('Solar Altitude'!H54)*SIN('Input Data'!$G$3))-SIN('eq of time'!H$5))/(COS('Solar Altitude'!H54)*COS('Input Data'!$G$3)))","v":-3.0957621818630736},{"$f":"-ACOS(((SIN('Solar Altitude'!I54)*SIN('Input Data'!$G$3))-SIN('eq of time'!I$5))/(COS('Solar Altitude'!I54)*COS('Input Data'!$G$3)))","v":-3.0649172176886541},{"$f":"-ACOS(((SIN('Solar Altitude'!J54)*SIN('Input Data'!$G$3))-SIN('eq of time'!J$5))/(COS('Solar Altitude'!J54)*COS('Input Data'!$G$3)))","v":-3.0737777094114138},{"$f":"-ACOS(((SIN('Solar Altitude'!K54)*SIN('Input Data'!$G$3))-SIN('eq of time'!K$5))/(COS('Solar Altitude'!K54)*COS('Input Data'!$G$3)))","v":-3.1377639750566084},{"$f":"-ACOS(((SIN('Solar Altitude'!L54)*SIN('Input Data'!$G$3))-SIN('eq of time'!L$5))/(COS('Solar Altitude'!L54)*COS('Input Data'!$G$3)))","v":-2.9959943010857266},{"$f":"-ACOS(((SIN('Solar Altitude'!M54)*SIN('Input Data'!$G$3))-SIN('eq of time'!M$5))/(COS('Solar Altitude'!M54)*COS('Input Data'!$G$3)))","v":-2.8251233159428448},{"$f":"-ACOS(((SIN('Solar Altitude'!N54)*SIN('Input Data'!$G$3))-SIN('eq of time'!N$5))/(COS('Solar Altitude'!N54)*COS('Input Data'!$G$3)))","v":-2.3460621260835679}]

{"sheet":"AST","index":18,"n_rows":25,"n_cols":13,"rows_kept":25,"cut":false,"hidden":true,"merged":[]}
[null,"Jan","Feb","Mar","Apr","May","Jun","Jul","Aug","Sep","Oct","Nov","Dec"]
[1,{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":0.69444444444444453},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":0.6494444444444446},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":0.75611111111111129},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":0.8994444444444446},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":0.93611111111111123},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":0.85777777777777797},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":0.7777777777777779},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":0.84111111111111125},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":1.0061111111111112},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":1.137777777777778},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":1.1111111111111112},{"$f":"(60*$A2+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":0.90777777777777791}]
[2,{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":1.6944444444444444},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":1.6494444444444445},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":1.7561111111111112},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":1.8994444444444445},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":1.9361111111111111},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":1.8577777777777778},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":1.7777777777777779},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":1.8411111111111111},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":2.0061111111111112},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":2.137777777777778},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":2.1111111111111112},{"$f":"(60*$A3+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":1.9077777777777778}]
[3,{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":2.6944444444444446},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":2.6494444444444443},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":2.7561111111111112},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":2.8994444444444443},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":2.9361111111111113},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":2.8577777777777778},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":2.7777777777777781},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":2.8411111111111111},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":3.0061111111111112},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":3.137777777777778},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":3.1111111111111116},{"$f":"(60*$A4+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":2.907777777777778}]
[4,{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":3.6944444444444446},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":3.6494444444444443},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":3.7561111111111112},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":3.8994444444444443},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":3.9361111111111113},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":3.8577777777777778},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":3.7777777777777781},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":3.8411111111111111},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":4.0061111111111112},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":4.137777777777778},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":4.1111111111111116},{"$f":"(60*$A5+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":3.907777777777778}]
[5,{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":4.6944444444444446},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":4.6494444444444447},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":4.7561111111111112},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":4.8994444444444447},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":4.9361111111111118},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":4.8577777777777786},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":4.7777777777777777},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":4.841111111111112},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":5.0061111111111112},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":5.1377777777777771},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":5.1111111111111116},{"$f":"(60*$A6+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":4.9077777777777785}]
[6,{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":5.6944444444444446},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":5.6494444444444447},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":5.7561111111111112},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":5.8994444444444447},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":5.9361111111111118},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":5.8577777777777786},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":5.7777777777777777},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":5.841111111111112},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":6.0061111111111112},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":6.1377777777777771},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":6.1111111111111116},{"$f":"(60*$A7+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":5.9077777777777785}]
[7,{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":6.6944444444444446},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":6.6494444444444447},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":6.7561111111111112},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":6.8994444444444447},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":6.9361111111111118},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":6.8577777777777786},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":6.7777777777777777},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":6.841111111111112},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":7.0061111111111112},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":7.1377777777777771},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":7.1111111111111116},{"$f":"(60*$A8+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":6.9077777777777785}]
[8,{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":7.6944444444444446},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":7.6494444444444447},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":7.7561111111111112},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":7.8994444444444447},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":7.9361111111111118},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":7.8577777777777786},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":7.7777777777777777},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":7.841111111111112},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":8.0061111111111121},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":8.137777777777778},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":8.1111111111111107},{"$f":"(60*$A9+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":7.9077777777777785}]
[9,{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":8.6944444444444446},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":8.6494444444444447},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":8.7561111111111121},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":8.8994444444444447},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":8.93611111111111},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":8.8577777777777786},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":8.7777777777777768},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":8.8411111111111111},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":9.0061111111111121},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":9.137777777777778},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":9.1111111111111107},{"$f":"(60*$A10+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":8.9077777777777776}]
[10,{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":9.6944444444444446},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":9.6494444444444447},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":9.7561111111111121},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":9.8994444444444447},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":9.93611111111111},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":9.8577777777777786},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":9.7777777777777768},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":9.8411111111111111},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":10.006111111111112},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":10.137777777777778},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":10.111111111111111},{"$f":"(60*$A11+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":9.9077777777777776}]
[11,{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":10.694444444444445},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":10.649444444444445},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":10.756111111111112},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":10.899444444444445},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":10.93611111111111},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":10.857777777777779},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":10.777777777777777},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":10.841111111111111},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":11.006111111111112},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":11.137777777777778},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":11.111111111111111},{"$f":"(60*$A12+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":10.907777777777778}]
[12,{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":11.694444444444445},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":11.649444444444445},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":11.756111111111112},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":11.899444444444445},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":11.93611111111111},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":11.857777777777779},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":11.777777777777777},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":11.841111111111111},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":12.006111111111112},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":12.137777777777778},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":12.111111111111111},{"$f":"(60*$A13+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":11.907777777777778}]
[13,{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":12.694444444444445},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":12.649444444444445},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":12.756111111111112},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":12.899444444444445},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":12.93611111111111},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":12.857777777777779},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":12.777777777777777},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":12.841111111111111},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":13.006111111111112},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":13.137777777777778},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":13.111111111111111},{"$f":"(60*$A14+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":12.907777777777778}]
[14,{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":13.694444444444445},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":13.649444444444445},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":13.756111111111112},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":13.899444444444445},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":13.93611111111111},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":13.857777777777779},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":13.777777777777777},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":13.841111111111111},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":14.006111111111112},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":14.137777777777778},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":14.111111111111111},{"$f":"(60*$A15+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":13.907777777777778}]
[15,{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":14.694444444444445},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":14.649444444444445},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":14.756111111111112},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":14.899444444444445},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":14.93611111111111},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":14.857777777777779},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":14.777777777777777},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":14.841111111111111},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":15.006111111111112},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":15.137777777777778},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":15.111111111111111},{"$f":"(60*$A16+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":14.907777777777778}]
[16,{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":15.694444444444445},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":15.649444444444445},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":15.756111111111112},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":15.899444444444445},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":15.93611111111111},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":15.857777777777779},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":15.777777777777777},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":15.841111111111111},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":16.00611111111111},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":16.137777777777778},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":16.111111111111111},{"$f":"(60*$A17+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":15.907777777777778}]
[17,{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":16.694444444444443},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":16.649444444444445},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":16.75611111111111},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":16.899444444444445},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":16.93611111111111},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":16.857777777777777},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":16.777777777777779},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":16.841111111111111},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":17.00611111111111},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":17.137777777777778},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":17.111111111111111},{"$f":"(60*$A18+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":16.907777777777778}]
[18,{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":17.694444444444446},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":17.649444444444445},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":17.756111111111114},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":17.899444444444445},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":17.936111111111114},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":17.857777777777777},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":17.777777777777779},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":17.841111111111111},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":18.006111111111114},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":18.137777777777782},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":18.111111111111111},{"$f":"(60*$A19+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":17.907777777777778}]
[19,{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":18.694444444444446},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":18.649444444444445},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":18.756111111111114},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":18.899444444444445},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":18.936111111111114},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":18.857777777777777},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":18.777777777777779},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":18.841111111111111},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":19.006111111111114},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":19.137777777777782},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":19.111111111111111},{"$f":"(60*$A20+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":18.907777777777778}]
[20,{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":19.694444444444446},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":19.649444444444445},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":19.756111111111114},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":19.899444444444445},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":19.936111111111114},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":19.857777777777777},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":19.777777777777779},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":19.841111111111111},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":20.006111111111114},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":20.137777777777782},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":20.111111111111111},{"$f":"(60*$A21+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":19.907777777777778}]
[21,{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":20.694444444444446},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":20.649444444444445},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":20.756111111111114},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":20.899444444444445},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":20.936111111111114},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":20.857777777777777},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":20.777777777777779},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":20.841111111111111},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":21.006111111111114},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":21.137777777777782},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":21.111111111111111},{"$f":"(60*$A22+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":20.907777777777778}]
[22,{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":21.694444444444446},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":21.649444444444445},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":21.756111111111114},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":21.899444444444445},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":21.936111111111114},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":21.857777777777777},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":21.777777777777779},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":21.841111111111111},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":22.006111111111114},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":22.137777777777782},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":22.111111111111111},{"$f":"(60*$A23+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":21.907777777777778}]
[23,{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":22.694444444444446},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":22.649444444444445},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":22.756111111111114},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":22.899444444444445},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":22.936111111111114},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":22.857777777777777},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":22.777777777777779},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":22.841111111111111},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":23.006111111111114},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":23.137777777777782},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":23.111111111111111},{"$f":"(60*$A24+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":22.907777777777778}]
[24,{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!C$3)/60","v":23.694444444444446},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!D$3)/60","v":23.649444444444445},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!E$3)/60","v":23.756111111111114},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!F$3)/60","v":23.899444444444445},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!G$3)/60","v":23.936111111111114},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!H$3)/60","v":23.857777777777777},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!I$3)/60","v":23.777777777777779},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!J$3)/60","v":23.841111111111111},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!K$3)/60","v":24.006111111111114},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!L$3)/60","v":24.137777777777782},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!M$3)/60","v":24.111111111111111},{"$f":"(60*$A25+4*('Operative BP'!$P$20-'Input Data'!$F$5)+'eq of time'!N$3)/60","v":23.907777777777778}]

{"sheet":"Stack Ventilation","index":19,"n_rows":33,"n_cols":35,"rows_kept":33,"cut":false,"hidden":true,"merged":[[0,22,0,34],[0,8,0,20]]}
[null,null,null,null,null,null,null,null,"South Stack CFM",null,null,null,null,null,null,null,null,null,null,null,null,null,"South Delta T"]
[null,null,null,null,null,null,null,null,{"$f":"'Operative BP'!AP31","v":0},{"$f":"'Operative BP'!AQ31","v":"Jan"},{"$f":"'Operative BP'!AR31","v":"Feb"},{"$f":"'Operative BP'!AS31","v":"Mar"},{"$f":"'Operative BP'!AT31","v":"Apr"},{"$f":"'Operative BP'!AU31","v":"May"},{"$f":"'Operative BP'!AV31","v":"Jun"},{"$f":"'Operative BP'!AW31","v":"Jul"},{"$f":"'Operative BP'!AX31","v":"Aug"},{"$f":"'Operative BP'!AY31","v":"Sep"},{"$f":"'Operative BP'!AZ31","v":"Oct"},{"$f":"'Operative BP'!BA31","v":"Nov"},{"$f":"'Operative BP'!BB31","v":"Dec"},null,{"$f":"'Operative BP'!AP4","v":0},{"$f":"'Operative BP'!AQ4","v":"Jan"},{"$f":"'Operative BP'!AR4","v":"Feb"},{"$f":"'Operative BP'!AS4","v":"Mar"},{"$f":"'Operative BP'!AT4","v":"Apr"},{"$f":"'Operative BP'!AU4","v":"May"},{"$f":"'Operative BP'!AV4","v":"Jun"},{"$f":"'Operative BP'!AW4","v":"Jul"},{"$f":"'Operative BP'!AX4","v":"Aug"},{"$f":"'Operative BP'!AY4","v":"Sep"},{"$f":"'Operative BP'!AZ4","v":"Oct"},{"$f":"'Operative BP'!BA4","v":"Nov"},{"$f":"'Operative BP'!BB4","v":"Dec"}]
["Q",{"$f":"60*B4*B9*SQRT(2*B13*(B11-B12)*((D18-D19)/D19))","v":10309.063766450579},"cfm",null,null,null,null,null,{"$f":"'Operative BP'!AP32","v":1},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X3)/('Dry Bulb'!D5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y3)/('Dry Bulb'!E5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z3)/('Dry Bulb'!F5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA3)/('Dry Bulb'!G5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB3)/('Dry Bulb'!H5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC3)/('Dry Bulb'!I5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD3)/('Dry Bulb'!J5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE3)/('Dry Bulb'!K5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF3)/('Dry Bulb'!L5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG3)/('Dry Bulb'!M5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH3)/('Dry Bulb'!N5+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI3)/('Dry Bulb'!O5+459.67)))","v":0},null,{"$f":"'Operative BP'!AP5","v":1},{"$f":"('Operative BP'!AQ5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA5*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB5*$B$10)/(0.018033*$B$8)","v":0}]
["Discharge coefficient",0.6,null,null,null,null,null,null,{"$f":"'Operative BP'!AP33","v":2},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X4)/('Dry Bulb'!D6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y4)/('Dry Bulb'!E6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z4)/('Dry Bulb'!F6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA4)/('Dry Bulb'!G6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB4)/('Dry Bulb'!H6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC4)/('Dry Bulb'!I6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD4)/('Dry Bulb'!J6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE4)/('Dry Bulb'!K6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF4)/('Dry Bulb'!L6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG4)/('Dry Bulb'!M6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH4)/('Dry Bulb'!N6+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI4)/('Dry Bulb'!O6+459.67)))","v":0},null,{"$f":"'Operative BP'!AP6","v":2},{"$f":"('Operative BP'!AQ6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA6*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB6*$B$10)/(0.018033*$B$8)","v":0}]
["Height of Stack",{"$f":"'Operative BP'!P9","v":15},"ft",null,null,null,null,null,{"$f":"'Operative BP'!AP34","v":3},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X5)/('Dry Bulb'!D7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y5)/('Dry Bulb'!E7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z5)/('Dry Bulb'!F7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA5)/('Dry Bulb'!G7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB5)/('Dry Bulb'!H7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC5)/('Dry Bulb'!I7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD5)/('Dry Bulb'!J7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE5)/('Dry Bulb'!K7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF5)/('Dry Bulb'!L7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG5)/('Dry Bulb'!M7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH5)/('Dry Bulb'!N7+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI5)/('Dry Bulb'!O7+459.67)))","v":0},null,{"$f":"'Operative BP'!AP7","v":3},{"$f":"('Operative BP'!AQ7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA7*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB7*$B$10)/(0.018033*$B$8)","v":0}]
["Width of Stack",{"$f":"'Operative BP'!P3","v":30},"ft",null,null,null,null,null,{"$f":"'Operative BP'!AP35","v":4},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X6)/('Dry Bulb'!D8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y6)/('Dry Bulb'!E8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z6)/('Dry Bulb'!F8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA6)/('Dry Bulb'!G8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB6)/('Dry Bulb'!H8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC6)/('Dry Bulb'!I8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD6)/('Dry Bulb'!J8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE6)/('Dry Bulb'!K8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF6)/('Dry Bulb'!L8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG6)/('Dry Bulb'!M8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH6)/('Dry Bulb'!N8+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI6)/('Dry Bulb'!O8+459.67)))","v":0},null,{"$f":"'Operative BP'!AP8","v":4},{"$f":"('Operative BP'!AQ8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA8*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB8*$B$10)/(0.018033*$B$8)","v":0}]
["Depth of Stack",2,"ft",null,null,null,null,null,{"$f":"'Operative BP'!AP36","v":5},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X7)/('Dry Bulb'!D9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y7)/('Dry Bulb'!E9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z7)/('Dry Bulb'!F9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA7)/('Dry Bulb'!G9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB7)/('Dry Bulb'!H9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC7)/('Dry Bulb'!I9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD7)/('Dry Bulb'!J9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE7)/('Dry Bulb'!K9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF7)/('Dry Bulb'!L9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG7)/('Dry Bulb'!M9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH7)/('Dry Bulb'!N9+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI7)/('Dry Bulb'!O9+459.67)))","v":0},null,{"$f":"'Operative BP'!AP9","v":5},{"$f":"('Operative BP'!AQ9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA9*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB9*$B$10)/(0.018033*$B$8)","v":0}]
["Volume of Stack",{"$f":"B7*B6*B5","v":900},"ft3",null,null,null,null,null,{"$f":"'Operative BP'!AP37","v":6},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X8)/('Dry Bulb'!D10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y8)/('Dry Bulb'!E10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z8)/('Dry Bulb'!F10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA8)/('Dry Bulb'!G10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB8)/('Dry Bulb'!H10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC8)/('Dry Bulb'!I10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD8)/('Dry Bulb'!J10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE8)/('Dry Bulb'!K10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF8)/('Dry Bulb'!L10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG8)/('Dry Bulb'!M10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH8)/('Dry Bulb'!N10+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI8)/('Dry Bulb'!O10+459.67)))","v":0},null,{"$f":"'Operative BP'!AP10","v":6},{"$f":"('Operative BP'!AQ10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA10*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB10*$B$10)/(0.018033*$B$8)","v":0}]
["Opening Area",{"$f":"B6*B7","v":60},"ft2",null,null,null,null,null,{"$f":"'Operative BP'!AP38","v":7},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X9)/('Dry Bulb'!D11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y9)/('Dry Bulb'!E11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z9)/('Dry Bulb'!F11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA9)/('Dry Bulb'!G11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB9)/('Dry Bulb'!H11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC9)/('Dry Bulb'!I11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD9)/('Dry Bulb'!J11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE9)/('Dry Bulb'!K11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF9)/('Dry Bulb'!L11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG9)/('Dry Bulb'!M11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH9)/('Dry Bulb'!N11+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI9)/('Dry Bulb'!O11+459.67)))","v":203.10395882426269},null,{"$f":"'Operative BP'!AP11","v":7},{"$f":"('Operative BP'!AQ11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA11*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB11*$B$10)/(0.018033*$B$8)","v":9.3603990100314064E-3}]
["Fraction of Solar Ht Retained in Cavity",0.1,null,null,null,null,null,null,{"$f":"'Operative BP'!AP39","v":8},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X10)/('Dry Bulb'!D12+459.67)))","v":1859.2268840763261},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y10)/('Dry Bulb'!E12+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z10)/('Dry Bulb'!F12+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA10)/('Dry Bulb'!G12+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB10)/('Dry Bulb'!H12+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC10)/('Dry Bulb'!I12+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD10)/('Dry Bulb'!J12+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE10)/('Dry Bulb'!K12+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF10)/('Dry Bulb'!L12+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG10)/('Dry Bulb'!M12+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH10)/('Dry Bulb'!N12+459.67)))","v":3107.3751957745558},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI10)/('Dry Bulb'!O12+459.67)))","v":2901.6051931256015},null,{"$f":"'Operative BP'!AP12","v":8},{"$f":"('Operative BP'!AQ12*$B$10)/(0.018033*$B$8)","v":0.78437251267855568},{"$f":"('Operative BP'!AR12*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS12*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT12*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU12*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV12*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW12*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX12*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY12*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ12*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA12*$B$10)/(0.018033*$B$8)","v":2.2442735913535929},{"$f":"('Operative BP'!BB12*$B$10)/(0.018033*$B$8)","v":1.9165010375730902}]
["Hn",{"$f":"B5/2","v":7.5},"ft",null,null,{"$f":"B11/3.28","v":2.2865853658536586},"m",null,{"$f":"'Operative BP'!AP40","v":9},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X11)/('Dry Bulb'!D13+459.67)))","v":4681.7663190477097},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y11)/('Dry Bulb'!E13+459.67)))","v":1783.0091954543932},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z11)/('Dry Bulb'!F13+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA11)/('Dry Bulb'!G13+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB11)/('Dry Bulb'!H13+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC11)/('Dry Bulb'!I13+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD11)/('Dry Bulb'!J13+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE11)/('Dry Bulb'!K13+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF11)/('Dry Bulb'!L13+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG11)/('Dry Bulb'!M13+459.67)))","v":2863.3557494516831},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH11)/('Dry Bulb'!N13+459.67)))","v":5572.2263513199696},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI11)/('Dry Bulb'!O13+459.67)))","v":5082.2681187700564},null,{"$f":"'Operative BP'!AP13","v":9},{"$f":"('Operative BP'!AQ13*$B$10)/(0.018033*$B$8)","v":4.9999542334008593},{"$f":"('Operative BP'!AR13*$B$10)/(0.018033*$B$8)","v":0.73078432626214584},{"$f":"('Operative BP'!AS13*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT13*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU13*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV13*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW13*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX13*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY13*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ13*$B$10)/(0.018033*$B$8)","v":1.9619980294098305},{"$f":"('Operative BP'!BA13*$B$10)/(0.018033*$B$8)","v":7.2838383607330872},{"$f":"('Operative BP'!BB13*$B$10)/(0.018033*$B$8)","v":5.9126343128483194}]
["Hb",0,"ft",null,null,{"$f":"B12/3.28","v":0},"m",null,{"$f":"'Operative BP'!AP41","v":10},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X12)/('Dry Bulb'!D14+459.67)))","v":6361.4614407623449},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y12)/('Dry Bulb'!E14+459.67)))","v":2896.4303368374344},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z12)/('Dry Bulb'!F14+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA12)/('Dry Bulb'!G14+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB12)/('Dry Bulb'!H14+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC12)/('Dry Bulb'!I14+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD12)/('Dry Bulb'!J14+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE12)/('Dry Bulb'!K14+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF12)/('Dry Bulb'!L14+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG12)/('Dry Bulb'!M14+459.67)))","v":3157.1863456334659},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH12)/('Dry Bulb'!N14+459.67)))","v":7169.7433355368103},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI12)/('Dry Bulb'!O14+459.67)))","v":6839.4020220988359},null,{"$f":"'Operative BP'!AP14","v":10},{"$f":"('Operative BP'!AQ14*$B$10)/(0.018033*$B$8)","v":9.2830077610870472},{"$f":"('Operative BP'!AR14*$B$10)/(0.018033*$B$8)","v":1.9398503567999561},{"$f":"('Operative BP'!AS14*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT14*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU14*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV14*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW14*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX14*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY14*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ14*$B$10)/(0.018033*$B$8)","v":2.4020630695039911},{"$f":"('Operative BP'!BA14*$B$10)/(0.018033*$B$8)","v":12.14937081480012},{"$f":"('Operative BP'!BB14*$B$10)/(0.018033*$B$8)","v":10.771416786905048}]
["Gravity",32.173999999999999,"ft/s2",null,null,null,null,null,{"$f":"'Operative BP'!AP42","v":11},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X13)/('Dry Bulb'!D15+459.67)))","v":7558.1599619716681},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y13)/('Dry Bulb'!E15+459.67)))","v":2552.9306020795179},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z13)/('Dry Bulb'!F15+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA13)/('Dry Bulb'!G15+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB13)/('Dry Bulb'!H15+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC13)/('Dry Bulb'!I15+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD13)/('Dry Bulb'!J15+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE13)/('Dry Bulb'!K15+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF13)/('Dry Bulb'!L15+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG13)/('Dry Bulb'!M15+459.67)))","v":2544.221722788835},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH13)/('Dry Bulb'!N15+459.67)))","v":8311.904765287587},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI13)/('Dry Bulb'!O15+459.67)))","v":8071.9991751621174},null,{"$f":"'Operative BP'!AP15","v":11},{"$f":"('Operative BP'!AQ15*$B$10)/(0.018033*$B$8)","v":13.168029788066141},{"$f":"('Operative BP'!AR15*$B$10)/(0.018033*$B$8)","v":1.5169228706333562},{"$f":"('Operative BP'!AS15*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT15*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU15*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV15*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW15*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX15*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY15*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ15*$B$10)/(0.018033*$B$8)","v":1.5686865450135938},{"$f":"('Operative BP'!BA15*$B$10)/(0.018033*$B$8)","v":16.439011161770583},{"$f":"('Operative BP'!BB15*$B$10)/(0.018033*$B$8)","v":15.092262441445127}]
["Atm",101325,"Pa",null,null,null,null,null,{"$f":"'Operative BP'!AP43","v":12},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X14)/('Dry Bulb'!D16+459.67)))","v":8413.0290767252955},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y14)/('Dry Bulb'!E16+459.67)))","v":1850.6274572021837},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z14)/('Dry Bulb'!F16+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA14)/('Dry Bulb'!G16+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB14)/('Dry Bulb'!H16+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC14)/('Dry Bulb'!I16+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD14)/('Dry Bulb'!J16+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE14)/('Dry Bulb'!K16+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF14)/('Dry Bulb'!L16+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG14)/('Dry Bulb'!M16+459.67)))","v":2246.1112128266668},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH14)/('Dry Bulb'!N16+459.67)))","v":9067.9154762710514},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI14)/('Dry Bulb'!O16+459.67)))","v":9006.5954387584279},null,{"$f":"'Operative BP'!AP16","v":12},{"$f":"('Operative BP'!AQ16*$B$10)/(0.018033*$B$8)","v":16.394452232862566},{"$f":"('Operative BP'!AR16*$B$10)/(0.018033*$B$8)","v":0.80095255566881896},{"$f":"('Operative BP'!AS16*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT16*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU16*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV16*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW16*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX16*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY16*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ16*$B$10)/(0.018033*$B$8)","v":1.2282585667529478},{"$f":"('Operative BP'!BA16*$B$10)/(0.018033*$B$8)","v":19.657460862971764},{"$f":"('Operative BP'!BB16*$B$10)/(0.018033*$B$8)","v":18.867239334511233}]
["Pressure at top",{"$f":"0.0342*B14*(F11-F12)*((1/F19)-(1/F18))","v":1.2136754421745746},"Pa",null,null,null,null,null,{"$f":"'Operative BP'!AP44","v":13},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X15)/('Dry Bulb'!D17+459.67)))","v":8220.7361681829188},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y15)/('Dry Bulb'!E17+459.67)))","v":2077.6434406445615},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z15)/('Dry Bulb'!F17+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA15)/('Dry Bulb'!G17+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB15)/('Dry Bulb'!H17+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC15)/('Dry Bulb'!I17+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD15)/('Dry Bulb'!J17+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE15)/('Dry Bulb'!K17+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF15)/('Dry Bulb'!L17+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG15)/('Dry Bulb'!M17+459.67)))","v":2821.3069806911772},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH15)/('Dry Bulb'!N17+459.67)))","v":8298.1568463837266},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI15)/('Dry Bulb'!O17+459.67)))","v":8604.312359798032},null,{"$f":"'Operative BP'!AP17","v":13},{"$f":"('Operative BP'!AQ17*$B$10)/(0.018033*$B$8)","v":15.713002342032564},{"$f":"('Operative BP'!AR17*$B$10)/(0.018033*$B$8)","v":1.0146865517023225},{"$f":"('Operative BP'!AS17*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT17*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU17*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV17*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW17*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX17*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY17*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ17*$B$10)/(0.018033*$B$8)","v":1.9442480013345056},{"$f":"('Operative BP'!BA17*$B$10)/(0.018033*$B$8)","v":16.527797415977492},{"$f":"('Operative BP'!BB17*$B$10)/(0.018033*$B$8)","v":17.290474552697379}]
[null,{"$f":"B15*0.004","v":4.8547017686982981E-3},"inches of water",null,null,null,null,null,{"$f":"'Operative BP'!AP45","v":14},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X16)/('Dry Bulb'!D18+459.67)))","v":7397.0329504570727},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y16)/('Dry Bulb'!E18+459.67)))","v":2917.4393441028442},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z16)/('Dry Bulb'!F18+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA16)/('Dry Bulb'!G18+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB16)/('Dry Bulb'!H18+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC16)/('Dry Bulb'!I18+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD16)/('Dry Bulb'!J18+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE16)/('Dry Bulb'!K18+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF16)/('Dry Bulb'!L18+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG16)/('Dry Bulb'!M18+459.67)))","v":3400.835400600276},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH16)/('Dry Bulb'!N18+459.67)))","v":7273.8444389124943},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI16)/('Dry Bulb'!O18+459.67)))","v":7710.2568284057379},null,{"$f":"'Operative BP'!AP18","v":14},{"$f":"('Operative BP'!AQ18*$B$10)/(0.018033*$B$8)","v":12.761292334720705},{"$f":"('Operative BP'!AR18*$B$10)/(0.018033*$B$8)","v":2.0082378345493224},{"$f":"('Operative BP'!AS18*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT18*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU18*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV18*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW18*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX18*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY18*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ18*$B$10)/(0.018033*$B$8)","v":2.8324209394902544},{"$f":"('Operative BP'!BA18*$B$10)/(0.018033*$B$8)","v":12.72044603768177},{"$f":"('Operative BP'!BB18*$B$10)/(0.018033*$B$8)","v":13.921943851007926}]
[null,null,null,null,null,null,null,null,{"$f":"'Operative BP'!AP46","v":15},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X17)/('Dry Bulb'!D19+459.67)))","v":6191.5144900709683},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y17)/('Dry Bulb'!E19+459.67)))","v":3081.9360800592876},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z17)/('Dry Bulb'!F19+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA17)/('Dry Bulb'!G19+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB17)/('Dry Bulb'!H19+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC17)/('Dry Bulb'!I19+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD17)/('Dry Bulb'!J19+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE17)/('Dry Bulb'!K19+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF17)/('Dry Bulb'!L19+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG17)/('Dry Bulb'!M19+459.67)))","v":2735.6148042529148},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH17)/('Dry Bulb'!N19+459.67)))","v":5750.9017199447371},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI17)/('Dry Bulb'!O19+459.67)))","v":6257.5691993654655},null,{"$f":"'Operative BP'!AP19","v":15},{"$f":"('Operative BP'!AQ19*$B$10)/(0.018033*$B$8)","v":8.94993093860454},{"$f":"('Operative BP'!AR19*$B$10)/(0.018033*$B$8)","v":2.2456428870536111},{"$f":"('Operative BP'!AS19*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT19*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU19*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV19*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW19*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX19*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY19*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ19*$B$10)/(0.018033*$B$8)","v":1.8357126663356644},{"$f":"('Operative BP'!BA19*$B$10)/(0.018033*$B$8)","v":7.9699549403069581},{"$f":"('Operative BP'!BB19*$B$10)/(0.018033*$B$8)","v":9.1826091794846754}]
["Ti",95,null,{"$f":"B18+459.67","v":554.67000000000007},"rankine",{"$f":"D18*0.5555556","v":308.15002465200007},"K",null,{"$f":"'Operative BP'!AP47","v":16},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X18)/('Dry Bulb'!D20+459.67)))","v":4339.1340658222471},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y18)/('Dry Bulb'!E20+459.67)))","v":520.2035974800026},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z18)/('Dry Bulb'!F20+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA18)/('Dry Bulb'!G20+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB18)/('Dry Bulb'!H20+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC18)/('Dry Bulb'!I20+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD18)/('Dry Bulb'!J20+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE18)/('Dry Bulb'!K20+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF18)/('Dry Bulb'!L20+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG18)/('Dry Bulb'!M20+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH18)/('Dry Bulb'!N20+459.67)))","v":3127.6782452551138},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI18)/('Dry Bulb'!O20+459.67)))","v":4262.6107113865801},null,{"$f":"'Operative BP'!AP20","v":16},{"$f":"('Operative BP'!AQ20*$B$10)/(0.018033*$B$8)","v":4.3972455117780962},{"$f":"('Operative BP'!AR20*$B$10)/(0.018033*$B$8)","v":6.393613105774261E-2},{"$f":"('Operative BP'!AS20*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT20*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU20*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV20*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW20*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX20*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY20*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ20*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA20*$B$10)/(0.018033*$B$8)","v":2.3534619037774078},{"$f":"('Operative BP'!BB20*$B$10)/(0.018033*$B$8)","v":4.2551368542400416}]
["To",70,null,{"$f":"B19+459.67","v":529.67000000000007},"rankine",{"$f":"D19*0.5555556","v":294.26113465200007},"K",null,{"$f":"'Operative BP'!AP48","v":17},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X19)/('Dry Bulb'!D21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y19)/('Dry Bulb'!E21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z19)/('Dry Bulb'!F21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA19)/('Dry Bulb'!G21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB19)/('Dry Bulb'!H21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC19)/('Dry Bulb'!I21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD19)/('Dry Bulb'!J21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE19)/('Dry Bulb'!K21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF19)/('Dry Bulb'!L21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG19)/('Dry Bulb'!M21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH19)/('Dry Bulb'!N21+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI19)/('Dry Bulb'!O21+459.67)))","v":1125.8280921451133},null,{"$f":"'Operative BP'!AP21","v":17},{"$f":"('Operative BP'!AQ21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA21*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB21*$B$10)/(0.018033*$B$8)","v":0.29571444967103022}]
[null,null,null,null,null,null,null,null,{"$f":"'Operative BP'!AP49","v":18},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X20)/('Dry Bulb'!D22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y20)/('Dry Bulb'!E22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z20)/('Dry Bulb'!F22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA20)/('Dry Bulb'!G22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB20)/('Dry Bulb'!H22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC20)/('Dry Bulb'!I22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD20)/('Dry Bulb'!J22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE20)/('Dry Bulb'!K22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF20)/('Dry Bulb'!L22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG20)/('Dry Bulb'!M22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH20)/('Dry Bulb'!N22+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI20)/('Dry Bulb'!O22+459.67)))","v":0},null,{"$f":"'Operative BP'!AP22","v":18},{"$f":"('Operative BP'!AQ22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA22*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB22*$B$10)/(0.018033*$B$8)","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"'Operative BP'!AP50","v":19},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X21)/('Dry Bulb'!D23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y21)/('Dry Bulb'!E23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z21)/('Dry Bulb'!F23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA21)/('Dry Bulb'!G23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB21)/('Dry Bulb'!H23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC21)/('Dry Bulb'!I23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD21)/('Dry Bulb'!J23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE21)/('Dry Bulb'!K23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF21)/('Dry Bulb'!L23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG21)/('Dry Bulb'!M23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH21)/('Dry Bulb'!N23+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI21)/('Dry Bulb'!O23+459.67)))","v":0},null,{"$f":"'Operative BP'!AP23","v":19},{"$f":"('Operative BP'!AQ23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA23*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB23*$B$10)/(0.018033*$B$8)","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"'Operative BP'!AP51","v":20},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X22)/('Dry Bulb'!D24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y22)/('Dry Bulb'!E24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z22)/('Dry Bulb'!F24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA22)/('Dry Bulb'!G24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB22)/('Dry Bulb'!H24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC22)/('Dry Bulb'!I24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD22)/('Dry Bulb'!J24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE22)/('Dry Bulb'!K24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF22)/('Dry Bulb'!L24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG22)/('Dry Bulb'!M24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH22)/('Dry Bulb'!N24+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI22)/('Dry Bulb'!O24+459.67)))","v":0},null,{"$f":"'Operative BP'!AP24","v":20},{"$f":"('Operative BP'!AQ24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA24*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB24*$B$10)/(0.018033*$B$8)","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"'Operative BP'!AP52","v":21},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X23)/('Dry Bulb'!D25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y23)/('Dry Bulb'!E25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z23)/('Dry Bulb'!F25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA23)/('Dry Bulb'!G25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB23)/('Dry Bulb'!H25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC23)/('Dry Bulb'!I25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD23)/('Dry Bulb'!J25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE23)/('Dry Bulb'!K25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF23)/('Dry Bulb'!L25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG23)/('Dry Bulb'!M25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH23)/('Dry Bulb'!N25+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI23)/('Dry Bulb'!O25+459.67)))","v":0},null,{"$f":"'Operative BP'!AP25","v":21},{"$f":"('Operative BP'!AQ25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA25*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB25*$B$10)/(0.018033*$B$8)","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"'Operative BP'!AP53","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X24)/('Dry Bulb'!D26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y24)/('Dry Bulb'!E26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z24)/('Dry Bulb'!F26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA24)/('Dry Bulb'!G26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB24)/('Dry Bulb'!H26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC24)/('Dry Bulb'!I26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD24)/('Dry Bulb'!J26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE24)/('Dry Bulb'!K26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF24)/('Dry Bulb'!L26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG24)/('Dry Bulb'!M26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH24)/('Dry Bulb'!N26+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI24)/('Dry Bulb'!O26+459.67)))","v":0},null,{"$f":"'Operative BP'!AP26","v":22},{"$f":"('Operative BP'!AQ26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA26*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB26*$B$10)/(0.018033*$B$8)","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"'Operative BP'!AP54","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X25)/('Dry Bulb'!D27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y25)/('Dry Bulb'!E27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z25)/('Dry Bulb'!F27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA25)/('Dry Bulb'!G27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB25)/('Dry Bulb'!H27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC25)/('Dry Bulb'!I27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD25)/('Dry Bulb'!J27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE25)/('Dry Bulb'!K27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF25)/('Dry Bulb'!L27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG25)/('Dry Bulb'!M27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH25)/('Dry Bulb'!N27+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI25)/('Dry Bulb'!O27+459.67)))","v":0},null,{"$f":"'Operative BP'!AP27","v":23},{"$f":"('Operative BP'!AQ27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA27*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB27*$B$10)/(0.018033*$B$8)","v":0}]
[null,null,null,null,null,null,null,null,{"$f":"'Operative BP'!AP55","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((X26)/('Dry Bulb'!D28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Y26)/('Dry Bulb'!E28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((Z26)/('Dry Bulb'!F28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AA26)/('Dry Bulb'!G28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AB26)/('Dry Bulb'!H28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AC26)/('Dry Bulb'!I28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AD26)/('Dry Bulb'!J28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AE26)/('Dry Bulb'!K28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AF26)/('Dry Bulb'!L28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AG26)/('Dry Bulb'!M28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AH26)/('Dry Bulb'!N28+459.67)))","v":0},{"$f":"60*$B$4*$B$9*SQRT(2*$B$13*($B$11-$B$12)*((AI26)/('Dry Bulb'!O28+459.67)))","v":0},null,{"$f":"'Operative BP'!AP28","v":24},{"$f":"('Operative BP'!AQ28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AR28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AS28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AT28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AU28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AV28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AW28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AX28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AY28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!AZ28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BA28*$B$10)/(0.018033*$B$8)","v":0},{"$f":"('Operative BP'!BB28*$B$10)/(0.018033*$B$8)","v":0}]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.4999999999999997E-2,"lbs"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"1/S31","v":13.333333333333334},"ft3/lb"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"0.24/S32","v":1.7999999999999999E-2}]